-- ================================================================
-- Copyright (C) 2006 by HUAWEI TECHNOLOGIES. All rights reserved
--
-- Description:The mib file is for management of VRRP extension
-- Reference:
-- Version: V1.0
-- History:
-- 2006.6.20, publish
-- ================================================================

    HUAWEI-VRRP-EXT-MIB DEFINITIONS ::= BEGIN
		IMPORTS
                   hwDatacomm
                     FROM HUAWEI-MIB
                   Integer32, Counter64, OBJECT-TYPE, MODULE-IDENTITY                  
                     FROM SNMPv2-SMI
                   RowStatus, DisplayString
                     FROM SNMPv2-TC
                   InterfaceIndex
                     FROM IF-MIB
                   VrId
                     FROM VRRP-MIB
                   EnabledStatus
                     FROM P-BRIDGE-MIB;
                     
                    
    hwVrrpExt MODULE-IDENTITY
        LAST-UPDATED "200705200000Z"        -- 
        ORGANIZATION
            "Huawei Technologies Co., Ltd."
        CONTACT-INFO
            "R&D Beijing, Huawei Technologies co.,Ltd.
            Huawei Bld.,NO.3 Xinxi Rd.,
            Shang-Di Information Industry Base,
            Hai-Dian District Beijing P.R. China
            Zip:100085
            Http://www.huawei.com                                      
            E-mail:support@huawei.com"
        DESCRIPTION
            "It supplies for VRRP tracking function."
        ::= { hwDatacomm 127 }

    hwVrrpExtGlobal      OBJECT IDENTIFIER ::= { hwVrrpExt 1 }

    hwVrrpExtFreeArpInterval OBJECT-TYPE
	SYNTAX Integer32 (30..1200)
	UNITS "seconds"
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"An interval of sending gratuitous-ARP."	
	::= { hwVrrpExtGlobal 1 }

    hwVrrpExtVIPPingCtr OBJECT-TYPE
	SYNTAX 	INTEGER
		{
		enable(1),
		disable(2)
		}
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"A switch decides whether the system responds to a request message or not, 
		 which is sent to virtual ip address. "
	DEFVAL { disable }
	::= { hwVrrpExtGlobal 2 }
	    
    hwVrrpExtSsTimer OBJECT-TYPE
	SYNTAX Integer32 (0..255)
	UNITS "seconds"
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"A switch decides whether the system enable VRRP SS function and set the size of VRRP SS timer or not,
		 which decide the VRRP packet advertisement interval during slave switchover."	
	DEFVAL { 100 }
	::= { hwVrrpExtGlobal 3 }
    
    hwVrrpExtLearnAdvIntervalFlag OBJECT-TYPE
	SYNTAX EnabledStatus	
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
		"A switch decides whether the system learn VRRP packet advertisement interval or not,
		 which is sended from the master router in one virtual router standby. "
	DEFVAL { enabled }
	::= { hwVrrpExtGlobal 4 }

        vrrpExtOperations      OBJECT IDENTIFIER ::= { hwVrrpExt 2 }
				
                hwVrrpTrackInterTable OBJECT-TYPE
                        SYNTAX SEQUENCE OF HWVrrpTrackInterEntry
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "The VRRP tracking interface table, it can accomodate eight rows at most."
                        ::= { vrrpExtOperations 1 }
               
                hwVrrpTrackInterEntry OBJECT-TYPE
                        SYNTAX HWVrrpTrackInterEntry
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "An entry in the VRRP tracking interface table."
                        INDEX { hwVrrpTrackInterVRID,hwVrrpTrackInterStandByIfnet,hwVrrpTrackInterIfnet }
                        ::= { hwVrrpTrackInterTable 1 }
                
                HWVrrpTrackInterEntry ::=
                        SEQUENCE { 
                                hwVrrpTrackInterVRID
                                        VrId,
                                hwVrrpTrackInterStandByIfnet
                                        InterfaceIndex,        
                                hwVrrpTrackInterIfnet
                                        InterfaceIndex,                                
                                hwVrrpTrackInterPriReduce
                                        Integer32,                               
                                hwVrrpTrackInterOperRowStatus
                                        RowStatus,
                                hwVrrpTrackInterPriIncrease
                                        Integer32                                         
                         }
                hwVrrpTrackInterVRID OBJECT-TYPE
                        SYNTAX VrId
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "The index of the VRRP tracking interface table, it identifies the standby's ID."
                        ::= { hwVrrpTrackInterEntry 1 }

                hwVrrpTrackInterStandByIfnet OBJECT-TYPE
                        SYNTAX InterfaceIndex
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "The index of the VRRP tracking interface table, it identifies the standby's interface index."
                        ::= { hwVrrpTrackInterEntry 2 }

                hwVrrpTrackInterIfnet OBJECT-TYPE
                        SYNTAX InterfaceIndex
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "The index of the VRRP tracking interface table, it identifies the tracked interface index."
                        ::= { hwVrrpTrackInterEntry 3 }                
           
                hwVrrpTrackInterPriReduce OBJECT-TYPE
                        SYNTAX Integer32 (0..255)
                        MAX-ACCESS read-create
                        STATUS current
                        DESCRIPTION
                                "If the tracked interface is down, priority of standby will reduce this value. '0' 
                                 specifies this attribute hasn't been configured. The minimum availability value is '1'."
                        ::= { hwVrrpTrackInterEntry 4 } 
                        
                hwVrrpTrackInterOperRowStatus OBJECT-TYPE
                        SYNTAX RowStatus
                        MAX-ACCESS read-create
                        STATUS current
                        DESCRIPTION
                                "The row status variable. "
                        ::= { hwVrrpTrackInterEntry 5 }                    
                        
                hwVrrpTrackInterPriIncrease OBJECT-TYPE
                        SYNTAX Integer32 (0..255)
                        MAX-ACCESS read-create
                        STATUS current
                        DESCRIPTION
                                "If the tracked interface is down, this value will be added to the priority of standby.
                                '0' specifies this attribute hasn't been configured. The minimum availability value is '1'."
                        ::= { hwVrrpTrackInterEntry 6 } 
                        
                                                
                hwVrrpTrackBfdTable OBJECT-TYPE
                        SYNTAX SEQUENCE OF HWVrrpTrackBfdEntry
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "The VRRP tracking BFD table, it can append eight rows at most."
                        ::= { vrrpExtOperations 2 }
               
                hwVrrpTrackBfdEntry OBJECT-TYPE
                        SYNTAX HWVrrpTrackBfdEntry
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "An entry in the VRRP tracking BFD table."
                        INDEX { hwVrrpTrackInterVRID,hwVrrpTrackInterStandByIfnet,hwVrrpTrackBfdId }
                        ::= { hwVrrpTrackBfdTable 1 }
                
                HWVrrpTrackBfdEntry ::=
                        SEQUENCE {                                 
                                hwVrrpTrackBfdId
                                        Integer32,                                        
                                hwVrrpTrackBfdPriReduce
                                        Integer32,                                                               
                                hwVrrpTrackBfdOperRowStatus
                                        RowStatus,
                                hwVrrpTrackBfdPriIncrease
                                        Integer32,  
                                hwVrrpTrackBfdType
                                        INTEGER                                      
                         }

                hwVrrpTrackBfdId OBJECT-TYPE
                        SYNTAX Integer32 (1..8191)
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "The index of the table, it only identifies BFD link."
                        ::= { hwVrrpTrackBfdEntry 1 }

                hwVrrpTrackBfdPriReduce OBJECT-TYPE
                        SYNTAX Integer32 (0..255)
                        MAX-ACCESS read-create
                        STATUS current
                        DESCRIPTION
                                "If the tracked BFD is down, the priority of standby will reduce this value.
                                '0' specifies this attribute hasn't been configured. 
                                The minimum availability value is '1'."
                        ::= { hwVrrpTrackBfdEntry 2 } 
                        
                hwVrrpTrackBfdOperRowStatus OBJECT-TYPE
                        SYNTAX RowStatus
                        MAX-ACCESS read-create
                        STATUS current
                        DESCRIPTION
                                "The row status variable. "
                        ::= { hwVrrpTrackBfdEntry 3 }  
                                                         
                hwVrrpTrackBfdPriIncrease OBJECT-TYPE
                        SYNTAX Integer32 (0..255)
                        MAX-ACCESS read-create
                        STATUS current
                        DESCRIPTION
                                "If the tracked BFD is down, this value will be added to the priority of standby.
                                '0' specifies this attribute hasn't been configured. 
                                The minimum availability value is '1'."
                        ::= { hwVrrpTrackBfdEntry 4 }   
                        
                hwVrrpTrackBfdType OBJECT-TYPE
                        SYNTAX INTEGER
                                {
                                link(1),
                                peer(2),
                                normal(3)   
                        }

                        MAX-ACCESS read-create
                        STATUS current
                        DESCRIPTION
                                "The bfd type that vrrp tracks,including Normal, Link, Peer. 
                                The attribute cannot be modified after created.                                
                                "      
                        DEFVAL { normal }
                        ::= { hwVrrpTrackBfdEntry 5 }                 
                                                                      
                                            
				hwAdminVrrpCfgTable OBJECT-TYPE
                        SYNTAX SEQUENCE OF HWAdminVrrpCfgEntry
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "The admin-vrrp's configure table."
                        ::= { vrrpExtOperations 3 }
               
                hwAdminVrrpCfgEntry OBJECT-TYPE
                        SYNTAX HWAdminVrrpCfgEntry
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "The admin-vrrp's configure entry."
                        INDEX { hwAdminVrrpCfgIfIndex, hwAdminVrrpCfgVRID}
                        ::= { hwAdminVrrpCfgTable 1 }
                
                HWAdminVrrpCfgEntry ::=
                        SEQUENCE {    
                        	hwAdminVrrpCfgIfIndex
                                        InterfaceIndex,                             
                                hwAdminVrrpCfgVRID
                                        VrId,                                                                                       
                                hwAdminVrrpCfgOperRowStatus
                                        RowStatus                                                                    
                         }
                         
                hwAdminVrrpCfgIfIndex OBJECT-TYPE
                        SYNTAX InterfaceIndex 
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "The admin-vrrp's configure interface index."
                        ::= { hwAdminVrrpCfgEntry 1 } 

                hwAdminVrrpCfgVRID OBJECT-TYPE
                        SYNTAX VrId 
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "The admin-vrrp's configure VRID."
                        ::= { hwAdminVrrpCfgEntry 2 }


                        
                hwAdminVrrpCfgOperRowStatus OBJECT-TYPE
                        SYNTAX RowStatus
                        MAX-ACCESS read-create
                        STATUS current
                        DESCRIPTION
                                "The row status variable. "
                        ::= { hwAdminVrrpCfgEntry 3 }                                                   
                                                         
                                                
				hwAdminVrrpMemberTable OBJECT-TYPE
                        SYNTAX SEQUENCE OF HWAdminVrrpMemberEntry
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "The admin-vrrp's configure table."
                        ::= { vrrpExtOperations 4 }
               
                hwAdminVrrpMemberEntry OBJECT-TYPE
                        SYNTAX HWAdminVrrpMemberEntry
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "The admin-vrrp's configure entry."
                        INDEX { hwAdminVrrpCfgIfIndex,hwAdminVrrpCfgVRID,hwAdminVrrpMemberIfIndex,hwAdminVrrpMemberVRID}
                        ::= { hwAdminVrrpMemberTable 1 }
                
                HWAdminVrrpMemberEntry ::=
                        SEQUENCE {        
                        
                                hwAdminVrrpMemberIfIndex
                                       InterfaceIndex,                          
                                hwAdminVrrpMemberVRID
                                        VrId,                                        
                                hwAdminVrrpMemberDiscardPkts
                                        Counter32,                                                                       
                                hwAdminVrrpMemberOperRowStatus
                                        RowStatus,     
                                hwAdminVrrpMemberFlowdownMode
                                		EnabledStatus                                                                       
                         }   

                hwAdminVrrpMemberIfIndex OBJECT-TYPE
                        SYNTAX InterfaceIndex 
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "The admin-vrrp's member interface index."
                        ::= { hwAdminVrrpMemberEntry 1 } 
                        
                hwAdminVrrpMemberVRID OBJECT-TYPE
                        SYNTAX VrId 
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "The admin-vrrp's member VRID."
                        ::= { hwAdminVrrpMemberEntry 2 }                     


                        
                hwAdminVrrpMemberDiscardPkts OBJECT-TYPE
                        SYNTAX Counter32
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "The admin-vrrp's member discarded packets."
                        ::= { hwAdminVrrpMemberEntry 3 }          
                hwAdminVrrpMemberOperRowStatus OBJECT-TYPE
                        SYNTAX RowStatus
                        MAX-ACCESS read-create
                        STATUS current
                        DESCRIPTION
                                "The row status variable. "
                        ::= { hwAdminVrrpMemberEntry 4 }                
                hwAdminVrrpMemberFlowdownMode OBJECT-TYPE
                        SYNTAX 	EnabledStatus	
                        MAX-ACCESS read-create
                        STATUS current
                        DESCRIPTION
                                "The mode of flowdown interface. "    
                        DEFVAL { enabled } 

                        ::= { hwAdminVrrpMemberEntry 5 }  
                                                         
                                          
				hwVrrpStatResetTable OBJECT-TYPE
                        SYNTAX SEQUENCE OF HWVrrpStatResetEntry
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "The vrrp statistics reset Table."
                        ::= { vrrpExtOperations 5 }
               
                hwVrrpStatResetEntry OBJECT-TYPE
                        SYNTAX HWVrrpStatResetEntry
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "The vrrp statistics reset entry."
                        INDEX { hwVrrpStatResetIfIndex,hwVrrpStatResetVRID}
                        ::= { hwVrrpStatResetTable 1 }
                
                HWVrrpStatResetEntry ::=
                        SEQUENCE {       
                        
                                hwVrrpStatResetIfIndex
                                        InterfaceIndex,                           
                                hwVrrpStatResetVRID
                                        VrId,                                                                                                      
                                hwVrrpStatResetFlag
                                        INTEGER                                                                    
                         }

                hwVrrpStatResetIfIndex OBJECT-TYPE
                        SYNTAX InterfaceIndex 
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "The vrrp's configure interface index."
                        ::= { hwVrrpStatResetEntry 1 } 
                        
                        
                hwVrrpStatResetVRID OBJECT-TYPE
                        SYNTAX VrId 
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "The vrrp vrid."
                        ::= { hwVrrpStatResetEntry 2 }


                        
                hwVrrpStatResetFlag OBJECT-TYPE
                        SYNTAX 	INTEGER	
                        {
							enable(1),
							disable(2)
						}
                        MAX-ACCESS read-write
                        STATUS current
                        DESCRIPTION
                                "A reset signal of vrrp statistics. "    
                        DEFVAL { disable } 

                        ::= { hwVrrpStatResetEntry 3 }  
                                                  
                                
				hwAdminVrrpTrackIfTable OBJECT-TYPE
						SYNTAX SEQUENCE OF HwAdminVrrpTrackIfEntry
						MAX-ACCESS not-accessible
						STATUS current
						DESCRIPTION 
							"The interface bound to VRRP table."
						::= { vrrpExtOperations  6 }
		        
				hwAdminVrrpTrackIfEntry  OBJECT-TYPE
						SYNTAX HwAdminVrrpTrackIfEntry
						MAX-ACCESS not-accessible
						STATUS current
						DESCRIPTION 
							"Entries of the interface bound to VRRP table."
						INDEX{ hwAdminVrrpTrackIfIndex }
						::= { hwAdminVrrpTrackIfTable 1}
		
				HwAdminVrrpTrackIfEntry  ::=
						SEQUENCE {
						hwAdminVrrpTrackIfIndex
							InterfaceIndex,  
						hwAdminVrrpIfIndex
							InterfaceIndex,						                        
						hwAdminVrrpVrid
							VrId,	        		
						hwAdminVrrpTrackIfRowStatus     
							RowStatus          
							}
		
				hwAdminVrrpTrackIfIndex  OBJECT-TYPE
						SYNTAX  InterfaceIndex
						MAX-ACCESS not-accessible
						STATUS current
						DESCRIPTION 
							"The number of the interface."
						::= { hwAdminVrrpTrackIfEntry 1 }  
				        
				hwAdminVrrpIfIndex  OBJECT-TYPE
						SYNTAX  InterfaceIndex
						MAX-ACCESS read-create
						STATUS current
						DESCRIPTION 
							"The administrator VRRP's configure interface index."
						::= { hwAdminVrrpTrackIfEntry 2 }
				          
		
				hwAdminVrrpVrid  OBJECT-TYPE
						SYNTAX  VrId
						MAX-ACCESS read-create
						STATUS current
						DESCRIPTION 
							"The administrator VRRP vrid."
						::= { hwAdminVrrpTrackIfEntry 3 }
				
				hwAdminVrrpTrackIfRowStatus  OBJECT-TYPE
						SYNTAX  RowStatus
						MAX-ACCESS read-create
						STATUS current
						DESCRIPTION 
							"Current operation status of the row."
						::= { hwAdminVrrpTrackIfEntry 4 }   
						
						
					                       
                                                                                  
			hwVrrpTrackEfmTable OBJECT-TYPE
                        SYNTAX SEQUENCE OF HWVrrpTrackEfmEntry
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "The VRRP tracking EFM table."
                        ::= { vrrpExtOperations 7 }
               
             hwVrrpTrackEfmEntry OBJECT-TYPE
                        SYNTAX HWVrrpTrackEfmEntry
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "An entry in the VRRP tracking EFM table."
                        INDEX { hwVrrpTrackEfmIfIndex,hwVrrpTrackEfmVRID,hwVrrpTrackEfmIndex }
                        ::= { hwVrrpTrackEfmTable 1 }
                
             HWVrrpTrackEfmEntry ::=
                        SEQUENCE {                                 
                                hwVrrpTrackEfmIfIndex
                                        InterfaceIndex,  
                                hwVrrpTrackEfmIfName
                                        DisplayString,                                               
                                hwVrrpTrackEfmVRID
                                        VrId,                                                             
                                hwVrrpTrackEfmIndex   
                                        InterfaceIndex, 
                                hwVrrpTrackEfmName
                                        DisplayString,            
                                hwVrrpTrackEfmOperRowStatus
                                        RowStatus
                                       
                         }

             hwVrrpTrackEfmIfIndex OBJECT-TYPE
                        SYNTAX InterfaceIndex 
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "The index of the table, it identifies vrrp's interface index."
                        ::= { hwVrrpTrackEfmEntry 1 }         
                        
             hwVrrpTrackEfmIfName OBJECT-TYPE
                        SYNTAX DisplayString (SIZE (0..255))
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "A textual string containing information about the interface of vrrp."
                        ::= { hwVrrpTrackEfmEntry 2 }
           

             hwVrrpTrackEfmVRID OBJECT-TYPE
                        SYNTAX VrId 
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "The index of the table, it identifies vrrp's vrid."
                        ::= { hwVrrpTrackEfmEntry 3 } 
                
             hwVrrpTrackEfmIndex OBJECT-TYPE
                        SYNTAX InterfaceIndex 
                        MAX-ACCESS not-accessible
                        STATUS current
                        DESCRIPTION
                                "The index of the table, it identifies EFM's interface index."
                        ::= { hwVrrpTrackEfmEntry 4 }     
            hwVrrpTrackEfmName OBJECT-TYPE
                        SYNTAX DisplayString (SIZE (0..255))
                        MAX-ACCESS read-only
                        STATUS current
                        DESCRIPTION
                                "A textual string containing information about the interface of efm."
                        ::= { hwVrrpTrackEfmEntry 5 }
            
                        
             hwVrrpTrackEfmOperRowStatus OBJECT-TYPE
                        SYNTAX RowStatus
                        MAX-ACCESS read-create
                        STATUS current
                        DESCRIPTION
                                "The row status variable. "
                        ::= { hwVrrpTrackEfmEntry 6 }  
                                                         
                         
                                                                        
        	vrrpExtConformance     OBJECT IDENTIFIER ::= { hwVrrpExt 3 }   
                        
                hwvrrpExtCompliances OBJECT IDENTIFIER ::= { vrrpExtConformance 1 }
                
                hwvrrpExtGroups OBJECT IDENTIFIER ::= { hwvrrpExtCompliances 1 }     
                                
                hwvrrpExtGlobalGroup OBJECT-GROUP
                        OBJECTS { hwVrrpExtFreeArpInterval, hwVrrpExtVIPPingCtr, hwVrrpExtSsTimer, hwVrrpExtLearnAdvIntervalFlag }
                        STATUS current
                        DESCRIPTION 
                                "The VRRP global attributes."
                        ::= { hwvrrpExtGroups 1 }                  
                                        
                hwvrrpExtTrackInterGroup OBJECT-GROUP
                        OBJECTS { hwVrrpTrackInterPriReduce, hwVrrpTrackInterOperRowStatus, hwVrrpTrackInterPriIncrease }
                        STATUS current
                        DESCRIPTION 
                                "The VRRP tracking inter attributes."
                        ::= { hwvrrpExtGroups 2 }       
                                                
                hwvrrpExtTrackBFDGroup OBJECT-GROUP
                        OBJECTS { hwVrrpTrackBfdPriReduce, hwVrrpTrackBfdOperRowStatus, hwVrrpTrackBfdPriIncrease,hwVrrpTrackBfdType }
                        STATUS current
                        DESCRIPTION 
                                "The VRRP tracking BFD attributes."
                        ::= { hwvrrpExtGroups 3 }  
                hwAdminVrrpCfgGroup OBJECT-GROUP
                        OBJECTS {  hwAdminVrrpCfgOperRowStatus }
                        STATUS current
                        DESCRIPTION 
                                "The AdminVrrpCfg attributes."
                        ::= { hwvrrpExtGroups 4 }    
                hwAdminVrrpMemberGroup OBJECT-GROUP
                        OBJECTS { hwAdminVrrpMemberDiscardPkts,hwAdminVrrpMemberOperRowStatus,hwAdminVrrpMemberFlowdownMode}
                        STATUS current
                        DESCRIPTION 
                                "The AdminVrrpMember attributes."
                        ::= { hwvrrpExtGroups 5 }   
                hwVrrpStatResetGroup OBJECT-GROUP
                        OBJECTS { hwVrrpStatResetFlag}
                        STATUS current
                        DESCRIPTION 
                                "The VrrpStatReset attributes."
                        ::= { hwvrrpExtGroups 6 }         
                hwAdminVrrpTrackIfGroup OBJECT-GROUP
                        OBJECTS { hwAdminVrrpIfIndex,hwAdminVrrpVrid,hwAdminVrrpTrackIfRowStatus }
                        STATUS current
                        DESCRIPTION 
                                "The AdminVrrpTrackIf attributes."
                        ::= { hwvrrpExtGroups 7 }      
                        
                hwVrrpTrackEfmGroup OBJECT-GROUP
                        OBJECTS {hwVrrpTrackEfmIfName,hwVrrpTrackEfmName,hwVrrpTrackEfmOperRowStatus }
                        STATUS current
                        DESCRIPTION 
                                "The VrrpTrackEfm attributes."
                        ::= { hwvrrpExtGroups 8 }                                                                                                                                                  
END
