-- *****************************************************************
-- CISCO-ENTITY-DISPLAY-MIB: Cisco Entity DISPLAY MIB file
--   
-- Jan 2003, Arvind Prabhudev, Mickey Spiegel, Sonal Maheshwari
--   
-- Copyright (c) 2003, 2009 by Cisco Systems, Inc.
-- All rights reserved.
-- *****************************************************************

CISCO-ENTITY-DISPLAY-MIB DEFINITIONS ::= BEGIN

IMPORTS
    Unsigned32,
    MODULE-IDENTITY,
    OBJECT-TYPE
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE,
    OBJECT-GROUP
        FROM SNMPv2-CONF
    TEXTUAL-CONVENTION,
    TruthValue
        FROM SNMPv2-TC
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    entPhysicalIndex
        FROM ENTITY-MIB
    ciscoMgmt
        FROM CISCO-SMI;


ciscoEntityDisplayMIB MODULE-IDENTITY
    LAST-UPDATED    "200910050000Z"
    ORGANIZATION    "Cisco Systems, Inc."
    CONTACT-INFO
            "Cisco Systems
            Customer Service

            Postal: 170 W Tasman Drive
            San Jose, CA  95134
            USA

            Tel: +1 800 553-NETS

            E-mail: cs-displaymib@cisco.com"
    DESCRIPTION
        "This MIB module provides information about the
        status of display devices such as Light Emitting
        Diodes (LEDs) and alphanumeric displays present
        on the physical entities contained by the managed
        system."
    REVISION        "200910050000Z"
    DESCRIPTION
        "Added the enumeration 'greenAndAmber' to
        CDisplayColor TEXTUAL-CONVENTION.
        Added support for ceDisplayBeaconGroup."
    REVISION        "200303200000Z"
    DESCRIPTION
        "Initial version of this MIB."
    ::= { ciscoMgmt 344 }



-- Textual Conventions

CDisplayType ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "An integer value that indicates the type of
        display device."
    SYNTAX          INTEGER  {
                        led(1),
                        alphanumeric(2)
                    }

CDisplayColor ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "An integer value that describes the color of the
        display.

        'greenAndAmber'    - Indicates that the display color
                             toggles between green and amber."
    SYNTAX          INTEGER  {
                        unknown(1),
                        white(2),
                        red(3),
                        green(4),
                        yellow(5),
                        amber(6),
                        blue(7),
                        greenAndAmber(8)
                    }

CDisplayState ::= TEXTUAL-CONVENTION
    STATUS          current
    DESCRIPTION
        "An integer value that describes the state of the
        display."
    SYNTAX          INTEGER  {
                        unknown(1),
                        off(2),
                        on(3),
                        blinking(4)
                    }
-- MIB Object Definitions

ciscoEntityDisplayMIBObjects  OBJECT IDENTIFIER
    ::= { ciscoEntityDisplayMIB 1 }

-- This table contains current display status information.

ceDisplayTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CeDisplayEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table provides information about the display
        devices on the physical entities in the managed
        system and their current display status."
    ::= { ciscoEntityDisplayMIBObjects 1 }

ceDisplayEntry OBJECT-TYPE
    SYNTAX          CeDisplayEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry in the ceDisplayTable that provides
        information about an LED or an alphanumeric display
        in the system including its current display status."
    INDEX           {
                        entPhysicalIndex,
                        ceDisplayIndex
                    } 
    ::= { ceDisplayTable 1 }

CeDisplayEntry ::= SEQUENCE {
        ceDisplayIndex Unsigned32,
        ceDisplayType  CDisplayType,
        ceDisplayName  SnmpAdminString,
        ceDisplayState CDisplayState,
        ceDisplayColor CDisplayColor,
        ceDisplayText  SnmpAdminString
}

ceDisplayIndex OBJECT-TYPE
    SYNTAX          Unsigned32 (1..1024)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An arbitrary index that uniquely identifies an LED or
        an alphanumeric display on the physical entity
        identified by entPhysicalIndex." 
    ::= { ceDisplayEntry 1 }

ceDisplayType OBJECT-TYPE
    SYNTAX          CDisplayType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the type of display described
        in this entry. i.e. whether it is an LED display or
        an alphanumeric display." 
    ::= { ceDisplayEntry 2 }

ceDisplayName OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object provides a human-readable string which is
        the name for the display device specified in this entry." 
    ::= { ceDisplayEntry 3 }

ceDisplayState OBJECT-TYPE
    SYNTAX          CDisplayState
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the current display state for
        the display specified in this entry." 
    ::= { ceDisplayEntry 4 }

ceDisplayColor OBJECT-TYPE
    SYNTAX          CDisplayColor
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object indicates the color currently seen on
        the display specified in this entry. If the display
        specified by this entry is an alphanumeric display,
        i.e. ceDisplayType is of type 'alphanumeric' then,
        color may not apply and the agent may choose to
        indicate this by setting this object to 'unknown'." 
    ::= { ceDisplayEntry 5 }

ceDisplayText OBJECT-TYPE
    SYNTAX          SnmpAdminString
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This object provides a human-readable string which is
        the text currently displayed in the alphanumeric display
        specified in this entry. If the display specified by
        this entry is an LED, i.e. ceDisplayType is of type 'led'
        then, this object would be an empty string." 
    ::= { ceDisplayEntry 6 }
 


ceDisplayBeaconTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF CeDisplayBeaconEntry 
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "This table provides functionality to manage
        beacon display devices in the managed system."
    ::= { ciscoEntityDisplayMIBObjects 2 }

ceDisplayBeaconEntry OBJECT-TYPE
    SYNTAX          CeDisplayBeaconEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry containing management information of
        beacon functionality of a particular beacon 
        display device.

        Only those display devices, as specified by 
        entPhysicalIndex in ENTITY-MIB, that support 
        beacon functionality will be populated in this 
        table."
    INDEX           {
                        entPhysicalIndex,
                        ceDisplayIndex
                    } 
    ::= { ceDisplayBeaconTable 1 }

CeDisplayBeaconEntry ::= SEQUENCE {
        ceDisplayBeaconEnabled TruthValue
}

ceDisplayBeaconEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "This object specifies if the beacon functionality is
        administratively enabled for this display device.

        'true'    - beacon functionality is administratively 
                    enabled
        'false'   - beacon functionality is administratively 
                    disabled." 
    ::= { ceDisplayBeaconEntry 1 }
 

-- MIB Conformance Information

ceDisplayMIBConformance  OBJECT IDENTIFIER
    ::= { ciscoEntityDisplayMIB 2 }

ceDisplayMIBCompliances  OBJECT IDENTIFIER
    ::= { ceDisplayMIBConformance 1 }

ceDisplayMIBGroups  OBJECT IDENTIFIER
    ::= { ceDisplayMIBConformance 2 }


-- Compliance Statements

ceDisplayMIBCompliance MODULE-COMPLIANCE
    STATUS          deprecated
    DESCRIPTION
        "The compliance statement for entities that implement the
        CISCO-ENTITY-DISPLAY-MIB.

        This compliance statement is deprecated and superceded by
        ceDisplayMIBCompliance2."
    MODULE          -- this module
    MANDATORY-GROUPS { ceDisplayGroup }

    GROUP           ceDisplayLEDGroup
    DESCRIPTION
        "This group is required when the display entity is an
        LED."

    GROUP           ceDisplayAlphaNumericGroup
    DESCRIPTION
        "This group is required when the display entity is an
        alphanumeric display."
    ::= { ceDisplayMIBCompliances 1 }

ceDisplayMIBCompliance2 MODULE-COMPLIANCE
    STATUS          current
    DESCRIPTION
        "The compliance statement for entities that implement the
        CISCO-ENTITY-DISPLAY-MIB."
    MODULE          -- this module
    MANDATORY-GROUPS { ceDisplayGroup }

    GROUP           ceDisplayLEDGroup
    DESCRIPTION
        "This group is required when the display entity is an
        LED."

    GROUP           ceDisplayAlphaNumericGroup
    DESCRIPTION
        "This group is required when the display entity is an
        alphanumeric display."

    GROUP           ceDisplayBeaconGroup
    DESCRIPTION
        "This group is required when system supports beacon
        functionality."

    OBJECT          ceDisplayBeaconEnabled
    MIN-ACCESS      read-only
    DESCRIPTION
        "Write access is not required."
    ::= { ceDisplayMIBCompliances 2 }

-- MIB groupings

ceDisplayGroup OBJECT-GROUP
    OBJECTS         {
                        ceDisplayType,
                        ceDisplayName,
                        ceDisplayState
                    }
    STATUS          current
    DESCRIPTION
        "A collection of managed objects that provide information
        about a display in the system including its current state."
    ::= { ceDisplayMIBGroups 1 }

ceDisplayLEDGroup OBJECT-GROUP
    OBJECTS         { ceDisplayColor }
    STATUS          current
    DESCRIPTION
        "A collection of objects relevant to LED display."
    ::= { ceDisplayMIBGroups 2 }

ceDisplayAlphaNumericGroup OBJECT-GROUP
    OBJECTS         { ceDisplayText }
    STATUS          current
    DESCRIPTION
        "A collection of objects relevant to alphanumeric display."
    ::= { ceDisplayMIBGroups 3 }

ceDisplayBeaconGroup OBJECT-GROUP
    OBJECTS         { ceDisplayBeaconEnabled }
    STATUS          current
    DESCRIPTION
        "A collection of objects relevant to beacon
        functionality."
    ::= { ceDisplayMIBGroups 4 }

END







