-- ArubaOS 3.2.0.0_16376
-- vim:set ts=4 sw=4:
WLSX-SYSTEMEXT-MIB DEFINITIONS ::= BEGIN

   IMPORTS
       TEXTUAL-CONVENTION,
       MODULE-IDENTITY,
       OBJECT-TYPE,
       snmpModules,
       Integer32,
	   Counter32,
	   IpAddress,
	   TimeTicks,
	   NOTIFICATION-TYPE
           FROM SNMPv2-SMI

       TDomain,
       DisplayString,
       PhysAddress,
       TAddress,
       TimeInterval,
       RowStatus,
       StorageType,
       TestAndIncr,
	   MacAddress,
	   TruthValue
           FROM SNMPv2-TC

	   ArubaSwitchRole,
       ArubaActiveState,
       ArubaCardType
	   		FROM ARUBA-TC

       OBJECT-GROUP
           FROM SNMPv2-CONF
	wlsxEnterpriseMibModules
           FROM ARUBA-MIB;

   wlsxSystemExtMIB MODULE-IDENTITY 
       LAST-UPDATED "0707300652Z"
       ORGANIZATION "Aruba Wireless Networks"
       CONTACT-INFO
            "Postal:    1322 Crossman Avenue
                        Sunnyvale, CA 94089
            E-mail:     dl-support@arubanetworks.com
            Phone:      +1 408 227 4500"
       DESCRIPTION
           "This MIB module defines MIB objects which provide
            System level information about the Aruba controller."
       REVISION        "0707300652Z"
       DESCRIPTION
           "The initial revision."
       ::= { wlsxEnterpriseMibModules 2 }

   wlsxSystemExtGroup       OBJECT IDENTIFIER ::= { wlsxSystemExtMIB 1 }
   wlsxSystemExtTableGenNumberGroup OBJECT IDENTIFIER ::= { wlsxSystemExtMIB 2 }

   -- wlsxSystemExtGroup contains objects to describe a controller.

   wlsxSysExtSwitchIp OBJECT-TYPE
        SYNTAX       IpAddress
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"Controller IP as configured by the user. This IP address uniquely 
			identifies the controller."
        ::= { wlsxSystemExtGroup 1 }

   wlsxSysExtHostname OBJECT-TYPE
        SYNTAX       DisplayString (SIZE(1..32))
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"Name of the controller."
        ::= { wlsxSystemExtGroup 2 }

   wlsxSysExtModelName OBJECT-TYPE
        SYNTAX       DisplayString (SIZE(1..32))
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"Model Name of the controller."
        ::= { wlsxSystemExtGroup 3 }

   wlsxSysExtSwitchRole OBJECT-TYPE
        SYNTAX      ArubaSwitchRole
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"Role of this controller in the Aruba Domain."
        ::= { wlsxSystemExtGroup 4 }

   wlsxSysExtSwitchMasterIp OBJECT-TYPE
        SYNTAX       IpAddress
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"
			 Switch IP of the master controller.
			"
        ::= { wlsxSystemExtGroup 5 }

   wlsxSysExtSwitchDate OBJECT-TYPE
        SYNTAX       DisplayString(SIZE(0..64))
        MAX-ACCESS   read-write
        STATUS       current
        DESCRIPTION
			"
			System notion of the local date and time of day.
			"
        ::= { wlsxSystemExtGroup 6 }

   wlsxSysExtSwitchBaseMacaddress OBJECT-TYPE
        SYNTAX       MacAddress
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"
			The Base MAC address of the controller.
			"
        ::= { wlsxSystemExtGroup 7 }

   wlsxSysExtFanTrayAssemblyNumber OBJECT-TYPE
        SYNTAX       DisplayString(SIZE(0..64))
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"
			Assembly number of the Fan tray.
			"
        ::= { wlsxSystemExtGroup 8 }

   wlsxSysExtFanTraySerialNumber OBJECT-TYPE
        SYNTAX       DisplayString(SIZE(0..64))
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"
			Serial number of the Fan tray
			"
        ::= { wlsxSystemExtGroup 9 }

   wlsxSysExtInternalTemparature OBJECT-TYPE
        SYNTAX       DisplayString(SIZE(0..64))
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"
			Internal temparature in the controller.
			"
        ::= { wlsxSystemExtGroup 10 }

   wlsxSysExtLicenseSerialNumber OBJECT-TYPE
        SYNTAX       DisplayString(SIZE(0..64))
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"
			The license serial number of the controller.
			"
        ::= { wlsxSystemExtGroup 11 }
         
   wlsxSysExtSwitchLicenseCount OBJECT-TYPE
        SYNTAX       Integer32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"
			 The number of licenses installed on the controller
			"
        ::= { wlsxSystemExtGroup 12 }

 -- Table lists all the processors and their corresponding Load.

   wlsxSysExtProcessorTable  OBJECT-TYPE 
	  SYNTAX       SEQUENCE OF WlsxSysExtProcessorEntry 
	  MAX-ACCESS   not-accessible		
      STATUS       current 
      DESCRIPTION 
	  	"
			The table of processors contained by the controller.
		"
	
      ::= { wlsxSystemExtGroup 13 } 

   wlsxSysExtProcessorEntry OBJECT-TYPE 
	  SYNTAX       WlsxSysExtProcessorEntry 
	  MAX-ACCESS   not-accessible		
      STATUS       current 
      DESCRIPTION 
	  "
	  	An entry for one processor contained by the controller.
	  "
	  INDEX { sysExtProcessorID}
      ::= { wlsxSysExtProcessorTable 1 } 

   WlsxSysExtProcessorEntry ::=
     SEQUENCE {
         sysExtProcessorID		Integer32,
         sysExtProcessorDescr 	DisplayString,
		 sysExtProcessorLoad	Integer32
     }

   sysExtProcessorID OBJECT-TYPE
         SYNTAX       Integer32
         MAX-ACCESS   not-accessible
         STATUS       current
         DESCRIPTION
            "
			Processor Index.
            "
        ::= { wlsxSysExtProcessorEntry 1 }

   sysExtProcessorDescr OBJECT-TYPE
        SYNTAX      DisplayString(SIZE(0..64))
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "
			Description of the processor.
            "
        ::= { wlsxSysExtProcessorEntry 2 }

   sysExtProcessorLoad OBJECT-TYPE
        SYNTAX       Integer32 (0..100)
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"
			The average, over the last minute, of the percentage of
			time that this processor was not idle.
			"
        ::= { wlsxSysExtProcessorEntry 3 }

   -- Table contains all the storage devices in the controller and their
   -- utilization numbers.

   wlsxSysExtStorageTable  OBJECT-TYPE 
	  SYNTAX       SEQUENCE OF WlsxSysExtStorageEntry 
	  MAX-ACCESS   not-accessible		
      STATUS       current 
      DESCRIPTION 
		"
		The table of Storage-devices contained by the controller.
		"
	
      ::= { wlsxSystemExtGroup 14 } 

   wlsxSysExtStorageEntry OBJECT-TYPE 
	  SYNTAX       WlsxSysExtStorageEntry 
	  MAX-ACCESS   not-accessible		
      STATUS       current 
      DESCRIPTION 
             "
			 	An entry for one long-term storage device contained by the 
				controller.
			 "
	  INDEX { sysExtStorageIndex }
      ::= { wlsxSysExtStorageTable 1 } 

   WlsxSysExtStorageEntry ::=
     SEQUENCE {
         sysExtStorageIndex		Integer32,
         sysExtStorageType 		INTEGER,
		 sysExtStorageSize		Integer32,
		 sysExtStorageUsed		Integer32,
		 sysExtStorageName		DisplayString
   }

   sysExtStorageIndex OBJECT-TYPE
         SYNTAX       Integer32
         MAX-ACCESS   not-accessible
         STATUS       current
         DESCRIPTION
            "
			Index into the table.
            "
        ::= { wlsxSysExtStorageEntry 1 }

   sysExtStorageType OBJECT-TYPE
        SYNTAX      INTEGER {
						ram(1),
						flashMemory(2)
					}

         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Type of the storage.
            "
        ::= { wlsxSysExtStorageEntry 2 }

   sysExtStorageSize OBJECT-TYPE
        SYNTAX      Integer32

         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Total size of the storage filesystem in MB.
            "
        ::= { wlsxSysExtStorageEntry 3 }

   sysExtStorageUsed OBJECT-TYPE
        SYNTAX      Integer32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Used Storage in MB.
            "
        ::= { wlsxSysExtStorageEntry 4 }

   sysExtStorageName OBJECT-TYPE
        SYNTAX      DisplayString(SIZE(0..64))
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Name of the storage filesystem.
            "
        ::= { wlsxSysExtStorageEntry 5 }

-- This table describes the memory utilization of the controller

   wlsxSysExtMemoryTable  OBJECT-TYPE 
	  SYNTAX       SEQUENCE OF WlsxSysExtMemoryEntry 
	  MAX-ACCESS   not-accessible		
      STATUS       current 
      DESCRIPTION 
		"
		The memory status of the controller
		"
	
      ::= { wlsxSystemExtGroup 15 } 

   wlsxSysExtMemoryEntry OBJECT-TYPE 
	  SYNTAX       WlsxSysExtMemoryEntry 
	  MAX-ACCESS   not-accessible		
      STATUS       current 
      DESCRIPTION 
             "
		An entry for one memory region on the controller.  Currently,
		only the control processor memory is monitored.
	     "
	  INDEX { sysExtMemoryIndex }
      ::= { wlsxSysExtMemoryTable 1 } 

   WlsxSysExtMemoryEntry ::=
     SEQUENCE {
     sysExtMemoryIndex	Integer32,
	 sysExtMemorySize	Integer32,
	 sysExtMemoryUsed	Integer32,
	 sysExtMemoryFree	Integer32
   }

   sysExtMemoryIndex OBJECT-TYPE
         SYNTAX       Integer32
         MAX-ACCESS   not-accessible
         STATUS       current
         DESCRIPTION
            "
			Index into the table.
            "
        ::= { wlsxSysExtMemoryEntry 1 }

   sysExtMemorySize OBJECT-TYPE
        SYNTAX      Integer32

         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
	    		Total memory in KB.
            "
        ::= { wlsxSysExtMemoryEntry 2 }

   sysExtMemoryUsed OBJECT-TYPE
        SYNTAX      Integer32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
	    		Used memory in KB.
            "
        ::= { wlsxSysExtMemoryEntry 3 }

   sysExtMemoryFree OBJECT-TYPE
        SYNTAX      Integer32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
	    		Free memory in KB.
            "
        ::= { wlsxSysExtMemoryEntry 4 }

-- This table lists the different Hardware Modules in the controller.

   wlsxSysExtCardTable  OBJECT-TYPE 
	  SYNTAX       SEQUENCE OF WlsxSysExtCardEntry 
	  MAX-ACCESS   not-accessible		
      STATUS       current 
      DESCRIPTION 
		"
		The table of Hardware modules in the controller.
		"
	
      ::= { wlsxSystemExtGroup 16 } 

   wlsxSysExtCardEntry OBJECT-TYPE 
	  SYNTAX       WlsxSysExtCardEntry 
	  MAX-ACCESS   not-accessible		
      STATUS       current 
      DESCRIPTION 
             "
			 	An entry for one Hardware Module in the controller.
			 "
	  INDEX { sysExtCardSlot }
      ::= { wlsxSysExtCardTable 1 } 

   WlsxSysExtCardEntry ::=
     SEQUENCE {
		 sysExtCardSlot						Integer32,
         sysExtCardType 					ArubaCardType,
		 sysExtCardNumOfPorts				Integer32,
		 sysExtCardNumOfFastethernetPorts	Integer32,
		 sysExtCardNumOfGigPorts			Integer32,
		 sysExtCardSerialNo					DisplayString,
		 sysExtCardAssemblyNo				DisplayString,
		 sysExtCardManufacturingDate		DisplayString,
		 sysExtCardHwRevision				DisplayString,
		 sysExtCardFpgaRevision				DisplayString,
		 sysExtCardSwitchChip				DisplayString,
		 sysExtCardStatus					ArubaActiveState,
		 sysExtCardUserSlot					Integer32
   }

   sysExtCardSlot OBJECT-TYPE
         SYNTAX      Integer32
         MAX-ACCESS   not-accessible
         STATUS       current
         DESCRIPTION
            "
			Slot in which this card is located, offset by one.  For the user-visible
			slot number see sysExtCardUserSlot
            "
        ::= { wlsxSysExtCardEntry 1 }

   sysExtCardType OBJECT-TYPE
         SYNTAX      ArubaCardType
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Type of the Card.
            "
        ::= { wlsxSysExtCardEntry 2 }

   sysExtCardNumOfPorts OBJECT-TYPE
         SYNTAX      Integer32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
		    Number of data ports on the card.	
            "
        ::= { wlsxSysExtCardEntry 3 }

   sysExtCardNumOfFastethernetPorts OBJECT-TYPE
        SYNTAX      Integer32
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Number of Fastethernet ports on the card.
            "
        ::= { wlsxSysExtCardEntry 4 }

   sysExtCardNumOfGigPorts OBJECT-TYPE
        SYNTAX      Integer32

         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Number of Gigabit ethernet ports on the card.
            "
        ::= { wlsxSysExtCardEntry 5 }

   sysExtCardSerialNo OBJECT-TYPE
        SYNTAX      DisplayString(SIZE(0..64))
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Serial number of the card.
            "
        ::= { wlsxSysExtCardEntry 6 }

   sysExtCardAssemblyNo OBJECT-TYPE
        SYNTAX      DisplayString(SIZE(0..64))
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Assembly Number of the card.
            "
        ::= { wlsxSysExtCardEntry 7 }

   sysExtCardManufacturingDate OBJECT-TYPE
        SYNTAX      DisplayString
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Card manufacturing date.
            "
        ::= { wlsxSysExtCardEntry 8 }

   sysExtCardHwRevision OBJECT-TYPE
        SYNTAX      DisplayString(SIZE(0..64))

         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Hardware revision of the card.
            "
        ::= { wlsxSysExtCardEntry 9 }

   sysExtCardFpgaRevision OBJECT-TYPE
        SYNTAX      DisplayString(SIZE(0..64))

         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Fpga revision number.
            "
        ::= { wlsxSysExtCardEntry 10 }

   sysExtCardSwitchChip OBJECT-TYPE
        SYNTAX      DisplayString(SIZE(0..64))

         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Switching Chip version.
            "
        ::= { wlsxSysExtCardEntry 11 }

   sysExtCardStatus OBJECT-TYPE
        SYNTAX      ArubaActiveState

         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Status of the card.
            "
        ::= { wlsxSysExtCardEntry 12 }

   sysExtCardUserSlot OBJECT-TYPE
        SYNTAX      Integer32

         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			User-visible (zero-based) slot number.
            "
        ::= { wlsxSysExtCardEntry 13 }

-- This table lists the Fans in the controller.

   wlsxSysExtFanTable  OBJECT-TYPE 
	  SYNTAX       SEQUENCE OF WlsxSysExtFanEntry 
	  MAX-ACCESS   not-accessible		
      STATUS       current 
      DESCRIPTION 
		"
		The table of all the fans in the controller.
		"
	
      ::= { wlsxSystemExtGroup 17 } 

   wlsxSysExtFanEntry OBJECT-TYPE 
	  SYNTAX       WlsxSysExtFanEntry 
	  MAX-ACCESS   not-accessible		
      STATUS       current 
      DESCRIPTION 
             "
			 	An entry for one fan.
			 "
	  INDEX { sysExtFanIndex }
      ::= { wlsxSysExtFanTable 1 } 

   WlsxSysExtFanEntry ::=
     SEQUENCE {
         sysExtFanIndex			Integer32,
		 sysExtFanStatus		ArubaActiveState
   }

   sysExtFanIndex OBJECT-TYPE
         SYNTAX       Integer32
         MAX-ACCESS   not-accessible
         STATUS       current
         DESCRIPTION
            "
			Index into the table.
            "
        ::= { wlsxSysExtFanEntry 1 }

   sysExtFanStatus OBJECT-TYPE
         SYNTAX      ArubaActiveState
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Status of the Fan.
            "
        ::= { wlsxSysExtFanEntry 2 }

-- This table lists the Power supplies in the controller.

   wlsxSysExtPowerSupplyTable  OBJECT-TYPE 
	  SYNTAX       SEQUENCE OF WlsxSysExtPowerSupplyEntry 
	  MAX-ACCESS   not-accessible		
      STATUS       current 
      DESCRIPTION 
		"
		The table of Power supplies in the controller.
		"
	
      ::= { wlsxSystemExtGroup 18 } 

   wlsxSysExtPowerSupplyEntry OBJECT-TYPE 
	  SYNTAX       WlsxSysExtPowerSupplyEntry 
	  MAX-ACCESS   not-accessible		
      STATUS       current 
      DESCRIPTION 
             "
			 An entry for one power supply.
			 "
	  INDEX { sysExtPowerSupplyIndex }
      ::= { wlsxSysExtPowerSupplyTable 1 } 

   WlsxSysExtPowerSupplyEntry ::=
     SEQUENCE {
         sysExtPowerSupplyIndex			Integer32,
		 sysExtPowerSupplyStatus		ArubaActiveState
   }

   sysExtPowerSupplyIndex OBJECT-TYPE
         SYNTAX       Integer32
         MAX-ACCESS   not-accessible
         STATUS       current
         DESCRIPTION
            "
			Index into the table.
            "
        ::= { wlsxSysExtPowerSupplyEntry 1 }

   sysExtPowerSupplyStatus OBJECT-TYPE
         SYNTAX      ArubaActiveState
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Status of the power supply.
            "
        ::= { wlsxSysExtPowerSupplyEntry 2 }

-- Switch List Table contains all the controllers in the domain. This table is 
-- valid only, when queried from the master controller.

   wlsxSysExtSwitchListTable  OBJECT-TYPE 
	  SYNTAX       SEQUENCE OF WlsxSysExtSwitchListEntry 
	  MAX-ACCESS   not-accessible		
      STATUS       current 
      DESCRIPTION 
	  	"This Table will list all the controllers in the Aruba Domain.
		 It will be populated only on the master controller. Local controllers
		 return empty table.
		"
	
      ::= { wlsxSystemExtGroup 19 } 

     wlsxSysExtSwitchListEntry OBJECT-TYPE 
	  SYNTAX       WlsxSysExtSwitchListEntry 
	  MAX-ACCESS   not-accessible		
      STATUS       current 
      DESCRIPTION 
             "Switch List Entry"
	  INDEX { sysExtSwitchIPAddress}
      ::= { wlsxSysExtSwitchListTable 1 } 

     WlsxSysExtSwitchListEntry ::=
     SEQUENCE {
         sysExtSwitchIPAddress	IpAddress,
         sysExtSwitchRole 		ArubaSwitchRole,
		 sysExtSwitchLocation	DisplayString,
		 sysExtSwitchSWVersion	DisplayString,
		 sysExtSwitchStatus		ArubaActiveState,
		 sysExtSwitchName		DisplayString,
		 sysExtSwitchSerNo      DisplayString
     }

     sysExtSwitchIPAddress OBJECT-TYPE
         SYNTAX       IpAddress
         MAX-ACCESS   not-accessible
         STATUS       current
         DESCRIPTION
            "
			IP Address of the controller.
            "
        ::= { wlsxSysExtSwitchListEntry 1 }

     sysExtSwitchRole OBJECT-TYPE
        SYNTAX      ArubaSwitchRole
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			 Role of the controller.
            "
        ::= { wlsxSysExtSwitchListEntry 2 }

     sysExtSwitchLocation OBJECT-TYPE
        SYNTAX      DisplayString(SIZE(0..64))
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Location of the controller
            "
        ::= { wlsxSysExtSwitchListEntry 3 }

     sysExtSwitchSWVersion OBJECT-TYPE
        SYNTAX      DisplayString(SIZE(0..64))
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Software version the controller is running.
            "
        ::= { wlsxSysExtSwitchListEntry 4 }

     sysExtSwitchStatus OBJECT-TYPE
        SYNTAX      ArubaActiveState
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Status of the controller.
            "
        ::= { wlsxSysExtSwitchListEntry 5 }

     sysExtSwitchName OBJECT-TYPE
        SYNTAX      DisplayString(SIZE(0..128))
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Host name of the controller.
            "
        ::= { wlsxSysExtSwitchListEntry 6 }

     sysExtSwitchSerNo OBJECT-TYPE
        SYNTAX      DisplayString(SIZE(0..32))
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			Serial number of the controller.
            "
        ::= { wlsxSysExtSwitchListEntry 7 }

-- The license table lists all valid licenses installed on the controller

   wlsxSysExtSwitchLicenseTable  OBJECT-TYPE 
	  SYNTAX       SEQUENCE OF WlsxSysExtLicenseEntry
	  MAX-ACCESS   not-accessible		
      STATUS       current 
      DESCRIPTION 
	  	"This table lists all licenses installed on the controller.
		"
	
      ::= { wlsxSystemExtGroup 20 } 

     wlsxSysExtLicenseEntry OBJECT-TYPE 
	 	SYNTAX      WlsxSysExtLicenseEntry
	 	MAX-ACCESS   not-accessible		
     	STATUS       current 
     	DESCRIPTION 
             "License Entry"
	  	INDEX { sysExtLicenseIndex }
      ::= { wlsxSysExtSwitchLicenseTable 1 } 

     WlsxSysExtLicenseEntry ::=
     SEQUENCE {
     	 sysExtLicenseIndex         Integer32,
         sysExtLicenseKey			DisplayString,
         sysExtLicenseInstalled		DisplayString,
         sysExtLicenseExpires		DisplayString,
         sysExtLicenseFlags			DisplayString,
         sysExtLicenseService 		DisplayString
     }

     sysExtLicenseIndex OBJECT-TYPE
         SYNTAX       Integer32
         MAX-ACCESS   not-accessible
         STATUS       current
         DESCRIPTION
            "
			License ID number
            "
        ::= { wlsxSysExtLicenseEntry 1 }

     sysExtLicenseKey OBJECT-TYPE
         SYNTAX       DisplayString
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			License Key
            "
        ::= { wlsxSysExtLicenseEntry 2 }

     sysExtLicenseInstalled OBJECT-TYPE
         SYNTAX       DisplayString
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			License installation time
            "
        ::= { wlsxSysExtLicenseEntry 3 }

     sysExtLicenseExpires OBJECT-TYPE
         SYNTAX       DisplayString
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			License expiry time
            "
        ::= { wlsxSysExtLicenseEntry 4 }

     sysExtLicenseFlags OBJECT-TYPE
         SYNTAX       DisplayString
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			License flags; E - enabled; A - auto-generated;
			               R - reboot required to activate
            "
        ::= { wlsxSysExtLicenseEntry 5 }

     sysExtLicenseService OBJECT-TYPE
         SYNTAX       DisplayString
         MAX-ACCESS   read-only
         STATUS       current
         DESCRIPTION
            "
			The service enabled by this license.
            "
        ::= { wlsxSysExtLicenseEntry 6 }

   wlsxSysExtMMSCompatLevel OBJECT-TYPE
        SYNTAX       Integer32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"
			 Lists the compatibility level of this controller with the MMS
			"
        ::= { wlsxSystemExtGroup 21 }

   wlsxSysExtMMSConfigID OBJECT-TYPE
        SYNTAX       Integer32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"
			 This Object represents the value of the MMS Configuration ID in the controller.
			"
        ::= { wlsxSystemExtGroup 22 }

   wlsxSysExtControllerConfigID OBJECT-TYPE
        SYNTAX       Integer32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"
			 This Object represents the value of the Controller's Configuration ID.
			"
        ::= { wlsxSystemExtGroup 23 }

   wlsxSysExtIsMMSConfigUpdateEnabled OBJECT-TYPE
        SYNTAX       TruthValue
        MAX-ACCESS   read-write
        STATUS       current
        DESCRIPTION
			"
			This objects indicates whether the controller is configured to accept configuration snapshots from MMS.
			"
        ::= { wlsxSystemExtGroup 24 }

   wlsxSysExtSwitchLastReload OBJECT-TYPE
        SYNTAX       DisplayString(SIZE(0..128))
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"
			 The reason for the last controller reload
			"
        ::= { wlsxSystemExtGroup 25 }

   wlsxSysExtLastStatsReset OBJECT-TYPE
        SYNTAX       TimeTicks
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"
			 Last time switch stats was reset
			"
        ::= { wlsxSystemExtGroup 26 }


   wlsxSysExtUserTableGenNumber OBJECT-TYPE
        SYNTAX       Integer32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"
			This objects denotes the number of times the user table was 
			modified since reboot.
			"
        ::= { wlsxSystemExtTableGenNumberGroup 1 }

   wlsxSysExtAPBssidTableGenNumber OBJECT-TYPE
        SYNTAX       Integer32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"
			This objects denotes the number of times the AP BSSID table was 
			modified since reboot.
			"
        ::= { wlsxSystemExtTableGenNumberGroup 2 }


   wlsxSysExtAPRadioTableGenNumber OBJECT-TYPE
        SYNTAX       Integer32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"
			This objects denotes the number of times the Radio table was 
			modified since reboot.
			"
        ::= { wlsxSystemExtTableGenNumberGroup 3 }


   wlsxSysExtAPTableGenNumber OBJECT-TYPE
        SYNTAX       Integer32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"
			This objects denotes the number of times the AP table was 
			modified since reboot.
			"
        ::= { wlsxSystemExtTableGenNumberGroup 4 }


   wlsxSysExtSwitchListTableGenNumber OBJECT-TYPE
        SYNTAX       Integer32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"
			This objects denotes the number of times the Switch list table was 
			modified since reboot.
			"
        ::= { wlsxSystemExtTableGenNumberGroup 5 }


   wlsxSysExtPortTableGenNumber OBJECT-TYPE
        SYNTAX       Integer32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"
			This objects denotes the number of times the port table was 
			modified since reboot.
			"
        ::= { wlsxSystemExtTableGenNumberGroup 6 }


   wlsxSysExtVlanTableGenNumber OBJECT-TYPE
        SYNTAX       Integer32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"
			This objects denotes the number of times the Vlan table was 
			modified since reboot.
			"
        ::= { wlsxSystemExtTableGenNumberGroup 7 }


   wlsxSysExtVlanInterfaceTableGenNumber OBJECT-TYPE
        SYNTAX       Integer32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"
			This objects denotes the number of times the Vlan Interface table 
			was modified since reboot.
			"
        ::= { wlsxSystemExtTableGenNumberGroup 8 }

   wlsxSysExtLicenseTableGenNumber OBJECT-TYPE
        SYNTAX       Integer32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"
			This objects denotes the number of times the license table
			was modified since reboot.
			"
        ::= { wlsxSystemExtTableGenNumberGroup 9 }

   wlsxSysExtMonAPTableGenNumber OBJECT-TYPE
        SYNTAX       Integer32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"
			This objects denotes the number of times the monitored AP table
			was modified since reboot.
			"
        ::= { wlsxSystemExtTableGenNumberGroup 10 }

   wlsxSysExtMonStationTableGenNumber OBJECT-TYPE
        SYNTAX       Integer32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
			"
			This objects denotes the number of times the monitored station table
			was modified since reboot.
			"
        ::= { wlsxSystemExtTableGenNumberGroup 11 }


END

