
ALCATEL-IND1-VLAN-STACKING-MIB DEFINITIONS ::= BEGIN

        IMPORTS
                MODULE-IDENTITY, 
                OBJECT-IDENTITY,
		OBJECT-TYPE, 
                Integer32		        FROM SNMPv2-SMI
		OBJECT-GROUP, 
                MODULE-COMPLIANCE	        FROM SNMPv2-CONF
		softentIND1VlanStackingMgt	FROM ALCATEL-IND1-BASE
		RowStatus			FROM SNMPv2-TC 
		InterfaceIndex 			FROM IF-MIB
		;

        alcatelIND1VLANStackingMIB MODULE-IDENTITY
		LAST-UPDATED "200704030000Z"
		ORGANIZATION "Alcatel-Lucent"
		CONTACT-INFO
                "Please consult with Customer Service to ensure the most appropriate
                version of this document is used with the products in question:
 	
				                   Alcatel-Lucent, Enterprise Solutions Division
			                    (Formerly Alcatel Internetworking, Incorporated)
				                         26801 West Agoura Road
			 	                       Agoura Hills, CA  91301-5122
			      		                United States Of America
	
                Telephone:	    North America	+1 800 995 2696
				                        Latin America 	+1 877 919 9526
                                Europe		+31 23 556 0100
                                Asia		+65 394 7933
                                All Other	+1 818 878 4507
	
                Electronic Mail:	support@ind.alcatel.com
                World Wide Web:		http://alcatel-lucent.com/wps/portal/enterprise
                File Transfer Protocol:	ftp://ftp.ind.alcatel.com/pub/products/mibs"
                DESCRIPTION
                "The parameters for configuration of the VLAN Stacking feature, 
                including the association between ports and svlans.

                The right to make changes in specification and other information
                contained in this document without prior notice is reserved.

                No liability shall be assumed for any incidental, indirect, special, or
                consequential damages whatsoever arising from or related to this 
                document or the information contained herein.

                Vendors, end-users, and other interested parties are granted
                non-exclusive license to use this specification in connection with 
                management of the products for which it is intended to be used.

                               Copyright (C) 1995-2006 Alcatel-Lucent
	                                 ALL RIGHTS RESERVED WORLDWIDE"
		::= { softentIND1VlanStackingMgt 1}


alcatelIND1VLANStackingMIBObjects OBJECT-IDENTITY
        STATUS current
        DESCRIPTION
            "Branch For VLAN Stacking Managed Objects."
     	::= { alcatelIND1VLANStackingMIB 1 }

alcatelIND1VLANStackingMIBConformance OBJECT-IDENTITY
        STATUS current
        DESCRIPTION
            "Branch For VLAN Stacking Conformance Information."
    	::= { alcatelIND1VLANStackingMIB 2 }

alcatelIND1VLANStackingMIBGroups OBJECT-IDENTITY
        STATUS current
        DESCRIPTION
            "Branch For VLAN Stacking Units Of Conformance."
     	::= { alcatelIND1VLANStackingMIBConformance 1 }

alcatelIND1VLANStackingMIBCompliances OBJECT-IDENTITY
        STATUS current
        DESCRIPTION
            "Branch For VLAN Stacking Compliance Statements."
    	 ::= { alcatelIND1VLANStackingMIBConformance 2 }




-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

--  The VLAN Stacking Port Table 

     alaVlanStackingPort OBJECT IDENTIFIER ::= { alcatelIND1VLANStackingMIBObjects 1 }

-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

alaVstkPortTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF  AlaVstkPortEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
        "A table that contains port-specific information for the VLAN Stacking feature. 
        An entry in this table is created when a port is configured with VLAN stacking 
        capability, OR when a port is configured with a specific vendor ethertype, a particular 
        bridge protocol action."
        ::= { alaVlanStackingPort 1 }

alaVstkPortEntry  OBJECT-TYPE
        SYNTAX  AlaVstkPortEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
        "A VLAN Stacking port entry."
        INDEX   { alaVstkPortNumber }
        ::= { alaVstkPortTable 1 }

AlaVstkPortEntry ::= SEQUENCE 
        {
                alaVstkPortNumber		InterfaceIndex,
		alaVstkPortType			INTEGER,
		alaVstkPortVendorTpid		Integer32,
		alaVstkPortBpduTreatment	INTEGER, 
		alaVstkPortAcceptFrameType	INTEGER,
		alaVstkPortLookupMiss		INTEGER,
		alaVstkPortDefaultSvlan		INTEGER,
		alaVstkPortRowStatus		RowStatus,
		alaVstkPortLegacyStpBpdu	INTEGER
        }

alaVstkPortNumber OBJECT-TYPE
        SYNTAX  InterfaceIndex
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
        "The  port ifindex of the port for which this entry contains 
        VLAN Stacking management information. "
        ::= { alaVstkPortEntry 1 }

alaVstkPortType  OBJECT-TYPE
        SYNTAX  INTEGER
        {
                userCustomer (1),
                userProvider (2),
                network (3)
        }
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
        "The type of this VLAN Stacking port. User-customer (1) is  a VLAN Stacking 
        user port connected to customer network. User-provider (2) is a VLAN Stacking
        user port used to run provider management traffic. Network (2) indicates a network 
        facing port."
        DEFVAL { userCustomer }
        ::= { alaVstkPortEntry 2 }

alaVstkPortVendorTpid  OBJECT-TYPE
        SYNTAX  Integer32 
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
        "The TPID for this port. It is used for the incoming data
        traffic parsing and it is substituted to the 802.1Q standard Tpid for 
        the outgoing data traffic. This is used for compatibility with other vendor 
        equipment. The default value is the standard value 0x88a8."
        DEFVAL { 34984 }
        ::= { alaVstkPortEntry 3 }

alaVstkPortBpduTreatment  OBJECT-TYPE
        SYNTAX  INTEGER
        {
                flooded (1),
                dropped (2)
        }
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
        "The customer bpdu treatment for this port. It defines the type of 
        processing  applied to the user's bridge protocol data unit. 
        The bridge protocol treatment (flooded) floods any user's bridge protocol data unit 
        to all user ports and network ports on the same SVLAN.
        The bridge protocol (dropped) drops any user's bridge protocol data unit."
        DEFVAL { flooded }
        ::= { alaVstkPortEntry 4 }

alaVstkPortAcceptFrameType  OBJECT-TYPE
        SYNTAX  INTEGER
        {
                tagged (1),
                untagged (2),
                all (3)
        }
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
        "The acceptable frame types on this port." 
        DEFVAL { all }
        ::= { alaVstkPortEntry 5 }

alaVstkPortLookupMiss  OBJECT-TYPE
        SYNTAX  INTEGER
        {
                drop (1),
                default (2)
        }
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
        "Treatment of tagged packets upon vlan lookup miss. Drop (1) means that on lookup
        miss the packets will be dropped. Default (2) means that on lookup miss the
        default SVLAN for that port will be used to tunnel the packets. 
        This is significant only for user port."
        DEFVAL { default }
        ::= { alaVstkPortEntry 6 }

alaVstkPortDefaultSvlan  OBJECT-TYPE
        SYNTAX  INTEGER (1..4094)
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
        "The default svlan of this port."
        ::= { alaVstkPortEntry 7 }

alaVstkPortRowStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
        "The status of this table entry.  The supported value supported for set are 
        createAndGo (4) and destroy(6), to create or remove a vlan-stacking port."
        ::= { alaVstkPortEntry 8 }	

alaVstkPortLegacyStpBpdu  OBJECT-TYPE
        SYNTAX  INTEGER
        {
                enable (1),
                disable (2)
        }
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
        "The legacy STP BPDU treatment for this port. It defines the type of processing 
         applied to STP legacy BPDUs on network ports. Legacy BPDU refer to conventional/customer
         BPDUs with MAC address 01:80:c2:00:00:00 and its processing on network ports can be 
         enabled/disabled by this object.By default the value is disabled i.e 
         provider MAC BPDU with MAC address 01:80:c2:00:00:08 would be processed at network ports."
        DEFVAL { disable }
        ::= { alaVstkPortEntry 9 }


-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

--  The VLAN Stacking svlan/port association Table 

    alaVlanStackingSvlanPort OBJECT IDENTIFIER ::= { alcatelIND1VLANStackingMIBObjects 2 }

-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

alaVstkSvlanPortTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF  AlaVstkSvlanPortEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
        "A table that contains svlan/ipmvlan-port association for the VLAN Stacking feature."
        ::= { alaVlanStackingSvlanPort 1 }
        
alaVstkSvlanPortEntry  OBJECT-TYPE
        SYNTAX  AlaVstkSvlanPortEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
        "The svlan/ipmvlan-port association."
        INDEX   { alaVstkSvlanPortSvlanNumber, alaVstkSvlanPortPortNumber,
                alaVstkSvlanPortCvlanNumber}
        ::= { alaVstkSvlanPortTable 1 }
        
AlaVstkSvlanPortEntry ::=   SEQUENCE 
        {
                alaVstkSvlanPortSvlanNumber		INTEGER,
		alaVstkSvlanPortPortNumber		InterfaceIndex,
                alaVstkSvlanPortCvlanNumber		INTEGER,
                alaVstkSvlanPortMode		INTEGER,
		alaVstkSvlanPortRowStatus		RowStatus
        }

alaVstkSvlanPortSvlanNumber  OBJECT-TYPE
        SYNTAX  INTEGER (1..4094)
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
        "Number identifying the svlan/ipmvlan."
        ::= { alaVstkSvlanPortEntry 1 }

alaVstkSvlanPortPortNumber OBJECT-TYPE
        SYNTAX  InterfaceIndex
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
        "The port ifindex of the port associated to the svlan/ipmvlan."
        ::= { alaVstkSvlanPortEntry 2 }

alaVstkSvlanPortCvlanNumber  OBJECT-TYPE
        SYNTAX  INTEGER (1..4094)
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
        "The customer vlan id associated to the svlan/ipmvlan."
        ::= { alaVstkSvlanPortEntry 3 }

alaVstkSvlanPortMode  OBJECT-TYPE
        SYNTAX  INTEGER 
        {
        	doubleTag (1),
        	translate (2)
        }
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
        "The vlan stacking mode: double tagging (1) or vlan translation/mapping (2).
	Only translation mode is valid in case of IPM Vlans"
        ::= { alaVstkSvlanPortEntry 4 }
        
alaVstkSvlanPortRowStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
        "The status of this table entry.  The supported value for set are 
        createAndGo (4) and destroy(6), to add or remove an 
        svlan-port association."
        ::= { alaVstkSvlanPortEntry 5 }	



-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx
-- COMPLIANCE
-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

alcatelIND1VLANStackingMIBCompliance MODULE-COMPLIANCE
        STATUS  current
        DESCRIPTION
        "Compliance statement for VLAN Stacking."
        MODULE  MANDATORY-GROUPS
                {
                        vlanStackingPortGroup,
        		vlanStackingSvlanPortGroup
                }
        ::= { alcatelIND1VLANStackingMIBCompliances 1 }


-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx
-- UNITS OF CONFORMANCE
-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

vlanStackingPortGroup OBJECT-GROUP
        OBJECTS
        {
                alaVstkPortNumber,	   --  The VLAN Stacking Port Table 
                alaVstkPortType,
                alaVstkPortVendorTpid,
                alaVstkPortBpduTreatment,
                alaVstkPortAcceptFrameType,
                alaVstkPortLookupMiss,
                alaVstkPortDefaultSvlan,
                alaVstkPortRowStatus
        }
        STATUS  current
        DESCRIPTION
        "Collection of objects for management of VLAN Stacking Ports."
        ::= { alcatelIND1VLANStackingMIBGroups 1 }

vlanStackingSvlanPortGroup OBJECT-GROUP
        OBJECTS
        {
                alaVstkSvlanPortSvlanNumber,
	    	alaVstkSvlanPortPortNumber,
                alaVstkSvlanPortCvlanNumber,
                alaVstkSvlanPortMode,
	    	alaVstkSvlanPortRowStatus
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for svlan-port associations."
        ::= { alcatelIND1VLANStackingMIBGroups 2 }
		
END

