
-- *****************************************************************************
-- Juniper-SLEP-MIB
--
-- Juniper Networks Enterprise MIB
--   Serial Line Encapsulation Protocol MIB
--
-- Copyright (c) 2000, 2001 Unisphere Networks, Inc.
-- Copyright (c) 2002 Juniper Networks, Inc.
--   All Rights Reserved.
-- *****************************************************************************

Juniper-SLEP-MIB  DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Counter32
        FROM SNMPv2-SMI
    RowStatus
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF
    InterfaceIndex, InterfaceIndexOrZero
        FROM IF-MIB
    juniMibs
        FROM Juniper-MIBs
    JuniNextIfIndex, JuniEnable
        FROM Juniper-TC;

juniSlepMIBS  MODULE-IDENTITY
    LAST-UPDATED "200209162144Z"  -- 16-Sep-02 05:44 PM EDT
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
        "       Juniper Networks, Inc.
        Postal: 10 Technology Park Drive
                Westford, MA  01886-3146
                USA
        Tel:    +1 978 589 5800
        E-mail: mib@Juniper.net"
    DESCRIPTION
        "The Serial Line Encapulation Protocol (SLEP) MIB for the Juniper
        Networks enterprise."
    -- Revision History
    REVISION    "200209162144Z"  -- 16-Sep-02 05:44 PM EDT  - JUNOSe 5.0
    DESCRIPTION
        "Replaced Unisphere names with Juniper names."
    REVISION    "200104031910Z"  -- 03-Apr-01 03:10 PM EDT  - JUNOSe 3.1
    DESCRIPTION
        "Add juniSledDownWhenLooped attribute."
    REVISION    "200001030000Z"  --  3-Jan-00               - JUNOSe 1.3
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { juniMibs 15 }


-- ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Managed objects
-- ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniSlepObjects     OBJECT IDENTIFIER ::= { juniSlepMIBS 1 }

--
-- This MIB contains managed objects for the Serial Line Encapulation
-- Protocol sublayer interface.
--
-- Management objects are provided to query for an available
-- interface index, and to create/delete interfaces of that type.
-- Creating/deleting these interface types using this MIB has the
-- side effect of creating/deleting corresponding entries in the
-- Interface MIB ifTable/ifXTable, and in the Juniper Enterprise
-- Interface MIB juniIfTable.
--
juniSlepIfLayer    OBJECT IDENTIFIER ::= { juniSlepObjects 1 }

-- //////////////////////////////////////////////////////////////////////
--
-- Serial Line Encapulation Interface Layer
--
-- This layer is managed with the following elements:
--
--  o NextIfIndex (generator for SLEP Ifndex selection)
--  o Interface Table (creation/configuration/deletion of SLEP interfaces)
--
-- //////////////////////////////////////////////////////////////////////
--
-- IfIndex selection for creating new SLEP interfaces
--
juniSlepNextIfIndex OBJECT-TYPE
    SYNTAX      JuniNextIfIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Coordinate ifIndex value allocation for entries in juniSlepIfTable.

        A GET of this object returns the next available ifIndex value to be used
        to create an entry in the associated interface table; or zero, if no
        valid ifIndex value is available.  This object also returns a value of
        zero when it is the lexicographic successor of a varbind presented in an
        SNMP GETNEXT or GETBULK request, for which circumstance it is assumed
        that ifIndex allocation is unintended.

        Successive GETs will typically return different values, thus avoiding
        collisions among cooperating management clients seeking to create table
        entries simultaneously."
    ::= { juniSlepIfLayer 1 }


--
-- The Slep Interface Table
--
juniSlepIfTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniSlepIfEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The parameters for the SLEP service on this interface."
    ::= { juniSlepIfLayer 2 }

juniSlepIfEntry OBJECT-TYPE
    SYNTAX      JuniSlepIfEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The Parameters for a particular SLEP interface.

        Creating/deleting entries in this table causes corresponding entries for
        be created/deleted in ifTable/ifXTable/juniIfTable."
    INDEX     { juniSlepIfIndex }
    ::= { juniSlepIfTable 1 }

JuniSlepIfEntry ::= SEQUENCE {
    juniSlepIfIndex         InterfaceIndex,
    juniSlepKeepAliveTimer  INTEGER,
    juniSlepIfLowerIfIndex  InterfaceIndexOrZero,
    juniSlepIfRowStatus     RowStatus,
    juniSlepDownWhenLooped  JuniEnable }

juniSlepIfIndex   OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ifIndex value of the corresponding ifEntry."
    ::= { juniSlepIfEntry 1 }

juniSlepKeepAliveTimer OBJECT-TYPE
    SYNTAX      INTEGER (0..6553)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The interface keep alive timer for this entry.  The time in seconds
        that this entity will wait for sending a keep-alive-message to the
        remote SLEP entity, and the time in seconds that this entity will wait
        for the reception of a keep-alive-message from the remote SLEP entity."
    DEFVAL    { 10 }
    ::= { juniSlepIfEntry 2 }

juniSlepIfLowerIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The ifIndex of an interface over which this SLEP interface is to be
        layered.  A value of zero indicates no layering.  An implementation may
        choose to require that a nonzero value be configured at entry creation."
    ::= { juniSlepIfEntry 3 }

juniSlepIfRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
            juniSlepIfRowStatus
            juniSlepIfLowerIfIndex

        In addition, when creating an entry the following conditions must hold:

            A value for juniSlepIfIndex must have been determined previously, by
            reading juniSlepNextIfIndex.

            The interface identified by juniSlepIfLowerIfIndex must exist, and
            must be an interface type that permits layering of SLEP Interface
            above it.

        A corresponding entry in ifTable/ifXTable/juniIfTable is created/
        destroyed as a result of creating/destroying an entry in this table."
    ::= { juniSlepIfEntry 4 }

juniSlepDownWhenLooped OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The down-when-looped control for this entry.  This attribute determines
        if loop detection is enabled for the interface.  If set to disable, loop
        detection is disabled for the interface."
    DEFVAL    { disable }
    ::= { juniSlepIfEntry 5 }


--
-- The Slep Interface Statistics Table
--
juniSlepIfStatisticsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniSlepIfStatisticsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The statistics for the SLEP service on this interface."
    ::= { juniSlepIfLayer 3 }

juniSlepIfStatisticsEntry OBJECT-TYPE
    SYNTAX      JuniSlepIfStatisticsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The statistics for a particular SLEP interface."
    INDEX     { juniSlepIfStatsIndex }
    ::= { juniSlepIfStatisticsTable 1 }

JuniSlepIfStatisticsEntry ::= SEQUENCE {
    juniSlepIfStatsIndex             InterfaceIndex,
    juniSlepKeepAliveFailures        Counter32,
    juniSlepLinkStatusTooLongPackets Counter32,
    juniSlepLinkStatusBadFCSs        Counter32 }

juniSlepIfStatsIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ifIndex value of that identifies this entry."
    ::= { juniSlepIfStatisticsEntry 1 }

juniSlepKeepAliveFailures OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of link drops due to keep-alive failures."
    ::= { juniSlepIfStatisticsEntry 2 }

juniSlepLinkStatusTooLongPackets OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets that were too long for this SLEP entity."
    ::= { juniSlepIfStatisticsEntry 3 }

juniSlepLinkStatusBadFCSs OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of FCS's errors for this SLEP entity."
    ::= { juniSlepIfStatisticsEntry 4 }


-- ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Notifications
-- ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- No notifications are defined in this MIB.  Placeholders follow.
-- juniSlepTrapControl  OBJECT IDENTIFIER ::= { juniSlepMIBS 2 }
-- juniSlepTraps        OBJECT IDENTIFIER ::= { juniSlepMIBS 3 }
-- juniSlepPrefix       OBJECT IDENTIFIER ::= { juniSlepTraps 0 }


-- ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Conformance information
-- ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniSlepConformance OBJECT IDENTIFIER ::= { juniSlepMIBS 4 }
juniSlepCompliances OBJECT IDENTIFIER ::= { juniSlepConformance 1 }
juniSlepGroups      OBJECT IDENTIFIER ::= { juniSlepConformance 2 }

--
-- compliance statements
--
juniSlepCompliance  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        SLEP MIB.  This compliance statement became obsolete when the
        juniSlepDownWhenLooped object was added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniSlepGroup }
    ::= { juniSlepCompliances 1 }                                  -- JUNOSe 1.3

juniSlepCompliance2  MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for entities which implement the Juniper
        SLEP MIB."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniSlepGroup2 }
    ::= { juniSlepCompliances 2 }                                  -- JUNOSe 3.1

--
-- units of conformance
--
juniSlepGroup  OBJECT-GROUP
    OBJECTS {
        juniSlepNextIfIndex,
        juniSlepKeepAliveTimer,
        juniSlepIfLowerIfIndex,
        juniSlepIfRowStatus,
        juniSlepKeepAliveFailures,
        juniSlepLinkStatusTooLongPackets,
        juniSlepLinkStatusBadFCSs }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of SLEP interfaces
        in a Juniper product.  This group became obsolete when the
        juniSlepDownWhenLooped object was added."
    ::= { juniSlepGroups 1 }

juniSlepGroup2  OBJECT-GROUP
    OBJECTS {
        juniSlepNextIfIndex,
        juniSlepKeepAliveTimer,
        juniSlepIfLowerIfIndex,
        juniSlepIfRowStatus,
        juniSlepDownWhenLooped,
        juniSlepKeepAliveFailures,
        juniSlepLinkStatusTooLongPackets,
        juniSlepLinkStatusBadFCSs }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing management of SLEP interfaces in a
        Juniper product."
    ::= { juniSlepGroups 2 }

END
