-- ==================================================================
-- Copyright (C) 2007 by  HUAWEI TECHNOLOGIES. All rights reserved.
-- 
-- Description: HUAWEI Private MIB
-- Reference:
-- Version: V1.0
-- History: V1.0 qiyanqing, 2007-05-14, publish

-- ==================================================================


    HUAWEI-TUNNEL-TE-MIB DEFINITIONS ::= BEGIN
 
        IMPORTS
            hwDatacomm            
                FROM HUAWEI-MIB    
            InterfaceIndex            
                FROM IF-MIB            
            MplsIndexType            
                FROM MPLS-LSR-STD-MIB            
            MplsTunnelIndex, MplsTunnelInstanceIndex, MplsExtendedTunnelId            
                FROM MPLS-TC-STD-MIB            
            SnmpAdminString            
                FROM SNMP-FRAMEWORK-MIB            
            OBJECT-GROUP, NOTIFICATION-GROUP            
                FROM SNMPv2-CONF            
            Integer32, Unsigned32, Counter32, Counter64, BITS, OBJECT-TYPE, 
            MODULE-IDENTITY, NOTIFICATION-TYPE            
                FROM SNMPv2-SMI
            TruthValue, TimeStamp, RowStatus            
                FROM SNMPv2-TC;
    
        hwTunnelTeMib MODULE-IDENTITY 
            LAST-UPDATED "200706101559Z"        -- June 10, 2007 at 15:59 GMT
            ORGANIZATION 
                "Huawei Technologies Co., Ltd."
            CONTACT-INFO 
                "MPLS Team Huawei Technologies co.,Ltd.
                 Huawei Bld.,NO.3 Xinxi Rd., 
                 Shang-Di Information Industry Base,
                 Hai-Dian District Beijing P.R. China
                 http://www.huawei.com
                 Zip:100085
                "
            DESCRIPTION 
                "This MIB contains private managed object  
                definitions for the binding information."
            REVISION "200606301554Z"        -- June 30, 2006 at 15:54 GMT
            DESCRIPTION
                "Initial version 2006/06/10,MPLS LSPM MIB GROUP."
            ::= { hwDatacomm 151 }
        
    
    
--
-- Node definitions
--
    

        hwTunnelTeMibObject OBJECT IDENTIFIER ::= { hwTunnelTeMib 1 }
        
            
  
     hwTunnelDiffServTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwTunnelDiffServEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
            "The table describes the different service mode of tunnel."
        ::= { hwTunnelTeMibObject  1}   
        


     hwTunnelDiffServEntry OBJECT-TYPE
        SYNTAX HwTunnelDiffServEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
            "Interface different service mode attribute configuration."
        INDEX   { hwTunnelDiffServIndex } 
        ::= {hwTunnelDiffServTable 1}

     HwTunnelDiffServEntry    ::=
        SEQUENCE {
            hwTunnelDiffServIndex
                     InterfaceIndex,
            hwTunnelDiffServMode
                     INTEGER,
            hwTunnelDiffServServiceClass
                     INTEGER,
            hwTunnelDiffServColor
                     INTEGER,  
            hwTunnelTeFlowQueue
                     OCTET STRING
                 }    
                 

      hwTunnelDiffServIndex OBJECT-TYPE
            SYNTAX InterfaceIndex
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Uniquely identifies a set of tunnel instances
                between a pair of ingress and egress LSRs.
                Managers should obtain new values for row
                creation in this table by reading mplsTunnelIndexNext. 
                When the MPLS signalling protocol is rsvp(2),this value 
                should be equal to the value signalled in the Tunnel ID 
                of the session object. When the MPLS signalling protocol 
                is crldp(3) this value should be equal to the value 
                signalled in the LSP ID. Reference to MPLS-TE-STD-MIB."
            ::= { hwTunnelDiffServEntry 1 } 
            
      hwTunnelDiffServMode OBJECT-TYPE
         SYNTAX  INTEGER
        {
                pipe(1),
                uniform(2)
        }
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION
                "Different service mode of TE interface, default is uniform."
        ::= { hwTunnelDiffServEntry 2 } 
        
      hwTunnelDiffServServiceClass OBJECT-TYPE
         SYNTAX INTEGER {
                            be(1),
                            af1(2),
                            af2(3),
                            af3(4),
                            af4(5),
                            ef(6),
                            cs6(7),
                            cs7(8),
                            invalidClass(255)
                        }
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION
                "PHB in the ingress PE, the value must be 
                 be,af1,af2,af3,af4,ef,cs6,cs7.The default class is invalidClass(255)."
        ::= { hwTunnelDiffServEntry 3 }    
        
  
      hwTunnelDiffServColor OBJECT-TYPE
         SYNTAX    INTEGER
            {
                green(1),
                yellow(2), 
                red(3),
                invalidColor(255)
            }
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION
                "Remarked color of packet in the ingress 
                 PE, the value must be green,yellow,red.The default color is invalidColor(255)."
        ::= { hwTunnelDiffServEntry 4 }   
        
     hwTunnelTeFlowQueue OBJECT-TYPE
         SYNTAX OCTET STRING (SIZE (0..31))
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION
                "Name of flow-queue template."
        ::= { hwTunnelDiffServEntry 5 }
       
     hwTunnelTeVsiTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwTunnelTeVsiEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
            "The table describes the VPN binding of Tunnel."
        ::= { hwTunnelTeMibObject  2 }   
        

     hwTunnelTeVsiEntry OBJECT-TYPE
        SYNTAX HwTunnelTeVsiEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
            "The L2VPN VSI binding configuration of tunnel interface."
        INDEX   { hwTunnelTeVsiIndex,hwTunnelTeVsiName } 
        ::= {hwTunnelTeVsiTable 1}

     HwTunnelTeVsiEntry    ::=
        SEQUENCE {
            hwTunnelTeVsiIndex
                     InterfaceIndex,
            hwTunnelTeVsiName
                     OCTET STRING,
            hwTunnelTeVsiCir 
                     Integer32,
            hwTunnelTeVsiPir
                     Integer32,
            hwTunnelTeVsiFlowQueue
                     OCTET STRING
                 }    
                 
      hwTunnelTeVsiIndex OBJECT-TYPE
            SYNTAX InterfaceIndex
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Uniquely identifies a set of tunnel instances
                between a pair of ingress and egress LSRs.
                Managers should obtain new values for row
                creation in this table by reading mplsTunnelIndexNext. 
                When the MPLS signalling protocol is rsvp(2),this value 
                should be equal to the value signalled in the tunnel ID 
                of the session object. When the MPLS signalling protocol 
                is crldp(3) this value should be equal to the value 
                signalled in the LSP ID. Reference to MPLS-TE-STD-MIB."
            ::= { hwTunnelTeVsiEntry 1 } 
            
      hwTunnelTeVsiName OBJECT-TYPE
         SYNTAX OCTET STRING (SIZE (0..47)) 
         MAX-ACCESS  not-accessible
         STATUS  current
         DESCRIPTION
                "The name of VSI that the TE interface bind."
        ::= { hwTunnelTeVsiEntry 2 }    
        
  
      hwTunnelTeVsiCir OBJECT-TYPE
         SYNTAX Integer32 (100..10000000)
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION
                "The Committed Information Rate of the VSI."
        ::= { hwTunnelTeVsiEntry 3}
        
  
      hwTunnelTeVsiPir OBJECT-TYPE
         SYNTAX Integer32 (100..10000000)
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION
                "The Peak Information Rate of the VSI."
        ::= { hwTunnelTeVsiEntry 4 }
        
  
      hwTunnelTeVsiFlowQueue OBJECT-TYPE
         SYNTAX OCTET STRING (SIZE (0..31))
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION
                "Name of flow-queue template."
        ::= { hwTunnelTeVsiEntry 5 }
    
     
     hwTunnelTeVllTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwTunnelTeVllEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
            "The table describes the VLL binding of tunnel."
        ::= { hwTunnelTeMibObject  3 }   
        

     hwTunnelTeVllEntry OBJECT-TYPE
        SYNTAX HwTunnelTeVllEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
            "The VLL binding configuration of tunnel interface."
        INDEX   { hwTunnelTeVllIndex,hwTunnelTeVllInterfaceName } 
        ::= {hwTunnelTeVllTable 1}

     HwTunnelTeVllEntry    ::=
        SEQUENCE { 
                 hwTunnelTeVllIndex
                     InterfaceIndex,    
                 hwTunnelTeVllInterfaceName  
                     OCTET STRING,
               hwTunnelTeVllCir 
                     Integer32,
            hwTunnelTeVllPir
                     Integer32,
           hwTunnelTeVllFlowQueue
                     OCTET STRING
                 }    
                 
      hwTunnelTeVllIndex OBJECT-TYPE
            SYNTAX InterfaceIndex
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Uniquely identifies a set of tunnel instances
                between a pair of ingress and egress LSRs.
                Managers should obtain new values for row
                creation in this table by reading mplsTunnelIndexNext. 
                When the MPLS signalling protocol is rsvp(2),this value 
                should be equal to the value signalled in the tunnel ID 
                of the session object. When the MPLS signalling protocol 
                is crldp(3) this value should be equal to the value 
                signalled in the LSP ID. Reference to MPLS-TE-STD-MIB."
            ::= { hwTunnelTeVllEntry 1 }   
            
       hwTunnelTeVllInterfaceName OBJECT-TYPE
         SYNTAX OCTET STRING (SIZE (0..47)) 
         MAX-ACCESS  not-accessible
         STATUS  current
         DESCRIPTION
                "The interface name of VLL binding."
        ::= { hwTunnelTeVllEntry 2 }           
        
                   
      hwTunnelTeVllCir OBJECT-TYPE
         SYNTAX Integer32 (100..10000000)
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION
                "The Committed Information Rate of the VLL."
        ::= { hwTunnelTeVllEntry 3}
        
  
      hwTunnelTeVllPir OBJECT-TYPE
         SYNTAX Integer32 (100..10000000)
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION
                "The Peak Information Rate of the VLL."
        ::= { hwTunnelTeVllEntry 4 }
        
  
      hwTunnelTeVllFlowQueue OBJECT-TYPE
         SYNTAX OCTET STRING (SIZE (0..31))
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION
                "Name of flow-queue template."
        ::= { hwTunnelTeVllEntry 5 }
        
     hwTunnelTeL3vpnTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwTunnelTeL3vpnEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
            "The table describes the L3VPN binding of tunnel."
        ::= { hwTunnelTeMibObject  4 }   
        

     hwTunnelTeL3vpnEntry OBJECT-TYPE
        SYNTAX HwTunnelTeL3vpnEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
            "The L3VPN binding configuration of tunnel interface."
        INDEX   { hwTunnelTeL3vpnIndex,hwTunnelTeL3vpnName } 
        ::= {hwTunnelTeL3vpnTable 1}

     HwTunnelTeL3vpnEntry    ::=
        SEQUENCE {
            hwTunnelTeL3vpnIndex
                     InterfaceIndex,
            hwTunnelTeL3vpnName
                     OCTET STRING,
            hwTunnelTeL3vpnCir 
                     Integer32,
            hwTunnelTeL3vpnPir
                     Integer32,
            hwTunnelTeL3vpnFlowQueue
                     OCTET STRING
                 }    
                 
      hwTunnelTeL3vpnIndex OBJECT-TYPE
            SYNTAX InterfaceIndex
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Uniquely identifies a set of tunnel instances
                between a pair of ingress and egress LSRs.
                Managers should obtain new values for row
                creation in this table by reading mplsTunnelIndexNext. 
                When the MPLS signalling protocol is rsvp(2),this value 
                should be equal to the value signalled in the tunnel ID 
                of the session object. When the MPLS signalling protocol 
                is crldp(3) this value should be equal to the value 
                signalled in the LSP ID. Reference to MPLS-TE-STD-MIB."
            ::= { hwTunnelTeL3vpnEntry 1 } 
            
  
      hwTunnelTeL3vpnName OBJECT-TYPE
         SYNTAX OCTET STRING (SIZE (0..47))
         MAX-ACCESS  not-accessible
         STATUS  current
         DESCRIPTION
                "The name of VPN instance that the TE interface bind."
        ::= { hwTunnelTeL3vpnEntry 2 }
        
  
      hwTunnelTeL3vpnCir OBJECT-TYPE
         SYNTAX Integer32 (100..10000000)
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION
                "The Committed Information Rate of the L3VPN."
        ::= { hwTunnelTeL3vpnEntry 3}
        
  
      hwTunnelTeL3vpnPir OBJECT-TYPE
         SYNTAX Integer32 (100..10000000)
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION
                "The Peak Information Rate of the L3VPN."
        ::= { hwTunnelTeL3vpnEntry 4 }
        
  
      hwTunnelTeL3vpnFlowQueue OBJECT-TYPE
         SYNTAX OCTET STRING (SIZE (0..31))
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION
                "Name of flow-queue template."
        ::= { hwTunnelTeL3vpnEntry 5 }
 
      hwTunnelTeStatisticsTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwTunnelTeStatisticsEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
            "The table describes the up/down state transition counts of the  TE tunnel interface."
        ::= { hwTunnelTeMibObject  5 }   

      hwTunnelTeStatisticsEntry OBJECT-TYPE
        SYNTAX HwTunnelTeStatisticsEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
            "The up/down state transition counts of TE tunnel interface.
             The index of the table is hwTunnelTeStatisticsIfIndex."
        INDEX   { hwTunnelTeStatisticsIfIndex} 
        ::= {hwTunnelTeStatisticsTable 1}

      HwTunnelTeStatisticsEntry    ::=
         SEQUENCE { 
                hwTunnelTeStatisticsIfIndex      InterfaceIndex,    
                    hwTunnelTeUpDownStatistics       Unsigned32,
                    hwTunnTeCounterDiscontinuityTime TimeStamp
                  }    
                 
      hwTunnelTeStatisticsIfIndex OBJECT-TYPE
         SYNTAX InterfaceIndex
         MAX-ACCESS not-accessible
         STATUS current
         DESCRIPTION
                "Uniquely identifies a set of tunnel instances
                between a pair of ingress and egress LSRs.
                Managers should obtain new values for row
                creation in this table by reading mplsTunnelIndexNext."
          ::= { hwTunnelTeStatisticsEntry 1 }   
            
       hwTunnelTeUpDownStatistics OBJECT-TYPE
          SYNTAX Unsigned32 
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
               "Describes the up/down transition counts of the TE tunnel interface."
          ::= { hwTunnelTeStatisticsEntry 2 }  
          
        hwTunnTeCounterDiscontinuityTime OBJECT-TYPE
          SYNTAX TimeStamp 
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
               "The value of sysUpTime on the most recent occasion at which this interface's up/down transition  counters suffered a discontinuity."
          ::= { hwTunnelTeStatisticsEntry 3 }          
               
 
               
               
               
          
      hwCtTemplateTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwCtTemplateEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
            "The table describes the CT template configuration on the device."
        ::= { hwTunnelTeMibObject  6 }   

      hwCtTemplateEntry OBJECT-TYPE
        SYNTAX HwCtTemplateEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
            "The CT template configuration on the device.
             The index of the table is hwCtTemplateIndex."
        INDEX   { hwCtTemplateIndex } 
        ::= {hwCtTemplateTable 1}

      HwCtTemplateEntry    ::=
         SEQUENCE { 
                    hwCtTemplateIndex                Integer32,  
                    hwCtTemplateName                 OCTET STRING,  
                    hwCtTemplateCt0                  Unsigned32,
                    hwCtTemplateCt1                  Unsigned32,
                    hwCtTemplateCt2                  Unsigned32,
                    hwCtTemplateCt3                  Unsigned32,
                    hwCtTemplateCt4                  Unsigned32,
                    hwCtTemplateCt5                  Unsigned32,                    
                    hwCtTemplateCt6                  Unsigned32,  
                    hwCtTemplateCt7                  Unsigned32,
                    hwCtTemplateCommit               INTEGER, 
                    hwCtTemplateRowStatus            RowStatus
                    }    
                    
        hwCtTemplateIndex OBJECT-TYPE
         SYNTAX Integer32 (1..4096)
         MAX-ACCESS not-accessible
         STATUS current
         DESCRIPTION
                "It uniquely identifies a set of CT templates.
                Managers should obtain new values for row
                creation in this table by reading hwCtTemplateIndex."
          ::= { hwCtTemplateEntry 1 } 
          
         hwCtTemplateName OBJECT-TYPE
             SYNTAX OCTET STRING (SIZE (1..19))
             MAX-ACCESS read-create
             STATUS current
             DESCRIPTION
                "The CT template name."
             ::= { hwCtTemplateEntry 2 } 
          
         hwCtTemplateCt0 OBJECT-TYPE
             SYNTAX Unsigned32
             MAX-ACCESS read-create
             STATUS current
             DESCRIPTION
                "The CT0 bandwidth of the CT template."
             ::= { hwCtTemplateEntry 3 }    
             
         hwCtTemplateCt1 OBJECT-TYPE
             SYNTAX Unsigned32 (0..32000000)
             MAX-ACCESS read-create
             STATUS current
             DESCRIPTION
                "The CT1 bandwidth of the CT template."
             ::= { hwCtTemplateEntry 4 }    
             
         hwCtTemplateCt2 OBJECT-TYPE
             SYNTAX Unsigned32 (0..32000000)
             MAX-ACCESS read-create
             STATUS current
             DESCRIPTION
                "The CT2 bandwidth of the CT template."
             ::= { hwCtTemplateEntry 5 }    
             
         hwCtTemplateCt3 OBJECT-TYPE
             SYNTAX Unsigned32 (0..32000000)
             MAX-ACCESS read-create
             STATUS current
             DESCRIPTION
                "The CT3 bandwidth of the CT template."
             ::= { hwCtTemplateEntry 6 }    
             
         hwCtTemplateCt4 OBJECT-TYPE
             SYNTAX Unsigned32 (0..32000000)
             MAX-ACCESS read-create
             STATUS current
             DESCRIPTION
                "The CT4 bandwidth of the CT template."
             ::= { hwCtTemplateEntry 7 }    
             
         hwCtTemplateCt5 OBJECT-TYPE
             SYNTAX Unsigned32 (0..32000000)
             MAX-ACCESS read-create
             STATUS current
             DESCRIPTION
                "The CT5 bandwidth of the CT template."
             ::= { hwCtTemplateEntry 8 }    
             
         hwCtTemplateCt6 OBJECT-TYPE
             SYNTAX Unsigned32 (0..32000000)
             MAX-ACCESS read-create
             STATUS current
             DESCRIPTION
                "The CT6 bandwidth of the CT template."
             ::= { hwCtTemplateEntry 9 }    
             
         hwCtTemplateCt7 OBJECT-TYPE
             SYNTAX Unsigned32 (0..32000000)
             MAX-ACCESS read-create
             STATUS current
             DESCRIPTION
                "The CT7 bandwidth of the CT template."
             ::= { hwCtTemplateEntry 10 }    
             
          hwCtTemplateCommit OBJECT-TYPE
             SYNTAX  INTEGER{ 
                             notCommit(1),
                             commit(2)
                             }
             MAX-ACCESS read-create
             STATUS current
             DESCRIPTION
                "The commit flag of the CT template,1 indicates commit,0 indicates not commit."
             ::= { hwCtTemplateEntry 11 }  
               
         hwCtTemplateRowStatus OBJECT-TYPE
            SYNTAX      RowStatus
            MAX-ACCESS  read-create
            STATUS      current
            DESCRIPTION
               "This object is used to create and delete rows in the CT template."
            ::= { hwCtTemplateEntry 12 }

          
      ----------------------
      
                 
               
          
      hwCtConfigTunnelCtTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwCtConfigTunnelCtEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
            "The table describes the CT configuration in the TE tunnel interface."
        ::= { hwTunnelTeMibObject  7 }   

      hwCtConfigTunnelCtEntry OBJECT-TYPE
        SYNTAX HwCtConfigTunnelCtEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
            "The table describes the CT configuration in the TE tunnel interface.
             The index of the table is hwCtConfigTunnelCtIfIndex."
        INDEX   { hwCtConfigTunnelCtIfIndex} 
        ::= {hwCtConfigTunnelCtTable 1}

      HwCtConfigTunnelCtEntry    ::=
         SEQUENCE { 
                        hwCtConfigTunnelCtIfIndex                InterfaceIndex,  
                        hwCtConfigTunnelName                     OCTET STRING,
                        hwCtConfigTunnelCommit                   INTEGER, 
                        hwCtConfigTemplateName                   OCTET STRING,  
                        hwCtConfigTunnelCt0Band                  Unsigned32,
                            hwCtConfigTunnelCt1Band                  Unsigned32,
                            hwCtConfigTunnelCt2Band                  Unsigned32,
                            hwCtConfigTunnelCt3Band                  Unsigned32,
                            hwCtConfigTunnelCt4Band                  Unsigned32,
                            hwCtConfigTunnelCt5Band                  Unsigned32,                    
                            hwCtConfigTunnelCt6Band                  Unsigned32,  
                            hwCtConfigTunnelCt7Band                  Unsigned32
                    }    
                    
        hwCtConfigTunnelCtIfIndex OBJECT-TYPE
            SYNTAX InterfaceIndex
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Uniquely identifies a set of tunnels
                between a pair of ingress and egress LSRs.
                Managers should obtain new values for row
                creation in this table by reading mplsTunnelIndexNext. 
                When the MPLS signalling protocol is rsvp(2),this value 
                should be equal to the value signalled in the tunnel ID 
                of the session object. When the MPLS signalling protocol 
                is crldp(3) this value should be equal to the value 
                signalled in the LSP ID. Reference to MPLS-TE-STD-MIB."
            ::= { hwCtConfigTunnelCtEntry 1 } 
            
         hwCtConfigTunnelName OBJECT-TYPE
                SYNTAX OCTET STRING (SIZE (0..64)) 
                MAX-ACCESS  read-only
                STATUS  current
                DESCRIPTION
                "The name of the TE tunnel interface."
                 ::= { hwCtConfigTunnelCtEntry 2 }    
                 
         hwCtConfigTunnelCommit OBJECT-TYPE
             SYNTAX  INTEGER{ 
                            notCommit(1),
                            commit(2)
                            }
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "The commit flag of the TE tunnel interface,1 indicates commit,0 indicates not commit."
                ::= { hwCtConfigTunnelCtEntry 3 }  
    
                                
         hwCtConfigTemplateName OBJECT-TYPE
             SYNTAX OCTET STRING (SIZE (1..19))
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "The CT template name."
                ::= { hwCtConfigTunnelCtEntry 4 }     
             
              
         hwCtConfigTunnelCt0Band OBJECT-TYPE
             SYNTAX Unsigned32 (0..32000000)
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "The CT0 bandwidth value of the TE tunnel interface."
             ::= { hwCtConfigTunnelCtEntry 5 }    
             
         hwCtConfigTunnelCt1Band OBJECT-TYPE
             SYNTAX Unsigned32 (0..32000000)
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "The CT1 bandwidth value of the TE tunnel interface."
             ::= { hwCtConfigTunnelCtEntry 6 }    
             
         hwCtConfigTunnelCt2Band OBJECT-TYPE
             SYNTAX Unsigned32 (0..32000000)
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "The CT2 bandwidth value of the TE tunnel interface."
             ::= { hwCtConfigTunnelCtEntry 7 }    
             
         hwCtConfigTunnelCt3Band OBJECT-TYPE
             SYNTAX Unsigned32 (0..32000000)
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "The CT3 bandwidth value of the TE tunnel interface."
             ::= { hwCtConfigTunnelCtEntry 8 }    
             
         hwCtConfigTunnelCt4Band OBJECT-TYPE
             SYNTAX Unsigned32 (0..32000000)
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "The CT4 bandwidth value of the TE tunnel interface."
             ::= { hwCtConfigTunnelCtEntry 9 }    
             
         hwCtConfigTunnelCt5Band OBJECT-TYPE
             SYNTAX Unsigned32 (0..32000000)
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "The CT5 bandwidth value of the TE tunnel interface."
             ::= { hwCtConfigTunnelCtEntry 10 }    
             
         hwCtConfigTunnelCt6Band OBJECT-TYPE
             SYNTAX Unsigned32 (0..32000000)
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "The CT6 bandwidth value of the TE tunnel interface."
             ::= { hwCtConfigTunnelCtEntry 11 }    
             
         hwCtConfigTunnelCt7Band OBJECT-TYPE
             SYNTAX Unsigned32 (0..32000000)
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "The CT7 bandwidth value of the TE tunnel interface."
             ::= { hwCtConfigTunnelCtEntry 12 }    
                                                 
      
      
      --------------
      
                 
          
     hwCtStatisticsTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HwCtStatisticsEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
            "The table describes flow statistics of the TE tunnel interface VPN configuration."
        ::= { hwTunnelTeMibObject  8 }   

      hwCtStatisticsEntry OBJECT-TYPE
        SYNTAX HwCtStatisticsEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
            "The table describes the statistics in the TE tunnel interface with CT configuration.
             The index of the table is hwCtStatisticsIfIndex."
        INDEX   { hwCtStatisticsIfIndex } 
        ::= {hwCtStatisticsTable 1}
  
      HwCtStatisticsEntry    ::=
         SEQUENCE { 
                    hwCtStatisticsIfIndex                 InterfaceIndex,
                        hwCtStatisticsTunnelName              OCTET STRING,    
                        hwCtStatisticsCt0OutByteRate          Counter64,                   
                        hwCtStatisticsCt0OutPktRate           Counter64,  
                    hwCtStatisticsCt0OutPkt               Counter64, 
                    hwCtStatisticsCt0OutPktByte           Counter64,   
                    hwCtStatisticsCt0OutErrorPkt          Counter64,    
                    hwCtStatisticsCt1OutByteRate          Counter64,
                    hwCtStatisticsCt1OutPktRate           Counter64, 
                    hwCtStatisticsCt1OutPkt               Counter64, 
                    hwCtStatisticsCt1OutPktByte           Counter64,   
                    hwCtStatisticsCt1OutErrorPkt          Counter64, 
                    hwCtStatisticsCt2OutByteRate          Counter64,
                    hwCtStatisticsCt2OutPktRate           Counter64, 
                    hwCtStatisticsCt2OutPkt               Counter64, 
                    hwCtStatisticsCt2OutPktByte           Counter64,   
                    hwCtStatisticsCt2OutErrorPkt          Counter64, 
                    hwCtStatisticsCt3OutByteRate          Counter64,
                        hwCtStatisticsCt3OutPktRate           Counter64,                      
                    hwCtStatisticsCt3OutPkt               Counter64, 
                    hwCtStatisticsCt3OutPktByte           Counter64,   
                    hwCtStatisticsCt3OutErrorPkt          Counter64, 
                    hwCtStatisticsCt4OutByteRate          Counter64,
                         hwCtStatisticsCt4OutPktRate           Counter64,                     
                    hwCtStatisticsCt4OutPkt               Counter64, 
                    hwCtStatisticsCt4OutPktByte           Counter64,   
                    hwCtStatisticsCt4OutErrorPkt          Counter64, 
                    hwCtStatisticsCt5OutByteRate          Counter64,
                        hwCtStatisticsCt5OutPktRate           Counter64,                      
                    hwCtStatisticsCt5OutPkt               Counter64, 
                    hwCtStatisticsCt5OutPktByte           Counter64,   
                    hwCtStatisticsCt5OutErrorPkt          Counter64,  
                    hwCtStatisticsCt6OutByteRate          Counter64,
                        hwCtStatisticsCt6OutPktRate           Counter64,                      
                    hwCtStatisticsCt6OutPkt               Counter64, 
                    hwCtStatisticsCt6OutPktByte           Counter64,   
                    hwCtStatisticsCt6OutErrorPkt          Counter64, 
                    hwCtStatisticsCt7OutByteRate          Counter64,
                        hwCtStatisticsCt7OutPktRate           Counter64,                      
                    hwCtStatisticsCt7OutPkt               Counter64, 
                    hwCtStatisticsCt7OutPktByte           Counter64,   
                    hwCtStatisticsCt7OutErrorPkt          Counter64
                    }    
                    
        hwCtStatisticsIfIndex OBJECT-TYPE
            SYNTAX InterfaceIndex
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Uniquely identifies a set of tunnels
                between a pair of ingress and egress LSRs.
                Managers should obtain new values for row
                creation in this table by reading mplsTunnelIndexNext. 
                When the MPLS signalling protocol is rsvp(2),this value 
                should be equal to the value signalled in the tunnel ID 
                of the session object. When the MPLS signalling protocol 
                is crldp(3) this value should be equal to the value 
                signalled in the LSP ID. Reference to MPLS-TE-STD-MIB."
            ::= { hwCtStatisticsEntry 1 } 
            
         hwCtStatisticsTunnelName OBJECT-TYPE
                SYNTAX OCTET STRING (SIZE (0..64)) 
                MAX-ACCESS  read-only
                STATUS  current
                DESCRIPTION
                "The name of the TE tunnel interface."
                 ::= { hwCtStatisticsEntry 2 }  

         hwCtStatisticsCt0OutByteRate OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the rate in bytes/sec out from the CT0 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 3 }    
                
                
                
         hwCtStatisticsCt0OutPktRate      OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the rate in packets/sec out from the CT0 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 4 }    
             
         hwCtStatisticsCt0OutPkt OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the out packets from the CT0 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 5 }  
                  
         hwCtStatisticsCt0OutPktByte OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the out bytes from the CT0 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 6 }   
      
         hwCtStatisticsCt0OutErrorPkt OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the error packets from the CT0 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 7 }   

         hwCtStatisticsCt1OutByteRate OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the rate in bytes/sec out from CT1 the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 8 }                  
                
         hwCtStatisticsCt1OutPktRate      OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the rate in packets/sec out from the CT0 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 9 }    
                   
                  
             
         hwCtStatisticsCt1OutPkt OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the out packets from the CT1 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 10 }    
         hwCtStatisticsCt1OutPktByte OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the out packet bytes from the CT1 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 11 }   
      
         hwCtStatisticsCt1OutErrorPkt OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the error packets from the CT1 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 12 }   
      
 
         hwCtStatisticsCt2OutByteRate OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the rate in bytes/sec out from the CT2 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 13 }    
                 
         hwCtStatisticsCt2OutPktRate      OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the rate in packets/sec out from the CT2 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 14 }    
   
 
             
         hwCtStatisticsCt2OutPkt OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the out packets from the CT2 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 15 }    
         hwCtStatisticsCt2OutPktByte OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the out packet bytes from the CT2 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 16 }   
      
         hwCtStatisticsCt2OutErrorPkt OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the error packets from the CT2 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 17 }   
      

         hwCtStatisticsCt3OutByteRate OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "The CT3 out in bytes/sec out of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 18 }    
                
         hwCtStatisticsCt3OutPktRate      OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the rate in packets/sec out from the CT0 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 19 }    
                   
                
                
             
         hwCtStatisticsCt3OutPkt OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the out packets from the CT3 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 20 }    
         hwCtStatisticsCt3OutPktByte OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the out packet bytes from the CT3 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 21 }   
      
         hwCtStatisticsCt3OutErrorPkt OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the error packets from the CT0 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 22 }   
      
 
         hwCtStatisticsCt4OutByteRate OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "The CT4 out in bytes/sec out of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 23 }  
                
                 
         hwCtStatisticsCt4OutPktRate      OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the rate in packets/sec out from the CT4 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 24 }    
                    
             
         hwCtStatisticsCt4OutPkt OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the out packets from the CT4 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 25 } 
                   
         hwCtStatisticsCt4OutPktByte OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the out packet bytes from the CT4 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 26 }   
      
         hwCtStatisticsCt4OutErrorPkt OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the error packets from the CT4 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 27 }   
      
 
         hwCtStatisticsCt5OutByteRate OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "The CT5 out in bytes/sec out of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 28 }  
                
                
         hwCtStatisticsCt5OutPktRate      OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the rate in packets/sec out from the CT5 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 29 }    
                     
             
         hwCtStatisticsCt5OutPkt OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the out packets from the CT5 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 30 }    
         hwCtStatisticsCt5OutPktByte OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the out packet bytes from the CT5 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 31 }   
      
         hwCtStatisticsCt5OutErrorPkt OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the error packets from the CT5 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 32 }   
      

         hwCtStatisticsCt6OutByteRate OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "The CT6 out in bytes/sec out of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 33 } 
                
                 
         hwCtStatisticsCt6OutPktRate      OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the rate in packets/sec out from the CT6 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 34 }    
                     
             
         hwCtStatisticsCt6OutPkt OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the out packets from the CT6 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 35 }    
         hwCtStatisticsCt6OutPktByte OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the out packet bytes from the CT6 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 36 }   
      
         hwCtStatisticsCt6OutErrorPkt OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the error packets from the CT6 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 37 }   
      

         hwCtStatisticsCt7OutByteRate OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "The CT7 out in bytes/sec out of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 38 }    

                
         hwCtStatisticsCt7OutPktRate      OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the rate in packets/sec out from the CT7 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 39 }    
   
             
         hwCtStatisticsCt7OutPkt OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the out packets from the CT7 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 40 }    
         hwCtStatisticsCt7OutPktByte OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the out packet bytes from the CT7 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 41 }   
      
         hwCtStatisticsCt7OutErrorPkt OBJECT-TYPE
             SYNTAX Counter64
             MAX-ACCESS read-only
             STATUS current
             DESCRIPTION
                "It counts the error packets from the CT7 of the TE tunnel interface with VPN configuration."
                ::= { hwCtStatisticsEntry 42 }   
      
      
                      
             

-- Node definitions
--
    

        
        hwCtFlowTemplateTable  OBJECT-TYPE
        SYNTAX SEQUENCE OF HwCtFlowTemplateEntry 
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
            "The table describes max 8 of the CT-FLOW-Mapping template configuration on the device.
            "
        ::= { hwTunnelTeMibObject  9}    
       
           hwCtFlowTemplateEntry  OBJECT-TYPE
        SYNTAX  HwCtFlowTemplateEntry 
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
            "The table describes the CT-FLOW-Mapping template configuration on the device.
            "
        INDEX   { hwCtFlowTemplateID } 
        ::= { hwCtFlowTemplateTable  1} 
        
        HwCtFlowTemplateEntry  ::=
        SEQUENCE 
        {
            hwCtFlowTemplateID Integer32,
            
            hwCtFlowTemplateName  OCTET STRING, 
                                    
            hwCt0Cos INTEGER,
           
            hwCt0Scheduler  INTEGER,
            
            hwCt0Valid INTEGER , 
                                    
            hwCt1Cos INTEGER,
           
            hwCt1Scheduler  INTEGER,
            
            hwCt1Valid INTEGER ,
                        
            hwCt2Cos INTEGER,
           
            hwCt2Scheduler  INTEGER,
            
            hwCt2Valid INTEGER ,
                        
            hwCt3Cos INTEGER,
           
            hwCt3Scheduler  INTEGER,
            
            hwCt3Valid INTEGER ,
                         
            hwCt4Cos INTEGER,
           
            hwCt4Scheduler  INTEGER,
            
            hwCt4Valid INTEGER ,
                        
            hwCt5Cos INTEGER,
           
            hwCt5Scheduler  INTEGER,
            
            hwCt5Valid INTEGER ,
                        
            hwCt6Cos INTEGER,
           
            hwCt6Scheduler  INTEGER,
            
            hwCt6Valid INTEGER ,
                        
            hwCt7Cos INTEGER,
           
            hwCt7Scheduler  INTEGER,
            
            hwCt7Valid INTEGER ,
            
            hwCtFlowTemplateCommit INTEGER,
            
            hwCtFlowTemplateRowStatus RowStatus        
 
        } 
         
        hwCtFlowTemplateID  OBJECT-TYPE
        SYNTAX Integer32 (1..8)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
            "The index of CT-FLOW templat."
        ::= {hwCtFlowTemplateEntry 1}
        
        hwCtFlowTemplateName OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (1..60))
        MAX-ACCESS  read-create
        STATUS  current
        DESCRIPTION
                "The name of CT-FLOW template."
        ::= { hwCtFlowTemplateEntry 11 } 
        
        --CT0参数定义
        hwCt0Cos  OBJECT-TYPE
        SYNTAX INTEGER {
                            be(1),
                            af1(2),
                            af2(3),
                            af3(4),
                            af4(5),
                            ef(6),
                            cs6(7),
                            cs7(8)
                        }
         MAX-ACCESS  read-create
         STATUS  current
         DESCRIPTION
                "The Value of class of service must be in 'be,af1,af2,af3,af4,ef,cs6,cs7'."
        ::= { hwCtFlowTemplateEntry 12 }
        
        hwCt0Scheduler  OBJECT-TYPE
         SYNTAX INTEGER {
                            pq(1),
                            wfq(2),
                            lpq(3)
                        }
         MAX-ACCESS  read-create
         STATUS  current
         DESCRIPTION
                "Scheduler name."
        ::= { hwCtFlowTemplateEntry 13 }
   
        hwCt0Valid OBJECT-TYPE
        SYNTAX INTEGER {
                            valid(1),
                            invalid(2)
                        }
        MAX-ACCESS  read-create
        STATUS  current
        DESCRIPTION
                "The state of CT-FLOW templat row."
        ::= { hwCtFlowTemplateEntry 14 }                            
        --CT0参数定义结束
        --CT1参数定义
        hwCt1Cos  OBJECT-TYPE
        SYNTAX INTEGER {
                            be(1),
                            af1(2),
                            af2(3),
                            af3(4),
                            af4(5),
                            ef(6),
                            cs6(7),
                            cs7(8)
                        }
         MAX-ACCESS  read-create
         STATUS  current
         DESCRIPTION
                "The Value of class of service must be in 'be,af1,af2,af3,af4,ef,cs6,cs7'."
        ::= { hwCtFlowTemplateEntry 15 }
        
        hwCt1Scheduler  OBJECT-TYPE
         SYNTAX INTEGER {
                            pq(1),
                            wfq(2),
                            lpq(3)
                        }
         MAX-ACCESS  read-create
         STATUS  current
         DESCRIPTION
                "Scheduler name."
        ::= { hwCtFlowTemplateEntry 16 }
   
        hwCt1Valid OBJECT-TYPE
        SYNTAX INTEGER {
                            valid(1),
                            invalid(2)
                        }

        MAX-ACCESS  read-create
        STATUS  current
        DESCRIPTION
                "The state of CT-FLOW templat row."
        ::= { hwCtFlowTemplateEntry 17 }                            
        --CT1参数定义结束
        --CT2参数定义
        hwCt2Cos  OBJECT-TYPE
        SYNTAX INTEGER {
                            be(1),
                            af1(2),
                            af2(3),
                            af3(4),
                            af4(5),
                            ef(6),
                            cs6(7),
                            cs7(8)
                        }
         MAX-ACCESS  read-create
         STATUS  current
         DESCRIPTION
                "The Value of class of service must be in 'be,af1,af2,af3,af4,ef,cs6,cs7'."
        ::= { hwCtFlowTemplateEntry 18 }
        
        hwCt2Scheduler  OBJECT-TYPE
         SYNTAX INTEGER {
                            pq(1),
                            wfq(2),
                            lpq(3)
                        }
         MAX-ACCESS  read-create
         STATUS  current
         DESCRIPTION
                "Scheduler name."
        ::= { hwCtFlowTemplateEntry 19 }
   
        hwCt2Valid OBJECT-TYPE
         SYNTAX INTEGER {
                            valid(1),
                            invalid(2)
                        }

        MAX-ACCESS  read-create
        STATUS  current
        DESCRIPTION
                "The state of CT-FLOW templat row."
        ::= { hwCtFlowTemplateEntry 20 }                            
        --CT2参数定义结束                            
        --CT3参数定义
        hwCt3Cos  OBJECT-TYPE
        SYNTAX INTEGER {
                            be(1),
                            af1(2),
                            af2(3),
                            af3(4),
                            af4(5),
                            ef(6),
                            cs6(7),
                            cs7(8)
                        }
         MAX-ACCESS  read-create
         STATUS  current
         DESCRIPTION
                "The Value of class of service must be in 'be,af1,af2,af3,af4,ef,cs6,cs7'."
        ::= { hwCtFlowTemplateEntry 21 }
        
        hwCt3Scheduler  OBJECT-TYPE
         SYNTAX INTEGER {
                            pq(1),
                            wfq(2),
                            lpq(3)
                        }
         MAX-ACCESS  read-create
         STATUS  current
         DESCRIPTION
                "Scheduler name."
        ::= { hwCtFlowTemplateEntry 22 }
   
        hwCt3Valid OBJECT-TYPE
         SYNTAX INTEGER {
                            valid(1),
                            invalid(2)
                        }
        MAX-ACCESS  read-create
        STATUS  current
        DESCRIPTION
                "The state of CT-FLOW templat row."
        ::= { hwCtFlowTemplateEntry 23 }                            
        --CT3参数定义结束 
        --CT4参数定义
        hwCt4Cos  OBJECT-TYPE
        SYNTAX INTEGER {
                            be(1),
                            af1(2),
                            af2(3),
                            af3(4),
                            af4(5),
                            ef(6),
                            cs6(7),
                            cs7(8)
                        }
         MAX-ACCESS  read-create
         STATUS  current
         DESCRIPTION
                "The Value of class of service must be in 'be,af1,af2,af3,af4,ef,cs6,cs7'."
        ::= { hwCtFlowTemplateEntry 24 }
        
        hwCt4Scheduler  OBJECT-TYPE
         SYNTAX INTEGER {
                            pq(1),
                            wfq(2),
                            lpq(3)
                        }
         MAX-ACCESS  read-create
         STATUS  current
         DESCRIPTION
                "Scheduler name."
        ::= { hwCtFlowTemplateEntry 25 }
   
        hwCt4Valid OBJECT-TYPE
        SYNTAX INTEGER {
                            valid(1),
                            invalid(2)
                        }
        MAX-ACCESS  read-create
        STATUS  current
        DESCRIPTION
                "The state of CT-FLOW templat row."
        ::= { hwCtFlowTemplateEntry 26 }                            
        --CT4参数定义结束                  
        --CT5参数定义
        hwCt5Cos  OBJECT-TYPE
        SYNTAX INTEGER {
                            be(1),
                            af1(2),
                            af2(3),
                            af3(4),
                            af4(5),
                            ef(6),
                            cs6(7),
                            cs7(8)
                        }
         MAX-ACCESS  read-create
         STATUS  current
         DESCRIPTION
                "The Value of class of service must be in 'be,af1,af2,af3,af4,ef,cs6,cs7'."
        ::= { hwCtFlowTemplateEntry 27 }
        
        hwCt5Scheduler  OBJECT-TYPE
         SYNTAX INTEGER {
                            pq(1),
                            wfq(2),
                            lpq(3)
                        }
         MAX-ACCESS  read-create
         STATUS  current
         DESCRIPTION
                "Scheduler name."
        ::= { hwCtFlowTemplateEntry 28 }
   
        hwCt5Valid OBJECT-TYPE
        SYNTAX INTEGER {
                            valid(1),
                            invalid(2)
                        }
        MAX-ACCESS  read-create
        STATUS  current
        DESCRIPTION
                "The state of CT-FLOW templat row."
        ::= { hwCtFlowTemplateEntry 29 }                            
        --CT5参数定义结束                
        --CT6参数定义
        hwCt6Cos  OBJECT-TYPE
        SYNTAX INTEGER {
                            be(1),
                            af1(2),
                            af2(3),
                            af3(4),
                            af4(5),
                            ef(6),
                            cs6(7),
                            cs7(8)
                        }
         MAX-ACCESS  read-create
         STATUS  current
         DESCRIPTION
                "The Value of class of service must be in 'be,af1,af2,af3,af4,ef,cs6,cs7'."
        ::= { hwCtFlowTemplateEntry 30 }
        
        hwCt6Scheduler  OBJECT-TYPE
         SYNTAX INTEGER {
                            pq(1),
                            wfq(2),
                            lpq(3)
                        }
         MAX-ACCESS  read-create
         STATUS  current
         DESCRIPTION
                "Scheduler name."
        ::= { hwCtFlowTemplateEntry 31 }
   
        hwCt6Valid OBJECT-TYPE
        SYNTAX INTEGER {
                            valid(1),
                            invalid(2)
                        }
        MAX-ACCESS  read-create
        STATUS  current
        DESCRIPTION
                "The state of CT-FLOW templat row."
        ::= { hwCtFlowTemplateEntry 32 }                            
        --CT6参数定义结束                
        --CT7参数定义
        hwCt7Cos  OBJECT-TYPE
        SYNTAX INTEGER {
                            be(1),
                            af1(2),
                            af2(3),
                            af3(4),
                            af4(5),
                            ef(6),
                            cs6(7),
                            cs7(8)
                        }
         MAX-ACCESS  read-create
         STATUS  current
         DESCRIPTION
                "The Value of class of service must be in 'be,af1,af2,af3,af4,ef,cs6,cs7'."
        ::= { hwCtFlowTemplateEntry 33 }
        
        hwCt7Scheduler  OBJECT-TYPE
         SYNTAX INTEGER {
                            pq(1),
                            wfq(2),
                            lpq(3)
                        }
         MAX-ACCESS  read-create
         STATUS  current
         DESCRIPTION
                "Scheduler name."
        ::= { hwCtFlowTemplateEntry 34 }
   
        hwCt7Valid OBJECT-TYPE
        SYNTAX INTEGER {
                            valid(1),
                            invalid(2)
                       }
        MAX-ACCESS  read-create
        STATUS  current
        DESCRIPTION
                "The state of CT-FLOW templat row."
        ::= { hwCtFlowTemplateEntry 35 }                            
        --CT7参数定义结束                
        
        hwCtFlowTemplateCommit OBJECT-TYPE
        SYNTAX INTEGER {
                            commit(1),
                            nocommit(2)
                       }
        MAX-ACCESS  read-create
        STATUS  current
        DESCRIPTION
                "The state of CT-FLOW templat commit."
        ::= { hwCtFlowTemplateEntry 36 }                            

        hwCtFlowTemplateRowStatus OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS  read-create
        STATUS  current
        DESCRIPTION
                "The state of CT-FLOW templat."
        ::= { hwCtFlowTemplateEntry 51 }     
             
         

        hwDsteInterfaceCfgTable  OBJECT-TYPE 
        SYNTAX SEQUENCE OF  HwDsteInterfaceCfgEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
            "The DS-TE configuration at interface."
        ::= { hwTunnelTeMibObject  10}
        
        hwDsteInterfaceCfgEntry  OBJECT-TYPE
        SYNTAX  HwDsteInterfaceCfgEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
            "The DS-TE configuration at interface."
        INDEX   { hwDsteIfIndex } 
        ::= { hwDsteInterfaceCfgTable  1}      

        HwDsteInterfaceCfgEntry ::=  
        SEQUENCE
        {
            hwDsteIfIndex InterfaceIndex ,
                       
            hwAppliedCtFlowTemplateName  OCTET STRING,
            
            hwCtBandWidthShareCfg INTEGER
        }
         
        hwDsteIfIndex  OBJECT-TYPE
        SYNTAX InterfaceIndex
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
            "A unique value, greater than zero, for eachinterface.  
            It is recommended that values are assigned contiguously starting from 1.
            The value for each interface sub-layer must remain constant at least from one re-initialization of the entity's network management system to the next re-initialization."
        ::= {hwDsteInterfaceCfgEntry 1}

        hwAppliedCtFlowTemplateName OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (1..60))
        MAX-ACCESS  read-create
        STATUS  current
        DESCRIPTION
                "The name of CT-FLOW template."
        ::= { hwDsteInterfaceCfgEntry 11 } 
        
        hwCtBandWidthShareCfg  OBJECT-TYPE
        SYNTAX INTEGER {
                            share(1),
                            unshare(2)
                       }
         MAX-ACCESS  read-create
         STATUS  current
         DESCRIPTION
                "The Value of Ct BandWidth configuration for DS-TE.
                 That must be in 'Share,UnShare'."
        ::= { hwDsteInterfaceCfgEntry 12 }
      
        hwTunnelTeConformance OBJECT IDENTIFIER ::= { hwTunnelTeMib 3 }
        
        hwTunnelTeGroups OBJECT IDENTIFIER ::= { hwTunnelTeConformance 3 }
        
        hwTunnelTeCompliances OBJECT IDENTIFIER ::= {hwTunnelTeConformance 1}
        
            
        hwTunnelDiffServGroup OBJECT-GROUP
            OBJECTS { hwTunnelDiffServMode, hwTunnelDiffServServiceClass,hwTunnelDiffServColor,hwTunnelTeFlowQueue}
            STATUS current
            DESCRIPTION 
                "Describes the different service mode of tunnel."
            ::= { hwTunnelTeGroups 1 }
            
        hwTunnelTeVsiGroup OBJECT-GROUP
            OBJECTS { hwTunnelTeVsiCir, hwTunnelTeVsiPir,hwTunnelTeVsiFlowQueue}
            STATUS current
            DESCRIPTION 
                "Describes the VSI binding of tunnel."
            ::= { hwTunnelTeGroups 2 }  
            
        hwTunnelTeVllGroup OBJECT-GROUP
            OBJECTS { hwTunnelTeVllCir, hwTunnelTeVllPir,hwTunnelTeVllFlowQueue}
            STATUS current
            DESCRIPTION 
                "Describes the VLL binding of tunnel."
            ::= { hwTunnelTeGroups 3 }
            
        hwTunnelTeL3vpnGroup OBJECT-GROUP
            OBJECTS { hwTunnelTeL3vpnCir, hwTunnelTeL3vpnPir,hwTunnelTeL3vpnFlowQueue}
            STATUS current
            DESCRIPTION 
                "Describes the L3VPN binding of tunnel."
            ::= { hwTunnelTeGroups 4 }   
        hwTunnelTeStatisticsGroup OBJECT-GROUP
            OBJECTS { hwTunnelTeUpDownStatistics,hwTunnTeCounterDiscontinuityTime}
            STATUS current
            DESCRIPTION 
                "Describes the up/down count of the TE tunnel."
            ::= { hwTunnelTeGroups 5 }
            
       hwCtTemplateGroup OBJECT-GROUP
            OBJECTS { hwCtTemplateName ,
                      hwCtTemplateCt0 ,
                      hwCtTemplateCt1 , 
                      hwCtTemplateCt2 ,
                      hwCtTemplateCt3 ,
                      hwCtTemplateCt4 ,
                      hwCtTemplateCt5 ,
                      hwCtTemplateCt6 ,
                      hwCtTemplateCt7,
                      hwCtTemplateCommit,
                      hwCtTemplateRowStatus
                      }
            STATUS current
            DESCRIPTION 
                "Describes CT template."
            ::= { hwTunnelTeGroups 6 } 
             
       hwCtConfigCtGroup OBJECT-GROUP
            OBJECTS {
                        hwCtConfigTunnelName ,
                        hwCtConfigTunnelCommit ,
                        hwCtConfigTemplateName ,                       
                        hwCtConfigTunnelCt0Band  ,
                        hwCtConfigTunnelCt1Band  ,
                        hwCtConfigTunnelCt2Band  ,
                        hwCtConfigTunnelCt3Band  ,
                        hwCtConfigTunnelCt4Band  ,
                        hwCtConfigTunnelCt5Band  ,
                        hwCtConfigTunnelCt6Band  ,
                        hwCtConfigTunnelCt7Band}
            STATUS current
            DESCRIPTION 
                "Describes the CT configuration of the TE tunnel interface."
            ::= { hwTunnelTeGroups 7 } 
        
       hwCtStatisticsGroup OBJECT-GROUP
            OBJECTS {
                        hwCtStatisticsTunnelName ,
                        hwCtStatisticsCt0OutByteRate ,
                        hwCtStatisticsCt0OutPktRate           ,  
                    hwCtStatisticsCt0OutPkt               ,  
                    hwCtStatisticsCt0OutPktByte           ,   
                    hwCtStatisticsCt0OutErrorPkt          ,    
                    hwCtStatisticsCt1OutByteRate          ,  
                    hwCtStatisticsCt1OutPktRate           ,  
                    hwCtStatisticsCt1OutPkt               ,  
                    hwCtStatisticsCt1OutPktByte           ,   
                    hwCtStatisticsCt1OutErrorPkt          ,  
                    hwCtStatisticsCt2OutByteRate          ,  
                    hwCtStatisticsCt2OutPktRate           ,  
                    hwCtStatisticsCt2OutPkt               ,  
                    hwCtStatisticsCt2OutPktByte           ,   
                    hwCtStatisticsCt2OutErrorPkt          ,  
                    hwCtStatisticsCt3OutByteRate          ,  
                        hwCtStatisticsCt3OutPktRate           ,                      
                    hwCtStatisticsCt3OutPkt               ,  
                    hwCtStatisticsCt3OutPktByte           ,   
                    hwCtStatisticsCt3OutErrorPkt          ,  
                    hwCtStatisticsCt4OutByteRate          ,  
                         hwCtStatisticsCt4OutPktRate           ,                     
                    hwCtStatisticsCt4OutPkt               ,  
                    hwCtStatisticsCt4OutPktByte           ,   
                    hwCtStatisticsCt4OutErrorPkt          ,  
                    hwCtStatisticsCt5OutByteRate          ,  
                        hwCtStatisticsCt5OutPktRate           ,                      
                    hwCtStatisticsCt5OutPkt               ,  
                    hwCtStatisticsCt5OutPktByte           ,   
                    hwCtStatisticsCt5OutErrorPkt          ,  
                    hwCtStatisticsCt6OutByteRate          ,  
                        hwCtStatisticsCt6OutPktRate           ,                      
                    hwCtStatisticsCt6OutPkt               ,  
                    hwCtStatisticsCt6OutPktByte           ,   
                    hwCtStatisticsCt6OutErrorPkt          ,  
                    hwCtStatisticsCt7OutByteRate          ,  
                        hwCtStatisticsCt7OutPktRate           ,                      
                    hwCtStatisticsCt7OutPkt               ,  
                    hwCtStatisticsCt7OutPktByte           ,   
                    hwCtStatisticsCt7OutErrorPkt  
                    }
                    
            STATUS current
            DESCRIPTION 
                "Describes the CT  of the TE tunnel interface."
            ::= { hwTunnelTeGroups 8 }     
             
            hwCtFlowTemplateGroup OBJECT-GROUP
            OBJECTS {     
                        --hwCtFlowTemplateID ,
                        hwCtFlowTemplateName   , 
                        hwCt0Cos ,
                        hwCt0Scheduler  ,
                        hwCt0Valid  , 
                        hwCt1Cos ,
                        hwCt1Scheduler  ,
                        hwCt1Valid  ,
                        hwCt2Cos ,
                        hwCt2Scheduler  ,
                        hwCt2Valid  ,
                        hwCt3Cos ,
                        hwCt3Scheduler  ,
                        hwCt3Valid  ,
                        hwCt4Cos ,
                        hwCt4Scheduler  ,
                        hwCt4Valid  ,
                        hwCt5Cos ,
                        hwCt5Scheduler  ,
                        hwCt5Valid  ,
                        hwCt6Cos ,
                        hwCt6Scheduler  ,
                        hwCt6Valid  ,
                        hwCt7Cos ,
                        hwCt7Scheduler  ,
                        hwCt7Valid  ,
                        hwCtFlowTemplateCommit ,
                        hwCtFlowTemplateRowStatus       
                    }
            STATUS current
            DESCRIPTION 
                "The table describes the CT-FLOW-Mapping template configuration on the device."
            ::= { hwTunnelTeGroups 10 }     
            
            hwDsteInterfaceCfgGroup OBJECT-GROUP
            OBJECTS {     
                       --hwDsteIfIndex  ,
                       hwAppliedCtFlowTemplateName   ,
                       hwCtBandWidthShareCfg 
                    }
            STATUS current
            DESCRIPTION 
                "The table describes the CT-FLOW-Mapping template configuration on the device."
            ::= { hwTunnelTeGroups 11 }     
  
        
            
         hwTunnelDsTeTrap OBJECT IDENTIFIER ::= { hwTunnelTeMib 2 }                    
    
        
        hwMplsFqShortage NOTIFICATION-TYPE
            OBJECTS { hwCtConfigTunnelName }
            STATUS current
            DESCRIPTION 
                "This notification is generated when FQ (flow-queue) template resources are shortage."
            ::= { hwTunnelDsTeTrap 1 }  
            
        hwMplsSqShortage NOTIFICATION-TYPE
            OBJECTS { hwCtConfigTunnelName }
            STATUS current
            DESCRIPTION 
                "This notification is generated when SQ (subscriber-queue) resources are shortage."
            ::= { hwTunnelDsTeTrap 2 }  
            
        hwMplsSqBandwidthExceed NOTIFICATION-TYPE
            OBJECTS { hwCtConfigTunnelName }
            STATUS current
            DESCRIPTION 
                "This notification is generated when the total bandwidth of SQ (subscriber-queue) exceeds 10G bit/s in one LPU."
            ::= { hwTunnelDsTeTrap 3 }

        hwMplsHsbFqShortage NOTIFICATION-TYPE
            OBJECTS { hwCtConfigTunnelName }
            STATUS current
            DESCRIPTION 
                "This notification is generated when FQ (flow-queue) template resources in HSB are shortage."
            ::= { hwTunnelDsTeTrap 4 }  
            
        hwMplsHsbSqShortage NOTIFICATION-TYPE
            OBJECTS { hwCtConfigTunnelName }
            STATUS current
            DESCRIPTION 
                "This notification is generated when SQ (subscriber-queue) resources in HSB are shortage."
            ::= { hwTunnelDsTeTrap 5 }  
            
        hwMplsHsbSqBandwidthExceed NOTIFICATION-TYPE
            OBJECTS { hwCtConfigTunnelName }
            STATUS current
            DESCRIPTION 
                "This notification is generated when the total bandwidth of SQ (subscriber-queue) in HSB exceeds 10G bit/s in one LPU."
            ::= { hwTunnelDsTeTrap 6 }

        hwTunnelTeTrapGroup NOTIFICATION-GROUP
            NOTIFICATIONS { hwMplsHsbSqBandwidthExceed, hwMplsHsbSqShortage, hwMplsHsbFqShortage, hwMplsSqBandwidthExceed, hwMplsSqShortage, hwMplsFqShortage }
            STATUS  current
            DESCRIPTION
                "The HUAWEI Tunnel Te trap info."
            ::= { hwTunnelTeGroups 9 }



               
    
-- compliance statements
         
         hwTunnelTeCompliance MODULE-COMPLIANCE
            STATUS current
            DESCRIPTION 
                "The compliance statement for HUAWEI-TUNNEL-TE-MIB."
            MODULE -- this module
                MANDATORY-GROUPS { hwTunnelDiffServGroup,
                hwTunnelTeVsiGroup,
                hwTunnelTeVllGroup,
                hwTunnelTeL3vpnGroup,
                hwTunnelTeStatisticsGroup,
                hwCtTemplateGroup,
                hwCtConfigCtGroup,
                hwCtStatisticsGroup,
                hwTunnelTeTrapGroup,
                hwCtFlowTemplateGroup,
                hwDsteInterfaceCfgGroup}
            ::= { hwTunnelTeCompliances 1 }   

                    
    
    END

--
-- HUAWEI-TUNNEL-TE-MIB.mib
--
