CISCOSB-BaudRate-MIB DEFINITIONS ::= BEGIN

-- Title:               CISCOSB LOCALIZATION ROS
--                      This Private MIB supports the baudrate of the local terminal of ROS products
-- Version:             7.39
-- Date:                14 Apr 2005



IMPORTS
    switch001                                    FROM CISCOSB-MIB
    OBJECT-TYPE,
    MODULE-IDENTITY                         FROM SNMPv2-SMI;

rlRs232 MODULE-IDENTITY
         LAST-UPDATED "200504140000Z"
		 ORGANIZATION "Cisco Small Business"

		 CONTACT-INFO
		 "Postal: 170 West Tasman Drive
		 San Jose , CA 95134-1706
		 USA

		 Website: Cisco Small Business Home http://www.cisco.com/smb>;,
		 Cisco Small Business Support Community <http://www.cisco.com/go/smallbizsupport>"

         DESCRIPTION
                "The private MIB module definition for baudrate."
         REVISION "200504140000Z"
         DESCRIPTION
                "Initial revision."
        ::= { switch001 104 }

rlRs232MibVersion OBJECT-TYPE
    SYNTAX  INTEGER
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "MIB's version, the current version is 1."
    ::= { rlRs232 1 }

rlRs232AutoBaudRateStatus OBJECT-TYPE
    SYNTAX  INTEGER {
        enable(1),
        disable(2)
    }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Show the current Auto BaudRate status"
    ::= { rlRs232 2 }

rlRs232AutoBaudRateStatusAfterReset OBJECT-TYPE
    SYNTAX  INTEGER {
        enable(1),
        disable(2)
    }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Show/Set the Auto BaudRate status after reset"
    ::= { rlRs232 3 }

rlRs232BaudRate OBJECT-TYPE
    SYNTAX  INTEGER {
        baud2400(1),
        baud4800(2),
        baud9600(3),
        baud19200(4),
        baud38400(5),
        baud57600(6),
        baud115200(7)
    }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Show/Set the current Baud Rate status"
    ::= { rlRs232 4 }

END

