ALCATEL-IND1-DHCP-SRV-MIB DEFINITIONS ::= BEGIN

        IMPORTS
                Unsigned32, IpAddress,
                MODULE-IDENTITY, OBJECT-TYPE,
                NOTIFICATION-TYPE, OBJECT-IDENTITY
                                        FROM SNMPv2-SMI
                MacAddress, DisplayString, DateAndTime
                                        FROM SNMPv2-TC
                MODULE-COMPLIANCE, OBJECT-GROUP,
                NOTIFICATION-GROUP
                                        FROM SNMPv2-CONF
		InetAddress, InetAddressType
                        		FROM INET-ADDRESS-MIB
                softentIND1DhcpSrv
                                        FROM ALCATEL-IND1-BASE;


                alcatelIND1DhcpSrvMIB MODULE-IDENTITY
                LAST-UPDATED "200812100000Z"
                ORGANIZATION "Alcatel - Architects Of An Internet World"
                CONTACT-INFO
                "Please consult with Customer Service to insure the most appropriate
                version of this document is used with the products in question:

                        Alcatel Internetworking, Incorporated
                        (Division 1, Formerly XYLAN Corporation)
                        26801 West Agoura Road
                        Agoura Hills, CA  91301-5122
                        United States Of America

                        Telephone:      North America  +1 800 995 2696
                                        Latin America  +1 877 919 9526
                                        Europe         +31 23 556 0100
                                        Asia           +65 394 7933
                                        All Other      +1 818 878 4507

                Electronic Mail:         support@ind.alcatel.com
                World Wide Web:          http://www.ind.alcatel.com
                File Transfer Protocol:  ftp://ftp.ind.alcatel.com/pub/products/mibs"

                DESCRIPTION
                        "This module describes an authoritative enterprise-specific Simple
                        Network Management Protocol (SNMP) Management Information Base (MIB):

                        For the Birds Of Prey Product Line
                        DhcpSrv for dynamically assigning IP to clients.

                        The right to make changes in specification and other information
                        contained in this document without prior notice is reserved.

                        No liability shall be assumed for any incidental, indirect, special, or
                        consequential damages whatsoever arising from or related to this
                        document or the information contained herein.

                        Vendors, end-users, and other interested parties are granted
                        non-exclusive license to use this specification in connection with
                        management of the products for which it is intended to be used.

                        Copyright (C) 1995-2002 Alcatel Internetworking, Incorporated
                        ALL RIGHTS RESERVED WORLDWIDE"

                REVISION      "200910260000Z"
                DESCRIPTION
                        "The Dynamic Host Configuration Protocol (DHCP) provides a framework
                        for passing configuration information to hosts on a TCPIP network.
                        DHCP is based on the Bootstrap Protocol (BOOTP), adding the
                        capability of automatic allocation of reusable network addresses and
                        additional configuration options.

                        This MIB provides the configuration information for DHCP Server."
                ::= { softentIND1DhcpSrv 1 }

-- --------------------------------------------------------------
                alcatelIND1DhcpSrvMIBNotifications OBJECT-IDENTITY
                STATUS current
                DESCRIPTION
                        "Branch For DHCP Server Subsystem Notifications."
                ::= { alcatelIND1DhcpSrvMIB 0 }

                alcatelIND1DhcpSrvMIBObjects OBJECT-IDENTITY
                STATUS current
                DESCRIPTION
                        "Branch For DHCP Server Subsystem Managed Objects."
                ::= { alcatelIND1DhcpSrvMIB 1 }

                alcatelIND1DhcpSrvMIBConformance OBJECT-IDENTITY
                STATUS current
                DESCRIPTION
                        "Branch for DhcpSrv Module MIB Subsystem Conformance Information."
                ::= { alcatelIND1DhcpSrvMIB 2 }

                alcatelIND1DhcpSrvMIBGroups OBJECT-IDENTITY
                STATUS current
                DESCRIPTION
                        "Branch for DhcpSrv Module MIB Subsystem Units of Conformance."
                ::= { alcatelIND1DhcpSrvMIBConformance 1 }

                alcatelIND1DhcpSrvMIBCompliances OBJECT-IDENTITY
                STATUS current
                DESCRIPTION
                        "Branch for DhcpSrv Module MIB Subsystem Compliance Statements."
                ::= { alcatelIND1DhcpSrvMIBConformance 2 }

-- --------------------------------------------------------------


alaDhcpSrvGlobalConfigStatus OBJECT-TYPE
        SYNTAX INTEGER
                {
                  enable(1),
                  disable(2)
                }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This object is used to enable(1) or disable(2) DHCP Server on the switch."
	DEFVAL { disable }
::= { alcatelIND1DhcpSrvMIBObjects 1 }

alaDhcpSrvGlobalRestart OBJECT-TYPE
        SYNTAX INTEGER
                {
                  inactive(1),
                  restart(2)
                }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This object is used to restart(2) the DHCP Server on the switch. Default value is
            inactive(1) which user can not set."
        DEFVAL { inactive }
::= { alcatelIND1DhcpSrvMIBObjects 2 }

alaDhcpSrvGlobalClearStat OBJECT-TYPE
        SYNTAX INTEGER
                {
                  default(1),
                  reset(2)
                }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                "Defines the global clear statistics control for DHCP Server.
                default(1) - default value for this object,
                reset(2)   - indicates that all statistic related to DHCP
                             server in the system should get cleared."
        DEFVAL  { default }
::= { alcatelIND1DhcpSrvMIBObjects 3 }

-- --------------------------------------------------------------

alaDhcpSrvLease OBJECT IDENTIFIER ::= { alcatelIND1DhcpSrvMIBObjects 4 }

alaDhcpSrvLeaseTable OBJECT-TYPE
        SYNTAX       SEQUENCE OF AlaDhcpSrvLeaseEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "DHCP server lease table."
::= { alaDhcpSrvLease 1 }

alaDhcpSrvLeaseEntry OBJECT-TYPE
        SYNTAX       AlaDhcpSrvLeaseEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "DHCP server lease entry."
        INDEX { alaDhcpSrvLeaseInetAddressType, alaDhcpSrvLeaseInetAddress }
::= { alaDhcpSrvLeaseTable 1 }

AlaDhcpSrvLeaseEntry ::= SEQUENCE {
		alaDhcpSrvLeaseInetAddressType  InetAddressType,
                alaDhcpSrvLeaseInetAddress      InetAddress,
                alaDhcpSrvLeaseMACAddress       MacAddress,
                alaDhcpSrvLeaseLeaseGrant       DateAndTime,
                alaDhcpSrvLeaseLeaseExpiry      DateAndTime,
                alaDhcpSrvLeaseType             INTEGER
        }

alaDhcpSrvLeaseInetAddressType OBJECT-TYPE
        SYNTAX          InetAddressType
	MAX-ACCESS	not-accessible
	STATUS          current
	DESCRIPTION
	    "Thie object specifies the type of DHCP Server lease address.
	    Currently only InetAddressIPv4(1) is supported."
::= { alaDhcpSrvLeaseEntry 1 }

alaDhcpSrvLeaseInetAddress OBJECT-TYPE
        SYNTAX          InetAddress (SIZE(1 .. 16))
        MAX-ACCESS      not-accessible 
        STATUS          current
        DESCRIPTION
            "This object specifies IP address assigned to the client."
::= { alaDhcpSrvLeaseEntry 2 }

alaDhcpSrvLeaseMACAddress OBJECT-TYPE
        SYNTAX          MacAddress
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
            "MAC address assigned to the client."
::= { alaDhcpSrvLeaseEntry 3 }

alaDhcpSrvLeaseLeaseGrant OBJECT-TYPE
        SYNTAX          DateAndTime
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
            "Lease granted time for the client."
::= { alaDhcpSrvLeaseEntry 4 }

alaDhcpSrvLeaseLeaseExpiry OBJECT-TYPE
        SYNTAX          DateAndTime
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
            "Lease expiry of the client."
::= { alaDhcpSrvLeaseEntry 5 }

alaDhcpSrvLeaseType OBJECT-TYPE
        SYNTAX          INTEGER
                          {
                            unavailable(1),
                            dynamic(2),
                            manual(3)
                          }
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
            "Type of the lease."
::= { alaDhcpSrvLeaseEntry 6 }

-- --------------------------------------------------------------
-- Trap Description
-- --------------------------------------------------------------
alaDhcpSrvTrapsObj OBJECT IDENTIFIER ::= { alcatelIND1DhcpSrvMIBObjects 5 }

-- Notifications

alaDhcpSrvLeaseUtilizationThresholdTrap NOTIFICATION-TYPE
        OBJECTS  {
                    alaDhcpSrvLeaseThresholdStatus,
                    alaDhcpSrvSubnetDescriptor
                 }
        STATUS   current
        DESCRIPTION
                "When the lease utilization in a subnet exceeds or deceeds threshold
                value set by the application, a notification is sent to the Management Entity,
                with the DHCP Server lease utilization information."
        ::= { alcatelIND1DhcpSrvMIBNotifications 1 }

-- Notification Objects

alaDhcpSrvLeaseThresholdStatus OBJECT-TYPE
        SYNTAX  INTEGER
                {
                    crossedBelow80Threshold(1),
                    crossedAbove80Threshold(2),
                    reached100Threshold(3)
                }
        MAX-ACCESS  accessible-for-notify
        STATUS  current
        DESCRIPTION
                "This object specifies the threshold status of subnet utilization."
        ::= { alaDhcpSrvTrapsObj 1 }

alaDhcpSrvSubnetDescriptor OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS  accessible-for-notify
        STATUS  current
        DESCRIPTION
                "This object specifies the subnet Descriptor. If the subnet belongs
                to shared network, this object specifies the shared network name, else
                specifies the Subnet IP."
        ::= { alaDhcpSrvTrapsObj 2 }

-- -------------------------------------------------------------
-- COMPLIANCE
-- -------------------------------------------------------------
alcatelIND1DhcpSrvMIBCompliance MODULE-COMPLIANCE
        STATUS    current
        DESCRIPTION
            "Compliance statement for DHCP Server."
        MODULE
        MANDATORY-GROUPS
        {
                alaDhcpSrvGlobalConfigGroup,
                alaDhcpSrvLeaseGroup,
                alaDhcpSrvNotificationGroup
        }
        ::= { alcatelIND1DhcpSrvMIBCompliances 1 }

-- -------------------------------------------------------------
-- UNITS OF CONFORMANCE
-- -------------------------------------------------------------
alaDhcpSrvGlobalConfigGroup OBJECT-GROUP
        OBJECTS
        {
                alaDhcpSrvGlobalConfigStatus,
                alaDhcpSrvGlobalRestart,
                alaDhcpSrvGlobalClearStat
        }
        STATUS  current
        DESCRIPTION
            "Collection of objects for management of DHCP Server Global Configuration."
        ::= { alcatelIND1DhcpSrvMIBGroups 1 }

alaDhcpSrvLeaseGroup OBJECT-GROUP
        OBJECTS
        {
                alaDhcpSrvLeaseMACAddress,
                alaDhcpSrvLeaseLeaseGrant,
                alaDhcpSrvLeaseLeaseExpiry,
                alaDhcpSrvLeaseType
        }
        STATUS  current
        DESCRIPTION
            "Collection of objects for DHCP Server Lease Configuration."
::= { alcatelIND1DhcpSrvMIBGroups 2 }

alaDhcpSrvNotificationGroup NOTIFICATION-GROUP
        NOTIFICATIONS
        {
                alaDhcpSrvLeaseUtilizationThresholdTrap
        }
        STATUS  current
        DESCRIPTION
            "Collection of objects for DHCP Server Trap information."
::= { alcatelIND1DhcpSrvMIBGroups 3 }

-- -------------------------------------------------------------

END

