-- 
--  $RCSfile: extreme.mib,v $ - ExtremeWare enterprise MIB
-- 
--  Copyright (c) 1997 - 2002 by Extreme Networks Inc.
--  
-- 	  Extreme Networks
--       http://www.extremenetworks.com
-- 
-- 
-- This file contains multiple ASN.1 Module definitions
--


EXTREME-BASE-MIB DEFINITIONS ::= BEGIN

	IMPORTS
		enterprises 		FROM RFC1155-SMI
                OBJECT-TYPE, OBJECT-IDENTITY    FROM SNMPv2-SMI
		TEXTUAL-CONVENTION 	FROM SNMPv2-TC
                MODULE-COMPLIANCE, OBJECT-GROUP       FROM SNMPv2-CONF;


	--  Organization & Product branches
    
        extremenetworks		OBJECT IDENTIFIER ::= { enterprises 1916 }
        extremeV1Traps            OBJECT IDENTIFIER ::= { extremenetworks 0 }
	extremeAgent            OBJECT IDENTIFIER ::= { extremenetworks 1 }
	extremeProduct          OBJECT IDENTIFIER ::= { extremenetworks 2 }
	extremeMisc             OBJECT IDENTIFIER ::= { extremenetworks 3 }
   	extremeV2Traps	        OBJECT IDENTIFIER ::= { extremenetworks 4 } 

    --
    -- Extreme Products
    --    
    summit1			OBJECT IDENTIFIER ::= { extremeProduct 1 }
                        -- 8 x 1Gbps

	summit2			OBJECT IDENTIFIER ::= { extremeProduct 2 }
                        -- 2 x 1Gbps, 16 x 10/100Mbps

	summit3			OBJECT IDENTIFIER ::= { extremeProduct 3 }
                        -- 1 x 1Gbps, 24 x 10/100Mbps

	summit4			OBJECT IDENTIFIER ::= { extremeProduct 4 }
                        -- 6 x 1Gbps, 16 x 10/100Mbps UTP

	summit4fx		OBJECT IDENTIFIER ::= { extremeProduct 5 }
                        -- 6 x 1Gbps, 16 x 10/100Mbps fiber FX

	summit48 		OBJECT IDENTIFIER ::= { extremeProduct 6 }
                        -- 2 x 1Gbps, 48 x 10/100Mbps

	summit24 		OBJECT IDENTIFIER ::= { extremeProduct 7 }
                        -- 1 x 1Gbps, 24 x 10/100Mbps

	blackDiamond6800 	     OBJECT IDENTIFIER ::= { extremeProduct 8 }
                   -- chassis based system with dual msm and 8 switching cards

	blackDiamond6808 	    OBJECT IDENTIFIER ::= { extremeProduct 11 }
                   -- black diamond with the inferno chipset aka MSM64

	summit7iSX 		OBJECT IDENTIFIER ::= { extremeProduct 12 }
                        -- 4 x 1Gbps GBIC, 28 x 1Gbps MT-RJ

	summit7iTX 		OBJECT IDENTIFIER ::= { extremeProduct 13 }
                        -- 4 x 1Gbps GBIC, 28 x 10/100/1000 Base-TX

	summit1iTX 		OBJECT IDENTIFIER ::= { extremeProduct 14 }
                    -- 2 x 1Gbps MT-RJ, 6 x 10/100/1000 Base-TX inferno chipset

	summit5i 		OBJECT IDENTIFIER ::= { extremeProduct 15 }
                        -- 4 x 1Gbps GBIC, 12 x 1Gbps MT-RJ inferno chipset

	summit48i 		OBJECT IDENTIFIER ::= { extremeProduct 16 }
                        -- 2 x 1Gbps GBIC, 48 x 10/100Mbps inferno chipset

	alpine3808 	        OBJECT IDENTIFIER ::= { extremeProduct 17 }
          -- mini chassis based on the inferno chipset with 8 switching cards

	summit1iSX 		OBJECT IDENTIFIER ::= { extremeProduct 19 }
                        -- 2 x 1Gbps GBIC, 6 x 1Gbps MT-RJ inferno chipset

	alpine3804 	        OBJECT IDENTIFIER ::= { extremeProduct 20 }
          -- mini chassis based on the inferno chipset with 4 switching cards

	summit5iLX 		OBJECT IDENTIFIER ::= { extremeProduct 21 }
                    -- 4 x 1Gbps GBIC, 12 x 10/100/1000 Base-TX inferno chipset

	summit5iTX 		OBJECT IDENTIFIER ::= { extremeProduct 22 }
                    -- 4 x 1Gbps GBIC, 12 x 10/100/1000 Base-TX inferno chipset

	enetSwitch24Port	OBJECT IDENTIFIER ::= { extremeProduct 23 }
		    --  24 x 10/100 Mbps  

	blackDiamond6816 	OBJECT IDENTIFIER ::= { extremeProduct 24 }
                    -- black diamond with 4 msm's and 16 switching cards

	summit24e3 		OBJECT IDENTIFIER ::= { extremeProduct 25 }
                    -- 2 x 1Gbps GBIC, 24 x 10/100 Base-TX

	alpine3802 	        OBJECT IDENTIFIER ::= { extremeProduct 26 }
          -- mini chassis based on the inferno chipset with 2-3 switching cards

	blackDiamond6804 	     OBJECT IDENTIFIER ::= { extremeProduct 27 }
                   -- chassis based system with 2 msm's and 4 switching cards

	summit48si		OBJECT IDENTIFIER ::= { extremeProduct 28 }
		    -- 2 x 1Gbps GBIC, 48 x 10/100Mbps, 1u
        	
	summitPx1		OBJECT IDENTIFIER ::= { extremeProduct 30 }
		    --	1 x 1Gbps GBIC

	summit24e2TX	OBJECT IDENTIFIER ::= { extremeProduct 40 }
		    --  2 x 1000Base-T, 24 x 10/100 Base-TX

	summit24e2SX	OBJECT IDENTIFIER ::= { extremeProduct 41 }

		    --  2 x 1Gbps GBIC, 24 x 10/100 Base-TX
        summit200-24    OBJECT IDENTIFIER ::= { extremeProduct 53 }
                    --  2 x 1Gbps GBIC, 24 x 10/100 Base-TX
 
        summit200-48    OBJECT IDENTIFIER ::= { extremeProduct 54 }
                    --  2 x 1Gbps GBIC, 48 x 10/100 Base-TX
 
        summit400-48t   OBJECT IDENTIFIER ::= { extremeProduct 58 }
                    --  4 x 1Gbps fiber/copper, 44 x 1000 Base-T
 
        summit400-24x   OBJECT IDENTIFIER ::= { extremeProduct 59 }
                    --  4 x 1Gbps fiber/copper, 20 x 1Gbps fiber
                    
        summit400-24t   OBJECT IDENTIFIER ::= { extremeProduct 63 }
                    --  4 x 1Gbps fiber/copper, 20 x 1Gbps fiber
                    
        summit400-24p   OBJECT IDENTIFIER ::= { extremeProduct 64 }
                    --  4 x 1Gbps fiber/copper, 20 x 1Gbps fiber
                    
        summit300-24   OBJECT IDENTIFIER ::= { extremeProduct 61 }
                    --  2 x 1Gbps GBIC, 24 x 10/100 Base-TX POE

        summit300-48   OBJECT IDENTIFIER ::= { extremeProduct 55 }
                    --  2 x 1Gbps GBIC, 48 x 10/100 Base-TX POE

	extremeStack   OBJECT IDENTIFIER ::= { extremeProduct 67 }
		    --  stack entity comprising of (1..8) stackables
		    
	summit200-24fx   OBJECT IDENTIFIER ::= { extremeProduct 70 }
                    --  2 x 1Gbps fiber/copper, 24 x 100FX
------------------------------------------------------------------------------

--
-- Assorted OIDs that are pointed to by other MIBs
--
          extremeOids
              OBJECT IDENTIFIER ::= { extremeMisc 1 }

--
-- OIDs for as-yet-unstandardised 802.3 MAU types
--     (see MAU MIB for usage)
--
          extremeMauType
              OBJECT IDENTIFIER ::= { extremeOids 1 }

          extremeMauType1000BaseSX OBJECT IDENTIFIER
              ::= { extremeMauType 1 }
--                      "X fiber over short-wavelength laser PMD as specified
--                        in clause 38, duplex mode unknown"

          extremeMauType1000BaseLX OBJECT IDENTIFIER
              ::= { extremeMauType 2 }
--                      "X fiber over long-wavelength laser PMD as specified
--                        in clause 38, duplex mode unknown"

          extremeMauType1000BaseCX OBJECT IDENTIFIER
              ::= { extremeMauType 3 }
--                      "X copper over 150-ohm balanced cable PMD as specified
--                        in clause 39, duplex mode unknown"

          extremeMauType1000BaseSXFD OBJECT IDENTIFIER
              ::= { extremeMauType 4 }
--                      "X fiber over short-wavelength laser PMD as specified
--                        in clause 38, full-duplex mode"

          extremeMauType1000BaseLXFD OBJECT IDENTIFIER
              ::= { extremeMauType 5 }
--                      "X fiber over long-wavelength laser PMD as specified
--                        in clause 38, full-duplex mode"

          extremeMauType1000BaseCXFD OBJECT IDENTIFIER
              ::= { extremeMauType 6 }
--                      "X copper over 150-ohm balanced cable PMD as specified
--                        in clause 39, full-duplex mode"

          extremeMauType1000BaseWDMHD OBJECT IDENTIFIER
              ::= { extremeMauType 7 }
--                      "Gigabit WDM, half duplex"
          extremeMauType1000BaseWDMFD OBJECT IDENTIFIER
              ::= { extremeMauType 8 }
--                      "Gigabit WDM, full duplex"

          extremeMauType1000BaseLX70HD OBJECT IDENTIFIER
              ::= { extremeMauType 9 }
--                      "Gigabit LX70, half duplex"

          extremeMauType1000BaseLX70FD OBJECT IDENTIFIER
              ::= { extremeMauType 10 }
--                      "Gigabit LX70, full duplex"

          extremeMauType1000BaseZXHD OBJECT IDENTIFIER
              ::= { extremeMauType 11 }
--                      "Gigabit ZX, half duplex"

          extremeMauType1000BaseZXFD OBJECT IDENTIFIER
              ::= { extremeMauType 12 }
--                      "Gigabit ZX, full duplex"

          extremeMauType1000BaseLX100HD OBJECT IDENTIFIER
              ::= { extremeMauType 13 }
--                      "Gigabit LX100, half duplex"

          extremeMauType1000BaseLX100FD OBJECT IDENTIFIER
              ::= { extremeMauType 14 }
--                      "Gigabit LX100, full duplex"

-- ===============================================================================

--
-- Extreme MIB Objects
--
        extremeSystem    OBJECT IDENTIFIER ::= { extremeAgent 1 }
        extremeVlan      OBJECT IDENTIFIER ::= { extremeAgent 2 }
        extremeQos       OBJECT IDENTIFIER ::= { extremeAgent 3 }
        extremePort      OBJECT IDENTIFIER ::= { extremeAgent 4 }
        extremeVC        OBJECT IDENTIFIER ::= { extremeAgent 5 }
        extremeTrapPoll  OBJECT IDENTIFIER ::= { extremeAgent 6 }
        extremeQosPolicy OBJECT IDENTIFIER ::= { extremeAgent 7 }
        extremeDlcs      OBJECT IDENTIFIER ::= { extremeAgent 8 }
        extremeFileTransfer OBJECT IDENTIFIER ::= { extremeAgent 10 }
        extremeRtStats   OBJECT IDENTIFIER ::= { extremeAgent 11 }
        extremeEsrp      OBJECT IDENTIFIER ::= { extremeAgent 12 }
        extremeEdp       OBJECT IDENTIFIER ::= { extremeAgent 13 }
        extremeSlb       OBJECT IDENTIFIER ::= { extremeAgent 14 }
        extremeOspf      OBJECT IDENTIFIER ::= { extremeAgent 15 }
        extremeFdb	     OBJECT IDENTIFIER ::= { extremeAgent 16 }
        extremeStp       OBJECT IDENTIFIER ::= { extremeAgent 17 }
	    extremePOSMib    OBJECT IDENTIFIER ::= { extremeAgent 20 }
	    extremeNPMib     OBJECT IDENTIFIER ::= { extremeAgent 21 }
	    extremeNetFlow     OBJECT IDENTIFIER ::= { extremeAgent 22 }
        extremeSnmpv3      OBJECT IDENTIFIER ::= { extremeAgent 23 }
        extremeCable      OBJECT IDENTIFIER ::= { extremeAgent 24 }
        extremeDosMib      OBJECT IDENTIFIER ::= { extremeAgent 28 }
        extremeEnhDosMib      OBJECT IDENTIFIER ::= { extremeAgent 29 }
        extremeWireless  OBJECT IDENTIFIER ::= { extremeAgent 25 }
	extremeEntity	 OBJECT IDENTIFIER ::= { extremeAgent 31 }
        extremeAP        OBJECT IDENTIFIER ::= { extremeWireless 1 }
        extremeLAC       OBJECT IDENTIFIER ::= { extremeWireless 2 }


PortList ::= TEXTUAL-CONVENTION
       STATUS      current
       DESCRIPTION
           "Each octet within this value specifies a set of eight
           ports, with the first octet specifying ports 1 through
           8, the second octet specifying ports 9 through 16, etc.
           Within each octet, the most significant bit represents
           the lowest numbered port, and the least significant bit
           represents the highest numbered port.  Thus, each port
           of the bridge is represented by a single bit within the
           value of this object.  If that bit has a value of '1'
           then that port is included in the set of ports; the port
           is not included if its bit has a value of '0'. If the
           object has a length of 0 then it is taken to refer to all
           of the ports in a given device."
       SYNTAX      OCTET STRING

L4Port ::= TEXTUAL-CONVENTION
        STATUS  current
        DESCRIPTION
           "The value of a transport layer (layer-4) port number, in network
           byte order. A value of 0 indicates all allowed values of this 
           field i.e. wildcard."
        SYNTAX  INTEGER (0|1..65535)

ExtremeGenAddr ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
            "The value of an address."
    SYNTAX      OCTET STRING (SIZE (0..20))

ExtremeDeviceId ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
            "The switch identifier used by Extreme EDP protocol."
    SYNTAX      OCTET STRING (SIZE (8))

WPACipherSet ::= TEXTUAL-CONVENTION
	STATUS current
	DESCRIPTION
		"A set of supported ciphers which can be advertised
	 	 by WPA stations.  Each set bit indicates support for
		 a given cipher suite.  The special value none is 
		 allowed for representing the absence of information.
		 The value other is used to indicate an unknown cipher."
	SYNTAX BITS {
		none(0),
		wep64(1),
		tkip(2),
		wrap(3),
		ccmp(4),
		wep128(5),
		other(6) }

WPAKeyMgmtSet ::= TEXTUAL-CONVENTION
	STATUS current
	DESCRIPTION
		"A set of supported key management suites.  For more info
		 see IEEE 802.11i D3.0 section 7."
	SYNTAX BITS {
		none(0),
		dot1x(1),
		psk(2)
	}

ClientAuthType ::= TEXTUAL-CONVENTION
STATUS current
DESCRIPTION "Type of client specified in the netlogin traps as well as the client table. For
wired clients, only none, netlogin and dot1x are valid"
SYNTAX INTEGER { none(0),
    open(1),
    wep(2),
    mac-based(3),
    dot1x(4),
    wpa-psk(5),
    web-based (6),
    wpa(7),
    wpa2(8),
    wpa2-psk(9)}

WirelessRemoteConnectBindingType ::= TEXTUAL-CONVENTION
STATUS current
DESCRIPTION "The type of binding to be used when mapping APs to virtual ports"
SYNTAX INTEGER { 
    none(0),
    mac-address(1),
    serial-number(2),
    ip-address(3)}

END


-- ===========================================================================

--
-- Extreme System objects
--

EXTREME-SYSTEM-MIB DEFINITIONS ::= BEGIN

        IMPORTS
                MODULE-IDENTITY FROM SNMPv2-SMI
		OBJECT-TYPE     FROM SNMPv2-SMI
                Unsigned32	FROM SNMPv2-SMI
                TruthValue      FROM SNMPv2-TC
		DisplayString   FROM RFC1213-MIB
                extremeAgent   FROM EXTREME-BASE-MIB
		PortList	FROM EXTREME-BASE-MIB
                IpAddress       FROM SNMPv2-SMI;

        extremeSystem MODULE-IDENTITY
                LAST-UPDATED "0007240000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION "Extreme System objects: objects common to all platforms"
        ::= { extremeAgent 1 }

        extremeSystemCommon OBJECT IDENTIFIER
        ::= { extremeSystem 1 }

--
--  System group
--
--  Objects common to all platforms
--
--  Configuration save objects.  These objects are used by the network
--  management application to save configuration changes into the
--  persistant store.  There are 2 stores on the device; a primary and
--  a secondary.

        extremeSaveConfiguration OBJECT-TYPE
               	SYNTAX INTEGER {
                    	saveToPrimary(1),
                        saveToSecondary(2)
        	}
                MAX-ACCESS read-write
                STATUS current
                DESCRIPTION
            	"When this object is set, the device will copy the contents
		of the configuration database to a buffer and save it to the 
		persistant store specified by the value of the object.  The 
		save is	performed asynchronously, and the snmp agent will
                continue to respond to both gets and sets while the save is
                taking place.  A network management application may use the
		extremeSaveStatus object to determine when the asynchronous
		save operation has completed."
	::= { extremeSystemCommon 3 }

	extremeSaveStatus OBJECT-TYPE
               	SYNTAX INTEGER { saveInProgress(1), saveNotInProgress(2) }
                MAX-ACCESS	read-only
                STATUS current
                DESCRIPTION
           	"This object will return the status of a save operation invoked
		by setting the extremeSaveConfiguration object.  A network
		management application can read this object to determine that a
		save operation has completed."
	::= { extremeSystemCommon 4 }                

        extremeCurrentConfigInUse OBJECT-TYPE
                SYNTAX INTEGER { primary(1), secondary(2) }
        	MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "Shows which NVRAM configuration store was used at last boot"
	::= { extremeSystemCommon 5 }                

        extremeConfigToUseOnReboot OBJECT-TYPE
                SYNTAX INTEGER { primary(1), secondary(2) }
        	MAX-ACCESS read-write
                STATUS current
                DESCRIPTION
        	"Controls which NVRAM configuration store will be used 
                on next reboot."
	::= { extremeSystemCommon 6 }               
 
        extremeOverTemperatureAlarm OBJECT-TYPE
                SYNTAX TruthValue
        	MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "Alarm status of overtemperature sensor in device 
                enclosure."
	::= { extremeSystemCommon 7 }

        extremeCurrentTemperature OBJECT-TYPE
                SYNTAX INTEGER (0..100)
        	MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "Current temperature in degrees celcius measured inside
                device enclosure."
	::= { extremeSystemCommon 8 }

--
-- Table of operational status of all internal Fans
--
        extremeFanStatusTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF ExtremeFanStatusEntry
		MAX-ACCESS  not-accessible
		STATUS current
                DESCRIPTION
                "Table of operational status of all internal cooling fans."
	::= { extremeSystemCommon 9 }

        extremeFanStatusEntry OBJECT-TYPE
		SYNTAX  ExtremeFanStatusEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
                "Entry in table of all internal cooling fans."
		INDEX { extremeFanNumber }
	::= { extremeFanStatusTable 1 }

	ExtremeFanStatusEntry ::=
		SEQUENCE {
			extremeFanNumber
				INTEGER,
			extremeFanOperational
				TruthValue,
		        extremeFanEntPhysicalIndex 
				INTEGER
		}

        extremeFanNumber OBJECT-TYPE
                SYNTAX INTEGER
        	MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "Identifier of cooling fan, numbered from the front and/or 
                left side of device."
	::= { extremeFanStatusEntry 1 }

        extremeFanOperational OBJECT-TYPE
                SYNTAX TruthValue
        	MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "Operational status of a cooling fan."
	::= { extremeFanStatusEntry 2 }

        extremeFanEntPhysicalIndex OBJECT-TYPE
                SYNTAX INTEGER
        	MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "The entity index for this fan entity in the entity table."
	::= { extremeFanStatusEntry 3 }

        extremePrimaryPowerOperational OBJECT-TYPE
                SYNTAX TruthValue
        	MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "Operational status of internal power supply of a device."
	::= { extremeSystemCommon 10 }

        extremeRedundantPowerStatus OBJECT-TYPE
                SYNTAX INTEGER { notPresent(1), presentOK(2), presentNotOK(3) }
        	MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "Operational status of an external redundant power supply to a device."
	::= { extremeSystemCommon 11 }

        extremeRedundantPowerAlarm OBJECT-TYPE
                SYNTAX TruthValue
        	MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "Alarm state of an external redundant power supply to a device. 
                Alarm state indicates either fan failure or overtemperature 
                condition."
	::= { extremeSystemCommon 12 }

        extremePrimarySoftwareRev  OBJECT-TYPE
            SYNTAX DisplayString (SIZE(0..15))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The software revision of the primary image stored in 
                this device.  This string will have a zero length if 
                the revision is unknown, invalid or not present. This
                will also be reported in RMON2 probeSoftwareRev if this
                is the software image currently running in the device."
	::= { extremeSystemCommon 13 }

        extremeSecondarySoftwareRev  OBJECT-TYPE
            SYNTAX DisplayString (SIZE(0..15))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The software revision of the secondary image stored in 
                this device.  This string will have a zero length if 
                the revision is unknown, invalid or not present. This
                will also be reported in RMON2 probeSoftwareRev if this
                is the software image currently running in the device."
	::= { extremeSystemCommon 14 }

        extremeImageToUseOnReboot OBJECT-TYPE
                SYNTAX INTEGER { primary(1), secondary(2) }
        	MAX-ACCESS read-write
                STATUS current
                DESCRIPTION
        	"Controls which image will be used 
                on next reboot."
	::= { extremeSystemCommon 15 }               

        extremeSystemID  OBJECT-TYPE
            SYNTAX DisplayString (SIZE(0..126))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This represents the System ID of the Summit Switch."
	::= { extremeSystemCommon 16 }

        extremeSystemBoardID  OBJECT-TYPE
            SYNTAX DisplayString (SIZE(0..126))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This represents the Board ID of the Summit Switch."
	::= { extremeSystemCommon 17 }

        extremeSystemLeftBoardID  OBJECT-TYPE
            SYNTAX DisplayString (SIZE(0..126))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This represents the Left Board ID of the Summit Switch."
	::= { extremeSystemCommon 18 }

        extremeSystemRightBoardID  OBJECT-TYPE
            SYNTAX DisplayString (SIZE(0..126))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This represents the Right Board ID of the Summit Switch."
	::= { extremeSystemCommon 19 }

	-- Add variables to report power supply data
	extremeInputPowerVoltage OBJECT-TYPE
		SYNTAX  INTEGER {
			v110 (1),
			v220 (2),
			v48DC (3)
		}	
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"The input power voltage at which the system is currently operating."
	::= { extremeSystemCommon 20 }

        extremePowerStatus OBJECT-TYPE
                SYNTAX INTEGER { notPresent(1), presentOK(2), presentNotOK(3) }
        	MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "Operational status of the power supply to a device."
	::= { extremeSystemCommon 21 }

        extremePowerAlarm OBJECT-TYPE
                SYNTAX TruthValue
        	MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "Alarm state of the power supply to a device. 
                Alarm state indicates either fan failure or overtemperature 
                condition."
	::= { extremeSystemCommon 22 }

        extremeRmonEnable OBJECT-TYPE
                SYNTAX TruthValue
        	MAX-ACCESS read-write
                STATUS current
                DESCRIPTION
                      "Setting this to true will cause the agent to 
		       start collecting RMON statistics."
	::= { extremeSystemCommon 23 }

-- OID extremeSystemCommon.24 has been deprecated and extremeCpuTasktable
-- has been moved to extremeSystemCommon.29 with new name extremeCpuTask2table

   extremeBootROMVersion OBJECT-TYPE
		SYNTAX DisplayString (SIZE(0..15))	
        	MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
		  "The software revision of the bootrom on the device. 
                   This string will have a zero length if the revision is 
                   unknown or invalid."
		       
	::= { extremeSystemCommon 25 }

   extremeDot1dTpFdbTableEnable OBJECT-TYPE
		SYNTAX TruthValue
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
		 "Setting this to true will cause GetNext operations on 			  the dot1dTpFdbTable to be allowed. Note that Get operations 			  are always allowed."

	::= { extremeSystemCommon 26 }

        extremePowerSupplyTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF ExtremePowerSupplyEntry
		MAX-ACCESS  not-accessible
		STATUS current
                DESCRIPTION
                "Table of status of all power supplies in the system."
	::= { extremeSystemCommon 27 }

        extremePowerSupplyEntry OBJECT-TYPE
		SYNTAX  ExtremePowerSupplyEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
                "An entry indicating the status of a specific power supply."
		INDEX { extremePowerSupplyNumber }
	::= { extremePowerSupplyTable 1 }

	ExtremePowerSupplyEntry ::=
		SEQUENCE {
			extremePowerSupplyNumber
				INTEGER,
			extremePowerSupplyStatus
				INTEGER,
                        extremePowerSupplyInputVoltage
				INTEGER,
                        extremePowerSupplySerialNumber
                                DisplayString,
		        extremePowerSupplyEntPhysicalIndex 
				INTEGER
		}

        extremePowerSupplyNumber OBJECT-TYPE
                SYNTAX INTEGER
        	MAX-ACCESS accessible-for-notify
                STATUS current
                DESCRIPTION
                	"Power supply number."
	::= { extremePowerSupplyEntry 1 }

        extremePowerSupplyStatus OBJECT-TYPE
                SYNTAX INTEGER { notPresent(1), presentOK(2), presentNotOK(3) }
        	MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                	"Status of the power supply."
	::= { extremePowerSupplyEntry 2 }

	extremePowerSupplyInputVoltage OBJECT-TYPE
		SYNTAX INTEGER { v110 (1), v220 (2), v48DC (3), unknown(4) }
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
			"Input voltage of the power supply"
	::= { extremePowerSupplyEntry 3 }

        extremePowerSupplySerialNumber OBJECT-TYPE
                SYNTAX DisplayString (SIZE(0..126))
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                        " The serial number of the power supply unit."
         ::= { extremePowerSupplyEntry 4 }

        extremePowerSupplyEntPhysicalIndex OBJECT-TYPE
                SYNTAX INTEGER
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                        " The entity index for this psu entity in the entity
                table."
         ::= { extremePowerSupplyEntry 5 }

     extremeCpuAggregateUtilization OBJECT-TYPE
        SYNTAX INTEGER
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                  "The aggregate CPU utilization since
		   the time the start started executing."
	::= { extremeSystemCommon 28 }

--
-- The CPU Task table lists all executing tasks 
--
        extremeCpuTask2Table OBJECT-TYPE
		SYNTAX  SEQUENCE OF ExtremeCpuTask2Entry
		MAX-ACCESS  not-accessible
		STATUS current
                DESCRIPTION
                  "Table of CPU tasks that are active."
	::= { extremeSystemCommon 29 }

        extremeCpuTask2Entry OBJECT-TYPE
		SYNTAX  ExtremeCpuTask2Entry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
                  "An entry in table of describes a single task."
        INDEX { extremeCpuTask2CpuId, extremeCpuTask2Name }
	::= { extremeCpuTask2Table 1 }

	ExtremeCpuTask2Entry ::=
		SEQUENCE {
			extremeCpuTask2CpuId
				Unsigned32,
			extremeCpuTask2Name
				DisplayString,
           	extremeCpuTask2Id
				Unsigned32,
			extremeCpuTask2Pc
				Unsigned32,
			extremeCpuTask2Status
				DisplayString,
			extremeCpuTask2Utilization
				Unsigned32,
			extremeCpuTask2MaxUtilization
				Unsigned32
		}

	  extremeCpuTask2CpuId OBJECT-TYPE
            SYNTAX Unsigned32
        	MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                  "CPU on which this task last executed or is executing.
                   The primary CPU has a value of 1."
	::= { extremeCpuTask2Entry 1 }

        extremeCpuTask2Name OBJECT-TYPE
            SYNTAX DisplayString (SIZE(0..31))
        	MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                  "Name associated with the reported task id."
	::= { extremeCpuTask2Entry 2 }

    
        extremeCpuTask2Id OBJECT-TYPE
                SYNTAX Unsigned32
        	MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                  "Task identifier assigned by the operating system when
                   this task is spawned."
	::= { extremeCpuTask2Entry 3 }

        extremeCpuTask2Pc OBJECT-TYPE
            SYNTAX Unsigned32
        	MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                  "The value of the program counter for this task.
		   It indicates the address of the next instruction
                   that would be executed once the operating system
 		   resumes this task." 
	::= { extremeCpuTask2Entry 4 }

        extremeCpuTask2Status OBJECT-TYPE
            SYNTAX DisplayString
        	MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                  "The current status of the task as reported by the
	  	   operating system."
	::= { extremeCpuTask2Entry 5 }

        extremeCpuTask2Utilization OBJECT-TYPE
            SYNTAX Unsigned32
        	MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                  "The current CPU utilization by this task. This
		   is the utilization when the task last executed."
	::= { extremeCpuTask2Entry 6 }

        extremeCpuTask2MaxUtilization OBJECT-TYPE
            SYNTAX Unsigned32
        	MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                  "The maximum CPU utilization by this task since
		   the time the start started executing. This value
		   may be cleared."
	::= { extremeCpuTask2Entry 7 }

        extremeAuthFailSrcAddr  OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS  accessible-for-notify
            STATUS current
            DESCRIPTION
                "The IP address of the originator of the bad SNMP 
                request that caused the generation of an authentication 
                failure trap."
        ::= { extremeSystemCommon 30 }

        extremeCpuTransmitPriority      OBJECT-TYPE
            SYNTAX INTEGER {
                   normal(1),
                   high(2)
                   }
            MAX-ACCESS                  read-write
            STATUS                      deprecated
            DESCRIPTION
                "The CPU transmit priority."
         ::= { extremeSystemCommon 31 }

        extremeImageBooted OBJECT-TYPE
                SYNTAX INTEGER { primary(1), secondary(2) }
        	  MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
        	"The image with which the switch was last booted, using which it is currently running."
	::= { extremeSystemCommon 32 }               
        
        extremeMsmFailoverCause OBJECT-TYPE
            SYNTAX INTEGER { never(1),
                             admin(2),
                             exception(3), 
                             removal(4),
                             hwFailure(5), 
                             watchdog(6),
                             keepalive(7) 
                           }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
        "The cause of the last MSM failover. never(1) means an
                MSM Failover has not occurred since the last reboot. 
                admin(2) means the failover was initiated by the user. 
                exception(3) means the former master MSM encountered a 
                software exception condition. removal(4) means the master 
                MSM was physically removed from the chassis. hwFailure(5) 
                means a diagnostic failure was detected in the master MSM. 
                watchdog(6) means that the master MSM hardware watchdog 
                timer expired. keepalive(7) means the master MSM failed to 
                respond to slave keepalive requests. The MSM failover will 
                have been hitless only in the admin(2) and exception(3) 
                cases "
        ::= { extremeSystemCommon 33 }


extremeImageTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF ExtremeImageEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		"A table containing information about each software image."
        ::= { extremeSystemCommon 34 }

	extremeImageEntry OBJECT-TYPE
		SYNTAX  ExtremeImageEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		"A table entry containing information about each software image."
		INDEX	  { extremeImageNumber }
			::= { extremeImageTable 1 }

	ExtremeImageEntry ::= SEQUENCE {
		extremeImageNumber 		INTEGER,
                extremeMajorVersion             INTEGER,
                extremeSubMajorVersion          INTEGER,
                extremeMinorVersion             INTEGER,
                extremeBuildNumber              INTEGER,
                extremeTechnologyReleaseNumber  INTEGER,
                extremeSustainingReleaseNumber  INTEGER,
                extremeBranchRevisionNumber     INTEGER,
                extremeImageType                INTEGER,
                extremeImageDescription         DisplayString,
                extremeImageSecurity            INTEGER,
                extremePatchVersion             INTEGER
	}

	extremeImageNumber OBJECT-TYPE
		SYNTAX  INTEGER {
                       cur(0),
                       pri(1),
                       sec(2)
                }
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"A unique integer identifying the particular software
                image."
		::= { extremeImageEntry 1 }

	extremeMajorVersion   OBJECT-TYPE
		SYNTAX  INTEGER
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"The ExtremeWare Release Major Version."
		::= { extremeImageEntry 2 }

        extremeSubMajorVersion   OBJECT-TYPE
		SYNTAX  INTEGER
		MAX-ACCESS  read-only
		STATUS deprecated
		DESCRIPTION
		"The ExtremeWare Release Sub-major Version. This object is
                 deprecated from extremeware 7.3. The extremeMinorVersion
                 gets the value of extremeSubMajorVersion and the new
                 extremePatchVersion gets the value of old extremeMinorVersion
                 value."
		::= { extremeImageEntry 3 }
                
        extremeMinorVersion   OBJECT-TYPE
		SYNTAX  INTEGER
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"The ExtremeWare Release Minor Version."
		::= { extremeImageEntry 4 }
                
        extremeBuildNumber   OBJECT-TYPE
		SYNTAX  INTEGER
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"The ExtremeWare Build Number."
		::= { extremeImageEntry 5 }
                
        extremeTechnologyReleaseNumber   OBJECT-TYPE
		SYNTAX  INTEGER
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"The Technology Release version. This value is zero for
                all but TR releases."
		::= { extremeImageEntry 6 }
                
        extremeSustainingReleaseNumber   OBJECT-TYPE
		SYNTAX  INTEGER
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"The Sustaining Release number for the ExtremeWare version."
		::= { extremeImageEntry 7 }
                
        extremeBranchRevisionNumber   OBJECT-TYPE
		SYNTAX  INTEGER
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"The incremental build on specified branch."
		::= { extremeImageEntry 8 }
                
        extremeImageType   OBJECT-TYPE
		SYNTAX  INTEGER {
                       trunk(0),
                       branch(1),
                       patch(2),
                       technology(3),
                       beta(4)
                      }
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"The branch type from which the image was built."
		::= { extremeImageEntry 9 }
                
        extremeImageDescription   OBJECT-TYPE
		SYNTAX  DisplayString (SIZE(0..13))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
		"A unique string that can be used to identify the specific patch,
                technology, or development branch release."
		::= { extremeImageEntry 10 }
                
        extremeImageSecurity   OBJECT-TYPE
		SYNTAX  INTEGER {
                       unknown(0),
                       nossh(1),
                       ssh(2)
                      }
		MAX-ACCESS  read-only
		STATUS deprecated
		DESCRIPTION
		"Indicates whether image was built with ssh.This object
                 is deprecated, the ssh capability can be obtained from
                 the extremeImageSshCapability of the ImageFeatureTable"
		::= { extremeImageEntry 11 }
               
        extremePatchVersion   OBJECT-TYPE
		SYNTAX  INTEGER
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"The ExtremeWare Release Patch Version."
		::= { extremeImageEntry 12 }
                
extremeImageFeatureTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF ExtremeImageFeatureEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		"A table containing information about the software features."
        ::= { extremeSystemCommon 35 }

	extremeImageFeatureEntry OBJECT-TYPE
		SYNTAX  ExtremeImageFeatureEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		"A table entry containing information about software features."
		INDEX	  { extremeImageFeatureNumber }
			::= { extremeImageFeatureTable 1 }

	ExtremeImageFeatureEntry ::= SEQUENCE {
                extremeImageFeatureNumber 		INTEGER,
                extremeImageSshCapability       INTEGER,
                extremeImageUAACapability       INTEGER
	}

        extremeImageFeatureNumber OBJECT-TYPE
		SYNTAX  INTEGER {
                       cur(0),
                       pri(1),
                       sec(2)
                }
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"A unique integer identifying the particular software
                image."
		::= { extremeImageFeatureEntry 1 }

        extremeImageSshCapability   OBJECT-TYPE
		SYNTAX  INTEGER {
                       unknown(0),
                       nossh(1),
                       ssh(2)
                      }
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"Indicates whether image has ssh capability."
		::= { extremeImageFeatureEntry 2 }

        extremeImageUAACapability   OBJECT-TYPE
		SYNTAX  INTEGER {
                       unknown(0),
                       nouaa(1),
                       uaa(2)
                      }
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"Indicates whether image has Wireless(UAA) components."
		::= { extremeImageFeatureEntry 3 }

---------------------------------------------------------------------------
	-- Objects specific to Chassis products
	extremeChassisGroup OBJECT IDENTIFIER ::=	{ extremeSystem 2}

	extremeMasterMSMSlot OBJECT-TYPE
		SYNTAX  INTEGER
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"The extremeSlotNumber of the master MSM module."
	::= { extremeChassisGroup 1  }
	
	extremeChassisPortsPerSlot OBJECT-TYPE
		SYNTAX  INTEGER
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"The maximum number of ports that can be accomodated
		in a single slot. This number would change to accomodate
		blades with higher port density than current ones."
	::= { extremeChassisGroup 3  }
	
	extremeSlotTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF ExtremeSlotEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		"A table containing information about each slot in the 
		chassis."
			::= { extremeChassisGroup 2 }

	extremeSlotEntry OBJECT-TYPE
		SYNTAX  ExtremeSlotEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		"A table entry containing information about the module in 
		each slot of the chassis."
		INDEX	  { extremeSlotNumber }
			::= { extremeSlotTable 1 }

	ExtremeSlotEntry ::= SEQUENCE {
		extremeSlotNumber 		INTEGER,	
		extremeSlotName			DisplayString,
		extremeSlotModuleConfiguredType	INTEGER,
		extremeSlotModuleInsertedType	INTEGER,
		extremeSlotModuleState		INTEGER,	
		extremeSlotModuleSerialNumber	DisplayString
	}

	extremeSlotNumber OBJECT-TYPE
		SYNTAX  INTEGER
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"A unique integer identifying the particular slot 
		in the chassis."
		::= { extremeSlotEntry 1 }

	extremeSlotName   OBJECT-TYPE
		SYNTAX  DisplayString
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"A name identifying the particular slot in the chassis."
		::= { extremeSlotEntry 2 }

	extremeSlotModuleConfiguredType OBJECT-TYPE
		SYNTAX  INTEGER	{
			none(1),
			fe32(2),
			g4x(3),
			g6x(4),
			fe32fx(5),
			f48ti(7),
			g8xi(8),
			g8ti(9),
			g12sxi(10),
			g12ti(11),
			fm32t(21),
			gm4x(22),
			gm4sx(23),
			gm4t(24),
            wdm8(25),
			fm24f(26),
			fm24sf(27),
			fm24te(28),
			f96ti(29),
	        wdm4(30),
			f32fi(31),
            tenGx3(32),
            tenGigLR(33),
            g16x3(34),
            g24t3(35),
            gm16x3(36),
            gm16t3(37),
            fm16t3(38),
            fm32p(39),
            fm8v(50), -- vdsl blade
            wm4t1(51), -- 4port t1
            wm4t3(52), -- 4port t3
            wm1t3(53), -- 1port t3
            wm4e1(54),  -- 4port e1
			p3c(101),
            p12c(102),
            arm(103),
            mpls(104),
            sma(105),
            p48c(106),
            a3c(107),
            a12c(108),
	        pxm(200),
            s300fixed(201)
		}
		MAX-ACCESS  read-write
		STATUS current
		DESCRIPTION
		"The configured module type for the given slot. 
		At startup, the module-type is none(1). It is 
		possible to configure the module-type even if there 
		is no module in the slot. If the current module in the 
		slot is different than the requested configured module-type, 
		then the current configuration for the module is erased and 
		the card will be restarted. The new configured module-type 
		will be recorded. Since the configured module type is different 
		than the actual module type, a moduleMismatch trap will be sent,
 		and the extremeSlotModuleState for that module will show a 
		mismatch(3). Setting this variable to none(1) will clear the 
		previously assigned module-type of this slot, and all 
		configuration information related to the slot will be erased."
		::= { extremeSlotEntry 3 }

	extremeSlotModuleInsertedType OBJECT-TYPE
		SYNTAX  INTEGER	{
			none(1),
			fe32(2),
			g4x(3),
			g6x(4),
			fe32fx(5),
			msm(6),
			f48ti(7),
			g8xi(8),
			g8ti(9),
			g12sxi(10),
			g12ti(11),
			msm64i(18),
			alpine3808(19),
			alpine3804(20),
			fm32t(21),
			gm4x(22),
			gm4sx(23),
			gm4t(24),
            wdm8(25),
			fm24f(26), 
			fm24sf(27),
			fm24te(28),
			f96ti(29),
	        wdm4(30),
			f32fi(31),
            tenGx3(32),
            tenGigLR(33),   
            g16x3(34),
            g24t3(35),
            gm16x3(36),
            gm16t3(37),
            fm16t3(38),
            fm32p(39),
            fm8v(50), -- vdsl blade
            wm4t1(51), -- 4port t1
            wm4t3(52), -- 4port t3
            wm1t3(53), -- 1port t3
            wm4e1(54),  -- 4port e1
            alpine3802(55),
			p3c(101),
            p12c(102),
            arm(103),
            mpls(104),
            sma(105),
            p48c(106),
            a3c(107),
            a12c(108),
	        pxm(200),
            s300fixed(201),
            msm3(202)
		}
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"The module type inserted into the slot. It is possible 
		to have a slot inserted into the slot even though 
		extremeSlotConfiguredType is none(1)."
		::= { extremeSlotEntry 4 }

	extremeSlotModuleState OBJECT-TYPE
		SYNTAX  INTEGER	{
			notPresent(1),
			testing(2),
			mismatch(3),
			failed(4),
			operational(5),
                        powerdown(6),
			unknown(7),
                        present(8),
                        poweron(9),
                        post(10),
                        downloading(11),
                        booting(12),
                        offline(13),
                        initializing(14),
                        invalid(100) 

		}
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"The state of the module inserted in this slot."
		::= { extremeSlotEntry 5 }

	extremeSlotModuleSerialNumber OBJECT-TYPE
		SYNTAX  DisplayString
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"The serial number of the module inserted in this slot."
		::= { extremeSlotEntry 6 }
	extremeSystemHealthCheck OBJECT IDENTIFIER
		::= { extremeSystem 3 }

	extremeHealthCheckErrorType OBJECT-TYPE
		SYNTAX INTEGER { 
				unknown(1), 
				cpuPacket(2), 
				backplane(3), 
				hardwareFail(4),
				pbusChecksum(5)
				}			
		MAX-ACCESS accessible-for-notify
		STATUS current
		DESCRIPTION
		"The error reported in the system health check trap"
		::= { extremeSystemHealthCheck 1 }

	extremeHealthCheckAction OBJECT-TYPE
		SYNTAX INTEGER {
				syslogOnly(1),
				healthCheckTrap(2),
				ioModuleDown(3),
				systemDown(4),
				autoRecovery(5)
				}
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"The action/alarm level that has been configured for health check."
		::= { extremeSystemHealthCheck 2 }

	extremeHealthCheckMaxRetries OBJECT-TYPE
		SYNTAX INTEGER
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"The maximum number of times a module restart will be attempted if it fails. 
		If extremeHealthCheckAction is not autorecovery(5), then this value is zero."
		::= { extremeSystemHealthCheck 3 }

-- =========================================================================== 
 
  extremeSystemThresholds OBJECT IDENTIFIER
        ::= { extremeSystem  4 }

  extremeCpuUtilRisingThreshold OBJECT-TYPE
        SYNTAX INTEGER (0..100)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
                  "Rising threshold for CPU Aggregation utilization trap"
	::= { extremeSystemThresholds 1 }

  extremeCpuTaskUtilPair OBJECT-TYPE
                SYNTAX DisplayString 
        	    MAX-ACCESS accessible-for-notify
                STATUS current
                DESCRIPTION
                  "TaskName/CPU_% Util pair reported in CPU Utilization trap"
	::= { extremeSystemThresholds 2 }


END



-- =========================================================================

--
-- Extreme VLAN objects
--

EXTREME-VLAN-MIB DEFINITIONS ::= BEGIN

-- =========================================================================
--
--	Interpretation of the Interface Table for VLAN and encapsulation
--	interfaces:
-- 
--	OBJECT	VALUE/USE
--
--	ifIndex	Same interpretation as RFC1573.  A unique value,
--			greater than zero for each VLAN/Encapsulation interface.
--
--	ifDescr	Same interpretation as RFC1573.  A textual string
--			containing information about the interface.  This
--			string should include the name of the manufacturer,
--			the product name, the version of the software, and that
--			the entry is a vlan or encapsulation interface.
--
--			Example: "VLAN Red"
--			Example: "802.1Q Encapsulation Tag 004"
--
--	ifType	propVirtual(53)
--
--	ifMtu		Equivalent to the least common denominator MTU of the
--			set of ports associated with the VLAN or ENCAPS interface.
--			For example, if the VLAN contains one ethernet port, then
--			the value of this object is 1518.  If the VLAN contains
--			all FDDI ports, the value of this object is 4500.  If
--			a vlan contains a mix of ethernet and FDDI ports, the
--			value of this object is 1518.  If there are no ports associated
--			with the interface, then the ifMtu is zero.
--
--	ifSpeed		The value of this object is zero, as defined by RFC1573
--			for sub-layers that have no concept of bandwidth.             
--
--	ifPhysAddress	The value of this object is always equal to a null octet
--			string.
--
--	ifAdminStatus	Always equal to up(1).  SetRequest-PDUs fail.
--
--	ifOperStatus	The value of this object is equal to up(1) if the
--			ifOperStatus of at least one port in in the set of ports
--			stacked below the VLAN layer is up(1).  The value of this 
--			object is down(2) if the ifOperStatus of all ports stacked
--			below the vlan layer is down(2).  The value of this
--			object is down(2) if there are no ports stacked below the
--	   		the vlan sublayer.
--
--	ifLastChange 	Same interpretation as RFC1573.  The value of sysUpTime
--		 	at the time the interface entered its current operational
--			state.  If the current state was entered prior to the 
--			last re-initialization of the local network management
--			subsystem, then this object contains a zero value.
--	 
--	ifInOctets	These objects  return NO_SUCH_NAME on reads and writes. 
--	ifInUcastPkts  	This approach is more desireable than returning zero
--	ifInNUcastPkt	on reads because NMS's cannot differentiate between
--	ifInDiscards	returning a zero for non-support vs returning a real
--	ifInErrors	zero value for the counter.  Inability to distinguish
--	ifInUnknownProtos between these two cases would essentially prevent
--	ifOutOctets	future implementation of these objects, therefore
--	ifOutUcastPkts	NO_SUCH_NAME is returned to indicate no-support.
--	ifOutNUcastPkts	Future implementations may choose to return real values
--	ifOutDiscards	for these counters.
--	ifOutDiscards				"
--	ifOutErrors				"
--	ifLinkUpDownTrapEnable                  "
--	ifConnectorPresent			"
--	ifHighSpeed				"
--	ifName					"
--
--	ifOutQLen	Deprecated in RFC1573.  Set to zero if present.
--	ifSpecific	Deprecated in RFC1573.  Set to {0.0} if present. 
--
--	linkUp TRAP	Not supported for the vlan/encaps sublayers
--	linkDown TRAP	Not supported for the vlan/encaps sublayer
--
-- ======================================================================


	IMPORTS
                MODULE-IDENTITY FROM SNMPv2-SMI
		RowStatus, TruthValue       FROM SNMPv2-TC
		DisplayString   FROM RFC1213-MIB
		OBJECT-TYPE     FROM SNMPv2-SMI
                IpAddress	FROM SNMPv2-SMI
                extremeAgent    FROM EXTREME-BASE-MIB
		PortList	FROM EXTREME-BASE-MIB
		extremeSlotNumber FROM EXTREME-SYSTEM-MIB
                Counter64         FROM SNMPv2-SMI;

        extremeVlan MODULE-IDENTITY
                LAST-UPDATED "0007240000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION "Extreme Virtual LAN objects"
        ::= { extremeAgent 2 }

        --
	-- The objects are arranged into the following groups:
	--
	extremeVlanGroup		OBJECT IDENTIFIER ::= { extremeVlan 1 }
	extremeVirtualGroup	        OBJECT IDENTIFIER ::= { extremeVlan 2 }
	extremeEncapsulationGroup	OBJECT IDENTIFIER ::= { extremeVlan 3 }
        extremeVlanIpGroup		OBJECT IDENTIFIER ::= { extremeVlan 4 }
	extremeProtocolGroup	        OBJECT IDENTIFIER ::= { extremeVlan 5 }
	extremeVlanOpaqueGroup		OBJECT IDENTIFIER ::= { extremeVlan 6 }
	extremeVlanStackGroup		OBJECT IDENTIFIER ::= { extremeVlan 7 }
        extremeVlanStatsGroup           OBJECT IDENTIFIER ::= { extremeVlan 8 }
        extremeVlanAggregationGroup	OBJECT IDENTIFIER ::= { extremeVlan 9 }
   	extremeVlanTranslationGroup 	OBJECT IDENTIFIER ::= { extremeVlan 10 }

	--	
	--
	-- Extreme Networks Vlan Type Textual Convention
	--
	--  vlanLayer2(1) = The globally identified VLAN interface is protocol
	--  independent and based on port grouping.  The configuration of
	--  port grouping is controlled through the ifStackTable.
	--

	ExtremeVlanType ::= INTEGER {
		vlanLayer2(1)
	}

	--
	-- All groups in this MIB are optional.  Support for a 
	-- particular group is dependent upon the capabilities
	-- of the network device.
	--
	-- The VLAN Group
	--
	--	The VLAN mapping group contains objects for
	--	identifying VLANs within a device, and for mapping
	--	these VLANs to a global identifier.  It consists of the
	--	extremeVlanGlobalMappingTable and the extremeVlanIfTable.
	--
	-- The Virtual Group
	--
	--	The virtual group contains the extremeNextVirtIfIndex object.
	--	In the future, other groups and object will be added as
	--	capabilities are added.
	--
	-- The Encapsulation Group
	--
	--	The Encapsulation Group contains objects for identifying
	--	and configuring encapsulation entries within a device.
	--	It consists of the extremeVlanEncapsIfTable.
	--
	-- The Forwarding Database Group
	--
	--	Contains objects for managing MAC-layer FDBs, including
	--	the extremeVlanDot1qStaticTable


	--
	-- The Extreme Networks VLAN Global Mapping Table
	--
	-- This table is implemented by all Extreme Networks network devices  
	-- that support interfaces to globally identified VLANs.
	--

        extremeVlanGlobalMappingTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF ExtremeVlanGlobalMappingEntry
		MAX-ACCESS  not-accessible
		STATUS deprecated
		DESCRIPTION
			"This table lists VLAN interfaces that are globally
			identified.  A single entry exists in this list for
                        each VLAN interface in the system that is bound to
                        a global identifier."
		::= { extremeVlanGroup 1 }

	extremeVlanGlobalMappingEntry OBJECT-TYPE
		SYNTAX  ExtremeVlanGlobalMappingEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
			"An individual VLAN interface global mapping entry.
			Entries in this table are created by setting the
			extremeVlanIfGlobalIdentifier object in the
			extremeVlanIfTable to a non-zero value."
		INDEX { extremeVlanGlobalMappingIdentifier }
		::= { extremeVlanGlobalMappingTable 1 }

	ExtremeVlanGlobalMappingEntry ::=
		SEQUENCE {
			extremeVlanGlobalMappingIdentifier
				INTEGER (0..65535),
			extremeVlanGlobalMappingIfIndex
				INTEGER
		}

        extremeVlanGlobalMappingIdentifier OBJECT-TYPE
                SYNTAX  INTEGER (0..65535)
                MAX-ACCESS	read-only
                STATUS current
                DESCRIPTION
            	  "An index into the extremeVlanGlobalMappingTable and an
		  administratively assigned global VLAN identifier.  The
		  value of this object globally identifies the VLAN interface.
		  For VLAN interfaces, on different network devices, which are
		  part of the same globally identified VLAN, the value of this
		  object will be the same."
        ::= { extremeVlanGlobalMappingEntry 1 }

	extremeVlanGlobalMappingIfIndex OBJECT-TYPE
		SYNTAX  INTEGER
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		 "The value of extremeVlanIfIndex for the VLAN interface in the
		 extremeVlanIfTable, which is bound to the global identifier
		 specified by this entry."
		::= { extremeVlanGlobalMappingEntry 2 }

	--
	-- The Extreme Networks VLAN Interface Table
	--
	-- This table is implemented by all Extreme Networks network devices  
	-- that support VLAN interfaces.
	--

        extremeVlanIfTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF ExtremeVlanIfEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
			"This table lists VLAN interfaces that exist within
			a device.  A single entry exists in this list for each
			VLAN interface in the system.  A VLAN interface may
			be created, destroyed and/or mapped to a globally 
			identified vlan."
		::= { extremeVlanGroup 2 }

	extremeVlanIfEntry OBJECT-TYPE
		SYNTAX  ExtremeVlanIfEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		    "An individual VLAN interface entry.  When an NMS wishes
		    to create a new entry in this table, it must obtain a 
		    non-zero index from the extremeNextAvailableVirtIfIndex
		    object.  Row creation in this table will fail if the
		    chosen index value does not match the current value 
		    returned from the extremeNextAvailableVirtIfIndex object."
		INDEX { extremeVlanIfIndex }
		::= { extremeVlanIfTable 1 }

        ExtremeVlanIfEntry ::=
		SEQUENCE {
			extremeVlanIfIndex
				INTEGER,
			extremeVlanIfDescr
				DisplayString,
			extremeVlanIfType
				ExtremeVlanType,
			extremeVlanIfGlobalIdentifier
				INTEGER,
			extremeVlanIfStatus
				RowStatus,
			extremeVlanIfIgnoreStpFlag
				TruthValue,
			extremeVlanIfIgnoreBpduFlag
				TruthValue,
                        extremeVlanIfLoopbackModeFlag
                                TruthValue,
                        extremeVlanIfVlanId
                                INTEGER
		}

        extremeVlanIfIndex OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS 	read-create
                STATUS current
                DESCRIPTION
            	  "The index value of this row and the vlan's ifIndex in the
	     	  ifTable. The NMS obtains the index value for this row by
		  reading the extremeNextAvailableVirtIfIndex object."
        ::= { extremeVlanIfEntry 1 }

        extremeVlanIfDescr OBJECT-TYPE
		SYNTAX	DisplayString (SIZE(0..32))
		MAX-ACCESS	read-create
		STATUS	current
		DESCRIPTION
			"This is a description of the VLAN interface."
	::= {extremeVlanIfEntry 2}

        extremeVlanIfType OBJECT-TYPE
                SYNTAX 	ExtremeVlanType
                MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
			"The VLAN interface type."
        ::= { extremeVlanIfEntry 3 }

        extremeVlanIfGlobalIdentifier OBJECT-TYPE
                SYNTAX  INTEGER (0..65535)
                MAX-ACCESS	read-create 
                STATUS deprecated
                DESCRIPTION
		"An administratively assigned global VLAN identifier.  For
		VLAN interfaces, on different network devices, which are
		part of the same globally identified VLAN, the value of this
		object will be the same.  

		The binding between a global identifier and a VLAN 
		interface can be created or removed.  To create a binding
		an NMS must write a non-zero value to this object.  To
		delete a binding, the NMS must write a zero to this
		object. The value 1 is reserved for the default VLAN and
		this cannot be deleted or re-assigned."
	::= { extremeVlanIfEntry 4 }

        extremeVlanIfStatus OBJECT-TYPE
                SYNTAX  RowStatus
                MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
                    "The status column for this VLAN interface. 
        	    This OBJECT can be set to:

            		active(1)
			createAndGo(4)
            		createAndWait(5)
            		destroy(6)

                    The following values may be read:
            		active(1)
			notInService(2)
           		notReady(3).
			
		    Setting this object to createAndGo(4) causes the agent
		    to attempt to create and commit the row based on 
		    the contents of the objects in the row.  If all necessary
		    information is present in the row and the values are
		    acceptible to the agent, the agent will change the 
		    status to active(1).  If any of the necessary objects  
		    are not available, the agent will reject the creation
		    request.	

		    Setting this object to createAndWait(5) causes a row
		    in this table to be created.  The agent sets the
		    status to notInService(2) if all of the information is
		    present in the row and the values are acceptable to the
		    agent; otherwise, the agent sets the status to notReady(3).

		    Setting this object to active(1) is only valid when
		    the current status is active(1) or notInService(2).  

		    When the state of the row transitions is set to active(1),
		    the agent creates the corresponding row in the ifTable.

		    Setting this object to destroy(6) will remove the
                    corresponding VLAN interface, remove the entry in this
                    table, and the corresponding entries in the
                    extremeVlanGlobalMappingTable and the ifTable.

		    In order for a set of this object to destroy(6) to succeed,
		    all dependencies on this row must have been removed. These
		    will include any stacking dependencies in the ifStackTable
                    and any protocol specific tables dependencies."
        ::= { extremeVlanIfEntry 6 }

        extremeVlanIfIgnoreStpFlag OBJECT-TYPE
     		SYNTAX		TruthValue
                MAX-ACCESS	read-write
                STATUS		current
                DESCRIPTION
            	"Enable/disable STP for this VLAN interface. Setting this
			object to true will cause the ports on this VLAN to ignore
			STP BPDUs. When a vlan is first created, the Default value 
			is FALSE, which means that the VLAN uses STP port information"
        ::= { extremeVlanIfEntry 7 }

	extremeVlanIfIgnoreBpduFlag OBJECT-TYPE
     		SYNTAX		TruthValue
                MAX-ACCESS	read-write
                STATUS		current
                DESCRIPTION
            	"Setting this object to true causes this VLAN's BPDU's to be ignored by 
		the Spanning Tree process. This can be used to keep the root bridge within 
		one's own network when external switches also fall within the same Spanning 
		Tree Domain. When a vlan is first created, the Default value is FALSE."
        ::= { extremeVlanIfEntry 8 }

	extremeVlanIfLoopbackModeFlag OBJECT-TYPE
     		SYNTAX		TruthValue
                MAX-ACCESS	read-write
                STATUS		current
                DESCRIPTION
            	"Setting this object to true causes loopback mode to be enabled on this VLAN."
        ::= { extremeVlanIfEntry 9 }

        extremeVlanIfVlanId OBJECT-TYPE
                SYNTAX          INTEGER
                MAX-ACCESS      read-only
                STATUS current
                DESCRIPTION
                    "The VLAN ID of this VLAN."
        ::= { extremeVlanIfEntry 10 }

        --
	-- The Extreme Networks VLAN Encapsulation Interface Table
	--
	-- VLAN Encapsulation refers to the ability to multiplex
	-- several VLANs over a single network segment by explicitly
	-- labeling eack packet with a tag that identifies the packet's
	-- VLAN membership.
	--
	-- The only tagging scheme supported by this MIB is IEEE 802.1Q
        -- Some ports support tagging, some don't.  For ports that support 
        -- tagging, they may have some VLANs that operate in tagging mode, 
        -- some not in tagging mode.
	--
	-- The encapsulation interface will be creatable by the NMS using
	-- the extremeVlanIfTable.  This table will allow the NMS to define 
	-- certain attributes of the encapsulation including an encapsulation 
	-- algorithm and a tag value.  Using the ifStack table, an encapsulation
	-- interface may be stacked underneath a VLAN interface and on top of port(s).
	-- 
	-- Example ifTable Stacking:
	--
	--		+=======================+=======================+
	--		|     VLAN Xface 9      |       VLAN Xface 11   |
	--		+=======================+=======================+
	--		+=======================+
	--		|      ENCAPS Xface 10  |
	--		+=======================+
	--		+=====+=====+=====+=====+=====+=====+=====+=====+
	--		|  1  |  2  |  3  |  4  |  5  |  6  |  7  |  8  |<=== Ports
	--		+=====+=====+=====+=====+=====+=====+=====+=====+
	--
	-- ifStackTable Instances:
	--		ifStackHigher	ifStackLower
	--                   0               9
	--                   0               11
	--                   1               0
	--                   2               0
	--                   3               0
	--                   4               0
	--                   9               10
	--                  10               1
	--                  10               2
	--                  10               3
	--                  10               4
	--                  11               5
	--                  11               6
	--                  11               7
	--                  11               8
	--
	-- A stack that contains a VLAN, encapsulation and a port interface,
        -- specifies:
	--
	--  For packets received through the given port that use the given
        --   encapsulation scheme and contain the given tag, those packets
        --   are members of the given VLAN.
	--
	--  For unencapsulated packets from the given VLAN that are to be
        --   transmitted out the given port, those packets must first be
        --   encapsulated using the given encapsulation algorithm and tag.
	-- 
	-- This table is implemented by all Extreme Networks network devices  
	-- that support the encapsulation of multiple VLANs over a single
	-- interface.

	ExtremeVlanEncapsType ::= INTEGER { 
		vlanEncaps8021q(1)
	}


	extremeVlanEncapsIfTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF ExtremeVlanEncapsIfEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
			"This table lists VLAN encapsulation interfaces that
			exist within a device.  A single entry exists in this
			list for each VLAN encapsulation interface in the
			system.  A VLAN encapsulation interface may be created
			or destroyed."
		::= { extremeEncapsulationGroup 1 }

	extremeVlanEncapsIfEntry OBJECT-TYPE
		SYNTAX  ExtremeVlanEncapsIfEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
			"An individual VLAN encapsulation interface entry. 
			When an NMS wishes to create a new entry in this table,
			it must obtain a non-zero index from the
			extremeNextAvailableVirtIfIndex object.  Row creation
			in this table will fail if the chosen index value does
			not match the current value returned from the
			extremeNextAvailableVirtIfIndex object."
		INDEX { extremeVlanEncapsIfIndex }
		::= { extremeVlanEncapsIfTable 1 }

	ExtremeVlanEncapsIfEntry ::=
		SEQUENCE {
			extremeVlanEncapsIfIndex
				INTEGER,
			extremeVlanEncapsIfType
				ExtremeVlanEncapsType,
			extremeVlanEncapsIfTag
				INTEGER,
			extremeVlanEncapsIfStatus
				RowStatus
		}

	extremeVlanEncapsIfIndex OBJECT-TYPE
		SYNTAX  INTEGER
		MAX-ACCESS 	read-create
		STATUS current
		DESCRIPTION
			"The index value of this row and the encapsulation
			interface's ifIndex in the ifTable.  The NMS obtains
			the index value used for creating a row in this table
			by reading the extremeNextAvailableVirtIfIndex object."
        ::= { extremeVlanEncapsIfEntry 1 }

	extremeVlanEncapsIfType OBJECT-TYPE
		SYNTAX	ExtremeVlanEncapsType
		MAX-ACCESS	read-create
		STATUS	current
		DESCRIPTION
			"The encapsulation algorithm used when encapsulating
			packets transmitted, or de-encapsulating packets
			received through this interface."
	::= {extremeVlanEncapsIfEntry 2}

	extremeVlanEncapsIfTag OBJECT-TYPE
		SYNTAX 	INTEGER
		MAX-ACCESS  read-create
		STATUS current
		DESCRIPTION
			"The tag used when encapsulating packets transmitted,
			or de-encapsulating packets received through this
			interface."
        ::= { extremeVlanEncapsIfEntry 3 }

	extremeVlanEncapsIfStatus OBJECT-TYPE
		SYNTAX  RowStatus
		MAX-ACCESS  read-create
		STATUS current
		DESCRIPTION
			"The row status for this VLAN encapsulation interface. 

			 This OBJECT can be set to:

				active(1)
				createAndGo(4)
				createAndWait(5)
				destroy(6)

			The following values may be read:
				active(1)
				notReady(3).
			
			In order for a row to become active, the NMS must set
			extremeVlanEncapsIfTagType and extremeVlanEncapsIfTag
			to some valid and consistent values.  

			Setting this object to createAndGo(4) causes the agent
			to attempt to create and commit the row based on the
			contents of the objects in the row. If all necessary
			information is present in the row, the agent will
			create the row and change the status to active(1).  If
			any of the necessary objects are not available, or
			specify an invalid configuration, the row will not be
			created and the agent will return an appropriate error.

			Setting this object to createAndWait(5) causes a row in
			in this table to be created.  If all necessary objects
			in the row have been assigned values and specify a
			valid configuration, the status of the row will be set
			to notInService(2); otherwise, the status will be set
			to notReady(3).  

			This object may only be set to createAndGo(4) or
			createAndWait(5) if it does not exist.

			Setting this object to active(1) when the status is
			notInService(2) causes the agent to commit the
			row.  Setting this object to active(1) when its value
			is already active(1) is a no-op.

			Setting this object to destroy(6) will remove the
			corresponding VLAN encapsulation interface, remove the
			entry in this table, and remove the corresponding entry
			in the ifTable.

			In order for a set of this object to destroy(6) to
			succeed, all dependencies on this row must have been
			removed.  These will include any references to this
			interface in the ifStackTable."
        ::= { extremeVlanEncapsIfEntry 4 }

	--
	-- The extremeNextAvailableVirtIfIndex
	--

	extremeNextAvailableVirtIfIndex OBJECT-TYPE
		SYNTAX	INTEGER
		MAX-ACCESS	read-only
		STATUS	current
		DESCRIPTION
			"The value of the next available virtual ifIndex.  This
			 object is used by an NMS to select an index value 
			 for row-creation in tables indexed by ifIndex.  The 
			 current value of this object is changed to a new
			 value when the current value is written to an agent's
			 table, that is indexed by ifIndex.  Row creation
			 using the current value of this object, allocates
			 a virtual ifIndex.  Note the following:
			
			 1. A newly created row does not have to be active(1)
			    for the agent to allocate the virtual ifIndex.

			 2. Race conditions between multiple NMS's end when
			    a row is created.  Rows are deemed created when
			    a setRequest is successfully committed (i.e.
			    the errorStats is noError(0)).

			3.  An agent that exhausts its supply of virual
			    ifIndex values returns zero as the value of this
			    object. This can be used by an NMS as an indication
			    to deleted unused rows and reboot the device."
		::= { extremeVirtualGroup 1 }		 


	--
    	--  The IP VLAN Interface Information Table
	--
	--	The IP VLAN Interface Information table is supported by 
	--	network devices that support IP VLAN interfaces. 
	--
	--	A row must be created in this table for each IP
	--	VLAN interface. The index used is the
	--	same index as that used to create the IP VLAN interface
	--	in the extremeVlanIfTable. 
	--	

	extremeVlanIpTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF ExtremeVlanIpEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
			"A list of IP VLAN interface information
			entries.  Entries in this table are related
			to entries in the extremeVlanIfTable by using the
			same index."
		::= { extremeVlanIpGroup 1 }

	extremeVlanIpEntry OBJECT-TYPE
		SYNTAX  ExtremeVlanIpEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
			"A extremeVlanIpEntry contains layer 3
			information about a particular IP VLAN
			interface."
		INDEX	{ extremeVlanIfIndex }
		::= { extremeVlanIpTable 1 }

	ExtremeVlanIpEntry ::=
		SEQUENCE {
			extremeVlanIpNetAddress
				IpAddress,
			extremeVlanIpNetMask
				IpAddress,
			extremeVlanIpStatus
				RowStatus,	
			extremeVlanIpForwardingState
                                TruthValue
		}

	extremeVlanIpNetAddress OBJECT-TYPE
		SYNTAX  IpAddress 
		MAX-ACCESS  read-create
		STATUS current
		DESCRIPTION
		    "The IP network number for the IP VLAN interface defined
		    in the extremeVlanIfTable identified with the same index."
		::= { extremeVlanIpEntry 1 }

	extremeVlanIpNetMask OBJECT-TYPE
		SYNTAX  IpAddress 
		MAX-ACCESS  read-create
		STATUS current
		DESCRIPTION
			"The IP network mask corresponding to the IP Network
			address defined by extremeVlanIpIpNetAddress.  "
		::= { extremeVlanIpEntry 2 }

	extremeVlanIpStatus OBJECT-TYPE
		SYNTAX  RowStatus
		MAX-ACCESS  read-create
		STATUS current
		DESCRIPTION
		"The status column for this IP VLAN entry.
		This object can be set to:
            		active(1)
			createAndGo(4)
            		destroy(6)

            	The following values may be read:
            		active(1)

		Setting this object to active(1) or createAndGo(4) causes 
                the agent to attempt to create and commit the row based on 
		the contents of the objects in the row.  If all necessary
		information is present in the row and the values are
		acceptible to the agent, the agent will change the 
		status to active(1).  If any of the necessary objects  
		are not available, the agent will reject the row 
		creation request.

		Setting this object to createAndWait(5) is not supported.

		When the status changes to active(1), the agent applies the
		IP parmeters to the IP VLAN interface identified by the
		corresponding value of the extremeVlanIpIndex object.

		Setting this object to destroy(6) will remove the IP
		parmeters from the IP VLAN interface and remove the
		entry from this table."
		::= { extremeVlanIpEntry 3 }

	extremeVlanIpForwardingState OBJECT-TYPE
		SYNTAX  TruthValue 
		MAX-ACCESS  read-create
		STATUS current
		DESCRIPTION
			"Indicates whether the IP Forwarding  on this Vlan is
                         Enable or not. A true value indicates that the Vlan is
                         Enable."
		::= { extremeVlanIpEntry 4 }

-- 
-- Protocol Definition Table
--
-- we choose to define our own table as existing tables are 
-- overcomplex (RMON Protocol MIB, etc.)
--
	extremeVlanProtocolTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF ExtremeVlanProtocolEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
                       "Table of defined combinations of protocol IDs 
                        that make up one protocol definition name. 
                        All members of one protocol definition share 
                        the same extremeVlanProtocolIndex. A given 
                        protocol ID may appear in the definition of 
                        just one protocol definition. This table will
                        typically contain some default entries for
                        popular protocols chosen by ExtremeWare."
	::= { extremeProtocolGroup 1 }

	extremeVlanProtocolEntry OBJECT-TYPE
		SYNTAX  ExtremeVlanProtocolEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
                       "One member protocol ID of a protocol definition."
        	INDEX { extremeVlanProtocolIndex, 
                        extremeVlanProtocolIdIndex }

	::= { extremeVlanProtocolTable 1 }

	ExtremeVlanProtocolEntry ::= SEQUENCE {
                extremeVlanProtocolIndex INTEGER,
                extremeVlanProtocolIdIndex INTEGER,
                extremeVlanProtocolName DisplayString,
                extremeVlanProtocolDllEncapsType INTEGER,
                extremeVlanProtocolId INTEGER,
                extremeVlanProtocolStatus RowStatus
        }
        extremeVlanProtocolIndex OBJECT-TYPE
                SYNTAX INTEGER (0..7)
                MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
                      "An index representing a protocol grouping of
                        protocol ID values. A limited number of
                        protocol groupings may be defined (up to 7 
                        in ExtremeWare)."
	::= { extremeVlanProtocolEntry 1 }

        extremeVlanProtocolIdIndex OBJECT-TYPE
                SYNTAX INTEGER (0..6)
                MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
                      "An index representing a particular protocol ID
                        within a protocol grouping. A limited number of
                        protocol IDs may be defined per 
                        extremeVlanProtocolIndex (up to 6 in ExtremeWare)."
	::= { extremeVlanProtocolEntry 2 }

      	extremeVlanProtocolName OBJECT-TYPE
                SYNTAX  DisplayString (SIZE(0..31))
                MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
                      "A human-readable string representing this protocol.
                        This string should be the same for all entries
                        sharing a given extremeVlanProtocolIndex. 
                        A ExtremeVlanProtocolEntry with 
                        extremeVlanProtocolName of ANY represents a match 
                        on all protocols: this entry may not be modified."
	::= { extremeVlanProtocolEntry 3 }

        extremeVlanProtocolDllEncapsType OBJECT-TYPE 
                SYNTAX  INTEGER { any(1), ethertype(2), 
                                  llc(3), llcSnapEthertype(4), none(5) }
                MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
                      "Represents the type of data-link encapsulation 
                        in which the extremeVlanProtocolId protocol ID 
                        is carried. The value any(1) is used to indicate 
                        a wildcard and matches all encapsulations and 
                        protocol IDs that are not explicitly mentioned 
                        in this table. Entries of type any(1) may not 
                        be created. The value none(5) is used to indicate 
                        that no protocol IDs match this entry. A value
                        of none(5) may not be set by a manager."
	::= { extremeVlanProtocolEntry 4 }

        extremeVlanProtocolId OBJECT-TYPE
                SYNTAX  INTEGER (0..65535)
                MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
                      "The protocol ID: for entries of type ethertype(2)
                        or llcSnapEthertype(4) this represents a 16-bit
                        protocol ID. For entries of type llc(3) it 
                        represents a concatenation of LLC DSAP+SSAP in
                        network byte order. This value is not valid
                        for extremeVlanProtocolDllEncapsType values of
                        any(1) or none(5)."
	::= { extremeVlanProtocolEntry 5 }

        extremeVlanProtocolStatus OBJECT-TYPE
                SYNTAX RowStatus
                MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
                        "The row status variable, used according to
                        row installation and removal conventions."
	::= { extremeVlanProtocolEntry 6 }


--
-- Protocol-based VLAN Table
--
	extremeVlanProtocolVlanTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF ExtremeVlanProtocolVlanEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
                       "Table to apply one of the protocol definitions 
                        in extremeVlanProtocolTable to a given VLAN 
                        This applies to all ports that are untagged 
                        in this VLAN). A limited number of protocols
                        may be applied simultaneously in one device
                        (up to 8 in ExtremeWare)."
	::= { extremeProtocolGroup 2 }

	extremeVlanProtocolVlanEntry OBJECT-TYPE
		SYNTAX  ExtremeVlanProtocolVlanEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
                       "A mapping of untagged packets of one protocol 
                        onto a particular VLAN."
        	INDEX { extremeVlanProtocolVlanIfIndex, 
                        extremeVlanProtocolVlanProtocolIndex }
	::= { extremeVlanProtocolVlanTable 1 }

	ExtremeVlanProtocolVlanEntry ::= SEQUENCE {
		extremeVlanProtocolVlanIfIndex INTEGER,
		extremeVlanProtocolVlanProtocolIndex INTEGER,
                extremeVlanProtocolVlanStatus RowStatus
        }

        extremeVlanProtocolVlanIfIndex OBJECT-TYPE
                SYNTAX INTEGER
                MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
            	    "The index value of this row and the vlan's ifIndex in the
	     	    ifTable. The NMS obtains the index value for this row by
		    reading the extremeNextAvailableVirtIfIndex object."
	::= { extremeVlanProtocolVlanEntry 1 }

        extremeVlanProtocolVlanProtocolIndex OBJECT-TYPE
                SYNTAX INTEGER
                MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
                      "An index representing a protocol grouping of
                        protocol ID values. A limited number of
                        protocol groupings may be defined (up to 7 
                        in ExtremeWare)."
	::= { extremeVlanProtocolVlanEntry 2 }


        extremeVlanProtocolVlanStatus OBJECT-TYPE
                SYNTAX RowStatus
                MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
                        "The row status variable, used according to
                        row installation and removal conventions."
	::= { extremeVlanProtocolVlanEntry 3 }

	--
	-- The Extreme Networks VLAN Opaque Table
	--
	-- This table is implemented by all Extreme Networks network devices  
	-- that support VLAN interfaces.
	--

        extremeVlanOpaqueTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF ExtremeVlanOpaqueEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
			"This table lists the ports associated with each VLAN interface."
		::= { extremeVlanOpaqueGroup 1 }

	extremeVlanOpaqueEntry OBJECT-TYPE
		SYNTAX  ExtremeVlanOpaqueEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		    "This represents the tagged and untagged ports on each slot per vlan."
		INDEX { extremeVlanIfIndex, extremeSlotNumber }
		::= { extremeVlanOpaqueTable 1 }

        ExtremeVlanOpaqueEntry ::=
		SEQUENCE {
			extremeVlanOpaqueTaggedPorts
				PortList,
			extremeVlanOpaqueUntaggedPorts
				PortList
		}


        extremeVlanOpaqueTaggedPorts OBJECT-TYPE
		SYNTAX	PortList
		MAX-ACCESS	read-only
		STATUS	current
		DESCRIPTION
			"Each bit in the octet string represents one port.
 			A 1 means that the port is a tagged port in that vlan. 
			The bit value for a port is 0 otherwise."
		::= { extremeVlanOpaqueEntry 1}

        extremeVlanOpaqueUntaggedPorts OBJECT-TYPE
                SYNTAX PortList
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
			"Each bit in the octet string represents one port.
 			A 1 means that the port is an untagged port in that vlan. 
			The bit value for a port is 0 otherwise."
	        ::= { extremeVlanOpaqueEntry 2 }


	--
	-- The Extreme Networks VLAN Stack Table
	--
	-- This table is essentially the ifStackTable without entries for any ports
	--

        extremeVlanStackTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF ExtremeVlanStackEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
			"Represents those components of the ifStackTable that do not
                         contain a Physical interface."
		::= { extremeVlanStackGroup 1 }

	extremeVlanStackEntry OBJECT-TYPE
		SYNTAX  ExtremeVlanStackEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		    "Each entry in this read-only table defines which interfaces are
                     on top of which one. All information in the table is also
                     contained in ifStackTable. The Physical interfaces in the 
                     ifStackTable are not represented here."
		INDEX { extremeVlanStackHigherLayer, extremeVlanStackLowerLayer }
		::= { extremeVlanStackTable 1 }

        ExtremeVlanStackEntry ::=
		SEQUENCE {
			extremeVlanStackHigherLayer
				INTEGER,
			extremeVlanStackLowerLayer
				INTEGER
		}


        extremeVlanStackHigherLayer OBJECT-TYPE
		SYNTAX	INTEGER
		MAX-ACCESS	read-only
		STATUS	current
		DESCRIPTION
			"The higher layer in the logical vlan hierarchy."
		::= { extremeVlanStackEntry 1}

        extremeVlanStackLowerLayer OBJECT-TYPE
                SYNTAX INTEGER
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
			"The lower layer in the logical vlan hierarchy."
	        ::= { extremeVlanStackEntry 2 }

        extremeVlanL2StatsTable OBJECT-TYPE
		SYNTAX          SEQUENCE OF ExtremeVlanL2StatsEntry
		MAX-ACCESS      not-accessible
		STATUS          current
		DESCRIPTION
                    "This tables contains per-VLAN layer 2 statistics information."
		::= { extremeVlanStatsGroup 1 }

	extremeVlanL2StatsEntry OBJECT-TYPE
		SYNTAX          ExtremeVlanL2StatsEntry
		MAX-ACCESS      not-accessible
		STATUS          current
		DESCRIPTION
		    ""
		INDEX { extremeVlanIfIndex }
		::= { extremeVlanL2StatsTable 1 }

        ExtremeVlanL2StatsEntry ::=
		SEQUENCE {
                    extremeVlanL2StatsIfDescr                          DisplayString,
                    extremeVlanL2StatsPktsToCpu                     Counter64,
                    extremeVlanL2StatsPktsLearnt                      Counter64,
                    extremeVlanL2StatsIgmpCtrlPktsSnooped       Counter64,
                    extremeVlanL2StatsIgmpDataPktsSwitched     Counter64
		}
        
         extremeVlanL2StatsIfDescr      OBJECT-TYPE
		SYNTAX	                DisplayString (SIZE(0..32))
		MAX-ACCESS              read-only
		STATUS	                current
		DESCRIPTION
			"This is a description(name) of the VLAN."
	::= {extremeVlanL2StatsEntry 1}

         extremeVlanL2StatsPktsToCpu    OBJECT-TYPE
                SYNTAX                  Counter64
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION
			"The total number of packets of this VLAN sent to the CPU."
	        ::= { extremeVlanL2StatsEntry 2 }

        extremeVlanL2StatsPktsLearnt    OBJECT-TYPE
                SYNTAX                  Counter64
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION
			"The total number of packets learnt on this VLAN."
	        ::= { extremeVlanL2StatsEntry 3 }

        extremeVlanL2StatsIgmpCtrlPktsSnooped   OBJECT-TYPE
                SYNTAX                          Counter64
                MAX-ACCESS                      read-only
                STATUS                          current
                DESCRIPTION
			"The total number of IGMP control packets snooped on this VLAN."
	        ::= { extremeVlanL2StatsEntry 4 }

        extremeVlanL2StatsIgmpDataPktsSwitched  OBJECT-TYPE
                SYNTAX                          Counter64
                MAX-ACCESS                      read-only
                STATUS                          current
                DESCRIPTION
			"The total number of IGMP data packets switched on this VLAN."
	        ::= { extremeVlanL2StatsEntry 5 }

        extremeVlanAggregationTable OBJECT-TYPE
                SYNTAX      SEQUENCE OF ExtremeVlanAggregationEntry
                MAX-ACCESS  not-accessible
                STATUS      current
                DESCRIPTION
                "This table contains the VLAN aggregation information."
                ::= { extremeVlanAggregationGroup 1 }

        extremeVlanAggregationEntry       OBJECT-TYPE
                SYNTAX      ExtremeVlanAggregationEntry
                MAX-ACCESS  not-accessible
                STATUS      current
                DESCRIPTION
                "Information about the individual VLAN aggregation entry."
                INDEX   { extremeVlanAggregationSuperVlanIfIndex, 
                          extremeVlanAggregationSubVlanIfIndex }
                ::= { extremeVlanAggregationTable 1 }

        ExtremeVlanAggregationEntry ::= SEQUENCE {
                extremeVlanAggregationSuperVlanIfIndex      	INTEGER,
                extremeVlanAggregationSubVlanIfIndex		INTEGER,
                extremeVlanAggregationSubVlanStartIpNetAddress  IpAddress,
                extremeVlanAggregationSubVlanStartIpNetMask	IpAddress,
                extremeVlanAggregationSubVlanEndIpNetAddress	IpAddress,
                extremeVlanAggregationSubVlanEndIpNetMask	IpAddress,
                extremeVlanAggregationStatus		        RowStatus
        }
       
        extremeVlanAggregationSuperVlanIfIndex    OBJECT-TYPE
                SYNTAX      INTEGER
                MAX-ACCESS  read-only
                STATUS      current
                DESCRIPTION
                "The Super Vlan index for this entry."
                ::= { extremeVlanAggregationEntry 1 }

        extremeVlanAggregationSubVlanIfIndex    OBJECT-TYPE
                SYNTAX      INTEGER
                MAX-ACCESS  read-only
                STATUS      current
                DESCRIPTION
                "The Sub Vlan index for this entry."
                ::= { extremeVlanAggregationEntry 2 }

        extremeVlanAggregationSubVlanStartIpNetAddress    OBJECT-TYPE
                SYNTAX      IpAddress
                MAX-ACCESS  read-create
                STATUS      current
                DESCRIPTION
                "This represents the start network address of the IP range."
                ::= { extremeVlanAggregationEntry 3 }
       
        extremeVlanAggregationSubVlanStartIpNetMask    OBJECT-TYPE
                SYNTAX      IpAddress
                MAX-ACCESS  read-only
                STATUS      current
                DESCRIPTION
                "This represents the start network address mask of the IP range"
                ::= { extremeVlanAggregationEntry 4 }
                                         
        extremeVlanAggregationSubVlanEndIpNetAddress    OBJECT-TYPE
                SYNTAX      IpAddress
                MAX-ACCESS  read-create
                STATUS      current
                DESCRIPTION
                "This represents the end network address of the IP range."
                ::= { extremeVlanAggregationEntry 5 }
               
        extremeVlanAggregationSubVlanEndIpNetMask    OBJECT-TYPE
                SYNTAX      IpAddress
                MAX-ACCESS  read-only
                STATUS      current
                DESCRIPTION
                "This represents the end network address mask of the IP range."
                ::= { extremeVlanAggregationEntry 6 }                                         
        extremeVlanAggregationStatus		OBJECT-TYPE
               SYNTAX       RowStatus
               MAX-ACCESS   read-create
               STATUS	    current
               DESCRIPTION
               "The status of this entry."
               ::= { extremeVlanAggregationEntry 7 }
        
        extremeVlanAggregationConfigTable OBJECT-TYPE
                SYNTAX      SEQUENCE OF ExtremeVlanAggregationConfigEntry
                MAX-ACCESS  not-accessible
                STATUS      current
                DESCRIPTION
                "This table contains the sub VLAN proxy setting information."
                ::= { extremeVlanAggregationGroup 2 }
        
        extremeVlanAggregationConfigEntry       OBJECT-TYPE
                SYNTAX      ExtremeVlanAggregationConfigEntry
                MAX-ACCESS  not-accessible
                STATUS      current
                DESCRIPTION
                "Information about the individual VLAN aggregation entry."
                INDEX   { extremeVlanAggregationConfigSuperVlanIfIndex }
                ::= { extremeVlanAggregationConfigTable 1 }
        
        ExtremeVlanAggregationConfigEntry ::= SEQUENCE {
                extremeVlanAggregationConfigSuperVlanIfIndex 	INTEGER,
                extremeVlanAggregationConfigSubVlanProxyEnable	TruthValue
        }

        extremeVlanAggregationConfigSuperVlanIfIndex    OBJECT-TYPE
                SYNTAX      INTEGER
                MAX-ACCESS  read-only
                STATUS      current
                DESCRIPTION
                "The Super Vlan index for this entry."
                ::= { extremeVlanAggregationConfigEntry 1 }

        extremeVlanAggregationConfigSubVlanProxyEnable    OBJECT-TYPE
                SYNTAX      TruthValue
                MAX-ACCESS  read-create
                STATUS      current
                DESCRIPTION
                "The boolean flag that prevents normal communication between sub vlans."
                ::= { extremeVlanAggregationConfigEntry 2 }
    

        extremeVlanTranslationTable OBJECT-TYPE
                SYNTAX      SEQUENCE OF ExtremeVlanTranslationEntry
                MAX-ACCESS  not-accessible
                STATUS      current
                DESCRIPTION
                "This table contains the VLAN translation information."
                ::= { extremeVlanTranslationGroup 1 }

        extremeVlanTranslationEntry       OBJECT-TYPE
                SYNTAX      ExtremeVlanTranslationEntry
                MAX-ACCESS  not-accessible
                STATUS      current
                DESCRIPTION
                "Information about the individual VLAN translation entry."
                INDEX   { extremeVlanTranslationSuperVlanIfIndex, 
                          extremeVlanTranslationMemberVlanIfIndex }
                ::= { extremeVlanTranslationTable 1 }

        ExtremeVlanTranslationEntry ::= SEQUENCE {
                  extremeVlanTranslationSuperVlanIfIndex     	INTEGER,
                  extremeVlanTranslationMemberVlanIfIndex	INTEGER,
                  extremeVlanTranslationStatus			RowStatus
        }
          
        extremeVlanTranslationSuperVlanIfIndex    OBJECT-TYPE
                SYNTAX      INTEGER
                MAX-ACCESS  read-only
                STATUS      current
                DESCRIPTION
                        "The Super Vlan index for this entry."
                ::= { extremeVlanTranslationEntry 1 }

        extremeVlanTranslationMemberVlanIfIndex    OBJECT-TYPE
                SYNTAX      INTEGER
                MAX-ACCESS  read-only
                STATUS      current
                DESCRIPTION
                        "The member Vlan index for this entry."
                ::= { extremeVlanTranslationEntry 2 }
     
        extremeVlanTranslationStatus		OBJECT-TYPE
               SYNTAX		RowStatus
               MAX-ACCESS	read-create
               STATUS		current
               DESCRIPTION
            	    "The status of this entry."
               ::= { extremeVlanTranslationEntry 3 }

END



-- ===============================================================================

--
-- Extreme QoS objects
--

EXTREME-QOS-MIB DEFINITIONS ::= BEGIN

        IMPORTS
                MODULE-IDENTITY FROM SNMPv2-SMI
		OBJECT-TYPE     FROM SNMPv2-SMI
                TruthValue      FROM SNMPv2-TC
		DisplayString   FROM RFC1213-MIB
		RowStatus       FROM SNMPv2-TC
		ifIndex                 FROM RFC1213-MIB
		extremeVlanIfIndex	FROM EXTREME-VLAN-MIB
                extremeAgent            FROM EXTREME-BASE-MIB;

        extremeQos MODULE-IDENTITY
                LAST-UPDATED "0007240000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION "Extreme Quality-of-Service objects"
        ::= { extremeAgent 3 }

	extremeQosCommon	OBJECT IDENTIFIER ::= { extremeQos 1 }


	extremeUnitPaceMode OBJECT-TYPE
       	        SYNTAX  INTEGER {
            	        notApplicable(1),
                        normalEthernet(2),
                        lowLatency(3)
		}
                MAX-ACCESS	read-write
                STATUS deprecated
                DESCRIPTION
            	"This object specifies whether the device currently
                recognises and gives priority treatment to the 
                forwarding of packets with the PACE(tm) bit set in 
                their MAC Source Address fields.
                
                PACE(tm) mode applies to the whole unit only and
                is only valid when device is in Ingress QoS mode
                as specified by extremeQosMode ingress(1). This
                object will report notApplicable(1) when in 
                egress(2) mode. Set operations with value
                notApplicable(1) will be rejected."
	::= { extremeQosCommon 1 }                

--
-- Select QoS Mode
--
	extremeQosMode OBJECT-TYPE
		SYNTAX  INTEGER { ingress(1), egress(2) }
		MAX-ACCESS  read-write
		STATUS deprecated
		DESCRIPTION
                      "Indicates which QoS mode the device should
                       use. ingress(1) applies priority-based QoS based 
                       on the incoming packet's destination IP or MAC
                       address, 802.1p priority, PACE(tm), Source Port or
                       VLAN. egress(2) applies priority- and bandwidth-based
                       QoS based on destination IP or MAC address or VLAN.
                       See ExtremeWare documentation for further information."
	::= { extremeQosCommon 4 }

--
-- Reset all QoS settings to defaults
--
	extremeQosUnconfigure OBJECT-TYPE
		SYNTAX  TruthValue
		MAX-ACCESS  read-write
		STATUS deprecated
		DESCRIPTION
                      "Setting this to true will reset all QoS settings
                        in the device to factory defaults. Reads from this
                        value return an undefined value."
	::= { extremeQosCommon 5 }


--
-- QoS Profile table
--

	extremeQosProfileTable	OBJECT-TYPE
		SYNTAX	SEQUENCE OF ExtremeQosProfileEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
			"This table lists QoS profiles."
		::= { extremeQosCommon 6 }

	extremeQosProfileEntry	OBJECT-TYPE
		SYNTAX	ExtremeQosProfileEntry
		MAX-ACCESS	not-accessible
		STATUS	current
		DESCRIPTION
			"An individual QoS profile Entry."
		INDEX {extremeQosProfileIndex}
		::= {extremeQosProfileTable 1}

	ExtremeQosProfileEntry ::= SEQUENCE {
                extremeQosProfileIndex          INTEGER,
                extremeQosProfileName           DisplayString,
                extremeQosProfileMinBw          INTEGER,
                extremeQosProfileMaxBw          INTEGER,
                extremeQosProfilePriority       INTEGER,
                extremeQosProfileRowStatus      RowStatus
        }

        extremeQosProfileIndex OBJECT-TYPE
                SYNTAX  INTEGER (1..65535)
                MAX-ACCESS	read-create
                STATUS	current
                DESCRIPTION
                        "An index that uniquely identifies an entry in the
                        qos table."
                ::= { extremeQosProfileEntry 1}

        extremeQosProfileName OBJECT-TYPE
                SYNTAX	DisplayString (SIZE (0..127))
                MAX-ACCESS 	read-create
                STATUS	current
                DESCRIPTION
                        "A unique qos profile name."
                ::= {extremeQosProfileEntry 2}

        extremeQosProfileMinBw  OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
                 "The minumum percentage of bandwidth that this queue requires.
                 The Switch is required to provide the minumum amount of 
                 bandwidth to the queue. The lowest possible value is 0%."
                DEFVAL { 0 }
                ::= {extremeQosProfileEntry 3 }

                
        extremeQosProfileMaxBw	OBJECT-TYPE
                SYNTAX	INTEGER
        	MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
                 "The maximum percentage of bandwidth that this queue is
                 permitted to use.

                 If a non-default value is set for this object then it negates
                 any previously set value of extremeQosProfileMaxSustBwBps. In 
                 In addition, a set operation that supplies non-default values
                 for both this object and for extremeQosProfileMaxSustBwBps
                 will be rejected by the agent. In other words, you may supply
                 either an absolute or a percent limit, not both."
                DEFVAL { 100 }
                ::= {extremeQosProfileEntry 4 }

        extremeQosProfilePriority OBJECT-TYPE
                SYNTAX  INTEGER {
                                low(1),
                                lowHi(2),
                                normal(3),
                                normalHi(4),
                                medium(5),
                                mediumHi(6),
                                high(7),
                                highHi(8)
                }
                MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
                        "The level of priority in which this queue will be
                        serviced by the Switch."
                ::= {extremeQosProfileEntry 5 }

        extremeQosProfileRowStatus OBJECT-TYPE
                SYNTAX	RowStatus
                MAX-ACCESS 	read-create
                STATUS	current
                DESCRIPTION
                    "The status of the extremeQosProfile entry.
                    This object can be set to:
                                active(1)
                        	createAndGo(4)
                                createAndWait(5)
                                destroy(6)

                    The following values may be read:
                                active(1)
                                notInService(2)
                                notReady(3).
                        
                    Setting this object to createAndGo(4) causes the agent
                    to attempt to create and commit the row based on 
                    the contents of the objects in the row.  If all necessary
                    information is present in the row and the values are
                    acceptible to the agent, the agent will change the 
                    status to active(1).  If any of the necessary objects  
                    are not available, the agent will reject the creation
                    request.        

                    Setting this object to createAndWait(5) causes a row
                    in this table to be created.  The agent sets the
                    status to notInService(2) if all of the information is
                    present in the row and the values are acceptable to the
                    agent; otherwise, the agent sets the status to notReady(3).

                    Setting this object to active(1) is only valid when
                    the current status is active(1) or notInService(2).  

                    When the state of the row transitions is set to active(1),
                    the agent creates the corresponding row in the ifTable..

                    Setting this object to destroy(6) will remove the
                    corresponding QoS Profile Entry.

                    In order for a set of this object to destroy(6) to succeed,
                    all dependencies on this row must have been removed.  These
                    will include any stacking dependencies in the ifStackTable
                    and any protocol specific tables dependencies."
        ::= { extremeQosProfileEntry 6 }

--
-- VLAN-based QoS Table
--
       	extremeQosByVlanMappingTable	OBJECT-TYPE

		SYNTAX  SEQUENCE OF ExtremeQosByVlanMappingEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		  "Table to associate a Vlan with the QoS profile that the
		   Vlan is using. Every Vlan is assigned a Qos Profile and
		   hence there is an entry in this table corresponding to every
		   entry in the extremeVlanIfTable."
		::= { extremeQosCommon 7 }

	extremeQosByVlanMappingEntry	OBJECT-TYPE
		SYNTAX	ExtremeQosByVlanMappingEntry
		MAX-ACCESS	not-accessible
		STATUS	current
		DESCRIPTION
                        "The QoS associated with a particular Vlan."
		INDEX {extremeVlanIfIndex}
		::= {extremeQosByVlanMappingTable 1}

	ExtremeQosByVlanMappingEntry ::= SEQUENCE {
        	extremeQosByVlanMappingQosProfileIndex	INTEGER
	}

	extremeQosByVlanMappingQosProfileIndex OBJECT-TYPE
		SYNTAX	INTEGER (1..65535)
		MAX-ACCESS	read-write
		STATUS	current
		DESCRIPTION
		    "Value of extremeQosProfileIndex that uniquely 
                    identifies a QoS Profile entry in extremeQosProfileTable.
                    This indicates the QoS to be given to traffic for this
                    Vlan in the absence of any other more specific 
                    configuration information for this traffic."
	::= { extremeQosByVlanMappingEntry 1 }

--
-- Per Port QOS Table
--
	extremePerPortQosTable	OBJECT-TYPE
		SYNTAX	SEQUENCE OF ExtremePerPortQosEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		    "Global Qos Profiles are defined in the
	            extremeQosProfileTable. This table contains a list
                    of ports for which the definition of certain global
		    Qos Profiles has been overridden. The new definition
                    of the Qos profile parameters is in this table."
		::= { extremeQosCommon 8 }

	extremePerPortQosEntry	OBJECT-TYPE
		SYNTAX	ExtremePerPortQosEntry
		MAX-ACCESS	not-accessible
		STATUS	current
		DESCRIPTION
			"An individual overridden QoS profile Entry."
		INDEX {ifIndex, extremePerPortQosIndex}
		::= {extremePerPortQosTable 1}

	ExtremePerPortQosEntry ::= SEQUENCE {
                extremePerPortQosIndex          INTEGER,
                extremePerPortQosMinBw          INTEGER,
                extremePerPortQosMaxBw          INTEGER,
                extremePerPortQosPriority       INTEGER,
                extremePerPortQosRowStatus      RowStatus
        }

        extremePerPortQosIndex OBJECT-TYPE
                SYNTAX  INTEGER (1..65535)
                MAX-ACCESS	read-create
                STATUS	current
                DESCRIPTION
                        "The value of this variable is the same as the value
			of extremeQosProfileIndex of the Qos Profile which
			is overridden (for the port specified by ifIndex) by 
			the definition in this table."
                ::= { extremePerPortQosEntry 1}

        extremePerPortQosMinBw  OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
                   "The minumum percentage of bandwidth that this queue on the
		   specified port requires. The Switch is required to provide 
		   the minumum amount of bandwidth to the queue. The lowest 
		   possible value is 0%."
                DEFVAL { 0 }
                ::= {extremePerPortQosEntry 2 }

                
        extremePerPortQosMaxBw	OBJECT-TYPE
                SYNTAX	INTEGER
        	MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
                 "The maximum percentage of bandwidth that this queue on the
                 specified port is permitted to use."
                DEFVAL { 100 }
                ::= {extremePerPortQosEntry 3 }

        extremePerPortQosPriority OBJECT-TYPE
                SYNTAX  INTEGER {
                                low(1),
                                lowHi(2),
                                normal(3),
                                normalHi(4),
                                medium(5),
                                mediumHi(6),
                                high(7),
                                highHi(8)
                }
                MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
                 "The level of priority in which this queue will be
                 serviced by the Switch."
                ::= {extremePerPortQosEntry 4 }

        extremePerPortQosRowStatus OBJECT-TYPE
                SYNTAX	RowStatus
                MAX-ACCESS 	read-create
                STATUS	current
                DESCRIPTION
                 "The status of the extremePerPortQos entry.
		 This object can be set to 
            		active(1)
			createAndGo(4)
                 The following value may be read:
            		active(1)
		 Note that a destroy(6) is not supported. A row will only be
		 deleted from this table when the Qos Profile indicated
		 in that row is changed globally."

        ::= { extremePerPortQosEntry 5 }

        
--
-- QoS Ingress Priority
--
	extremeQosIngressPriorityTable	OBJECT-TYPE
		SYNTAX	SEQUENCE OF ExtremeQosIngressPriorityEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
			"This table lists QoS ingress priority settings."
		::= { extremeQosCommon 9 }

	extremeQosIngressPriorityEntry	OBJECT-TYPE
		SYNTAX	ExtremeQosIngressPriorityEntry
		MAX-ACCESS	not-accessible
		STATUS	current
		DESCRIPTION
			"An individual QoS ingress priority Entry."
		INDEX {extremeQosIngressPriorityIndex}
		::= {extremeQosIngressPriorityTable 1}

	ExtremeQosIngressPriorityEntry ::= SEQUENCE {
                extremeQosIngressPriorityIndex          INTEGER,
                extremeQosIngressPriorityName           DisplayString,
                extremeQosIngressPriorityValue          INTEGER
        }

        extremeQosIngressPriorityIndex OBJECT-TYPE
                SYNTAX  INTEGER (1..65535)
                MAX-ACCESS	read-only
                STATUS	current
                DESCRIPTION
                        "An index that uniquely identifies an entry in the
                        qos ingress priority table."
                ::= { extremeQosIngressPriorityEntry 1}

        extremeQosIngressPriorityName OBJECT-TYPE
                SYNTAX	DisplayString (SIZE (0..15))
                MAX-ACCESS 	read-only
                STATUS	current
                DESCRIPTION
                        "A qos ingress priority name."
                ::= {extremeQosIngressPriorityEntry 2}
                
        extremeQosIngressPriorityValue OBJECT-TYPE
                SYNTAX  INTEGER (0..15)
                MAX-ACCESS	read-only
                STATUS	current
                DESCRIPTION
                        "The ingress Qos priority value."
                ::= { extremeQosIngressPriorityEntry 3}
                

--
-- IQoS Profile table
--

	extremeIQosProfileTable	OBJECT-TYPE
		SYNTAX	SEQUENCE OF ExtremeIQosProfileEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
			"This table lists ingress QoS profiles."
		::= { extremeQosCommon 10 }

	extremeIQosProfileEntry	OBJECT-TYPE
		SYNTAX	ExtremeIQosProfileEntry
		MAX-ACCESS	not-accessible
		STATUS	current
		DESCRIPTION
			"An individual ingress QoS profile Entry."
		INDEX {ifIndex ,
                       extremeIQosProfileIndex}
		::= {extremeIQosProfileTable 1}

	ExtremeIQosProfileEntry ::= SEQUENCE {
                extremeIQosProfileIndex          INTEGER,
                extremeIQosProfileName           DisplayString,
                extremeIQosProfileMinBwType      INTEGER,
                extremeIQosProfileMinBw          INTEGER,
                extremeIQosProfileMaxBwType      INTEGER,
                extremeIQosProfileMaxBw          INTEGER,
                extremeIQosProfileRED            INTEGER,
                extremeIQosProfileMaxBuf         INTEGER
        }

        extremeIQosProfileIndex OBJECT-TYPE
                SYNTAX  INTEGER (1..65535)
                MAX-ACCESS	read-only
                STATUS	current
                DESCRIPTION
                        "An index that uniquely identifies an entry in the
                        ingress Qos table."
                ::= { extremeIQosProfileEntry 1}
                
        extremeIQosProfileName OBJECT-TYPE
                SYNTAX	DisplayString (SIZE (0..127))
                MAX-ACCESS 	read-only
                STATUS	current
                DESCRIPTION
                        "A unique ingress Qos profile name."
                ::= {extremeIQosProfileEntry 2}
                
        extremeIQosProfileMinBwType  OBJECT-TYPE
                SYNTAX  INTEGER {
			percentage(1),
			kbps(2),
                        mbps(3)
		}
                MAX-ACCESS  read-only  
                STATUS current
                DESCRIPTION
                   "The type of the current minimum bandwith setting. A value
                   of 1 signifies that the minimum bandwith value is a percentage
                   of the configurable port bandwidth. A value of 2 or 3 signifies
                   a guaranteed minimum available bandwidth in Kbps or Mbps
                   respectively."
                ::= {extremeIQosProfileEntry 3 }

        extremeIQosProfileMinBw  OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                 "The guaranteed minimum bandwidth for this queue, expressed as either
                 a percentage or a specific bandwidth value, as specified by the value
                 of extremeIQosProfileMinBwType."
                DEFVAL { 0 }
                ::= {extremeIQosProfileEntry 4 }
                
        extremeIQosProfileMaxBwType  OBJECT-TYPE
                SYNTAX  INTEGER {
			percentage(1),
			kbps(2),
                        mbps(3)
		}
                MAX-ACCESS  read-only  
                STATUS current
                DESCRIPTION
                   "The type of the current maximum bandwith setting. A value
                   of 1 signifies that the maximum bandwith value is a percentage
                   of the configurable port bandwidth. A value of 2 or 3 signifies
                   a maximum allowed bandwidth in Kbps or Mbps respectively."
                ::= {extremeIQosProfileEntry 5 }
                
        extremeIQosProfileMaxBw	OBJECT-TYPE
                SYNTAX	INTEGER
        	MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                 "The maximum allowed input bandwidth for this queue, expressed as 
                 either a percentage or a specific bandwidth value, as specified by 
                 the value of extremeIQosProfileMaxBwType."
                DEFVAL { 0 }
                ::= {extremeIQosProfileEntry 6 }

        extremeIQosProfileRED OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                        "The Random Early Drop threshold. When the input queue fill
                        ratio exceeds this percentage, frames start to drop randomly
                        with a linear increasing drop probability as the queue fill
                        count approaches the max queue size. A value of 100 indicates
                        that this feature is currently disabled."
                ::= {extremeIQosProfileEntry 7 }

        extremeIQosProfileMaxBuf OBJECT-TYPE
                SYNTAX	INTEGER
                MAX-ACCESS 	read-only
                STATUS	current
                DESCRIPTION
                    "The percentage of the total ingress queue size to use. Lower values
                    can be used to reduce the max latency through this queue, but with
                    potentially greater loss with bursty traffic."
        ::= { extremeIQosProfileEntry 8 }
        

--
-- VLAN-based Ingress QoS Table
--
       	extremeIQosByVlanMappingTable	OBJECT-TYPE

		SYNTAX  SEQUENCE OF ExtremeIQosByVlanMappingEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		  "Table to associate a Vlan with the ingress QoS profile 
                  that the Vlan is using. Every Vlan is assigned a Qos Profile 
                  and hence there is an entry in this table corresponding to
                  every entry in the extremeVlanIfTable."
		::= { extremeQosCommon 11 }

	extremeIQosByVlanMappingEntry	OBJECT-TYPE
		SYNTAX	ExtremeIQosByVlanMappingEntry
		MAX-ACCESS	not-accessible
		STATUS	current
		DESCRIPTION
                        "The ingress QoS associated with a particular Vlan."
		INDEX {extremeVlanIfIndex}
		::= {extremeIQosByVlanMappingTable 1}

	ExtremeIQosByVlanMappingEntry ::= SEQUENCE {
        	extremeIQosByVlanMappingIQosProfileIndex	INTEGER
	}

	extremeIQosByVlanMappingIQosProfileIndex OBJECT-TYPE
		SYNTAX	INTEGER (1..65535)
		MAX-ACCESS	read-only
		STATUS	current
		DESCRIPTION
		    "Value of extremeIQosProfileIndex that uniquely 
                    identifies an ingress QoS Profile entry in extremeIQosProfileTable.
                    This indicates the QoS to be given to traffic for this
                    Vlan in the absence of any other more specific 
                    configuration information for this traffic."
	::= { extremeIQosByVlanMappingEntry 1 }



END

-- ===============================================================================

--
-- Extreme Port objects
--

EXTREME-PORT-MIB DEFINITIONS ::= BEGIN

        IMPORTS
                MODULE-IDENTITY         FROM SNMPv2-SMI
		RowStatus               FROM SNMPv2-TC
		OBJECT-TYPE             FROM SNMPv2-SMI
		ifIndex                 FROM RFC1213-MIB
        ClientAuthType          FROM EXTREME-BASE-MIB
                extremeAgent            FROM EXTREME-BASE-MIB
                Counter64               FROM SNMPv2-SMI
		extremeVlanIfIndex	FROM EXTREME-VLAN-MIB
                Counter32, TimeTicks    FROM SNMPv2-SMI 
                IpAddress               FROM SNMPv2-SMI 
                MacAddress              FROM SNMPv2-TC
                DisplayString           FROM RFC1213-MIB;

        extremePort MODULE-IDENTITY
                LAST-UPDATED "0007240000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION "Extreme network port objects"
        ::= { extremeAgent 4 }

--
-- Load-sharing. Table exists but support removed for 6.0.
--
	extremePortLoadshareTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF ExtremePortLoadshareEntry
		MAX-ACCESS  not-accessible
		STATUS deprecated
		DESCRIPTION
                      "A table of bindings between a master port 
                        and its load-sharing slaves: create/delete 
                        entries here to add/delete a port to/from a 
                        load-sharing group. Default is empty table. 
                        There are restrictions on what row creates 
                        will be accepted by each device - see Summit 
                        release notes for details."
	::= { extremePort 1 }

	extremePortLoadshareEntry OBJECT-TYPE
		SYNTAX  ExtremePortLoadshareEntry
		MAX-ACCESS  not-accessible
		STATUS deprecated
		DESCRIPTION
                      "A binding between a master port and one
                       of its load-sharing slave ports."
                INDEX { extremePortLoadshareMasterIfIndex, 
                        extremePortLoadshareSlaveIfIndex } 
	::= { extremePortLoadshareTable 1 }

	ExtremePortLoadshareEntry ::= SEQUENCE {
                extremePortLoadshareMasterIfIndex INTEGER, 
                extremePortLoadshareSlaveIfIndex INTEGER,
   		extremePortLoadshareGrouping	INTEGER,
                extremePortLoadshareStatus RowStatus 
	}

	extremePortLoadshareMasterIfIndex OBJECT-TYPE
                SYNTAX INTEGER
                MAX-ACCESS  read-create
                STATUS deprecated
                DESCRIPTION
                      "The ifIndex value which identifies the
                       port controlling a loadsharing group
                       of ports which includes
                       extremePortLoadshareSlaveIfIndex."
        ::= { extremePortLoadshareEntry 1 }

	extremePortLoadshareSlaveIfIndex OBJECT-TYPE
                SYNTAX INTEGER
                MAX-ACCESS  read-create
                STATUS deprecated
                DESCRIPTION
                      "The ifIndex value which identifies the
                       port which is a member of a loadsharing 
                       group controlled by 
                        extremePortLoadshareMasterIfIndex."
        ::= { extremePortLoadshareEntry 2 }

	extremePortLoadshareGrouping OBJECT-TYPE
                SYNTAX INTEGER { other (1), pair (2), quad (4) }
                MAX-ACCESS  read-create
                STATUS deprecated
                DESCRIPTION
                      "The Grouping value which identifies if load sharing is
                      in pair or quad."
        ::= { extremePortLoadshareEntry 3 }

	extremePortLoadshareStatus OBJECT-TYPE
                SYNTAX  RowStatus
                MAX-ACCESS  read-create
                STATUS deprecated
                DESCRIPTION
                        "The row status variable, used according to
                        row installation and removal conventions."
        ::= { extremePortLoadshareEntry 4 }

-- Support dropped in 6.0

-- Summitlink Table

        extremePortSummitlinkTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF ExtremePortSummitlinkEntry
		MAX-ACCESS  not-accessible
		STATUS deprecated
		DESCRIPTION
                      "A table of Extreme link configuration
                        and status information. Contains a row 
                        for only those ports that are capable of 
                        operating in Summitlink-mode."
	::= { extremePort 2 }

	extremePortSummitlinkEntry OBJECT-TYPE
		SYNTAX  ExtremePortSummitlinkEntry
		MAX-ACCESS  not-accessible
		STATUS deprecated
		DESCRIPTION
                      "Link configuration and status information
                        for a Summitlink Port."
               INDEX { ifIndex }
	::= { extremePortSummitlinkTable 1 }

        ExtremePortSummitlinkEntry ::=  SEQUENCE {
                extremePortSummitlinkAdminMode INTEGER,
                extremePortSummitlinkOperMode INTEGER,
                extremePortSummitlinkState INTEGER,
                extremePortSummitlinkRejectReason INTEGER
        } 

        extremePortSummitlinkAdminMode OBJECT-TYPE
                SYNTAX INTEGER { ethernetOnly(1), summitlinkOnly(2) }
                MAX-ACCESS  read-write
                STATUS deprecated
                DESCRIPTION
                      "Configurable operating mode for this
                       Summitlink port. Configure to summitlinkOnly(1)
                       before connecting this port to a SummitVC device."
                DEFVAL { ethernetOnly }
        ::= { extremePortSummitlinkEntry 1 }

        extremePortSummitlinkOperMode OBJECT-TYPE
                SYNTAX INTEGER { ethernetOnly(1), summitlinkOnly(2) }
                MAX-ACCESS  read-only
                STATUS deprecated
                DESCRIPTION
                      "Actual Operating mode."
                DEFVAL { ethernetOnly }
        ::= { extremePortSummitlinkEntry 2 }
 
        extremePortSummitlinkState OBJECT-TYPE
                SYNTAX INTEGER { up(1), down(2) }
                MAX-ACCESS  read-only
                STATUS deprecated
                DESCRIPTION
                      "Current status of a Summitlink link. Where a port
                        has redundant PMD capability, this indicates up if
                        either of the PMDs has an active link."
        ::= { extremePortSummitlinkEntry 3 }

        extremePortSummitlinkRejectReason OBJECT-TYPE
                SYNTAX INTEGER { none(1), other(2), stackMisconnected(3) }
                MAX-ACCESS  read-only
                STATUS deprecated
                DESCRIPTION
                     "If a Summitlink connection has been attempted 
                        and failed to reach the up(1) state, this 
                        indicates the potential source of the failure."
        ::= { extremePortSummitlinkEntry 4 }


--
-- New load share table for 6.0
--
	extremePortLoadshare2Table OBJECT-TYPE
		SYNTAX  SEQUENCE OF ExtremePortLoadshare2Entry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
                      "A table of bindings between a master port 
                        and its load-sharing slaves: create/delete 
                        entries here to add/delete a port to/from a 
                        load-sharing group. Default is empty table. 
                        There are restrictions on what row creates 
                        will be accepted by each device - see Summit 
                        release notes for details."
	::= { extremePort 3 }

	extremePortLoadshare2Entry OBJECT-TYPE
		SYNTAX  ExtremePortLoadshare2Entry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
                      "A binding between a master port and one
                       of its load-sharing slave ports."
                INDEX { extremePortLoadshare2MasterIfIndex, 
                        extremePortLoadshare2SlaveIfIndex } 
	::= { extremePortLoadshare2Table 1 }

	ExtremePortLoadshare2Entry ::= SEQUENCE {
                extremePortLoadshare2MasterIfIndex INTEGER, 
                extremePortLoadshare2SlaveIfIndex  INTEGER,
   		extremePortLoadshare2Algorithm	   INTEGER,
                extremePortLoadshare2Status        RowStatus 
	}

	extremePortLoadshare2MasterIfIndex OBJECT-TYPE
                SYNTAX INTEGER
                MAX-ACCESS  not-accessible
                STATUS current
                DESCRIPTION
                      "The ifIndex value which identifies the
                       port controlling a loadsharing group
                       of ports which includes
                       extremePortLoadshareSlaveIfIndex."
        ::= { extremePortLoadshare2Entry 1 }

	extremePortLoadshare2SlaveIfIndex OBJECT-TYPE
                SYNTAX INTEGER
                MAX-ACCESS  not-accessible
                STATUS current
                DESCRIPTION
                      "The ifIndex value which identifies the
                       port which is a member of a loadsharing 
                       group controlled by extremePortLoadshare2MasterIfIndex."
        ::= { extremePortLoadshare2Entry 2 }

	extremePortLoadshare2Algorithm OBJECT-TYPE
                SYNTAX INTEGER { ingressPortOffset (1),
                                 hash (2),
                                 roundRobin (3) }
                MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
                      "This value identifies the load sharing algorithm
                      to be used for this group of load shared ports."
        ::= { extremePortLoadshare2Entry 3 }

	extremePortLoadshare2Status OBJECT-TYPE
                SYNTAX  RowStatus
                MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
                        "The row status variable, used according to
                        row installation and removal conventions."
        ::= { extremePortLoadshare2Entry 4 }

----
-- Port Rate Shape Table
----
	extremePortRateShapeTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF ExtremePortRateShapeEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
                      "A list of ports that have ingress rate limiting
                       enforced."
	::= { extremePort 4 }

	extremePortRateShapeEntry OBJECT-TYPE
		SYNTAX  ExtremePortRateShapeEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
                      "An entry that is either a rate limited or
                       a loopback port. Any vlan that has rate
		       limited ports should have one loopback port
		       defined. The traffic parameters for the rate
		       limited ports correspond to those that are
		       defined for the loopback port in the
		       extremePerPortQosTable."
                INDEX { ifIndex, extremeVlanIfIndex }
	::= { extremePortRateShapeTable 1 }

	ExtremePortRateShapeEntry ::= SEQUENCE {
   		extremePortRateShapePortType	  INTEGER,
		extremePortRateShapeLoopbackTag   INTEGER,
                extremePortRateShapeStatus        RowStatus 
	}

	extremePortRateShapePortType OBJECT-TYPE
                SYNTAX INTEGER {
			rateLimited(1),
			loopBack(2)
		}
                MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
                      "Whether a loopback or rate limited port." 
        ::= { extremePortRateShapeEntry 1 }

	extremePortRateShapeLoopbackTag OBJECT-TYPE
		SYNTAX 	INTEGER (2..4094)
		MAX-ACCESS  read-create
		STATUS current
		DESCRIPTION
			"An unique internal tag that will needs to be set
			up for the vlan corresponding to this entry for
			adding ingress rate limited ports to the corresponding
			vlan."
        ::= { extremePortRateShapeEntry 2 }

	extremePortRateShapeStatus OBJECT-TYPE
                SYNTAX  RowStatus
                MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
                        "The row status variable, used according to
                        row installation and removal conventions."
        ::= { extremePortRateShapeEntry 3 }

--
-- Per Port QoSReport Table
--
	extremePortUtilizationTable	OBJECT-TYPE
		SYNTAX	SEQUENCE OF ExtremePortUtilizationEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		    "Global Qos Profiles are defined in the
	            extremeQosProfileTable. This table contains a list
                    of ports for which certain QoS parms are reported."
		::= { extremePort 5 }

	extremePortUtilizationEntry	OBJECT-TYPE
		SYNTAX	ExtremePortUtilizationEntry
		MAX-ACCESS	not-accessible
		STATUS	current
		DESCRIPTION
			"An individual QoSReport Entry."
		INDEX {ifIndex}
		::= {extremePortUtilizationTable 1}

	ExtremePortUtilizationEntry ::= SEQUENCE {
                extremePortUtilizationAvgTxBw        INTEGER,
                extremePortUtilizationAvgRxBw        INTEGER,
                extremePortUtilizationPeakTxBw       INTEGER,
                extremePortUtilizationPeakRxBw       INTEGER 
        }

        extremePortUtilizationAvgTxBw  OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS  read-only  
                STATUS current
                DESCRIPTION
                   "The reported average bandwidth in the txmit direction. When displayed
                    it shows as an Integer value i.e 99.99% is displayed as 9999."
                ::= {extremePortUtilizationEntry 1 }

                
        extremePortUtilizationAvgRxBw	OBJECT-TYPE
                SYNTAX	INTEGER
        	MAX-ACCESS  read-only  
                STATUS current
                DESCRIPTION
                 "The reported average bandwidth in the receive direction. When displayed
                    it shows as an Integer value i.e 99.99% is displayed as 9999." 
                ::= {extremePortUtilizationEntry 2 }

        extremePortUtilizationPeakTxBw  OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                   "The reported peak bandwidth in the txmit direction. When displayed
                    it shows as an Integer value i.e 99.99% is displayed as 9999."
                ::= {extremePortUtilizationEntry 3 }


        extremePortUtilizationPeakRxBw  OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                 "The reported peak bandwidth in the receive direction. When displayed
                    it shows as an Integer value i.e 99.99% is displayed as 9999."
                ::= {extremePortUtilizationEntry 4 }

--
-- Per Port Information Table
--
       extremePortInfoTable   OBJECT-TYPE
               SYNTAX  SEQUENCE OF ExtremePortInfoEntry
               MAX-ACCESS  not-accessible
               STATUS current
               DESCRIPTION
                "This table contains a list of port information."
               ::= { extremePort 6 }

       extremePortInfoEntry   OBJECT-TYPE
               SYNTAX  ExtremePortInfoEntry
               MAX-ACCESS      not-accessible
               STATUS  current
               DESCRIPTION
                   "An individual Port Information Entry."
               INDEX {ifIndex}
               ::= {extremePortInfoTable 1}

       ExtremePortInfoEntry ::= SEQUENCE {
               extremePortInfoFilterUpCounter        Counter32,
               extremePortInfoFilterDownCounter      Counter32
       }

       extremePortInfoFilterUpCounter  OBJECT-TYPE
               SYNTAX  Counter32
               MAX-ACCESS  read-write
               STATUS current
               DESCRIPTION
                 "The reported Port Filter up counter value.
                  This counter indicates the number of times a port's link
                  state has transitioned from DOWN to UP state. "
               ::= {extremePortInfoEntry 1 }


       extremePortInfoFilterDownCounter        OBJECT-TYPE
               SYNTAX        Counter32
               MAX-ACCESS  read-write
               STATUS current
               DESCRIPTION
                 "The reported Port Filter down counter value.
                  This counter indicates the number of times a port's link
                  state has transitioned from UP to DOWN state. "
               ::= {extremePortInfoEntry 2 }

--
-- extremePortXenpakVendor Table
--

        extremePortXenpakVendorTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF ExtremePortXenpakVendorEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
                      "A table of Extreme Xenpak Module Vendor Name
                        and type information. Contains a row 
                        for only those ports that are part of 
                        Xenpak module ."
	::= { extremePort 7 }

	extremePortXenpakVendorEntry OBJECT-TYPE
		SYNTAX  ExtremePortXenpakVendorEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
                      "Vendor name and type for Xenpak module."
               INDEX { ifIndex }
	::= { extremePortXenpakVendorTable 1 }

        ExtremePortXenpakVendorEntry ::=  SEQUENCE {
                extremePortXenpakVendorName DisplayString
        } 

      	extremePortXenpakVendorName OBJECT-TYPE
                SYNTAX  DisplayString (SIZE(0..22))
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                      "A human-readable string representing Vendor name 
                        of this module.
                        This string should be the same for all entries
                        having the same Xenpak module: 
                        this entry may not be modified."
	::= { extremePortXenpakVendorEntry 1 }

--
-- Per Port Ingress Statistics Table
--

        extremePortIngressStats OBJECT IDENTIFIER
        ::= { extremePort 8 }

	extremePortIngressStatsPortTable	OBJECT-TYPE
		SYNTAX	SEQUENCE OF ExtremePortIngressPortStatsEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		    "Port ingress statistics are returned for ports which
                    support ingress queuing. This table contains a list
                    of counters for each port."
		::= { extremePortIngressStats 1 }

	extremePortIngressPortStatsEntry	OBJECT-TYPE
		SYNTAX	ExtremePortIngressPortStatsEntry
		MAX-ACCESS	not-accessible
		STATUS	current
		DESCRIPTION
			"An individual IngressStats Entry."
		INDEX {ifIndex}
		::= {extremePortIngressStatsPortTable 1}

	ExtremePortIngressPortStatsEntry ::= SEQUENCE {
                extremePortIngressStatsLinkStatus         INTEGER,
                extremePortIngressStatsPortHighPriBytes   Counter64,
                extremePortIngressStatsPortLowPriBytes    Counter64,
                extremePortIngressStatsPortDroppedBytes   Counter64,
                extremePortIngressStatsTxXoff             Counter64 
        }


        extremePortIngressStatsLinkStatus  OBJECT-TYPE
                SYNTAX  INTEGER {
			ready(1),
			active(2),
                        disabled(3),
                        notPresent(4)
		}
                MAX-ACCESS  read-only  
                STATUS current
                DESCRIPTION
                   "The current status of the link. Ready indicates the port is ready
                   to accept a link; Active indicates the link is present at this port;
                   Disabled shows that the link is disabled at this port; Not Present
                   means the link is not present at this port."
                ::= {extremePortIngressPortStatsEntry 1 }

                
        extremePortIngressStatsPortHighPriBytes	OBJECT-TYPE
                SYNTAX	Counter64
        	MAX-ACCESS  read-only  
                STATUS current
                DESCRIPTION
                 "The sum of all per queue CIR counts for this port, which indicates the
                 bytes forwarded for high-priority packets." 
                ::= {extremePortIngressPortStatsEntry 2 }

        extremePortIngressStatsPortLowPriBytes  OBJECT-TYPE
                SYNTAX  Counter64
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                   "The sum of all per queue PR counts for this port, which indicates the
                   bytes forwarded for low-priority packets."
                ::= {extremePortIngressPortStatsEntry 3 }

        extremePortIngressStatsPortDroppedBytes  OBJECT-TYPE
                SYNTAX  Counter64
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                 "The total number of bytes dropped for this port."
                ::= {extremePortIngressPortStatsEntry 4 }
                
        extremePortIngressStatsTxXoff  OBJECT-TYPE
                SYNTAX  Counter64
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                 "The number of XOFF Flow Control packets sent from this port due to
                 receive traffic congestion."
                ::= {extremePortIngressPortStatsEntry 5 }
                

--
-- Per Queue Ingress Statistics Table
--        

        extremePortIngressStatsQueueTable	OBJECT-TYPE
		SYNTAX	SEQUENCE OF ExtremePortIngressQueueStatsEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		    "Port ingress statistics are returned for ingress queues. 
                    This table contains a list of counters for each ingress
                    queue."
		::= { extremePortIngressStats 2 }

        extremePortIngressQueueStatsEntry	OBJECT-TYPE
		SYNTAX	ExtremePortIngressQueueStatsEntry
		MAX-ACCESS	not-accessible
		STATUS	current
		DESCRIPTION
			"An individual IngressStatsQueue Entry."
		INDEX {ifIndex,
                       extremePortIngressStatsQueueIndex}
		::= {extremePortIngressStatsQueueTable 1}

	ExtremePortIngressQueueStatsEntry ::= SEQUENCE {
                extremePortIngressStatsQueueIndex          INTEGER,
                extremePortIngressStatsQueueHighPriBytes   Counter64,
                extremePortIngressStatsQueueLowPriBytes    Counter64,
                extremePortIngressStatsQueuePercentDropped INTEGER
        }
        

        extremePortIngressStatsQueueIndex  OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS  read-only  
                STATUS current
                DESCRIPTION
                   "The ingress queue being queried."
                ::= {extremePortIngressQueueStatsEntry 1 }

        extremePortIngressStatsQueueHighPriBytes	OBJECT-TYPE
                SYNTAX	Counter64
        	MAX-ACCESS  read-only  
                STATUS current
                DESCRIPTION
                 "The sum of all per queue CIR counts for this queue, which indicates the
                 bytes forwarded for high-priority packets." 
                ::= {extremePortIngressQueueStatsEntry 2 }

        extremePortIngressStatsQueueLowPriBytes  OBJECT-TYPE
                SYNTAX  Counter64
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                   "The sum of all per queue PR counts for this queue, which indicates the
                   bytes forwarded for low-priority packets."
                ::= {extremePortIngressQueueStatsEntry 3 }

        extremePortIngressStatsQueuePercentDropped  OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                 "The percentage of receive bytes dropped by this queue relative to the total
                 number of bytes input to this queue."
                ::= {extremePortIngressQueueStatsEntry 4 }

                

--
-- Per Port Egress Rate Limit Table
--
	extremePortEgressRateLimitTable	OBJECT-TYPE
		SYNTAX	SEQUENCE OF ExtremePortEgressRateLimitEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		    "Port egress rate limit statistics for a port."
		::= { extremePort 9 }

	extremePortEgressRateLimitEntry	OBJECT-TYPE
		SYNTAX	ExtremePortEgressRateLimitEntry
		MAX-ACCESS	not-accessible
		STATUS	current
		DESCRIPTION
			"An individual EgressRateLimit Entry."
		INDEX {ifIndex}
		::= {extremePortEgressRateLimitTable 1}

	ExtremePortEgressRateLimitEntry ::= SEQUENCE {
                extremePortEgressRateLimitType               INTEGER,
                extremePortEgressRateLimitValue              INTEGER
        }
        
        extremePortEgressRateLimitType  OBJECT-TYPE
                SYNTAX  INTEGER {
			percentage(1),
			kbps(2),
                        mbps(3)
		}
                MAX-ACCESS  read-only  
                STATUS current
                DESCRIPTION
                   "The type of the current egress rate setting. A value of 1 
                   signifies that the egress rate limit value is represented by
                   a percentage of the maximum configurable port bandwidth. A value 
                   of 2 or 3 signifies the rate is configured in Kbps or Mbps
                   respectively."
                ::= {extremePortEgressRateLimitEntry 1 }

                
        extremePortEgressRateLimitValue	OBJECT-TYPE
                SYNTAX	INTEGER
        	MAX-ACCESS  read-only  
                STATUS current
                DESCRIPTION
                 "The configured egress rate value." 
                ::= {extremePortEgressRateLimitEntry 2 }

--
-- Clients connected to the Port
--
	extremeWiredClientTable	OBJECT-TYPE
		SYNTAX	SEQUENCE OF ExtremeWiredClientEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		    "This table contains the entries for authenticated Clinets."
		::= { extremePort 10 }

extremeWiredClientEntry OBJECT-TYPE
        SYNTAX          ExtremeWiredClientEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
        "An entry in the extremeWiredClientTable."
    INDEX {ifIndex, extremeWiredClientID}
        ::= { extremeWiredClientTable 1 }

ExtremeWiredClientEntry ::= SEQUENCE {
        extremeWiredClientID                     MacAddress,
        extremeWiredClientState                  INTEGER,
        extremeWiredClientVLAN                   INTEGER,
        extremeWiredClientPriority               INTEGER,
        extremeWiredClientAuthType               ClientAuthType,
		extremeWiredClientLastStateChangeTime    TimeTicks,
        extremeWiredClientIP                     IpAddress}

extremeWiredClientID OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The Unique MAC Address of the station for which this address
         table entry pertains."
    ::= { extremeWiredClientEntry 1 }

extremeWiredClientState OBJECT-TYPE
    SYNTAX INTEGER { authenticated (1),
                        unauthenticated (2) }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "This attribute shall indicate the current state of the client. 
         The attribute is enumerated as follows:

        1 - Authenticated - client is authenticated.
        2 - Unauthenticated - the client is connect but unauthenticated.
        "
    ::= { extremeWiredClientEntry 2 }

extremeWiredClientVLAN OBJECT-TYPE
    SYNTAX          INTEGER
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This is the per-client VLAN which was pushed over
         by a RADIUS server or other mechanism."
    ::= { extremeWiredClientEntry 3 }

extremeWiredClientPriority OBJECT-TYPE
    SYNTAX          INTEGER
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This is a per-client 802.1p value which was either
         configured by the RADIUS server or statically through
         the port configuration table."
    ::= { extremeWiredClientEntry 4 }

extremeWiredClientAuthType OBJECT-TYPE
    SYNTAX          ClientAuthType
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "This is an indication of what access method was
         used to authenticated the client."
    ::= { extremeWiredClientEntry 5 }

extremeWiredClientLastStateChangeTime OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is the sysUpTime of the switch when the clients state changed last"
    ::= { extremeWiredClientEntry 6 }

extremeWiredClientIP OBJECT-TYPE
    SYNTAX          IpAddress
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "IP Address of the wired client."
    ::= { extremeWiredClientEntry 7 }

        

END
-- ============================================================================

-- Support dropped in 6.0

--
-- Extreme Virtual Chassis objects
--

EXTREME-VC-MIB DEFINITIONS ::= BEGIN

        IMPORTS
                MODULE-IDENTITY FROM SNMPv2-SMI
		OBJECT-TYPE     FROM SNMPv2-SMI
                TruthValue      FROM SNMPv2-TC
		ifIndex         FROM RFC1213-MIB
                extremeAgent    FROM EXTREME-BASE-MIB;

        extremeVC MODULE-IDENTITY
                LAST-UPDATED "9801090000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION "Extreme Virtual Chassis objects"
        ::= { extremeAgent 5 }

--
-- Virtual Chassis Link Table
-- 

        extremeVCLinkTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF ExtremeVCLinkEntry
		MAX-ACCESS  not-accessible
		STATUS deprecated
		DESCRIPTION
                      "A table of information about any neighbouring
                       Extreme Virtual Chassis device. Only contains 
                       valid data for ports that are configured to 
                       have extremePortSummitlinkAdminMode set to
                       summitlinkOnly have an active link or 
		       have had an active link since the last time 
		       they were configured in Summitlink mode."
	::= { extremeVC 1 }

	extremeVCLinkEntry OBJECT-TYPE
		SYNTAX  ExtremeVCLinkEntry
		MAX-ACCESS  not-accessible
		STATUS deprecated
		DESCRIPTION
                      "Neighbour information for a single Summitlink
                       Port."
                INDEX { ifIndex }
	::= { extremeVCLinkTable 1 }

        ExtremeVCLinkEntry ::=  SEQUENCE {
		extremeVCLinkValid     TruthValue,
                extremeVCLinkDeviceId  INTEGER,
                extremeVCLinkPortIndex INTEGER
        } 

        extremeVCLinkValid OBJECT-TYPE 
                SYNTAX TruthValue
                MAX-ACCESS  read-only
                STATUS deprecated
                DESCRIPTION
                      "Flag indicating whether other columns of this
                      table contain data."
	::= { extremeVCLinkEntry 1 }

        extremeVCLinkDeviceId OBJECT-TYPE 
                SYNTAX INTEGER
                MAX-ACCESS  read-only
                STATUS deprecated
                DESCRIPTION
                      "ID of the current SummitVC device
                        connected to this Summitlink port."
	::= { extremeVCLinkEntry 2 }

        extremeVCLinkPortIndex OBJECT-TYPE
                SYNTAX INTEGER
                MAX-ACCESS  read-only
                STATUS deprecated
                DESCRIPTION
                      "The Summitlink subchannel number that the Summit 
                        device on the other side of the neighbouring 
                        SummitVC will use to reach this device."
	::= { extremeVCLinkEntry 3 }
END


-- ============================================================================

--
-- Extreme Trap-based polling objects
--

EXTREME-TRAPPOLL-MIB DEFINITIONS ::= BEGIN

        IMPORTS
                MODULE-IDENTITY         FROM SNMPv2-SMI
		OBJECT-TYPE             FROM SNMPv2-SMI
		RowStatus               FROM SNMPv2-TC
                Integer32, TimeTicks    FROM SNMPv2-SMI
		trapDestIndex           FROM RMON2-MIB
                extremeAgent            FROM EXTREME-BASE-MIB;

        extremeTrapPoll MODULE-IDENTITY
                LAST-UPDATED "9801090000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION "Extreme SmartTraps trap-based-polling objects"
        ::= { extremeAgent 6 }


        extremeSmartTrapRulesTable OBJECT-TYPE
        	SYNTAX	SEQUENCE OF ExtremeSmartTrapRulesEntry
        	MAX-ACCESS 	not-accessible
        	STATUS	current
        	DESCRIPTION	
			"A table of rules that are used to 
                        generate extremeSmartTraps."	
	::= { extremeTrapPoll 1 } 

        extremeSmartTrapRulesEntry OBJECT-TYPE
        	SYNTAX	ExtremeSmartTrapRulesEntry
        	MAX-ACCESS 	not-accessible
        	STATUS	current
        	DESCRIPTION	
			"Each row in the table represents a rule."
        	INDEX	{ extremeSmartTrapRulesIndex } 
	::= { extremeSmartTrapRulesTable 1 } 

        ExtremeSmartTrapRulesEntry ::= SEQUENCE {
		extremeSmartTrapRulesIndex		INTEGER,
		extremeSmartTrapRulesRowStatus		RowStatus,
		extremeSmartTrapRulesDesiredOID	        OBJECT IDENTIFIER,
		extremeSmartTrapRulesSupportedOID	OBJECT IDENTIFIER,
		extremeSmartTrapRulesOperation		INTEGER,
		extremeSmartTrapRulesTrapDestIndex      Integer32
	}

        extremeSmartTrapRulesIndex 	OBJECT-TYPE
        	SYNTAX	INTEGER
        	MAX-ACCESS 	read-only
        	STATUS	current
        	DESCRIPTION	
			"An index into the extremeSmartTraps rules table. "
	::= { extremeSmartTrapRulesEntry 1 }

        extremeSmartTrapRulesRowStatus 	OBJECT-TYPE
        	SYNTAX	RowStatus
        	MAX-ACCESS 	read-create
        	STATUS	current
        	DESCRIPTION	
			"Indicates the status of row. "
	::= { extremeSmartTrapRulesEntry 2 }

        extremeSmartTrapRulesDesiredOID	OBJECT-TYPE
        	SYNTAX	OBJECT IDENTIFIER
        	MAX-ACCESS 	read-create
        	STATUS	current
        	DESCRIPTION	
                "The OID for which the rule is desired. When the OID 
                specified by this object undergoes an operation 
                specified by extremeSmartTrapRulesOperation, then 
                an entry in the extremeSmartTrapInstanceTable is created."
	::= { extremeSmartTrapRulesEntry 3 }

        extremeSmartTrapRulesSupportedOID	OBJECT-TYPE
        	SYNTAX	OBJECT IDENTIFIER
        	MAX-ACCESS 	read-only
        	STATUS	current
        	DESCRIPTION	
                "The OID for which this entry is created. This is 
                based on the granularity supported by the agent 
                corresponding to the extremeSmartTrapRulesDesiredOID 
                that the management station desires. This object has a 
                value that is a prefix of, or is equal to the value of 
                ExtremeSmartTrapRulesDesiredOID. The agent specifes 
                this value before setting the extremeSmartTrapRulesRowStatus 
                to active."
	::= { extremeSmartTrapRulesEntry 4 }

        extremeSmartTrapRulesOperation	OBJECT-TYPE
        	SYNTAX	INTEGER {
			add(1),
			delete(2),
			modify(3),
			any(4)
		}
        	MAX-ACCESS 	read-create
        	STATUS	current
        	DESCRIPTION	
                "The write operations on extremeSmartTrapRulesDesiredOID 
                for which extremeSmartTrapsInstanceEntry should be created."
	::= { extremeSmartTrapRulesEntry 5 }

        extremeSmartTrapRulesTrapDestIndex OBJECT-TYPE
        	SYNTAX	Integer32
        	MAX-ACCESS 	read-create
        	STATUS	current
        	DESCRIPTION	
                "A pointer to a row in RMON2's trapDestTable that was
                created by the management station that defined 
                this rule. Any extremeSmartTraps generated by this agent due
                to this rule will be sent to the trapDestCommunity/
                trapDestAddress and will include trapDestOwner specified by 
                this trapDestTable entry.

                This also allows a manager to identify if the rule was defined 
                by itself, or by another (possibly older) instance of the 
                management server process. The manager should initiate a 
                poll only for traps received which indicate its own rules. 

                Subprocesses within a single manager might also uniquely 
                create their own entries within trapDestTable using 
                different trapDestOwner strings: when a trap is received, 
                the manager can authenticate if the trap was generated due 
                to one of its rules and route the notification to the
                appropriate subprocess."
	::= { extremeSmartTrapRulesEntry 6 }

--
-- Table for storing information about the occurence of changes 
-- according to the rules in extremeSmartTrapRulesTable.
--
-- This is a read-only table maintained by the agent. 

        extremeSmartTrapInstanceTable  OBJECT-TYPE
        	SYNTAX	SEQUENCE OF ExtremeSmartTrapInstanceEntry
        	MAX-ACCESS 	not-accessible
        	STATUS	current
        	DESCRIPTION	
		"A table representing containing information about
                which variables have changed according to the 
                rules defined in extremeSmartTrapRulesTable."
	::= { extremeTrapPoll 2 }
	
        extremeSmartTrapInstanceEntry	 OBJECT-TYPE
        	SYNTAX	ExtremeSmartTrapInstanceEntry
        	MAX-ACCESS 	not-accessible
        	STATUS	current
        	DESCRIPTION	
                "An entry corresponding to a change in value of one of 
                the OIDs defined in extremeSmartTrapRulesTable. Entries
                are indexed by a pointer to the relevant row in 
                RMON2 trapDestTable that a manager created in order to
                receive trap notifications of these events.

                Entries are created in this table whenever the value of 
                one of the OIDs defined by extremeSmartTrapRulesSupportedOID 
                changes. Entries are deleted when a get or get-next operation 
                is performed on that entry. A get operation for a non-existent 
                entry returns a noSuchInstance error."

               	INDEX { trapDestIndex, extremeSmartTrapInstanceSubindex } 
	::= { extremeSmartTrapInstanceTable 1 } 

        ExtremeSmartTrapInstanceEntry ::= SEQUENCE {
		extremeSmartTrapInstanceSubindex	INTEGER,
		extremeSmartTrapInstanceRule		INTEGER,
		extremeSmartTrapInstanceChangedOid	OBJECT IDENTIFIER,
		extremeSmartTrapInstanceActualOperation	INTEGER,
		extremeSmartTrapInstanceChangeTime	TimeTicks
	}

        extremeSmartTrapInstanceSubindex OBJECT-TYPE
        	SYNTAX	INTEGER 
        	MAX-ACCESS 	read-only
        	STATUS	current
        	DESCRIPTION	
                "An additional index into the table of extremeSmartTrap 
                instance data. Each row which has the same OID for the
                same management station (i.e. same cookie) is assigned
                a unique value by the agent in order to differentiate 
                between multiple instances."
	::= { extremeSmartTrapInstanceEntry 1 } 

        extremeSmartTrapInstanceRule OBJECT-TYPE
        	SYNTAX	INTEGER 
        	MAX-ACCESS 	read-only
        	STATUS	current
        	DESCRIPTION	
                "The index of the rule from the 
                extremeSmartTrapRulesTable for which this entry 
                was created."
	::= { extremeSmartTrapInstanceEntry 2 } 

        extremeSmartTrapInstanceChangedOid OBJECT-TYPE
        	SYNTAX	OBJECT IDENTIFIER
        	MAX-ACCESS 	read-only
        	STATUS	current
        	DESCRIPTION	
                "The OID value that has changed."
	::= { extremeSmartTrapInstanceEntry 3 } 

        extremeSmartTrapInstanceActualOperation OBJECT-TYPE
        	SYNTAX	INTEGER {
       			add(1),
			delete(2),
			modify(3)
		}				
        	MAX-ACCESS 	read-only
        	STATUS	current
        	DESCRIPTION	
                "The operation that was recently performed on 
                this extremeSmartTrapInstanceChangedOid."
	::= { extremeSmartTrapInstanceEntry 4 } 

        extremeSmartTrapInstanceChangeTime OBJECT-TYPE
        	SYNTAX	TimeTicks
        	MAX-ACCESS 	read-only
        	STATUS	current
        	DESCRIPTION	
                "The sysUpTime when this entry was created."
	::= { extremeSmartTrapInstanceEntry 5 }
	
--
-- Flush control for Trap table
--
        extremeSmartTrapFlushInstanceTableIndex OBJECT-TYPE
        	SYNTAX	INTEGER 
        	MAX-ACCESS 	read-write
        	STATUS	current
        	DESCRIPTION	
                "When this object is set, the agent will delete all rows
                from the extremeSmartTrapInstanceTable which meet the
                following rules: 
		1. The InstanceTableIndex is equal to the value obtained by 
		taking the two most significant bytes of this integer and
		right-shifting it by two bytes as an unsigned int.
		2. The InstanceTableSubIndex is less than or equal to the
                value obtained by masking this object value with 0x0000FFFF.
                If the value obtained is zero, then all rows with the specified
                InstanceTableIndex should be deleted."
	::= { extremeTrapPoll 3 } 

END

-- ============================================================================

--
-- Extreme Policy-Based QoS
--

EXTREME-PBQOS-MIB DEFINITIONS ::= BEGIN

	IMPORTS
                MODULE-IDENTITY, OBJECT-TYPE, IpAddress, Counter64
                                FROM SNMPv2-SMI
                TruthValue, RowStatus
                                FROM SNMPv2-TC
                ifEntry         FROM IF-MIB
      		OwnerString     FROM RMON-MIB
		DisplayString	FROM RFC1213-MIB 
                extremeAgent, PortList, L4Port
                                FROM EXTREME-BASE-MIB;

        extremeQosPolicy MODULE-IDENTITY
                LAST-UPDATED "9903030000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION 
                        "Extreme QoS Policy configuration objects"
        ::= { extremeAgent 7 }

--
-- ============================================================================
--        Rules
-- ============================================================================
-- 
-- Policy rules are used to define the forwarding behaviour of either data
-- traffic or of signaling messages e.g. RSVP. At the ExtremeWare device <->
-- EEM interface, rules are of the following format:
-- 
-- <rule> ::= <rule_id>, <scope>, <direction>, <filter>, <treatment>
-- 
-- <rule_id> ::= INTEGER
-- <scope> ::= signaled | inband
-- <direction> ::= forward | backward | any
--
-- <filter> ::= <inport> | 
--               <outports>, <filterspec> |
--               <outports>, <iptosspec>
-- 
-- <inport> ::= <physport> | any
-- <outports> ::= <physport>* | any
-- <physport> ::= INTEGER | SLOT:INTEGER
-- 
-- The following fields may be used for classification of traffic into a QoS treatment:
-- - IP destination/range
-- - IP source/range
-- - Incoming IP Type-of-Service/mask/match
-- - transport-layer ProtocolNumber (TCP,UDP,other,any)
-- - TCP/UDP destination port number
-- - TCP/UDP source port number
--
-- These may be used in limited combinations to form compound patterns e.g.
-- IntServ filterspecs based on {IP src/dest, IP protocol number, TCP/UDP
-- src/dest} 5-tuples.
-- 
-- <filterspec> ::= <ipsrcrange> <ipdestrange> <ipproto> <srcport> <dstport>
-- <ipsrcrange> ::= IPADDRESS IPADDRESS
-- <ipdestrange> ::= IPADDRESS IPADDRESS
-- <ipproto> ::= tcp | udp | other | any
-- <srcport> ::= INTEGER(0..65535) | any
-- <dstport> ::= INTEGER(0..65535) | any
-- 
-- <iptosspec> ::= <iptosmatch> <iptosmask>  - match if IPTOS & iptosmask == iptosmatch
-- <iptosmatch> ::= INTEGER 0..255
-- <iptosmask> ::= INTEGER 0..255
-- 
-- N.B. IPTOS support is not available on first generation (1-G) silicon
-- IPTOS values are therefore ignored in EW 5.0.
--
-- Each rule is assigned an identifier, unique within each device. The rule is 
-- tagged as applying to either signaled data flows (i.e. RSVP) or to be
-- applied directly to the data itself. The direction of flow is also specified
-- : these apply to the direction of the *data* flow and indicate whether the
-- rule should be applied to one or both directions of a matching data or
-- signal flow.
--
-- This table specifies which physical input and output ports and what traffic
-- patterns are included in a rule.
-- 
-- Note: these filter fields are in addition to the existing extremeQosByVlanMappingTable 
-- table. ExtremeWare currently has a fixed precedence of filter rules: VLAN has the lowest 
-- precedence, followed by source physicalport, 802.1p, MAC and then IP/TCP/UDP as highest 
-- precedence. This implies that any entry in this extremeQosFilterTable takes precedence over 
-- any VLAN match that might indicate a QoS profile in extremeQosByVlanMappingTable. In addition, 
-- any entry that indicates a <filterspec> that is not "any" takes precedence over a filter 
-- indicating an individual <inport>. Any attempt to write a rule that indicates an individual
-- extremeQosRuleInPort as well as non-DEFVAL value for any of {<ipsrcrange> <ipdestrange> 
-- <ipproto> <srcport> <dstport>} will be rejected by the agent.
-- 
-- In other words, in the language of policy management, there is an implied rule precedence 
-- which is used to resolve conflicts in the case where an incoming data packet could potentially
-- be classified as matching 2 or more rules. Some conflicts can be indicated at the time a 
-- policy rule is applied to the device but others can only be detected and resolved at the
-- time a rule is invoked by an incoming message.
--

	extremeNextAvailableQosRuleIndex OBJECT-TYPE
		SYNTAX	        INTEGER
		MAX-ACCESS	read-only
		STATUS	        current
		DESCRIPTION
		"The value of the next available QoS Rule index. This
		 object is used by an NMS to select an index value 
		 for row-creation in the extremeQosRuleTable. The 
		 current value of this object is changed to a new
		 value when the current value is written to an agent's
		 table. Row creation using the current value of this object
                 allocates a extremeQosRuleIndex.  Note the following:
		
		 1. A newly created row does not have to be active(1)
		    for the agent to allocate the extremeQosRuleIndex.

		 2. Race conditions between multiple NMS's end when
		    a row is created.  Rows are deemed created when
		    a setRequest is successfully committed (i.e.
		    the errorStats is noError(0)).

		3.  An agent that exhausts its supply of extremeQosRuleIndex
		    values returns zero as the value of this
		    object.  This can be used by an NMS as an indication
		    to deleted unused rows and reboot the device."
	::= { extremeQosPolicy 1 }		 

	extremeQosClearIPFdb OBJECT-TYPE
		SYNTAX      TruthValue
		MAX-ACCESS  read-write
		STATUS      current
		DESCRIPTION
                      "Setting this to true will clear the hardware IP
                       flow table."
	::= { extremeQosPolicy 4 }

	extremeQosClearFdb OBJECT-TYPE
		SYNTAX      TruthValue
		MAX-ACCESS  read-write
		STATUS      current
		DESCRIPTION
                      "Setting this to true will clear the hardware MAC
                       flow table."
	::= { extremeQosPolicy 5 }


        extremeQosRuleTable OBJECT-TYPE
 		SYNTAX  SEQUENCE OF ExtremeQosRuleEntry
		MAX-ACCESS  not-accessible
		STATUS  current
                DESCRIPTION
                "Table of QoS policy rules. Entries that duplicate the exact
                same set of policy conditions are not allowed."
	::= { extremeQosPolicy 2 }

        extremeQosRuleEntry OBJECT-TYPE
		SYNTAX  ExtremeQosRuleEntry
		MAX-ACCESS  not-accessible
		STATUS  current
		DESCRIPTION
                "Entry in table of QoS policy rules"
               INDEX { extremeQosRuleIndex } 
	::= { extremeQosRuleTable 1 }

        ExtremeQosRuleEntry ::= SEQUENCE
        {
                extremeQosRuleIndex             INTEGER,
                extremeQosRuleScope             INTEGER,
                extremeQosRuleDirection         INTEGER,
                extremeQosRuleInPort            INTEGER,
                extremeQosRuleInPortMask        PortList,
                extremeQosRuleDestAddrStart     IpAddress,
                extremeQosRuleDestAddrEnd       IpAddress,
                extremeQosRuleSrcAddrStart      IpAddress,
                extremeQosRuleSrcAddrEnd        IpAddress,
                extremeQosRuleProtocol          INTEGER,
                extremeQosRuleDestL4PortStart   L4Port,
                extremeQosRuleSourceL4PortStart L4Port,
                extremeQosRuleTosMask           OCTET STRING,
                extremeQosRuleTosMatch          OCTET STRING,
                extremeQosRuleQosProfileIndex   INTEGER,
                extremeQosRuleOwner             OwnerString,
                extremeQosRuleRowStatus         RowStatus,
                extremeQosRuleDestL4PortEnd     L4Port,
                extremeQosRuleSourceL4PortEnd   L4Port,
		extremeQosRulePrecedence	INTEGER,
		extremeQosRuleCounter           Counter64,
		extremeQosRuleName		DisplayString
        }

        extremeQosRuleIndex  OBJECT-TYPE
		SYNTAX          INTEGER
		MAX-ACCESS 	read-create
		STATUS          current
		DESCRIPTION
		"An index into the table of QoS policy pattern
                rules. The index for a manager to use for creating
                new rows is determined by reading the value of 
                extremeNextAvailableQosRuleIndex."
	::= { extremeQosRuleEntry 1 }

        extremeQosRuleScope  OBJECT-TYPE
		SYNTAX  INTEGER { any (1), signaled(2), inband(3) }
		MAX-ACCESS 	read-create
		STATUS  current
		DESCRIPTION
		"The scope of conditions in which this rule applies.
                The value 'signaled' means that the policy rule is
                applied only to QoS signaling messages e.g. RSVP. The
                value 'inband' means that the policy rule is applied
                only to data traffic passing through this node. the
                value 'any' means that the policy is applied to any
                of the above conditions. 

                Only the value 'any' is supported in ExtremeWare 6.0."
                DEFVAL { any }
	::= { extremeQosRuleEntry 2 }

        extremeQosRuleDirection  OBJECT-TYPE
		SYNTAX          INTEGER { any(1), forward(2), backward(3) }
		MAX-ACCESS 	read-create
		STATUS          current
		DESCRIPTION
		"The direction in which this rule applies. The value
                'forward' means that the rule is applied to data streams
                in the direction specified by the classification pattern.
                The value 'backward' means that the rule is applied in
                the reverse direction. The value 'any' means that the
                rule is applied for traffic in either direction of data
                flow. Note that the direction is applied to where the data 
                flow itself will go, not to the direction of any signaling 
                messages e.g. RSVP.

                Only the value 'forward' is supported in ExtremeWare 6.0."
                DEFVAL { forward }
	::= { extremeQosRuleEntry 3 }

        extremeQosRuleInPort  OBJECT-TYPE
		SYNTAX          INTEGER
		MAX-ACCESS 	read-create
		STATUS          current
		DESCRIPTION
		"The ifIndex value of the physical switch input port for which 
                this rule applies. Rules that indicate an individual value
                for this object have a lower precedence in ExtremeWare than
                rules that specify IP patterns. Conversely, rules that use IP
                patterns must apply to all physical ports and specify a value
                of 0 for this object.

                Any attempt to write a rule that indicates an individual
                value for this object together with non-default values for any 
                of { extremeQosRuleDestAddrStart, extremeQosRuleDestAddrEnd,
                extremeQosRuleSrcAddrStart, extremeQosRuleSrcAddrEnd,
                extremeQosRuleProtocol, extremeQosRuleDestL4PortStart,
                extremeQosRuleDestL4PortEnd, extremeQosRuleSourceL4PortStart,
                extremeQosRuleSourceL4PortEnd and extremeQosRuleInPortMask }
                will be rejected by the agent."
                DEFVAL { 0 }
	::= { extremeQosRuleEntry 4 }

        extremeQosRuleInPortMask  OBJECT-TYPE
		SYNTAX          PortList
		MAX-ACCESS 	read-create
		STATUS          current
		DESCRIPTION
		"The list of physical switch input ports which further
	        qualifies an IP flow. This object is an octet string
        	with the MSB of octet 0 indicating port 0 and LSB indicating
		port 7. Similarly, the MSB of octet 1 indicates port 8 and it's 
		LSB indicates port 15 and so on. The port numbers are 0-based.
		This object has no meaning for rules defined on physical ports
		that are not associated with an IP flow. Port based rules can be 
		defined by assigning a non zero value to extremeQosRuleInPort. Any
		attempt to set this value without specifying the source/destination 
		address range and/or source/destination l4 port range will be rejected
                by the agent. For IP flows that apply to all physical ports
                in the switch, this will be a zero length octet string."
	::= { extremeQosRuleEntry 5 }

        extremeQosRuleDestAddrStart  OBJECT-TYPE
		SYNTAX          IpAddress
		MAX-ACCESS 	read-create
		STATUS          current
		DESCRIPTION
		"The start of the destination IP address range for which this
                 rule applies.If this object has any value other than the
                 default then this rule takes precedence over any rule that
                 specifies an individual physical input port, a VLAN or any
                 incoming implicit 802.1p traffic class rule.

                Any attempt to write a rule that indicates a non-default value
                for this object together with an individual port value for
                extremeQosRuleInPort will be rejected by the agent."
                DEFVAL { '00000000'h }      -- 0.0.0.0
	::= { extremeQosRuleEntry 6 }

        extremeQosRuleDestAddrEnd  OBJECT-TYPE
		SYNTAX          IpAddress
		MAX-ACCESS 	read-create
		STATUS          current
		DESCRIPTION
		"The end of the destination IP address range for which this
                 rule applies. If this object has any value other than the
                 default then this rule takes precedence over any rule that
                 specifies an individual physical input port, a VLAN or any
                 incoming implicit 802.1p traffic class rule.

                Any attempt to write a rule that indicates a non-default value
                for this object together with an individual port value for
                extremeQosRuleInPort will be rejected by the agent."
                DEFVAL { 'ffffffff'h }      -- 255.255.255.255
	::= { extremeQosRuleEntry 7 }

        extremeQosRuleSrcAddrStart  OBJECT-TYPE
		SYNTAX          IpAddress
		MAX-ACCESS 	read-create
		STATUS          current
		DESCRIPTION
		"The start of the source IP address range for which this rule 
                applies. If this object has any value other than the default
                then this rule takes precedence over any rule that specifies
                an individual physical input port, a VLAN or any incoming
                implicit 802.1p traffic class rule.

                Any attempt to write a rule that indicates a non-default value
                for this object together with an individual port value for
                extremeQosRuleInPort will be rejected by the agent."
                DEFVAL { '00000000'h }      -- 0.0.0.0
	::= { extremeQosRuleEntry 8 }

        extremeQosRuleSrcAddrEnd  OBJECT-TYPE
		SYNTAX          IpAddress
		MAX-ACCESS 	read-create
		STATUS          current
		DESCRIPTION
		"The end of the source IP address range for which this rule 
                applies. If this object has any value other than the default
                then this rule takes precedence over any rule that specifies
                an individual physical input port, a VLAN or any incoming
                implicit 802.1p traffic class rule.

                Any attempt to write a rule that indicates a non-default value
                for this object together with an individual port value for
                extremeQosRuleInPort will be rejected by the agent."
                DEFVAL { 'ffffffff'h }      -- 255.255.255.255
	::= { extremeQosRuleEntry 9 }

        extremeQosRuleProtocol  OBJECT-TYPE
		SYNTAX          INTEGER { any(1), udp(2), tcp(3), other(4), 
					  tcpPermitEstablished(5), icmp(6) }
		MAX-ACCESS 	read-create
		STATUS          current
		DESCRIPTION
		"The IP protocol number for which this rule applies. If this 
                object has any value other than 'any' then this rule
                takes precedence over any rule that specifies an individual
                physical input port, a VLAN or any incoming implicit 802.1p
                traffic class rule.

                Any attempt to write a rule that indicates a non-default value
                for this object together with an individual port value for
                extremeQosRuleInPort will be rejected by the agent."
                DEFVAL { any }
	::= { extremeQosRuleEntry 10 }

        extremeQosRuleDestL4PortStart  OBJECT-TYPE
		SYNTAX          L4Port
		MAX-ACCESS 	read-create
		STATUS          current
		DESCRIPTION
		"The destination starting layer 4 port number that would
                be used to match an IP flow. The value of 0 means that all
                layer 4 information would be ignored when matching an IP
                flow. If this object has any value other than 0 then this
                rule takes precedence over any rule that specifies an
                individual physical input port, a VLAN or any incoming
                implicit 802.1p traffic class rule.

                Any attempt to write a rule that indicates a non-default value
                for this object together with an individual port value for
                extremeQosRuleInPort will be rejected by the agent.

		Any attempt to write an ICMP rule specifying an IP pattern
		with a non-default value for this object will be rejected by the
		agent."
                DEFVAL { 0 }
	::= { extremeQosRuleEntry 11 }

        extremeQosRuleSourceL4PortStart  OBJECT-TYPE
		SYNTAX          L4Port
		MAX-ACCESS 	read-create
		STATUS          current
		DESCRIPTION
		"The source starting layer 4 port number that would be
                used to match an IP flow. The value of 0 means that all
                layer 4 information would be ignored when matching an IP
                flow. If this object has any value other than 0 then this
                rule takes precedence over any rule that specifies an
                individual physical input port, a VLAN or any incoming
                implicit 802.1p traffic class rule.

                Any attempt to write a rule that indicates a non-default value
                for this object together with an individual port value for
                extremeQosRuleInPort will be rejected by the agent.

		NOTE: For an ICMP rule that specifies an IP pattern, this 
		object has a different meaning in that it specifies the ICMP Type
		and Code values, in the following manner: The value of the Type must
		be shifted to the left by 8 bits and logical ORed with the value of the 
		Code. The result will be stored in this object. In this case, this 
		object can only contain values between 0 and 65535 inclusive since the 
		ICMP Type and Code values are limited between 0 and 255 each."

                DEFVAL { 0 }
	::= { extremeQosRuleEntry 12 }

        extremeQosRuleTosMask  OBJECT-TYPE
		SYNTAX          OCTET STRING (SIZE (1))
		MAX-ACCESS 	read-create
		STATUS          deprecated
		DESCRIPTION
		"A mask for the incoming IP Type-of-Service field to be applied
                when matching. The value of 0 means that any incoming IP ToS
                field is ignored.

                Only the default value is supported in ExtremeWare 6.0."
                DEFVAL { '00'h }
	::= { extremeQosRuleEntry 13 }

        extremeQosRuleTosMatch  OBJECT-TYPE
		SYNTAX          OCTET STRING (SIZE (1))
		MAX-ACCESS 	read-create
		STATUS          deprecated
		DESCRIPTION
		"If the value of the incoming IP Type-of-Service field, after 
                applying a mask of extremeQosRuleTosMask, is this value then
                this rule is applied. 

                Only the default value is supported in ExtremeWare 6.0."
                DEFVAL { '00'h }
	::= { extremeQosRuleEntry 14 }

        extremeQosRuleQosProfileIndex  OBJECT-TYPE
		SYNTAX          INTEGER 
		MAX-ACCESS 	read-create
		STATUS          current
		DESCRIPTION
		"A pointer into the extremeQosProfileTable indicating the 
                QoS treatment and actions to be applied to traffic matching
                this rule. A value of 0 means that this traffic will be
                dropped/discarded. The default value is that this traffic
                gets the default QoS treatment and actions."
                DEFVAL { 1 }
	::= { extremeQosRuleEntry 15 }

        extremeQosRuleOwner  OBJECT-TYPE
		SYNTAX          OwnerString(SIZE (0..32))
		MAX-ACCESS 	read-create
		STATUS          current
		DESCRIPTION
                	"Indicates the identity of the manager that 
			configured this entry."
	::= { extremeQosRuleEntry 16 }

        extremeQosRuleRowStatus  OBJECT-TYPE
		SYNTAX          RowStatus
		MAX-ACCESS 	read-create
		STATUS          current
		DESCRIPTION
		  "The row status for this QoS rule. 

		  This OBJECT can be set to:

				active(1)
				createAndGo(4)
				createAndWait(5)
				destroy(6)

		  The following values may be read:
				active(1)
				notReady(3). "
 	::= { extremeQosRuleEntry 17 }

        extremeQosRuleDestL4PortEnd  OBJECT-TYPE
		SYNTAX          L4Port
		MAX-ACCESS 	read-create
		STATUS          current
		DESCRIPTION
		"The destination last layer 4 port number that would
                determine the l4 port range to match an IP flow. The value
                of 0 means that all layer 4 information would be ignored
                when matching an IP flow. If this object has any value other
                than 0 then this rule takes precedence over any rule that
                specifies an individual physical input port, a VLAN or any
                incoming implicit 802.1p traffic class rule.

                Any attempt to write a rule that indicates a non-default value
                for this object together with an individual port value for
                extremeQosRuleInPort will be rejected by the agent.

		Any attempt to write an ICMP rule specifying an IP pattern
		with a non-default value for this object will be rejected by the
		agent." 
                DEFVAL { 0 }
	::= { extremeQosRuleEntry 18 }

        extremeQosRuleSourceL4PortEnd  OBJECT-TYPE
		SYNTAX          L4Port
		MAX-ACCESS 	read-create
		STATUS          current
		DESCRIPTION
		"The source last layer 4 port number that would determine
                the l4 port range to match an IP flow. The value of 0 means
                that all layer 4 information would be ignored when matching
                an IP flow. If this object has any value other than 0 then
                this rule takes precedence over any rule that specifies an
                individual physical input port, a VLAN or any incoming
                implicit 802.1p traffic class rule.

                Any attempt to write a rule that indicates a non-default value
                for this object together with an individual port value for
                extremeQosRuleInPort will be rejected by the agent.

		Any attempt to write an ICMP rule specifying an IP pattern with
		a non-default value for this object will be rejected by the agent."
                DEFVAL { 0 }
	::= { extremeQosRuleEntry 19 }

        extremeQosRulePrecedence  OBJECT-TYPE
		SYNTAX          INTEGER
		MAX-ACCESS 	read-create
		STATUS          current
		DESCRIPTION
		"The precedence used to select one rule over potentially 
                multiple rules that might match an L3/L4 flow. The rule
		with highest precedence  takes precedence over any rule
		that specifies a matching flow, individual physical input
		port, a VLAN or any incoming implicit 802.1p traffic class
		rule.

                Any attempt to write a rule that indicates a non-default value
                for this object together with an individual port value for
                extremeQosRuleInPort will be rejected by the agent."
                DEFVAL { 0 }
	::= { extremeQosRuleEntry 20 }

        extremeQosRuleCounter  OBJECT-TYPE
		SYNTAX          Counter64
		MAX-ACCESS 	read-only
		STATUS          current
		DESCRIPTION
		" " 
                DEFVAL { 0 }
	::= { extremeQosRuleEntry 21 }

	extremeQosRuleName OBJECT-TYPE
		SYNTAX 		DisplayString (SIZE (0..32))
                MAX-ACCESS 	read-create
                STATUS		current
                DESCRIPTION
                "A unique Qos rule name. If this is not specified then the system 
		generates one automatically."
        ::= { extremeQosRuleEntry 22 }

-- ================================================================================
-- Treatment/Action/QoSProfile
-- ================================================================================
-- 
-- Several parameters are accessible, to a greater or lesser extent, for 
-- specifying the treatment received by traffic that is classified as matching
-- a static rule.
-- 
-- The following can be thought of as represented by a "per-hop behaviour" in 
-- IETF DiffServ terminology or by a "QoS Profile" in Extreme terminology:
--      - relative priority
--      - minimum guaranteed bandwidth
--      - maximum limit on bandwidth
--      - limit on peak bandwidth
--      - reserved buffer allocation
--      - maximum limit on buffer allocation
--      - filter/drop
-- 
-- In addition, the following actions can also be thought of as a part of the
-- treatment:
--      - trap to policy server
--      - outgoing IP TOS/mark/mask
--      - outgoing 802.1p mark
-- 
-- A set of parameters specify the scheduling characteristics of per-class 
-- queues and the marking of traffic that exits those queues. The term
-- "flowspec" is used loosely here although it has many of the characteristics
-- of an IntServ flowspec.
-- 
-- <treatment> ::= drop | <qos_profile>
--
-- <qos_profile> ::= <flowspec>, <action>
-- 
-- <flowspec> ::= <tokenBucket> | <absoluteBw> | <percentBw>, <buffers>, <priority>
-- <tokenBucket> ::= peakBW, sustBW, bucketSize
-- <absoluteBW> ::= minBW, maxPeakBW, maxSustBW
-- <percentBW> ::= minBWpercent, maxSustBWpercent, maxPeakBWpercent
-- <buffers> ::= maxQueueLength, minBufferAlloc
-- <priority> ::= relativePriority
-- 
-- <action> ::= <trap_to_server>, <mark_iptos>, <mark_8021p>
-- <trap_to_server> ::= TRUE | FALSE
-- <mark_iptos> ::= new_set_pattern, new_clear_pattern
-- <mark_8021p> ::= INTEGER 0..7 | unchanged
-- 
-- On any device using first-generation silicon, additional 
-- parameters are hard coded:
-- 
-- mark_iptos = 0,0   (i.e. IPTOS unchanged)
-- 
-- Note: for the ExtremeWare 4.0 release, some of the parameters are not 
-- exposed for modification through this interface: these are represented as
-- read-only - 6.0 behaviour is currently undefined. 
--
-- In particular, hard-coded values for the following are used in 4.0:
--    maxPeakBWpercent ::= line rate or 100%
--    maxQueueLength ::= infinite or something approaching total buffers in
--                       the device
--    minBufferAlloc ::= fixed at compile time <insert EW4.0 defaults>
--    mark_8021p ::= for packets entering untagged: 0, 2, 4 or 6 depending on
--                   queue number for packets entering tagged: unchanged.
--
-- 
-- Existing table:
--
-- extremeQosProfileTable INDEX { extremeQosProfileIndex} SEQUENCE OF
-- {
--      extremeQosProfileIndex	        INTEGER ,
--      extremeQosProfileName	        DisplayString,
--	extremeQosProfileMinBw	        INTEGER (0..100),
--	extremeQosProfileMaxBw		INTEGER (0..100),
--	extremeQosProfilePriority	INTEGER {low, normal, medium, high}
--	extremeQosProfileRowStatus	RowStatus
-- }
--
-- Added the following "flowspec" columns to extremeQosProfileTable:
--
--        extremeQosProfileMinBwBps             INTEGER,
--        extremeQosProfileMaxSustBwBps         INTEGER,
--        extremeQosProfileMaxPeakBwBps         INTEGER,
--        extremeQosProfileBucketSizeOctets     INTEGER,
--        extremeQosProfileMaxPeakBwPercent     INTEGER (0..100),
--        extremeQosProfileMaxQueueLengthOctets INTEGER,
--        extremeQosProfileMinBufferAllocOctets INTEGER
--
-- Added the following "action" columns to extremeQosProfileTable:
-- 
--        extremeTrapToServer     TruthValue,     - send trap to policy server
--        extremeMarkIpTosSet     OCTET STRING (SIZE (1)),
--        extremeMarkIpTosClear   OCTET STRING (SIZE (1)),
--        extremeMark8021p        INTEGER (0..7) or unchanged(8)  - see above



-- ===========================================================================
--        Capabilities
-- ===========================================================================

        extremeQosCapabilitiesTable OBJECT-TYPE
 		SYNTAX  SEQUENCE OF ExtremeQosCapabilitiesEntry
		MAX-ACCESS  not-accessible
		STATUS  current
                DESCRIPTION
                "Table of per-port QoS policy capabilities. An entry only
                 exists in this table for ifTable entries representing
                 physical ports. On a modular system with mixed capability
                 silicon it is necessary to indicate the QoS capabilities to
                 a manager."
	::= { extremeQosPolicy 3 }

        extremeQosCapabilitiesEntry OBJECT-TYPE
		SYNTAX  ExtremeQosCapabilitiesEntry
		MAX-ACCESS  not-accessible
		STATUS  current
		DESCRIPTION
                "Entry in table of QoS policy capabilities for a given switch
                 port."
                AUGMENTS { ifEntry }
	::= { extremeQosCapabilitiesTable 1 }

        ExtremeQosCapabilitiesEntry ::= SEQUENCE
        {
                extremeQosCapMarkIpTosCapable         TruthValue,
                extremeQosCapMatchIpTosCapable        TruthValue
        }

        extremeQosCapMarkIpTosCapable  OBJECT-TYPE
		SYNTAX          TruthValue
		MAX-ACCESS 	read-only
		STATUS          current
		DESCRIPTION
		"This port is capable of supporting policies that involve
                the changing of IP TOS octet values."
	::= { extremeQosCapabilitiesEntry 1 }

        extremeQosCapMatchIpTosCapable  OBJECT-TYPE
		SYNTAX          TruthValue
		MAX-ACCESS 	read-only
		STATUS          current
		DESCRIPTION
		"This port is capable of supporting policies that involve
                packet classification based on matching of IP TOS octet 
                values."
	::= { extremeQosCapabilitiesEntry 2 }

END

-- ===========================================================================

--
-- Extreme Dynamic-Link Context System (DLCS) reporting
--

EXTREME-DLCS-MIB DEFINITIONS ::= BEGIN

	IMPORTS
                MODULE-IDENTITY, OBJECT-TYPE, IpAddress, TimeTicks
                                FROM SNMPv2-SMI
                TruthValue      FROM SNMPv2-TC
		DisplayString   FROM RFC1213-MIB
                extremeAgent
                                FROM EXTREME-BASE-MIB;

        extremeDlcs MODULE-IDENTITY
                LAST-UPDATED "9903040000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION 
                        "Extreme Dynamic-Link Context System (DLCS) status objects"
        ::= { extremeAgent 8 }


--
-- Enable/disable DLCS
--
	extremeDlcsEnable OBJECT-TYPE
		SYNTAX      TruthValue
		MAX-ACCESS  read-write
		STATUS      current
		DESCRIPTION
                      "Setting this to true will allow the agent to start 
                        collecting DLCS binding information."
	::= { extremeDlcs 1 }

	extremeDlcsNetbiosEnable OBJECT-TYPE
		SYNTAX      TruthValue
		MAX-ACCESS  read-write
		STATUS      current
		DESCRIPTION
                      "Setting this to true will allow the agent to start 
                        collecting DLCS binding information using the
                        NetBios protocol."
	::= { extremeDlcs 2 }

	extremeDlcsKerberos5Enable OBJECT-TYPE
		SYNTAX      TruthValue
		MAX-ACCESS  read-write
		STATUS      current
		DESCRIPTION
                      "Setting this to true will allow the agent to start 
                        collecting DLCS binding information using the
                        Kerberos V5 protocol."
	::= { extremeDlcs 3 }

	extremeDlcsRsvpEnable OBJECT-TYPE
		SYNTAX      TruthValue
		MAX-ACCESS  read-write
		STATUS      current
		DESCRIPTION
                      "Setting this to true will allow the agent to start 
                        collecting DLCS binding information using the RSVP
                        protocol."
	::= { extremeDlcs 4 }

	extremeDlcsDnsEnable OBJECT-TYPE
		SYNTAX      TruthValue
		MAX-ACCESS  read-write
		STATUS      current
		DESCRIPTION
                      "Setting this to true will allow the agent to start 
                        collecting DLCS binding information using the
                        DNS protocol."
	::= { extremeDlcs 5 }

--
-- DLCS Binding Table
--
--
-- How is this table used?
-- 
-- (1) Manager creates extremeSmartTrapRulesEntry with
-- extremeSmartTrapRulesIndex = XXXX
-- extremeSmartTrapRulesDesiredOID = extremeDlcsBindingTable
-- extremeSmartTrapRulesOperation = any
-- 
-- (2) Events are reported by agent creating a extremeSmartTrapInstanceEntry with:
-- 
-- extremeSmartTrapInstanceRule = XXXX
-- extremeSmartTrapInstanceChangedOid = extremeDlcsBindingIndex
-- extremeSmartTrapInstanceActualOperation = add, delete or modify
-- 
-- and generating the actual trap.
-- 

        extremeDlcsBindingTable OBJECT-TYPE
 		SYNTAX      SEQUENCE OF ExtremeDlcsBindingEntry
		MAX-ACCESS  not-accessible
		STATUS      current
                DESCRIPTION
                "Table of DLCS Binding information. Entries are added and deleted
                by the agent based on information gathered from the local network 
                environment. Multiple entries may exist for almost identical sets
                of bindings although the agent will ensure that exactly matching
                entries are coalesced."
	::= { extremeDlcs 6 }

        extremeDlcsBindingEntry OBJECT-TYPE
		SYNTAX  ExtremeDlcsBindingEntry
		MAX-ACCESS  not-accessible
		STATUS  current
		DESCRIPTION
                "Entry in table of DLCS bindings."
               INDEX { extremeDlcsBindingIndex } 
	::= { extremeDlcsBindingTable 1 }

        ExtremeDlcsBindingEntry ::= SEQUENCE
        {
                extremeDlcsBindingIndex         INTEGER,
                extremeDlcsBindingType          BITS,
                extremeDlcsBindingSource        INTEGER,
                extremeDlcsBindingUser          DisplayString,
                extremeDlcsBindingGroup         DisplayString,
                extremeDlcsBindingApplication   DisplayString,
                extremeDlcsBindingHost          DisplayString,
                extremeDlcsBindingIpAddress     IpAddress,
                extremeDlcsBindingPhysPort      INTEGER,
                extremeDlcsBindingUpdateTime    TimeTicks
        }

        extremeDlcsBindingIndex  OBJECT-TYPE
            SYNTAX INTEGER
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "An index into this table, chosen by the agent. This has
                no significance to the manager beyond its uniqueness
                within this agent."
	::= { extremeDlcsBindingEntry 1 }

        extremeDlcsBindingType  OBJECT-TYPE
            SYNTAX  BITS { user2ip(0), user2port(1), ip2port(2), 
                           application2user(3), application2ip(4), 
                           host2ip(5), group2ip(6), group2port(7), 
                           user2group(8) }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The type of binding expressed here. A given bit is set if DLCS
                has detected that the two relevant items are bound together. 
                e.g. an entry with application2user(3) set to 1 implies that
                the username extremeDlcsBindingUser has been seen to be using 
                the application extremeDlcsBindingApplication. In addition, if
                this entry also has user2port(1) set to 1 then this user and
                application have been detected as running on the physical
                switch port extremeDlcsBindingPhysPort."
	::= { extremeDlcsBindingEntry 2 }

        extremeDlcsBindingSource  OBJECT-TYPE
            SYNTAX  INTEGER { other (1), local(2), netbiosquery(3),
			 netbiosbind (4), dns(5), kerberos5(6), rsvp(7) }
            MAX-ACCESS  read-only
            STATUS  current
            DESCRIPTION
                "The source of the information binding."
	::= { extremeDlcsBindingEntry 3 }

        extremeDlcsBindingUser  OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The User name detected by DLCS. A string of length zero
		 indicates no valid User name has been detected for this
		 binding."
	::= { extremeDlcsBindingEntry 4 }

        extremeDlcsBindingGroup  OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The Group name detected by DLCS. A string of length zero
                 indicates no valid Group name has been detected for this
		 binding."
	::= { extremeDlcsBindingEntry 5 }

        extremeDlcsBindingApplication  OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The Application name detected by DLCS. A string of length 
                zero indicates no valid Application name has been detected 
                for this binding."
	::= { extremeDlcsBindingEntry 6 }

        extremeDlcsBindingHost  OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The Host name detected by DLCS. A string of length 
                zero indicates no valid Host name has been detected 
                for this binding."
	::= { extremeDlcsBindingEntry 7 }

        extremeDlcsBindingIpAddress  OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The IP address detected by DLCS. A value of 0.0.0.0
                indicates no valid IP address has been detected 
                for this binding."
	::= { extremeDlcsBindingEntry 8 }

        extremeDlcsBindingPhysPort  OBJECT-TYPE
            SYNTAX INTEGER
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The physical port number (ifIndex) detected by DLCS.
                This is valid in all bindings."
	::= { extremeDlcsBindingEntry 9 }

        extremeDlcsBindingUpdateTime  OBJECT-TYPE
            SYNTAX TimeTicks
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The value of sysUpTime when this entry was last updated."
	::= { extremeDlcsBindingEntry 10 }

END

-- ===========================================================================


EXTREME-FILETRANSFER-MIB DEFINITIONS ::= BEGIN

IMPORTS
      MODULE-IDENTITY, IpAddress, OBJECT-TYPE		
                        FROM SNMPv2-SMI
      DisplayString, TestAndIncr, RowStatus
			FROM SNMPv2-TC
      OwnerString       FROM RMON-MIB
      extremeAgent	FROM EXTREME-BASE-MIB;

extremeFileTransfer	MODULE-IDENTITY
	LAST-UPDATED	"9810211630Z"
	ORGANIZATION	"Extreme Networks, Inc."
	CONTACT-INFO	"www.extremenetworks.com"
	DESCRIPTION	"Extreme File transfer objects"
	::= {extremeAgent 10}

-- The file transfer group

extremeFileTransferGroup OBJECT IDENTIFIER ::= { extremeFileTransfer 1 }

extremeFileTransferNextAvailableIndex OBJECT-TYPE
	SYNTAX  TestAndIncr
	MAX-ACCESS  read-only
	STATUS  current
	DESCRIPTION
	      "The index of the next free row in the extremeFileTransferTable."
	::= { extremeFileTransferGroup 1}

extremeFileTransferTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF FileTransferEntry
	MAX-ACCESS  not-accessible
	STATUS  current
	DESCRIPTION
		"A table of pending and completed file transfers."
	::= { extremeFileTransferGroup 2 }

extremeFileTransferEntry OBJECT-TYPE
	SYNTAX	FileTransferEntry
	MAX-ACCESS  not-accessible
	STATUS  current
	DESCRIPTION
                "A table entry containing information on a pending
                or completed file transfer."
	INDEX	{ extremeFileTransferIndex }
	::= { extremeFileTransferTable 1 }

FileTransferEntry ::=
	SEQUENCE {
		extremeFileTransferIndex			INTEGER,
		extremeFileTransferServerAddress		IpAddress,
		extremeFileTransferFileName                    DisplayString,
		extremeFileTransferOperation			INTEGER,
		extremeFileTransferScheduledTime		OCTET STRING,
		extremeFileTransferStartAdminStatus		INTEGER,
		extremeFileTransferStartOperStatus		INTEGER,
		extremeFileTransferLastExecutionStatus		INTEGER,
		extremeFileTransferOwner                       OwnerString,
		extremeFileTransferRowStatus			RowStatus
	}
		
extremeFileTransferIndex OBJECT-TYPE
        SYNTAX  INTEGER
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
		"An index into the file transfer table."
        ::= { extremeFileTransferEntry 1 }

extremeFileTransferServerAddress OBJECT-TYPE
        SYNTAX  IpAddress
        MAX-ACCESS  read-create
        STATUS  current
        DESCRIPTION
		"This is the address of the TFTP server from which to
		download the image or configuration or upload the 
		configuration."
        ::= { extremeFileTransferEntry 2 }

extremeFileTransferFileName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(0..64))
        MAX-ACCESS  read-create
        STATUS  current
        DESCRIPTION
		"This is the name of the file to be downloaded or uploaded."
        ::= { extremeFileTransferEntry 3 }

extremeFileTransferOperation OBJECT-TYPE
         SYNTAX  INTEGER {
                    downloadImageToPrimaryImmediate(1),
                    downloadImageToSecondaryImmediate(2),
                    downloadConfigImmediate(3),
                    uploadConfigImmediate(4),
                    scheduleConfigUploadPeriodic(5),
                    scheduleConfigUploadOnce(6),
                    scheduleImageDownloadToPrimaryOnce(7),
                    scheduleImageDownloadToSecondaryOnce(8),
		    scheduleConfigDownloadOnce(9)
                 }
         MAX-ACCESS  read-create
         STATUS  current
         DESCRIPTION 
                 "Indication of the file transfer operation.
                  This object allows configuration of uploads and/or
                  downloads either immediately or at a scheduled time.

		  A value of downloadImageToPrimaryImmediate(1) or 
		  downloadImageToSecondaryImmediate(2) describes immediate 
		  download of a software image to either the primary or 
		  secondary permanent store. A value of 
		  downloadConfigImmediate(3) describes immediate download
		  of a configuration file to non-volatile store. A value
		  of uploadConfigImmediate(4) describes the immediate upload
		  of the currently running configuration to the server.

		  A value of scheduleConfigUploadOnce(6) describes a single 
		  upload of the current configuration to the server at the 
		  time extremeFileTransferScheduledTime. A value of 
		  scheduleConfigUploadPeriodic(5) describes daily uploads 
		  of the current configuration to the server at the time 
		  extremeFileTransferScheduledTime every day.

		  A value of scheduleImageDownloadToPrimaryOnce(7) or 
		  scheduleImageDownloadToSecondaryOnce(8) describes a single 
		  download of a software image to either the primary or 
		  secondary permanent store at the time
		  extremeFileTransferScheduledTime.

		  This object can be modified only if
		  extremeFileTransferStartOperStatus for this entry is idle(1).

                  Note that any attempts to modify this object including
                  row creation which would result in multiple downloads
                  would cause the operation to fail. Managers are
                  strongly recommened to examine the 
                  extremeFileTransferStartOperStatus object for the entries
                  in the table to determine the status of downloads
                  before attempting to modify this object."
         ::= { extremeFileTransferEntry 4 }

extremeFileTransferScheduledTime OBJECT-TYPE -- This convention is from RMON2
        SYNTAX  OCTET STRING (SIZE (0 | 8 | 11))
        MAX-ACCESS  read-create
        STATUS  current
        DESCRIPTION
                "The time of the day at which the file transfer operation 
                should be initiated. This object is meaningful only for
                scheduled file transfers.

                field  octets  contents                  range
                -----  ------  --------                  -----
                1      1-2   year                      0..65536
                2       3    month                     1..12
                3       4    day                       1..31
                4       5    hour                      0..23
                5       6    minutes                   0..59
                6       7    seconds                   0..60
                                         (use 60 for leap-second)
                7       8    deci-seconds              0..9
                8       9    direction from UTC        '+' / '-'
                9      10    hours from UTC            0..11
                10      11    minutes from UTC         0..59

                For example, Tuesday May 26, 1992 at 1:30:15 PM
                EDT would be displayed as:

                     1992-5-26,13:30:15.0,-4:0

                Note that if only local time is known, then
                timezone information (fields 8-10) is not
                present, and if no time information is known, the null
                string is returned."
        ::= { extremeFileTransferEntry 5 }
	
extremeFileTransferStartAdminStatus OBJECT-TYPE
         SYNTAX  INTEGER {
                    start(1),
                    cancel(2)       
                 }
         MAX-ACCESS  read-create
         STATUS  current
         DESCRIPTION 
                 "Writing to this object initiates the upload/download or
                 schedules one. The extremeFileTransferStartOperStatus object
                 should be checked before attempting to set this object.
                 This object cannot be modified while the 
                 extremeFileTransferStartOperStatus is inProgress(3). This
		 object can be set start(1) only if the
		 extremeFileTransferStartOperStatus is idle(1). A scheduled
		 upload/download will be cancelled by setting the value of
		 this object to cancel(2)."
         DEFVAL { cancel }
        ::= { extremeFileTransferEntry 6}
	
extremeFileTransferStartOperStatus OBJECT-TYPE
        SYNTAX  INTEGER {
                  idle(1),
                  scheduled(2),
                  inProgress(3)
                }
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION 
		"The agent sets this value to reflect the current status of 
                the file transfer operation. Reading this object is meaningful 
                only if the extremeFileTransferRowStatus is active(1). The
		current status is determined by the agent by examining the
		values for extremeFileTransferOperation and
		extremeFileTransferStartAdminStatus."
        ::= { extremeFileTransferEntry 7 }

extremeFileTransferLastExecutionStatus OBJECT-TYPE
        SYNTAX  INTEGER { -- These values are from RMON-2
                    success(1),
                    statusUnknown(2),
                    generalError(3),
                    noResponseFromServer(4),
                    checksumError(5),
                    incompatibleImage(6),
                    tftpFileNotFound(7),
                    tftpAccessViolation(8),
		    fileTooLarge(9),
		    downloadInProgress(10)
                }
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION 
		"The  status of the last file transfer operation. This value 
                is returned as statusUnknown(1) until the
		extremeFileTransferRowStatus is set to active(1) or when the
		extremeFileTransferStartOperStatus is inProgress(3). After an
		upload/download, the agent will update this value with the
		result of the file transfer. Managers should read this object
		before modifying extremeFileTransferOperation because the
		agent would set this value to statusUnknown(2) in such cases."
        ::= { extremeFileTransferEntry 8 }

extremeFileTransferOwner OBJECT-TYPE
        SYNTAX  OwnerString(SIZE (0..32))
        MAX-ACCESS  read-create
        STATUS  current
        DESCRIPTION
                "Indicates the identity of the manager that configured this
                 file transfer entry."
        ::= { extremeFileTransferEntry 9 }

extremeFileTransferRowStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS  read-create
        STATUS  current
        DESCRIPTION
                "The status of this table entry. This object can not be
		modified while the extremeFileTransferStatus is inProgress(1).
		Setting this object to notInService(2) or destroy(6) will
		cancel any scheduled uploads if this entry was configured for
		one.

                Note that any attempts to create new rows which would result
		in multiple downloads would cause the row creation to fail.
		Similarly, attempting to delete a row while
		extremeFileTransferStartOperStatus is inProgress(3) would fail.
		Managers are strongly recommened to examine the
		extremeFileTransferStartOperStatus object for the entries in 
                the table to determine the status of downloads before
		attempting row creation/deletion."
        ::= { extremeFileTransferEntry 10 }

END

-- ===========================================================================

EXTREME-RTSTATS-MIB DEFINITIONS ::= BEGIN

	IMPORTS
                MODULE-IDENTITY, OBJECT-TYPE, TimeTicks,
                	Counter32 FROM SNMPv2-SMI
                extremeAgent    FROM EXTREME-BASE-MIB;

        extremeRtStats MODULE-IDENTITY
                LAST-UPDATED "9906240000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION 
                        "Extreme real time stats related objects"
        ::= { extremeAgent 11 }

          extremeRtStatsTable OBJECT-TYPE
              SYNTAX SEQUENCE OF ExtremeRtStatsEntry
              MAX-ACCESS not-accessible
              STATUS current
              DESCRIPTION
                  "A list of real time stats entries."
              ::= { extremeRtStats 1 }

          extremeRtStatsEntry OBJECT-TYPE
              SYNTAX ExtremeRtStatsEntry
              MAX-ACCESS not-accessible
              STATUS current
              DESCRIPTION
                  "The last sample of Ethernet statistics on a
                  particular Ethernet interface.  This sample is
                  associated with the RMON historyControlEntry 
		  which set up the parameters for a regular collection 
		  of these samples."
              INDEX { extremeRtStatsIndex }
              ::= { extremeRtStatsTable 1 }

          ExtremeRtStatsEntry ::= SEQUENCE {
              extremeRtStatsIndex               INTEGER (1..65535),
              extremeRtStatsIntervalStart       TimeTicks,
              extremeRtStatsCRCAlignErrors      Counter32,
              extremeRtStatsUndersizePkts       Counter32,
              extremeRtStatsOversizePkts        Counter32,
              extremeRtStatsFragments           Counter32,
              extremeRtStatsJabbers             Counter32,
              extremeRtStatsCollisions          Counter32,
              extremeRtStatsTotalErrors         Counter32,
              extremeRtStatsUtilization         INTEGER (0..10000)
          }

          extremeRtStatsIndex OBJECT-TYPE
              SYNTAX INTEGER (1..65535)
              MAX-ACCESS read-only
              STATUS current
              DESCRIPTION
                  "The history of which this entry is a part.  The
                  history identified by a particular value of this
                  index is the same history as identified by the same 
                  value of historyControlIndex of the RMON historyControl
                  table."
              ::= { extremeRtStatsEntry 1 }

          extremeRtStatsIntervalStart OBJECT-TYPE
              SYNTAX TimeTicks
              MAX-ACCESS read-only
              STATUS current
              DESCRIPTION
                  "The value of sysUpTime at the start of the interval
                  over which this sample was measured."
              ::= { extremeRtStatsEntry 2 }

          extremeRtStatsCRCAlignErrors OBJECT-TYPE
              SYNTAX Counter32
              MAX-ACCESS read-only
              STATUS current
              DESCRIPTION
                  "The number of packets received during the last 
		  sampling interval that had a length (excluding 
		  framing bits but including FCS octets) between 64 
		  and 1518 octets, inclusive, but had either a bad 
		  Frame Check Sequence (FCS) with an integral number 
		  of octets (FCS Error) or a bad FCS with a non-integral 
		  number of octets (Alignment Error)."
              ::= { extremeRtStatsEntry 3 }

          extremeRtStatsUndersizePkts OBJECT-TYPE
              SYNTAX Counter32
              MAX-ACCESS read-only
              STATUS current
              DESCRIPTION
                  "The number of packets received during the last
                  sampling interval that were less than 64 octets
                  long (excluding framing bits but including FCS
                  octets) and were otherwise well formed."
              ::= { extremeRtStatsEntry 4 }

          extremeRtStatsOversizePkts OBJECT-TYPE
              SYNTAX Counter32
              MAX-ACCESS read-only
              STATUS current
              DESCRIPTION
                  "The number of packets received during the 
                  last sampling interval that were longer than 
                  1518 octets (excluding framing bits but including
                  FCS octets) but were otherwise well formed."
              ::= { extremeRtStatsEntry 5 }

          extremeRtStatsFragments OBJECT-TYPE
              SYNTAX Counter32
              MAX-ACCESS read-only
              STATUS current
              DESCRIPTION
                  "The total number of packets received during the
                  last sampling interval that were less than 64 octets 
                  in length (excluding framing bits but including FCS
                  octets) had either a bad Frame Check Sequence (FCS)
                  with an integral number of octets (FCS Error) or a bad
                  FCS with a non-integral number of octets (Alignment
                  Error)."
              ::= { extremeRtStatsEntry 6 }

          extremeRtStatsJabbers OBJECT-TYPE
              SYNTAX Counter32
              MAX-ACCESS read-only
              STATUS current
              DESCRIPTION
                  "The number of packets received during the last
                  sampling interval that were longer than 1518 octets
                  (excluding framing bits but including FCS octets),
                  and  had either a bad Frame Check Sequence (FCS)
                  with an integral number of octets (FCS Error) or
                  a bad FCS with a non-integral number of octets
                  (Alignment Error)."
              ::= { extremeRtStatsEntry 7 }

          extremeRtStatsCollisions OBJECT-TYPE
              SYNTAX Counter32
              MAX-ACCESS read-only
              STATUS current
              DESCRIPTION
                  "The best estimate of the total number of collisions
                  on this Ethernet segment during this sampling
                  interval."
              ::= { extremeRtStatsEntry 8 }

          extremeRtStatsTotalErrors OBJECT-TYPE
              SYNTAX Counter32
              MAX-ACCESS read-only
              STATUS current
              DESCRIPTION
                  "The total number of errors on this Ethernet segment 
                  during this sampling interval. This is the sum of the
                  crc, fragments, jabbers and collisions counters over
                  this sampling interval."
              ::= { extremeRtStatsEntry 9 }

          extremeRtStatsUtilization OBJECT-TYPE
              SYNTAX INTEGER (0..10000)
              MAX-ACCESS read-only
              STATUS current
              DESCRIPTION
                  "The best estimate of the mean physical layer
                  network utilization on this interface during this
                  sampling interval, in hundredths of a percent."
              ::= { extremeRtStatsEntry 10 }


END

-- ==================================================================================
EXTREME-ESRP-MIB DEFINITIONS ::= BEGIN

        IMPORTS
                MODULE-IDENTITY         FROM SNMPv2-SMI
		RowStatus               FROM SNMPv2-TC
		MacAddress              FROM SNMPv2-TC
		OBJECT-TYPE             FROM SNMPv2-SMI
		IpAddress               FROM SNMPv2-SMI
                TruthValue              FROM SNMPv2-TC
                ExtremeGenAddr          FROM EXTREME-BASE-MIB
                extremeAgent            FROM EXTREME-BASE-MIB;

        extremeEsrp MODULE-IDENTITY
                LAST-UPDATED "0007240000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION "Extreme Standby Routing Protocol information"
        ::= { extremeAgent 12 }

	extremeEsrpTable	OBJECT-TYPE
		SYNTAX	SEQUENCE OF ExtremeEsrpEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
			"This table contains ESRP information for this device."
		::= { extremeEsrp 2 }

	extremeEsrpEntry	OBJECT-TYPE
		SYNTAX	ExtremeEsrpEntry
		MAX-ACCESS	not-accessible
		STATUS	current
		DESCRIPTION
			"An individual entry of this table contains ESRP information for				 a given vlan belonging to a given ESRP group."
		INDEX {extremeEsrpVlanIfIndex, extremeEsrpGroup}
		::= {extremeEsrpTable 1}

	ExtremeEsrpEntry ::= SEQUENCE {
                extremeEsrpVlanIfIndex        INTEGER,
                extremeEsrpGroup              INTEGER,
                extremeEsrpRowStatus          RowStatus,
                extremeEsrpNetAddress         ExtremeGenAddr,
                extremeEsrpState              INTEGER,
                extremeEsrpPriority           INTEGER,
                extremeEsrpElectionAlgorithm  INTEGER,
                extremeEsrpHelloTimer         INTEGER,
                extremeEsrpActivePorts        INTEGER,
                extremeEsrpTrackedActivePorts INTEGER,
                extremeEsrpTrackedIpRoutes    INTEGER,
                extremeEsrpTrackedPings       INTEGER,
                extremeEsrpNumTransitionsToMaster INTEGER,
                extremeEsrpNumTransitionsToSlave  INTEGER,
                extremeEsrpInternalActivePorts    INTEGER
        }

        extremeEsrpVlanIfIndex OBJECT-TYPE
                SYNTAX  INTEGER (1..65535)
                MAX-ACCESS	accessible-for-notify
                STATUS	current
                DESCRIPTION
                        "Any index to this table has a value that is
                        the same as the ifIndex of one of the vlans
                        present in the ifTable."
                ::= { extremeEsrpEntry 1 }

         extremeEsrpGroup OBJECT-TYPE
                SYNTAX	INTEGER (1..65535)
                MAX-ACCESS 	accessible-for-notify
                STATUS	current
                DESCRIPTION
                        "Indicates a gateway addresses this router backs
                        up. Any gateway address can be backed up by a
                        group of routers with one as the master and the
                        others as backup. An instance of this object 
                        refers to one such group. Only the default group
                        1 is supported currently."
                ::= { extremeEsrpEntry 2 }

          extremeEsrpRowStatus OBJECT-TYPE
                SYNTAX  RowStatus
                MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
                        "The status of this entry."
                ::= { extremeEsrpEntry 3 }
                
          extremeEsrpNetAddress OBJECT-TYPE
                SYNTAX  ExtremeGenAddr
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                        "The IP/IPX address of this vlan. This entry
                        is null if no address has been assigned to the
                        vlan."
                ::= { extremeEsrpEntry 4 }
                
          extremeEsrpState OBJECT-TYPE
                SYNTAX	INTEGER {
                        neutral(1),
                        master(2),
                        slave(3)
                }
        	MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                        "This indicates the ESRP state of this ESRP router."
                ::= { extremeEsrpEntry 5 }

        extremeEsrpPriority OBJECT-TYPE
                SYNTAX  INTEGER  (1..255)
                MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
                        "The priority which would be advertised by this
                        router for determining the esrp master."
                ::= { extremeEsrpEntry 6 }

         extremeEsrpElectionAlgorithm OBJECT-TYPE
                SYNTAX	INTEGER {
                        portsTrackPriorityMac(1),
                        trackPortsPriorityMac(2),
                        priorityPortsTrackMac(3),
		        priorityTrackPortsMac(4),
		        priorityMacOnly(5)
                }
                MAX-ACCESS read-create
                STATUS	current
                DESCRIPTION
                    "The algorithm to use in selecting the esrp master."
        ::= { extremeEsrpEntry 7 }

        extremeEsrpHelloTimer OBJECT-TYPE
                SYNTAX  INTEGER  (1..255)
                MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
                        "The time interval for exchanging hello messages."
                ::= { extremeEsrpEntry 8 }

        extremeEsrpActivePorts OBJECT-TYPE
                SYNTAX  INTEGER  (1..65535)
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                        "The number of physical ports that are in this
                        vlan."
                ::= { extremeEsrpEntry 9 }

        extremeEsrpTrackedActivePorts OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                        "The total number of ports belonging to the vlans
                        that are tracked by this esrp router."
                ::= { extremeEsrpEntry 10 }

        extremeEsrpTrackedIpRoutes OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                        "The total number of ip routes that are tracked
                        by this esrp router."
                ::= { extremeEsrpEntry 11 }

        extremeEsrpTrackedPings OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                        "The total number of ip addresses that are ping-tracked
                        by this esrp router."
                ::= { extremeEsrpEntry 12 }

        extremeEsrpNumTransitionsToMaster OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                        "The total number of transitions to Master
                        by this esrp router."
                ::= { extremeEsrpEntry 13 }

        extremeEsrpNumTransitionsToSlave OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                        "The total number of transitions to Slave
                        by this esrp router."
                ::= { extremeEsrpEntry 14 }

        extremeEsrpInternalActivePorts OBJECT-TYPE
                SYNTAX  INTEGER  (1..65535)
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                        "The number of internal physical ports that are
                        in this vlan."
                ::= { extremeEsrpEntry 15 }

	extremeEsrpNeighborTable	OBJECT-TYPE
		SYNTAX	SEQUENCE OF ExtremeEsrpNeighborEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
			"This table contains ESRP information received from the ESRP 
			 neighbors of this device."
		::= { extremeEsrp 3 }

	extremeEsrpNeighborEntry	OBJECT-TYPE
		SYNTAX	ExtremeEsrpNeighborEntry
		MAX-ACCESS	not-accessible
		STATUS	current
		DESCRIPTION
			"Each individual entry of this table contains ESRP information 
			of one ESRP neighbor."
		INDEX {extremeEsrpVlanIfIndex,
                       extremeEsrpGroup,
                       extremeEsrpNeighborMacAddress}
		::= {extremeEsrpNeighborTable 1}

	ExtremeEsrpNeighborEntry  ::= SEQUENCE {
                extremeEsrpNeighborMacAddress  MacAddress,
                extremeEsrpNeighborGroup       INTEGER,
                extremeEsrpNeighborNetAddress  ExtremeGenAddr,
                extremeEsrpNeighborState       INTEGER,
                extremeEsrpNeighborPriority    INTEGER,
                extremeEsrpNeighborElectionAlgorithm INTEGER,
                extremeEsrpNeighborHelloTimer  INTEGER,
                extremeEsrpNeighborActivePorts INTEGER,
                extremeEsrpNeighborTrackedActivePorts  INTEGER,
                extremeEsrpNeighborTrackedIpRoutes     INTEGER,
                extremeEsrpNeighborInternalActivePorts INTEGER
        }

        extremeEsrpNeighborMacAddress OBJECT-TYPE
                SYNTAX  MacAddress
                MAX-ACCESS  not-accessible
                STATUS current
                DESCRIPTION
                        "Mac address of other esrp routers that backup
                        this gateway address."
                ::= { extremeEsrpNeighborEntry 1 }

         extremeEsrpNeighborGroup OBJECT-TYPE
                SYNTAX	INTEGER (1..65535)
                MAX-ACCESS 	not-accessible
                STATUS	current
                DESCRIPTION
                        "Indicates a gateway addresses this router backs
                        up. Any gateway address can be backed up by a
                        group of routers with one as the master and the
                        others as backup. An instance of this object 
                        refers to one such group. Note that this object
                        is defined in addition to extremeEsrpGroup.
                        Whereas the extremeEsrpGroup refers to the group
                        information advertised by this host the
                        extremeEsrpNeighborGroup refers to the group
                        information reported by the neighbor. There
                        might be a conflict. Only the default group
                        1 is supported currently."
                ::= { extremeEsrpNeighborEntry 2 }

        extremeEsrpNeighborNetAddress OBJECT-TYPE
                SYNTAX  ExtremeGenAddr
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                        "The network layer address of this router. This
                        may be null if no address was assigned."
                ::= { extremeEsrpNeighborEntry 3 }

        extremeEsrpNeighborState OBJECT-TYPE
                SYNTAX	INTEGER {
                        neutral(1),
                        master(2),
                        slave(3)
                }
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                        "State of the esrp neighbor."
                ::= { extremeEsrpNeighborEntry 4 }

        extremeEsrpNeighborPriority OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                        "The priority reported by this esrp neighbor."
                ::= { extremeEsrpNeighborEntry 5 }

         extremeEsrpNeighborElectionAlgorithm OBJECT-TYPE
                SYNTAX	INTEGER {
                        portAndPriority(1),
                        priority(2),
                        priorityThenPort(3)
                }
                MAX-ACCESS read-only
                STATUS	current
                DESCRIPTION
                    "The algorithm to use in selecting the esrp master
                    reported by this esrp neighbor."
                ::= { extremeEsrpNeighborEntry 6 }

         extremeEsrpNeighborHelloTimer OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                        "The time interval for exchanging hello messages
                        configured at this esrp neighbor."
                ::= { extremeEsrpNeighborEntry 7 }

        extremeEsrpNeighborActivePorts OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                        "The number of physical ports that are in present
                        in the neighbor's vlan."
                ::= { extremeEsrpNeighborEntry 8 }

        extremeEsrpNeighborTrackedActivePorts OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                        "The total number of ports belonging to the vlans
                        that are tracked by this esrp neighbor."
                ::= { extremeEsrpNeighborEntry 9 }

        extremeEsrpNeighborTrackedIpRoutes OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                        "The total number of ip routes that are tracked
                        by this esrp neighbor."
                ::= { extremeEsrpNeighborEntry 10 }

        extremeEsrpNeighborInternalActivePorts OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                        "The number of internal ports that are in present
                        in the neighbor."
                ::= { extremeEsrpNeighborEntry 11 }

	extremeEsrpTrackVlanTable	OBJECT-TYPE
		SYNTAX	SEQUENCE OF ExtremeEsrpTrackVlanEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
			"A table containing information on the VLANs tracked by 
			this ESRP router."
		::= { extremeEsrp 4 }

	extremeEsrpTrackVlanEntry	OBJECT-TYPE
		SYNTAX	ExtremeEsrpTrackVlanEntry
		MAX-ACCESS	not-accessible
		STATUS	current
		DESCRIPTION
			"An entry in the table of tracked VLAN information."
		INDEX {extremeEsrpVlanIfIndex,
                       extremeEsrpGroup,
                       extremeEsrpTrackVlanIfIndex}
		::= {extremeEsrpTrackVlanTable 1}

	ExtremeEsrpTrackVlanEntry ::= SEQUENCE {
                extremeEsrpTrackVlanIfIndex INTEGER,
                extremeEsrpTrackVlanRowStatus RowStatus
        }

        extremeEsrpTrackVlanIfIndex OBJECT-TYPE
                SYNTAX  INTEGER   (1..65535)
                MAX-ACCESS  not-accessible
                STATUS current
                DESCRIPTION
                        "The ifIndex of the tracked vlan."
                ::= { extremeEsrpTrackVlanEntry 1 }

        extremeEsrpTrackVlanRowStatus OBJECT-TYPE
                SYNTAX  RowStatus
                MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
                        "The status of this entry."
                ::= { extremeEsrpTrackVlanEntry 2 }


	extremeEsrpTrackIpRouteTable	OBJECT-TYPE
		SYNTAX	SEQUENCE OF ExtremeEsrpTrackIpRouteEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
			"A table containing information on the IP routes tracked
			by this ESRP router."
		::= { extremeEsrp 5 }

	extremeEsrpTrackIpRouteEntry	OBJECT-TYPE
		SYNTAX	ExtremeEsrpTrackIpRouteEntry
		MAX-ACCESS	not-accessible
		STATUS	current
		DESCRIPTION
			"An entry in the table of tracked IP routes information."
		INDEX {extremeEsrpVlanIfIndex,
                       extremeEsrpGroup,
                       extremeEsrpTrackIpRouteIpAddress,
                       extremeEsrpTrackIpRouteNetMask}
		::= {extremeEsrpTrackIpRouteTable 1}

	ExtremeEsrpTrackIpRouteEntry ::= SEQUENCE {
                extremeEsrpTrackIpRouteIpAddress IpAddress,
                extremeEsrpTrackIpRouteNetMask   IpAddress,
                extremeEsrpTrackIpRouteRowStatus RowStatus
        }

        extremeEsrpTrackIpRouteIpAddress OBJECT-TYPE
                SYNTAX  IpAddress
                MAX-ACCESS  not-accessible
                STATUS current
                DESCRIPTION
                        "The ifIndex of the tracked vlan."
                ::= { extremeEsrpTrackIpRouteEntry 1 }

        extremeEsrpTrackIpRouteNetMask OBJECT-TYPE
                SYNTAX  IpAddress
                MAX-ACCESS  not-accessible
                STATUS current
                DESCRIPTION
                        "The ifIndex of the tracked vlan."
                ::= { extremeEsrpTrackIpRouteEntry 2 }

        extremeEsrpTrackIpRouteRowStatus OBJECT-TYPE
                SYNTAX  RowStatus
                MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
                        "The status of this entry."
                ::= { extremeEsrpTrackIpRouteEntry 3 }

	extremeEsrpPortTable	OBJECT-TYPE
		SYNTAX	SEQUENCE OF ExtremeEsrpPortEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
			"A table containing information on the ports belonging 
			to the ESRP vlans on this router."
		::= { extremeEsrp 6 }

	extremeEsrpPortEntry	OBJECT-TYPE
		SYNTAX	ExtremeEsrpPortEntry
		MAX-ACCESS	not-accessible
		STATUS	current
		DESCRIPTION
			"An entry in the table of ESRP port information."
		INDEX {extremeEsrpVlanIfIndex, extremeEsrpPortIfIndex}
		::= {extremeEsrpPortTable 1}

	ExtremeEsrpPortEntry ::= SEQUENCE {
                extremeEsrpPortIfIndex    INTEGER,
                extremeEsrpPortState      TruthValue
        }

        extremeEsrpPortIfIndex OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS  not-accessible
                STATUS current
                DESCRIPTION
                        "The ifIndex of the physical port that is part
                        of the vlan specified by the extremeEsrpVlanIfIndex."
                ::= { extremeEsrpPortEntry 1 }

        extremeEsrpPortState OBJECT-TYPE
                SYNTAX  TruthValue
                MAX-ACCESS  read-write
                STATUS current
                DESCRIPTION
                        "Indicates if esrp is enabled or disabled on this
                        port."
                ::= { extremeEsrpPortEntry 2 }


END

-- ===========================================================================

EXTREME-EDP-MIB DEFINITIONS ::= BEGIN

        IMPORTS
                MODULE-IDENTITY         FROM SNMPv2-SMI
		OBJECT-TYPE             FROM SNMPv2-SMI
		IpAddress               FROM SNMPv2-SMI
		ifIndex                 FROM RFC1213-MIB
		DisplayString           FROM RFC1213-MIB
                TruthValue              FROM SNMPv2-TC
                ExtremeDeviceId         FROM EXTREME-BASE-MIB
                extremeAgent            FROM EXTREME-BASE-MIB;


        extremeEdp MODULE-IDENTITY
                LAST-UPDATED "9910200000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION "Extreme Discovery Protocol information"
        ::= { extremeAgent 13 }

	extremeEdpTable	OBJECT-TYPE
		SYNTAX	SEQUENCE OF ExtremeEdpEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
			"This table contains EDP information of this device."
		::= { extremeEdp 2 }

	extremeEdpEntry	OBJECT-TYPE
		SYNTAX	ExtremeEdpEntry
		MAX-ACCESS	not-accessible
		STATUS	current
		DESCRIPTION
			"An entry in the table of EDP information of this device."
		INDEX {extremeEdpPortIfIndex, extremeEdpNeighborId}
		::= {extremeEdpTable 1}

	ExtremeEdpEntry ::= SEQUENCE {
                extremeEdpPortIfIndex             INTEGER,
                extremeEdpNeighborId              ExtremeDeviceId,
                extremeEdpNeighborName            DisplayString,
                extremeEdpNeighborSoftwareVersion DisplayString,
                extremeEdpNeighborSlot      	  INTEGER,
                extremeEdpNeighborPort      	  INTEGER,
                extremeEdpEntryAge        	  INTEGER
        }

        extremeEdpPortIfIndex OBJECT-TYPE
                SYNTAX  INTEGER (1..65535)
                MAX-ACCESS	accessible-for-notify
                STATUS	current
                DESCRIPTION
                        "The ifIndex of the physical port on which this
			entry was discovered via edp."
                ::= { extremeEdpEntry 1 }

        extremeEdpNeighborId  OBJECT-TYPE
                SYNTAX	ExtremeDeviceId
                MAX-ACCESS 	accessible-for-notify
                STATUS	current
                DESCRIPTION
                        "The identifier associated with the neighbor."
                ::= { extremeEdpEntry 2 }

        extremeEdpNeighborName  OBJECT-TYPE
		SYNTAX	DisplayString
                MAX-ACCESS 	read-only
                STATUS	current
                DESCRIPTION
                        "The identifier associated with the neighbor."
                ::= { extremeEdpEntry 3 }

        extremeEdpNeighborSoftwareVersion  OBJECT-TYPE
		SYNTAX	DisplayString
                MAX-ACCESS 	read-only
                STATUS	current
                DESCRIPTION
                        "The identifier associated with the neighbor."
                ::= { extremeEdpEntry 4 }

        extremeEdpNeighborSlot  OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS 	read-only
                STATUS	current
                DESCRIPTION
                        "The slot on which this neighbor received the
			edp message."
                ::= { extremeEdpEntry 5 }

        extremeEdpNeighborPort  OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS 	read-only
                STATUS	current
                DESCRIPTION
                        "The port on which this neighbor received the
			edp message."
                ::= { extremeEdpEntry 6 }

        extremeEdpEntryAge  OBJECT-TYPE
                SYNTAX	INTEGER
                MAX-ACCESS 	read-only
                STATUS	current
                DESCRIPTION
                        "The time in seconds since this entry was last
			updated."
                ::= { extremeEdpEntry 7 }


	extremeEdpNeighborTable	OBJECT-TYPE
		SYNTAX	SEQUENCE OF ExtremeEdpNeighborEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
			"This table contains EDP neighbor information."
		::= { extremeEdp 3 }

	extremeEdpNeighborEntry	OBJECT-TYPE
		SYNTAX	ExtremeEdpNeighborEntry
		MAX-ACCESS	not-accessible
		STATUS	current
		DESCRIPTION
			"An entry in the table of EDP Neighbor information."
		INDEX {extremeEdpPortIfIndex, extremeEdpNeighborId,
                       extremeEdpNeighborVlanName}
		::= {extremeEdpNeighborTable 1}

	ExtremeEdpNeighborEntry ::= SEQUENCE {
                extremeEdpNeighborVlanName      DisplayString,
                extremeEdpNeighborVlanId        INTEGER,
                extremeEdpNeighborVlanIpAddress IpAddress
        }

        extremeEdpNeighborVlanName  OBJECT-TYPE
		SYNTAX	DisplayString (SIZE(1..64))
                MAX-ACCESS 	not-accessible
                STATUS	current
                DESCRIPTION
                        "The name of the vlan configured on and reported
			by this edp neighbor."
                ::= { extremeEdpNeighborEntry 1 }

        extremeEdpNeighborVlanId  OBJECT-TYPE
		SYNTAX	INTEGER
                MAX-ACCESS 	read-only
                STATUS	current
                DESCRIPTION
                        "The vlan identifier associated with this vlan
			configured on this neighbor."
                ::= { extremeEdpNeighborEntry 2 }

        extremeEdpNeighborVlanIpAddress  OBJECT-TYPE
		SYNTAX	IpAddress
                MAX-ACCESS 	read-only
                STATUS	current
                DESCRIPTION
                        "The ip address of the reported vlan."
                ::= { extremeEdpNeighborEntry 3 }


	extremeEdpPortTable	OBJECT-TYPE
		SYNTAX	SEQUENCE OF ExtremeEdpPortEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
			""
		::= { extremeEdp 4 }

	extremeEdpPortEntry	OBJECT-TYPE
		SYNTAX	ExtremeEdpPortEntry
		MAX-ACCESS	not-accessible
		STATUS	current
		DESCRIPTION
			""
		INDEX {ifIndex}
		::= {extremeEdpPortTable 1}

	ExtremeEdpPortEntry ::= SEQUENCE {
                extremeEdpPortState      TruthValue
        }

        extremeEdpPortState OBJECT-TYPE
                SYNTAX  TruthValue
                MAX-ACCESS  read-write
                STATUS current
                DESCRIPTION
                        "Indicates if edp is enabled or disabled on this
                        port."
                ::= { extremeEdpPortEntry 1 }

END

-- ===========================================================================

EXTREME-SLB-MIB DEFINITIONS ::= BEGIN

	IMPORTS
		MODULE-IDENTITY		FROM SNMPv2-SMI
		OBJECT-TYPE		FROM SNMPv2-SMI
		IpAddress		FROM SNMPv2-SMI
		TruthValue		FROM SNMPv2-TC
		extremeAgent		FROM EXTREME-BASE-MIB;


	extremeSlb MODULE-IDENTITY
		LAST-UPDATED "0003080000Z"
		ORGANIZATION "Extreme Networks, Inc."
		CONTACT-INFO "www.extremenetworks.com"
		DESCRIPTION "Extreme Server Load Balancing information"
	::= { extremeAgent 14 }


	extremeSlbRealServerTable	OBJECT-TYPE
		SYNTAX	SEQUENCE OF ExtremeSlbRealServerEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
			"This table contains information about a real server.
			It currently indicates only whether the server is up."
		::= { extremeSlb 1 }

	extremeSlbRealServerEntry	OBJECT-TYPE
		SYNTAX	ExtremeSlbRealServerEntry
		MAX-ACCESS	not-accessible
		STATUS	current
		DESCRIPTION
			"An entry in the table of real server information."
		INDEX {extremeSlbRealServerIpAddress}
		::= {extremeSlbRealServerTable 1}

	ExtremeSlbRealServerEntry ::= SEQUENCE {
		extremeSlbRealServerIpAddress	IpAddress,
		extremeSlbRealServerUp		TruthValue
	}

	extremeSlbRealServerIpAddress	OBJECT-TYPE
		SYNTAX	IpAddress
		MAX-ACCESS 	not-accessible
		STATUS	current
		DESCRIPTION
			"The IP address of the real server."
		::= { extremeSlbRealServerEntry 1 }

	extremeSlbRealServerUp		OBJECT-TYPE
		SYNTAX	TruthValue
		MAX-ACCESS	read-write
		STATUS	current
		DESCRIPTION
			"Indicates whether the server is operational.
			If the server is up, the load balancer may send
			traffic to applications on the server.  If the
			server is not up, the load balancer will send no
			traffic to the server.  This status may be written
			by an external device that knows the state of the
			server."
		::= { extremeSlbRealServerEntry 2 }


	extremeSlbRealAppTable		OBJECT-TYPE
		SYNTAX	SEQUENCE OF ExtremeSlbRealAppEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
			"This table contains information about an application
			on a particular TCP or UDP port of a real server.
			It currently indicates only whether the application is
			up."
		::= { extremeSlb 2 }

	extremeSlbRealAppEntry		OBJECT-TYPE
		SYNTAX	ExtremeSlbRealAppEntry
		MAX-ACCESS	not-accessible
		STATUS	current
		DESCRIPTION
			"An entry in the table of real server application information."
		INDEX {extremeSlbRealAppIpAddress,
		       extremeSlbRealAppPort}
		::= {extremeSlbRealAppTable 1}

	ExtremeSlbRealAppEntry ::= SEQUENCE {
		extremeSlbRealAppIpAddress	IpAddress,
		extremeSlbRealAppPort		INTEGER (0..65535),
		extremeSlbRealAppUp		TruthValue
	}

	extremeSlbRealAppIpAddress	OBJECT-TYPE
		SYNTAX	IpAddress
		MAX-ACCESS 	not-accessible
		STATUS	current
		DESCRIPTION
			"The IP address of the real server."
		::= { extremeSlbRealAppEntry 1 }

	extremeSlbRealAppPort		OBJECT-TYPE
		SYNTAX	INTEGER (0..65535)
		MAX-ACCESS	not-accessible
		STATUS	current
		DESCRIPTION
			"The TCP or UDP port on the real server that the
			application is using."
		::= { extremeSlbRealAppEntry 2 }

	extremeSlbRealAppUp		OBJECT-TYPE
		SYNTAX	TruthValue
		MAX-ACCESS	read-write
		STATUS	current
		DESCRIPTION
			"Indicates whether the application is operational.
			If the application is up, the load balancer may
			send traffic to it.  If the application is not up,
			the load balancer will send no traffic to it, but
			the load balancer may send traffic to other
			applications on the same server."
		::= { extremeSlbRealAppEntry 3 }

END

-- ===========================================================================
EXTREME-OSPF-MIB DEFINITIONS ::= BEGIN

	IMPORTS
		MODULE-IDENTITY	FROM SNMPv2-SMI
		OBJECT-TYPE		FROM SNMPv2-SMI
		TruthValue		FROM SNMPv2-TC
		RowStatus               FROM SNMPv2-TC
		extremeAgent	        FROM EXTREME-BASE-MIB
		extremeVlanIfIndex      FROM EXTREME-VLAN-MIB
                IpAddress	        FROM SNMPv2-SMI;


	extremeOspf MODULE-IDENTITY
		LAST-UPDATED "0006280000Z"
		ORGANIZATION "Extreme Networks, Inc."
		CONTACT-INFO "www.extremenetworks.com"
		DESCRIPTION "Extreme specific OSPF information"
	::= { extremeAgent 15 }


	extremeOspfInterfaceTable	OBJECT-TYPE
		SYNTAX	SEQUENCE OF ExtremeOspfInterfaceEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
			"This table contains Extreme Networks specific information 
			about OSPF interfaces."
		::= { extremeOspf 1 }

	extremeOspfInterfaceEntry	OBJECT-TYPE
		SYNTAX	ExtremeOspfInterfaceEntry
		MAX-ACCESS	not-accessible
		STATUS	current
		DESCRIPTION
			"An entry in the table containing Extreme Networks specific 
			OSPF interface information."
		INDEX {extremeVlanIfIndex}
		::= {extremeOspfInterfaceTable 1}

	ExtremeOspfInterfaceEntry ::= SEQUENCE {
                extremeOspfAreaId               IpAddress,
		extremeOspfInterfacePassive	TruthValue,
                extremeOspfInterfaceStatus      RowStatus 
	}

        extremeOspfAreaId OBJECT-TYPE
            SYNTAX   IpAddress
            MAX-ACCESS   read-write
            STATUS   current
            DESCRIPTION
               "A 32-bit integer uniquely identifying an area.
               Area ID 0.0.0.0 is used for the OSPF backbone."
          ::= { extremeOspfInterfaceEntry 1 }



	extremeOspfInterfacePassive	OBJECT-TYPE
		SYNTAX	TruthValue
		MAX-ACCESS	read-write
		STATUS	current
		DESCRIPTION
			"Indicates whether the OSPF interface on this Vlan is
			Passive or not. Passive interfaces do not send routing
			updates. A true value indicates that the interface is passive."
		::= { extremeOspfInterfaceEntry 2 }

	extremeOspfInterfaceStatus OBJECT-TYPE
                SYNTAX  RowStatus
                MAX-ACCESS  read-create
                STATUS current
                DESCRIPTION
                        "The row status variable, used according to
                        row installation and removal conventions."
        ::= { extremeOspfInterfaceEntry 3 }

END

-- ============================================================================
EXTREME-FDB-MIB DEFINITIONS ::= BEGIN

      IMPORTS
                MODULE-IDENTITY         FROM SNMPv2-SMI
		    OBJECT-TYPE             FROM SNMPv2-SMI
		    IpAddress               FROM SNMPv2-SMI
                    Counter64		    FROM SNMPv2-SMI
                DisplayString, MacAddress, RowStatus       FROM SNMPv2-TC
                extremeAgent, PortList      FROM EXTREME-BASE-MIB;


        extremeFdb MODULE-IDENTITY
                LAST-UPDATED "0010310000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION "Extreme FDB and IP FDB tables."
        ::= { extremeAgent 16 }

	extremeFdbMacFdbTable	OBJECT-TYPE
		SYNTAX	SEQUENCE OF ExtremeFdbMacFdbEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
			"A table that contains information about the hardware MAC
			 FDB table."

		::= { extremeFdb 1 }

	extremeFdbMacFdbEntry	OBJECT-TYPE
		SYNTAX	ExtremeFdbMacFdbEntry
		MAX-ACCESS	not-accessible
		STATUS	current
		DESCRIPTION
			"An entry in the table of MAC FDB information."
		INDEX { extremeFdbMacFdbVlanIfIndex, extremeFdbMacFdbSequenceNumber }
		::= {extremeFdbMacFdbTable 1}

	ExtremeFdbMacFdbEntry ::= SEQUENCE {
		 extremeFdbMacFdbVlanIfIndex	 INTEGER,	
	         extremeFdbMacFdbSequenceNumber	 INTEGER,
                 extremeFdbMacFdbMacAddress	 MacAddress,
                 extremeFdbMacFdbPortIfIndex	 INTEGER,
                 extremeFdbMacFdbStatus		 INTEGER
              }

          extremeFdbMacFdbVlanIfIndex OBJECT-TYPE
              SYNTAX  INTEGER
              MAX-ACCESS  not-accessible
              STATUS  current
              DESCRIPTION
                      "The ifIndex of the Vlan on which this mac is learned."
              ::= { extremeFdbMacFdbEntry 1 }

        extremeFdbMacFdbSequenceNumber OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS	not-accessible
                STATUS	current
                DESCRIPTION
                        "The sequence number of this FDB entry in the forwarding database."
                ::= { extremeFdbMacFdbEntry 2 }

          extremeFdbMacFdbMacAddress OBJECT-TYPE
              SYNTAX  MacAddress
              MAX-ACCESS  read-only
              STATUS  current
              DESCRIPTION
                      "A MAC address for which the bridge has
                      forwarding and/or filtering information."
              ::= { extremeFdbMacFdbEntry 3 }

          extremeFdbMacFdbPortIfIndex OBJECT-TYPE
              SYNTAX  INTEGER
              MAX-ACCESS  read-only
              STATUS  current
              DESCRIPTION
                      "Either the value '0', or the IfIndex of the
                      port on which a frame having a source address
                      equal to the value of the corresponding instance
                      of dot1dTpFdbAddress has been seen.  A value of
                      '0' indicates that the port IfIndex has not been
                      learned but that the bridge does have some
                      forwarding/filtering information about this
                      address (e.g. in the dot1dStaticTable)."
              ::= { extremeFdbMacFdbEntry 4 }

          extremeFdbMacFdbStatus OBJECT-TYPE
              SYNTAX  INTEGER {
                          other(1),
                          invalid(2),
                          learned(3),
                          self(4),
                          mgmt(5)
                      }
              MAX-ACCESS  read-only
              STATUS  current
              DESCRIPTION
                      "The status of this entry.  
                      This is the value of dot1dTpFdbStatus in RFC1493."
              ::= { extremeFdbMacFdbEntry 5 }


	extremeFdbIpFdbTable	OBJECT-TYPE
		SYNTAX	SEQUENCE OF ExtremeFdbIpFdbEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
			"A table that contains information about the hardware IP
			 FDB table."
		::= { extremeFdb 2 }

	extremeFdbIpFdbEntry	OBJECT-TYPE
		SYNTAX	ExtremeFdbIpFdbEntry
		MAX-ACCESS	not-accessible
		STATUS	current
		DESCRIPTION
			"An entry in the table of IP FDB information."
		INDEX { extremeFdbIpFdbSequenceNumber }
		::= {extremeFdbIpFdbTable 1}

	ExtremeFdbIpFdbEntry ::= SEQUENCE {
		  extremeFdbIpFdbSequenceNumber  INTEGER,
	          extremeFdbIpFdbIPAddress	 IpAddress,
                  extremeFdbIpFdbMacAddress	 MacAddress,
		  extremeFdbIpFdbVlanIfIndex	 INTEGER,
                  extremeFdbIpFdbPortIfIndex	 INTEGER
              }


	extremeFdbIpFdbSequenceNumber OBJECT-TYPE
              SYNTAX  INTEGER
              MAX-ACCESS  not-accessible
              STATUS  current
              DESCRIPTION
                      "The sequence number of this entry in the IP FDB"
              ::= { extremeFdbIpFdbEntry 1 }

        extremeFdbIpFdbIPAddress OBJECT-TYPE
                SYNTAX  IpAddress
                MAX-ACCESS	read-only
                STATUS	current
                DESCRIPTION
                        "The IP Address of the IP FDB entry"
                ::= { extremeFdbIpFdbEntry 2 }

          extremeFdbIpFdbMacAddress OBJECT-TYPE
              SYNTAX  MacAddress
              MAX-ACCESS  read-only
              STATUS  current
              DESCRIPTION
                      "The MAC address corresponding to the IP Address."
              ::= { extremeFdbIpFdbEntry 3 }

        extremeFdbIpFdbVlanIfIndex OBJECT-TYPE
              SYNTAX  INTEGER
              MAX-ACCESS  read-only
              STATUS  current
              DESCRIPTION
                      "The ifIndex of the Vlan on which this ip is learned"
              ::= { extremeFdbIpFdbEntry 4 }

          extremeFdbIpFdbPortIfIndex OBJECT-TYPE
              SYNTAX  INTEGER
              MAX-ACCESS  read-only
              STATUS  current
              DESCRIPTION
                      "The IfIndex of the port on which this entry was learned"
              ::= { extremeFdbIpFdbEntry 5 }

	  extremeFdbPermFdbTable	OBJECT-TYPE
		SYNTAX          	SEQUENCE OF ExtremeFdbPermFdbEntry
		MAX-ACCESS		not-accessible
		STATUS			current
		DESCRIPTION
		"This table contains information on the secure-mac permanent FDB entries.
                It may later be extended to display other types of permanent FDB entries."

		::= { extremeFdb 3 }
	  
	  extremeFdbPermFdbEntry	OBJECT-TYPE
		SYNTAX			ExtremeFdbPermFdbEntry
		MAX-ACCESS		not-accessible
		STATUS          	current
		DESCRIPTION
		"An entry in the table of secure-mac permanent FDB information."

		INDEX { extremeFdbPermFdbFilterNum, 
                extremeFdbPermFdbMacAddress, extremeFdbPermFdbVlanId }
		::= { extremeFdbPermFdbTable 1 }

          ExtremeFdbPermFdbEntry ::= SEQUENCE {
                extremeFdbPermFdbFilterNum      INTEGER,
		extremeFdbPermFdbMacAddress	MacAddress,
	  	extremeFdbPermFdbVlanId		INTEGER,
		extremeFdbPermFdbPortList      	PortList,
		extremeFdbPermFdbFlags		BITS,
		extremeFdbPermFdbStatus 	RowStatus
              }

        extremeFdbPermFdbFilterNum	OBJECT-TYPE
                SYNTAX			INTEGER
                MAX-ACCESS		read-only
                STATUS        		current
                DESCRIPTION
                      "This object always returns 1. In future, it may be used to 
                      provide additional capability."
                ::= { extremeFdbPermFdbEntry 1 }


        extremeFdbPermFdbMacAddress	OBJECT-TYPE
                SYNTAX			MacAddress
                MAX-ACCESS		read-only
                STATUS        		current
                DESCRIPTION
                      "The is the MAC Address to which this FDB entry pertains."
                ::= { extremeFdbPermFdbEntry 2 }

        extremeFdbPermFdbVlanId		OBJECT-TYPE
              SYNTAX			INTEGER
              MAX-ACCESS		read-only
              STATUS            	current
              DESCRIPTION
                      "The VLAN ID of the VLAN to which this FDB entry pertains."
              ::= { extremeFdbPermFdbEntry 3 }

        extremeFdbPermFdbPortList	OBJECT-TYPE
              SYNTAX			PortList
              MAX-ACCESS		read-create
              STATUS			current
              DESCRIPTION
                      "This is the list of port(s) on which the given MAC Address is configured
                      Note that this port list is constructed assuming there are as many ports 
                      per slot as given in the object extremeChassisPortsPerSlot. 
                      Thus, if extremeChassisPortsPerSlot is 128, then the 129th bit in the port 
                      list (reading left to right) indicates port 2:1. Similarly, the 256th bit 
                      would indicate port 2:128 while the 257th bit would indicate port 3:1. Note 
                      especially that the bit positions in port list do not depend on the actual 
                      physical presence or absence of the given ports on the blade or of any 
                      blade itself."
                      
              ::= { extremeFdbPermFdbEntry 4 }


       extremeFdbPermFdbFlags		OBJECT-TYPE
            SYNTAX  BITS {
	                isSecure(0)
	         }                
	                
           MAX-ACCESS			read-create
           STATUS			current
           DESCRIPTION 
	       	"This object contains the flags associated with the FDB entry. The flags 
		are similar to those displayed on the device Command Line Interface. 
		At present, only the isSecure bit i.e. bit 0 will be supported and it will 
                always be ON since only secure-mac entries are configurable and displayed 
                in this table."
	    ::= { extremeFdbPermFdbEntry 5 }

       extremeFdbPermFdbStatus		OBJECT-TYPE
              SYNTAX			RowStatus                      
              MAX-ACCESS		read-create
              STATUS			current
              DESCRIPTION
                      "The status of this entry as per standard RowStatus conventions. 
                      Note however, that createAndWait and notInService states are not 
                      supported."

              ::= { extremeFdbPermFdbEntry 6 }


        extremeFdbMacFdbCounterTable    OBJECT-TYPE
              SYNTAX    SEQUENCE OF ExtremeFdbMacFdbCounterEntry
              MAX-ACCESS  not-accessible
              STATUS current
              DESCRIPTION
                  "A table that contains change counters for the Operational FDB.  
                   Each entry in the table corresponds to an individual port.  Whenever
                   a change occurs to the operational FDB (MAC learned, aged out or
                   removed), the counter associated with the port is incremented by one.
             
                   The counters are reset at agent startup and when the port is down.  
                   They are not cleared when the port is enabled or disabled."

              ::= { extremeFdb 5 }

        extremeFdbMacFdbCounterEntry    OBJECT-TYPE
              SYNTAX    ExtremeFdbMacFdbCounterEntry
              MAX-ACCESS    not-accessible
              STATUS    current
              DESCRIPTION
                   "An entry in the table of MAC FDB change counters."
              INDEX { extremeFdbMacFdbCounterPortIfIndex }
              ::= {extremeFdbMacFdbCounterTable 1}

        ExtremeFdbMacFdbCounterEntry ::= SEQUENCE {
              extremeFdbMacFdbCounterPortIfIndex     INTEGER,
              extremeFdbMacFdbCounterValue           Counter64
        }

        extremeFdbMacFdbCounterPortIfIndex OBJECT-TYPE
              SYNTAX  INTEGER
              MAX-ACCESS  not-accessible
              STATUS  current
              DESCRIPTION
                  "The ifIndex of the Port for which the counte applies."
              ::= { extremeFdbMacFdbCounterEntry 1 }

        extremeFdbMacFdbCounterValue OBJECT-TYPE
              SYNTAX  Counter64
              MAX-ACCESS read-only 
              STATUS  current
              DESCRIPTION
                      "The count of the number of FDB changes for the given port
                       since the counter was last reset."
              ::= { extremeFdbMacFdbCounterEntry 2 }

END
-- ===========================================================================

EXTREME-STP-EXTENSIONS-MIB DEFINITIONS ::= BEGIN

IMPORTS
	MODULE-IDENTITY, OBJECT-TYPE		FROM SNMPv2-SMI
        TruthValue		FROM SNMPv2-TC
	BridgeId, Timeout	FROM BRIDGE-MIB
	DisplayString		FROM RFC1213-MIB
	Counter32, TimeTicks	FROM SNMPv2-SMI
	RowStatus               FROM SNMPv2-TC
	extremeVlanIfIndex	FROM EXTREME-VLAN-MIB
	extremeAgent, PortList	FROM EXTREME-BASE-MIB
	NOTIFICATION-TYPE	FROM SNMPv2-SMI
        dot1dStpPort            FROM BRIDGE-MIB;

        extremeStp MODULE-IDENTITY
                LAST-UPDATED "0007240000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION "Extreme STP extensions"
        ::= { extremeAgent 17 }

	extremeStpDomainTable	OBJECT-TYPE
		SYNTAX						SEQUENCE OF ExtremeStpDomainEntry
		MAX-ACCESS					not-accessible
		STATUS						current
		DESCRIPTION
		"This table contains STP information per STP domain."
		::= { extremeStp 1 }

	extremeStpDomainEntry	OBJECT-TYPE
		SYNTAX						ExtremeStpDomainEntry
		MAX-ACCESS					not-accessible
		STATUS						current
		DESCRIPTION
		"An entry in the extremeStpDomain Table."
		INDEX		{ extremeStpDomainStpdInstance }
		::= { extremeStpDomainTable 1 }

	ExtremeStpDomainEntry ::= SEQUENCE {
		extremeStpDomainStpdInstance			INTEGER,
		extremeStpDomainStpdName			DisplayString,
		extremeStpDomainStpEnabled			TruthValue,
		extremeStpDomainRstpEnabled			TruthValue,
		extremeStpDomainStpdTag				INTEGER,
		extremeStpDomainNumPorts			INTEGER,
		extremeStpDomainBridgeId			BridgeId,
		extremeStpDomainBridgePriority			INTEGER,
		extremeStpDomainDesignatedRoot			BridgeId,
		extremeStpDomainRootPortIfIndex			INTEGER,
		extremeStpDomainRootCost			INTEGER,	
		extremeStpDomainRRFailoverEnabled		TruthValue,	
		extremeStpDomainMaxAge				Timeout,		
		extremeStpDomainHelloTime			Timeout,
		extremeStpDomainForwardDelay			Timeout,
		extremeStpDomainBridgeMaxAge			Timeout,
		extremeStpDomainBridgeHelloTime			Timeout,
		extremeStpDomainBridgeForwardDelay		Timeout,
		extremeStpDomainHoldTime			Timeout,
		extremeStpDomainTopChanges			Counter32,
		extremeStpDomainTimeSinceTopologyChange		TimeTicks,
		extremeStpDomainRowStatus			RowStatus
		}

		extremeStpDomainStpdInstance			OBJECT-TYPE
		SYNTAX						INTEGER
		MAX-ACCESS					accessible-for-notify
		STATUS						current
		DESCRIPTION
		"The unique identifier of this STP domain."
		::= { extremeStpDomainEntry 1 }

		extremeStpDomainStpdName			OBJECT-TYPE
		SYNTAX						DisplayString (SIZE(1..31))
		MAX-ACCESS					read-only
		STATUS						current
		DESCRIPTION
		"The name associated with this STP domain."
		::= { extremeStpDomainEntry 2 }

		extremeStpDomainStpEnabled			OBJECT-TYPE
		SYNTAX						TruthValue
		MAX-ACCESS					read-only
		STATUS						current
		DESCRIPTION
		"The Enabled/Disabled state of STP on this STP domain."
		::= { extremeStpDomainEntry 3 }


		extremeStpDomainRstpEnabled			OBJECT-TYPE
		SYNTAX						TruthValue
		MAX-ACCESS					read-only
		STATUS						current
		DESCRIPTION
		"The Enabled/Disabled state of Rapid STP on this STP domain."
		::= { extremeStpDomainEntry 4 }


		extremeStpDomainStpdTag				OBJECT-TYPE
		SYNTAX						INTEGER (1..4095)
		MAX-ACCESS					read-only
		STATUS						current
		DESCRIPTION
		"The StpdId of this STP domain which appears as the 802.1Q tag. Therefore, 
		it must be the VLAN tag of one of the wholly-contained VLANs of this STP
		domain."
		::= { extremeStpDomainEntry 5 }

		extremeStpDomainNumPorts			OBJECT-TYPE
		SYNTAX						INTEGER
		MAX-ACCESS					read-only
		STATUS						current
		DESCRIPTION
		"The number of physical ports belonging to this STP domain."
		::= { extremeStpDomainEntry 6 }

		extremeStpDomainBridgeId			OBJECT-TYPE
		SYNTAX						BridgeId
		MAX-ACCESS					read-only
		STATUS						current
		DESCRIPTION
		"The bridge identifier of this bridge for this STP domain."
		::= { extremeStpDomainEntry 7 }

		extremeStpDomainBridgePriority			OBJECT-TYPE
		SYNTAX						INTEGER (0..65535)
		MAX-ACCESS					read-only
		STATUS						current
		DESCRIPTION
		"The bridge priority of this bridge for this STP domain."
		::= { extremeStpDomainEntry 8 }

		extremeStpDomainDesignatedRoot			OBJECT-TYPE
		SYNTAX						BridgeId
		MAX-ACCESS					read-only
		STATUS						current
		DESCRIPTION
		"The root bridge identifier for this STP domain as determined by the STP
		running on this bridge for this STP domain"
		::= { extremeStpDomainEntry 9 }

		extremeStpDomainRootPortIfIndex			OBJECT-TYPE
		SYNTAX						INTEGER
		MAX-ACCESS					read-only
		STATUS						current
		DESCRIPTION
		"The port ifIndex of the root port of this bridge for this STP domain."
		::= { extremeStpDomainEntry 10 }

		extremeStpDomainRootCost			OBJECT-TYPE
		SYNTAX						INTEGER
		MAX-ACCESS					read-only
		STATUS						current
		DESCRIPTION
		"The cost of the path from this bridge to the root bridge of this STP domain"
		::= { extremeStpDomainEntry 11 }

		extremeStpDomainRRFailoverEnabled		OBJECT-TYPE
		SYNTAX						TruthValue
		MAX-ACCESS					read-only
		STATUS						current
		DESCRIPTION
		"The Enabled/Disabled state of Rapid Root Failover for this bridge on 
		this STP domain."
		::= { extremeStpDomainEntry 12 }

		extremeStpDomainMaxAge				OBJECT-TYPE
		SYNTAX						Timeout
		MAX-ACCESS					read-only
		STATUS						current
		DESCRIPTION
		"The maximum allowable age, in units of hundredths of a second, of STP 
		information learned by this bridge for this STP domain, after which it 
		is discarded. This is the value currently being used by the bridge."
		::= { extremeStpDomainEntry 13 }

		extremeStpDomainHelloTime			OBJECT-TYPE
		SYNTAX						Timeout
		MAX-ACCESS					read-only
		STATUS						current
		DESCRIPTION
		"The time, in hundredths of a second, between successive transmissions
		of Configuration BPDUs when this bridge is(or is trying to become) the 
		root bridge for this STP domain. This is the value currently being used
		by this bridge."
		::= { extremeStpDomainEntry 14 }

		extremeStpDomainForwardDelay			OBJECT-TYPE
		SYNTAX						Timeout
		MAX-ACCESS					read-only
		STATUS						current
		DESCRIPTION
		"The forward delay time, in hundredths of a second, currently
		being used by this bridge on this STP domain."
		::= { extremeStpDomainEntry 15 }

		extremeStpDomainBridgeMaxAge			OBJECT-TYPE
		SYNTAX						Timeout (600..4000)
		MAX-ACCESS					read-only
		STATUS						current
		DESCRIPTION
		"This is the value of MaxAge used by all other bridges in 
		this STP domain when this bridge is the root bridge."
		::= { extremeStpDomainEntry 16 }

		extremeStpDomainBridgeHelloTime			OBJECT-TYPE
		SYNTAX						Timeout (100..1000)
		MAX-ACCESS					read-only
		STATUS						current
		DESCRIPTION
		"This is the value of HelloTime used by all other bridges in
		this STP domain when this bridge is the root bridge."
		::= { extremeStpDomainEntry 17 }

		extremeStpDomainBridgeForwardDelay		OBJECT-TYPE
		SYNTAX						Timeout (400..3000)
		MAX-ACCESS					read-only
		STATUS						current
		DESCRIPTION
		"This is the value of ForwardDelay used by all other bridges in
		this STP domain when this bridge is the root bridge."

		::= { extremeStpDomainEntry 18 }

		extremeStpDomainHoldTime			OBJECT-TYPE
		SYNTAX						Timeout
		MAX-ACCESS					read-only
		STATUS						current
		DESCRIPTION
		"This is the Hold Time, in hundredths of a second, for this
		STP domain."
		::= { extremeStpDomainEntry 19 }

		extremeStpDomainTopChanges			OBJECT-TYPE
		SYNTAX						Counter32
		MAX-ACCESS					read-only
		STATUS						current
		DESCRIPTION
		"The number of topology changes detected by this bridge for
		this STP domain since the management entity was initialized
		or reset."
		::= { extremeStpDomainEntry 20 }

		extremeStpDomainTimeSinceTopologyChange		OBJECT-TYPE
		SYNTAX						TimeTicks
		MAX-ACCESS					read-only
		STATUS						current
		DESCRIPTION
		"The time, in hundredths of a second, since a topology change
		was last detected by this bridge for this STP domain."
		::= { extremeStpDomainEntry 21 }

		extremeStpDomainRowStatus			OBJECT-TYPE
		SYNTAX						RowStatus
		MAX-ACCESS					read-only
		STATUS						current
		DESCRIPTION
		"The status of this entry, as per standard RowStatus conventions."
		::= { extremeStpDomainEntry 22 }

		
	extremeStpPortTable			OBJECT-TYPE
		SYNTAX				SEQUENCE OF ExtremeStpPortEntry
		MAX-ACCESS			not-accessible
		STATUS				current
		DESCRIPTION
		"This table contains port-specific information per STP domain."
	::= { extremeStp 2 }

	extremeStpPortEntry			OBJECT-TYPE
		SYNTAX				ExtremeStpPortEntry
		MAX-ACCESS			not-accessible
		STATUS				current
		DESCRIPTION
		"An entry in the extremeStpPort table."
		INDEX		{ extremeStpDomainStpdInstance, extremeStpPortPortIfIndex }
		::= { extremeStpPortTable 1 }	

	ExtremeStpPortEntry ::= SEQUENCE {
		extremeStpPortPortIfIndex	INTEGER,
                extremeStpPortStpEnabled        TruthValue,
		extremeStpPortPortMode		INTEGER,
		extremeStpPortPortState		INTEGER,
		extremeStpPortPortPriority	INTEGER,
		extremeStpPortPortId		OCTET STRING,
		extremeStpPortPathCost		INTEGER,
		extremeStpPortDesignatedCost	INTEGER,
                extremeStpPortDesignatedRoot    BridgeId,
		extremeStpPortDesignatedBridge	BridgeId,
		extremeStpPortDesignatedPort	OCTET STRING,
		extremeStpPortRowStatus		RowStatus		
		}

	extremeStpPortPortIfIndex		OBJECT-TYPE
		SYNTAX				INTEGER
		MAX-ACCESS		        not-accessible
		STATUS				current
		DESCRIPTION
		"The ifIndex of the physical port for which this entry contains STP information."
		::= { extremeStpPortEntry 1 }

	extremeStpPortStpEnabled		OBJECT-TYPE
		SYNTAX				TruthValue
		MAX-ACCESS			read-only
		STATUS				current
		DESCRIPTION
		"The enabled/disabled state of this STP instance on this port."
		::= { extremeStpPortEntry 2 }


	extremeStpPortPortMode			OBJECT-TYPE
		SYNTAX				INTEGER { 
							dot1d(1), 
							emistp(2), 
							pvstp(3), 
							dot1w(4)
							}
		MAX-ACCESS				read-only
		STATUS					current
		DESCRIPTION
		"The port mode of this port in this STP domain."
		::= { extremeStpPortEntry 3 }

	extremeStpPortPortState			OBJECT-TYPE
		SYNTAX				INTEGER { 
							disabled(1),
							blocking(2),
							listening(3),
							learning(4),
							forwarding(5)
						}
									 
		MAX-ACCESS			read-only
		STATUS				current
		DESCRIPTION
		"The port state of this port in this STP domain."
		::= { extremeStpPortEntry 4 }

	extremeStpPortPortPriority		OBJECT-TYPE
		SYNTAX				INTEGER (0..31)
		MAX-ACCESS			read-only
		STATUS				current
		DESCRIPTION
		"The port priority of this port in this STP domain."
		::= { extremeStpPortEntry 5 }

	extremeStpPortPortId			OBJECT-TYPE
		SYNTAX				OCTET STRING (SIZE(2))
		MAX-ACCESS			read-only
		STATUS				current
		DESCRIPTION
		"The port identifier of this port in this STP domain."
		::= { extremeStpPortEntry 6 }

	extremeStpPortPathCost			OBJECT-TYPE
		SYNTAX				INTEGER (1..65535)
		MAX-ACCESS			read-only
		STATUS				current
		DESCRIPTION
		"The path cost of this port for this STP domain."
		::= { extremeStpPortEntry 7 }

	extremeStpPortDesignatedCost		OBJECT-TYPE
		SYNTAX				INTEGER
		MAX-ACCESS			read-only
		STATUS				current
		DESCRIPTION
		"The path cost, for this STP domain, of the Designated Port of the 
		segment connected to this port."
		::= { extremeStpPortEntry 8 }

        extremeStpPortDesignatedRoot            OBJECT-TYPE
                SYNTAX                          BridgeId
                MAX-ACCESS                      read-only
                STATUS                          current
                DESCRIPTION
                    "The root bridge identifier, for this STP domain, that is sent in the 
                    Configuration BPDUs transmitted by the Designated Bridge for the segment
                    to which this port is attached."
                ::= { extremeStpPortEntry 9 }

	extremeStpPortDesignatedBridge		OBJECT-TYPE
		SYNTAX				BridgeId
		MAX-ACCESS			read-only
		STATUS				current
		DESCRIPTION
		"The bridge identifier for the bridge considered to be the Designated Bridge,
		in this STP domain, for the segment connected to this port."
		::= { extremeStpPortEntry 10 }

	extremeStpPortDesignatedPort		OBJECT-TYPE
		SYNTAX				OCTET STRING(SIZE(2))
		MAX-ACCESS			read-only
		STATUS				current
		DESCRIPTION
		"The port identifier of the Designated Port on this port's segment, for this
		STP domain."
		::= { extremeStpPortEntry 11 }

	extremeStpPortRowStatus			OBJECT-TYPE
		SYNTAX				RowStatus
		MAX-ACCESS			read-only
		STATUS				current
		DESCRIPTION
		"The status of this entry, as per standard RowStatus conventions."
		::= { extremeStpPortEntry 12 }


	extremeStpVlanPortTable		OBJECT-TYPE
		SYNTAX			SEQUENCE OF ExtremeStpVlanPortEntry
		MAX-ACCESS		not-accessible
		STATUS			current
		DESCRIPTION
		"This table contains information of the ports belonging to a STP domain on a per VLAN basis."
		::= { extremeStp 3 }

	extremeStpVlanPortEntry		OBJECT-TYPE
		SYNTAX			ExtremeStpVlanPortEntry
		MAX-ACCESS		not-accessible
		STATUS			current
		DESCRIPTION
		"An entry in the extremeStpVlanPort table."
		INDEX		{ extremeVlanIfIndex, extremeStpDomainStpdInstance }
	::= { extremeStpVlanPortTable 1 }

	ExtremeStpVlanPortEntry ::= SEQUENCE {
		extremeStpVlanPortPortMask		PortList,
		extremeStpVlanPortRowStatus		RowStatus
		}

	extremeStpVlanPortPortMask	OBJECT-TYPE
	SYNTAX				PortList
	MAX-ACCESS			read-only
	STATUS				current
	DESCRIPTION
	"The list of ports in this STP domain and in this VLAN."
	::= { extremeStpVlanPortEntry 1 }

	extremeStpVlanPortRowStatus	OBJECT-TYPE
	SYNTAX				RowStatus
	MAX-ACCESS			read-only
	STATUS				current
	DESCRIPTION
	"The status of this entry, as per standard RowStatus conventions."
	::= { extremeStpVlanPortEntry 2 }

--
-- TRAP
--
         extremeStpTraps OBJECT IDENTIFIER
              ::= { extremeStp 4 }

	 extremeStpTrapsPrefix     OBJECT IDENTIFIER
          ::= { extremeStpTraps 0 }

        extremeStpEdgePortBlocked NOTIFICATION-TYPE 
           OBJECTS { dot1dStpPort  }
           STATUS current
           DESCRIPTION
                  "The extremeStpEdgePortBlocked notification is  
                   generated when the STP's edge port is
                   Blocked  due to the misconfiguration"
           ::= { extremeStpTrapsPrefix 1 }

END

-- ============================================================================

EXTREME-EAPS-MIB DEFINITIONS ::= BEGIN

        IMPORTS
                MODULE-IDENTITY         FROM SNMPv2-SMI
		OBJECT-TYPE             FROM SNMPv2-SMI
                DisplayString           FROM RFC1213-MIB
                extremeAgent            FROM EXTREME-BASE-MIB;

        extremeEaps MODULE-IDENTITY
                LAST-UPDATED "0007240000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION "Ethernet Automatic Protection Switching information"
        ::= { extremeAgent 18 }

	extremeEapsTable OBJECT-TYPE
		SYNTAX SEQUENCE OF ExtremeEapsEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"This table contains EAPS information about all EAPS
                         domains on this device."
		::= { extremeEaps 1 }

	extremeEapsEntry OBJECT-TYPE
		SYNTAX ExtremeEapsEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"An individual entry of this table contains EAPS 
                         information related to that EAPS domain."
		INDEX { extremeEapsName }
		::= { extremeEapsTable 1 }

	ExtremeEapsEntry ::= SEQUENCE {
		extremeEapsName		DisplayString (SIZE(0..32)),
		extremeEapsMode		INTEGER, 
		extremeEapsState	INTEGER
	}

        extremeEapsName  OBJECT-TYPE
            SYNTAX DisplayString (SIZE(0..32))
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The EAPS domain name."
	::= { extremeEapsEntry 1 }

        extremeEapsMode OBJECT-TYPE
                SYNTAX  INTEGER {
			invalid(0),
			master(1),
			transit(2)
		}
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                        "This indicates the mode of the EAPS domain."
                ::= { extremeEapsEntry 2 }

        extremeEapsState OBJECT-TYPE
                SYNTAX	INTEGER {
                        idle(0),
                        complete(1),
                        failed(2),
			linksup(3),
			linkdown(4),
			preforwarding(5),
			init(6)
                }
        	MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                        "This indicates the current EAPS state of this EAPS 
                         domain."
                ::= { extremeEapsEntry 3 }

        extremeEapsPrevState OBJECT-TYPE
                SYNTAX	INTEGER {
                        idle(0),
                        complete(1),
                        failed(2),
			linksup(3),
			linkdown(4),
			preforwarding(5),
			init(6)
                }
        	MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                        "This indicates the previous EAPS state of this EAPS 
                         domain. Used in state change traps information."
                ::= { extremeEaps 2 }

END

-- ===========================================================================

--
-- APS POS definitions
--
EXTREME-POS-MIB DEFINITIONS ::= BEGIN

	 IMPORTS
                MODULE-IDENTITY FROM SNMPv2-SMI
		OBJECT-TYPE     FROM SNMPv2-SMI
                Unsigned32	FROM SNMPv2-SMI
                TruthValue      FROM SNMPv2-TC
		DisplayString   FROM RFC1213-MIB
		IpAddress	FROM SNMPv2-SMI
                extremeAgent    FROM EXTREME-BASE-MIB
		PortList	FROM EXTREME-BASE-MIB;

        extremePOSMib MODULE-IDENTITY
                LAST-UPDATED "0007240000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION "Extreme POS objects: objects common to POS MIBs"
        ::= { extremeAgent 20 }


	extremeAps OBJECT IDENTIFIER
        ::= { extremePOSMib 1 }

        extremeApsConfig OBJECT IDENTIFIER
        ::= { extremeAps 1 }

        extremeApsConfigEnabled                         OBJECT-TYPE
                SYNTAX  TruthValue
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                "Global APS enablement"
        ::= { extremeApsConfig 1  }

--
-- APS Group Configuration Table
--

        extremeApsGroupConfigTable                      OBJECT-TYPE
                SYNTAX  SEQUENCE OF ExtremeApsGroupConfigEntry
                MAX-ACCESS  not-accessible
                STATUS current
                DESCRIPTION
                        "This table contains configuration information
                         by defined APS group."
                ::= { extremeApsConfig 2 }

        extremeApsGroupConfigEntry                      OBJECT-TYPE
                SYNTAX  ExtremeApsGroupConfigEntry
                MAX-ACCESS      not-accessible
                STATUS  current
                DESCRIPTION
                        ""
                INDEX {extremeApsGroupConfigGroupNumber}
                ::= {extremeApsGroupConfigTable 1}

        ExtremeApsGroupConfigEntry ::= SEQUENCE {
                extremeApsGroupConfigGroupNumber        INTEGER (1..65535),
                extremeApsGroupConfigRevertMode         INTEGER,
                extremeApsGroupConfigRevertMinutes      INTEGER (0..12),
                extremeApsGroupConfigDirection          INTEGER,
                extremeApsGroupConfigTimerInterval      INTEGER,
                extremeApsGroupConfigTimerMisses        INTEGER,
                extremeApsGroupConfigAuthenticate       TruthValue,
                extremeApsGroupConfigAuthString         DisplayString
        }

        extremeApsGroupConfigGroupNumber                OBJECT-TYPE
                SYNTAX  INTEGER (1..65535)
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The group number which uniquely identifies
                         the APS group."
                ::= { extremeApsGroupConfigEntry 1 }

        extremeApsGroupConfigRevertMode                 OBJECT-TYPE
                SYNTAX  INTEGER {
                                revertive (1),
                                nonRevertive (2)
                                }
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The revertive mode configured for the APS
                         group.  This indicates whether APS will
                         switch-back automatically after the working
                         line error is cleared.  In non-revertive
                         mode, manual intervention is required for
                         switch-back."
                ::= { extremeApsGroupConfigEntry 2 }

        extremeApsGroupConfigRevertMinutes              OBJECT-TYPE
                SYNTAX  INTEGER (0..12)
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The number of minutes APS will wait after
                         the error has been cleared before switching
                         back to the working line.  During this
                         interval, the K1 request will indicate
                         WTR (wait-to-restore).  This field is only
                         valid in revertive mode."
                ::= { extremeApsGroupConfigEntry 3 }

        extremeApsGroupConfigDirection                  OBJECT-TYPE
                SYNTAX  INTEGER {
                                bidirectional (1),
                                unidirectional (2)
                                }
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The directional mode configured for the
                         APS group.  This indicates whether protection
                         switches are coordinated between both POS
                         equipment and ADM (bidirectional) or not
                         (unidirectional)."
                ::= { extremeApsGroupConfigEntry 4 }

        extremeApsGroupConfigTimerInterval              OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The number of seconds between APS out-of-band
                         peer protocol hello messages.  This value is
                         relevant when the working line and protection
                         line exist is physically different chassis."
                ::= { extremeApsGroupConfigEntry 5 }

        extremeApsGroupConfigTimerMisses                OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The number of APS out-of-band peer protocol
                         messages transmitted without receiving a
                         response before the protection switch declares
                         the working switch inoperable.  When this occurs
                         the protection switch initiates a line switch
                         over via APS."
                ::= { extremeApsGroupConfigEntry 6 }

        extremeApsGroupConfigAuthenticate               OBJECT-TYPE
                SYNTAX  TruthValue
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "When enabled, the authentication string on both
                         working and protection switches must match."
                ::= { extremeApsGroupConfigEntry 7 }

        extremeApsGroupConfigAuthString                 OBJECT-TYPE
                SYNTAX  DisplayString (SIZE(0..8))
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "If configured, this is the authentication string
                         that must match between working and protection
                         switches.  This field is relevant if the APS group
                         is configured to authenticate."
                ::= { extremeApsGroupConfigEntry 8 }

--
-- APS Port Configuration Table
--

        extremeApsPortConfigTable                       OBJECT-TYPE
                SYNTAX  SEQUENCE OF ExtremeApsPortConfigEntry
                MAX-ACCESS  not-accessible
                STATUS current
                DESCRIPTION
                        "This table contains configuration information
                         for APS ports."
                ::= { extremeApsConfig 3 }

        extremeApsPortConfigEntry                       OBJECT-TYPE
                SYNTAX  ExtremeApsPortConfigEntry
                MAX-ACCESS      not-accessible
                STATUS  current
                DESCRIPTION
                        ""
                INDEX {extremeApsPortConfigGroupNumber,
                       extremeApsPortConfigPortNumber}
                ::= {extremeApsPortConfigTable 1}

        ExtremeApsPortConfigEntry ::= SEQUENCE {
                extremeApsPortConfigGroupNumber         INTEGER (1..65535),
                extremeApsPortConfigPortNumber          INTEGER,
                extremeApsPortConfigPortType            INTEGER
        }

        extremeApsPortConfigGroupNumber                 OBJECT-TYPE
                SYNTAX  INTEGER (1..65535)
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The group number which uniquely identifies
                         the APS group."
                ::= { extremeApsPortConfigEntry 1 }

        extremeApsPortConfigPortNumber                  OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The value of ifIndex that identifies the port."
                ::= { extremeApsPortConfigEntry 2 }

        extremeApsPortConfigPortType                    OBJECT-TYPE
                SYNTAX  INTEGER {
                                working (1),
                                protection (2)
                                }
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The port type designation."
                ::= { extremeApsPortConfigEntry 3 }

--
-- APS Protection Port Additional Configuration Table
--

        extremeApsProtectPortConfigTable                OBJECT-TYPE
                SYNTAX  SEQUENCE OF ExtremeApsProtectPortConfigEntry
                MAX-ACCESS  not-accessible
                STATUS current
                DESCRIPTION
                        "This table contains configuration information
                         for APS protection ports."
                ::= { extremeApsConfig 4 }

        extremeApsProtectPortConfigEntry                OBJECT-TYPE
                SYNTAX  ExtremeApsProtectPortConfigEntry
                MAX-ACCESS      not-accessible
                STATUS  current
                DESCRIPTION
                        ""
                INDEX {extremeApsProtectPortConfigGroupNumber,
                       extremeApsProtectPortConfigPortNumber}
                ::= {extremeApsProtectPortConfigTable 1}

        ExtremeApsProtectPortConfigEntry ::= SEQUENCE {
                extremeApsProtectPortConfigGroupNumber   INTEGER (1..65535),
                extremeApsProtectPortConfigPortNumber    INTEGER,
                extremeApsProtectPortConfigWorkingIpAddr IpAddress
        }

        extremeApsProtectPortConfigGroupNumber          OBJECT-TYPE
                SYNTAX  INTEGER (1..65535)
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The group number which uniquely identifies
                         the APS group."
                ::= { extremeApsProtectPortConfigEntry 1 }

        extremeApsProtectPortConfigPortNumber           OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The value of ifIndex that identifies
                         the protection port."
                ::= { extremeApsProtectPortConfigEntry 2 }

        extremeApsProtectPortConfigWorkingIpAddr        OBJECT-TYPE
                SYNTAX  IpAddress
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The IP address of the working switch.  If the
                         working and protection lines reside on the same
                         chassis, this IP address will be a local address."
                ::= { extremeApsProtectPortConfigEntry 3 }

        extremeApsStatus OBJECT IDENTIFIER
        ::= { extremeAps 2 }

--
-- APS Group Status Table
--
        extremeApsGroupTable                            OBJECT-TYPE
                SYNTAX  SEQUENCE OF ExtremeApsGroupEntry
                MAX-ACCESS  not-accessible
                STATUS current
                DESCRIPTION
                        "This table contains run-time information
                         by defined APS group."
                ::= { extremeApsStatus 1 }

        extremeApsGroupEntry                            OBJECT-TYPE
                SYNTAX  ExtremeApsGroupEntry
                MAX-ACCESS      not-accessible
                STATUS  current
                DESCRIPTION
                        ""
                INDEX {extremeApsGroupGroupNumber}
                ::= {extremeApsGroupTable 1}

        ExtremeApsGroupEntry ::= SEQUENCE {
                extremeApsGroupGroupNumber              INTEGER (1..65535),
                extremeApsGroupActivePort               INTEGER,
                extremeApsGroupEffectiveDirection       INTEGER,
                extremeApsGroupPeerProtoStatus          INTEGER
        }

        extremeApsGroupGroupNumber                      OBJECT-TYPE
                SYNTAX  INTEGER (1..65535)
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The group number which uniquely identifies
                         the APS group."
                ::= { extremeApsGroupEntry 1 }

        extremeApsGroupActivePort                       OBJECT-TYPE
                SYNTAX  INTEGER {
                                working (1),
                                protection (2)
                                }
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The APS port which is currently carrying the
                         network traffic."
                ::= { extremeApsGroupEntry 2 }

        extremeApsGroupEffectiveDirection               OBJECT-TYPE
                SYNTAX  INTEGER {
                                bidirectional (1),
                                unidirectional (2)
                                }
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The effective directional mode for the APS
                         group.  When this value differs from the
                         configured directional mode, check the
                         ADM and switch provisioning for a mis-
                         configuration."
                ::= { extremeApsGroupEntry 3 }

        extremeApsGroupPeerProtoStatus                  OBJECT-TYPE
                SYNTAX  INTEGER {
                                established (1),
                                closed (2)
                                }
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The APS out-of-band peer protocol status
                         for a group."
                ::= { extremeApsGroupEntry 4 }

--
-- APS Protection Port Table
--

        extremeApsProtectPortTable                      OBJECT-TYPE
                SYNTAX  SEQUENCE OF ExtremeApsProtectPortEntry
                MAX-ACCESS  not-accessible
                STATUS current
                DESCRIPTION
                        "This table contains run-time information
                         by defined APS protection port."
                ::= { extremeApsStatus 2 }

        extremeApsProtectPortEntry                      OBJECT-TYPE
                SYNTAX  ExtremeApsProtectPortEntry
                MAX-ACCESS      not-accessible
                STATUS  current
                DESCRIPTION
                        ""
                INDEX {extremeApsProtectPortGroupNumber,
                       extremeApsProtectPortPortNumber}
                ::= {extremeApsProtectPortTable 1}

        ExtremeApsProtectPortEntry ::= SEQUENCE {
                extremeApsProtectPortGroupNumber         INTEGER (1..65535),
                extremeApsProtectPortPortNumber          INTEGER,
                extremeApsProtectPortTransmitK1          OCTET STRING,
                extremeApsProtectPortTransmitK2          OCTET STRING,
                extremeApsProtectPortReceiveK1           OCTET STRING,
                extremeApsProtectPortReceiveK2           OCTET STRING,
                extremeApsProtectPortSwitchInitByWorking INTEGER,
                extremeApsProtectPortSwitchInitByProtect INTEGER,
                extremeApsProtectPortSwitchInitByADM     INTEGER,
                extremeApsProtectPortSwitchInitByCmd     INTEGER,
                extremeApsProtectPortSuccessfulSwitches  INTEGER,
                extremeApsProtectPortHelloProtFails      INTEGER

        }

        extremeApsProtectPortGroupNumber                OBJECT-TYPE
                SYNTAX  INTEGER (1..65535)
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The group number which uniquely identifies
                         the APS group."
                ::= { extremeApsProtectPortEntry 1 }

        extremeApsProtectPortPortNumber                 OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                         "The value of ifIndex that identifies
                          the protection port."
                ::= { extremeApsProtectPortEntry 2 }

        extremeApsProtectPortTransmitK1                 OBJECT-TYPE
                SYNTAX  OCTET STRING (SIZE(1))
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                         "The K1 overhead byte currently being transmitted
                          on the indicated protection port."
                ::= { extremeApsProtectPortEntry 3 }

        extremeApsProtectPortTransmitK2                 OBJECT-TYPE
                SYNTAX  OCTET STRING (SIZE(1))
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                         "The K2 overhead byte currently being transmitted
                          on the indicated protection port."
                ::= { extremeApsProtectPortEntry 4 }

        extremeApsProtectPortReceiveK1                  OBJECT-TYPE
                SYNTAX  OCTET STRING (SIZE(1))
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                         "The K1 overhead byte currently being received
                          on the indicated protection port."
                ::= { extremeApsProtectPortEntry 5 }

        extremeApsProtectPortReceiveK2                  OBJECT-TYPE
                SYNTAX  OCTET STRING (SIZE(1))
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                         "The K2 overhead byte currently being received
                          on the indicated protection port."
                ::= { extremeApsProtectPortEntry 6 }

        extremeApsProtectPortSwitchInitByWorking        OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                         "The number of switches that have been
                          initiated by the working-line router."
                ::= { extremeApsProtectPortEntry 7 }

        extremeApsProtectPortSwitchInitByProtect        OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                         "The number of switches that have been
                          initiated by the protection-line router."
                ::= { extremeApsProtectPortEntry 8 }

        extremeApsProtectPortSwitchInitByADM            OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                         "The number of switches that have been
                          initiated by the ADM."
                ::= { extremeApsProtectPortEntry 9 }
        extremeApsProtectPortSwitchInitByCmd            OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                         "The number of switches that have been
                          initiated by an external CLI command."
                ::= { extremeApsProtectPortEntry 10 }
        extremeApsProtectPortSuccessfulSwitches         OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                         "The number of successful APS line switches."
                ::= { extremeApsProtectPortEntry 11 }
        extremeApsProtectPortHelloProtFails             OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                         "The number of APS out-of-band peer protocol
                          failures recorded.  This situation causes
                          the protection-line router to initiate a
                          line switch."
                ::= { extremeApsProtectPortEntry 12 }

        extremeApsErrors OBJECT IDENTIFIER
        ::= { extremeAps 3 }

--
-- APS Line Errors Table
--

        extremeApsLineErrorTable                        OBJECT-TYPE
                SYNTAX  SEQUENCE OF ExtremeApsLineErrorEntry
                MAX-ACCESS  not-accessible
                STATUS current
                DESCRIPTION
                        "This table contains APS line error
                         information."
                ::= { extremeApsErrors 1 }

        extremeApsLineErrorEntry                        OBJECT-TYPE
                SYNTAX  ExtremeApsLineErrorEntry
                MAX-ACCESS      not-accessible
                STATUS  current
                DESCRIPTION
                        ""
                INDEX {extremeApsLineErrorGroupNumber,
                       extremeApsLineErrorPortNumber}
                ::= {extremeApsLineErrorTable 1}

        ExtremeApsLineErrorEntry ::= SEQUENCE {
                extremeApsLineErrorGroupNumber            INTEGER (1..65535),
                extremeApsLineErrorPortNumber             INTEGER,
                extremeApsLineErrorSignalDegradeActive    TruthValue,
                extremeApsLineErrorBERSignalDegradeActive TruthValue,
                extremeApsLineErrorSignalFailActive       TruthValue,
                extremeApsLineErrorBERSignalFailActive    TruthValue,
                extremeApsLineErrorSignalDegrades         INTEGER,
                extremeApsLineErrorBERSignalDegrades      INTEGER,
                extremeApsLineErrorSignalFails            INTEGER,
                extremeApsLineErrorBERSignalFails         INTEGER
        }

        extremeApsLineErrorGroupNumber                  OBJECT-TYPE
                SYNTAX  INTEGER (1..65535)
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The group number which uniquely identifies the
                         APS group."
                ::= { extremeApsLineErrorEntry 1 }

        extremeApsLineErrorPortNumber                   OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The ifIndex value which identifies the APS port."
                ::= { extremeApsLineErrorEntry 2 }

        extremeApsLineErrorSignalDegradeActive          OBJECT-TYPE
                SYNTAX  TruthValue
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "Indicates whether a signal degrade condition
                         currently exists on the line."
                ::= { extremeApsLineErrorEntry 3 }

        extremeApsLineErrorBERSignalDegradeActive       OBJECT-TYPE
                SYNTAX  TruthValue
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "Indicates whether a signal degrade condition
                         due to excessive Bit-Error-Rate currently exists
                         on the line."
                ::= { extremeApsLineErrorEntry 4 }

        extremeApsLineErrorSignalFailActive             OBJECT-TYPE
                SYNTAX  TruthValue
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "Indicates whether a signal fail condition
                         currently exists on the line."
                ::= { extremeApsLineErrorEntry 5 }

        extremeApsLineErrorBERSignalFailActive          OBJECT-TYPE
                SYNTAX  TruthValue
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "Indicates whether a signal fail condition
                         due to excessive Bit-Error-Rate currently
                         exists on the line."
                ::= { extremeApsLineErrorEntry 6 }

        extremeApsLineErrorSignalDegrades               OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The number of signal degrades that have
                         been recorded on the line."
                ::= { extremeApsLineErrorEntry 7 }

        extremeApsLineErrorBERSignalDegrades            OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The number of signal degrades due to excessive
                         Bit-Error-Rate that have been recorded on the
                         line."
                ::= { extremeApsLineErrorEntry 8 }

        extremeApsLineErrorSignalFails                  OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The number of signal fails that have
                         been recorded on the line."
                ::= { extremeApsLineErrorEntry 9 }

        extremeApsLineErrorBERSignalFails               OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The number of signal fails due to excessive
                         Bit-Error-Rate that have been recorded on the
                         line."
                ::= { extremeApsLineErrorEntry 10 }

--
-- APS Protocol Errors Table
--

        extremeApsProtocolErrorTable                    OBJECT-TYPE
                SYNTAX  SEQUENCE OF ExtremeApsProtocolErrorEntry
                MAX-ACCESS  not-accessible
                STATUS current
                DESCRIPTION
                        "This table contains APS protocol error
                         information.  These errors are relevant
                         for APS protection ports."
                ::= { extremeApsErrors 2 }

        extremeApsProtocolErrorEntry                    OBJECT-TYPE
                SYNTAX  ExtremeApsProtocolErrorEntry
                MAX-ACCESS      not-accessible
                STATUS  current
                DESCRIPTION
                        ""
                INDEX {extremeApsProtocolErrorGroupNumber,
                       extremeApsProtocolErrorPortNumber}
                ::= {extremeApsProtocolErrorTable 1}

        ExtremeApsProtocolErrorEntry ::= SEQUENCE {
                extremeApsProtocolErrorGroupNumber             INTEGER (1..65535),
                extremeApsProtocolErrorPortNumber              INTEGER,
                extremeApsProtocolErrorModeMismatchDefect      TruthValue,
                extremeApsProtocolErrorProtSwitchByteDefect    TruthValue,
                extremeApsProtocolErrorChannelMismatchDefect   TruthValue,
                extremeApsProtocolErrorFarEndProtectDefect     TruthValue,
                extremeApsProtocolErrorModeMismatchFailure     TruthValue,
                extremeApsProtocolErrorProtSwitchByteFailure   TruthValue,
                extremeApsProtocolErrorChannelMismatchFailure  TruthValue,
                extremeApsProtocolErrorFarEndProtectFailure    TruthValue,
                extremeApsProtocolErrorModeMismatchNumFails    INTEGER,
                extremeApsProtocolErrorProtSwitchByteNumFails  INTEGER,
                extremeApsProtocolErrorChannelMismatchNumFails INTEGER,
                extremeApsProtocolErrorFarEndProtectNumFails   INTEGER
        }

        extremeApsProtocolErrorGroupNumber              OBJECT-TYPE
                SYNTAX  INTEGER (1..65535)
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The group number which uniquely identifies the
                         APS group."
                ::= { extremeApsProtocolErrorEntry 1 }

        extremeApsProtocolErrorPortNumber               OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The ifIndex value which identifies the APS
                         protection port."
                ::= { extremeApsProtocolErrorEntry 2 }

        extremeApsProtocolErrorModeMismatchDefect       OBJECT-TYPE
                SYNTAX  TruthValue
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "Indicates whether a Mode Mismatch defect currently
                         exists on the port."
                ::= { extremeApsProtocolErrorEntry 3 }

        extremeApsProtocolErrorProtSwitchByteDefect     OBJECT-TYPE
                SYNTAX  TruthValue
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "Indicates whether a Protection Switching Byte defect
                         currently exists on the port."
                ::= { extremeApsProtocolErrorEntry 4 }

        extremeApsProtocolErrorChannelMismatchDefect    OBJECT-TYPE
                SYNTAX  TruthValue
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "Indicates whether a Channel Mismatch defect currently
                         exists on the port."
                ::= { extremeApsProtocolErrorEntry 5 }

        extremeApsProtocolErrorFarEndProtectDefect      OBJECT-TYPE
                SYNTAX  TruthValue
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "Indicates whether a Far-End Protection defect currently
                         exists on the port."
                ::= { extremeApsProtocolErrorEntry 6 }

        extremeApsProtocolErrorModeMismatchFailure      OBJECT-TYPE
                SYNTAX  TruthValue
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "Indicates whether a Mode Mismatch failure currently
                         exists on the port."
                ::= { extremeApsProtocolErrorEntry 7 }

        extremeApsProtocolErrorProtSwitchByteFailure    OBJECT-TYPE
                SYNTAX  TruthValue
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "Indicates whether a Protection Switching Byte failure
                         currently exists on the port."
                ::= { extremeApsProtocolErrorEntry 8 }

        extremeApsProtocolErrorChannelMismatchFailure   OBJECT-TYPE
                SYNTAX  TruthValue
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "Indicates whether a Channel Mismatch failure currently
                         exists on the port."
                ::= { extremeApsProtocolErrorEntry 9 }

        extremeApsProtocolErrorFarEndProtectFailure     OBJECT-TYPE
                SYNTAX  TruthValue
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "Indicates whether a Far-End Protection failure currently
                         exists on the port."
                ::= { extremeApsProtocolErrorEntry 10 }

        extremeApsProtocolErrorModeMismatchNumFails     OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The number of Mode Mismatch failures that have
                         been recorded."
                ::= { extremeApsProtocolErrorEntry 11 }

        extremeApsProtocolErrorProtSwitchByteNumFails   OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The number of Protection Switching Byte failures
                         that have been recorded."
                ::= { extremeApsProtocolErrorEntry 12 }

        extremeApsProtocolErrorChannelMismatchNumFails  OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The number of Channel Mismatch failures that have
                         been recorded."
                ::= { extremeApsProtocolErrorEntry 13 }

        extremeApsProtocolErrorFarEndProtectNumFails    OBJECT-TYPE
                SYNTAX  INTEGER
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The number of Far-End Protection failures that have
                         been recorded."
                ::= { extremeApsProtocolErrorEntry 14 }

END
		
--- Extreme NetFlow has moved under extremeAgent tree; as extremeAgent.22 
-- ============================================================================
EXTREME-NETFLOW-MIB DEFINITIONS ::= BEGIN

      IMPORTS
                MODULE-IDENTITY         FROM SNMPv2-SMI
		    OBJECT-TYPE             FROM SNMPv2-SMI
		    IpAddress               FROM SNMPv2-SMI
                MacAddress              FROM SNMPv2-TC
                TruthValue          FROM SNMPv2-TC
                extremeAgent            FROM EXTREME-BASE-MIB;


        extremeNetFlow MODULE-IDENTITY
                LAST-UPDATED "0010310000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION "Extreme NetFlow tables."
        ::= { extremeAgent 22 }

        extremeNetFlowConfigPort OBJECT IDENTIFIER
        ::= { extremeNetFlow 1 }

        extremeNetFlowConfigGroup OBJECT IDENTIFIER
        ::= { extremeNetFlow 2 }


        extremeNetFlowGroupCollectorTable                  OBJECT-TYPE
                SYNTAX  SEQUENCE OF ExtremeNetFlowGroupCollectorEntry
                MAX-ACCESS  not-accessible
                STATUS current
                DESCRIPTION
                        "This table contains configuration information
                         for a defined NetFlow group flow entry."
                ::= { extremeNetFlowConfigGroup 2 }

        extremeNetFlowGroupCollectorEntry                      OBJECT-TYPE
                SYNTAX   ExtremeNetFlowGroupCollectorEntry
                MAX-ACCESS      not-accessible
                STATUS  current
                DESCRIPTION
                        ""
                INDEX {extremeNetFlowGroupNumber,
                       extremeNetFlowCollectorId}
                ::= {extremeNetFlowGroupCollectorTable 1}


        ExtremeNetFlowGroupCollectorEntry ::= SEQUENCE {
                extremeNetFlowGroupNumber             INTEGER,
                extremeNetFlowCollectorId             INTEGER,
                extremeNetFlowGroupPingEnabled        TruthValue,
                extremeNetFlowGroupSourceIp           IpAddress,
                extremeNetFlowCollectorIpAddress      IpAddress,
                extremeNetFlowCollectorUdpPort        INTEGER,
                extremeNetFlowCollectorStatusUp       TruthValue,
                extremeNetFlowCollectorDowntime       INTEGER,
		extremeNetFlowCollectorPacketsTx      INTEGER
        }

        extremeNetFlowGroupNumber                   OBJECT-TYPE
                SYNTAX  INTEGER (1..32)
                MAX-ACCESS      not-accessible
                STATUS  current
                DESCRIPTION
                        "The group number."
                ::= { extremeNetFlowGroupCollectorEntry 1 }

        extremeNetFlowCollectorId               OBJECT-TYPE
                SYNTAX  INTEGER (1..8)
                MAX-ACCESS      not-accessible
                STATUS  current
                DESCRIPTION
                        "The collector number."
                ::= { extremeNetFlowGroupCollectorEntry 2 }

        extremeNetFlowGroupPingEnabled        OBJECT-TYPE
                SYNTAX  TruthValue
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                        "Flag indicating if ping is enabled for the group"
                ::= { extremeNetFlowGroupCollectorEntry 3 }

        extremeNetFlowGroupSourceIp              OBJECT-TYPE
                SYNTAX  IpAddress
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                        "Source IP address for the group."
                ::= { extremeNetFlowGroupCollectorEntry 4 }

        extremeNetFlowCollectorIpAddress              OBJECT-TYPE
                SYNTAX  IpAddress
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                        "The collector's configured IP address."
                ::= { extremeNetFlowGroupCollectorEntry 5 }

        extremeNetFlowCollectorUdpPort                        OBJECT-TYPE
                SYNTAX  INTEGER (1..65535)
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The collector's configured UDP port number."
                ::= { extremeNetFlowGroupCollectorEntry 6 }

        extremeNetFlowCollectorStatusUp                  OBJECT-TYPE
                SYNTAX  TruthValue
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                        "Flag indicating if the collector is up."
                ::= { extremeNetFlowGroupCollectorEntry 7 }

        extremeNetFlowCollectorDowntime                       OBJECT-TYPE
                SYNTAX  INTEGER (1..65535)
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The downtime value for the collector."
                ::= { extremeNetFlowGroupCollectorEntry 8 }
		
	extremeNetFlowCollectorPacketsTx                      OBJECT-TYPE
                SYNTAX  INTEGER (1..65535)
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The transmit packet count for the collector."
                ::= { extremeNetFlowGroupCollectorEntry 9 }



--
-- NetFlow Port Configuration Table
--

        extremeNetFlowPortConfigTable                   OBJECT-TYPE
                SYNTAX  SEQUENCE OF ExtremeNetFlowPortConfigEntry
                MAX-ACCESS  not-accessible
                STATUS current
                DESCRIPTION
                        "This table contains configuration information
                         for a defined NetFlow port."
                ::= { extremeNetFlowConfigPort 1 }

        extremeNetFlowPortConfigEntry                   OBJECT-TYPE
                SYNTAX  ExtremeNetFlowPortConfigEntry
                MAX-ACCESS      not-accessible
                STATUS  current
                DESCRIPTION
                        ""
                INDEX {extremeNetFlowPortConfigPortIndex}
                ::= {extremeNetFlowPortConfigTable 1}


        ExtremeNetFlowPortConfigEntry ::= SEQUENCE {
                extremeNetFlowPortConfigPortIndex       INTEGER,
                extremeNetFlowPortConfigEnabled         TruthValue,
                extremeNetFlowPortConfigTimout          INTEGER,
                extremeNetFlowPortOverFlowPackets       INTEGER
        }

        extremeNetFlowPortConfigPortIndex               OBJECT-TYPE
                SYNTAX  INTEGER (1..65535)
                MAX-ACCESS      not-accessible
                STATUS  current
                DESCRIPTION
                        "The index value for the port."
                ::= { extremeNetFlowPortConfigEntry 1 }

        extremeNetFlowPortConfigEnabled              OBJECT-TYPE
                SYNTAX  TruthValue
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                        "Flag indicating if port is enabled."
                ::= { extremeNetFlowPortConfigEntry 2 }

        extremeNetFlowPortConfigTimout                       OBJECT-TYPE
                SYNTAX  INTEGER (1..65535)
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The port timeout value."
                ::= { extremeNetFlowPortConfigEntry 3 }

        extremeNetFlowPortOverFlowPackets                      OBJECT-TYPE
                SYNTAX  INTEGER (1..65535)
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The number of packets not accounted for due to lack of resources.  Implemented on PoS ports only"
                ::= { extremeNetFlowPortConfigEntry 4 }



--
-- NetFlow Port Filter Entry Configuration Table
--

        extremeNetFlowPortFilterConfigTable                     OBJECT-TYPE
                SYNTAX  SEQUENCE OF ExtremeNetFlowPortFilterConfigEntry
                MAX-ACCESS  not-accessible
                STATUS current
                DESCRIPTION
                        "This table contains configuration information
                         for a defined NetFlow filter."
                ::= { extremeNetFlowConfigPort 2 }

        extremeNetFlowPortFilterConfigEntry                     OBJECT-TYPE
                SYNTAX  ExtremeNetFlowPortFilterConfigEntry
                MAX-ACCESS      not-accessible
                STATUS  current
                DESCRIPTION
                        ""
                INDEX {extremeNetFlowPortConfigPortNumber,
                       extremeNetFlowPortConfigFilterEgress,
                       extremeNetFlowPortConfigFilterNumber}
                ::= {extremeNetFlowPortFilterConfigTable 1}

        ExtremeNetFlowPortFilterConfigEntry ::= SEQUENCE {
                extremeNetFlowPortConfigPortNumber      INTEGER,
                extremeNetFlowPortConfigFilterEgress    TruthValue,
                extremeNetFlowPortConfigFilterNumber    INTEGER,
                extremeNetFlowPortEnabled               TruthValue,
                extremeNetFlowFilterEnabled             TruthValue,
                extremeNetFlowDestIpAddress             IpAddress,
                extremeNetFlowDestIpAddressMask         IpAddress,
                extremeNetFlowSourceIpAddress           IpAddress,
                extremeNetFlowSourceIpAddressMask       IpAddress,
                extremeNetFlowDestPort                  INTEGER,
                extremeNetFlowDestPortMask              INTEGER,
                extremeNetFlowSourcePort                INTEGER,
                extremeNetFlowSourcePortMask            INTEGER,
                extremeNetFlowProtocol                  INTEGER,
                extremeNetFlowProtocolMask              INTEGER,
                extremeNetFlowFilterGroupNumber         INTEGER,
                extremeNetFlowMatchAllFlag              TruthValue,
                extremeNetFlowMatchNoneFlag             TruthValue
        }

        extremeNetFlowPortConfigPortNumber                     OBJECT-TYPE
                SYNTAX  INTEGER (1..65535)
                MAX-ACCESS      not-accessible
                STATUS  current
                DESCRIPTION
                        "The port number for the filter."
                ::= { extremeNetFlowPortFilterConfigEntry 1 }

        extremeNetFlowPortConfigFilterEgress                     OBJECT-TYPE
                SYNTAX  TruthValue
                MAX-ACCESS      not-accessible
                STATUS          current
                DESCRIPTION
                        "Flag indicating whether this is a request for an
			 egress filter (1) or an ingress filter (0)."
                ::= { extremeNetFlowPortFilterConfigEntry 2 }

        extremeNetFlowPortConfigFilterNumber                     OBJECT-TYPE
                SYNTAX  INTEGER (1..8)
                MAX-ACCESS      not-accessible
                STATUS  current
                DESCRIPTION
                        "The filter number being requested (1-8)."
                ::= { extremeNetFlowPortFilterConfigEntry 3 }

        extremeNetFlowPortEnabled                                OBJECT-TYPE
                SYNTAX  TruthValue
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                        "Flag indicating whether port is enabled."
                ::= { extremeNetFlowPortFilterConfigEntry 4 }

        extremeNetFlowFilterEnabled                    OBJECT-TYPE
                SYNTAX  TruthValue
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                        "Flag indicating whether filter is enabled."
                ::= { extremeNetFlowPortFilterConfigEntry 5 }

        extremeNetFlowDestIpAddress                    OBJECT-TYPE
                SYNTAX  IpAddress
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                        "Filter Destination IP address."
                ::= { extremeNetFlowPortFilterConfigEntry 6 }

        extremeNetFlowDestIpAddressMask                OBJECT-TYPE
                SYNTAX  IpAddress
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                        "Filter Destination IP address Mask."
                ::= { extremeNetFlowPortFilterConfigEntry 7 }

        extremeNetFlowSourceIpAddress                  OBJECT-TYPE
                SYNTAX  IpAddress
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                        "Filter Source IP address."
                ::= { extremeNetFlowPortFilterConfigEntry 8 }

        extremeNetFlowSourceIpAddressMask              OBJECT-TYPE
                SYNTAX  IpAddress
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                        "Filter Source IP address Mask."
                ::= { extremeNetFlowPortFilterConfigEntry 9 }

        extremeNetFlowDestPort                         OBJECT-TYPE
                SYNTAX  INTEGER (1..65535)
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The destination port (valid for TCP and UDP flows only)."
                ::= { extremeNetFlowPortFilterConfigEntry 10 }

        extremeNetFlowDestPortMask                     OBJECT-TYPE
                SYNTAX  INTEGER (1..65535)
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The destination port mask."
                ::= { extremeNetFlowPortFilterConfigEntry 11 }

        extremeNetFlowSourcePort                       OBJECT-TYPE
                SYNTAX  INTEGER (1..65535)
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The source port (valid for TCP and UDP flows only)."
                ::= { extremeNetFlowPortFilterConfigEntry 12 }

        extremeNetFlowSourcePortMask                   OBJECT-TYPE
                SYNTAX  INTEGER (1..65535)
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The source port mask."
                ::= { extremeNetFlowPortFilterConfigEntry 13 }

        extremeNetFlowProtocol                         OBJECT-TYPE
                SYNTAX  INTEGER (1..65535)
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The IP protocol for the filter."
                ::= { extremeNetFlowPortFilterConfigEntry 14 }

        extremeNetFlowProtocolMask                     OBJECT-TYPE
                SYNTAX  INTEGER (1..65535)
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The IP protocol mask."
                ::= { extremeNetFlowPortFilterConfigEntry 15 }

        extremeNetFlowFilterGroupNumber                OBJECT-TYPE
                SYNTAX  INTEGER (1..32)
                MAX-ACCESS      read-only
                STATUS  current
                DESCRIPTION
                        "The Group Number."
                ::= { extremeNetFlowPortFilterConfigEntry 16 }

        extremeNetFlowMatchAllFlag                     OBJECT-TYPE
                SYNTAX  TruthValue
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                        "Filter is set to match all flows."
                ::= { extremeNetFlowPortFilterConfigEntry 17 }

        extremeNetFlowMatchNoneFlag                    OBJECT-TYPE
                SYNTAX  TruthValue
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                        "Filter is set to not match any flows."
                ::= { extremeNetFlowPortFilterConfigEntry 18 }
	

END


-- ===========================================================================

EXTREME-SNMPV3-MIB DEFINITIONS ::= BEGIN

    IMPORTS  
                MODULE-IDENTITY                 FROM SNMPv2-SMI
		OBJECT-TYPE                     FROM SNMPv2-SMI
                TruthValue                      FROM SNMPv2-TC
		extremeAgent                    FROM EXTREME-BASE-MIB
                snmpTargetAddrEntry             FROM SNMP-TARGET-MIB;

            
        extremeSnmpv3 MODULE-IDENTITY
                LAST-UPDATED "0007240000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION "Extreme-specific SNMPv3 objects"
        ::= { extremeAgent 23 }

	extremeTarget	OBJECT IDENTIFIER ::= { extremeSnmpv3 1 }
	
	extremeTargetAddrExtTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF ExtremeTargetAddrExtEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		"This table is an extension to the snmpTargetAddrTable found in the 
		SNMP-TARGET-MIB. It contains Extreme Networks specific objects needed for
		each management target."
			::= { extremeTarget 1 }

	extremeTargetAddrExtEntry OBJECT-TYPE
		SYNTAX  ExtremeTargetAddrExtEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		"An entry in the extremeTargetAddrExtTable."
                AUGMENTS { snmpTargetAddrEntry }
			::= { extremeTargetAddrExtTable 1 }

	ExtremeTargetAddrExtEntry ::= SEQUENCE {
		extremeTargetAddrExtIgnoreMPModel		TruthValue,
                extremeTargetAddrExtStandardMode                TruthValue,
                extremeTargetAddrExtTrapDestIndex               INTEGER,
                extremeTargetAddrExtUseEventComm                TruthValue
	}
	
	
	extremeTargetAddrExtIgnoreMPModel OBJECT-TYPE
		SYNTAX TruthValue
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
		"When this object is set to TRUE, the version of the trap/notification sent to 
		the corresponding management target (trap receiver) will be the same as in 
		releases of Extremeware prior to 7.1.0. Thus, the value of the 
		snmpTargetParamsMPModel object in the snmpTargetParamsTable will be ignored while
		determining the version of the trap/notification to be sent. When a trap-receiver
		is created via the RMON trapDestTable or from the CLI command 'configure snmp add
		trapreceiver ....', the value of this object will be set to TRUE for the 
		corresponding entry in this table."
                DEFVAL { false }
		::= { extremeTargetAddrExtEntry 1 }

	extremeTargetAddrExtStandardMode OBJECT-TYPE
		SYNTAX TruthValue
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
		"When this object is set to TRUE, the management target will be treated as 
		a 'standard mode' one, in that any Extreme Networks specific extra varbinds 
		present in a standards-based trap/notification will not be sent to this 
		management target. Only the varbinds defined in the standard will be sent."
                DEFVAL { false }
		::= { extremeTargetAddrExtEntry 2 }

	extremeTargetAddrExtTrapDestIndex OBJECT-TYPE
		SYNTAX INTEGER
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"This object contains the value of the trapDestIndex in the corresponding 
		entry of the RMON trapDestTable."
		::= { extremeTargetAddrExtEntry 3 }

        extremeTargetAddrExtUseEventComm OBJECT-TYPE
                SYNTAX TruthValue
                MAX-ACCESS read-write
                STATUS current
                DESCRIPTION
                "This object is used only when sending RMON alarms as SNMPv3 traps.
                When it is set to TRUE and an RMON risingAlarm or fallingAlarm is being sent
                for an event, then the eventCommunity in the RMON event table is compared to 
                the snmpTargetAddrName in the snmpTargetAddrTable. The alarm is sent to the 
                target only when the two are the same. This behavior is exhibited only when the
                snmpTargetParamsMPModel corresponding to the target indicates an SNMPv3 trap. For 
                SNMPv1/v2c traps, the community in the RMON trapDestTable is used for the 
                comparision, which is the 'regular' method, as per the standards.
                When this object is set to FALSE, then the RMON alarm (if being sent as an SNMPv3
                trap) is sent without using the event community for any comparision."
                DEFVAL { true }        
		::= { extremeTargetAddrExtEntry 4 }
END

-- ===========================================================================

-- ===========================================================================

EXTREME-CABLE-MIB DEFINITIONS ::= BEGIN

    IMPORTS  
        MODULE-IDENTITY     FROM SNMPv2-SMI
		OBJECT-TYPE         FROM SNMPv2-SMI
        TruthValue          FROM SNMPv2-TC
		extremeAgent        FROM EXTREME-BASE-MIB
		extremeV2Traps		FROM EXTREME-BASE-MIB
        extremenetworks		FROM EXTREME-BASE-MIB
		DisplayString       FROM RFC1213-MIB
		NOTIFICATION-TYPE	FROM SNMPv2-SMI;
            
    extremeCable MODULE-IDENTITY
                LAST-UPDATED "0007240000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION "Extreme-specific Cable objects"
        ::= { extremeAgent 24 }

        extremeDiagConfigGroup OBJECT IDENTIFIER
	::= { extremeCable 1 }

	extremeDiagConfigTime OBJECT-TYPE
 		SYNTAX DisplayString  (SIZE(16))
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
	        "Indicates the time at which the Diagnostics information 
		 will be collected for the ports which have 
		 Auto-Diagnostics configured. Time must be given in hh:mm:ss format
		 where hh, mm and ss are in decimals"
		::= { extremeDiagConfigGroup 1  }
		
	extremeDiagConfigRoF OBJECT-TYPE
		SYNTAX INTEGER {true (1), false (2)}
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
	        "Indicates whether a port should return to INIT state on 
		 Diagnostics Failure. If TRUE the port will be restarted 
		 even if the Diagnostics indicate a Failure. If FALSE the 
		 port will be moved to DIAG_FAIL state"
		::= { extremeDiagConfigGroup 2  }

	extremeDiagPortConfigTable OBJECT-TYPE
		SYNTAX SEQUENCE OF ExtremeDiagPortCfgEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
	        "Table, which contains the diagnostic configuration 
		 information for the ports"
		::= { extremeCable 2  }

	extremeDiagPortConfigEntry OBJECT-TYPE
		SYNTAX ExtremeDiagPortCfgEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
	        "Each row represents port related diagnostics 
		 configuration"
		INDEX { extremeDiagPortCfgPortIfIndex, extremeDiagPortCfgMode }
		::= { extremeDiagPortConfigTable 1  }

	ExtremeDiagPortCfgEntry ::=
		SEQUENCE {
				extremeDiagPortCfgPortIfIndex
					INTEGER,
				extremeDiagPortCfgMode
					INTEGER,
				extremeDiagPortCfgStatus
					INTEGER 
			}

	extremeDiagPortCfgPortIfIndex OBJECT-TYPE
		SYNTAX INTEGER
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
	        "IfIndex of the Port for which the information in this row applies"
		::= { extremeDiagPortConfigEntry 1  }

	extremeDiagPortCfgMode OBJECT-TYPE
		SYNTAX INTEGER {auto (1), manual (2)}
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
	        "The mode of operation. The port can be configured to have
		 either manual diagnostics or auto-diagnostics collected."
		::= { extremeDiagPortConfigEntry 2 }

	extremeDiagPortCfgStatus OBJECT-TYPE
		SYNTAX INTEGER {enable (1), disable (2), run (3), diagfail(4)}
		MAX-ACCESS read-write
		STATUS current
		DESCRIPTION
	        "Specifies whether Diagnostics are enabled or disabled for 
		 the port. In the manual mode, enable and disable will disable the
		 corresponding bit in the manual Diag portmask. Once the run command is
		 given the Manual Diagnostics starts running. <diagfail> indicates the
		 diagnostics for the port has failed. <diagfail> is a read-only value and
		 cannot be used for setting the status of the port"
		::= { extremeDiagPortConfigEntry 3  }

    extremeDiagPortDiagTable OBJECT-TYPE
		SYNTAX SEQUENCE OF ExtremeDiagPortDiagEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
		 "Table contains the diagnostic information for the ports"
		::= { extremeCable 3  }

        extremeDiagPortDiagEntry OBJECT-TYPE
		SYNTAX ExtremeDiagPortDiagEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
		 "Each row represents port related diagnostics information"
		INDEX { extremeDiagPortDiagPortIfIndex, extremeDiagPortDiagMode }
		::= { extremeDiagPortDiagTable 1 }

        ExtremeDiagPortDiagEntry ::=
		SEQUENCE {
				extremeDiagPortDiagPortIfIndex
					INTEGER,
				extremeDiagPortDiagMode
					INTEGER,
				extremeDiagPortSpeed
				    INTEGER,
				extremeDiagPortSwapAB
					INTEGER,
				extremeDiagPortSwapCD
					INTEGER,
				extremeDiagPortPairAPol
					INTEGER,
				extremeDiagPortPairAFlen
					INTEGER,
				extremeDiagPortPairALen
					INTEGER,
				extremeDiagPortPairASkew
					INTEGER,
				extremeDiagPortPairAStatus
					INTEGER,
				extremeDiagPortPairBPol
					INTEGER,
				extremeDiagPortPairBFlen
					INTEGER,
				extremeDiagPortPairBLen
					INTEGER,
				extremeDiagPortPairBSkew
					INTEGER,
				extremeDiagPortPairBStatus
					INTEGER,
				extremeDiagPortPairCPol
					INTEGER,
				extremeDiagPortPairCFlen
					INTEGER,
				extremeDiagPortPairCLen
					INTEGER,
				extremeDiagPortPairCSkew
					INTEGER,
				extremeDiagPortPairCStatus
					INTEGER,
				extremeDiagPortPairDPol
					INTEGER,
				extremeDiagPortPairDFlen
					INTEGER,
				extremeDiagPortPairDLen
					INTEGER,
				extremeDiagPortPairDSkew
					INTEGER,
				extremeDiagPortPairDStatus
					INTEGER,
				extremeDiagPortDateTime
				    DisplayString	
			}

	extremeDiagPortDiagPortIfIndex OBJECT-TYPE
		SYNTAX INTEGER
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
	        "IfIndex of the Port for which the information in this row applies"
		::= { extremeDiagPortDiagEntry 1  }

	extremeDiagPortDiagMode OBJECT-TYPE
		SYNTAX INTEGER {auto (1), manual (2)}
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
	        "The mode of operation. The port can be configured to have
		 either manual diagnostics or auto-diagnostics collected."
		::= { extremeDiagPortDiagEntry 2 }

	extremeDiagPortSpeed OBJECT-TYPE
		SYNTAX INTEGER { speed10 (1), speed100 (2), speed1000 (3), unknown (4)}
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"Specifies the speed of the port"
		::= { extremeDiagPortDiagEntry 3  }

	extremeDiagPortSwapAB OBJECT-TYPE
		SYNTAX INTEGER {swap(1), noswap(2), unknown(3)}
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"Specifies whether pairA pairB cables are swapped"
		::= { extremeDiagPortDiagEntry 4  }

	extremeDiagPortSwapCD OBJECT-TYPE
		SYNTAX INTEGER {swap(1), noswap(2), unknown(3)}
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"Specifies whether pairC and pairD cables are swapped"
		::= { extremeDiagPortDiagEntry 5  }

	extremeDiagPortPairAPol OBJECT-TYPE
		SYNTAX INTEGER {positive(1), negative(2), unknown(3)}
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"Specifies the polarity of pairA cables"
		::= { extremeDiagPortDiagEntry 6  }

	extremeDiagPortPairAFlen OBJECT-TYPE
		SYNTAX INTEGER
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"Specifies the distance of Fault in the pairA cables"
		::= { extremeDiagPortDiagEntry 7  }

	extremeDiagPortPairALen OBJECT-TYPE
		SYNTAX INTEGER
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"Specifies the length of the pairA cables"
		::= { extremeDiagPortDiagEntry 8  }

	extremeDiagPortPairASkew OBJECT-TYPE
		SYNTAX INTEGER
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
	        "Skew of pairA cables with respect to the fastest pair"
		::= { extremeDiagPortDiagEntry 9  }

	extremeDiagPortPairAStatus OBJECT-TYPE
		SYNTAX INTEGER {open(1), short(2), terminated(3), imperror(4), unknown(5)}
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
	        "Indicates whether pairA cables are properly terminated, 
		 short or open"
		::= { extremeDiagPortDiagEntry 10  }

	extremeDiagPortPairBPol OBJECT-TYPE
		SYNTAX INTEGER {positive(1), negative(2), unknown(3)}
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"Specifies the polarity of pairB cables"
		::= { extremeDiagPortDiagEntry 11  }

	extremeDiagPortPairBFlen OBJECT-TYPE
		SYNTAX INTEGER
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"Specifies the distance of Fault in the pairB cables"
		::= { extremeDiagPortDiagEntry 12  }

	extremeDiagPortPairBLen OBJECT-TYPE
		SYNTAX INTEGER
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"Specifies the length of the pairB cables"
		::= { extremeDiagPortDiagEntry 13  }

	extremeDiagPortPairBSkew OBJECT-TYPE
		SYNTAX INTEGER
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"Skew of pairB cables with respect to the fastest pair"
		::= {  extremeDiagPortDiagEntry 14 }

	extremeDiagPortPairBStatus OBJECT-TYPE
		SYNTAX INTEGER {open(1), short(2), terminated(3), imperror(4), unknown(5)}
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
	        "Indicates whether pairB cables are properly terminated, 
		 short or open"
		::= { extremeDiagPortDiagEntry 15 }

	extremeDiagPortPairCPol OBJECT-TYPE
		SYNTAX INTEGER {positive(1), negative(2), unknown(3)}
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"Specifies the polarity of pairC cables"
		::= { extremeDiagPortDiagEntry 16  }

	extremeDiagPortPairCFlen OBJECT-TYPE
		SYNTAX INTEGER
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"Specifies the distance of Fault in the pairC cables"
		::= { extremeDiagPortDiagEntry 17  }

	extremeDiagPortPairCLen OBJECT-TYPE
		SYNTAX INTEGER
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"Specifies the length of the pairC cables"
		::= { extremeDiagPortDiagEntry 18 }

	extremeDiagPortPairCSkew OBJECT-TYPE
		SYNTAX INTEGER
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
	        "Skew of pairC cables with respect to the fastest pair"
		::= { extremeDiagPortDiagEntry 19 }

	extremeDiagPortPairCStatus OBJECT-TYPE
		SYNTAX INTEGER {open(1), short(2), terminated(3), imperror(4), unknown(5)}
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
	        "Indicates whether pairC cables are properly terminated, 
		 short or open"
		::= {  extremeDiagPortDiagEntry 20}

	extremeDiagPortPairDPol OBJECT-TYPE
		SYNTAX INTEGER {positive(1), negative(2), unknown(3)}
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"Specifies the polarity of pairD cables"
		::= { extremeDiagPortDiagEntry 21  }

	extremeDiagPortPairDFlen OBJECT-TYPE
		SYNTAX INTEGER
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"Specifies the distance of Fault in the pairD cables"
		::= { extremeDiagPortDiagEntry 22  }

	extremeDiagPortPairDLen OBJECT-TYPE
		SYNTAX INTEGER
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"Specifies the length of the pairD cables"
		::= { extremeDiagPortDiagEntry 23 }

	extremeDiagPortPairDSkew OBJECT-TYPE
		SYNTAX INTEGER
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
	        "Skew of pairD cables with respect to the fastest pair"
		::= { extremeDiagPortDiagEntry 24 }

	extremeDiagPortPairDStatus OBJECT-TYPE
		SYNTAX INTEGER {open(1), short(2), terminated(3), imperror(4), unknown(5)}
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
	        "Indicates whether pairD cables are properly terminated, 
		 short or open"
		::= { extremeDiagPortDiagEntry 25 }

	extremeDiagPortDateTime OBJECT-TYPE
 		SYNTAX DisplayString  (SIZE(64))
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
	        "Date and time at which the Diagnostic information was 
		 collected"
		::= { extremeDiagPortDiagEntry 26 }

	extremeDiagPortStatsTable  OBJECT-TYPE
		SYNTAX SEQUENCE OF ExtremeDiagPortStatsEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
	        "Table, which contains the diagnostic statistic information
		 for the ports"
		::= { extremeCable 4  }

	extremeDiagPortStatsEntry OBJECT-TYPE
		SYNTAX ExtremeDiagPortStatsEntry
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
	        "Each row represents port related diagnostics statistics
		 information"
		INDEX { extremeDiagPortStatsPortIfIndex }
		::= { extremeDiagPortStatsTable 1 }

	ExtremeDiagPortStatsEntry ::=
		SEQUENCE {
				extremeDiagPortStatsPortIfIndex
					INTEGER,
				extremeDiagPortStatsNumDiag
					INTEGER,
				extremeDiagPortStatsNumSuccess
					INTEGER,
				extremeDiagPortStatsNumFail
					INTEGER,
				extremeDiagPortStatsNumChange
					INTEGER,
				extremeDiagPortStatsNumAbort
					INTEGER
			}

	extremeDiagPortStatsPortIfIndex OBJECT-TYPE
		SYNTAX INTEGER
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
	        "IfIndex of the Port for which the information in this row applies"
		::= { extremeDiagPortStatsEntry 1  }

	extremeDiagPortStatsNumDiag OBJECT-TYPE
		SYNTAX INTEGER
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
	        "Number of times Diagnostics information collected for this
		 port"
		::= {   extremeDiagPortStatsEntry 2 }

	extremeDiagPortStatsNumSuccess OBJECT-TYPE
		SYNTAX INTEGER
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
	        "Number of times Diagnostics for this port completed 
		 successfully without any errors"
		::= {   extremeDiagPortStatsEntry 3 }

	extremeDiagPortStatsNumFail OBJECT-TYPE
		SYNTAX INTEGER
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
	        "Number of times Diagnostics for this port Failed due to 
		 errors in the cable pairs"
		::= {   extremeDiagPortStatsEntry 4 }

	extremeDiagPortStatsNumChange OBJECT-TYPE
		SYNTAX INTEGER
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
	        "Number of times Diagnostics Changed for this port"
		::= {   extremeDiagPortStatsEntry 5 }

	extremeDiagPortStatsNumAbort OBJECT-TYPE
		SYNTAX INTEGER
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
	        "Number of times Diagnostics was aborted by the user for this port"
		::= {   extremeDiagPortStatsEntry 6 }

--TRAPS MIB Definitions for CDM
  
   extremeCableTraps 	OBJECT IDENTIFIER
	::= { extremeV2Traps 13 }

   extremeCableTrapsPrefix   OBJECT IDENTIFIER
	::= { extremeCableTraps 0 }

   extremeTrapDiagPortDiagnostics NOTIFICATION-TYPE
	OBJECTS { extremeDiagPortCfgPortIfIndex,
                  extremeDiagPortCfgMode,
                  extremeDiagPortCfgStatus }
	STATUS current
	DESCRIPTION
   	  "Indicates the status of Diagnostics for a port. The status indicates 
   	  whether Diagnostics for a particular port failed"
	    ::= { extremeCableTrapsPrefix 1 }

END


-- ===========================================================================

EXTREME-NP-MIB DEFINITIONS ::= BEGIN

	IMPORTS
                MODULE-IDENTITY FROM SNMPv2-SMI
		OBJECT-TYPE     FROM SNMPv2-SMI
                Unsigned32	FROM SNMPv2-SMI
		Counter32	FROM SNMPv2-SMI
		Counter64	FROM SNMPv2-SMI
                IpAddress       FROM SNMPv2-SMI
		DisplayString   FROM RFC1213-MIB
		extremeAgent    FROM EXTREME-BASE-MIB;
		


        extremeNPMib MODULE-IDENTITY
                LAST-UPDATED "0007240000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION "Extreme NP objects: NP card information"
        ::= { extremeAgent 21 }

	extremeNPModule	OBJECT IDENTIFIER ::= { extremeNPMib 1 }
	
	extremeNPModuleTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF ExtremeNPModuleEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		"A table containing information about each Intelligent
		module in the chassis."
			::= { extremeNPModule 1 }

	extremeNPModuleEntry OBJECT-TYPE
		SYNTAX  ExtremeNPModuleEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		"A table entry containing information about the
		intelligent modules configured in the chassis.
		This table does not contain rows for the slots
		which do not have a network processor based module."
		INDEX	  { extremeNPModuleSlotNumber }
			::= { extremeNPModuleTable 1 }

	ExtremeNPModuleEntry ::= SEQUENCE {
		extremeNPModuleSlotNumber		INTEGER,		
		extremeNPModuleDescription		DisplayString,
		extremeNPModuleCurrentSoftware		DisplayString,
		extremeNPModulePrimarySoftware		DisplayString,
		extremeNPModuleSecondarySoftware	DisplayString,
		extremeNPModuleBootromVersion		DisplayString,
		extremeNPModuleProcessorState		OCTET STRING
	}
	
	
	extremeNPModuleSlotNumber OBJECT-TYPE
		SYNTAX INTEGER(1..8)
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"A unique integer identifying the particular slot 
		in the chassis."
		::= { extremeNPModuleEntry 1 }

	extremeNPModuleDescription   OBJECT-TYPE
		SYNTAX  DisplayString (SIZE(0..32))
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"A description of the particular slot in the chassis."
		::= { extremeNPModuleEntry 2 }

	extremeNPModuleCurrentSoftware   OBJECT-TYPE
		SYNTAX  DisplayString (SIZE(0..160))
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"The version of the software currently running on the module."
		::= { extremeNPModuleEntry 3 }

	extremeNPModulePrimarySoftware   OBJECT-TYPE
		SYNTAX  DisplayString (SIZE(0..160))
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"The version of software in the primary image of the module."
		::= { extremeNPModuleEntry 4 }
					   
	extremeNPModuleSecondarySoftware   OBJECT-TYPE
		SYNTAX  DisplayString (SIZE(0..160))
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"The version of software in the secondary image of the module."
		::= { extremeNPModuleEntry 5 }

	extremeNPModuleBootromVersion   OBJECT-TYPE
		SYNTAX  DisplayString (SIZE(0..80))
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"The version of bootrom that the module will use when restarting."
		::= { extremeNPModuleEntry 6 }

	extremeNPModuleProcessorState   OBJECT-TYPE
		SYNTAX  OCTET STRING (SIZE (8))
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"An Octet String indicating the status of the various processors
		on an Intelligent Module. Each byte in the Octet String represents
		state for one processor.
		For the Avalanche based PoS and ARM modules, the first byte (from MSB)
		represents the state of the General Purpose Processor, the second byte
		the state of Network Processor 1, and the third byte the state of Network
		Processor 2 and so on. A value of 0 in each byte indicates that the
		Processor is not operational, while a value 1 indicates that it is."
		::= { extremeNPModuleEntry 7 }
		
	  
--		
-- SMA Module
--

	extremeSMAModule OBJECT IDENTIFIER ::= { extremeNPMib 2 }
	
	extremeSMATable OBJECT-TYPE
		SYNTAX  SEQUENCE OF ExtremeSMAEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		"A table containing information about each SMA
		module in the chassis."
			::= { extremeSMAModule 1 }

	extremeSMAEntry OBJECT-TYPE
		SYNTAX  ExtremeSMAEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		"A table entry containing information about the
		SMA modules configured in the chassis.
		This table does not contain rows for the slots
		which do not have an SMA module."
		INDEX	  { extremeSMASlotNumber }
			::= { extremeSMATable 1 }

	ExtremeSMAEntry ::= SEQUENCE {	      
		extremeSMASlotNumber			INTEGER,  
		extremeSMAProtocolVersion		INTEGER,
		extremeSMAServiceVersion		DisplayString,
		extremeSMAUpTime			Unsigned32,
		extremeSMACpuUtilization                Unsigned32,
		extremeSMAMemUtilization                Unsigned32,
		extremeSMAQosBroadcaster                Unsigned32,		
		extremeSMANumFromBroadcaster            Unsigned32,		
		extremeSMANumToListener                 Unsigned32,
		extremeSMABytesBroadcaster		Counter64,
		extremeSMABytesListener			Counter64
	}
	
	extremeSMASlotNumber OBJECT-TYPE
		SYNTAX INTEGER(1..8)
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"A unique integer identifying the particular slot 
		in the chassis."
		::= { extremeSMAEntry 1 }
				
	extremeSMAProtocolVersion OBJECT-TYPE
		SYNTAX INTEGER(1..255)
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"Protocol version."
		::= { extremeSMAEntry 2 }
	
	extremeSMAServiceVersion OBJECT-TYPE
		SYNTAX DisplayString (SIZE(0..128))
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"Service release version."
		::= { extremeSMAEntry 3 }
		
	extremeSMAUpTime OBJECT-TYPE
		SYNTAX Unsigned32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"Continuous operating time of the module in seconds."
		::= { extremeSMAEntry 4 }
		
	extremeSMACpuUtilization OBJECT-TYPE
		SYNTAX Unsigned32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"Percentage of CPU utilized in the last 5 seconds."
		::= { extremeSMAEntry 5 }
	
	extremeSMAMemUtilization OBJECT-TYPE
		SYNTAX Unsigned32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"Percentage of memory utilized."		
		::= { extremeSMAEntry 6 }

	extremeSMAQosBroadcaster OBJECT-TYPE
		SYNTAX Unsigned32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION		
		"60 second rolling average of %QoS.
		Number of bytes received / Number of bytes expected per duration.
		Note: this can potentially exceed 100%."
		::= { extremeSMAEntry 7 }			
				
        extremeSMANumFromBroadcaster OBJECT-TYPE
		SYNTAX Unsigned32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"The total number of broadcasters sending streams."
		::= { extremeSMAEntry 8 }
				
	extremeSMANumToListener OBJECT-TYPE
		SYNTAX Unsigned32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION		
		"The total number of listeners connected."
		::= { extremeSMAEntry 9 }
		
	extremeSMABytesBroadcaster OBJECT-TYPE
		SYNTAX Counter64
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION		
		"The total number of media bytes received from the broadcasters."
		::= { extremeSMAEntry 10 }
		
	extremeSMABytesListener OBJECT-TYPE
		SYNTAX Counter64
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION		
		"The total number of data bytes sent to listeners."
		::= { extremeSMAEntry 11 }


--		
-- ATM Module
--

	extremeATMModule OBJECT IDENTIFIER ::= { extremeNPMib 3 }
	
	extremeATMCellPduTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF ExtremeATMCellPduEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		"A table containing information about each ATM
		module in the chassis."
			::= { extremeATMModule 1 }

	extremeATMCellPduEntry OBJECT-TYPE
		SYNTAX  ExtremeATMCellPduEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		"A table entry containing information about the
		ATM modules configured in the chassis.
		This table does not contain rows for the slots
		which do not have an ATM module."
		INDEX	  { extremeATMPortNumber }
			::= { extremeATMCellPduTable 1 }


	ExtremeATMCellPduEntry ::= SEQUENCE {	      
  		extremeATMPortNumber         INTEGER,  
                extremeATMRxCell             Unsigned32,
                extremeATMTxCell             Unsigned32,
                extremeATMRxCellHecError     Unsigned32,   
                extremeATMRxCellError        Unsigned32,
                extremeATMRxAAL5Pdu          Unsigned32,
                extremeATMTxAAL5Pdu          Unsigned32,
                extremeATMRxAAL5Bytes        Counter64,
                extremeATMTxAAL5Bytes        Counter64,
                extremeATMPortStatus         DisplayString
	}


	extremeATMPortNumber OBJECT-TYPE
		SYNTAX INTEGER(1..64)
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"A unique integer identifying the particular port number
		in the chassis."
		::= { extremeATMCellPduEntry 1 }

	extremeATMRxCell OBJECT-TYPE
		SYNTAX Unsigned32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"The number of ATM cell Received."
		::= { extremeATMCellPduEntry 2 }

	extremeATMTxCell OBJECT-TYPE
		SYNTAX Unsigned32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"The number of ATM cell Transmitted."
		::= { extremeATMCellPduEntry 3 }
				
	extremeATMRxCellHecError OBJECT-TYPE
		SYNTAX Unsigned32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"The number of received cells with HEC error."
		::= { extremeATMCellPduEntry 4 }
				
	extremeATMRxCellError OBJECT-TYPE
		SYNTAX Unsigned32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"The number of received cells discarded due to other error."
		::= { extremeATMCellPduEntry 5 }
				

        extremeATMRxAAL5Pdu OBJECT-TYPE      
		SYNTAX Unsigned32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"The number AAL-5 PDU Received."
		::= { extremeATMCellPduEntry 6 }

        extremeATMTxAAL5Pdu OBJECT-TYPE      
		SYNTAX Unsigned32
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"The number AAL-5 PDU Transmitted."
		::= { extremeATMCellPduEntry 7 }

        extremeATMRxAAL5Bytes OBJECT-TYPE      
		SYNTAX Counter64
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"The number AAL-5 PDU Octetd Received."
		::= { extremeATMCellPduEntry 8 }

        extremeATMTxAAL5Bytes OBJECT-TYPE      
		SYNTAX Counter64
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"The number AAL-5 PDU Octetd Transmitted."
		::= { extremeATMCellPduEntry 9 }

	extremeATMPortStatus OBJECT-TYPE
		SYNTAX DisplayString (SIZE(0..4))
		MAX-ACCESS  read-only
		STATUS current
		DESCRIPTION
		"ATM port status."
		::= { extremeATMCellPduEntry 10 }


-- Table 2
	extremeATMVpiVciTable OBJECT-TYPE
		SYNTAX  SEQUENCE OF ExtremeATMVpiVciEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		"A table containing information about each ATM
		module in the chassis."
			::= { extremeATMModule 2 }

	extremeATMVpiVciEntry OBJECT-TYPE
		SYNTAX  ExtremeATMVpiVciEntry
		MAX-ACCESS  not-accessible
		STATUS current
		DESCRIPTION
		"A table entry containing information about the
		ATM modules configured in the chassis.
		This table does not contain rows for the slots
		which do not have an ATM module."
		INDEX	  { extremeATMPortNum,
                            extremeATMPvc        }
			::= { extremeATMVpiVciTable 1 }

	ExtremeATMVpiVciEntry ::= SEQUENCE {	      
  		extremeATMPortNum            INTEGER,  
                extremeATMPvc                INTEGER,
                extremeATMVpi                INTEGER,
                extremeATMVci                INTEGER
	}

	extremeATMPortNum OBJECT-TYPE
		SYNTAX INTEGER(1..64)
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"A unique integer identifying the particular port number
		in the chassis."
		::= { extremeATMVpiVciEntry 1 }

	extremeATMPvc OBJECT-TYPE
		SYNTAX INTEGER(1..3072)
                MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"A unique integer identifying the pvc number configured
		on a single port."
		::= { extremeATMVpiVciEntry 2 }

	extremeATMVpi OBJECT-TYPE
		SYNTAX INTEGER(0..15)
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"A unique integer identifying the VPI value
		of the configured PVCs."
		::= { extremeATMVpiVciEntry 3 }

	extremeATMVci OBJECT-TYPE
		SYNTAX INTEGER(17..4095)
		MAX-ACCESS read-only
		STATUS current
		DESCRIPTION
		"A unique integer identifying the VCI value
		of the configured PVCs."
		::= { extremeATMVpiVciEntry 4 }

--              
-- MPLS TLS Module
--

        extremeMplsModule OBJECT IDENTIFIER ::= { extremeNPMib 4 }
        
        extremeMplsTlsTable OBJECT-TYPE
                SYNTAX  SEQUENCE OF ExtremeMplsTlsEntry
                MAX-ACCESS  not-accessible
                STATUS current
                DESCRIPTION
                "A table containing information about each MPLS TLS
                tunnel in the chassis."
                        ::= { extremeMplsModule 1 }

        extremeMplsTlsEntry OBJECT-TYPE
                SYNTAX  ExtremeMplsTlsEntry
                MAX-ACCESS  not-accessible
                STATUS current
                DESCRIPTION
                "A table entry containing information about the
                MPLS TLS tunnel."
                INDEX     { extremeMplsTlsNum }
                        ::= { extremeMplsTlsTable 1 }


        ExtremeMplsTlsEntry ::= SEQUENCE {            
                extremeMplsTlsNum            INTEGER, 
                extremeMplsTlsName           DisplayString,  
                extremeMplsTlsLocalIpAddr    IpAddress,
                extremeMplsTlsPeerIpAddr     IpAddress,
                extremeMplsTlsLocalVlanID    Unsigned32,   
                extremeMplsTlsLocalVlanName  DisplayString,
                extremeMplsTlsDynamic        Unsigned32,
                extremeMplsTlsType           Unsigned32,
                extremeMplsTlsVcID           Unsigned32,
                extremeMplsTlsLocalGroupID   Unsigned32,
                extremeMplsTlsRemoteGroupID  Unsigned32,
                extremeMplsTlsVcState        DisplayString,
                extremeMplsTlsIngressVcLabel Unsigned32,
                extremeMplsTlsEgressVcLabel  Unsigned32, 
                extremeMplsTlsPacketTx       Unsigned32,
                extremeMplsTlsPacketRx       Unsigned32,
                extremeMplsTlsOctetTx        Counter64,
                extremeMplsTlsOctetRx        Counter64
        }

        extremeMplsTlsNum OBJECT-TYPE
                SYNTAX INTEGER (1..16384)
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "An index used to reference each configured TLS tunnel."
                ::= { extremeMplsTlsEntry 1 }

        extremeMplsTlsName OBJECT-TYPE
                SYNTAX DisplayString (SIZE(0..31))
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "The user defined TLS tunnel identifier name."
                ::= { extremeMplsTlsEntry 2 }

        extremeMplsTlsLocalIpAddr OBJECT-TYPE
                SYNTAX IpAddress
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "The TLS tunnel local endpoint IP address, only valid if TLS tunnel
                is Dynamic. Otherwise, this field is set to zero."
                ::= { extremeMplsTlsEntry 3 }

        extremeMplsTlsPeerIpAddr OBJECT-TYPE
                SYNTAX IpAddress
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "The TLS tunnel peer endpoint IP address."
                ::= { extremeMplsTlsEntry 4 }

        extremeMplsTlsLocalVlanID  OBJECT-TYPE
                SYNTAX Unsigned32
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "The local Egress Vlan ID."
                ::= { extremeMplsTlsEntry 5 }
                                
        extremeMplsTlsLocalVlanName  OBJECT-TYPE
                SYNTAX DisplayString (SIZE(0..31))
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "The local Egress Vlan Name."
                ::= { extremeMplsTlsEntry 6 }
                                
        extremeMplsTlsDynamic OBJECT-TYPE
                SYNTAX Unsigned32
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "Flag indicating that the TLS tunnel is Dynamic. If set, the TLS tunnel
                is dynamically signaled. If zero, the TLS tunnel is statically configured."
                ::= { extremeMplsTlsEntry 7 }
                                
        extremeMplsTlsType OBJECT-TYPE
                SYNTAX Unsigned32
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "The TLS tunnel type
                0- MPLS, Static
                1- MPLS, Martini ."
                ::= { extremeMplsTlsEntry 8 }

        extremeMplsTlsVcID OBJECT-TYPE      
                SYNTAX Unsigned32
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "The configured VC ID, only valid if TLS tunnel is Dynamic.
                Otherwise, this field is set to zero."
                ::= { extremeMplsTlsEntry 9 }

        extremeMplsTlsLocalGroupID OBJECT-TYPE      
                SYNTAX Unsigned32
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "The configured Local Group ID, only valid if TLS tunnel is Dynamic.
                Otherwise, this field is set to zero."
                ::= { extremeMplsTlsEntry 10 }

        extremeMplsTlsRemoteGroupID OBJECT-TYPE      
                SYNTAX Unsigned32
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "The learned Remote Group ID, only valid if TLS tunnel is Dynamic.
                Otherwise, this field is set to zero."
                ::= { extremeMplsTlsEntry 11 }

        extremeMplsTlsIngressVcLabel OBJECT-TYPE
                SYNTAX Unsigned32
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                "The TLS tunnel VLAN Ingress Label. If the TLS tunnel is Static,
                this value is configured. If TLS tunnel is Dynamic,
                this value is dynamically allocated from the TLS
                label range and signaled to the TLS tunnel peer."
                ::= { extremeMplsTlsEntry 12 }

        extremeMplsTlsEgressVcLabel OBJECT-TYPE
                SYNTAX Unsigned32
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                "The TLS tunnel VLAN Egress Label. If the TLS tunnel is Static,
                this value is configured. If TLS tunnel is Dynamic,
                this value is learned from the TLS tunnel peer."
                ::= { extremeMplsTlsEntry 13 }

        extremeMplsTlsVcState OBJECT-TYPE      
                SYNTAX DisplayString (SIZE(0..79))
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                "The TLS tunnel VC state. Valid states include:
                - Idle
                - No LSP Available
                - Waiting for LDP session
                - Pending label mapping
                - Pending local configuration
                - MTU incompatibility
                - Up
                - Unknown
                - Error .. General failure
                - Error .. Targeted LDP session failure
                - Error .. Bridge configuration problem
                - Error .. Ingress label allocation failure
                - Error .. Failure sending TLS label mapping
                - Error .. Patricia tree insertion failure
                - Error .. Failure programming TLS hardware
                - Error .. MPLS not initialized
                - Error .. Unknown."
                ::= { extremeMplsTlsEntry 14 }

        extremeMplsTlsPacketTx  OBJECT-TYPE
                SYNTAX Unsigned32
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                "The number of Packets Transmitted on this TLS tunnel."
                ::= { extremeMplsTlsEntry 15 }

        extremeMplsTlsPacketRx OBJECT-TYPE
                SYNTAX Unsigned32
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                "The number of Packets Received on this TLS tunnel."
                ::= { extremeMplsTlsEntry 16 }

        extremeMplsTlsOctetTx OBJECT-TYPE
                SYNTAX Counter64
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                "The number of Octets Transmitted on this TLS tunnel."
                ::= { extremeMplsTlsEntry 17 }

        extremeMplsTlsOctetRx OBJECT-TYPE
                SYNTAX Counter64
                MAX-ACCESS  read-only
                STATUS current
                DESCRIPTION
                "The number of Octets Received on this TLS tunnel."
                ::= { extremeMplsTlsEntry 18 }

END

-- ============================================================================
--
-- Extreme Services
--

EXTREME-POE-MIB DEFINITIONS ::= BEGIN
	IMPORTS 
        MODULE-IDENTITY 	FROM SNMPv2-SMI
	    OBJECT-TYPE 		FROM SNMPv2-SMI
	    NOTIFICATION-TYPE	FROM SNMPv2-SMI
	    Integer32		    FROM SNMPv2-SMI
	    Gauge32 		    FROM SNMPv2-SMI
	    Counter32 		    FROM SNMPv2-SMI
        TruthValue		    FROM SNMPv2-TC
       	extremeAgent 		FROM EXTREME-BASE-MIB
        extremeV2Traps		FROM EXTREME-BASE-MIB
        pethMainPseGroupIndex,
        pethPsePortGroupIndex,
        pethPsePortIndex    FROM POWER-ETHERNET-MIB;



        extremePoE MODULE-IDENTITY
                LAST-UPDATED "0007240000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION "Extreme Power over Ethernet MIB objects"
        ::= { extremeAgent 27 }

        extremePethMain   OBJECT IDENTIFIER ::= {extremePoE 1}
        extremePethPort   OBJECT IDENTIFIER ::= {extremePoE 2}
--        powerEthernetMIB  OBJECT IDENTIFIER ::= {extremePoE 3}
        extremePethSystem OBJECT IDENTIFIER ::= {extremePoE 4}
--        extremePethTraps  OBJECT IDENTIFIER ::= {extremeV2Traps 12}


-- extremePethSystem
extremePethSystemAdminEnable OBJECT-TYPE
          SYNTAX INTEGER   {
                  enable(1),
                  disable(2)
          }
          MAX-ACCESS            read-write
          STATUS                current
          DESCRIPTION
                  "Controls whether inline power is provided by the system."
          DEFVAL                { enable }
          ::= { extremePethSystem 1 }

extremePethSystemDisconnectPrecedence OBJECT-TYPE
          SYNTAX INTEGER   {
                  lowestPriority(1),
                  denyPort(2)
          }
          MAX-ACCESS            read-write
          STATUS                current
          DESCRIPTION
               "Controls the disconnect function of power management.
                When the power drain exceeds the available power budget,
                due to a rise in power consumption after power is allocated
                to the ports, the PoE controller disconnects one of the ports
                to prevent overload on the power supply. There are two controls:
                Lowest-priority: next port connected causes a shutdown of the 
                                 lowest priority port.
                Deny-port:       next port is denied power, regardless of priority."
          DEFVAL                { denyPort }
          ::= { extremePethSystem 2 }

extremePethSystemUsageThreshold OBJECT-TYPE
          SYNTAX      Integer32  (1..99)
          UNITS      "%"
          MAX-ACCESS  read-write
          STATUS      current
          DESCRIPTION
                  "The usage threshold expressed in percents for
                   comparing the measured power and initiating
                   an alarm if the threshold is exceeded."
          ::= { extremePethSystem 3 }

extremePethSystemPowerSupplyMode OBJECT-TYPE
          SYNTAX INTEGER   {
                  redundant(1),
                  loadSharing(2),
                  notApplicable(3)
          }
          MAX-ACCESS  read-write
          STATUS      current
          DESCRIPTION
                  "Controls whether the power supply operate in
                   redundant or load-sharing mode.  Systems which do not
                   provide redundant or load-sharing operations will return
                   an error on setting, and notApplicable on read."
         ::= { extremePethSystem 4 }

extremePethSystemLegacyEnable OBJECT-TYPE
          SYNTAX INTEGER   {
                  enable(1),
                  disable(2)
          }
          MAX-ACCESS            read-write
          STATUS                current
          DESCRIPTION
                  "Controls whether legacy is supported by the system.  This is only supported on 
                   S300-24 stackables currently."
          DEFVAL                { disable }
          ::= { extremePethSystem 5 }



-- Per Slot Table
extremePethPseSlotTable OBJECT-TYPE
          SYNTAX      SEQUENCE OF ExtremePethPseSlotEntry
          MAX-ACCESS  not-accessible
          STATUS      current
          DESCRIPTION
              "A table of objects that provides power management capabilities per slot."
          ::= { extremePethMain 2 }

extremePethPseSlotEntry OBJECT-TYPE
          SYNTAX      ExtremePethPseSlotEntry
          MAX-ACCESS  not-accessible
          STATUS      current
          DESCRIPTION
              "A set of objects that display and control the power characteristics of a slot."
          INDEX    { extremePethSlotNumber }
          ::= { extremePethPseSlotTable 1 }

ExtremePethPseSlotEntry ::= SEQUENCE {
        extremePethSlotNumber                 Integer32,
        extremePethSlotPowerLimit             Integer32,
        extremePethSlotConsumptionPower       Gauge32,
        extremePethSlotClearConnectHistory    INTEGER,
        extremePethSlotReservedConsumptionPower Gauge32,
        extremePethSlotCommonConsumptionPower Gauge32,
        extremePethSlotAdminEnable            INTEGER,
        extremePethSlotPoeStatus              INTEGER,
        extremePethSlotPoeResetSystem         INTEGER,
	    extremePethSlotMaxAvailPower          Gauge32,
        extremePethSlotMaxCapacity            Gauge32,
        extremePethSlotBackupPSU              INTEGER,
        extremePethSlotPSUActive              INTEGER,
	    extremePethSlotMeasuredPower          Gauge32,
     	extremePethSlotMainPseIndex		      Integer32
}

extremePethSlotNumber  OBJECT-TYPE
          SYNTAX                Integer32
          MAX-ACCESS            not-accessible
          STATUS                current
          DESCRIPTION
                  "Slot number. This is the same as the Group Index"
          ::= { extremePethPseSlotEntry 1 }

extremePethSlotPowerLimit  OBJECT-TYPE
          SYNTAX                Integer32
          UNITS                 "watts"
          MAX-ACCESS            read-write
          STATUS                current
          DESCRIPTION
                  "The configured maximum amount of inline power available to
                  slot. The operational power available to the slot is based
                  upon other operational and configuration parameters, such as
                  the power-supply mode and status. This number is provided by
                  the object extremePethSlotMaxAvailPower.  extremePethSlotPowerLimit 
                  may be greater than extremePethSlotMaxAvailPower, however, cannot 
                  exceed the maximum slot capacity, provided by extremePethSlotMaxCapacity"
          ::= { extremePethPseSlotEntry 2 }

extremePethSlotConsumptionPower  OBJECT-TYPE
          SYNTAX                Gauge32
          UNITS                 "watts"
          MAX-ACCESS            read-only
          STATUS                current
          DESCRIPTION
                  "The amount of power allocated to PoE devices on the slot expressed in mWatts.
                   The amount of power allocated to a PoE device is based upon the PoE device 
                   class and/or the port's extremePethPortViolationPrecedence setting. For
                   example, in the default configuration of extremePethPortViolationPrecedence 
                   set to maxAdvertisedOperator(3), and the extremePethPortOperatorLimit set to 
                   15400, a PoE device is allocated 15.4 watts."
          ::= { extremePethPseSlotEntry 3 }

extremePethSlotClearConnectHistory  OBJECT-TYPE
          SYNTAX                INTEGER { set(1),
                                          clear(2)
                                        }
          MAX-ACCESS            read-write
          STATUS                current
          DESCRIPTION
                  "Clears the port connection history of the specified slot.
                   Reading the value always reurns clear(2)."
          ::= { extremePethPseSlotEntry 4 }

extremePethSlotReservedConsumptionPower  OBJECT-TYPE
          SYNTAX                Gauge32
          UNITS                 "Milliwatts"
          MAX-ACCESS            read-only
          STATUS                current
          DESCRIPTION
                  "The amount of reserved power consumed on the slot expressed in Milliwatts."
          ::= { extremePethPseSlotEntry 5 }

extremePethSlotCommonConsumptionPower  OBJECT-TYPE
          SYNTAX                Gauge32
          UNITS                 "Milliwatts"
          MAX-ACCESS            read-only
          STATUS                current
          DESCRIPTION
                  "The amount of common power allocated on the slot expressed in Milliwatts.
                   This value is computed by the formula:
                   extremePethSlotConsumptionPower - extremePethSlotReservedConsumptionPower."
          ::= { extremePethPseSlotEntry 6 }

extremePethSlotAdminEnable OBJECT-TYPE
          SYNTAX INTEGER   {
                  enable(1),
                  disable(2)
          }
          MAX-ACCESS            read-write
          STATUS                current
          DESCRIPTION           "Controls whether inline power is provided by the slot."
          DEFVAL                { enable }
          ::= { extremePethPseSlotEntry 7 }

extremePethSlotPoeStatus OBJECT-TYPE
          SYNTAX INTEGER   {
                  initializing(1),
                  operational(2),
                  downloadFail(3),
                  calibrationRequired(4),
                  invalidFirmware(5),
                  mismatchVersion(6),
                  updating(7),
                  invalidDevice(8),
                  notOperational(9),
                  other(10)
          }
          MAX-ACCESS            read-only
          STATUS                current
          DESCRIPTION           
             "Describes the status of the PoE system on the slot.
              initializing - PoE controller is under initialization,
              operational - PoE controller is operational and is ready or
                            providing power,
              downloadFail - PoE controller required update and the update
                             failed, PoE reset is required to re-update,
              calibrationRequired - PoE contoller is operational, however
                                    calibration is required to provide power,
              invalidFirmware - PoE controller contains invalid firmware,
              mismatchVersion - PoE controller update completed, however
                                version mismatches expected, reboot,
              updating        - PoE controller is being updated,
              invalidDevice   - PoE controller detected an invalid/bad PoE
                                device.
              notOperational  - PoE controller is not yet operational
              other           - PoE controller is in undefined stats."
          ::= { extremePethPseSlotEntry 8 }

extremePethSlotPoeResetSystem OBJECT-TYPE
          SYNTAX                INTEGER { set(1), clear(2) }
          MAX-ACCESS		    read-write
          STATUS		        current
          DESCRIPTION
                "Resets the PoE system on the slot. Reading returns clear(2)"
          ::= { extremePethPseSlotEntry 9 }

extremePethSlotMaxAvailPower  OBJECT-TYPE
          SYNTAX                Gauge32
          UNITS                 "watts"
          MAX-ACCESS            read-only
          STATUS                current
          DESCRIPTION
                  "The maximum power available to the slot expressed in Watts.
	               The value depends on various configuration parameters and
                   power-supply modes and status."
          ::= { extremePethPseSlotEntry 10 }

extremePethSlotMaxCapacity  OBJECT-TYPE
          SYNTAX                Gauge32
          UNITS                 "watts"
          MAX-ACCESS            read-only
          STATUS                current
          DESCRIPTION
                  "The maximum capacity of the slot expressed in Watts. This
                   provides the hardware limitation of the slot. Actual
                   amount of power is dependant on system status. The
                   object extremePethSlotPowerLimit must not be greater than
                   this amount."
          ::= { extremePethPseSlotEntry 11 }

extremePethSlotBackupPSU OBJECT-TYPE
          SYNTAX INTEGER   {
                  none(1),
                  internal(2),
                  external(3),
                  notApplicable(4)
          }
          MAX-ACCESS            read-write
          STATUS                current
          DESCRIPTION           "Controls the backup power supply for inline power for the slot.
                                 A system which does not allow the backup PSU to be
                                 configured will return an error upon setting."
          ::= { extremePethPseSlotEntry 12 }

extremePethSlotPSUActive OBJECT-TYPE
          SYNTAX INTEGER   {
                  none(1),
                  internal(2),
                  external(3)
          }
          MAX-ACCESS            read-only
          STATUS                current
          DESCRIPTION           "Inline Power supply status indication for the slot. Indicates which PSU
                                 is currently active.  In the case of a failover a none indication can
                                 occur until one of the PSU has finished powering up."
          ::= { extremePethPseSlotEntry 13 }

extremePethSlotMeasuredPower  OBJECT-TYPE
          SYNTAX                Gauge32
          UNITS                 "milliwatts"
          MAX-ACCESS            read-only
          STATUS                current
          DESCRIPTION
                  "The measured amount of power for all PoE device on the 
                   slot."
          ::= { extremePethPseSlotEntry 14 }

extremePethSlotMainPseIndex   OBJECT-TYPE
          SYNTAX                Integer32
          MAX-ACCESS            read-only
          STATUS                current
          DESCRIPTION
                  "The index into the PethMainPseTable. Provides the
	               mapping of the slot identifier to pethMainPseGroupIndex."
          ::= { extremePethPseSlotEntry 15 }


extremePethPsePortTable OBJECT-TYPE
          SYNTAX      SEQUENCE OF ExtremePethPsePortEntry
          MAX-ACCESS  not-accessible
          STATUS      current
          DESCRIPTION
              "A table of objects that extends the standard pethPsePortTable."
          ::= { extremePethPort 1 }

extremePethPsePortEntry OBJECT-TYPE
          SYNTAX      ExtremePethPsePortEntry
          MAX-ACCESS  not-accessible
          STATUS      current
          DESCRIPTION
            "A set of objects that display and control the power characteristics 
             of a powerEthernet PSE port. This table extends the standard pethPsePortTable."
          INDEX    { pethPsePortGroupIndex, pethPsePortIndex }
          ::= { extremePethPsePortTable 1 }

ExtremePethPsePortEntry ::= SEQUENCE {
	extremePethPortOperatorLimit        Integer32,
    extremePethPortReservedBudget       Integer32,
    extremePethPortViolationPrecedence  INTEGER,
    extremePethPortClearFault           INTEGER,
    extremePethPortResetPower           INTEGER,
	extremePethPortMeasuredPower	    Gauge32
}

extremePethPortOperatorLimit  OBJECT-TYPE
          SYNTAX Integer32 (3000..20000)  
          UNITS			"Milliwatts"
          MAX-ACCESS	read-write
          STATUS		current
          DESCRIPTION
             "Controls individual port maximum power level."
          DEFVAL 		{ 15400 }
          ::= { extremePethPsePortEntry 1 }

extremePethPortReservedBudget  OBJECT-TYPE
          SYNTAX Integer32 (0..20000)  
          UNITS			"Milliwatts"
          MAX-ACCESS	read-write
          STATUS		current
          DESCRIPTION
             "Controls individual port maximum power level. Value is 0 or 
              in the range of 3000..20000"
          DEFVAL 		{ 0 }
          ::= { extremePethPsePortEntry  2 }

extremePethPortViolationPrecedence OBJECT-TYPE
          SYNTAX		INTEGER {advertisedClass(1),
                                 operatorLimit(2),
                                 maxAdvertisedOperator(3),
                                 none(4) }  
          MAX-ACCESS	read-write
          STATUS		current
          DESCRIPTION
                "Sets the violation precedence for the specified ports. A value of 
                 advertised-class will remove/deny power in the case an 802.3af compliant 
                 PD consumes power beyond its advertised class limit. A value of 
                 operator-limit will remove/deny power should the PD consume power 
                 beyond the configured operator-limit. A value of max-class-operator will 
                 remove/deny power if the PD consumes power beyond the maximum of the 
                 detected class limit and the operator-limit. A value of none will 
                 remove/deny power in case the PD device exceeds the maximum allowable 
                 wattage according to regulatory maximum of 20 W. Default is 
                 max-class-operator which allows operation of both 802.3af compliant and 
                 legacy PDs."
          ::= { extremePethPsePortEntry  3 }

extremePethPortClearFault OBJECT-TYPE
          SYNTAX        INTEGER { set(1), clear(2) }
          MAX-ACCESS	read-write
          STATUS		current
          DESCRIPTION
                "Clears the fault condition.  Reading always returns clear(2)."
          ::= { extremePethPsePortEntry 4 }

extremePethPortResetPower OBJECT-TYPE
          SYNTAX        INTEGER { set(1), clear(2) }
          MAX-ACCESS	read-write
          STATUS		current
          DESCRIPTION
                "Resets the power on the port.  Reading always returns clear(2)"
          ::= { extremePethPsePortEntry 5 }

extremePethPortMeasuredPower  OBJECT-TYPE
          SYNTAX                Gauge32
          UNITS                 "Milliwatts"
          MAX-ACCESS            read-only
          STATUS                current
          DESCRIPTION
                  "The amount of power consumed on the port expressed in Milliwatts."
          ::= { extremePethPsePortEntry 6 }

END
-- ********************************************************************* 
--  EXTREME 802.11 Access Point Management Information Base, based
--  on IEEE 802.11 AP MIB.
-- ********************************************************************* 
EXTREMEdot11AP-MIB DEFINITIONS ::= BEGIN 
	
	
	IMPORTS 
	MODULE-IDENTITY 	FROM SNMPv2-SMI
	OBJECT-TYPE 		FROM SNMPv2-SMI
	TruthValue 		FROM SNMPv2-TC 
	extremeAP		FROM EXTREME-BASE-MIB
	ifIndex 		FROM RFC1213-MIB
	Unsigned32		FROM SNMPv2-SMI;

-- ********************************************************************* 
--  MODULE IDENTITY 
-- ********************************************************************* 

	extremeDot11ap MODULE-IDENTITY
	LAST-UPDATED "0211140000Z" 
	ORGANIZATION "Extreme Networks"
	CONTACT-INFO " " 

	DESCRIPTION 
	"This MIB module provides managemetn of a set of APs.  It is based
	 on the IEEE AP MIB with additions for better indexing."
    ::= { extremeAP 21 }

-- ********************************************************************* 
--  Major sections 
-- ********************************************************************* 

-- ********************************************************************* 
--  End of EXTREME AP MIB
-- ********************************************************************* 
END 





-- ************************************************************** --
-- 			LAC MIB					   --
--                                                                 --
-- This MIB makes reference to two new terms: wireless port and    --
-- wireless interface.  A wireless port refers to the physical     --
-- connection between a LAC and an access point, together with the --
-- access point chassis.  Thus a wireless port is the unit of mani --
-- pulation for images, version, etc.                              --
--                                                                 --
-- A wireless interface is a channel or antenna on a single wirele --
-- ss port.  There can be one or more wireless interfaces on a     --
-- wireless port.                                                  --
-- ************************************************************** --


EXTREME-WIRELESS-MIB DEFINITIONS ::= BEGIN

	IMPORTS 
		ifIndex			FROM IF-MIB
		InterfaceIndex          FROM IF-MIB
        MODULE-IDENTITY 	FROM SNMPv2-SMI
		OBJECT-TYPE     	FROM SNMPv2-SMI
		NOTIFICATION-TYPE	FROM SNMPv2-SMI
		RowStatus		FROM SNMPv2-TC
        Unsigned32		FROM SNMPv2-SMI
		IpAddress		FROM SNMPv2-SMI
		TimeTicks		FROM SNMPv2-SMI
		Counter32 		FROM SNMPv2-SMI
        Counter64 		FROM SNMPv2-SMI
        Integer32               FROM SNMPv2-SMI
        TruthValue     	FROM SNMPv2-TC
		MacAddress		FROM SNMPv2-TC
		DisplayString  	FROM RFC1213-MIB
        extremeAgent   	FROM EXTREME-BASE-MIB
        ExtremeDeviceId     FROM EXTREME-BASE-MIB
		extremeV2Traps		FROM EXTREME-BASE-MIB
        ClientAuthType          FROM EXTREME-BASE-MIB
		WPACipherSet 		FROM EXTREME-BASE-MIB
		WPAKeyMgmtSet 		FROM EXTREME-BASE-MIB
        WirelessRemoteConnectBindingType FROM EXTREME-BASE-MIB
		InetAddressType		FROM INET-ADDRESS-MIB
		InetAddress    		FROM INET-ADDRESS-MIB
		extremeAP		FROM EXTREME-BASE-MIB
		extremeLAC		FROM EXTREME-BASE-MIB
		TEXTUAL-CONVENTION	FROM SNMPv2-TC;

        extremeWireless MODULE-IDENTITY
                LAST-UPDATED "0211230000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION "Extreme Wireless Access Tables"
        ::= { extremeAgent 25 }

	extremeAPTraps 		OBJECT IDENTIFIER ::= { extremeV2Traps 5 }
	extremeAPTrapsPrefix 	OBJECT IDENTIFIER ::= { extremeAPTraps 0 }
	extremeLACGeneral 	OBJECT IDENTIFIER ::= { extremeLAC 1 }
	extremeProfile 		OBJECT IDENTIFIER ::= { extremeLAC 2 }


-- ************************************************************** --
-- ************************************************************** --
Dot11Type ::= TEXTUAL-CONVENTION
	  STATUS	current
	  DESCRIPTION
		"The current standard supports A, B, G interfaces."
	  SYNTAX INTEGER { a(1), b(2), g(3), bg(4) }

Dot11Speed ::= TEXTUAL-CONVENTION
	  STATUS	current
	  DESCRIPTION   "Specifies the speed in Mbps to use for the interface. A value of 0 indicates auto."
	SYNTAX BITS { 	speed1(0),
			speed2(1),
			speed5(2),
			speed11(3),
			speed6(4),
			speed9(5),
			speed12(6),
			speed18(7),
			speed24(8),
			speed36(9),
			speed48(10),
			speed54(11)}

-- Added for DFS support. To be used for listing channels on 
-- which Radar interference was detected.
Dot11AChannel ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION "Specifies the channel number for 802.11A interface."
    SYNTAX BITS { 
            channel36(0),
            channel40(1),
            channel44(2),
            channel52(3),
            channel56(4),
            channel60(5),
            channel64(6),
            channel100(7),
            channel104(8),
            channel108(9),
            channel112(10),
            channel116(11),
            channel120(12),
            channel124(13),
            channel128(14),
            channel132(15),
            channel140(16)
            }

Dot11AuthMode ::= TEXTUAL-CONVENTION
	STATUS     current
	DESCRIPTION "Specifies the allowed authentication type."
	SYNTAX		INTEGER { open(0), shared(1)}

NetworkAuthMode ::= TEXTUAL-CONVENTION
	STATUS     current
	DESCRIPTION "Specifies the allowed authentication type."
	SYNTAX		INTEGER { none(0), webNetlogin(1), macRadius(2), wpaPlusLegacy(3), wpaOnly(4), wpa2PlusWPA(5), wpa2Only(6)}

ExtremeWirelessCountryCode ::= TEXTUAL-CONVENTION
    STATUS     current
    DESCRIPTION "Specifies the country code the AP operates in."
    SYNTAX INTEGER { 
                        unitedStates(840),
                        japan(392),
                        taiwan(158),
                        newZealand(554),
                        albania              ( 8),       
                        algeria              ( 12),      
                        argentina            ( 32),      
                        armenia              ( 51),      
                        australia            ( 36),      
                        austria              ( 40),      
                        azerbaijan           ( 31),      
                        bahrain              ( 48),      
                        belarus              ( 112),     
                        belgium              ( 56),      
                        belize               ( 84),      
                        bolivia              ( 68),      
                        brazil               ( 76),      
                        bruneiDarussalam    ( 96),      
                        bulgaria             ( 100),     
                        canada               ( 124),     
                        chile                ( 152),     
                        china                ( 156),     
                        colombia             ( 170),     
                        costaRica           ( 188),     
                        croatia              ( 191),     
                        cyprus               ( 196),
                        czech                ( 203),     
                        denmark              ( 208),     
                        dominicanRepublic   ( 214),     
                        ecuador              ( 218),     
                        egypt                ( 818),     
                        elSalvador          ( 222),     
                        estonia              ( 233),     
                        faeroeIslands       ( 234),     
                        finland              ( 246),     
                        france               ( 250),     
                        georgia              ( 268),     
                        germany              ( 276),     
                        greece               ( 300),     
                        guatemala            ( 320),     
                        honduras             ( 340),     
                        hongKong            ( 344),     
                        hungary              ( 348),     
                        iceland              ( 352),     
                        india                ( 356),     
                        indonesia            ( 360),     
                        iran                 ( 364),     
                        iraq                 ( 368),     
                        ireland              ( 372),     
                        israel               ( 376),     
                        italy                ( 380),     
                        jamaica              ( 388),     
                        japan1               ( 393),     
                        japan2               ( 394),     
                        japan3               ( 395),     
                        jordan               ( 400),     
                        kazakhstan           ( 398),     
                        kenya                ( 404),     
                        koreaNorth          ( 408),     
                        koreaRoc            ( 410),     
                        koreaRoc2           ( 411),     
                        kuwait               ( 414),     
                        latvia               ( 428),     
                        lebanon              ( 422),     
                        libya                ( 434),     
                        liechtenstein        ( 438),     
                        lithuania            ( 440),     
                        luxembourg           ( 442),     
                        macau                ( 446),     
                        macedonia            ( 807),     
                        malaysia             ( 458),     
                        mexico               ( 484),     
                        monaco               ( 492),     
                        morocco              ( 504),     
                        netherlands          ( 528),     
                        nicaragua            ( 558),     
                        norway               ( 578),     
                        oman                 ( 512),     
                        pakistan             ( 586),     
                        panama               ( 591),     
                        paraguay             ( 600),     
                        peru                 ( 604),     
                        philippines          ( 608),     
                        poland               ( 616),     
                        portugal             ( 620),     
                        puertoRico          ( 630),     
                        qatar                ( 634),     
                        romania              ( 642),     
                        russia               ( 643),     
                        saudiArabia         ( 682),     
                        singapore            ( 702),     
                        slovakia             ( 703),     
                        slovenia             ( 705),     
                        southAfrica         ( 710),     
                        spain                ( 724),     
                        sweden               ( 752),     
                        switzerland          ( 756),     
                        syria                ( 760),     
                        thailand             ( 764),     
                        trinidadTYobago    ( 780),     
                        tunisia              ( 788),     
                        turkey               ( 792),     
                        uae                  ( 784),     
                        ukraine              ( 804),     
                        unitedKingdom       ( 826),     
                        uruguay              ( 858),     
                        uzbekistan           ( 860),     
                        venezuela            ( 862),     
                        vietNam             ( 704),     
                        yemen                ( 887),     
                        zimbabwe             ( 716),     
                        restOfTheWorld       ( 0),
                        extremeDefault       ( 998),
                        unknown              ( 999)
                        }

ExtremeWirelessAntennaType ::= TEXTUAL-CONVENTION
    STATUS     current
    DESCRIPTION "Specifies Antenna type attached to the access-point. 
    The integrated antenna is specified by CTL table on PCI eeprom.
    The detachable model 15901 is an omni-directional antenna.
    The detachable model 15902 is a  directional antenna."
    SYNTAX    INTEGER { integrated(0), detachable15901(1), detachable15902(2) }


ExtremeWirelessAntennaLocation ::= TEXTUAL-CONVENTION
    STATUS     current
    DESCRIPTION "Specifies whether the antenna is an indoor or outdoor antenna"
    SYNTAX	 INTEGER { indoor(0), outdoor(1) }

ExtremeWirelessPhysInterfaceIndex ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION  "The value of a physical interface number. Each radio on an AP
			corresponds to a physical interface. There can be multiple
			virtual interface on each physical interface. The format
			for the physical interface is xxxxyy where xxxx is the
			port IF index to which the AP is connected. YY is the 
			interface index within that AP."
    SYNTAX      Integer32(1..2147483647)

ExtremeWirelessVirtInterfaceIndex ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION  "The value of a virtual interface number. Each radio on an AP
			corresponds to a physical interface. There can be multiple
			virtual interface on each physical interface. The format
			for the virtual interface is xxxxyyzz where xxxx is the
			port IF index to which the AP is connected. YY is the 
			physical interface index within that AP and ZZ is the index
			of the virtual interface within that physical interface."
    SYNTAX      Integer32(1..2147483647)

ExtremeWirelessChannelAutoSelectStatus ::= TEXTUAL-CONVENTION
    STATUS        current
    DESCRIPTION   "Specifies the status of the channel auto-selection process."
    SYNTAX BITS {       notApplicable(0),
                        inProgress(1),
                        success(2),
                        radarInterferenceDuringScan(3),
                        radarInterferenceDuringOperation(4),
                        restartedDueToInterference(5)}


-- ************************************************************** --
--                      Device wide Properties                     --
-- ************************************************************** --	
extremeAPTotalAuthFailures OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS 	read-only
	STATUS		current
	DESCRIPTION
		"This variable gives the total number of
		 Authentication failures that have been seen by all
		 the wireless ports."
	::= { extremeLACGeneral 1 }

extremeAPTotalDetectedStations OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"This variable gives the total number of detected
		 stations on all the wireless ports."
	::= { extremeLACGeneral 2 }

extremeAPTotalAssociatedStations OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"This variable gives the total number of associated
		 stations on all the wireless ports."
	::= { extremeLACGeneral 3 }

extremeAPTotalAuthenticatedStations OBJECT-TYPE
	SYNTAX          INTEGER
	MAX-ACCESS      read-only
	STATUS          current
	DESCRIPTION
	   "This variable gives the total number of authenticated
       stations on all the wireless ports."
	::= { extremeLACGeneral 4 }

extremeWirelessCfgMgmtVLAN OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This value indicates the VLAN tag that should be
                 applied to all control traffic between the AP and
                 the platform."
        ::= { extremeLACGeneral 5 }

extremeWirelessCfgNetmask OBJECT-TYPE
	SYNTAX		IpAddress
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This value is the subnet of the Mgmt Vlan"
	::= { extremeLACGeneral 6 }

extremeWirelessCfgGateway OBJECT-TYPE
	SYNTAX		IpAddress
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This value is assigned to the APs as the gateway
		for the management vlan."
	::= { extremeLACGeneral 7 }

extremeWirelessCfgEnableWirelessTraps OBJECT-TYPE
	SYNTAX		TruthValue
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"If set to TRUE the wireless port will send traps for
		 Authentication and association events.  
		 If set to FALSE no traps will be generated.
		 Note: We always generate the wireless port status
		 traps."
	::= { extremeLACGeneral 8 }

extremeWirelessCfgCountryCode OBJECT-TYPE
	SYNTAX		 ExtremeWirelessCountryCode
        MAX-ACCESS       read-write
        STATUS           current
        DESCRIPTION
                "This variable allows configuration of the 
                 country code in which the AP will operate.

                 Setting this value will enable the AP to range
                 check frequency and other regulatory settings."
        ::= { extremeLACGeneral 10 }


-- ************************************************************** --
--             Wireless Port Configuration Table                   --
--                                                                 --
-- The configuration table contains one entry for each port on the --
-- device which can host wireless function.  Configuration of the  --
-- port is done without regard to the presence or absence of an AP --
-- on that port.                                                   --
--                                                                 --
-- ************************************************************** --
extremeWirelessPortCfgTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF ExtremeWirelessPortCfgEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"This table contains one entry per wireless port that
		 the user has configured.  The AP does not have to be
		 plugged in for the user to configure it via this 
		 table."
	::= { extremeLAC 3 }

extremeWirelessPortCfgEntry OBJECT-TYPE
	SYNTAX		ExtremeWirelessPortCfgEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		""
	INDEX { extremeWirelessPortIfIndex }
	::= { extremeWirelessPortCfgTable 1 }

ExtremeWirelessPortCfgEntry ::= SEQUENCE {
	extremeWirelessPortIfIndex		        InterfaceIndex,
	extremeWirelessPortCfgIpAddress		    IpAddress,
	extremeWirelessPortCfgLocation		    DisplayString,
	extremeWirelessPortCfgDetectedTimeout	TimeTicks,
	extremeWirelessPortCfgClientWatchdog    TruthValue,
	extremeWirelessPortLastChange		    TimeTicks,
	extremeWirelessPortState		        INTEGER,
    extremeWirelessPortAntennaType          ExtremeWirelessAntennaType,
    extremeWirelessPortAntennaLocation      ExtremeWirelessAntennaLocation,
    extremeWirelessPortBootstrapServerAddressType  InetAddressType,
    extremeWirelessPortBootstrapServerAddress      InetAddress,
    extremeWirelessPortBootstrapFilePath    DisplayString,
    extremeWirelessPortBootLoaderServerAddressType InetAddressType,
    extremeWirelessPortBootLoaderServerAddress     InetAddress,
    extremeWirelessPortBootLoaderFilePath   DisplayString,
    extremeWirelessPortRuntimeServerAddressType    InetAddressType,
    extremeWirelessPortRuntimeServerAddress        InetAddress,
    extremeWirelessPortRuntimeFilePath      DisplayString,
    extremeWirelessPortMultiBootMode        INTEGER
}


extremeWirelessPortIfIndex OBJECT-TYPE
	SYNTAX		InterfaceIndex
	MAX-ACCESS	read-only 
	STATUS		current
	DESCRIPTION
		"This is the MIB-II ifIndex of the port this entry
		 describes."
	::= { extremeWirelessPortCfgEntry 1 }

extremeWirelessPortCfgIpAddress OBJECT-TYPE
	SYNTAX		IpAddress
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This value is assigned to the port for external
		 management."
	::= { extremeWirelessPortCfgEntry 2 }

extremeWirelessPortCfgLocation OBJECT-TYPE
	SYNTAX		DisplayString
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This describes the physical location of the wireless 
		 port."
	::= { extremeWirelessPortCfgEntry 3 }

extremeWirelessPortCfgDetectedTimeout OBJECT-TYPE
	SYNTAX		TimeTicks
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This is the number of seconds a station can stay
		 in the detected station table without authenticating."
	::= { extremeWirelessPortCfgEntry 4 }

extremeWirelessPortCfgClientWatchdog OBJECT-TYPE
	SYNTAX		TruthValue
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"Setting this value to true will force the AP to 
		 run a watch-dog process for system health."
	::= { extremeWirelessPortCfgEntry 5 }

extremeWirelessPortLastChange OBJECT-TYPE
	SYNTAX		TimeTicks
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The value of sysUpTime when the port entered its last state"
	::= { extremeWirelessPortCfgEntry 6 }

extremeWirelessPortState OBJECT-TYPE
	SYNTAX 		INTEGER {
				disabled(1),
				enabled(2),
				reset(3),
				addressing(4),
				register(5),
				syncing(6),
				online(7),
				error(8)
			}
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The current state of the wireless part of this port.

		 enabled  : Port is actively looking for wireless
			    interfaces.

		 disabled : Port is administratively unable to detect
			    new interfaces.

		 reset    : Interfaces have been detected and are 
			    being brought up (access point is booting).

		 addressing : IP Address is being assigned.

		 register : Interfaces are registering for service

		 syncing  : Interfaces are retrieving their 
			    configuration and updating their state.

		 online   : Interfaces are operational.

		 If an error occurs the wireless port will 
		 transistion to the error state."
	::= { extremeWirelessPortCfgEntry 7 }

-- TODO: What is the meaning of this variable?
extremeWirelessPortAntennaType OBJECT-TYPE
	SYNTAX	        ExtremeWirelessAntennaType	
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This is the type of the Antenna for Detachable product.
		 For Altitude-2d series, further selection is available
                 through this variable."
	::= { extremeWirelessPortCfgEntry 8 }

extremeWirelessPortAntennaLocation OBJECT-TYPE
	SYNTAX		ExtremeWirelessAntennaLocation
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This specifies the location the detachable antenna."
	::= { extremeWirelessPortCfgEntry 9 }

extremeWirelessPortBootstrapServerAddressType OBJECT-TYPE
	SYNTAX		InetAddressType
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
        "The type of address specified in the object 'extremeWirelessPortBootstrapServerAddress'.
        Currently, only 'ipv4' and 'dns' are supported."
	::= { extremeWirelessPortCfgEntry 10 }

extremeWirelessPortBootstrapServerAddress OBJECT-TYPE
	SYNTAX		InetAddress (SIZE (1..255))
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This specifies the TFTP server address from where the AP gets the Bootstrap Image.
        This can be a DNS name or an IPv4 address."
	::= { extremeWirelessPortCfgEntry 11 }

extremeWirelessPortBootstrapFilePath OBJECT-TYPE
	SYNTAX		DisplayString
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This specifies the TFTP FileName of the AP Bootstrap Image."
	::= { extremeWirelessPortCfgEntry 12 }

extremeWirelessPortBootLoaderServerAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "The type of address specified in the object 'extremeWirelessPortBootLoaderServerAddress'.
    Currently, only 'ipv4' and 'dns' are supported."
    ::= { extremeWirelessPortCfgEntry 13 }

extremeWirelessPortBootLoaderServerAddress OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (1..255))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "This specifies the TFTP server address from where the AP gets the Bootloader Image.
    This can be a DNS name or an IPv4 address."
    ::= { extremeWirelessPortCfgEntry 14 }

extremeWirelessPortBootLoaderFilePath OBJECT-TYPE
	SYNTAX		DisplayString
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This specifies the TFTP FileName of the AP Bootloader Image."
	::= { extremeWirelessPortCfgEntry 15 }

extremeWirelessPortRuntimeServerAddressType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "The type of address specified in the object 'extremeWirelessPortRuntimeServerAddress'.
    Currently, only 'ipv4' and 'dns' are supported."
    ::= { extremeWirelessPortCfgEntry 16 }

extremeWirelessPortRuntimeServerAddress OBJECT-TYPE
    SYNTAX      InetAddress (SIZE (1..255))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
    "This specifies the TFTP server address from where the AP gets the Runtime Image.
    This can be a DNS name or an IPv4 address."
    ::= { extremeWirelessPortCfgEntry 17 }

extremeWirelessPortRuntimeFilePath OBJECT-TYPE
	SYNTAX		DisplayString
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This specifies the TFTP FileName of the AP Runtime Image."
	::= { extremeWirelessPortCfgEntry 18 }

extremeWirelessPortMultiBootMode OBJECT-TYPE
    SYNTAX INTEGER { a300 (0),
        a-bp (1)}
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This is used to identify the image with which the AP boots up. This is enumerated as follows:
        0 - a300 - This specifies that AP will bootup with Extreme's A300 image
        1 - a-bp - This specifies that AP will bootup with Siemen''s Beacon Point Image."
	::= { extremeWirelessPortCfgEntry 19 }
-- ************************************************************** --
--                    Wireless Port Status Table                   --
--                                                                 --
-- Status table has one entry for every attached AP.  Each entry   --
-- contains a duplicate of the values which are configured in the  --
-- configuration table, as well as status and other information    --
-- learned from the device.                                        --
-- ************************************************************** --
extremeWirelessPortStatusTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF ExtremeWirelessPortStatusEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"This table contains one entry per detected AP."
	::= { extremeAP 1 }

extremeWirelessPortStatusEntry OBJECT-TYPE
	SYNTAX		ExtremeWirelessPortStatusEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		""
	INDEX { extremeWirelessPortIfIndex }
	::= { extremeWirelessPortStatusTable 1 }

ExtremeWirelessPortStatusEntry ::= SEQUENCE {
	extremeWirelessPortIpAddress		     IpAddress,
	extremeWirelessPortNetmask		         IpAddress,
	extremeWirelessPortGateway		         IpAddress,
	extremeWirelessPortManagementIP		     IpAddress,
	extremeWirelessPortEnableWirelessTraps   TruthValue,
	extremeWirelessPortLocation		         DisplayString,
	extremeWirelessPortDetectedMaxAge	     TimeTicks,
	extremeWirelessPortMgmtVLAN		         INTEGER,
	extremeWirelessPortBootromVersion	     DisplayString,
	extremeWirelessPortSWVersion		     DisplayString,
	extremeWirelessPortSysDescr		         DisplayString,
	extremeWirelessPortManufacturerName	     DisplayString,
	extremeWirelessPortProductName		     DisplayString,
	extremeWirelessPortSerialNumber 	     DisplayString,
	extremeWirelessPortEdpNeighborId	     ExtremeDeviceId,
	extremeWirelessPortClearCounters	     TruthValue,
	extremeWirelessPortClearLog		         TruthValue,
	extremeWirelessPortWatchdogReset	     TruthValue,
	extremeWirelessPortNumPhysInterfaces	 INTEGER,
	extremeWirelessPortHWVersion	         DisplayString,
	extremeWirelessPortMacAddress            MacAddress,
	extremeWirelessPortRadiusPortID		     DisplayString,
    extremeWirelessPortBootUpTime            TimeTicks,
    extremeWirelessPortCountryCode		     ExtremeWirelessCountryCode,
	extremeWirelessPortWallclockTime         INTEGER,
	extremeWirelessPortPartNumber		     DisplayString,
	extremeWirelessPortPartRevision          DisplayString,
	extremeWirelessPortUpTime                TimeTicks,
    extremeWirelessPortStatusAntennaType     ExtremeWirelessAntennaType,
    extremeWirelessPortStatusAntennaLocation ExtremeWirelessAntennaLocation,
    extremeWirelessPortStatusAntenna2point4GHZGain INTEGER,
    extremeWirelessPortStatusAntenna5GHZGain INTEGER,
    extremeWirelessPortPrimaryBootloaderVersion     DisplayString,
    extremeWirelessPortSecondaryBootloaderVersion   DisplayString,
    extremeWirelessPortCurrentBootloaderInUse       INTEGER
}


extremeWirelessPortIpAddress OBJECT-TYPE
	SYNTAX		IpAddress
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This value is assigned to the port for external
		 management."
	::= { extremeWirelessPortStatusEntry 1 }

extremeWirelessPortNetmask OBJECT-TYPE
	SYNTAX		IpAddress
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This value is assigned to the AP for external
		 management."
	::= { extremeWirelessPortStatusEntry 2 }

extremeWirelessPortGateway OBJECT-TYPE
	SYNTAX		IpAddress
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This value is assigned to the AP for external
		 management."
	::= { extremeWirelessPortStatusEntry 3 }

extremeWirelessPortManagementIP OBJECT-TYPE
	SYNTAX		IpAddress
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This value is used by the AP when sending out Management 
		packets to the external world. This IP is used as src-ip 
		address in Syslog messages, as NAS-Identifier in Radius requests, 
		and as Agent-Addr in SNMP trap pdu's."
	::= { extremeWirelessPortStatusEntry 4 }

extremeWirelessPortEnableWirelessTraps OBJECT-TYPE
	SYNTAX		TruthValue
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"If set to TRUE the wireless port will send traps for
		 Authentication and association successful events.  
		 If set to FALSE no traps will be generated.

		 Note: We always generate the wireless port status
		 traps."
	::= { extremeWirelessPortStatusEntry 5 }

extremeWirelessPortLocation OBJECT-TYPE
	SYNTAX		DisplayString
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This describes the physical location of the wireless 
		 port."
	::= { extremeWirelessPortStatusEntry 6 }

extremeWirelessPortDetectedMaxAge OBJECT-TYPE
	SYNTAX		TimeTicks
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This is the number of seconds a station can stay
		 in the detected station table without authenticating."
	::= { extremeWirelessPortStatusEntry 7 }

extremeWirelessPortMgmtVLAN OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"This value indicates the VLAN tag that should be
		 applied to all control traffic between the AP and
		 the platform."
	::= { extremeWirelessPortStatusEntry 8 }

extremeWirelessPortBootromVersion OBJECT-TYPE
	SYNTAX		DisplayString
	MAX-ACCESS		read-only
	STATUS		current
	DESCRIPTION
		"This is the current version of the bootrom on this AP."
	::= { extremeWirelessPortStatusEntry 9 }

extremeWirelessPortSWVersion OBJECT-TYPE
	SYNTAX		DisplayString
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"This is the current software version of this AP."
	::= { extremeWirelessPortStatusEntry 10 }

extremeWirelessPortSysDescr OBJECT-TYPE
	SYNTAX		DisplayString
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"This is the equivalent value of sysDescr from the AP."
	::= { extremeWirelessPortStatusEntry 11 }

extremeWirelessPortManufacturerName OBJECT-TYPE
	SYNTAX		DisplayString
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		" "
	REFERENCE "dot11ManufacturerName"
	::= { extremeWirelessPortStatusEntry 12 }

extremeWirelessPortProductName OBJECT-TYPE
	SYNTAX		DisplayString
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		" "
	REFERENCE "dot11ProductName"
	::= { extremeWirelessPortStatusEntry 13 }

extremeWirelessPortSerialNumber OBJECT-TYPE
	SYNTAX		DisplayString
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"This is the unique serial number for this device."
	::= { extremeWirelessPortStatusEntry 14 }

extremeWirelessPortEdpNeighborId  OBJECT-TYPE
	SYNTAX		ExtremeDeviceId
	MAX-ACCESS 	read-only
	STATUS		current
	DESCRIPTION
      		"EDP assigns a unique ID to each neighbor to 
		 disambiguate references.  This can be used to index 
		 into the extremeEdpTable."
	::= { extremeWirelessPortStatusEntry 15 }

extremeWirelessPortClearCounters OBJECT-TYPE
	SYNTAX		TruthValue
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This value can be set to true to force the device
		 to reset it's counters.  A read will return false."
	::= { extremeWirelessPortStatusEntry 16 }

extremeWirelessPortClearLog OBJECT-TYPE
	SYNTAX		TruthValue
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This value can be set to true to force the device
		 to clear its local log store.  A read will return
		 false."
	::= { extremeWirelessPortStatusEntry 17 }

extremeWirelessPortWatchdogReset OBJECT-TYPE
	SYNTAX		TruthValue
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This is to enable/disable watchdog timer reset on timeout. 
		Default is enable. If it is enabled, system should reset
		when the watchdog kicks in. On next bootup, it should 
		send out an syslog message to syslog server.  If it is 
		disabled, it should record the error and not reset the system."
	::= { extremeWirelessPortStatusEntry 18 }

extremeWirelessPortNumPhysInterfaces OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-only
	STATUS		current		
	DESCRIPTION
		"Each wireless port has a set of physical interface which are
		 numbered 1-N.  This variable gives the number of 
		 physical interfaces on this AP."
	::= { extremeWirelessPortStatusEntry 19 }

extremeWirelessPortHWVersion OBJECT-TYPE
	SYNTAX		DisplayString
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"This is the current hardware version of this AP."
	::= { extremeWirelessPortStatusEntry 20 }


extremeWirelessPortMacAddress OBJECT-TYPE
        SYNTAX MacAddress
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Unique MAC Address assigned to the ethernet interface on the AP."
	::= { extremeWirelessPortStatusEntry 21 }

extremeWirelessPortRadiusPortID OBJECT-TYPE
	SYNTAX	DisplayString
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"A string value that should be sent by the AP to the radius
		server as the Port-ID radius attribute in authentication requests"
	::= { extremeWirelessPortStatusEntry 22 }

extremeWirelessPortBootUpTime OBJECT-TYPE
        	SYNTAX	TimeTicks
        	MAX-ACCESS 	read-write
        	STATUS	current
        	DESCRIPTION	
                "The sysUpTime of the LAC when the port was booted up.
		Should be set only during the AP boot up."
	::= { extremeWirelessPortStatusEntry 23 }

extremeWirelessPortCountryCode OBJECT-TYPE
               	SYNTAX ExtremeWirelessCountryCode
        	MAX-ACCESS 	read-write
        	STATUS	current
        	DESCRIPTION	
                "The country code that the AP is programmed to operate in."
	::= { extremeWirelessPortStatusEntry 24 }

extremeWirelessPortWallclockTime OBJECT-TYPE
        	SYNTAX	INTEGER
        	MAX-ACCESS 	read-write
        	STATUS	current
        	DESCRIPTION	
                "The wall clock time as known to the LAC. 
			Expressed in number of seconds since Jan 1, 1970"
	::= { extremeWirelessPortStatusEntry 25 }

extremeWirelessPortPartNumber OBJECT-TYPE
	SYNTAX		DisplayString
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This describes the part number of the AP."
	::= { extremeWirelessPortStatusEntry 26 }

extremeWirelessPortPartRevision OBJECT-TYPE
	SYNTAX		DisplayString
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This describes the revision of the AP."
	::= { extremeWirelessPortStatusEntry 27 }

extremeWirelessPortUpTime OBJECT-TYPE
        	SYNTAX	TimeTicks
        	MAX-ACCESS 	read-write
        	STATUS	current
        	DESCRIPTION	
                "The number of seconds the port has been in the online state."
	::= { extremeWirelessPortStatusEntry 28 }

extremeWirelessPortStatusAntennaType OBJECT-TYPE
        SYNTAX          ExtremeWirelessAntennaType
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This is the type of the Antenna for Detachable product.
                 For Altitude-2d series, further selection is available
                 through this variable."
        ::= { extremeWirelessPortStatusEntry 29 }

extremeWirelessPortStatusAntennaLocation OBJECT-TYPE
        SYNTAX          ExtremeWirelessAntennaLocation
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This specifies the location the detachable antenna."
        ::= { extremeWirelessPortStatusEntry 30 }

extremeWirelessPortStatusAntenna2point4GHZGain OBJECT-TYPE
        SYNTAX      INTEGER
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
               "This specifies 2.4GHz gain value for detachable antenna in dbi"
        ::= { extremeWirelessPortStatusEntry 31 }

extremeWirelessPortStatusAntenna5GHZGain OBJECT-TYPE
        SYNTAX      INTEGER
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
               "This specifies 5GHz gain value for detachable antenna in dbi"
        ::= { extremeWirelessPortStatusEntry 32 }

extremeWirelessPortPrimaryBootloaderVersion OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
        "This is the version of the primary bootloader on this AP."
        ::= { extremeWirelessPortStatusEntry 33 }

extremeWirelessPortSecondaryBootloaderVersion OBJECT-TYPE
        SYNTAX      DisplayString
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
        "This is the version of the Secondary bootloader on this AP."
        ::= { extremeWirelessPortStatusEntry 34 }

extremeWirelessPortCurrentBootloaderInUse OBJECT-TYPE
	SYNTAX INTEGER { primary(1),
			         secondary(2) }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
        "This specifies if the bootloader booted is primary or secondary one."
        ::= { extremeWirelessPortStatusEntry 35 }
-- ************************************************************** --
--                 Wireless Port Syslog Status Table               --
-- ************************************************************** --
extremeWirelessPortLogStatusTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF ExtremeWirelessPortLogStatusEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"This table contains one entry for each wireless port
		 which is configured via the configuration table."
	::= { extremeAP 2 }

extremeWirelessPortLogStatusEntry OBJECT-TYPE
	SYNTAX		ExtremeWirelessPortLogStatusEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		""
	INDEX { extremeWirelessPortIfIndex, 
		extremeWirelessPortLogStatusIndex }
	::= { extremeWirelessPortLogStatusTable 1 }

ExtremeWirelessPortLogStatusEntry ::= SEQUENCE {
	extremeWirelessPortLogStatusIndex	INTEGER,
	extremeWirelessPortLogStatusDestIp	InetAddress,
	extremeWirelessPortLogStatusDestIpType  InetAddressType,
	extremeWirelessPortLogStatusPort	INTEGER,
	extremeWirelessPortLogStatusFacility	INTEGER,
	extremeWirelessPortLogStatusSeverity	INTEGER,
	extremeWirelessPortLogStatusStatus      TruthValue }

extremeWirelessPortLogStatusIndex OBJECT-TYPE
	SYNTAX		INTEGER(1..9)
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"There are 9 entries in this table to correspond to
		 the 8 entries configured in the cfg table plus one
		 for the LAC."
	::= { extremeWirelessPortLogStatusEntry 1 }

extremeWirelessPortLogStatusDestIp OBJECT-TYPE
	SYNTAX		InetAddress
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This is the IP address to which syslog messsages
		 will be sent.  A value of 0.0.0.0 indicates that
		 this entry is disabled. The source IP for every syslog
		message comes from the ManagementIP field in 
		extremeWirelessPortStatusTable"
	::= { extremeWirelessPortLogStatusEntry 2 }

extremeWirelessPortLogStatusDestIpType          OBJECT-TYPE
        SYNTAX                                  InetAddressType
        MAX-ACCESS                              read-write
        STATUS                                  current
        DESCRIPTION
            "The type of address specified in the object
                'extremeWirelessPortLogStatusDestIp.
             Currently, only 'ipv4' and 'dns' are supported."
        DEFVAL { ipv4 }
      ::= { extremeWirelessPortLogStatusEntry 3 }

extremeWirelessPortLogStatusPort OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This is the port to which syslog messages will be
		 sent."
	::= { extremeWirelessPortLogStatusEntry 4 }

extremeWirelessPortLogStatusFacility OBJECT-TYPE
	SYNTAX		INTEGER(0..7)
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"Optional value for syslog facility local0-7."
	::= { extremeWirelessPortLogStatusEntry 5 }

extremeWirelessPortLogStatusSeverity               OBJECT-TYPE
            SYNTAX  INTEGER { 
				critical (0),
				error (1),
				warning (2),
				notice (3),
				info (4),
				debugSummary (5),
				debugVerbose (6),
				debugData (7)					
				}
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                    "The syslog message severity. All syslog
 			messages that have a severity >= specified severity, 
			will be sent to	this syslog server."
            DEFVAL { debugData }
            ::= { extremeWirelessPortLogStatusEntry 6 }

extremeWirelessPortLogStatusStatus OBJECT-TYPE
                SYNTAX TruthValue
                MAX-ACCESS  read-write
                STATUS current
                DESCRIPTION
                        "Specifies whether the log server is enabled or not."
        ::= { extremeWirelessPortLogStatusEntry 7 }


-- ************************************************************** --
--                   Wireless Port Log Table                       --
-- ************************************************************** --
extremeWirelessPortLogTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF ExtremeWirelessPortLogEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"This table allows access to the syslog entries on
		 particular wireless ports."
	::= { extremeAP 3 }

extremeWirelessPortLogEntry OBJECT-TYPE
	SYNTAX		ExtremeWirelessPortLogEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		""
	INDEX { extremeWirelessPortIfIndex, 
		extremeWirelessPortLogIndex }
	::= { extremeWirelessPortLogTable 1 }

ExtremeWirelessPortLogEntry ::= SEQUENCE {
	extremeWirelessPortLogIndex	INTEGER,
	extremeWirelessPortLogMessage	DisplayString }

extremeWirelessPortLogIndex OBJECT-TYPE
	SYNTAX		INTEGER(0..65535)
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"This is an arbitrary integer which is assinged to
		 entries in order of their insertion."
	::= { extremeWirelessPortLogEntry 1 }

extremeWirelessPortLogMessage OBJECT-TYPE
	SYNTAX		DisplayString
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"This is the formatted syslog message which was sent."
	::= { extremeWirelessPortLogEntry 2 }
	
-- ************************************************************** --
--           Wireless Physical Interface Ctl Table                 --
-- This table allows for the configuration of parameters that deal --
-- with physical interfaces. Each radio on the AP is represented by--
-- a physical interface. Each physical interface can have multiple --
-- (upto 8) virtual interfaces. RF properties are configured on the--
-- physical interface using the extremeWirelessInterfaceRFCtlTable --
-- Security parameters are configured on the virtual interface     --
-- using the extremeWirelessInterfaceSecurityCtlTable          --
-- ************************************************************** --

extremeWirelessPhysInterfaceCtlTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF ExtremeWirelessPhysInterfaceCtlEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"This table provides configuration of per-physical interface
		 values."
	::= { extremeAP 4 }

ExtremeWirelessPhysInterfaceCtlEntry ::= SEQUENCE {
	extremeWirelessPhysInterfaceIndex 		ExtremeWirelessPhysInterfaceIndex,
	extremeWirelessPhysInterfacePHYChannel	     INTEGER,
	extremeWirelessPhysInterfaceSpeed			Dot11Speed,
	extremeWirelessPhysInterfaceNumVirtInterfaces INTEGER,
    extremeWirelessPhysInterfaceChannelAutoSelectStatus ExtremeWirelessChannelAutoSelectStatus,
    extremeWirelessPhysInterfaceRadarInterfaceChannelList Dot11AChannel
}


extremeWirelessPhysInterfaceCtlEntry OBJECT-TYPE
	SYNTAX		ExtremeWirelessPhysInterfaceCtlEntry
	MAX-ACCESS	not-accessible
	STATUS		current	
	DESCRIPTION
		"Each entry is indexed by the wirelessInterfaceIndex, and
		represents a wireless interface."
	INDEX { extremeWirelessPhysInterfaceIndex }
	::= { extremeWirelessPhysInterfaceCtlTable 1 }

extremeWirelessPhysInterfaceIndex OBJECT-TYPE
	SYNTAX	ExtremeWirelessPhysInterfaceIndex
	MAX-ACCESS	accessible-for-notify
	STATUS		current
	DESCRIPTION
		"This is the ifIndex of an individual physical interface on an AP.
		Each radio will have a unique value."
	::= { extremeWirelessPhysInterfaceCtlEntry 1 }


extremeWirelessPhysInterfacePHYChannel OBJECT-TYPE
	SYNTAX		INTEGER (0..99)
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This is the RF channel which will be used by 
		 this transmitter.  Range should be established
		 by configuration of RegDomain and PHYType."
	::= { extremeWirelessPhysInterfaceCtlEntry 2 }

extremeWirelessPhysInterfaceSpeed OBJECT-TYPE
	SYNTAX		Dot11Speed 
	MAX-ACCESS	 read-write
	STATUS		 current
	DESCRIPTION
		"This value indicates the current setting for 
		 Tx speed for the interface. Only one of thebits of this bit set can be set.
		 If all bits are unset (ie a 0 is passed as a value) then 
		 it means that the interface should choose a speed
		 based on some algorithm."
	::= { extremeWirelessPhysInterfaceCtlEntry 3 }

extremeWirelessPhysInterfaceNumVirtInterfaces OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	 read-write
	STATUS		 current
	DESCRIPTION
		"Each physical interface has a number of virtual interfaces
	 	 This specifies the number of virt interfaces."
	::= { extremeWirelessPhysInterfaceCtlEntry 4 }

-- Added for DFS
extremeWirelessPhysInterfaceChannelAutoSelectStatus OBJECT-TYPE
    SYNTAX          ExtremeWirelessChannelAutoSelectStatus 
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "This OID reflects the status of the channel auto selection process."
        ::= { extremeWirelessPhysInterfaceCtlEntry 5 }

-- Added for DFS
extremeWirelessPhysInterfaceRadarInterfaceChannelList OBJECT-TYPE
        SYNTAX          Dot11AChannel 
        MAX-ACCESS       read-only
        STATUS           current
        DESCRIPTION
                "This OID reflects the list oc 802.11(a) channels on which
radar interference was detected."
        ::= { extremeWirelessPhysInterfaceCtlEntry 6 }

	
	
-- ************************************************************** --
--           Wireless Virtual  Interface Ctl Table                 --
-- This table allows for the configuration of parameters that deal --
-- with virtual interfaces. Each radio on the AP is represented by--
-- a physical interface. Each physical interface can have multiple --
-- (upto 8) virtual interfaces. RF properties are configured on the--
-- physical interface using the extremeWirelessInterfaceRFCtlTable --
-- Security parameters are configured on the virtual interface     --
-- using the extremeWirelessInterfaceSecurityCtlTable          --
-- ************************************************************** --
extremeWirelessVirtInterfaceCtlTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF ExtremeWirelessVirtInterfaceCtlEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"This table provides configuration of per-physical-interface
		 values."
	::= { extremeAP 6 }

ExtremeWirelessVirtInterfaceCtlEntry ::= SEQUENCE {
	extremeWirelessVirtInterfaceIndex 		        ExtremeWirelessVirtInterfaceIndex,
	extremeWirelessVirtInterfaceMacAddress		    MacAddress,
	extremeWirelessVirtInterfaceMaxClients		    INTEGER,
	extremeWirelessVirtInterfaceWirelessBridging	TruthValue,
	extremeWirelessVirtInterfaceLastStateChange	    TimeTicks,
	extremeWirelessVirtInterfaceState		        INTEGER,
    extremeWirelessVirtInterfaceIappEnabled         TruthValue,
    extremeWirelessVirtInterfaceSvpEnabled          TruthValue
}

extremeWirelessVirtInterfaceCtlEntry OBJECT-TYPE
	SYNTAX		ExtremeWirelessVirtInterfaceCtlEntry
	MAX-ACCESS	not-accessible
	STATUS		current	
	DESCRIPTION
		"Each entry is indexed by the wirelessInterfaceIndex, and
		represents a virtual wireless interface."
	INDEX { extremeWirelessVirtInterfaceIndex }
	::= { extremeWirelessVirtInterfaceCtlTable 1 }

extremeWirelessVirtInterfaceIndex OBJECT-TYPE
	SYNTAX	ExtremeWirelessVirtInterfaceIndex
	MAX-ACCESS	accessible-for-notify
	STATUS		current
	DESCRIPTION
		"This is the ifIndex of an individual interface on an AP.
		Each virtual interface will have a unique value."
	::= { extremeWirelessVirtInterfaceCtlEntry 1 }
	
extremeWirelessVirtInterfaceMacAddress OBJECT-TYPE
	SYNTAX		MacAddress
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The maximum number of clients that can associate with this virtual interface."
	::= { extremeWirelessVirtInterfaceCtlEntry 2 }

extremeWirelessVirtInterfaceMaxClients OBJECT-TYPE
	SYNTAX		INTEGER (1..128)
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"The maximum number of clients that can associate with this virtual interface."
	::= { extremeWirelessVirtInterfaceCtlEntry 3 }

extremeWirelessVirtInterfaceWirelessBridging OBJECT-TYPE
	SYNTAX		TruthValue
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This specifies whether wireless bridging is enabled on this interface.
		 If wireless bridging is enabled then traffic originating from a client on this
		 interface will be bridged to clients on the same VLAN on this or other 
		 virtual interfaces that have wireless bridging enabled. So basically
		 wireless bridging should be enabled on both the source and the destination
		 virtual interface for traffic to be bridged."
	::= { extremeWirelessVirtInterfaceCtlEntry 4 }

extremeWirelessVirtInterfaceLastStateChange OBJECT-TYPE
	SYNTAX		TimeTicks
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The value of sysUpTime when the virtual interface entered its current state"
	::= { extremeWirelessVirtInterfaceCtlEntry 5 }

extremeWirelessVirtInterfaceState OBJECT-TYPE
	SYNTAX		INTEGER { enabled(1), disabled(2) } 
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This value specifies whether the virtual interface is active or not"
	::= { extremeWirelessVirtInterfaceCtlEntry 6 }

extremeWirelessVirtInterfaceIappEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
    "IAPP status. A value of TRUE indicates IAPP is enabled on the
    interface."
    ::= { extremeWirelessVirtInterfaceCtlEntry 7 }

extremeWirelessVirtInterfaceSvpEnabled OBJECT-TYPE
    SYNTAX          TruthValue
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
    "SVP status. A value of TRUE indicates SVP is enabled on the
    interface."
    ::= { extremeWirelessVirtInterfaceCtlEntry 8 }

-- ************************************************************** --
--              Wireless Interface Security Ctl Table              --
-- This table allows for the configuration of per-wireless-intf    --
-- security parameters. Each Wireless interface is represented in  --
-- ifTable, and is represented by extremeWirelessInterfaceIfIndex. --
-- ************************************************************** --
extremeWirelessVirtInterfaceSecurityCtlTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF ExtremeWirelessVirtInterfaceSecurityCtlEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"This table provides configuration of per-interface
		 values."
	::= { extremeAP 7 }

extremeWirelessVirtInterfaceSecurityCtlEntry OBJECT-TYPE
	SYNTAX		ExtremeWirelessVirtInterfaceSecurityCtlEntry
	MAX-ACCESS	not-accessible
	STATUS		current	
	DESCRIPTION
		"Each entry is indexed by the wirelessInterfaceIndex, and
		represents a wireless interface."
	INDEX { extremeWirelessVirtInterfaceIndex }
	::= { extremeWirelessVirtInterfaceSecurityCtlTable 1 }

ExtremeWirelessVirtInterfaceSecurityCtlEntry ::= SEQUENCE {
	extremeWirelessVirtInterfaceESSName		OCTET STRING,
	extremeWirelessVirtInterfaceSSIDInBeacon	TruthValue,
	extremeWirelessVirtInterfaceDot11AuthMode	Dot11AuthMode, 
	extremeWirelessVirtInterfaceNetworkAuthMode	NetworkAuthMode, 
	extremeWirelessVirtInterfaceDataVlan	INTEGER,
	extremeWirelessVirtInterfaceIgnoreVSAVlan	TruthValue,
	extremeWirelessVirtInterfaceWEPDefaultKey	INTEGER,
	extremeWirelessVirtInterfaceEncryptionLength 		INTEGER
}

extremeWirelessVirtInterfaceESSName OBJECT-TYPE
	SYNTAX		OCTET STRING
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"The ESS ID of this interface."
	::= { extremeWirelessVirtInterfaceSecurityCtlEntry 1 }

extremeWirelessVirtInterfaceSSIDInBeacon OBJECT-TYPE
	SYNTAX		TruthValue
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"Does this interface generate a beacon with the
		 SSID in it?"
	::= { extremeWirelessVirtInterfaceSecurityCtlEntry 2 }

extremeWirelessVirtInterfaceDot11AuthMode OBJECT-TYPE
	SYNTAX		Dot11AuthMode
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"Setting this to true indicates whether to use open or shared authentication"
	::= { extremeWirelessVirtInterfaceSecurityCtlEntry 3 }

extremeWirelessVirtInterfaceNetworkAuthMode OBJECT-TYPE
	SYNTAX		NetworkAuthMode
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This specifies the authentication mode to use on top of dot11 MAC authentication"
	::= { extremeWirelessVirtInterfaceSecurityCtlEntry 4 }

extremeWirelessVirtInterfaceDataVlan OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This is the VLAN to use for client data in case of the VLAN is not received as a VSA. 
		This VLAN is also used for authentication types like PSK, WEP, etc"
	::= { extremeWirelessVirtInterfaceSecurityCtlEntry 5 }

extremeWirelessVirtInterfaceIgnoreVSAVlan OBJECT-TYPE
	SYNTAX		TruthValue
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"If this is set then the VLAN returned as a VSA will be ignored and the Data Vlan specified above
		will be used instead"
	::= { extremeWirelessVirtInterfaceSecurityCtlEntry 6 }

extremeWirelessVirtInterfaceWEPDefaultKey OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This value indicates the index in dot11WEPDefaultKeyTable that 
		identifies the key this interface will use to decrypt packets."
	::= { extremeWirelessVirtInterfaceSecurityCtlEntry 7 }

extremeWirelessVirtInterfaceEncryptionLength OBJECT-TYPE
	SYNTAX      INTEGER { none(0),
	 		      sixtyfour(64),
                              onetwentyeight(128)  }
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This is the length of the encryption key to use in case
	         of dot1x legacy mode and WEP. If this length is 0 then no WEP encryption."
	::= { extremeWirelessVirtInterfaceSecurityCtlEntry 8 }

-- ************************************************************** --
--              Wireless Interface Dot1x Ctl Table              --
-- This table allows for the configuration of per-wireless-intf    --
-- dot1x parameters. Each Wireless interface is represented in  --
-- ifTable, and is represented by extremeWirelessVirtInterfaceIfIndex. --
-- ************************************************************** --
extremeWirelessVirtInterfaceDot1xCtlTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF ExtremeWirelessVirtInterfaceDot1xCtlEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"There is one entry in this table for each virtual interface 
		It reflects the dot1x security config"
	::= { extremeAP 8 }

extremeWirelessVirtInterfaceDot1xCtlEntry OBJECT-TYPE
	SYNTAX	ExtremeWirelessVirtInterfaceDot1xCtlEntry
	MAX-ACCESS	not-accessible
	STATUS	current
	DESCRIPTION
		""
	INDEX { extremeWirelessVirtInterfaceIndex }
	::= { extremeWirelessVirtInterfaceDot1xCtlTable 1 }

ExtremeWirelessVirtInterfaceDot1xCtlEntry ::= SEQUENCE {
	extremeWirelessVirtInterfaceKeyMgmtSuite		WPAKeyMgmtSet,
	extremeWirelessVirtInterfaceMcastCipherSuite	WPACipherSet,
	extremeWirelessVirtInterfaceDot1xPSKValue		OCTET STRING,
	extremeWirelessVirtInterfaceDot1xPSKPassPhrase	DisplayString,
	extremeWirelessVirtInterfaceDot1xReAuthPeriod	INTEGER,
	extremeWirelessVirtInterfaceGroupUpdateTimeOut	Unsigned32,
	extremeWirelessVirtInterfacePairwiseUpdateTimeOut Unsigned32,
        extremeWirelessVirtInterfaceDot11iPreauthEnable TruthValue
}

extremeWirelessVirtInterfaceKeyMgmtSuite OBJECT-TYPE
	SYNTAX	WPAKeyMgmtSet
	MAX-ACCESS	read-write
	STATUS	current
	DESCRIPTION
		"This bitmask configures the authentication suites to be used."
	::= { extremeWirelessVirtInterfaceDot1xCtlEntry 1 }

extremeWirelessVirtInterfaceMcastCipherSuite OBJECT-TYPE
	SYNTAX	WPACipherSet
	MAX-ACCESS	read-write
	STATUS	current
	DESCRIPTION
		"This configures the cipher suite to use for mcast traffic. The cipher suite to use for unicast traffic
		 is derived from this using the following algorithm:
			Mcast cipher = WEP (64/128), Unicast cipher = TKIP
			Mcast cipher = TKIP, Unicast cipher = TKIP
			Mcast cipher = AES, Unicast cipher = AES.
		 This therefore determines the max unicast cipher suite the client can use to associate with 
		 this interface."
	::= { extremeWirelessVirtInterfaceDot1xCtlEntry 2 }


extremeWirelessVirtInterfaceDot1xPSKValue OBJECT-TYPE
	SYNTAX		OCTET STRING (SIZE(32))
	MAX-ACCESS	read-write
	STATUS		current	
	DESCRIPTION
		"The Pre-Shared Key (PSK) for when WPA in PSK mode is
		 the selected authentication suite."
	REFERENCE "dot11RSNConfigPSKValue"
	::= { extremeWirelessVirtInterfaceDot1xCtlEntry 3 }

extremeWirelessVirtInterfaceDot1xPSKPassPhrase OBJECT-TYPE
	SYNTAX		DisplayString
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
	"The PSK, for when WPA in PSK mode is the selected authentication
	 suite, is configured by extremeWirelessVirtInterfaceKeyMgmtSuite.
	 An alternative manner of setting the PSK uses the password-to-key
	 algorithm defined in section XXX. This variable provides a means
	 to enter a pass phrase. When this object is written, the RSN
	 entity shall use the password-to-key algorithm specified in
	 section XXX to derive a pre-shared and populate
	 extremeWirelessVirtInerfaceDot1xPSKValue with this key.
	 This object is logically write-only. Reading this variable shall
	 return unsuccessful status or null or zero."
	::= { extremeWirelessVirtInterfaceDot1xCtlEntry 4 }

extremeWirelessVirtInterfaceDot1xReAuthPeriod OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"Number of seconds a clients authentication will last before
		 the AP automatically issues a reauthentication request."
	::= { extremeWirelessVirtInterfaceDot1xCtlEntry 5 }

extremeWirelessVirtInterfaceGroupUpdateTimeOut OBJECT-TYPE
	SYNTAX		Unsigned32 (1..1440)
	UNITS		"minutes"
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"The time in minutes after which the RSN group
		 update handshake will be retried. The timer shall
		 start at the moment the group update message is
		 sent."
	REFERENCE "dot11RSNConfigGroupUpdateTimeOut"
	DEFVAL		{ 100 } -- 
	::= { extremeWirelessVirtInterfaceDot1xCtlEntry 6 }

extremeWirelessVirtInterfacePairwiseUpdateTimeOut OBJECT-TYPE
	SYNTAX		Unsigned32 (1..1440)
	UNITS		"minutes"
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"The time in minutes after which the RSN 4-way
		 handshake will be retried. The timer shall start at
		 the moment a 4-way message is sent."
	REFERENCE "dot11RSNConfigPairwiseUpdateTimeOut"
	DEFVAL		{ 100 } -- 
	::= { extremeWirelessVirtInterfaceDot1xCtlEntry 7 }

extremeWirelessVirtInterfaceDot11iPreauthEnable OBJECT-TYPE
        SYNTAX          TruthValue
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "Enables/Disable 802.11i pre-authentication."
        ::= { extremeWirelessVirtInterfaceDot1xCtlEntry 8 }

-- ************************************************************** --
--                     Default WEP Key Table                       --
-- ************************************************************** --
extremeWirelessVirtInterfaceWEPKeyTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF ExtremeWirelessVirtInterfaceWEPKeyEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"This table contains per-profile WEP keys.

		 Reference ieee802dot11.1.2.3."
	::= { extremeAP 9 }

extremeWirelessVirtInterfaceWEPKeyEntry OBJECT-TYPE
	SYNTAX	ExtremeWirelessVirtInterfaceWEPKeyEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		" "
	INDEX { extremeWirelessVirtInterfaceIndex, extremeWirelessVirtInterfaceWEPKeyIndex }
	::= { extremeWirelessVirtInterfaceWEPKeyTable 1 }
	
ExtremeWirelessVirtInterfaceWEPKeyEntry ::= SEQUENCE {
	extremeWirelessVirtInterfaceWEPKeyIndex	INTEGER,
	extremeWirelessVirtInterfaceWEPKey		OCTET STRING,
	extremeWirelessVirtInterfaceWEPKeyStatus	TruthValue }
	
extremeWirelessVirtInterfaceWEPKeyIndex OBJECT-TYPE
	SYNTAX 		INTEGER(1..4)
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"There can be upto 4 wep keys for any wireless
		 interface. Four of the keys are to be used with
		 WEP Authentication, and the other four with MAC Auth."
	::= { extremeWirelessVirtInterfaceWEPKeyEntry 1 }

extremeWirelessVirtInterfaceWEPKey OBJECT-TYPE
	SYNTAX		OCTET STRING (SIZE(1..19))
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION
		"This is a write-only wep key."
	::= { extremeWirelessVirtInterfaceWEPKeyEntry 2 }

extremeWirelessVirtInterfaceWEPKeyStatus OBJECT-TYPE
	SYNTAX		TruthValue
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION
		"Specifies whether the key is present or not."
	::= { extremeWirelessVirtInterfaceWEPKeyEntry 3 }

-- ************************************************************** --
--              Wireless Interface RF Ctl Table                    --
-- This table allows for the configuration of per-wireless-intf    --
-- RF parameters. Each Wireless interface is represented in        --
-- ifTable, and is represented by extremeWirelessPhysInterfaceIfIndex. --
-- ************************************************************** --
extremeWirelessPhysInterfaceRFCtlTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF ExtremeWirelessPhysInterfaceRFCtlEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"This table provides configuration of per-interface
		 values."
	::= { extremeAP 10 }

extremeWirelessPhysInterfaceRFCtlEntry OBJECT-TYPE
	SYNTAX		ExtremeWirelessPhysInterfaceRFCtlEntry
	MAX-ACCESS	not-accessible
	STATUS		current	
	DESCRIPTION
		"Each entry is indexed by the wirelessInterfaceIndex, and
		represents a wireless interface."
	INDEX { extremeWirelessPhysInterfaceIndex }
	::= { extremeWirelessPhysInterfaceRFCtlTable 1 }

ExtremeWirelessPhysInterfaceRFCtlEntry ::= SEQUENCE {
	extremeWirelessPhysInterfaceBeaconPeriod 	INTEGER,
	extremeWirelessPhysInterfaceTxPowerLevel 	INTEGER,
	extremeWirelessPhysInterfaceDTIMPeriod 	INTEGER,
	extremeWirelessPhysInterfaceFragLength	INTEGER,
	extremeWirelessPhysInterfaceLongRetry 	INTEGER,	
	extremeWirelessPhysInterfaceShortRetry 	INTEGER,
	extremeWirelessPhysInterfaceRTSThreshold 	INTEGER,
	extremeWirelessPhysInterfaceSupportedDataRatesRxValue Dot11Speed,
	extremeWirelessPhysInterfaceSupportedDataRatesTxValue Dot11Speed,
	extremeWirelessPhysInterfacePHYType		     Dot11Type,
	extremeWirelessPhysInterfacePHYSupportedTypes     BITS,
	extremeWirelessPhysInterfacePreamble		INTEGER,
    extremeWirelessPhysInterfaceAbsTxPowerLevel INTEGER
}

extremeWirelessPhysInterfaceBeaconPeriod OBJECT-TYPE
	SYNTAX		INTEGER 
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This is the beacon interval to use"
	::= { extremeWirelessPhysInterfaceRFCtlEntry 1 }

extremeWirelessPhysInterfaceTxPowerLevel OBJECT-TYPE
	SYNTAX		INTEGER (1..100)
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This is the % of max power to transmit at."
	::= { extremeWirelessPhysInterfaceRFCtlEntry 2 }

extremeWirelessPhysInterfaceDTIMPeriod OBJECT-TYPE
	SYNTAX		INTEGER 
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This is the DTIM period."
	::= { extremeWirelessPhysInterfaceRFCtlEntry 3 }

extremeWirelessPhysInterfaceFragLength OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		" "
	REFERENCE "ieee802dot11.2.1.1.5."
	::= { extremeWirelessPhysInterfaceRFCtlEntry 4 }

extremeWirelessPhysInterfaceLongRetry OBJECT-TYPE
	SYNTAX		INTEGER (1..255)
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION		
		"Attribute indicates the maximum number of transmission
		 attempts of a frame whose size is > RTS."
	REFERENCE "dot11LongRetryLimit"
	::= { extremeWirelessPhysInterfaceRFCtlEntry 5 }

extremeWirelessPhysInterfaceShortRetry OBJECT-TYPE
	SYNTAX		INTEGER (1..255)
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION		
		"Attribute indicates the maximum number of transmission
		 attempts of a frame whose size is <= RTS."
	REFERENCE "dot11ShortRetryLimit"
	::= { extremeWirelessPhysInterfaceRFCtlEntry 6 }

extremeWirelessPhysInterfaceRTSThreshold OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-write
	STATUS		current	
	DESCRIPTION 
		" "
	REFERENCE "ieee802dot11.2.1.1.2."
	::= { extremeWirelessPhysInterfaceRFCtlEntry 7 }

extremeWirelessPhysInterfaceSupportedDataRatesRxValue OBJECT-TYPE
	SYNTAX		Dot11Speed
	MAX-ACCESS	read-only
	STATUS		current	
	DESCRIPTION 
		"A bitmask of all supported datarates for Rx."
	::= { extremeWirelessPhysInterfaceRFCtlEntry 8 }
	
extremeWirelessPhysInterfaceSupportedDataRatesTxValue OBJECT-TYPE
	SYNTAX		Dot11Speed
	MAX-ACCESS	read-only
	STATUS		current	
	DESCRIPTION 
		"A bitmask of all supported datarates for Tx."
	::= { extremeWirelessPhysInterfaceRFCtlEntry 9 }

extremeWirelessPhysInterfacePHYType OBJECT-TYPE
	SYNTAX	       Dot11Type
	MAX-ACCESS     read-write
	STATUS	       current
	DESCRIPTION
		"This variable selects between 802.11 a/b/g 
		 for this transmitter.  It should be used by
		 ap to range check frequency, etc."
	::= { extremeWirelessPhysInterfaceRFCtlEntry 10 }

extremeWirelessPhysInterfacePHYSupportedTypes OBJECT-TYPE
	SYNTAX 		BITS { bsupported(0),
			       asupported(1),
			       gsupported(2) }
	MAX-ACCESS 	read-only
	STATUS 		current
	DESCRIPTION
		"This is the 802.11 standard supported by this
		 interface as a bitmask"
	::= { extremeWirelessPhysInterfaceRFCtlEntry 11 }

extremeWirelessPhysInterfacePreamble OBJECT-TYPE
	SYNTAX		INTEGER { short(0),
				  long(1) }
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This changes the 802 preamble expected by the
		 interface."
	::= { extremeWirelessPhysInterfaceRFCtlEntry 12 }

extremeWirelessPhysInterfaceAbsTxPowerLevel OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "This is the absolute value of max power to transmit level in dBm."
    ::= { extremeWirelessPhysInterfaceRFCtlEntry 13 }

-- ************************************************************** --
-- Wireless Interface Status Table
-- ************************************************************** --
extremeWirelessInterfaceStatusTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF ExtremeWirelessInterfaceStatusEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
	"This table provides statistics and information on the
	current condition of each wireless interace.
	There is one entry per virtual and physical wireless 
	interface in this table.  The values for the physical 
	interfaces represent the sum of the values for all sub
	interfaces."
	::= { extremeAP 5 }

extremeWirelessInterfaceStatusEntry OBJECT-TYPE
	SYNTAX		ExtremeWirelessInterfaceStatusEntry
	MAX-ACCESS	not-accessible
	STATUS		current	
	DESCRIPTION
	"Each entry in this table is indexed by either a virtual or
	a physical ifIndex."
	INDEX { ifIndex }
	::= { extremeWirelessInterfaceStatusTable 1 }
	
ExtremeWirelessInterfaceStatusEntry ::= SEQUENCE {
	extremeWirelessIntfTotalDetected    Unsigned32,
	extremeWirelessIntfTotalAuthed      Unsigned32,
	extremeWirelessIntfTotalAuthFailed  Unsigned32,
	extremeWirelessIntfTotalAssoc       Unsigned32,
    extremeWirelessIntfTotalAssocFailed Unsigned32,
	extremeWirelessIntfRateDetected     Unsigned32,
	extremeWirelessIntfRateAuthed       Unsigned32,
	extremeWirelessIntfRateAuthFailed   Unsigned32,
    extremeWirelessIntfRateAssoc        Unsigned32,
    extremeWirelessIntfRateAssocFailed  Unsigned32,
    extremeWirelessIntfBlockTime        Unsigned32,
	extremeWirelessIntfCurrentDetected    Unsigned32,
	extremeWirelessIntfCurrentAuthed      Unsigned32,
	extremeWirelessIntfCurrentAssoc       Unsigned32,
	extremeWirelessIntfCurrentForwarding  Unsigned32}

	
extremeWirelessIntfTotalDetected OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of stations which have entered
	the detected state on this wireless interface since the last
	time the counters were cleared."
	::= { extremeWirelessInterfaceStatusEntry 1 }
	
extremeWirelessIntfTotalAuthed OBJECT-TYPE	
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of stations which have entered
	the authenticated state on this wireless interface since the 
	last time the counters were cleared.  Note that this is equal 
	to the number of stations which have entered the forwarding 
	state.  This is not necessaryly equivalent to the number of
	stations which have succeeded in MAC-level authentication."
	::= { extremeWirelessInterfaceStatusEntry 2 }
	
extremeWirelessIntfTotalAuthFailed OBJECT-TYPE	
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of stations which have failed
	to authenticate on this wireless interface.  Note that no
	distinction is made between a MAC-layer or higher-layer
	authentication failure."
	::= { extremeWirelessInterfaceStatusEntry 3 }
	
extremeWirelessIntfTotalAssoc OBJECT-TYPE	
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of stations which have entered
	the associated state on this wireless interface since the 
	last time the counters were cleared."
	::= { extremeWirelessInterfaceStatusEntry 4 }

extremeWirelessIntfTotalAssocFailed OBJECT-TYPE   
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the total number of stations which have failed
    the association on this wireless interface since the 
    last time the counters were cleared."
    ::= { extremeWirelessInterfaceStatusEntry 5 }

extremeWirelessIntfRateDetected OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the rate of clients being detected on this 
	 interface over a 5 second period using EMWA averaging."
	::= { extremeWirelessInterfaceStatusEntry 6 }

extremeWirelessIntfRateAuthed OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives teh rate of clients being authenticated on this 
    interface over a 5 second period using EMWA averaging."
	::= { extremeWirelessInterfaceStatusEntry 7 }

extremeWirelessIntfRateAuthFailed OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the rate of clients failed authentication on this
	 interface over a 5 second period using EMWA averaging."
	::= { extremeWirelessInterfaceStatusEntry 8 }

extremeWirelessIntfRateAssoc OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the rate of clients being associated on this 
    interface over a 5 second period using EMWA averaging."
    ::= { extremeWirelessInterfaceStatusEntry 9 }

extremeWirelessIntfRateAssocFailed OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the rate of clients failing association on this 
    interface over a 5 second period using EMWA averaging."
    ::= { extremeWirelessInterfaceStatusEntry 10 }

extremeWirelessIntfBlockTime OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "This value specifies the number of ticks until traffic will be 
    allowed back on this interface.  A non-zero value indicates that
    traffic has been blocked, most likely due to countermeasures."
    ::= { extremeWirelessInterfaceStatusEntry 11 }

extremeWirelessIntfCurrentDetected OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the current number of stations which are in
	the detected state on this wireless interface."
	::= { extremeWirelessInterfaceStatusEntry 12 }
	
extremeWirelessIntfCurrentAuthed OBJECT-TYPE	
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the current number of stations which are in
	the authenticated state on this wireless interface."
	::= { extremeWirelessInterfaceStatusEntry 13 }
	
extremeWirelessIntfCurrentAssoc OBJECT-TYPE	
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the current number of stations which are in
	the associated state on this wireless interface."
	::= { extremeWirelessInterfaceStatusEntry 14 }

extremeWirelessIntfCurrentForwarding OBJECT-TYPE	
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the current number of stations which are in
	the forwarding state on this wireless interface."
	::= { extremeWirelessInterfaceStatusEntry 15 }

--TODO: Do we need to fix this table
-- ************************************************************** --
--                     AP Wireless Client Table                    --
-- ************************************************************** --
extremeWirelessClientTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF ExtremeWirelessClientEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"This table augments the Dot11AccessPointAddressTableEntry
		 to add a per-client VLAN entry."
	::= { extremeAP 11 }
	
extremeWirelessClientEntry OBJECT-TYPE
	SYNTAX		ExtremeWirelessClientEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
	"An entry in the extremeWirelessClientTable. It is possible
	 for there to be multiple IEEE 802.11 interfaces on one agent,
	 each with its unique MAC address. The relationship between an
	 IEEE 802.11 interface and an interface in the context of the
	 Internet-standard MIB is one-to-one. As such, the value of an
	 ifIndex object instance can be directly used to identify
	 corresponding instances of the objects defined herein. by
	 ifIndex."
    INDEX {ifIndex, extremeWirelessClientID} 
	::= { extremeWirelessClientTable 1 }

ExtremeWirelessClientEntry ::= SEQUENCE {
	extremeWirelessClientID 		MacAddress, 
	extremeWirelessClientState 		INTEGER, 
	extremeWirelessClientEncryption 	WPACipherSet, 
	extremeWirelessClientSignalStrength INTEGER, 
	extremeWirelessClientLinkQuality 	INTEGER, 
	extremeWirelessClientVLAN		INTEGER,
	extremeWirelessClientPriority		INTEGER,
	extremeWirelessClientAuthType		ClientAuthType,
	extremeWirelessClientLastStateChangeTime 	TimeTicks, 
	extremeWirelessClientTxFrames		Counter32,
	extremeWirelessClientRxFrames		Counter32,
	extremeWirelessClientTxBytes		Counter64,
	extremeWirelessClientRxBytes		Counter64,
	extremeWirelessClientLastPacketType	INTEGER,
	extremeWirelessClientSSID		OCTET STRING,
	extremeWirelessClientStatus		RowStatus,
    extremeWirelessClientIP	                IpAddress,
    extremeWirelessClientUsername           DisplayString,
    extremeWirelessClientDecryptionFailures Counter32,
    extremeWirelessClientMICFailures        Counter32}

extremeWirelessClientID OBJECT-TYPE 
    SYNTAX MacAddress 
    MAX-ACCESS read-only 
    STATUS current 
    DESCRIPTION 
	"The Unique MAC Address of the station for which this address 
	 table entry pertains." 
    ::= { extremeWirelessClientEntry 1 } 

extremeWirelessClientState OBJECT-TYPE 
    SYNTAX INTEGER { detected (1),
			authenticated (2), 
			associated (3) ,
			data-forwarding (4)} 
    MAX-ACCESS read-only 
    STATUS current 
    DESCRIPTION 
	"This attribute shall indicate the current state of the connection
	 between a wireless station and the AP. The attribute is
	 enumerated as follows: 

	1 - Detected - station has been detected, but not is communicating with AP
	2 - Authenticated - station is authenticated but not currently 
			associated. 
	3 - Associated - station is authenticated and associated 
	4 - Data-forwarding - station is on the network
	It is assumed that if an station is deauthenticated, or disassociated 
	then it no longer has an entry the AP's Address Table." 
    ::= { extremeWirelessClientEntry 2 } 

extremeWirelessClientEncryption OBJECT-TYPE 
    SYNTAX WPACipherSet
    MAX-ACCESS read-only 
    STATUS current 
    DESCRIPTION 
	"This attribute is contains the encryption mechanism being used 
	 by the station in an AP that allows mixed encryption modes." 
    ::= { extremeWirelessClientEntry 3 } 

extremeWirelessClientSignalStrength OBJECT-TYPE 
    SYNTAX INTEGER (1..100) 
    MAX-ACCESS read-only 
    STATUS current 
    DESCRIPTION 
	"This attribute shall specify the signal strength of the last
	 frame received from the station in - dBm. e.g. a value of 50
	 implies -50 dBm." 
    ::= { extremeWirelessClientEntry 4 } 

extremeWirelessClientLinkQuality OBJECT-TYPE 
    SYNTAX INTEGER (1..100) 
    MAX-ACCESS read-only 
    STATUS current 
    DESCRIPTION 
	"This attribute shall contain an indication of the quality 
	 of the signal as measured in the last frame received from the 
	 station. TBD format of this attribute" 
    ::= { extremeWirelessClientEntry 5 } 

extremeWirelessClientVLAN OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"This is the per-client VLAN which was pushed over
		 by a RADIUS server or other mechanism."
	::= { extremeWirelessClientEntry 6 }

extremeWirelessClientPriority OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"This is a per-client 802.1p value which was either
		 configured by the RADIUS server or statically through
		 the port configuration table."
	::= { extremeWirelessClientEntry 7 }

extremeWirelessClientAuthType OBJECT-TYPE
	SYNTAX		ClientAuthType
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"This is an indication of what access method was 
		 used to authenticated the client.  The strongest
		 mechanism used should be listed here, in case more
		 than one was used.  For example, if a combination of
		 mac-based shared-key and dot1x were used, this value
		 should indicated dot1x."
	::= { extremeWirelessClientEntry 8 }

extremeWirelessClientLastStateChangeTime OBJECT-TYPE
	SYNTAX		TimeTicks
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"This is the sysUpTime of the switch when the clients state changed last"
	::= { extremeWirelessClientEntry 9 }

extremeWirelessClientTxFrames OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"This is the number of packets transmitted to the client"
	::= { extremeWirelessClientEntry 10 }

extremeWirelessClientRxFrames OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"This is the number of packets transmitted by the client"
	::= { extremeWirelessClientEntry 11 }

extremeWirelessClientTxBytes OBJECT-TYPE
	SYNTAX	Counter64
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"This is the number of bytes transmitted to the client"
	::= { extremeWirelessClientEntry 12 }

extremeWirelessClientRxBytes OBJECT-TYPE
	SYNTAX	Counter64
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"This is the number of bytes transmitted by the client"
	::= { extremeWirelessClientEntry 13 }

extremeWirelessClientLastPacketType OBJECT-TYPE
	SYNTAX	INTEGER { data (0),
				psPoll (1),
				probeRequest (2),
				disassociation (3),
				deauthentication (4),
				association (5),
				reassociation (6),
				authentication (7) }
--				inf-beacon (8),
--				adhoc-beacon (9) }				
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"This the the last packet type seen from the specific client"
	::= { extremeWirelessClientEntry 14 }

extremeWirelessClientSSID OBJECT-TYPE
	SYNTAX	OCTET STRING
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"The SSID that this client was using"
	::= { extremeWirelessClientEntry 15 }

extremeWirelessClientStatus OBJECT-TYPE
	SYNTAX	RowStatus
	MAX-ACCESS	read-write
	STATUS	current
	DESCRIPTION
		"This variable is used to delete an entry from the table.
		The only value this can be set to, is delete (6).
		
		If an entry is deleted, that is already in Associated or 
		data-forwarding state, then the AP should dis-associate the 
		particular client by sending a disassociate message.
		
		If an entry is in Authenticated state, and is deleted, then 
		the AP should 'deAuthenticate' that client.
		
		If an entry is in 'detected' state and is deleted, then the
		entry should just be removed from the table."
	::= { extremeWirelessClientEntry 16 }

extremeWirelessClientIP OBJECT-TYPE
	SYNTAX		IpAddress
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"IP Address of the wireless client."
	::= { extremeWirelessClientEntry 17 }

    extremeWirelessClientUsername OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
    "Username (if any) of the wireless client."
    ::= { extremeWirelessClientEntry 18 }

extremeWirelessClientDecryptionFailures OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"This is the number of failures during decrypting packets from this client."
	::= { extremeWirelessClientEntry 19 }

extremeWirelessClientMICFailures OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"This is the number of MIC failures for this client."
	::= { extremeWirelessClientEntry 20 }

-- ************************************************************** --
--                  RF Profile Table                         	   --
-- ************************************************************** --
extremeRFProfile OBJECT IDENTIFIER ::= { extremeProfile 1 }

extremeRFProfileTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF ExtremeRFProfileEntry
	MAX-ACCESS 	not-accessible
	STATUS		current	
	DESCRIPTION
		"There is one entry in this table for each RF profile
		 defined on the LAC.  Configuration for wireless intf.
		 should only be done by manipulating these variables.

		 Changes here will be reflected in the corresponding
		 802dot11 MIB variables (see references below).

		 On bootup this table should be populated with one
		 default entry for each supported type (A, G, etc)."
	::= { extremeRFProfile 1 } 

extremeRFProfileEntry OBJECT-TYPE
	SYNTAX		ExtremeRFProfileEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		""
	INDEX { extremeRFProfileIndex }
	::= { extremeRFProfileTable 1 }

ExtremeRFProfileEntry ::= SEQUENCE {
	extremeRFProfileIndex		INTEGER,
	extremeRFProfileName		DisplayString,
	extremeRFProfileType		Dot11Type,
	extremeRFProfileBeaconInterval 	INTEGER,
	extremeRFProfileDTIM		INTEGER,
	extremeRFProfileFragLength	INTEGER,
	extremeRFProfileRTSThresh	INTEGER,
	extremeRFProfilePreamble	INTEGER,
	extremeRFProfileShortRetry	INTEGER,
	extremeRFProfileLongRetry	INTEGER,
	extremeRFProfileStatus		RowStatus }

extremeRFProfileIndex OBJECT-TYPE
	SYNTAX		INTEGER(1..34)
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"Integer index for this table.  This is here to avoid
		 having to index into the table via the string name."
	::= { extremeRFProfileEntry 1 }

extremeRFProfileName OBJECT-TYPE
	SYNTAX		DisplayString (SIZE(1..32))
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION
		"String name of this profile.  The value |default| is
		 a special token and should not be allowed."
	::= { extremeRFProfileEntry 2 }

extremeRFProfileType OBJECT-TYPE
	SYNTAX		Dot11Type
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION
		"This is the type of this RF profile.  This
		 will decide the ranges of some of the values
		 (i.e. channel)."
	::= { extremeRFProfileEntry 3 }

extremeRFProfileBeaconInterval OBJECT-TYPE
	SYNTAX		INTEGER(1..65535)
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION
		"This is the number of TU between beacon frames."
	REFERENCE "ieee802dot11.1.1.1.12."
	::= { extremeRFProfileEntry 5 }

extremeRFProfileDTIM OBJECT-TYPE
	SYNTAX		INTEGER(1..255)
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION
		" "
	REFERENCE "ieee802dot11.1.1.1.13."
	::= { extremeRFProfileEntry 6 }

extremeRFProfileFragLength OBJECT-TYPE
	SYNTAX		INTEGER(256..2345)
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION
		" "
	REFERENCE "ieee802dot11.2.1.1.5."
	::= { extremeRFProfileEntry 7 }

extremeRFProfileRTSThresh OBJECT-TYPE
	SYNTAX		INTEGER(0..2347)
	MAX-ACCESS	read-create
	STATUS		current	
	DESCRIPTION 
		" "
	REFERENCE "ieee802dot11.2.1.1.2."
	::= { extremeRFProfileEntry 8 }

extremeRFProfilePreamble OBJECT-TYPE
	SYNTAX		INTEGER { short(0),
				  long(1) }
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION
		"This changes the 802 preamble expected by the
		 interface."
	::= { extremeRFProfileEntry 9 }

extremeRFProfileShortRetry OBJECT-TYPE
        SYNTAX	        INTEGER (1..255)
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION
		"Attribute indicates the maximum number of transmission
		 attempts of a frame whose size is <= RTS."
	REFERENCE "dot11ShortRetryLimit"
	::= { extremeRFProfileEntry 11 }

extremeRFProfileLongRetry OBJECT-TYPE
	SYNTAX		INTEGER (1..255)
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION		
		"Attribute indicates the maximum number of transmission
		 attempts of a frame whose size is > RTS."
	REFERENCE "dot11LongRetryLimit"
	::= { extremeRFProfileEntry 12 }

extremeRFProfileStatus OBJECT-TYPE
	SYNTAX		RowStatus
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION
		"Standard row-status semantics."
	::= { extremeRFProfileEntry 13 }


-- ************************************************************** --
--                      Security Profile Table                     --
-- ************************************************************** --


extremeSecurityProfile OBJECT IDENTIFIER ::= { extremeProfile 2 }

extremeSecurityProfileTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF ExtremeSecurityProfileEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"There is one entry in this table per security 
		 profile on the LAC.  Each profile is identified by a
		 string name."
	::= { extremeSecurityProfile 1 }

extremeSecurityProfileEntry OBJECT-TYPE
	SYNTAX		ExtremeSecurityProfileEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		""
	INDEX { extremeSecurityProfileIndex }
	::= { extremeSecurityProfileTable 1 }

ExtremeSecurityProfileEntry ::= SEQUENCE {
	extremeSecurityProfileIndex 		INTEGER,
	extremeSecurityProfileName		DisplayString,
	extremeSecurityProfileESSName		OCTET STRING,
	extremeSecurityProfileSSIDInBeacon		TruthValue,
	extremeSecurityProfileDot11AuthMode	Dot11AuthMode,
	extremeSecurityProfileNetworkAuthMode	NetworkAuthMode,
	extremeSecurityProfileDataVlan			INTEGER,
	extremeSecurityProfileIgnoreVSAVlan		TruthValue,
    extremeSecurityWEPDefaultKey  INTEGER,
	extremeSecurityProfileEncryptionLength 	INTEGER, 
	extremeSecurityProfileStatus		RowStatus }

extremeSecurityProfileIndex OBJECT-TYPE
	SYNTAX		INTEGER(1..32)
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"This is an integer index used instead of string
		 name."
	::= { extremeSecurityProfileEntry 1 }

extremeSecurityProfileName OBJECT-TYPE
	SYNTAX		DisplayString (SIZE(1..32))
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION
		"This is a unique string name which identifies this
		 profile.  The token |default| is special and should
		 not be allowed."
	::= { extremeSecurityProfileEntry 2 }

extremeSecurityProfileESSName OBJECT-TYPE
	SYNTAX OCTET STRING (SIZE(0..32))
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION
		"This is the desired ESS name."
	REFERENCE "ieee802dot11.1.1.1.9"
	::= { extremeSecurityProfileEntry 3 }

extremeSecurityProfileSSIDInBeacon OBJECT-TYPE
	SYNTAX		TruthValue
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION
		"Setting this value to true will have the channel
		 place the ssid in the beacon frame."
	::= { extremeSecurityProfileEntry 4 }

extremeSecurityProfileDot11AuthMode OBJECT-TYPE
	SYNTAX		Dot11AuthMode
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"Specified whether to use open or shared authentication"
	::= { extremeSecurityProfileEntry 5 }

extremeSecurityProfileNetworkAuthMode OBJECT-TYPE
	SYNTAX		NetworkAuthMode
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"This specifies the authentication to use on top of dot11 mac authentication"
	::= { extremeSecurityProfileEntry 6 }

extremeSecurityProfileDataVlan OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"This specifies the VLAN to use in case it does not come back as a VSA or in case the IgnoreVSAVlan is set
		 to true"
	::= { extremeSecurityProfileEntry 7 }

extremeSecurityProfileIgnoreVSAVlan OBJECT-TYPE
 	SYNTAX		TruthValue
 	MAX-ACCESS	read-create
 	STATUS		current
 	DESCRIPTION     "This specifies if Vlan associations in VSAs from the radius server has to be ignored or not"
 	::= { extremeSecurityProfileEntry 8 }

extremeSecurityWEPDefaultKey OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION
		"This value indicates the index in extremeWEPKeyTable that 
		identifies the key this interface will use to decrypt packets."
	::= { extremeSecurityProfileEntry 9 }

extremeSecurityProfileEncryptionLength OBJECT-TYPE
    SYNTAX      INTEGER { none(0),
			  sixtyfour(64),
                          onetwentyeight(128)  }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This gives the size in bits of the key.
         This variable defines the length of all WEP keys and also
         the encryption to use in case of legacy dot1x.
         If the encryption is set to none then no WEP encryption is set."
    ::= { extremeSecurityProfileEntry 10 }

-- extremeSecurityEnableWebNetlogin OBJECT-TYPE
--        SYNTAX          TruthValue
--        MAX-ACCESS      read-create
--        STATUS          current
--        DESCRIPTION
--                "Enable disable netlogin on the wireless interface where
--                security profile is applied."
--        ::= { extremeSecurityProfileEntry 11 }

extremeSecurityProfileStatus OBJECT-TYPE
	SYNTAX		RowStatus
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION
		"Standard row-creation semantics."
	::= { extremeSecurityProfileEntry 11 }

extremeSecurityDot1xConfigTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF ExtremeSecurityDot1xConfigEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"There is one entry in this table per security 
		 profile on the LAC. It reflects the dot1x security config"
	::= { extremeSecurityProfile 2 }

extremeSecurityDot1xConfigEntry OBJECT-TYPE
	SYNTAX	ExtremeSecurityDot1xConfigEntry
	MAX-ACCESS	not-accessible
	STATUS	current
	DESCRIPTION
		""
	INDEX { extremeSecurityProfileIndex }
	::= { extremeSecurityDot1xConfigTable 1 }

ExtremeSecurityDot1xConfigEntry ::= SEQUENCE {
	extremeSecurityKeyMgmtSuite		WPAKeyMgmtSet,
	extremeSecurityMcastCipherSuite	WPACipherSet,
	extremeSecurityDot1xPSKValue		OCTET STRING,
	extremeSecurityDot1xPSKPassPhrase	DisplayString,
	extremeSecurityDot1xReAuthPeriod	INTEGER,
	extremeSecurityGroupUpdateTimeOut	Unsigned32,
	extremeSecurityPairwiseUpdateTimeOut Unsigned32,
        extremeSecurityDot11iPreauthEnabled     TruthValue
}

extremeSecurityKeyMgmtSuite OBJECT-TYPE
	SYNTAX	WPAKeyMgmtSet
	MAX-ACCESS	read-write
	STATUS	current
	DESCRIPTION
		"This bitmask configures the authentication suites to be used."
	::= { extremeSecurityDot1xConfigEntry 1 }

extremeSecurityMcastCipherSuite OBJECT-TYPE
	SYNTAX	WPACipherSet
	MAX-ACCESS	read-write
	STATUS	current
	DESCRIPTION
		"This configures the cipher suite to use for mcast traffic. The cipher suite to use for unicast traffic
		 is derived from this using the following algorithm:
			Mcast cipher = WEP (64/128), Unicast cipher = TKIP
			Mcast cipher = TKIP, Unicast cipher = TKIP
			Mcast cipher = AES, Unicast cipher = AES.
		 This therefore determines the max unicast cipher suite the client can use to associate with 
		 this interface."
	::= { extremeSecurityDot1xConfigEntry 2 }


extremeSecurityDot1xPSKValue OBJECT-TYPE
	SYNTAX		OCTET STRING (SIZE(32))
	MAX-ACCESS	read-write
	STATUS		current	
	DESCRIPTION
		"The Pre-Shared Key (PSK) for when RSN in PSK mode is
		 the selected authentication suite."
	REFERENCE "dot11RSNConfigPSKValue"
	::= { extremeSecurityDot1xConfigEntry 3 }

extremeSecurityDot1xPSKPassPhrase OBJECT-TYPE
	SYNTAX		DisplayString
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
	"The PSK, for when WPA in PSK mode is the selected authentication
	 suite, is configured by extremeSecurityKeyMgmtSuite.
	 An alternative manner of setting the PSK uses the password-to-key
	 algorithm defined in section XXX. This variable provides a means
	 to enter a pass phrase. When this object is written, the RSN entity
	 shall use the password-to-key algorithm specified in section XXX to
	 derive a pre-shared and populate extremeSecurityDot1xPSKValue with this key.
	 This object is logically write-only. Reading this variable shall
	 return unsuccessful status or null or zero."
	::= { extremeSecurityDot1xConfigEntry 4 }

extremeSecurityDot1xReAuthPeriod OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"Number of seconds a clients authentication will last before
		 the AP automatically issues a reauthentication request."
	::= { extremeSecurityDot1xConfigEntry 5 }

extremeSecurityGroupUpdateTimeOut OBJECT-TYPE
	SYNTAX		Unsigned32 (1..1440)
	UNITS		"minutes"
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"The time in minutes after which the RSN group
		 update handshake will be retried. The timer shall
		 start at the moment the group update message is
		 sent."
	REFERENCE "dot11RSNConfigGroupUpdateTimeOut"
	DEFVAL		{ 100 } -- 
	::= { extremeSecurityDot1xConfigEntry 6 }

extremeSecurityPairwiseUpdateTimeOut OBJECT-TYPE
	SYNTAX		Unsigned32 (1..1440)
	UNITS		"minutes"
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"The time in minutes after which the RSN 4-way
		 handshake will be retried. The timer shall start at
		 the moment a 4-way message is sent."
	REFERENCE "dot11RSNConfigPairwiseUpdateTimeOut"
	DEFVAL		{ 100 } -- 
	::= { extremeSecurityDot1xConfigEntry 7 }

extremeSecurityDot11iPreauthEnabled OBJECT-TYPE
        SYNTAX          TruthValue
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION     "Whether preauth is enabled or not"
        ::= { extremeSecurityDot1xConfigEntry 8 }


-- ************************************************************** --
--                     Default WEP Key Table                       --
-- ************************************************************** --
extremeWEPKeyTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF ExtremeWEPKeyEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"This table contains per-profile WEP keys.

		 Reference ieee802dot11.1.2.3."
	::= { extremeSecurityProfile 4 }

extremeWEPKeyEntry OBJECT-TYPE
	SYNTAX	ExtremeWEPKeyEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		" "
	INDEX { extremeSecurityProfileIndex, extremeWEPKeyIndex }
	::= { extremeWEPKeyTable 1 }
	
ExtremeWEPKeyEntry ::= SEQUENCE {
	extremeWEPKeyIndex	INTEGER,
	extremeWEPKey		OCTET STRING,
	extremeWEPKeyStatus	RowStatus }
	
extremeWEPKeyIndex OBJECT-TYPE
	SYNTAX 		INTEGER(0..8)
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"There can be upto 8 wep keys for any wireless
		 interface. Four of the keys are to be used with
		 WEP Authentication, and the other four with MAC Auth."
	::= { extremeWEPKeyEntry 1 }

extremeWEPKey OBJECT-TYPE
	SYNTAX		OCTET STRING (SIZE(1..19))
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION
		"This is a write-only wep key."
	::= { extremeWEPKeyEntry 2 }

extremeWEPKeyStatus OBJECT-TYPE
	SYNTAX		RowStatus
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION
		"Standard row-creation semantics."
	::= { extremeWEPKeyEntry 3 }

-- ************************************************************** --
--              Wireless Physical Interface Config Table           --
-- ************************************************************** --
extremeWirelessPhysInterfaceConfigTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF ExtremeWirelessPhysInterfaceConfigEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"This table contains the configured bindings between	
		 physical wireless interfaces and RF profiles and other
		 RF properties. There is one instance of a physical wireless
		 interface per radio on the AP.

		 Entries in this table have a duration that exceeds
		 the lifetime of entries in the wirelessPhysInterfaceCtlTable.
		 A configured binding spans the reset or removal of 
		 a wireless interface.

		 Entries can be removed from this table by the user.

		 If there is a mismatch between a new wireless port
		 and a previously configured profile, the default
		 profile will be applied and this table will be
		 updated."
	::= { extremeProfile 3 }

extremeWirelessPhysInterfaceConfigEntry OBJECT-TYPE
	SYNTAX	ExtremeWirelessPhysInterfaceConfigEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		" "
	INDEX { extremeWirelessPhysInterfaceIndex }
	::= { extremeWirelessPhysInterfaceConfigTable 1 }

ExtremeWirelessPhysInterfaceConfigEntry ::= SEQUENCE {
	extremeWirelessPhysInterfaceConfigRFProfile		INTEGER,
	extremeWirelessPhysInterfaceConfigRFChannel		INTEGER,
	extremeWirelessPhysInterfaceConfigSpeed		Dot11Speed,
	extremeWirelessPhysInterfaceConfigPowerLevel	INTEGER 
}
	
extremeWirelessPhysInterfaceConfigRFProfile OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION
		"This is the index into the extremeRFProfileTable for
		 the RF profile that this wireless interface is bound 
		 to.  

		 The default value is equivalent to the profile index for
		 the interface-appropriate default in the table."
	::= { extremeWirelessPhysInterfaceConfigEntry 1 }
		 
extremeWirelessPhysInterfaceConfigRFChannel	OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION
		"This is the RF channel which has been selected for this
		 wireless interface.  It should be one of the supported 
		 channels as given by the phy tables in the dot11 mib."
	::= { extremeWirelessPhysInterfaceConfigEntry 2 }

extremeWirelessPhysInterfaceConfigSpeed OBJECT-TYPE
	SYNTAX		Dot11Speed
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION
		"This is the speed to configure the interface at. A value of 0 indicates
		 automatic speed detection."
	::= { extremeWirelessPhysInterfaceConfigEntry 3 }

extremeWirelessPhysInterfaceConfigPowerLevel OBJECT-TYPE
	SYNTAX		INTEGER 
	MAX-ACCESS 	read-create
	STATUS		current
	DESCRIPTION
		"This value specifies the tx power (in % of max power) to use."
	::= { extremeWirelessPhysInterfaceConfigEntry 4 }

-- ************************************************************** --
--              Wireless Virtual  Interface Config Table           --
-- ************************************************************** --
extremeWirelessVirtInterfaceConfigTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF ExtremeWirelessVirtInterfaceConfigEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"This table contains the configured bindings between	
		 virtual wireless interfaces and security profiles and other
		 security properties. There are upto 8 virtual interface for
		 each physical interface.

		 Entries in this table have a duration that exceeds
		 the lifetime of entries in the wirelessVirtInterfaceCtlTable.
		 A configured binding spans the reset or removal of 
		 a wireless interface.

		 Entries can be removed from this table by the user."

	::= { extremeProfile 4 }

extremeWirelessVirtInterfaceConfigEntry OBJECT-TYPE
	SYNTAX	ExtremeWirelessVirtInterfaceConfigEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		" "
	INDEX { extremeWirelessVirtInterfaceIndex }
	::= { extremeWirelessVirtInterfaceConfigTable 1 }

ExtremeWirelessVirtInterfaceConfigEntry ::= SEQUENCE {
	extremeWirelessVirtInterfaceConfigSecurityProfile	INTEGER,
	extremeWirelessVirtInterfaceConfigMaxClients			INTEGER,
	extremeWirelessVirtInterfaceConfigWirelessBridging		TruthValue,
	extremeWirelessVirtInterfaceConfigState			INTEGER
}
	
extremeWirelessVirtInterfaceConfigSecurityProfile OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This is the index into the extremeSecurityProfileTable for
		 the security profile that this wireless interface is bound 
		 to.  

		 The default value is equivalent to the profile index for
		 the interface-appropriate default in the table."
	::= { extremeWirelessVirtInterfaceConfigEntry 1 }

extremeWirelessVirtInterfaceConfigMaxClients OBJECT-TYPE
	SYNTAX		INTEGER (1..128)
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The maximum number of clients that can associate with this virtual interface."
	::= { extremeWirelessVirtInterfaceConfigEntry 2 }

extremeWirelessVirtInterfaceConfigWirelessBridging OBJECT-TYPE
	SYNTAX		TruthValue
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This specifies whether wireless bridging is enabled on this interface.
		 If wireless bridging is enabled then traffic originating from a client on this
		 interface will be bridged to clients on the same VLAN on this or other 
		 virtual interfaces that have wireless bridging enabled. So basically
		 wireless bridging should be enabled on both the source and the destination
		 virtual interface for traffic to be bridged."
	::= { extremeWirelessVirtInterfaceConfigEntry 3 }

extremeWirelessVirtInterfaceConfigState OBJECT-TYPE
	SYNTAX		INTEGER { enabled(0), disabled(1) } 
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This value specifies whether the virtual interface is active or not"
	::= { extremeWirelessVirtInterfaceConfigEntry 4 }

-- ************************************************************** --
--                      Antenna Profile Table                     --
-- ************************************************************** --

extremeAntennaProfile OBJECT IDENTIFIER ::= { extremeProfile 5 }

extremeAntennaProfileTable OBJECT-TYPE
SYNTAX  SEQUENCE OF ExtremeAntennaProfileEntry
    	MAX-ACCESS  not-accessible
    	STATUS      current
    	DESCRIPTION
        	"There is one entry in this table per  antenna
         	profile on the LAC.  Each profile is identified by a
         	string name."
    	::= { extremeAntennaProfile 1 }

extremeAntennaProfileEntry OBJECT-TYPE
SYNTAX      ExtremeAntennaProfileEntry
MAX-ACCESS  not-accessible
STATUS      current
DESCRIPTION
""
    	INDEX { extremeAntennaProfileIndex }
    	::= { extremeAntennaProfileTable 1 }

ExtremeAntennaProfileEntry ::= SEQUENCE
{
    extremeAntennaProfileIndex 		INTEGER,
    extremeAntennaProfileName		DisplayString,
    extremeAntennaProfile2point4GHZGain	INTEGER,
    extremeAntennaProfile5GHZGain		INTEGER,
    extremeAntennaProfileStatus		RowStatus 
}

extremeAntennaProfileIndex OBJECT-TYPE
    SYNTAX      INTEGER(1..32)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
    "This is an integer index used instead of string name."
    ::= { extremeAntennaProfileEntry 1 }

extremeAntennaProfileName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..32))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
    "This is a unique string name which identifies this
      profile.  The token |default| is special and should
      not be allowed."
    ::= { extremeAntennaProfileEntry 2 }

extremeAntennaProfile2point4GHZGain OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This specifies 2.4GHz gain value for detachable antenna in dbi"
    ::= { extremeAntennaProfileEntry 3 }

extremeAntennaProfile5GHZGain OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This specifies 5GHz gain value for detachable antenna in dbi"
    ::= { extremeAntennaProfileEntry 4 }

extremeAntennaProfileStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Standard row-creation semantics."
    ::= { extremeAntennaProfileEntry 5 }

-- ************************************************************** --
--                   RemoteConnect configuration                         --
-- ************************************************************** --


extremeWirelessRemoteConnectGlobalCfgGroup OBJECT IDENTIFIER ::=   { extremeProfile 6 }

extremeWirelessRemoteConnectGlobalBindingType OBJECT-TYPE
  SYNTAX		WirelessRemoteConnectBindingType
  MAX-ACCESS  read-write
  STATUS current
  DESCRIPTION
  "Global Binding Tye"
 ::= { extremeWirelessRemoteConnectGlobalCfgGroup 1 }

extremeWirelessRemoteConnectBindingTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessRemoteConnectBindingEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"This table specifies the RemoteConnect binding configuration for various ports."
	::= { extremeProfile 7 }

extremeWirelessRemoteConnectBindingEntry OBJECT-TYPE
	SYNTAX 		ExtremeWirelessRemoteConnectBindingEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		" "
	INDEX { extremeWirelessRemoteConnectBindingPortIndex }
	::= { extremeWirelessRemoteConnectBindingTable 1 }

ExtremeWirelessRemoteConnectBindingEntry ::= SEQUENCE {
	extremeWirelessRemoteConnectBindingPortIndex	INTEGER,
	extremeWirelessRemoteConnectBindingIfIndex	Integer32,
	extremeWirelessRemoteConnectBindingType	WirelessRemoteConnectBindingType,
	extremeWirelessRemoteConnectBindingMAC	MacAddress,
	extremeWirelessRemoteConnectBindingSerial	OCTET STRING,
	extremeWirelessRemoteConnectBindingIPAddressType	InetAddressType,
	extremeWirelessRemoteConnectBindingIPAddress	InetAddress,
	extremeWirelessRemoteConnectBindingEnabled	TruthValue,
	extremeWirelessRemoteConnectBindingBound	TruthValue,
	extremeWirelessRemoteConnectBindingRowStatus	RowStatus}

extremeWirelessRemoteConnectBindingPortIndex	OBJECT-TYPE
	SYNTAX	INTEGER(1..48)
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION	"The index of this binding. This maps one-to-one with the value
			specified in the CLI. For example, if you say v:1 in the CLI, then
			this value should be 1."
	::= { extremeWirelessRemoteConnectBindingEntry 1}

extremeWirelessRemoteConnectBindingIfIndex	OBJECT-TYPE
	SYNTAX	Integer32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION	"This is the IF index that is used in the extremeWirelessPortConfigTable
			etc to refer to this RemoteConnect port."
	::= { extremeWirelessRemoteConnectBindingEntry 2}

extremeWirelessRemoteConnectBindingType OBJECT-TYPE
	SYNTAX		WirelessRemoteConnectBindingType
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION
		"This is the type of binding. Based on this, one of the following columns will be valid."
	::= { extremeWirelessRemoteConnectBindingEntry 3 }

extremeWirelessRemoteConnectBindingMAC OBJECT-TYPE
	SYNTAX		MacAddress
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION	"The MAC address of the AP that is bound to this virtual port. 
			This is valid only if the extremeWirelessRemoteConnectBindingType is set to
			mac-address"
	::= { extremeWirelessRemoteConnectBindingEntry 4}

extremeWirelessRemoteConnectBindingSerial OBJECT-TYPE
	SYNTAX		OCTET STRING
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION	"The serial number of the AP that is bound to this virtual port. 
			This is valid only if the extremeWirelessRemoteConnectBindingType is set to
			serial-number"
	::= { extremeWirelessRemoteConnectBindingEntry 5}

extremeWirelessRemoteConnectBindingIPAddressType OBJECT-TYPE
	SYNTAX		InetAddressType
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION	"The IP address type of the AP that is bound to this virtual port. 
			This is valid only if the extremeWirelessRemoteConnectBindingType is set to
			ip-address"
	::= { extremeWirelessRemoteConnectBindingEntry 6}

extremeWirelessRemoteConnectBindingIPAddress OBJECT-TYPE
	SYNTAX		InetAddress
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION	"The IP address of the AP that is bound to this virtual port. 
			This is valid only if the extremeWirelessRemoteConnectBindingType is set to
			ip-address"
	::= { extremeWirelessRemoteConnectBindingEntry 7}

extremeWirelessRemoteConnectBindingEnabled	OBJECT-TYPE
	SYNTAX		TruthValue
	MAX-ACCESS	read-write
	STATUS 		current
	DESCRIPTION	"An entry in this table can be created but left as disabled. If you 
			set this variable to True then the RemoteConnect controller will consider
			this binding when trying to map APs to RemoteConnect ports. Else, it will
			ignore it."
	::= {extremeWirelessRemoteConnectBindingEntry 8}

extremeWirelessRemoteConnectBindingBound	OBJECT-TYPE
	SYNTAX		TruthValue
	MAX-ACCESS	read-write
	STATUS 		current
	DESCRIPTION	"Specifies if an AP has come up and has been matched to this binding.
			If this is true, then the extremeWirelessPortStatus table will have
			an entry for this RemoteConnect port."
	::= {extremeWirelessRemoteConnectBindingEntry 9}

extremeWirelessRemoteConnectBindingRowStatus	OBJECT-TYPE
	SYNTAX		RowStatus
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION	"RowStatus attribute. When this row is deleted, the binding goes away"
	::= {extremeWirelessRemoteConnectBindingEntry 10}

-- **************************************************************************************
-- This table specifies how the controller should choose to redirect certain APs to other
-- controllers
-- **************************************************************************************
extremeWirelessRemoteConnectRedirectBindingTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessRemoteConnectRedirectBindingEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"This table specifies the RemoteConnect redirection configuration for various ports."
	::= { extremeProfile 8 }

extremeWirelessRemoteConnectRedirectBindingEntry OBJECT-TYPE
	SYNTAX 		ExtremeWirelessRemoteConnectRedirectBindingEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		" "
	INDEX { extremeWirelessRemoteConnectRedirectBindingIndex }
	::= { extremeWirelessRemoteConnectRedirectBindingTable 1 }

ExtremeWirelessRemoteConnectRedirectBindingEntry ::= SEQUENCE {
	extremeWirelessRemoteConnectRedirectBindingIndex	INTEGER,
	extremeWirelessRemoteConnectRedirectBindingType	WirelessRemoteConnectBindingType,
	extremeWirelessRemoteConnectRedirectBindingMAC	MacAddress,
	extremeWirelessRemoteConnectRedirectBindingSerial	OCTET STRING,
	extremeWirelessRemoteConnectRedirectBindingIPAddressType	InetAddressType,
	extremeWirelessRemoteConnectRedirectBindingIPAddress	InetAddress,
	extremeWirelessRemoteConnectRedirectBindAttachSwitchIPAddrType	InetAddressType,
	extremeWirelessRemoteConnectRedirectBindAttachSwitchIPAddr	InetAddress,
	extremeWirelessRemoteConnectRedirectBindingEnabled		TruthValue,
	extremeWirelessRemoteConnectRedirectBindingNumRedirects	Counter32,
	extremeWirelessRemoteConnectRedirectBindingRowStatus		RowStatus}

extremeWirelessRemoteConnectRedirectBindingIndex	OBJECT-TYPE
	SYNTAX	INTEGER(1..255)
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION	"The index of this RedirectBinding."
	::= { extremeWirelessRemoteConnectRedirectBindingEntry 1}

extremeWirelessRemoteConnectRedirectBindingType OBJECT-TYPE
	SYNTAX		WirelessRemoteConnectBindingType
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION
		"This is the type of RedirectBinding. Based on this, one of the following columns will be valid."
	::= { extremeWirelessRemoteConnectRedirectBindingEntry 2 }

extremeWirelessRemoteConnectRedirectBindingMAC OBJECT-TYPE
	SYNTAX		MacAddress
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION	"The MAC address of the AP that will be redirected. 
			This is valid only if the extremeWirelessRemoteConnectRedirectBindingType is set to
			mac-address"
	::= { extremeWirelessRemoteConnectRedirectBindingEntry 3}

extremeWirelessRemoteConnectRedirectBindingSerial OBJECT-TYPE
	SYNTAX		OCTET STRING
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION	"The serial number of the AP that is bound to this virtual port. 
			This is valid only if the extremeWirelessRemoteConnectRedirectBindingType 
			is set to serial-number"
	::= { extremeWirelessRemoteConnectRedirectBindingEntry 4}

extremeWirelessRemoteConnectRedirectBindingIPAddressType OBJECT-TYPE
	SYNTAX		InetAddressType
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION	"The IP address type of the AP that will be redirected. 
			This is valid only if the extremeWirelessRemoteConnectRedirectBindingType 
			is set to ip-address"
	::= { extremeWirelessRemoteConnectRedirectBindingEntry 5}

extremeWirelessRemoteConnectRedirectBindingIPAddress OBJECT-TYPE
	SYNTAX		InetAddress
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION	"The IP address of the AP that will be redirected. 
			This is valid only if the extremeWirelessRemoteConnectRedirectBindingType 
			is set to ip-address"
	::= { extremeWirelessRemoteConnectRedirectBindingEntry 6}

extremeWirelessRemoteConnectRedirectBindAttachSwitchIPAddrType OBJECT-TYPE
	SYNTAX		InetAddressType
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION	"The IP address type of the slave "
	::= { extremeWirelessRemoteConnectRedirectBindingEntry 7}

extremeWirelessRemoteConnectRedirectBindAttachSwitchIPAddr OBJECT-TYPE
	SYNTAX		InetAddress
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION	"The IP address of the slave"
	::= { extremeWirelessRemoteConnectRedirectBindingEntry 8}

extremeWirelessRemoteConnectRedirectBindingEnabled	OBJECT-TYPE
	SYNTAX		TruthValue
	MAX-ACCESS	read-write
	STATUS 		current
	DESCRIPTION	"An entry in this table can be created but left as disabled. If you 
			set this variable to True then the RemoteConnect controller will consider
			this RedirectBinding when trying to redirect APs. Else, it will
			ignore it."
	::= {extremeWirelessRemoteConnectRedirectBindingEntry 9}

extremeWirelessRemoteConnectRedirectBindingNumRedirects	OBJECT-TYPE
	SYNTAX		Counter32
	MAX-ACCESS	read-only
	STATUS 		current
	DESCRIPTION	"The number of times this redirect has been invoked."
	::= {extremeWirelessRemoteConnectRedirectBindingEntry 10}

extremeWirelessRemoteConnectRedirectBindingRowStatus	OBJECT-TYPE
	SYNTAX	RowStatus
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION	"Standard row status semantics."
	::= {extremeWirelessRemoteConnectRedirectBindingEntry 11}

-- **************************************************************************************
-- This table specifies the list of APs that could not be bound or redirected due to 
-- a lack of mapping on this controller
-- **************************************************************************************

extremeWirelessRemoteConnectDeviceDBGroup OBJECT IDENTIFIER ::=   { extremeProfile 9 }

extremeWirelessRemoteConnectDeviceDBTimeOut OBJECT-TYPE
  SYNTAX  INTEGER (0 | 30..3600)
  MAX-ACCESS  read-write
  STATUS current
  DESCRIPTION
  "Timeout value for unbound APs entry in seconds. 0 for disable"
 ::= { extremeWirelessRemoteConnectDeviceDBGroup 1 }


extremeWirelessRemoteConnectUnboundAPsTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessRemoteConnectUnboundAPsEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"This table contains the list of APs that could not be bound or redirected."
	::= { extremeProfile 10 }

extremeWirelessRemoteConnectUnboundAPsEntry OBJECT-TYPE
	SYNTAX 		ExtremeWirelessRemoteConnectUnboundAPsEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		" "
	INDEX { extremeWirelessRemoteConnectUnboundAPsIndex }
	::= { extremeWirelessRemoteConnectUnboundAPsTable 1 }

ExtremeWirelessRemoteConnectUnboundAPsEntry ::= SEQUENCE {
	extremeWirelessRemoteConnectUnboundAPsIndex	INTEGER,
	extremeWirelessRemoteConnectUnboundAPsMAC	MacAddress,
	extremeWirelessRemoteConnectUnboundAPsSerial	OCTET STRING,
	extremeWirelessRemoteConnectUnboundAPsIPAddressType	InetAddressType,
	extremeWirelessRemoteConnectUnboundAPsIPAddress	InetAddress,
	extremeWirelessRemoteConnectUnboundAPsNumAttempts	Counter32,
	extremeWirelessRemoteConnectUnboundAPsRowStatus	RowStatus}

extremeWirelessRemoteConnectUnboundAPsIndex	OBJECT-TYPE
	SYNTAX	INTEGER(0..65535)
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION	"The index of this table."
	::= { extremeWirelessRemoteConnectUnboundAPsEntry 1}

extremeWirelessRemoteConnectUnboundAPsMAC OBJECT-TYPE
	SYNTAX		MacAddress
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION	"The MAC address of the unbound AP."
	::= { extremeWirelessRemoteConnectUnboundAPsEntry 2}

extremeWirelessRemoteConnectUnboundAPsSerial OBJECT-TYPE
	SYNTAX		OCTET STRING
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION	"The serial number of the unbound AP"
	::= { extremeWirelessRemoteConnectUnboundAPsEntry 3}

extremeWirelessRemoteConnectUnboundAPsIPAddressType OBJECT-TYPE
	SYNTAX		InetAddressType
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION	"The IP address type of the unbound AP"
	::= { extremeWirelessRemoteConnectUnboundAPsEntry 4}

extremeWirelessRemoteConnectUnboundAPsIPAddress OBJECT-TYPE
	SYNTAX		InetAddress
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION	"The IP address of the unbound AP"
	::= { extremeWirelessRemoteConnectUnboundAPsEntry 5}

extremeWirelessRemoteConnectUnboundAPsNumAttempts	OBJECT-TYPE
	SYNTAX		Counter32
	MAX-ACCESS	read-only
	STATUS 		current
	DESCRIPTION	"The number of times this AP contacted this controller."
	::= {extremeWirelessRemoteConnectUnboundAPsEntry 6}

extremeWirelessRemoteConnectUnboundAPsRowStatus	OBJECT-TYPE
	SYNTAX	RowStatus
	MAX-ACCESS	read-create
	STATUS		current
	DESCRIPTION	"Standard row status semantics. Only valid value to set is destroy (6)."
	::= {extremeWirelessRemoteConnectUnboundAPsEntry 7}

-- ************************************************************** --
--                   RADIUS Server Configuration                   --
-- The Radius Server Table on the Ethernet switch is implemented   --
-- using the extremeAuthServerTable, defines under extremeServices --
--                                                                 --
-- The extremeAPAuthServerTable is implemented per wireless port.  --
-- Each AP will have to implement this table to allow the LAC to   --
-- propogate configuration information.                            --
-- ************************************************************** --
extremeAPAuthServerTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF ExtremeAPAuthServerEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"This table is proxied by the wireless APs.  It 
		 allows the wireless concentrator to configure the 
		 APs security settings."
	::= { extremeAP 12 }

extremeAPAuthServerEntry OBJECT-TYPE
	SYNTAX 		ExtremeAPAuthServerEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		" "
	INDEX { extremeWirelessPortIfIndex, extremeAPAuthServerIndex }
	::= { extremeAPAuthServerTable 1 }

ExtremeAPAuthServerEntry ::= SEQUENCE {
	extremeAPAuthServerIndex		INTEGER,
	extremeAPAuthServerAddressType          InetAddressType,
	extremeAPAuthServerAddress 		InetAddress,
	extremeAPAuthServerPort                 INTEGER,
	extremeAPAuthServerSecret 		OCTET STRING,
	extremeAPAuthServerReTransmit		INTEGER,
	extremeAPAuthServerStatus		TruthValue}

extremeAPAuthServerIndex OBJECT-TYPE
	SYNTAX		INTEGER (1..2)
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"Integer representing either primary (1) or backup
		 (2) server."
	::= { extremeAPAuthServerEntry 1 }

extremeAPAuthServerAddressType          OBJECT-TYPE
        SYNTAX                          InetAddressType
        MAX-ACCESS                      read-only
        STATUS                          current
        DESCRIPTION
            "The type of address specified in the object
                'extremeAuthServerAddress'.
             Currently, only 'ipv4' and 'dns' are supported."
        DEFVAL { ipv4 }
      ::= { extremeAPAuthServerEntry 2 }

extremeAPAuthServerAddress OBJECT-TYPE
        SYNTAX          InetAddress
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "IP address of the radius server.  The act of
                 assigning an IP address enables the client to use
                 the server.  Setting this value to 0.0.0.0 disables
                 this entry."
        ::= { extremeAPAuthServerEntry 3 }

extremeAPAuthServerPort                    OBJECT-TYPE
       SYNTAX                          INTEGER (0..65535)
       MAX-ACCESS                      read-only
       STATUS                          current
       DESCRIPTION
           "The UDP port number of the remote syslog server
                to which syslog messages will be sent."
     ::= { extremeAPAuthServerEntry 4 }

extremeAPAuthServerSecret OBJECT-TYPE
        SYNTAX          OCTET STRING
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "This is the shared secret between the Authenticator
                 and radius server.  This is logically write-only."
        ::= { extremeAPAuthServerEntry 5 }

extremeAPAuthServerReTransmit OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This is the timeout in seconds after which the 
		 Authenticator will re transmit requests to the
		 radius server."
	::= { extremeAPAuthServerEntry 6 }

extremeAPAuthServerStatus OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS  read-write
        STATUS current
        DESCRIPTION
                "Specifies whether the DNS entry is in use or not"
	::= { extremeAPAuthServerEntry 7 }

-- ************************************************************** --
-- Scan Configuration Table : This table provides the ability to   --
-- configure the parameters associated with ON-Channel scanning    --
-- for other access points.                                        --
-- ************************************************************** --
extremeWirelessScanCfgTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessScanCfgEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"This table contains one entry per wireless interface.  It
	 allows for configuration of active and passive scan
	 parameters."
	 ::= { extremeAP 24 }

extremeWirelessScanCfgEntry OBJECT-TYPE
	SYNTAX ExtremeWirelessScanCfgEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	""
	INDEX { ifIndex }
	 ::= { extremeWirelessScanCfgTable 1 }

ExtremeWirelessScanCfgEntry ::= SEQUENCE {
	extremeWirelessScanEnable			TruthValue,
	extremeWirelessScanSendProbe			TruthValue,
	extremeWirelessScanProbeInterval		Unsigned32,
	extremeWirelessScanResultTableSize		Unsigned32,
	extremeWirelessScanResultTimeout		Unsigned32,
	extremeWirelessScanResetStats			TruthValue,
	extremeWirelessScanClearTable			TruthValue,
	extremeWirelessScanSendAPAddedTrap		TruthValue,
	extremeWirelessScanSendAPRemovedTrap		TruthValue,
	extremeWirelessScanSendAPUpdatedTrap		TruthValue
}

extremeWirelessScanEnable OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"By setting this to true the wireless interface will collect
	 information from beacons and (possible) probe responses.  If
	 this value is set to false this information will not be 
	 collected."
	DEFVAL { true }
	 ::= { extremeWirelessScanCfgEntry 1 }

extremeWirelessScanSendProbe OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"If this value is set to TRUE the wireless interface will send
	 probe requests to the broadcast SSID every ProbeInterval.  The
	 results of these probes will be recorded in the scan results
	 table.  If this is false, the AP will only collect information
	 from beacon frames."
	DEFVAL { false }
	 ::= { extremeWirelessScanCfgEntry 2 }

extremeWirelessScanProbeInterval OBJECT-TYPE
	SYNTAX Unsigned32
	UNITS "milliseconds"
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"This allows for the configuration of the interval over which
	 probe requests will be sent."
	DEFVAL { 100 }
	 ::= { extremeWirelessScanCfgEntry 3 }

extremeWirelessScanResultTableSize OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"This parameter permits the configuration of the result table
	 size.  If there are more entries discovered than there are 
	 room for the new entry will replace the oldest entry in the
	 table.  In this case a new entry trap will be sent with the
	 OverFlow value set to TRUE."
	DEFVAL { 1024 }
	 ::= { extremeWirelessScanCfgEntry 4 }

extremeWirelessScanResultTimeout OBJECT-TYPE
	SYNTAX Unsigned32
	UNITS "seconds"
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"By default the scan result table will age out entries which
	 haven't been updated for some time.  When an entry is aged
	 out of the table a scanResultAgeOut trap is generated.  
	 Setting this value to 0 will disable the aging out of entries."
	DEFVAL { 3600 }
	 ::= { extremeWirelessScanCfgEntry 5 }

extremeWirelessScanResetStats OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"Setting this to TRUE will cause the scan module to reset its
	 internal statistics, as well as the packet counts for each 
	 entry in the scan results table.  It will *not* remove any
	 entries in the scan table."
	 ::= { extremeWirelessScanCfgEntry 6 }

extremeWirelessScanClearTable OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"Setting this to TRUE will cause the scan module to reset its
	 internal table.  All currently detected stations will be 
	 removed.  Scan statistics (i.e. watermark) will not be reset."
	 ::= { extremeWirelessScanCfgEntry 7 }

extremeWirelessScanSendAPAddedTrap OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"Setting this to TRUE will cause the scan module to send a trap
	 whenever a new entry is added to the scan results table.  If
	 this value is false the scan module will suppress the trap."
	DEFVAL { true }
	 ::= { extremeWirelessScanCfgEntry 8 }

extremeWirelessScanSendAPRemovedTrap OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"Setting this to TRUE will cause the scan module to send a trap
	 whenever an entry is removed from the scan results table."
	DEFVAL { true }
	 ::= { extremeWirelessScanCfgEntry 9 }

extremeWirelessScanSendAPUpdatedTrap OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"Setting this to TRUE will cause the scan module to send a trap
	 whenever an entry is updated in the scan results table.  This 
	 will happen if the list of IEs sent from a particular MAC address
	 changes."
	DEFVAL { true }
	 ::= { extremeWirelessScanCfgEntry 10 }

-- ************************************************************** --
-- Off-Channel AP Scan : This table provides the ability to confi  --
-- ure and start an off-channel scan for other APs.                --
-- ************************************************************** --
extremeWirelessOffChannelScanCfgTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessOffChannelScanCfgEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"This table contains one entry per wireless interface.  It
	 allows for configuration of off-channel scan.  To start an
	 off-channel scan the management station should write values
	 for channel list, min and max wait.  Toggling the start
	 value at this point will start an off-channel scan, unless
	 one is already running.
	 Results of the off-channel scan are reported to the scan
	 results table together with the results of passive scan."
	 ::= { extremeAP 25 }

extremeWirelessOffChannelScanCfgEntry OBJECT-TYPE
	SYNTAX ExtremeWirelessOffChannelScanCfgEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	""
	INDEX { ifIndex }
	 ::= { extremeWirelessOffChannelScanCfgTable 1 }

ExtremeWirelessOffChannelScanCfgEntry ::= SEQUENCE {
	extremeWirelessOffChannelScanStart		TruthValue,
	extremeWirelessOffChannelScanList		BITS,
	extremeWirelessOffChannelScanMinWait		Unsigned32,
	extremeWirelessOffChannelScanMaxWait		Unsigned32,
	extremeWirelessOffChannelContinuous		TruthValue
}

extremeWirelessOffChannelScanStart OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"Setting this to TRUE will cause the scan module to start an
	 off-channel scan.  The radio will be disabled for the 
	 duration of the scan.  The scan module will change to each 
	 of the specified channels in order.  It will then conduct 
	 passive (and perhaps active) scans on that channel for the 
	 configured intervals.  When the scan is finished the radio 
	 will be re-enabled.
	 The scan will wait on each channel for at least MinWait 
	 milliseconds even if it sees no traffic on the channel. It
	 will wait for at most MaxWait msecs even if it sees traffic.
	 As a result the best case time for the scan is given by:
	 	# Of Channels * extremeWirelessOffChannelScanMinWait
 	 The worst case completion time is given by:
	 	# Of Channels * extremeWirelessOffChannelScanMaxWait
	 Results of the off-channnel scan a reported to the scan 
	 results table."
	 ::= { extremeWirelessOffChannelScanCfgEntry 1 }

extremeWirelessOffChannelScanList OBJECT-TYPE
	SYNTAX BITS {
		scanAll(0),
		scanEvery(1),
		scanChannel1(2),
		scanChannel2(3),
		scanChannel3(4),
		scanChannel4(5),
		scanChannel5(6),
		scanChannel6(7),
		scanChannel7(8),
		scanChannel8(9),
		scanChannel9(10),
		scanChannel10(11),
		scanChannel11(12),
		scanChannel12(13),
		scanChannel13(14),
		scanChannel14(15),
		scanChannel34(16),
		scanChannel36(17),
		scanChannel40(18),
		scanChannel44(19),
		scanChannel48(20),
		scanChannel52(21),
		scanChannel56(22),
		scanChannel60(23),
		scanChannel64(24),
		scanChannel100(25),
		scanChannel104(26),
		scanChannel108(27),
		scanChannel113(28),
		scanChannel116(29),
		scanChannel120(30),
		scanChannel124(31),
		scanChannel128(32),
		scanChannel132(33),
		scanChannel140(34),
		scanChannel149(35),
		scanChannel153(36),
		scanChannel157(37),
		scanChannel161(38),
		scanChannel165(39)
	}
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"This value controls the channels which will be scanned during
	 the off-channel scan.  Two special values should be noted:
	 
	 all -   causes the radio to scan all channels supported by
	         the configured country code.  While on each channel
		     the radio will send out probe requests if the value
		     of extremeWirelessScanSendProbeRequest is true.
	 every - causes the radio to scan all channels, even those
	 	     which are restricted by the country code.  The
			 radio will only send probe request on channels that
			 are legal for that country code."
	 ::= { extremeWirelessOffChannelScanCfgEntry 2 }

extremeWirelessOffChannelScanMinWait OBJECT-TYPE
	SYNTAX Unsigned32
	UNITS "milliseconds"
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"This value controls the minimum time the off-channel scan
	 will wait on a particular channel if it doesn't see any
	 traffic."
	 DEFVAL { 1 }
	 ::= { extremeWirelessOffChannelScanCfgEntry 3 }

extremeWirelessOffChannelScanMaxWait OBJECT-TYPE
	SYNTAX Unsigned32
	UNITS "milliseconds"
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"This value controls the maximum time the off-channel scan will
	 wait on a particular channel even if it is receiving beacons
	 etc."
	 DEFVAL { 10 }
	 ::= { extremeWirelessOffChannelScanCfgEntry 4 }

extremeWirelessOffChannelContinuous OBJECT-TYPE
 	SYNTAX TruthValue
 	MAX-ACCESS read-write
 	STATUS current
 
 	DESCRIPTION
 	"Setting this value to true results in the off-channel scan
 	looping on the configured values until the channel scan is
 	disabled."
 	DEFVAL { false }
 	 ::= { extremeWirelessOffChannelScanCfgEntry 5 }
 


-- ************************************************************** --
-- Scan Status Table : This table contains information about the   --
-- current status of the scan feature.                             --
-- ************************************************************** --
extremeWirelessScanStatusTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessScanStatusEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"This table contains one entry per wireless interface.  It
	 provides status and statistics information for the scan 
	 feature operating on that wireless interface."
	 ::= { extremeAP 26 }

extremeWirelessScanStatusEntry OBJECT-TYPE
	SYNTAX ExtremeWirelessScanStatusEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	""
	INDEX { ifIndex }
	 ::= { extremeWirelessScanStatusTable 1 }

ExtremeWirelessScanStatusEntry ::= SEQUENCE {
	extremeWirelessScanCurrentTableSize 	Unsigned32,
	extremeWirelessScanTableWatermark 	Unsigned32,
	extremeWirelessScanTotalOverflows	Unsigned32,
	extremeWirelessScanTotalTimeouts	Unsigned32,
	extremeWirelessScanOffChannelRunning	TruthValue,
	extremeWirelessScanCurrentChannel	Unsigned32,
	extremeWirelessScanLastElement		TimeTicks,
	extremeWirelessScanNumProbes		Unsigned32
}

extremeWirelessScanCurrentTableSize OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This indicates the current number of entries in the scan results
	 table."
	 ::= { extremeWirelessScanStatusEntry 1 }

extremeWirelessScanTableWatermark OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This indicates the largest size the results table has reached
	 since the status values have been reset, or the system has
	 booted."
	 ::= { extremeWirelessScanStatusEntry 2 }

extremeWirelessScanTotalOverflows OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of entries which have been removed
	 to make room for a newer entry.   This should be equal to the
	 number of AP added traps the system has generated with the 
	 overflow value set to true."
	 ::= { extremeWirelessScanStatusEntry 3 }

extremeWirelessScanTotalTimeouts OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of entries which have been removed
	 because they have become stale.  This should be equal to the 
	 number of AP removed traps sent by the system."
	 ::= { extremeWirelessScanStatusEntry 4 }

extremeWirelessScanOffChannelRunning OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"If this value is true it indicates that an off-channel scan is
	 currently running.  This implies that the radio is current
	 disabled."
	 ::= { extremeWirelessScanStatusEntry 5 }

extremeWirelessScanCurrentChannel OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"If the value of extremeWirelessScanOffChannelRunning is true
	 this variable give the value of the current channel the AP is
	 scanning on.  If a scan is not running, the value of this variable
	 is undefined."
	 ::= { extremeWirelessScanStatusEntry 6 }

extremeWirelessScanLastElement OBJECT-TYPE
	SYNTAX TimeTicks
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the sysUpTime when the last new station was inserted
	 in the results table."
	 ::= { extremeWirelessScanStatusEntry 7 }

extremeWirelessScanNumProbes OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of probe requests sent by this wireless 
	 interface."
	 ::= { extremeWirelessScanStatusEntry 8 }

-- ************************************************************** --
-- Scan Results Table : This table provides information collected  --
-- during on and off-channel scans about the APs discovered.       --
-- ************************************************************** --
extremeWirelessScanResultsTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessScanResultsEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"This table contains one entry per wireless interface.  It
	 provides status and statistics information for the scan 
	 feature operating on that wireless interface."
	 ::= { extremeAP 27 }

extremeWirelessScanResultsEntry OBJECT-TYPE
	SYNTAX ExtremeWirelessScanResultsEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	""
	INDEX { ifIndex, extremeWirelessScanResultsStationId }
	 ::= { extremeWirelessScanResultsTable 1 }

ExtremeWirelessScanResultsEntry ::= SEQUENCE {
	extremeWirelessScanResultsStationId		 MacAddress,
	extremeWirelessScanResultsFirstSeen		 TimeTicks,
	extremeWirelessScanResultsLastChange		 TimeTicks,
	extremeWirelessScanResultsPacketTime		 INTEGER,
	extremeWirelessScanResultsPacketRate	 	 INTEGER,
	extremeWirelessScanResultsChannel		 INTEGER,
	extremeWirelessScanResultsMinRSS		 INTEGER,
	extremeWirelessScanResultsMaxRSS		 INTEGER,
	extremeWirelessScanResultsAvgRSS		 INTEGER,
	extremeWirelessScanResultsTotalBeacons		 Unsigned32,
	extremeWirelessScanResultsTotalProbes		 Unsigned32,
	extremeWirelessScanResultsDiscoveredBy		 INTEGER,
	extremeWirelessScanResultsDSSOFDM		 TruthValue,
	extremeWirelessScanResultsRSNEnabled		 TruthValue,
	extremeWirelessScanResultsGShortSlot		 TruthValue,
	extremeWirelessScanResultsChannelAgility	 TruthValue,
	extremeWirelessScanResultsPBCC			 TruthValue,
	extremeWirelessScanResultsPreamble		 TruthValue,
	extremeWirelessScanResultsPrivacy		 TruthValue,
	extremeWirelessScanResultsCFPollReq		 TruthValue,
	extremeWirelessScanResultsCFPollable		 TruthValue,
	extremeWirelessScanResultsNetworkType 		 INTEGER,
	extremeWirelessScanResultsSSID 			 OCTET STRING,
	extremeWirelessScanResultsRateSet		 OCTET STRING,
	extremeWirelessScanResultsExtRateSet		 OCTET STRING,
	extremeWirelessScanResultsDSSParameter		 INTEGER,
	extremeWirelessScanResultsTIMCount	 	 INTEGER,
	extremeWirelessScanResultsTIMPeriod	 	 INTEGER,
	extremeWirelessScanResultsTIMTrafficInd	 	 TruthValue,
	extremeWirelessScanResultsCountryCode		 OCTET STRING,
	extremeWirelessScanWPAIEPresent			 TruthValue,
	extremeWirelessScanWPAVersion			 Unsigned32,
	extremeWirelessScanWPAIEMcastCipher		 WPACipherSet,
	extremeWirelessScanWPAUcastCipherCount		 Unsigned32,
	extremeWirelessScanWPAUcastCipher		 WPACipherSet,
	extremeWirelessScanWPAKeyMgmtCount		 Unsigned32,
	extremeWirelessScanWPAKeyMgmtSuite		 WPAKeyMgmtSet,
	extremeWirelessScanResultsIEBlob	 	 OCTET STRING
}
	
extremeWirelessScanResultsStationId OBJECT-TYPE
	SYNTAX MacAddress
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the MAC address of the detected station."
	 ::= { extremeWirelessScanResultsEntry 1 }

extremeWirelessScanResultsFirstSeen OBJECT-TYPE
	SYNTAX TimeTicks
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the sysUpTime when this station entry was created."
	 ::= { extremeWirelessScanResultsEntry 2 }

extremeWirelessScanResultsLastChange OBJECT-TYPE
	SYNTAX TimeTicks
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the sysUpTime of the station entry the last time it was
	 updated (i.e. a beacon etc was received)."
	 ::= { extremeWirelessScanResultsEntry 3 }

extremeWirelessScanResultsPacketTime OBJECT-TYPE
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the timestamp field from the last beacon/probe response
	 received from this station."
	 ::= { extremeWirelessScanResultsEntry 4 }

extremeWirelessScanResultsPacketRate OBJECT-TYPE
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the rate at which the last packet was sent by the
	 station.

	 TODO: What are the units here on rate?"
	 ::= { extremeWirelessScanResultsEntry 5 }

extremeWirelessScanResultsChannel OBJECT-TYPE
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the channel the last packet received by this station
	 was recieved on."
	 ::= { extremeWirelessScanResultsEntry 6 }

extremeWirelessScanResultsMinRSS OBJECT-TYPE
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the smallest RSS value of any packet recieved from this
	 station."
	 ::= { extremeWirelessScanResultsEntry 7 }

extremeWirelessScanResultsMaxRSS OBJECT-TYPE
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the largest RSS value of any packet recieved from this
	 station."
	 ::= { extremeWirelessScanResultsEntry 8 }

extremeWirelessScanResultsAvgRSS OBJECT-TYPE
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is a running average of RSS values of all the packets
	 received from this station."
	 ::= { extremeWirelessScanResultsEntry 9 }

extremeWirelessScanResultsTotalBeacons OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This counter gives the total number of beacons received from this
	 station."
	 ::= { extremeWirelessScanResultsEntry 10 }

extremeWirelessScanResultsTotalProbes OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This counter gives the total number of probe responses
	 received from this station."
	 ::= { extremeWirelessScanResultsEntry 11 }

extremeWirelessScanResultsDiscoveredBy OBJECT-TYPE
	SYNTAX INTEGER { probe (1),
   		         beacon (2) }
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the type of packet which cause this results entry to be
	 created."
	 ::= { extremeWirelessScanResultsEntry 12 }

extremeWirelessScanResultsDSSOFDM OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"TODO : What is this?"
	 ::= { extremeWirelessScanResultsEntry 13 }

extremeWirelessScanResultsRSNEnabled OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"Indicates if RSN capabilities are enabled on the sending station."
	 ::= { extremeWirelessScanResultsEntry 14 }

extremeWirelessScanResultsGShortSlot OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"TODO : What is this?"
	 ::= { extremeWirelessScanResultsEntry 15 }

extremeWirelessScanResultsChannelAgility OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"TODO : What is this?"
	 ::= { extremeWirelessScanResultsEntry 16 }

extremeWirelessScanResultsPBCC OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"TODO : What is this?"
	 ::= { extremeWirelessScanResultsEntry 17 }

extremeWirelessScanResultsPreamble OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"TODO : What is this?"
	 ::= { extremeWirelessScanResultsEntry 18 }

extremeWirelessScanResultsPrivacy OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is true if MAC-based privacy is invoked on the sending
	 station."
	 ::= { extremeWirelessScanResultsEntry 19 }

extremeWirelessScanResultsCFPollReq OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"TODO: What is this?"
	 ::= { extremeWirelessScanResultsEntry 20 }

extremeWirelessScanResultsCFPollable OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"TODO: What is this?"
	 ::= { extremeWirelessScanResultsEntry 21 }

extremeWirelessScanResultsNetworkType OBJECT-TYPE
	SYNTAX INTEGER { ibss (1),
   		   	 bss  (2) }
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This indicates what type of network it is.  If this value is IBSS
	 the last beacon/probe response was sent by a host operating in
	 ad-hoc mode."
	 ::= { extremeWirelessScanResultsEntry 22 }

extremeWirelessScanResultsSSID OBJECT-TYPE
	SYNTAX OCTET STRING
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This provides the value of the SSID value as is was recieved in
	 the beacon or probe response.  If no SSID was sent in the probe
	 this value is NULL."
	 ::= { extremeWirelessScanResultsEntry 23 }

extremeWirelessScanResultsRateSet OBJECT-TYPE
	SYNTAX OCTET STRING
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This provides the value of the rate set IE as it was received in
	 the beacon or probe response.  If no rate set was recieved then
	 this value is NULL."
	 ::= { extremeWirelessScanResultsEntry 24 }

extremeWirelessScanResultsExtRateSet OBJECT-TYPE
	SYNTAX OCTET STRING
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This provides the value of the extended rate set IE as it was 
	 received in the beacon or probe response.  If no rate set was 
	 recieved then this value is NULL."
	 ::= { extremeWirelessScanResultsEntry 25 }

extremeWirelessScanResultsDSSParameter OBJECT-TYPE
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"Provides the value of the DSS parameter IE, which is the channel."
	 ::= { extremeWirelessScanResultsEntry 26 }

extremeWirelessScanResultsTIMCount OBJECT-TYPE
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"TODO: What is this?"
	 ::= { extremeWirelessScanResultsEntry 27 }

extremeWirelessScanResultsTIMPeriod OBJECT-TYPE
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"TODO: What is this?"
	 ::= { extremeWirelessScanResultsEntry 28 }

extremeWirelessScanResultsTIMTrafficInd OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"TODO: What is this?"
	 ::= { extremeWirelessScanResultsEntry 29 }

extremeWirelessScanResultsCountryCode OBJECT-TYPE
	SYNTAX OCTET STRING
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"Value of country code supplied by the IE"
	 ::= { extremeWirelessScanResultsEntry 30 }

extremeWirelessScanWPAIEPresent OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"If this value is true it indicates that WPA information was
	 gathered from this AP in the last beacon.  It implies that
	 the WPA variables below are valid.
	 If this value is false it indicates that this AP did not 
	 send a WPA IE in its last beacon, and the values below are
	 meaningless."
	::= { extremeWirelessScanResultsEntry 31 }

extremeWirelessScanWPAVersion OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This value gives the version of WPA supported by this AP.
	 See IEEE 802.11i Draft 3.0 section 7 for meaning of various
	 values."
	::= { extremeWirelessScanResultsEntry 32 }

extremeWirelessScanWPAIEMcastCipher OBJECT-TYPE
	SYNTAX WPACipherSet
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This value gives the single multicast cipher supported by this
	 AP."
	::= { extremeWirelessScanResultsEntry 33 }

extremeWirelessScanWPAUcastCipherCount OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This value gives the total number of unicast ciphers supported
	 by this AP.  It corresponds to the number of bits set in the 
	 extremeWirelessScanWPAUcastCipher variable."
	::= { extremeWirelessScanResultsEntry 34 }

extremeWirelessScanWPAUcastCipher OBJECT-TYPE
	SYNTAX WPACipherSet
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the list of cipher suites which are supported by 
	 this AP."
	::= { extremeWirelessScanResultsEntry 35 }

extremeWirelessScanWPAKeyMgmtCount OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of key-management schemes supported by
	 this AP.  It corresponds to the number of bits set in the
	 extremeWirelessScanWPAKeyMgmtSuite variable."
	::= { extremeWirelessScanResultsEntry 36 }

extremeWirelessScanWPAKeyMgmtSuite OBJECT-TYPE
	SYNTAX WPAKeyMgmtSet
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This indicates the supported key-management suites supported
	 by this AP."
	::= { extremeWirelessScanResultsEntry 37 }

extremeWirelessScanResultsIEBlob OBJECT-TYPE
	SYNTAX OCTET STRING
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"All the IEs received in the last packet encoded as a blob of
	 Type, Length, Value tuples."
	 ::= { extremeWirelessScanResultsEntry 38 }

-- ************************************************************** --
-- Probe Info Configuration Table : This table allows for config   --
-- for the collection of probe request packets.  The AP uses this  --
-- to populate the client information tables.                      --
-- ************************************************************** --
extremeWirelessProbeInfoCfgTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessProbeInfoCfgEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"This table contains one entry per physical and virtual interface.
	 It controls the collection of client information via PROBE REQ
	 packets."
	 ::= { extremeAP 28 } 

extremeWirelessProbeInfoCfgEntry OBJECT-TYPE
	SYNTAX ExtremeWirelessProbeInfoCfgEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"Note that the ifIndex here can be either a physical or virtual
	 wireless interface index."
	INDEX { ifIndex }
	 ::= { extremeWirelessProbeInfoCfgTable 1 }

ExtremeWirelessProbeInfoCfgEntry ::= SEQUENCE {
	extremeWirelessProbeInfoEnable		 TruthValue,
	extremeWirelessProbeInfoKeepIEs		 TruthValue,
	extremeWirelessProbeInfoTableSize	 Unsigned32,
	extremeWirelessProbeInfoTimeout		 Unsigned32,
	extremeWirelessProbeInfoTableClear	 TruthValue,
	extremeWirelessProbeInfoSourceClear	 MacAddress,
	extremeWirelessProbeInfoTableStatsClear  TruthValue,
	extremeWirelessProbeInfoSourceStatsClear MacAddress,
	extremeWirelessProbeInfoSendAddedTrap    TruthValue,
	extremeWirelessProbeInfoSendRemovedTrap  TruthValue }

extremeWirelessProbeInfoEnable OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"If this is set to TRUE then this virtual or physical
	interface will register with the MAC layer to receive
	notification of PROBE REQ packets.  In the case of 
	a virtual interface this implies the receipt of directed
	PROBE REQ packets.  If set to FALSE no PROBE REQ packets
	will be received, and current entries will eventually
	timeout."
	DEFVAL { true }
	 ::= { extremeWirelessProbeInfoCfgEntry 1 }

extremeWirelessProbeInfoKeepIEs OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"If this value is set to TRUE then the rate IE which
	 is carried in the PROBE REQ packet will be recorded.
	 If FALSE, no rate information will be kept."
	 DEFVAL { false }
	 ::= { extremeWirelessProbeInfoCfgEntry 2 }

extremeWirelessProbeInfoTableSize OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"This value sets the maximum size of the probe info 
	 results table, which limits the number of clients this
	 AP can record PROBE REQ information from."
	 DEFVAL { 128 }
	 ::= { extremeWirelessProbeInfoCfgEntry 3 }

extremeWirelessProbeInfoTimeout OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"This is the timeout, in seconds, for an entry in the 
	 probe info table.  Once a PROBE REQ has not been heard
	 from a client in this time period, it's entry is removed.
	 The value 0 is a sentinel, indicating no timeout."
	 DEFVAL { 3600 }
	 ::= { extremeWirelessProbeInfoCfgEntry 4 }

extremeWirelessProbeInfoTableClear OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"Setting this value to TRUE causes all entries in the 
	 probe info table to be removed.  Reading this value
	 has no meaning."
	 ::= { extremeWirelessProbeInfoCfgEntry 5 }

extremeWirelessProbeInfoSourceClear OBJECT-TYPE
	SYNTAX MacAddress
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"Setting this to the value of some MAC address results in
	 any matching MAC address in the probe info table being
	 removed.  Reading this value has no meaning."
	 ::= { extremeWirelessProbeInfoCfgEntry 6 }

extremeWirelessProbeInfoTableStatsClear OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"Setting this to TRUE results in all historical statistics
	 in the probe info table being set to 0.  No entries will
	 be removed.  Reading this has no meaning."
	 ::= { extremeWirelessProbeInfoCfgEntry 7 }

extremeWirelessProbeInfoSourceStatsClear OBJECT-TYPE
	SYNTAX MacAddress
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"Setting this to a MAC address will clear the historical
	 stats associated with the matching MAC address in the
	 probe info table.  Reading this has no meaning."
	 ::= { extremeWirelessProbeInfoCfgEntry 8 }

extremeWirelessProbeInfoSendAddedTrap OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"Setting this to TRUE will cause the management module to
	 send a trap whenever a new PROBE REQ source is added to 
	 the probe info table.  Setting this to FALSE will 
	 suppress the trap."
	 DEFVAL { false }
	 ::= { extremeWirelessProbeInfoCfgEntry 9 }

extremeWirelessProbeInfoSendRemovedTrap OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"Setting this to TRUE will cause the management module to
	 send a trap whenever a PROBE REQ source is removed from
	 the probe info table.  Setting this to false will 
	 suppress the trap."
	 DEFVAL { false }
	 ::= { extremeWirelessProbeInfoCfgEntry 10 }

-- ************************************************************** --
-- Probe Info Status Table : This table gives current status of    --
-- the probe request storage feature.                              --
-- ************************************************************** --
extremeWirelessProbeInfoStatusTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessProbeInfoStatusEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"This table contains one entry per physical and virtual interface.
	 It gives debugging and status information for the operation of the
	 probe info feature on that interface."
	 ::= { extremeAP 29 }

extremeWirelessProbeInfoStatusEntry OBJECT-TYPE
	SYNTAX ExtremeWirelessProbeInfoStatusEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"Note that the ifIndex here can be either a physical or virtual
	 wireless interface index."
	INDEX { ifIndex }
	 ::= { extremeWirelessProbeInfoStatusTable 1 }

ExtremeWirelessProbeInfoStatusEntry ::= SEQUENCE {
	extremeWirelessProbeInfoStatusCurrentTableSize Unsigned32,
	extremeWirelessProbeInfoStatusWatermark	       Unsigned32,
	extremeWirelessProbeInfoStatusTotalOverflows   Unsigned32,
	extremeWirelessProbeInfoStatusTotalTimeouts    Unsigned32,
	extremeWirelessProbeInfoStatusLastElement      TimeTicks,
	extremeWirelessProbeInfoStatusTotalProbes      Unsigned32
}

extremeWirelessProbeInfoStatusCurrentTableSize OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the current number of entries in the probe 
	 info table for this interface."
	 ::= { extremeWirelessProbeInfoStatusEntry 1 }

extremeWirelessProbeInfoStatusWatermark OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the maximum size the probe info table has been
	 since the statistics have been reset."
	 ::= { extremeWirelessProbeInfoStatusEntry 2 }

extremeWirelessProbeInfoStatusTotalOverflows OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of times an entry in the probe info
	 table was overwritten because the table was full."
	 ::= { extremeWirelessProbeInfoStatusEntry 3 }

extremeWirelessProbeInfoStatusTotalTimeouts OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of times an entry in the probe info
	 table was timed out."
	 ::= { extremeWirelessProbeInfoStatusEntry 4 }

extremeWirelessProbeInfoStatusLastElement OBJECT-TYPE
	SYNTAX TimeTicks
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the sysUpTime the last time an entry was added
	 to the probe info table (or modified)."
	 ::= { extremeWirelessProbeInfoStatusEntry 5 }

extremeWirelessProbeInfoStatusTotalProbes OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of PROBE REQ packets that
	 this interface has gotten."
	 ::= { extremeWirelessProbeInfoStatusEntry 6 }

-- ************************************************************** --
-- Probe Info Table : This table contains information on the probe --
-- request packets recieved from particular hosts.                 --
-- ************************************************************** --
extremeWirelessProbeInfoTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessProbeInfoEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"This table contains one entry for each source MAC from which
	 a PROBE REQ packet has been received.  Entries are added when
	 a packet is recieved from a new source mac.  Entries are 
	 removed via management action, or by timeout or overflow."
	 ::= { extremeAP 30 }

extremeWirelessProbeInfoEntry OBJECT-TYPE
	SYNTAX ExtremeWirelessProbeInfoEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"Note that the ifIndex here can be either a physical or virtual
	 wireless interface index.  In addition, this table is indexed
	 by the MAC address of the PROBE REQ source."
	INDEX { ifIndex, extremeWirelessProbeInfoSource }
	 ::= { extremeWirelessProbeInfoTable 1 }

ExtremeWirelessProbeInfoEntry ::= SEQUENCE {
	extremeWirelessProbeInfoSource		MacAddress,
	extremeWirelessProbeInfoTotalProbes	Unsigned32,
	extremeWirelessProbeInfoTotalProbeResp	Unsigned32,
	extremeWirelessProbeInfoRateIESize	Unsigned32,
	extremeWirelessProbeInfoRateIE		OCTET STRING,
	extremeWirelessProbeInfoFirstSeen 	TimeTicks,
	extremeWirelessProbeInfoLastChange	TimeTicks,
	extremeWirelessProbeInfoLastRSS		INTEGER,
	extremeWirelessProbeInfoLastRate	INTEGER,
	extremeWirelessProbeInfoLastChannel	INTEGER }

extremeWirelessProbeInfoSource OBJECT-TYPE
	SYNTAX MacAddress
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the MAC address of the source which sent us the 
	 PROBE REQ packets described by this entry."
	 ::= { extremeWirelessProbeInfoEntry 1 }

extremeWirelessProbeInfoTotalProbes OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of PROBE REQ packets we have
	 received from this source since the last time the stats
	 were cleared."
	 ::= { extremeWirelessProbeInfoEntry 2 }

extremeWirelessProbeInfoTotalProbeResp OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of PROBE RESP packets we have
	 sent to this source.  This may not be equal to PROBE REQ
	 based on rxmit, misses, etc."
	 ::= { extremeWirelessProbeInfoEntry 3 }

extremeWirelessProbeInfoRateIESize OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the size of the rate-ie field in bytes.  This
	 may be 0, at which point there is no rate-ie."
	 ::= { extremeWirelessProbeInfoEntry 4 }

extremeWirelessProbeInfoRateIE OBJECT-TYPE
	SYNTAX OCTET STRING
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the rate IE as recieved in the last PROBE REQ
	 packet.  It is encoded as a TLV exactly as it was in the
	 frame.  This field may return NULL if storing of rate IE
	 fields is disabled."
	 ::= { extremeWirelessProbeInfoEntry 5 }

extremeWirelessProbeInfoFirstSeen OBJECT-TYPE
	SYNTAX TimeTicks
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the sysUpTime the first time a PROBE REQ was
	 seen from this source."
	 ::= { extremeWirelessProbeInfoEntry 6 }

extremeWirelessProbeInfoLastChange OBJECT-TYPE
	SYNTAX TimeTicks
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the sysUpTime the last time a PROBE REQ was
	 seen from this source."
	 ::= { extremeWirelessProbeInfoEntry 7 }

extremeWirelessProbeInfoLastRSS OBJECT-TYPE
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the RSSI from the last PROBE REQ packet received
	 from this station."
	 ::= { extremeWirelessProbeInfoEntry 8 }

extremeWirelessProbeInfoLastRate OBJECT-TYPE
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the rate at which the last packet was received
	 from this station."
	 ::= { extremeWirelessProbeInfoEntry 9 }

extremeWirelessProbeInfoLastChannel OBJECT-TYPE
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the channel on which the last PROBE REQ from
	 this station was heard.  PROBE REQs may be heard during
	 an off-channel scan, at which point this may not be
	 equal to the current channel."
	 ::= { extremeWirelessProbeInfoEntry 10 }

-- ************************************************************** --
-- Per Client Historical Diagnostic Table : This table allows for  --
-- configuration of diagnostic information collection.             --
-- ************************************************************** -- 
extremeWirelessClientDiagCfgTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessClientDiagCfgEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"This table contains one row per wireless interface.  Each row
	 contains configuration values for collection of per-client
	 diagnostic information."
	 ::= { extremeAP 31 }

extremeWirelessClientDiagCfgEntry OBJECT-TYPE
	SYNTAX ExtremeWirelessClientDiagCfgEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"There is one entry in this table per virtual interface
	 (SSID)."
	INDEX { ifIndex }
	 ::= { extremeWirelessClientDiagCfgTable 1 }

ExtremeWirelessClientDiagCfgEntry ::= SEQUENCE {
	extremeWirelessClientDiagCfgEnable		TruthValue,
	extremeWirelessClientDiagCfgClearClient		MacAddress,
	extremeWirelessClientDiagCfgTableSize		Unsigned32,
	extremeWirelessClientDiagCfgTimeout		Unsigned32
}

extremeWirelessClientDiagCfgEnable OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"Setting this to TRUE enables the collection of historical 
	 information on this virtual interface.  This implies that 
	 stations which send ASSOC or AUTH packets will have new 
	 entries created in the table for this interface."
	 DEFVAL { true }
	 ::= { extremeWirelessClientDiagCfgEntry 1 }

extremeWirelessClientDiagCfgClearClient OBJECT-TYPE
	SYNTAX MacAddress
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"Setting this to the MAC address of a client in the diag
	 tables will clear the counters for that client.  The entry
	 will not be removed from the table, but all summation 
	 counters will be cleared."
	 ::= { extremeWirelessClientDiagCfgEntry 2 }

extremeWirelessClientDiagCfgTableSize OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"This value will configure the maximum size of the diag table.
	 The value is specified in number of entries.  A value of 0
	 implies no upper limit."
	 DEFVAL { 128 }
	 ::= { extremeWirelessClientDiagCfgEntry 3 }

extremeWirelessClientDiagCfgTimeout OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"This value will configure the timeout of an entry from the
	 diagnostics tables.  The value is given in seconds.  A value
	 of 0 implies no timeout."
	 DEFVAL { 3600 }
	 ::= { extremeWirelessClientDiagCfgEntry 4 }

-- ************************************************************** --
-- Per client historical feature status                            --
-- ************************************************************** --
extremeWirelessClientDiagStatusTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessClientDiagStatusEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"This table contains one entry per virtual interface.  Values
	 stored here give current status of the historical client diag
	 feature."
	 ::= { extremeAP 32 }

extremeWirelessClientDiagStatusEntry OBJECT-TYPE
	SYNTAX ExtremeWirelessClientDiagStatusEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"Note that ifIndex here is virtual ifIndex (SSID)."
	INDEX { ifIndex }
	 ::= { extremeWirelessClientDiagStatusTable 1 }

ExtremeWirelessClientDiagStatusEntry ::= SEQUENCE {
	extremeWirelessClientDiagCurrentTableSize	Unsigned32,
	extremeWirelessClientDiagTableWatermark		Unsigned32,
	extremeWirelessClientDiagTotalOverflows		Unsigned32,
	extremeWirelessClientDiagTotalTimeouts		Unsigned32,
	extremeWirelessClientDiagLastElement		TimeTicks,
	extremeWirelessClientDiagSupportsSizeCounters	TruthValue,
	extremeWirelessClientDiagSupportsSpeedCounters	TruthValue,
	extremeWirelessClientDiagSupportsPacketCounters	TruthValue
}

extremeWirelessClientDiagCurrentTableSize OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the current size, in entries of the client diag
	 tables."
	 ::= { extremeWirelessClientDiagStatusEntry 1 }

extremeWirelessClientDiagTableWatermark OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the maximum size the client diag table has been
	 since the last time the statistics were cleared."
	 ::= { extremeWirelessClientDiagStatusEntry 2 }

extremeWirelessClientDiagTotalOverflows OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the total number of times an entry has been
	 replaced by a newer entry because there was no room
	 left in the table."
	 ::= { extremeWirelessClientDiagStatusEntry 3 }

extremeWirelessClientDiagTotalTimeouts OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the total number of times an entry has been
	 aged-out of the table."
	 ::= { extremeWirelessClientDiagStatusEntry 4 }

extremeWirelessClientDiagLastElement OBJECT-TYPE
	SYNTAX TimeTicks
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is sysUpTime when the last entry was added to
	 the table."
	 ::= { extremeWirelessClientDiagStatusEntry 5 }

extremeWirelessClientDiagSupportsSpeedCounters OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This value indicates if this AP supports the speed-based
	 counters from the extremeWirelessClientSpeedCountersTable."
	 ::= { extremeWirelessClientDiagStatusEntry 6 }

extremeWirelessClientDiagSupportsSizeCounters OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This value indicates if this AP supports the size-based
	 counters from the extremeWirelessClientMACSizeCounterTable."
	 ::= { extremeWirelessClientDiagStatusEntry 7 }

extremeWirelessClientDiagSupportsPacketCounters OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This value indicates if this AP supports the packet-based
	 counters from the extremeWirelessClientPacketCountersTable."
	 ::= { extremeWirelessClientDiagStatusEntry 8 }

-- ************************************************************** --
-- Per Client Historical Diagnostics : This table contains info    --
-- about state transitions for each client.
-- ************************************************************** --
extremeWirelessClientDiagTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessClientDiagEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"This table contains information on a per-client basis.  Rows are
	 indexed first by virtual interface, then by client MAC."
	 ::= { extremeAP 33 }

extremeWirelessClientDiagEntry OBJECT-TYPE
	SYNTAX ExtremeWirelessClientDiagEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"Note that ifIndex here is virtual ifIndex (SSID)."
	INDEX { ifIndex, extremeWirelessClientDiagMac }
	 ::= { extremeWirelessClientDiagTable 1 }

ExtremeWirelessClientDiagEntry ::= SEQUENCE {
	extremeWirelessClientDiagMac			MacAddress,
	extremeWirelessClientDiagStateWatermark		INTEGER,
	extremeWirelessClientDiagEntersInDetected	Unsigned32,
	extremeWirelessClientDiagErrorsInDetected	Unsigned32,
	extremeWirelessClientDiagAuthReqInDetected	Unsigned32,
	extremeWirelessClientDiagOtherReqInDetected	Unsigned32,
	extremeWirelessClientDiagMgmtActionInDetected	Unsigned32,
	extremeWirelessClientDiagTimeOutInDetected	Unsigned32,
	extremeWirelessClientDiagEntersInAuth		Unsigned32,
	extremeWirelessClientDiagErrorsInAuth		Unsigned32,
	extremeWirelessClientDiagAssocReqInAuth		Unsigned32,
	extremeWirelessClientDiagOtherReqInAuth		Unsigned32,
	extremeWirelessClientDiagMgmtActionInAuth	Unsigned32,
	extremeWirelessClientDiagTimeOutInAuth		Unsigned32,
	extremeWirelessClientDiagEntersInAssoc		Unsigned32,
	extremeWirelessClientDiagErrorsInAssoc		Unsigned32,
	extremeWirelessClientDiagMgmtActionInAssoc	Unsigned32,
	extremeWirelessClientDiagTimeOutInAssoc		Unsigned32,
	extremeWirelessClientDiagEntersInForward	Unsigned32,
	extremeWirelessClientDiagMgmtActionInForward	Unsigned32,
	extremeWirelessClientDiagTimeOutInForward	Unsigned32,
	extremeWirelessClientDiagTotal802Auths		Unsigned32,
	extremeWirelessClientDiagTotalNetLoginAuths	Unsigned32
}

extremeWirelessClientDiagMac OBJECT-TYPE
	SYNTAX MacAddress
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"This is the MAC address of the station this entry 
	 describes."
	 ::= { extremeWirelessClientDiagEntry 1 }

extremeWirelessClientDiagStateWatermark OBJECT-TYPE
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"This is the highest state this client has been in."
	::= { extremeWirelessClientDiagEntry 2 }

extremeWirelessClientDiagEntersInDetected OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"This is the total number of times the client has entered
	 the detected state."
	::= { extremeWirelessClientDiagEntry 3 }

extremeWirelessClientDiagErrorsInDetected OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"This is the total number of errors this client has 
	 experienced since the counters were cleared."
	::= { extremeWirelessClientDiagEntry 4 }

extremeWirelessClientDiagAuthReqInDetected OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"This is the total number of AUTH REQ packets received
	 from this client while it was in the detected state."
	::= { extremeWirelessClientDiagEntry 5 }

extremeWirelessClientDiagOtherReqInDetected OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"This is the total number of REQ packets received from
	 this client while it was in detected state that were
	 not AUTH REQ packets."
	::= { extremeWirelessClientDiagEntry 6 }

extremeWirelessClientDiagMgmtActionInDetected OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"This is the total number of times management initiated
	 action (i.e. force-disassociate) was received for this
	 client in the detected state."
	::= { extremeWirelessClientDiagEntry 7 }

extremeWirelessClientDiagTimeOutInDetected OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"This is the total number of timeouts which happened to
	 this client in the detected state."
	::= { extremeWirelessClientDiagEntry 8 }

extremeWirelessClientDiagEntersInAuth OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"This is the total number of times the client has entered
	 the AUTHED state."
	::= { extremeWirelessClientDiagEntry 9 }

extremeWirelessClientDiagErrorsInAuth OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"This is the total number of times the client has had
	 errors in the AUTHED state."
	::= { extremeWirelessClientDiagEntry 10 }

extremeWirelessClientDiagAssocReqInAuth OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"This is the total number of ASSOC REQ or REASSOC REQ
	 packets received from this client while in the AUTHED 
	 state."
	::= { extremeWirelessClientDiagEntry 11 }

extremeWirelessClientDiagOtherReqInAuth OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"This is the total number of non-ASSOC/REASSOC packets
	 received from this client while in the AUTHED state."
	::= { extremeWirelessClientDiagEntry 12 }

extremeWirelessClientDiagMgmtActionInAuth OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"This is the total number of management initiated action
	 which this client experienced while in the AUTHED state."
	::= { extremeWirelessClientDiagEntry 13 }

extremeWirelessClientDiagTimeOutInAuth OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"This is the total number of times this client timed out
	 while in the authed state."
	::= { extremeWirelessClientDiagEntry 14 }

extremeWirelessClientDiagEntersInAssoc OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"This is the total number of times this client has entered
	 the associated state."
	::= { extremeWirelessClientDiagEntry 15 }

extremeWirelessClientDiagErrorsInAssoc OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"This is the total number of errors this client has had
	 in the associated state."
	::= { extremeWirelessClientDiagEntry 16 }

extremeWirelessClientDiagMgmtActionInAssoc OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"This is the total number of management actions which have
	 happened to this client in the associated state."
	::= { extremeWirelessClientDiagEntry 17 }

extremeWirelessClientDiagTimeOutInAssoc OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"This is the total number of times this station has been
	 timed-out in the associated state."
	::= { extremeWirelessClientDiagEntry 18 }

extremeWirelessClientDiagEntersInForward OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"This is the total number of times this client has entered
	 the forwarding state."
	::= { extremeWirelessClientDiagEntry 19 }

extremeWirelessClientDiagMgmtActionInForward OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"This is the total number of times this client has
	 experience a management action while in forwarding."
	::= { extremeWirelessClientDiagEntry 20 }

extremeWirelessClientDiagTimeOutInForward OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"This is the total number of timeouts this client has
	 experienced while in forwarding."
	::= { extremeWirelessClientDiagEntry 21 }

extremeWirelessClientDiagTotal802Auths OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"This is the total number of times this client has tried
	 to authenticate using 802.1x."
	::= { extremeWirelessClientDiagEntry 22 }

extremeWirelessClientDiagTotalNetLoginAuths OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"This is the total number of times this client has tried
	 to authenticate using NetLogin."
	::= { extremeWirelessClientDiagEntry 23 }

-- ************************************************************** --
-- Per Client Association Information : This table gives history   --
-- on the association packets sent by each client on the AP.       --
-- ************************************************************** --
extremeWirelessClientAssocInfoTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessClientAssocInfoEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"This table contains one row per client on a wireless interface.
	 It gives information about the association history and parameters
	 of that client."
	 ::= { extremeAP 34 }

extremeWirelessClientAssocInfoEntry OBJECT-TYPE
	SYNTAX ExtremeWirelessClientAssocInfoEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"Note that ifIndex here is virtual ifIndex (SSID)."
	INDEX { ifIndex, extremeWirelessClientDiagMac }
	 ::= { extremeWirelessClientAssocInfoTable 1 }

ExtremeWirelessClientAssocInfoEntry ::= SEQUENCE {
	extremeWirelessClientAssocInfoAssociated		TruthValue,
	extremeWirelessClientAssocInfoTotalAssocReq		Unsigned32,
	extremeWirelessClientAssocInfoTotalReAssocReq		Unsigned32,
	extremeWirelessClientAssocInfoTotalAssocResp		Unsigned32,
	extremeWirelessClientAssocInfoTotalAssocOK		Unsigned32,
	extremeWirelessClientAssocInfoTotalAssocFail		Unsigned32,
	extremeWirelessClientAssocInfoTotalDisassocReq		Unsigned32,
	extremeWirelessClientAssocInfoTotalDisassocResp		Unsigned32,
	extremeWirelessClientAssocInfoRateIE			OCTET STRING,
	extremeWirelessClientAssocInfoLastAssoc			TimeTicks,
	extremeWirelessClientAssocInfoLastError			TimeTicks,
	extremeWirelessClientAssocInfoLastErrorType		INTEGER,
	extremeWirelessClientAssocInfoErrorRateMismatch		Unsigned32,
	extremeWirelessClientAssocInfoErrorBadState		Unsigned32,
	extremeWirelessClientAssocInfoErrorBadCapability	Unsigned32,
	extremeWirelessClientAssocInfoErrorCounterMeasure	Unsigned32,
	extremeWirelessClientAssocInfoErrorMcastCipher		Unsigned32,
	extremeWirelessClientAssocInfoErrorMaxAssoc 		Unsigned32,
	extremeWirelessClientAssocInfoErrorRSNRequired		Unsigned32,
	extremeWirelessClientAssocInfoErrorRSNMismatch 		Unsigned32,
	extremeWirelessClientAssocInfoErrorOther		Unsigned32,
	extremeWirelessClientAssocInfoWPAIEPresent		TruthValue,
	extremeWirelessClientAssocInfoWPAVersion		Unsigned32,
	extremeWirelessClientAssocInfoWPAIEMcastCipher		WPACipherSet,
	extremeWirelessClientAssocInfoWPAUcastCipherCount	Unsigned32,
	extremeWirelessClientAssocInfoWPAUcastCipher		WPACipherSet,
	extremeWirelessClientAssocInfoWPAKeyMgmtCount		Unsigned32,
	extremeWirelessClientAssocInfoWPAKeyMgmtSuite		WPAKeyMgmtSet,
	extremeWirelessClientAssocIEBlob			OCTET STRING
}

extremeWirelessClientAssocInfoAssociated OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the current MAC-layer association status of 
	 this client."
	 ::= { extremeWirelessClientAssocInfoEntry 1 }

extremeWirelessClientAssocInfoTotalAssocReq OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of ASSOC REQ pdus recieved
	 from this client since the last time the counters were
	 cleared."
	 ::= { extremeWirelessClientAssocInfoEntry 2 }

extremeWirelessClientAssocInfoTotalReAssocReq OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of REASSOC REQ PDUs received
	 from this client since the last time the counters were
	 cleared."
	 ::= { extremeWirelessClientAssocInfoEntry 3 }

extremeWirelessClientAssocInfoTotalAssocResp OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of ASSOC RESP pdus sent to
	 this client since the last time the counters were cleared."
	 ::= { extremeWirelessClientAssocInfoEntry 4 }

extremeWirelessClientAssocInfoTotalAssocOK OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of ASSOC RESP PDUs which
	 carried a status = ok response."
	 ::= { extremeWirelessClientAssocInfoEntry 5 }

extremeWirelessClientAssocInfoTotalAssocFail OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of ASSOC RESP PDUs which
	 carried a status = failed response."
	 ::= { extremeWirelessClientAssocInfoEntry 6 }

extremeWirelessClientAssocInfoTotalDisassocReq OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of ASSOC RESP PDUs which
	 carried a status = failed response."
	 ::= { extremeWirelessClientAssocInfoEntry 7 }

extremeWirelessClientAssocInfoTotalDisassocResp OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of ASSOC RESP PDUs which
	 carried a status = failed response."
	 ::= { extremeWirelessClientAssocInfoEntry 8 }

extremeWirelessClientAssocInfoRateIE OBJECT-TYPE
	SYNTAX OCTET STRING
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the value of the rate IE carried in the last
	 ASSOC REQ packet if this wireless interface is configured
	 to keep IEs.  If it's not, this will be NULL.  The IE
	 is encoded as a series of bytes exactly as the value 
	 portion of the IE in the PDU."
	 ::= { extremeWirelessClientAssocInfoEntry 9 }

extremeWirelessClientAssocInfoLastAssoc OBJECT-TYPE
	SYNTAX TimeTicks
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is sysUpTime when the last ASSOC REQ was received
	 from this client."
	 ::= { extremeWirelessClientAssocInfoEntry 10 }

extremeWirelessClientAssocInfoLastError OBJECT-TYPE
	SYNTAX TimeTicks
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is sysUpTime when the last ASSOC RESP was sent to
	 this client with a failure status."
	 ::= { extremeWirelessClientAssocInfoEntry 11 }

extremeWirelessClientAssocInfoLastErrorType OBJECT-TYPE
	SYNTAX INTEGER { noError(0),
			 rateMismatch(1),
			 badState(2),
			 badCapability(3),
			 couterMeasure(4),
			 mcastCipher(5),
			 maxAssoc(6),
			 rsnRequired(7),
			 rsnMismatch(8),
			 otherError(9) }
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is an enumerated type which indicates which was the
	 last error this client experienced during association."
	 ::= { extremeWirelessClientAssocInfoEntry 12 }

extremeWirelessClientAssocInfoErrorRateMismatch OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the total number of failed associations due to 
	 a mismatch of the rate IEs."
	 ::= { extremeWirelessClientAssocInfoEntry 13 }

extremeWirelessClientAssocInfoErrorBadState OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the total number of failed associations due to 
	 the client being in the wrong state."
	 ::= { extremeWirelessClientAssocInfoEntry 14 }

extremeWirelessClientAssocInfoErrorBadCapability OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the total number of failed associations due to 
	 the client having a capability mismatch with the AP."
	 ::= { extremeWirelessClientAssocInfoEntry 15 }

extremeWirelessClientAssocInfoErrorCounterMeasure OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the total number of failed associations due to 
	 the client being subject to a counter measure."
	 ::= { extremeWirelessClientAssocInfoEntry 16 }

extremeWirelessClientAssocInfoErrorMcastCipher OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the total number of failed associations due to 
	 the client not supporting the current multicast cipher."
	 ::= { extremeWirelessClientAssocInfoEntry 17 }

extremeWirelessClientAssocInfoErrorMaxAssoc OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the total number of failed associations due to 
	 the AP having too many associations already."
	 ::= { extremeWirelessClientAssocInfoEntry 18 }

extremeWirelessClientAssocInfoErrorRSNRequired OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the total number of failed associations due to 
	 the client not supplying the (required) RSN IE."
	 ::= { extremeWirelessClientAssocInfoEntry 19 }

extremeWirelessClientAssocInfoErrorRSNMismatch OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the total number of failed associations due to 
	 the client's RSN IE not matching supported features on 
	 the AP."
	 ::= { extremeWirelessClientAssocInfoEntry 20 }

extremeWirelessClientAssocInfoErrorOther OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the total number of failed associations due to 
	 the client's RSN IE not matching supported features on 
	 the AP."
	 ::= { extremeWirelessClientAssocInfoEntry 21 }

extremeWirelessClientAssocInfoWPAIEPresent OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"If this value is true it indicates that WPA information was
	 gathered from this station in the last association request.
	 If true, it implies the values of the WPA variables below 
	 are valid.  If false, it indicates that this station did not
	 send a WPA IE in its last association."
	::= { extremeWirelessClientAssocInfoEntry 22 }

extremeWirelessClientAssocInfoWPAVersion OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This value gives the version of WPA supported by this station.
	 See IEEE 802.11i Draft 3.0 section 7 for meaning of various
	 values."
	::= { extremeWirelessClientAssocInfoEntry 23 }

extremeWirelessClientAssocInfoWPAIEMcastCipher OBJECT-TYPE
	SYNTAX WPACipherSet
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This value gives the single multicast cipher supported by this
	 client."
	::= { extremeWirelessClientAssocInfoEntry 24 }

extremeWirelessClientAssocInfoWPAUcastCipherCount OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of set bits in the ucast cipher
	 variable below.  In this case this number should always
	 be 1."
	::= { extremeWirelessClientAssocInfoEntry 25 }

extremeWirelessClientAssocInfoWPAUcastCipher OBJECT-TYPE
	SYNTAX WPACipherSet
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the cipher suites which was requested by 
	 this client during its last assoc req."
	::= { extremeWirelessClientAssocInfoEntry 26 }

extremeWirelessClientAssocInfoWPAKeyMgmtCount OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This value gives the number of key management suites 
	 requested by this client in the last assoc. req message.
	 It indicates the number of set bits in the mgmt suite 
	 variable below."
	::= { extremeWirelessClientAssocInfoEntry 27 }

extremeWirelessClientAssocInfoWPAKeyMgmtSuite OBJECT-TYPE
	SYNTAX WPAKeyMgmtSet
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"Gives the key management suite requested by this client 
	 during its last association request."
	::= { extremeWirelessClientAssocInfoEntry 28 }

extremeWirelessClientAssocIEBlob OBJECT-TYPE
	SYNTAX OCTET STRING
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the IE list sent in the association frame encoded as
	 a series of TLVs."
	::= { extremeWirelessClientAssocInfoEntry 29 }


-- ************************************************************** --
-- Authentication Information Table : This table contains infor on --
-- the MAC-layer authentication of each client which has tried to  --
-- authenticate with this AP.
-- ************************************************************** --
extremeWirelessClientAuthInfoTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessClientAuthInfoEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"This table contains one row per client on a wireless interface.
	 It gives information about the authentication history and params
	 of that client."
	 ::= { extremeAP 35 }

extremeWirelessClientAuthInfoEntry OBJECT-TYPE
	SYNTAX ExtremeWirelessClientAuthInfoEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"Note that ifIndex here is virtual ifIndex (SSID)."
	INDEX { ifIndex, extremeWirelessClientDiagMac }
	 ::= { extremeWirelessClientAuthInfoTable 1 }

ExtremeWirelessClientAuthInfoEntry ::= SEQUENCE {
	extremeWirelessClientAuthInfoCurrentAuth	TruthValue,
	extremeWirelessClientAuthInfoTotalAuths		Unsigned32,
	extremeWirelessClientAuthInfoTotalAuthResp	Unsigned32,
	extremeWirelessClientAuthInfoTotalAuthsOK	Unsigned32,
	extremeWirelessClientAuthInfoTotalAuthsFailed	Unsigned32,
	extremeWirelessClientAuthInfoTotalDeauthReq     Unsigned32,
	extremeWirelessClientAuthInfoTotalDeauthResp    Unsigned32,
	extremeWirelessClientAuthInfoTotalOpen		Unsigned32,
	extremeWirelessClientAuthInfoTotalShared	Unsigned32,
	extremeWirelessClientAuthInfoLastAuth		TimeTicks,
	extremeWirelessClientAuthInfoLastAuthType	INTEGER,
	extremeWirelessClientAuthInfoLastError		TimeTicks,
	extremeWirelessClientAuthInfoLastErrorType	INTEGER,
	extremeWirelessClientAuthInfoErrorResourceFailure  Unsigned32,
	extremeWirelessClientAuthInfoErrorSequenceNum	Unsigned32,
	extremeWirelessClientAuthInfoErrorChallengeText	Unsigned32,
	extremeWirelessClientAuthInfoErrorTypeMismatch	Unsigned32,
	extremeWirelessClientAuthInfoErrorKeyIndex	Unsigned32,
	extremeWirelessClientAuthInfoErrorOther         Unsigned32
}

extremeWirelessClientAuthInfoCurrentAuth OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the current MAC-layer authentication status of the
	 client."
	 ::= { extremeWirelessClientAuthInfoEntry 1 }

extremeWirelessClientAuthInfoTotalAuths OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the total number of AUTH REQ packets received from 
	 this client since the last time the counters were cleared."
	 ::= { extremeWirelessClientAuthInfoEntry 2 }

extremeWirelessClientAuthInfoTotalAuthResp OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the total number of AUTH RESP packets sent to
	 this client since the last time the counters were cleared."
	 ::= { extremeWirelessClientAuthInfoEntry 3 }

extremeWirelessClientAuthInfoTotalAuthsOK OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the total number of AUTH RESP packets sent to
	 this client which carried a STATUS = OK message."
	 ::= { extremeWirelessClientAuthInfoEntry 4 }

extremeWirelessClientAuthInfoTotalAuthsFailed OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the total number of AUTH RESP packets sent to
	 this client which carried a STATUS = Failed message."
	 ::= { extremeWirelessClientAuthInfoEntry 5 }

extremeWirelessClientAuthInfoTotalDeauthReq OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the total number of DEAUTH REQ packets sent from
	 this client."
	 ::= { extremeWirelessClientAuthInfoEntry 6 }

extremeWirelessClientAuthInfoTotalDeauthResp OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the total number of DEAUTH RESP packets sent to
	 this client."
	 ::= { extremeWirelessClientAuthInfoEntry 7 }

extremeWirelessClientAuthInfoTotalOpen OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the total number of AUTH REQ packets which 
	 requested open authentication from the AP."
	 ::= { extremeWirelessClientAuthInfoEntry 8 }

extremeWirelessClientAuthInfoTotalShared OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the total number of AUTH REQ packets which 
	 requested shared authentication from the AP."
	 ::= { extremeWirelessClientAuthInfoEntry 9 }

extremeWirelessClientAuthInfoLastAuth OBJECT-TYPE
	SYNTAX TimeTicks
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the sysUpTime the last time this client sent
	 a request for authentication."
	 ::= { extremeWirelessClientAuthInfoEntry 10 }

extremeWirelessClientAuthInfoLastAuthType OBJECT-TYPE
	SYNTAX INTEGER { open(1), shared(2) }
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the last type of authentication requested by 
	 this client."
	 ::= { extremeWirelessClientAuthInfoEntry 11 }

extremeWirelessClientAuthInfoLastError OBJECT-TYPE
	SYNTAX TimeTicks
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the sysUpTime of the last authentication failure
	 for this client."
	 ::= { extremeWirelessClientAuthInfoEntry 12 }

extremeWirelessClientAuthInfoLastErrorType OBJECT-TYPE
    SYNTAX INTEGER { noError(0),
        resourceFailure(1),
        sequenceNumber(2),
        challengeText(3),
        algorithmMismatch(4),
        keyIndex(5),
        otherError(6) }
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the OID of the last error counter that was 
	 incremented for this client."
	 ::= { extremeWirelessClientAuthInfoEntry 13 }

extremeWirelessClientAuthInfoErrorResourceFailure OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the total number of authentication failures 
	 which have resulted from resource failures."
	 ::= { extremeWirelessClientAuthInfoEntry 14 }

extremeWirelessClientAuthInfoErrorSequenceNum OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the total number of authentication failures 
	 which have resulted from bad packet sequence numbers."
	 ::= { extremeWirelessClientAuthInfoEntry 15 }

extremeWirelessClientAuthInfoErrorChallengeText OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the total number of authentication failures 
	 which have resutled from challenge text mismatch."
	 ::= { extremeWirelessClientAuthInfoEntry 16 }

extremeWirelessClientAuthInfoErrorTypeMismatch OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the total number of authentication failures 
	 which have resutled from the requested authentication
	 type (i.e. open/shared) not matching what this virutal
	 interface is configured for."
	 ::= { extremeWirelessClientAuthInfoEntry 17 }

extremeWirelessClientAuthInfoErrorKeyIndex OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the total number of authentication failures 
	 which have resulted from key index mismatches."
	 ::= { extremeWirelessClientAuthInfoEntry 18 }

extremeWirelessClientAuthInfoErrorOther OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This is the total number of authentication failures 
	 which have resulted from unspecified errors."
	 ::= { extremeWirelessClientAuthInfoEntry 19 }


-- ************************************************************** --
-- Client MAC information : This table contains statistics and     --
-- information on each client which has tried to authenticate with --
-- this virtual interface.
-- ************************************************************** --
extremeWirelessClientMACInfoTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessClientMACInfoEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"This table contains one entry per source MAC which has tried to
	 authenticate with this virtual interface (SSID).  Entries
	 are created when AUTH or REATH REQ packets are received from
	 new clients.  Entries can be aged out, removed by management
	 action, or overwritten by an overflow."
	 ::= { extremeAP 36 }

extremeWirelessClientMACInfoEntry OBJECT-TYPE
	SYNTAX ExtremeWirelessClientMACInfoEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	""
	INDEX { ifIndex, extremeWirelessClientDiagMac }
	 ::= { extremeWirelessClientMACInfoTable 1 }

ExtremeWirelessClientMACInfoEntry ::= SEQUENCE {
	extremeWirelessClientMACInfoMinRSS		INTEGER,
	extremeWirelessClientMACInfoMaxRSS		INTEGER,
	extremeWirelessClientMACInfoAvgRSS		INTEGER,
	extremeWirelessClientMACInfoTotalProbeReq	Unsigned32,
	extremeWirelessClientMACInfoTotalAuthReq	Unsigned32,
	extremeWirelessClientMACInfoTotalAssocReq	Unsigned32,
	extremeWirelessClientMACInfoTotalReAssocReq	Unsigned32,
	extremeWirelessClientMACInfoTotalDeAssocReq	Unsigned32,
	extremeWirelessClientMACInfoTotalDeAuthReq	Unsigned32,
	extremeWirelessClientMACInfoTotalPsPoll		Unsigned32,
	extremeWirelessClientMACInfoTotalData		Unsigned32,
	extremeWirelessClientMACInfoNavValue		Unsigned32
}

extremeWirelessClientMACInfoMinRSS OBJECT-TYPE
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the minimum RSS indication of any packet we have
	 seen from this client.  A value of 0 indicates that RSSI has
	 been unavailable."
	 ::= { extremeWirelessClientMACInfoEntry 1 }

extremeWirelessClientMACInfoMaxRSS OBJECT-TYPE
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the maximum RSS indication of any packet we have
	 seen from this client.  A value of 0 indicates that RSSI has
	 been unavailable."
	 ::= { extremeWirelessClientMACInfoEntry 2 }

extremeWirelessClientMACInfoAvgRSS OBJECT-TYPE
	SYNTAX INTEGER
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the average RSS indication of any packet we have
	 seen from this client.  A value of 0 indicates that RSSI has
	 been unavailable."
	 ::= { extremeWirelessClientMACInfoEntry 3 }

extremeWirelessClientMACInfoTotalProbeReq OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of PROBE REQ packets recieved from
	 this client since the counters have been cleared."
	 ::= { extremeWirelessClientMACInfoEntry 4 }

extremeWirelessClientMACInfoTotalAuthReq OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of AUTH REQ packets recieved from
	 this client since the counters have been cleared."
	 ::= { extremeWirelessClientMACInfoEntry 5 }

extremeWirelessClientMACInfoTotalAssocReq OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of ASSOC REQ packets recieved from
	 this client since the counters have been cleared."
	 ::= { extremeWirelessClientMACInfoEntry 6 }

extremeWirelessClientMACInfoTotalReAssocReq OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of REASSOC REQ packets recieved from
	 this client since the counters have been cleared."
	 ::= { extremeWirelessClientMACInfoEntry 7 }

extremeWirelessClientMACInfoTotalDeAssocReq OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of DEASSOC REQ packets recieved from
	 this client since the counters have been cleared."
	 ::= { extremeWirelessClientMACInfoEntry 8 }

extremeWirelessClientMACInfoTotalDeAuthReq OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of DEAUTH REQ packets recieved from
	 this client since the counters have been cleared."
	 ::= { extremeWirelessClientMACInfoEntry 9 }

extremeWirelessClientMACInfoTotalPsPoll OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of PS POLL packets recieved from
	 this client since the counters have been cleared."
	 ::= { extremeWirelessClientMACInfoEntry 10 }

extremeWirelessClientMACInfoTotalData OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of data frames received from this
	 client since the counters have been cleared."
	 ::= { extremeWirelessClientMACInfoEntry 11 }

extremeWirelessClientMACInfoNavValue OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"TODO: Is this an average, total, what?"
	 ::= { extremeWirelessClientMACInfoEntry 12 }


-- ************************************************************** --
-- Size Based Counters : This table gives per-client histogram     --
-- counters based on the size of received packets/fragments.       --
-- ************************************************************** --
extremeWirelessClientSizeCounterTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessClientSizeCounterEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"There is one entry in this table for each client which has
	 tried to authenticate with this virtual interface.  A new 
	 entry is created when an AUTH or REATH REQ packet is received
	 from a new station.  Entries are removed by management action,
	 timeout or overwritten due to overflow.
	 
	 Entries in this table are also indexed by virtual interface.
	 A client which has tried to authenticate to multiple virtual	
	 interfaces may have more than one entry in this table."
	 ::= { extremeAP 37 }

extremeWirelessClientSizeCounterEntry OBJECT-TYPE
	SYNTAX ExtremeWirelessClientSizeCounterEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	""
	INDEX { ifIndex, extremeWirelessClientDiagMac }
	 ::= { extremeWirelessClientSizeCounterTable 1 }

ExtremeWirelessClientSizeCounterEntry ::= SEQUENCE {
	extremeWirelessClientFrameSizeReXmit64		Unsigned32,
	extremeWirelessClientFrameSizeReXmit128		Unsigned32,
	extremeWirelessClientFrameSizeReXmit256		Unsigned32,
	extremeWirelessClientFrameSizeReXmit512		Unsigned32,
	extremeWirelessClientFrameSizeReXmit1024	Unsigned32,
	extremeWirelessClientFrameSizeReXmit2048	Unsigned32,
	extremeWirelessClientFrameSizeTX64		Unsigned32,
	extremeWirelessClientFrameSizeTX128		Unsigned32,
	extremeWirelessClientFrameSizeTX256		Unsigned32,
	extremeWirelessClientFrameSizeTX512		Unsigned32,
	extremeWirelessClientFrameSizeTX1024		Unsigned32,
	extremeWirelessClientFrameSizeTX2048		Unsigned32,
	extremeWirelessClientFrameSizeRX64		Unsigned32,
	extremeWirelessClientFrameSizeRX128		Unsigned32,
	extremeWirelessClientFrameSizeRX256		Unsigned32,
	extremeWirelessClientFrameSizeRX512		Unsigned32,
	extremeWirelessClientFrameSizeRX1024		Unsigned32,
	extremeWirelessClientFrameSizeRX2048		Unsigned32,
	extremeWirelessClientFrameSizeErrorTX64		Unsigned32,
	extremeWirelessClientFrameSizeErrorTX128	Unsigned32,
	extremeWirelessClientFrameSizeErrorTX256	Unsigned32,
	extremeWirelessClientFrameSizeErrorTX512	Unsigned32,
	extremeWirelessClientFrameSizeErrorTX1024	Unsigned32,
	extremeWirelessClientFrameSizeErrorTX2048	Unsigned32,
	extremeWirelessClientFrameSizeErrorRX64		Unsigned32,
	extremeWirelessClientFrameSizeErrorRX128	Unsigned32,
	extremeWirelessClientFrameSizeErrorRX256	Unsigned32,
	extremeWirelessClientFrameSizeErrorRX512	Unsigned32,
	extremeWirelessClientFrameSizeErrorRX1024	Unsigned32,
	extremeWirelessClientFrameSizeErrorRX2048	Unsigned32,
	extremeWirelessClientPacketSizeTX64		Unsigned32,
	extremeWirelessClientPacketSizeTX128		Unsigned32,
	extremeWirelessClientPacketSizeTX256		Unsigned32,
	extremeWirelessClientPacketSizeTX512		Unsigned32,
	extremeWirelessClientPacketSizeTX1024		Unsigned32,
	extremeWirelessClientPacketSizeTX2048		Unsigned32,
	extremeWirelessClientPacketSizeRX64		Unsigned32,
	extremeWirelessClientPacketSizeRX128		Unsigned32,
	extremeWirelessClientPacketSizeRX256		Unsigned32,
	extremeWirelessClientPacketSizeRX512		Unsigned32,
	extremeWirelessClientPacketSizeRX1024		Unsigned32,
	extremeWirelessClientPacketSizeRX2048		Unsigned32
}

extremeWirelessClientFrameSizeReXmit64 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags retransmitted to this
	 client which were less than or equal to 64 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 1 }

extremeWirelessClientFrameSizeReXmit128 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags retransmitted to this
	 client which were between 64 and 128 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 2 }

extremeWirelessClientFrameSizeReXmit256 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags retransmitted to this
	 client which were between 128 and 256 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 3 }

extremeWirelessClientFrameSizeReXmit512 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags retransmitted to this
	 client which were between 256 and 512 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 4 }

extremeWirelessClientFrameSizeReXmit1024 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags retransmitted to this
	 client which were between 512 and 1024 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 5 }

extremeWirelessClientFrameSizeReXmit2048 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags retransmitted to this
	 client which were between 1024 and 2048 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 6 }

extremeWirelessClientFrameSizeTX64 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags transmitted to this
	 client which were less than or equal to 64 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 7 }

extremeWirelessClientFrameSizeTX128 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags transmitted to this
	 client which were between 64 and 128 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 8 }

extremeWirelessClientFrameSizeTX256 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags transmitted to this
	 client which were between 128 and 256 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 9 }

extremeWirelessClientFrameSizeTX512 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags transmitted to this
	 client which were between 256 and 512 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 10 }

extremeWirelessClientFrameSizeTX1024 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags transmitted to this
	 client which were between 512 and 1024 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 11 }

extremeWirelessClientFrameSizeTX2048 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags transmitted to this
	 client which were between 1024 and 2048 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 12 }

extremeWirelessClientFrameSizeRX64 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags received from this
	 client which were less than or equal to 64 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 13 }

extremeWirelessClientFrameSizeRX128 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags received from this
	 client which were between 64 and 128 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 14 }

extremeWirelessClientFrameSizeRX256 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags received from this
	 client which were between 128 and 256 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 15 }

extremeWirelessClientFrameSizeRX512 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags received from this
	 client which were between 256 and 512 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 16 }

extremeWirelessClientFrameSizeRX1024 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags received from this
	 client which were between 512 and 1024 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 17 }

extremeWirelessClientFrameSizeRX2048 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags received from this
	 client which were between 1024 and 2048 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 18 }

extremeWirelessClientFrameSizeErrorTX64 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which failed to be sent from
	 this client with a length between 0 and 64 bytes."
	 ::= { extremeWirelessClientSizeCounterEntry 19 }

extremeWirelessClientFrameSizeErrorTX128 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which failed to be sent from
	 this client with a length between 65 and 128 bytes."
	 ::= { extremeWirelessClientSizeCounterEntry 20 }

extremeWirelessClientFrameSizeErrorTX256 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which failed to be sent from
	 this client with a length between 129 and 256 bytes."
	 ::= { extremeWirelessClientSizeCounterEntry 21 }

extremeWirelessClientFrameSizeErrorTX512 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which failed to be sent from
	 this client with a length between 257 and 512 bytes."
	 ::= { extremeWirelessClientSizeCounterEntry 22 }

extremeWirelessClientFrameSizeErrorTX1024 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which failed to be sent from
	 this client with a length between 513 and 1024 bytes."
	 ::= { extremeWirelessClientSizeCounterEntry 23 }

extremeWirelessClientFrameSizeErrorTX2048 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which failed to be sent from
	 this client with a length between 1025 and 2048 bytes."
	 ::= { extremeWirelessClientSizeCounterEntry 24 }

extremeWirelessClientFrameSizeErrorRX64 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were received with
	 an FCS or other error and a length between 0 and 64 bytes."
	 ::= { extremeWirelessClientSizeCounterEntry 25 }

extremeWirelessClientFrameSizeErrorRX128 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were received with
	 an FCS or other error and a length between 65 and 128 bytes."
	 ::= { extremeWirelessClientSizeCounterEntry 26 }

extremeWirelessClientFrameSizeErrorRX256 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were received with
	 an FCS or other error and a length between 129 and 256 bytes."
	 ::= { extremeWirelessClientSizeCounterEntry 27 }

extremeWirelessClientFrameSizeErrorRX512 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were received with
	 an FCS or other error and a length between 257 and 512 bytes."
	 ::= { extremeWirelessClientSizeCounterEntry 28 }

extremeWirelessClientFrameSizeErrorRX1024 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were received with
	 an FCS or other error and a length between 513 and 1024 bytes."
	 ::= { extremeWirelessClientSizeCounterEntry 29 }

extremeWirelessClientFrameSizeErrorRX2048 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were received with
	 an FCS or other error and a length between 1025 and 2048 bytes."
	 ::= { extremeWirelessClientSizeCounterEntry 30 }

extremeWirelessClientPacketSizeTX64 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of packets transmitted to this
	 client which were less than or equal to 64 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 31 }

extremeWirelessClientPacketSizeTX128 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of packets transmitted to this
	 client which were between 64 and 128 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 32 }

extremeWirelessClientPacketSizeTX256 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of packets transmitted to this
	 client which were between 128 and 256 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 33 }

extremeWirelessClientPacketSizeTX512 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of packets transmitted to this
	 client which were between 256 and 512 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 34 }

extremeWirelessClientPacketSizeTX1024 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of packets transmitted to this
	 client which were between 512 and 1024 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 35 }

extremeWirelessClientPacketSizeTX2048 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of packets transmitted to this
	 client which were between 1024 and 2048 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 36 }

extremeWirelessClientPacketSizeRX64 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of packets received from this
	 client which were less than or equal to 64 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 37 }

extremeWirelessClientPacketSizeRX128 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of packets received from this
	 client which were between 64 and 128 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 38 }

extremeWirelessClientPacketSizeRX256 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of packets received from this
	 client which were between 128 and 256 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 39 }

extremeWirelessClientPacketSizeRX512 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of packets received from this
	 client which were between 256 and 512 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 40 }

extremeWirelessClientPacketSizeRX1024 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of packets received from this
	 client which were between 512 and 1024 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 41 }

extremeWirelessClientPacketSizeRX2048 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of packets received from this
	 client which were between 1024 and 2048 bytes in length."
	 ::= { extremeWirelessClientSizeCounterEntry 42 }

-- ************************************************************** --
-- Per Client Speed : This table gives a histogram of statistics   --
-- based on the speed of transmission/reception of packets on a    --
-- virtual interface.                                              --
-- ************************************************************** --
extremeWirelessClientSpeedCounterTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessClientSpeedCounterEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"This table is indexed by wireless interface index.  These
	 are the virtual interfaces corresponding to the SSID.  Support
	 for this table is optional, indicated by the value of the variable
	 extremeWirelessClientDiagSupportsSpeedCounters in the status table."
	 ::= { extremeAP 38 }

extremeWirelessClientSpeedCounterEntry OBJECT-TYPE
	SYNTAX ExtremeWirelessClientSpeedCounterEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"The ifIndex here is the wireless interface (SSID).  It is expected
	 that an entry will be created in this table only after a client
	 sends a AUTH or REATH packet to the SSID."
	INDEX { ifIndex, extremeWirelessClientDiagMac }
	 ::= { extremeWirelessClientSpeedCounterTable 1 }

ExtremeWirelessClientSpeedCounterEntry ::= SEQUENCE {
	extremeWirelessClientSpeedReXmit1	Unsigned32,
	extremeWirelessClientSpeedReXmit2	Unsigned32,
	extremeWirelessClientSpeedReXmit5p5	Unsigned32,
	extremeWirelessClientSpeedReXmit6	Unsigned32,
	extremeWirelessClientSpeedReXmit9	Unsigned32,
	extremeWirelessClientSpeedReXmit12	Unsigned32,
	extremeWirelessClientSpeedReXmit18	Unsigned32,
	extremeWirelessClientSpeedReXmit24	Unsigned32,
	extremeWirelessClientSpeedReXmit36	Unsigned32,
	extremeWirelessClientSpeedReXmit48	Unsigned32,
	extremeWirelessClientSpeedReXmit54	Unsigned32,
	extremeWirelessClientSpeedTX1		Unsigned32,
	extremeWirelessClientSpeedTX2		Unsigned32,
	extremeWirelessClientSpeedTX5p5		Unsigned32,
	extremeWirelessClientSpeedTX6		Unsigned32,
	extremeWirelessClientSpeedTX9		Unsigned32,
	extremeWirelessClientSpeedTX12		Unsigned32,
	extremeWirelessClientSpeedTX18		Unsigned32,
	extremeWirelessClientSpeedTX24		Unsigned32,
	extremeWirelessClientSpeedTX36		Unsigned32,
	extremeWirelessClientSpeedTX48		Unsigned32,
	extremeWirelessClientSpeedTX54		Unsigned32,
	extremeWirelessClientSpeedRX1		Unsigned32,
	extremeWirelessClientSpeedRX2		Unsigned32,
	extremeWirelessClientSpeedRX5p5		Unsigned32,
	extremeWirelessClientSpeedRX6		Unsigned32,
	extremeWirelessClientSpeedRX9		Unsigned32,
	extremeWirelessClientSpeedRX12		Unsigned32,
	extremeWirelessClientSpeedRX18		Unsigned32,
	extremeWirelessClientSpeedRX24		Unsigned32,
	extremeWirelessClientSpeedRX36		Unsigned32,
	extremeWirelessClientSpeedRX48		Unsigned32,
	extremeWirelessClientSpeedRX54		Unsigned32
}

extremeWirelessClientSpeedReXmit1	OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were retransmitted to
	 the given client at 1 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 1 }

extremeWirelessClientSpeedReXmit2	OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were retransmitted to
	 the given client at 2 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 2 }

extremeWirelessClientSpeedReXmit5p5 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were retransmitted to
	 the given client at 5 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 3 }

extremeWirelessClientSpeedReXmit6 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were retransmitted to
	 the given client at 6 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 4 }

extremeWirelessClientSpeedReXmit9 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were retransmitted to
	 the given client at 9 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 5 }

extremeWirelessClientSpeedReXmit12 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were retransmitted to
	 the given client at 12 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 6 }

extremeWirelessClientSpeedReXmit18 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were retransmitted to
	 the given client at 18 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 7 }

extremeWirelessClientSpeedReXmit24 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were retransmitted to
	 the given client at 24 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 8 }
	
extremeWirelessClientSpeedReXmit36 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were retransmitted to
	 the given client at 36 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 9 }

extremeWirelessClientSpeedReXmit48 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were retransmitted to
	 the given client at 48 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 10 }

extremeWirelessClientSpeedReXmit54 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were retransmitted to
	 the given client at 54 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 11 }

extremeWirelessClientSpeedTX1	OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were transmitted to
	 the given client at 1 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 12 }

extremeWirelessClientSpeedTX2	OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were transmitted to
	 the given client at 2 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 13 }

extremeWirelessClientSpeedTX5p5 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were transmitted to
	 the given client at 5 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 14 }

extremeWirelessClientSpeedTX6 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were transmitted to
	 the given client at 6 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 15 }

extremeWirelessClientSpeedTX9 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were transmitted to
	 the given client at 9 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 16 }

extremeWirelessClientSpeedTX12 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were transmitted to
	 the given client at 12 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 17 }

extremeWirelessClientSpeedTX18 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were transmitted to
	 the given client at 18 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 18 }

extremeWirelessClientSpeedTX24 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were transmitted to
	 the given client at 24 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 19 }
	
extremeWirelessClientSpeedTX36 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were transmitted to
	 the given client at 36 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 20 }

extremeWirelessClientSpeedTX48 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were transmitted to
	 the given client at 48 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 21 }

extremeWirelessClientSpeedTX54 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were transmitted to
	 the given client at 54 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 22 }

extremeWirelessClientSpeedRX1	OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were received from
	 the given client at 1 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 23 }

extremeWirelessClientSpeedRX2	OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were received from
	 the given client at 2 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 24 }

extremeWirelessClientSpeedRX5p5 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were received from
	 the given client at 5 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 25 }

extremeWirelessClientSpeedRX6 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were received from
	 the given client at 6 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 26 }

extremeWirelessClientSpeedRX9 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were received from
	 the given client at 9 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 27 }

extremeWirelessClientSpeedRX12 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were received from
	 the given client at 12 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 28 }

extremeWirelessClientSpeedRX18 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were received from
	 the given client at 18 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 29 }

extremeWirelessClientSpeedRX24 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were received from
	 the given client at 24 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 30 }
	
extremeWirelessClientSpeedRX36 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were received from
	 the given client at 36 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 31 }

extremeWirelessClientSpeedRX48 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were received from
	 the given client at 48 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 32 }

extremeWirelessClientSpeedRX54 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frags which were received from
	 the given client at 54 Mbps."
	::= { extremeWirelessClientSpeedCounterEntry 33 }

-- ************************************************************** --
-- Frame Size Table : This table presents a historgram of frames   --
--                    based on type and size.                      --
-- ************************************************************** --
extremeWirelessIntfFrameSizeTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessIntfFrameSizeEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"There is one entry in this table for each virtual and
	 physical interface.  Values for physical interfaces are
	 summations of the values for the constituent virtual 
	 interfaces."
	 ::= { extremeAP 39 }

extremeWirelessIntfFrameSizeEntry OBJECT-TYPE
	SYNTAX ExtremeWirelessIntfFrameSizeEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	""
	INDEX { ifIndex }
	 ::= { extremeWirelessIntfFrameSizeTable 1 }
ExtremeWirelessIntfFrameSizeEntry ::= SEQUENCE {
	extremeWirelessIntfFrameSizeMgmtTX64	Unsigned32,
	extremeWirelessIntfFrameSizeMgmtTX128	Unsigned32,
	extremeWirelessIntfFrameSizeMgmtTX256	Unsigned32,
	extremeWirelessIntfFrameSizeMgmtTX512	Unsigned32,
	extremeWirelessIntfFrameSizeMgmtTX1024	Unsigned32,
	extremeWirelessIntfFrameSizeMgmtTX2048	Unsigned32,
	extremeWirelessIntfFrameSizeMgmtRX64	Unsigned32,
	extremeWirelessIntfFrameSizeMgmtRX128	Unsigned32,
	extremeWirelessIntfFrameSizeMgmtRX256	Unsigned32,
	extremeWirelessIntfFrameSizeMgmtRX512	Unsigned32,
	extremeWirelessIntfFrameSizeMgmtRX1024	Unsigned32,
	extremeWirelessIntfFrameSizeMgmtRX2048	Unsigned32,
	extremeWirelessIntfFrameSizeCtlTX64	Unsigned32,
	extremeWirelessIntfFrameSizeCtlTX128	Unsigned32,
	extremeWirelessIntfFrameSizeCtlTX256	Unsigned32,
	extremeWirelessIntfFrameSizeCtlTX512	Unsigned32,
	extremeWirelessIntfFrameSizeCtlTX1024	Unsigned32,
	extremeWirelessIntfFrameSizeCtlTX2048	Unsigned32,
	extremeWirelessIntfFrameSizeCtlRX64	Unsigned32,
	extremeWirelessIntfFrameSizeCtlRX128	Unsigned32,
	extremeWirelessIntfFrameSizeCtlRX256	Unsigned32,
	extremeWirelessIntfFrameSizeCtlRX512	Unsigned32,
	extremeWirelessIntfFrameSizeCtlRX1024	Unsigned32,
	extremeWirelessIntfFrameSizeCtlRX2048	Unsigned32,
	extremeWirelessIntfFrameSizeDataTX64	Unsigned32,
	extremeWirelessIntfFrameSizeDataTX128	Unsigned32,
	extremeWirelessIntfFrameSizeDataTX256	Unsigned32,
	extremeWirelessIntfFrameSizeDataTX512	Unsigned32,
	extremeWirelessIntfFrameSizeDataTX1024	Unsigned32,
	extremeWirelessIntfFrameSizeDataTX2048	Unsigned32,
	extremeWirelessIntfFrameSizeDataRX64	Unsigned32,
	extremeWirelessIntfFrameSizeDataRX128	Unsigned32,
	extremeWirelessIntfFrameSizeDataRX256	Unsigned32,
	extremeWirelessIntfFrameSizeDataRX512	Unsigned32,
	extremeWirelessIntfFrameSizeDataRX1024	Unsigned32,
	extremeWirelessIntfFrameSizeDataRX2048	Unsigned32 }

extremeWirelessIntfFrameSizeMgmtTX64 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of management-type frames transmitted 
	 on this interface which were less than or equal to 64 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 1 }

extremeWirelessIntfFrameSizeMgmtTX128 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of management-type frames transmitted 
	 on this interface which were between 65 and 128 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 2 }

extremeWirelessIntfFrameSizeMgmtTX256 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of management-type frames transmitted 
	 on this interface which were between 129 and 256 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 3 }

extremeWirelessIntfFrameSizeMgmtTX512 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of management-type frames transmitted 
	 on this interface which were between 257 and 512 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 4 }

extremeWirelessIntfFrameSizeMgmtTX1024 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of management-type frames transmitted 
	 on this interface which were between 513 and 1024 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 5 }

extremeWirelessIntfFrameSizeMgmtTX2048 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of management-type frames transmitted 
	 on this interface which were between 1025 and 2048 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 6 }

extremeWirelessIntfFrameSizeMgmtRX64 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of management-type frames received 
	 on this interface which were less than or equal to 64 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 7 }

extremeWirelessIntfFrameSizeMgmtRX128 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of management-type frames received 
	 on this interface which were between 65 and 128 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 8 }

extremeWirelessIntfFrameSizeMgmtRX256 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of management-type frames received 
	 on this interface which were between 129 and 256 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 9 }

extremeWirelessIntfFrameSizeMgmtRX512 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of management-type frames received 
	 on this interface which were between 257 and 512 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 10 }

extremeWirelessIntfFrameSizeMgmtRX1024 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of management-type frames received 
	 on this interface which were between 513 and 1024 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 11 }

extremeWirelessIntfFrameSizeMgmtRX2048 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of management-type frames received 
	 on this interface which were between 1025 and 2048 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 12 }

extremeWirelessIntfFrameSizeCtlTX64 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of control-type frames transmitted 
	 on this interface which were less than or equal to 64 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 13 }

extremeWirelessIntfFrameSizeCtlTX128 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of control-type frames transmitted 
	 on this interface which were between 65 and 128 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 14 }

extremeWirelessIntfFrameSizeCtlTX256 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of control-type frames transmitted 
	 on this interface which were between 129 and 256 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 15 }

extremeWirelessIntfFrameSizeCtlTX512 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of control-type frames transmitted 
	 on this interface which were between 257 and 512 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 16 }

extremeWirelessIntfFrameSizeCtlTX1024 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of control-type frames transmitted 
	 on this interface which were between 513 and 1024 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 17 }

extremeWirelessIntfFrameSizeCtlTX2048 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of control-type frames transmitted 
	 on this interface which were between 1025 and 2048 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 18 }

extremeWirelessIntfFrameSizeCtlRX64 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of control-type frames received 
	 on this interface which were less than or equal to 64 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 19 }

extremeWirelessIntfFrameSizeCtlRX128 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of control-type frames received 
	 on this interface which were between 65 and 128 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 20 }

extremeWirelessIntfFrameSizeCtlRX256 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of control-type frames received 
	 on this interface which were between 129 and 256 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 21 }

extremeWirelessIntfFrameSizeCtlRX512 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of control-type frames received 
	 on this interface which were between 257 and 512 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 22 }

extremeWirelessIntfFrameSizeCtlRX1024 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of control-type frames received 
	 on this interface which were between 513 and 1024 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 23 }

extremeWirelessIntfFrameSizeCtlRX2048 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of control-type frames received 
	 on this interface which were between 1025 and 2048 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 24 }

extremeWirelessIntfFrameSizeDataTX64 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of data-type frames transmitted 
	 on this interface which were less than or equal to 64 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 25 }

extremeWirelessIntfFrameSizeDataTX128 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of data-type frames transmitted 
	 on this interface which were between 65 and 128 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 26 }

extremeWirelessIntfFrameSizeDataTX256 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of data-type frames transmitted 
	 on this interface which were between 129 and 256 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 27 }

extremeWirelessIntfFrameSizeDataTX512 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of data-type frames transmitted 
	 on this interface which were between 257 and 512 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 28 }

extremeWirelessIntfFrameSizeDataTX1024 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of data-type frames transmitted 
	 on this interface which were between 513 and 1024 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 29 }

extremeWirelessIntfFrameSizeDataTX2048 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of data-type frames transmitted 
	 on this interface which were between 1025 and 2048 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 30 }

extremeWirelessIntfFrameSizeDataRX64 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of data-type frames received 
	 on this interface which were less than or equal to 64 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 31 }

extremeWirelessIntfFrameSizeDataRX128 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of data-type frames received 
	 on this interface which were between 65 and 128 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 32 }

extremeWirelessIntfFrameSizeDataRX256 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of data-type frames received 
	 on this interface which were between 129 and 256 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 33 }

extremeWirelessIntfFrameSizeDataRX512 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of data-type frames received 
	 on this interface which were between 257 and 512 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 34 }

extremeWirelessIntfFrameSizeDataRX1024 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of data-type frames received 
	 on this interface which were between 513 and 1024 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 35 }

extremeWirelessIntfFrameSizeDataRX2048 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of data-type frames received 
	 on this interface which were between 1025 and 2048 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeEntry 36 }

-- ************************************************************** --
-- Frame errors by size.                                           --
-- ************************************************************** --
extremeWirelessIntfFrameSizeErrorTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessIntfFrameSizeErrorEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"There is one entry in this table for each virtual and
	 physical interface.  Values for physical interfaces are
	 summations of the values for the constituent virtual 
	 interfaces."
	 ::= { extremeAP 40 }

extremeWirelessIntfFrameSizeErrorEntry OBJECT-TYPE
	SYNTAX ExtremeWirelessIntfFrameSizeErrorEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	""
	INDEX { ifIndex }
	 ::= { extremeWirelessIntfFrameSizeErrorTable 1 }


ExtremeWirelessIntfFrameSizeErrorEntry ::= SEQUENCE {
	extremeWirelessIntfFrameSizeReXmit64	Unsigned32,
	extremeWirelessIntfFrameSizeReXmit128	Unsigned32,
	extremeWirelessIntfFrameSizeReXmit256	Unsigned32,
	extremeWirelessIntfFrameSizeReXmit512	Unsigned32,
	extremeWirelessIntfFrameSizeReXmit1024	Unsigned32,
	extremeWirelessIntfFrameSizeReXmit2048	Unsigned32,
	extremeWirelessIntfFrameSizeErrorTX64	Unsigned32,
	extremeWirelessIntfFrameSizeErrorTX128	Unsigned32,
	extremeWirelessIntfFrameSizeErrorTX256	Unsigned32,
	extremeWirelessIntfFrameSizeErrorTX512	Unsigned32,
	extremeWirelessIntfFrameSizeErrorTX1024	Unsigned32,
	extremeWirelessIntfFrameSizeErrorTX2048	Unsigned32,
	extremeWirelessIntfFrameSizeErrorRX64	Unsigned32,
	extremeWirelessIntfFrameSizeErrorRX128	Unsigned32,
	extremeWirelessIntfFrameSizeErrorRX256	Unsigned32,
	extremeWirelessIntfFrameSizeErrorRX512	Unsigned32,
	extremeWirelessIntfFrameSizeErrorRX1024	Unsigned32,
	extremeWirelessIntfFrameSizeErrorRX2048	Unsigned32 }

extremeWirelessIntfFrameSizeReXmit64 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames retransmitted on this 
	 interface which were less than or equal to 64 bytes
	 in length."
	 ::= { extremeWirelessIntfFrameSizeErrorEntry 1 }

extremeWirelessIntfFrameSizeReXmit128 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames retransmitted on this 
	 interface which were between 65 and 128 bytes in length."
	 ::= { extremeWirelessIntfFrameSizeErrorEntry 2 }

extremeWirelessIntfFrameSizeReXmit256 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames retransmitted on this 
	 interface which were between 129 and 256 bytes in length."
	 ::= { extremeWirelessIntfFrameSizeErrorEntry 3 }

extremeWirelessIntfFrameSizeReXmit512 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames retransmitted on this 
	 interface which were between 257 and 512 bytes in length."
	 ::= { extremeWirelessIntfFrameSizeErrorEntry 4 }

extremeWirelessIntfFrameSizeReXmit1024 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames retransmitted on this 
	 interface which were between 513 and 1024 bytes in length."
	 ::= { extremeWirelessIntfFrameSizeErrorEntry 5 }

extremeWirelessIntfFrameSizeReXmit2048 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames retransmitted on this 
	 interface which were between 1025 and 2048 bytes in length."
	 ::= { extremeWirelessIntfFrameSizeErrorEntry 6 }

extremeWirelessIntfFrameSizeErrorTX64 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which failed to be 
	 transmitted interface which were less than or equal 
	 to 64 bytes in length."
	 ::= { extremeWirelessIntfFrameSizeErrorEntry 7 }

extremeWirelessIntfFrameSizeErrorTX128 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which failed to be 
	 transmitted interface which were between 65 and 128
	 bytes in length."
	 ::= { extremeWirelessIntfFrameSizeErrorEntry 8 }

extremeWirelessIntfFrameSizeErrorTX256 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which failed to be 
	 transmitted interface which were between 129 and 256
	 bytes in length."
	 ::= { extremeWirelessIntfFrameSizeErrorEntry 9 }

extremeWirelessIntfFrameSizeErrorTX512 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which failed to be 
	 transmitted interface which were between 257 and 512
	 bytes in length."
	 ::= { extremeWirelessIntfFrameSizeErrorEntry 10 }

extremeWirelessIntfFrameSizeErrorTX1024 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which failed to be 
	 transmitted interface which were between 513 and 1024
	 bytes in length."
	 ::= { extremeWirelessIntfFrameSizeErrorEntry 11 }

extremeWirelessIntfFrameSizeErrorTX2048 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which failed to be 
	 transmitted interface which were between 1025 and 2048
	 bytes in length."
	 ::= { extremeWirelessIntfFrameSizeErrorEntry 12 }

extremeWirelessIntfFrameSizeErrorRX64 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which had errors on
	 receive on this interface which were less than or equal 
	 to 64 bytes in length."
	 ::= { extremeWirelessIntfFrameSizeErrorEntry 13 }

extremeWirelessIntfFrameSizeErrorRX128 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which had errors on
	 receive on this interface which were between 65 and
	 128 bytes in length."
	 ::= { extremeWirelessIntfFrameSizeErrorEntry 14 }

extremeWirelessIntfFrameSizeErrorRX256 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which had errors on
	 receive on this interface which were between 129 and
	 256 bytes in length."
	 ::= { extremeWirelessIntfFrameSizeErrorEntry 15 }

extremeWirelessIntfFrameSizeErrorRX512 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which had errors on
	 receive on this interface which were between 257 and
	 512 bytes in length."
	 ::= { extremeWirelessIntfFrameSizeErrorEntry 16 }

extremeWirelessIntfFrameSizeErrorRX1024 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which had errors on
	 receive on this interface which were between 513 and
	 1024 bytes in length."
	 ::= { extremeWirelessIntfFrameSizeErrorEntry 17 }

extremeWirelessIntfFrameSizeErrorRX2048 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which had errors on
	 receive on this interface which were between 1025 and
	 2048 bytes in length."
	 ::= { extremeWirelessIntfFrameSizeErrorEntry 18 }

-- ************************************************************** --
-- TX/RX Histogram based on speed.
-- ************************************************************** --
extremeWirelessIntfFrameSpeedTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessIntfFrameSpeedEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"There is one entry in this table for each virtual and
	 physical interface.  Values for physical interfaces are
	 summations of the values for the constituent virtual 
	 interfaces."
	 ::= { extremeAP 41 }

extremeWirelessIntfFrameSpeedEntry OBJECT-TYPE
	SYNTAX ExtremeWirelessIntfFrameSpeedEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	""
	INDEX { ifIndex }
	 ::= { extremeWirelessIntfFrameSpeedTable 1 }

ExtremeWirelessIntfFrameSpeedEntry ::= SEQUENCE {
	extremeWirelessIntfSpeedMgmtTX1		Unsigned32,
	extremeWirelessIntfSpeedMgmtTX2		Unsigned32,
	extremeWirelessIntfSpeedMgmtTX5p5	Unsigned32,
	extremeWirelessIntfSpeedMgmtTX6		Unsigned32,
	extremeWirelessIntfSpeedMgmtTX9		Unsigned32,
    extremeWirelessIntfSpeedMgmtTX11    Unsigned32,
	extremeWirelessIntfSpeedMgmtTX12	Unsigned32,
	extremeWirelessIntfSpeedMgmtTX18	Unsigned32,
	extremeWirelessIntfSpeedMgmtTX24	Unsigned32,
	extremeWirelessIntfSpeedMgmtTX36	Unsigned32,
	extremeWirelessIntfSpeedMgmtTX48	Unsigned32,
	extremeWirelessIntfSpeedMgmtTX54	Unsigned32,
	extremeWirelessIntfSpeedMgmtRX1		Unsigned32,
	extremeWirelessIntfSpeedMgmtRX2		Unsigned32,
	extremeWirelessIntfSpeedMgmtRX5p5	Unsigned32,
	extremeWirelessIntfSpeedMgmtRX6		Unsigned32,
	extremeWirelessIntfSpeedMgmtRX9		Unsigned32,
	extremeWirelessIntfSpeedMgmtRX11	Unsigned32,
	extremeWirelessIntfSpeedMgmtRX12	Unsigned32,
	extremeWirelessIntfSpeedMgmtRX18	Unsigned32,
	extremeWirelessIntfSpeedMgmtRX24	Unsigned32,
	extremeWirelessIntfSpeedMgmtRX36	Unsigned32,
	extremeWirelessIntfSpeedMgmtRX48	Unsigned32,
	extremeWirelessIntfSpeedMgmtRX54	Unsigned32,
	extremeWirelessIntfSpeedCtlTX1		Unsigned32,
	extremeWirelessIntfSpeedCtlTX2		Unsigned32,
	extremeWirelessIntfSpeedCtlTX5p5	Unsigned32,
	extremeWirelessIntfSpeedCtlTX6		Unsigned32,
	extremeWirelessIntfSpeedCtlTX9		Unsigned32,
    extremeWirelessIntfSpeedCtlTX11     Unsigned32,
	extremeWirelessIntfSpeedCtlTX12		Unsigned32,
	extremeWirelessIntfSpeedCtlTX18		Unsigned32,
	extremeWirelessIntfSpeedCtlTX24		Unsigned32,
	extremeWirelessIntfSpeedCtlTX36		Unsigned32,
	extremeWirelessIntfSpeedCtlTX48		Unsigned32,
	extremeWirelessIntfSpeedCtlTX54		Unsigned32,
	extremeWirelessIntfSpeedCtlRX1		Unsigned32,
	extremeWirelessIntfSpeedCtlRX2		Unsigned32,
	extremeWirelessIntfSpeedCtlRX5p5	Unsigned32,
	extremeWirelessIntfSpeedCtlRX6		Unsigned32,
	extremeWirelessIntfSpeedCtlRX9		Unsigned32,
    extremeWirelessIntfSpeedCtlRX11     Unsigned32,
	extremeWirelessIntfSpeedCtlRX12		Unsigned32,
	extremeWirelessIntfSpeedCtlRX18		Unsigned32,
	extremeWirelessIntfSpeedCtlRX24		Unsigned32,
	extremeWirelessIntfSpeedCtlRX36		Unsigned32,
	extremeWirelessIntfSpeedCtlRX48		Unsigned32,
	extremeWirelessIntfSpeedCtlRX54		Unsigned32,
	extremeWirelessIntfSpeedDataTX1		Unsigned32,
	extremeWirelessIntfSpeedDataTX2		Unsigned32,
	extremeWirelessIntfSpeedDataTX5p5	Unsigned32,
	extremeWirelessIntfSpeedDataTX6		Unsigned32,
	extremeWirelessIntfSpeedDataTX9		Unsigned32,
    extremeWirelessIntfSpeedDataTX11    Unsigned32,
	extremeWirelessIntfSpeedDataTX12	Unsigned32,
	extremeWirelessIntfSpeedDataTX18	Unsigned32,
	extremeWirelessIntfSpeedDataTX24	Unsigned32,
	extremeWirelessIntfSpeedDataTX36	Unsigned32,
	extremeWirelessIntfSpeedDataTX48	Unsigned32,
	extremeWirelessIntfSpeedDataTX54	Unsigned32,
	extremeWirelessIntfSpeedDataRX1		Unsigned32,
	extremeWirelessIntfSpeedDataRX2		Unsigned32,
	extremeWirelessIntfSpeedDataRX5p5	Unsigned32,
	extremeWirelessIntfSpeedDataRX6		Unsigned32,
	extremeWirelessIntfSpeedDataRX9		Unsigned32,
    extremeWirelessIntfSpeedDataRX11    Unsigned32,
	extremeWirelessIntfSpeedDataRX12	Unsigned32,
	extremeWirelessIntfSpeedDataRX18	Unsigned32,
	extremeWirelessIntfSpeedDataRX24	Unsigned32,
	extremeWirelessIntfSpeedDataRX36	Unsigned32,
	extremeWirelessIntfSpeedDataRX48	Unsigned32,
	extremeWirelessIntfSpeedDataRX54	Unsigned32 }

extremeWirelessIntfSpeedMgmtTX1 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of management-type frames transmitted
	 on this interface at 1Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 1 }

extremeWirelessIntfSpeedMgmtTX2 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of management-type frames transmitted
	 on this interface at 2Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 2 }

extremeWirelessIntfSpeedMgmtTX5p5 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of management-type frames transmitted
	 on this interface at 5.5Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 3 }

extremeWirelessIntfSpeedMgmtTX6 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of management-type frames transmitted
	 on this interface at 6Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 4 }

extremeWirelessIntfSpeedMgmtTX9 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of management-type frames transmitted
	 on this interface at 9Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 5 }

extremeWirelessIntfSpeedMgmtTX11 OBJECT-TYPE
     SYNTAX      Unsigned32
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "This gives the number of management-type frames transmitted
     on this interface at 11Mbps."
     ::= { extremeWirelessIntfFrameSpeedEntry 6 }

extremeWirelessIntfSpeedMgmtTX12 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of management-type frames transmitted
	 on this interface at 12Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 7 }

extremeWirelessIntfSpeedMgmtTX18 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of management-type frames transmitted
	 on this interface at 18Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 8 }

extremeWirelessIntfSpeedMgmtTX24 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of management-type frames transmitted
	 on this interface at 24Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 9 }

extremeWirelessIntfSpeedMgmtTX36 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of management-type frames transmitted
	 on this interface at 36Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 10 }

extremeWirelessIntfSpeedMgmtTX48 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of management-type frames transmitted
	 on this interface at 48Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 11 }

extremeWirelessIntfSpeedMgmtTX54 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of management-type frames transmitted
	 on this interface at 54Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 12 }

extremeWirelessIntfSpeedMgmtRX1 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of management-type frames recieved
	 on this interface at 1Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 13 }

extremeWirelessIntfSpeedMgmtRX2 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of management-type frames recieved
	 on this interface at 2Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 14 }

extremeWirelessIntfSpeedMgmtRX5p5 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of management-type frames recieved
	 on this interface at 5.5Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 15 }

extremeWirelessIntfSpeedMgmtRX6 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of management-type frames recieved
	 on this interface at 6Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 16 }

extremeWirelessIntfSpeedMgmtRX9 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of management-type frames recieved
	 on this interface at 9Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 17 }

extremeWirelessIntfSpeedMgmtRX11 OBJECT-TYPE
     SYNTAX      Unsigned32
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "This gives the number of management-type frames recieved
     on this interface at 11Mbps."
     ::= { extremeWirelessIntfFrameSpeedEntry 18 }

extremeWirelessIntfSpeedMgmtRX12 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of management-type frames recieved
	 on this interface at 12Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 19 }

extremeWirelessIntfSpeedMgmtRX18 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of management-type frames recieved
	 on this interface at 18Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 20 }

extremeWirelessIntfSpeedMgmtRX24 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of management-type frames recieved
	 on this interface at 24Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 21 }

extremeWirelessIntfSpeedMgmtRX36 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of management-type frames recieved
	 on this interface at 36Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 22 }

extremeWirelessIntfSpeedMgmtRX48 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of management-type frames recieved
	 on this interface at 48Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 23 }

extremeWirelessIntfSpeedMgmtRX54 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of management-type frames recieved
	 on this interface at 54Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 24 }

extremeWirelessIntfSpeedCtlTX1 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of control-type frames transmitted
	 on this interface at 1Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 25 }

extremeWirelessIntfSpeedCtlTX2 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of control-type frames transmitted
	 on this interface at 2Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 26 }

extremeWirelessIntfSpeedCtlTX5p5 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of control-type frames transmitted
	 on this interface at 5.5Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 27 }

extremeWirelessIntfSpeedCtlTX6 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of control-type frames transmitted
	 on this interface at 6Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 28 }

extremeWirelessIntfSpeedCtlTX9 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of control-type frames transmitted
	 on this interface at 9Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 29 }

extremeWirelessIntfSpeedCtlTX11 OBJECT-TYPE
     SYNTAX      Unsigned32
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "This gives the number of control-type frames transmitted
     on this interface at 11Mbps."
     ::= { extremeWirelessIntfFrameSpeedEntry 30 }

extremeWirelessIntfSpeedCtlTX12 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of control-type frames transmitted
	 on this interface at 12Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 31 }

extremeWirelessIntfSpeedCtlTX18 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of control-type frames transmitted
	 on this interface at 18Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 32 }

extremeWirelessIntfSpeedCtlTX24 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of control-type frames transmitted
	 on this interface at 24Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 33 }

extremeWirelessIntfSpeedCtlTX36 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of control-type frames transmitted
	 on this interface at 36Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 34 }

extremeWirelessIntfSpeedCtlTX48 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of control-type frames transmitted
	 on this interface at 48Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 35 }

extremeWirelessIntfSpeedCtlTX54 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of control-type frames transmitted
	 on this interface at 54Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 36 }

extremeWirelessIntfSpeedCtlRX1 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of control-type frames recieved
	 on this interface at 1Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 37 }

extremeWirelessIntfSpeedCtlRX2 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of control-type frames recieved
	 on this interface at 2Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 38 }

extremeWirelessIntfSpeedCtlRX5p5 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of control-type frames recieved
	 on this interface at 5.5Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 39 }

extremeWirelessIntfSpeedCtlRX6 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of control-type frames recieved
	 on this interface at 6Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 40 }

extremeWirelessIntfSpeedCtlRX9 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of control-type frames recieved
	 on this interface at 9Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 41 }

extremeWirelessIntfSpeedCtlRX11 OBJECT-TYPE
     SYNTAX      Unsigned32
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "This gives the number of control-type frames recieved
     on this interface at 11Mbps."
     ::= { extremeWirelessIntfFrameSpeedEntry 42 }


extremeWirelessIntfSpeedCtlRX12 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of control-type frames recieved
	 on this interface at 12Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 43 }

extremeWirelessIntfSpeedCtlRX18 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of control-type frames recieved
	 on this interface at 18Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 44 }

extremeWirelessIntfSpeedCtlRX24 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of control-type frames recieved
	 on this interface at 24Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 45 }

extremeWirelessIntfSpeedCtlRX36 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of control-type frames recieved
	 on this interface at 36Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 46 }

extremeWirelessIntfSpeedCtlRX48 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of control-type frames recieved
	 on this interface at 48Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 47 }

extremeWirelessIntfSpeedCtlRX54 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of control-type frames recieved
	 on this interface at 54Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 48 }

extremeWirelessIntfSpeedDataTX1 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of data-type frames transmitted
	 on this interface at 1Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 49 }

extremeWirelessIntfSpeedDataTX2 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of data-type frames transmitted
	 on this interface at 2Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 50 }

extremeWirelessIntfSpeedDataTX5p5 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of data-type frames transmitted
	 on this interface at 5.5Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 51 }

extremeWirelessIntfSpeedDataTX6 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of data-type frames transmitted
	 on this interface at 6Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 52 }

extremeWirelessIntfSpeedDataTX9 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of data-type frames transmitted
	 on this interface at 9Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 53 }

extremeWirelessIntfSpeedDataTX11 OBJECT-TYPE
     SYNTAX      Unsigned32
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "This gives the number of data-type frames transmitted
     on this interface at 11Mbps."
     ::= { extremeWirelessIntfFrameSpeedEntry 54 }

extremeWirelessIntfSpeedDataTX12 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of data-type frames transmitted
	 on this interface at 12Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 55 }

extremeWirelessIntfSpeedDataTX18 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of data-type frames transmitted
	 on this interface at 18Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 56 }

extremeWirelessIntfSpeedDataTX24 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of data-type frames transmitted
	 on this interface at 24Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 57 }

extremeWirelessIntfSpeedDataTX36 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of data-type frames transmitted
	 on this interface at 36Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 58 }

extremeWirelessIntfSpeedDataTX48 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of data-type frames transmitted
	 on this interface at 48Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 59 }

extremeWirelessIntfSpeedDataTX54 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of data-type frames transmitted
	 on this interface at 54Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 60 }

extremeWirelessIntfSpeedDataRX1 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of data-type frames recieved
	 on this interface at 1Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 61 }

extremeWirelessIntfSpeedDataRX2 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of data-type frames recieved
	 on this interface at 2Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 62 }

extremeWirelessIntfSpeedDataRX5p5 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of data-type frames recieved
	 on this interface at 5.5Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 63 }

extremeWirelessIntfSpeedDataRX6 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of data-type frames recieved
	 on this interface at 6Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 64 }

extremeWirelessIntfSpeedDataRX9 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of data-type frames recieved
	 on this interface at 9Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 65 }

extremeWirelessIntfSpeedDataRX11 OBJECT-TYPE
     SYNTAX      Unsigned32
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
     "This gives the number of data-type frames recieved
     on this interface at 11Mbps."
     ::= { extremeWirelessIntfFrameSpeedEntry 66 }

extremeWirelessIntfSpeedDataRX12 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of data-type frames recieved
	 on this interface at 12Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 67 }

extremeWirelessIntfSpeedDataRX18 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of data-type frames recieved
	 on this interface at 18Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 68 }

extremeWirelessIntfSpeedDataRX24 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of data-type frames recieved
	 on this interface at 24Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 69 }

extremeWirelessIntfSpeedDataRX36 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of data-type frames recieved
	 on this interface at 36Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 70 }

extremeWirelessIntfSpeedDataRX48 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of data-type frames recieved
	 on this interface at 48Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 71 }

extremeWirelessIntfSpeedDataRX54 OBJECT-TYPE
	SYNTAX		Unsigned32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This gives the number of data-type frames recieved
	 on this interface at 54Mbps."
	 ::= { extremeWirelessIntfFrameSpeedEntry 72 }

-- ************************************************************** --
-- Error Histograms of retransmission by frame speed.              --
-- ************************************************************** --
extremeWirelessIntfFrameSpeedErrorTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessIntfFrameSpeedErrorEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"There is one entry in this table for each virtual and
	 physical interface.  Values for physical interfaces are
	 summations of the values for the constituent virtual 
	 interfaces."
	 ::= { extremeAP 42 }

extremeWirelessIntfFrameSpeedErrorEntry OBJECT-TYPE
	SYNTAX ExtremeWirelessIntfFrameSpeedErrorEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	""
	INDEX { ifIndex }
	 ::= { extremeWirelessIntfFrameSpeedErrorTable 1 }

ExtremeWirelessIntfFrameSpeedErrorEntry ::= SEQUENCE {
	extremeWirelessIntfSpeedReXmit1		Unsigned32,
	extremeWirelessIntfSpeedReXmit2		Unsigned32,
	extremeWirelessIntfSpeedReXmit5p5	Unsigned32,
	extremeWirelessIntfSpeedReXmit6		Unsigned32,
	extremeWirelessIntfSpeedReXmit9		Unsigned32,
    extremeWirelessIntfSpeedReXmit11    Unsigned32,
	extremeWirelessIntfSpeedReXmit12	Unsigned32,
	extremeWirelessIntfSpeedReXmit18	Unsigned32,
	extremeWirelessIntfSpeedReXmit24	Unsigned32,
	extremeWirelessIntfSpeedReXmit36	Unsigned32,
	extremeWirelessIntfSpeedReXmit48	Unsigned32,
	extremeWirelessIntfSpeedReXmit54	Unsigned32,
    extremeWirelessIntfSpeedErrorTX1    Unsigned32,
    extremeWirelessIntfSpeedErrorTX2    Unsigned32,
    extremeWirelessIntfSpeedErrorTX5p5  Unsigned32,
    extremeWirelessIntfSpeedErrorTX6    Unsigned32,
    extremeWirelessIntfSpeedErrorTX9    Unsigned32,
    extremeWirelessIntfSpeedErrorTX11   Unsigned32,
    extremeWirelessIntfSpeedErrorTX12   Unsigned32,
    extremeWirelessIntfSpeedErrorTX18   Unsigned32,
    extremeWirelessIntfSpeedErrorTX24   Unsigned32,
    extremeWirelessIntfSpeedErrorTX36   Unsigned32,
    extremeWirelessIntfSpeedErrorTX48   Unsigned32,
    extremeWirelessIntfSpeedErrorTX54   Unsigned32,
	extremeWirelessIntfSpeedErrorRX1	Unsigned32,
	extremeWirelessIntfSpeedErrorRX2	Unsigned32,
	extremeWirelessIntfSpeedErrorRX5p5	Unsigned32,
	extremeWirelessIntfSpeedErrorRX6	Unsigned32,
	extremeWirelessIntfSpeedErrorRX9	Unsigned32,
    extremeWirelessIntfSpeedErrorRX11   Unsigned32,
	extremeWirelessIntfSpeedErrorRX12	Unsigned32,
	extremeWirelessIntfSpeedErrorRX18	Unsigned32,
	extremeWirelessIntfSpeedErrorRX24	Unsigned32,
	extremeWirelessIntfSpeedErrorRX36	Unsigned32,
	extremeWirelessIntfSpeedErrorRX48	Unsigned32,
	extremeWirelessIntfSpeedErrorRX54	Unsigned32 }

extremeWirelessIntfSpeedReXmit1	OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which were retransmitted on
	 this interface at 1 Mbps."
	::= { extremeWirelessIntfFrameSpeedErrorEntry 1 }

extremeWirelessIntfSpeedReXmit2	OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which were retransmitted on
	 this interface at 2 Mbps."
	::= { extremeWirelessIntfFrameSpeedErrorEntry 2 }

extremeWirelessIntfSpeedReXmit5p5 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which were retransmitted on
	 this interface at 5 Mbps."
	::= { extremeWirelessIntfFrameSpeedErrorEntry 3 }

extremeWirelessIntfSpeedReXmit6 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which were retransmitted on
	 this interface at 6 Mbps."
	::= { extremeWirelessIntfFrameSpeedErrorEntry 4 }

extremeWirelessIntfSpeedReXmit9 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which were retransmitted on
	 this interface at 9 Mbps."
	::= { extremeWirelessIntfFrameSpeedErrorEntry 5 }

extremeWirelessIntfSpeedReXmit11 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were retransmitted on
    this interface at 11 Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 6 }

extremeWirelessIntfSpeedReXmit12 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which were retransmitted on
	 this interface at 12 Mbps."
	::= { extremeWirelessIntfFrameSpeedErrorEntry 7 }

extremeWirelessIntfSpeedReXmit18 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which were retransmitted on
	 this interface at 18 Mbps."
	::= { extremeWirelessIntfFrameSpeedErrorEntry 8 }

extremeWirelessIntfSpeedReXmit24 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which were retransmitted on
	 this interface at 24 Mbps."
	::= { extremeWirelessIntfFrameSpeedErrorEntry 9 }
	
extremeWirelessIntfSpeedReXmit36 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which were retransmitted on
	 this interface at 36 Mbps."
	::= { extremeWirelessIntfFrameSpeedErrorEntry 10 }

extremeWirelessIntfSpeedReXmit48 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which were retransmitted on
	 this interface at 48 Mbps."
	::= { extremeWirelessIntfFrameSpeedErrorEntry 11 }

extremeWirelessIntfSpeedReXmit54 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which were retransmitted on
	 this interface at 54 Mbps."
	::= { extremeWirelessIntfFrameSpeedErrorEntry 12 }

extremeWirelessIntfSpeedErrorTX1 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were transmited with errors
    on this interface at 1Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 13 }

extremeWirelessIntfSpeedErrorTX2 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were transmited with errors
    on this interface at 2Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 14 }

extremeWirelessIntfSpeedErrorTX5p5 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were transmited with errors
    on this interface at 5.5Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 15 }

extremeWirelessIntfSpeedErrorTX6 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were transmited with errors
    on this interface at 6Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 16 }

extremeWirelessIntfSpeedErrorTX9 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were transmited with errors
    on this interface at 9Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 17 }

extremeWirelessIntfSpeedErrorTX11 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were transmited with errors
    on this interface at 11Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 18 }

extremeWirelessIntfSpeedErrorTX12 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were transmited with errors
    on this interface at 12Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 19 }

extremeWirelessIntfSpeedErrorTX18 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were transmited with errors
    on this interface at 18Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 20 }

extremeWirelessIntfSpeedErrorTX24 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were transmited with errors
    on this interface at 24Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 21 }

extremeWirelessIntfSpeedErrorTX36 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were transmited with errors
    on this interface at 36Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 22 }

extremeWirelessIntfSpeedErrorTX48 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were transmited with errors
    on this interface at 48Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 23 }

extremeWirelessIntfSpeedErrorTX54 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were transmited with errors
    on this interface at 54Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 24 }

extremeWirelessIntfSpeedErrorRX1 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which were received with errors
	 on this interface at 1Mbps."
	::= { extremeWirelessIntfFrameSpeedErrorEntry 25 }

extremeWirelessIntfSpeedErrorRX2 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which were received with errors
	 on this interface at 2Mbps."
	::= { extremeWirelessIntfFrameSpeedErrorEntry 26 }

extremeWirelessIntfSpeedErrorRX5p5 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which were received with errors
	 on this interface at 5.5Mbps."
	::= { extremeWirelessIntfFrameSpeedErrorEntry 27 }

extremeWirelessIntfSpeedErrorRX6 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which were received with errors
	 on this interface at 6Mbps."
	::= { extremeWirelessIntfFrameSpeedErrorEntry 28 }

extremeWirelessIntfSpeedErrorRX9 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which were received with errors
	 on this interface at 9Mbps."
	::= { extremeWirelessIntfFrameSpeedErrorEntry 29 }

extremeWirelessIntfSpeedErrorRX11 OBJECT-TYPE
    SYNTAX Unsigned32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
    "This gives the number of frames which were received with errors
    on this interface at 11Mbps."
    ::= { extremeWirelessIntfFrameSpeedErrorEntry 30 }

extremeWirelessIntfSpeedErrorRX12 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which were received with errors
	 on this interface at 12Mbps."
	::= { extremeWirelessIntfFrameSpeedErrorEntry 31 }

extremeWirelessIntfSpeedErrorRX18 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which were received with errors
	 on this interface at 18Mbps."
	::= { extremeWirelessIntfFrameSpeedErrorEntry 32 }

extremeWirelessIntfSpeedErrorRX24 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which were received with errors
	 on this interface at 24Mbps."
	::= { extremeWirelessIntfFrameSpeedErrorEntry 33 }

extremeWirelessIntfSpeedErrorRX36 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which were received with errors
	 on this interface at 36Mbps."
	::= { extremeWirelessIntfFrameSpeedErrorEntry 34 }

extremeWirelessIntfSpeedErrorRX48 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which were received with errors
	 on this interface at 48Mbps."
	::= { extremeWirelessIntfFrameSpeedErrorEntry 35 }

extremeWirelessIntfSpeedErrorRX54 OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the number of frames which were received with errors
	 on this interface at 54Mbps."
	::= { extremeWirelessIntfFrameSpeedErrorEntry 36 }

-- ************************************************************** --
-- Interface utilization/noise.                                    --
-- ************************************************************** --
extremeWirelessIntfUtilizationTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessIntfUtilizationEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"There is one entry in this table for each virtual and
	 physical interface.  Values for physical interfaces are
	 summations of the values for the constituent virtual 
	 interfaces."
	 ::= { extremeAP 43 }

extremeWirelessIntfUtilizationEntry OBJECT-TYPE
	SYNTAX ExtremeWirelessIntfUtilizationEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	""
	INDEX { ifIndex }
	 ::= { extremeWirelessIntfUtilizationTable 1 }

ExtremeWirelessIntfUtilizationEntry ::= SEQUENCE {
	extremeWirelessIntfUtilizationNav	         Unsigned32,
	extremeWirelessIntfUtilizationNoiseFloor	 Unsigned32 }

extremeWirelessIntfUtilizationNav OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the instantaneous NAV value on this interface, or
	 some increasing-metric of utilization."
	::= { extremeWirelessIntfUtilizationEntry 1 }

extremeWirelessIntfUtilizationNoiseFloor OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the noise floor in dBm for this interface."
	::= { extremeWirelessIntfUtilizationEntry 2 }

-- ************************************************************** --
-- Opaque client MIBs. These mibs are provided as a performance    --
-- gain for the LAC management of the switch.                      --
--                                                                 --
-- Some of the items in this table are encoded as a series of TLVs.--
-- In this case, they are encoded as:                              --
--                                                                 --
--   | Type (8 bits) | length (8 bits) | value (variable) |        --
--                                                                 --
-- type - equal to the index field of the element                  --
--        in the table this value corresponds to.                  --
--                                                                 --
-- length - equal to the length in bytes of the value              --
--                                                                 --
-- value -  this is the value.  Integer value are NBO,             --
--          strings are non-null terminated ASCII.                 --
--                                                                 --
-- ************************************************************** --
extremeWirelessOpaqueTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF ExtremeWirelessOpaqueEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		" "
	::= { extremeAP 99 }

extremeWirelessOpaqueEntry OBJECT-TYPE
	SYNTAX		ExtremeWirelessOpaqueEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		" "
	INDEX { ifIndex }
	::= { extremeWirelessOpaqueTable 1 }

ExtremeWirelessOpaqueEntry ::= SEQUENCE {
	extremeWirelessClientData		OCTET STRING,
	extremeWirelessPAEStatsData		OCTET STRING,
	extremeWirelessPAEDiagData		OCTET STRING,
	extremeWirelessScanResultsData		OCTET STRING,
	extremeWirelessProbeInfoData		OCTET STRING,
	extremeWirelessClientDiagData		OCTET STRING,
	extremeWirelessClientAssocData		OCTET STRING,
	extremeWirelessClientAuthData		OCTET STRING,
	extremeWirelessClientMACInfoData	OCTET STRING,
	extremeWirelessSizeCounterData		OCTET STRING,
	extremeWirelessSpeedCounterData		OCTET STRING }

extremeWirelessClientData OBJECT-TYPE
	SYNTAX		OCTET STRING
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	""
	::= { extremeWirelessOpaqueEntry 1 }	

extremeWirelessPAEStatsData OBJECT-TYPE
	SYNTAX		OCTET STRING
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	""
	::= { extremeWirelessOpaqueEntry 2 }	

extremeWirelessPAEDiagData OBJECT-TYPE
	SYNTAX		OCTET STRING
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	""
	::= { extremeWirelessOpaqueEntry 3 }

extremeWirelessScanResultsData OBJECT-TYPE
	SYNTAX		OCTET STRING
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This is the contents of the scan results table encoded
	 as a series of TLVs."
	::= { extremeWirelessOpaqueEntry 4 }

extremeWirelessProbeInfoData OBJECT-TYPE
	SYNTAX		OCTET STRING
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This is the contents of the probe info table encoded 
	 as a series of TLVs.    Each item is encoded as the
	 entry above."
	::= { extremeWirelessOpaqueEntry 5 }

extremeWirelessClientDiagData OBJECT-TYPE
	SYNTAX		OCTET STRING
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This is the contents of the client diag table encoded 
	 as a series of TLVs.    Each item is encoded as the
	 entry above."
	::= { extremeWirelessOpaqueEntry 6 }

extremeWirelessClientAssocData OBJECT-TYPE
	SYNTAX		OCTET STRING
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This is the contents of the client assoc table encoded 
	 as a series of TLVs.    Each item is encoded as the
	 entry above.  Note that since the MAC address is not a
	 member of the table (it is an index) it will be encoded
	 as type = 0."
	::= { extremeWirelessOpaqueEntry 7 }

extremeWirelessClientAuthData OBJECT-TYPE
	SYNTAX		OCTET STRING
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This is the contents of the client auth table encoded 
	 as a series of TLVs.    Each item is encoded as the
	 entry above.  Note that since the MAC address is not a
	 member of the table (it is an index) it will be encoded
	 as type = 0."
	::= { extremeWirelessOpaqueEntry 8 }

extremeWirelessClientMACInfoData OBJECT-TYPE
	SYNTAX		OCTET STRING
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This is the contents of the client MAC info table 
	 encoded as a series of TLVs.    Each item is encoded 
	 as the entry above.  Note that since the MAC address 
	 is not a member of the table (it is an index) it will 
	 be encoded as type = 0."
	::= { extremeWirelessOpaqueEntry 9 }

extremeWirelessSizeCounterData OBJECT-TYPE
	SYNTAX		OCTET STRING
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This is the contents of the client size counter table
	 encoded as a series of TLVs.    Each item is encoded 
	 as the entry above.  Note that since the MAC address 
	 is not a member of the table (it is an index) it will 
	 be encoded as type = 0."
	::= { extremeWirelessOpaqueEntry 10 }

extremeWirelessSpeedCounterData OBJECT-TYPE
	SYNTAX		OCTET STRING
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This is the contents of the client speed counter table
	 encoded as a series of TLVs.    Each item is encoded 
	 as the entry above.  Note that since the MAC address 
	 is not a member of the table (it is an index) it will 
	 be encoded as type = 0."
	::= { extremeWirelessOpaqueEntry 11 }

-- ************************************************************** --
-- TRACE MIBS                                                      --
--                                                                 --
-- These mibs are provided on a per-wireless port basis to support --
-- configurable tracing.  Each subsystem associated with a         --
-- wireless port has an entry in the trace module table.  These    --
-- entries allow for configuration of the current trace level.     --
-- statistics on each modules tracing output are also kept.  At    --
-- a global level several statistics are available from the trace  --
-- table.                                                          --
-- ************************************************************** --
extremeWirelessTraceTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessTraceTableEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	 "This table contains one entry per wireless port.  This
          allows access to various stastics about the tracing mod  --
          ule on that wireless port."
	::= { extremeAP 100 }

extremeWirelessTraceEntry OBJECT-TYPE
	SYNTAX 		ExtremeWirelessTraceTableEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	""
	INDEX { ifIndex }
	::= { extremeWirelessTraceTable 1 }

ExtremeWirelessTraceTableEntry ::= SEQUENCE {
	extremeWirelessTraceMsgsOut	INTEGER,
	extremeWirelessTraceBytesOut	INTEGER,
	extremeWirelessTraceSuppressed  INTEGER,
	extremeWirelessTraceOtherErr	INTEGER,
	extremeWirelessTraceOpaque	OCTET STRING }

extremeWirelessTraceMsgsOut OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-only
	STATUS 		current
	DESCRIPTION
	"This gives the number of trace messages the system has
	 sent out to the syslog server.  Suppressed messages are
	 not counted toward this total."
	::= { extremeWirelessTraceEntry 1 }

extremeWirelessTraceBytesOut OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This give the number of bytes total sent out by the
	 trace system.  This is a simple sum of the string
	 lengths of all messages sent out."
	::= { extremeWirelessTraceEntry 2 }

extremeWirelessTraceSuppressed OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This variable is incremented whenever a message is
	 not sent out because the trace level of that system
	 is lower than the message level."
	::= { extremeWirelessTraceEntry 3 }

extremeWirelessTraceOtherErr OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This variable is incremented when a message is not 
	 sent out due to internal errors (i.e. out of memory)."
	::= { extremeWirelessTraceEntry 4 }

extremeWirelessTraceOpaque OBJECT-TYPE
	SYNTAX		OCTET STRING
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
	"This is the opaque representation of the module table
	 to optimize retreival."
	::= { extremeWirelessTraceEntry 5 }

extremeWirelessTraceModuleTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessTraceModuleEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	 "This table contains one entry per trace module.  Each entry
	  is indexed by an arbitrary integer value."
	::= { extremeAP 101 }

extremeWirelessTraceModuleEntry OBJECT-TYPE
	SYNTAX ExtremeWirelessTraceModuleEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	""
	INDEX { ifIndex, extremeWirelessTraceModuleId }
	::= { extremeWirelessTraceModuleTable 1 }

ExtremeWirelessTraceModuleEntry ::= SEQUENCE {
	extremeWirelessTraceModuleId	     INTEGER,
	extremeWirelessTraceModuleDesc       DisplayString,
	extremeWirelessTraceModuleHeader     DisplayString,
	extremeWirelessTraceModuleLevel      INTEGER,
	extremeWirelessTraceModuleSuppressed INTEGER,
	extremeWirelessTraceModuleMsgsOut    INTEGER,
	extremeWirelessTraceModuleBytesOut   INTEGER }

extremeWirelessTraceModuleId	     OBJECT-TYPE
	SYNTAX	INTEGER(0..65535)
	MAX-ACCESS not-accessible
	STATUS 	current
	DESCRIPTION
	"This is an arbitrary integer index which is assigned to each
	 trace module."
	::= { extremeWirelessTraceModuleEntry 1 }

extremeWirelessTraceModuleDesc	     OBJECT-TYPE
	SYNTAX	DisplayString
	MAX-ACCESS read-only
	STATUS 	current
	DESCRIPTION
	"This is a string which briefly describes the purpose of this
	 debug trace.  It may include whitespace.  An example is:
		802.1x State Machine"
	::= { extremeWirelessTraceModuleEntry 2 }

extremeWirelessTraceModuleHeader     OBJECT-TYPE
	SYNTAX	DisplayString
	MAX-ACCESS read-only
	STATUS 	current
	DESCRIPTION
	"This is a string which is prepended to the syslog messages
	 sent out by this debug level.  It is short (5-6 characters) 
	 and does not contain white space. (i.e. DOT1X)"
	::= { extremeWirelessTraceModuleEntry 3 }

extremeWirelessTraceModuleLevel     OBJECT-TYPE
	SYNTAX	INTEGER(0..5)
	MAX-ACCESS read-write
	STATUS 	current
	DESCRIPTION
	"This value is the current debug level for this module.  A
	 lower value indicates that fewer messages will be generated
	 by the component.  A write on this value will update the
	 current debug level."
	::= { extremeWirelessTraceModuleEntry 4 }

extremeWirelessTraceModuleSuppressed     OBJECT-TYPE
	SYNTAX	INTEGER
	MAX-ACCESS read-only
	STATUS 	current
	DESCRIPTION
	"This value indicates the number of messages logged by
	 this module which have not been sent out because the
	 current log level is less than the level at which the
	 message should be logged."
	::= { extremeWirelessTraceModuleEntry 5 }

extremeWirelessTraceModuleMsgsOut     OBJECT-TYPE
	SYNTAX	INTEGER
	MAX-ACCESS read-only
	STATUS 	current
	DESCRIPTION
	"This value indicates the number messages which have
	 been logged by this component."
	::= { extremeWirelessTraceModuleEntry 6 }

extremeWirelessTraceModuleBytesOut     OBJECT-TYPE
	SYNTAX	INTEGER
	MAX-ACCESS read-only
	STATUS 	current
	DESCRIPTION
	"This value indicates the number of bytes which have
	 been logged by this component.  This count includes 
	 the header specified in extremeWirelessTraceModuleHeader."
	::= { extremeWirelessTraceModuleEntry 7 }

-- ************************************************************** --
--                    Log Diagnostic Counters                      --
--                                                                 --
-- The logging subsystem uses the following division : the event   --
-- logging system recieves all messages.  These message are then   --
-- passed to the syslog facility for remote logging, and then msgs --
-- may be stored in the NVRAM in the case where the log level is   --
-- greater than the log threshold.                                 --
-- ************************************************************** --
extremeWirelessLogDiagTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessLogDiagEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"This table contains counters per-log level for the event log,
	 syslog and NVRAM subsystems for logging."
	::= { extremeAP 102 }

extremeWirelessLogDiagEntry OBJECT-TYPE
	SYNTAX	ExtremeWirelessLogDiagEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"There is one entry in this table per physical port."
	INDEX { ifIndex }
	::= { extremeWirelessLogDiagTable 1 }

ExtremeWirelessLogDiagEntry ::= SEQUENCE {
	extremeWirelessLogDiagEventLogTotalCount Unsigned32,
	extremeWirelessLogDiagEventLogTotalEmergCount Unsigned32,
	extremeWirelessLogDiagEventLogTotalAlertCount Unsigned32,
	extremeWirelessLogDiagEventLogTotalCritCount Unsigned32,
	extremeWirelessLogDiagEventLogTotalErrorCount Unsigned32,
	extremeWirelessLogDiagEventLogTotalWarnCount Unsigned32,
	extremeWirelessLogDiagEventLogTotalNoticeCount Unsigned32,
	extremeWirelessLogDiagEventLogTotalInfoCount Unsigned32,
	extremeWirelessLogDiagEventLogTotalDebugCount Unsigned32,
	extremeWirelessLogDiagEventLogTotalSuppressedCount Unsigned32,
	extremeWirelessLogDiagEventLogTotalByteCount Unsigned32,
	extremeWirelessLogDiagSyslogTotalEventCount Unsigned32,
	extremeWirelessLogDiagSyslogTotalSuppressedCount Unsigned32,
	extremeWirelessLogDiagSyslogTotalByteCount Unsigned32,
	extremeWirelessLogDiagNVRAMTotalEventCount Unsigned32,
	extremeWirelessLogDiagNVRAMTotalSuppressedCount Unsigned32,
	extremeWirelessLogDiagNVRAMTotalDroppedCount Unsigned32,
	extremeWirelessLogDiagNVRAMTotalByteCount Unsigned32,
	extremeWirelessLogDiagClearStats TruthValue }

extremeWirelessLogDiagEventLogTotalCount OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of messages logged since the
	 last time the statistics were cleared."
	::= { extremeWirelessLogDiagEntry 1 }

extremeWirelessLogDiagEventLogTotalEmergCount OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of messages logged at the EMERG
	 level."
	::= { extremeWirelessLogDiagEntry 2 }

extremeWirelessLogDiagEventLogTotalAlertCount OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of messages logged at the ALERT
	 level."
	::= { extremeWirelessLogDiagEntry 3 }

extremeWirelessLogDiagEventLogTotalCritCount OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of messages logged at the CRIT
	 level."
	::= { extremeWirelessLogDiagEntry 4 }

extremeWirelessLogDiagEventLogTotalErrorCount OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of messages logged at the ERROR
	 level."
	::= { extremeWirelessLogDiagEntry 5 }

extremeWirelessLogDiagEventLogTotalWarnCount OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of messages logged at the WARN
	 level."
	::= { extremeWirelessLogDiagEntry 6 }

extremeWirelessLogDiagEventLogTotalNoticeCount OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of messages logged at the NOTICE
	 level."
	::= { extremeWirelessLogDiagEntry 7 }

extremeWirelessLogDiagEventLogTotalInfoCount OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of messages logged at the INFO
	 level."
	::= { extremeWirelessLogDiagEntry 8 }

extremeWirelessLogDiagEventLogTotalDebugCount OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of messages logged at the DEBUG
	 level."
	::= { extremeWirelessLogDiagEntry 9 }

extremeWirelessLogDiagEventLogTotalSuppressedCount OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of messages which were suppressed
	 due to log level."
	::= { extremeWirelessLogDiagEntry 10 }

extremeWirelessLogDiagEventLogTotalByteCount OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of bytes logged by the logging
	 subsystem."
	::= { extremeWirelessLogDiagEntry 11 }

extremeWirelessLogDiagSyslogTotalEventCount OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of messages which have been sent
	 out to remote syslog servers."
	::= { extremeWirelessLogDiagEntry 12 }

extremeWirelessLogDiagSyslogTotalSuppressedCount OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of syslog messages which have been 
	 suppressed due to log level."
	::= { extremeWirelessLogDiagEntry 13 }

extremeWirelessLogDiagSyslogTotalByteCount OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"This gives the total number of bytes of syslog messages which have
	 been logged."
	::= { extremeWirelessLogDiagEntry 14 }

extremeWirelessLogDiagNVRAMTotalEventCount OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"Total number of messages which have been logged to NVRAM."
	::= { extremeWirelessLogDiagEntry 15 }

extremeWirelessLogDiagNVRAMTotalSuppressedCount OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"Total number of messages which have been suppressed by NVRAM
	 due to NVRAM threashold."
	::= { extremeWirelessLogDiagEntry 16 }

extremeWirelessLogDiagNVRAMTotalDroppedCount OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"Total number of messages which have been dropped by the 
	 NVRAM."
	::= { extremeWirelessLogDiagEntry 17 }

extremeWirelessLogDiagNVRAMTotalByteCount OBJECT-TYPE
	SYNTAX Unsigned32
	MAX-ACCESS read-only
	STATUS current
	DESCRIPTION
	"Total number of bytes which have been written to the NVRAM."
	::= { extremeWirelessLogDiagEntry 18 }

extremeWirelessLogDiagClearStats OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS read-write
	STATUS current
	DESCRIPTION
	"Setting this value to TRUE causes the statistics to be reset to
	 0.  Reading this value has no meaning."
	::= { extremeWirelessLogDiagEntry 19 }

-- ************************************************************** --
--                           TRAPS                                 --
--                                                                 --
-- NOTE: We define client Authentication and association traps but --
--       performance may dictate that this not be done.  In that   --
--       case we have already provided the Authentication and      --
--       association totals which can be watched from RMON.        --
--                                                                 --
-- NOTE: The MAP State Change trap is not sent when the MAP is     --
--       first discovered.  The first trap is sent by EDP.         --
-- ************************************************************** --
extremeWirelessPortStateChange NOTIFICATION-TYPE
	OBJECTS { ifIndex,
		  extremeWirelessPortState }
	STATUS current
	DESCRIPTION
		"This trap is generated when a wireless port moves 
		 into enabled, disabled or online."
	::= { extremeAPTrapsPrefix 1 }

extremeWirelessPortBootFailure NOTIFICATION-TYPE
       OBJECTS { extremeWirelessPortIfIndex }
       STATUS current
       DESCRIPTION
               "This trap is sent by the platform if a wireless 
		port fails to boot too many times."
       ::= { extremeAPTrapsPrefix 2 }

extremeWirelessClientStationAgedOut NOTIFICATION-TYPE
       OBJECTS { ifIndex, extremeWirelessClientID }
       STATUS current
       DESCRIPTION
               "This trap is generated when a client is aged out 
		of the table."
       ::= { extremeAPTrapsPrefix 3 }

extremeWirelessNetloginClientAssociated NOTIFICATION-TYPE
       OBJECTS { ifIndex, extremeWirelessClientID }
       STATUS current
       DESCRIPTION
               "This trap is generated when a client has associated 
		to an interface that is web based network login 
		enabled."
       ::= { extremeAPTrapsPrefix 4 }

extremeWirelessAPAdded NOTIFICATION-TYPE
       OBJECTS { ifIndex, 
		 extremeWirelessScanResultsStationId,
		 extremeWirelessScanResultsFirstSeen,
		 extremeWirelessScanResultsLastChange,
		 extremeWirelessScanResultsPacketRate,
		 extremeWirelessScanResultsChannel,
		 extremeWirelessScanResultsAvgRSS,
		 extremeWirelessScanResultsSSID,
		 extremeWirelessScanResultsRSNEnabled,
		 extremeWirelessScanResultsPrivacy,
		 extremeWirelessScanResultsNetworkType,
		 extremeWirelessScanWPAIEMcastCipher,
		 extremeWirelessScanWPAUcastCipherCount,
	 	 extremeWirelessScanWPAUcastCipher,
		 extremeWirelessScanWPAKeyMgmtCount,
		 extremeWirelessScanWPAKeyMgmtSuite,
         extremeWirelessScanResultsRateSet,      
         extremeWirelessScanResultsExtRateSet }
       STATUS current
       DESCRIPTION
               "This is generated when a new AP is added to the
	 	scan results table.  It will ony be generated if
	 	the value of extremeWirelessScanSendAPAddedTrap
		is true."
       ::= { extremeAPTrapsPrefix 5 }

extremeWirelessAPRemoved NOTIFICATION-TYPE
       OBJECTS { ifIndex, extremeWirelessScanResultsStationId }
       STATUS current
       DESCRIPTION
               "This is generated when an AP is removed from the
	 	scan results table.  It will ony be generated if
	 	the value of extremeWirelessScanSendAPRemovedTrap
		is true."
       ::= { extremeAPTrapsPrefix 6 }

extremeWirelessAPUpdated NOTIFICATION-TYPE
       OBJECTS { ifIndex, 
		 extremeWirelessScanResultsStationId,
		 extremeWirelessScanResultsFirstSeen,
		 extremeWirelessScanResultsLastChange,
		 extremeWirelessScanResultsPacketRate,
		 extremeWirelessScanResultsChannel,
		 extremeWirelessScanResultsAvgRSS,
		 extremeWirelessScanResultsSSID,
		 extremeWirelessScanResultsRSNEnabled,
		 extremeWirelessScanResultsPrivacy,
		 extremeWirelessScanResultsNetworkType,
		 extremeWirelessScanWPAIEMcastCipher,
		 extremeWirelessScanWPAUcastCipherCount,
	 	 extremeWirelessScanWPAUcastCipher,
		 extremeWirelessScanWPAKeyMgmtCount,
		 extremeWirelessScanWPAKeyMgmtSuite,
         extremeWirelessScanResultsRateSet,
         extremeWirelessScanResultsExtRateSet }
       STATUS current
       DESCRIPTION
               "This is generated when the IEs recorded for an AP
		in the scan results table change.  It will only be
		generated if the value of SendAPUpdatedTrap is true."
       ::= { extremeAPTrapsPrefix 7 }

extremeWirelessProbeInfoAdded NOTIFICATION-TYPE
       OBJECTS { ifIndex, extremeWirelessProbeInfoSource }
       STATUS current
       DESCRIPTION
               "This is generated when a new station is added to the
		probe info table.  It will only be generated if the 
		value of extremeWirelessProbeInfoSendAddedTrap is true."
       ::= { extremeAPTrapsPrefix 8 }

extremeWirelessProbeInfoRemoved NOTIFICATION-TYPE
       OBJECTS { ifIndex, extremeWirelessProbeInfoSource }
       STATUS current
       DESCRIPTION
               "This is generated when a station is removed from the
		probe info table.  It will only be generated if the 
		value of extremeWirelessProbeInfoSendRemovedTrap is 
		true."
       ::= { extremeAPTrapsPrefix 9 }

extremeWirelessOffChannelScanStarted NOTIFICATION-TYPE
	OBJECTS { ifIndex, extremeWirelessOffChannelScanList }
        STATUS current
        DESCRIPTION
                "This is generated when an off-channel scan starts
                 running."
        ::= { extremeAPTrapsPrefix 10 }

extremeWirelessOffChannelScanFinished NOTIFICATION-TYPE
        OBJECTS { ifIndex, extremeWirelessOffChannelScanList }
        STATUS current
        DESCRIPTION
                "This is generated when an off-channel scan finishes
                 running."
        ::= { extremeAPTrapsPrefix 11 }

extremeWirelessCounterMeasureStarted NOTIFICATION-TYPE
        OBJECTS { ifIndex, extremeWirelessCounterMeasureSource }
        STATUS current
        DESCRIPTION
        "This trap is generated when counter measures are started
        on a wireless interface."
        ::= { extremeAPTrapsPrefix 12 }

extremeWirelessCounterMeasureStopped NOTIFICATION-TYPE
        OBJECTS { ifIndex }
        STATUS current
        DESCRIPTION
        "This trap is generated when counter measures are stopped
        on a wireless interface."
        ::= { extremeAPTrapsPrefix 13 }

--DFS related
extremeWirelessInterfaceChannelRescan NOTIFICATION-TYPE
        OBJECTS { ifIndex,
                  extremeWirelessPhysInterfacePHYChannel,
                  extremeWirelessPhysInterfaceChannelAutoSelectStatus
            }
        STATUS current
        DESCRIPTION
                "This trap is generated when a wireless interface tries to
autoselect a channel. It indicates whether a particular channel scan was
successful, or if it failed then the reason for the failure."
        ::= { extremeAPTrapsPrefix 14 }

        --
        -- TODO: Should we move this somewhere else?
        --
extremeWirelessCounterMeasureSource OBJECT-TYPE
        SYNTAX INTEGER { clientReport(1),
            micFailure(2) }
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
            "This value is used in the counter measure traps to indicate the
            reason that counter measures have been invoked."
            ::= { extremeAP 44 }

extremeWirelessClientWPAStatsTable OBJECT-TYPE
	SYNTAX SEQUENCE OF ExtremeWirelessClientWPAStatsEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"This table contains information of the WPA state transitions
	on a per-client basis.  Rows are indexed first by virtual
	interface, then by client MAC."
	 ::= { extremeAP 47 }

extremeWirelessClientWPAStatsEntry OBJECT-TYPE
	SYNTAX ExtremeWirelessClientWPAStatsEntry
	MAX-ACCESS not-accessible
	STATUS current
	DESCRIPTION
	"Note that ifIndex here is virtual ifIndex (SSID)."
	INDEX { ifIndex, extremeWirelessClientDiagMac }
	 ::= { extremeWirelessClientWPAStatsTable 1 }

ExtremeWirelessClientWPAStatsEntry ::= SEQUENCE {
	extremeWirelessClientWPAStatsStarts	Counter32,
	extremeWirelessClientWPAStatsPairwiseKeySuccesses	Counter32,
	extremeWirelessClientWPAStatsPairwiseKeyFailures	Counter32,
	extremeWirelessClientWPAStatsGroupKeySuccesses		Counter32,
	extremeWirelessClientWPAStatsGroupKeyFailures		Counter32,
	extremeWirelessClientWPAStatsPairwiseKey1Sends		Counter32,
	extremeWirelessClientWPAStatsPairwiseKey3Sends		Counter32,
	extremeWirelessClientWPAStatsGroupKeySends			Counter32,
	extremeWirelessClientWPAStatsEAPOLKeyReceivedInPairwise1Key	Counter32,
	extremeWirelessClientWPAStatsEAPOLKeyReceivedInPairwise3Key	Counter32,
	extremeWirelessClientWPAStatsEAPOLKeyReceivedInGroupKey		Counter32,
	extremeWirelessClientWPAStatsDoubleEAPOLKeyReceived		Counter32,
	extremeWirelessClientWPAStatsEAPOLKeyIgnores			Counter32,
	extremeWirelessClientWPAStatsEAPOLKeyErrors			Counter32,
	extremeWirelessClientWPAStatsEAPOLKeyAborts			Counter32,
	extremeWirelessClientWPAStatsEAPOLKeyVerificationSuccesses	Counter32
}
extremeWirelessClientWPAStatsStarts OBJECT-TYPE
	SYNTAX Counter32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"Number of starts of the WPA key exchange process"
	 ::= { extremeWirelessClientWPAStatsEntry 1 }

extremeWirelessClientWPAStatsPairwiseKeySuccesses OBJECT-TYPE
	SYNTAX Counter32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"Number of successes in the pairwise key handshake"
	 ::= { extremeWirelessClientWPAStatsEntry 2 }

extremeWirelessClientWPAStatsPairwiseKeyFailures OBJECT-TYPE
	SYNTAX Counter32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"Number of failures the pairwise key handshake"
	 ::= { extremeWirelessClientWPAStatsEntry 3 }

extremeWirelessClientWPAStatsGroupKeySuccesses OBJECT-TYPE
	SYNTAX Counter32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"Number of successes of the group key exchange"
	 ::= { extremeWirelessClientWPAStatsEntry 4 }

extremeWirelessClientWPAStatsGroupKeyFailures OBJECT-TYPE
	SYNTAX Counter32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"Number of failures of the group key handshake"
	 ::= { extremeWirelessClientWPAStatsEntry 5 }

extremeWirelessClientWPAStatsPairwiseKey1Sends OBJECT-TYPE
	SYNTAX Counter32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"Number of times the first packet of the pairwise key exchange was sent."
	 ::= { extremeWirelessClientWPAStatsEntry 6 }

extremeWirelessClientWPAStatsPairwiseKey3Sends OBJECT-TYPE
	SYNTAX Counter32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"Number of times the third packet of the pairwise key exchange was sent."
	 ::= { extremeWirelessClientWPAStatsEntry 7 }

extremeWirelessClientWPAStatsGroupKeySends OBJECT-TYPE
	SYNTAX Counter32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"Number of times the group key packet was sent."
	 ::= { extremeWirelessClientWPAStatsEntry 8 }

extremeWirelessClientWPAStatsEAPOLKeyReceivedInPairwise1Key OBJECT-TYPE
	SYNTAX Counter32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"Number of times an EAPOL Key packet was recieved after
	sending the 1st pairwise key exchange packet"
	 ::= { extremeWirelessClientWPAStatsEntry 9 }

extremeWirelessClientWPAStatsEAPOLKeyReceivedInPairwise3Key OBJECT-TYPE
	SYNTAX Counter32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"Number of times an EAPOL Key packet was recieved after
	sending the 3rd pairwise key exchange packet"
	 ::= { extremeWirelessClientWPAStatsEntry 10 }

extremeWirelessClientWPAStatsEAPOLKeyReceivedInGroupKey OBJECT-TYPE
	SYNTAX Counter32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"Number of times an EAPOL Key packet was recieved after
	sending the group key packet"
	 ::= { extremeWirelessClientWPAStatsEntry 11 }

extremeWirelessClientWPAStatsDoubleEAPOLKeyReceived OBJECT-TYPE
	SYNTAX Counter32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"Number of times an EAPOL Key packet was recieved when already
	processing a previous key packet."
	 ::= { extremeWirelessClientWPAStatsEntry 12 }

extremeWirelessClientWPAStatsEAPOLKeyIgnores OBJECT-TYPE
	SYNTAX Counter32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"Number of times an EAPOL Key packet was ignored."
	 ::= { extremeWirelessClientWPAStatsEntry 13 }

extremeWirelessClientWPAStatsEAPOLKeyErrors OBJECT-TYPE
	SYNTAX Counter32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"Number of times an EAPOL Key packet was errored."
	 ::= { extremeWirelessClientWPAStatsEntry 14 }

extremeWirelessClientWPAStatsEAPOLKeyAborts OBJECT-TYPE
	SYNTAX Counter32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"Number of times an EAPOL Key packet caused the WPA state machine to abort."
	 ::= { extremeWirelessClientWPAStatsEntry 15 }

extremeWirelessClientWPAStatsEAPOLKeyVerificationSuccesses OBJECT-TYPE
	SYNTAX Counter32
	MAX-ACCESS read-only
	STATUS	   current
	DESCRIPTION
	"Number of times an EAPOL Key packet was verified correctly."
	 ::= { extremeWirelessClientWPAStatsEntry 16 }

END
-- *********************************************************************
--  Extreme 802.11f MIB.  Based on IEEE MIB with addition of ifIndex for
--  demux.
-- ********************************************************************* 
EXTREMEdot11f-MIB DEFINITIONS ::= BEGIN 
	IMPORTS 

	MODULE-IDENTITY FROM SNMPv2-SMI
	extremeAP FROM EXTREME-BASE-MIB;


-- ********************************************************************* 
--  MODULE IDENTITY 
-- ********************************************************************* 

	extremeDot11f MODULE-IDENTITY 
	LAST-UPDATED "0107020000Z" 
	ORGANIZATION "Extreme Networks"
	CONTACT-INFO 
		" "

	DESCRIPTION 
	"This MIB module provides management of IAPP on a set of APs.
	 It is functionally identical to the IAPP MIB from the IEEE
	 with the addition of a new index."
    ::= { extremeAP 22 }

END


-- << end >>

-- ============================================================================
--
-- Extreme Traps
--

EXTREME-TRAP-MIB DEFINITIONS ::= BEGIN

        IMPORTS
        extremenetworks, extremeV1Traps		FROM EXTREME-BASE-MIB
		extremeSlotNumber		FROM EXTREME-SYSTEM-MIB
		extremeSlotModuleConfiguredType	FROM EXTREME-SYSTEM-MIB
		extremeSlotModuleInsertedType	FROM EXTREME-SYSTEM-MIB
		extremeSlotModuleState		FROM EXTREME-SYSTEM-MIB
        extremePowerSupplyNumber, extremeFanNumber
					 	FROM EXTREME-SYSTEM-MIB	
		extremeCurrentTemperature	FROM EXTREME-SYSTEM-MIB	
        extremeEsrpGroup, extremeEsrpState,
		extremeEsrpNetAddress  FROM EXTREME-ESRP-MIB
        extremeEsrpActivePorts, extremeEsrpInternalActivePorts
						FROM EXTREME-ESRP-MIB
        extremeEsrpTrackedActivePorts, extremeEsrpTrackedIpRoutes
						FROM EXTREME-ESRP-MIB
        extremeVlanIfIndex, extremeVlanIfDescr FROM EXTREME-VLAN-MIB
		extremeEdpPortIfIndex, extremeEdpNeighborId,
		extremeEdpEntryAge, extremeEdpNeighborVlanName,
		extremeEdpNeighborVlanIpAddress	       FROM EXTREME-EDP-MIB
		sysUpTime, sysDescr, ifPhysAddress,
                ifDescr                                FROM RFC1213-MIB
                ifAlias                                FROM IF-MIB
                NOTIFICATION-TYPE		       FROM SNMPv2-SMI;

          extremeOverheat NOTIFICATION-TYPE
              OBJECTS   { sysUpTime, sysDescr, extremeCurrentTemperature }
	      STATUS current
              DESCRIPTION
                          "A overheat trap indicates that the on board
                          tempature sensor has reported a overheat 
                          condition.  System will shutdown until unit has
			  suficiently cooled such that operation may begin
                          again.  A cold start trap will be issued when
                          the unit has come back on line."
              ::= {extremeV1Traps 6} 

          extremeFanfailed NOTIFICATION-TYPE
              OBJECTS   { sysUpTime, sysDescr, extremeFanNumber }
	      STATUS current
              DESCRIPTION
                          "A fan failed trap indicates one or more of the
                          cooling fans inside the device has failed.  A
                          fanOK trap will be sent once the fan has attained
                          normal operation."
              ::= {extremeV1Traps 7}

          extremeFanOK NOTIFICATION-TYPE
              OBJECTS   { sysUpTime, sysDescr, extremeFanNumber }
	      STATUS current
              DESCRIPTION
                          "A fan has transitioned out of a failure state and
                          is now operating correctly."
              ::= {extremeV1Traps 8} 

          extremeInvalidLoginAttempt NOTIFICATION-TYPE
              OBJECTS   { sysUpTime, sysDescr }
	      STATUS current
              DESCRIPTION
                "A user attempted to login to console or by telnet but was
                 refused access due to incorrect username or password"
              ::= {extremeV1Traps 9} 

          extremePowerSupplyFail NOTIFICATION-TYPE
              OBJECTS   { sysUpTime, sysDescr, extremePowerSupplyNumber }
	      STATUS current
              DESCRIPTION
                "One or more sources of power to this agent has failed.
                 Presumably a redundant power-supply has taken over."
              ::= {extremeV1Traps 10} 

          extremePowerSupplyGood NOTIFICATION-TYPE
              OBJECTS   { sysUpTime, sysDescr, extremePowerSupplyNumber }
	      STATUS current
              DESCRIPTION
                 "One or more previously bad sources of power to this agent 
                 has come back to life without causing an agent restart."
              ::= {extremeV1Traps 11} 

          extremeRpsAlarm NOTIFICATION-TYPE
              OBJECTS   { sysUpTime, sysDescr }
	      STATUS current
              DESCRIPTION
                          "Attached Redundant Power Supply device is indicating
                           an alarm condition."
              ::= {extremeV1Traps 12} 

          extremeRpsNoAlarm NOTIFICATION-TYPE
              OBJECTS   { sysUpTime, sysDescr }
	      STATUS current
              DESCRIPTION
                          "Attached Redundant Power Supply device is no longer
                           indicating an alarm condition."
              ::= {extremeV1Traps 13} 

--
-- SmartTrap definition
--
        extremeSmartTrap NOTIFICATION-TYPE
                OBJECTS   { sysUpTime, sysDescr }
	        STATUS current
        	DESCRIPTION
                "Signifies that the value of one of the object identifiers 
                (or the value of an object below that in the MIB tree) 
                defined in the extremeSmartTrapRulesTable has changed, 
                and hence a new entry has been created in the 
                extremeSmartTrapInstanceTable. Such a trap is sent 
                at most once every thirty seconds if one or more entry 
                was created in the last thirty seconds." 
              ::= {extremeV1Traps 14} 

--
-- Traps for Black Diamond
--
	extremeModuleStateChanged NOTIFICATION-TYPE
		OBJECTS { sysUpTime, extremeSlotNumber, 
                            extremeSlotModuleConfiguredType, 
                            extremeSlotModuleInsertedType, 
                            extremeSlotModuleState }
	        STATUS current
		DESCRIPTION
		"Signifies that the value of the extremeSlotModuleState for 
		the specified extremeSlotNumber has changed."
              ::= {extremeV1Traps 15} 

--	extremeModuleOverheat TRAP-TYPE
--		ENTERPRISE  extremenetworks
--		VARIABLES {sysUpTime, extremeSlotNumber }
--		DESCRIPTION
--		"Signifies that the temperature sensor on the module 
--		inside this slot has reported an Overheat condition."
--	::= 16

	extremeEsrpStateChange NOTIFICATION-TYPE
        	OBJECTS {sysUpTime, sysDescr, extremeVlanIfIndex,
			extremeVlanIfDescr, extremeEsrpGroup, extremeEsrpState,
			extremeEsrpNetAddress, ifPhysAddress,
                        extremeEsrpActivePorts, extremeEsrpInternalActivePorts,
                        extremeEsrpTrackedActivePorts, extremeEsrpTrackedIpRoutes
                }
		STATUS current
        DESCRIPTION
        "Signifies Esrp state change"
        ::= {extremeV1Traps 17}

        extremeSlbUnitAdded NOTIFICATION-TYPE
		STATUS current
                DESCRIPTION
                "The server load balancer has activated a group of virtual
                servers that it normally would not activate.  This may be
                due to the failure of another server load balancer."
                
        ::= {extremeV1Traps 18}

        extremeSlbUnitRemoved NOTIFICATION-TYPE
		STATUS current
                DESCRIPTION
                "The server load balancer has deactivated a group of virtual
                servers that it normally has active.  This indicates that
                something is wrong in the server load balancer; for example,
                its ping check may be failing."
        ::= {extremeV1Traps 19}

	extremeEdpNeighborAdded NOTIFICATION-TYPE
        	OBJECTS {sysUpTime, extremeEdpPortIfIndex,
			extremeEdpNeighborId, extremeEdpEntryAge,
			ifAlias, ifDescr
                }
	STATUS current
        DESCRIPTION
        "This node discovers a new neighbor through Extreme Discovery
	 Protocol."
        ::= {extremeV1Traps 20}

	extremeEdpNeighborRemoved NOTIFICATION-TYPE
        	OBJECTS {sysUpTime, extremeEdpPortIfIndex,
			extremeEdpNeighborId, extremeEdpEntryAge,
			ifAlias, ifDescr
                }
	STATUS current
        DESCRIPTION
        "No EDP updates are received from this neighbor within
	the configured timeout period and this neighbor entry is aged
	out by the device."
        ::= {extremeV1Traps 21}
        
END


EXTREME-V2TRAP-MIB DEFINITIONS ::= BEGIN

	IMPORTS 
	extremeV2Traps				FROM EXTREME-BASE-MIB
    sysDescr,sysUpTime                      FROM RFC1213-MIB
	extremeCpuTaskUtilPair,
    extremeCpuAggregateUtilization,
    extremeCpuUtilRisingThreshold		FROM EXTREME-SYSTEM-MIB
	extremeNPModuleProcessorState	        FROM EXTREME-NP-MIB
	extremeEsrpGroup, extremeEsrpState      FROM EXTREME-ESRP-MIB
	extremeVlanIfIndex, extremeVlanIfDescr  FROM EXTREME-VLAN-MIB
 	extremeHealthCheckErrorType, extremeSlotNumber, 	
	extremeHealthCheckAction, extremeHealthCheckMaxRetries,	
    extremeMasterMSMSlot, extremeMsmFailoverCause FROM EXTREME-SYSTEM-MIB
    ifIndex                 FROM RFC1213-MIB
    extremeIQosProfileIndex FROM EXTREME-QOS-MIB
    bgpPeerRemoteAddr                       FROM BGP4-MIB
	extremeEapsName, extremeEapsMode, extremeEapsState,
	extremeEapsPrevState			FROM EXTREME-EAPS-MIB
    extremePethSlotPSUActive            FROM EXTREME-POE-MIB
    extremePethSlotMainPseIndex         FROM EXTREME-POE-MIB

	NOTIFICATION-TYPE, OBJECT-TYPE , IpAddress            FROM SNMPv2-SMI
    ClientAuthType                          FROM EXTREME-BASE-MIB
    DisplayString                    FROM RFC1213-MIB
    MacAddress ,TimeStamp            FROM SNMPv2-TC;

    extremeCoreSCTraps     OBJECT IDENTIFIER
	::= { extremeV2Traps 1 }

    extremeCoreSCTrapPrefix	OBJECT IDENTIFIER
	::= { extremeCoreSCTraps 0 }

    extremeHealthCheckFailed NOTIFICATION-TYPE
        OBJECTS {	
          	     sysDescr, 
         		 extremeSlotNumber, 
		    	 extremeHealthCheckErrorType,
			     extremeHealthCheckAction, 
			     extremeHealthCheckMaxRetries
                }
	    STATUS current
        DESCRIPTION
                "Cpu HealthCheck has failed."
                ::= { extremeCoreSCTrapPrefix 1 }

-- Aggregate CPU utilization Trap definition
--
    extremeCpuUtilizationRisingTrap NOTIFICATION-TYPE
            OBJECTS   { extremeCpuTaskUtilPair,
                          extremeCpuAggregateUtilization,
                          extremeCpuUtilRisingThreshold}
            STATUS    current
        	DESCRIPTION "CPU Utilizations Rising trap generated when
                        extremeCpuUtilRisingThreshold is touched/crossed "
	        ::= { extremeCoreSCTrapPrefix 2 }

    extremeCpuUtilizationFallingTrap NOTIFICATION-TYPE
            OBJECTS   { extremeCpuTaskUtilPair,
                          extremeCpuAggregateUtilization,
                          extremeCpuUtilRisingThreshold}
            STATUS    current
        	DESCRIPTION "CPU Utilization Falling Trap is generated when the
                    extremeCpuAggregateUtilization falls below 80% of the
                    extremeCpuUtilRisingThreshold"
            ::= { extremeCoreSCTrapPrefix 3 }

    extremeProcessorStateChangeTrap NOTIFICATION-TYPE
            OBJECTS {sysDescr,               
                     extremeSlotNumber,
                     extremeNPModuleProcessorState}
            STATUS      current
            DESCRIPTION
            "Failed processor on module has been detected."
            ::= { extremeCoreSCTrapPrefix 4 }

    extremeMsmFailoverTrap NOTIFICATION-TYPE
            OBJECTS {sysDescr,
                     extremeMasterMSMSlot,
                     extremeMsmFailoverCause}
            STATUS      current
            DESCRIPTION
            "MSM failover occurred."
            ::= { extremeCoreSCTrapPrefix 5 }


    extremeEsrpTimedOutFailedOverMaster NOTIFICATION-TYPE
            OBJECTS {sysDescr, 
                     extremeVlanIfIndex,
                     extremeVlanIfDescr,                     
                     extremeEsrpState}
            STATUS      current
            DESCRIPTION
            "The master node performed a hitless MSM failover, but the 
            master failed to resume normal operation within the reelect timeout.
            Thus, a new master (this switch) was elected." 
            ::= { extremeCoreSCTrapPrefix 6 }


-- Triumph support
--        

      extremeRateLimitExceededTrap NOTIFICATION-TYPE
            OBJECTS {extremeRateLimitExceededTrapType,
                     extremeRateLimitExceededTrapIndicator,
                     ifIndex ,
                     extremeIQosProfileIndex,
                     extremeExceededByteCount}
            STATUS      current
            DESCRIPTION
            "Committed Information Rate exceeded."
        ::= { extremeCoreSCTrapPrefix 7 }
        
      extremeRateLimitExceededTrapType OBJECT-TYPE
                SYNTAX INTEGER {
			exceededCIR(1),
			droppedBytes(2)
                        }
                MAX-ACCESS accessible-for-notify
                STATUS current
                DESCRIPTION
                "The trap condition being reported."
            ::= { extremeRateLimitExceededTrap 1 }
            
      extremeRateLimitExceededTrapIndicator OBJECT-TYPE
                SYNTAX INTEGER {
			clear(0),
			set(1)
                        }
                MAX-ACCESS accessible-for-notify
                STATUS current
                DESCRIPTION
                "The trap condition being reported."
            ::= { extremeRateLimitExceededTrap 2 }
            
      extremeExceededByteCount OBJECT-TYPE
                SYNTAX INTEGER
                MAX-ACCESS accessible-for-notify
                STATUS current
                DESCRIPTION
                "The number of bytes that exceeded the rate."
            ::= { extremeRateLimitExceededTrap 4 }

-- end Triumph support
--

    extremeBgpTraps     OBJECT IDENTIFIER
		    ::= { extremeV2Traps 2 }

	extremeBgpTrapsPrefix     OBJECT IDENTIFIER
            ::= { extremeBgpTraps 0 }

    extremeBgpPrefixReachedThreshold NOTIFICATION-TYPE
            OBJECTS { bgpPeerRemoteAddr}
            STATUS  current
            DESCRIPTION
                    "The extremeBgpPrefixReachedThreshold notification is generated
                     when the number of prefixes received over this 
                     peer session reaches the threshold limit."
                ::= { extremeBgpTrapsPrefix 1 }

    extremeBgpPrefixMaxExceeded NOTIFICATION-TYPE
            OBJECTS { bgpPeerRemoteAddr}
            STATUS  current
            DESCRIPTION
                    "The extremeBgpPrefixMaxExceeded notification is generated
                     when the number of prefixes received over this 
                     peer session reaches the maximum configured limit."
                ::= { extremeBgpTrapsPrefix 2 }

    extremeSecurityTraps     OBJECT IDENTIFIER
		::= { extremeV2Traps 3 }

	extremeSecurityTrapsPrefix     OBJECT IDENTIFIER
          ::= { extremeSecurityTraps 0 }


	extremeMacLimitExceeded NOTIFICATION-TYPE
        OBJECTS { extremeMacSecurityVlanIfIndex, 
                  extremeMacSecurityVlanDescr, 
                  extremeMacSecurityMacAddress, 
                  extremeMacSecurityPortIfIndex,
                  extremeMacSecurityVlanId }
	    STATUS      current
		DESCRIPTION
		    "This trap will be generated, for a port on which limit-learning has been 
             configured,  when a new MAC address exceeding the limit is learnt on that 
             port."
       ::= { extremeSecurityTrapsPrefix 1 }

    extremeUnauthorizedPortForMacDetected NOTIFICATION-TYPE
                   OBJECTS { extremeMacSecurityVlanIfIndex, 
                             extremeMacSecurityVlanDescr, 
                             extremeMacSecurityVlanId,
                             extremeMacSecurityMacAddress, 
                             extremeMacSecurityPortIfIndex }
                             
	    STATUS      current
		DESCRIPTION
		    "This trap will be generated when a MAC Address is learnt on a port on which 
             it is not not authorized. This will happen when the MAC address is statically 
             configured  as a 'secure mac' on some other port(s)."
        ::= { extremeSecurityTrapsPrefix 2 }

	extremeMacDetectedOnLockedPort NOTIFICATION-TYPE
                   OBJECTS { extremeMacSecurityVlanIfIndex, 
                             extremeMacSecurityVlanDescr, 
                             extremeMacSecurityVlanId,
                             extremeMacSecurityMacAddress, 
                             extremeMacSecurityPortIfIndex }
                             
	   	STATUS      current
		DESCRIPTION
		    "This trap will be generated on a port for which lock-learning has been 
		    configured, when a new MAC address is learnt on that port."
            ::= { extremeSecurityTrapsPrefix 3 }

    extremeMacSecurityVlanIfIndex OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      accessible-for-notify
        STATUS          current
        DESCRIPTION
                "The ifIndex of the VLAN on which the MAC address was received."
        ::= { extremeSecurityTraps 1 }

    extremeMacSecurityVlanDescr OBJECT-TYPE
         SYNTAX DisplayString (SIZE(0..32))
         MAX-ACCESS accessible-for-notify
         STATUS current
         DESCRIPTION
             "The description(name) of the VLAN on which the MAC address was received."
         ::= { extremeSecurityTraps 2 }

    extremeMacSecurityMacAddress  OBJECT-TYPE
         SYNTAX MacAddress
         MAX-ACCESS accessible-for-notify
         STATUS current
         DESCRIPTION
             "The received MAC address."
         ::= { extremeSecurityTraps 3 }

    extremeMacSecurityPortIfIndex  OBJECT-TYPE
         SYNTAX INTEGER
         MAX-ACCESS accessible-for-notify
         STATUS current
         DESCRIPTION
             "The ifIndex of the port on which the MAC address was received."
         ::= { extremeSecurityTraps 4 }

     extremeMacSecurityVlanId  OBJECT-TYPE
         SYNTAX INTEGER
         MAX-ACCESS accessible-for-notify
         STATUS current
         DESCRIPTION
             "The VLAN ID of the VLAN on which the MAC address was received."
        ::= { extremeSecurityTraps 5 }
                

      extremeNetloginUserLogin NOTIFICATION-TYPE
            OBJECTS { 	extremeNetloginStationMac,
		                extremeNetloginStationAddr,
		                extremeNetloginPortIfIndex,
                        extremeNetloginAuthType,
                        extremeNetloginSystemTime,
                        extremeNetloginUser, 
                        extremeNetloginSrcVlan,
                        extremeNetloginDestVlan,
                        extremeNetloginSessionStatus
                    }
	    	STATUS      current
		    DESCRIPTION
		    "This trap will be generated when a netlogin supplicant passes 
            authentication and logs in successfully into the network."
            ::= { extremeSecurityTrapsPrefix 4}



      extremeNetloginUserLogout NOTIFICATION-TYPE
            OBJECTS { 	extremeNetloginStationMac,
		                extremeNetloginStationAddr,
		                extremeNetloginPortIfIndex,
                        extremeNetloginAuthType,
                        extremeNetloginSystemTime,
                        extremeNetloginUser, 
                        extremeNetloginSrcVlan,
                        extremeNetloginDestVlan,
                        extremeNetloginSessionStatus
                    }
	    	STATUS      current
		    DESCRIPTION
            "This trap will be generated when a netlogin supplicant logs out. 
            This trap is meant to notify logout event only for already 
            authenticated and logged in supplicant. "
            ::= { extremeSecurityTrapsPrefix 5}


      extremeNetloginAuthFailure NOTIFICATION-TYPE
            OBJECTS { 	extremeNetloginStationMac,
		                extremeNetloginStationAddr,
		                extremeNetloginPortIfIndex,
                        extremeNetloginAuthType,
                        extremeNetloginSystemTime,
                        extremeNetloginUser, 
                        extremeNetloginSrcVlan,
                        extremeNetloginDestVlan,
                        extremeNetloginSessionStatus
                    }
	    	STATUS      current
		    DESCRIPTION
            "This trap will be generated upon authentication failure for a 
             netlogin supplicant"
            ::= { extremeSecurityTrapsPrefix 6 }


      extremeNetloginStationMac  OBJECT-TYPE
            SYNTAX  MacAddress
            MAX-ACCESS accessible-for-notify
      	    STATUS       current
     	    DESCRIPTION
            "MAC address of netlogin supplicant"
            ::= { extremeSecurityTraps 6 }

      extremeNetloginStationAddr  OBJECT-TYPE
            SYNTAX  IpAddress
            MAX-ACCESS accessible-for-notify
      	    STATUS       current
     	    DESCRIPTION
            "MAC address of netlogin supplicant"
            ::= { extremeSecurityTraps 7 }


      extremeNetloginPortIfIndex   OBJECT-TYPE
            SYNTAX  INTEGER
            MAX-ACCESS accessible-for-notify
      	    STATUS       current
     	    DESCRIPTION
            "IfIndex of authenticator port to which the netlogin supplicant is 
            connected"
            ::= { extremeSecurityTraps 8}

      extremeNetloginAuthType  OBJECT-TYPE
	        SYNTAX      ClientAuthType 
            MAX-ACCESS accessible-for-notify
      	    STATUS       current
     	    DESCRIPTION
            "IF supplicant is authenticated using remote authentication server
            as RADIUS or locally using authenticator local user database"
            ::= { extremeSecurityTraps 9}

      extremeNetloginSystemTime OBJECT-TYPE
            SYNTAX  TimeStamp
            MAX-ACCESS accessible-for-notify
            STATUS  current
            DESCRIPTION
                "The time when a netlogin event occurs and  is 
                meaningful for accounting purposes."
            ::= { extremeSecurityTraps 10}

        extremeNetloginUser  OBJECT-TYPE
        SYNTAX DisplayString (SIZE(1..64))
        MAX-ACCESS accessible-for-notify
      	STATUS       current
     	DESCRIPTION
	    "Information containing type of session as NETLOGIN or DOT1X
        concatenated with userName  i,e  '[NETLOGIN | DOT1X]:<username>' "
        ::= { extremeSecurityTraps 11}

        extremeNetloginSrcVlan  OBJECT-TYPE
        SYNTAX DisplayString (SIZE(1..64))
        MAX-ACCESS accessible-for-notify
      	STATUS       current
     	DESCRIPTION
        "Upon successful login this vlan will represent the one in which 
        user resides before authentication while upon logout this vlan will 
        be the one in which user resides before logout. "
        ::= { extremeSecurityTraps 12}

        extremeNetloginDestVlan  OBJECT-TYPE
        SYNTAX DisplayString (SIZE(1..64))
        MAX-ACCESS accessible-for-notify
      	STATUS       current
     	DESCRIPTION
        "The description (name) of the VLAN in which user moves after 
        successful login or logout."
        ::= { extremeSecurityTraps 13}
        
        extremeNetloginSessionStatus   OBJECT-TYPE
     	SYNTAX       INTEGER {
                        success (1),
                        sessionReset (2),
         				fDBAgingInitiatedLogout    (3),
         				userInitiatedLogout    (4),
				        sessionRefreshInitiatedLogout (5),
				        authenticationFailure  (6),
				        remoteAuthenticationServerFailure (7)
				}
 		MAX-ACCESS accessible-for-notify
   		STATUS       current
   		DESCRIPTION
        "
        -success (1) 
            Successful login
 	    -sessionReset (2)
            Administrator has initialized Authentication State.
	    -fDBAgingInitiatedLogout (3)
 	        Logout initiated due to FDB aging of client MAC
	    -userInitiatedLogout(4)
            Graceful logout attempt from user
        -sessionRefreshInitiatedLogout (5)
            (Valid for web-based mode only) Logout initiated by 
            session-refresh mechanism.
	   -authenticationFailure(6)
            Authentication Failure
	    -remoteAuthenticationServerFailure (7)
            Remote Authentication server Failure.
	    "
   	 ::= { extremeSecurityTraps 14 }

        extremeNMSTraps     OBJECT IDENTIFIER
		    ::= { extremeV2Traps 4 }

	    extremeNMSTrapsPrefix     OBJECT IDENTIFIER
            ::= { extremeNMSTraps 0 }

        extremeNMSDeviceAddress  OBJECT-TYPE
              SYNTAX IpAddress
              MAX-ACCESS  accessible-for-notify
              STATUS current
              DESCRIPTION
                  "The IP address of the device modified by Extreme's Network Management Application."
	          ::= { extremeNMSTraps 1 }

	    extremeNMSInventoryChanged NOTIFICATION-TYPE
            OBJECTS { extremeNMSDeviceAddress }
	    	STATUS      current
		    DESCRIPTION
		    "This trap is sent by Extreme's Network Management Applications when a change
                    in its inventory database occurs. This trap is not send by a router or switch."
		    ::= { extremeNMSTrapsPrefix 1 }

        extremeNMSTopologyChanged NOTIFICATION-TYPE
	    	STATUS      current
		    DESCRIPTION
		    "This trap is sent by Extreme's Network Management Applications when a change 
                    in its Topology database occurs. This trap is not send by a router or switch."
		    ::= { extremeNMSTrapsPrefix 2 }

        


    extremeEapsTraps     OBJECT IDENTIFIER
		::= { extremeV2Traps 7 }

	extremeEapsTrapsPrefix     OBJECT IDENTIFIER
          ::= { extremeEapsTraps 0 }

        extremeEapsStateChange NOTIFICATION-TYPE
            OBJECTS {	extremeEapsName, 
			extremeEapsMode, 
			extremeEapsPrevState,
			extremeEapsState}
            STATUS  current
            DESCRIPTION
                    "The extremeEapsStateChange notification is generated
                     when the EAPS domain has a state change."
                ::= { extremeEapsTrapsPrefix 1 }

        extremeEapsFailTimerExpFlagSet NOTIFICATION-TYPE
            OBJECTS {	extremeEapsName, 
			extremeEapsMode, 
			extremeEapsPrevState,
			extremeEapsState}
            STATUS  current
            DESCRIPTION
                    "The extremeEapsFailTimerExpFlagSet notification is 
                     generated when the EAPS domain's fail timer expires
                     for the first time, while its state is not in Fail state."
                ::= { extremeEapsTrapsPrefix 2 }

        extremeEapsFailTimerExpFlagClear NOTIFICATION-TYPE
            OBJECTS {	extremeEapsName, 
			extremeEapsMode, 
			extremeEapsPrevState,
			extremeEapsState}
            STATUS  current
            DESCRIPTION
                    "The extremeEapsFailTimerExpFlagClear notification is 
                     generated when the EAPS domain's Fail timer expired flag 
                     is cleared."
                ::= { extremeEapsTrapsPrefix 3 }


        extremeEapsLinkDownRingComplete NOTIFICATION-TYPE
            OBJECTS {	extremeEapsName, 
			extremeEapsMode, 
			extremeEapsPrevState,
			extremeEapsState}
            STATUS  current
            DESCRIPTION
                    "If a Transit is in Link-Down state, and it receives a 
                     Health-Check-Pdu from the Master indicating the ring is
                     Complete, it means there is some problem with the Transit
                     switch that has issued this trap message."
                ::= { extremeEapsTrapsPrefix 4 }

-- Extreme PoE Notifications
extremePethTraps  OBJECT IDENTIFIER ::= {extremeV2Traps 12}

extremePethNotificationPrefix     OBJECT IDENTIFIER
		::= { extremePethTraps 0 }

        extremePethPSUStatusNotification NOTIFICATION-TYPE
            OBJECTS     { extremePethSlotPSUActive, extremePethSlotMainPseIndex }
            STATUS      current
            DESCRIPTION
                " This Notification indicates a change in the PoE PSU for the slot."
            ::= { extremePethNotificationPrefix 1 }

 extremeElrpTraps       OBJECT IDENTIFIER
                ::= { extremeV2Traps 6 }

        extremeElrpTrapsPrefix  OBJECT IDENTIFIER
          ::= { extremeElrpTraps 0 }

        extremeElrpVlanLoopDetected NOTIFICATION-TYPE
            OBJECTS { extremeVlanIfDescr}
            STATUS  current
            DESCRIPTION
                     " The extremeElrpVlanLoopDetected notification is generated
                       when the ELRP client detects a loop in the vlan."
                ::= { extremeElrpTrapsPrefix 1 }



    extremeEapsSharedLinkTraps     OBJECT IDENTIFIER
		::= { extremeV2Traps 9 }

	extremeEapsSharedLinkTrapsPrefix     OBJECT IDENTIFIER
          ::= { extremeEapsSharedLinkTraps 0 }

        extremeSegmentPort  OBJECT-TYPE
              SYNTAX INTEGER (0..65535)
              MAX-ACCESS  accessible-for-notify
              STATUS current
              DESCRIPTION
                  "The EAPS Shared Link's Segment Id."
	          ::= { extremeEapsSharedLinkTraps 1 }

        extremeSharedPort  OBJECT-TYPE
              SYNTAX INTEGER (0..65535)
              MAX-ACCESS  accessible-for-notify
              STATUS current
              DESCRIPTION
                  "The EAPS Shared Link's Shared port."
	          ::= { extremeEapsSharedLinkTraps 2 }

        extremeEapsSegmentTimerExpFlagSet NOTIFICATION-TYPE
            OBJECTS {	extremeSegmentPort, 
                        extremeSharedPort
                    }
            STATUS  current
            DESCRIPTION
                    "The extremeEapsFailTimerExpFlagSet notification is 
                     generated when the EAPS domain's segment timer expires
                     for the first time."
                ::= { extremeEapsSharedLinkTrapsPrefix 1 }

        extremeEapsSegmentTimerExpFlagClear NOTIFICATION-TYPE
            OBJECTS {	extremeSegmentPort,
                        extremeSharedPort
                    }
            STATUS  current
            DESCRIPTION
                    "The extremeEapsSegmentTimerExpFlagClear notification is 
                     generated when the EAPS domain's Segment Fail timer 
                     expired flag is cleared."
                ::= { extremeEapsSharedLinkTrapsPrefix 2 }
     
END

-- ===================================================
--
-- Extreme Services
--

EXTREME-SERVICES-MIB DEFINITIONS ::= BEGIN
    IMPORTS
        MODULE-IDENTITY, OBJECT-TYPE    FROM SNMPv2-SMI
        InetAddressType, InetAddress    FROM INET-ADDRESS-MIB
        extremeAgent                    FROM EXTREME-BASE-MIB
        TruthValue, RowStatus           FROM SNMPv2-TC;

        
        extremeServices MODULE-IDENTITY
                      LAST-UPDATED "0007240000Z"
                      ORGANIZATION "Extreme Networks, Inc."
                      CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION "Extreme Upper layer services objects"
        ::= { extremeAgent 26 }

	extremeSyslog OBJECT IDENTIFIER ::= {extremeServices 1} 
	extremeDNS OBJECT IDENTIFIER ::= {extremeServices 3} 
    extremeAuthServer   OBJECT IDENTIFIER ::= {extremeServices 4}

	AuthServerType ::= TEXTUAL-CONVENTION
	  STATUS	current
	  DESCRIPTION
		"The type of authentication/accounting server."
	  SYNTAX INTEGER { radius(1), radius-acct(2), tacacs(3), tacacs-acct(4) }

	AuthServerAccessType ::= TEXTUAL-CONVENTION
	  STATUS	current
	  DESCRIPTION
		"Specifies whether the server is for authenticating mangement or netlogin accesses"
	  SYNTAX INTEGER { mgmt-access(1), netlogin(2) }

        extremeRemoteSyslogServerTable      OBJECT-TYPE
            SYNTAX       SEQUENCE OF ExtremeRemoteSyslogServerEntry
            MAX-ACCESS          not-accessible
            STATUS              current
            DESCRIPTION     
                "This table is used to configure remote syslog 
		servers and contains information on the same."
            ::= { extremeSyslog 1 }

        extremeRemoteSyslogServerEntry      OBJECT-TYPE
            SYNTAX              ExtremeRemoteSyslogServerEntry
            MAX-ACCESS          not-accessible
            STATUS              current
            DESCRIPTION
                "An entry in the extremeRemoteSyslogServerTable."
            INDEX { extremeRemoteSyslogServerAddressType, 				     	     
	    	    extremeRemoteSyslogServerAddress,
                    extremeRemoteSyslogServerPort, 			                 
		    extremeRemoteSyslogServerFacility
                    }
            ::= { extremeRemoteSyslogServerTable 1 }

        ExtremeRemoteSyslogServerEntry ::= SEQUENCE {
                extremeRemoteSyslogServerAddressType InetAddressType,
                extremeRemoteSyslogServerAddress     InetAddress,
                extremeRemoteSyslogServerPort        INTEGER,
                extremeRemoteSyslogServerFacility    INTEGER,
                extremeRemoteSyslogServerSeverity    BITS,
                extremeRemoteSyslogServerStatus      RowStatus
        }
         
        extremeRemoteSyslogServerAddressType          OBJECT-TYPE
                SYNTAX                          InetAddressType
                MAX-ACCESS                      read-only
                STATUS                          current
                DESCRIPTION
                    "The type of address specified in the object 				
		    'extremeRemoteSyslogServerAddress'.
                    Currently, only 'ipv4' and 'dns' are supported."
                DEFVAL { ipv4 }
            ::= { extremeRemoteSyslogServerEntry 1 }

      extremeRemoteSyslogServerAddress           OBJECT-TYPE
                SYNTAX                  InetAddress (SIZE (1..255))
                MAX-ACCESS              read-only
                STATUS                  current
                DESCRIPTION
                    "The address of the remote syslog server. This 
		    can be a DNS name or an IPv4 address." 
                    
            ::= { extremeRemoteSyslogServerEntry 2 }

     extremeRemoteSyslogServerPort                    OBJECT-TYPE
                SYNTAX                          INTEGER (0..65535)
                MAX-ACCESS                      read-only
                STATUS                          current
                DESCRIPTION
                    "The UDP port number of the remote syslog server 				
		    to which syslog messages will
                    be sent."
            ::= { extremeRemoteSyslogServerEntry 3 }

      extremeRemoteSyslogServerFacility               OBJECT-TYPE
                SYNTAX                          INTEGER {
                                                local0(1),
                                                local1(2),
                                                local2(3),
                                                local3(4),
                                                local4(5),
                                                local5(6),
                                                local6(7),
                                                local7(8)
                                                }
                MAX-ACCESS                      read-only
                STATUS                          current
                DESCRIPTION
                    "The facility which will be sent in all syslog 				
		    messages to this remote syslog server."
            ::= { extremeRemoteSyslogServerEntry 4 }

      extremeRemoteSyslogServerSeverity               OBJECT-TYPE
            SYNTAX  BITS { 
				critical(0),
				error(1),
				warning(2),
				notice(3),
				info(4),
				debugSummary(5),
				debugVerbose(6),
				debugData(7)					
				}
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                    "The syslog message severity. All syslog messages of the specified severity for
                    which the Bits are set, will be sent to this syslog server. When setting this object
                    in a 'createAndGo' request, all lower bits upto and including the desired bit position
                    must be set. For example, if bit info(4) needs to be set then bits critical(0), 
                    error(1), warning(2), notice(3) and info(4) must also be set in the request. 
                    Consequently, all syslog messages of a given severity and higher will be sent to 
                    the syslog server. It is not possible to send messages that match only a few selected
                    non-contiguous severities."
                DEFVAL { '11111111'B }
            ::= { extremeRemoteSyslogServerEntry 5 }

      extremeRemoteSyslogServerStatus               OBJECT-TYPE
                SYNTAX                          RowStatus
                MAX-ACCESS                      read-create
                STATUS                          current
                DESCRIPTION
                    "The status of the Row as per standard row  				
		    status conventions. Only 'createAndGo', 'active' and 
		    'destroy' will be supported. It is not possible
		    to change the values of the objects of a row 					
		    once it has been created, except by 'destroy'ing and 
		    re-creating the row."
                   
            ::= { extremeRemoteSyslogServerEntry 6 }

        extremeEnableRemoteSyslog OBJECT-TYPE
                SYNTAX TruthValue
        	MAX-ACCESS read-write
                STATUS current
                DESCRIPTION
                "The enable/disable status of remote syslog messages."
	::= { extremeSyslog 2 }

extremeDNSServerTable      OBJECT-TYPE
        SYNTAX              SEQUENCE OF ExtremeDNSServerEntry
        MAX-ACCESS          not-accessible
        STATUS              current
        DESCRIPTION     
            "This table is used to configure DNS servers. There can be at most two
             rows in this table."
      ::= { extremeDNS 1 }

extremeDNSServerEntry      OBJECT-TYPE
        SYNTAX              ExtremeDNSServerEntry
        MAX-ACCESS          not-accessible
        STATUS              current
        DESCRIPTION
            "An entry in the extremeDNSServerTable."
        INDEX { extremeDNSServerAddressIndex
              }
     ::= { extremeDNSServerTable 1 }

ExtremeDNSServerEntry ::= SEQUENCE {
                extremeDNSServerAddressIndex    INTEGER,
                extremeDNSServerAddressType     InetAddressType,
                extremeDNSServerAddress         InetAddress
        }

      extremeDNSServerAddressIndex              OBJECT-TYPE
        SYNTAX          INTEGER
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "This is an integer index. Only 1 and 2 are supported for this"
            ::= { extremeDNSServerEntry 1 }

      extremeDNSServerAddressType                OBJECT-TYPE
                SYNTAX                       InetAddressType 
                MAX-ACCESS                   read-only
                STATUS                       current
                DESCRIPTION
                    "The address type of the DNS server. This can be a DNS name or
                    an IPv4 address."

            ::= { extremeDNSServerEntry 2 }

      extremeDNSServerAddress                OBJECT-TYPE
                SYNTAX                       InetAddress (SIZE (1..255))
                MAX-ACCESS                   read-only
                STATUS                       current
                DESCRIPTION
                    "The address of the DNS server. This can be a DNS name or
                    an IPv4 address."

            ::= { extremeDNSServerEntry 3 }

extremeAuthServerEnableTable OBJECT-TYPE
      SYNTAX     SEQUENCE OF ExtremeAuthServerEnableEntry
      MAX-ACCESS not-accessible
      STATUS     current 
      DESCRIPTION
         "This table is used to enable/disable Auth servers"
   ::=   { extremeAuthServer 1 }

extremeAuthServerEnableEntry   OBJECT-TYPE
        SYNTAX                 ExtremeAuthServerEnableEntry
        MAX-ACCESS             not-accessible
        STATUS                 current
        DESCRIPTION
            "An entry in the extremeAuthServerEnableTable."
        INDEX { extremeAuthServerEnableServerType,
                extremeAuthServerEnableAccessType }
     ::= { extremeAuthServerEnableTable 1 }

ExtremeAuthServerEnableEntry ::= SEQUENCE {
        extremeAuthServerEnableServerType    AuthServerType,
        extremeAuthServerEnableAccessType    AuthServerAccessType,
        extremeAuthServerEnable              TruthValue }

extremeAuthServerEnableServerType OBJECT-TYPE
	SYNTAX		AuthServerType
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"Specifies whether this is a radius/radius-acct/tacacs/tacacs-acct server"
	::= { extremeAuthServerEnableEntry 1 }

extremeAuthServerEnableAccessType OBJECT-TYPE
	SYNTAX		AuthServerAccessType
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"Specifies whether this server is for management access or netlogin access."
	::= { extremeAuthServerEnableEntry 2 }

extremeAuthServerEnable OBJECT-TYPE
  SYNTAX  TruthValue
  MAX-ACCESS  read-write
  STATUS current
  DESCRIPTION
  "Enable/Disable the Radius/tacas Server"
  DEFVAL { false }
 ::= { extremeAuthServerEnableEntry 3 }

extremeAuthServerTable      OBJECT-TYPE
        SYNTAX              SEQUENCE OF ExtremeAuthServerEntry
        MAX-ACCESS          not-accessible
        STATUS              current
        DESCRIPTION     
            "This table is used to configure radius/tacacs servers."
      ::= { extremeAuthServer 2 }

extremeAuthServerEntry      OBJECT-TYPE
        SYNTAX              ExtremeAuthServerEntry
        MAX-ACCESS          not-accessible
        STATUS              current
        DESCRIPTION
            "An entry in the extremeAuthServerTable."
        INDEX { extremeAuthServerIndex
              }
     ::= { extremeAuthServerTable 1 }

ExtremeAuthServerEntry ::= SEQUENCE {
        extremeAuthServerIndex    INTEGER,
        extremeAuthServerAddressType     InetAddressType,
        extremeAuthServerAddress         InetAddress,
	extremeAuthServerClientAddressType InetAddressType,
	extremeAuthServerClientAddress	InetAddress,
	extremeAuthServerPort 		INTEGER,
	extremeAuthServerSecret 	OCTET STRING,
	extremeAuthServerReTransmit	INTEGER,
	extremeAuthServerType		 AuthServerType,
	extremeAuthServerIsPrimary	TruthValue,
	extremeAuthServerAccessType	AuthServerAccessType,
	extremeAuthServerStatus		RowStatus}

extremeAuthServerIndex OBJECT-TYPE
	SYNTAX		INTEGER(1..8)
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"Integer index of the server."
	::= { extremeAuthServerEntry 1 }

extremeAuthServerAddressType OBJECT-TYPE
	SYNTAX		InetAddressType
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"Type IP address of the radius/tacas server. "
	::= { extremeAuthServerEntry 2 }

extremeAuthServerAddress OBJECT-TYPE
	SYNTAX		InetAddress
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"IP address of the radius/tacas server."
	::= { extremeAuthServerEntry 3 }

extremeAuthServerClientAddressType OBJECT-TYPE
	SYNTAX		InetAddressType
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"Type of IP address to use as the SRC address when
		 contacting the the radius/tacas server. The radius/tacas server
		 should be configured with this address as one of its
		 clients. The switch should have a VLAN with this IP
		 address."
	::= { extremeAuthServerEntry 4 }

extremeAuthServerClientAddress OBJECT-TYPE
	SYNTAX		InetAddress
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"IP address to use as the SRC address when contacting the
		 the radius/tacas server. The radius/tacas server should be
                 configured with this address as one of its clients. The 
                 switch should have a VLAN with this IP address."
	::= { extremeAuthServerEntry 5 }

extremeAuthServerPort OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"Port number of the radius/tacas server."
	::= { extremeAuthServerEntry 6 }

extremeAuthServerSecret OBJECT-TYPE
	SYNTAX		OCTET STRING
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This is the shared secret between the Authenticator
		 and radius/tacas server.  This is logically write-only."
	::= { extremeAuthServerEntry 7 }

extremeAuthServerReTransmit OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"This is the timeout in seconds after which the 
		 Authenticator will re transmit requests to the
		 radius/tacas server."
	::= { extremeAuthServerEntry 8 }

extremeAuthServerType OBJECT-TYPE
	SYNTAX		AuthServerType
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"Specifies whether this is a radius/radius-acct/tacacs/tacacs-acct server"
	::= { extremeAuthServerEntry 9 }

extremeAuthServerIsPrimary OBJECT-TYPE
	SYNTAX		TruthValue
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"Specifies whether this is the primary or the
		secondary server. Is TRUE if the server is primary."
	::= { extremeAuthServerEntry 10 }

extremeAuthServerAccessType OBJECT-TYPE
	SYNTAX		AuthServerAccessType
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"Specifies whether this server is for management access or netlogin access"
	::= { extremeAuthServerEntry 11 }

extremeAuthServerStatus               OBJECT-TYPE
          SYNTAX                          RowStatus
          MAX-ACCESS                      read-create
          STATUS                          current
          DESCRIPTION
                    "The status of the Row as per standard row  				
		    status conventions. Only 'createAndGo', 'active' and 
		    'destroy' will be supported. It is not possible
		    to change the values of the objects of a row 					
		    once it has been created, except by 'destroy'ing and 
		    re-creating the row."
                   
            ::= { extremeAuthServerEntry 12 }


END

EXTREME-DOS-MIB DEFINITIONS ::= BEGIN

    IMPORTS  
        MODULE-IDENTITY     FROM SNMPv2-SMI
		OBJECT-TYPE         FROM SNMPv2-SMI
        TruthValue          FROM SNMPv2-TC
		extremeAgent        FROM EXTREME-BASE-MIB
		extremeV2Traps		FROM EXTREME-BASE-MIB
        extremenetworks		FROM EXTREME-BASE-MIB
		DisplayString       FROM RFC1213-MIB
                TimeTicks		FROM SNMPv2-SMI
		NOTIFICATION-TYPE	FROM SNMPv2-SMI;

        extremeDosMib MODULE-IDENTITY
                LAST-UPDATED "0401020000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION "Extreme Dos protect objects information"
        ::= { extremeAgent 28 }

        extremeDosProtect OBJECT IDENTIFIER ::= { extremeDosMib 1 }


extremeDosEnable    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The Flag indicates whether DOS protection is enabled or disabled."
    DEFVAL { false }
    ::= { extremeDosProtect 1 }


extremeDosNoticeLevel    OBJECT-TYPE
    SYNTAX      INTEGER(150..100000)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The number of packets per second to be received for logging."
    DEFVAL { 4000 }
    ::= { extremeDosProtect 2 }

extremeDosAlertLevel    OBJECT-TYPE
    SYNTAX      INTEGER(150..100000)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The number of packets per second to be received for ACL creation."
    DEFVAL { 4000 }
    ::= { extremeDosProtect 3 }

extremeDosFilterType    OBJECT-TYPE
    SYNTAX      INTEGER {
		destination (1),
		source	    (2),
		destinationAndSource (3)
		}
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The type of access list filter to be set when threshold pakets are received"
    DEFVAL { destination }
    ::= { extremeDosProtect 4 }

extremeDosAclTimeout    OBJECT-TYPE
    SYNTAX      INTEGER(2..300)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The timeout interval period over which DOS protect is exercised."
    DEFVAL { 15 }
    ::= { extremeDosProtect 5 }

extremeDosAclRulePrecedence    OBJECT-TYPE
    SYNTAX      INTEGER(0..25588)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The DOS filter Rule Precedence."
    DEFVAL { 10 }
    ::= { extremeDosProtect 6 }

extremeDosMessagesEnable    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The Flag indicates whether DOS messages are enabled or disabled."
    DEFVAL { true }
    ::= { extremeDosProtect 7 }

extremeDosPortTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF ExtremeDosPortEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "This table contains the port wise listing of DOS attributes."
    ::= { extremeDosProtect 8 }

extremeDosPortEntry       OBJECT-TYPE
    SYNTAX      ExtremeDosPortEntry
    MAX-ACCESS  not-accessible 
    STATUS      current
    DESCRIPTION
            "Information about the Dos attributes of a particular port."
    INDEX   { extremeDosIfIndex }
    ::= { extremeDosPortTable 1 }

ExtremeDosPortEntry ::= SEQUENCE {
      extremeDosIfIndex          		INTEGER,
      extremeDosPortTrusted			TruthValue,
      extremeDosIsDosActive			TruthValue
}

extremeDosIfIndex    OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The index for this entry."
    ::= { extremeDosPortEntry 1 }

extremeDosPortTrusted    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
            "Indicates whether the port is trusted or untrusted."
    DEFVAL { false }
    ::= { extremeDosPortEntry 2 }

extremeDosIsDosActive    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Indicates whether DOS is active on this port."
    ::= { extremeDosPortEntry 3 }


--TRAPS MIB Definitions for DOS
  
--   extremeDosThresholdReached	TRAP-TYPE
--   ENTERPRISE  extremenetworks
--   VARIABLES   {extremeDosAlertLevel}
--   DESCRIPTION
--   	  "The extremeDosThresholdReached notification is generated when the
--   	  DOS threshold is crossed"
--   ::= 23

--   extremeDosThresholdCleared	TRAP-TYPE
--   ENTERPRISE  extremenetworks
--   VARIABLES   {extremeDosAlertLevel}
--   DESCRIPTION
--   	  "The extremeDosThresholdCleared notification is generated when the
--   	  DOS threshold is Cleared"
--   ::= 24


   extremeDosTraps 	OBJECT IDENTIFIER
	::= { extremeV2Traps 14 }

   extremeDosTrapsPrefix   OBJECT IDENTIFIER
	::= { extremeDosTraps 0 }

   extremeDosThresholdCleared NOTIFICATION-TYPE
	OBJECTS { extremeDosAlertLevel }
	STATUS current
	DESCRIPTION
		"The extremeDosThresholdCleared notification is generated when
		the DOS threshold is cleared ."
	    ::= { extremeDosTrapsPrefix 1 }

    extremeDosThresholdReached NOTIFICATION-TYPE
	OBJECTS { extremeDosAlertLevel }
	STATUS current
	DESCRIPTION
		"The extremeDosThresholdReached notification is generated when
		the DOS threshold is crossed for any of the ports."
	    ::= { extremeDosTrapsPrefix 2 }
END

EXTREME-ENH-DOS-MIB DEFINITIONS ::= BEGIN

        IMPORTS
                MODULE-IDENTITY FROM SNMPv2-SMI
                OBJECT-TYPE     FROM SNMPv2-SMI
                DisplayString   FROM RFC1213-MIB   
                TimeTicks		FROM SNMPv2-SMI
	            TruthValue, RowStatus           FROM SNMPv2-TC
                extremeAgent    FROM EXTREME-BASE-MIB
		extremeV2Traps		FROM EXTREME-BASE-MIB;



        extremeEnhDosMib MODULE-IDENTITY
                LAST-UPDATED "0401020000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION "Extreme Enhanced Dos protect objects information"
        ::= { extremeAgent 29 }

        extremeEnhDosProtect OBJECT IDENTIFIER ::= { extremeEnhDosMib 1 }


extremeEnhDosEnableRateLimit    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The Flag indicates whether Enhanced DOS protection with rate limit is enabled or disabled."
    DEFVAL { false }
    ::= { extremeEnhDosProtect 1 }

extremeEnhDosEnableIpFdb    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The Flag indicates whether Enhanced DOS protection against IPFDB thrashing is enabled or disabled."
    DEFVAL { false }
    ::= { extremeEnhDosProtect 2 }

extremeEnhDosEnableBenchMark    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The Flag indicates whether Enhanced DOS protection with benchmarking  is enabled or disabled."
    DEFVAL { false }
    ::= { extremeEnhDosProtect 3 }

extremeEnhDosCacheSize    OBJECT-TYPE
    SYNTAX      INTEGER(100..262144)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The Enhanced DOS Cache Size. The number of DA/SA pairs"
    DEFVAL { 262144 }
    ::= { extremeEnhDosProtect 4 }


--------------   The DOS Port Table ------------------------------

extremeEnhDosPortTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF ExtremeEnhDosPortEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "This table contains the port wise listing of Enhanced DOS attributes."
    ::= { extremeEnhDosProtect 5 }

extremeEnhDosPortEntry       OBJECT-TYPE
    SYNTAX      ExtremeEnhDosPortEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "Information about the Dos attributes of a particular port."
    INDEX   { extremeEnhDosPortIfIndex }
    ::= { extremeEnhDosPortTable 1 }

ExtremeEnhDosPortEntry ::= SEQUENCE {
      extremeEnhDosPortIfIndex          	INTEGER,
      extremeEnhDosPortTrusted			TruthValue,
      extremeEnhDosPortAlarmState          	TruthValue,
      extremeEnhDosPortLearnLimit			INTEGER,
      extremeEnhDosPortLearnWindow         	INTEGER,
      extremeEnhDosPortAgingTime			INTEGER,
      extremeEnhDosPortRateLimitEnable		TruthValue,
      extremeEnhDosPortIpFdbEnable		TruthValue,
      extremeEnhDosPortBenchMarkEnable		TruthValue,
      extremeEnhDosPortRateLimitThreshold		INTEGER,
      extremeEnhDosPortRateLimitDropProbability	INTEGER,
      extremeEnhDosPortRateLimitLearningWindow	INTEGER,
      extremeEnhDosPortRateLimitProtocol      	INTEGER
}


extremeEnhDosPortIfIndex    OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The index for this entry."
    ::= { extremeEnhDosPortEntry 1 }

extremeEnhDosPortTrusted    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
            "Indicates whether the port is trusted or untrusted."
    DEFVAL { false }
    ::= { extremeEnhDosPortEntry 2 }

extremeEnhDosPortAlarmState    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Indicates whether the port is in alarm state or not."
    DEFVAL { false }
    ::= { extremeEnhDosPortEntry 3 }

extremeEnhDosPortLearnLimit    OBJECT-TYPE
    SYNTAX      INTEGER(1..1953125)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
            "The number of packets allowed on the port before an entry is
	created in the forwarding table."
    DEFVAL { 100 }
    ::= { extremeEnhDosPortEntry 4 }

extremeEnhDosPortLearnWindow    OBJECT-TYPE
    SYNTAX      INTEGER(1..300)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
            "The duration to be considered to reach the threshold for creating an entry
	  in the forwarding table."
    DEFVAL { 60 }
    ::= { extremeEnhDosPortEntry 5 }

extremeEnhDosPortAgingTime    OBJECT-TYPE
    SYNTAX      INTEGER(1..300)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
            "The duration to be considered for aging out entries created on this port."
    DEFVAL { 30 }
    ::= { extremeEnhDosPortEntry 6 }

extremeEnhDosPortRateLimitEnable    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
            "Indicates whether the rate limit is enabled for this port."
    DEFVAL { false }
    ::= { extremeEnhDosPortEntry 7 }

extremeEnhDosPortIpFdbEnable    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
            "Indicates whether the DOS protection against IP FDB thrashing is enabled for this port."
    DEFVAL { false }
    ::= { extremeEnhDosPortEntry 8 }


extremeEnhDosPortBenchMarkEnable    OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
            "Indicates whether the bench marking is enabled for this port."
    DEFVAL { false }
    ::= { extremeEnhDosPortEntry 9 }

extremeEnhDosPortRateLimitThreshold    OBJECT-TYPE
    SYNTAX      INTEGER(100..1953125)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
            "The number of packets allowed on the port within the learning window before the rate limit is applied."
    DEFVAL { 100 }
    ::= { extremeEnhDosPortEntry 10 }

extremeEnhDosPortRateLimitDropProbability    OBJECT-TYPE
    SYNTAX      INTEGER(5..100)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
            "The probability that the packet is discarded after the reaching the threshold."
    DEFVAL { 50 }
    ::= { extremeEnhDosPortEntry 11 }


extremeEnhDosPortRateLimitLearningWindow    OBJECT-TYPE
    SYNTAX      INTEGER(1..300)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
            "The duration to be considered after which the rate limit is applied."
    DEFVAL { 60 }
    ::= { extremeEnhDosPortEntry 12 }

extremeEnhDosPortRateLimitProtocol    OBJECT-TYPE
    SYNTAX      INTEGER {
		icmp	(1),
		all	(2)
	}
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
            "The protocol packets to be considered for rate limit filtering."
    DEFVAL { icmp }
    ::= { extremeEnhDosPortEntry 13 }


------- The DOS Port Statistics Table (READ-ONLY)-----------------

extremeEnhDosPortStatisticsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF ExtremeEnhDosPortStatisticsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "This table contains the port wise listing of DOS statistics."
    ::= { extremeEnhDosProtect 6 }

extremeEnhDosPortStatisticsEntry       OBJECT-TYPE
    SYNTAX      ExtremeEnhDosPortStatisticsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "Information about the DOS statistics of a particular port."
    INDEX   { extremeEnhDosPortStatisticsIfIndex }
    ::= { extremeEnhDosPortStatisticsTable 1 }

ExtremeEnhDosPortStatisticsEntry ::= SEQUENCE {
      extremeEnhDosPortStatisticsIfIndex 		INTEGER,
      extremeEnhDosPortStatisticsRateLimitFilteredPackets  INTEGER
}

extremeEnhDosPortStatisticsIfIndex    OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The index for this entry."
    ::= { extremeEnhDosPortStatisticsEntry 1 }

extremeEnhDosPortStatisticsRateLimitFilteredPackets    OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The number of packets filetered on this port."
    ::= { extremeEnhDosPortStatisticsEntry 2 }
  
                                                 
                  
--TRAPS MIB Definitions for ENHDOS
  
--   extremeEnhDosThresholdReached	TRAP-TYPE
--   ENTERPRISE  extremenetworks
--   VARIABLES   {extremeEnhDosPortIfIndex,extremeEnhDosPortRateLimitThreshold}
--   DESCRIPTION
--   	  "The extremeDosThresholdReached notification is generated when the
--   	  DOS threshold is crossed"
--   ::= 25

--   extremeEnhDosThresholdCleared	TRAP-TYPE
--   ENTERPRISE  extremenetworks
--   VARIABLES   {extremeEnhDosPortIfIndex,extremeEnhDosPortRateLimitThreshold}
--   DESCRIPTION
--   	  "The extremeDosThresholdCleared notification is generated when the
--   	  DOS threshold is Cleared"
--   ::= 26

                


extremeEnhDosTraps 	OBJECT IDENTIFIER
	::= { extremeV2Traps 11 }

   extremeEnhDosTrapsPrefix   OBJECT IDENTIFIER
	::= { extremeEnhDosTraps 0 }

   extremeEnhDosThresholdReached NOTIFICATION-TYPE
	OBJECTS { extremeEnhDosPortIfIndex,
		  extremeEnhDosPortRateLimitThreshold }
	STATUS current
	DESCRIPTION
		"The extremeDosThresholdReached notification is generated when
		the DOS threshold is crossed for any of the ports."
	    ::= { extremeEnhDosTrapsPrefix 1 }

    extremeEnhDosThresholdCleared NOTIFICATION-TYPE
	OBJECTS { extremeEnhDosPortIfIndex,
		  extremeEnhDosPortRateLimitThreshold }
	STATUS current
	DESCRIPTION
		"The extremeEnhDosThresholdCleared notification is generated when
		the DOS threshold is cleared for any of the ports."
	    ::= { extremeEnhDosTrapsPrefix 2 }
END

EXTREME-ENTITY-MIB DEFINITIONS ::= BEGIN

        IMPORTS
                MODULE-IDENTITY FROM SNMPv2-SMI
		OBJECT-TYPE     FROM SNMPv2-SMI
		Unsigned32         FROM SNMPv2-SMI
		entPhysicalIndex   FROM ENTITY-MIB
                extremeAgent    FROM EXTREME-BASE-MIB;

        extremeEntity MODULE-IDENTITY
                LAST-UPDATED "0409170000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION "Extreme FRU Odometer objects"
        ::= { extremeAgent 31 }


--
--    FRU Table
--

	extremeEntityFRUTable OBJECT-TYPE
             SYNTAX SEQUENCE OF ExtremeEntityFRUEntry
	     MAX-ACCESS	not-accessible
	     STATUS current
	     DESCRIPTION
		"A table containing information about each FRU in the chassis
		based on Entity MIB"
		    ::= { extremeEntity 1 }

	extremeEntityFRUEntry OBJECT-TYPE
	     SYNTAX ExtremeEntityFRUEntry
	     MAX-ACCESS not-accessible
	     STATUS current
	     DESCRIPTION
		"Entry in the table for a FRU Entity"
	     INDEX	{ entPhysicalIndex }
	     	    ::= { extremeEntityFRUTable 1 }

	ExtremeEntityFRUEntry ::= SEQUENCE {
	     extremeEntityFRUStartTime		Unsigned32,
	     extremeEntityFRUOdometer		Unsigned32,
	     extremeEntityFRUOdometerUnit	INTEGER
	}

	extremeEntityFRUStartTime OBJECT-TYPE
	     SYNTAX Unsigned32
	     MAX-ACCESS read-only
	     STATUS current
	     DESCRIPTION
		"First Recorded Start Date/Time. The units are represented
                 as the standard time_t value of the start Date/Time"
	     	   ::= { extremeEntityFRUEntry 1 }

	extremeEntityFRUOdometer OBJECT-TYPE
	     SYNTAX Unsigned32
	     MAX-ACCESS read-only
	     STATUS current
	     DESCRIPTION
		"Number of time units in service."
	     	   ::= { extremeEntityFRUEntry 2 }

	extremeEntityFRUOdometerUnit OBJECT-TYPE
	     SYNTAX INTEGER {
		days(1),
		seconds(2)
	     }
	     MAX-ACCESS read-only
	     STATUS current
	     DESCRIPTION
		"Time unit used to represent value reported by extremeEntityFRUOdometer. Depending on the underlying hardware capability, the agent implementation can choose the time-unit used to represent the Odometer value."
		  ::= { extremeEntityFRUEntry 3 }

END	





EXTREME-STACKING-MIB DEFINITIONS ::= BEGIN

        IMPORTS
                MODULE-IDENTITY FROM SNMPv2-SMI
		OBJECT-TYPE     FROM SNMPv2-SMI
		NOTIFICATION-TYPE FROM SNMPv2-SMI
		Unsigned32	FROM SNMPv2-SMI
		IpAddress         FROM SNMPv2-SMI
		MacAddress	FROM SNMPv2-TC
		sysUpTime, sysDescr, ifIndex, DisplayString   FROM RFC1213-MIB
		TruthValue	FROM SNMPv2-TC
                extremeAgent    FROM EXTREME-BASE-MIB
		extremeCurrentTemperature	FROM EXTREME-SYSTEM-MIB;

        extremeStackable MODULE-IDENTITY
                LAST-UPDATED "0409270000Z"
                ORGANIZATION "Extreme Networks, Inc."
                CONTACT-INFO "www.extremenetworks.com"
                DESCRIPTION "Extreme Stackable MIB objects"
        ::= { extremeAgent 33 }

-- 
-- Stack Detection Scalar 
--
	extremeStackDetection OBJECT-TYPE
             SYNTAX TruthValue
	     MAX-ACCESS	read-write
	     STATUS current
	     DESCRIPTION
		"This field provides the information as to whether the stacking
             is enabled (True) or disabled (False) for the system. The stacking
	     feature is supported from extremeware version 7.4 and above"
		    ::= { extremeStackable 1 }

--
--	StackMember Table
--

	extremeStackMemberTable OBJECT-TYPE
             SYNTAX SEQUENCE OF ExtremeStackMemberEntry
	     MAX-ACCESS	not-accessible
	     STATUS current
	     DESCRIPTION
		"A table containing information about each stack member that are
             a part of this stacking. If extremeStackDetection is not enabled,
             we wouldnt not have any rows for this table."
		    ::= { extremeStackable 2 }

	extremeStackMemberEntry OBJECT-TYPE
	     SYNTAX ExtremeStackMemberEntry
	     MAX-ACCESS not-accessible
	     STATUS current
	     DESCRIPTION
		"Entry in the table for a StackMember Entity"
	     INDEX	{ extremeStackMemberSlotId }
	     	    ::= { extremeStackMemberTable 1 }

	ExtremeStackMemberEntry ::= SEQUENCE {
	     extremeStackMemberSlotId		INTEGER,
	     extremeStackMemberType	        OBJECT IDENTIFIER,	
	     extremeStackMemberOperStatus	INTEGER,
	     extremeStackMemberRole		INTEGER,
	     extremeStackMemberEntPhysicalIndex INTEGER,
	     extremeStackMemberMACAddress       MacAddress,	
	     extremeStackMemberCurImageVersion  DisplayString,
	     extremeStackMemberPriImageVersion  DisplayString,
	     extremeStackMemberSecImageVersion  DisplayString,
	     extremeStackMemberBootRomVersion   DisplayString,
	     extremeStackMemberCurConfig	DisplayString,
	     extremeStackMemberConfigSelected	INTEGER,
	     extremeStackMemberImageSelected	INTEGER,
	     extremeStackMemberStackPriority	INTEGER,
	     extremeStackMemberMgmtIpAddress	IpAddress,
	     extremeStackMemberSysLocation      DisplayString,
             extremeStackMemberAutoConfig	TruthValue, 	  
	     extremeStackMemberStackStatus	INTEGER
	}

	extremeStackMemberSlotId OBJECT-TYPE
	     SYNTAX INTEGER(1..8)
	     MAX-ACCESS read-only
	     STATUS current
	     DESCRIPTION
		"The slot id of the stack member in the stack"
	     	   ::= { extremeStackMemberEntry 1 }

	extremeStackMemberType OBJECT-TYPE
	     SYNTAX OBJECT IDENTIFIER
	     MAX-ACCESS read-only
	     STATUS current
	     DESCRIPTION
		"The type of device of the stack member. This field reflects
 	    the individual sysOid of the member"
	     	   ::= { extremeStackMemberEntry 2 }

	extremeStackMemberOperStatus OBJECT-TYPE
	     SYNTAX INTEGER {
		up (1),
		down(2),
		mismatch (3)
	     }
	     MAX-ACCESS read-only
	     STATUS current
	     DESCRIPTION
		"The operational status of the stack member. When the stack 
	comes up, if there is a vector mismatch namely license mismatch or
	platform mismatch between the master and the member, the member
	remains in the mismatch state. Further communication with the member
	is not possible"
	     	   ::= { extremeStackMemberEntry 3 }

	extremeStackMemberRole OBJECT-TYPE
	     SYNTAX INTEGER {
		master (1),
		slave  (2)
	     }
	     MAX-ACCESS read-only
	     STATUS current
	     DESCRIPTION
		"The role of the stack member as to whether it is acting as a
	master or a slave"
	     	   ::= { extremeStackMemberEntry 4 }

	extremeStackMemberEntPhysicalIndex OBJECT-TYPE
	     SYNTAX INTEGER 
	     MAX-ACCESS read-only
	     STATUS current
	     DESCRIPTION
		"The entPhysicalIndex of the corresponding device as defined
	in the ENTITY-MIB"
	     	   ::= { extremeStackMemberEntry 5 }

	extremeStackMemberMACAddress OBJECT-TYPE
	     SYNTAX MacAddress 
	     MAX-ACCESS read-only
	     STATUS current
	     DESCRIPTION
		"The Mac address of the stack member"
	     	   ::= { extremeStackMemberEntry 6 }

	extremeStackMemberCurImageVersion OBJECT-TYPE
	     SYNTAX DisplayString (SIZE(0..255)) 
	     MAX-ACCESS read-only
	     STATUS current
	     DESCRIPTION
		"The current image version of the stack member"
	     	   ::= { extremeStackMemberEntry 7 }

	extremeStackMemberPriImageVersion OBJECT-TYPE
	     SYNTAX DisplayString (SIZE(0..255)) 
	     MAX-ACCESS read-only
	     STATUS current
	     DESCRIPTION
		"The primary image version of the stack member"
	     	   ::= { extremeStackMemberEntry 8 }

	extremeStackMemberSecImageVersion OBJECT-TYPE
	     SYNTAX DisplayString (SIZE(0..255)) 
	     MAX-ACCESS read-only
	     STATUS current
	     DESCRIPTION
		"The secondary image version of the stack member"
	     	   ::= { extremeStackMemberEntry 9 }

	extremeStackMemberBootRomVersion OBJECT-TYPE
	     SYNTAX DisplayString (SIZE(0..255)) 
	     MAX-ACCESS read-only
	     STATUS current
	     DESCRIPTION
		"The boot rom version of the stack member"
	     	   ::= { extremeStackMemberEntry 10 }

	extremeStackMemberCurConfig OBJECT-TYPE
	     SYNTAX DisplayString (SIZE(0..255)) 
	     MAX-ACCESS read-only
	     STATUS current
	     DESCRIPTION
		"The current configuration of the stack member"
	     	   ::= { extremeStackMemberEntry 11 }

	extremeStackMemberConfigSelected OBJECT-TYPE
	     SYNTAX INTEGER {
		primary   (1),
		secondary (2)
	     }
	     MAX-ACCESS read-only
	     STATUS current
	     DESCRIPTION
		"The config selected to be used on reboot for the stack member"
	     	   ::= { extremeStackMemberEntry 12 }

	extremeStackMemberImageSelected OBJECT-TYPE
	     SYNTAX INTEGER {
		primary   (1),
		secondary (2)
	     }
	     MAX-ACCESS read-only
	     STATUS current
	     DESCRIPTION
		"The  image selected to be used on reboot for the stack member"
	     	   ::= { extremeStackMemberEntry 13 }

	extremeStackMemberStackPriority OBJECT-TYPE
	     SYNTAX INTEGER 
	     MAX-ACCESS read-only
	     STATUS current
	     DESCRIPTION
		"The stack priority of the stack member. The stack priority is
	used for the master election algorithm. The member with the highest 
	priority comes up as the master. If there are more than one switch with
	highest priority, the member with the least MAC among them comes up as
	the master"
	     	   ::= { extremeStackMemberEntry 14 }

	extremeStackMemberMgmtIpAddress OBJECT-TYPE
	     SYNTAX IpAddress 
	     MAX-ACCESS read-only
	     STATUS current
	     DESCRIPTION
		"The fallback mgmt ip address which was configured through CLI
	for this stack member. This ipaddress can be used to communicate with 
	this member, if it comes up as the master. The ipaddress is associated
	with the vlan configured"
	     	   ::= { extremeStackMemberEntry 15 }

	extremeStackMemberSysLocation OBJECT-TYPE
	      SYNTAX      DisplayString (SIZE (0..255))
              MAX-ACCESS  read-write
              STATUS      current
              DESCRIPTION
                  "The physical location of this node (e.g., `telephone
        closet, 3rd floor').  If the location is unknown, the value
        is the zero-length string."
	     	   ::= { extremeStackMemberEntry 16 }

	extremeStackMemberAutoConfig OBJECT-TYPE
	     SYNTAX TruthValue
	     MAX-ACCESS read-only
	     STATUS 	current
	     DESCRIPTION
		   " This field provides the information whether the config
	of the stack member is autogenerated(true) or not(false)" 
	     	   ::= { extremeStackMemberEntry 17 }
			

	extremeStackMemberStackStatus OBJECT-TYPE
	     SYNTAX INTEGER {
		enable  (1),
		disable (2)
	     } 
	     MAX-ACCESS read-write
	     STATUS current
	     DESCRIPTION
		"This status is used for disabling the stacking feature for
	the stack member. If stacking is enabled for the stack member we get
	the information as enable, if we mark it as disable, the stack member
	is removed from the stack and the corresponding row disappears"
	     	   ::= { extremeStackMemberEntry 18 }

--
--  	Stacking Port Table
--
	extremeStackingPortTable OBJECT-TYPE
             SYNTAX SEQUENCE OF ExtremeStackingPortEntry
	     MAX-ACCESS	not-accessible
	     STATUS current
	     DESCRIPTION
		"A table containing information about each stacking port
	in the stack. If extremeStackDetection is not enabled, we would not
	have any rows for this table"
		    ::= { extremeStackable 3 }

	extremeStackingPortEntry OBJECT-TYPE
	     SYNTAX ExtremeStackingPortEntry
	     MAX-ACCESS not-accessible
	     STATUS current
	     DESCRIPTION
		"Entry in the table for each stacking port in the stack"
	     INDEX	{ extremeStackingPortIfIndex }
	     	    ::= { extremeStackingPortTable 1 }

	ExtremeStackingPortEntry ::= SEQUENCE {
	     extremeStackingPortIfIndex		INTEGER,
	     extremeStackingPortRemoteMac       MacAddress,
	     extremeStackingPortLinkSpeed	Unsigned32,
	     extremeStackingPortLinkStatus	INTEGER
	}

          extremeStackingPortIfIndex OBJECT-TYPE
              SYNTAX  INTEGER(1..65535)
              MAX-ACCESS  read-only
              STATUS  current
              DESCRIPTION
                      "A unique value for each interface.  Its value
                      ranges between 1 and the value of ifNumber.  The
                      value for each interface must remain constant at
                      least from one re-initialization of the entity's
                      network management system to the next re-
                      initialization."
	     	   ::= { extremeStackingPortEntry 1 }

	extremeStackingPortRemoteMac OBJECT-TYPE
	     SYNTAX MacAddress 
	     MAX-ACCESS read-only
	     STATUS current
	     DESCRIPTION
		"The Mac address of the remote system, this stacking port 
	is connected to. The value of the mac address will be 00:00:00:00:00:00
	if the stacking link is not active."
	     	   ::= { extremeStackingPortEntry 2 }

	extremeStackingPortLinkSpeed OBJECT-TYPE
	     SYNTAX Unsigned32 
	     MAX-ACCESS read-only
	     STATUS current
	     DESCRIPTION
		"The Speed of the stacking port link in bps. The speed will be
	zero if the link is not up"
	     	   ::= { extremeStackingPortEntry 3 }

	extremeStackingPortLinkStatus OBJECT-TYPE
	     SYNTAX INTEGER {
		up (1),
		down  (2) 
	    } 
	     MAX-ACCESS read-only
	     STATUS current
	     DESCRIPTION
		"The Link status of the stacking port link "
	     	   ::= { extremeStackingPortEntry 4 }


    extremeStackableTraps     OBJECT IDENTIFIER
		    ::= { extremeStackable 4 }

	extremeStackTrapsPrefix     OBJECT IDENTIFIER
            ::= { extremeStackableTraps 0 }

    extremeStackMemberOverheat NOTIFICATION-TYPE
            OBJECTS {sysUpTime, sysDescr, extremeCurrentTemperature,
			extremeStackMemberSlotId}
            STATUS  current
            DESCRIPTION
                    "The extremeStackMemberOverheat notification is generated
                     when the temperature of the stack member reaches the 
		threshold temperature"
                ::= { extremeStackTrapsPrefix 1 }

    extremeStackMemberStatusChanged NOTIFICATION-TYPE
            OBJECTS { extremeStackMemberSlotId, extremeStackMemberOperStatus}
            STATUS  current
            DESCRIPTION
                    "The extremeStackMemberStatusChanged notification is 
		generated when the operational status of the stack member 
		changes"
                ::= { extremeStackTrapsPrefix 2 }

    extremeStackingPortStatusChanged NOTIFICATION-TYPE
            OBJECTS { ifIndex, extremeStackingPortRemoteMac,
		extremeStackingPortLinkSpeed, extremeStackingPortLinkStatus}
            STATUS  current
            DESCRIPTION
                    "The extremeStackingPortStatusChanged notification is 
		generated when the operational status of the stacking port 
		changes"
                ::= { extremeStackTrapsPrefix 3 }


END	
