FOUNDRY-SN-MAC-AUTHENTICATION-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Integer32
      FROM SNMPv2-SMI
    MacAddress, TimeStamp
      FROM SNMPv2-TC
    InterfaceIndex
      FROM IF-MIB;


snMacAuth MODULE-IDENTITY
    LAST-UPDATED "201006020000Z"  -- 04 June 2010
    ORGANIZATION "Brocade Communications Systems, Inc."
    CONTACT-INFO
             "Technical Support Center
              130 Holger Way,
              San Jose, CA  95134
              Email:  ipsupport@brocade.com
              Phone: 1-800-752-8061
              URL:  www.brocade.com"
    DESCRIPTION
             "Management Information Base module for MAC authentication
              configuration and statistics.

              Copyright 1996-2010 Brocade Communications Systems, Inc.
              All rights reserved.
              This Brocade Communications Systems SNMP Management Information Base Specification
              embodies Brocade Communications Systems' confidential and proprietary
              intellectual property. Brocade Communications Systems retains all
              title and ownership in the Specification, including any revisions.

              This Specification is supplied AS IS, and Brocade Communications Systems makes
              no warranty, either express or implied, as to the use,
              operation, condition, or performance of the specification, and any unintended
              consequence it may on the user environment."

    REVISION        "201006020000Z"  -- 04 June 2010
    DESCRIPTION
        "Changed the ORGANIZATION, CONTACT-INFO and DESCRIPTION fields."

    REVISION     "200706250000Z" -- June 25, 2007
    DESCRIPTION
            ""
   ::= { iso(1) org(3) dod(6) internet(1) private(4) enterprises(1) foundry(1991) products(1) switch(1) snSwitch(3) 28 }


-- MAC Authentication MIBs

snMacAuthGlobal		OBJECT IDENTIFIER ::= { snMacAuth 1 }

snMacAuthClearGlobalCmd OBJECT-TYPE
	SYNTAX     INTEGER { valid(0), clear(1) }
	MAX-ACCESS read-write
	STATUS     current
	DESCRIPTION
		"valid(0) - a SNMP-GET of this mib shows that it is valid command to use.
		 clear(1) - represents clear MAC Authentication table for all ports."
	::= { snMacAuthGlobal 1 }

snMacAuthGlobalConfigState OBJECT-TYPE
	SYNTAX     INTEGER { disabled(0), enabled(1) }
	MAX-ACCESS read-write
	STATUS     current
	DESCRIPTION
		"Enable/disable MAC authentication on the global level."
	::= { snMacAuthGlobal 2 }

--
-- MAC Authentication Clear Interface command Table
--

snMacAuthClearIfCmdTable OBJECT-TYPE
	SYNTAX     SEQUENCE OF SnMacAuthClearIfCmdEntry
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION
		"The status of clearing an MAC Authentication entry for an interface."
	::= { snMacAuth 2 }

snMacAuthClearIfCmdEntry OBJECT-TYPE
	SYNTAX     SnMacAuthClearIfCmdEntry
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION
		"An entry of clearing an MAC Authentication entry for an interface."
	INDEX { snMacAuthClearIfCmdIfIndex }
	::= { snMacAuthClearIfCmdTable 1 }

SnMacAuthClearIfCmdEntry ::= SEQUENCE {
    snMacAuthClearIfCmdIfIndex     InterfaceIndex,
    snMacAuthClearIfCmdAction      INTEGER
}

snMacAuthClearIfCmdIfIndex OBJECT-TYPE
    SYNTAX     InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
            "ifIndex value of the local interface on which a clear command is issued and monitored."
	::= { snMacAuthClearIfCmdEntry 1 }

snMacAuthClearIfCmdAction      OBJECT-TYPE
	SYNTAX     INTEGER { valid(0), clear(1) }
	MAX-ACCESS read-write
	STATUS     current
	DESCRIPTION
		"valid(0) - a SNMP-GET of this mib shows that it is valid command to use.
		 clear(1) - represents clearing an MAC Authentication entry for an interface."
	::= { snMacAuthClearIfCmdEntry 2 }

--
-- MAC Authentication Table
--

snMacAuthTable OBJECT-TYPE
	SYNTAX     SEQUENCE OF SnMacAuthEntry
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION
		"MAC Authentication table."
	::= { snMacAuth 3 }

snMacAuthEntry OBJECT-TYPE
	SYNTAX     SnMacAuthEntry
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION
		"An entry in the MAC Authentication table."
	INDEX { snMacAuthIfIndex, snMacAuthVlanId, snMacAuthMac }
	::= { snMacAuthTable 1 }

SnMacAuthEntry ::= SEQUENCE {
    snMacAuthIfIndex               InterfaceIndex,
    snMacAuthVlanId                Integer32,
    snMacAuthMac                   MacAddress,
    snMacAuthState                 INTEGER,
    snMacAuthTimeStamp             TimeStamp,
    snMacAuthAge                   Integer32,
    snMacAuthDot1x                 INTEGER
}

snMacAuthIfIndex OBJECT-TYPE
    SYNTAX     InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
    	"In order to identify a particular interface, this
		object shall identify the instance of the ifIndex
		object, defined in RFC 2863."
	::= { snMacAuthEntry 1 }

snMacAuthVlanId OBJECT-TYPE
     SYNTAX     Integer32
     MAX-ACCESS not-accessible
     STATUS     current
     DESCRIPTION
        "The ID of a VLAN of which this port is a member. Port must
        be untagged. For tagged port which belongs to multiple
        VLANs, this object return 0 which is an invalid VLAN ID
        value."
     ::= { snMacAuthEntry 2 }

snMacAuthMac OBJECT-TYPE
	SYNTAX     MacAddress
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION
		"MAC Address to be authenticated."
	::= { snMacAuthEntry 3 }

snMacAuthState OBJECT-TYPE
	SYNTAX     INTEGER { authenticate(1), unauthenticate(2) }
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION
		"."
	::= { snMacAuthEntry 4 }

snMacAuthTimeStamp OBJECT-TYPE
	SYNTAX     TimeStamp
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION
		"Timestamp at which the MAC was authenticated or failed to be authenticated."
	::= { snMacAuthEntry 5 }

snMacAuthAge OBJECT-TYPE
	SYNTAX     Integer32
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION
		"Age of the mac session in which the MAC address is authenticated."
	::= { snMacAuthEntry 6 }

snMacAuthDot1x OBJECT-TYPE
	SYNTAX     INTEGER { disabled(0), enabled(1) }
	MAX-ACCESS read-only
	STATUS     current
	DESCRIPTION
		"Indicates whether the Dot1x is enabled or not."
	::= { snMacAuthEntry 7 }

--
-- MAC Authentication MAC Session Clear Table
--

snMacAuthClearMacSessionTable OBJECT-TYPE
	SYNTAX     SEQUENCE OF SnMacAuthClearMacSessionEntry
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION
		"The status of clearing an MAC Session entry indexed by a MAC address."
	::= { snMacAuth 4 }

snMacAuthClearMacSessionEntry OBJECT-TYPE
	SYNTAX     SnMacAuthClearMacSessionEntry
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION
		"An entry of clearing an MAC Session entry indexed by a MAC address."
	INDEX { snMacAuthClearMacSessionIfIndex, snMacAuthClearMacSessionMac }
	::= { snMacAuthClearMacSessionTable 1 }

SnMacAuthClearMacSessionEntry ::= SEQUENCE {
    snMacAuthClearMacSessionIfIndex InterfaceIndex,
    snMacAuthClearMacSessionMac     MacAddress,
    snMacAuthClearMacSessionAction  INTEGER
}

snMacAuthClearMacSessionIfIndex OBJECT-TYPE
    SYNTAX     InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
            "ifIndex value of the local interface on which a clear command is issued and monitored."
	::= { snMacAuthClearMacSessionEntry 1 }

snMacAuthClearMacSessionMac OBJECT-TYPE
	SYNTAX     MacAddress
	MAX-ACCESS not-accessible
	STATUS     current
	DESCRIPTION
		"An MAC Session entry indexed by a MAC address."
	::= { snMacAuthClearMacSessionEntry 2 }

snMacAuthClearMacSessionAction OBJECT-TYPE
	SYNTAX     INTEGER { valid(0), clear(1) }
	MAX-ACCESS read-write
	STATUS     current
	DESCRIPTION
		"valid(0) - a SNMP-GET of this mib shows that it is valid command to use.
		 clear(1) - represents clearing an MAC Session entry indexed by a MAC address."
	::= { snMacAuthClearMacSessionEntry 3 }

END

