-- Title:  TRANZEO  Private MIB
--          This Private MIB supports Tranzeo Sixth Generation product line.
--	Tranzeo Wireless Technologies Inc.
--	19473 Fraser Way
--	Pitt Meadows, BC
--	Canada V3Y 2V4
--	
--
--
-- Version:    0.2
-- Date:       Wednesday December 27  2006
-- Comments:   This is the first private MIB created for Tranzeo.  It will contain basic oid's not already included in MIB-II or 802.11 MIB.
--    iso(1).org(3).dod(6).internet(1).private(4).enterprises(24575).


-- Version  Date  Authors Decription
--
-- v0.1    Nov 28    MR, QA Technician
--          2006
-- v0.2    Dec 27
--		2006	   MR, QA Technician


TRANZEO-MIB DEFINITIONS ::= BEGIN

IMPORTS


     enterprises, OBJECT-TYPE
            FROM RFC1155-SMI;


tranzeo           OBJECT IDENTIFIER ::= { enterprises 24575 }
signal           	OBJECT IDENTIFIER ::= { tranzeo 1 }


rssi OBJECT-TYPE
   SYNTAX INTEGER (-110..0)
   ACCESS read-only
   STATUS mandatory
   DESCRIPTION
       "This object represents the average received signal strength on the current channel. A 0 means no wireless connection."
   ::= { signal 1 }

signallow OBJECT-TYPE
   SYNTAX INTEGER (-110..0)
   ACCESS read-only
   STATUS mandatory
   DESCRIPTION
       "This object represents the lowest received signal strength on the current channel. A 0 means no wireless connection."
   ::= { rssi 1 }

signalaverage OBJECT-TYPE
   SYNTAX INTEGER (-110..0)
   ACCESS read-only
   STATUS mandatory
   DESCRIPTION
       "This object represents the average received signal strength on the current channel. A 0 means no wireless connection."
   ::= { rssi 2 }

signalhigh OBJECT-TYPE
   SYNTAX INTEGER (-110..0)
   ACCESS read-only
   STATUS mandatory
   DESCRIPTION
       "This object represents the highest received signal strength on the current channel. A 0 means no wireless connection."
   ::= { rssi 3 }

noise OBJECT-TYPE
   SYNTAX INTEGER (-110..0)
   ACCESS read-only
   STATUS mandatory
   DESCRIPTION
       "This object represents the noise on the current channel. A 0 means no wireless connection."
   ::= { signal 2 }

noiselow OBJECT-TYPE
   SYNTAX INTEGER (-110..0)
   ACCESS read-only
   STATUS mandatory
   DESCRIPTION
       "This object represents the lowest noise on the current channel. A 0 means no wireless connection."
   ::= { noise 1 }

noiseaverage OBJECT-TYPE
   SYNTAX INTEGER (-110..0)
   ACCESS read-only
   STATUS mandatory
   DESCRIPTION
       "This object represents the average noise on the current channel. A 0 means no wireless connection."
   ::= { noise 2 }

noisehigh OBJECT-TYPE
   SYNTAX INTEGER (-110..0)
   ACCESS read-only
   STATUS mandatory
   DESCRIPTION
       "This object represents the highest noise on the current channel. A 0 means no wireless connection."
   ::= { noise 3 }


END

