
--  ============================================================================
-- Copyright (C) by  HUAWEI TECHNOLOGIES. All rights reserved.
-- 
-- Description:  
-- Reference:  
-- Version: V1.0
-- History:
-- 
-- 
-- ============================================================================

    HUAWEI-RBRP-MIB DEFINITIONS ::= BEGIN
 
        IMPORTS
            hwDatacomm            
                FROM HUAWEI-MIB            
            InterfaceIndex            
                FROM IF-MIB            
            OBJECT-GROUP, NOTIFICATION-GROUP            
                FROM SNMPv2-CONF            
            IpAddress, Integer32, Counter32, OBJECT-TYPE, MODULE-IDENTITY, 
            NOTIFICATION-TYPE            
                FROM SNMPv2-SMI            
            RowStatus, MacAddress, TEXTUAL-CONVENTION            
                FROM SNMPv2-TC;
    
    

        hwRBRPMIB MODULE-IDENTITY 
            LAST-UPDATED "200703310130Z"        -- March 31, 2007 at 01:30 GMT
            ORGANIZATION 
                "Huawei Technologies co.,Ltd."
            CONTACT-INFO 
                " R&D BeiJing, Huawei Technologies co.,Ltd.
                Huawei Bld.,NO.3 Xinxi Rd., 
                Shang-Di Information Industry Base,
                Hai-Dian District Beijing P.R. China
                Zip:100085 
                Http://www.huawei.com                                       
                E-mail:support@huawei.com "
            DESCRIPTION 
                "The MIB module for RBRP feature.                          
                RPR Bridge Redundancy Protocol (RBRP) is the protocol for detecting 
                and initializing the intersection ring configuration, and providing 
                protection for data transfer from one rpr ring to another one via 
                intersection rpr stations."
            ::= { hwDatacomm 117 }
        
    

        EnabledStatus ::= TEXTUAL-CONVENTION
            STATUS current
            DESCRIPTION 
                "A simple status value for the object."
            SYNTAX INTEGER
                {
                enabled(1),
                disabled(2)
                }
            
    

-- ----------------------------------------------------                 
        hwRBRPMibObject OBJECT IDENTIFIER ::= { hwRBRPMIB 1 }
        
        hwRBRPLocalDeviceID OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "Set the identity which distinguishes local device 
                from other devices in a specific group."
            ::= { hwRBRPMibObject 1 }
        
        hwRBRPWrapToNormalTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HWRBRPWrapToNormalEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Table contains WrapToNormalDelay information in the  ring-if ."
            ::= { hwRBRPMibObject 2 }
        
        hwRBRPWrapToNormalEntry OBJECT-TYPE
            SYNTAX HWRBRPWrapToNormalEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "An entry contains WrapToNormalDelay information of ring-if 
                in the device."
            INDEX { hwRBRPRingIfIndex }
            ::= { hwRBRPWrapToNormalTable 1 }
        
        HWRBRPWrapToNormalEntry ::=
            SEQUENCE { 
                hwRBRPRingIfIndex
                    InterfaceIndex,
                hwRBRPWrapToNormalVal
                    INTEGER
             }

        hwRBRPRingIfIndex OBJECT-TYPE
            SYNTAX InterfaceIndex
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "RPR logic interface index."
            ::= { hwRBRPWrapToNormalEntry 1 }
        
        hwRBRPWrapToNormalVal OBJECT-TYPE
            SYNTAX INTEGER (0..100)
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "This object sets WrapToNormalDelay time of ring-if."
            ::= { hwRBRPWrapToNormalEntry 11 }
        


        hwRBRPGroupCfgTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HWRBRPGroupCfgEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Table contains group based configuration information 
                for RBRP."
            ::= { hwRBRPMibObject 3 }
        

        hwRBRPGroupCfgEntry OBJECT-TYPE
            SYNTAX HWRBRPGroupCfgEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "An entry, which contains configuration information for
                a specific group, is created for each group in the device
                and deleted when the device exit the group."
            INDEX { hwRBRPGroupCfgGroupID }
            ::= { hwRBRPGroupCfgTable 1 }
        
        HWRBRPGroupCfgEntry ::=
            SEQUENCE { 
                hwRBRPGroupCfgGroupID
                    Integer32,
                hwRBRPPriorityValue
                    INTEGER,
                hwRBRPPreemptedEnable
                    EnabledStatus,
                hwRBRPStatePromptSwitchEnable
                    EnabledStatus,
                hwRBRPPreemptDelayValue
                    Integer32,
                hwRBRPGroupCfgRowStatus
                    RowStatus
             }


        hwRBRPGroupCfgGroupID OBJECT-TYPE
            SYNTAX Integer32 (1..255)
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This object distinguishes a specific group from other 
                groups in the device."
            ::= { hwRBRPGroupCfgEntry 1 }
        

        hwRBRPPriorityValue OBJECT-TYPE
            SYNTAX INTEGER (0..255)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object indicates the device's priority which 
                determines the status of a device in a specific group.
                The non-unready device with the largest priority value 
                is in active status.
                When a device's priority is equal to another device's,
                the DeviceId will be the determining factor of a device's
                status."
            DEFVAL { 100 }
            ::= { hwRBRPGroupCfgEntry 11 }
        

        hwRBRPPreemptedEnable OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "If PreemptedEnable is configured in a device which is
                in active status in a specific group, its status could
                be preempted by device with larger priority value."
            DEFVAL { disabled }
            ::= { hwRBRPGroupCfgEntry 12 }
        

        hwRBRPStatePromptSwitchEnable OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "If StatePromptSwitchEnable is configured on a common station which 
                belongs to a specific group, The common station moves from standby 
                state to active state  promptly when multiple-site faults occur to 
                the primary ring."
            DEFVAL { disabled }
            ::= { hwRBRPGroupCfgEntry 13 }
        

        hwRBRPPreemptDelayValue OBJECT-TYPE
            SYNTAX Integer32 (60..1200)
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "This object is used to set the delay for the station moving from the active state
                to the ready state after preempted."
            DEFVAL { 120 }
            ::= { hwRBRPGroupCfgEntry 14 }
        

        hwRBRPGroupCfgRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "RowStatus, Now support three value:CreateAndGo,Active,Destroy."
            ::= { hwRBRPGroupCfgEntry 51 }
        

        hwRBRPPGRingIfCfgTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwRBRPPGRingIfCfgEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Table contains configuration information of ring-if in
                specific group."
            ::= { hwRBRPMibObject 4 }
        

        hwRBRPPGRingIfCfgEntry OBJECT-TYPE
            SYNTAX HwRBRPPGRingIfCfgEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "An entry contains configuration information of ring-if in
                specific group."
            INDEX { hwRBRPPGGroupID, hwRBRPRingType }
            ::= { hwRBRPPGRingIfCfgTable 1 }
        
        HwRBRPPGRingIfCfgEntry ::=
            SEQUENCE { 
                hwRBRPPGGroupID
                    Integer32,
                hwRBRPRingType
                    Integer32,
                hwRBRPRGRingIfIndex
                    InterfaceIndex,
                hwRBRPGroupRowStatus
                    RowStatus
             }


        hwRBRPPGGroupID OBJECT-TYPE
            SYNTAX Integer32 (1..255)
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This object distinguishes a specific group from other 
                groups in the device."
            ::= { hwRBRPPGRingIfCfgEntry 1 }
        

        hwRBRPRingType OBJECT-TYPE
            SYNTAX Integer32 (1..2)
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This object indicates a ring-if is on the primary rpr ring
                or on the secondary rpr ring."
            ::= { hwRBRPPGRingIfCfgEntry 2 }
        

        hwRBRPRGRingIfIndex OBJECT-TYPE
            SYNTAX InterfaceIndex
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "RPR logic interface index."
            ::= { hwRBRPPGRingIfCfgEntry 11 }
        

        hwRBRPGroupRowStatus OBJECT-TYPE
            SYNTAX RowStatus
            MAX-ACCESS read-create
            STATUS current
            DESCRIPTION
                "RowStatus, Now support three value:CreateAndGo,Active,Destroy."
            ::= { hwRBRPPGRingIfCfgEntry 51 }
        

        hwRBRPPStatisTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HWRBRPPStatisEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Table contains statistics information of RBRP packets."
            ::= { hwRBRPMibObject 5 }
        

        hwRBRPPStatisEntry OBJECT-TYPE
            SYNTAX HWRBRPPStatisEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "An entry contains statistics information of RBRP packets."
            INDEX { hwRBRPStatisGroupID }
            ::= { hwRBRPPStatisTable 1 }
        
        HWRBRPPStatisEntry ::=
            SEQUENCE { 
                hwRBRPStatisGroupID
                    Integer32,
                hwRBRPStatisRevPacketsNum
                    Counter32,
                hwRBRPStatisRevByteNum
                    Counter32,
                hwRBRPStatisSendPacketsNum
                    Counter32,
                hwRBRPStatisSendByteNum
                    Counter32,
                hwRBRPClearStatisticPacket
                    EnabledStatus
             }


        hwRBRPStatisGroupID OBJECT-TYPE
            SYNTAX Integer32 (1..255)
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This object distinguishes a specific group from other 
                groups in the device."
            ::= { hwRBRPPStatisEntry 1 }
        

        hwRBRPStatisRevPacketsNum OBJECT-TYPE
            SYNTAX Counter32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the number of RBRP packets received 
                from a specific group."
            ::= { hwRBRPPStatisEntry 11 }
        

        hwRBRPStatisRevByteNum OBJECT-TYPE
            SYNTAX Counter32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the number of RBRP bytes received 
                from a specific group."
            ::= { hwRBRPPStatisEntry 12 }
        

        hwRBRPStatisSendPacketsNum OBJECT-TYPE
            SYNTAX Counter32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the number of RBRP packets sendedd 
                to a specific group."
            ::= { hwRBRPPStatisEntry 13 }
        

        hwRBRPStatisSendByteNum OBJECT-TYPE
            SYNTAX Counter32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the number of RBRP bytes sendedd 
                to a specific group."
            ::= { hwRBRPPStatisEntry 14 }
        

        hwRBRPClearStatisticPacket OBJECT-TYPE
            SYNTAX EnabledStatus
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "Clear the statistics information of RBRP packets."
            ::= { hwRBRPPStatisEntry 15 }
        

        hwRBRPGroupInfoTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwRBRPGroupInfoEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "Table contains RBRP group information."
            ::= { hwRBRPMibObject 6 }
        

        hwRBRPGroupInfoEntry OBJECT-TYPE
            SYNTAX HwRBRPGroupInfoEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "An entry contains RBRP group information."
            INDEX { hwRBRPGroupID, hwRBRPDeviceId }
            ::= { hwRBRPGroupInfoTable 1 }
        
        HwRBRPGroupInfoEntry ::=
            SEQUENCE { 
                hwRBRPGroupID
                    Integer32,
                hwRBRPDeviceId
                    IpAddress,
                hwRBRPPrimaryRPRMacAddress
                    MacAddress,
                hwRBRPSecondaryRPRMacAddress
                    MacAddress,
                hwRBRPPriority
                    Integer32,
                hwRBRPCurrentStatus
                    Integer32
             }


        hwRBRPGroupID OBJECT-TYPE
            SYNTAX Integer32 (1..255)
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This object distinguishes a specific group from other 
                groups in the device."
            ::= { hwRBRPGroupInfoEntry 1 }
        

        hwRBRPDeviceId OBJECT-TYPE
            SYNTAX IpAddress
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "This object distinguishes a specific device from other 
                devices in the groups."
            ::= { hwRBRPGroupInfoEntry 2 }
        

        hwRBRPPrimaryRPRMacAddress OBJECT-TYPE
            SYNTAX MacAddress
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the mac address of rpr station on the 
                primary rpr ring."
            ::= { hwRBRPGroupInfoEntry 11 }
        

        hwRBRPSecondaryRPRMacAddress OBJECT-TYPE
            SYNTAX MacAddress
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the mac address of rpr station on the 
                secondary rpr ring."
            ::= { hwRBRPGroupInfoEntry 12 }
        

        hwRBRPPriority OBJECT-TYPE
            SYNTAX Integer32 (0..255)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the priority of a device
                in specific group."
            ::= { hwRBRPGroupInfoEntry 13 }
        

        hwRBRPCurrentStatus OBJECT-TYPE
            SYNTAX Integer32 (1..4)
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "This object indicates the status of a device 
                in specific group.
                Now support four state:Unready, Ready, Standby, and Active."
            ::= { hwRBRPGroupInfoEntry 14 }
        

        hwRBRPTraps OBJECT IDENTIFIER ::= { hwRBRPMIB 2 }
        

        hwRBRPDeviceIDConflict NOTIFICATION-TYPE
            OBJECTS { hwRBRPCurrentStatus }
            STATUS current
            DESCRIPTION 
                "The device id conflict defect.
                When a device id conflict defect is present,
                a notification may be generated."
            ::= { hwRBRPTraps 1 }
        

        hwRBRPUnreadyStatus NOTIFICATION-TYPE
            OBJECTS { hwRBRPPreemptedEnable }
            STATUS current
            DESCRIPTION 
                "The Unready status defect.
                When an Unready status defect is present,
                a notification may be generated."
            ::= { hwRBRPTraps 2 }
        

        hwRBRPClearUnreadyStatus NOTIFICATION-TYPE
            OBJECTS { hwRBRPPreemptedEnable }
            STATUS current
            DESCRIPTION 
                "The Unready status restore.
                When a Ready status is present,
                a notification may be generated."
            ::= { hwRBRPTraps 3 }
        

        hwRBRPConformance OBJECT IDENTIFIER ::= { hwRBRPMIB 3 }
        

        hwRBRPGroups OBJECT IDENTIFIER ::= { hwRBRPConformance 1 }
        

        hwRBRPLoclaDeveceIDGroup OBJECT-GROUP
            OBJECTS { hwRBRPLocalDeviceID }
            STATUS current
            DESCRIPTION 
                "Description."
            ::= { hwRBRPGroups 1 }
        

        hwRBRPWrapToNormalGroup OBJECT-GROUP
            OBJECTS { hwRBRPWrapToNormalVal }
            STATUS current
            DESCRIPTION 
                "Description."
            ::= { hwRBRPGroups 2 }
        

        hwRBRPGroupCfgGroup OBJECT-GROUP
            OBJECTS { hwRBRPPriorityValue, hwRBRPPreemptDelayValue, hwRBRPGroupCfgRowStatus, hwRBRPStatePromptSwitchEnable, hwRBRPPreemptedEnable
                 }
            STATUS current
            DESCRIPTION 
                "Description."
            ::= { hwRBRPGroups 3 }
        

        hwRBRPPGRingIfCfgGroup OBJECT-GROUP
            OBJECTS { hwRBRPRGRingIfIndex, hwRBRPGroupRowStatus }
            STATUS current
            DESCRIPTION 
                "Description."
            ::= { hwRBRPGroups 4 }
        

        hwRBRPPStatisGroup OBJECT-GROUP
            OBJECTS { hwRBRPStatisRevPacketsNum, hwRBRPStatisRevByteNum, hwRBRPStatisSendPacketsNum, hwRBRPStatisSendByteNum, hwRBRPClearStatisticPacket
                 }
            STATUS current
            DESCRIPTION 
                "Description."
            ::= { hwRBRPGroups 5 }
        

        hwRBRPGroupInfoGroup OBJECT-GROUP
            OBJECTS { hwRBRPCurrentStatus, hwRBRPPriority, hwRBRPSecondaryRPRMacAddress, hwRBRPPrimaryRPRMacAddress }
            STATUS current
            DESCRIPTION 
                "Description."
            ::= { hwRBRPGroups 6 }
        

        hwRBRPTrapGroup NOTIFICATION-GROUP
            NOTIFICATIONS { hwRBRPClearUnreadyStatus, hwRBRPDeviceIDConflict, hwRBRPUnreadyStatus }
            STATUS current
            DESCRIPTION 
                "Description."
            ::= { hwRBRPGroups 7 }
        
    
    END

--
-- HUAWEI-RBRP-MIB.my
--
