
-- *****************************************************************************
-- Juniper-IP-MIB
--
-- Juniper Networks Enterprise MIB
--   Extensions for IP Protocol Management
--
-- Copyright (c) 1998, 1999 Redstone Communications, Inc.
-- Copyright (c) 1999, 2002 Unisphere Networks, Inc.
-- Copyright (c) 2002-2008 Juniper Networks, Inc.
--   All Rights Reserved.
-- *****************************************************************************

Juniper-IP-MIB  DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Integer32, NOTIFICATION-TYPE, Unsigned32, IpAddress, Counter64,
    Gauge32
        FROM SNMPv2-SMI
    TruthValue, RowStatus
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF
    InterfaceIndex, InterfaceIndexOrZero, ifIndex
        FROM IF-MIB
    ipCidrRouteEntry
        FROM IP-FORWARD-MIB
    ipCidrRouteNumber
        FROM IP-FORWARD-MIB
    juniMibs
        FROM Juniper-MIBs
    JuniEnable, JuniIpAddrLessIf, JuniNextIfIndex
        FROM Juniper-TC;


juniIpMIB  MODULE-IDENTITY
    LAST-UPDATED "200701172302Z"  -- 17-Jan-07 06:02 PM EST
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
        "       Juniper Networks, Inc.
        Postal: 10 Technology Park Drive
                Westford, MA  01886-3146
                USA
        Tel:    +1 978 589 5800
        E-mail: mib@Juniper.net"
    DESCRIPTION
        "The IP Protocol MIB for the Juniper Networks enterprise."
    -- Revision History                                     
    REVISION    "200701172302Z"  -- 17-Jan-07 06:02 PM EST  - JUNOSe 7.3.2
    DESCRIPTION
        "Added warm-restart replay initial sequence preference for an IP
        interface by adding juniIpIfInitSeqPrefOper and juniIpIfInitSeqPrefAdmin."
    REVISION    "200503301349Z"  -- 30-Mar-05 01:49 PM IST  - JUNOSe 7.0
    DESCRIPTION
         "Added IP Route Summary support for Unicast and Multicast Routes."
    REVISION    "200504292037Z"  -- 29-Apr-05 04:37 PM EDT  - JUNOSe 7.0
    DESCRIPTION
         "Added RLI-1925 Source Address Validation Failure Traps support."
    REVISION    "200409201349Z"  -- 20-Sep-04 09:49 AM EDT  - JUNOSe 6.1
    DESCRIPTION
         "Added RLI-1684 Route Table Maximum Route support."
    REVISION    "200409101526Z"  -- 04-Sep-10 10:26 AM EST  - JUNOSe 6.0
    DESCRIPTION
	"Obsoleted the following objects:
	   juniIpVpnIdOui
	   juniIpVpnIdIndex"
    REVISION    "200311031526Z"  -- 03-Nov-03 10:26 AM EST  - JUNOSe 5.2
    DESCRIPTION
        "Added support to juniIpIfEntry for TCP MSS configuration."
    REVISION    "200306251948Z"  -- 25-Jun-03 03:48 PM EDT  - JUNOSe 5.1
    DESCRIPTION
        "Added IP interface summary statistics support - juniIpIfSummary.
         Added support for Interface Mirroring by adding juniIpIfAnalyzerMode.
         Added support to juniIpIfEntry for IP interface auto configure."
    REVISION    "200302111905Z"  -- 11-Feb-03 02:05 PM EST  - JUNOSe 5.0
    DESCRIPTION
        "Replaced Unisphere names with Juniper names.
         In juniIpInterfaceGroup, added juniIpIfRouterIndex
         In juniIpIfTable, to support unnumbered interfaces referencing numbered
         interfaces in addition to loopback interfaces, the following objects
         were deprecated:
            juniIpIfLoopback
            juniIpIfLoopbackUid
         and the following objects were added:
            juniIpIfInheritNum
            juniIpIfInheritNumUid
         In juniIpAddrTable, to support unnumbered interfaces referencing
         numbered interfaces in addition to loopback interfaces, the following
         object was deprecated:
            juniIpAdEntUnnumLoopbackIfIndex
         and the following object was added:
            juniIpAdEntUnnumInheritNumIfIndex
         Added new types to juniIpIfType."
    REVISION    "200210231853Z"  -- 23-Oct-02 02:53 PM EDT  - JUNOSe 4.1
    DESCRIPTION
        "Added the following scalar objects:
            juniIpBgpCommunityNewFormat
            juniIpBgpAsConfedSetNewFormat
         Obsoleted the following objects:
            juniIpArpTimeout
            juniIpRouteLimit "
    REVISION    "200204032206Z"  -- 03-Apr-02 05:06 PM EST  - JUNOSe 4.0
    DESCRIPTION
        "Obsoleted the following objects with the introduction of QoS:
            juniIpIfStatsInForwardedPackets
            juniIpIfStatsInForwardedOctets
            juniIpIfStatsOutRequestedPackets
            juniIpIfStatsOutRequesteOctets
            juniIpIfStatsGreenOutSchedDropPackets
            juniIpIfStatsYellowOutSchedDropPackets
            juniIpIfStatsRedOutSchedDropOctets
            juniIpIfStatsGreenOutSchedDropOctets
            juniIpIfStatsYellowOutSchedDropOctets
            juniIpIfStatsRedOutSchedDropOctet "
    REVISION    "200107051400Z"  -- 05-Jul-01 10:00 AM EDT  - JUNOSe 3.2
    DESCRIPTION
        "Added the juniIpIfAssocTable."
    REVISION    "200106181911Z"  -- 18-Jun-01 03:11 PM EDT  - JUNOSe 3.0
    DESCRIPTION
        "o In juniIpIfTable, added the following:
            juniIpIfSAValidation
            juniIpIfCreationType
            juniIpIfProfileId
            juniIpIfAlwaysUp
            juniIpIfLoopback
            juniIpIfLoopbackUid
            juniIpIfDebounceTime
            juniIpIfForwarding
            juniIpIfForceFragmentation
            juniIpIfSharesLowerUid
            juniIpIfFilterOptions
            juniIpIfName
            juniIpIfArpTimeout
            juniIpIfAdminSpeed
            juniIpIfMultipathMode
            juniIpIfSharedNhAddr
            juniIpIfSharedNhRouterId
            juniIpIfPrimaryIpAddress
            juniIpIfPrimaryIpMask
            juniIpIfOperDebounceTime
         o In juniIpAddrTable, added juniIpAdEntIsSecondary
         o In juniIpAddrTable, deprecated juniIpAdEntIgmpEnable
         o Added following scalars:
            juniIpDebounceTime
            juniIpRouterId
            juniIpSourceRoutingAdminStatus
            juniIpVpnIdOui
            juniIpVpnIdIndex
         o In juniIpIfStatsTable, added:
            juniIpIfStatsGreenOutSchedDropPackets
            juniIpIfStatsYellowOutSchedDropPackets
            juniIpIfStatsRedOutSchedDropPackets
            juniIpIfStatsGreenOutSchedDropOctets
            juniIpIfStatsYellowOutSchedDropOctets
            juniIpIfStatsRedOutSchedDropOctets
         o Changed the type of juniIpRouteStaticNextHop to JuniIpAddrLessIf to
           support setting static routes next hop values to unnumbered IP
           interfaces.  This type is a Juniper TC, which can transparently
           support the original IpAddress type, so existing clients are not
           negatively affected by this change."
    REVISION    "200007310000Z"  -- 31-Jul-00               - JUNOSe 2.2
    DESCRIPTION
        "o Added extended IP interface statistics."
    REVISION      "9911090000Z"  --  9-Nov-99               - JUNOSe 1.3
    DESCRIPTION
        "o In juniIpIfTable, added null(5) enumeration value for juniIpIfType.
         o Added juniIpIfTypeId object."
    REVISION      "9909160000Z"  -- 16-Sep-99               - JUNOSe 1.1
    DESCRIPTION
        "o In juniIpAddrTable, added juniIpAdEntUnnumLoopbackIfIndex,
           juniIpAdEntIrdpEnable, juniIpAdEntAccessRouteEnable,
           juniIpAdEntAccessRouteHost.
         o In juniIpRouteStaticTable, changed Tos to Preference, and added Tag.
         o Added juniIpCidrRouteTable (proprietary extensions to standard
           ipCidrRouteTable)."
    REVISION      "9811190000Z"  -- 19-Nov-98               - JUNOSe 1.0
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { juniMibs 12 }
   
 
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Managed objects
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniIpObjects     OBJECT IDENTIFIER ::= { juniIpMIB 1 }

juniIpInterface   OBJECT IDENTIFIER ::= { juniIpObjects 1 }
juniIpAddress     OBJECT IDENTIFIER ::= { juniIpObjects 2 }
juniIpRoute       OBJECT IDENTIFIER ::= { juniIpObjects 3 }
juniIpGlobals     OBJECT IDENTIFIER ::= { juniIpObjects 4 }
juniIpIfSummary   OBJECT IDENTIFIER ::= { juniIpObjects 5 }
juniIpRouteSummary   OBJECT IDENTIFIER ::= { juniIpObjects 6 }

-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- IP Global attributes
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniIpDebounceTime  OBJECT-TYPE
    SYNTAX      Integer32 (0..60000)
    UNITS       "milliseconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The time in milliseconds that an event has to be in the same state
        before being reported."
    DEFVAL    { 0 }
    ::= { juniIpGlobals 1 }

juniIpRouterId  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The router-id that this IP router will use to identify itself."
    ::= { juniIpGlobals 2 }

juniIpSourceRoutingAdminStatus  OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The administrative setting for source routing."
    ::= { juniIpGlobals 3 }

juniIpVpnIdOui  OBJECT-TYPE
    SYNTAX      Integer32 (0..16777215)
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "The OUI portion of the VPN identifier.  This object must be set
        coincident with the index portion of the VpnId (juniIpVpnIdIndex),
        otherwise the set will fail."
    ::= { juniIpGlobals 4 }

juniIpVpnIdIndex  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "The index portion of the VPN identifier.  This object must be set
         coincident with the OUI portion of the VpnId (juniIpVpnOui), otherwise
         the set will fail."
    ::= { juniIpGlobals 5 }

juniIpBgpCommunityNewFormat  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The BGP community format to be used.  Set to true to use the community
        number, as number format."
    DEFVAL    { false }
    ::= { juniIpGlobals 6 }

juniIpBgpAsConfedSetNewFormat  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The BGP as confederation set format to be used.  Set to true to display
        the confederation set as a comma separated list, enclosed in squared
        braces."
    DEFVAL    { false }
    ::= { juniIpGlobals 7 }

-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- IP Interface Summary Statistics Attributes
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniIpIfSummaryTotalIntf  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IP interfaces."
    ::= { juniIpIfSummary 1 }

juniIpIfSummaryTotalIntfUp  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IP interfaces in operational state UP."
    ::= { juniIpIfSummary 2 }

juniIpIfSummaryTotalIntfDown  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IP interfaces in operational state DOWN."
    ::= { juniIpIfSummary 3 }

juniIpIfSummaryTotalIntfProtUp  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IP interfaces in protocol state UP."
    ::= { juniIpIfSummary 4 }

juniIpIfSummaryTotalIntfProtDown  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IP interfaces in protocol state DOWN."
    ::= { juniIpIfSummary 5 }

juniIpIfSummaryTotalIntfProtNotPresent  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IP interfaces in protocol state NOT PRESENT."
    ::= { juniIpIfSummary 6 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- IP Route Summary Statistics Attributes
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniIpRouteUnicastSummary   OBJECT IDENTIFIER ::= { juniIpRouteSummary 1 }
juniIpRouteMulticastSummary   OBJECT IDENTIFIER ::= { juniIpRouteSummary 2 }

-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- IP Route Unicast Summary Statistics Attributes
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++

juniIpRouteSummaryUnicastTotalRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Unicast IP routes."
    ::= { juniIpRouteUnicastSummary 1 }

juniIpRouteSummaryUnicastTotalBytes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Total number of bytes in unicast route entries."
    ::= { juniIpRouteUnicastSummary  2 }

juniIpRouteSummaryUnicastIsisRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Unicast IP ISIS routes."
    ::= { juniIpRouteUnicastSummary  3 }

juniIpRouteSummaryUnicastIsisLevel1Routes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Unicast IP Level 1 ISIS routes."
    ::= { juniIpRouteUnicastSummary  4 }                       
    

juniIpRouteSummaryUnicastIsisLevel2Routes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Unicast IP Level 2 ISIS routes."
    ::= { juniIpRouteUnicastSummary  5 }


juniIpRouteSummaryUnicastRipRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Unicast IP RIP routes."
    ::= { juniIpRouteUnicastSummary  6 }

juniIpRouteSummaryUnicastStaticRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION                   
        "The total number of Unicast IP Static routes."
    ::= { juniIpRouteUnicastSummary  7 }


juniIpRouteSummaryUnicastConnectedRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Unicast IP Connected routes."
    ::= { juniIpRouteUnicastSummary  8 }     
    
juniIpRouteSummaryUnicastBgpRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Unicast IP BGP routes."
    ::= { juniIpRouteUnicastSummary  9 }

juniIpRouteSummaryUnicastOspfRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Unicast IP OSPF routes."
    ::= { juniIpRouteUnicastSummary  10 }

juniIpRouteSummaryUnicastIntraAreaOspfRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Unicast IP Intra Area OSPF routes."
    ::= { juniIpRouteUnicastSummary  11 }
                                 

juniIpRouteSummaryUnicastInterAreaOspfRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Unicast IP Inter Area OSPF routes."
    ::= { juniIpRouteUnicastSummary  12 }
    
juniIpRouteSummaryUnicastExternalOspfRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Unicast IP External OSPF routes."
    ::= { juniIpRouteUnicastSummary  13 }
    
                                         
juniIpRouteSummaryUnicastOtherInternalRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Unicast IP Other Internal routes."
    ::= { juniIpRouteUnicastSummary  14}

juniIpRouteSummaryUnicastAccessRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Unicast IP Access routes."
    ::= { juniIpRouteUnicastSummary  15 }    
    
juniIpRouteSummaryUnicastIntCreatedAccessHostRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Unicast IP Internally Created Access Host routes."
    ::= { juniIpRouteUnicastSummary  16 }
                                          
juniIpRouteSummaryUnicastIntDialoutRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Unicast IP Internally Created Dialout routes."
    ::= { juniIpRouteUnicastSummary  17 }
       
juniIpRouteSummaryUnicastRouteMemoryActive  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Unicast IP Route Memory Storage."
    ::= { juniIpRouteUnicastSummary  18 }
                                          
juniIpRouteSummaryUnicastLastRouteAddedOrDeletedIP  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
 		"IP address for last Unicast route added or deleted."
    ::= { juniIpRouteUnicastSummary  19 }

juniIpRouteSummaryUnicastLastRouteAddedOrDeletedMask  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Subnet mask for last Unicast route added or deleted."
    ::= { juniIpRouteUnicastSummary  20 }

juniIpRouteSummaryUnicastLastRouteAddedOrDeletedClient  OBJECT-TYPE
    SYNTAX      INTEGER { 
    				inValid(0),
                    isis(1),
                    rip(2),
	        		ospf(3),
	        		static(4),
	        		local(5),
	        		bgp(6),
	        		mbgp(7),
	        		staticLow(8),
                    ospfInternal(9),
                    ospfExternal(10),
                    dvmrp(11),
                    dvmrpAggregate(12),
                    hidden(13),
                    access(14),
                    accessInternal(15),
                    dialOut(16),
                    default(17) }

    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Client for last Unicast route added or deleted."
    ::= { juniIpRouteUnicastSummary  21 }

juniIpRouteSummaryUnicastLastRouteAddedOrDeletedDate  OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(0..30))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Date for last Unicast route added or deleted."
    ::= { juniIpRouteUnicastSummary  22 }
    
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- IP Route Multicast Summary Statistics Attributes
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++

juniIpRouteSummaryMulticastTotalRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Multicast IP routes."
    ::= { juniIpRouteMulticastSummary   1 }

juniIpRouteSummaryMulticastTotalBytes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Total number of bytes in multicast route entries."
	::= { juniIpRouteMulticastSummary  2 }

juniIpRouteSummaryMulticastIsisRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Multicast IP ISIS routes."
    ::= { juniIpRouteMulticastSummary  3 }
                        
juniIpRouteSummaryMulticastLevel1IsisRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Multicast IP Level 1 ISIS routes."
    ::= { juniIpRouteMulticastSummary  4 }                        
    

juniIpRouteSummaryMulticastLevel2IsisRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Multicast IP Level 2 ISIS routes."
    ::= { juniIpRouteMulticastSummary  5 }

juniIpRouteSummaryMulticastRipRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Multicast IP RIP routes."
    ::= { juniIpRouteMulticastSummary  6 }

juniIpRouteSummaryMulticastStaticRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Multicast IP Static routes."
    ::= { juniIpRouteMulticastSummary  7 }


juniIpRouteSummaryMulticastConnectedRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Multicast IP Connected routes."
    ::= { juniIpRouteMulticastSummary  8 }

juniIpRouteSummaryMulticastBgpRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Multicast IP BGP routes."
    ::= { juniIpRouteMulticastSummary  9 }

juniIpRouteSummaryMulticastOspfRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Multicast IP OSPF routes."
    ::= { juniIpRouteMulticastSummary  10 }

juniIpRouteSummaryMulticastIntraAreaOspfRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Multicast IP Intra Area OSPF routes."
    ::= { juniIpRouteMulticastSummary  11 }
    
juniIpRouteSummaryMulticastInterAreaOspfRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Multicast IP Inter Area OSPF routes."
    ::= { juniIpRouteMulticastSummary  12 }      
    
juniIpRouteSummaryMulticastExternalOspfRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Multicast IP External OSPF routes."
    ::= { juniIpRouteMulticastSummary  13 }    
    
juniIpRouteSummaryMulticastOtherInternalRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Multicast IP Other Internal routes."
    ::= { juniIpRouteMulticastSummary  14}

juniIpRouteSummaryMulticastAccessRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Multicast IP Access routes."
    ::= { juniIpRouteMulticastSummary  15 }

juniIpRouteSummaryMulticastIntCreatedAccessHostRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Multicast IP Internally Created Access Host routes."
    ::= { juniIpRouteMulticastSummary  16 }

juniIpRouteSummaryMultiastIntDialoutRoutes  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of Multicast IP Internally Created Dialout routes."
    ::= { juniIpRouteMulticastSummary  17 }   
    
juniIpRouteSummaryMulticastRouteMemoryActive  OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Multicast IP Route Memory Storage."
    ::= { juniIpRouteMulticastSummary  18 }
    
juniIpRouteSummaryMulticastLastRouteAddedOrDeletedIP  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "IP address for last Multicast route added or deleted."
    ::= { juniIpRouteMulticastSummary  19 }

juniIpRouteSummaryMulticastLastRouteAddedOrDeletedMask  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Subnet Mask for last Multicast route added or deleted."
    ::= { juniIpRouteMulticastSummary  20 }

juniIpRouteSummaryMulticastLastRouteAddedOrDeletedClient  OBJECT-TYPE
    SYNTAX      INTEGER { 
    				inValid(0),
                    isis(1),
                    rip(2),
	        		ospf(3),
	        		static(4),
	        		local(5),
	        		bgp(6),
	        		mbgp(7),
	        		staticLow(8),
                    ospfInternal(9),
                    ospfExternal(10),
                    dvmrp(11),
                    dvmrpAggregate(12),
                    hidden(13),
                    access(14),
                    accessInternal(15),
                    dialOut(16),
                    default(17)
 	 }

    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
         "Client for last Multicast route added or deleted."   
	::= { juniIpRouteMulticastSummary  21}

juniIpRouteSummaryMulticastLastRouteAddedOrDeletedDate  OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(0..30))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
         "Date for last Multicast route added or deleted."    
	::= { juniIpRouteMulticastSummary  22} 


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- IP Interface attributes
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
--
-- IfIndex selection for creating new IP interfaces
--
juniIpNextIfIndex  OBJECT-TYPE
    SYNTAX      JuniNextIfIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Coordinate ifIndex value allocation for entries in juniIpIfTable.

        A GET of this object returns the next available ifIndex value to be used
        to create an entry in the associated interface table; or zero, if no
        valid ifIndex value is available.  This object also returns a value of
        zero when it is the lexicographic successor of a varbind presented in an
        SNMP GETNEXT or GETBULK request, for which circumstance it is assumed
        that ifIndex allocation is unintended.

        Successive GETs will typically return different values, thus avoiding
        collisions among cooperating management clients seeking to create table
        entries simultaneously.  "
    ::= { juniIpInterface 1 }


--
-- The IP Interface Table
--
juniIpIfTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIpIfEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for IP interfaces present in the system."
    ::= { juniIpInterface 2 }

juniIpIfEntry  OBJECT-TYPE
    SYNTAX      JuniIpIfEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of an IP interface.
        Creating/deleting entries in this table causes corresponding entries for
        be created/deleted in ifTable/ifXTable/juniIfTable."
    INDEX     { juniIpIfIndex }
    ::= { juniIpIfTable 1 }

JuniIpIfEntry ::= SEQUENCE {
    juniIpIfIndex                InterfaceIndex,
    juniIpIfRowStatus            RowStatus,
    juniIpIfLowerIfIndex         InterfaceIndexOrZero,
    juniIpIfType                 INTEGER,
    juniIpIfTypeId               Unsigned32,
    juniIpIfSAValidationEnable   JuniEnable,
    juniIpIfCreationType         INTEGER,
    juniIpIfProfileId            Unsigned32,
    juniIpIfAlwaysUp             JuniEnable,
    juniIpIfLoopback             JuniEnable,
    juniIpIfLoopbackUid          InterfaceIndexOrZero,
    juniIpIfDebounceTime         Integer32,
    juniIpIfForwarding           JuniEnable,
    juniIpIfForceFragmentation   JuniEnable,
    juniIpIfSharesLowerUid       JuniEnable,
    juniIpIfFilterOptions        Unsigned32,
    juniIpIfName                 OCTET STRING,
    juniIpIfArpTimeout           Unsigned32,
    juniIpIfAdminSpeed           Unsigned32,
    juniIpIfMultipathMode        INTEGER,
    juniIpIfSharedNhAddr         IpAddress,
    juniIpIfSharedNhRouterId     Unsigned32,
    juniIpIfPrimaryIpAddress     IpAddress,
    juniIpIfPrimaryIpMask        IpAddress,
    juniIpIfOperDebounceTime     Integer32,
    juniIpIfRouterIndex          Unsigned32,
    juniIpIfInheritNum           JuniEnable,
    juniIpIfInheritNumUid        InterfaceIndexOrZero,
    juniIpIfAnalyzerMode         INTEGER,
    juniIpIfAutoConfigure        JuniEnable,
    juniIpIfTcpMss               Integer32,
    juniIpIfInitSeqPrefOper      Unsigned32,
    juniIpIfInitSeqPrefAdmin     Unsigned32,
    juniIpIfArpSpoofCheck        JuniEnable }

juniIpIfIndex  OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ifIndex of the IP interface.  When creating entries in this table,
        suitable values for this object are determined by reading
        juniIpNextIfIndex."
    ::= { juniIpIfEntry 1 }

juniIpIfRowStatus  OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
            juniIpIfRowStatus
            juniIpIfLowerIfIndex

        In addition, when creating an entry the following conditions must hold:

            A value for juniIpIfIndex must have been determined previously,
            typically by reading juniIpNextIfIndex.

            The interface identified by a nonzero juniIpIfLowerIfIndex must
            exist.

            If juniIpIfType is configured to be 'loopback' or 'null',
            juniIpIfLowerIfIndex must be set to zero.

            The selected value of juniIpIfType must be compatible with the
            underlying media interface identified by juniIpIfLowerIfIndex.

        Once created, the following objects may not be modified:
            juniIpIfLowerIfIndex
            juniIpIfType
            juniIpIfTypeId

        A corresponding entry in ifTable/ifXTable/juniIfTable is created/
        destroyed as a result of creating/destroying an entry in this table."
    ::= { juniIpIfEntry 2 }

juniIpIfLowerIfIndex  OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The ifIndex of a media interface over which this IP interface is to be
        layered.  A value of zero is used when juniIpIfType is specified to be
        loopback(4) or null(5)."
    ::= { juniIpIfEntry 3 }

juniIpIfType  OBJECT-TYPE
    SYNTAX      INTEGER {
                    other(0),
                    broadcast(1),
                    pointToPoint(2),
                    nbma(3),
                    loopback(4),
                    null(5),
                    bgpMplsVpn(6),
                    vrfInternal(7),
                    dialout(8) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The type of network interface."
    DEFVAL    { pointToPoint }
    ::= { juniIpIfEntry 4 }

juniIpIfTypeId  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "A numerical distinguisher relevant for the loopback and null IP
        interface types.
            loopback    Must be unique for all IP interfaces of this type.
            null        Must be unique for all IP interfaces of this type.
                        (FOR IMPLEMENTATIONS THAT SUPPORT ONE AND ONLY ONE NULL
                        INTERFACE, THE VALUE ZERO MUST BE USED.)

        For all other IP interface types, this object is not relevant, reports a
        value of zero when read, and must be given a value of zero if explicitly
        configured during creation."
    DEFVAL    { 0 }
    ::= { juniIpIfEntry 5 }

juniIpIfSAValidationEnable  OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enable/disable source address validation on this IP network interface."
    DEFVAL    { disable }
    ::= { juniIpIfEntry 6 }

juniIpIfCreationType  OBJECT-TYPE
    SYNTAX      INTEGER {
                    static(1),
                    dynamic(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specify if the interface was created due to static configuration or due
        to some dynamic event.  Dynamic interfaces are not stored in NVS."
    ::= { juniIpIfEntry 7 }

juniIpIfProfileId  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Identified the profile used when creating a dynamic interface."
    DEFVAL    { 0 }
    ::= { juniIpIfEntry 8 }

juniIpIfAlwaysUp  OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "When enabled, the interface is determined to be up regardless of the
        state of any lower layer interfaces."
    DEFVAL    { disable }
    ::= { juniIpIfEntry 9 }

juniIpIfLoopback  OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      deprecated
    DESCRIPTION
        "Indicates whether the interface is a loopback type interface.

        This object has been replaced by juniIpIfInheritNum."
    DEFVAL    { disable }
    ::= { juniIpIfEntry 10 }

juniIpIfLoopbackUid  OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-create
    STATUS      deprecated
    DESCRIPTION
        "Specify the interface index of a loopback interface whose IP address
        should be used when sourcing traffic on this interface.  Useful for
        unnumbered interfaces.

        This object has been replaced by juniIpIfInheritNumUid."
    DEFVAL    { 0 }
    ::= { juniIpIfEntry 11 }

juniIpIfDebounceTime  OBJECT-TYPE
    SYNTAX      Integer32 (0..60000)
    UNITS       "milliseconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the time in milliseconds that a layer 2 interface must remain
        in a state before it is conveyed to the IP layer.  Useful for interfaces
        that experience brief outages that should not constitute a route flap.
        A value of 0 indicates that the feature is disabled."
    DEFVAL    { 0 }
    ::= { juniIpIfEntry 12 }

juniIpIfForwarding  OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enable/disable the forwarding of IP traffic to/from this interface.
        This is currently only applicable to the out-of-band management port."
    DEFVAL    { enable }
    ::= { juniIpIfEntry 13 }

juniIpIfForceFragmentation  OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Force the fragmentation of all IP packets greater than the interface
        MTU even if the DF bit is set."
    DEFVAL    { disable }
    ::= { juniIpIfEntry 14 }

juniIpIfSharesLowerUid  OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Identifies the interface as sharing a lower interface with another
        interface vs owning it outright."
    ::= { juniIpIfEntry 15 }

juniIpIfFilterOptions  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Bit mask to configure the interface to filter packets with IP header
        options.  Currently, either no bits or all bits may be set."
    DEFVAL    { 0 }
    ::= { juniIpIfEntry 16 }

juniIpIfName  OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(0..255))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specify the IP interface discriminator for an IP interface not attached
        to a layer 2 interface with a specific location."
    DEFVAL    { ''H }
    ::= { juniIpIfEntry 17 }

juniIpIfArpTimeout  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specify the ARP timeout for this interface in seconds."
    DEFVAL    { 21600 }
    ::= { juniIpIfEntry 18 }


juniIpIfAdminSpeed  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Set an administrative speed for the interface that overrides the speed
        learned from the lower layer.  A value of 0 indicates no speed is
        specified."
    DEFVAL    { 0 }
    ::= { juniIpIfEntry 19 }

juniIpIfMultipathMode  OBJECT-TYPE
    SYNTAX      INTEGER {
                    hashed(1),
                    roundRobin(2) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Configure the mode this interface should use when forwarding equal-cost
        multipath traffic."
    DEFVAL    { hashed }
    ::= { juniIpIfEntry 20 }

juniIpIfSharedNhAddr  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The IP address of either a direct or indirect next-hop toward which
        this shared interface should point."
    DEFVAL    { 0 }
    ::= { juniIpIfEntry 21 }

juniIpIfSharedNhRouterId  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The identifier for the domain of a virtual router in which the
        juniIpIfSharedNhAddr should be resolved."
    DEFVAL    { 0 }
    ::= { juniIpIfEntry 22 }

juniIpIfPrimaryIpAddress  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The IP address of the primary IP network on an interface."
    ::= { juniIpIfEntry 23 }

juniIpIfPrimaryIpMask  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The IP address mask of the primary IP network on an interface."
    ::= { juniIpIfEntry 24 }

juniIpIfOperDebounceTime  OBJECT-TYPE
    SYNTAX      Integer32 (0..60000)
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the operational time in milliseconds that a layer2 interface
        must remain in a state before it is conveyed to the IP layer.  Useful
        for interfaces that experience brief outages that should not constitute
        a route flap.  A value of 0 indicates that the feature is disabled."
    ::= { juniIpIfEntry 25 }

juniIpIfRouterIndex  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The index or ID of the router."
    ::= { juniIpIfEntry 26 }

juniIpIfInheritNum  OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates whether this numbered interface is referenced by unnumbered
        interfaces."
    ::= { juniIpIfEntry 27 }

juniIpIfInheritNumUid  OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specify the interface index of a numbered interface whose IP address
        should be used when sourcing traffic on this interface.  Useful for
        unnumbered interfaces."
    DEFVAL    { 0 }
    ::= { juniIpIfEntry 28 }

juniIpIfAnalyzerMode  OBJECT-TYPE
    SYNTAX      INTEGER {
                    disable(0),
                    enable(1),
                    default(2) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Used to set the interface to analyzer mode.  When enabled(1), all IP
        packets entering this interface and all non-mirror IP packets leaving
        this interface will be dropped.  The value default(2) specifies that
        this interface will be the default analyzer port for the virtual-router
        where the interface resides."
    DEFVAL    { disable }
    ::= { juniIpIfEntry 29 }

juniIpIfAutoConfigure  OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "When enabled, IP subscriber interfaces are created dynamically based on
        any attributes defined in the service-profile and the rules associated
        with the DCM profile selected for this subscriber."
    DEFVAL    { disable }
    ::= { juniIpIfEntry 30 }

juniIpIfTcpMss  OBJECT-TYPE
    SYNTAX      Integer32 (0|160..10240)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Configures TCP MSS value for an IP interface.  When configured, MSS
        value of TCP SYN packets received or transmitted on the interface will
        be compared with the configured value and lowest of the two will replace
        the value in the packet."
    DEFVAL    { 0 }
    ::= { juniIpIfEntry 31 }

juniIpIfInitSeqPrefOper  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the operational warm-restart replay initial sequence
        preference value for an IP interface.  Following an HA SRP switchover,
        high-preference (value 1) IP interfaces are replayed first, followed by
        static routes, and then low-preference (value 0) IP interfaces.  This
        allows static routes that are dependent on high-preference interfaces to
        be resolved and routing protocols to exchange information with peers
        over high-preference interfaces before low-preference interfaces are
        replayed.  An IP interface is designated as high-preference either (1)
        implicitly by configuring an IGP or PIM protocol on that interface, or
        (2) explicitly by juniIpIfInitSeqPrefAdmin (or CLI) configuration."
    ::= { juniIpIfEntry 32 }

juniIpIfInitSeqPrefAdmin  OBJECT-TYPE
    SYNTAX      Unsigned32 (0..1)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Configures the warm-restart replay initial sequence preference value
        for an IP interface.  See the juniIpIfInitSeqPrefOper description for more
        information."
    DEFVAL    { 0 }
    ::= { juniIpIfEntry 33 }

juniIpIfArpSpoofCheck  OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "When enabled, IP ARP spoof checking is performed on ARP packets
        received on the IP interface."
    DEFVAL    { enable }
    ::= { juniIpIfEntry 34 }

--
-- The IP Interface Statistics Table
--
juniIpIfStatsTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIpIfStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for IP interfaces present in the system."
    ::= { juniIpInterface 3 }

juniIpIfStatsEntry  OBJECT-TYPE
    SYNTAX      JuniIpIfStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry contains statistics for an IP interface."
    INDEX     { juniIpIfStatsIndex }
    ::= { juniIpIfStatsTable 1 }

JuniIpIfStatsEntry ::= SEQUENCE {
    juniIpIfStatsIndex                       InterfaceIndex,
    juniIpIfStatsInPackets                   Counter64,
    juniIpIfStatsInOctets                    Counter64,
    juniIpIfStatsInPoliciedPackets           Counter64,
    juniIpIfStatsInPoliciedOctets            Counter64,
    juniIpIfStatsInErrorPackets              Counter64,
    juniIpIfStatsInSpoofedPackets            Counter64,
    juniIpIfStatsInForwardedPackets          Counter64,
    juniIpIfStatsInForwardedOctets           Counter64,
    juniIpIfStatsOutForwardedPackets         Counter64,
    juniIpIfStatsOutForwardedOctets          Counter64,
    juniIpIfStatsOutSchedDropPackets         Counter64,
    juniIpIfStatsOutSchedDropOctets          Counter64,
    juniIpIfStatsOutRequestedPackets         Counter64,
    juniIpIfStatsOutRequestedOctets          Counter64,
    juniIpIfStatsOutPoliciedPackets          Counter64,
    juniIpIfStatsOutPoliciedOctets           Counter64,
    juniIpIfStatsGreenOutSchedDropPackets    Counter64,
    juniIpIfStatsYellowOutSchedDropPackets   Counter64,
    juniIpIfStatsRedOutSchedDropPackets      Counter64,
    juniIpIfStatsGreenOutSchedDropOctets     Counter64,
    juniIpIfStatsYellowOutSchedDropOctets    Counter64,
    juniIpIfStatsRedOutSchedDropOctets       Counter64 }

juniIpIfStatsIndex  OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ifIndex of the IP interface."
    ::= { juniIpIfStatsEntry 1 }

juniIpIfStatsInPackets  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets received on this interface."
    ::= { juniIpIfStatsEntry 2 }

juniIpIfStatsInOctets  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of octets received on this interface."
    ::= { juniIpIfStatsEntry 3 }

juniIpIfStatsInPoliciedPackets  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to rate limiters attached to this
        interface."
    ::= { juniIpIfStatsEntry 4 }

juniIpIfStatsInPoliciedOctets  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of octets dropped due to rate limiters attached to this
        interface."
    ::= { juniIpIfStatsEntry 5 }

juniIpIfStatsInErrorPackets  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets received with errors on this interface."
    ::= { juniIpIfStatsEntry 6 }

juniIpIfStatsInSpoofedPackets  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets received on this interface with destination
        unknown."
    ::= { juniIpIfStatsEntry 7 }

juniIpIfStatsInForwardedPackets  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The number of packets received on this interface that were forwarded
        by any interface in the system."
    ::= { juniIpIfStatsEntry 8 }

juniIpIfStatsInForwardedOctets  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The number of octets received on this interface that were forwarded by
        any interface in the system."
    ::= { juniIpIfStatsEntry 9 }

juniIpIfStatsOutForwardedPackets  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets forwarded by this interface."
    ::= { juniIpIfStatsEntry 10 }

juniIpIfStatsOutForwardedOctets  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of octets forwarded by this interface."
    ::= { juniIpIfStatsEntry 11 }

juniIpIfStatsOutSchedDropPackets  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped at this interface due to output queue
        congestion."
    ::= { juniIpIfStatsEntry 12 }

juniIpIfStatsOutSchedDropOctets  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of octets dropped at this interface due to output queue
        congestion."
    ::= { juniIpIfStatsEntry 13 }

juniIpIfStatsOutRequestedPackets  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The number of packets requested for transmission at this interface."
    ::= { juniIpIfStatsEntry 14 }

juniIpIfStatsOutRequestedOctets  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The number of octets requested for transmission at this interface."
    ::= { juniIpIfStatsEntry 15 }

juniIpIfStatsOutPoliciedPackets  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of packets dropped due to rate limiters attached to this
        interface."
    ::= { juniIpIfStatsEntry 16 }

juniIpIfStatsOutPoliciedOctets  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of octets dropped due to rate limiters attached to this
        interface."
    ::= { juniIpIfStatsEntry 17 }

juniIpIfStatsGreenOutSchedDropPackets  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The number of packets dropped at this interface due to output queue
        congestion in the green output queue.  The green output queue has lowest
        drop probability."
    ::= { juniIpIfStatsEntry 18 }

juniIpIfStatsYellowOutSchedDropPackets  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The number of packets dropped at this interface due to output queue
        congestion in the yellow output queue.  The yellow output queue has
        medium level drop probability."
    ::= { juniIpIfStatsEntry 19 }

juniIpIfStatsRedOutSchedDropPackets  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The number of packets dropped at this interface due to output queue
        congestion in the red output queue.  The red output queue has highest
        level drop probability."
    ::= { juniIpIfStatsEntry 20 }

juniIpIfStatsGreenOutSchedDropOctets  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The number of octets dropped at this interface due to output queue
        congestion in the green output queue.  The green output queue has the
        lowest drop probability."
    ::= { juniIpIfStatsEntry 21 }

juniIpIfStatsYellowOutSchedDropOctets  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The number of octets dropped at this interface due to output queue
        congestion in the yellow output queue.  The yellow output queue has the
        medium drop probability."
    ::= { juniIpIfStatsEntry 22 }

juniIpIfStatsRedOutSchedDropOctets  OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      obsolete
    DESCRIPTION
        "The number of octets dropped at this interface due to output queue
        congestion in the red output queue.  The red output queue has the
        highest drop probability."
    ::= { juniIpIfStatsEntry 23 }


--
-- The IP Interface Association Table
--
juniIpIfAssocTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIpIfAssocEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries of interfaces present in the system."
    ::= { juniIpInterface 4 }

juniIpIfAssocEntry  OBJECT-TYPE
    SYNTAX      JuniIpIfAssocEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry in this table returns the ifIndex of the IP interface
        associated with the lower layer ifIndex supplied as the index to this
        table.

        The purpose of this table is to translate L2 interfaces to corresponding
        L3 interfaces for billing applications.  Since interesting billing
        related statistics are kept at L3, it is often useful to know the L2-L3
        relationship.  Note that this table is not confined to L2-L3
        relationships.  Any interface sublayer can be used to access this table
        to determine the relationship with the L3 interface."
    INDEX     { juniIpIfAssocLowerIfIndex }
    ::= { juniIpIfAssocTable 1 }

JuniIpIfAssocEntry ::= SEQUENCE {
    juniIpIfAssocLowerIfIndex    InterfaceIndex,
    juniIpIfAssocIpIfIndex       InterfaceIndexOrZero }

juniIpIfAssocLowerIfIndex  OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ifIndex of the lower layer interface."
    ::= { juniIpIfAssocEntry 1 }

juniIpIfAssocIpIfIndex  OBJECT-TYPE
    SYNTAX     InterfaceIndexOrZero
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The ifIndex of the IP interface associated with the lower layer
        juniIpIfAssocLowerIfIndex.  In cases where there is not a 1 to 1
        relationship between lower layer and higher layer IP interface, a zero
        value juniIpIfAssocIpIfIndex is returned; this includes the case where
        an IP interface has not yet been configued at the top of the interface
        column.

        An example usage of this table:

        Assume a user needs to know the ifIndex relationship for all interfaces
        with the L3 IP interface.

        Then starting at the bottom of the stack below, the ATM and AAL5's
        ifIndex would be used to access the table.  The agent will return 0 for
        each of these cases because multiple customer's traffic is demultiplexed
        at these levels.

         IP_1
         PPP        IP_2
         ATM1483_1  ATM1483_2
           \         /
              AAL5
              ATM

        If the ATM1483_1 ifIndex is used to access this table, then the value of
        juniIpIfAssocLowerIfIndex will be set to the ifIndex of IP_1.
        Similarily, if the ATM1483_2 ifIndex is used to access this table, the
        juniIpifAssocLowerIfIndex will set to the ifIndex of IP_2."
    ::= { juniIpIfAssocEntry 2 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- IP Address attributes
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
--
-- IP globals
--
juniIpAddrGlobals  OBJECT IDENTIFIER ::= { juniIpAddress 1 }

juniIpArpTimeout  OBJECT-TYPE
    SYNTAX      Integer32 (1..60)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "Timeout, in seconds, for ARP requests issued by this entity."
    ::= { juniIpAddrGlobals 1 }

--
-- IP Address management
--
juniIpAddrTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIpAddrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "IP addressing information for this entity's IP network interfaces.
        Representation of both numbered and unnumbered IP interfaces is
        supported."
    ::= { juniIpAddress 2 }

juniIpAddrEntry  OBJECT-TYPE
    SYNTAX      JuniIpAddrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "IP addressing information for one of this entity's IP network
        interfaces.  This interface could be either numbered or unnumbered.

        The following objects correspond to (read-only) counterparts in the
        IP-MIB ipAddrTable:
            juniIpAdEntAddr
            juniIpAdEntIfIndex
            juniIpAdEntNetMask
            juniIpAdEntBcastAddr
            juniIpAdEntReasmMaxSize "
    INDEX     { juniIpAdEntAddr }
    ::= { juniIpAddrTable 1 }

JuniIpAddrEntry ::= SEQUENCE {
    juniIpAdEntAddr                     JuniIpAddrLessIf,
    juniIpAdEntIfIndex                  InterfaceIndex,
    juniIpAdEntNetMask                  IpAddress,
    juniIpAdEntBcastAddr                Integer32,
    juniIpAdEntReasmMaxSize             Integer32,
    juniIpAdEntRowStatus                RowStatus,
    juniIpAdEntAdminStatus              JuniEnable,
    juniIpAdEntArpRspEnable             JuniEnable,
    juniIpAdEntProxyArpRspEnable        JuniEnable,
    juniIpAdEntIgmpEnable               JuniEnable,
    juniIpAdEntDirectedBcastEnable      JuniEnable,
    juniIpAdEntIcmpRedirectEnable       JuniEnable,
    juniIpAdEntIcmpMaskReplyEnable      JuniEnable,
    juniIpAdEntIcmpUnreachEnable        JuniEnable,
    juniIpAdEntMtu                      Integer32,
    juniIpAdEntUnnumLoopbackIfIndex     InterfaceIndexOrZero,
    juniIpAdEntIrdpEnable               JuniEnable,
    juniIpAdEntAccessRouteEnable        JuniEnable,
    juniIpAdEntAccessRouteHost          IpAddress,
    juniIpAdEntIsSecondary              JuniEnable,
    juniIpAdEntUnnumInheritNumIfIndex   InterfaceIndexOrZero }

juniIpAdEntAddr  OBJECT-TYPE
    SYNTAX      JuniIpAddrLessIf
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The IP address for a numbered IP network interface, if this object's
        value has the form 'a.b.c.d', where 'a' is nonzero; or, the ifIndex
        (interpreting the low 24 bits of this value as an integer) of an
        unnumbered ('address-less') IP interface, if this object's value has the
        form '0.b.c.d'."
    ::= { juniIpAddrEntry 1 }

juniIpAdEntIfIndex  OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The ifIndex of the network interface to which this entry's IP
        addressing mode pertains."
    ::= { juniIpAddrEntry 2 }

juniIpAdEntNetMask  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The IP subnet mask associated with the IP address of this entry.  The
        network and host bit fields of the mask are filled with 1's and 0's,
        respectively.

        If this entry represents an unnumbered IP interface, this object should
        have a value of all ones."
    DEFVAL    { 'ffffffff'H }
    ::= { juniIpAddrEntry 3 }

juniIpAdEntBcastAddr  OBJECT-TYPE
    SYNTAX      Integer32 (0..1)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the least-significant bit in the IP broadcast address used
        for sending datagrams on the IP network interface associated with this
        entry.  For example, when the Internet standard all-ones broadcast
        address is used, the value will be 1.  This value applies to both the
        subnet and network broadcasts addresses used by the entity on this
        interface."
    ::= { juniIpAddrEntry 4 }

juniIpAdEntReasmMaxSize  OBJECT-TYPE
    SYNTAX      Integer32 (0..65535)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The size of the largest IP datagram which this entity can re-assemble
        from incoming IP fragmented datagrams received on this interface."
    ::= { juniIpAddrEntry 5 }

juniIpAdEntRowStatus  OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls the creation/deletion of entries in this table according to
        the RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        To create entries for both numbered and unnumbered IP interfaces, the
        following entry objects MUST be explicitly configured:
            juniIpAdEntRowStatus
            juniIpAdEntIfIndex

        To create an entry for a numbered IP interface, the following conditions
        must also hold:
            <none>

        To create an entry for an unnumbered IP interface, the following
        conditions must also hold:

            juniIpAdEntUnnumInheritNumIfIndex must be configured with a nonzero
            ifIndex value of an IP numbered interface."
    ::= { juniIpAddrEntry 6 }

juniIpAdEntAdminStatus  OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enable/disable operation of IP on this IP network interface."
    DEFVAL    { enable }
    ::= { juniIpAddrEntry 7 }

juniIpAdEntArpRspEnable  OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enable/disable ARP response on this IP network interface."
    DEFVAL    { enable }
    ::= { juniIpAddrEntry 8 }

juniIpAdEntProxyArpRspEnable  OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enable/disable proxy ARP response on this IP network interface."
    DEFVAL    { disable }
    ::= { juniIpAddrEntry 9 }

juniIpAdEntIgmpEnable  OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      deprecated
    DESCRIPTION
        "Enable/disable IGMP operation on this IP network interface."
    DEFVAL    { disable }
    ::= { juniIpAddrEntry 10 }

juniIpAdEntDirectedBcastEnable  OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enable/disable forwarding of directed broadcasts on this IP network
        interface."
    DEFVAL    { disable }
    ::= { juniIpAddrEntry 11 }

juniIpAdEntIcmpRedirectEnable  OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enable/disable transmission of ICMP Redirect messages on this IP
        network interface."
    DEFVAL    { disable }
    ::= { juniIpAddrEntry 12 }

juniIpAdEntIcmpMaskReplyEnable  OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enable/disable transmission of ICMP Mask Reply messages on this IP
        network interface."
    DEFVAL    { disable }
    ::= { juniIpAddrEntry 13 }

juniIpAdEntIcmpUnreachEnable  OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enable/disable transmission of ICMP Unreachable messages on this IP
        network interface."
    DEFVAL    { disable }
    ::= { juniIpAddrEntry 14 }

juniIpAdEntMtu  OBJECT-TYPE
    SYNTAX      Integer32 (0..65535)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The configured MTU size for this IP network interface.  If set to zero,
        the default MTU size, as determined by the underlying network media, is
        used."
    ::= { juniIpAddrEntry 15 }

juniIpAdEntUnnumLoopbackIfIndex  OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-create
    STATUS      deprecated
    DESCRIPTION
        "For unnumbered interfaces, the ifIndex of the IP loopback interface
        whose IP address is used as the source IP address for IP packets
        transmitted on the unnumbered network.

        For numbered interfaces, this object has a value of zero.

        This object has been replaced by juniIpAdEntUnnumInheritNumIfIndex."
    DEFVAL    { 0 }
    ::= { juniIpAddrEntry 16 }

juniIpAdEntIrdpEnable  OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls whether ICMP Router Discovery Protocol operation is permitted
        to be sent on this network."
    DEFVAL    { enable }
    ::= { juniIpAddrEntry 17 }

juniIpAdEntAccessRouteEnable  OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If enabled, then establishment/loss of a point-to-point network
        connection causes a host route for the remote host to be created/deleted
        automatically."
    DEFVAL    { disable }
    ::= { juniIpAddrEntry 18 }

juniIpAdEntAccessRouteHost  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "If an access route has been established, the IP address of the remote
        host is reported by this object; otherwise, this object contains the
        value 0.0.0.0."
    ::= { juniIpAddrEntry 19 }

juniIpAdEntIsSecondary  OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "If enabled, then the IP address corresponding to this entry is a
        secondary address.  If disabled, then the IP address corresponding to
        this entry is te primary address."
    DEFVAL    { disable }
    ::= { juniIpAddrEntry 20 }

juniIpAdEntUnnumInheritNumIfIndex  OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "For unnumbered interfaces, the ifIndex of the IP numbered interface
        whose IP address is used as the source IP address for IP packets
        transmitted on the unnumbered network.

        For numbered interfaces, this object has a value of zero."
    DEFVAL    { 0 }
    ::= { juniIpAddrEntry 21 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- IP Route
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
--
-- Route Globals
--
juniIpRouteGlobals  OBJECT IDENTIFIER ::= { juniIpRoute 1 }

juniIpRouteLimit  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "Maximum number of IP routes maintained by this entity.

        Setting a value lower than the current number of routes prevents
        additional routes from being learned or configured, but does not cause
        existing excess routes to be deleted to enforce the new limit."
    ::= { juniIpRouteGlobals 1 }

juniIpRouteTableLimit  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The VRF Route Table Maximum Number of Routes Limit."
    DEFVAL    { 0 }
    ::= { juniIpRouteGlobals 2 }

juniIpRouteTableWarnPercent  OBJECT-TYPE
    SYNTAX      Unsigned32 (0..100)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The VRF Route Table Percentage of the Route Limit at which to issue a warning.
         The percentage is only valid when juniIpRouteTableWarnOnly is false. It must be set to 0 if
         juniIpRouteTableWarnOnly is true."
    DEFVAL    { 0 }
    ::= { juniIpRouteGlobals 3 }

juniIpRouteTableWarnOnly  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The VRF Route Table Maximum Number of Routes Warning flag. 
         Do not actually limit the number of routes in the table"
    DEFVAL    { false }
    ::= { juniIpRouteGlobals 4 }

juniIpRouteTableWarnThreshold OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The computed number of route to issue a warning. If juniIpRouteTableWarnOnly is true
         this value will be juniIpRouteTableLimit and if juniIpRouteTableWarnOnly is false it will
         be juniIpRouteTableLimit * juniIpRouteTableWarnPercentage" 
    ::= { juniIpRouteGlobals 5 }

--
-- Static Route Table
--
juniIpRouteStaticTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIpRouteStaticEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table of static routes configured on this entity.

        The object definitions and indexing for this table are chosen to closely
        align with the IP-FORWARD-MIB's ipCidrRouteTable.

        This  table serves three purposes:
        1. Provide the means for configuring static routes.
        2. Provide an efficient view of static routes (otherwise they must be
           observed by traversing the entire routing table).
        3. Provide view of static routes configured on network interfaces that
           are currently inactive.  (In this implementation, static routes
           configured on inactive interfaces are not visible in the routing
           table.)"
    ::= { juniIpRoute 2 }

juniIpRouteStaticEntry  OBJECT-TYPE
    SYNTAX      JuniIpRouteStaticEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A static route."
    INDEX     { juniIpRouteStaticDest,
                juniIpRouteStaticMask,
                juniIpRouteStaticPref,
                juniIpRouteStaticNextHop }
    ::= { juniIpRouteStaticTable 1 }

JuniIpRouteStaticEntry ::= SEQUENCE {
    juniIpRouteStaticDest        IpAddress,
    juniIpRouteStaticMask        IpAddress,
    juniIpRouteStaticPref        Integer32,
    juniIpRouteStaticNextHop     JuniIpAddrLessIf,
    juniIpRouteStaticRowStatus   RowStatus,
    juniIpRouteStaticIfIndex     Integer32,
    juniIpRouteStaticStatus      INTEGER,
    juniIpRouteStaticNextHopAS   Integer32,
    juniIpRouteStaticMetric      Integer32,
    juniIpRouteStaticTag         Unsigned32 }

juniIpRouteStaticDest  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The destination IP address of this route.

        This object may not take a Multicast (Class D) address value.

        Any assignment (implicit or otherwise) of an instance of this object to
        a value x must be rejected if the bitwise logical-AND of x with the
        value of the corresponding instance of the juniIpRouteStaticMask object
        is not equal to x."
    ::= { juniIpRouteStaticEntry 1 }

juniIpRouteStaticMask  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicate the mask to be logical-ANDed with the destination address
        before being compared to the value in the juniIpRouteStaticDest field.
        For those systems that do not support arbitrary subnet masks, an agent
        constructs the value of the juniIpRouteStaticMask by reference to the IP
        Address Class.

        Any assignment (implicit or otherwise) of an instance of this object to
        a value x must be rejected if the bitwise logical-AND of x with the
        value of the corresponding instance of the juniIpRouteStaticDest object
        is not equal to juniIpRouteStaticDest."
    ::= { juniIpRouteStaticEntry 2 }

-- The following convention is included for specification
-- of TOS Field contents.  At this time, the Host Requirements
-- and the Router Requirements documents disagree on the width
-- of the TOS field.  This mapping describes the Router
-- Requirements mapping, and leaves room to widen the TOS field
-- without impact to fielded systems.

juniIpRouteStaticPref  OBJECT-TYPE
    SYNTAX      Integer32 (0..255)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The preference of this static route.  Higher values correspond to
        higher preference.  A static route with preference of zero will never be
        installed as an active route."
    ::= { juniIpRouteStaticEntry 3 }

juniIpRouteStaticNextHop  OBJECT-TYPE
    SYNTAX      JuniIpAddrLessIf
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The address of the next hop toward the destination."
    ::= { juniIpRouteStaticEntry 4 }

juniIpRouteStaticRowStatus  OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The row status variable, used according to row installation and removal
        conventions."
    ::= { juniIpRouteStaticEntry 5 }

juniIpRouteStaticIfIndex  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The ifIndex value which identifies the local interface through which
        the next hop of this route should be reached.  A value of zero means the
        router should automatically determine the interface through which the
        specified next-hop address is reached.

        An implementation may disallow non-zero values from being configured."
    DEFVAL    { 0 }
    ::= { juniIpRouteStaticEntry 6 }

juniIpRouteStaticStatus  OBJECT-TYPE
    SYNTAX      INTEGER {
                    active(0),
                    inactive(1),
                    incomplete(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The operational status of this static route.

        active(0) indicates this route is currently being used to reach the
        specified destination.

        inactive(1) indicates this route is considered valid, but currently is
        superseded by another routing table entry for the destination, having a
        higher preference value.

        incomplete(2) indicates this route entry contains information that is
        incomplete, or is inconsistent with other system configuration (for
        example, the interface specified in juniIpRouteStaticIfIndex does not
        exist)."
    ::= { juniIpRouteStaticEntry 7 }

juniIpRouteStaticNextHopAS  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The Autonomous System Number of the Next Hop.  The semantics of this
        object are determined by the routing-protocol specified in the route's
        ipCidrRouteProto value.  When this object is unknown or not relevant its
        value should be set to zero."
    DEFVAL    { 0 }
    ::= { juniIpRouteStaticEntry 8 }

juniIpRouteStaticMetric  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The primary routing metric for this route.  The semantics of this
        metric are determined by the routing-protocol specified in the route's
        ipCidrRouteProto value.  If this metric is not used, its value should be
        set to -1."
    DEFVAL    { -1 }
    ::= { juniIpRouteStaticEntry 9 }

juniIpRouteStaticTag  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "A tag value for this static route."
    DEFVAL    { 0 }
    ::= { juniIpRouteStaticEntry 10 }


--
-- Extensions to IP CIDR Route Table
--
juniIpCidrRouteTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIpCidrRouteEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table of routes active on this entity.  This table is an augmentation
        of the IP-FORWARD-MIB's ipCidrRouteTable."
    ::= { juniIpRoute 3 }

juniIpCidrRouteEntry  OBJECT-TYPE
    SYNTAX      JuniIpCidrRouteEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Additional attributes of an active route."
    AUGMENTS  { ipCidrRouteEntry }
    ::= { juniIpCidrRouteTable 1 }

JuniIpCidrRouteEntry ::= SEQUENCE {
    juniIpCidrRoutePref  Integer32,
    juniIpCidrRouteArea  IpAddress,
    juniIpCidrRouteTag   Unsigned32 }

juniIpCidrRoutePref  OBJECT-TYPE
    SYNTAX      Integer32 (0..255)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The preference of this route.  Higher values correspond to higher
        preference."
    ::= { juniIpCidrRouteEntry 1 }

juniIpCidrRouteArea  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The Area to which this route pertains.  A value of 0.0.0.0 indicates no
        area is identified."
    ::= { juniIpCidrRouteEntry 2 }

juniIpCidrRouteTag  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A tag value for this route."
    ::= { juniIpCidrRouteEntry 3 }

--
-- The IP Route BFD Table
--
 
juniIpRouteStaticBFDTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIpRouteStaticBFDEntry 
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The Juniper IP interface table describes the BFD-specific
        characteristics of interfaces."
    ::= { juniIpRoute 4 }

juniIpRouteStaticBFDEntry OBJECT-TYPE
    SYNTAX      JuniIpRouteStaticBFDEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The Juniper IP interface table describes the BFD-specific
        characteristics of one interface."
    AUGMENTS  { juniIpRouteStaticEntry } 
    ::= { juniIpRouteStaticBFDTable 1 }

JuniIpRouteStaticBFDEntry ::= SEQUENCE {
    juniIpRouteStaticBfdEnable   TruthValue,
    juniIpRouteStaticBfdMinRxInterval   Integer32,
    juniIpRouteStaticBfdMinTxInterval   Integer32,
    juniIpRouteStaticBfdMultiplier	Integer32
}

juniIpRouteStaticBfdEnable   OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This variable indicates whether BFD session on the interface is active or not"
    DEFVAL    { false }
    ::= { juniIpRouteStaticBFDEntry 1 }
    
juniIpRouteStaticBfdMinRxInterval   OBJECT-TYPE
    SYNTAX      Integer32 (100..65535)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This variable specifies upper-limit on rate local-system requires remote-system to
         transmit bfd control-packets [milliseconds]"
    DEFVAL    { 300 }
    ::= { juniIpRouteStaticBFDEntry 2 }

juniIpRouteStaticBfdMinTxInterval   OBJECT-TYPE
    SYNTAX      Integer32 (100..65535)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This variable specifies lower-limit on rate local-system requires remote-system to 
         transmit bfd control-packets [milliseconds]"
    DEFVAL    { 300 }                 
    ::= { juniIpRouteStaticBFDEntry 3 }

juniIpRouteStaticBfdMultiplier	OBJECT-TYPE
    SYNTAX      Integer32 (1..255)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This variable specifies detection-multiplier "
    DEFVAL    { 3 }                         
    ::= { juniIpRouteStaticBFDEntry 4 }
    
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Notifications
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- No notifications are defined in this MIB.  Placeholders follow.
juniIpTrapEnables OBJECT IDENTIFIER ::= { juniIpMIB 2 }
juniIpTraps       OBJECT IDENTIFIER ::= { juniIpMIB 3 }
juniIpTrapPrefix  OBJECT IDENTIFIER ::= { juniIpTraps 0 }
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Trap Definitions
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++

juniIpSaValidateTrapEnable  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Set to true to enable source address validation traps."
    DEFVAL    { false }
    ::= { juniIpTrapEnables 1 }

juniIpRouteTableTrapRouteLimitExceeded NOTIFICATION-TYPE
     OBJECTS {juniIpRouteTableLimit, ipCidrRouteNumber}
     STATUS       current
     DESCRIPTION
         "The  juniIpRouteTableTrapRouteLimitExceeded Trap indicates that the configured
          route Table Limit has been exceeded. Issued once every 5 minutes that
          the limit is being exceeded."
        ::= { juniIpTrapPrefix 1 }

juniIpRouteTableTrapRouteLimitRemove NOTIFICATION-TYPE
     OBJECTS {juniIpRouteTableLimit, ipCidrRouteNumber}
     STATUS       current
     DESCRIPTION
         "The  juniIpRouteTableTrapRouteTableLimitRemove Trap indicates that routes have been
          freed up for 30 seconds and the Route Table Limit is no longer being violated.
          Issued once."
        ::= { juniIpTrapPrefix 2 }

juniIpRouteTableTrapWarnThresholdExceeded NOTIFICATION-TYPE
     OBJECTS {juniIpRouteTableLimit, juniIpRouteTableWarnThreshold, ipCidrRouteNumber}
     STATUS       current
     DESCRIPTION
         "The  juniIpRouteTableTrapWarnThresholdExceeded Trap indicates that the computed
          warning threshold has been exceeded.
          Issued once every 5 minutes that the warning threshold is being execeeded."

     ::= { juniIpTrapPrefix 3 }

juniIpTrapSaValidationFailure NOTIFICATION-TYPE
     OBJECTS {ifIndex, juniIpIfSaValFailSrcIpAddr, juniIpIfSaValFailDestIpAddr}
     STATUS       current
     DESCRIPTION
         "The  juniIpTrapSaValidationFailure Trap indicates that a source address validation
          failure occurred on an interface.  The interface on which the failure occurred,
          the source ip address and the destination ip address of the packet causing the
          failure are returned."

     ::= { juniIpTrapPrefix 4 }
  
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Notification control objects
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniIpMIBNotificationObjects  OBJECT IDENTIFIER ::= { juniIpTraps 1 }

juniIpIfSaValFailSrcIpAddr  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The source IP address of the packet that caused the last source address
         validation failure on the IP interface."
    ::= { juniIpMIBNotificationObjects 1 }

juniIpIfSaValFailDestIpAddr  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  accessible-for-notify
    STATUS      current
    DESCRIPTION
        "The destination IP address of the packet that caused the last source address
         validation failure on the IP interface."
    ::= { juniIpMIBNotificationObjects 2 }

-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Conformance information
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniIpConformance     OBJECT IDENTIFIER ::= { juniIpMIB 4 }
juniIpCompliances     OBJECT IDENTIFIER ::= { juniIpConformance 1 }
juniIpGroups          OBJECT IDENTIFIER ::= { juniIpConformance 2 }

--
-- compliance statements
--
juniIpCompliance  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        IP MIB.  This statement became obsolete when the IP interface and IP
        address groups changed and the global objects were added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpInterfaceGroup,
            juniIpAddressGroup,
            juniIpRouteGroup }
    ::= { juniIpCompliances 1 }                                    -- JUNOSe 2.2

juniIpCompliance2  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        IP MIB.  This statement became obsolete when the juniIpIfAssocTable was
        added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpInterfaceGroup2,
            juniIpAddressGroup2,
            juniIpRouteGroup,
            juniIpGlobalGroup }
    ::= { juniIpCompliances 2 }                                    -- JUNOSe 3.0

juniIpCompliance3  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        IP MIB.  This statement became obsolete when the QoS related objects
        were obsoleted."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpInterfaceGroup3,
            juniIpAddressGroup2,
            juniIpRouteGroup,
            juniIpGlobalGroup }
    ::= { juniIpCompliances 3 }                                   -- JUNOSe 3.2

juniIpCompliance4  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the
        Juniper IP MIB.  This statement became obsolete when the QoS related
        objects were obsoleted."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpInterfaceGroup4,
            juniIpAddressGroup2,
            juniIpRouteGroup,
            juniIpGlobalGroup }
    ::= { juniIpCompliances 4 }                                    -- JUNOSe 4.0

juniIpCompliance5  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        IP MIB.  This statement became obsolete when support was added for
        router index and unnumbered interfaces referencing numbered interfaces."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpInterfaceGroup4,
            juniIpAddressGroup3,
            juniIpRouteGroup2,
            juniIpGlobalGroup2 }
    ::= { juniIpCompliances 5 }                                    -- JUNOSe 4.1

juniIpCompliance6  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        IP MIB.  This statement became obsolete when interface mirroring and 
        interface auto configure support was added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpInterfaceGroup5,
            juniIpAddressGroup4,
            juniIpRouteGroup2,
            juniIpGlobalGroup2 }
    ::= { juniIpCompliances 6 }                                    -- JUNOSe 5.0

juniIpCompliance7  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        IP MIB.  This statement became obsolete when interface TCP MSS feature
        was added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpInterfaceGroup6,
            juniIpAddressGroup4,
            juniIpRouteGroup2,
            juniIpGlobalGroup2,
            juniIpIfSummaryGroup }
    ::= { juniIpCompliances 7 }                                    -- JUNOSe 5.1

juniIpCompliance8  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        IP MIB. This statement became obsolete when  juniIpVpnIdOui and 
	juniIpVpnIdIndex were obsoleted."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpInterfaceGroup7,
            juniIpAddressGroup4,
            juniIpRouteGroup2,
            juniIpGlobalGroup2,
            juniIpIfSummaryGroup }
    ::= { juniIpCompliances 8 }                                    -- JUNOSe 5.2


juniIpCompliance9  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for entities which implement the Juniper IP
        MIB."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpInterfaceGroup7,
            juniIpAddressGroup4,
            juniIpRouteGroup2,
            juniIpGlobalGroup3,
            juniIpIfSummaryGroup,
            juniIpNotificationsGroup }
    ::= { juniIpCompliances 9 }                                    -- JUNOSe 6.0

juniIpCompliance10  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for entities which implement the Juniper IP
        MIB."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpInterfaceGroup7,
            juniIpAddressGroup4,
            juniIpRouteGroup3,
            juniIpGlobalGroup3,
            juniIpIfSummaryGroup,
            juniIpNotificationsGroup }
    ::= { juniIpCompliances 10 }                                    -- JUNOSe 6.1
                                  

juniIpCompliance11  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for entities which implement the Juniper IP
        MIB. This statement became obsolete when  juniIpVpnIdOui and 
	juniIpVpnIdIndex were obsoleted."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpInterfaceGroup7,
            juniIpAddressGroup4,
            juniIpRouteGroup3,
            juniIpGlobalGroup3,
            juniIpIfSummaryGroup,
            juniIpNotificationGroup1,
            juniIpMIBNotificationObjectsGroup,
            juniIpRouteSummaryGroup }
    ::= { juniIpCompliances 11 }                                    -- JUNOSe 7.0
                        
juniIpCompliance12  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for entities which implement the Juniper IP
        MIB. This statement became obsolete when juniIpIfInitSeqPrefOper and
        juniIpIfInitSeqPrefAdmin were added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpInterfaceGroup7,
            juniIpAddressGroup4,
            juniIpRouteGroup3,
            juniIpGlobalGroup3,
            juniIpIfSummaryGroup,
            juniIpNotificationGroup1,
            juniIpMIBNotificationObjectsGroup,
            juniIpRouteSummaryGroup,
            juniIpRouteStaticBFDGroup }
    ::= { juniIpCompliances 12 }                                    -- JUNOSe 7.3
                        
juniIpCompliance13  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for entities which implement the Juniper IP
        MIB. This statement became obsolete when juniIpIfArpSpoofCheck was added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpInterfaceGroup8,
            juniIpAddressGroup4,
            juniIpRouteGroup3,
            juniIpGlobalGroup3,
            juniIpIfSummaryGroup,
            juniIpNotificationGroup1,
            juniIpMIBNotificationObjectsGroup,
            juniIpRouteSummaryGroup,
            juniIpRouteStaticBFDGroup }
    ::= { juniIpCompliances 13 }                                  -- JUNOSe 7.3.2

juniIpCompliance14  MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for entities which implement the Juniper IP
        MIB."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpInterfaceGroup9,
            juniIpAddressGroup4,
            juniIpRouteGroup3,
            juniIpGlobalGroup3,
            juniIpIfSummaryGroup,
            juniIpNotificationGroup1,
            juniIpMIBNotificationObjectsGroup,
            juniIpRouteSummaryGroup,
            juniIpRouteStaticBFDGroup }
    ::= { juniIpCompliances 14 }                                  -- JUNOSe 9.3

--
-- units of conformance
--
juniIpInterfaceGroup  OBJECT-GROUP
    OBJECTS {
        juniIpNextIfIndex,

        juniIpIfRowStatus,
        juniIpIfLowerIfIndex,
        juniIpIfType,
        juniIpIfTypeId,

        juniIpIfStatsInPackets,
        juniIpIfStatsInOctets,
        juniIpIfStatsInPoliciedPackets,
        juniIpIfStatsInPoliciedOctets,
        juniIpIfStatsInErrorPackets,
        juniIpIfStatsInSpoofedPackets,
        juniIpIfStatsInForwardedPackets,
        juniIpIfStatsInForwardedOctets,
        juniIpIfStatsOutForwardedPackets,
        juniIpIfStatsOutForwardedOctets,
        juniIpIfStatsOutSchedDropPackets,
        juniIpIfStatsOutSchedDropOctets,
        juniIpIfStatsOutRequestedPackets,
        juniIpIfStatsOutRequestedOctets,
        juniIpIfStatsOutPoliciedPackets,
        juniIpIfStatsOutPoliciedOctets }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects for managing IP interface capabilities
        in a Juniper product.  This group became obsolete when new objects were
        added to the juniIpIfTable and the juniIpIfStatsTable."
    ::= { juniIpGroups 1 }                                         -- JUNOSe 2.2

juniIpAddressGroup  OBJECT-GROUP
    OBJECTS {
        juniIpArpTimeout,

        juniIpAdEntRowStatus,
        juniIpAdEntIfIndex,
        juniIpAdEntNetMask,
        juniIpAdEntAdminStatus,
        juniIpAdEntArpRspEnable,
        juniIpAdEntProxyArpRspEnable,
        juniIpAdEntIgmpEnable,
        juniIpAdEntDirectedBcastEnable,
        juniIpAdEntIcmpRedirectEnable,
        juniIpAdEntIcmpMaskReplyEnable,
        juniIpAdEntIcmpUnreachEnable,
        juniIpAdEntMtu,
        juniIpAdEntUnnumLoopbackIfIndex,
        juniIpAdEntIrdpEnable,
        juniIpAdEntAccessRouteEnable,
        juniIpAdEntAccessRouteHost }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects for managing IP address capabilities in
        a Juniper product.  This group became obsolete when
        juniIpAdEntIgmpEnable was deprecated and juniIpAdEntIsSecondary was
        added."
    ::= { juniIpGroups 2 }                                         -- JUNOSe 2.2

juniIpRouteGroup  OBJECT-GROUP
    OBJECTS {
        juniIpRouteLimit,

        juniIpRouteStaticDest,
        juniIpRouteStaticMask,
        juniIpRouteStaticPref,
        juniIpRouteStaticNextHop,
        juniIpRouteStaticRowStatus,
        juniIpRouteStaticIfIndex,
        juniIpRouteStaticStatus,
        juniIpRouteStaticNextHopAS,
        juniIpRouteStaticMetric,
        juniIpRouteStaticTag,

        juniIpCidrRoutePref,
        juniIpCidrRouteArea,
        juniIpCidrRouteTag }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects for managing IP routing capabilities in
        a Juniper product.  This group became obsolete when juniIpRouteLimit was
        obsoleted."
    ::= { juniIpGroups 3 }                                         -- JUNOSe 2.2

juniIpGlobalGroup  OBJECT-GROUP
    OBJECTS {
        juniIpDebounceTime,
        juniIpRouterId,
        juniIpSourceRoutingAdminStatus,
        juniIpVpnIdOui,
        juniIpVpnIdIndex }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of IP global objects for managing instances of IP
        in a Juniper product.  This group became obsolete when BGP new format
        objects were added."
    ::= { juniIpGroups 4 }                                         -- JUNOSe 3.0

juniIpInterfaceGroup2  OBJECT-GROUP
    OBJECTS {
        juniIpNextIfIndex,

        juniIpIfRowStatus,
        juniIpIfLowerIfIndex,
        juniIpIfType,
        juniIpIfTypeId,
        juniIpIfSAValidationEnable,
        juniIpIfCreationType,
        juniIpIfProfileId,
        juniIpIfAlwaysUp,
        juniIpIfLoopback,
        juniIpIfLoopbackUid,
        juniIpIfDebounceTime,
        juniIpIfForwarding,
        juniIpIfForceFragmentation,
        juniIpIfSharesLowerUid,
        juniIpIfFilterOptions,
        juniIpIfName,
        juniIpIfArpTimeout,
        juniIpIfAdminSpeed,
        juniIpIfMultipathMode,
        juniIpIfSharedNhAddr,
        juniIpIfSharedNhRouterId,
        juniIpIfPrimaryIpAddress,
        juniIpIfPrimaryIpMask,
        juniIpIfOperDebounceTime,

        juniIpIfStatsInPackets,
        juniIpIfStatsInOctets,
        juniIpIfStatsInPoliciedPackets,
        juniIpIfStatsInPoliciedOctets,
        juniIpIfStatsInErrorPackets,
        juniIpIfStatsInSpoofedPackets,
        juniIpIfStatsInForwardedPackets,
        juniIpIfStatsInForwardedOctets,
        juniIpIfStatsOutForwardedPackets,
        juniIpIfStatsOutForwardedOctets,
        juniIpIfStatsOutSchedDropPackets,
        juniIpIfStatsOutSchedDropOctets,
        juniIpIfStatsOutRequestedPackets,
        juniIpIfStatsOutRequestedOctets,
        juniIpIfStatsOutPoliciedPackets,
        juniIpIfStatsOutPoliciedOctets,
        juniIpIfStatsGreenOutSchedDropPackets,
        juniIpIfStatsYellowOutSchedDropPackets,
        juniIpIfStatsRedOutSchedDropPackets,
        juniIpIfStatsGreenOutSchedDropOctets,
        juniIpIfStatsYellowOutSchedDropOctets,
        juniIpIfStatsRedOutSchedDropOctets }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects for managing IP interface capabilities
        in a Juniper product.  This group became obsolete when the
        juniIpIfAssocTable was added."
    ::= { juniIpGroups 5 }                                         -- JUNOSe 3.0

juniIpAddressGroup2  OBJECT-GROUP
    OBJECTS {
        juniIpArpTimeout,

        juniIpAdEntRowStatus,
        juniIpAdEntIfIndex,
        juniIpAdEntNetMask,
        juniIpAdEntBcastAddr,
        juniIpAdEntReasmMaxSize,
        juniIpAdEntAdminStatus,
        juniIpAdEntArpRspEnable,
        juniIpAdEntProxyArpRspEnable,
        juniIpAdEntDirectedBcastEnable,
        juniIpAdEntIcmpRedirectEnable,
        juniIpAdEntIcmpMaskReplyEnable,
        juniIpAdEntIcmpUnreachEnable,
        juniIpAdEntMtu,
        juniIpAdEntUnnumLoopbackIfIndex,
        juniIpAdEntIrdpEnable,
        juniIpAdEntAccessRouteEnable,
        juniIpAdEntAccessRouteHost,
        juniIpAdEntIsSecondary }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects for managing IP address capabilities in
        a Juniper product.  This group became obsolete when when
        juniIpArpTimeout was obsoleted."
    ::= { juniIpGroups 6 }                                         -- JUNOSe 3.0

juniIpInterfaceGroup3  OBJECT-GROUP
    OBJECTS {
        juniIpNextIfIndex,

        juniIpIfRowStatus,
        juniIpIfLowerIfIndex,
        juniIpIfType,
        juniIpIfTypeId,
        juniIpIfSAValidationEnable,
        juniIpIfCreationType,
        juniIpIfProfileId,
        juniIpIfAlwaysUp,
        juniIpIfLoopback,
        juniIpIfLoopbackUid,
        juniIpIfDebounceTime,
        juniIpIfForwarding,
        juniIpIfForceFragmentation,
        juniIpIfSharesLowerUid,
        juniIpIfFilterOptions,
        juniIpIfName,
        juniIpIfArpTimeout,
        juniIpIfAdminSpeed,
        juniIpIfMultipathMode,
        juniIpIfSharedNhAddr,
        juniIpIfSharedNhRouterId,
        juniIpIfPrimaryIpAddress,
        juniIpIfPrimaryIpMask,
        juniIpIfOperDebounceTime,

        juniIpIfStatsInPackets,
        juniIpIfStatsInOctets,
        juniIpIfStatsInPoliciedPackets,
        juniIpIfStatsInPoliciedOctets,
        juniIpIfStatsInErrorPackets,
        juniIpIfStatsInSpoofedPackets,
        juniIpIfStatsInForwardedPackets,
        juniIpIfStatsInForwardedOctets,
        juniIpIfStatsOutForwardedPackets,
        juniIpIfStatsOutForwardedOctets,
        juniIpIfStatsOutSchedDropPackets,
        juniIpIfStatsOutSchedDropOctets,
        juniIpIfStatsOutRequestedPackets,
        juniIpIfStatsOutRequestedOctets,
        juniIpIfStatsOutPoliciedPackets,
        juniIpIfStatsOutPoliciedOctets,
        juniIpIfStatsGreenOutSchedDropPackets,
        juniIpIfStatsYellowOutSchedDropPackets,
        juniIpIfStatsRedOutSchedDropPackets,
        juniIpIfStatsGreenOutSchedDropOctets,
        juniIpIfStatsYellowOutSchedDropOctets,
        juniIpIfStatsRedOutSchedDropOctets,

        juniIpIfAssocIpIfIndex }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects for managing IP interface capabilities
        in a Juniper product.  This group became obsolete when the QoS related
        objects were obsoleted."
    ::= { juniIpGroups 7 }                                         -- JUNOSe 3.2

juniIpInterfaceGroup4  OBJECT-GROUP
    OBJECTS {
        juniIpNextIfIndex,

        juniIpIfRowStatus,
        juniIpIfLowerIfIndex,
        juniIpIfType,
        juniIpIfTypeId,
        juniIpIfSAValidationEnable,
        juniIpIfCreationType,
        juniIpIfProfileId,
        juniIpIfAlwaysUp,
        juniIpIfLoopback,
        juniIpIfLoopbackUid,
        juniIpIfDebounceTime,
        juniIpIfForwarding,
        juniIpIfForceFragmentation,
        juniIpIfSharesLowerUid,
        juniIpIfFilterOptions,
        juniIpIfName,
        juniIpIfArpTimeout,
        juniIpIfAdminSpeed,
        juniIpIfMultipathMode,
        juniIpIfSharedNhAddr,
        juniIpIfSharedNhRouterId,
        juniIpIfPrimaryIpAddress,
        juniIpIfPrimaryIpMask,
        juniIpIfOperDebounceTime,

        juniIpIfStatsInPackets,
        juniIpIfStatsInOctets,
        juniIpIfStatsInPoliciedPackets,
        juniIpIfStatsInPoliciedOctets,
        juniIpIfStatsInErrorPackets,
        juniIpIfStatsInSpoofedPackets,
        juniIpIfStatsOutForwardedPackets,
        juniIpIfStatsOutForwardedOctets,
        juniIpIfStatsOutSchedDropPackets,
        juniIpIfStatsOutSchedDropOctets,
        juniIpIfStatsOutPoliciedPackets,
        juniIpIfStatsOutPoliciedOctets,

        juniIpIfAssocIpIfIndex }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects for managing IP interface capabilities
        in a Juniper product.  This group became obsolete when the
        juniIpIfInheritNum and juniIpIfInheritNumUid objects were added and
        juniIpIfLoopback and juniIpIfLoopbackUid were deprecated."
    ::= { juniIpGroups 8 }                                         -- JUNOSe 4.0

juniIpAddressGroup3  OBJECT-GROUP
    OBJECTS {
        juniIpAdEntRowStatus,
        juniIpAdEntIfIndex,
        juniIpAdEntNetMask,
        juniIpAdEntBcastAddr,
        juniIpAdEntReasmMaxSize,
        juniIpAdEntAdminStatus,
        juniIpAdEntArpRspEnable,
        juniIpAdEntProxyArpRspEnable,
        juniIpAdEntDirectedBcastEnable,
        juniIpAdEntIcmpRedirectEnable,
        juniIpAdEntIcmpMaskReplyEnable,
        juniIpAdEntIcmpUnreachEnable,
        juniIpAdEntMtu,
        juniIpAdEntUnnumLoopbackIfIndex,
        juniIpAdEntIrdpEnable,
        juniIpAdEntAccessRouteEnable,
        juniIpAdEntAccessRouteHost,
        juniIpAdEntIsSecondary }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects for managing IP address capabilities in
        a Juniper product.  This group became obsolete when the
        juniIpAdEntUnnumInheritNumIfIndex object was added and
        juniIpAdEntUnnumLoopbackIfIndex was deprecated."
    ::= { juniIpGroups 9 }                                         -- JUNOSe 4.1

juniIpRouteGroup2  OBJECT-GROUP
    OBJECTS {
        juniIpRouteStaticDest,
        juniIpRouteStaticMask,
        juniIpRouteStaticPref,
        juniIpRouteStaticNextHop,
        juniIpRouteStaticRowStatus,
        juniIpRouteStaticIfIndex,
        juniIpRouteStaticStatus,
        juniIpRouteStaticNextHopAS,
        juniIpRouteStaticMetric,
        juniIpRouteStaticTag,

        juniIpCidrRoutePref,
        juniIpCidrRouteArea,
        juniIpCidrRouteTag }
    STATUS      obsolete
    DESCRIPTION
        "A collection of objects for managing IP routing capabilities in a
        Juniper product."
    ::= { juniIpGroups 10 }                                        -- JUNOSe 4.1

juniIpGlobalGroup2  OBJECT-GROUP
    OBJECTS {
        juniIpDebounceTime,
        juniIpRouterId,
        juniIpSourceRoutingAdminStatus,
        juniIpVpnIdOui,
        juniIpVpnIdIndex,
        juniIpBgpCommunityNewFormat,
        juniIpBgpAsConfedSetNewFormat }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of IP global objects for managing instances of IP
        in a Juniper product. This group became obsolete when juniIpVpnIdOui and 
	juniIpVpnIdIndex were obsoleted."
    ::= { juniIpGroups 11 }                                        -- JUNOSe 4.1

juniIpInterfaceGroup5  OBJECT-GROUP
    OBJECTS {
        juniIpNextIfIndex,

        juniIpIfRowStatus,
        juniIpIfLowerIfIndex,
        juniIpIfType,
        juniIpIfTypeId,
        juniIpIfSAValidationEnable,
        juniIpIfCreationType,
        juniIpIfProfileId,
        juniIpIfAlwaysUp,
        juniIpIfDebounceTime,
        juniIpIfForwarding,
        juniIpIfForceFragmentation,
        juniIpIfSharesLowerUid,
        juniIpIfFilterOptions,
        juniIpIfName,
        juniIpIfArpTimeout,
        juniIpIfAdminSpeed,
        juniIpIfMultipathMode,
        juniIpIfSharedNhAddr,
        juniIpIfSharedNhRouterId,
        juniIpIfPrimaryIpAddress,
        juniIpIfPrimaryIpMask,
        juniIpIfOperDebounceTime,
        juniIpIfRouterIndex,
        juniIpIfInheritNum,
        juniIpIfInheritNumUid,

        juniIpIfStatsInPackets,
        juniIpIfStatsInOctets,
        juniIpIfStatsInPoliciedPackets,
        juniIpIfStatsInPoliciedOctets,
        juniIpIfStatsInErrorPackets,
        juniIpIfStatsInSpoofedPackets,
        juniIpIfStatsOutForwardedPackets,
        juniIpIfStatsOutForwardedOctets,
        juniIpIfStatsOutSchedDropPackets,
        juniIpIfStatsOutSchedDropOctets,
        juniIpIfStatsOutPoliciedPackets,
        juniIpIfStatsOutPoliciedOctets,

        juniIpIfAssocIpIfIndex }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects for managing IP interface capabilities
        in a Juniper product.  This group became obsolete when the
        juniIpIfAnalyzerMode object was added."
    ::= { juniIpGroups 12 }                                        -- JUNOSe 5.0

juniIpAddressGroup4  OBJECT-GROUP
    OBJECTS {
        juniIpAdEntRowStatus,
        juniIpAdEntIfIndex,
        juniIpAdEntNetMask,
        juniIpAdEntBcastAddr,
        juniIpAdEntReasmMaxSize,
        juniIpAdEntAdminStatus,
        juniIpAdEntArpRspEnable,
        juniIpAdEntProxyArpRspEnable,
        juniIpAdEntDirectedBcastEnable,
        juniIpAdEntIcmpRedirectEnable,
        juniIpAdEntIcmpMaskReplyEnable,
        juniIpAdEntIcmpUnreachEnable,
        juniIpAdEntMtu,
        juniIpAdEntIrdpEnable,
        juniIpAdEntAccessRouteEnable,
        juniIpAdEntAccessRouteHost,
        juniIpAdEntIsSecondary,
        juniIpAdEntUnnumInheritNumIfIndex }
    STATUS      current
    DESCRIPTION
        "A collection of objects for managing IP address capabilities in a
        Juniper product."
    ::= { juniIpGroups 13 }                                        -- JUNOSe 5.0

juniIpInterfaceDeprecatedGroup  OBJECT-GROUP
    OBJECTS {
        juniIpIfLoopback,
        juniIpIfLoopbackUid }
    STATUS      deprecated
    DESCRIPTION
        "A collection of deprecated objects for managing IP interface
        capabilities in a Juniper product.  This group may continue to be
        support on some products."
    ::= { juniIpGroups 14 }                                        -- JUNOSe 5.0

juniIpAddressDeprecatedGroup  OBJECT-GROUP
    OBJECTS {
        juniIpAdEntIgmpEnable,
        juniIpAdEntUnnumLoopbackIfIndex }
    STATUS      deprecated
    DESCRIPTION
        "A collection of deprecated objects for managing IP address capabilities
        in a Juniper product.  This group may continue to be support on some
        products."
    ::= { juniIpGroups 15 }                                        -- JUNOSe 5.0

juniIpInterfaceGroup6  OBJECT-GROUP
    OBJECTS {
        juniIpNextIfIndex,

        juniIpIfRowStatus,
        juniIpIfLowerIfIndex,
        juniIpIfType,
        juniIpIfTypeId,
        juniIpIfSAValidationEnable,
        juniIpIfCreationType,
        juniIpIfProfileId,
        juniIpIfAlwaysUp,
        juniIpIfDebounceTime,
        juniIpIfForwarding,
        juniIpIfForceFragmentation,
        juniIpIfSharesLowerUid,
        juniIpIfFilterOptions,
        juniIpIfName,
        juniIpIfArpTimeout,
        juniIpIfAdminSpeed,
        juniIpIfMultipathMode,
        juniIpIfSharedNhAddr,
        juniIpIfSharedNhRouterId,
        juniIpIfPrimaryIpAddress,
        juniIpIfPrimaryIpMask,
        juniIpIfOperDebounceTime,
        juniIpIfRouterIndex,
        juniIpIfInheritNum,
        juniIpIfInheritNumUid,
        juniIpIfAnalyzerMode,
        juniIpIfAutoConfigure,

        juniIpIfStatsInPackets,
        juniIpIfStatsInOctets,
        juniIpIfStatsInPoliciedPackets,
        juniIpIfStatsInPoliciedOctets,
        juniIpIfStatsInErrorPackets,
        juniIpIfStatsInSpoofedPackets,
        juniIpIfStatsOutForwardedPackets,
        juniIpIfStatsOutForwardedOctets,
        juniIpIfStatsOutSchedDropPackets,
        juniIpIfStatsOutSchedDropOctets,
        juniIpIfStatsOutPoliciedPackets,
        juniIpIfStatsOutPoliciedOctets,

        juniIpIfAssocIpIfIndex }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects for managing IP interface capabilities
        in a Juniper product.  This group became obsolete when the
        juniIpIfTcpMss object was added."
    ::= { juniIpGroups 16 }                                        -- JUNOSe 5.1

juniIpIfSummaryGroup  OBJECT-GROUP
    OBJECTS {
        juniIpIfSummaryTotalIntf,
        juniIpIfSummaryTotalIntfUp,
        juniIpIfSummaryTotalIntfDown,
        juniIpIfSummaryTotalIntfProtUp,
        juniIpIfSummaryTotalIntfProtDown,
        juniIpIfSummaryTotalIntfProtNotPresent }
    STATUS      current
    DESCRIPTION
        "A collection of IP Interface Summary Statistics."
    ::= { juniIpGroups 17 }                                        -- JUNOSe 5.1

juniIpInterfaceGroup7  OBJECT-GROUP
    OBJECTS {
        juniIpNextIfIndex,

        juniIpIfRowStatus,
        juniIpIfLowerIfIndex,
        juniIpIfType,
        juniIpIfTypeId,
        juniIpIfSAValidationEnable,
        juniIpIfCreationType,
        juniIpIfProfileId,
        juniIpIfAlwaysUp,
        juniIpIfDebounceTime,
        juniIpIfForwarding,
        juniIpIfForceFragmentation,
        juniIpIfSharesLowerUid,
        juniIpIfFilterOptions,
        juniIpIfName,
        juniIpIfArpTimeout,
        juniIpIfAdminSpeed,
        juniIpIfMultipathMode,
        juniIpIfSharedNhAddr,
        juniIpIfSharedNhRouterId,
        juniIpIfPrimaryIpAddress,
        juniIpIfPrimaryIpMask,
        juniIpIfOperDebounceTime,
        juniIpIfRouterIndex,
        juniIpIfInheritNum,
        juniIpIfInheritNumUid,
        juniIpIfAnalyzerMode,
        juniIpIfAutoConfigure,
        juniIpIfTcpMss,

        juniIpIfStatsInPackets,
        juniIpIfStatsInOctets,
        juniIpIfStatsInPoliciedPackets,
        juniIpIfStatsInPoliciedOctets,
        juniIpIfStatsInErrorPackets,
        juniIpIfStatsInSpoofedPackets,
        juniIpIfStatsOutForwardedPackets,
        juniIpIfStatsOutForwardedOctets,
        juniIpIfStatsOutSchedDropPackets,
        juniIpIfStatsOutSchedDropOctets,
        juniIpIfStatsOutPoliciedPackets,
        juniIpIfStatsOutPoliciedOctets,

        juniIpIfAssocIpIfIndex }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects for managing IP interface capabilities
        in a Juniper product.  This group became obsolete when the
        juniIpIfInitSeqPrefOper and juniIpIfInitSeqPrefAdmin objects were added."
    ::= { juniIpGroups 18 }                                        -- JUNOSe 5.2

juniIpGlobalGroup3  OBJECT-GROUP
    OBJECTS {
        juniIpDebounceTime,
        juniIpRouterId,
        juniIpSourceRoutingAdminStatus,
        juniIpBgpCommunityNewFormat,
        juniIpBgpAsConfedSetNewFormat }
    STATUS      current
    DESCRIPTION
        "A collection of IP global objects for managing instances of IP in a
        Juniper product."
    ::= { juniIpGroups 19 } 

juniIpRouteGroup3  OBJECT-GROUP
    OBJECTS {
        juniIpRouteTableLimit,
        juniIpRouteTableWarnPercent,
        juniIpRouteTableWarnOnly,
        juniIpRouteTableWarnThreshold,
        juniIpRouteStaticDest,
        juniIpRouteStaticMask,
        juniIpRouteStaticPref,
        juniIpRouteStaticNextHop,
        juniIpRouteStaticRowStatus,
        juniIpRouteStaticIfIndex,
        juniIpRouteStaticStatus,
        juniIpRouteStaticNextHopAS,
        juniIpRouteStaticMetric,
        juniIpRouteStaticTag,

        juniIpCidrRoutePref,
        juniIpCidrRouteArea,
        juniIpCidrRouteTag }
    STATUS      current
    DESCRIPTION
        "A collection of objects for managing IP routing capabilities in a
        Juniper product."
    ::= { juniIpGroups 20 }                                        -- JUNOSe 6.1

juniIpNotificationGroup  NOTIFICATION-GROUP
    NOTIFICATIONS {
        juniIpRouteTableTrapRouteLimitExceeded,
        juniIpRouteTableTrapRouteLimitRemove,
        juniIpRouteTableTrapWarnThresholdExceeded }
    STATUS      obsolete
    DESCRIPTION
        "The management notifications pertaining to IP Route Table state changes."
    ::= { juniIpGroups 21 }                                   -- JUNOSe 6.1

juniIpNotificationGroup1  NOTIFICATION-GROUP
    NOTIFICATIONS {
        juniIpRouteTableTrapRouteLimitExceeded,
        juniIpRouteTableTrapRouteLimitRemove,
        juniIpRouteTableTrapWarnThresholdExceeded,
        juniIpTrapSaValidationFailure }
    STATUS      current
    DESCRIPTION
        "The management notifications pertaining to IP."
    ::= { juniIpGroups 22 }                                   -- JUNOSe 7.0

juniIpMIBNotificationObjectsGroup  OBJECT-GROUP
    OBJECTS {
        juniIpIfSaValFailSrcIpAddr,
        juniIpIfSaValFailDestIpAddr }
    STATUS      current
    DESCRIPTION
        "The management notification objects pertaining to IP."
    ::= { juniIpGroups 23 }                                   -- JUNOSe 7.0

juniIpRouteSummaryGroup  OBJECT-GROUP
    OBJECTS {
        juniIpRouteSummaryUnicastTotalRoutes,
        juniIpRouteSummaryUnicastTotalBytes,
        juniIpRouteSummaryUnicastIsisRoutes,
        juniIpRouteSummaryUnicastIsisLevel1Routes,
        juniIpRouteSummaryUnicastIsisLevel2Routes,
        juniIpRouteSummaryUnicastRipRoutes,
        juniIpRouteSummaryUnicastStaticRoutes,
        juniIpRouteSummaryUnicastConnectedRoutes,
        juniIpRouteSummaryUnicastBgpRoutes,
        juniIpRouteSummaryUnicastOspfRoutes,      
        juniIpRouteSummaryUnicastIntraAreaOspfRoutes,
        juniIpRouteSummaryUnicastOtherInternalRoutes,
        juniIpRouteSummaryUnicastExternalOspfRoutes,
        juniIpRouteSummaryUnicastInterAreaOspfRoutes,
        juniIpRouteSummaryUnicastAccessRoutes,
        juniIpRouteSummaryUnicastIntCreatedAccessHostRoutes,
        juniIpRouteSummaryUnicastIntDialoutRoutes,
	juniIpRouteSummaryUnicastRouteMemoryActive,
        juniIpRouteSummaryUnicastLastRouteAddedOrDeletedIP,
        juniIpRouteSummaryUnicastLastRouteAddedOrDeletedMask,
        juniIpRouteSummaryUnicastLastRouteAddedOrDeletedClient,
        juniIpRouteSummaryUnicastLastRouteAddedOrDeletedDate,
        juniIpRouteSummaryMulticastTotalRoutes,
        juniIpRouteSummaryMulticastTotalBytes,
        juniIpRouteSummaryMulticastIsisRoutes,
        juniIpRouteSummaryMulticastLevel1IsisRoutes,
        juniIpRouteSummaryMulticastLevel2IsisRoutes,
        juniIpRouteSummaryMulticastRipRoutes,
        juniIpRouteSummaryMulticastStaticRoutes,
        juniIpRouteSummaryMulticastConnectedRoutes,
        juniIpRouteSummaryMulticastBgpRoutes,
        juniIpRouteSummaryMulticastOspfRoutes,
        juniIpRouteSummaryMulticastIntraAreaOspfRoutes,
        juniIpRouteSummaryMulticastInterAreaOspfRoutes,
        juniIpRouteSummaryMulticastExternalOspfRoutes,
        juniIpRouteSummaryMulticastOtherInternalRoutes,
        juniIpRouteSummaryMulticastAccessRoutes,
        juniIpRouteSummaryMulticastIntCreatedAccessHostRoutes,
        juniIpRouteSummaryMultiastIntDialoutRoutes,
	juniIpRouteSummaryMulticastRouteMemoryActive,
        juniIpRouteSummaryMulticastLastRouteAddedOrDeletedIP,
        juniIpRouteSummaryMulticastLastRouteAddedOrDeletedMask,
        juniIpRouteSummaryMulticastLastRouteAddedOrDeletedClient,
        juniIpRouteSummaryMulticastLastRouteAddedOrDeletedDate }
    STATUS      current
    DESCRIPTION
        "The management notifications pertaining to IP Route Table state changes."
    ::= { juniIpGroups 24 }                                   -- JUNOSe 7.0
    
juniIpRouteStaticBFDGroup  OBJECT-GROUP
    OBJECTS {
        juniIpRouteStaticBfdEnable,
    	juniIpRouteStaticBfdMinRxInterval,
    	juniIpRouteStaticBfdMinTxInterval,
    	juniIpRouteStaticBfdMultiplier
 }
    STATUS      current
    DESCRIPTION
        "The management notifications pertaining to IP Route Table state changes."
    ::= { juniIpGroups 25 }     
    
juniIpInterfaceGroup8  OBJECT-GROUP
    OBJECTS {
        juniIpNextIfIndex,

        juniIpIfRowStatus,
        juniIpIfLowerIfIndex,
        juniIpIfType,
        juniIpIfTypeId,
        juniIpIfSAValidationEnable,
        juniIpIfCreationType,
        juniIpIfProfileId,
        juniIpIfAlwaysUp,
        juniIpIfDebounceTime,
        juniIpIfForwarding,
        juniIpIfForceFragmentation,
        juniIpIfSharesLowerUid,
        juniIpIfFilterOptions,
        juniIpIfName,
        juniIpIfArpTimeout,
        juniIpIfAdminSpeed,
        juniIpIfMultipathMode,
        juniIpIfSharedNhAddr,
        juniIpIfSharedNhRouterId,
        juniIpIfPrimaryIpAddress,
        juniIpIfPrimaryIpMask,
        juniIpIfOperDebounceTime,
        juniIpIfRouterIndex,
        juniIpIfInheritNum,
        juniIpIfInheritNumUid,
        juniIpIfAnalyzerMode,
        juniIpIfAutoConfigure,
        juniIpIfTcpMss,
        juniIpIfInitSeqPrefOper,
        juniIpIfInitSeqPrefAdmin,

        juniIpIfStatsInPackets,
        juniIpIfStatsInOctets,
        juniIpIfStatsInPoliciedPackets,
        juniIpIfStatsInPoliciedOctets,
        juniIpIfStatsInErrorPackets,
        juniIpIfStatsInSpoofedPackets,
        juniIpIfStatsOutForwardedPackets,
        juniIpIfStatsOutForwardedOctets,
        juniIpIfStatsOutSchedDropPackets,
        juniIpIfStatsOutSchedDropOctets,
        juniIpIfStatsOutPoliciedPackets,
        juniIpIfStatsOutPoliciedOctets,

        juniIpIfAssocIpIfIndex }
    STATUS      obsolete
    DESCRIPTION
        "A collection of objects for managing IP interface capabilities in a
        Juniper product."
    ::= { juniIpGroups 26 }                                      -- JUNOSe 7.3.2

juniIpInterfaceGroup9  OBJECT-GROUP
    OBJECTS {
        juniIpNextIfIndex,

        juniIpIfRowStatus,
        juniIpIfLowerIfIndex,
        juniIpIfType,
        juniIpIfTypeId,
        juniIpIfSAValidationEnable,
        juniIpIfCreationType,
        juniIpIfProfileId,
        juniIpIfAlwaysUp,
        juniIpIfDebounceTime,
        juniIpIfForwarding,
        juniIpIfForceFragmentation,
        juniIpIfSharesLowerUid,
        juniIpIfFilterOptions,
        juniIpIfName,
        juniIpIfArpTimeout,
        juniIpIfAdminSpeed,
        juniIpIfMultipathMode,
        juniIpIfSharedNhAddr,
        juniIpIfSharedNhRouterId,
        juniIpIfPrimaryIpAddress,
        juniIpIfPrimaryIpMask,
        juniIpIfOperDebounceTime,
        juniIpIfRouterIndex,
        juniIpIfInheritNum,
        juniIpIfInheritNumUid,
        juniIpIfAnalyzerMode,
        juniIpIfAutoConfigure,
        juniIpIfTcpMss,
        juniIpIfInitSeqPrefOper,
        juniIpIfInitSeqPrefAdmin,
		juniIpIfArpSpoofCheck,

        juniIpIfStatsInPackets,
        juniIpIfStatsInOctets,
        juniIpIfStatsInPoliciedPackets,
        juniIpIfStatsInPoliciedOctets,
        juniIpIfStatsInErrorPackets,
        juniIpIfStatsInSpoofedPackets,
        juniIpIfStatsOutForwardedPackets,
        juniIpIfStatsOutForwardedOctets,
        juniIpIfStatsOutSchedDropPackets,
        juniIpIfStatsOutSchedDropOctets,
        juniIpIfStatsOutPoliciedPackets,
        juniIpIfStatsOutPoliciedOctets,

        juniIpIfAssocIpIfIndex }
    STATUS      current
    DESCRIPTION
        "A collection of objects for managing IP interface capabilities in a
        Juniper product."
    ::= { juniIpGroups 27 }                                      -- JUNOSe 9.3

END
