--  =================================================================
-- Copyright (C) 2008 by  HUAWEI TECHNOLOGIES. All rights reserved
-- 
-- Description: HUAWEI DLDP MIB, this mib will maintain information of DLDP 
--              protocol for datacomm product.  
-- Reference:
-- Version:     V1.00
-- History:
--  
--  V1.00 2008-07-15 initial version
-- =================================================================

HUAWEI-DLDP-MIB DEFINITIONS ::= BEGIN
    IMPORTS
    TruthValue,MacAddress,TEXTUAL-CONVENTION,RowStatus
        FROM SNMPv2-TC

    MODULE-IDENTITY, OBJECT-TYPE, Integer32, Counter32,
    OBJECT-IDENTITY, Unsigned32, NOTIFICATION-TYPE
        FROM SNMPv2-SMI
                
    hwDatacomm
        FROM HUAWEI-MIB
               
    EnabledStatus
        FROM P-BRIDGE-MIB;
 
    hwDldpMIB MODULE-IDENTITY
        LAST-UPDATED "200807151430Z"        -- July 15, 2008 at 14:30 GMT
        ORGANIZATION 
            "Huawei Technologies co.,Ltd."
        CONTACT-INFO 
            "R&D NanJing, Huawei Technologies co.,Ltd.
            High hope mansion, 
            Baixia road,
            Nanjing city
            Zip:100085
            Http://www.huawei.com
            E-mail:support@huawei.com        
            Zip:100000
            "
        DESCRIPTION
            "This file is a DLDP-MIB. It provides the functions such as
           globally enabling or disabling the DLDP protocol, enabling the global
           alarm, clearing statistics on ports and configuring work mode."
            ::= { hwDatacomm 173 }  
         
      -- Textual Convention
                 
        PortIndex ::= TEXTUAL-CONVENTION
               STATUS    current
            DESCRIPTION
                "Each port is uniquely identified by a port number. The port number ranges from 0
                to 575."
              SYNTAX Integer32(0..575) 
              
    -- ============================================================================
    -- Node definitions
    -- ============================================================================ 

    hwDldpObjects  OBJECT IDENTIFIER ::= { hwDldpMIB 1}
    
    hwDldpPortTrapObjects OBJECT IDENTIFIER ::= { hwDldpMIB 2}

    hwDldpTraps OBJECT IDENTIFIER ::= { hwDldpMIB 3 }  
    
    hwDldpConformance  OBJECT IDENTIFIER ::= { hwDldpMIB 4 }
 

  -- ============================================================================
  --
  -- ======================= Objects definitions=================================
  --
  -- ============================================================================  

  hwDldpConfiguration  OBJECT IDENTIFIER ::= { hwDldpObjects 1}
  hwDldpStatistics     OBJECT IDENTIFIER ::= { hwDldpObjects 2} 

    hwDldpEnable OBJECT-TYPE 
        SYNTAX   EnabledStatus 
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Globally enable or disable the DLDP configuration. If the hwDldpEnable 
                is 1, DLDP is enabled. If the hwDldpEnable is 2, DLDP is disabled. 
            By default, DLDP is disabled."   
        DEFVAL { 2 }
        ::= { hwDldpConfiguration 1 }   

    hwDldpUnidirectionalShutdown OBJECT-TYPE 
        SYNTAX   INTEGER 
           { 
            auto(1),
            manual(2)
        }
        MAX-ACCESS read-write
        STATUS  current
        DESCRIPTION
            "When the device discovers a one-way link, the shutdown mode of port. The modes include
            auto and manual. By default, DLDP is auto."
        DEFVAL { 1 }        
        ::= { hwDldpConfiguration 2 }     
    
    hwDldpWorkMode OBJECT-TYPE 
        SYNTAX   INTEGER 
           { 
            normal(1),
            enhance(2)
        }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "It configures the work mode of the DLDP protocol, including normal and enhanced mode.
            By default, the mode is enhanced." 
        DEFVAL { 2 }  
        ::= { hwDldpConfiguration 3 } 
        
   hwDldpAdvertInterval OBJECT-TYPE 
        SYNTAX Integer32(1..100)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Global interval for sending advertisement packets for the DLDP configuration.
            By default, the interval is 5s."     
        DEFVAL { 5 }
        ::= { hwDldpConfiguration 4 }
        
   hwDelayDownTimer OBJECT-TYPE 
        SYNTAX Integer32(1..5)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Global timeout of DelayDown timer. The value rangs from 1s to 5s,
            By default, the time is 1s."     
        DEFVAL { 1 }
        ::= { hwDldpConfiguration 5 }
        
   hwDldpAuthenMode OBJECT-TYPE 
        SYNTAX   INTEGER 
           { 
            none(1),
            md5(2),
            simple(3)
        }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Global authentication mode of the DLDP configuration. It has three authentication
             modes, including none, md5,and simple. By default the authentication mode
             is none."     
        DEFVAL { 1 }
        ::= { hwDldpConfiguration 6 }
        
   hwDldpMd5Password OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (1..24)) 
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Global md5 password for authentication when authentication is md5."
        ::= { hwDldpConfiguration 7 }
    
   hwDldpSimplePassword OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (1..16)) 
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Global simple password for authentication when authentication is simple."
        ::= { hwDldpConfiguration 8 }
  
   hwDldpPortTable  OBJECT-TYPE
      SYNTAX SEQUENCE OF HwDldpPortEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION 
            "DLDP port configuration table."
      ::= { hwDldpConfiguration  9 }
      
   hwDldpPortEntry OBJECT-TYPE
        SYNTAX HwDldpPortEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
               "Entries of the DLDP port configuration table."
        INDEX{ hwDldpPortIndex }
        ::= { hwDldpPortTable 1}  
  
   HwDldpPortEntry ::=
        SEQUENCE{    
                    hwDldpPortIndex            PortIndex,
                    hwDldpPortStateReset       TruthValue,
                    hwDldpPortState            INTEGER,
                    hwDldpPortLinkState        INTEGER,
                    hwDldpResetStatistics      TruthValue,
                    hwDldpRowStatus            RowStatus                                     
                    }
                    
   hwDldpPortIndex  OBJECT-TYPE
        SYNTAX PortIndex
        MAX-ACCESS not-accessible
        STATUS current
           DESCRIPTION 
                   "It describes enabled DLDP port index. Each port is uniquely identified by a port number. It ranges from 0
                    to 575."     
           ::= {hwDldpPortEntry 1}
                      
   hwDldpPortStateReset OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-create
        STATUS current
           DESCRIPTION 
               "It describes the DLDP status of the reset port."
           DEFVAL { false }    
           ::= {hwDldpPortEntry 2}
           
       hwDldpPortState OBJECT-TYPE
        SYNTAX INTEGER
        { 
            initial(1),
            inactive(2),
            active(3),
            advertisement(4), 
            probe(5),
            disable(6),
            delayDown(7)            
        }
        MAX-ACCESS read-only
        STATUS current
           DESCRIPTION 
               "Port state has seven states, including initial, inactive, active,
               advertisement, probe, disable, and delayDown."     
           ::= {hwDldpPortEntry 3}
       
       
    hwDldpPortLinkState OBJECT-TYPE
        SYNTAX INTEGER
        {
           up(1),
            down(2)     
        }
        MAX-ACCESS read-only
        STATUS current
           DESCRIPTION 
               "Port state has two modes, including up and down."     
           ::= {hwDldpPortEntry 4}
             
       hwDldpResetStatistics OBJECT-TYPE
           SYNTAX TruthValue
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "It clears the statistics of packets received and sent on the current 
             port."
        ::= { hwDldpPortEntry 5 }
        
       hwDldpRowStatus OBJECT-TYPE
           SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            " Operation of CreateAndGo can be
             used to create a new instance, and operation of Destroy be 
             used to destroy an existent index. But these operations 
             will not take effect if they are not activated by running the
             command of activating or setting mib node of hwDldpEnable."
        ::= { hwDldpPortEntry 6 }
        
    hwDldpNeighbourTable  OBJECT-TYPE
      SYNTAX SEQUENCE OF HwDldpNeighbourEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION 
            "DLDP Neighbour configuration table."
      ::= { hwDldpConfiguration  10 }
      
   hwDldpNeighbourEntry OBJECT-TYPE
        SYNTAX HwDldpNeighbourEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
               "Entries of the DLDP Neighbour configuration table."
        INDEX{ hwDldpPortIndex, hwDldpNeighbourMacAddr, hwDldpNeighbourPortIndex}
        ::= { hwDldpNeighbourTable 1}
                    
       HwDldpNeighbourEntry ::=
        SEQUENCE  {    
                    hwDldpNeighbourMacAddr
                            MacAddress,
                    hwDldpNeighbourPortIndex
                            Integer32,
                    hwDldpNeighbourPortName
                            OCTET STRING,
                    hwDldpNeighbourState
                               INTEGER,                           
                    hwDldpNeighbourAgeTime
                            Integer32        
                    }
                     
   hwDldpNeighbourMacAddr OBJECT-TYPE
        SYNTAX MacAddress
        MAX-ACCESS not-accessible
        STATUS current
           DESCRIPTION 
               "When the activated port detects a neighbor, it can record the neighbor information, including
               MAC address of neighbor. The port may detect multiple neighbors."   
           ::= {hwDldpNeighbourEntry 1}
                                
       hwDldpNeighbourPortIndex OBJECT-TYPE
        SYNTAX  Integer32(0..65535)
        MAX-ACCESS not-accessible
        STATUS current
           DESCRIPTION 
               "When the activated port detects a neighbor, it can record the port index of the neighbour."     
           ::= {hwDldpNeighbourEntry 2}
           
       hwDldpNeighbourPortName OBJECT-TYPE
        SYNTAX  OCTET STRING(SIZE(0..255))
        MAX-ACCESS read-only
        STATUS current
           DESCRIPTION 
               "When the activated port detects a neighbor, it can record the port name of the neighbour."     
           ::= {hwDldpNeighbourEntry 3}
           
    hwDldpNeighbourState OBJECT-TYPE
        SYNTAX INTEGER
        {
           unknown(1),
           oneWay(2),
           twoWay(3)
        }
        MAX-ACCESS read-only
        STATUS current
           DESCRIPTION 
               "When the activated port detects a neighbor, it can record the state of the neighbour, and its value includes unknown, one way, and two way."
           ::= {hwDldpNeighbourEntry 4}
            
    hwDldpNeighbourAgeTime OBJECT-TYPE
        SYNTAX  Integer32(3..300)
        MAX-ACCESS read-only
        STATUS current
           DESCRIPTION 
               "When the activated port detects a neighbor, it can record the aging time of the neighbor. The aging time
               is three times the interval for sending advertisement packets." 
           DEFVAL { 15 }    
           ::= {hwDldpNeighbourEntry 5}
           
   hwDldpPortStatisticsTable  OBJECT-TYPE
      SYNTAX SEQUENCE OF HwDldpPortStatisticsEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION 
            "DLDP port statics configuration table."
      ::= { hwDldpStatistics  1 }
      
   hwDldpPortStatisticsEntry OBJECT-TYPE
        SYNTAX HwDldpPortStatisticsEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION 
               "Entries of the table of the packets sent or received on the DLDP port."
        INDEX{ hwDldpPortIndex }
        ::= { hwDldpPortStatisticsTable 1}  
  
   HwDldpPortStatisticsEntry ::=
        SEQUENCE  {    
                    hwDldpPortStatisticsTx
                              Counter32,
                    hwDldpPortStatisticsRxTotal
                              Counter32,
                    hwDldpPortStatisticsRxError
                               Counter32,
                    hwDldpPortStatisticsRxLoop
                              Counter32,
                    hwDldpPortStatisticsRxValid
                              Counter32,        
                    hwDldpPortStatisticsRxAuthenFail
                              Counter32                                               
                    }
                   
    hwDldpPortStatisticsTx OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
                   "It describes the number of packets sent on the activated port."     
           ::= {hwDldpPortStatisticsEntry 1}
           
        hwDldpPortStatisticsRxTotal OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
                   "It describes the number of packets received on the activated port."     
           ::= {hwDldpPortStatisticsEntry 2}

     hwDldpPortStatisticsRxError OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
                   "It describes the number of error packets received on the activated port."     
           ::= {hwDldpPortStatisticsEntry 3}
           
        hwDldpPortStatisticsRxLoop OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
                   "It describes the number of loop packets received on the activated port."     
           ::= {hwDldpPortStatisticsEntry 4}
           
        hwDldpPortStatisticsRxValid OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
                   "It describes the number of valid packets received on the activated port."     
           ::= {hwDldpPortStatisticsEntry 5}
           
        hwDldpPortStatisticsRxAuthenFail OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION 
                   "It describes the number of authentication failure packets received on the activated port."     
           ::= {hwDldpPortStatisticsEntry 6}
     
     hwDldpTrapPortIndex OBJECT-TYPE 
        SYNTAX PortIndex
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
            "It describes the index of the activated port that detected one way or found that two way is resumed."     
        ::= { hwDldpPortTrapObjects 1 }
                         
---Notifycation        
      hwDldpUnidirectionalLink  NOTIFICATION-TYPE
      OBJECTS {hwDldpTrapPortIndex}
      STATUS current    
    DESCRIPTION 
          "Notify the NMS that the DLDP detected one way. The hwDldpNeighbourPortIndex node is the port index."
    ::= { hwDldpTraps 1}

      hwDldpLinkResume  NOTIFICATION-TYPE
      OBJECTS {hwDldpTrapPortIndex}
     STATUS current    
    DESCRIPTION 
          "Notify the NMS that the DLDP detected that unidirectional link was resumed. The hwDldpNeighbourPortIndex node is port index."
    ::= { hwDldpTraps 2}  
        
    --
    -- ***********************************************************
    --
    -- HAUWEIDLDPMIBCONFORMANCE
    --
    -- ***********************************************************
    --
     
    hwDldpCompliances OBJECT IDENTIFIER ::= { hwDldpConformance 1 }
    hwDldpGroups OBJECT IDENTIFIER ::= { hwDldpConformance 2 }
    -- compliance statements
    hwDldpCompliance MODULE-COMPLIANCE
    STATUS current
    DESCRIPTION
        "The compliance statement for SNMP entities which implement
        the HUAWEI-DLDP-MIB."
    MODULE -- this module
    MANDATORY-GROUPS { 
    hwDldpConfigGroup,
    hwDldpStatisticsGroup,
    hwDldpPortGroup,
    hwDldpPortTrapGroup,
    hwDldpTrapGroup
    }
    ::= { hwDldpCompliances 1 }    
       
    -- MIB groupings
    hwDldpConfigGroup OBJECT-GROUP
    OBJECTS {  
    hwDldpEnable,
    hwDldpUnidirectionalShutdown,
    hwDldpWorkMode,
    hwDldpAdvertInterval,
    hwDelayDownTimer, 
    hwDldpAuthenMode,
    hwDldpMd5Password,
    hwDldpSimplePassword
    }
    STATUS current
    DESCRIPTION
        "The collection of objects which are used to configure the
        DLDP implementation behavior.
        This group is mandatory for agents which implement the DLDP."
    ::= { hwDldpGroups 1 }     
    
    hwDldpStatisticsGroup OBJECT-GROUP
    OBJECTS {  
    hwDldpPortStatisticsTx,    
    hwDldpPortStatisticsRxTotal,
    hwDldpPortStatisticsRxError,
    hwDldpPortStatisticsRxLoop,
    hwDldpPortStatisticsRxValid,
    hwDldpPortStatisticsRxAuthenFail        
    }
    STATUS current
    DESCRIPTION
        "The collection of objects which are used to represent DLDP
         statistics.
        This group is mandatory for agents which implement the DLDP
        and have the capability of receiving and transmitting DLDP frames."
    ::= { hwDldpGroups 2 } 
   
    hwDldpPortGroup OBJECT-GROUP
    OBJECTS {  
    hwDldpPortStateReset,
    hwDldpPortState,
    hwDldpPortLinkState,
    hwDldpResetStatistics,
    hwDldpRowStatus,
    hwDldpNeighbourPortName,
    hwDldpNeighbourState,
    hwDldpNeighbourAgeTime     
    }
    STATUS current
    DESCRIPTION
        "The collection of objects indicates the information of port."
    ::= { hwDldpGroups 3 } 
    
    hwDldpPortTrapGroup OBJECT-GROUP
    OBJECTS { hwDldpTrapPortIndex }
    STATUS current
    DESCRIPTION
        "The collection of objects indicates that the activated port index detected one way or found that two way is resumed." 
    ::= { hwDldpGroups 4 }
    
       hwDldpTrapGroup NOTIFICATION-GROUP
    NOTIFICATIONS {  
    hwDldpUnidirectionalLink,
    hwDldpLinkResume            
    }
    STATUS current
    DESCRIPTION
        "The collection of notifications used to indicate that the HUAWEI-DLDP-MIB
        data is consistent and indicate the general status information.
        This group is mandatory for agents which implement the DLDP
        and have the capability of receiving DLDP frames."
    ::= { hwDldpGroups 5 }  
    
END     
    
--
-- HUAWEI-DLDP-MIB.mib
--     
