DS3-MIB DEFINITIONS ::= BEGIN

     IMPORTS
          MODULE-IDENTITY, OBJECT-TYPE,
          NOTIFICATION-TYPE, transmission         FROM SNMPv2-SMI
          DisplayString, TimeStamp, TruthValue    FROM SNMPv2-TC
          MODULE-COMPLIANCE, OBJECT-GROUP,
          NOTIFICATION-GROUP                      FROM SNMPv2-CONF
          InterfaceIndex                          FROM IF-MIB
          PerfCurrentCount, PerfIntervalCount,
          PerfTotalCount                          FROM PerfHist-TC-MIB;

     ds3 MODULE-IDENTITY
         LAST-UPDATED "9808012130Z"
         ORGANIZATION "IETF Trunk MIB Working Group"
         CONTACT-INFO
           "        David Fowler

            Postal: Newbridge Networks Corporation
                    600 March Road
                    Kanata, Ontario, Canada K2K 2E6

                    Tel: +1 613 591 3600
                    Fax: +1 613 599 3667

            E-mail: davef@newbridge.com"
         DESCRIPTION
              "The is the MIB module that describes
               DS3 and E3 interfaces objects."

         ::= { transmission 30 }

     -- The DS3/E3 Near End Group

     -- The DS3/E3 Near End Group consists of four tables:
     --    DS3/E3 Configuration
     --    DS3/E3 Current
     --    DS3/E3 Interval
     --    DS3/E3 Total

     -- the DS3/E3 Configuration Table

     dsx3ConfigTable OBJECT-TYPE
          SYNTAX  SEQUENCE OF Dsx3ConfigEntry
          MAX-ACCESS  not-accessible
          STATUS  current
          DESCRIPTION
                 "The DS3/E3 Configuration table."
          ::= { ds3 5 }

     dsx3ConfigEntry OBJECT-TYPE
          SYNTAX  Dsx3ConfigEntry
          MAX-ACCESS  not-accessible
          STATUS  current
          DESCRIPTION
                 "An entry in the DS3/E3 Configuration table."
          INDEX   { dsx3LineIndex }
          ::= { dsx3ConfigTable 1 }

     Dsx3ConfigEntry ::=
          SEQUENCE {
              dsx3LineIndex                        InterfaceIndex,
              dsx3IfIndex                          InterfaceIndex,
              dsx3TimeElapsed                      INTEGER,
              dsx3ValidIntervals                   INTEGER,
              dsx3LineType                         INTEGER,
              dsx3LineCoding                       INTEGER,
              dsx3SendCode                         INTEGER,
              dsx3CircuitIdentifier                DisplayString,
              dsx3LoopbackConfig                   INTEGER,
              dsx3LineStatus                       INTEGER,
              dsx3TransmitClockSource              INTEGER,
              dsx3InvalidIntervals                 INTEGER,
              dsx3LineLength                       INTEGER,
              dsx3LineStatusLastChange             TimeStamp,
              dsx3LineStatusChangeTrapEnable       INTEGER,
              dsx3LoopbackStatus                   INTEGER,
              dsx3Channelization                   INTEGER,
              dsx3Ds1ForRemoteLoop                 INTEGER
     }

     dsx3LineIndex OBJECT-TYPE
          SYNTAX  InterfaceIndex
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "This object should be made equal to ifIndex.  The
                 next paragraph describes its previous usage.
                 Making the object equal to ifIndex allows propoer
                 use of ifStackTable.

                 Previously, this object was the identifier of a
                 DS3/E3 Interface on a managed device.  If there is
                 an ifEntry that is directly associated with this
                 and only this DS3/E3 interface, it should have the
                 same value as ifIndex.  Otherwise, number the
                 dsx3LineIndices with an unique identifier
                 following the rules of choosing a number that is
                 greater than ifNumber and numbering the inside
                 interfaces (e.g., equipment side) with even
                 numbers and outside interfaces (e.g, network side)
                 with odd numbers."
          ::= { dsx3ConfigEntry 1 }

     dsx3IfIndex OBJECT-TYPE
          SYNTAX  InterfaceIndex
          MAX-ACCESS  read-only
          STATUS  deprecated
          DESCRIPTION
                 "This value for this object is equal to the value
                 of ifIndex from the Interfaces table of MIB II
                 (RFC 1213)."
          ::= { dsx3ConfigEntry 2 }

     dsx3TimeElapsed OBJECT-TYPE
          SYNTAX  INTEGER (0..899)
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The number of seconds that have elapsed since the
                 beginning of the near end current error-
                 measurement period.  If, for some reason, such as
                 an adjustment in the system's time-of-day clock,
                 the current interval exceeds the maximum value,
                 the agent will return the maximum value."

          ::= { dsx3ConfigEntry 3 }

     dsx3ValidIntervals OBJECT-TYPE
          SYNTAX  INTEGER (0..96)
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The number of previous near end intervals for
                 which data was collected.  The value will be
                 96 unless the interface was brought online within
                 the last 24 hours, in which case the value will be
                 the number of complete 15 minute near end
                 intervals since the interface has been online.  In
                 the case where the agent is a proxy, it is
                 possible that some intervals are unavailable.  In
                 this case, this interval is the maximum interval
                 number for which data is available."
          ::= { dsx3ConfigEntry 4 }

     dsx3LineType OBJECT-TYPE
          SYNTAX  INTEGER {
                     dsx3other(1),
                     dsx3M23(2),
                     dsx3SYNTRAN(3),
                     dsx3CbitParity(4),
                     dsx3ClearChannel(5),
                     e3other(6),
                     e3Framed(7),
                     e3Plcp(8)
                 }
          MAX-ACCESS  read-write
          STATUS  current
          DESCRIPTION
                 "This variable indicates the variety of DS3 C-bit
                 or E3 application implementing this interface. The
                 type of interface affects the interpretation of
                 the usage and error statistics.  The rate of DS3
                 is 44.736 Mbps and E3 is 34.368 Mbps.  The
                 dsx3ClearChannel value means that the C-bits are
                 not used except for sending/receiving AIS.
                 The values, in sequence, describe:

                 TITLE:            SPECIFICATION:
                 dsx3M23            ANSI T1.107-1988 [9]
                 dsx3SYNTRAN        ANSI T1.107-1988 [9]
                 dsx3CbitParity     ANSI T1.107a-1990 [9a]
                 dsx3ClearChannel   ANSI T1.102-1987 [8]
                 e3Framed           CCITT G.751 [12]
                 e3Plcp             ETSI T/NA(91)18 [13]."
          ::= { dsx3ConfigEntry 5 }

     dsx3LineCoding OBJECT-TYPE
          SYNTAX  INTEGER {
                     dsx3Other(1),
                     dsx3B3ZS(2),
                     e3HDB3(3)
                 }
          MAX-ACCESS  read-write
          STATUS  current
          DESCRIPTION
                 "This variable describes the variety of Zero Code
                 Suppression used on this interface, which in turn
                 affects a number of its characteristics.

                 dsx3B3ZS and e3HDB3 refer to the use of specified
                 patterns of normal bits and bipolar violations
                 which are used to replace sequences of zero bits
                 of a specified length."
          ::= { dsx3ConfigEntry 6 }

     dsx3SendCode OBJECT-TYPE
          SYNTAX  INTEGER {
                    dsx3SendNoCode(1),
                    dsx3SendLineCode(2),
                    dsx3SendPayloadCode(3),
                    dsx3SendResetCode(4),
                    dsx3SendDS1LoopCode(5),
                    dsx3SendTestPattern(6)
                    }
          MAX-ACCESS  read-write
          STATUS  current
          DESCRIPTION
                 "This variable indicates what type of code is
                 being sent across the DS3/E3 interface by the
                 device.  (These are optional for E3 interfaces.)
                 Setting this variable causes the interface to
                 begin sending the code requested.
                 The values mean:

                    dsx3SendNoCode
                        sending looped or normal data

                    dsx3SendLineCode
                        sending a request for a line loopback

                    dsx3SendPayloadCode
                        sending a request for a payload loopback
                        (i.e., all DS1/E1s in a DS3/E3 frame)

                    dsx3SendResetCode
                        sending a loopback deactivation request

                    dsx3SendDS1LoopCode
                        requesting to loopback a particular DS1/E1
                        within a DS3/E3 frame.  The DS1/E1 is
                        indicated in dsx3Ds1ForRemoteLoop.

                    dsx3SendTestPattern
                        sending a test pattern."
          ::= { dsx3ConfigEntry 7 }

     dsx3CircuitIdentifier OBJECT-TYPE
          SYNTAX  DisplayString (SIZE (0..255))
          MAX-ACCESS  read-write
          STATUS  current
          DESCRIPTION
                 "This variable contains the transmission vendor's
                 circuit identifier, for the purpose of
                 facilitating troubleshooting."
          ::= { dsx3ConfigEntry 8 }

     dsx3LoopbackConfig OBJECT-TYPE
          SYNTAX  INTEGER {
                      dsx3NoLoop(1),
                      dsx3PayloadLoop(2),
                      dsx3LineLoop(3),
                      dsx3OtherLoop(4),
                      dsx3InwardLoop(5),
                      dsx3DualLoop(6)
                    }
          MAX-ACCESS  read-write
          STATUS  current
          DESCRIPTION
               "This variable represents the desired loopback
               configuration of the DS3/E3 interface.

               The values mean:

               dsx3NoLoop
                 Not in the loopback state.  A device that is
                 not capable of performing a loopback on
                 the interface shall always return this as
                 its value.

               dsx3PayloadLoop
                 The received signal at this interface is looped
                 through the device.  Typically the received signal
                 is looped back for retransmission after it has
                 passed through the device's framing function.

               dsx3LineLoop
                 The received signal at this interface does not
                 go through the device (minimum penetration) but
                 is looped back out.

               dsx3OtherLoop
                 Loopbacks that are not defined here.

               dsx3InwardLoop
                 The sent signal at this interface is looped back
                 through the device.

               dsx3DualLoop
                 Both dsx1LineLoop and dsx1InwardLoop will be
                 active simultaneously."
          ::= { dsx3ConfigEntry 9 }

     dsx3LineStatus OBJECT-TYPE
          SYNTAX  INTEGER (1..4095)
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "This variable indicates the Line Status of the
                 interface.  It contains loopback state information
                 and failure state information.  The dsx3LineStatus
                 is a bit map represented as a sum, therefore, it
                 can represent multiple failures and a loopback
                 (see dsx3LoopbackConfig object for the type of
                 loopback) simultaneously.  The dsx3NoAlarm must be
                 set if and only if no other flag is set.

                 If the dsx3loopbackState bit is set, the loopback
                 in effect can be determined from the
                 dsx3loopbackConfig object.
       The various bit positions are:
        1     dsx3NoAlarm         No alarm present
        2     dsx3RcvRAIFailure   Receiving Yellow/Remote
                                  Alarm Indication
        4     dsx3XmitRAIAlarm    Transmitting Yellow/Remote
                                  Alarm Indication
        8     dsx3RcvAIS          Receiving AIS failure state
       16     dsx3XmitAIS         Transmitting AIS
       32     dsx3LOF             Receiving LOF failure state
       64     dsx3LOS             Receiving LOS failure state
      128     dsx3LoopbackState   Looping the received signal
      256     dsx3RcvTestCode     Receiving a Test Pattern
      512     dsx3OtherFailure    any line status not defined
                                  here
     1024     dsx3UnavailSigState Near End in Unavailable Signal
                                  State
     2048     dsx3NetEquipOOS     Carrier Equipment Out of Service"
     ::= { dsx3ConfigEntry 10 }

dsx3TransmitClockSource OBJECT-TYPE
     SYNTAX  INTEGER {
                loopTiming(1),
                localTiming(2),
                throughTiming(3)
            }
     MAX-ACCESS  read-write
     STATUS  current
     DESCRIPTION
            "The source of Transmit Clock.

            loopTiming indicates that the recovered receive clock
            is used as the transmit clock.

            localTiming indicates that a local clock source is used
            or that an external clock is attached to the box
            containing the interface.

            throughTiming indicates that transmit clock is derived
            from the recovered receive clock of another DS3
            interface."
          ::= { dsx3ConfigEntry 11 }

     dsx3InvalidIntervals OBJECT-TYPE
          SYNTAX  INTEGER (0..96)
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                      "The number of intervals in the range from 0 to
                 dsx3ValidIntervals for which no data is
                 available.  This object will typically be zero
                 except in cases where the data for some intervals
                 are not available (e.g., in proxy situations)."
          ::= { dsx3ConfigEntry 12 }

     dsx3LineLength OBJECT-TYPE
          SYNTAX  INTEGER (0..64000)
          UNITS "meters"
          MAX-ACCESS  read-write
          STATUS  current
          DESCRIPTION
                 "The length of the ds3 line in meters.  This
                 object provides information for line build out
                 circuitry if it exists and can use this object to
                 adjust the line build out."
          ::= { dsx3ConfigEntry 13 }

     dsx3LineStatusLastChange OBJECT-TYPE
          SYNTAX  TimeStamp
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The value of MIB II's sysUpTime object at the
                 time this DS3/E3 entered its current line status
                 state.  If the current state was entered prior to
                 the last re-initialization of the proxy-agent,
                 then this object contains a zero value."
          ::= { dsx3ConfigEntry 14 }

     dsx3LineStatusChangeTrapEnable  OBJECT-TYPE
          SYNTAX      INTEGER {
                         enabled(1),
                         disabled(2)
                      }
          MAX-ACCESS  read-write
          STATUS      current
          DESCRIPTION
                 "Indicates whether dsx3LineStatusChange traps
                 should be generated for this interface."
          DEFVAL { disabled }
          ::= { dsx3ConfigEntry 15 }

     dsx3LoopbackStatus  OBJECT-TYPE
          SYNTAX      INTEGER (1..127)
          MAX-ACCESS  read-only
          STATUS      current
          DESCRIPTION
                 "This variable represents the current state of the
                 loopback on the DS3 interface.  It contains
                 information about loopbacks established by a
                 manager and remotely from the far end.

                 The dsx3LoopbackStatus is a bit map represented as
                 a sum, therefore is can represent multiple
                 loopbacks simultaneously.

                 The various bit positions are:
                  1  dsx3NoLoopback
                  2  dsx3NearEndPayloadLoopback
                  4  dsx3NearEndLineLoopback
                  8  dsx3NearEndOtherLoopback
                 16  dsx3NearEndInwardLoopback
                 32  dsx3FarEndPayloadLoopback
                 64  dsx3FarEndLineLoopback"

     ::= { dsx3ConfigEntry 16 }

     dsx3Channelization  OBJECT-TYPE
          SYNTAX      INTEGER {
                         disabled(1),
                         enabledDs1(2),
                         enabledDs2(3)
                      }
          MAX-ACCESS  read-write
          STATUS      current
          DESCRIPTION
                 "Indicates whether this ds3/e3 is channelized or
                 unchannelized.  The value of enabledDs1 indicates
                 that this is a DS3 channelized into DS1s.  The
                 value of enabledDs3 indicated that this is a DS3
                 channelized into DS2s.  Setting this object will
                 cause the creation or deletion of DS2 or DS1
                 entries in the ifTable.  "
     ::= { dsx3ConfigEntry 17 }

     dsx3Ds1ForRemoteLoop  OBJECT-TYPE
          SYNTAX      INTEGER (0..29)

          MAX-ACCESS  read-write
          STATUS      current
          DESCRIPTION
                 "Indicates which ds1/e1 on this ds3/e3 will be
                 indicated in the remote ds1 loopback request.  A
                 value of 0 means no DS1 will be looped.  A value
                 of 29 means all ds1s/e1s will be looped."
     ::= { dsx3ConfigEntry 18 }

     -- the DS3/E3 Current Table

     dsx3CurrentTable OBJECT-TYPE
          SYNTAX  SEQUENCE OF Dsx3CurrentEntry
          MAX-ACCESS  not-accessible
          STATUS  current
          DESCRIPTION
                 "The DS3/E3 current table contains various
                 statistics being collected for the current 15
                 minute interval."
          ::= { ds3 6 }

     dsx3CurrentEntry OBJECT-TYPE
          SYNTAX  Dsx3CurrentEntry
          MAX-ACCESS  not-accessible
          STATUS  current
          DESCRIPTION
                 "An entry in the DS3/E3 Current table."
          INDEX   { dsx3CurrentIndex }
          ::= { dsx3CurrentTable 1 }

     Dsx3CurrentEntry ::=
          SEQUENCE {
              dsx3CurrentIndex           InterfaceIndex,
              dsx3CurrentPESs            PerfCurrentCount,
              dsx3CurrentPSESs           PerfCurrentCount,
              dsx3CurrentSEFSs           PerfCurrentCount,
              dsx3CurrentUASs            PerfCurrentCount,
              dsx3CurrentLCVs            PerfCurrentCount,
              dsx3CurrentPCVs            PerfCurrentCount,
              dsx3CurrentLESs            PerfCurrentCount,
              dsx3CurrentCCVs            PerfCurrentCount,
              dsx3CurrentCESs            PerfCurrentCount,
              dsx3CurrentCSESs           PerfCurrentCount
         }

     dsx3CurrentIndex OBJECT-TYPE
          SYNTAX  InterfaceIndex
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The index value which uniquely identifies the
                 DS3/E3 interface to which this entry is
                 applicable.  The interface identified by a
                 particular value of this index is the same
                 interface as identified by the same value an
                 dsx3LineIndex object instance."
          ::= { dsx3CurrentEntry 1 }

     dsx3CurrentPESs OBJECT-TYPE
          SYNTAX  PerfCurrentCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The counter associated with the number of P-bit
                 Errored Seconds."
          ::= { dsx3CurrentEntry 2 }

     dsx3CurrentPSESs OBJECT-TYPE
          SYNTAX  PerfCurrentCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The counter associated with the number of P-bit
                 Severely Errored Seconds."
          ::= { dsx3CurrentEntry 3 }

     dsx3CurrentSEFSs OBJECT-TYPE
          SYNTAX  PerfCurrentCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The counter associated with the number of
                 Severely Errored Framing Seconds."
          ::= { dsx3CurrentEntry 4 }

     dsx3CurrentUASs OBJECT-TYPE
          SYNTAX  PerfCurrentCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The counter associated with the number of
                 Unavailable Seconds."
          ::= { dsx3CurrentEntry 5 }

     dsx3CurrentLCVs OBJECT-TYPE
          SYNTAX  PerfCurrentCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The counter associated with the number of Line
                 Coding Violations."
          ::= { dsx3CurrentEntry 6 }

     dsx3CurrentPCVs OBJECT-TYPE
          SYNTAX  PerfCurrentCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The counter associated with the number of P-bit
                 Coding Violations."
          ::= { dsx3CurrentEntry 7 }

     dsx3CurrentLESs OBJECT-TYPE
          SYNTAX  PerfCurrentCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The number of Line Errored Seconds."
          ::= { dsx3CurrentEntry 8 }

     dsx3CurrentCCVs OBJECT-TYPE
          SYNTAX  PerfCurrentCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The number of C-bit Coding Violations."
          ::= { dsx3CurrentEntry 9 }

     dsx3CurrentCESs OBJECT-TYPE
          SYNTAX  PerfCurrentCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The number of C-bit Errored Seconds."
          ::= { dsx3CurrentEntry 10 }

     dsx3CurrentCSESs OBJECT-TYPE
          SYNTAX  PerfCurrentCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The number of C-bit Severely Errored Seconds."
          ::= { dsx3CurrentEntry 11 }

     -- the DS3/E3 Interval Table

     dsx3IntervalTable OBJECT-TYPE
          SYNTAX  SEQUENCE OF Dsx3IntervalEntry
          MAX-ACCESS  not-accessible
          STATUS  current
          DESCRIPTION
                 "The DS3/E3 Interval Table contains various
                 statistics collected by each DS3/E3 Interface over
                 the previous 24 hours of operation.  The past 24
                 hours are broken into 96 completed 15 minute
                 intervals.  Each row in this table represents one
                 such interval (identified by dsx3IntervalNumber)
                 and for one specific interface (identifed by
                 dsx3IntervalIndex)."

          ::= { ds3 7 }

     dsx3IntervalEntry OBJECT-TYPE
          SYNTAX  Dsx3IntervalEntry
          MAX-ACCESS  not-accessible
          STATUS  current
          DESCRIPTION
                 "An entry in the DS3/E3 Interval table."
          INDEX   { dsx3IntervalIndex, dsx3IntervalNumber }
          ::= { dsx3IntervalTable 1 }

     Dsx3IntervalEntry ::=
          SEQUENCE {
              dsx3IntervalIndex           InterfaceIndex,
              dsx3IntervalNumber          INTEGER,
              dsx3IntervalPESs            PerfIntervalCount,
              dsx3IntervalPSESs           PerfIntervalCount,
              dsx3IntervalSEFSs           PerfIntervalCount,
              dsx3IntervalUASs            PerfIntervalCount,
              dsx3IntervalLCVs            PerfIntervalCount,
              dsx3IntervalPCVs            PerfIntervalCount,
              dsx3IntervalLESs            PerfIntervalCount,
              dsx3IntervalCCVs            PerfIntervalCount,
              dsx3IntervalCESs            PerfIntervalCount,
              dsx3IntervalCSESs           PerfIntervalCount,
              dsx3IntervalValidData       TruthValue
          }

     dsx3IntervalIndex OBJECT-TYPE
          SYNTAX  InterfaceIndex
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The index value which uniquely identifies the
                 DS3/E3 interface to which this entry is
                 applicable.  The interface identified by a
                 particular value of this index is the same
                 interface as identified by the same value an
                 dsx3LineIndex object instance."
          ::= { dsx3IntervalEntry 1 }

     dsx3IntervalNumber OBJECT-TYPE
          SYNTAX  INTEGER (1..96)
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "A number between 1 and 96, where 1 is the most
                 recently completed 15 minute interval and 96 is
                 the 15 minutes interval completed 23 hours and 45
                 minutes prior to interval 1."
          ::= { dsx3IntervalEntry 2 }

     dsx3IntervalPESs OBJECT-TYPE
          SYNTAX  PerfIntervalCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The counter associated with the number of P-bit
                 Errored Seconds."
          ::= { dsx3IntervalEntry 3 }

     dsx3IntervalPSESs OBJECT-TYPE
          SYNTAX  PerfIntervalCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The counter associated with the number of P-bit
                 Severely Errored Seconds."
          ::= { dsx3IntervalEntry 4 }

     dsx3IntervalSEFSs OBJECT-TYPE
          SYNTAX  PerfIntervalCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The counter associated with the number of
                 Severely Errored Framing Seconds."
          ::= { dsx3IntervalEntry 5 }

     dsx3IntervalUASs OBJECT-TYPE
          SYNTAX  PerfIntervalCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The counter associated with the number of
                 Unavailable Seconds.  This object may decrease if
                 the occurance of unavailable seconds occurs across
                 an inteval boundary."
          ::= { dsx3IntervalEntry 6 }

     dsx3IntervalLCVs OBJECT-TYPE
          SYNTAX  PerfIntervalCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The counter associated with the number of Line
                 Coding Violations."
          ::= { dsx3IntervalEntry 7 }

     dsx3IntervalPCVs OBJECT-TYPE
          SYNTAX  PerfIntervalCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The counter associated with the number of P-bit
                 Coding Violations."
          ::= { dsx3IntervalEntry 8 }

     dsx3IntervalLESs OBJECT-TYPE
          SYNTAX  PerfIntervalCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The number of Line Errored  Seconds  (BPVs  or
                 illegal  zero  sequences)."
          ::= { dsx3IntervalEntry 9 }

     dsx3IntervalCCVs OBJECT-TYPE
          SYNTAX  PerfIntervalCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The number of C-bit Coding Violations."
          ::= { dsx3IntervalEntry 10 }

     dsx3IntervalCESs OBJECT-TYPE
          SYNTAX  PerfIntervalCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The number of C-bit Errored Seconds."
          ::= { dsx3IntervalEntry 11 }

     dsx3IntervalCSESs OBJECT-TYPE
          SYNTAX  PerfIntervalCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The number of C-bit Severely Errored Seconds."
          ::= { dsx3IntervalEntry 12 }

     dsx3IntervalValidData OBJECT-TYPE
          SYNTAX  TruthValue
          MAX-ACCESS read-only
          STATUS current
          DESCRIPTION
                 "This variable indicates if the data for this
                 interval is valid."
          ::= { dsx3IntervalEntry 13 }

     -- the DS3/E3 Total

     dsx3TotalTable OBJECT-TYPE
          SYNTAX  SEQUENCE OF Dsx3TotalEntry
          MAX-ACCESS  not-accessible
          STATUS  current
          DESCRIPTION
                 "The DS3/E3 Total Table contains the cumulative
                 sum of the various statistics for the 24 hour
                 period preceding the current interval."
          ::= { ds3 8 }

     dsx3TotalEntry OBJECT-TYPE
          SYNTAX  Dsx3TotalEntry
          MAX-ACCESS  not-accessible
          STATUS  current
          DESCRIPTION
                 "An entry in the DS3/E3 Total table."
         INDEX   { dsx3TotalIndex }
          ::= { dsx3TotalTable 1 }

     Dsx3TotalEntry ::=
          SEQUENCE {
              dsx3TotalIndex      InterfaceIndex,
              dsx3TotalPESs       PerfTotalCount,
              dsx3TotalPSESs      PerfTotalCount,
              dsx3TotalSEFSs      PerfTotalCount,
              dsx3TotalUASs       PerfTotalCount,
              dsx3TotalLCVs       PerfTotalCount,
              dsx3TotalPCVs       PerfTotalCount,
              dsx3TotalLESs       PerfTotalCount,
              dsx3TotalCCVs       PerfTotalCount,
              dsx3TotalCESs       PerfTotalCount,
              dsx3TotalCSESs      PerfTotalCount
          }

     dsx3TotalIndex OBJECT-TYPE
          SYNTAX  InterfaceIndex
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The index value which uniquely identifies the
                 DS3/E3 interface to which this entry is
                 applicable.  The interface identified by a
                 particular value of this index is the same
                 interface as identified by the same value an
                 dsx3LineIndex object instance."
          ::= { dsx3TotalEntry 1 }

     dsx3TotalPESs OBJECT-TYPE
          SYNTAX  PerfTotalCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The counter associated with the number of P-bit
                 Errored Seconds, encountered by a DS3 interface in
                 the previous 24 hour interval. Invalid 15 minute
                 intervals count as 0."
          ::= { dsx3TotalEntry 2 }

     dsx3TotalPSESs OBJECT-TYPE
          SYNTAX  PerfTotalCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The counter associated with the number of P-bit
                 Severely Errored Seconds, encountered by a DS3
                 interface in the previous 24 hour interval.
                 Invalid 15 minute intervals count as 0."
          ::= { dsx3TotalEntry 3 }

     dsx3TotalSEFSs OBJECT-TYPE
          SYNTAX  PerfTotalCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The counter associated with the number of
                 Severely Errored Framing Seconds, encountered by a
                 DS3/E3 interface in the previous 24 hour interval.
                 Invalid 15 minute intervals count as 0."
          ::= { dsx3TotalEntry 4 }

     dsx3TotalUASs OBJECT-TYPE
          SYNTAX  PerfTotalCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The counter associated with the number of
                 Unavailable Seconds, encountered by a DS3
                 interface in the previous 24 hour interval.

                 Invalid 15 minute intervals count as 0."
          ::= { dsx3TotalEntry 5 }

     dsx3TotalLCVs OBJECT-TYPE
          SYNTAX  PerfTotalCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The counter associated with the number of Line
                 Coding Violations encountered by a DS3/E3
                 interface in the previous 24 hour interval.
                 Invalid 15 minute intervals count as 0."
          ::= { dsx3TotalEntry 6 }

     dsx3TotalPCVs OBJECT-TYPE
          SYNTAX  PerfTotalCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The counter associated with the number of P-bit
                 Coding Violations, encountered by a DS3 interface
                 in the previous 24 hour interval. Invalid 15
                 minute intervals count as 0."
          ::= { dsx3TotalEntry 7 }

     dsx3TotalLESs OBJECT-TYPE
          SYNTAX  PerfTotalCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The number of Line Errored  Seconds  (BPVs  or
                 illegal  zero  sequences) encountered by a DS3/E3
                 interface in the previous 24 hour interval.
                 Invalid 15 minute intervals count as 0."
          ::= { dsx3TotalEntry 8 }

     dsx3TotalCCVs OBJECT-TYPE
          SYNTAX  PerfTotalCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The number of C-bit Coding Violations encountered
                 by a DS3 interface in the previous 24 hour
                 interval. Invalid 15 minute intervals count as 0."
          ::= { dsx3TotalEntry 9 }

     dsx3TotalCESs OBJECT-TYPE
          SYNTAX  PerfTotalCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The number of C-bit Errored Seconds encountered
                 by a DS3 interface in the previous 24 hour
                 interval. Invalid 15 minute intervals count as 0."
          ::= { dsx3TotalEntry 10 }

     dsx3TotalCSESs OBJECT-TYPE
          SYNTAX  PerfTotalCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The number of C-bit Severely Errored Seconds
                 encountered by a DS3 interface in the previous 24
                 hour interval. Invalid 15 minute intervals count
                 as 0."
          ::= { dsx3TotalEntry 11 }

     -- The DS3 Far End Group

     -- The DS3 Far End Group consists of four tables :
     --   DS3 Far End Configuration
     --   DS3 Far End Current
     --   DS3 Far End Interval
     --   DS3 Far End Total

     -- The DS3 Far End Configuration Table

     dsx3FarEndConfigTable OBJECT-TYPE
          SYNTAX  SEQUENCE OF Dsx3FarEndConfigEntry
          MAX-ACCESS  not-accessible
          STATUS  current
          DESCRIPTION
                 "The DS3 Far End Configuration Table contains
                 configuration information reported in the C-bits
                 from the remote end."
          ::= { ds3 9 }

     dsx3FarEndConfigEntry OBJECT-TYPE
          SYNTAX  Dsx3FarEndConfigEntry
          MAX-ACCESS  not-accessible
          STATUS  current
          DESCRIPTION
                 "An entry in the DS3 Far End Configuration table."
         INDEX   { dsx3FarEndLineIndex }
          ::= { dsx3FarEndConfigTable 1 }

     Dsx3FarEndConfigEntry ::=
          SEQUENCE {
              dsx3FarEndLineIndex          InterfaceIndex,
             dsx3FarEndEquipCode           DisplayString,
             dsx3FarEndLocationIDCode      DisplayString,
             dsx3FarEndFrameIDCode         DisplayString,
             dsx3FarEndUnitCode            DisplayString,
             dsx3FarEndFacilityIDCode      DisplayString
          }

     dsx3FarEndLineIndex OBJECT-TYPE
          SYNTAX  InterfaceIndex
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The index value which uniquely identifies the DS3
                 interface to which this entry is applicable.  The
                 interface identified by a particular value of this
                 index is the same interface as identified by the
                 same value an dsx3LineIndex object instance."
         ::= { dsx3FarEndConfigEntry 1 }

     dsx3FarEndEquipCode OBJECT-TYPE
          SYNTAX  DisplayString (SIZE (0..10))
          MAX-ACCESS  read-write
          STATUS  current
          DESCRIPTION
                 "This is the Far End Equipment Identification code
                 that describes the specific piece of equipment.
                 It is sent within the Path Identification
                 Message."
          ::= { dsx3FarEndConfigEntry 2 }

     dsx3FarEndLocationIDCode OBJECT-TYPE
          SYNTAX  DisplayString (SIZE (0..11))
          MAX-ACCESS  read-write
          STATUS  current
          DESCRIPTION
                 "This is the Far End Location Identification code
                 that describes the specific location of the
                 equipment.  It is sent within the Path
                 Identification Message."
          ::= { dsx3FarEndConfigEntry 3 }

     dsx3FarEndFrameIDCode OBJECT-TYPE
          SYNTAX  DisplayString (SIZE (0..10))
          MAX-ACCESS  read-write
          STATUS  current
          DESCRIPTION
                 "This is the Far End Frame Identification code
                 that identifies where the equipment is located
                 within a building at a given location.  It is sent
                 within the Path Identification Message."
          ::= { dsx3FarEndConfigEntry 4 }

     dsx3FarEndUnitCode OBJECT-TYPE
          SYNTAX  DisplayString (SIZE (0..6))
          MAX-ACCESS  read-write
          STATUS  current
          DESCRIPTION
                 "This is the Far End code that identifies the
                 equipment location within a bay.  It is sent
                 within the Path Identification Message."
          ::= { dsx3FarEndConfigEntry 5 }

     dsx3FarEndFacilityIDCode OBJECT-TYPE
          SYNTAX  DisplayString (SIZE (0..38))
          MAX-ACCESS  read-write
          STATUS  current
          DESCRIPTION
                 "This code identifies a specific Far End DS3 path.
                 It is sent within the Path Identification
                 Message."
          ::= { dsx3FarEndConfigEntry 6 }

     -- The DS3 Far End Current

     dsx3FarEndCurrentTable OBJECT-TYPE
          SYNTAX  SEQUENCE OF Dsx3FarEndCurrentEntry
          MAX-ACCESS  not-accessible
          STATUS  current
          DESCRIPTION
                 "The DS3 Far End Current table contains various
                 statistics being collected for the current 15
                 minute interval.  The statistics are collected
                 from the far end block error code within the C-
                 bits."
          ::= { ds3 10 }

     dsx3FarEndCurrentEntry OBJECT-TYPE
          SYNTAX  Dsx3FarEndCurrentEntry
          MAX-ACCESS  not-accessible
          STATUS  current
          DESCRIPTION
                 "An entry in the DS3 Far End Current table."
          INDEX   { dsx3FarEndCurrentIndex }
          ::= { dsx3FarEndCurrentTable 1 }

     Dsx3FarEndCurrentEntry ::=
          SEQUENCE {
              dsx3FarEndCurrentIndex        InterfaceIndex,
              dsx3FarEndTimeElapsed         INTEGER,
              dsx3FarEndValidIntervals      INTEGER,
              dsx3FarEndCurrentCESs         PerfCurrentCount,
              dsx3FarEndCurrentCSESs        PerfCurrentCount,
              dsx3FarEndCurrentCCVs         PerfCurrentCount,
              dsx3FarEndCurrentUASs         PerfCurrentCount,
              dsx3FarEndInvalidIntervals    INTEGER
         }

      dsx3FarEndCurrentIndex OBJECT-TYPE
          SYNTAX  InterfaceIndex
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The index value which uniquely identifies the DS3
                 interface to which this entry is applicable.  The
                 interface identified by a particular value of this
                 index is identical to the interface identified by
                 the same value of dsx3LineIndex."
          ::= { dsx3FarEndCurrentEntry 1 }

     dsx3FarEndTimeElapsed OBJECT-TYPE
          SYNTAX  INTEGER (0..899)
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The number of seconds that have elapsed since the
                 beginning of the far end current error-measurement
                 period.  If, for some reason, such as an
                 adjustment in the system's time-of-day clock, the
                 current interval exceeds the maximum value, the
                 agent will return the maximum value."
          ::= { dsx3FarEndCurrentEntry 2 }

     dsx3FarEndValidIntervals OBJECT-TYPE
          SYNTAX  INTEGER (0..96)
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The number of previous far end intervals for
                 which data was collected.  The value will be
                 96 unless the interface was brought online within
                 the last 24 hours, in which case the value will be
                 the number of complete 15 minute far end intervals
                 since the interface has been online."
          ::= { dsx3FarEndCurrentEntry 3 }

     dsx3FarEndCurrentCESs OBJECT-TYPE
          SYNTAX  PerfCurrentCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The counter associated with the number of Far Far
                 End C-bit Errored Seconds."
          ::= { dsx3FarEndCurrentEntry 4 }

     dsx3FarEndCurrentCSESs OBJECT-TYPE
          SYNTAX  PerfCurrentCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The counter associated with the number of Far End
                 C-bit Severely Errored Seconds."
          ::= { dsx3FarEndCurrentEntry 5 }

     dsx3FarEndCurrentCCVs OBJECT-TYPE
          SYNTAX  PerfCurrentCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The counter associated with the number of Far End
                 C-bit Coding Violations reported via the far end
                 block error count."
          ::= { dsx3FarEndCurrentEntry 6 }

     dsx3FarEndCurrentUASs OBJECT-TYPE
          SYNTAX  PerfCurrentCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The counter associated with the number of Far End
                 unavailable seconds."
          ::= { dsx3FarEndCurrentEntry 7 }

     dsx3FarEndInvalidIntervals OBJECT-TYPE
          SYNTAX  INTEGER (0..96)
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The number of intervals in the range from 0 to
                 dsx3FarEndValidIntervals for which no data is
                 available.  This object will typically be zero
                 except in cases where the data for some intervals
                 are not available (e.g., in proxy situations)."
          ::= { dsx3FarEndCurrentEntry 8 }

     -- The DS3 Far End Interval Table

     dsx3FarEndIntervalTable OBJECT-TYPE
          SYNTAX  SEQUENCE OF Dsx3FarEndIntervalEntry
          MAX-ACCESS  not-accessible
          STATUS  current
          DESCRIPTION
                 "The DS3 Far End Interval Table contains various
                 statistics collected by each DS3 interface over
                 the previous 24 hours of operation.  The past 24
                 hours are broken into 96 completed 15 minute
                 intervals."
          ::= { ds3 11 }

     dsx3FarEndIntervalEntry OBJECT-TYPE
          SYNTAX  Dsx3FarEndIntervalEntry
          MAX-ACCESS  not-accessible
          STATUS  current
          DESCRIPTION
                 "An entry in the DS3 Far End Interval table."
          INDEX   { dsx3FarEndIntervalIndex,
                    dsx3FarEndIntervalNumber }
          ::= { dsx3FarEndIntervalTable 1 }

     Dsx3FarEndIntervalEntry ::=
          SEQUENCE {
               dsx3FarEndIntervalIndex      InterfaceIndex,
               dsx3FarEndIntervalNumber     INTEGER,
               dsx3FarEndIntervalCESs       PerfIntervalCount,
               dsx3FarEndIntervalCSESs      PerfIntervalCount,
               dsx3FarEndIntervalCCVs       PerfIntervalCount,
               dsx3FarEndIntervalUASs       PerfIntervalCount,
               dsx3FarEndIntervalValidData  TruthValue
         }

     dsx3FarEndIntervalIndex OBJECT-TYPE
          SYNTAX  InterfaceIndex
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The index value which uniquely identifies the DS3
                 interface to which this entry is applicable.  The
                 interface identified by a particular value of this
                 index is identical to the interface identified by
                 the same value of dsx3LineIndex."
          ::= { dsx3FarEndIntervalEntry 1 }

     dsx3FarEndIntervalNumber OBJECT-TYPE
         SYNTAX  INTEGER (1..96)
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION
                 "A number between 1 and 96, where 1 is the most
                 recently completed 15 minute interval and 96 is
                 the 15 minutes interval completed 23 hours and 45
                 minutes prior to interval 1."
         ::= { dsx3FarEndIntervalEntry 2 }

     dsx3FarEndIntervalCESs OBJECT-TYPE
         SYNTAX  PerfIntervalCount
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION
                 "The counter associated with the number of Far End
                 C-bit Errored Seconds encountered by a DS3
                 interface in one of the previous 96, individual 15
                 minute, intervals. In the case where the agent is
                 a proxy and data is not available, return
                 noSuchInstance."
        ::= { dsx3FarEndIntervalEntry 3 }

     dsx3FarEndIntervalCSESs OBJECT-TYPE
         SYNTAX  PerfIntervalCount
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION
                 "The counter associated with the number of Far End
                 C-bit Severely Errored Seconds."
        ::= { dsx3FarEndIntervalEntry 4 }

     dsx3FarEndIntervalCCVs OBJECT-TYPE
          SYNTAX  PerfIntervalCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The counter associated with the number of Far End
                 C-bit Coding Violations reported via the far end
                 block error count."
          ::= { dsx3FarEndIntervalEntry 5 }

     dsx3FarEndIntervalUASs OBJECT-TYPE
          SYNTAX  PerfIntervalCount
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The counter associated with the number of Far End
                 unavailable seconds."
          ::= { dsx3FarEndIntervalEntry 6 }

     dsx3FarEndIntervalValidData OBJECT-TYPE
          SYNTAX  TruthValue
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "This variable indicates if the data for this
                 interval is valid."
          ::= { dsx3FarEndIntervalEntry 7 }

     -- The DS3 Far End Total

     dsx3FarEndTotalTable OBJECT-TYPE
          SYNTAX  SEQUENCE OF Dsx3FarEndTotalEntry
          MAX-ACCESS  not-accessible
          STATUS  current
          DESCRIPTION
                 "The DS3 Far End Total Table contains the
                 cumulative sum of the various statistics for the
                 24 hour period preceding the current interval."
          ::= { ds3 12 }

     dsx3FarEndTotalEntry OBJECT-TYPE
          SYNTAX  Dsx3FarEndTotalEntry
          MAX-ACCESS  not-accessible
          STATUS  current
          DESCRIPTION
                 "An entry in the DS3 Far End Total table."
          INDEX   { dsx3FarEndTotalIndex }
          ::= { dsx3FarEndTotalTable 1 }

     Dsx3FarEndTotalEntry ::=
          SEQUENCE {
              dsx3FarEndTotalIndex       InterfaceIndex,
              dsx3FarEndTotalCESs        PerfTotalCount,
              dsx3FarEndTotalCSESs       PerfTotalCount,
              dsx3FarEndTotalCCVs        PerfTotalCount,
              dsx3FarEndTotalUASs        PerfTotalCount
          }

     dsx3FarEndTotalIndex OBJECT-TYPE
          SYNTAX  InterfaceIndex
          MAX-ACCESS  read-only
          STATUS  current
          DESCRIPTION
                 "The index value which uniquely identifies the DS3
                 interface to which this entry is applicable.  The
                 interface identified by a particular value of this
                 index is identical to the interface identified by
                 the same value of dsx3LineIndex."
          ::= { dsx3FarEndTotalEntry 1 }

     dsx3FarEndTotalCESs OBJECT-TYPE
         SYNTAX  PerfTotalCount
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION
                 "The counter associated with the number of Far End
                 C-bit Errored Seconds encountered by a DS3
                 interface in the previous 24 hour interval.
                 Invalid 15 minute intervals count as 0."
         ::= { dsx3FarEndTotalEntry 2 }

     dsx3FarEndTotalCSESs OBJECT-TYPE
         SYNTAX  PerfTotalCount
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION
                 "The counter associated with the number of Far End
                 C-bit Severely Errored Seconds encountered by a
                 DS3 interface in the previous 24 hour interval.
                 Invalid 15 minute intervals count as 0."
         ::= { dsx3FarEndTotalEntry 3 }

     dsx3FarEndTotalCCVs OBJECT-TYPE
         SYNTAX  PerfTotalCount
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION
                 "The counter associated with the number of Far End
                 C-bit Coding Violations reported via the far end
                 block error count encountered by a DS3 interface
                 in the previous 24 hour interval. Invalid 15
                 minute intervals count as 0."
         ::= { dsx3FarEndTotalEntry 4 }

     dsx3FarEndTotalUASs OBJECT-TYPE
         SYNTAX  PerfTotalCount
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION
                 "The counter associated with the number of Far End
                 unavailable seconds encountered by a DS3 interface
                 in the previous 24 hour interval.  Invalid 15
                 minute intervals count as 0."
         ::= { dsx3FarEndTotalEntry 5 }

     -- the DS3/E3 Fractional Table

     -- This table is deprecated.

     dsx3FracTable OBJECT-TYPE
         SYNTAX  SEQUENCE OF Dsx3FracEntry
         MAX-ACCESS  not-accessible
         STATUS  deprecated
         DESCRIPTION
                 "This table is deprecated in favour of using
                 ifStackTable.

                 Implementation of this table was optional.  It was
                 designed for those systems dividing a DS3/E3 into
                 channels containing different data streams that
                 are of local interest.

                 The DS3/E3 fractional table identifies which
                 DS3/E3 channels associated with a CSU are being
                 used to support a logical interface, i.e., an
                 entry in the interfaces table from the Internet-
                 standard MIB.

                 For example, consider a DS3 device with 4 high
                 speed links carrying router traffic, a feed for
                 voice, a feed for video, and a synchronous channel
                 for a non-routed protocol.  We might describe the
                 allocation of channels, in the dsx3FracTable, as
                 follows:
                 dsx3FracIfIndex.2. 1 = 3  dsx3FracIfIndex.2.15 = 4
                 dsx3FracIfIndex.2. 2 = 3  dsx3FracIfIndex.2.16 = 6
                 dsx3FracIfIndex.2. 3 = 3  dsx3FracIfIndex.2.17 = 6
                 dsx3FracIfIndex.2. 4 = 3  dsx3FracIfIndex.2.18 = 6
                 dsx3FracIfIndex.2. 5 = 3  dsx3FracIfIndex.2.19 = 6
                 dsx3FracIfIndex.2. 6 = 3  dsx3FracIfIndex.2.20 = 6
                 dsx3FracIfIndex.2. 7 = 4  dsx3FracIfIndex.2.21 = 6
                 dsx3FracIfIndex.2. 8 = 4  dsx3FracIfIndex.2.22 = 6
                 dsx3FracIfIndex.2. 9 = 4  dsx3FracIfIndex.2.23 = 6
                 dsx3FracIfIndex.2.10 = 4  dsx3FracIfIndex.2.24 = 6
                 dsx3FracIfIndex.2.11 = 4  dsx3FracIfIndex.2.25 = 6
                 dsx3FracIfIndex.2.12 = 5  dsx3FracIfIndex.2.26 = 6
                 dsx3FracIfIndex.2.13 = 5  dsx3FracIfIndex.2.27 = 6
                 dsx3FracIfIndex.2.14 = 5  dsx3FracIfIndex.2.28 = 6
                 For dsx3M23, dsx3 SYNTRAN, dsx3CbitParity, and
                 dsx3ClearChannel  there are 28 legal channels,
                 numbered 1 throug h 28.

                 For e3Framed there are 16 legal channels, numbered
                 1 through 16.  The channels (1..16) correspond
                 directly to the equivalently numbered time-slots."
          ::= { ds3 13 }

     dsx3FracEntry OBJECT-TYPE
          SYNTAX  Dsx3FracEntry
          MAX-ACCESS  not-accessible
          STATUS  deprecated
          DESCRIPTION
                         "An entry in the DS3 Fractional table."
         INDEX   { dsx3FracIndex, dsx3FracNumber }
         ::= { dsx3FracTable 1 }

     Dsx3FracEntry ::=
          SEQUENCE {
              dsx3FracIndex     INTEGER,
              dsx3FracNumber    INTEGER,
              dsx3FracIfIndex   INTEGER
         }

     dsx3FracIndex OBJECT-TYPE
         SYNTAX  INTEGER (1..'7fffffff'h)
         MAX-ACCESS  read-only
         STATUS  deprecated
         DESCRIPTION
                 "The index value which uniquely identifies  the
                 DS3  interface  to which this entry is applicable
                 The interface identified by a  particular value
                 of  this  index is the same interface as
                 identified by the same value  an  dsx3LineIndex
                 object instance."
        ::= { dsx3FracEntry 1 }

     dsx3FracNumber OBJECT-TYPE
         SYNTAX  INTEGER (1..31)
         MAX-ACCESS  read-only
         STATUS  deprecated
         DESCRIPTION
                 "The channel number for this entry."
        ::= { dsx3FracEntry 2 }

     dsx3FracIfIndex OBJECT-TYPE
         SYNTAX  INTEGER (1..'7fffffff'h)
         MAX-ACCESS  read-write
         STATUS  deprecated
         DESCRIPTION
                 "An index value that uniquely identifies an
                 interface.  The interface identified by a
                 particular value of this index is the same
                 interface as  identified by the same value an
                 ifIndex object instance. If no interface is
                 currently using a channel, the value should be
                 zero.  If a single interface occupies more  than
                 one  time slot,  that ifIndex value will be found
                 in multiple time slots."
        ::= { dsx3FracEntry 3 }

      -- Ds3 TRAPS

     ds3Traps OBJECT IDENTIFIER ::= { ds3 15 }

     dsx3LineStatusChange NOTIFICATION-TYPE
         OBJECTS { dsx3LineStatus,
                   dsx3LineStatusLastChange }
         STATUS  current
         DESCRIPTION
                 "A dsx3LineStatusChange trap is sent when the
                 value of an instance of dsx3LineStatus changes. It
                 can be utilized by an NMS to trigger polls.  When
                 the line status change results in a lower level
                 line status change (i.e. ds1), then no traps for
                 the lower level are sent."
                    ::= { ds3Traps 0 1 }

                 -- conformance information

                 ds3Conformance OBJECT IDENTIFIER ::= { ds3 14 }

                 ds3Groups      OBJECT IDENTIFIER ::= {
                 ds3Conformance 1 } ds3Compliances OBJECT
                 IDENTIFIER ::= { ds3Conformance 2 }

                 -- compliance statements

                 ds3Compliance MODULE-COMPLIANCE
                     STATUS  current
                     DESCRIPTION
                             "The compliance statement for DS3/E3
                             interfaces."
         MODULE  -- this module
             MANDATORY-GROUPS { ds3NearEndConfigGroup,
                                ds3NearEndStatisticsGroup }

             GROUP       ds3FarEndGroup
             DESCRIPTION
                 "Implementation of this group is optional for all
                 systems that attach to a DS3 Interface.  However,
                 only C-bit Parity and SYNTRAN DS3 applications
                 have the capability (option) of providing this
                 information."
             GROUP       ds3NearEndOptionalConfigGroup
             DESCRIPTION
                 "Implementation of this group is optional for all
                 systems that attach to a DS3 interface."

             OBJECT      dsx3LineType
             MIN-ACCESS  read-only
             DESCRIPTION
                 "Write access for the line type is not required."

             OBJECT      dsx3LineCoding
             MIN-ACCESS  read-only
             DESCRIPTION
                 "Write access for the line coding is not
                 required."

             OBJECT      dsx3SendCode
             MIN-ACCESS  read-only
             DESCRIPTION
                 "Write access for the send code is not required."

             OBJECT      dsx3LoopbackConfig
             MIN-ACCESS  read-only
             DESCRIPTION
                 "Write access for loopbacks is not required."

             OBJECT      dsx3TransmitClockSource
             MIN-ACCESS  read-only
             DESCRIPTION
                 "Write access for the transmit clock source is not
                 required."

             OBJECT      dsx3LineLength
             MIN-ACCESS  read-only
             DESCRIPTION
                 "Write access for the line length is not
                 required."

             OBJECT      dsx3Channelization
             MIN-ACCESS  read-only
             DESCRIPTION
                 "Write access for the channelization is not
                 required."

         ::= { ds3Compliances 1 }

     -- units of conformance

     ds3NearEndConfigGroup  OBJECT-GROUP
         OBJECTS { dsx3LineIndex,
                   dsx3TimeElapsed,
                   dsx3ValidIntervals,
                   dsx3LineType,
                   dsx3LineCoding,
                   dsx3SendCode,
                   dsx3CircuitIdentifier,
                   dsx3LoopbackConfig,
                   dsx3LineStatus,
                   dsx3TransmitClockSource,
                   dsx3InvalidIntervals,
                   dsx3LineLength,
                   dsx3LoopbackStatus,
                   dsx3Channelization,
                   dsx3Ds1ForRemoteLoop }
         STATUS  current
         DESCRIPTION
                 "A collection of objects providing configuration
                 information applicable to all DS3/E3 interfaces."
         ::= { ds3Groups 1 }

     ds3NearEndStatisticsGroup OBJECT-GROUP
         OBJECTS { dsx3CurrentIndex,
                   dsx3CurrentPESs,
                   dsx3CurrentPSESs,
                   dsx3CurrentSEFSs,
                   dsx3CurrentUASs,
                   dsx3CurrentLCVs,
                   dsx3CurrentPCVs,
                   dsx3CurrentLESs,
                   dsx3CurrentCCVs,
                   dsx3CurrentCESs,
                   dsx3CurrentCSESs,
                   dsx3IntervalIndex,
                   dsx3IntervalNumber,
                   dsx3IntervalPESs,
                   dsx3IntervalPSESs,
                   dsx3IntervalSEFSs,
                   dsx3IntervalUASs,
                   dsx3IntervalLCVs,
                   dsx3IntervalPCVs,
                   dsx3IntervalLESs,
                   dsx3IntervalCCVs,
                   dsx3IntervalCESs,
                   dsx3IntervalCSESs,
                   dsx3IntervalValidData,
                   dsx3TotalIndex,
                   dsx3TotalPESs,
                   dsx3TotalPSESs,
                   dsx3TotalSEFSs,
                   dsx3TotalUASs,
                   dsx3TotalLCVs,
                   dsx3TotalPCVs,
                   dsx3TotalLESs,
                   dsx3TotalCCVs,
                   dsx3TotalCESs,
                   dsx3TotalCSESs }
         STATUS  current
         DESCRIPTION
                 "A collection of objects providing statistics
                 information applicable to all DS3/E3 interfaces."
         ::= { ds3Groups 2 }

     ds3FarEndGroup  OBJECT-GROUP
         OBJECTS { dsx3FarEndLineIndex,
                   dsx3FarEndEquipCode,
                   dsx3FarEndLocationIDCode,
                   dsx3FarEndFrameIDCode,
                   dsx3FarEndUnitCode,
                   dsx3FarEndFacilityIDCode,
                   dsx3FarEndCurrentIndex,
                   dsx3FarEndTimeElapsed,
                   dsx3FarEndValidIntervals,
                   dsx3FarEndCurrentCESs,
                   dsx3FarEndCurrentCSESs,
                   dsx3FarEndCurrentCCVs,
                   dsx3FarEndCurrentUASs,
                   dsx3FarEndInvalidIntervals,
                   dsx3FarEndIntervalIndex,
                   dsx3FarEndIntervalNumber,
                   dsx3FarEndIntervalCESs,
                   dsx3FarEndIntervalCSESs,
                   dsx3FarEndIntervalCCVs,
                   dsx3FarEndIntervalUASs,
                   dsx3FarEndIntervalValidData,
                   dsx3FarEndTotalIndex,
                   dsx3FarEndTotalCESs,
                   dsx3FarEndTotalCSESs,
                   dsx3FarEndTotalCCVs,
                   dsx3FarEndTotalUASs }
         STATUS  current
         DESCRIPTION
                 "A collection of objects providing remote
                 configuration and statistics information
                 applicable to C-bit Parity and SYNTRAN DS3
                 interfaces."
         ::= { ds3Groups 3 }

     ds3DeprecatedGroup OBJECT-GROUP
         OBJECTS { dsx3IfIndex,
                   dsx3FracIndex,
                   dsx3FracNumber,
                   dsx3FracIfIndex }
         STATUS  deprecated
         DESCRIPTION
                 "A collection of obsolete objects that may be
                 implemented for backwards compatibility."
         ::= { ds3Groups 4 }

     ds3NearEndOptionalConfigGroup OBJECT-GROUP
         OBJECTS { dsx3LineStatusLastChange,
                   dsx3LineStatusChangeTrapEnable }
         STATUS    current
         DESCRIPTION
                 "A collection of objects that may be implemented
                 on DS3/E3 interfaces."
         ::= { ds3Groups 5 }

     ds3NearEndOptionalTrapGroup NOTIFICATION-GROUP
         NOTIFICATIONS { dsx3LineStatusChange }
         STATUS    current
         DESCRIPTION
                 "A collection of notifications that may be
                 implemented on DS3/E3 interfaces."
         ::= { ds3Groups 6 }

END
