ALCATEL-IND1-NTP-MIB DEFINITIONS ::= BEGIN

IMPORTS
  OBJECT-IDENTITY, MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE, 
  IpAddress, Counter32, Unsigned32, Integer32
FROM SNMPv2-SMI
  DisplayString, RowStatus
FROM SNMPv2-TC
  MODULE-COMPLIANCE,
  OBJECT-GROUP,
  NOTIFICATION-GROUP
FROM SNMPv2-CONF
  InetAddress, InetAddressType
FROM INET-ADDRESS-MIB
  softentIND1Ntp
FROM ALCATEL-IND1-BASE;

alcatelIND1NTPMIB MODULE-IDENTITY
    LAST-UPDATED "200704030000Z"
    ORGANIZATION "Alcatel-Lucent"
    CONTACT-INFO
        "Please consult with Customer Service to ensure the most appropriate
         version of this document is used with the products in question:

        Alcatel-Lucent,Enterprise Solutions Division
        (Formerly Alcatel Internetworking, Incorporated)
        26801 West Agoura Road
        Agoura Hills, CA  91301-5122
        United States Of America

        Telephone:             North America  +1 800 995 2696
                               Latin America  +1 877 919 9526
                               Europe         +31 23 556 0100
                               Asia           +65 394 7933
                               All Other      +1 818 878 4507

        Electronic Mail:         support@ind.alcatel.com
        World Wide Web:          http://alcatel-lucent.com/wps/portal/enterprise
        File Transfer Protocol:  ftp://ftp.ind.alcatel.com/pub/products/mibs"

    DESCRIPTION
        "This module describes an authoritative enterprise-specific Simple
         Network Management Protocol (SNMP) Management Information Base (MIB):

             Propietary NTP MIB definitions

         The right to make changes in specification and other information
         contained in this document without prior notice is reserved.

         No liability shall be assumed for any incidental, indirect, special,
         or consequential damages whatsoever arising from or related to this
         document or the information contained herein.

         Vendors, end-users, and other interested parties are granted
         non-exclusive license to use this specification in connection with
         management of the products for which it is intended to be used.

                   Copyright (C) 1995-2007 Alcatel-Lucent
                       ALL RIGHTS RESERVED WORLDWIDE"

    REVISION      "200704030000Z"
    DESCRIPTION
        "The latest version of this MIB Module."

    ::= { softentIND1Ntp 1 }

    alcatelIND1NTPMIBObjects OBJECT-IDENTITY 
        STATUS current
        DESCRIPTION
            "Branch For NTP Subsystem Managed Objects."
        ::= { alcatelIND1NTPMIB 1 }


-- ************************************************************************
--  NTP Global Configuration
-- ************************************************************************

    alaNtpConfig         OBJECT IDENTIFIER ::= { alcatelIND1NTPMIBObjects 1 }
    alaNtpInfo           OBJECT IDENTIFIER ::= { alcatelIND1NTPMIBObjects 2 }
    alaNtpStats          OBJECT IDENTIFIER ::= { alcatelIND1NTPMIBObjects 3 }
    alaNtpStatsStat      OBJECT IDENTIFIER ::= { alcatelIND1NTPMIBObjects 4 }
    alaNtpStatsLoop      OBJECT IDENTIFIER ::= { alcatelIND1NTPMIBObjects 5 }
    alaNtpStatsIo        OBJECT IDENTIFIER ::= { alcatelIND1NTPMIBObjects 6 }
    alaNtpAccess         OBJECT IDENTIFIER ::= { alcatelIND1NTPMIBObjects 7 }
    alaNtpLocalInfo      OBJECT IDENTIFIER ::= { alcatelIND1NTPMIBObjects 8 }



    alaIND1NtpMIBConformance OBJECT-IDENTITY
        STATUS current
        DESCRIPTION
            "Branch For Ntp Subsystem Managed Objects."
            ::= { alcatelIND1NTPMIB 2 }

    alaIND1NtpMIBGroups OBJECT-IDENTITY
        STATUS current
        DESCRIPTION
            "Branch For Ntp Subsystem Managed Objects."
            ::= { alaIND1NtpMIBConformance 1}

    alaIND1NtpMIBCompliances OBJECT-IDENTITY
        STATUS current
        DESCRIPTION
            "Branch For Ntp Subsystem Managed Objects."
            ::= { alaIND1NtpMIBConformance 2}

--
--

-- NTP configuration

alaNtpEnable OBJECT-TYPE
  SYNTAX        INTEGER {
                  enable(1),
                  disable(2)
                }
  MAX-ACCESS    read-write
  STATUS        current
  DESCRIPTION   "Enables/disables NTP clock discipline."
  DEFVAL		{ disable }
  ::= {alaNtpConfig 1}

alaNtpMonitorEnable OBJECT-TYPE
  SYNTAX        INTEGER {
                  enable(1),
                  disable(2)
                }
  MAX-ACCESS    read-write
  STATUS        current
  DESCRIPTION   "Enables/disables NTP monitor."
  DEFVAL		{ disable }
  ::= {alaNtpConfig 2}

alaNtpBroadcastEnable OBJECT-TYPE
  SYNTAX        INTEGER {
                  enable(1),
                  disable(2)
                }
  MAX-ACCESS    read-write
  STATUS        current
  DESCRIPTION   "Enables/disables NTP broadcast client."
  DEFVAL		{ disable }
  ::= {alaNtpConfig 3}


-- NTP Peer Table

alaNtpPeerTable OBJECT-TYPE
  SYNTAX        SEQUENCE OF NtpPeerEntry
  MAX-ACCESS    not-accessible
  STATUS        current
  DESCRIPTION   "Table containing the synchronization host this
    switch will be associated with."
  ::= {alaNtpConfig 4}

alaNtpPeerEntry OBJECT-TYPE
  SYNTAX        NtpPeerEntry
  MAX-ACCESS    not-accessible
  STATUS        current
  DESCRIPTION   "Each entry corresponds to a synchronization host."
  INDEX       {   alaNtpPeerAddressType, alaNtpPeerAddress   }
  ::= {alaNtpPeerTable 1}

NtpPeerEntry ::= SEQUENCE {
                alaNtpPeerAddressType
                   InetAddressType,
                alaNtpPeerAddress
                   InetAddress,
                alaNtpPeerIpAddress
                   IpAddress,
                alaNtpPeerType
                   INTEGER,
                alaNtpPeerAuth
                   INTEGER,
                alaNtpPeerVersion
                   INTEGER,
                alaNtpPeerMinpoll
                   INTEGER,
                alaNtpPeerPrefer
                   INTEGER,
                alaNtpPeerAdmin
                   RowStatus,
                alaNtpPeerName
                   DisplayString,
                alaNtpPeerStratum
                   INTEGER
                }

alaNtpPeerAddressType OBJECT-TYPE
      SYNTAX        InetAddressType
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION   "The InetAddress type of the synchronization host.
                    Only types InetAddressIPv4 (1) and InetAddressDNS (16)
                    are supported."
      ::={ alaNtpPeerEntry 1 }

alaNtpPeerAddress OBJECT-TYPE
      SYNTAX        InetAddress
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION   "The InetAddress of the synchronization host."
      ::={ alaNtpPeerEntry 2 }

alaNtpPeerIpAddress OBJECT-TYPE
      SYNTAX        IpAddress
      MAX-ACCESS    read-only
      STATUS        current
      DESCRIPTION   "The IP address of the synchronization host derrived
                    from the InetAddress."
      ::={ alaNtpPeerEntry 3 }

alaNtpPeerType OBJECT-TYPE
      SYNTAX        INTEGER  {
                      active(1),
                      passive(2),
                      client(3),
                      server(4),
                      broadcast(5),
                      bclient(8)
                    }
      MAX-ACCESS    read-write
      STATUS        current
      DESCRIPTION   "Type of synchronization host that will communicate
                    with this switch.  "
      DEFVAL		{ client }
      ::= { alaNtpPeerEntry 4 }

alaNtpPeerAuth OBJECT-TYPE
      SYNTAX        INTEGER ( 0 .. 65535 )
      MAX-ACCESS    read-write
      STATUS        current
      DESCRIPTION   "The authorization keyid for the remote host."
      DEFVAL		{ 0 }
      ::= { alaNtpPeerEntry 5 }

alaNtpPeerVersion OBJECT-TYPE
      SYNTAX        INTEGER ( 1 .. 255 )
      MAX-ACCESS    read-write
      STATUS        current
      DESCRIPTION   "The NTP version to communicate with the remote host."
      DEFVAL		{ 4 }
      ::= { alaNtpPeerEntry 6 }

alaNtpPeerMinpoll OBJECT-TYPE
      SYNTAX        INTEGER ( 4 .. 10 )
      MAX-ACCESS    read-write
      STATUS        current
      DESCRIPTION   "The minimum poll duration to the remote host.  This
                    value is a power of 2 seconds when the poll will occur.
                    For example, 4 (2 to the power 4) is 16 seconds.  The
                    maximum poll value is 10."
      DEFVAL		{ 6 }
      ::= { alaNtpPeerEntry 7 }

alaNtpPeerPrefer OBJECT-TYPE
      SYNTAX        INTEGER {
                      prefer (1),
                      noPrefer(2)
                    }
      MAX-ACCESS    read-write
      STATUS        current
      DESCRIPTION   "Marks the host as a preferred connection."
      DEFVAL		{ noPrefer }
      ::= { alaNtpPeerEntry 8 }

alaNtpPeerAdmin OBJECT-TYPE
      SYNTAX        RowStatus
      MAX-ACCESS    read-write
      STATUS        current
      DESCRIPTION   "Used in accordance to installation and removal conventions
                    for conceptual rows.  The RowStatus values that are
                    supported are the following:
                      active(1) - The row is active and valid.
                      createAndGo(4) - The row will be created and activated.
                      destroy(6) - The row will be destroyed."
      ::={ alaNtpPeerEntry 9 }

alaNtpPeerName OBJECT-TYPE
      SYNTAX        DisplayString
      MAX-ACCESS    read-only
      STATUS        current
      DESCRIPTION   "The DNS name for the peer association derrived from
                    the InetAddress."
      ::={ alaNtpPeerEntry 10 }

alaNtpPeerStratum OBJECT-TYPE
      SYNTAX        INTEGER ( 1 .. 16 )
      MAX-ACCESS    read-write
      STATUS        current
      DESCRIPTION   "The stratum level of the remote peer. If this
                      number is 16, the remote peer has not been
                      synchronized.  This parameter can only be set with 
                      a LOCALCLOCK server."
      DEFVAL		{ 5 }
      ::= { alaNtpPeerEntry 11 }

--

alaNtpAuthDelay OBJECT-TYPE
    SYNTAX        INTEGER ( 0 .. 65535 )
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION   "This field sets a specified time interval
                  that is added to timestamps included in
                  requests to the server that required
                  authentication. Typically this delay is
                  needed in cases of long delay paths, or servers
                  whose clocks are unsynchronized. Value is
                  in milli-seconds"
    DEFVAL		{ 0 }
    ::={ alaNtpConfig 5 }

alaNtpBroadcastDelay OBJECT-TYPE
    SYNTAX        INTEGER ( 0 .. 65535 )
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION   "This field sets a specified time interval
                  that is added to timestamps included in
                  messages from broadcast servers.  Value is 
                  in milli-seconds"
    DEFVAL		{ 4000 }
    ::={ alaNtpConfig 6 }

alaNtpKeysFile OBJECT-TYPE
    SYNTAX        DisplayString
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION   "Name of the file which has the authorization keys."
    ::={ alaNtpConfig 7 }

alaNtpConfigReqKeyId OBJECT-TYPE
    SYNTAX        INTEGER ( 0 .. 65535 )
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION   "Request messages ask for information from the NTP
                  entity such as timestamp information, statistics, etc.
                  This changes the authentication key identifier for
                  request messages sent from the switch to another NTP
                  entity."
    DEFVAL		{ 0 }
    ::={ alaNtpConfig 8 }

alaNtpConfigCtlKeyId OBJECT-TYPE
    SYNTAX        INTEGER ( 0 .. 65535 )
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION   "Control messages attempt to change the configuration
                  of the NTP entity in some fashion.  This changes
                  the authentication key identifier for control messages
                  sent from the switch to another NTP entity."
    DEFVAL		{ 0 }
    ::={ alaNtpConfig 9 }

alaNtpConfigCfgKeyId OBJECT-TYPE
    SYNTAX        INTEGER ( 0 .. 65535 )
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION   "Configuration messages changes information on the
                  NTP entity."
    DEFVAL		{ 0 }
    ::={ alaNtpConfig 10 }

alaNtpPrecision OBJECT-TYPE
    SYNTAX        INTEGER( -20..-1 )
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION   "This sets the server's advertised precision."
    DEFVAL		{ -6 }
    ::={ alaNtpConfig 11 }

alaNtpPeerTests OBJECT-TYPE
    SYNTAX        INTEGER {
                    enable(1),
                    disable(2)
                  }
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION   "Enables/disable NTP peer synchronization tests.
                  Disabling peer tests allows the NTP client to
                  synchonize with servers that are themselves
                  unsynchronized or would otherwise be eliminated
                  by other time source tests."
    DEFVAL        { enable }
    ::={ alaNtpConfig 12 }

alaNtpSysStratum OBJECT-TYPE
    SYNTAX        Integer32 ( 2 .. 16 )
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION  "The stratum level of the local server. If this number 
                  is 16 it indicates that the switch is not synchronized.
                  This helps the clients to select clocks with lower stratum 
                  number"
    DEFVAL		{ 16  }
    ::= { alaNtpConfig 13}

alaNtpMaxAssociation	OBJECT-TYPE
    SYNTAX        Integer32 ( 0 .. 64 )
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION  "The maximum number of peer and client associations that 
                  the switch will serve. This helps ensure that the switch 
                  isn't overwhelmed by huge numbers of NTP synchronization 
                  requests"
    DEFVAL		{ 32  }
    ::= { alaNtpConfig 14}

alaNtpAuthenticate	OBJECT-TYPE
    SYNTAX        INTEGER {
                  enable(1),
                  disable(2)
                	}
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION  "Enable/Disable authentication of the NTP requests on the 
                  switch"
    DEFVAL		{ enable }
    ::= { alaNtpConfig 15}


-- NTP Information

alaNtpPeerListTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF NtpPeerListEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION   "Used to display a brief list of all NTP associations
                  related to this switch (servers, peers, etc.)."
    ::= {alaNtpInfo 1}

alaNtpPeerListEntry OBJECT-TYPE
    SYNTAX        NtpPeerListEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION   "Each entry corresponds to one association."
    INDEX   {  alaNtpPeerListAddressType, alaNtpPeerListAddress  }
    ::= {alaNtpPeerListTable 1}

NtpPeerListEntry ::= SEQUENCE {
    alaNtpPeerListAddressType
       InetAddressType,
    alaNtpPeerListAddress
       InetAddress,
    alaNtpPeerListIpAddress
       IpAddress,
    alaNtpPeerListLocal
       IpAddress,
    alaNtpPeerListStratum
       INTEGER,
    alaNtpPeerListPoll
       INTEGER,
    alaNtpPeerListReach
       INTEGER,
    alaNtpPeerListDelay
       DisplayString,
    alaNtpPeerListOffset
       DisplayString,
    alaNtpPeerListDispersion
       DisplayString,
    alaNtpPeerListSynced
       INTEGER,
    alaNtpPeerListName
       DisplayString
    }

alaNtpPeerListAddressType OBJECT-TYPE
        SYNTAX        InetAddressType
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   "The InetAddress type of the synchronization host.
                      InetAddressIPv4 (1) is the only type currently
                      supported."
        ::={ alaNtpPeerListEntry 1 }

alaNtpPeerListAddress OBJECT-TYPE
        SYNTAX        InetAddress
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   "The InetAddress of the association."
        ::={ alaNtpPeerListEntry 2 }

alaNtpPeerListIpAddress OBJECT-TYPE
        SYNTAX        IpAddress
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The IP address of the association."
        ::={ alaNtpPeerListEntry 3 }

alaNtpPeerListLocal OBJECT-TYPE
        SYNTAX        IpAddress
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The local interface address assigned by
                      NTP to the remote association. If this address is
                      0.0.0.0, then the local address has yet to be
                      determined."
        ::={ alaNtpPeerListEntry 4 }

alaNtpPeerListStratum OBJECT-TYPE
        SYNTAX        INTEGER ( 1 .. 16 )
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The stratum level of the remote peer. If this
                      number is 16, the remote peer has not been
                      synchronized."
        ::={ alaNtpPeerListEntry 5 }

alaNtpPeerListPoll OBJECT-TYPE
        SYNTAX        INTEGER ( 1 .. 65535 )
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The polling interval, in seconds."
        ::={ alaNtpPeerListEntry 6 }

alaNtpPeerListReach OBJECT-TYPE
        SYNTAX        INTEGER ( 1 .. 255 )
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The reachability register of the remote
                      association, in octal format. This number is
                      determined by the NTP algorithm."
        ::={ alaNtpPeerListEntry 7 }

alaNtpPeerListDelay OBJECT-TYPE
        SYNTAX        DisplayString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The currently estimated delay of this remote
                      association, in seconds. This time is determined
                      by the NTP algorithm."
        ::={ alaNtpPeerListEntry 8 }

alaNtpPeerListOffset OBJECT-TYPE
        SYNTAX        DisplayString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The currently estimated offset of this remote
                      association, in seconds. This time is determined
                      by the NTP algorithm."
        ::={ alaNtpPeerListEntry 9 }

alaNtpPeerListDispersion OBJECT-TYPE
        SYNTAX        DisplayString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The currently estimated dispersion of this remote
                      association, in seconds. This time is determined
                      by the NTP algorithm."
        ::={ alaNtpPeerListEntry 10 }

alaNtpPeerListSynced OBJECT-TYPE
        SYNTAX        INTEGER {
                        synchronized(1),
                        notSynchronized(2)
                      }
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "Indicates that NTP is synchronized with this
                      entity."
        ::={ alaNtpPeerListEntry 11 }

alaNtpPeerListName OBJECT-TYPE
        SYNTAX        DisplayString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The DNS name for the peer association,"
        ::={ alaNtpPeerListEntry 12 }

--



-- alaNtpLocalInfo 
--     "Used to display information about the local
--     switch's implementation of NTP."

alaNtpInfoPeer OBJECT-TYPE
    SYNTAX        IpAddress
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION   "The IP address of the remote association."
    ::={ alaNtpLocalInfo 1 }

alaNtpInfoMode OBJECT-TYPE
    SYNTAX        DisplayString
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION   "The peer mode of this remote association."
    ::={ alaNtpLocalInfo 2 }

alaNtpInfoLeapIndicator OBJECT-TYPE
    SYNTAX        INTEGER {
                    noLeapWarning(0),
                    leapAddSecond(1),
                    leapDeleteSecond(2),
                    leapNotInSync(3)
                  }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION   "The status of leap second insertion for
                  this association."
    ::={ alaNtpLocalInfo 3 }

alaNtpInfoStratum OBJECT-TYPE
    SYNTAX        INTEGER ( 1 .. 16 )
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION   "The stratum level of the remote peer.
                  If this number is 16, the remote peer has not
                  been synchronized."
    ::={ alaNtpLocalInfo 4 }

alaNtpInfoPrecision OBJECT-TYPE
    SYNTAX        INTEGER( -20..-4 )
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION   "The advertised precision of the switch.
                  It will be a number between -4 and -20."
    ::={ alaNtpLocalInfo 5 }

alaNtpInfoDistance OBJECT-TYPE
    SYNTAX        DisplayString
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION   "This is a signed fixed-point number indicating
                  the total roundtrip delay to the primary reference
                  source at the root of the synchronization subnet,
                  in seconds."
    ::={ alaNtpLocalInfo 6 }

alaNtpInfoDispersion OBJECT-TYPE
    SYNTAX        DisplayString
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION   "This is a signed fixed-point number indicating
                  the maximum error relative to the primary reference
                  source at the root of the synchronization subnet,
                  in seconds."
    ::={ alaNtpLocalInfo 7 }

alaNtpInfoReferenceId OBJECT-TYPE
    SYNTAX        DisplayString
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION   "This is a 32-bit code identifying the particular
                  reference clock.  Can be an IP address."
    ::={ alaNtpLocalInfo 8 }

alaNtpInfoReferenceTime OBJECT-TYPE
    SYNTAX        DisplayString
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION   "This is the local time at which the local clock
                  was last set or corrected."
    ::={ alaNtpLocalInfo 9 }

alaNtpInfoFrequency OBJECT-TYPE
    SYNTAX        DisplayString
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION   "A number determining the local clocks frequency
                  in relation to a reference clock's Pulse per
                  Second (PPS). If the clock is running in perfect
                  synchronization, this number should be 1. Otherwise,
                  it will be slightly lower or higher in order to
                  compensate for the time difference."
    ::={ alaNtpLocalInfo 10 }

alaNtpInfoStability OBJECT-TYPE
    SYNTAX        DisplayString
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION   "The stability of the clock in relation to a
                  reference clock's Pulse per Second (PPS)."
    ::={ alaNtpLocalInfo 11 }

alaNtpInfoBroadcastDelay OBJECT-TYPE
    SYNTAX        DisplayString
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION   "The broadcast delay, in seconds, of this association."
    ::={ alaNtpLocalInfo 12 }

alaNtpInfoAuthDelay OBJECT-TYPE
    SYNTAX        DisplayString
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION   "The authentication delay, in seconds, of this
                  association."
    ::={ alaNtpLocalInfo 13 }


-- ************************************************************************
--  Peer Show Table
-- ************************************************************************
alaNtpPeerShowTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF NtpPeerShowEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION   "Used to display a brief list of all NTP associations
                  related to this switch (servers, peers, etc.)."
    ::= {alaNtpInfo 3}

alaNtpPeerShowEntry OBJECT-TYPE
      SYNTAX        NtpPeerShowEntry
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION   "Each entry corresponds to one association."
      INDEX       { alaNtpPeerShowRemoteAddressType, 
                    alaNtpPeerShowRemoteAddress }
      ::= {alaNtpPeerShowTable 1}

NtpPeerShowEntry ::= SEQUENCE {
        alaNtpPeerShowRemoteAddressType
          InetAddressType,
        alaNtpPeerShowRemoteAddress
          InetAddress,
        alaNtpPeerShowRemoteIpAddress
          IpAddress,
        alaNtpPeerShowLocal
          IpAddress,
        alaNtpPeerShowHmode
          DisplayString,
        alaNtpPeerShowPmode
          DisplayString,
        alaNtpPeerShowStratum
          INTEGER,
        alaNtpPeerShowPrecision
          INTEGER,
        alaNtpPeerShowLeapIndicator
          INTEGER,
        alaNtpPeerShowReferenceId
          DisplayString,
        alaNtpPeerShowRootDistance
          DisplayString,
        alaNtpPeerShowRootDispersion
          DisplayString,
        alaNtpPeerShowPpoll
          INTEGER,
        alaNtpPeerShowHpoll
          INTEGER,
        alaNtpPeerShowKeyid
          INTEGER,
        alaNtpPeerShowVersion
          INTEGER,
        alaNtpPeerShowAssociation
          INTEGER,
        alaNtpPeerShowValid
          INTEGER,
        alaNtpPeerShowReach
          INTEGER,
        alaNtpPeerShowUnreach
          INTEGER,
        alaNtpPeerShowFlash
          INTEGER,
        alaNtpPeerShowBroadcastOffset
          DisplayString,
        alaNtpPeerShowTTL
          INTEGER,
        alaNtpPeerShowTimer
          INTEGER,
        alaNtpPeerShowFlags
          INTEGER,
        alaNtpPeerShowReferenceTime
          DisplayString,
        alaNtpPeerShowOriginateTime
          DisplayString,
        alaNtpPeerShowReceiveTime
          DisplayString,
        alaNtpPeerShowTransmitTime
          DisplayString,
        alaNtpPeerShowOffset
          DisplayString,
        alaNtpPeerShowDelay
          DisplayString,
        alaNtpPeerShowDispersion
          DisplayString,
        alaNtpPeerShowName
          DisplayString,
        alaNtpPeerShowStatus
          BITS
        }

alaNtpPeerShowRemoteAddressType OBJECT-TYPE
        SYNTAX        InetAddressType
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   "The InetAddress type of the synchronization host.
                      InetAddressIPv4 (1) is the only type currently
                      supported."
        ::={ alaNtpPeerShowEntry 1 }

alaNtpPeerShowRemoteAddress OBJECT-TYPE
        SYNTAX        InetAddress
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   "The InetAddress of the remote association."
        ::={ alaNtpPeerShowEntry 2 }

alaNtpPeerShowRemoteIpAddress OBJECT-TYPE
        SYNTAX        IpAddress
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The IP address of the remote association."
        ::={ alaNtpPeerShowEntry 3 }


alaNtpPeerShowLocal OBJECT-TYPE
        SYNTAX        IpAddress
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The local interface address assigned by NTP to the
                      remote associations."
        ::={ alaNtpPeerShowEntry 4 }

alaNtpPeerShowHmode OBJECT-TYPE
        SYNTAX        DisplayString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The host mode of this remote association."
        ::={ alaNtpPeerShowEntry 5 }

alaNtpPeerShowPmode OBJECT-TYPE
        SYNTAX        DisplayString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The peer mode of this remote association."
        ::={ alaNtpPeerShowEntry 6 }

alaNtpPeerShowStratum OBJECT-TYPE
        SYNTAX        INTEGER ( 1 .. 16 )
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The stratum level of the remote peer."
        ::={ alaNtpPeerShowEntry 7 }

alaNtpPeerShowPrecision OBJECT-TYPE
        SYNTAX        INTEGER(-20..-4)
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The advertised precision of this association,
                      which is a number from -4 to -20."
        ::={ alaNtpPeerShowEntry 8 }

alaNtpPeerShowLeapIndicator OBJECT-TYPE
        SYNTAX        INTEGER {
                        noLeapWarning(0),
                        leapAddSecond(1),
                        leapDeleteSecond(2),
                        leapNotInSync(3)
                      }
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The status of leap second insertion for
                      this association."
        ::={ alaNtpPeerShowEntry 9 }

alaNtpPeerShowReferenceId OBJECT-TYPE
        SYNTAX        DisplayString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "This is a 32-bit code identifying the peers primary
                       reference source.  Normally an IP address."
        ::={ alaNtpPeerShowEntry 10 }

alaNtpPeerShowRootDistance OBJECT-TYPE
        SYNTAX        DisplayString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "This is a signed fixed-point number indicating
                      the total roundtrip delay to the primary reference
                      source at the root of the synchronization subnet,
                      in seconds."
        ::={ alaNtpPeerShowEntry 11 }

alaNtpPeerShowRootDispersion OBJECT-TYPE
        SYNTAX        DisplayString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "This is a signed fixed-point number indicating
                      the maximum error relative to the primary reference
                      source at the root of the synchronization subnet,
                      in seconds."
        ::={ alaNtpPeerShowEntry 12 }

alaNtpPeerShowPpoll OBJECT-TYPE
        SYNTAX        INTEGER ( 0 .. 255 )
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The poll time for this association when it is a peer."
        ::={ alaNtpPeerShowEntry 13 }

alaNtpPeerShowHpoll OBJECT-TYPE
        SYNTAX        INTEGER ( 0 .. 255 )
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The poll time for this association when it is a host."
        ::={ alaNtpPeerShowEntry 14 }

alaNtpPeerShowKeyid OBJECT-TYPE
        SYNTAX        INTEGER ( 0 .. 65535 )
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "This is an integer identifying the cryptographic
                      key used to generate the message authentication code."
        ::={ alaNtpPeerShowEntry 15 }

alaNtpPeerShowVersion OBJECT-TYPE
        SYNTAX        INTEGER ( 1 .. 255 )
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "What version of NTP this association is using."
        ::={ alaNtpPeerShowEntry 16 }

alaNtpPeerShowAssociation OBJECT-TYPE
        SYNTAX        INTEGER ( 0 .. 65535 )
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of seconds since this NTP entity was
                      associated with the switch."
        ::={ alaNtpPeerShowEntry 17 }

alaNtpPeerShowValid OBJECT-TYPE
        SYNTAX        INTEGER {
                        false(0),
                        true(1)
                      }
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "This is an integer indicating the validity
                      of current NTP system variables.  The validity
                      is made false if system variable are changed
                      and a new peer sample under the changed
                      configuration has not been received."
        ::={ alaNtpPeerShowEntry 18 }

alaNtpPeerShowReach OBJECT-TYPE
        SYNTAX        INTEGER ( 0 .. 255 )
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "This is a shift register used to determine the
                      reachability status of this peer."
        ::={ alaNtpPeerShowEntry 19 }

alaNtpPeerShowUnreach OBJECT-TYPE
        SYNTAX        INTEGER ( 0 .. 15 )
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of times this NTP entity was unreachable."
        ::={ alaNtpPeerShowEntry 20 }

alaNtpPeerShowFlash OBJECT-TYPE
        SYNTAX        INTEGER ( 0 .. 32767 )
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "This bitmap reveals the state at the last grumble from
                      the peer and are most handy for diagnosing problems.

                      Duplicate packet:                       0x0001
                      Bogus packet:                           0x0002
                      Protocol unsynchronized:                0x0004
                      Access denied:                          0x0008
                      Authentication failure:                 0x0010
                      Peer clock unsynchronized:              0x0020
                      Peer stratum out:                       0x0040
                      Root delay/dispersion bounds check:     0x0080
                      Peer delay dispersion bounds check:     0x0100
                      Autokey failed:                         0x0200
                      Proventic not confirmed:                0x0400"

        ::={ alaNtpPeerShowEntry 21 }

alaNtpPeerShowBroadcastOffset OBJECT-TYPE
        SYNTAX        DisplayString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The broadcast delay."
        ::={ alaNtpPeerShowEntry 22 }

alaNtpPeerShowTTL OBJECT-TYPE
        SYNTAX        INTEGER ( 0 .. 255 )
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "This field displays the Time-to-Live (TTL) time
                      in seconds and the mode (unicast, multicast, or
                      broadcast) of NTP messages sent to a broadcast address."
        ::={ alaNtpPeerShowEntry 23 }

alaNtpPeerShowTimer OBJECT-TYPE
        SYNTAX        INTEGER ( 0 .. 2147483647 )
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The time to next poll in seconds."
        ::={ alaNtpPeerShowEntry 24 }

alaNtpPeerShowFlags OBJECT-TYPE
        SYNTAX        INTEGER ( 0 .. 255 )
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "This details which flags have been configured for this peer.
                      Association configured:                 0x01
                      System peer:                            0x02
                      Enabled for burst mode synchronization: 0x04
                      Reference clock:                        0x08
                      Preferred server:                       0x10
                      Authentable:                            0x20
                      Synchronization candidate:              0x40
                      Synchronization candidates short-list:  0x80"

        ::={ alaNtpPeerShowEntry 25 }

alaNtpPeerShowReferenceTime OBJECT-TYPE
        SYNTAX        DisplayString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "This is the local time, in timestamp format, when
                      the peer clock was last updated."
        ::={ alaNtpPeerShowEntry 26 }

alaNtpPeerShowOriginateTime OBJECT-TYPE
        SYNTAX        DisplayString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "This is the local time, in timestamp format, of
                      the peer when its latest NTP message was sent."
        ::={ alaNtpPeerShowEntry 27 }

alaNtpPeerShowReceiveTime OBJECT-TYPE
        SYNTAX        DisplayString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "This is the local time, in timestamp format, when
                      the latest NTP message from the peer arrived."
        ::={ alaNtpPeerShowEntry 28 }

alaNtpPeerShowTransmitTime OBJECT-TYPE
        SYNTAX        DisplayString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "This is the local time, in timestamp format, at
                      which the last NTP message was sent from this
                      association."
        ::={ alaNtpPeerShowEntry 29 }

alaNtpPeerShowOffset OBJECT-TYPE
        SYNTAX        DisplayString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The currently estimated offset of this remote
                      association, in seconds."
        ::={ alaNtpPeerShowEntry 30 }

alaNtpPeerShowDelay OBJECT-TYPE
        SYNTAX        DisplayString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The currently estimated delay of this remote
                      association, in seconds."
        ::={ alaNtpPeerShowEntry 31 }

alaNtpPeerShowDispersion OBJECT-TYPE
        SYNTAX        DisplayString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The currently estimated dispersion of this remote
                      association, in seconds."
        ::={ alaNtpPeerShowEntry 32 }

alaNtpPeerShowName OBJECT-TYPE
        SYNTAX        DisplayString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The DNS name for the peer association,"
        ::={ alaNtpPeerShowEntry 33 }

alaNtpPeerShowStatus OBJECT-TYPE
        SYNTAX BITS {
            rejected(0),
            falsticker(1),
            excess(2),
            outlyer(3),
            candidate(4),
            exceedsMaxDistance(5),
            selected(6),
            selectedPPS(7),
            reachable(8),
            authenticated(9),
            authenticationRequired(10),
            configured(11)
        }
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "Peer selection status:                 Bits 0 - 7
                        - Rejected due to high stratum
                          and/or failed sanity checks:        1
                        - Designated falsticker by the
                          intersection algorithm:             2
                        - Excess, culled from the end of
                          the candidate list:                 3
                        - Outlyer, discarded by the
                          clustering algorithm:               4
                        - Candidate, included in the final
                          selection set:                      5
                        - Selected for synchronization; but
                          distance exceeds maximum:           6
                        - Selected for synchronization:       7
                        - Selected for synchronization,
                          PPS signal in use:                  8

                      Peer association status:                Bits 9 - 12
                        - Peer association configured:        9
                        - Peer authentication required:       10
                        - Last peer message authenticated:    11 
                        - Peer reachable:                     12"

        ::={ alaNtpPeerShowEntry 34 }



-- NTP statistics

-- alaNtpStatsStat 
--     "The local server statistics."

alaNtpStatsStatUptime OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of seconds the local NTP server has
                      been associated with the switch."
        ::={ alaNtpStatsStat 1 }

alaNtpStatsStatReset OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of seconds since the last time the
                      local NTP server has been restarted."
        ::={ alaNtpStatsStat 2 }

alaNtpStatsStatBadStratum OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of NTP packets received that had a
                      corrupted stratum bit in the data of the packet."
        ::={ alaNtpStatsStat 3 }

alaNtpStatsStatOldVersion OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of NTP packets received that were
                      of an older version of NTP (either version 1 or 2)."
        ::={ alaNtpStatsStat 4 }

alaNtpStatsStatNewVersion OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of NTP packets received that were
                      version 3 of NTP."
        ::={ alaNtpStatsStat 5 }

alaNtpStatsStatUnknownVersion OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of NTP packets received that the
                      version was unknown (most likely due to packet
                      corruption)."
        ::={ alaNtpStatsStat 6 }

alaNtpStatsStatBadLength OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of NTP packets received that did not
                      fit the NTP packet structure (most likely due to
                      packet corruption)."
        ::={ alaNtpStatsStat 7 }

alaNtpStatsStatProcessed OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The total number of NTP packets processed."
        ::={ alaNtpStatsStat 8 }

alaNtpStatsStatBadAuth OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of NTP packets rejected because they
                      did not meet authentication standards."
        ::={ alaNtpStatsStat 9 }

alaNtpStatsStatLimitRejects OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of NTP packets rejected because they
                      did not meet authentication standards."
        ::={ alaNtpStatsStat 10 }

alaNtpStatsPeerTable OBJECT-TYPE
        SYNTAX        SEQUENCE OF NtpStatsPeerEntry
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   "Table containing the synchronization host statistics."
        ::= {alaNtpStats 2}

alaNtpStatsPeerEntry OBJECT-TYPE
        SYNTAX        NtpStatsPeerEntry
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   "Each entry corresponds to a synchronization host."
        INDEX       { alaNtpStatsPeerAddressType, alaNtpStatsPeerAddress }
        ::= {alaNtpStatsPeerTable 1}

NtpStatsPeerEntry ::= SEQUENCE {
                alaNtpStatsPeerAddressType
                   InetAddressType,
                alaNtpStatsPeerAddress
                   InetAddress,
                alaNtpStatsPeerIpAddress
                   IpAddress,
                alaNtpStatsPeerLocal
                   IpAddress,
                alaNtpStatsPeerLastRcv
                   Counter32,
                alaNtpStatsPeerNextSend
                   Counter32,
                alaNtpStatsPeerReachChange
                   Counter32,
                alaNtpStatsPeerPacketsSent
                   Counter32,
                alaNtpStatsPeerPacketsRcvd
                   Counter32,
                alaNtpStatsPeerBadAuth
                   Counter32,
                alaNtpStatsPeerBogusOrigin
                   Counter32,
                alaNtpStatsPeerDuplicate
                   Counter32,
                alaNtpStatsPeerBadDispersion
                   Counter32,
                alaNtpStatsPeerBadRefTime
                   Counter32,
                alaNtpStatsPeerCandidateOrder
                   Counter32,
                alaNtpStatsPeerReset
                   INTEGER,
                alaNtpStatsPeerName
                   DisplayString
                }

alaNtpStatsPeerAddressType OBJECT-TYPE
        SYNTAX        InetAddressType
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   "The InetAddress type of the synchronization host.
                      InetAddressIPv4 (1) is the only type currently
                      supported."
        ::={ alaNtpStatsPeerEntry 1 }

alaNtpStatsPeerAddress OBJECT-TYPE
        SYNTAX        InetAddress
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   "The InetAddress of the synchronization host."
        ::={ alaNtpStatsPeerEntry 2 }

alaNtpStatsPeerIpAddress OBJECT-TYPE
        SYNTAX        IpAddress
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The IP address of the synchronization host."
        ::={ alaNtpStatsPeerEntry 3 }

alaNtpStatsPeerLocal OBJECT-TYPE
        SYNTAX        IpAddress
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The local interface address assigned by
                      NTP to the remote association."
        ::={ alaNtpStatsPeerEntry 4 }

alaNtpStatsPeerLastRcv OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The time since the last packet was received."
        ::= { alaNtpStatsPeerEntry 5 }

alaNtpStatsPeerNextSend OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The time until the next packet is to be sent."
        ::= { alaNtpStatsPeerEntry 6 }

alaNtpStatsPeerReachChange OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The time that the peer has been reachable."
        ::= { alaNtpStatsPeerEntry 7 }

alaNtpStatsPeerPacketsSent OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of packets that have been sent."
        ::= { alaNtpStatsPeerEntry 8 }

alaNtpStatsPeerPacketsRcvd OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of packets that have been received."
        ::= { alaNtpStatsPeerEntry 9 }

alaNtpStatsPeerBadAuth OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of packets received with bad
                      authentication."
        ::= { alaNtpStatsPeerEntry 10 }

alaNtpStatsPeerBogusOrigin OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of bogus packets."
        ::= { alaNtpStatsPeerEntry 11 }

alaNtpStatsPeerDuplicate OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of duplicated packets received."
        ::= { alaNtpStatsPeerEntry 12 }

alaNtpStatsPeerBadDispersion OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number bad dispersions."
        ::= { alaNtpStatsPeerEntry 13 }

alaNtpStatsPeerBadRefTime OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        deprecated
        DESCRIPTION   "The number of bad reference times received."
        ::= { alaNtpStatsPeerEntry 14 }

alaNtpStatsPeerCandidateOrder OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The order of synchronization candidates."
        ::= { alaNtpStatsPeerEntry 15 }

alaNtpStatsPeerReset OBJECT-TYPE
        SYNTAX        INTEGER ( 0 .. 2147483647 )
        MAX-ACCESS    read-write
        STATUS        current
        DESCRIPTION   "The number of seconds since the statistics for this
                      peer were last reset.  Writing any value will reset 
                      the peer statistics.  "
        DEFVAL		{ 0 }
        ::= { alaNtpStatsPeerEntry 16 }

alaNtpStatsPeerName OBJECT-TYPE
        SYNTAX        DisplayString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The DNS name for the peer association,"
        ::={ alaNtpStatsPeerEntry 17 }


--

-- alaNtpStatsLoop 
--     "The loop filter is used to control and correct
--      the phase of timestamps as processed by the local
--      clock. The loop filter examines timestamps sent to
--      and from the local clock and can adjust them to
--      account for natural wander and jitter."

alaNtpStatsLoopOffset OBJECT-TYPE
        SYNTAX        DisplayString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The currently estimated offset of this remote
                      association, in seconds. This counter indicates
                      the offset of the peer clock relative to the local
                      clock."
        ::={ alaNtpStatsLoop 1 }

alaNtpStatsLoopFrequency OBJECT-TYPE
        SYNTAX        DisplayString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "A number determining the local clocks frequency
                      in relation to a reference clocks Pulse per Second
                      (PPS). If the clock is running in perfect
                      synchronization, this number should be 1. Otherwise,
                      it will be slightly lower or higher in order to
                      compensate for the time discrepancy between the
                      reference clock and the local clock."
        ::={ alaNtpStatsLoop 2 }

alaNtpStatsLoopPollAdjust OBJECT-TYPE
        SYNTAX        INTEGER ( -30 .. 30 )
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "Determines the peer polling time."
        ::={ alaNtpStatsLoop 3 }

alaNtpStatsLoopWatchdog OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "Makes sure that NTP timer continues to run."
        ::={ alaNtpStatsLoop 4 }


--

-- alaNtpStatsIo
--    "General statistics on received and transmitted
--     NTP packets for this switch."
alaNtpStatsIoReset OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of seconds since the last restart of NTP."
        ::={ alaNtpStatsIo 1 }

alaNtpStatsIoRcvBuffers OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of switch receive buffers currently being
                      used by this NTP entity."
        ::={ alaNtpStatsIo 2 }

alaNtpStatsIoFreeRcvBuffers OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of free receive buffers."
        ::={ alaNtpStatsIo 3 }

alaNtpStatsIoUsedRcvBuffers OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of receive buffers currently being used."
        ::={ alaNtpStatsIo 4 }

alaNtpStatsIoRefills OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of times we added packets."
        ::={ alaNtpStatsIo 5 }

alaNtpStatsIoDroppedPackets OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of packets dropped."
        ::={ alaNtpStatsIo 6 }

alaNtpStatsIoIgnoredPackets OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of packets ignored."
        ::={ alaNtpStatsIo 7 }

alaNtpStatsIoRcvPackets OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The total number of NTP packets received by the switch."
        ::={ alaNtpStatsIo 8 }

alaNtpStatsIoSentPackets OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The total number of NTP packets sent by the switch."
        ::={ alaNtpStatsIo 9 }

alaNtpStatsIoNotSentPackets OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of NTP packets generated but not sent
                      due to restrictions."
        ::={ alaNtpStatsIo 10 }

alaNtpStatsIoInterrupts OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of times NTP information was interrupted
                      in the process of transmitting or receiving."
        ::={ alaNtpStatsIo 11 }

alaNtpStatsIoInterruptsRcv OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of packets received by the interrupt
      handler."
        ::={ alaNtpStatsIo 12 }

alaNtpStatsReset OBJECT-TYPE
        SYNTAX        INTEGER ( 0 .. 127 )
        MAX-ACCESS    read-write
        STATUS        current
        DESCRIPTION   "Resets the statistics counters for the following
                      subsystems:
                      0x01  - all peers
                      0x02  - i/o
                      0x04  - system
                      0x08  - memory
                      0x10  - timer
                      0x20  - authentication
                      0x40  - control"
        DEFVAL		{ 0 }
        ::={ alaNtpStats 5 }

alaNtpStatsMonitorTable OBJECT-TYPE
        SYNTAX        SEQUENCE OF NtpStatsMonitorEntry
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   "Table containing the association monitoring list."
        ::= {alaNtpStats 6}

alaNtpStatsMonitorEntry OBJECT-TYPE
        SYNTAX        NtpStatsMonitorEntry
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   "Each entry corresponds to a synchronization host."
        INDEX       { alaNtpStatsMonitorIndex  }
        ::= {alaNtpStatsMonitorTable 1}

NtpStatsMonitorEntry ::= SEQUENCE {
      alaNtpStatsMonitorIndex
         Unsigned32,
      alaNtpStatsMonitorAddress
         IpAddress,
      alaNtpStatsMonitorPort
         INTEGER,
      alaNtpStatsMonitorLocalAddress
         IpAddress,
      alaNtpStatsMonitorCount
         Counter32,
      alaNtpStatsMonitorMode
         DisplayString,
      alaNtpStatsMonitorVersion
         INTEGER,
      alaNtpStatsMonitorDrop
         Counter32,
      alaNtpStatsMonitorLast
         Counter32,
      alaNtpStatsMonitorFirst
         Counter32,
      alaNtpStatsMonitorName
         DisplayString
    }

alaNtpStatsMonitorIndex OBJECT-TYPE
        SYNTAX        Unsigned32 ( 1 .. 65535 )
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   "Table index."
        ::={ alaNtpStatsMonitorEntry 1 }

alaNtpStatsMonitorAddress OBJECT-TYPE
        SYNTAX        IpAddress
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The IP address of the remote association."
        ::={ alaNtpStatsMonitorEntry 2 }

alaNtpStatsMonitorPort OBJECT-TYPE
        SYNTAX        INTEGER ( 0 .. 65535 )
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The IP port number of the association."
        ::={ alaNtpStatsMonitorEntry 3 }

alaNtpStatsMonitorLocalAddress OBJECT-TYPE
        SYNTAX        IpAddress
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The local IP address of the association."
        ::={ alaNtpStatsMonitorEntry 4 }

alaNtpStatsMonitorCount OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of NTP packets received from
                      this association."
        ::={ alaNtpStatsMonitorEntry 5 }

alaNtpStatsMonitorMode OBJECT-TYPE
        SYNTAX        DisplayString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The mode the NTP association uses in relation
                      to the switch."
        ::={ alaNtpStatsMonitorEntry 6 }

alaNtpStatsMonitorVersion OBJECT-TYPE
        SYNTAX        INTEGER ( 1 .. 255 )
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The version of NTP the association is using."
        ::={ alaNtpStatsMonitorEntry 7 }

alaNtpStatsMonitorDrop OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of NTP packets received from this
                      association that were dropped."
        ::={ alaNtpStatsMonitorEntry 8 }

alaNtpStatsMonitorLast OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of seconds since the last NTP message
                      has been received from this association."
        ::={ alaNtpStatsMonitorEntry 9 }

alaNtpStatsMonitorFirst OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The number of seconds since the first NTP message
                      has been received from this association."
        ::={ alaNtpStatsMonitorEntry 10 }

alaNtpStatsMonitorName OBJECT-TYPE
        SYNTAX        DisplayString
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "The DNS name for the peer association,"
        ::={ alaNtpStatsMonitorEntry 11 }


-- NTP Admin control


-- NTP Access control

alaNtpAccessKeyIdTable OBJECT-TYPE
      SYNTAX        SEQUENCE OF NtpAccessKeyIdEntry
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION   "Table containing the trusted keys."
      ::={ alaNtpAccess 1 }

alaNtpAccessKeyIdEntry OBJECT-TYPE
      SYNTAX        NtpAccessKeyIdEntry
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION   "Entry of a trusted key."
      INDEX { alaNtpAccessKeyIdKeyId }
      ::={ alaNtpAccessKeyIdTable 1 }

NtpAccessKeyIdEntry ::= SEQUENCE {
    alaNtpAccessKeyIdKeyId
      INTEGER,
    alaNtpAccessKeyIdTrust
      INTEGER
    }

alaNtpAccessKeyIdKeyId OBJECT-TYPE
      SYNTAX        INTEGER ( 0 .. 65535 )
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION   "Keyid of the key in the key file."
      ::={ alaNtpAccessKeyIdEntry 1 }

alaNtpAccessKeyIdTrust OBJECT-TYPE
      SYNTAX        INTEGER {
                      trusted(1),
                      untrusted(2)
                    }
      MAX-ACCESS    read-write
      STATUS        current
      DESCRIPTION   "The current state of trust of the table entry."
      DEFVAL		{ untrusted }
      ::={ alaNtpAccessKeyIdEntry 2 }



alaNtpAccessRestrictedTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF NtpAccessRestrictedEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION   "Table containing the restricted addresses."
    ::={ alaNtpAccess 2 }

alaNtpAccessRestrictedEntry OBJECT-TYPE
    SYNTAX        NtpAccessRestrictedEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION   "Entry of a restricted address."
    INDEX {
      alaNtpAccessRestrictedIpAddress,
      alaNtpAccessRestrictedMask
    }
    ::={ alaNtpAccessRestrictedTable 1 }

NtpAccessRestrictedEntry ::= SEQUENCE {
      alaNtpAccessRestrictedIpAddress
        IpAddress,
      alaNtpAccessRestrictedMask
        IpAddress,
      alaNtpAccessRestrictedRestrictions
        INTEGER,
      alaNtpAccessRestrictedCount
        Counter32,
      alaNtpAccessRestrictedRowStatus
        RowStatus
    }

alaNtpAccessRestrictedIpAddress OBJECT-TYPE
        SYNTAX        IpAddress
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   "IP address to restrict."
        ::={ alaNtpAccessRestrictedEntry 1 }


alaNtpAccessRestrictedMask OBJECT-TYPE
        SYNTAX        IpAddress
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   "IP mask to restrict."
        ::={ alaNtpAccessRestrictedEntry 2 }

alaNtpAccessRestrictedRestrictions OBJECT-TYPE
        SYNTAX        INTEGER ( 0 .. 1023 )
        MAX-ACCESS    read-write
        STATUS        current
        DESCRIPTION   "A mask indicating the restrictions to apply
                      to the entry.
                      0x0001 - ignore, Ignore all packets from hosts.
                        Can't use this on default (0.0.0.0).
                      0x0002 - noserve, Ignore NTP packets other than
                        information queries and config-uration requests.
                      0x0004 - notrust, Treat these hosts normally in other
                        respects, but never use them as synchronization sources.
                      0x0008 - noquery, Ignore all NTP information
                        queries and configuration requests from the source.
                      0x0010 - nomodify, Ignore all NTP information
                        queries and configuration requests
                        that attempt to modify the state of the server.
                      0x0020 - nopeer, Provide stateless time service to
                        polling hosts, but do not allocate peer
                        memory resources to these hosts even if
                        they otherwise might be considered useful
                        as future synchronization partners.
                      0x0040 - notrap, Decline to provide control message
                        trap service to matching hosts.
                      0x0080 - lowpriotrap, Declare traps set by matching
                        hosts to be low priority.
                      0x0100 - limited, These hosts are subject to a
                        limitation of the number of clients from the same net.
                      0x0200 - version. Serves only current version.
                      0x0400 - demobilize. A demobilization packet (kod) packet is sent."
        DEFVAL		{ 0 }
        ::={ alaNtpAccessRestrictedEntry 3 }

alaNtpAccessRestrictedCount OBJECT-TYPE
        SYNTAX        Counter32
        MAX-ACCESS    read-only
        STATUS        current
        DESCRIPTION   "Number of packets matched."
        ::={ alaNtpAccessRestrictedEntry 4 }

alaNtpAccessRestrictedRowStatus OBJECT-TYPE
        SYNTAX        RowStatus
        MAX-ACCESS    read-write
        STATUS        current
        DESCRIPTION   "Used in accordance to installation and removal conventions
                      for conceptual rows.  The RowStatus values that are
                      supported are the following:
                        active(1) - The row is active and valid.
                        createAndGo(4) - The row will be created and activated.
                        destroy(6) - The row will be destroyed."
        ::={ alaNtpAccessRestrictedEntry 5 }

alaNtpAccessRereadKeyFile OBJECT-TYPE
        SYNTAX        INTEGER {
                        reload(1),
                        inProgress(2),
                        successful(3),
                        error(4)
                      }
        MAX-ACCESS    read-write
        STATUS        current
        DESCRIPTION   "Reloads the keyfile containing all currently
                      existing keys into the alaNtpAccessKeyIdTable in the
                      switch's memory. Reading this object will yield one of
                      the three following values:
                          inProgress(2),
                          successful(3),
                          failed(4)
                      A value of inProgress means that table reload procedure
                      is inProgress and not yet complete.  A sucessful reply
                      means the last attempted keyfile load completed successfully.
                      A failed response indicates the last attempt to reload failed.
                      Writing a value of 1 to this object initiates a reload of the
                      table."
        DEFVAL		{ successful }
        ::={ alaNtpAccess 3 }

-- Ntp Client IP Information (Deprecated)   
    
     ntpClientConfig OBJECT-TYPE   
         SYNTAX      INTEGER { default(1), nonLoopback0(2), userIp(3) }    
         MAX-ACCESS read-write   
         STATUS        deprecated   
         DESCRIPTION   
                 "The Agent Config Information   
                 1 -- Default(Loopback0 or closest IP)   
                 2 -- Non Loopback0   
                  3 -- Interface IP Specified by User"   
         DEFVAL        { 1 }   
         ::= { alcatelIND1NTPMIBObjects 9 }   
    
     ntpClientIP OBJECT-TYPE           
         SYNTAX     IpAddress   
         MAX-ACCESS read-write   
         STATUS        deprecated   
         DESCRIPTION   
                 "The interface IP Address to be used in NTP Packets   
                 for Source IP field."           
         ::= {  alcatelIND1NTPMIBObjects 10  }   
  
-- Ntp Source IP Information

    alaNtpSrcIpConfig OBJECT-TYPE
	SYNTAX      INTEGER { default(1), nonLoopback0(2), userIp(3) } 
	MAX-ACCESS read-write
	STATUS        obsolete 
	DESCRIPTION
		"The Agent Config Information
		1 -- Default(Loopback0 or closest IP)
		2 -- Non Loopback0
	 	3 -- Interface IP Specified by User
		This object has been obsoleted. Use the alaIpManagedIntfEntry objects 
		in AlcatelIND1Ip.mib"
	DEFVAL        { 1 }
	::= { alcatelIND1NTPMIBObjects 11 }

    alaNtpSrcIp OBJECT-TYPE	
	SYNTAX     IpAddress
	MAX-ACCESS read-write
	STATUS        obsolete 
	DESCRIPTION
		"The interface IP Address to be used in NTP Packets
		for Source IP field.
		This object has been obsoleted. Use the alaIpManagedIntfEntry objects
		in AlcatelIND1Ip.mib"
	::= {  alcatelIND1NTPMIBObjects 12  }

-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx
-- COMPLIANCE
-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

    alaIND1NtpMonitorMIBCompliance MODULE-COMPLIANCE
        STATUS  current
        DESCRIPTION
            "Compliance statement for Health Monitoring."
        MODULE
            MANDATORY-GROUPS
            {
                alaNtpConfigGroup,
                alaNtpInfoGroup,
                alaNtpStatsGroup,
                alaNtpStatsStatGroup,
                alaNtpStatsLoopGroup,
                alaNtpStatsIoGroup,
                alaNtpAccessGroup,
                alaNtpLocalInfoGroup,
		alaNtpEventsGroup,
		alaNtpSrcIpGroup
            }

        ::= { alaIND1NtpMIBCompliances 1 }


-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx
-- UNITS OF CONFORMANCE
-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

    alaNtpConfigGroup OBJECT-GROUP
        OBJECTS
        {
            alaNtpEnable,
            alaNtpMonitorEnable,
            alaNtpBroadcastEnable,
            alaNtpPeerIpAddress,
            alaNtpPeerType,
            alaNtpPeerAuth,
            alaNtpPeerVersion,
            alaNtpPeerMinpoll,
            alaNtpPeerPrefer,
            alaNtpPeerAdmin,
            alaNtpPeerName,
            alaNtpPeerStratum,
            alaNtpAuthDelay,
            alaNtpBroadcastDelay,
            alaNtpKeysFile,
            alaNtpConfigReqKeyId,
            alaNtpConfigCtlKeyId,
            alaNtpPrecision,
            alaNtpPeerTests,
	    alaNtpSysStratum,
	    alaNtpMaxAssociation,
	    alaNtpAuthenticate
        }
        STATUS  current
        DESCRIPTION
            "Collection of NTP configuration objects."
        ::= { alaIND1NtpMIBGroups 1 }



    alaNtpInfoGroup OBJECT-GROUP
        OBJECTS
        {
            alaNtpPeerListIpAddress,
            alaNtpPeerListLocal,
            alaNtpPeerListStratum,
            alaNtpPeerListPoll,
            alaNtpPeerListReach,
            alaNtpPeerListDelay,
            alaNtpPeerListOffset,
            alaNtpPeerListDispersion,
            alaNtpPeerListSynced,
            alaNtpPeerListName,
            alaNtpPeerShowRemoteIpAddress,
            alaNtpPeerShowLocal,
            alaNtpPeerShowHmode,
            alaNtpPeerShowPmode,
            alaNtpPeerShowStratum,
            alaNtpPeerShowPrecision,
            alaNtpPeerShowLeapIndicator,
            alaNtpPeerShowReferenceId,
            alaNtpPeerShowRootDistance,
            alaNtpPeerShowRootDispersion,
            alaNtpPeerShowPpoll,
            alaNtpPeerShowHpoll,
            alaNtpPeerShowKeyid,
            alaNtpPeerShowVersion,
            alaNtpPeerShowAssociation,
            alaNtpPeerShowValid,
            alaNtpPeerShowReach,
            alaNtpPeerShowUnreach,
            alaNtpPeerShowFlash,
            alaNtpPeerShowBroadcastOffset,
            alaNtpPeerShowTTL,
            alaNtpPeerShowTimer,
            alaNtpPeerShowFlags,
            alaNtpPeerShowReferenceTime,
            alaNtpPeerShowOriginateTime,
            alaNtpPeerShowReceiveTime,
            alaNtpPeerShowTransmitTime,
            alaNtpPeerShowOffset,
            alaNtpPeerShowDelay,
            alaNtpPeerShowDispersion,
            alaNtpPeerShowName,
            alaNtpPeerShowStatus,
	    alaNtpClientListVersion,
	    alaNtpClientKey
        }
        STATUS  current
        DESCRIPTION
            "Collection of NTP peer information objects."
        ::= { alaIND1NtpMIBGroups 2 }

    alaNtpStatsGroup OBJECT-GROUP
        OBJECTS
        {
            alaNtpStatsPeerIpAddress,
            alaNtpStatsPeerLocal,
            alaNtpStatsPeerLastRcv,
            alaNtpStatsPeerNextSend,
            alaNtpStatsPeerReachChange,
            alaNtpStatsPeerPacketsSent,
            alaNtpStatsPeerPacketsRcvd,
            alaNtpStatsPeerBadAuth,
            alaNtpStatsPeerBogusOrigin,
            alaNtpStatsPeerDuplicate,
            alaNtpStatsPeerBadDispersion,
            alaNtpStatsPeerBadRefTime,
            alaNtpStatsPeerCandidateOrder,
            alaNtpStatsPeerReset,
            alaNtpStatsPeerName,
            alaNtpStatsReset
        }
        STATUS  current
        DESCRIPTION
            "Collection of NTP peer information objects."
        ::= { alaIND1NtpMIBGroups 3 }

    alaNtpStatsStatGroup OBJECT-GROUP
        OBJECTS
        {
            alaNtpStatsStatUptime,
            alaNtpStatsStatReset,
            alaNtpStatsStatBadStratum,
            alaNtpStatsStatOldVersion,
            alaNtpStatsStatNewVersion,
            alaNtpStatsStatUnknownVersion,
            alaNtpStatsStatBadLength,
            alaNtpStatsStatProcessed,
            alaNtpStatsStatBadAuth,
            alaNtpStatsStatLimitRejects
        }
        STATUS  current
        DESCRIPTION
            "Collection of NTP statistic objects."
        ::= { alaIND1NtpMIBGroups 4 }

    alaNtpStatsLoopGroup OBJECT-GROUP
        OBJECTS
        {
            alaNtpStatsLoopOffset,
            alaNtpStatsLoopFrequency,
            alaNtpStatsLoopPollAdjust,
            alaNtpStatsLoopWatchdog
        }
        STATUS  current
        DESCRIPTION
            "Collection of NTP clocking objects."
        ::= { alaIND1NtpMIBGroups 5 }

    alaNtpStatsIoGroup OBJECT-GROUP
        OBJECTS
        {
            alaNtpStatsIoReset,
            alaNtpStatsIoRcvBuffers,
            alaNtpStatsIoFreeRcvBuffers,
            alaNtpStatsIoUsedRcvBuffers,
            alaNtpStatsIoRefills,
            alaNtpStatsIoDroppedPackets,
            alaNtpStatsIoIgnoredPackets,
            alaNtpStatsIoRcvPackets,
            alaNtpStatsIoSentPackets,
            alaNtpStatsIoNotSentPackets,
            alaNtpStatsIoInterrupts,
            alaNtpStatsIoInterruptsRcv
        }
        STATUS  current
        DESCRIPTION
            "Collection of NTP send and receive statistics objects."
        ::= { alaIND1NtpMIBGroups 6 }

    alaNtpAccessGroup OBJECT-GROUP
        OBJECTS
        {
            alaNtpAccessKeyIdTrust,
            alaNtpAccessRestrictedRestrictions,
            alaNtpAccessRestrictedCount,
            alaNtpAccessRestrictedRowStatus,
            alaNtpAccessRereadKeyFile
        }
        STATUS  current
        DESCRIPTION
            "Collection of NTP authentication control objects."
        ::= { alaIND1NtpMIBGroups 7 }

    alaNtpLocalInfoGroup OBJECT-GROUP
        OBJECTS
        {
            alaNtpInfoPeer,
            alaNtpInfoMode,
            alaNtpInfoLeapIndicator,
            alaNtpInfoStratum,
            alaNtpInfoPrecision,
            alaNtpInfoDistance,
            alaNtpInfoDispersion,
            alaNtpInfoReferenceId,
            alaNtpInfoReferenceTime,
            alaNtpInfoFrequency,
            alaNtpInfoStability,
            alaNtpInfoBroadcastDelay,
            alaNtpInfoAuthDelay
        }
        STATUS  current
        DESCRIPTION
            "Collection of NTP local clock information objects."
        ::= { alaIND1NtpMIBGroups 8 }

  alaNtpEventsGroup NOTIFICATION-GROUP
       NOTIFICATIONS
       {
           alaNtpMaxAssocTrap
       }
        STATUS  current
        DESCRIPTION
           "Notify the management entity on reaching the maximum allowable NTP client and peer associations."
       ::= { alaIND1NtpMIBGroups 9 }

  alaNtpSrcIpGroup OBJECT-GROUP
        OBJECTS
        {
	   alaNtpSrcIpConfig,
	   alaNtpSrcIp
	}
        STATUS  current
        DESCRIPTION
            "Collection of NTP source IP information objects."
        ::= { alaIND1NtpMIBGroups 10 }


-- new MIB objects to display the incoming client information

alaNtpClientListTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF NtpClientListEntry 
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION   "Used to display a brief list of all incoming NTP client associations
                  related to this switch."
    ::= {alaNtpInfo 4}

alaNtpClientListEntry OBJECT-TYPE
    SYNTAX        NtpClientListEntry 
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION   "Each entry corresponds to one association."
    INDEX   {  alaNtpClientListAddressType, alaNtpClientListAddress  }
    ::= {alaNtpClientListTable 1}

NtpClientListEntry ::= SEQUENCE {
    alaNtpClientListAddressType
       InetAddressType,
    alaNtpClientListAddress
       InetAddress,
    alaNtpClientListVersion
       Integer32,
    alaNtpClientKey
       Integer32
    }
alaNtpClientListAddressType OBJECT-TYPE
        SYNTAX        InetAddressType(1)
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   "The InetAddress type of the incoming client association.
                      InetAddressIPv4 (1) is the only type currently
                      supported."
        ::={ alaNtpClientListEntry 1 }

alaNtpClientListAddress OBJECT-TYPE
        SYNTAX        InetAddress
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION   "The InetAddress of the client."
        ::={ alaNtpClientListEntry 2 }

alaNtpClientListVersion OBJECT-TYPE
      SYNTAX        Integer32 (3..4) 
      MAX-ACCESS    read-only
      STATUS        current
      DESCRIPTION   "The NTP version used by the remote host for communication."
      DEFVAL		{ 4 }
      ::= { alaNtpClientListEntry 3 }
      
alaNtpClientKey OBJECT-TYPE
      SYNTAX        Integer32 (0..65535)
      MAX-ACCESS    read-only
      STATUS        current
      DESCRIPTION   "The authorization keyid for the remote host."
      DEFVAL		{ 0 }
      ::= { alaNtpClientListEntry 4 }

-- /* MIB changes for trap information */

-- --------------------------------------------------------------
-- NOTIFICATIONS (TRAPS)
-- These notifications will be sent to the management entity
-- Whenever the maximum number of NTP associations is reached.
-- --------------------------------------------------------------

alaNtpEvents OBJECT IDENTIFIER ::= { alcatelIND1NTPMIB 3 }
alaNtpEventsRoot OBJECT IDENTIFIER ::= { alaNtpEvents 0}

	alaNtpMaxAssocTrap NOTIFICATION-TYPE
	   OBJECTS { 
	       	alaNtpMaxAssociation
		   	}
	   STATUS   current
	   DESCRIPTION 
"Notify the management entity on reaching the maximum allowable NTP client and peer associations."
	    ::= { alaNtpEventsRoot 1 }

END

