CISCOSB-SYSMNG-MIB DEFINITIONS ::= BEGIN

-- Version:    7.50
-- Date:       31 Oct 2010
-- 31-Oct-2010 Added rlSysmngTcamAllocationsTable

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE,Counter32,
    Unsigned32                                  FROM SNMPv2-SMI
    TruthValue, RowStatus, RowPointer,
    TEXTUAL-CONVENTION,DisplayString            FROM SNMPv2-TC
    Counter64, OBJECT-TYPE                      FROM SNMPv2-SMI
    Percents,switch001                          FROM CISCOSB-MIB;


rlSysmngMib MODULE-IDENTITY
        LAST-UPDATED "201010310000Z"
		ORGANIZATION "Cisco Small Business"

		CONTACT-INFO
		"Postal: 170 West Tasman Drive
		San Jose , CA 95134-1706
		USA

		Website: Cisco Small Business Home http://www.cisco.com/smb>;,
		Cisco Small Business Support Community <http://www.cisco.com/go/smallbizsupport>"

        DESCRIPTION
             "The private MIB module definition for System Manager pool."
        REVISION "201010310000Z"
        DESCRIPTION
             "Initial revision."
        ::= { switch001 204 }

SysmngPoolType ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION
        "Supported TCAM pools."
    SYNTAX  INTEGER {
        router(1),
        iscsi(2),
        misc(3)           -- Miscellaneous pool - uses all TCAM entries that
                          --                      previous pools (Router/ISCSI)
                          --                      didn't reserved
}

-- System Manager Tcam Allocations Table

    rlSysmngTcamAllocations OBJECT IDENTIFIER
      ::= { rlSysmngMib 1 }

    rlSysmngTcamAllocationsTable OBJECT-TYPE
      SYNTAX         SEQUENCE OF RlSysmngTcamAllocationsEntry
      MAX-ACCESS     not-accessible
      STATUS         current
      DESCRIPTION
           "A table containing tcam allocations information.
           Each row represents objects for a defined profile."
      ::= { rlSysmngTcamAllocations 1 }

    rlSysmngTcamAllocationsEntry OBJECT-TYPE
      SYNTAX         RlSysmngTcamAllocationsEntry
      MAX-ACCESS     not-accessible
      STATUS         current
      DESCRIPTION
           "A Single entry containing tcam allocations information
            per predefined profile and specific pool."
      INDEX          { rlSysmngTcamAllocProfileName, rlSysmngTcamAllocPoolType }
      ::= { rlSysmngTcamAllocationsTable 1 }

    RlSysmngTcamAllocationsEntry ::= SEQUENCE {
      rlSysmngTcamAllocProfileName                          DisplayString,
      rlSysmngTcamAllocPoolType                             SysmngPoolType,

      rlSysmngTcamAllocMinRequiredEntries                   Unsigned32,
      rlSysmngTcamAllocStaticConfigEntries                  Unsigned32,
      rlSysmngTcamAllocInUseEntries                         Unsigned32,
      rlSysmngTcamAllocPoolSize                             Unsigned32
    }

     rlSysmngTcamAllocProfileName OBJECT-TYPE
      SYNTAX         DisplayString
      MAX-ACCESS     not-accessible
      STATUS         current
      DESCRIPTION
           "The profile name for tcam allocation.
            Must be unique per entry. This is an index into the table.
            'tcam0' profile contains policy tcam counters
            'tcam1' profile contains router tcam counters"
      ::= { rlSysmngTcamAllocationsEntry 1 }

    rlSysmngTcamAllocPoolType OBJECT-TYPE
      SYNTAX         SysmngPoolType
      MAX-ACCESS     not-accessible
      STATUS         current
      DESCRIPTION
           "Pool type.
            Must be unique per entry. This is an index into the table."
      ::= { rlSysmngTcamAllocationsEntry 2 }


   rlSysmngTcamAllocMinRequiredEntries OBJECT-TYPE
      SYNTAX         Unsigned32
      MAX-ACCESS     read-only
      STATUS         current
      DESCRIPTION
           "Number of minimal hardware entries, required by pool to operate."
      DEFVAL { 0 }
      ::= { rlSysmngTcamAllocationsEntry 3 }

    rlSysmngTcamAllocStaticConfigEntries OBJECT-TYPE
      SYNTAX         Unsigned32
      MAX-ACCESS     read-only
      STATUS         current
      DESCRIPTION
           "Number of hardware entries, in use by static configuration of the pool."
      DEFVAL { 0 }
      ::= { rlSysmngTcamAllocationsEntry 4 }

   rlSysmngTcamAllocInUseEntries OBJECT-TYPE
      SYNTAX         Unsigned32
      MAX-ACCESS     read-only
      STATUS         current
      DESCRIPTION
           "Total number of hardware entries, currently in use by the pool.
            This number includes minimum, static and dynamic entries."
      DEFVAL { 0 }
      ::= { rlSysmngTcamAllocationsEntry 5 }

   rlSysmngTcamAllocPoolSize OBJECT-TYPE
      SYNTAX         Unsigned32
      MAX-ACCESS     read-only
      STATUS         current
      DESCRIPTION
           "Total number of hardware entries reserved for the pool."
      DEFVAL { 0 }
      ::= { rlSysmngTcamAllocationsEntry 6 }


END
