-- SECTION 1: Top Level Definitions


SYNOPTICS-ETHERNET-MIB DEFINITIONS ::= BEGIN


-- Ethernet MIB Release 4.6.0
-- Revision 10/19/94

-- Copyright 1990-94 SynOptics Communications, Inc.
-- All rights reserved.
-- This SynOptics SNMP Management Information Base Specification
-- (Specification) embodies SynOptics' confidential and
-- proprietary intellectual property.  SynOptics retains all
-- title and ownership in the Specification, including any
-- revisions.

-- This Specification is supplied "AS IS," and SynOptics makes
-- no warranty, either express or implied, as to the use,
-- operation, condition, or performance of the Specification.


-- Imports

IMPORTS
	Counter, TimeTicks, Gauge, IpAddress
		FROM RFC1155-SMI
	DisplayString, PhysAddress
		FROM RFC1213-MIB
	OBJECT-TYPE
		FROM RFC-1212
	SnpxChassisType, SnpxBackplaneType
		FROM SYNOPTICS-ROOT-MIB
	s3000Ethernet, S3ModuleType
		FROM SYNOPTICS-COMMON-MIB;


-- Groups

s3000EnetConcentrator	OBJECT IDENTIFIER ::= { s3000Ethernet 1 }
s3000EnetBoard		OBJECT IDENTIFIER ::= { s3000Ethernet 2 }
s3000EnetLocBridge	OBJECT IDENTIFIER ::= { s3000EnetBoard 2 }
s3000EnetRemBridge	OBJECT IDENTIFIER ::= { s3000EnetBoard 3 }
s3000EnetRouter		OBJECT IDENTIFIER ::= { s3000EnetBoard 4 }
s3000EnetPort 		OBJECT IDENTIFIER ::= { s3000Ethernet 3 }
s3000EnetNmm		OBJECT IDENTIFIER ::= { s3000Ethernet 4 }
s3000EnetNode		OBJECT IDENTIFIER ::= { s3000Ethernet 5 }
s3000EnetTopology	OBJECT IDENTIFIER ::= { s3000Ethernet 6 }
s3000EnetNmmTopology	OBJECT IDENTIFIER ::= { s3000EnetTopology 1 }
s3000EnetBridTopology	OBJECT IDENTIFIER ::= { s3000EnetTopology 2 }
s3000EnetTopInfo	OBJECT IDENTIFIER ::= { s3000EnetTopology 3 }
s3000EnetThreshold	OBJECT IDENTIFIER ::= { s3000Ethernet 8 }
s3000EnetSADATraffic	OBJECT IDENTIFIER ::= { s3000Ethernet 9 }
s3000EnetPlusStatistics	OBJECT IDENTIFIER ::= { s3000Ethernet 10 }
s3000EnetPlusConc	OBJECT IDENTIFIER ::= { s3000EnetPlusStatistics 3 }
s3000EnetFrameSizeDist	OBJECT IDENTIFIER ::= { s3000Ethernet 11 }
s3000EnetFrameConc	OBJECT IDENTIFIER ::= { s3000EnetFrameSizeDist 3 }
s3000EnetProtoTypeDist	OBJECT IDENTIFIER ::= { s3000Ethernet 12 }
s3000EnetProtoConc	OBJECT IDENTIFIER ::= { s3000EnetProtoTypeDist 3 }
s3000EnetHosts		OBJECT IDENTIFIER ::= { s3000Ethernet 13 }

-- SECTION 2: Ethernet Status and Statistics Group

-- The Ethernet Status and Statistics group consists of Concentrator
--   Group, Board Table, Local Bridge Board Table, Local Bridge Port
--   Table, Remote Bridge Board Table, Remote Bridge Port Table, Router
--   Board Table, and Port Table.


-- Concentrator Group

-- Implementation of this group is mandatory for all
--   SynOptics Series 3000 Ethernet NMM agents

s3EnetConcRetimingStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		off(1),		-- retiming off
		on(2)		-- retiming on
		}
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"Does this concentrator have retiming turned on.
		Writing a 1 will turn off retiming and writing a
		2 will turn on retiming.  This will change the
		active state of retiming but will change the value
		in EEPROM only when agentWriteEeprom is set.The
		factory default of this state is on.

		Retiming cannot be disabled in the 2810 concentrator.
		The 2810 agent will implement this object as read-only."
	::= { s3000EnetConcentrator 1 }

s3EnetConcFrmsRxOk OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames that are successfully
		received by the concentrator.  This does not include
		frames received with a frame-too-long, runt, FCS, or
		alignment errors.

		This counter includes broadcast and multicast frames
		that are received."
	::= { s3000EnetConcentrator 2 }

s3EnetConcOctetsRxOk OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Contains a count of data and padding octets in frames
		that are successfully received by the concentrator.
		This does not include frames received with a
		frame-too-long, runt, FCS, or alignment errors.

		This counter includes octets in broadcast and multicast
		frames that are received.

		This counter does not include the octets in the
		CRC field. The octets in the address and length/type
		fields are counted."
	::= { s3000EnetConcentrator 3 }

s3EnetConcMcastFrmsRxOk OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames that are successfully
		received by the concentrator and are directed to an
		active non-broadcast group address.  This does not
		include frames received with a frame-too-long, runt,
		FCS, or alignment errors.

		Only frames that are for a multicast address that
		this interface is receiving are counted.  Broadcast
		packets are not included."
	::= { s3000EnetConcentrator 4 }

s3EnetConcBcastFrmsRxOk OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames that are successfully
		received by the concentrator and are directed to the
		broadcast group address.  This does not include frames
		received with a frame-too-long, runt, FCS, or
		alignment errors.

		Multicast packets are not included."
	::= { s3000EnetConcentrator 5 }

s3EnetConcColls OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of the collisions at the
		concentrator level.  For NMM+ this is a true counter.
		For other NMMs this is a summation of all the port
		level collision 'flags' for all ports."
	::= { s3000EnetConcentrator 6 }



-- MAC Receive Error Statistics

-- A hierarchical order has been established for those objects listed
--   below such that when multiple error conditions can be associated
--   with one frame, only one condition is counted.  This hierarchy,
--   in descending order is:

--	frame too long
--	runt frames
--	fragments
--	alignment error
--	frame check error


s3EnetConcTooLongErrors OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames that are received by
		the concentrator and exceed the maximum permitted
		frame size.  This counter is incremented when the
		frameTooLong error is detected."
	::= { s3000EnetConcentrator 7 }

s3EnetConcRuntErrors OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		concentrator that are less than the minimum permitted
		frame size and have a good FCS."
	::= { s3000EnetConcentrator 8 }

s3EnetConcFragErrors OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		concentrator that are less than the minimum permitted
		frame size and have a bad FCS or alignment error."
	::= { s3000EnetConcentrator 9 }

s3EnetConcAlignErrors OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		concentrator that are not an integral number of
		octets in length and do not pass the FCS check.
		This counter is incremented when the alignment
		Error status is detected."
	::= { s3000EnetConcentrator 10 }

s3EnetConcFcsErrors OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		concentrator that are an integral number of octets
		in length that do not pass the FCS check.  This
		counter is incremented when the frame Check Error
		status is detected."
	::= { s3000EnetConcentrator 11 }

s3EnetConcLateCollErrors OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a total concentrator count of the
		late collisions. For NMM+ this is a true counter.
		For other NMMs this is a summation of all the port
		level late collision 'flags' for all ports."
	::= { s3000EnetConcentrator 12 }

s3EnetConcSecureStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),
		concSecureOn(2),-- security active, controlled at conc level
		portCheckOn(3),	-- security controlled at port level
		slotCheckOn(4),	-- security controlled at board level
		concSecureOff(5)-- all concentrator security deactivated
		}
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"This s3EnetConcSecureStatus object indicates whether
		the security features (both allowed nodes and
		LattisSecure) for the concentrator are active or
		inactive.  If security is active, this object also
		indicates whether the allowed nodes feature is
		controlled at the concentrator, board, or port level.
		LattisSecure features are always controlled at the
		port level.  (See the Authorized Nodes tables for
		more information about how the allowed nodes and
		LattisSecure receive security features are
		configured.)

		If this object is set to concSecureOn(2), then the
		allowed nodes feature is controlled at the
		concentrator level and activated for every
		non-LattisSecure Ethernet port in the concentrator.
		If an authorized node violation occurs on any port,
		the action specified in s3EnetConcAuthAction is taken.

		If this object is set to portCheckOn(3), then allowed
		nodes is controlled at the port level by the
		s3EnetPortSecureStatus object for that port.  The
		port's s3EnetPortAuthAction determines the action
		taken when authorized nodes violations occur on that
		port.

		If this object is set to slotCheckOn(4), then allowed
		nodes is controlled at the board level by the
		s3EnetBoardSecureStatus object for that board.
		The board's s3EnetBoardAuthAction determines the
		action taken when authorized nodes violations
		occur on that board's ports.

		If this object is set to concentratorOff(5), then
		all security features, including LattisSecure, are
		deactivated for the entire concentrator.

		No matter what the status of this object, the board
		and port level SecureStatus and AuthAction are not
		lost even if they are not currently being used.  Thus,
		the user can change a port's status even if this object
		is slotCheckOn(4).  If this object is then changed to
		portCheckOn(3), then the change will take effect.

		The agent must support download of this object in the
		CFG file.

		In release 4.0, this object was called
		s3EnetConcAuthStatus."
	::= { s3000EnetConcentrator 13}

s3EnetConcAuthAction OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),
		noAction(2),	-- ignore auth violations
		sendTrap(3),	-- send trap to management station(s)
		partition(4),	-- partition the port with no time limit
		sendTrapPartition(5)-- do both sendTrap and partition
		}
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"If s3EnetConcSecureStatus is concSecureOn(2) and a
		violation occurs, then the action specified by this
		object will take place.  On a partition, only the
		port that the violation occurs on will be partitioned.

		This object does not apply to LattisSecure ports.

		The agent must support download of this object in
		the CFG file."
	::= { s3000EnetConcentrator 14 }

s3EnetConcSecurityLock OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),
		locked(2),
		notLocked(3)
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"If s3EnetConcSecurityLock is locked(2), the agent will
		refuse all requests to modify the 'security configuration'
		(defined below) by returning a BadValue return value.
		If s3EnetConcSecurityLock is notLocked(3), requests to
		modify security configuration will be handled in the
		usual manner.  SetRequests for objects not included
		in the security configuration are not affected by the
		state of this object.

		Objects that are part of the security configuration
		are s3EnetConcAuthStatus, s3EnetConcAuthAction,
		s3EnetBoardAuthStatus, s3EnetBoardAuthAction,
		s3EnetPortAuthStatus, s3EnetPortAuthAction,
		s3EnetPortAddrLearnMode, s3EnetPortTxSecurity,
		and all of the objects in the s3EnetAuthNodesTable."
	::= { s3000EnetConcentrator 15 }

s3EnetConcEnetChan OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),	-- unknown or other
		enetA(2),	-- Ethernet channel A
		enetB(3) 	-- Ethernet channel B
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Identifies the channel to which this NMM is
		currently monitoring."
	::= { s3000EnetConcentrator 16 }



-- Board Table


s3EnetBoardTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetBoardEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"A table of board-related objects.  The number of
		entries is given by the number of Ethernet host
		module and network management module boards that
		are contained in same backplane Ethernet segment
		as the reporting NMM."
	::= { s3000EnetBoard 1 }

s3EnetBoardEntry OBJECT-TYPE
	SYNTAX	S3EnetBoardEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"A table containing objects about Ethernet boards
		which are currently plugged into the 3000 chassis."
	INDEX	{ s3EnetBoardIndex }
	::= { s3EnetBoardTable 1 }

S3EnetBoardEntry ::= SEQUENCE {
	s3EnetBoardIndex
		INTEGER,
-- the bounded below are obsoleted
	s3EnetBoardType
		INTEGER,
	s3EnetBoardHwVer
		INTEGER,
	s3EnetBoardStatus
		INTEGER,
	s3EnetBoardReset
		INTEGER,
	s3EnetBoardPartStatus
		INTEGER,
	s3EnetBoardNmCntlStatus
		INTEGER,
	s3EnetBoardPsStatus
		INTEGER,
-- the bounded above are obsoleted
	s3EnetBoardFrmsRxOk
		Counter,
	s3EnetBoardOctetsRxOk
		Counter,
	s3EnetBoardMcastFrmsRxOk
		Counter,
	s3EnetBoardBcastFrmsRxOk
		Counter,
	s3EnetBoardColls
		Counter,
	s3EnetBoardTooLongErrors
		Counter,
	s3EnetBoardRuntErrors
		Counter,
	s3EnetBoardAlignErrors
		Counter,
	s3EnetBoardFcsErrors
		Counter,
	s3EnetBoardLateCollErrors
		Counter,
	s3EnetBoardAuthStatus
		INTEGER,
	s3EnetBoardAuthAction
		INTEGER,
	s3EnetBoardUpStamp
		TimeTicks
	}

 s3EnetBoardIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"A unique value for each board.  Its value ranges
		between 1 and 12.  The value for each board must
		remain constant at least from one re-initialization
		of the entity's network management system to the next
		re-initialization."
	::= { s3EnetBoardEntry 1 }

s3EnetBoardType OBJECT-TYPE
	SYNTAX	INTEGER {
		empty(1),	-- nothing installed
		other(2),	-- none of the following
		m3302(3),	-- Model 3302
		m3304-ST(4),	-- Model 3304-ST
		m3305(5),	-- Model 3305
		m3308(6),	-- Model 3308
		m3313(7),	-- Model 3313
		m3313M(8),	-- Model 3313M
		m3314-ST(9),	-- Model 3314
		m3314M-ST(10),	-- Model 3314M-ST
		m3323(11),	-- Model 3323
		m3324-ST(12),	-- Model 3324-ST
		m3301(16),	-- Model 3301
		m3307(17),	-- Model 3307
		m3356(18),	-- Model 3356
		m3383(24),	-- Model 3383
		m3384(25),	-- Model 3384
		m331x(26),	-- unknown 331x
		m3386(32),	-- Model 3386
		m3394(33),	-- Model 3394
		m3395(34),	-- Model 3395
		m3323S(35),	-- Model 3323S
		m3324S-ST(36),	-- Model 3324S-ST
		m3307A(37),	-- Model 3307A
		m3308A(38)	-- Model 3308A
		}
	ACCESS	read-only
	STATUS	obsolete
	DESCRIPTION
		"See s3SlotModuleType"
	::= { s3EnetBoardEntry 2 }

s3EnetBoardHwVer OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	obsolete
	DESCRIPTION
		"See s3CommonBoardHwVer"
	::= { s3EnetBoardEntry 3 }

s3EnetBoardStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		ok(1),		-- good status
		fail(2)		-- bad status
		}
	ACCESS	read-only
	STATUS	obsolete
	DESCRIPTION
		"See s3CommonBoardStatus"
	::= { s3EnetBoardEntry 4 }

s3EnetBoardReset OBJECT-TYPE
	SYNTAX	INTEGER {
		noReset(1),	-- not resetting
		reset(2)	-- resetting
		}
	ACCESS	read-write
	STATUS	obsolete
	DESCRIPTION
		"See s3CommonBoardReset"
	::= { s3EnetBoardEntry 5 }

s3EnetBoardPartStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		enabled(1),	-- board enabled
		partition(2)	-- board partitioned
		}
	ACCESS	read-write
	STATUS	obsolete
	DESCRIPTION
		"See s3CommonBoardPartStatus"
	::= { s3EnetBoardEntry 6 }

s3EnetBoardNmCntlStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		notNmControl(1),-- board not under NM control
		nmControl(2)	-- board under NM control
		}
	ACCESS	read-only
	STATUS	obsolete
	DESCRIPTION
		"See s3CommonBoardCntlStatus"
	::= { s3EnetBoardEntry 7 }

s3EnetBoardPsStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		ok(1),		-- good status
		fail(2)		-- bad status
		}
	ACCESS	read-only
	STATUS	obsolete
	DESCRIPTION
		"See s3CommonBoardPsStatus"
	::= { s3EnetBoardEntry 8 }

s3EnetBoardFrmsRxOk OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames that are successfully
		received by the board.  This does not include frames
		received with a frame-too-long, runt, FCS, or alignment
		errors.

		This counter includes broadcast and multicast frames
		that are received."
	::= { s3EnetBoardEntry 9 }

s3EnetBoardOctetsRxOk OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Contains a count of data and padding octets in frames
		that are successfully received by the board.  This does
		not include frames received with a frame-too-long, runt,
		FCS, or alignment errors.

		This counter includes octets in broadcast and multicast
		frames that are received.

		This counter does not include the octets in the
		CRC field. The octets in the address and length/type
		fields are counted."
	::= { s3EnetBoardEntry 10 }

s3EnetBoardMcastFrmsRxOk OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames that are successfully
		received by the board and are directed to an active
		non-broadcast group address.  This does not include
		frames received with a frame-too-long, runt, FCS, or
		alignment errors.

		Only frames that are for a multicast address that
		this interface is receiving are counted. Broadcast
		packets are not included."
	::= { s3EnetBoardEntry 11 }

s3EnetBoardBcastFrmsRxOk OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames that are successfully
		received by the board and are directed to the broadcast
		group address.  This does not include frames received
		with a frame-too-long, runt, FCS, or alignment errors.
		Multicast packets are not included."
	::= { s3EnetBoardEntry 12 }

s3EnetBoardColls OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a board level count of collisions.
		For NMM+ this is a true counter.  For other NMMs
		this is a summation of all the port level collision
		'flags' for this board."
	::= { s3EnetBoardEntry 13 }



-- MAC Receive Error Statistics

-- A hierarchical order has been established for those objects listed
--   below such that when multiple error condition can be associated
--   with one frame, only one condition is counted.  This hierarchy,
--   in descending order is:

--	frame Too Long
--	runt frames
--	alignment Error
--	frame Check Error


s3EnetBoardTooLongErrors OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames that are received by
		the board and exceed the maximum permitted frame size.
		This counter is incremented when the frameTooLong
		error is detected."
	::= { s3EnetBoardEntry 14 }

s3EnetBoardRuntErrors OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the board
		that are less than the minimum permitted frame size and
		have a good FCS."
	::= { s3EnetBoardEntry 15 }

s3EnetBoardAlignErrors OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the board
		that are not an integral number of octets in length and
		do not pass the FCS check.  This counter is incremented
		when the alignmentError status is detected."
	::= { s3EnetBoardEntry 16 }

s3EnetBoardFcsErrors OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the board
		that are an integral number of octets in length that
		do not pass the FCS check.  This counter is incremented
		when the frameCheckError status is detected."
	::= { s3EnetBoardEntry 17 }

s3EnetBoardLateCollErrors OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of the board level late collisions.
		For NMM+ this is a true counter.  For other NMMs this is a
		summation of all the port level late collision 'flags' for
		this board."
	::= { s3EnetBoardEntry 18 }

s3EnetBoardAuthStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),
		on(2),		-- allowed nodes activated on this board
		off(3)		-- allowed nodes deactivated on this board
		}
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"This object is only used if s3EnetConcSecureStatus is
		set to slotCheckOn(4).  In this case, turning this object
		on(2) means that any node that is heard on this board
		which is not allowed on this board (i.e., not in AuthNode
		table with the slotIndex equal to this board or 0 for all
		boards) will cause the action specified in
		s3EnetBoardAuthAction to take place.

		If s3EnetConcSecureStatus is set to slotCheckOn(4) but
		this object is set to off(3), then the authorized nodes
		feature for this board is deactivated.

		If s3EnetConcSecureStatus is not set to slotCheckOn(4),
		then this object will not be used but will maintain
		its settings unless explicitly changed.

		This object does not affect the configuration or
		functioning of security features on LattisSecure
		Host Modules."
	::= { s3EnetBoardEntry 19 }

s3EnetBoardAuthAction OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),
		noAction(2),	-- ignore auth violations
		sendTrap(3),	-- send trap to management station(s)
		partition(4),	-- partition the port with no time limit
		sendTrapPartition(5)-- do both sendTrap and partition
		}
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"If s3EnetConcSecureStatus is slotCheckOn(4) and
		s3EnetBoardAuthStatus is on(2) and an authorized nodes
		violation occurs on the board, then the action specified
		by this object will take place.  On a partition, only the
		port that the violation occurs on will be partitioned.

		This object does not apply to LattisSecure ports."
	::= { s3EnetBoardEntry 20 }

s3EnetBoardUpStamp OBJECT-TYPE
	SYNTAX	TimeTicks
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The time ( in hundredths of a second) that the board
		was first seen as a member of this NMM's segment."
	::= {s3EnetBoardEntry 21 }



-- Local Bridge Board Table


s3EnetLocBridgeSlotTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetLocBridgeEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"A table of Local Bridge Board entries.  The number of
		entries is determined by  the Concentrator Slot
		Configuration Table.  Only those entries that are
		Ethernet local bridges will have entries in this list."
	::= { s3000EnetLocBridge 1 }

s3EnetLocBridgeEntry OBJECT-TYPE
	SYNTAX	S3EnetLocBridgeEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"A table containing objects about Boards which are
		local bridges that are currently plugged into the
		3000 chassis."
	INDEX	{ s3EnetLocBridgeIndex }
	::= { s3EnetLocBridgeSlotTable 1 }

S3EnetLocBridgeEntry ::= SEQUENCE {
	s3EnetLocBridgeIndex
		INTEGER,
	s3EnetLocBridgeDescr
		DisplayString,
	s3EnetLocBridgePortCount
		INTEGER,
	s3EnetLocBridgeDiagSts
		OCTET STRING,
	s3EnetLocBridgeBootSts
		INTEGER,
	s3EnetLocBridgeStandbySts
		INTEGER
	}

s3EnetLocBridgeIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"A unique value for each board.  Its value ranges between
		1 and 12.  The value for each board must remain constant
		at least from one re-initialization of the entity's
		network management system to the next re-initialization."
	::= { s3EnetLocBridgeEntry 1 }

s3EnetLocBridgeDescr OBJECT-TYPE
	SYNTAX	DisplayString (SIZE(0..128))
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Description of the local bridge board."
	::= { s3EnetLocBridgeEntry 2 }

s3EnetLocBridgePortCount OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Number of ports that are on the local bridge board."
	::= { s3EnetLocBridgeEntry 3 }

s3EnetLocBridgeDiagSts OBJECT-TYPE
	SYNTAX	OCTET STRING (SIZE(4))
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Latest Diagnostic LED Status that has been recorded."
	::= { s3EnetLocBridgeEntry 4 }

s3EnetLocBridgeBootSts OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),	-- unknown booting status
		reqstToBoot(2),	-- board is requesting to boot
		notReqstToBoot(3)-- board is not requesting to boot
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The current status of the board as it relates
		to rebooting."
	::= { s3EnetLocBridgeEntry 5 }

s3EnetLocBridgeStandbySts OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),	-- unknown booting status
		standby(2), 	-- bridge is in standby mode
		notStandby(3)	-- bridge is operational and not standby
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This status says whether the local bridge is active
		or in standby mode."
	::= { s3EnetLocBridgeEntry 6 }



-- Local Bridge Port Table


s3EnetLocBridgePortTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetLocBridgePortEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"A table of Port entries that are part of a local
		bridge.  The number of entries is determined by knowing
		the number of local bridge boards that are installed
		by looking at s3ChassisSlotConfigTable and by knowing
		how many ports are on a local bridge board by looking at
		s3EnetLocBridgePortCount."
	::= { s3000EnetLocBridge 2 }

s3EnetLocBridgePortEntry OBJECT-TYPE
	SYNTAX	S3EnetLocBridgePortEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"A table containing objects about the ports of the
		local bridges that are currently plugged into the
		3000 chassis."
	INDEX	{ s3EnetLocBridgePortSlotIndex, s3EnetLocBridgePortIndex }
	::= { s3EnetLocBridgePortTable 1 }

S3EnetLocBridgePortEntry ::= SEQUENCE {
	s3EnetLocBridgePortSlotIndex
		INTEGER,
	s3EnetLocBridgePortIndex
		INTEGER,
	s3EnetLocBridgePortMdaId
		INTEGER,
	s3EnetLocBridgePortIf
		INTEGER,
	s3EnetLocBridgePortDescr
		DisplayString,
	s3EnetLocBridgePortOpSts
		INTEGER
	}

s3EnetLocBridgePortSlotIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"A unique value for each board.  Its value ranges
		between 1 and 12.  The value for each board must
		remain constant at least from one re-initialization
		of the entity's network management system to the
		next re-initialization."
	::= { s3EnetLocBridgePortEntry 1 }

s3EnetLocBridgePortIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"A unique value for each port.  Its value ranges
		between 1 and 12.  The value for each port must
		remain constant at least from one re-initialization
		of the entity's network management system to the
		next re-initialization."
	::= { s3EnetLocBridgePortEntry 2 }

s3EnetLocBridgePortMdaId OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Medium dependent ID for the port. See s3SlotModuleMdaId
		in the SynOptics Common MIB."
	::= { s3EnetLocBridgePortEntry 3 }

s3EnetLocBridgePortIf OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),	-- unknown interfaces
		etherEther(2),	-- ethernet to ethernet bridge
		etherTokenRing(3)-- ethernet to token ring bridge
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Bridge interface types."
	::= { s3EnetLocBridgePortEntry 4 }

s3EnetLocBridgePortDescr OBJECT-TYPE
	SYNTAX	DisplayString (SIZE(0..128))
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"A text description of the port."
	::= { s3EnetLocBridgePortEntry 5 }

s3EnetLocBridgePortOpSts OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),
		standby(2),
		notStandby(3)
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Operating status of the port."
	::= { s3EnetLocBridgePortEntry 6 }



-- Remote Bridge Board Table


s3EnetRemBridgeSlotTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetRemBridgeEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"A table of Remote Bridge Board entries.  The number
		of entries is determined by the Concentrator Slot
		Configuration Table.  Only those entries that are
		Ethernet remote bridges will have entries in this list."
	::= { s3000EnetRemBridge 1 }

s3EnetRemBridgeEntry OBJECT-TYPE
	SYNTAX	S3EnetRemBridgeEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"A table containing objects about Boards which are
		remote bridges that are currently plugged into the
		3000 chassis."
	INDEX	{ s3EnetRemBridgeIndex }
	::= { s3EnetRemBridgeSlotTable 1 }

S3EnetRemBridgeEntry ::= SEQUENCE {
	s3EnetRemBridgeIndex
		INTEGER,
	s3EnetRemBridgeDescr
		DisplayString ,
	s3EnetRemBridgePortCount
		INTEGER,
	s3EnetRemBridgeDiagSts
		OCTET STRING,
	s3EnetRemBridgeBootSts
		INTEGER,
	s3EnetRemBridgeStandbySts
		INTEGER
	}

s3EnetRemBridgeIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"A unique value for each board.  Its value ranges
		between 1 and 12.  The value for each board must
		remain constant at least from one re-initialization
		of the entity's network management system to the
		next re-initialization."
	::= { s3EnetRemBridgeEntry 1 }

s3EnetRemBridgeDescr OBJECT-TYPE
	SYNTAX	DisplayString (SIZE(0..128))
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Description of the board."
	::= { s3EnetRemBridgeEntry 2 }

s3EnetRemBridgePortCount OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Number of ports that are on the board."
	::= { s3EnetRemBridgeEntry 3 }

s3EnetRemBridgeDiagSts OBJECT-TYPE
	SYNTAX	OCTET STRING (SIZE(4))
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Latest Diagnostic LED Status that has been recorded."
	::= { s3EnetRemBridgeEntry 4 }

s3EnetRemBridgeBootSts OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),	-- unknown booting status
		reqstToBoot(2),	-- board is requesting to boot
		notReqstToBoot(3)-- board is not requesting to boot
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The current status of the board as it relates to rebooting."
	::= { s3EnetRemBridgeEntry 5 }

s3EnetRemBridgeStandbySts OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),	-- unknown booting status
		standby(2),	-- remote bridge is in standby mode
		notStandby(3)	-- remote bridge is active not in standby
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This status says whether the remote bridge is active
		or in standby mode."
	::= { s3EnetRemBridgeEntry 6 }



-- Remote Bridge Port Table


s3EnetRemBridgePortTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetRemBridgePortEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"A table of Port entries that are part of a remote
		bridge.  The number of entries is determined by
		knowing the number of remote bridge boards that are
		installed by looking at s3ChassisSlotConfigTable and
		by knowing how many ports are on a remote bridge
		board by looking at s3EnetRemBridgePortCount."
	::= { s3000EnetRemBridge 2 }

s3EnetRemBridgePortEntry OBJECT-TYPE
	SYNTAX	S3EnetRemBridgePortEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"A table containing objects about the ports of the
		remote bridges that are currently plugged into the
		3000 chassis."
	INDEX	{ s3EnetRemBridgePortSlotIndex,
		 s3EnetRemBridgePortIndex }
	::= { s3EnetRemBridgePortTable 1 }

S3EnetRemBridgePortEntry ::= SEQUENCE {
	s3EnetRemBridgePortSlotIndex
		INTEGER,
	s3EnetRemBridgePortIndex
		INTEGER,
	s3EnetRemBridgePortMdaId
		INTEGER,
	s3EnetRemBridgePortDescr
		DisplayString,
	s3EnetRemBridgePortOpSts
		INTEGER,
	s3EnetRemBridgePortRdySnd
		INTEGER,
	s3EnetRemBridgePortClrSnd
		INTEGER,
	s3EnetRemBridgePortCarDt
		INTEGER
	}

s3EnetRemBridgePortSlotIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"A unique value for each board.  Its value ranges
		between 1 and 12.  The value for each board must
		remain constant at least from one re-initialization
		of the entity's network management system to the
		next re-initialization."
	::= { s3EnetRemBridgePortEntry 1 }

s3EnetRemBridgePortIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"A unique value for each port.  Its value ranges
		between 1 and 12.  The value for each port must
		remain constant at least from one re-initialization
		of the entity's network management system to the next
		re-initialization."
	::= { s3EnetRemBridgePortEntry 2 }

s3EnetRemBridgePortMdaId OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),
		ethernet(2),
		x21Barrier(3),
		x21Unbarrier(4),
		rs232(5),
		rs449(6),
		v35(7),
		g703(8),
		t1(9)
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Medium dependent ID for the port."
	::= { s3EnetRemBridgePortEntry 3 }

s3EnetRemBridgePortDescr OBJECT-TYPE
	SYNTAX	DisplayString (SIZE(0..128))
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"A text description of the port."
	::= { s3EnetRemBridgePortEntry 4 }

s3EnetRemBridgePortOpSts OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),
		standby(2),
		operational(3),
		noLink(4)
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Operating status of the port."
	::= { s3EnetRemBridgePortEntry 5 }

s3EnetRemBridgePortRdySnd OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),	-- unknown status
		rdySnd(2),	-- ready to send
		notRdySnd(3)	-- not ready to send
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Ready to send status of the port."
	::= { s3EnetRemBridgePortEntry 6 }

s3EnetRemBridgePortClrSnd OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),	-- unknown status
		clrSnd(2),	-- clear to send
		notClrSnd(3)	-- not clear to send
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Clear to send status of the port."
	::= { s3EnetRemBridgePortEntry 7 }

s3EnetRemBridgePortCarDt OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),	-- unknown status
		carDt(2),	-- carrier detected
		noCarDt(3)	-- no carrier detected
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Carrier detect status of the port."
	::= { s3EnetRemBridgePortEntry 8 }



-- Router Board Table


s3EnetRouterSlotTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetRouterEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"A table of Router Board entries.  The number of
		entries is determined by  the Concentrator Slot
		Configuration Table.  Only those entries that
		are Ethernet routers will have entries in this list."
	::= { s3000EnetRouter 1 }

s3EnetRouterEntry OBJECT-TYPE
	SYNTAX	S3EnetRouterEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"A table containing objects about Boards which
		are routers that are currently plugged into the
		3000 chassis."
	INDEX	{ s3EnetRouterIndex }
	::= { s3EnetRouterSlotTable 1 }

S3EnetRouterEntry ::= SEQUENCE {
	s3EnetRouterIndex
		INTEGER,
	s3EnetRouterDescr
		DisplayString,
	s3EnetRouterDiagSts
		OCTET STRING,
	s3EnetRouterStandbySts
		INTEGER
	}

s3EnetRouterIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"A unique value for each board.  Its value ranges
		between 1 and 12.  The value for each board must
		remain constant at least from one re-initialization
		of the entity's network management system to the
		next re-initialization."
	::= { s3EnetRouterEntry 1 }

s3EnetRouterDescr OBJECT-TYPE
	SYNTAX	DisplayString (SIZE(0..128))
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Description of the router board."
	::= { s3EnetRouterEntry 2 }

s3EnetRouterDiagSts OBJECT-TYPE
	SYNTAX	OCTET STRING (SIZE(4))
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Latest Diagnostic LED Status that has been recorded."
	::= { s3EnetRouterEntry 3 }

s3EnetRouterStandbySts OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),	-- unknown booting status
		standby(2),	-- router is in standby mode
		notStandby(3)	-- router is operational, not in standby
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This status says whether the router is active or in
		standby mode."
	::= { s3EnetRouterEntry 4 }



-- Common Board Table

s3EnetCommonBoardTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetCommonBoardEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"Information maintained for each Ethernet board.  The
		information can be retrieved for any Ethernet board,
		even if the board is not on the same backplane Ethernet
		segment as this NMM.

		The instance is the slot number of the concentrator
		that the board occupies."
	::= { s3000EnetBoard 5 }

s3EnetCommonBoardEntry OBJECT-TYPE
	SYNTAX	S3EnetCommonBoardEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"There is one entry per Ethernet board in this table."
	INDEX	{ s3EnetCommonBoardIndex }
	::= { s3EnetCommonBoardTable 1 }

S3EnetCommonBoardEntry ::= SEQUENCE {
	s3EnetCommonBoardIndex
		INTEGER,
	s3EnetCommonBoardEnetAB
		INTEGER,
	s3EnetCommonBoardChanSwitch
		INTEGER,
	s3EnetCommonBoardRedund
		INTEGER
	}

s3EnetCommonBoardIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"A unique value for each board.  Its value ranges
		between 1 and 12. The value for each board must
		remain constant at least from one re-initialization
		of the entity's network management system to the
		next re-initialization."
	::= { s3EnetCommonBoardEntry 1 }

s3EnetCommonBoardEnetAB OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),	 -- unknown or other
		enetA(2),	 -- Ethernet channel A
		enetB(3),	 -- Ethernet channel B
		enetAandEnetB(4) -- Both Ethernet channels A and B
		}
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"The channel to which the board is connected.  The
		primary use of this object is for providing realtime
		switching of boards between channel A and channel B.
		It is also returned in the enetChannelChange trap, in
		which case it indicates a board is switched from one
		channel to the other.  The write capability of this
		object can only apply to those modules with channel
		switching function.  Any attempt to write this object
		for a non-switchable board, the agent will return
		badValue."
	::= { s3EnetCommonBoardEntry 2 }

s3EnetCommonBoardChanSwitch OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),
		switchCapable(2),
		notSwitchCapable(3)
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The agent will return switchCapable(2) for any
		Ethernet host board which can be switched between
		Ethernet channels.  The value notSwitchCapable(3)
		indicates that the Ethernet board can not be switched
		to another channel."
	::= { s3EnetCommonBoardEntry 3 }


s3EnetCommonBoardRedund OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),
		redundCapable(2),
		notRedundCapable(3)
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The agent will return redundCapable(2) for any Ethernet
		host board which can provide hardware and/or software
		controlled redundancy on the port level.  The value
		notRedundCapable(3) indicates that the Ethernet board
		can not support port redundancy."
	::= { s3EnetCommonBoardEntry 4 }


-- Port Table


s3EnetPortTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetPortEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"A list of port entries.  The number of entries is
		given by learning the type of board from the
		information in the s3ChassisSlotConfigTable."
	::= { s3000EnetPort 1 }

s3EnetPortEntry OBJECT-TYPE
	SYNTAX	S3EnetPortEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"A table containing objects about the Ports of
		each board plugged into the 3000 chassis which
		are on the same backplane Ethernet segment as
		the reporting NMM."
	INDEX	{ s3EnetPortBoardIndex, s3EnetPortIndex }
	::= { s3EnetPortTable 1 }

S3EnetPortEntry ::= SEQUENCE {
	s3EnetPortBoardIndex
		INTEGER,
	s3EnetPortIndex
		INTEGER,
	s3EnetPortLinkStatus
		INTEGER,
	s3EnetPortPartStatus
		INTEGER,
	s3EnetPortJabberStatus
		INTEGER,
	s3EnetPortFrmsRxOk
		Counter,
	s3EnetPortOctetsRxOk
		Counter,
	s3EnetPortMcastFrmsRxOk
		Counter,
	s3EnetPortBcastFrmsRxOk
		Counter,
	s3EnetPortColls
		Counter,
	s3EnetPortTooLongErrors
		Counter,
	s3EnetPortRuntErrors
		Counter,
	s3EnetPortAlignErrors
		Counter,
	s3EnetPortFcsErrors
		Counter,
	s3EnetPortLateCollErrors
		Counter,
	s3EnetPortAuthStatus
		INTEGER,
	s3EnetPortAuthAction
		INTEGER,
	s3EnetPortPartTime
		TimeTicks,
	s3EnetPortType
		INTEGER,
	s3EnetPortInterconStatus
		INTEGER,
	s3EnetPortAddrCollect
		INTEGER,
	s3EnetPortAddrLearnMode
		INTEGER,
	s3EnetPortTxSecurity
		INTEGER
	}

s3EnetPortBoardIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"A unique value for each board.  Its value ranges
		between 1 and 12.  The value for each board must
		remain constant at least from one reinitialization
		of the entity's network management system to the
		next reinitialization."
	::= { s3EnetPortEntry 1 }

s3EnetPortIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"A unique value for each port.  Its value is dependent
		on the board type.  The value for each port must
		remain constant at least from one re-initialization
		of the entity's network management system to the
		next re-initialization."
	::= { s3EnetPortEntry 2 }

s3EnetPortLinkStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		off(1),			-- link is not connected
		on(2),			-- link is connected
		other(3)		-- returned for AUI
		}
	ACCESS	read-only
	STATUS	deprecated
	DESCRIPTION
		"Tells whether the port is receiving link status."
	::= { s3EnetPortEntry 3 }

s3EnetPortPartStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		enabled(1),		-- port enabled
		partition(2),		-- port partitioned
		autoPartition(3),	-- port auto-partitioned
		timedPartition(4),	-- timed partition
		latSecPartition(5)	-- port partitioned by LattisSecure
		}
	ACCESS	read-write
	STATUS	deprecated
	DESCRIPTION
		"This indicates the operational status of the Port.
		Writing a partition(2) will partition the port
		indefinitely and enabled(1) will enable the port.

		If a timed partition is desired, then writing
		timedPartition(4) to this object at the same time
		that a time value is supplied in s3EnetPortPartTime
		is required. Timed partitions will not survive across
		a reset. In this case the port will go to the
		partition(2) state.

		The value latSecPartition(5) is returned when the port
		has been automatically partitioned by the LattisSecure
		Host Module because of a security violation.  The value
		autoPartition(3) is returned when the port has been
		automatically partitioned by the repeater using the
		802.3 repeater auto-partition function.

		The agent will not allow this object to be set to
		autoPartition(3) or latSecPartition(5) using an
		SNMP request."
	::= { s3EnetPortEntry 4 }

s3EnetPortJabberStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		ok(1),	
		jabbering(2)		-- Port receiving jabber
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Tells whether the DTE connected to the Port is
		jabbering or not."
	::= { s3EnetPortEntry 5 }

s3EnetPortFrmsRxOk OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames that are successfully
		received by the port.  This does not include frames
		received with a frame-too-long, runt, FCS, or alignment
		errors.  This counter includes broadcast and multicast
		frames that are received."
	::= { s3EnetPortEntry 6 }

s3EnetPortOctetsRxOk OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Contains a count of data and padding octets in frames
		that are successfully received by the port.  This does
		not include frames received with a frame-too-long, runt,
		FCS, or alignment errors.

		This counter includes octets in broadcast and multicast
		frames that are received.

		This counter does not include the octets in the
		CRC field. The octets in the address and length/type
		fields are counted."
	::= { s3EnetPortEntry 7 }

s3EnetPortMcastFrmsRxOk OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames that are successfully
		received by the port and are directed to an active
		non-broadcast group address.  This does not include
		frames received with a frame-too-long, runt, FCS, or
		alignment errors.

		Only frames that are for a multicast address that this
		interface is receiving are counted. Broadcast packets
		are not included."
	::= { s3EnetPortEntry 8 }

s3EnetPortBcastFrmsRxOk OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames that are successfully
		received by the port and are directed to the broadcast
		group address.  This does not include frames received
		with a frame-too-long, runt, FCS, or alignment errors.

		Multicast packets are not included."
	::= { s3EnetPortEntry 9 }

s3EnetPortColls OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of collisions. For NMM+ this is a
		true counter.  For other NMMs this is a count of the
		collision flags."
	::= { s3EnetPortEntry 10 }



-- Port MAC Error Statistics

-- A hierarchical order has been established for those objects listed
--   below such that when multiple error conditions can be associated
--   with one frame, only one condition is counted.  This hierarchy,
--   in descending order is:

--	frame too long
--	runt frames
--	alignment error
--	frame check error


s3EnetPortTooLongErrors OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames that are received by
		the port and exceed the maximum permitted frame size.
		This counter is incremented when the frameTooLong
		error is detected."
	::= { s3EnetPortEntry 11 }

s3EnetPortRuntErrors OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the port
		that are less than the minimum permitted frame size and
		have a good FCS."
	::= { s3EnetPortEntry 12 }

s3EnetPortAlignErrors OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the port
		that are not an integral number of octets in length and
		do not pass the FCS check.  This counter is incremented
		when the alignmentError status is detected."
	::= { s3EnetPortEntry 13 }

s3EnetPortFcsErrors OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received the port
		that are an integral number of octets in length that
		do not pass the FCS check.  This counter is incremented
		when the frameCheckError status is detected."
	::= { s3EnetPortEntry 14 }

s3EnetPortLateCollErrors OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of late collisions. For NMM+
		this is a true counter.  For other NMMs this is a count
		of the late collision flags."
	::= { s3EnetPortEntry 15 }

s3EnetPortAuthStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),
		on(2),		-- auth checking activated on this port
		off(3)		-- auth checking deactivated on this port
		}
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"This object is only used if s3EnetConcSecureStatus
		is set to portCheckOn(3) or if the port is on a
		LattisSecure Host Module.

		In this case, turning this object on(2) means that
		any node that heard on this port which is not allowed
		on this port will cause the action specified in
		s3EnetPortAuthAction to take place.

		This object does not affect the LattisSecure transmit
		security feature for the port.  It is incompatible with
		LattisSecure continuous learning mode.  If the value of
		s3EnetPortAddrLearnMode for a LattisSecure port is
		continuousLearn(3), turning this object to on(2) for
		that port will not have any affect.

		If s3EnetConcSecureStatus is set to portCheckOn(3) but
		this object is set to off(3), then all authorized nodes
		or LattisSecure receive security features for this port
		are deactivated.

		If s3EnetConcSecureStatus is not set to portCheckOn(3),
		then this object will not be used for allowed nodes,
		but will be used for LattisSecure."
	::= { s3EnetPortEntry 16 }

s3EnetPortAuthAction OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),
		noAction(2),	-- ignore auth violations
		sendTrap(3),	-- send trap to management station(s)
		partition(4),	-- partition the port with no time limit
		sendTrapPartition(5)-- do both sendTrap and partition
		}
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"If s3EnetConcSecureStatus is portCheckOn(3) or this
		port is on a LattisSecure Host Module, and
		s3EnetPortAuthStatus is on(2) and an authorized nodes
		violation occurs on this port, then the action specified
		by this object will take place on this port.

		If the port is a LattisSecure port, the authorized
		nodes security will be implemented by the LattisSecure
		Host Module."
	::= { s3EnetPortEntry 17 }

s3EnetPortPartTime OBJECT-TYPE
	SYNTAX	TimeTicks
	ACCESS	read-write
	STATUS	deprecated
	DESCRIPTION
		"When partitioning the port for a specified time,
		s3EnetPortPartStatus must be set with timedpartition(4)
		and this object must be supplied with the duration
		value.  If a PDU sets s3EnetPortPartStatus and not
		this object, the port will not be partitioned."
	::= { s3EnetPortEntry 18}

s3EnetPortType OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),		-- unknown or other
		tenBaseT(2),		-- 10BASE-T, "normal" or MDI-X
		tenBaseTMdi(3),		-- 10BASE-T, switched to MDI
		aui(4),			-- AUI (10Base5 to coax)
		bnc(5),			-- BNC (10Base2 to thinnet)
		foirl(6),		-- FOIRL
		tenBaseFL(7),		-- 10BASE-FL
		switch(8),		-- Switch, MDI-X
		switchMdi(9),		--  Switch, MDI
		tenBaseFLRedund(10)	-- 10BASE-FL, redundancy
		}
	ACCESS	read-only
	STATUS	deprecated
	DESCRIPTION
		"The media connection type for this port.

		Note that this object was called s3EnetPortMDIXSwitch
		in the Ethernet 3.3 and 4.0 MIBs."
	::= { s3EnetPortEntry 19 }

s3EnetPortInterconStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),	-- unknown or host
		interconnect(2)	-- identified as interconnect port
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This object tells whether the port is connected to a
		host or to an interconnect (defined to be another NMM
		that is sending hello messages).

		The NMM agent will assign this object the value other(1)
		on initialization.  If it sees hello messages coming in
		on the port, it will change the InterconStatus to be
		interconnect(2)."
	::= { s3EnetPortEntry 20 }

s3EnetPortAddrCollect OBJECT-TYPE
	SYNTAX	INTEGER {
		default(1),	-- follow default rules for
				--   address collection
		neverCollect(2),-- don't collect addrs,
				--   whatever intercon status
		alwaysCollect(3)-- do collect address, regardless
				--   of config
		}
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"This object tells whether the NMM should collect
		node address information from this port for the Find
		Nodes, Show Nodes, and Traffic Matrix (NMM+ only)
		tables.

		By default, the node addresses are collected only
		from ports that are not identified as interconnect
		ports.  In addition, allowed nodes checking is
		done only on ports that are not interconnect ports.
		This object provides a means of overriding the default
		for collection and checking of node addresses.

		Setting this variable to default(1) tells the NMM to
		collect and check addresses if and only the port has
		not been identified as an interconnect port.

		To disable node address collection and checking on a
		port, set this object to neverCollect(2).

		To collect and check node addresses for an interconnect
		port, set this object to alwaysCollect(3).

		This object and its default setting has no affect
		on LattisSecure receive or transmit security features.

		To restore the 'natural' value for the port, set this
		object to default(1)."
	::= { s3EnetPortEntry 21 }


s3EnetPortAddrLearnMode OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),	-- unknown or not LattisSecure port
		noAutoLearn(2),	-- auto learn off
		continuousLearn(3),-- continuously pick up new addresses
		oneShotLearn(4)	-- learn one address then quit learning
		}
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"This object indicates whether the port should
		automatically learn the port address by reading the
		source address on the incoming packets.  This object
		applies only to ports on a LattisSecure Host Module.
		For other ports, the agent  returns the value other.

		A Get will return the current learning mode of the port.

		Setting to noAutoLearn(2) can be used to turn off
		continuousLearn (3) or oneShotLearn(4).

		The value of this object is in effect regardless of the
		value of s3EnetConcSecureStatus or s3EnetPortAuthStatus.

		Continuous learning is not compatible with LattisSecure
		receive security, thus s3EnetPortAddrLearnMode should not
		be set to continuousLearn(3) when s3EnetPortAuthStatus
		is on(2).  If this combination is set, the receive
		security will not function.

		If this object is set to oneShotLearn(4), the agent will
		store the address (when it is learned) into the allowed
		nodes tables.  This can cause the current address to be
		written over.

		Because continuous learning is not compatible with
		receive security, addresses learned while the port
		is in continuous learning mode will not be stored in
		the allowed nodes tables.

		Attempts to set the value to other(1) on a LattisSecure
		port will be rejected by the agent.  Likewise, attempts
		to set the value to noAutoLearn(2), continuousLearn(3),
		or oneShotLearn(4) on a non-LattisSecure port will be
		rejected."
	::= { s3EnetPortEntry 22 }

s3EnetPortTxSecurity OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),	-- unknown or not LattisSecure port
		on(2),		-- LattisSecure transmit security enabled
		off(3)		-- LattisSecure transmit security disabled
		}
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"This value of this object is meaningful only when
		s3EnetConcSecureStatus is not set to concSecureOff(5)
		(i.e., if security features are activated on the
		concentrator).

		This object applies only to ports on LattisSecure Host
		Modules.  For other ports, the agent will return other(1)
		in response to a get request.

		The value off(3) indicates that LattisSecure transmit
		security is disabled on this LattisSecure port.  The
		value on(2) indicates that LattisSecure transmit security
		is enabled on this LattisSecure port.

		Attempts to set the value to other(1) on a LattisSecure
		port will be rejected by the agent.  Likewise, attempts
		to set the value to on(2) or off(3) on a non-LattisSecure
		port will be rejected."
	::= { s3EnetPortEntry 23 }



-- Common Port Table

s3EnetCommonPortTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetCommonPortEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"This table provides a list of port entries.  The
		number of entries is given for any Ethernet board
		in the concentrator, even if the board is not on the
		same Ethernet segment as this NMM."
	::= { s3000EnetPort 2 }

s3EnetCommonPortEntry OBJECT-TYPE
	SYNTAX	S3EnetCommonPortEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"A table containing objects about the ports of each
		Ethernet board plugged into the 3000-series chassis."
	INDEX	{ s3EnetCommonPortBoardIndex, s3EnetCommonPortIndex }
	::= { s3EnetCommonPortTable 1 }

S3EnetCommonPortEntry ::= SEQUENCE {
	s3EnetCommonPortBoardIndex
		INTEGER,
	s3EnetCommonPortIndex
		INTEGER,
	s3EnetCommonPortLinkStatus
		INTEGER,
	s3EnetCommonPortPartStatus
		INTEGER,
	s3EnetCommonPortType
		INTEGER,
	s3EnetCommonPortPartTime
		TimeTicks
	}

s3EnetCommonPortBoardIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"A unique value for each board.  Its value ranges
		between 1 and 12.  The value for each board must
		remain constant at least from one re-initialization
		of the entity's network management system to the
		next re-initialization."
	::= { s3EnetCommonPortEntry 1 }

s3EnetCommonPortIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"A unique value for each port.  Its value is dependent
		on the board type."
	::= { s3EnetCommonPortEntry 2 }

s3EnetCommonPortLinkStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		off(1),		-- link is not connected
		on(2),		-- link is connected
		other(3)	-- returned for AUI
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Tells whether the port is receiving link status."
	::= { s3EnetCommonPortEntry 3 }

s3EnetCommonPortPartStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		enabled(1),	   -- port enabled
		partition(2),	   -- port partitioned
		autoPartition(3),  -- port auto-partitioned
		timedPartition(4), -- timed partition
		latSecPartition(5) -- port partitioned by LattisSecure
		}
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"This indicates the operational status of the Port.
		Writing a partition(2) will partition the port
		indefinitely and enabled(1) will enable the port.

		If a timed partition is desired, then writing
		timedPartition(4) to this object at the same time
		that a time value is supplied in s3EnetCommonPortPartTime
		is required.  Timed partitions will not survive across
		a reset.  In this case the port will go to the
		partition(2) state.

		The value latSecPartition(5) is returned when the port
		has been automatically partitioned by the LattisSecure
		Host Module because of a security violation.  The value
		autoPartition(3) is returned when the port has been
		automatically partitioned by the repeater using the
		802.3 repeater auto-partition function.

		The agent will not allow this object to be set to
		autoPartition(3) or latSecPartition(5) using an SNMP
		request.

		Note that the value timedPartition(4)  is returned only
		when the board is timed partitioned by this NMM."
	::= { s3EnetCommonPortEntry 4 }

s3EnetCommonPortType OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),	-- unknown or other
		tenBaseT(2),	-- 10BASE-T, "normal" or MDI-X
		tenBaseTMdi(3),	-- 10BASE-T, switched to MDI
		aui(4),		-- AUI (10BASE5 to coax)
		bnc(5),		-- BNC(10BASE2 to thinnet)
		foirl(6),	-- FOIRL
		tenBaseFL(7),	-- 10BASE-FL
		switch(8),	-- Switch, MDI-X
		switchMdi(9),	-- Switch, MDI
		tenBaseFLRedund(10) -- 10BASE-FL, redundancy 
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The media connnection type for this port.

		Note that this object was called s3EnetPortMDIXSwitch
		in the Ethernet 3.3 and 4.0 MIBs."
	::= { s3EnetCommonPortEntry 5 }

s3EnetCommonPortPartTime OBJECT-TYPE
	SYNTAX	TimeTicks
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"When partitioning the port for a specified time,
		s3EnetCommonPortPartStatus must be set with
		timedPartition(4) and this object must be supplied
		with the duration value.  If a PDU sets
		s3EnetCommonPortPartStatus and not this object,
		the port will not be partitioned."
	::= { s3EnetCommonPortEntry 6 }


-- Redundant Port Table 

s3EnetRedPortTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetRedPortEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"A table of ports for each 10BASE-FL board with
		redundancy capability.  The number of boards is
		determined by checking s3EnetCommonBoardRedund having
		a value of redundCapable(2) for each board in table
		s3EnetCommonBoardTable."
	::= { s3000EnetPort 3 }

s3EnetRedPortEntry OBJECT-TYPE
	SYNTAX	S3EnetRedPortEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"An entry in the table of ports on boards with
		redundancy capability. Entries in the table cannot
		be created or deleted via SNMP.

		Row modification via SNMP is allowed only for ports
		that support either hardware or software redundancy,
		but the amount of modifications between the two varies.

		Entries for boards that support hardware-redundancy
		only allow the objects s3EnetRedPortRedundMode,
		s3EnetRedPortSwitchoverStatus, and
		s3EnetRedPortSwitchoverTime to be modified.
		The object s3EnetRedPortRedundMode can only
		be modified on certain agent versions (see the
		description of the object for more details).

		Entries for boards that support software-redundancy
		allow the objects s3EnetRedPortRedundMode,
		s3EnetRedPortCompanionSlotNo,
		s3EnetRedPortCompanionPortNo,
		s3EnetRedPortSwitchoverStatus, and
		s3EnetRedPortSwitchoverTime to be modified.

		Software-redundant pairs are configured by sending
		the objects s3EnetRedPortRedundMode,
		s3EnetRedPortCompanionSlotNo, and 
		s3EnetRedPortCompanionPortNo in the same SNMP SET
		PDU, with the object s3EnetRedPortRedundMode 
		set to the value of swActive(4) or swStandby(5).

		When changing an existing software-redundant pair,
		the existing pair must first be broken up by setting
		the object s3EnetRedPortRedundMode to standalone(1),
		and then a new pair must be configured as described
		above."
	INDEX	{ s3EnetRedPortBoardIndex,
		  s3EnetRedPortIndex }
	::= { s3EnetRedPortTable 1 }

S3EnetRedPortEntry  ::=  SEQUENCE {
	s3EnetRedPortBoardIndex
		INTEGER,
	s3EnetRedPortIndex
		INTEGER,
	s3EnetRedPortRedundMode
		INTEGER,
	s3EnetRedPortOperStatus
		INTEGER,
	s3EnetRedPortRemoteOperStatus
		INTEGER,
	s3EnetRedPortCompanionSlotNo
		INTEGER,
	s3EnetRedPortCompanionPortNo
		INTEGER,
	s3EnetRedPortSwitchoverStatus
		INTEGER,
	s3EnetRedPortSwitchoverTime
		TimeTicks,
	s3EnetRedPortCapability
		INTEGER
	}

s3EnetRedPortBoardIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The index of the slot containing the board.  The value
		for each board must remain constant at least from one
		re-initialization of the entity's network management
		system to the next re-initialization."
	::= { s3EnetRedPortEntry 1 }

s3EnetRedPortIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The index of the port on the module."
	::= { s3EnetRedPortEntry 2 }

s3EnetRedPortRedundMode OBJECT-TYPE
	SYNTAX	INTEGER {
		standAlone(1),
		hwActive(2),
		hwStandby(3),
		swActive(4),
		swStandby(5)
		}
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"The redundancy mode of the port. 

		The possible values read, which report the redundancy
		mode of the port, are:
		  standalone(1)...the port is not in any redundant pair.
		  hwActive(2).....the port is the active companion in
		                  a hardware-redundant pair.
		  hwStandby(3)....the port is the standby companion
		                  in a hardware-redundant pair.
		  swActive(4).....the port is the active companion in
		                  a software-redundant pair.
		  swStandby(5)....the port is the standby companion
		                  in a software-redundant pair.

		The values that can be written, which change the redundancy
		mode, are:
		  standalone(1)...causes the software-redundant pair
		                  to be broken up.
		  hwActive(2).....if the previous value was hwStandby(3),
		                  this value will cause the port to become
		                  the active port in the hardware-redundant
		                  pair (i.e., a switchover).
		  hwStandby(3)....if the previous value was hwActive(2),
		                  this value will cause the port to become
		                  the standby port in the hardware-redundant
		                  pair (i.e., a switchover).
		  swActive(4).....if the previous value was swStandby(5),
		                  this value will cause the port to become
		                  the active port in the software-redundant
		                  pair (i.e., a switchover).
		  swStandby(5)....if the previous value was swActive(4),
		                  this value will cause the port to become
		                  the standby port in the software-redundant
		                  pair (i.e., a switchover).

		Notes:  1.) The value standalone(1) cannot be written to
		            effect hardware-redundant pairs."
	::= { s3EnetRedPortEntry 3 }

s3EnetRedPortOperStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),
		ok(2),
		localFault(3),
		remoteFault(4)
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This object indicates port's redundancy status.
		The values are:
		  other(1).........none of the following
		  ok(2)............no fault
		  localFault(3)....the local port has sensed a fault condition.
		  remoteFault(4)...the remote port has sensed a fault
		                   condition and has signaled the local port
		                   accordingly.

		Either a localFault(3) or remoteFault(4) condition should
		cause a redundant port pair to switchover.

		Notes:  If the redundant link is generating on
		        10BASE-FL without remote fault capability,
		        the value remoteFault(4) will not be reported."
	::= { s3EnetRedPortEntry 4 }

s3EnetRedPortRemoteOperStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		snpxFLRemFltCpblPortUp(1),
		snpxFLFBRemFltCpblPortUp(2),
		tenBaseFLPortUp(3),
		tenBaseFBPortUp(4),
		snpxRemFltCpblPortFault(5),
		tenBaseFBPortFault(6),
		unknown(7)
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This object reflects the real time status of the
		received data from the remote port.

		A value of snpxFLRemFltCpblPortUp(1) indicates that
		the remote port is capable of 10BASE-FL signaling, as
		well as SynOptics proprietary remote fault signaling.
		A remote fault on such a port is indicated by
		snpxRemFltCpblPortFault(5).

		A value of snpxFLFBRemFltCpblPortUp(2) indicates that
		the remote port is capable of 10BASE-FL, 10BASE-FB and
		SynOptics proprietary remote fault signaling.  A remote
		fault on such a port is indicated by
		snpxRemFltCpblPortFault(5).

		A value of tenBaseFLPortUp(3) indicates that the remote
		port uses regular idle 10BASE-FL signaling, and is
		incapable of remote fault signaling.

		A value of tenBaseFBPortUp(4) indicates that the remote
		port uses 10BASE-FB synchronous signaling.  A remote
		fault on such a port is indicated by
		tenBaseFBPortFault(6).

		A value of unknown(7) indicates that the remote signal
		received is none of the above."
	::= { s3EnetRedPortEntry 5 }

s3EnetRedPortCompanionSlotNo OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"The slot number of the other port which is in the
		redundant pair.  In the case of a standalone port,
		a value of 0 will be returned.

		Note:  This object is only writable for ports that
		       support software-redundancy."
	::= { s3EnetRedPortEntry 6 }

s3EnetRedPortCompanionPortNo OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"The port number of the other port which is in the
		redundant pair.  In the case of a standalone port,
		a value of 0 will be returned.

		Note:  This object is only writable for ports that
		       support software-redundancy."
	::= { s3EnetRedPortEntry 7 }

s3EnetRedPortSwitchoverStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),
		timedSwitchover(2)
		}
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"The switchover status of the redundant port pair.

		The following values can be written:
		  timedSwitchover(2)...Immediately causes the active
		                         port to become the standby
		                         port, and the standby port to
		                         become the active port.  Then
		                         once the value of
		                         s3EnetRedPortSwitchoverTime
		                         has elapsed to zero, the ports
		                         revert back to their orignal
		                         roles.

		The following values can be read:
		  other(1).............The port is NOT undergoing a
		                         timed switchover.
		  timedSwitchover(2)...The port is undergoing a
		                         timed switchover.

		Notes:  1.) When writing timedSwitchover(2) to this
		            object, the SET request must also specify a
		            value for the object s3EnetRedSwitchoverTime.

		        2.) Once the timed switchover has taken place,
		            the value of this object reverts from
		            timedSwitchover(2) to other(1)."
	DEFVAL { other }
	::= { s3EnetRedPortEntry 8 }

s3EnetRedPortSwitchoverTime OBJECT-TYPE
	SYNTAX	TimeTicks
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"The length of time before the ports making up
		the redundant port pair revert back to their orignal
		active or standby roles as defined before the timed
		switchover was setup.

		The value of this object is meaningful (i.e., non-zero)
		only when the redundant port pair is undergoing a
		timed switchover, which is indicated by the object
		s3EnetRedPortSwitchoverStatus having the value
		of timedSwitchover(2).

		This object may only be written in the same SET
		request that changes the object
		s3EnetRedPortSwitchoverStatus to timedSwitchover(2).
		Afterwards, it indicates the amount of time left
		before the timed switchover is completed, at which
		time another switchover occurs and
		s3EnetRedPortSwitchoverStatus is changed to
		other(1).

		This object has the value of zero if the port is not
		undergoing a timed switchover, or if the amount
		of time is unavailable."
	DEFVAL { 0 }
	::= { s3EnetRedPortEntry 9 }

s3EnetRedPortCapability OBJECT-TYPE
	SYNTAX	INTEGER {
		hwRedOnly(1),
		swRedOnly(2),
		notRedunCapable(3)
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The redundancy capability of the port:
		  hwRedOnly(1).........hardware redundancy only.
		  swRedOnly(2).........software redundacy only.
		  notRedunCapable(3)...port not capable of being
		                       configured into a redundant
		                       port pair.

		A value of hwRedOnly(1) or swRedOnly(2) means that
		the port is capable of being configured into a
		redundant port pair."
	::= { s3EnetRedPortEntry 10 }


-- Redundant Ports  Table Last Change Timestamp

s3EnetRedPortLastChg OBJECT-TYPE
	SYNTAX	TimeTicks
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The value of sysUptime when the last change in the
		redundant ports table was observed by the agent."
	::= { s3000EnetPort 4 }


-- SECTION 3: Network Management Module Group

-- This group is OBSOLETE!


-- Module Group

s3EnetNmmType OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),	-- none of the following
		m3313(2),	-- Model 3313
		m3313M(3),	-- Model 3313M
		m3314-ST(4),	-- Model 3314-ST
		m3314M-ST(5),	-- Model 3314M-ST
		m3138(6)	-- Model 3138
		}
	ACCESS	read-only
	STATUS	obsolete
	DESCRIPTION
		"See s3AgentType"
	::= { s3000EnetNmm 1 }

s3EnetNmmMdaHwVer OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	obsolete
	DESCRIPTION
		"See AgentMdaHwVer"
	::= { s3000EnetNmm 2 }

s3EnetNmmFwVer OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	obsolete
	DESCRIPTION
		"See s3AgentFwVer"
	::= { s3000EnetNmm 3 }

s3EnetNmmSwMajorVer OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	obsolete
	DESCRIPTION
		"See s3AgentSwMajor"
	::= { s3000EnetNmm 4 }

s3EnetNmmSwMinorVer OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	obsolete
	DESCRIPTION
		"See s3AgentSwMinor"
	::= { s3000EnetNmm 5 }

s3EnetNmmStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		offline(1),	-- the nmm is offline
		online(2)	-- the nmm is online
	}
	ACCESS	read-only
	STATUS	obsolete
	DESCRIPTION
		"See s3AgentStatus"
	::= { s3000EnetNmm 6 }

s3EnetNmmMode OBJECT-TYPE
	SYNTAX	INTEGER {
		primary(1),	-- in primary mode
		secondary(2)	-- in secondary mode
	}
	ACCESS	read-write
	STATUS	obsolete
	DESCRIPTION
		"See s3AgentMode"
	::= { s3000EnetNmm 7 }

s3EnetNmmReset OBJECT-TYPE
	SYNTAX	INTEGER {
		notreset(1),	-- not reseting
		reset(2)	-- reset
	}
	ACCESS	read-write
	STATUS	obsolete
	DESCRIPTION
		"See s3AgentReset"
	::= { s3000EnetNmm 8 }

s3EnetNmmRestart OBJECT-TYPE
	SYNTAX	INTEGER {
		notrestart(1),	-- not restarting
		restart(2)	-- restart
	}
	ACCESS	read-write
	STATUS	obsolete
	DESCRIPTION
		"See s3AgentRestart"
	::= { s3000EnetNmm 9 }


-- EEPROM Configuration Group

s3EnetNmmIpAddr OBJECT-TYPE
	SYNTAX	IpAddress
	ACCESS	read-write
	STATUS	obsolete
	DESCRIPTION
		"See s3AgentIpAddr"
	::= { s3000EnetNmm 10 }

s3EnetNmmNetMask OBJECT-TYPE
	SYNTAX	IpAddress
	ACCESS	read-write
	STATUS	obsolete
	DESCRIPTION
		"See s3AgentNetMask"
	::= { s3000EnetNmm 11 }

s3EnetNmmDefaultGateway OBJECT-TYPE
	SYNTAX	IpAddress
	ACCESS	read-write
	STATUS	obsolete
	DESCRIPTION
		"See s3AgentDefaultGateway"
	::= { s3000EnetNmm 12 }

s3EnetNmmFileServerAddr OBJECT-TYPE
	SYNTAX	IpAddress
	ACCESS	read-write
	STATUS	obsolete
	DESCRIPTION
		"See s3AgentBootServerAddr"
	::= { s3000EnetNmm 13 }

s3EnetNmmBootFile OBJECT-TYPE
	SYNTAX	OCTET STRING (SIZE(0..64))
	ACCESS	read-write
	STATUS	obsolete
	DESCRIPTION
		"See s3AgentBootFile"
	::= { s3000EnetNmm 14 }

s3EnetNmmBootMode OBJECT-TYPE
	SYNTAX	INTEGER {
		eeprom(1),
		bootp(2)
		}
	ACCESS	read-write
	STATUS	obsolete
	DESCRIPTION
		"See s3AgentBootMode"
	::= { s3000EnetNmm 15 }

s3EnetNmmWriteEeprom OBJECT-TYPE
	SYNTAX	INTEGER {
		notWriteEeprom(1),
		writeEeprom(2)
		}
	ACCESS	read-write
	STATUS	obsolete
	DESCRIPTION
		"See s3AgentWriteEeprom"
	::= { s3000EnetNmm 16 }

s3EnetNmmBaudRate OBJECT-TYPE
	SYNTAX	Gauge
	ACCESS	read-only
	STATUS	obsolete
	DESCRIPTION
		"See s3AgentBaudRate"
	::= { s3000EnetNmm 17 }

s3EnetNmmInitString OBJECT-TYPE
	SYNTAX	OCTET STRING (SIZE(0..64))
	ACCESS	read-write
	STATUS	obsolete
	DESCRIPTION
		"See s3AgentInitString"
	::= { s3000EnetNmm 18 }

s3EnetNmmLocation OBJECT-TYPE
	SYNTAX	OCTET STRING (SIZE(0..64))
	ACCESS	read-write
	STATUS	obsolete
	DESCRIPTION
		"See s3AgentLocation"
	::= { s3000EnetNmm 19 }



-- Trap Server Table

s3EnetNmmTrapServerTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetNmmTrapServerEntry
	ACCESS	not-accessible
	STATUS	obsolete
	DESCRIPTION
		"See s3AgentTrapReceiverTable"
	::= { s3000EnetNmm 20 }

s3EnetNmmTrapServerEntry OBJECT-TYPE
	SYNTAX	S3EnetNmmTrapServerEntry
	ACCESS	not-accessible
	STATUS	obsolete
	DESCRIPTION
		"See s3AgentTrapReceiverEntry"
	INDEX	{ s3EnetNmmTrapServerAddress }
	::= { s3EnetNmmTrapServerTable 1 }

S3EnetNmmTrapServerEntry ::= SEQUENCE {
	s3EnetNmmTrapType
		INTEGER,
	s3EnetNmmTrapServerAddress
		IpAddress,
	s3EnetNmmTrapServerComm
		OCTET STRING
	}

s3EnetNmmTrapType OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),
		invalid(2)
		}
	ACCESS	read-write
	STATUS	obsolete
	DESCRIPTION
		"See s3AgentTrapRcvrStatus"
	::= { s3EnetNmmTrapServerEntry 1 }

s3EnetNmmTrapServerAddress OBJECT-TYPE
	SYNTAX	IpAddress
	ACCESS	read-write
	STATUS	obsolete
	DESCRIPTION
		"See s3AgentTrapRcvrNetAddress"
	::= { s3EnetNmmTrapServerEntry 2 }

s3EnetNmmTrapServerComm OBJECT-TYPE
	SYNTAX	OCTET STRING (SIZE(0..20))
	ACCESS	read-write
	STATUS	obsolete
	DESCRIPTION
		"See s3AgentTrapRcvrComm"
	::= { s3EnetNmmTrapServerEntry 3 }

s3EnetNmmAuthTrap OBJECT-TYPE
	SYNTAX	INTEGER {
		disable(1),
		enable(2)
		}
	ACCESS	read-write
	STATUS	obsolete
	DESCRIPTION
		"See s3AgentAuthTrap"
	::= { s3000EnetNmm 21 }



-- SECTION 4: Node Lists Group

-- The Node Lists group includes the Show Nodes, Find Nodes, and
--   Allowed Nodes tables.

-- Implementation of this group is mandatory for all
--   SynOptics Series 3000 Ethernet NMM agents


-- Show Nodes Table


s3EnetShowNodesTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetShowNodesEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"Table containing a list of all of the nodes that have
		been active during the aging interval that are currently
		connected to the network through this concentrator.
		This table is different from the FindNodes table in that
		this table is indexed using the slot, port, and MAC address
		attributes associated with the node.  This allows a
		manager to get all nodes based on slot, slot-port, or
		slot-port-MAC."
	::= { s3000EnetNode 1 }

s3EnetShowNodesEntry OBJECT-TYPE
	SYNTAX	S3EnetShowNodesEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"List of nodes active on the concentrator and the slot
		and port the nodes are on."
	INDEX	{ s3EnetShowNodesSlotIndex,
		 s3EnetShowNodesPortIndex,
		 s3EnetShowNodesMacAddress }
	::= { s3EnetShowNodesTable 1 }

S3EnetShowNodesEntry ::= SEQUENCE {
	s3EnetShowNodesSlotIndex
		INTEGER,
	s3EnetShowNodesPortIndex
		INTEGER,
	s3EnetShowNodesMacAddress
		PhysAddress,
	s3EnetShowNodesStatus
		INTEGER,
	s3EnetShowNodesVendorType
		INTEGER,
	s3EnetShowNodesAuthStatus
		INTEGER
	}

s3EnetShowNodesSlotIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The board number the node is on.  Valid entries are 1-12."
	::= { s3EnetShowNodesEntry 1 }

s3EnetShowNodesPortIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The port number the node is on.  Valid entries are 1-12."
	::= { s3EnetShowNodesEntry 2 }

s3EnetShowNodesMacAddress OBJECT-TYPE
	SYNTAX	PhysAddress (SIZE(6))
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This object contains the MAC address (i.e. the
		Ethernet address) of the node."
	::= { s3EnetShowNodesEntry 3 }

s3EnetShowNodesStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		active(1),	-- node has transmitted in past 5 seconds
		inactive(2)	-- node has not transmitted in past 5 secs
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The status of the node.  Determines whether the node
		has actively transmitted or not  over the last 5 seconds."
	::= { s3EnetShowNodesEntry 4 }

s3EnetShowNodesVendorType OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),	-- unknown vendor
		threeCom(2)	-- 3Com adapter card
		}
	ACCESS	read-only
	STATUS	deprecated
	DESCRIPTION
		"The vendor type of the adapter seen on this port.  If
		the vendor is unknown other(1) should be returned."
	::= { s3EnetShowNodesEntry 5 }

s3EnetShowNodesAuthStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),	-- unknown configuration
		network(2),	-- node learned by listening to network
		nmm(3),		-- node is NMM or known device from diff conc
		authorized(4)	-- node was authorized to use this slot/port.
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The object is used determine how the node was added to
		this table.  If the node was learned by listening to the
		network then on reads network(2) should be returned.  If
		the node is another NMM or known concentrator device,
		then nmm(3) is returned.  If the device's MAC
		address is unknown because of some unknown but legal
		configuration, then other(1) should be returned and
		s3EnetShowNodesMacAddress should return all zeros.
		If the node was entered into the AllowedNode list
		via management control, and was seen on a port that it
		was authorized to use, then authorized(4) should
		be returned."
	::= { s3EnetShowNodesEntry 6 }


-- Table Aging Control


s3EnetNodeAgeInterval OBJECT-TYPE
	SYNTAX	TimeTicks
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"The time used for aging of the nodes in tables
		s3EnetShowNodesTable and s3EnetFindNodesTable.
		Once a node has completely aged it will be
		removed from these tables.

		Note:
		Agents that implement the s3EnetSdTrafTable and
                s3EnetDsTrafTable tables and do not implement the
		the object s3EnetTrafAgeInterval (i.e., agents prior
		to version 5.3), also use s3EnetNodeAgeInterval to
		age the nodes in these two tables."
	::= { s3000EnetNode 2 }


-- Find Nodes Table


s3EnetFindNodesTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetFindNodesEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"Table containing a list of all of the nodes that have
		been active during the aging interval  that are
		currently connected to the network through this
		concentrator.  This table is different than the
		ShowNodes table in that this table is index using
		only the MAC address attribute associated with the node.
		This allows a manager to be able to quickly determine
		if a node with a particular MAC address is located
		on this concentrator or not."
	::= { s3000EnetNode 3 }

s3EnetFindNodesEntry OBJECT-TYPE
	SYNTAX	S3EnetFindNodesEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"Entry in the table containing the slot, port and MAC
		address of a node connected to the Ethernet through
		this concentrator."
	INDEX	{  s3EnetFindNodesMacAddress }
	::= { s3EnetFindNodesTable 1 }

S3EnetFindNodesEntry ::= SEQUENCE {
	s3EnetFindNodesMacAddress
		PhysAddress,
	s3EnetFindNodesSlotIndex
		INTEGER,
	s3EnetFindNodesPortIndex
		INTEGER
	}

s3EnetFindNodesMacAddress OBJECT-TYPE
	SYNTAX	PhysAddress (SIZE(6))
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"MAC address of node that this entry in the table is for."
	::=  { s3EnetFindNodesEntry 1 }

s3EnetFindNodesSlotIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The board that the node is connected through."
	::=  { s3EnetFindNodesEntry 2 }

s3EnetFindNodesPortIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The port that the node is connected through."
	::=  { s3EnetFindNodesEntry 3 }



-- Authorized Nodes Table

-- The authorized nodes table lists the MAC addresses of hosts that
--   are authorized to send packets into the concentrator.  Each entry
--   in the table must have a unique MAC address.  A MAC address may
--   be authorized to use a single port, any port on a board, or any
--   port in the concentrator.

-- This table can be modified in the following ways:
--    * initial download in a configuration file
--    * SNMP set request
--    * LattisSecure "one-shot" automatic address learning (addresses
--      learned while the port is in continuous auto learn mode will
--      not be stored in the allowed nodes tables).


s3EnetAuthNodesTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetAuthNodesEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"Table containing a list of MAC addresses and the slot
		and ports that the MAC address is allowed to be heard on,
		in case the authorized node feature is turned on.

		If a MAC is allowed on any slot and port then the entry
		will have the slot=0 and the port=0.  If the MAC address
		is allowed on a particular board then slot=allowed board
		and port=0.  If the MAC is only allowed on one port then
		the entry will contain a slot value and port value
		between 1-12.

		Allowed nodes for LattisSecure ports must be configured
		for that specific port.  The agent will reject an attempt
		to create a slot-level entry for slot=x, port=0, if the
		board in slot x is a LattisSecure Host Module.  Only a
		single address may be configured for a LattisSecure port.
		Adding a second address (with the same LattisSecure
		slot-port number) to the table will cause the first
		address to be replaced with the new entry.

		A MAC address can only appear in the table one time.
		To determine when a station heard on the network must
		be verified in this table please read the complete
		description of the authorized node list feature as
		described with object S3EnetConcAuthStatus.

		Entries in this table may be downloaded via the CFG file
		or can be added via SNMP.  All adds via SNMP will be
		lost when the system is reset."
	::= { s3000EnetNode 4 }

s3EnetAuthNodesEntry OBJECT-TYPE
	SYNTAX	S3EnetAuthNodesEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"Entry in the table containing a MAC address of a
		node that is allowed on the ethernet through this
		concentrator."
	INDEX	{ s3EnetAuthNodesMacAddr }
	::= { s3EnetAuthNodesTable 1 }

S3EnetAuthNodesEntry ::= SEQUENCE {
	s3EnetAuthNodesMacAddr
		PhysAddress,
	s3EnetAuthNodesSlotIndex
		INTEGER,
	s3EnetAuthNodesPortIndex
		INTEGER,
	s3EnetAuthNodesStatus
		INTEGER
	}

s3EnetAuthNodesMacAddr OBJECT-TYPE
	SYNTAX	PhysAddress (SIZE(6))
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"MAC address of node that this entry in the table
		is for."
	::=  { s3EnetAuthNodesEntry 1 }

s3EnetAuthNodesSlotIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"The board that the node is allowed to be heard through.
		If this object is 0, then the MAC address is allowed
		on any board in the concentrator.  In this case
		s3EnetAuthNodesPortIndex should also be 0.  Otherwise,
		this object describes the slot that the MAC address of
		this entry is allowed to connect to."
	::=  { s3EnetAuthNodesEntry 2 }

s3EnetAuthNodesPortIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"The port that the node is allowed to be heard through.
		If this object is 0, then the MAC address of this entry
		is allowed to connect to any port on the board (if
		s3EnetAuthNodesSlotIndex is not 0) or if
		s3EnetAuthNodesSlotIndex is 0, then the MAC address is
		allowed to be heard from any port on the concentrator.
		Otherwise, this object specifies which port on the
		s3EnetAuthNodesSlotIndex this MAC address is allowed
		to be heard on."
	::=  { s3EnetAuthNodesEntry 3 }

s3EnetAuthNodesStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		invalid(1),	-- delete entry
		valid(2)	-- add entry
		}
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"The status of the AuthNodes entry.  The primary use
		of this object is for modifying the AuthNodes table.
		It is also returned in the enetAuthViolation trap,
		in which case it indicates whether the violating
		MAC address was found in the AuthNodes table.

		Setting this entry to invalid(1) causes the entry to be
		deleted from the table.  Setting a new entry with valid(2)
		causes the entry to be created in the table.  The response
		to a get request or get-next request will always
		indicate a status of valid(2), since invalid entries
		are removed from the table."
	::= { s3EnetAuthNodesEntry 4 }


s3EnetMaxNodesPerPort OBJECT-TYPE
	SYNTAX	INTEGER (0..65535)
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"Maximun number of MAC address remembered by the
		agent on a per port basis, this number should be
		smaller than the maximum limit imposed by the agent."
	::= {s3000EnetNode 5}



-- SECTION 5: Ethernet Topology Group

-- The Ethernet Topology Group includes NMM and Bridge topology tables.

-- Implementation of this group is mandatory for all
--   SynOptics Series 3000 Ethernet agents


-- NMM Topology Table


s3EnetTopNmmTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetTopNmmEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"A table of the NMM's in the flat network."
	::= { s3000EnetNmmTopology 1 }

s3EnetTopNmmEntry OBJECT-TYPE
	SYNTAX	S3EnetTopNmmEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"Table that contains information about NMMs that are
		in the same flat network as this NMM."
	INDEX	{ s3EnetTopNmmSlot,
		 s3EnetTopNmmPort,
		 s3EnetTopNmmIpAddr }
	::= { s3EnetTopNmmTable 1 }

S3EnetTopNmmEntry ::= SEQUENCE {
	s3EnetTopNmmSlot
		INTEGER,
	s3EnetTopNmmPort
		INTEGER,
	s3EnetTopNmmIpAddr
		IpAddress,
	s3EnetTopNmmMacAddr
		PhysAddress,
	s3EnetTopNmmChassisType
		SnpxChassisType,
	s3EnetTopNmmBkplType
		SnpxBackplaneType,
	s3EnetTopNmmLocalSeg
		INTEGER,
	s3EnetTopNmmNumSeen
		INTEGER,
	s3EnetTopNmmModuleType
		S3ModuleType,
	s3EnetTopNmmNumLinks
		INTEGER,
	s3EnetTopNmmChgStatus
		INTEGER
	}

s3EnetTopNmmSlot OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Slot that the NMM this entry is for can be found using the
		topology protocol.  This is the slot from which a topology
		message was received."
	::= { s3EnetTopNmmEntry 1 }

s3EnetTopNmmPort OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Port that the NMM this entry is for can be found using the
		topology protocol.  This is the port from which a topology
		message was received."
	::= { s3EnetTopNmmEntry 2 }

s3EnetTopNmmIpAddr OBJECT-TYPE
	SYNTAX	IpAddress
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"IpAddress of the NMM this entry is for.  This is the
		IP address of the NMM that sent a topology message."
	::= { s3EnetTopNmmEntry 3 }

s3EnetTopNmmMacAddr OBJECT-TYPE
	SYNTAX	PhysAddress (SIZE(6))
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"MAC Address of the NMM this entry is for."
	::= { s3EnetTopNmmEntry 4 }

s3EnetTopNmmChassisType OBJECT-TYPE
	SYNTAX	SnpxChassisType
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Concentrator type of the NMM this entry is for.
		The enumerated values of this object are the same as
		defined in the common MIB for object s3ChassisType."
	::= { s3EnetTopNmmEntry 5 }

s3EnetTopNmmBkplType OBJECT-TYPE
	SYNTAX	SnpxBackplaneType
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Concentrator backplane type of the NMM this entry is for.
		The enumerated values of this object are the same as
		defined in the common MIB for object s3ChassisBkplType."
	::= { s3EnetTopNmmEntry 6 }

s3EnetTopNmmLocalSeg OBJECT-TYPE
	SYNTAX	INTEGER {
		true(1),
		false(2)
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Does this entry NMM exist in the same segment as this
		(the reporting) NMM."
	::= { s3EnetTopNmmEntry 7 }

s3EnetTopNmmNumSeen OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Number of NMMs visible from the slot-port pair that
		this NMM is seen through."
	::= { s3EnetTopNmmEntry 8 }

s3EnetTopNmmModuleType OBJECT-TYPE
	SYNTAX	S3ModuleType
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The module type of the NMM that this entry is for.
		The values of this object are equivalent to those defined
		in the common MIB for object s3SlotModuleType."
	::= { s3EnetTopNmmEntry 9 }

s3EnetTopNmmNumLinks OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Number of links through which NMMs are visible on this NMM."
	::= { s3EnetTopNmmEntry 10 }

s3EnetTopNmmChgStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		changed(1),	-- NMM detected topology change
		noChange(2)	-- NMM has not detected a top change
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"If this NMM has detected any change of topology relative
		to itself it will set this object to change(1), otherwise
		noChange(2) will be returned."
	::= { s3EnetTopNmmEntry 11 }


-- Update Time Interval

s3EnetTopNmmHelloTime OBJECT-TYPE
	SYNTAX	TimeTicks
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Hello Time interval used in the topology update protocol."
	::= { s3000EnetNmmTopology 2 }

-- Encoded Octet String for NMM Topology Table

s3EnetTopNmmSubsetTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetTopNmmSubsetEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"Encoded octet string of the s3EnetTopNmmTable."
	::= { s3000EnetNmmTopology 3 }

s3EnetTopNmmSubsetEntry OBJECT-TYPE
	SYNTAX	S3EnetTopNmmSubsetEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"Encoded octet string of the s3EnetTopNmmTable.
		Instance returned in Response PDU:
		  On GETs: instance specified is the instance returned.
		  On GET-NEXTs:  instance returned is the instance of
		    the last record contained in the octet string."
	INDEX	{ s3EnetTopNmmSlot,
		 s3EnetTopNmmPort,
		 s3EnetTopNmmIpAddr }
	::= { s3EnetTopNmmSubsetTable 1 }

S3EnetTopNmmSubsetEntry ::= SEQUENCE {
	s3EnetTopNmmSubset
		OCTET STRING
	}

s3EnetTopNmmSubset OBJECT-TYPE
	SYNTAX	OCTET STRING (SIZE(0..1400))
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Encoded octet string.  On reads it contains an integral
		number of s3EnetTopNmmEntry records.  All entries are
		the same size.  Values are specified in SynOptics
		technical documents."
	::= { s3EnetTopNmmSubsetEntry 1 }



-- Bridge Topology Table


s3EnetTopBridgeTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetTopBridgeEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"A table of Bridges that are in the same segment as
		this NMM network."
	::= { s3000EnetBridTopology 1 }

s3EnetTopBridgeEntry OBJECT-TYPE
	SYNTAX	S3EnetTopBridgeEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"Table that contains information about Bridges that
		are in the same segment as this NMM."
	INDEX	{ s3EnetTopBridgeIpAddr }
	::= { s3EnetTopBridgeTable 1 }

S3EnetTopBridgeEntry ::= SEQUENCE {
	s3EnetTopBridgeIpAddr
		IpAddress,
	s3EnetTopBridgeNumber
		INTEGER,
	s3EnetTopBridgeMacAddr
		PhysAddress,
	s3EnetTopBridgeType
		INTEGER,
	s3EnetTopBridgeStatus
		INTEGER,
	s3EnetTopBridgeSlotNum
		INTEGER,
	s3EnetTopBridgePortNum
		INTEGER,
	s3EnetTopBridgeModuleType
		S3ModuleType,
	s3EnetTopBridgeHelloPortNum
		INTEGER,
	s3EnetTopBridgeHelloPortType
		INTEGER,
	s3EnetTopBridgeHelloPortStatus
		INTEGER,
	s3EnetTopBridgeCompBridgeMac1
		PhysAddress,
	s3EnetTopBridgeCompBridgeMac2
		PhysAddress
	}

s3EnetTopBridgeIpAddr OBJECT-TYPE
	SYNTAX	IpAddress
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"IP address of the bridge from the Hello PDU."
	::= { s3EnetTopBridgeEntry 1 }

s3EnetTopBridgeNumber OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Bridge Number assigned to this bridge."
	::= { s3EnetTopBridgeEntry 2 }

s3EnetTopBridgeMacAddr OBJECT-TYPE
	SYNTAX	PhysAddress (SIZE(6))
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"MAC Address of this bridge."
	::= { s3EnetTopBridgeEntry 3 }

s3EnetTopBridgeType OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),	-- not of a defined type
		localSyn2Port(2),-- local synoptics bridge: 2 ported
		remoteSyn3Port(3),-- remote synoptics bridge: 3 ported
		etherSwitch(4)	-- Kalpana EtherSwitch
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Kind of bridge this entry represents."
	::= { s3EnetTopBridgeEntry 4 }

s3EnetTopBridgeStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),	-- unknown state
		active(2),
		standby(3)
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Current operational status of this bridge."
	::= { s3EnetTopBridgeEntry 5 }

s3EnetTopBridgeSlotNum OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Slot on the concentrator that the Hello PDU from
		the bridge was received."
	::= { s3EnetTopBridgeEntry 6 }

s3EnetTopBridgePortNum OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Port on concentrator that the Hello PDU from
		the bridge was received."
	::= { s3EnetTopBridgeEntry 7 }

s3EnetTopBridgeModuleType OBJECT-TYPE
	SYNTAX	S3ModuleType
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Module type of the board that the Hello PDU from the
		Bridge was received."
	::= { s3EnetTopBridgeEntry 8 }

s3EnetTopBridgeHelloPortNum OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Port Number on the Bridge from which the Hello PDU was sent."
	::= { s3EnetTopBridgeEntry 9 }

s3EnetTopBridgeHelloPortType OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),	-- not of a defined type
		ether(2),	-- ethernet interface
		tokenRing4(3),	-- token ring interface, 4 Mbits
		tokenRing16(4),	-- token ring interface, 16 Mbits
		fddi(5),	-- fddi interface
		t1(6)		-- t1 interface
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Type of the Port on the Bridge from which the Hello
		PDU was sent."
	::= { s3EnetTopBridgeEntry 10 }

s3EnetTopBridgeHelloPortStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),	-- unknown state
		active(2),
		standby(3)
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Status of the Port on the Bridge from which the Hello
		PDU was sent."
	::= { s3EnetTopBridgeEntry 11 }

s3EnetTopBridgeCompBridgeMac1 OBJECT-TYPE
	SYNTAX	PhysAddress (SIZE(6))
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Contains one of the 2 companion MAC addresses of the
		remote bridge.  If this entry is for a local bridge or
		is unknown, then this object  should
		contain the MAC address of 0:0:0:0:0:0."
	::= { s3EnetTopBridgeEntry 12 }

s3EnetTopBridgeCompBridgeMac2 OBJECT-TYPE
	SYNTAX	PhysAddress (SIZE(6))
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Contains one of the 2 companion MAC addresses of the
		remote bridge.  If this entry is for a local bridge
		or is unknown, then this object  should contain the
		MAC address of 0:0:0:0:0:0."
	::= { s3EnetTopBridgeEntry 13 }


-- Encoded Octet String for Bridge Topology Table

s3EnetTopBdgSubsetTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetTopBdgSubsetEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"Encoded octet string of the s3EnetTopBridgeTable."
	::= { s3000EnetBridTopology 2 }

s3EnetTopBdgSubsetEntry OBJECT-TYPE
	SYNTAX	S3EnetTopBdgSubsetEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"Encoded octet string of the s3EnetTopBridgeTable.
		Instance returned in Response PDU:
		  On GETs: instance specified is the instance returned.
		  On GET-NEXTs: instance returned is the instance
		     of the last record contained in the octet string."
	INDEX	{ s3EnetTopBridgeIpAddr }
	::= { s3EnetTopBdgSubsetTable 1 }

S3EnetTopBdgSubsetEntry ::= SEQUENCE {
	s3EnetTopBdgSubset
		OCTET STRING
	}

s3EnetTopBdgSubset OBJECT-TYPE
	SYNTAX	OCTET STRING (SIZE(0..1400))
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Encoded octet string.  On reads it contains an integral
		number of s3EnetTopBridgeEntry records.  All entries are
		the same size.  Values are specified in SynOptics
		technical documents."
	::= { s3EnetTopBdgSubsetEntry 1 }


-- Topology Status Objects

s3EnetTopNmmLstChg OBJECT-TYPE
	SYNTAX	TimeTicks
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The value of sysUpTime the last time an entry in the
		NMM topology table was added, deleted, or modified. If
		the NMM topology table has not changed since cold/warm
		start of the agent, then the value is zero."
	::= { s3000EnetTopInfo 1 }

s3EnetTopBridgeLstChg OBJECT-TYPE
	SYNTAX	TimeTicks
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The value of sysUpTime the last time an entry in the
		bridge topology table was added, deleted, or modified.
		If the bridge topology table has not changed since
		cold/warm start of the agent, then the value is zero."
	::= { s3000EnetTopInfo 2 }

-- SECTION 6: Threshold Group


-- The Threshold group consists of the threshold table.

-- Implementation of this group is mandatory for all
--   SynOptics Series 3000 Ethernet agents

-- Threshold Table

s3EnetThreshTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetThreshEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"The table of thresholds.

		There are three kinds of thresholds supported
		in the threshold table: port thresholds, slot
		thresholds, and concentrator thresholds.  The
		object s3EnetThreshObject in the threshold table
		is used to specify the kind of threshold for the
		table entry.

		When the value of the object s3EnetThreshObject
		is port(4), the threshold entry applies to a
		specific port, which is identified by the value
		of the objects s3EnetThreshSlot and
		s3EnetThreshPort.  The port must be on the same
		segment as the NMM in order for the NMM to
		monitor the threshold.

		When the value of the object s3EnetThreshObject
		is slot(3), the threshold entry applies to a
		specific slot, which is identified by the value
		of the object s3EnetThreshSlot.  The slot must
		be on the same segment as the NMM in order for
		the NMM to monitor the threshold.

		When the value of the object s3EnetThreshObject
		is concentrator(2), the threshold entry applies
		to the segment the NMM is connected to within
		the concentrator."
	::= { s3000EnetThreshold 1 }

s3EnetThreshEntry OBJECT-TYPE
	SYNTAX	S3EnetThreshEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"A row in the Ethernet Threshold Table.

		The following columns must be specified in a
		SNMP SET request to create a row in the table
		for each of the three kinds of thresholds (each
		name is prefixed by s3EnetThresh):

		   PORT          SLOT          CONCENTRATOR
		   =========     =========     ============
		   Status=(1)    Status=(1)    Status=(1)
		   Object=(4)    Object=(3)    Object=(2)
		   Slot          Slot
		   Port
		   Type          Type          Type
		   Condition     Condition     Condition 
		   SetValue      SetValue      SetValue
		   Action        Action        Action
		  *Duration      Duration      Duration

		with the object s3EnetThreshStatus set to the
		value addActive(1).

		Notes:  1.) The value of s3EnetThreshObject
		            selects the kind of threshold for
		            the row (i.e., for port thresholds
		            it is set to the value port(4), for
		            slot thresholds it is set to the
		            value slot(3), and for concentrator
		            thresholds it is set to the value
		            concentrator(2)).

		        2.) The object s3EnetThreshPort is not
		            used for creating slot level
		            thresholds, and is set to 0 by the
		            agent when the row is created.

		        3.) The objects s3EnetThreshPort and
		            s3EnetThreshSlot are not used for
		            creating concentrator level
		            thresholds, and are both set to
		            0 by the agent when the row is
		            created.

		        4.) The value of s3EnetThreshDuration
		            is ignored for port level link
		            status thresholds.

		To delete a row in the table, the object
		s3EnetThreshStatus needs to be specified in a
		SNMP SET request with its value equal to
		delDead(2)."
	INDEX	{ s3EnetThreshIndex }
	::= { s3EnetThreshTable 1 }

S3EnetThreshEntry ::= SEQUENCE {
	s3EnetThreshIndex
		INTEGER,
	s3EnetThreshStatus
		INTEGER,
	s3EnetThreshObject
		INTEGER,
	s3EnetThreshSlot
		INTEGER,
	s3EnetThreshPort
		INTEGER,
	s3EnetThreshType
		INTEGER,
	s3EnetThreshCondition
		INTEGER,
	s3EnetThreshSetValue
		INTEGER,
	s3EnetThreshActualValue
		INTEGER,
	s3EnetThreshAction
		INTEGER,
	s3EnetThreshExceedCount
		Counter,
	s3EnetThreshDuration
		TimeTicks
	}

s3EnetThreshIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The index into the threshold table."
	::= { s3EnetThreshEntry 1 }

s3EnetThreshStatus OBJECT-TYPE
	SYNTAX	INTEGER {
		addActive(1),
		delDead(2)
		}
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"The status of the threshold.

		The possible values for a write are:

		  addActive(1)...If the entry does not exist, the
		                   entry is created as long as
		                   the other necessary objects
		                   are in the SNMP SET request.
		                   If the entry does exist
		                   and is inactive, it is
		                   activated.
		  delDead(2).....Causes the entry to be deleted
		                   from the table.  It could take
		                   5 seconds after delDead(2) is
		                   written to actually delete the
		                   entry due to task scheduling.

		The possible values for a read are:

		  addActive(1)...This threshold entry is active.
		  delDead(2).....This threshold entry is inactive
		                   and will be deleted in 5
		                   seconds or less."
	::= { s3EnetThreshEntry 2 }

s3EnetThreshObject OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),
		concentrator(2),
		slot(3),
		port(4)
		}
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"Specifies the part of the concentrator the
		threshold applies.  The possible values are:

		  other(1)..........Unknown threshold (error)
		  concentrator(2)...The threshold applies to the
		                      segment the NMM is connected
		                      to within the concentrator
		  slot(3)...........The threshold applies to a
		                      specific slot in the
		                      concentrator identified by
		                      s3EnetThreshSlot
		  port(4)...........The threshold applies to a
		                      specific port in the
		                      concentrator identified by
		                      s3EnetThreshSlot and
		                      s3EnetThreshPort

		All values are read-write with the exception of
		other(1), which is read-only.

		See the description of the object s3EnetThreshType
		for the explanation of which thresholds are
		applicable to port(4), slot(3), and
		concentrator(2)."
	::= { s3EnetThreshEntry 3 }

s3EnetThreshSlot OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"If s3EnetThreshObject is slot(3) or port(4), then
		this contains a valid slot.  Otherwise, the contents
		of this object is meaningless."
	::= { s3EnetThreshEntry 4 }

s3EnetThreshPort OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"If s3EnetThreshObject is port(4), then this contains
		a valid port.  Otherwise, the contents of this object
		is meaningless."
	::= { s3EnetThreshEntry 5 }

s3EnetThreshType OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),
		goodBytes(2),
		goodPkts(3),
		badPkts(4),
		crcPkts(5),
		misaligned(6),
		runtPkts(7),
		fragPkts(8),
		tooLong(9),
		collision(10),
		lateColls(11),
		linkStatus(12),
		multicast(13),
		broadcast(14),
		shortEvents(15),
		srcAddrChanges(16),
		dataRateMismatches(17),
		networkErrors(18),
		badToGoodPktRatio(19),
		netErrToGoodPktRatio(20),
		colltoGoodPktRatio(21),
		collBackOffErr(22)
		}
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"Determines which type of threshold applies to
		this entry.  The possible values that can be
		read and written are listed below.

		Applicable to ALL Thresholds
		==============================================
		  goodBytes(2).........Count of good bytes
		  goodPkts(3)..........Count of good packets
		  badPkts(4)...........Count of bad packets
		  crcPkts(5)...........Count of packets with CRC
		                         errors
		  misaligned(6)........Count of misaligned packets
		  runtPkts(7)..........Count of runt packets
		  fragPkts(8)..........Count of fragmented packets
		  tooLong(9)...........Count of too long packets
		  collision(10)........Count of collisions
		  lateColls(11)........Count of late collisions

		  multicast(13)........Count of multicast packets
		  broadcast(14)........Count of broadcast packets
		  shortEvents(15)......Count of short events

		  dataRateMismatches(17)....
		                       Count of data rate
		                         mismatches
		  networkErrors(18).........
		                       Count of short events,
		                         late collisions, and
		                         data rate mismatches
		  badToGoodPktRatio(19).....
		                       Ratio of bad packets to
		                         good packets, where
		                         bad packets is the sum
		                         of packets with alignment
		                         errors, packets with FCS
		                         errors, runt packets, and
		                         packets that are too long
		  netErrToGoodPktRatio(20)...
		                       Ratio of network error
		                         packets to good packets,
		                         where network error
		                         packets is the sum of
		                         short event packets,
		                         packets with late
		                         collisions, and data
		                         rate mismatch packets
		  colltoGoodPktRatio(21).....
		                       Ratio of collision packets
		                         to good packets

		Applicable ONLY to Port Thresholds
		==============================================
		  linkStatus(12).......Status of the link
		  srcAddrChanges(16)...Count of source address
		                         changes

		Applicable ONLY to Concentrator Thresholds
		==============================================
		  collBackOffErr(22)...Count of collision backoff
		                         errors

		Note:  1.) The value other(1) can only be
		           read and it indicates the entry
		           has an invalid or unknown threshold
		           type."
	::= { s3EnetThreshEntry 6 }

s3EnetThreshCondition OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),
		crossValue(2),
		overValue(3),
		overRate(4),
		linkOn(5),
		linkOff(6),
		overRatio(7)
		}
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"Conditions that set off the threshold.  The
		possible values are:

		  other(1)........None of the following
		  crossValue(2)...The value of
		                    s3EnetThreshActualValue
		                    crosses the value of
		                    s3EnetThreshSetValue (i.e.,
		                    either from lower to higher
		                    or from higher to lower)
		  overValue(3)....The value of
		                    s3EnetThreshActualValue is
		                    greater than
		                    s3EnetThreshSetValue
		  overRate(4).....The rate of
		                    s3EnetThreshActualValue/sec
		                    is greater than
		                    s3EnetThreshSetValue/sec
		  linkOn(5).......The link status of the port
		                    has changed to ON
		  linkOff(6)......The link status of the port
		                    has changed to OFF
		  overRatio(7)....The ratio in
		                    s3EnetThreshActualValue is
		                    greater than
		                    s3EnetThreshSetValue.
		                    Both values are in units of
		                    0.01% (i.e., 100 equals 1.0%)

		The values that the object s3EnetThreshCondition
		can have is actually dependent on the value of the
		object s3EnetThreshType.  The table below shows
		the valid combinations between the two objects.

		If s3EnetThreshType      Allowed Values For
		    Is Equal To        s3EnetThreshCondition Are
		===================    =========================
		  goodBytes(2)                  2, 3, 4
		  goodPkts(3)                   2, 3, 4
		  badPkts(4)                    2, 3, 4
		  crcPkts(5)                    2, 3, 4
		  misaligned(6)                 2, 3, 4
		  runtPkts(7)                   2, 3, 4
		  fragPkts(8)                   2, 3, 4
		  tooLong(9)                    2, 3, 4
		  collision(10)                 2, 3, 4
		  lateColls(11)                 2, 3, 4
		  linkStatus(12)                5, 6
		  multicast(13)                 2, 3, 4
		  broadcast(14)                 2, 3, 4
		  shortEvents(15)               2, 3, 4
		  srcAddrChanges(16)            2, 3, 4
		  dataRateMismatches(17)        2, 3, 4
		  networkErrors(18)             2, 3, 4
		  badToGoodPktRatio(19)         7
		  netErrToGoodPktRatio(20)      7
		  colltoGoodPktRatio(21)        7
		  collBackOffErr(22)            2, 3, 4

		When the condition specified is crossValue(2) or
		overValue(3), the value of s3EnetThreshActualValue
		is accumulated from the beginning of the duration
		window and is checked every 5 seconds.

		When the condition specified is overRate(4) or
		overRatio(5), and the duration is less than or
		equal to 5 seconds, the value of
	        s3EnetThreshActualValue is based on the data
		accumulated during the 5 second sampling period.

		When the condition specified is overRate(4) or
		overRatio(5), and the duration is greater than
		5 seconds, the value of s3EnetThreshActualValue
		is based on the data accumulated during the
		entire duration window."
	::= { s3EnetThreshEntry 7 }

s3EnetThreshSetValue OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"Threshold setting value."
	::= { s3EnetThreshEntry 8 }

s3EnetThreshActualValue OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Current value of the threshold counter.  This
		object is set to zero at the begining of each
		duration window."
	::= { s3EnetThreshEntry 9 }

s3EnetThreshAction OBJECT-TYPE
	SYNTAX  INTEGER {
		other(1),
		noAction(2),
		sendTrap(3),
		res4(4),
		res5(5),
		partSlot(6),
		partSlotPort(7),
		res8(8),
		res9(9),
		trapPartSlot(10),
		trapPartSlotPort(11)
		}
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"Determines what action is to take place if the
		threshold condition occurs.  The possible values
		that can be read and written are listed below.

		Applicable to ALL Thresholds
		==============================================
		  noAction(2)............Take no action
		  sendTrap(3)............Send a trap


		Applicable ONLY to Port Thresholds
		==============================================
		  partSlot(6)............Partition the slot
		                          identified by
		                          s3EnetThreshSlot
		  partSlotPort(7)........Partition the port
		                          identified by
		                          s3EnetThreshSlot and
		                          s3EnetThreshPort

		Applicable ONLY to Slot Thresholds
		==============================================
		  trapPartSlot(10).......Send a trap and
		                           partition the slot
		                           identified by
		                           s3EnetThreshSlot
		  trapPartSlotPort(11)...Send a trap and
		                           partition the port
		                           identified by
		                           s3EnetThreshSlot and
		                           s3EnetThreshPort

		Notes:  1.) The value other(1) can only be
		            read and it indicates the entry
		            has an invalid or unknown threshold
		            action.

		        2.) The values res4(4), res5(5), res8(8),
		            and res9(9) are no longer used and
		            should never be read or written.

		The timing and frequency of the action taken when
		the threshold condition is met is dependent upon
		the type of condition (i.e., s3EnetThreshCondition)
		and the length of the duration window (i.e.,
		s3EnetThreshDuration).

		If the threshold conditionÊis crossValue(2), the
		action will be taken only ONCE during the duration
		window at the sampling period the condition is
		first met.

		If the threshold condition is overValue(3),
		linkOn(5), or linkOff(6), the action will be
		taken at each sampling period the condition
		is met until the end of the duration window.

		If the threshold condition is overRate(4) or
		overRatio(5) the action will be taken only ONCE
		at the end of the duration window if the
		condition is met."
	::= { s3EnetThreshEntry 10 }

s3EnetThreshExceedCount OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Counter for how many times the selected threshold
		has reached its setting value."
	::= { s3EnetThreshEntry 11 }

s3EnetThreshDuration OBJECT-TYPE
	SYNTAX	TimeTicks
	ACCESS	read-write
	STATUS	mandatory
	DESCRIPTION
		"Length of window over which threshold counts
		are summed, specified in intervals of 500
		TimeTicks (i.e., 5 seconds).  This window is
		broken down into 5 second sampling periods
		for purposes of checking the threshold
		conditions, and determining when the actions
		specified need to take place when the condition
		occurs.

		If this object is written with a value that is
		not evenly divisible by 500, the agent will
		internally round the value up to the closest
		integral of 500 before it is used in threshold
		calculations (i.e., a value of 12 can be
		written, but will be interpreted as 15).

		Notes:  1.) A value of zero indicates an
		            infinite duration window if the
		            value of s3EnetThreshCondition
		            is crossValue(2) or overValue(3).

		        2.) If the value of
		            s3EnetThreshCondition is
		            overRate(4) or overRatio(5),
	                    a value of zero is equivalent
		            to a duration window of 5
		            seconds.

		        3.) If the value of s3EnetThreshType
		            is linkStatus(12), this value of
		            this object is ignore and assumed
		            to be infinite."
	::= { s3EnetThreshEntry 12 }

s3EnetThreshTableSize OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The maximum number of entries in the table
		s3EnetThreshTable."
	::= { s3000EnetThreshold 2 }


-- SECTION 7: Traffic Matrix Group


-- This group consists of the SA-DA and the DA-SA tables

-- Implementation of this group is mandatory for all
--   SynOptics Series 3000 Ethernet agents


-- SA-DA Table

s3EnetSdTrafTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetSdTrafEntry
	ACCESS	not-accessible
	STATUS	deprecated
	DESCRIPTION
		"This table contains a list of entries which provide
		SA-DA traffic information.  Specifically  frame and
		byte counter values are provided per unique SA-DA
		pair.  The indexing scheme of this table allows an
		SA list to be retrieved using GETNEXT.  An SA list
		is a list of entries that have a common SA, however,
		different DAs."
	::= { s3000EnetSADATraffic 1 }

s3EnetSdTrafEntry OBJECT-TYPE
	SYNTAX	S3EnetSdTrafEntry
	ACCESS	not-accessible
	STATUS	deprecated
	DESCRIPTION
		"An entry in the SA-DA traffic table."
	INDEX	{ s3EnetSdTrafMacSA,
		 s3EnetSdTrafMacDA}
	::= { s3EnetSdTrafTable 1  }

S3EnetSdTrafEntry ::= SEQUENCE {
	s3EnetSdTrafMacSA
		PhysAddress,
	s3EnetSdTrafMacDA
		PhysAddress,
	s3EnetSdTrafFrames
		Counter,
	s3EnetSdTrafBytes
		Counter
	}

s3EnetSdTrafMacSA OBJECT-TYPE
	SYNTAX	PhysAddress (SIZE(6))
	ACCESS	read-only
	STATUS	deprecated
	DESCRIPTION
		"Source MAC address."
	::= { s3EnetSdTrafEntry 1 }

s3EnetSdTrafMacDA OBJECT-TYPE
	SYNTAX	PhysAddress (SIZE(6))
	ACCESS	read-only
	STATUS	deprecated
	DESCRIPTION
		"Destination MAC address."
	::= { s3EnetSdTrafEntry 2 }

s3EnetSdTrafFrames OBJECT-TYPE
	SYNTAX	Counter	
	ACCESS	read-only
	STATUS	deprecated
	DESCRIPTION
		"The number of good frames received by the concentrator
		for a SA-DA pair."
 	::= { s3EnetSdTrafEntry 3 }

s3EnetSdTrafBytes OBJECT-TYPE
	SYNTAX	Counter	
	ACCESS	read-only
	STATUS	deprecated
	DESCRIPTION
		"The number of bytes in good frames received by the
		concentrator for a SA-DA pair."
	::= { s3EnetSdTrafEntry 4 }



-- DA-SA Table

s3EnetDsTrafTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetDsTrafEntry
	ACCESS	not-accessible
	STATUS	deprecated
	DESCRIPTION
		"This table contains a list of entries which provide
		DA-SA traffic information.  Specifically frame and
		byte counter values are provided per unique DA-SA
		pair.  The indexing scheme of this table allows a
		DA list to be retrieved using GETNEXT.  A DA list
		is a list of entries that have a common DA, however,
		different SAs."
	::= { s3000EnetSADATraffic 2 }

s3EnetDsTrafEntry OBJECT-TYPE
	SYNTAX	S3EnetDsTrafEntry
	ACCESS	not-accessible
	STATUS	deprecated
	DESCRIPTION
		"An entry in the DA-SA table."
	INDEX	{ s3EnetDsTrafMacDA,
		 s3EnetDsTrafMacSA }
	::= { s3EnetDsTrafTable 1 }

S3EnetDsTrafEntry ::= SEQUENCE {
	s3EnetDsTrafMacDA
		PhysAddress,
	s3EnetDsTrafMacSA
		PhysAddress,
	s3EnetDsTrafFrames
		Counter,
	s3EnetDsTrafBytes
		Counter
	}

s3EnetDsTrafMacDA OBJECT-TYPE
	SYNTAX	PhysAddress (SIZE(6))	
	ACCESS	read-only
	STATUS	deprecated
	DESCRIPTION	
		"Destination MAC address."
	::= { s3EnetDsTrafEntry 1}

s3EnetDsTrafMacSA OBJECT-TYPE
	SYNTAX	PhysAddress (SIZE(6))	
	ACCESS	read-only
	STATUS	deprecated
	DESCRIPTION	
		"Source MAC address."
	::= { s3EnetDsTrafEntry 2 }

s3EnetDsTrafFrames OBJECT-TYPE
	SYNTAX	Counter	
	ACCESS	read-only
	STATUS	deprecated
	DESCRIPTION	
		"The number of good frames received by the concentrator
		for a DA-SA pair."
	::= { s3EnetDsTrafEntry 3 }

s3EnetDsTrafBytes OBJECT-TYPE
	SYNTAX	Counter	
	ACCESS	read-only
	STATUS	deprecated
	DESCRIPTION
		"The number of bytes in good frames received by the
		concentrator for a DA-SA pair."
	::= { s3EnetDsTrafEntry 4 }



-- Paged Traffic Matrix Table

s3EnetPagedTrafTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetPagedTrafEntry
	ACCESS	not-accessible
	STATUS	deprecated
	DESCRIPTION
		"This table contains a list of entries for the 'paged'
		Traffic Matrix table."
	::= { s3000EnetSADATraffic 3 }

s3EnetPagedTrafEntry OBJECT-TYPE
	SYNTAX	S3EnetPagedTrafEntry
	ACCESS	not-accessible
	STATUS	deprecated
	DESCRIPTION
		"A 'paged' entry in the Traffic Matrix table."
	INDEX	{ s3EnetTrafPageNo }
	::= {s3EnetPagedTrafTable 1 }

S3EnetPagedTrafEntry ::= SEQUENCE {
	s3EnetTrafPageNo
		INTEGER,
	s3EnetTrafPageEntries
		OCTET STRING
	}

s3EnetTrafPageNo OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	deprecated
	DESCRIPTION
		"A specific page in the Traffic Matrix table."
	::= { s3EnetPagedTrafEntry 1 }

s3EnetTrafPageEntries  OBJECT-TYPE
	SYNTAX	OCTET STRING (SIZE (1..400))
	ACCESS	read-only
	STATUS	deprecated
	DESCRIPTION
		"This OCTET STRING contains up to 20 valid Traffic
		Matrix table entries. The entries will not be in any
		logical order. Each entry consists of a 20-byte octet
		string including a 6-byte source MAC address, a 6-byte
		destination MAC address, a received good frame count,
		and a byte count in good frames received. The counters
		are 4-bytes each where the first one is high-order byte
		and the last one is low-order byte."
	::= { s3EnetPagedTrafEntry 2 }

s3EnetTrafAgeInterval OBJECT-TYPE
	SYNTAX	TimeTicks
	ACCESS	read-write
	STATUS	deprecated
	DESCRIPTION
		"The time used for aging of the nodes in tables
		s3EnetSdTrafTable and s3EnetDsTrafTable.
		Once a node has completely aged it will be
		removed from these tables.

		Note:
		Agents that do not implement this object
		(i.e., agents prior to version 5.3) use the
		object s3EnetNodeAgeInterval to perform this
		function."
	::= { s3000EnetSADATraffic 4 }

-- SECTION 8: Ethernet "PLUS" Statistics Group


-- This group consists of a port table, board table, and
--   concentrator group.

-- This group is mandatory for 3313S and 3314S NMMs agents.
--   This group is not implemented by other agents.


-- Port "PLUS" Statistics Table

s3EnetPlusPortTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetPlusPortEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"This table provides a list of entries, each entry
		providing information related to frame MAC level
		error conditions per port. This table is conceptually
		an extension to the s3EnetPortTable and is
		only implemented by the 3313S and 3314S NMMs."
	::= { s3000EnetPlusStatistics 1 }

s3EnetPlusPortEntry OBJECT-TYPE
	SYNTAX	S3EnetPlusPortEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"An entry in the Plus Port table."
	INDEX	{ s3EnetPlusPortBoardIndex,
		 s3EnetPlusPortIndex }
	::= { s3EnetPlusPortTable 1 }

S3EnetPlusPortEntry ::= SEQUENCE {
	s3EnetPlusPortBoardIndex
		INTEGER,
	s3EnetPlusPortIndex
		INTEGER,
	s3EnetPortFragments
		Counter,
	s3EnetPortShortEvents
		Counter,
	s3EnetPortAutoPartitions
		Counter,
	s3EnetPortRateMismatches
		Counter,
	s3EnetPortJabbers
		Counter,
	s3EnetPortLastSrcAddr
		PhysAddress,
	s3EnetPortSrcAddrChanges
		Counter
	}

s3EnetPlusPortBoardIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"A unique value for each board.  Its value ranges between
		1 and 12.  (This is the slot number.)"
	::= { s3EnetPlusPortEntry 1 }

s3EnetPlusPortIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"A unique value for each port.  Its value typically ranges
		between 1 and 12."
	::= { s3EnetPlusPortEntry 2 }

s3EnetPortFragments OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of fragments received by the
		board between 80-512 bits (64 bytes), inclusively,
		with invalid FCS or alignment errors.  (These
		commonly represent collision fragments, and are
		not errors.  Collision fragments were called
		FragErrors in the rev 3.x MIB, and were counted
		only on a per-board basis.)"
	::= { s3EnetPlusPortEntry 3 }

s3EnetPortShortEvents OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of fragments received by the
		port shorter than 80 bits."
	::= { s3EnetPlusPortEntry 4 }

s3EnetPortAutoPartitions OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of times the ports on the board
		have autopartitioned due to excessive collisions (more
		than 32 consecutive collisions).  This count is an
		approximation and may be less than the total count."
	::= { s3EnetPlusPortEntry 5 }

s3EnetPortRateMismatches OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of the occurrences of out of
		spec bit rates.  This indicates the number of times
		FIFO buffer over-runs or underruns due to transmission
		rate errors."
	::= { s3EnetPlusPortEntry 6 }

s3EnetPortJabbers OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of the times that MAU jabber
		lockup protection (MJLP) was invoked because transmission
		of data from this port exceeded 5 msec in duration.
		This information can be useful in identifying faulty
		stations."
	::= { s3EnetPlusPortEntry 7 }

s3EnetPortLastSrcAddr OBJECT-TYPE
	SYNTAX	PhysAddress (SIZE(6))
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This is the source address of the last packet
		received through this port."
	::={ s3EnetPlusPortEntry 8 }

s3EnetPortSrcAddrChanges OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This is the number of times that the
		s3EnetPortLastSrcAddr object for this has changed."
	::={ s3EnetPlusPortEntry 9 }



-- Board "PLUS" Statistics Table


s3EnetPlusBoardTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetPlusBoardEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"This table provides a list of entries, each entry
		providing information related to frame MAC level
		error conditions per board.  This table is conceptually
		an extension to the s3EnetboardTable and is
		only implemented by the 3313S and 3314S NMMs."
	::= { s3000EnetPlusStatistics 2 }

s3EnetPlusBoardEntry OBJECT-TYPE
	SYNTAX	S3EnetPlusBoardEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"An entry in the Plus Board table."
	INDEX	{ s3EnetPlusBoardIndex }
	::= { s3EnetPlusBoardTable 1 }

S3EnetPlusBoardEntry ::= SEQUENCE {
	s3EnetPlusBoardIndex
		INTEGER,
	s3EnetBoardFragments
		Counter,
	s3EnetBoardShortEvents
		Counter,
	s3EnetBoardAutoPartitions
		Counter,
	s3EnetBoardRateMismatches
		Counter,
	s3EnetBoardJabbers
		Counter
	}

s3EnetPlusBoardIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The board number part of an index."
	::= { s3EnetPlusBoardEntry 1 }

s3EnetBoardFragments OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of fragments received by the
		board between 80-512 bits (64 bytes), inclusively,
		with invalid FCS or alignment errors.  (These
		commonly represent collision fragments, and are
		not errors.  Collision fragments were called
		FragErrors in the rev 3.x MIB, and were counted
		only on a per-concentrator basis.)"
	::= { s3EnetPlusBoardEntry 2 }

s3EnetBoardShortEvents OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of fragments received by
		the board shorter than 80 bits."
	::= { s3EnetPlusBoardEntry 3 }

s3EnetBoardAutoPartitions OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of times the ports on this
		board have been autopartitioned due to excessive
		collisions (more than 32 consecutive collisions).
		This count is an approximation and may be less than
		the total count."
	::= { s3EnetPlusBoardEntry 4 }

s3EnetBoardRateMismatches OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of the occurrences of out of
		spec bit rates.  This indicates the number of times
		FIFO buffer over-runs or underruns due to
		transmission rate errors."
	::= { s3EnetPlusBoardEntry 5 }

s3EnetBoardJabbers OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of the times that MAU jabber
		lockup protection (MJLP) was invoked because
		transmission of data from a port on this board
		exceeded 5 msec in duration.  This information can
		be useful in identifying faulty stations."
	::= { s3EnetPlusBoardEntry 6 }



-- Concentrator "PLUS" Statistics Group


-- This group is conceptually an extension to the
--   s3000EnetConcentrator group and is only implemented by the
--   3313S and 3314S NMMs.

s3EnetConcShortEvents OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of fragments received by
		the concentrator shorter than 80 bits."
	::= { s3000EnetPlusConc 1 }

s3EnetConcAutoPartitions OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of times the ports on this
		concentrator have been autopartitioned due to
		excessive collisions (more than 32 consecutive
		collisions).  This count is based on a one-bit
		counter (flag) per port in the host modules, and
		will not always represent the total count."
	::= { s3000EnetPlusConc 2}

s3EnetConcRateMismatches OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of the occurrences of out
		of spec bit rates.  This indicates the number of
		times FIFO buffer over-runs or underruns due to
		transmission rate errors."
	::= { s3000EnetPlusConc 3 }

s3EnetConcJabbers OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of the times that MAU jabber
		lockup protection (MJLP) was invoked because
		transmission of data from a port on this
		concentrator exceeded 5 msec in duration.
		This information can be useful in identifying
		faulty stations."
	::= { s3000EnetPlusConc 4 }

s3EnetConcCollBackoffErrors OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a total concentrator count of the
		collision events that occur during the normal
		collision window (i.e., the collisions is not
		a late collision) and do not have a runt error."
	::= { s3000EnetPlusConc 5 }



-- SECTION 9: Frame Size Distribution Group


-- This group consists of a port table, board table, and concentrator group.

-- This group is mandatory for 3313S and 3314S NMMs agents.
--   This group is not implemented by other agents.


-- Port Frame Size Table

s3EnetFrSizePortTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetFrSizePortEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"This table provides a list of entries, each entry
		providing information related to frame sizes of
		packets received on a port.  The variables
		defined for the entries are only supported
		by 3313S and 3314S NMM."
	::= { s3000EnetFrameSizeDist 1 }

s3EnetFrSizePortEntry OBJECT-TYPE
	SYNTAX	S3EnetFrSizePortEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"An entry in the FrSize Port table."
	INDEX	{ s3EnetFrSizePortBoardIndex,
		 s3EnetFrSizePortIndex }
	::= { s3EnetFrSizePortTable 1 }

S3EnetFrSizePortEntry ::= SEQUENCE {
	s3EnetFrSizePortBoardIndex
		INTEGER,
	s3EnetFrSizePortIndex
		INTEGER,
	s3EnetFrSizePort64to127
		Counter,
	s3EnetFrSizePort128to255
		Counter,
	s3EnetFrSizePort256to511
		Counter,
	s3EnetFrSizePort512to1023
		Counter,
	s3EnetFrSizePort1024to1518
		Counter
	}

s3EnetFrSizePortBoardIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"A unique value for each board.  Its value ranges
		between 1 and 12.  (This is the slot number.)"
	::= { s3EnetFrSizePortEntry 1 }

s3EnetFrSizePortIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"A unique value for each port.  Its value typically
		ranges between 1 and 12."
	::= { s3EnetFrSizePortEntry 2 }

s3EnetFrSizePort64to127 OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		port that are in the range of 64 octets to 127
		octets, inclusive."
	::= { s3EnetFrSizePortEntry 3 }

s3EnetFrSizePort128to255 OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		port that are in the range of 128 octets to 255
		octets, inclusive."
	::= { s3EnetFrSizePortEntry 4 }


s3EnetFrSizePort256to511 OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		port that are in the range of 256 octets to 511
		octets, inclusive."
	::= { s3EnetFrSizePortEntry 5 }

s3EnetFrSizePort512to1023 OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		port that are in the range of 512 octets to 1023
		octets, inclusive."
	::= { s3EnetFrSizePortEntry 6 }

s3EnetFrSizePort1024to1518 OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		port that are in the range of 1024 octets to 1518
		octets, inclusive."
	::= { s3EnetFrSizePortEntry 7 }



-- Board Frame Size Table


s3EnetFrSizeBoardTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetFrSizeBoardEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"This table provides a list of entries, each entry
		providing information related to frame MAC level
		error conditions per board.  The variables defined
		for the entries are only supported by 3313S and
		3314S NMMs.  The use of any variable in this table
		for other NMMs will cause the NMMs to return
		noSuchName error status in the response."
	::= { s3000EnetFrameSizeDist 2 }

s3EnetFrSizeBoardEntry OBJECT-TYPE
	SYNTAX	S3EnetFrSizeBoardEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"An entry in the FrSize Board table."
	INDEX	{ s3EnetFrSizeBoardIndex }
	::= { s3EnetFrSizeBoardTable 1 }

S3EnetFrSizeBoardEntry ::= SEQUENCE {
	s3EnetFrSizeBoardIndex
		INTEGER,
	s3EnetFrSizeBoard64to127
		Counter,
	s3EnetFrSizeBoard128to255
		Counter,
	s3EnetFrSizeBoard256to511
		Counter,
	s3EnetFrSizeBoard512to1023
		Counter,
	s3EnetFrSizeBoard1024to1518
		Counter
	}

s3EnetFrSizeBoardIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"A unique value for each board.  Its value ranges between
		1 and 12.  (This is the slot number.)"
	::= { s3EnetFrSizeBoardEntry 1 }

s3EnetFrSizeBoard64to127 OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		board that are in the range of 64 octets to 127
		octets, inclusive."
	::= { s3EnetFrSizeBoardEntry 2 }

s3EnetFrSizeBoard128to255 OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		board that are in the range of 128 octets to 255
		octets, inclusive."
	::= { s3EnetFrSizeBoardEntry 3 }


s3EnetFrSizeBoard256to511 OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		board that are in the range of 256 octets to 511
		octets, inclusive."
	::= { s3EnetFrSizeBoardEntry 4 }

s3EnetFrSizeBoard512to1023 OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		board that are in the range of 512 octets to 1023
		octets, inclusive."
	::= { s3EnetFrSizeBoardEntry 5 }

s3EnetFrSizeBoard1024to1518 OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		board that are in the range of 1024 octets to 1518
		octets, inclusive."
	::= { s3EnetFrSizeBoardEntry 6 }



-- Concentrator Frame Size Group


-- This group is mandatory for 3313S and 3314S NMMs agents.
--   This group does not exist in other agents.

s3EnetFrSizeConc64to127 OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		concentrator that are in the range of 64 octets to 127
		octets, inclusive."
	::= { s3000EnetFrameConc 1 }

s3EnetFrSizeConc128to255 OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		concentrator that are in the range of 128 octets to 255
		octets, inclusive."
	::= { s3000EnetFrameConc 2 }


s3EnetFrSizeConc256to511 OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		concentrator that are in the range of 256 octets to 511
		octets, inclusive."
	::= { s3000EnetFrameConc 3 }

s3EnetFrSizeConc512to1023 OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		concentrator that are in the range of 512 octets to 1023
		octets, inclusive."
	::= { s3000EnetFrameConc 4 }

s3EnetFrSizeConc1024to1518 OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		concentrator that are in the range of 1024 octets to 1518
		octets, inclusive."
	::= { s3000EnetFrameConc 5 }



-- SECTION 10: Protocol Type Group


-- This group consists of a port table, board table, and concentrator
--   group.

-- This group is mandatory for 3313S and 3314S NMMs agents.  This group
--   does not exist in other agents.

-- Each good frame is counted as either 802.3 or Ethernet, and also
--   counted under one of the more specific protocol type categories.
--   If it does not fit into one of the more specific categories, it is
--   counted as an "other" protocol type.

-- Port Protocol Type Table

s3EnetProtoPortTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetProtoPortEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"This table provides a list of entries, each entry
		providing information related to packet protocol
		type distributions per port.  The variables defined
		for the entries are only supported by 3313S and
		3314S NMMs.  The use of any variable in this table
		for other NMMs will cause the NMMs to return
		noSuchName error status in the response."
	::= { s3000EnetProtoTypeDist 1 }

s3EnetProtoPortEntry OBJECT-TYPE
	SYNTAX	S3EnetProtoPortEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"An entry in the Proto Port table."
	INDEX	{ s3EnetProtoPortBoardIndex,
		 s3EnetProtoPortIndex }
	::= { s3EnetProtoPortTable 1 }

S3EnetProtoPortEntry ::= SEQUENCE {
	s3EnetProtoPortBoardIndex
		INTEGER,
	s3EnetProtoPortIndex
		INTEGER,
	s3EnetProtoPort8023Frames
		Counter,
	s3EnetProtoPortEthernetFrames
		Counter,
	s3EnetProtoPortOtherFrames
		Counter,
	s3EnetProtoPortSnaFrames
		Counter,
	s3EnetProtoPortIpFrames
		Counter,
	s3EnetProtoPortIsoFrames
		Counter,
	s3EnetProtoPortArpFrames
		Counter,
	s3EnetProtoPortDecIVFrames
		Counter,
	s3EnetProtoPortDecLatFrames
		Counter,
	s3EnetProtoPortEthTalkFrames
		Counter,
	s3EnetProtoPortXnsFrames
		Counter,
	s3EnetProtoPortIpxFrames
		Counter,
	s3EnetProtoPortDecLavcFrames
		Counter,
	s3EnetProtoPortNetBiosFrames
		Counter,
	s3EnetProtoPortBrdgSpanTreeFrames
		Counter
	}

s3EnetProtoPortBoardIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"A unique value for each board.  Its value ranges between
		1 and 12.  (This is the slot number.)"
	::= { s3EnetProtoPortEntry 1 }

s3EnetProtoPortIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"A unique value for each port.  Its value typically ranges
		between 1 and 12."
	::= { s3EnetProtoPortEntry 2 }

s3EnetProtoPort8023Frames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		port that are of 802.3 type."
	::= { s3EnetProtoPortEntry 3 }

s3EnetProtoPortEthernetFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		port that are of Ethernet type."
	::= { s3EnetProtoPortEntry 4 }

s3EnetProtoPortOtherFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		port that are of types not counted by individual
		counters below."
	::= { s3EnetProtoPortEntry 5 }

s3EnetProtoPortSnaFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		port that are of SNA type."
	::= { s3EnetProtoPortEntry 6 }

s3EnetProtoPortIpFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		port that are of IP type."
	::= { s3EnetProtoPortEntry 7 }

s3EnetProtoPortIsoFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		port that are of ISO type."
	::= { s3EnetProtoPortEntry 8 }

s3EnetProtoPortArpFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		port that are of ARP type."
	::= { s3EnetProtoPortEntry 9 }

s3EnetProtoPortDecIVFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		port that are of DECIV type."
	::= { s3EnetProtoPortEntry 10 }

s3EnetProtoPortDecLatFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		port that are of DECLAT type."
	::= { s3EnetProtoPortEntry 11 }

s3EnetProtoPortEthTalkFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		port that are of EtherTalk type."
	::= { s3EnetProtoPortEntry 12 }

s3EnetProtoPortXnsFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		port that are of XNS type."
	::= { s3EnetProtoPortEntry 13 }

s3EnetProtoPortIpxFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		port that are of IPX type."
	::= { s3EnetProtoPortEntry 14 }

s3EnetProtoPortDecLavcFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		port that are of DEC LAVC type."
	::= { s3EnetProtoPortEntry 15 }

s3EnetProtoPortNetBiosFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		port that are of NETBIOS type."
	::= { s3EnetProtoPortEntry 16 }

s3EnetProtoPortBrdgSpanTreeFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		port that are of Bridge Spanning Tree type."
	::= { s3EnetProtoPortEntry 17 }

-- Board Protocol Type Table


s3EnetProtoBoardTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetProtoBoardEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"This table provides a list of entries, each entry
		providing information related to packet protocol
		type distribution per board.  The variables defined
		for the entries are only supported by 3313S and
		3314S NMMs.  The use of any variable in this table
		for other NMMs will cause the NMMs to return
		noSuchName error status in the response."
	::= { s3000EnetProtoTypeDist 2 }

s3EnetProtoBoardEntry OBJECT-TYPE
	SYNTAX	S3EnetProtoBoardEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"An entry in the Proto Board table."
	INDEX	{ s3EnetProtoBoardIndex }
	::= { s3EnetProtoBoardTable 1 }

S3EnetProtoBoardEntry ::= SEQUENCE {
	s3EnetProtoBoardIndex
		INTEGER,
	s3EnetProtoBoard8023Frames
		Counter,
	s3EnetProtoBoardEthernetFrames
		Counter,
	s3EnetProtoBoardOtherFrames
		Counter,
	s3EnetProtoBoardSnaFrames
		Counter,
	s3EnetProtoBoardIpFrames
		Counter,
	s3EnetProtoBoardIsoFrames
		Counter,
	s3EnetProtoBoardArpFrames
		Counter,
	s3EnetProtoBoardDecIVFrames
		Counter,
	s3EnetProtoBoardDecLatFrames
		Counter,
	s3EnetProtoBoardEthTalkFrames
		Counter,
	s3EnetProtoBoardXnsFrames
		Counter,
	s3EnetProtoBoardIpxFrames
		Counter,
	s3EnetProtoBoardDecLavcFrames
		Counter,
	s3EnetProtoBoardNetBiosFrames
		Counter,
	s3EnetProtoBoardBrdgSpanTreeFrames
		Counter
	}

s3EnetProtoBoardIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"A unique value for each board.  Its value ranges between
		1 and 12.  (This is the slot number.)"
	::= { s3EnetProtoBoardEntry 1 }

s3EnetProtoBoard8023Frames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		board that are of 802.3 type."
	::= { s3EnetProtoBoardEntry 2 }

s3EnetProtoBoardEthernetFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		board that are of Ethernet type."
	::= { s3EnetProtoBoardEntry 3 }

s3EnetProtoBoardOtherFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		board that are of types not specified below."
	::= { s3EnetProtoBoardEntry 4 }

s3EnetProtoBoardSnaFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		board that are of SNA type."
	::= { s3EnetProtoBoardEntry 5 }

s3EnetProtoBoardIpFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		board that are of IP type."
	::= { s3EnetProtoBoardEntry 6 }

s3EnetProtoBoardIsoFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		board that are of ISO type."
	::= { s3EnetProtoBoardEntry 7 }

s3EnetProtoBoardArpFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		board that are of ARP type."
	::= { s3EnetProtoBoardEntry 8 }

s3EnetProtoBoardDecIVFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		board that are of DECIV type."
	::= { s3EnetProtoBoardEntry 9 }

s3EnetProtoBoardDecLatFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		board that are of DECLAT type."
	::= { s3EnetProtoBoardEntry 10 }

s3EnetProtoBoardEthTalkFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		board that are of EtherTalk type."
	::= { s3EnetProtoBoardEntry 11 }

s3EnetProtoBoardXnsFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		board that are of XNS type."
	::= { s3EnetProtoBoardEntry 12 }

s3EnetProtoBoardIpxFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		board that are of IPX type."
	::= { s3EnetProtoBoardEntry 13 }

s3EnetProtoBoardDecLavcFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		board that are of DEC LAVC type."
	::= { s3EnetProtoBoardEntry 14 }

s3EnetProtoBoardNetBiosFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		board that are of NETBIOS type."
	::= { s3EnetProtoBoardEntry 15 }

s3EnetProtoBoardBrdgSpanTreeFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		board that are of Bridge Spanning Tree type."
	::= { s3EnetProtoBoardEntry 16 }



-- Concentrator Protocol Type Group

-- This group is mandatory for 3313S and 3314S NMMs agents.
--   This group does not exist in other agents.

s3EnetProtoConc8023Frames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		concentrator that are of 802.3 type."
	::= { s3000EnetProtoConc 1 }

s3EnetProtoConcEthernetFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		concentrator that are of Ethernet type."
	::= { s3000EnetProtoConc 2 }

s3EnetProtoConcOtherFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		concentrator that are of types not specified below."
	::= { s3000EnetProtoConc 3 }

s3EnetProtoConcSnaFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		concentrator that are of SNA type."
	::= { s3000EnetProtoConc 4 }

s3EnetProtoConcIpFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		concentrator that are of IP type."
	::= { s3000EnetProtoConc 5 }

s3EnetProtoConcIsoFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		concentrator that are of ISO type."
	::= { s3000EnetProtoConc 6 }

s3EnetProtoConcArpFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		concentrator that are of ARP type."
	::= { s3000EnetProtoConc 7 }

s3EnetProtoConcDecIVFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		concentrator that are of DECIV type."
	::= { s3000EnetProtoConc 8 }

s3EnetProtoConcDecLatFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		concentrator that are of DECLAT type."
	::= { s3000EnetProtoConc 9 }

s3EnetProtoConcEthTalkFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		concentrator that are of EtherTalk type."
	::= { s3000EnetProtoConc 10 }

s3EnetProtoConcXnsFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		concentrator that are of XNS type."
	::= { s3000EnetProtoConc 11}

s3EnetProtoConcIpxFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		concentrator that are of IPX type."
	::= { s3000EnetProtoConc 12 }

s3EnetProtoConcDecLavcFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		concentrator that are of DEC LAVC type."
	::= { s3000EnetProtoConc 13 }

s3EnetProtoConcNetBiosFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		concentrator that are of NETBIOS type."
	::= { s3000EnetProtoConc 14 }

s3EnetProtoConcBrdgSpanTreeFrames OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"This contains a count of frames received by the
		concentrator that are of Bridge Spanning Tree type."
	::= { s3000EnetProtoConc 15 }



-- SECTION 11: Host Group


-- Host Table

s3EnetHostTableSize OBJECT-TYPE
	SYNTAX	INTEGER (0..65535)
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The current number of entries in table s3EnetHostTable."
	::= { s3000EnetHosts 1 }

s3EnetHostLastDeleteTime OBJECT-TYPE
	SYNTAX	TimeTicks
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The value of sysUpTime when the last entry was
		deleted from table s3EnetHostTable due to a shortage
		of resources. If no deletions have occurred, then
		the value is zero."
	::= { s3000EnetHosts 2 }

s3EnetHostTable OBJECT-TYPE
	SYNTAX	SEQUENCE OF S3EnetHostEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"A Table containing MAC/Network address pairs
		that have been detected on the segment."
	::= { s3000EnetHosts 3 }

s3EnetHostEntry	OBJECT-TYPE
	SYNTAX	S3EnetHostEntry
	ACCESS	not-accessible
	STATUS	mandatory
	DESCRIPTION
		"A row in the table of MAC/Network address
		pairs. Entries can not be created or deleted
		via SNMP operations. New entries are added when
		a new MAC/Network address pair is detected.
		An entry is removed to add a new entry when
		the table is full. The entry that is removed is
		the one that has been least recently observed."
	INDEX	{ s3EnetHostIndex }
	::= { s3EnetHostTable 1 }

S3EnetHostEntry ::= SEQUENCE {
	s3EnetHostIndex INTEGER,
	s3EnetHostObserveOrder INTEGER,
	s3EnetHostNetAddr OCTET STRING,
	s3EnetHostAddrType INTEGER,
	s3EnetHostMacAddress PhysAddress,
	s3EnetHostSlotIndex INTEGER,
	s3EnetHostPortIndex INTEGER,
	s3EnetHostLearnMethod INTEGER,
	s3EnetHostTimeStamp TimeTicks
	}

s3EnetHostIndex OBJECT-TYPE
	SYNTAX	INTEGER (1..65535)
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The index of the MAC/Network address pair.
		The value is between 1 and N, where N is the value
		of s3EnetHostTableSize. The association of this
		index to a pair may change when a pair is removed
		from the table due to a resource shortage.
		s3EnetHostLastDeleteTime must be monitored to
		determine when this condition has occured."
	::= { s3EnetHostEntry 1 }

s3EnetHostObserveOrder OBJECT-TYPE
	SYNTAX	INTEGER (1..65535)
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The relative ordering of the MAC/Network adddress
		pair. There is a global value that starts at 1 and
		increases by one for each observation of an address
		pair. When the maximum value of 65535 is reached,
		the next value will be 1. The global value is used
		to update this object each time the MAC/Network address
		pair is observed (and when the entry is initially
		created). Since the global value starts over again
		after it reaches its maximum value, there may be
		more than one entry that has the same value."
	::= { s3EnetHostEntry 2 }

s3EnetHostNetAddr OBJECT-TYPE
	SYNTAX	OCTET STRING
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The network address (in network order) of the
		MAC/Network address pair."
	::= { s3EnetHostEntry 3 }

s3EnetHostAddrType OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),
		ip(2),
		ipx(3)
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The type of address that is stored in the object
		s3EnetHostNetAddr for this entry. The values are:
		  other(1)...Unknown type
		  ip(2)......IP address
		  ipx(3).....IPX address"
	::= { s3EnetHostEntry 4 }

s3EnetHostMacAddress OBJECT-TYPE
	SYNTAX	PhysAddress (SIZE(6))
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The MAC address (in canonical order) of the
		MAC/Network address pair."
	::= { s3EnetHostEntry 5 }

s3EnetHostSlotIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The board index that the host is connected through."
	::= { s3EnetHostEntry 6 }

s3EnetHostPortIndex OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The port index that the host is connected through."
	::= { s3EnetHostEntry 7 }

s3EnetHostLearnMethod OBJECT-TYPE
	SYNTAX	INTEGER {
		other(1),
		arpRequest(2),
		arpResponse(3),
		ripRequest(4),
		ripResponse(5)
		}
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Indicates the method that was used to discover the
		MAC/Network address pair.  The methods that can be
		used for discovery are shown below.

		  other(1).........Indicates an unknown discovery
		                     method.
		  arpRequest(2)....Indicates that ARP request packets
		                     were used for discovery.
		  arpResponse(3)...Indicates that ARP response packets
		                     were used for discovery.
		  ripRequest(4)....Indicates that RIP request packets
		                     were used for discovery.
		  ripResponse(5)...Indicates that RIP response packets
		                     were used for discovery."
	::= { s3EnetHostEntry 8 }

s3EnetHostTimeStamp OBJECT-TYPE
	SYNTAX	TimeTicks
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"The value of sysUpTime when the MAC/Network address
		pair was last observed on the segment."
	::= { s3EnetHostEntry 9 }

END

