CISCOSB-EEE-MIB DEFINITIONS ::= BEGIN

-- Title:      CISCOSB EEE MIB
-- Version:    7.50
-- Date:       05 May 2010
--
IMPORTS
    switch001                                        FROM CISCOSB-MIB
    MODULE-IDENTITY, OBJECT-TYPE, Unsigned32    FROM SNMPv2-SMI
    TEXTUAL-CONVENTION, TruthValue              FROM SNMPv2-TC
    ifIndex, ifOperStatus                       FROM IF-MIB;

rlEee MODULE-IDENTITY  --  5-May-2010

        LAST-UPDATED  "201003150000Z"
		ORGANIZATION "Cisco Small Business"

		CONTACT-INFO
		"Postal: 170 West Tasman Drive
		San Jose , CA 95134-1706
		USA

		Website: Cisco Small Business Home http://www.cisco.com/smb>;,
		Cisco Small Business Support Community <http://www.cisco.com/go/smallbizsupport>"

        DESCRIPTION   "The private MIB module definition for Energy Efficient Ethernet feature."
        REVISION      "201005150000Z"
        DESCRIPTION   "Add Energy Efficient Ethernet support per port and per system"
::= { switch001  149}

----------------------
-- rlEeeEnable
----------------------
rlEeeEnable OBJECT-TYPE
    SYNTAX           TruthValue
    MAX-ACCESS       read-write
    STATUS           current
    DESCRIPTION
        "Enable the EEE mode globally"
    DEFVAL { false }
    ::= { rlEee 1 }

----------------------
-- rlEeePortTable
----------------------
rlEeePortTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlEeePortEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of EEE state of ports"
    ::= { rlEee 2 }

rlEeePortEntry OBJECT-TYPE
    SYNTAX      RlEeePortEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry of EEE state of bridge port"
    INDEX   { ifIndex }
    ::= { rlEeePortTable 1 }

RlEeePortEntry ::= SEQUENCE {
    rlEeePortAdminStatus        TruthValue,
    rlEeePortSupported          BITS,
    rlEeePortRemoteStatus       TruthValue,
    rlEeePortOperStatus         TruthValue
}

rlEeePortAdminStatus OBJECT-TYPE
    SYNTAX           TruthValue
    MAX-ACCESS       read-write
    STATUS           current
    DESCRIPTION
        "Enable/Disable EEE on ifindex"
    DEFVAL { false }
    ::= { rlEeePortEntry 1 }

rlEeePortSupported OBJECT-TYPE
    SYNTAX      BITS {
                    rlEeePortSupported10M(0),
                    rlEeePortSupported100M(1),
                    rlEeePortSupported1G(2),
                    rlEeePortSupported10G(3)
                }
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "Bit map that indicates whether EEE supported on the phy of the ifindex per speed
         0 - speed 10m; 1 - 100m; 2 - 1g; 3 - 10g"
    ::= { rlEeePortEntry 2 }

rlEeePortRemoteStatus OBJECT-TYPE
    SYNTAX           TruthValue
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "Indicates whether EEE active on remote link on current port's speed"
    ::= { rlEeePortEntry 3 }

rlEeePortOperStatus OBJECT-TYPE
    SYNTAX           TruthValue
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "Indicates whether EEE active on ifindex - ifoper is up,
                                                   rlEeePortSupported BIT is on in current port speed
                                                   rlEeePortLldpRemoteStatus is true,
                                                   rlEeeEnable is true,
                                                   rlEeePortAdminStatus is true"
    ::= { rlEeePortEntry 4 }

----------------------
-- rlEeePortLldpTable
----------------------

rlEeePortLldpTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlEeePortLldpEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of EEE LLDP"
    ::= { rlEee 3 }

rlEeePortLldpEntry OBJECT-TYPE
    SYNTAX      RlEeePortLldpEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry of EEE LLDP"
    INDEX   { ifIndex }
    ::= { rlEeePortLldpTable 1 }

RlEeePortLldpEntry ::= SEQUENCE {

    rlEeePortLldpAdminStatus    TruthValue,
    rlEeePortLldpOperStatus     TruthValue
}

rlEeePortLldpAdminStatus OBJECT-TYPE
    SYNTAX           TruthValue
    MAX-ACCESS       read-write
    STATUS           current
    DESCRIPTION
        "Enable/Disable EEE LLDP on ifindex"
    DEFVAL { false }
    ::= { rlEeePortLldpEntry 1 }

rlEeePortLldpOperStatus OBJECT-TYPE
    SYNTAX           TruthValue
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "Indicates whether EEE LLDP active on ifindex - rlEeePortLldpAdminStatus is true
                                                        lldpPortConfigAdminStatus is txAndRx,
                                                        rlLldpEnabled is true,
                                                        recieve a synch lldp packet"
    ::= { rlEeePortLldpEntry 2 }

----------------------
-- rlEeePortLldpLocalTable
----------------------

rlEeePortLldpLocalTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlEeePortLocalEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of EEE Local ports"
    ::= { rlEee 4 }

rlEeePortLldpLocalEntry OBJECT-TYPE
    SYNTAX      RlEeePortLocalEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry of EEE Local port"
    INDEX   { ifIndex }
    ::= { rlEeePortLldpLocalTable 1 }

RlEeePortLocalEntry ::= SEQUENCE {

    rlEeePortLldpLocalResolvedTx    Unsigned32,
    rlEeePortLldpLocalTx            Unsigned32,
    rlEeePortLldpLocalTxEcho        Unsigned32,
    rlEeePortLldpLocalResolvedRx    Unsigned32,
    rlEeePortLldpLocalRx            Unsigned32,
    rlEeePortLldpLocalRxEcho        Unsigned32
}

rlEeePortLldpLocalResolvedTx OBJECT-TYPE
    SYNTAX           Unsigned32
    UNITS            "uSec"
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "Indicates the current Tw_sys_tx configured in the local system, in micro-seconds"
    ::= { rlEeePortLldpLocalEntry 1 }

rlEeePortLldpLocalTx OBJECT-TYPE
    SYNTAX           Unsigned32
    UNITS            "uSec"
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "Indicates the value of Tw_sys_tx that the local system can support, in micro-seconds"
    ::= { rlEeePortLldpLocalEntry 2 }

rlEeePortLldpLocalTxEcho OBJECT-TYPE
    SYNTAX           Unsigned32
    UNITS            "uSec"
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "Indicates the remote system's Transmit Tw_sys_tx that was used by the local system
         to compute the Tw_sys_tx that it wants to request from the remote system, in micro-seconds"
    ::= { rlEeePortLldpLocalEntry 3 }

rlEeePortLldpLocalResolvedRx OBJECT-TYPE
    SYNTAX           Unsigned32
    UNITS            "uSec"
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "Indicates the current Tw_sys_tx configured by the remote system, in micro-seconds"
    ::= { rlEeePortLldpLocalEntry 4 }

rlEeePortLldpLocalRx OBJECT-TYPE
    SYNTAX           Unsigned32
    UNITS            "uSec"
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "Indicates the value of Tw_sys_tx that the local system requests from the remote system,
         in micro-seconds"
    ::= { rlEeePortLldpLocalEntry 5 }

rlEeePortLldpLocalRxEcho OBJECT-TYPE
    SYNTAX           Unsigned32
    UNITS            "uSec"
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "Indicates the remote system Receive Tw_sys_tx that was used by the local system
         to compute the Tw_sys_tx that it can support, in micro-seconds"
    ::= { rlEeePortLldpLocalEntry 6 }

----------------------
-- rlEeePortLldpRemoteTable
----------------------

rlEeePortLldpRemoteTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlEeePortRemoteEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of EEE remote ports"
    ::= { rlEee 5 }

rlEeePortLldpRemoteEntry OBJECT-TYPE
    SYNTAX      RlEeePortRemoteEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry of EEE remote port"
    INDEX   { ifIndex }
    ::= { rlEeePortLldpRemoteTable 1 }

RlEeePortRemoteEntry ::= SEQUENCE {

    rlEeePortLldpRemoteTx       Unsigned32,
    rlEeePortLldpRemoteRx       Unsigned32,
    rlEeePortLldpRemoteTxEcho   Unsigned32,
    rlEeePortLldpRemoteRxEcho   Unsigned32
}

rlEeePortLldpRemoteTx OBJECT-TYPE
    SYNTAX           Unsigned32
    UNITS            "uSec"
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "Indicates the value of Tw_sys_tx that the remote system can support, in micro-seconds"
    ::= { rlEeePortLldpRemoteEntry 1 }

rlEeePortLldpRemoteRx OBJECT-TYPE
    SYNTAX           Unsigned32
    UNITS            "uSec"
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "Indicates the value of Tw_sys_tx that the remote system requests from the local system,
         in micro-seconds"
    ::= { rlEeePortLldpRemoteEntry 2 }

rlEeePortLldpRemoteTxEcho OBJECT-TYPE
    SYNTAX           Unsigned32
    UNITS            "uSec"
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "Indicates the value of transmit Tw_sys_tx echoed back by the remote system, in micro-seconds"
    ::= { rlEeePortLldpRemoteEntry 3 }

rlEeePortLldpRemoteRxEcho OBJECT-TYPE
    SYNTAX           Unsigned32
    UNITS            "uSec"
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "Indicates the value Receive Tw_sys_tx echoed back by the remote system, in micro-seconds"
    ::= { rlEeePortLldpRemoteEntry 4 }



END


