CISCOSB-GREEN-MIB DEFINITIONS ::= BEGIN

-- Title:      CISCO GREEN ETHERNET MIB
-- Version:    7.47
-- Date:       25 Aug 2008
--
IMPORTS
    switch001                                        FROM CISCOSB-MIB
    MODULE-IDENTITY, OBJECT-TYPE, Unsigned32    FROM SNMPv2-SMI
    TEXTUAL-CONVENTION, TruthValue              FROM SNMPv2-TC
    PortList                                    FROM Q-BRIDGE-MIB
    ifIndex                                     FROM IF-MIB;

rlGreenEth MODULE-IDENTITY  -- August 15, 2008

        LAST-UPDATED  "200808150000Z"
		ORGANIZATION "Cisco Small Business"

		CONTACT-INFO
		"Postal: 170 West Tasman Drive
		San Jose , CA 95134-1706
		USA

		Website: Cisco Small Business Home http://www.cisco.com/smb>;,
		Cisco Small Business Support Community <http://www.cisco.com/go/smallbizsupport>"

        DESCRIPTION   "The private MIB module definition for Green Ethernet Energy Detect feature."
        REVISION      "200808150000Z"
        DESCRIPTION   "Add Green Ethernet Energy Detect and Short Reach support per port and per system rlGreenEthernet"
::= { switch001  134}

rlGreenEthEnergyDetectEnable OBJECT-TYPE
    SYNTAX           TruthValue
    MAX-ACCESS       read-write
    STATUS           current
    DESCRIPTION
        "This scalar defines Green Ethernet Enrgy-Detect Globaly"
    ::= { rlGreenEth 1 }

rlGreenEthShortReachEnable OBJECT-TYPE
    SYNTAX           TruthValue
    MAX-ACCESS       read-write
    STATUS           current
    DESCRIPTION
        "This scalar defines Green Ethernet Short-Reach Globaly"
    ::= { rlGreenEth 2 }

rlGreenEthCurrentEnergyConsumption OBJECT-TYPE
    SYNTAX           Unsigned32
    UNITS            "mWatt"
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "This scalar define Green Ethernet all modes current Energy consumption per system in mWatt
         in order to calculate current energy consumption in percent proportional to Consumption without Green Ethernet feature
         please use the following formula:
         (rlGreenEthCurrentEnergyConsumption/rlGreenEthCurrentMaxEnergyConsumption)*100"
    ::= { rlGreenEth 3 }

rlGreenEthCurrentMaxEnergyConsumption OBJECT-TYPE
    SYNTAX           Unsigned32
    UNITS            "mWatt"
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "This scalar define Green Ethernet current maximum consumption Energy consumption per system in mWatt,
         as it was without Green Ethernet feature."
    ::= { rlGreenEth 4 }

rlGreenEthCumulativePowerSaveMeter OBJECT-TYPE
    SYNTAX           Unsigned32
    UNITS            "Watt*Hour"
    MAX-ACCESS       read-only
    STATUS           current
    DESCRIPTION
        "This scalar define Green Ethernet cumulative power save per system in Watt*Hour"
    ::= { rlGreenEth 5 }

rlGreenEthShortReachThreshold OBJECT-TYPE
       SYNTAX      Unsigned32  (0..70)
       UNITS      "meter"
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
               "The usage threshold expressed in meter for
                determinate the cable length for Short-Reach"
       ::= { rlGreenEth 6 }

rlGreenEthCumulativePowerSaveMeterReset OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "The rlGreenEthCumulativePowerSaveMeterReset indicates that rlGreenEthCumulativePowerSaveMeter
            should be set to ziro.

            This object behaviors as write-only than
            reading this object will always return 'false'."
    DEFVAL{ false }
    ::= { rlGreenEth 7 }

RlGreenSavingType ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION
        "Green saving types:
         energyDetect(1)  uses energy detect
         shortReach(2)  uses Short Reach"
 SYNTAX  INTEGER {
        energyDetect (1),
        shortReach   (2)
    }

NonOperReasonType ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION
        "Reason why Green Ethernet is not activated saving on a port
         NP(1)                  Port is not present - Applicable in ED & SR
         LT(2)                  Link Type is not supported(fiber, auto media setect) - Applicable in ED & SR
         LU(3)                  Port link is up - Applicable only in ED
         LS(4)                  Link speed is not supported (100M,10M,10G) - Applicable only in SR
         LL(5)                  Link length received from VCT test exceed threshold - Applicable only in SR
         ER(6)                  Errors detected on line and port revered back to Long Reach(only in enhanced mode) - Applicable only in SR
         LD(7)                  Port link is Down - Applicable only in SR
         unknown(8)             In case that green Active or disable on port"


    SYNTAX  INTEGER {
        np(1),
        lt(2),
        lu(3),
        ls(4),
        ll(5),
        er(6),
        ld(7),
        unknown(8)
    }


rlGreenEthPortTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF RlGreenEthPortEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of green state of ports"
    ::= { rlGreenEth 8 }

rlGreenEthPortEntry OBJECT-TYPE
    SYNTAX      RlGreenEthPortEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry of green state of port"
    INDEX   { ifIndex,
              rlGreenEthPortSavingTypeValue  }
    ::= { rlGreenEthPortTable 1 }



RlGreenEthPortEntry ::= SEQUENCE {
    rlGreenEthPortSavingTypeValue         RlGreenSavingType,
    rlGreenEthPortAdminState              TruthValue,
    rlGreenEthPortOperState               TruthValue,
    rlGreenEthPortNonOperReason           NonOperReasonType
}

rlGreenEthPortSavingTypeValue OBJECT-TYPE
    SYNTAX      RlGreenSavingType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Green saving types"
    ::= { rlGreenEthPortEntry 1 }

rlGreenEthPortAdminState OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Active\non Active"
    ::= { rlGreenEthPortEntry 2 }

rlGreenEthPortOperState OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Active\non Active"
    ::= { rlGreenEthPortEntry 3 }


rlGreenEthPortNonOperReason OBJECT-TYPE
    SYNTAX      NonOperReasonType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Reason why saving mode is not activated"
    ::= { rlGreenEthPortEntry 4 }

rlGreenEthForceShortReachIfIndexList OBJECT-TYPE
    SYNTAX           PortList
    MAX-ACCESS       read-write
    STATUS           current
    DESCRIPTION
        "The ports that forced enable the Green Ethernet Short Reach configuration
          not considering VCT results."
    DEFVAL  { ''H } -- empty octet string
    ::= { rlGreenEth 9 }

END


