--
-- 
-- MIB generated by MG-SOFT Visual MIB Builder Version 4.0 Build 349
-- Friday, November 07, 2008 at 09:22:39
--
-- =================================================================
-- Copyright (C) 2006 by  HUAWEI TECHNOLOGIES. All rights reserved
-- 
-- Description: The HUAWEI-DC-BASE-MIB provides information about DataComm TRAPS
-- 
-- Reference:
-- Version:     V1.0
-- History:
-- 
-- =================================================================

    HUAWEI-BASE-TRAP-MIB DEFINITIONS ::= BEGIN
 
        IMPORTS
            entPhysicalIndex, entPhysicalContainedIn, entPhysicalClass, entPhysicalName            
                FROM ENTITY-MIB   
            hwDatacomm            
                FROM HUAWEI-MIB            
            IANAItuProbableCause, IANAItuEventType            
                FROM IANA-ITU-ALARM-TC-MIB            
            ifIndex            
                FROM IF-MIB            
            ItuPerceivedSeverity            
                FROM ITU-ALARM-TC-MIB            
            OBJECT-GROUP, MODULE-COMPLIANCE, NOTIFICATION-GROUP            
                FROM SNMPv2-CONF            
            Integer32, OBJECT-TYPE, MODULE-IDENTITY, NOTIFICATION-TYPE            
                FROM SNMPv2-SMI            
            DisplayString            
                FROM SNMPv2-TC;
    
    
        hwBaseTrapMIB MODULE-IDENTITY 
            LAST-UPDATED "200701170000Z"        -- January 17, 2007 at 00:00 GMT
            ORGANIZATION 
                "Huawei Technologies co.,Ltd."
            CONTACT-INFO 
                " R&D BeiJing, Huawei Technologies co.,Ltd.
                Huawei Bld.,NO.3 Xinxi Rd., 
                Shang-Di Information Industry Base,
                    Hai-Dian District Beijing P.R. China
                Zip:100085 
                Http://www.huawei.com                                       
                E-mail:support@huawei.com "
            DESCRIPTION 
                "This is the base trap definition for DataCom."
            ::= { hwDatacomm 129 }

        
    
    
--
-- Node definitions
--
    
        hwBaseTrapObject OBJECT IDENTIFIER ::= { hwBaseTrapMIB 1 }

        
        hwBaseTrapSeverity OBJECT-TYPE
            SYNTAX ItuPerceivedSeverity
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "To describe the level of trap."
            ::= { hwBaseTrapObject 1 }

        
        hwBaseTrapProbableCause OBJECT-TYPE
            SYNTAX IANAItuProbableCause
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "To describe the probable cause of trap."
            ::= { hwBaseTrapObject 2 }

        
        hwBaseTrapEventType OBJECT-TYPE
            SYNTAX IANAItuEventType
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "To describe the type of trap."
            ::= { hwBaseTrapObject 3 }

        
        hwBaseTrapRelativeResource OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "This object may contain a key word to indicate the relative
                resource of an entity.
                Such as:
                    hwEntityCommunicateError alarm may relate to a resource 
                    named 'IPC01'(A specified channel). So the trap may contain such a varbind in 
                    DisplayString style."
            ::= { hwBaseTrapObject 4 }

        
        hwBaseTrapReasonDescr OBJECT-TYPE
            SYNTAX DisplayString
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "To describe the reason of trap in DisplayString style."
            ::= { hwBaseTrapObject 5 }

        
        hwBaseThresholdTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwBaseThresholdEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "A table to config the threshold of each sensor."
            ::= { hwBaseTrapObject 6 }

        
        hwBaseThresholdEntry OBJECT-TYPE
            SYNTAX HwBaseThresholdEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The entry of threshold table."
            INDEX { entPhysicalIndex, hwBaseThresholdType, hwBaseThresholdIndex }
            ::= { hwBaseThresholdTable 1 }

        
        HwBaseThresholdEntry ::=
            SEQUENCE { 
                hwBaseThresholdType
                    INTEGER,
                hwBaseThresholdIndex
                    Integer32,
                hwBaseThresholdValue
                    Integer32,
                hwBaseThresholdUnit
                    INTEGER,
                hwBaseThresholdLowCritical
                    Integer32,
                hwBaseThresholdLowWarning
                    Integer32,
                hwBaseThresholdHighWarning
                    Integer32,
                hwBaseThresholdHighCritical
                    Integer32
             }

        hwBaseThresholdType OBJECT-TYPE
            SYNTAX INTEGER
                {
                temperatureSensor(1),
                humiditySensor(2),
                voltageSensor(3),
                currentSensor(4),
                powerSensor(5),
                portTraffic(6),
                portCrcError(7),
                portBroadcast(8)
                }
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The index to indicate the type of threshold for an entry.Such as
                temperature, humidity ,power supply......"
            ::= { hwBaseThresholdEntry 1 }

        
        hwBaseThresholdIndex OBJECT-TYPE
            SYNTAX Integer32 (1..2147483647)
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "A subindex to identify each sensor on physical entity."
            ::= { hwBaseThresholdEntry 2 }

        
        hwBaseThresholdValue OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The current value that been measured."
            ::= { hwBaseThresholdEntry 3 }

        
        hwBaseThresholdUnit OBJECT-TYPE
            SYNTAX INTEGER
                {
                percentage(1),
                centigrade1(2),
                centigrade2(3),
                voltage1(4),
                voltage2(5),
                current1(6),
                current2(7),
                power1(8),
                power2(9)
                }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The unit for this threshold value.
                
                percentage(1)         ---unit for humidity
                
                centigrade1(2)        ---unit for temperature
                centigrade2(3)        ---unit for hundredth of centigrade
                
                voltage1(4)           ---unit for volt (V)
                voltage2(5)           ---unit for thousandth of volt (mV)
                
                electric current:
                current1(6)           ---unit for milliampere (mA)
                current2(7)           ---unit for microampere (uA)
                
                power1(8)             ---unit for dbm(decibels above one milliwatt in 600 ohms)
                power2(9)             ---unit for hundredth of dbm(decibels above one milliwatt in 600 ohms)"
            ::= { hwBaseThresholdEntry 4 }

        
        hwBaseThresholdLowCritical OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The critical alarm threshold for falling alarm. It could be used
                for a more dangerous instance than hwBaseThresholdLowWarning.
                
                It should be equal to hwBaseThresholdLowWarning when don't support
                this threshold.
                "
            ::= { hwBaseThresholdEntry 5 }

        
        hwBaseThresholdLowWarning OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The normal warning threshold for falling alarm. "
            ::= { hwBaseThresholdEntry 6 }

        
        hwBaseThresholdHighWarning OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The normal warning threshold for rising alarm. "
            ::= { hwBaseThresholdEntry 7 }

        
        hwBaseThresholdHighCritical OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The critical alarm threshold for rising alarm. It could be used
                for a more dangerous instance than hwBaseThresholdHighWarning.
                
                It should be equal to hwBaseThresholdHighWarning when don't support
                this threshold."
            ::= { hwBaseThresholdEntry 8 }

        
        hwBaseUsageTable OBJECT-TYPE
            SYNTAX SEQUENCE OF HwBaseUsageEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "A table to config the threshold for each storage device."
            ::= { hwBaseTrapObject 7 }

        
        hwBaseUsageEntry OBJECT-TYPE
            SYNTAX HwBaseUsageEntry
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The entry for hwBaseUsageTable."
            INDEX { entPhysicalIndex, hwBaseUsageType, hwBaseUsageIndex }
            ::= { hwBaseUsageTable 1 }

        
        HwBaseUsageEntry ::=
            SEQUENCE { 
                hwBaseUsageType
                    INTEGER,
                hwBaseUsageIndex
                    Integer32,
                hwBaseUsageValue
                    Integer32,
                hwBaseUsageUnit
                    INTEGER,
                hwBaseUsageThreshold
                    Integer32
             }

        hwBaseUsageType OBJECT-TYPE
            SYNTAX INTEGER
                {
                cpuUtilization(1),
                memoryUtilization(2),
                diskUtilizatino(3),
                flashUtilizatino(4),
                cfCardUtilization(5)
                }
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "The index to indicate the type of threshold for an entry.Such as
                cpu,memory,flash and so on."
            ::= { hwBaseUsageEntry 1 }

        
        hwBaseUsageIndex OBJECT-TYPE
            SYNTAX Integer32 (1..2147483647)
            MAX-ACCESS not-accessible
            STATUS current
            DESCRIPTION
                "A subindex to identify each sensor on physical entity."
            ::= { hwBaseUsageEntry 2 }

        
        hwBaseUsageValue OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The current value that been measured."
            ::= { hwBaseUsageEntry 3 }

        
        hwBaseUsageUnit OBJECT-TYPE
            SYNTAX INTEGER { percentage(1) }
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                "The unit for this threshold value.
                
                percentage(1)         ---unit for cpu/men/disk/flash/cfCard
                "
            ::= { hwBaseUsageEntry 4 }

        
        hwBaseUsageThreshold OBJECT-TYPE
            SYNTAX Integer32
            MAX-ACCESS read-write
            STATUS current
            DESCRIPTION
                "The threshold of usage for storage device."
            ::= { hwBaseUsageEntry 5 }

        
        hwFIBOverloadModule OBJECT-TYPE
            SYNTAX INTEGER
                {
                ipv4(1),
                ipv6(2)
                }
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "module is ipv4 or ipv6"
            ::= { hwBaseTrapObject 8 }

        
        hwBaseFlowDirectionType OBJECT-TYPE
            SYNTAX INTEGER
                {
                inbound(1),
                outbound(2)
                }
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "
                The direction of data flow is specified.
                "
            ::= { hwBaseTrapObject 9 }

        
        hwPowerDirection OBJECT-TYPE
            SYNTAX INTEGER
                {
                inbound(1),
                outbound(2)
                }
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The direction of photoelectric power."
            ::= { hwBaseTrapObject 10 }


        hwBaseTrapTrafficDir OBJECT-TYPE
            SYNTAX INTEGER
                {
                trafficIn(1),
                trafficOut(2)
                }
            MAX-ACCESS accessible-for-notify
            STATUS current
            DESCRIPTION
                "The traffic flows in or out of the port."
            ::= { hwBaseTrapObject 11 }
        
    hwEntityRatedPower OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
            "The rated power of board."
        ::= { hwBaseTrapObject 12 }
        
    hwDevAvailablePower OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
            "Available power of the device."
        ::= { hwBaseTrapObject 13 }
        
    hwDeviceTotalPower OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
            "Total power of the device."
        ::= { hwBaseTrapObject 14 }
        
        hwBaseTraps OBJECT IDENTIFIER ::= { hwBaseTrapMIB 2 }

        
        hwEntityTrap OBJECT IDENTIFIER ::= { hwBaseTraps 1 }

        
        hwEntityRemove NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalContainedIn, entPhysicalName
                 }
            STATUS current
            DESCRIPTION 
                "Entity has been removed."
            ::= { hwEntityTrap 1 }

        
        hwEntityInsert NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalContainedIn, entPhysicalName
                 }
            STATUS current
            DESCRIPTION 
                "Entity has been inserted."
            ::= { hwEntityTrap 2 }

        
        hwEntityUnstable NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalContainedIn, entPhysicalName
                 }
            STATUS current
            DESCRIPTION 
                "Entity has been inserted but position unstable."
            ::= { hwEntityTrap 3 }

        
        hwEntityUnstableResume NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalContainedIn, entPhysicalName
                 }
            STATUS current
            DESCRIPTION 
                "Resume from entity position unstable situation."
            ::= { hwEntityTrap 4 }

        
        hwEntityReset NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalContainedIn, entPhysicalName, 
                hwBaseTrapRelativeResource, hwBaseTrapReasonDescr }
            STATUS current
            DESCRIPTION 
                "Entity will be reseted."
            ::= { hwEntityTrap 5 }

        
        hwEntityResetDone NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalContainedIn, entPhysicalName, 
                hwBaseTrapRelativeResource, hwBaseTrapReasonDescr }
            STATUS current
            DESCRIPTION 
                "Entity has been reseted and in good health now."
            ::= { hwEntityTrap 6 }

        
        hwEntityCommunicateError NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalContainedIn, entPhysicalName, 
                hwBaseTrapRelativeResource, hwBaseTrapReasonDescr }
            STATUS current
            DESCRIPTION 
                "Communication error has been detected.
                Include all kinds of communication error between boards."
            ::= { hwEntityTrap 7 }

        
        hwEntityCommunicateResume NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalContainedIn, entPhysicalName, 
                hwBaseTrapRelativeResource, hwBaseTrapReasonDescr }
            STATUS current
            DESCRIPTION 
                "Resume from communication error situation."
            ::= { hwEntityTrap 8 }

        
        hwEntityInvalid NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalContainedIn, entPhysicalName, 
                hwBaseTrapRelativeResource, hwBaseTrapReasonDescr }
            STATUS current
            DESCRIPTION 
                "Entity is invalid for some reason."
            ::= { hwEntityTrap 9 }

        
        hwEntityResume NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalContainedIn, entPhysicalName, 
                hwBaseTrapRelativeResource, hwBaseTrapReasonDescr }
            STATUS current
            DESCRIPTION 
                "Entity reusme from invalid situation."
            ::= { hwEntityTrap 10 }

        
        hwEntityLeaveMaster NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalContainedIn, entPhysicalName, 
                hwBaseTrapRelativeResource, hwBaseTrapReasonDescr }
            STATUS current
            DESCRIPTION 
                "Redundant entity leave master role."
            ::= { hwEntityTrap 11 }

        
        hwEntityBecomeMaster NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalContainedIn, entPhysicalName, 
                hwBaseTrapRelativeResource, hwBaseTrapReasonDescr }
            STATUS current
            DESCRIPTION 
                "Redundant entity become master role."
            ::= { hwEntityTrap 12 }

        
        hwEntityOffline NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalContainedIn, entPhysicalName, 
                hwBaseTrapRelativeResource, hwBaseTrapReasonDescr }
            STATUS current
            DESCRIPTION 
                "Entity change to OFFLINE status."
            ::= { hwEntityTrap 13 }

        
        hwEntityOnline NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalContainedIn, entPhysicalName, 
                hwBaseTrapRelativeResource, hwBaseTrapReasonDescr }
            STATUS current
            DESCRIPTION 
                "Entity change to ONLINE status."
            ::= { hwEntityTrap 14 }

        
        hwEntityCheckFail NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalContainedIn, entPhysicalName, 
                hwBaseTrapRelativeResource, hwBaseTrapReasonDescr }
            STATUS current
            DESCRIPTION 
                "
                Failure of self-check occurs to the board
                "
            ::= { hwEntityTrap 15 }

        
        hwEntityCheckResume NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalContainedIn, entPhysicalName, 
                hwBaseTrapRelativeResource, hwBaseTrapReasonDescr }
            STATUS current
            DESCRIPTION 
                "
                The status is recovered from the failure of board self-check
                "
            ::= { hwEntityTrap 16 }

        
        hwEntityRegFail NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalContainedIn, entPhysicalName, 
                hwBaseTrapRelativeResource, hwBaseTrapReasonDescr }
            STATUS current
            DESCRIPTION 
                "Entity fail in registration."
            ::= { hwEntityTrap 17 }

        
        hwEntityRegSuccess NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalContainedIn, entPhysicalName, 
                hwBaseTrapRelativeResource, hwBaseTrapReasonDescr }
            STATUS current
            DESCRIPTION 
                "Entity success in registration."
            ::= { hwEntityTrap 18 }

        
        hwEnvironmentTrap OBJECT IDENTIFIER ::= { hwBaseTraps 2 }

        
        hwTempRisingAlarm NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseThresholdValue, 
                hwBaseThresholdUnit, hwBaseThresholdHighWarning, hwBaseThresholdHighCritical }
            STATUS current
            DESCRIPTION 
                "Temperature rise over HIGH threshold."
            ::= { hwEnvironmentTrap 1 }

        
        hwTempRisingResume NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseThresholdValue, 
                hwBaseThresholdUnit, hwBaseThresholdHighWarning, hwBaseThresholdHighCritical }
            STATUS current
            DESCRIPTION 
                "Temperature back to normal level."
            ::= { hwEnvironmentTrap 2 }

        
        hwTempFallingAlarm NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseThresholdValue, 
                hwBaseThresholdUnit, hwBaseThresholdLowCritical, hwBaseThresholdLowWarning }
            STATUS current
            DESCRIPTION 
                "Temperature fall below LOW threshold."
            ::= { hwEnvironmentTrap 3 }

        
        hwTempFallingResume NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseThresholdValue, 
                hwBaseThresholdUnit, hwBaseThresholdLowCritical, hwBaseThresholdLowWarning }
            STATUS current
            DESCRIPTION 
                "Temperature back to normal level."
            ::= { hwEnvironmentTrap 4 }

        
        hwHumidityRisingAlarm NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseThresholdValue, 
                hwBaseThresholdUnit, hwBaseThresholdHighWarning, hwBaseThresholdHighCritical }
            STATUS current
            DESCRIPTION 
                "Humidity rise over HIGH threshold."
            ::= { hwEnvironmentTrap 5 }

        
        hwHumidityRisingResume NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseThresholdValue, 
                hwBaseThresholdUnit, hwBaseThresholdHighWarning, hwBaseThresholdHighCritical }
            STATUS current
            DESCRIPTION 
                "Humidity back to normal level."
            ::= { hwEnvironmentTrap 6 }

        
        hwHumidityFallingAlarm NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseThresholdValue, 
                hwBaseThresholdUnit, hwBaseThresholdLowCritical, hwBaseThresholdLowWarning }
            STATUS current
            DESCRIPTION 
                "Humidity fall below LOW threshold."
            ::= { hwEnvironmentTrap 7 }

        
        hwHumidityFallingResume NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseThresholdValue, 
                hwBaseThresholdUnit, hwBaseThresholdLowCritical, hwBaseThresholdLowWarning }
            STATUS current
            DESCRIPTION 
                "Humidity back to normal level."
            ::= { hwEnvironmentTrap 8 }

        
        hwVoltRisingAlarm NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseThresholdValue, 
                hwBaseThresholdUnit, hwBaseThresholdHighWarning, hwBaseThresholdHighCritical }
            STATUS current
            DESCRIPTION 
                "Voltage of power rise over HIGH threshold."
            ::= { hwEnvironmentTrap 9 }

        
        hwVoltRisingResume NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseThresholdValue, 
                hwBaseThresholdUnit, hwBaseThresholdHighWarning, hwBaseThresholdHighCritical }
            STATUS current
            DESCRIPTION 
                "Voltage back to normal level."
            ::= { hwEnvironmentTrap 10 }

        
        hwVoltFallingAlarm NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseThresholdValue, 
                hwBaseThresholdUnit, hwBaseThresholdLowCritical, hwBaseThresholdLowWarning }
            STATUS current
            DESCRIPTION 
                "Voltage of power fall below LOW threshold."
            ::= { hwEnvironmentTrap 11 }

        
        hwVoltFallingResume NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseThresholdValue, 
                hwBaseThresholdUnit, hwBaseThresholdLowCritical, hwBaseThresholdLowWarning }
            STATUS current
            DESCRIPTION 
                "Voltage back to normal level."
            ::= { hwEnvironmentTrap 12 }

        
        hwCurrentRisingAlarm NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseThresholdValue, 
                hwBaseThresholdUnit, hwBaseThresholdHighWarning, hwBaseThresholdHighCritical }
            STATUS current
            DESCRIPTION 
                "Current rise over HIGH threshold."
            ::= { hwEnvironmentTrap 13 }

        
        hwCurrentRisingResume NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseThresholdValue, 
                hwBaseThresholdUnit, hwBaseThresholdHighWarning, hwBaseThresholdHighCritical }
            STATUS current
            DESCRIPTION 
                "Current back to normal level."
            ::= { hwEnvironmentTrap 14 }

        
        hwCurrentFallingAlarm NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseThresholdValue, 
                hwBaseThresholdUnit, hwBaseThresholdLowCritical, hwBaseThresholdLowWarning }
            STATUS current
            DESCRIPTION 
                "Current fall below LOW threshold."
            ::= { hwEnvironmentTrap 15 }

        
        hwCurrentFallingResume NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseThresholdValue, 
                hwBaseThresholdUnit, hwBaseThresholdLowCritical, hwBaseThresholdLowWarning }
            STATUS current
            DESCRIPTION 
                "Current back to normal level."
            ::= { hwEnvironmentTrap 16 }

        
        hwPowerRisingAlarm NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseThresholdValue, 
                hwBaseThresholdUnit, hwBaseThresholdHighWarning, hwBaseThresholdHighCritical, hwPowerDirection }
            STATUS current
            DESCRIPTION 
                "Photoelectric power rise over HIGH threshold."
            ::= { hwEnvironmentTrap 17 }

        
        hwPowerRisingResume NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseThresholdValue, 
                hwBaseThresholdUnit, hwBaseThresholdHighWarning, hwBaseThresholdHighCritical, hwPowerDirection }
            STATUS current
            DESCRIPTION 
                "Photoelectric power back to normal level."
            ::= { hwEnvironmentTrap 18 }

        
        hwPowerFallingAlarm NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseThresholdValue, 
                hwBaseThresholdUnit, hwBaseThresholdLowCritical, hwBaseThresholdLowWarning, hwPowerDirection }
            STATUS current
            DESCRIPTION 
                "Photoelectric power fall below LOW threshold."
            ::= { hwEnvironmentTrap 19 }

        
        hwPowerFallingResume NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseThresholdValue, 
                hwBaseThresholdUnit, hwBaseThresholdLowCritical, hwBaseThresholdLowWarning, hwPowerDirection }
            STATUS current
            DESCRIPTION 
                "Photoelectric power back to normal level."
            ::= { hwEnvironmentTrap 20 }

    hwPowerInsufficiencyAlarm NOTIFICATION-TYPE
        OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalContainedIn, entPhysicalName, 
            hwEntityRatedPower, hwDevAvailablePower, hwDeviceTotalPower }
        STATUS current
        DESCRIPTION 
            "The available power of device is not enough for the board."
        ::= { hwEnvironmentTrap 21 }

    hwPowerInsufficiencyResume NOTIFICATION-TYPE
        OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalContainedIn, entPhysicalName, 
            hwEntityRatedPower, hwDevAvailablePower, hwDeviceTotalPower }
        STATUS current
        DESCRIPTION 
            "The available power of device becomes sufficient for the board."
        ::= { hwEnvironmentTrap 22 }
        
        hwPowerTrap OBJECT IDENTIFIER ::= { hwBaseTraps 3 }

        
        hwPowerOff NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalContainedIn, entPhysicalName
                 }
            STATUS current
            DESCRIPTION 
                "One of the power is shutting down."
            ::= { hwPowerTrap 1 }

        
        hwPowerOn NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalContainedIn, entPhysicalName
                 }
            STATUS current
            DESCRIPTION 
                "One of the power is starting up."
            ::= { hwPowerTrap 2 }
           
           
        hwPowerMixed NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalContainedIn, entPhysicalName
                 }
            STATUS current
            DESCRIPTION 
                "The power is not of the same type!"
            ::= { hwPowerTrap 3 }


        hwPowerMixedResume NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalContainedIn, entPhysicalName
                 }
            STATUS current
            DESCRIPTION 
                "The power is changed to the same type!"
            ::= { hwPowerTrap 4 }
        
        hwCPUTrap OBJECT IDENTIFIER ::= { hwBaseTraps 4 }

        
        hwCPUUtilizationRisingAlarm NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseTrapRelativeResource, 
                hwBaseUsageValue, hwBaseUsageUnit, hwBaseUsageThreshold }
            STATUS current
            DESCRIPTION 
                "CPU utilization exceed threshold."
            ::= { hwCPUTrap 1 }

        
        hwCPUUtilizationResume NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseTrapRelativeResource, 
                hwBaseUsageValue, hwBaseUsageUnit, hwBaseUsageThreshold }
            STATUS current
            DESCRIPTION 
                "CPU utilization back to normal level."
            ::= { hwCPUTrap 2 }

        
        hwPortTrap OBJECT IDENTIFIER ::= { hwBaseTraps 5 }

        
        hwPortPhysicalDown NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName }
            STATUS current
            DESCRIPTION 
                "One of the port physical connect down."
            ::= { hwPortTrap 1 }

        
        hwPortPhysicalUp NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName }
            STATUS current
            DESCRIPTION 
                "One of the port physical connect up."
            ::= { hwPortTrap 2 }

        
        hwPortPhysicalNoTrafficAlarm NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseTrapRelativeResource, hwBaseTrapTrafficDir }
            STATUS current
            DESCRIPTION 
                "One of the port has none traffic."
            ::= { hwPortTrap 3 }
            
        
        hwPortPhysicalNoTrafficClear NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseTrapRelativeResource, hwBaseTrapTrafficDir }
            STATUS current
            DESCRIPTION 
                "One of the port traffic resume."
            ::= { hwPortTrap 4 }
            
        
        hwPortPhysicalTrafficRisingAlarm NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseTrapRelativeResource, hwBaseThresholdValue, hwBaseThresholdUnit, hwBaseThresholdHighWarning, hwBaseTrapTrafficDir }
            STATUS current
            DESCRIPTION 
                "One of the port traffic rise over threshold."
            ::= { hwPortTrap 5 }
            
        
        hwPortPhysicalTrafficClear NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseTrapRelativeResource, hwBaseThresholdValue, hwBaseThresholdUnit, hwBaseThresholdLowWarning, hwBaseTrapTrafficDir }
            STATUS current
            DESCRIPTION 
                "One of the port traffic resume to normal level."
            ::= { hwPortTrap 6 }
            
        
        hwPortPhysicalCrcErrorRisingAlarm NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseTrapRelativeResource, hwBaseThresholdValue, hwBaseThresholdUnit, hwBaseThresholdHighWarning }
            STATUS current
            DESCRIPTION 
                "One of the port CRC error rise over threshold."
            ::= { hwPortTrap 7 }
            
        
        hwPortPhysicalCrcErrorClear NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseTrapRelativeResource, hwBaseThresholdValue, hwBaseThresholdUnit, hwBaseThresholdLowWarning }
            STATUS current
            DESCRIPTION 
                "One of the port CRC error resume to normal level."
            ::= { hwPortTrap 8 }
            
        
        hwPortPhysicalEthBroadcastRisingAlarm NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseTrapRelativeResource, hwBaseThresholdValue, hwBaseThresholdUnit, hwBaseThresholdHighWarning }
            STATUS current
            DESCRIPTION 
                "One of the Ethernet port broadcast rise over threshold."
            ::= { hwPortTrap 9 }
            
        
        hwPortPhysicalEthBroadcastClear NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseTrapRelativeResource, hwBaseThresholdValue, hwBaseThresholdUnit, hwBaseThresholdLowWarning }
            STATUS current
            DESCRIPTION 
                "One of the Ethernet port broadcast resume to normal level."
            ::= { hwPortTrap 10 }
            
        
        hwPortPhysicalEthHalfDuplexAlarm NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseTrapRelativeResource }
            STATUS current
            DESCRIPTION 
                "One of the Ethernet port works on the half-duplex mode."
            ::= { hwPortTrap 11 }
            
        
        hwPortPhysicalEthFullDuplexClear NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseTrapRelativeResource }
            STATUS current
            DESCRIPTION 
                "One of the Ethernet port works on the full-duplex mode."
            ::= { hwPortTrap 12 }
            
                                                
        hwStorageTrap OBJECT IDENTIFIER ::= { hwBaseTraps 6 }

        
        hwStorageUtilizationRisingAlarm NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseTrapRelativeResource, 
                hwBaseUsageValue, hwBaseUsageUnit, hwBaseUsageThreshold }
            STATUS current
            DESCRIPTION 
                "Storage device utilization rise over threshold."
            ::= { hwStorageTrap 1 }

        
        hwStorageUtilizationResume NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseTrapRelativeResource, 
                hwBaseUsageValue, hwBaseUsageUnit, hwBaseUsageThreshold }
            STATUS current
            DESCRIPTION 
                "Storage utilization resume to normal level."
            ::= { hwStorageTrap 2 }

        
        hwClockTrap OBJECT IDENTIFIER ::= { hwBaseTraps 7 }

        
        hwFanTrap OBJECT IDENTIFIER ::= { hwBaseTraps 8 }

        
        hwFibTrap OBJECT IDENTIFIER ::= { hwBaseTraps 9 }

        
        hwFIBOverloadSuspend NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, hwFIBOverloadModule }
            STATUS current
            DESCRIPTION 
                "The board is suspended for IPv4/IPv6 FIB capability overload."
            ::= { hwFibTrap 1 }

        
        hwFIBOverloadSusResume NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType }
            STATUS current
            DESCRIPTION 
                "The board is recovered for FIB capability overload suspend."
            ::= { hwFibTrap 2 }

        
        hwFIBOverloadForward NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, hwFIBOverloadModule }
            STATUS current
            DESCRIPTION 
                "The board is forwarding for IPv4/IPv6 FIB capability overload."
            ::= { hwFibTrap 3 }

        
        hwFIBOverloadFwResume NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, hwFIBOverloadModule }
            STATUS current
            DESCRIPTION 
                "The board is recovered for IPv4/IPv6 FIB capability overload forward."
            ::= { hwFibTrap 4 }

        
        hwPppTrap OBJECT IDENTIFIER ::= { hwBaseTraps 10 }

        
        hwPppLoopbackDetect NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, ifIndex }
            STATUS current
            DESCRIPTION 
                "The interface Loopback is detected."
            ::= { hwPppTrap 1 }

        
        hwPppLoopbackDetResume NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, ifIndex }
            STATUS current
            DESCRIPTION 
                "The interface is recovered for Loopback."
            ::= { hwPppTrap 2 }

        
        hwFlowControlTrap OBJECT IDENTIFIER ::= { hwBaseTraps 11 }

        
        hwFlowCongestion NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalClass, entPhysicalName, 
                hwBaseFlowDirectionType }
            STATUS current
            DESCRIPTION 
                "
                The object is in congested state and some of the frames are dropped.
                "
            ::= { hwFlowControlTrap 1 }

        
        hwFlowCongestionResume NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalClass, entPhysicalName, 
                hwBaseFlowDirectionType }
            STATUS current
            DESCRIPTION 
                "
                Alarms of the congested object are cleared.
                "
            ::= { hwFlowControlTrap 2 }

        hwDeviceAbnormalTrap OBJECT IDENTIFIER ::= { hwBaseTraps 12 }

        
        hwDeviceAbnormalRisingAlarm NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, entPhysicalName, hwBaseTrapRelativeResource }
            STATUS current
            DESCRIPTION 
                "Device abnormal or pulled out."
            ::= { hwDeviceAbnormalTrap 1 }

                
        hwResExhaustBfdTrap OBJECT IDENTIFIER ::= { hwBaseTraps 13 }

        
        hwResExhaustBfdAlarm NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType }
            STATUS current
            DESCRIPTION 
                "Failed to allocate resources for BFD because hardware resources were exhausted."
            ::= { hwResExhaustBfdTrap 1 }

        hwResExhaustBfdResume NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType }
            STATUS current
            DESCRIPTION 
                "BFD recovered from alarms of hardware resources exhausting."
            ::= { hwResExhaustBfdTrap 2 }   
            
        hwResExhaustOamTrap OBJECT IDENTIFIER ::= { hwBaseTraps 14 }

        
        hwResExhaustOamAlarm NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType }
            STATUS current
            DESCRIPTION 
                "Failed to allocate resources for OAM because hardware resources were exhausted. 
                MPLS OAM is short for Operation Administration and Maintenance by MPLS. 
                It is used for connectivity verification of MPLS LSP."
            ::= { hwResExhaustOamTrap 1 }

        hwResExhaustOamResume NOTIFICATION-TYPE
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType }
            STATUS current
            DESCRIPTION 
                "OAM recovered from alarms of hardware resources exhausting.
                MPLS OAM is short for Operation Administration and Maintenance by MPLS. 
                It is used for connectivity verification of MPLS LSP."
            ::= { hwResExhaustOamTrap 2 }

                    
        hwBaseTrapConformance OBJECT IDENTIFIER ::= { hwBaseTrapMIB 3 }

        
        hwBaseTrapCompliances OBJECT IDENTIFIER ::= { hwBaseTrapConformance 1 }

        
        hwBaseTrapCompliance MODULE-COMPLIANCE
            STATUS current
            DESCRIPTION 
                "Compliance statement for agents that provide full support for 
                hwBaseTrapMIB."
            MODULE -- this module
                MANDATORY-GROUPS { hwBaseObjectGroup }
            ::= { hwBaseTrapCompliances 1 }

        
        hwBaseTrapGroups OBJECT IDENTIFIER ::= { hwBaseTrapConformance 2 }

        
        hwBaseObjectGroup OBJECT-GROUP
            OBJECTS { hwBaseTrapSeverity, hwBaseTrapProbableCause, hwBaseTrapEventType, hwBaseThresholdValue, hwBaseThresholdUnit, 
                hwBaseThresholdLowCritical, hwBaseThresholdLowWarning, hwBaseThresholdHighWarning, hwBaseThresholdHighCritical, hwBaseUsageValue, 
                hwBaseUsageUnit, hwBaseUsageThreshold, hwDevAvailablePower, hwEntityRatedPower, hwDeviceTotalPower, hwBaseTrapReasonDescr, 
                hwBaseTrapRelativeResource, hwFIBOverloadModule, hwBaseFlowDirectionType, hwPowerDirection, hwBaseTrapTrafficDir
                 }
            STATUS current
            DESCRIPTION 
                "Group for base trap objects."
            ::= { hwBaseTrapGroups 1 }

        
        hwBaseTrapGroup NOTIFICATION-GROUP
            NOTIFICATIONS { hwEntityRemove, hwEntityInsert, hwEntityUnstable, hwEntityUnstableResume, hwEntityReset, 
                hwEntityResetDone, hwEntityCommunicateError, hwEntityCommunicateResume, hwEntityInvalid, hwEntityResume, 
                hwEntityLeaveMaster, hwEntityBecomeMaster, hwEntityOffline, hwEntityOnline, hwEntityRegFail, 
                hwEntityRegSuccess, hwTempRisingAlarm, hwTempRisingResume, hwTempFallingAlarm, hwTempFallingResume, 
                hwHumidityRisingAlarm, hwHumidityRisingResume, hwHumidityFallingAlarm, hwHumidityFallingResume, hwVoltRisingAlarm, 
                hwVoltRisingResume, hwVoltFallingAlarm, hwVoltFallingResume, hwCurrentRisingAlarm, hwCurrentRisingResume, 
                hwCurrentFallingAlarm, hwCurrentFallingResume, hwPowerRisingAlarm, hwPowerRisingResume, hwPowerFallingAlarm,hwPowerInsufficiencyAlarm, hwPowerInsufficiencyResume, 
                hwPowerFallingResume, hwPowerOff, hwPowerOn, hwPowerMixed, hwPowerMixedResume, hwCPUUtilizationRisingAlarm, hwCPUUtilizationResume, 
                hwPortPhysicalDown, hwPortPhysicalUp, hwPortPhysicalNoTrafficAlarm, hwPortPhysicalNoTrafficClear, hwPortPhysicalTrafficRisingAlarm, 
                hwPortPhysicalTrafficClear, hwPortPhysicalCrcErrorRisingAlarm, hwPortPhysicalCrcErrorClear, hwPortPhysicalEthBroadcastRisingAlarm, 
                hwPortPhysicalEthBroadcastClear, hwPortPhysicalEthHalfDuplexAlarm, hwPortPhysicalEthFullDuplexClear, 
                hwStorageUtilizationRisingAlarm, hwStorageUtilizationResume, hwFIBOverloadSuspend, 
                hwFIBOverloadSusResume, hwFIBOverloadForward, hwFIBOverloadFwResume, hwPppLoopbackDetect, hwPppLoopbackDetResume, 
                hwEntityCheckFail, hwEntityCheckResume, hwFlowCongestion, hwFlowCongestionResume, hwDeviceAbnormalRisingAlarm,
                hwResExhaustBfdAlarm, hwResExhaustBfdResume, hwResExhaustOamAlarm, hwResExhaustOamResume }
            STATUS current
            DESCRIPTION 
                "Group for all base traps."
            ::= { hwBaseTrapGroups 2 }

        
    
    END

--
-- HUAWEI-BASE-TRAP-MIB.mib
--
