FOUNDRY-SN-SW-L4-SWITCH-GROUP-MIB DEFINITIONS ::= BEGIN


-- Foundry L4 Switch Group MIB Release 1.0.0
-- Revision 0 01/08/2000

-- Copyright 1996-98 Foundry Networks, Inc.
-- All rights reserved.
-- This Foundry Networks SNMP Management Information Base Specification
-- (Specification) embodies Foundry Networks' confidential and
-- proprietary intellectual property. Foundry Networks retains all
-- title and ownership in the Specification, including any
-- revisions.

-- This Specification is supplied "AS IS," and Foundry Networks makes
-- no warranty, either express or implied, as to the use,
-- operation, condition, or performance of the Specification.

-- SECTION 1: Top Level Definitions


-- Imports

IMPORTS
	IpAddress, Counter, TimeTicks
			FROM RFC1155-SMI
	 Counter64		FROM SNMPv2-SMI
   
	OBJECT-TYPE             
		FROM RFC-1212
	snL4
		FROM FOUNDRY-SN-ROOT-MIB;

	-- textual conventions
	-- maximum of ports are 32.  

	--  Row Creation/Deletion Values

	     L4RowSts ::= INTEGER { other(1),
							  valid(2),
							  delete(3),
							  create(4),
							  modify(5)
							}
	--  L4 Status Values

	    L4Status ::= INTEGER { disabled(0), enabled(1) }

	--  L4 Server Name
        L4ServerName ::= OCTET STRING (SIZE(1..32))

	--  L4 Flag Values
	    L4Flag ::= INTEGER { false(0), true(1) }

	--  L4 Delete Sate
	     L4DeleteState ::= INTEGER { done(0),
									 waitunbind(1),
									 waitdelete(2)
									}

	--  WebCacheSate
	     WebCacheState ::= INTEGER { disabled(0),
									 enabled(1),
									 failed(2),
									 testing(3),
									 suspect(4),
									 shutdown(5),
									 active(6)
									}

        PhysAddress ::= OCTET STRING
    -- This data type is used to model media addresses.  For many
    -- types of media, this will be in a binary representation.
    -- For example, an ethernet address would be represented as
    -- a string of 6 octets.

	  DisplayString ::=
	      OCTET STRING
	  -- This data type is used to model textual information taken
	  -- from the NVT ASCII character set.  By convention, objects
	  -- with this syntax are declared as having
	  --
	  --      SIZE (0..255)
    

snL4Gen						OBJECT IDENTIFIER	  ::= { snL4 1  }
snL4VirtualServer			OBJECT IDENTIFIER	  ::= { snL4 2  }
snL4RealServer				OBJECT IDENTIFIER	  ::= { snL4 3  }
snL4VirtualServerPort		OBJECT IDENTIFIER	  ::= { snL4 4  }
snL4RealServerPort			OBJECT IDENTIFIER	  ::= { snL4 5  }
snL4Bind					OBJECT IDENTIFIER	  ::= { snL4 6  }
snL4VirtualServerStatus		OBJECT IDENTIFIER	  ::= { snL4 7  }
snL4RealServerStatus		OBJECT IDENTIFIER	  ::= { snL4 8  }
snL4VirtualServerPortStatus	OBJECT IDENTIFIER	  ::= { snL4 9  }
snL4RealServerPortStatus	OBJECT IDENTIFIER	  ::= { snL4 10 }
snL4Policy					OBJECT IDENTIFIER	  ::= { snL4 11 }
snL4PolicyPortAccess		OBJECT IDENTIFIER	  ::= { snL4 12 }
snL4Trap					OBJECT IDENTIFIER	  ::= { snL4 13 }
snL4WebCache				OBJECT IDENTIFIER	  ::= { snL4 14 }
snL4WebCacheGroup			OBJECT IDENTIFIER	  ::= { snL4 15 }
snL4WebCacheTrafficStats	OBJECT IDENTIFIER	  ::= { snL4 16 }
snL4WebUncachedTrafficStats	OBJECT IDENTIFIER	  ::= { snL4 17 }
snL4WebCachePort			OBJECT IDENTIFIER	  ::= { snL4 18 }
snL4RealServerCfg			OBJECT IDENTIFIER	  ::= { snL4 19 }
snL4RealServerPortCfg		OBJECT IDENTIFIER	  ::= { snL4 20 }
snL4VirtualServerCfg		OBJECT IDENTIFIER	  ::= { snL4 21  }
snL4VirtualServerPortCfg	OBJECT IDENTIFIER	  ::= { snL4 22  }
snL4RealServerStatistic		OBJECT IDENTIFIER	  ::= { snL4 23 }
snL4RealServerPortStatistic	OBJECT IDENTIFIER	  ::= { snL4 24 }
snL4VirtualServerStatistic		OBJECT IDENTIFIER	  ::= { snL4 25 }
snL4VirtualServerPortStatistic	OBJECT IDENTIFIER	  ::= { snL4 26 }
snL4GslbSiteRemoteServerIrons	OBJECT IDENTIFIER 	  ::= { snL4 27 }
snL4History						OBJECT IDENTIFIER 	  ::= { snL4 28 }


-- L4 General MIBs
                
snL4MaxSessionLimit 		OBJECT-TYPE
	SYNTAX	INTEGER	(0..1000000)
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"numbers of maximum session (L4 cache) entries"
	::= { snL4Gen 1 }

snL4TcpSynLimit 		OBJECT-TYPE
	SYNTAX	INTEGER	 (1..65535)
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Numbers of connection per second"
	::= { snL4Gen 2 }

--  Server load balancing
snL4slbGlobalSDAType	OBJECT-TYPE
	SYNTAX	 INTEGER {
	    leastconnection(1),
	    roundrobin(2),
	    weighted(3)
	}
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Global Session Distribution Algorithm(SDA)"
	::= { snL4Gen 3 }

snL4slbTotalConnections 		OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Total connections in this device"
	::= { snL4Gen 4 }

snL4slbLimitExceeds 		OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"exceeds snL4TCPSynLimit (numbers of connection per second)"
	::= { snL4Gen 5 }

-- Server load balancing traffic info

snL4slbForwardTraffic 		OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Client->Server"
	::= { snL4Gen 6 }

snL4slbReverseTraffic 		OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Server->Client"
	::= { snL4Gen 7 }

snL4slbDrops 		OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4Gen 8 }

snL4slbDangling 		OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4Gen 9 }

snL4slbDisableCount 		OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4Gen 10 }

snL4slbAged 		OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4Gen 11 }

snL4slbFinished 		OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"FIN_or_RST"
	::= { snL4Gen 12 }

--  Session

snL4FreeSessionCount 		OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Maximum sessions - used sessions"
	::= { snL4Gen 13 }


--  Hot stand-by
snL4BackupInterface 		OBJECT-TYPE
	SYNTAX	INTEGER	  (0..26)
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"backup monitoring port"
	::= { snL4Gen 14 }

snL4BackupMacAddr 		OBJECT-TYPE
	SYNTAX	PhysAddress
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Associated MAC address for backup monitoring port"
	::= { snL4Gen 15 }

snL4Active 		OBJECT-TYPE
	SYNTAX	L4Flag
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4Gen 16 }

snL4Redundancy 		OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4Gen 17 }

snL4Backup 		OBJECT-TYPE
	SYNTAX	L4Flag
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"true->StandBy,false->active"
	::= { snL4Gen 18 }

snL4BecomeActive 		OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"How many times this device become active"
	::= { snL4Gen 19 }

snL4BecomeStandBy 		OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"How many times this device become standby"
	::= { snL4Gen 20 }

snL4BackupState 		OBJECT-TYPE
	SYNTAX	 INTEGER {
		slbSyncComplete(0),
	    slbSyncReqMap(1),
	    slbSyncreqMac(2),
	    slbSyncreqServers(3),
	    slbSyncReqL4(4)
	}
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Backup state"
	::= { snL4Gen 21 }

snL4NoPDUSent 		OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4Gen 22 }


snL4NoPDUCount 		OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4Gen 23 }


snL4NoPortMap 		OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4Gen 24 }

snL4unsuccessfulConn 	OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Unsuccessfull connection"
	::= { snL4Gen 25 }

snL4PingInterval 	OBJECT-TYPE
	SYNTAX	INTEGER	 (1..10)
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Ping retries interval"
    DEFVAL { 2 }
	::= { snL4Gen 26 }

snL4PingRetry 	OBJECT-TYPE
	SYNTAX	INTEGER	(2..10)
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Ping retries attempts"
    DEFVAL { 4 }
	::= { snL4Gen 27 }

snL4TcpAge 	OBJECT-TYPE
	SYNTAX	INTEGER	(2..60)
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"TCP reset age"
    DEFVAL { 30 }
	::= { snL4Gen 28 }


snL4UdpAge 	OBJECT-TYPE
	SYNTAX	INTEGER	(2..60)
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"UDP reset age"
    DEFVAL { 5 }
	::= { snL4Gen 29 }


-- Enable/disable L4 traps

snL4EnableMaxSessionLimitReachedTrap        OBJECT-TYPE
	SYNTAX INTEGER { disabled(0), enabled(1) }
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"Enable/disable maximum number of connections reached trap."
	::= { snL4Gen 30 }

snL4EnableTcpSynLimitReachedTrap            OBJECT-TYPE
	SYNTAX INTEGER { disabled(0), enabled(1) }
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"Enable/disable the number of TCP SYN limits reached trap."
	::= { snL4Gen 31 }

snL4EnableRealServerUpTrap                  OBJECT-TYPE
	SYNTAX INTEGER { disabled(0), enabled(1) }
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"Enable/disable the real server up trap."
	::= { snL4Gen 32 }

snL4EnableRealServerDownTrap                OBJECT-TYPE
	SYNTAX INTEGER { disabled(0), enabled(1) }
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"Enable/disable the real server down trap."
	::= { snL4Gen 33 }

snL4EnableRealServerPortUpTrap              OBJECT-TYPE
	SYNTAX INTEGER { disabled(0), enabled(1) }
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"Enable/disable the real server TCP port up trap."
	::= { snL4Gen 34 }

snL4EnableRealServerPortDownTrap            OBJECT-TYPE
	SYNTAX INTEGER { disabled(0), enabled(1) }
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"Enable/disable the real server TCP port down trap."
	::= { snL4Gen 35 }

snL4EnableRealServerMaxConnLimitReachedTrap OBJECT-TYPE
	SYNTAX INTEGER { disabled(0), enabled(1) }
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"Enable/disable the real server maximum number of
		connections reached trap."
	::= { snL4Gen 36 }

snL4EnableBecomeStandbyTrap                 OBJECT-TYPE
	SYNTAX INTEGER { disabled(0), enabled(1) }
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"Enable/disable trap of the server load balancing
		switch changes state from active to standby."
	::= { snL4Gen 37 }

snL4EnableBecomeActiveTrap                  OBJECT-TYPE
	SYNTAX INTEGER { disabled(0), enabled(1) }
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"Enable/disable trap of the server load balancing
		switch changes state from standby to active."
	::= { snL4Gen 38 }

snL4slbRouterInterfacePortMask 	OBJECT-TYPE
	SYNTAX	INTEGER	
	ACCESS  read-write
	STATUS  deprecated
	DESCRIPTION
		"Router interface port mask.
		(It was obsoleted after release 07100, replaced by snL4slbRouterInterfacePortList)"
	::= { snL4Gen 39 }

------- Server Cache Group Global MIBs ----------
snL4MaxNumWebCacheGroup 		OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"The maximum number of server cache groups"
	::= { snL4Gen 40 }

snL4MaxNumWebCachePerGroup 		OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"The maximum number of WEB Cache servers in each of web cache group"
	::= { snL4Gen 41 }

snL4WebCacheStateful 		OBJECT-TYPE
	SYNTAX	L4Status
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"The WEB Cache servers cache-stateful"
	::= { snL4Gen 42 }

------- GSLB Group Global MIBs ----------
snL4EnableGslbHealthCheckIpUpTrap        OBJECT-TYPE
	SYNTAX INTEGER { disabled(0), enabled(1) }
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"Health check IP up."
	::= { snL4Gen 43 }

snL4EnableGslbHealthCheckIpDownTrap        OBJECT-TYPE
	SYNTAX INTEGER { disabled(0), enabled(1) }
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"Health check IP down."
	::= { snL4Gen 44 }


snL4EnableGslbHealthCheckIpPortUpTrap        OBJECT-TYPE
	SYNTAX INTEGER { disabled(0), enabled(1) }
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"Health check IP port up."
	::= { snL4Gen 45 }


snL4EnableGslbHealthCheckIpPortDownTrap        OBJECT-TYPE
	SYNTAX INTEGER { disabled(0), enabled(1) }
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"Health check IP port down."
	::= { snL4Gen 46 }


snL4EnableGslbRemoteGslbSiDownTrap        OBJECT-TYPE
	SYNTAX INTEGER { disabled(0), enabled(1) }
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"Connection to GSLB ServerIron is down."
	::= { snL4Gen 47 }


snL4EnableGslbRemoteGslbSiUpTrap        OBJECT-TYPE
	SYNTAX INTEGER { disabled(0), enabled(1) }
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"Connection to GSLB ServerIron is up."
	::= { snL4Gen 48 }


snL4EnableGslbRemoteSiDownTrap        OBJECT-TYPE
	SYNTAX INTEGER { disabled(0), enabled(1) }
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"GSLB connection to remote ServerIron is down."
	::= { snL4Gen 49 }


snL4EnableGslbRemoteSiUpTrap        OBJECT-TYPE
	SYNTAX INTEGER { disabled(0), enabled(1) }
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"GSLB connection to remote ServerIron is up."
	::= { snL4Gen 50 }

snL4slbRouterInterfacePortList 	OBJECT-TYPE
	SYNTAX	OCTET STRING
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Router interface port list. Each port index is a 16-bit integer
		in big endian order. 8-bit is the slot number, the other 8-bit
		is the port number."
	::= { snL4Gen 51 }


-- Virtual Server table

snL4VirtualServerTable  OBJECT-TYPE
	SYNTAX	SEQUENCE OF SnL4VirtualServerEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"Virtual Server table."
	::= { snL4VirtualServer 1 }

snL4VirtualServerEntry  OBJECT-TYPE
	SYNTAX	SnL4VirtualServerEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"An entry in L4 Virtual Server table."
	INDEX	{ snL4VirtualServerIndex }
	::= { snL4VirtualServerTable 1 }

SnL4VirtualServerEntry ::= SEQUENCE {
	snL4VirtualServerIndex
		INTEGER,
    snL4VirtualServerName
        L4ServerName,
    snL4VirtualServerVirtualIP
		IpAddress,
    snL4VirtualServerAdminStatus
        L4Status,
	snL4VirtualServerSDAType
		INTEGER,
	snL4VirtualServerRowStatus
		L4RowSts,
    snL4VirtualServerDeleteState
        L4DeleteState
	}

snL4VirtualServerIndex  OBJECT-TYPE
	SYNTAX	INTEGER (1..64)
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"The table index for a Virtual Server  entry."
	::= { snL4VirtualServerEntry 1 }


snL4VirtualServerName  OBJECT-TYPE
	SYNTAX	L4ServerName
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Virtual server name."
	::= { snL4VirtualServerEntry 2 }

snL4VirtualServerVirtualIP
	OBJECT-TYPE
	SYNTAX IpAddress
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Virtual Server IP Address."
	::= { snL4VirtualServerEntry 3 }

snL4VirtualServerAdminStatus	OBJECT-TYPE
	SYNTAX	L4Status
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Virtual Server status is ether disabled(0) or enabled(1)."
	::= { snL4VirtualServerEntry 4 }

snL4VirtualServerSDAType  OBJECT-TYPE
	SYNTAX	 INTEGER {
		default(0),
	    leastconnection(1),
	    roundrobin(2),
	    weighted(3)
	}
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"TCP/UDP Sessions Distribution Algorithms Type."
	::= { snL4VirtualServerEntry 5 }

 snL4VirtualServerRowStatus OBJECT-TYPE
	SYNTAX  L4RowSts
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"To create or delete a virtual server
		entry."
	::= {snL4VirtualServerEntry  6 }

snL4VirtualServerDeleteState	OBJECT-TYPE
	SYNTAX	L4DeleteState
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Delete operation state." 
	::= { snL4VirtualServerEntry 7 }


-- Real Server table

snL4RealServerTable  OBJECT-TYPE
	SYNTAX	SEQUENCE OF SnL4RealServerEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"Real Server table."
	::= { snL4RealServer 1 }

snL4RealServerEntry  OBJECT-TYPE
	SYNTAX	SnL4RealServerEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"An entry in the Real Server table."
	INDEX	{ snL4RealServerIndex }
	::= { snL4RealServerTable 1 }

SnL4RealServerEntry ::= SEQUENCE {
	snL4RealServerIndex
		INTEGER,
    snL4RealServerName
        L4ServerName,
    snL4RealServerIP
		IpAddress,
    snL4RealServerAdminStatus
        L4Status,
	snL4RealServerMaxConnections
		INTEGER,
	snL4RealServerWeight
		INTEGER,
	snL4RealServerRowStatus
		L4RowSts,
    snL4RealServerDeleteState
        L4DeleteState
	}

snL4RealServerIndex  OBJECT-TYPE
	SYNTAX	INTEGER (1..256)
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"The table index for a Real Server entry."
	::= { snL4RealServerEntry 1 }
snL4RealServerName  OBJECT-TYPE
	SYNTAX	L4ServerName
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Real server name."
	::= { snL4RealServerEntry 2 }

snL4RealServerIP
	OBJECT-TYPE
	SYNTAX IpAddress
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Real Server IP Address."
	::= { snL4RealServerEntry 3 }

snL4RealServerAdminStatus	OBJECT-TYPE
	SYNTAX	L4Status
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Real Server status is ether disabled(0) or enabled(1)."
	::= { snL4RealServerEntry 4 }

snL4RealServerMaxConnections 	OBJECT-TYPE
	SYNTAX	INTEGER	 (0..1000000)
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Real Server Maximum Connection allowed."
	::= { snL4RealServerEntry 5 }

 snL4RealServerWeight	OBJECT-TYPE
	SYNTAX	INTEGER	  (0..65000)
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Real Server weight"
	::= { snL4RealServerEntry 6 }

 snL4RealServerRowStatus OBJECT-TYPE
	SYNTAX  L4RowSts
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"To create or delete a real server entry."
	::= {snL4RealServerEntry  7 }

snL4RealServerDeleteState	OBJECT-TYPE
	SYNTAX	L4DeleteState
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Delete operation state." 
	::= { snL4RealServerEntry 8 }



-- Virtual Server Port table

snL4VirtualServerPortTable	       OBJECT-TYPE
	SYNTAX	SEQUENCE OF SnL4VirtualServerPortEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"Virtual Server Port table."
	::= { snL4VirtualServerPort 1 }

snL4VirtualServerPortEntry	       OBJECT-TYPE
	SYNTAX	SnL4VirtualServerPortEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"An entry in the Virtual Server Port table."
	INDEX	{ snL4VirtualServerPortIndex }
	::= { snL4VirtualServerPortTable 1 }

SnL4VirtualServerPortEntry ::= SEQUENCE {
	snL4VirtualServerPortIndex
		INTEGER,
	snL4VirtualServerPortServerName
        L4ServerName,
	snL4VirtualServerPortPort
		INTEGER,
	snL4VirtualServerPortAdminStatus
		L4Status,
	snL4VirtualServerPortSticky
		INTEGER,
	snL4VirtualServerPortConcurrent
		INTEGER,
	snL4VirtualServerPortRowStatus
		L4RowSts,
    snL4VirtualServerPortDeleteState
        L4DeleteState
	}


snL4VirtualServerPortIndex	       OBJECT-TYPE
	SYNTAX	INTEGER (1..2048)
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"The index for Virtual Server Port entry."
	::= { snL4VirtualServerPortEntry 1 }


snL4VirtualServerPortServerName	       OBJECT-TYPE
	SYNTAX	L4ServerName
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerPortEntry 2 }

snL4VirtualServerPortPort       OBJECT-TYPE
	SYNTAX	INTEGER	  (0..65535)
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerPortEntry 3 }


snL4VirtualServerPortAdminStatus		       OBJECT-TYPE
	SYNTAX	L4Status
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerPortEntry 4 }


 snL4VirtualServerPortSticky       OBJECT-TYPE
	 SYNTAX  INTEGER {
			disabled(0),
			enabled(1)       
			}
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerPortEntry 5 }


 snL4VirtualServerPortConcurrent       OBJECT-TYPE
	 SYNTAX  INTEGER {
			disabled(0),
			enabled(1)       
			}
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerPortEntry 6 }


 snL4VirtualServerPortRowStatus	 	       OBJECT-TYPE
	SYNTAX L4RowSts	
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"To create or delete a virtual server  port entry."
	::= { snL4VirtualServerPortEntry 7 }

snL4VirtualServerPortDeleteState	OBJECT-TYPE
	SYNTAX	L4DeleteState
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Delete operation state." 
	::= { snL4VirtualServerPortEntry 8 }




-- Real Server Port table

snL4RealServerPortTable	       OBJECT-TYPE
	SYNTAX	SEQUENCE OF SnL4RealServerPortEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"Real Server Port table."
	::= { snL4RealServerPort 1 }

snL4RealServerPortEntry	       OBJECT-TYPE
	SYNTAX	SnL4RealServerPortEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"An entry in the Real Server Port table."
	INDEX	{ snL4RealServerPortIndex }
	::= { snL4RealServerPortTable 1 }

SnL4RealServerPortEntry ::= SEQUENCE {
	snL4RealServerPortIndex
		INTEGER,
	snL4RealServerPortServerName
        L4ServerName,
	snL4RealServerPortPort
		INTEGER,
	snL4RealServerPortAdminStatus
		L4Status,
	snL4RealServerPortRowStatus
		L4RowSts,
    snL4RealServerPortDeleteState
        L4DeleteState
	}


snL4RealServerPortIndex	       OBJECT-TYPE
	SYNTAX	INTEGER (1..2048)
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"The index for Real Server Port entry."
	::= { snL4RealServerPortEntry 1 }
snL4RealServerPortServerName	       OBJECT-TYPE
	SYNTAX	L4ServerName
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerPortEntry 2 }

snL4RealServerPortPort       OBJECT-TYPE
	SYNTAX	INTEGER	 (0..65535)
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerPortEntry 3 }


snL4RealServerPortAdminStatus		       OBJECT-TYPE
	SYNTAX	L4Status
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerPortEntry 4 }

 snL4RealServerPortRowStatus	 	       OBJECT-TYPE
	SYNTAX L4RowSts	
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"To create or delete a Real server  port entry."
	::= { snL4RealServerPortEntry 5 }

snL4RealServerPortDeleteState	OBJECT-TYPE
	SYNTAX	L4DeleteState
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Delete operation state." 
	::= { snL4RealServerPortEntry 6 }



-- Bind table

snL4BindTable	       OBJECT-TYPE
	SYNTAX	SEQUENCE OF SnL4BindEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"Bind table."
	::= { snL4Bind 1 }

snL4BindEntry	       OBJECT-TYPE
	SYNTAX	SnL4BindEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"An entry in the Bind table."
	INDEX	{ snL4BindIndex }
	::= { snL4BindTable 1 }

SnL4BindEntry ::= SEQUENCE {
	snL4BindIndex
		INTEGER,
	snL4BindVirtualServerName
        L4ServerName,
	snL4BindVirtualPortNumber
		INTEGER,
	snL4BindRealServerName
        L4ServerName,
	snL4BindRealPortNumber
		INTEGER,
	snL4BindRowStatus
		INTEGER
	}


snL4BindIndex	       OBJECT-TYPE
	SYNTAX	INTEGER (1..2048)
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"The index for Bind entry."
	::= { snL4BindEntry 1 }

snL4BindVirtualServerName 	       OBJECT-TYPE
	SYNTAX	L4ServerName
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4BindEntry 2 }

snL4BindVirtualPortNumber        OBJECT-TYPE
	SYNTAX	INTEGER	 (0..65535)
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4BindEntry 3 }


 snL4BindRealServerName	       OBJECT-TYPE
	SYNTAX	L4ServerName
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4BindEntry 4 }

snL4BindRealPortNumber       OBJECT-TYPE
	SYNTAX	INTEGER	 (0..65535)
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4BindEntry 5 }
snL4BindRowStatus  	 	       OBJECT-TYPE
	SYNTAX	 INTEGER {
			  other(1),
			  valid(2),
			 delete(3),
			 create(4)
	}
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"To create or delete bind entry."
	::= { snL4BindEntry 6 }





-- Virtual Server Status table

snL4VirtualServerStatusTable  OBJECT-TYPE
	SYNTAX	SEQUENCE OF SnL4VirtualServerStatusEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"Virtual Server Status table."
	::= { snL4VirtualServerStatus 1 }

snL4VirtualServerStatusEntry  OBJECT-TYPE
	SYNTAX	SnL4VirtualServerStatusEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"An entry in L4 Virtual Server Status table."
	INDEX	{ snL4VirtualServerStatusIndex }
	::= { snL4VirtualServerStatusTable 1 }

SnL4VirtualServerStatusEntry ::= SEQUENCE {
	snL4VirtualServerStatusIndex
		INTEGER,
    snL4VirtualServerStatusName
        L4ServerName,
	snL4VirtualServerStatusReceivePkts
		Counter,
	snL4VirtualServerStatusTransmitPkts
		Counter,
	snL4VirtualServerStatusTotalConnections
		Counter
	}

snL4VirtualServerStatusIndex  OBJECT-TYPE
	SYNTAX	INTEGER (1..64)
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"The table index for a Virtual Server  Status entry."
	::= { snL4VirtualServerStatusEntry 1 }


snL4VirtualServerStatusName  OBJECT-TYPE
	SYNTAX	L4ServerName
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Virtual server name."
	::= { snL4VirtualServerStatusEntry 2 }


snL4VirtualServerStatusReceivePkts  OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS  mandatory
	DESCRIPTION
		"" 
	::= { snL4VirtualServerStatusEntry 3 }

snL4VirtualServerStatusTransmitPkts  OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS  mandatory
	DESCRIPTION
		"" 
	::= { snL4VirtualServerStatusEntry 4 }

snL4VirtualServerStatusTotalConnections  OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS  mandatory
	DESCRIPTION
		"" 
	::= { snL4VirtualServerStatusEntry 5 }


-- Real Server Status Table

snL4RealServerStatusTable  OBJECT-TYPE
	SYNTAX	SEQUENCE OF SnL4RealServerStatusEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"Real Server Status table."
	::= { snL4RealServerStatus 1 }

snL4RealServerStatusEntry  OBJECT-TYPE
	SYNTAX	SnL4RealServerStatusEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"An entry in the Real Server Status table."
	INDEX	{ snL4RealServerStatusIndex }
	::= { snL4RealServerStatusTable 1 }

SnL4RealServerStatusEntry ::= SEQUENCE {
	snL4RealServerStatusIndex
		INTEGER,
    snL4RealServerStatusName
        L4ServerName,
    snL4RealServerStatusRealIP
		IpAddress,
	snL4RealServerStatusReceivePkts
		Counter,
	snL4RealServerStatusTransmitPkts
		Counter,
	snL4RealServerStatusCurConnections
		INTEGER,
	snL4RealServerStatusTotalConnections
		Counter,
	snL4RealServerStatusAge
		INTEGER,
	snL4RealServerStatusState
		INTEGER,
	snL4RealServerStatusReassignments
		INTEGER,
	snL4RealServerStatusReassignmentLimit
		INTEGER,
	snL4RealServerStatusFailedPortExists
		INTEGER,
	snL4RealServerStatusFailTime
		INTEGER,
	snL4RealServerStatusPeakConnections
		INTEGER
	}

snL4RealServerStatusIndex  OBJECT-TYPE
	SYNTAX	INTEGER	 (1..256)
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"The table index for a Real Server Status entry."
	::= { snL4RealServerStatusEntry 1 }

snL4RealServerStatusName OBJECT-TYPE
	SYNTAX	L4ServerName
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerStatusEntry 2 }

snL4RealServerStatusRealIP OBJECT-TYPE
	SYNTAX	IpAddress
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerStatusEntry 3 }

snL4RealServerStatusReceivePkts	  OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerStatusEntry 4 }

snL4RealServerStatusTransmitPkts  OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerStatusEntry 5 }

snL4RealServerStatusCurConnections   OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerStatusEntry 6 }

snL4RealServerStatusTotalConnections   OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerStatusEntry 7 }

snL4RealServerStatusAge  OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerStatusEntry 8 }

snL4RealServerStatusState  OBJECT-TYPE
	SYNTAX	INTEGER	{
	serverdisabled(0),
	serverenabled(1),
	serverfailed(2),
	servertesting(3),
	serversuspect(4),
	servershutdown(5),
	serveractive(6)
	}
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerStatusEntry 9 }

snL4RealServerStatusReassignments  OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerStatusEntry 10 }

snL4RealServerStatusReassignmentLimit  OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerStatusEntry 11 }

snL4RealServerStatusFailedPortExists  OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerStatusEntry 12 }

snL4RealServerStatusFailTime  OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerStatusEntry 13 }


snL4RealServerStatusPeakConnections   OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerStatusEntry 14 }




-- Virtual Server Port Status table

snL4VirtualServerPortStatusTable	       OBJECT-TYPE
	SYNTAX	SEQUENCE OF SnL4VirtualServerPortStatusEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"Virtual Server Port Status table."
	::= { snL4VirtualServerPortStatus 1 }

snL4VirtualServerPortStatusEntry	       OBJECT-TYPE
	SYNTAX	SnL4VirtualServerPortStatusEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"An entry in the Virtual Server Port Status table."
	INDEX	{ snL4VirtualServerPortStatusIndex }
	::= { snL4VirtualServerPortStatusTable 1 }

SnL4VirtualServerPortStatusEntry ::= SEQUENCE {
	snL4VirtualServerPortStatusIndex
		INTEGER,
	snL4VirtualServerPortStatusPort
		INTEGER,
	snL4VirtualServerPortStatusServerName
        L4ServerName,
	snL4VirtualServerPortStatusCurrentConnection
		INTEGER,
	snL4VirtualServerPortStatusTotalConnection
		Counter,
	snL4VirtualServerPortStatusPeakConnection
		INTEGER
	}

snL4VirtualServerPortStatusIndex	       OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"The index for Virtual Server Port Status entry."
	::= { snL4VirtualServerPortStatusEntry 1 }

snL4VirtualServerPortStatusPort   OBJECT-TYPE
	SYNTAX	INTEGER	 (1..2048)
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerPortStatusEntry 2 }

 snL4VirtualServerPortStatusServerName 	       OBJECT-TYPE
	SYNTAX	L4ServerName
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerPortStatusEntry 3 }

 snL4VirtualServerPortStatusCurrentConnection 	       OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerPortStatusEntry 4 }

 snL4VirtualServerPortStatusTotalConnection		       OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerPortStatusEntry 5 }

 snL4VirtualServerPortStatusPeakConnection 	       OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerPortStatusEntry 6 }

-- Real Server Port Status table

snL4RealServerPortStatusTable	       OBJECT-TYPE
	SYNTAX	SEQUENCE OF SnL4RealServerPortStatusEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"Real Server Port Status table."
	::= { snL4RealServerPortStatus 1 }

snL4RealServerPortStatusEntry	       OBJECT-TYPE
	SYNTAX	SnL4RealServerPortStatusEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"An entry in the Real Server Port Status table."
	INDEX	{ snL4RealServerPortStatusIndex }
	::= { snL4RealServerPortStatusTable 1 }

SnL4RealServerPortStatusEntry ::= SEQUENCE {
	snL4RealServerPortStatusIndex
		INTEGER,
	snL4RealServerPortStatusPort
		INTEGER,
	snL4RealServerPortStatusServerName
        L4ServerName,
	snL4RealServerPortStatusReassignCount
		INTEGER,
	snL4RealServerPortStatusState
		INTEGER,
	snL4RealServerPortStatusFailTime
		INTEGER,
	snL4RealServerPortStatusCurrentConnection
		INTEGER,
	snL4RealServerPortStatusTotalConnection
		Counter,
	snL4RealServerPortStatusRxPkts
		Counter,
	snL4RealServerPortStatusTxPkts
		Counter,
	snL4RealServerPortStatusRxBytes
		Counter,
	snL4RealServerPortStatusTxBytes
		Counter,
	snL4RealServerPortStatusPeakConnection
		INTEGER
	}


snL4RealServerPortStatusIndex	       OBJECT-TYPE
	SYNTAX	INTEGER	  (1..2048)
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"The index for Real Server Port Status entry."
	::= { snL4RealServerPortStatusEntry 1 }

snL4RealServerPortStatusPort	       OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerPortStatusEntry 2 }

snL4RealServerPortStatusServerName	       OBJECT-TYPE
	SYNTAX	L4ServerName
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerPortStatusEntry 3 }

snL4RealServerPortStatusReassignCount	       OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerPortStatusEntry 4 }

 snL4RealServerPortStatusState	       OBJECT-TYPE
	SYNTAX	INTEGER	{
		disabled(0),
		enabled(1),
		failed(2),
		testing(3),
		suspect(4),
	    shutdown(5),
		active(6),
		unbound(7),
		awaitUnbind(8),
		awaitDelete(9)
	}
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Real server port state"
	::= { snL4RealServerPortStatusEntry 5 }

snL4RealServerPortStatusFailTime 	       OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Only useful, if real server port state is failed.
		 Indicating how seconds has been elapsed from the last retry."
 	::= { snL4RealServerPortStatusEntry 6 }

snL4RealServerPortStatusCurrentConnection	       OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Real server port current connection"
	::= { snL4RealServerPortStatusEntry 7 }

snL4RealServerPortStatusTotalConnection	       OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Real server port total connection"
	::= { snL4RealServerPortStatusEntry 8 }

snL4RealServerPortStatusRxPkts	       OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Real server port receive packets."
	::= { snL4RealServerPortStatusEntry 9 }


snL4RealServerPortStatusTxPkts	       OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Real server port transmit packets."
	::= { snL4RealServerPortStatusEntry 10 }


snL4RealServerPortStatusRxBytes	       OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Real server port receive bytes."
	::= { snL4RealServerPortStatusEntry 11 }

snL4RealServerPortStatusTxBytes	       OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Real server port transmit bytes."
	::= { snL4RealServerPortStatusEntry 12 }


snL4RealServerPortStatusPeakConnection	       OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"peak connection for real server port."
	::= { snL4RealServerPortStatusEntry 13 }




-- L4 policy table

snL4PolicyTable	  OBJECT-TYPE
	SYNTAX	SEQUENCE OF SnL4PolicyEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"L4 policy table."
	::= {snL4Policy  1 }

snL4PolicyEntry	  OBJECT-TYPE
	SYNTAX	SnL4PolicyEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"An entry of the L4 policy table."
	INDEX	{ snL4PolicyId }
	::= { snL4PolicyTable 1 }

SnL4PolicyEntry ::= SEQUENCE {
	snL4PolicyId
		INTEGER,
	snL4PolicyPriority
		INTEGER,
	snL4PolicyScope
		INTEGER,
	snL4PolicyProtocol
		INTEGER,
	snL4PolicyPort
		INTEGER,
	snL4PolicyRowStatus
		INTEGER
	}

snL4PolicyId         OBJECT-TYPE
	SYNTAX	INTEGER (1..64)
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"The  ID to identify a  entry."
	::= { snL4PolicyEntry 1 }

snL4PolicyPriority	   OBJECT-TYPE
	SYNTAX  INTEGER {
		level0(0),
		level1(1),
		level2(2),
		level3(3),
		level4(4),
		level5(5),
		level6(6),
		level7(7)
		}
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"The Stand alone stackable switch L4 Policy Priority values are:
		 normal(0)   		 -- normal prority
		 high(1) 	 		 -- high prority
		 cache(2) 	 		 -- prority for cache
		 transparent(3) 	 -- prority for transparent
		 The BigIron switch L4 Priority values are:
		level0(0), level1(1), level2(2), level3(3),
		level4(4), level5(5), level6(6), level7(7) "
	::= { snL4PolicyEntry 2 }

snL4PolicyScope	   OBJECT-TYPE
	SYNTAX	INTEGER { global(0), local(1) }
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		" Scope of the  local or global.
		  Global  automatic apply to all port.
		  Local  apply to a port."
	::= { snL4PolicyEntry 3 }

snL4PolicyProtocol     OBJECT-TYPE
	SYNTAX	INTEGER { udp(0), tcp(1) }

	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4PolicyEntry 4 }

snL4PolicyPort OBJECT-TYPE
	SYNTAX	INTEGER	 (0..65535)
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION ""
	::= { snL4PolicyEntry 5 }

snL4PolicyRowStatus  OBJECT-TYPE
	SYNTAX	INTEGER {
	    invalid(1),
	    valid(2),
	    delete(3),
	    create(4),
	    modify(5)
	}
	ACCESS	 read-write
	STATUS	 mandatory
	DESCRIPTION
		"This object is used to create and
		delete row in the table and control
		if they are used. The values
		that can be written are:
		delete(3)...deletes the row
		create(4)...creates a new row
		modify(5)...modifies an exsisting row

		If the row exists, then a SET with
		value of create(4) returns error
		'badValue'. Deleted rows go away
		immediately. The following values
		can be returned on reads:
		invalid(1)...Setting it to 'invalid' has the effect of
		             rendering it inoperative.
		valid(2).....the row exists and is valid"
	::= { snL4PolicyEntry 6 }

-- L4 policy port access table

snL4PolicyPortAccessTable	     OBJECT-TYPE
	SYNTAX	SEQUENCE OF SnL4PolicyPortAccessEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"ip interface L4 policy access table."
	::= {snL4PolicyPortAccess  1}

snL4PolicyPortAccessEntry	     OBJECT-TYPE
	SYNTAX	SnL4PolicyPortAccessEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"An entry of the ip interface L4 policy access  table."
	INDEX	{ snL4PolicyPortAccessPort }
	::= { snL4PolicyPortAccessTable 1 }

SnL4PolicyPortAccessEntry ::= SEQUENCE {
	snL4PolicyPortAccessPort
		INTEGER,
	snL4PolicyPortAccessList
		OCTET STRING,
	snL4PolicyPortAccessRowStatus
		INTEGER
	}

snL4PolicyPortAccessPort	     OBJECT-TYPE
	SYNTAX	INTEGER	
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"The ip interface to which the L4 policy  applies."
	::= { snL4PolicyPortAccessEntry 1 }

snL4PolicyPortAccessList  OBJECT-TYPE
	SYNTAX	OCTET STRING (SIZE(1..64))
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"An ip L4 policy  list, of which each octet contains
		a  ID number that forms a group of s. A
		valid entry in the snL4PolicyTable with the
		corresponding  ID number (i.e. snL4PolicyId)
		must have been created before a  list is initialized."
	::= { snL4PolicyPortAccessEntry 2 }

snL4PolicyPortAccessRowStatus   OBJECT-TYPE
	SYNTAX	 INTEGER {
	    invalid(1),
	    valid(2),
	    delete(3),
	    create(4),
	    modify(5)
	}
	ACCESS	 read-write
	STATUS	 mandatory
	DESCRIPTION
		"This object is used to create and
		delete row in the table and control
		if they are used. The values
		that can be written are:
		delete(3)...deletes the row
		create(4)...creates a new row
		modify(5)...modifies an exsisting row

		If the row exists, then a SET with
		value of create(4) returns error
		'badValue'. Deleted rows go away
		immediately. The following values
		can be returned on reads:
		invalid(1)...Setting it to 'invalid' has the effect of
		             rendering it inoperative.
		valid(2).....the row exists and is valid"
	::= { snL4PolicyPortAccessEntry 3 }

-- L4 trap variable binding objects

snL4TrapRealServerIP             OBJECT-TYPE
	SYNTAX IpAddress
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION
		"Real server IP address."
	::= { snL4Trap 1 }

snL4TrapRealServerName           OBJECT-TYPE
	SYNTAX L4ServerName
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION
		"Real server name."
	::= { snL4Trap 2 }

snL4TrapRealServerPort           OBJECT-TYPE
	SYNTAX INTEGER
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION
		"Transport protocol port number of the real server."
	::= { snL4Trap 3 }

snL4TrapRealServerCurConnections OBJECT-TYPE
	SYNTAX INTEGER
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION
		"Real Server current connections."
	::= { snL4Trap 4 }

snL4TrapLinkName OBJECT-TYPE
	SYNTAX L4ServerName
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION
		"Link name."
	::= { snL4Trap 5 }

snL4LinkVirtualInterface OBJECT-TYPE
	SYNTAX INTEGER
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION
		"Link virtual interface."
	::= { snL4Trap 6 }

-- Web Cache table

snL4WebCacheTable  OBJECT-TYPE
	SYNTAX	SEQUENCE OF SnL4WebCacheEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"Real Server table."
	::= { snL4WebCache 1 }

snL4WebCacheEntry  OBJECT-TYPE
	SYNTAX	SnL4WebCacheEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"An entry in the Real Server table."
	INDEX	{ snL4WebCacheIP }
	::= { snL4WebCacheTable 1 }

SnL4WebCacheEntry ::= SEQUENCE {
    snL4WebCacheIP
		IpAddress,
    snL4WebCacheName
        L4ServerName,
    snL4WebCacheAdminStatus
        L4Status,
	snL4WebCacheMaxConnections
		INTEGER,
	snL4WebCacheWeight
		INTEGER,
	snL4WebCacheRowStatus
		L4RowSts,
    snL4WebCacheDeleteState
        L4DeleteState
	}

snL4WebCacheIP
	OBJECT-TYPE
	SYNTAX IpAddress
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Real Server IP Address."
	::= { snL4WebCacheEntry 1 }

snL4WebCacheName  OBJECT-TYPE
	SYNTAX	L4ServerName
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Real server name."
	::= { snL4WebCacheEntry 2 }

snL4WebCacheAdminStatus	OBJECT-TYPE
	SYNTAX	L4Status
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Real Server status is ether disabled(0) or enabled(1)."
	::= { snL4WebCacheEntry 3 }

snL4WebCacheMaxConnections 	OBJECT-TYPE
	SYNTAX	INTEGER	 (0..1000000)
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Real Server Maximum Connection allowed."
	::= { snL4WebCacheEntry 4 }

 snL4WebCacheWeight	OBJECT-TYPE
	SYNTAX	INTEGER	  (1..65000)
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Real Server weight"
	::= { snL4WebCacheEntry 5 }

 snL4WebCacheRowStatus OBJECT-TYPE
	SYNTAX  L4RowSts
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"To create or delete a real server entry."
	::= {snL4WebCacheEntry  6 }

snL4WebCacheDeleteState	OBJECT-TYPE
	SYNTAX	L4DeleteState
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Delete operation state." 
	::= { snL4WebCacheEntry 7 }


-- Web Cache Group table


snL4WebCacheGroupTable  OBJECT-TYPE
	SYNTAX	SEQUENCE OF SnL4WebCacheGroupEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"Web Cache Group table."
	::= { snL4WebCacheGroup 1 }

snL4WebCacheGroupEntry  OBJECT-TYPE
	SYNTAX	SnL4WebCacheGroupEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"An entry in the  Web Cache Group table."
	INDEX	{ snL4WebCacheGroupId }
	::= { snL4WebCacheGroupTable 1 }

SnL4WebCacheGroupEntry ::= SEQUENCE {
	snL4WebCacheGroupId
		INTEGER,
    snL4WebCacheGroupName
        L4ServerName,
    snL4WebCacheGroupWebCacheIpList
		OCTET STRING,
    snL4WebCacheGroupDestMask
		IpAddress,
    snL4WebCacheGroupSrcMask
		IpAddress,
	snL4WebCacheGroupAdminStatus
		INTEGER,
	snL4WebCacheGroupRowStatus
		L4RowSts
	}

snL4WebCacheGroupId  OBJECT-TYPE
	SYNTAX	INTEGER 
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"The identification for a Web Cache Group entry.
		 The limit is from 1 to snL4MaxNumWebCacheGroup."
	::= { snL4WebCacheGroupEntry 1 }

snL4WebCacheGroupName  OBJECT-TYPE
	SYNTAX	L4ServerName
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Web Cache Group name."
	::= { snL4WebCacheGroupEntry 2 }

snL4WebCacheGroupWebCacheIpList
	OBJECT-TYPE
	SYNTAX	OCTET STRING
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"A list of the Server Cache Group Real Server IP Address.
		 The number of IP Address is from 1 (4 OCTETs) to the 
		 snL4MaxNumServersPerWebCacheGroup, maximum number of 
		 server IP Address allowed in the list."
	::= { snL4WebCacheGroupEntry 3 }

snL4WebCacheGroupDestMask 	OBJECT-TYPE
	SYNTAX  IpAddress
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Cache Server Group Destination Mask."
	::= { snL4WebCacheGroupEntry 4 }

snL4WebCacheGroupSrcMask 	OBJECT-TYPE
	SYNTAX  IpAddress
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Cache Server Group Source Mask."
	::= { snL4WebCacheGroupEntry 5 }

snL4WebCacheGroupAdminStatus OBJECT-TYPE
	SYNTAX  INTEGER {
		disabled(0),             
		enabled(1)
		}
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"The WEB Cache Group is set either
		 enabled(1)...........activated.
		 disabled(0)..........disabled."  
	::= { snL4WebCacheGroupEntry 6 }

 snL4WebCacheGroupRowStatus OBJECT-TYPE
	SYNTAX  L4RowSts
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"To create or delete a Web Cache Group entry."
	::= { snL4WebCacheGroupEntry 7 }


-- Web Cache Traffic Statistics Table 

snL4WebCacheTrafficStatsTable  OBJECT-TYPE
	SYNTAX	SEQUENCE OF SnL4WebCacheTrafficStatsEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"Web Cache Traffic Statistics table."
	::= { snL4WebCacheTrafficStats 1 }

snL4WebCacheTrafficStatsEntry  OBJECT-TYPE
	SYNTAX	SnL4WebCacheTrafficStatsEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"An entry in the Web Cache Traffic Statistics table."
	INDEX	{ snL4WebCacheTrafficIp , snL4WebCacheTrafficPort}
	::= { snL4WebCacheTrafficStatsTable 1 }

SnL4WebCacheTrafficStatsEntry ::= SEQUENCE {
    snL4WebCacheTrafficIp
		IpAddress,
    snL4WebCacheTrafficPort
		INTEGER,
    snL4WebCacheCurrConnections
		INTEGER,
    snL4WebCacheTotalConnections
		INTEGER,
	snL4WebCacheTxPkts
		Counter,
	snL4WebCacheRxPkts
		Counter,
	snL4WebCacheTxOctets
		Counter,
	snL4WebCacheRxOctets
		Counter,
    snL4WebCachePortState
		WebCacheState
	}

snL4WebCacheTrafficIp 	OBJECT-TYPE
	SYNTAX  IpAddress
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Cache Server IP Address."
	::= { snL4WebCacheTrafficStatsEntry 1 }

snL4WebCacheTrafficPort 		OBJECT-TYPE
    SYNTAX  INTEGER (0..65535)
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"The WEB Cache port is one of the protocol port such as UDP, TCP etc."
	::= { snL4WebCacheTrafficStatsEntry 2 }

snL4WebCacheCurrConnections 		OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Number of the current connections in WEB Cache group."
	::= { snL4WebCacheTrafficStatsEntry 3 }

snL4WebCacheTotalConnections 		OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"The total connections in WEB Cache group."
	::= { snL4WebCacheTrafficStatsEntry 4 }

snL4WebCacheTxPkts 		OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Number of the Packets sending from Client/Web-Server to Cache Server"
	::= { snL4WebCacheTrafficStatsEntry 5 }

snL4WebCacheRxPkts 		OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Number of the Packets sending from Cache Server to Client/Web-Server"
	::= { snL4WebCacheTrafficStatsEntry 6 }

snL4WebCacheTxOctets 		OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Number of the Octets sending from Client/Web-Server to Cache Server"
	::= { snL4WebCacheTrafficStatsEntry 7 }

snL4WebCacheRxOctets 		OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Number of the Octets sending from Cache Server to Client/Web-Server"
	::= { snL4WebCacheTrafficStatsEntry 8 }

snL4WebCachePortState	OBJECT-TYPE
	SYNTAX	WebCacheState
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Web Cache Port state." 
	::= { snL4WebCacheTrafficStatsEntry 9 }

-- Web Uncached Traffic Statistics Table 

snL4WebUncachedTrafficStatsTable  OBJECT-TYPE
	SYNTAX	SEQUENCE OF SnL4WebUncachedTrafficStatsEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"Web Uncached Traffic Statistics table."
	::= { snL4WebUncachedTrafficStats 1 }

snL4WebUncachedTrafficStatsEntry  OBJECT-TYPE
	SYNTAX	SnL4WebUncachedTrafficStatsEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"An entry in the Web Uncached Traffic Statistics table."
	INDEX	{ snL4WebServerPort, snL4WebClientPort }
	::= { snL4WebUncachedTrafficStatsTable 1 }

SnL4WebUncachedTrafficStatsEntry ::= SEQUENCE {
    snL4WebServerPort
		INTEGER,
    snL4WebClientPort
		INTEGER,
	snL4WebUncachedTxPkts
		Counter,
	snL4WebUncachedRxPkts
		Counter,
	snL4WebUncachedTxOctets
		Counter,
	snL4WebUncachedRxOctets
		Counter,
    snL4WebServerPortName
		DisplayString,
    snL4WebClientPortName
		DisplayString
	}

snL4WebServerPort 			OBJECT-TYPE
	SYNTAX  INTEGER 
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Web Server Port."
	::= { snL4WebUncachedTrafficStatsEntry 1 }

snL4WebClientPort 			OBJECT-TYPE
	SYNTAX  INTEGER 
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Web Client Port."
	::= { snL4WebUncachedTrafficStatsEntry 2 }

snL4WebUncachedTxPkts 		OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Number of the Packets sending from Client port to Web Server port"
	::= { snL4WebUncachedTrafficStatsEntry 3 }

snL4WebUncachedRxPkts 		OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Number of the Packets sending from Web Server port to Client port"
	::= { snL4WebUncachedTrafficStatsEntry 4 }

snL4WebUncachedTxOctets 	OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Number of the Octets sending from Client port to Web Server port"
	::= { snL4WebUncachedTrafficStatsEntry 5 }

snL4WebUncachedRxOctets 	OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Number of the Octets sending from Web Server port to Client port"
	::= { snL4WebUncachedTrafficStatsEntry 6 }

snL4WebServerPortName OBJECT-TYPE
	SYNTAX	DisplayString (SIZE(0..16))
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Web Server Port Name string."
	::= { snL4WebUncachedTrafficStatsEntry 7 }

snL4WebClientPortName OBJECT-TYPE
	SYNTAX	DisplayString (SIZE(0..16))
	ACCESS	read-only
	STATUS	mandatory
	DESCRIPTION
		"Web Client Port Name string."
	::= { snL4WebUncachedTrafficStatsEntry 8 }


-- Web Cache Server Port table

snL4WebCachePortTable	       OBJECT-TYPE
	SYNTAX	SEQUENCE OF SnL4WebCachePortEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"Real Server Port table."
	::= { snL4WebCachePort 1 }

snL4WebCachePortEntry	       OBJECT-TYPE
	SYNTAX	SnL4WebCachePortEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"An entry in the Real Server Port table."
	INDEX	{ snL4WebCachePortServerIp, snL4WebCachePortPort }
	::= { snL4WebCachePortTable 1 }

SnL4WebCachePortEntry ::= SEQUENCE {
    snL4WebCachePortServerIp
		IpAddress,
    snL4WebCachePortPort
		INTEGER,
	snL4WebCachePortAdminStatus
		L4Status,
	snL4WebCachePortRowStatus
		L4RowSts,
    snL4WebCachePortDeleteState
		L4DeleteState
	}


snL4WebCachePortServerIp 	OBJECT-TYPE
	SYNTAX  IpAddress
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Cache Server IP Address."
	::= { snL4WebCachePortEntry 1 }

snL4WebCachePortPort 		OBJECT-TYPE
    SYNTAX  INTEGER (0..65535)
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"The WEB Cache port is one of the protocol port such as UDP, TCP etc."
	::= { snL4WebCachePortEntry 2 }

snL4WebCachePortAdminStatus		       OBJECT-TYPE
	SYNTAX	L4Status
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4WebCachePortEntry 3 }

 snL4WebCachePortRowStatus	 	       OBJECT-TYPE
	SYNTAX 	L4RowSts	
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"To create or delete a Real server  port entry."
	::= { snL4WebCachePortEntry 4 }

snL4WebCachePortDeleteState	OBJECT-TYPE
	SYNTAX	L4DeleteState
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Delete operation state." 
	::= { snL4WebCachePortEntry 5 }

-- Real Server Configuration table 

snL4RealServerCfgTable  OBJECT-TYPE
	SYNTAX	SEQUENCE OF SnL4RealServerCfgEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"Real Server table."
	::= { snL4RealServerCfg 1 }

snL4RealServerCfgEntry  OBJECT-TYPE
	SYNTAX	SnL4RealServerCfgEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"An entry in the Real Server table."
	INDEX	{ snL4RealServerCfgIP }
	::= { snL4RealServerCfgTable 1 }

SnL4RealServerCfgEntry ::= SEQUENCE {
    snL4RealServerCfgIP
		IpAddress,
    snL4RealServerCfgName
        L4ServerName,
    snL4RealServerCfgAdminStatus
        L4Status,
	snL4RealServerCfgMaxConnections
		INTEGER,
	snL4RealServerCfgWeight
		INTEGER,
	snL4RealServerCfgRowStatus
		L4RowSts,
    snL4RealServerCfgDeleteState
        L4DeleteState
	}

snL4RealServerCfgIP		OBJECT-TYPE
	SYNTAX IpAddress
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Real Server IP Address."
	::= { snL4RealServerCfgEntry 1 }
snL4RealServerCfgName  OBJECT-TYPE
	SYNTAX	L4ServerName
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Real server name."
	::= { snL4RealServerCfgEntry 2 }

snL4RealServerCfgAdminStatus	OBJECT-TYPE
	SYNTAX	L4Status
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Real Server status is ether disabled(0) or enabled(1)."
	::= { snL4RealServerCfgEntry 3 }

snL4RealServerCfgMaxConnections 	OBJECT-TYPE
	SYNTAX	INTEGER	 (0..1000000)
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Real Server Maximum Connection allowed."
	::= { snL4RealServerCfgEntry 4 }

 snL4RealServerCfgWeight	OBJECT-TYPE
	SYNTAX	INTEGER	  (0..65000)
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Real Server weight"
	::= { snL4RealServerCfgEntry 5 }

 snL4RealServerCfgRowStatus OBJECT-TYPE
	SYNTAX  L4RowSts
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"To create or delete a real server entry."
	::= {snL4RealServerCfgEntry  6 }

snL4RealServerCfgDeleteState	OBJECT-TYPE
	SYNTAX	L4DeleteState
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Delete operation state." 
	::= { snL4RealServerCfgEntry 7 }


-- Real Server Port Statistic table

snL4RealServerPortCfgTable	       OBJECT-TYPE
	SYNTAX	SEQUENCE OF SnL4RealServerPortCfgEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"Real Server Port table."
	::= { snL4RealServerPortCfg 1 }

snL4RealServerPortCfgEntry	       OBJECT-TYPE
	SYNTAX	SnL4RealServerPortCfgEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"An entry in the Real Server Port table."
	INDEX	{snL4RealServerPortCfgIP,snL4RealServerPortCfgPort  }
	::= { snL4RealServerPortCfgTable 1 }

SnL4RealServerPortCfgEntry ::= SEQUENCE {
	snL4RealServerPortCfgIP
		IpAddress,
	snL4RealServerPortCfgPort
		INTEGER,
	snL4RealServerPortCfgServerName
        L4ServerName,
	snL4RealServerPortCfgAdminStatus
		L4Status,
	snL4RealServerPortCfgRowStatus
		L4RowSts,
    snL4RealServerPortCfgDeleteState
        L4DeleteState
	}


snL4RealServerPortCfgIP	       OBJECT-TYPE
	SYNTAX IpAddress
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"The IP address for the Real Server ."
	::= { snL4RealServerPortCfgEntry 1 }

snL4RealServerPortCfgPort       OBJECT-TYPE
	SYNTAX	INTEGER	 (0..65535)
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerPortCfgEntry 3 }


snL4RealServerPortCfgServerName	       OBJECT-TYPE
	SYNTAX	L4ServerName
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerPortCfgEntry 2 }

snL4RealServerPortCfgAdminStatus		       OBJECT-TYPE
	SYNTAX	L4Status
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerPortCfgEntry 4 }

 snL4RealServerPortCfgRowStatus	 	       OBJECT-TYPE
	SYNTAX L4RowSts	
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"To create or delete a Real server  port entry."
	::= { snL4RealServerPortCfgEntry 5 }

snL4RealServerPortCfgDeleteState	OBJECT-TYPE
	SYNTAX	L4DeleteState
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Delete operation state." 
	::= { snL4RealServerPortCfgEntry 6 }


-- Virtual Server Configuration table

snL4VirtualServerCfgTable  OBJECT-TYPE
	SYNTAX	SEQUENCE OF SnL4VirtualServerCfgEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"Virtual Server table."
	::= { snL4VirtualServerCfg 1 }

snL4VirtualServerCfgEntry  OBJECT-TYPE
	SYNTAX	SnL4VirtualServerCfgEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"An entry in L4 Virtual Server table."
	INDEX	{snL4VirtualServerCfgVirtualIP  }
	::= { snL4VirtualServerCfgTable 1 }

SnL4VirtualServerCfgEntry ::= SEQUENCE {
    snL4VirtualServerCfgVirtualIP
		IpAddress,
    snL4VirtualServerCfgName
        L4ServerName,
    snL4VirtualServerCfgAdminStatus
        L4Status,
	snL4VirtualServerCfgSDAType
		INTEGER,
	snL4VirtualServerCfgRowStatus
		L4RowSts,
    snL4VirtualServerCfgDeleteState
        L4DeleteState
	}

snL4VirtualServerCfgVirtualIP  	OBJECT-TYPE
	SYNTAX IpAddress
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Virtual Server IP Address."
	::= { snL4VirtualServerCfgEntry 1 }

snL4VirtualServerCfgName  OBJECT-TYPE
	SYNTAX	L4ServerName
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Virtual server name."
	::= { snL4VirtualServerCfgEntry 2 }

snL4VirtualServerCfgAdminStatus	OBJECT-TYPE
	SYNTAX	L4Status
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"Virtual Server status is ether disabled(0) or enabled(1)."
	::= { snL4VirtualServerCfgEntry 3 }

snL4VirtualServerCfgSDAType  OBJECT-TYPE
	SYNTAX	 INTEGER {
		default(0),
	    leastconnection(1),
	    roundrobin(2),
	    weighted(3)
	}
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"TCP/UDP Sessions Distribution Algorithms Type."
	::= { snL4VirtualServerCfgEntry 4 }

 snL4VirtualServerCfgRowStatus OBJECT-TYPE
	SYNTAX  L4RowSts
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"To create or delete a virtual server
		entry."
	::= {snL4VirtualServerCfgEntry  5 }

snL4VirtualServerCfgDeleteState	OBJECT-TYPE
	SYNTAX	L4DeleteState
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Delete operation state." 
	::= { snL4VirtualServerCfgEntry 6 }


-- Virtual Server Port Configuration table

snL4VirtualServerPortCfgTable	       OBJECT-TYPE
	SYNTAX	SEQUENCE OF SnL4VirtualServerPortCfgEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"Virtual Server Port table."
	::= { snL4VirtualServerPortCfg 1 }

snL4VirtualServerPortCfgEntry	       OBJECT-TYPE
	SYNTAX	SnL4VirtualServerPortCfgEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"An entry in the Virtual Server Port table."
	INDEX	{snL4VirtualServerPortCfgIP, snL4VirtualServerPortCfgPort  }
	::= { snL4VirtualServerPortCfgTable 1 }

SnL4VirtualServerPortCfgEntry ::= SEQUENCE {
	snL4VirtualServerPortCfgIP
		IpAddress,
	snL4VirtualServerPortCfgPort
		INTEGER,
	snL4VirtualServerPortCfgServerName
        L4ServerName,
	snL4VirtualServerPortCfgAdminStatus
		L4Status,
	snL4VirtualServerPortCfgSticky
		INTEGER,
	snL4VirtualServerPortCfgConcurrent
		INTEGER,
	snL4VirtualServerPortCfgRowStatus
		L4RowSts,
    snL4VirtualServerPortCfgDeleteState
        L4DeleteState
	}


snL4VirtualServerPortCfgIP       OBJECT-TYPE
	SYNTAX IpAddress
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Virtual Server IP Address."
	::= { snL4VirtualServerPortCfgEntry 1 }

snL4VirtualServerPortCfgPort       OBJECT-TYPE
	SYNTAX	INTEGER	  (0..65535)
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerPortCfgEntry 2 }


snL4VirtualServerPortCfgServerName	       OBJECT-TYPE
	SYNTAX	L4ServerName
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerPortCfgEntry 3 }

snL4VirtualServerPortCfgAdminStatus		       OBJECT-TYPE
	SYNTAX	L4Status
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerPortCfgEntry 4 }


 snL4VirtualServerPortCfgSticky       OBJECT-TYPE
	 SYNTAX  INTEGER {
			disabled(0),
			enabled(1)       
			}
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerPortCfgEntry 5 }


 snL4VirtualServerPortCfgConcurrent       OBJECT-TYPE
	 SYNTAX  INTEGER {
			disabled(0),
			enabled(1)       
			}
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerPortCfgEntry 6 }


 snL4VirtualServerPortCfgRowStatus	 	       OBJECT-TYPE
	SYNTAX L4RowSts	
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"To create or delete a virtual server  port entry."
	::= { snL4VirtualServerPortCfgEntry 7 }

snL4VirtualServerPortCfgDeleteState	OBJECT-TYPE
	SYNTAX	L4DeleteState
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Delete operation state." 
	::= { snL4VirtualServerPortCfgEntry 8 }



-- Virtual Server Statistic table

snL4VirtualServerStatisticTable  OBJECT-TYPE
	SYNTAX	SEQUENCE OF SnL4VirtualServerStatisticEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"Virtual Server Statistic table."
	::= { snL4VirtualServerStatistic 1 }

snL4VirtualServerStatisticEntry  OBJECT-TYPE
	SYNTAX	SnL4VirtualServerStatisticEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"An entry in L4 Virtual Server Statistic table."
	INDEX	{snL4VirtualServerStatisticIP  }
	::= { snL4VirtualServerStatisticTable 1 }

SnL4VirtualServerStatisticEntry ::= SEQUENCE {
	snL4VirtualServerStatisticIP 
		IpAddress,
    snL4VirtualServerStatisticName
        L4ServerName,
	snL4VirtualServerStatisticReceivePkts
		Counter,
	snL4VirtualServerStatisticTransmitPkts
		Counter,
	snL4VirtualServerStatisticTotalConnections
		Counter,
	snL4VirtualServerStatisticReceiveBytes
	   Counter64,
	snL4VirtualServerStatisticTransmitBytes
	   Counter64,
	snL4VirtualServerStatisticSymmetricState
	   INTEGER,
	snL4VirtualServerStatisticSymmetricPriority
	   INTEGER,
	snL4VirtualServerStatisticSymmetricKeep
	   INTEGER,
	snL4VirtualServerStatisticSymmetricActivates
	   Counter,
	snL4VirtualServerStatisticSymmetricInactives
	   Counter,
	snL4VirtualServerStatisticSymmetricBestStandbyMacAddr
	   PhysAddress,
	snL4VirtualServerStatisticSymmetricActiveMacAddr
	   PhysAddress
	}

snL4VirtualServerStatisticIP  OBJECT-TYPE
	SYNTAX IpAddress
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"The table index for a Virtual Server  Statistic entry."
	::= { snL4VirtualServerStatisticEntry 1 }


snL4VirtualServerStatisticName  OBJECT-TYPE
	SYNTAX	L4ServerName
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Virtual server name."
	::= { snL4VirtualServerStatisticEntry 2 }


snL4VirtualServerStatisticReceivePkts  OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS  mandatory
	DESCRIPTION
		"" 
	::= { snL4VirtualServerStatisticEntry 3 }

snL4VirtualServerStatisticTransmitPkts  OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS  mandatory
	DESCRIPTION
		"" 
	::= { snL4VirtualServerStatisticEntry 4 }

snL4VirtualServerStatisticTotalConnections  OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS  mandatory
	DESCRIPTION
		"" 
	::= { snL4VirtualServerStatisticEntry 5 }

snL4VirtualServerStatisticReceiveBytes  OBJECT-TYPE
	SYNTAX	Counter64
	ACCESS	read-only
	STATUS  mandatory
	DESCRIPTION
		"" 
	::= { snL4VirtualServerStatisticEntry 6 }

snL4VirtualServerStatisticTransmitBytes  OBJECT-TYPE
	SYNTAX	Counter64
	ACCESS	read-only
	STATUS  mandatory
	DESCRIPTION
		"" 
	::= { snL4VirtualServerStatisticEntry 7 }

snL4VirtualServerStatisticSymmetricState  OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS  mandatory
	DESCRIPTION
		"" 
	::= { snL4VirtualServerStatisticEntry 8 }

snL4VirtualServerStatisticSymmetricPriority  OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS  mandatory
	DESCRIPTION
		"" 
	::= { snL4VirtualServerStatisticEntry 9 }

snL4VirtualServerStatisticSymmetricKeep  OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS	read-only
	STATUS  mandatory
	DESCRIPTION
		"" 
	::= { snL4VirtualServerStatisticEntry 10 }

snL4VirtualServerStatisticSymmetricActivates  OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS  mandatory
	DESCRIPTION
		"" 
	::= { snL4VirtualServerStatisticEntry 11 }

snL4VirtualServerStatisticSymmetricInactives  OBJECT-TYPE
	SYNTAX	Counter
	ACCESS	read-only
	STATUS  mandatory
	DESCRIPTION
		"" 
	::= { snL4VirtualServerStatisticEntry 12 }

snL4VirtualServerStatisticSymmetricBestStandbyMacAddr  OBJECT-TYPE
	SYNTAX	PhysAddress
	ACCESS	read-only
	STATUS  mandatory
	DESCRIPTION
		"" 
	::= { snL4VirtualServerStatisticEntry 13 }

snL4VirtualServerStatisticSymmetricActiveMacAddr  OBJECT-TYPE
	SYNTAX	PhysAddress
	ACCESS	read-only
	STATUS  mandatory
	DESCRIPTION
		"" 
	::= { snL4VirtualServerStatisticEntry 14 }


-- Real Server Statistic Table

snL4RealServerStatisticTable  OBJECT-TYPE
	SYNTAX	SEQUENCE OF SnL4RealServerStatisticEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"Real Server Statistic table."
	::= { snL4RealServerStatistic 1 }

snL4RealServerStatisticEntry  OBJECT-TYPE
	SYNTAX	SnL4RealServerStatisticEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"An entry in the Real Server Statistic table."
	INDEX	{snL4RealServerStatisticRealIP  }
	::= { snL4RealServerStatisticTable 1 }

SnL4RealServerStatisticEntry ::= SEQUENCE {
    snL4RealServerStatisticRealIP 
		IpAddress,
    snL4RealServerStatisticName
        L4ServerName,
	snL4RealServerStatisticReceivePkts
		Counter,
	snL4RealServerStatisticTransmitPkts
		Counter,
	snL4RealServerStatisticCurConnections
		INTEGER,
	snL4RealServerStatisticTotalConnections
		Counter,
	snL4RealServerStatisticAge
		INTEGER,
	snL4RealServerStatisticState
		INTEGER,
	snL4RealServerStatisticReassignments
		INTEGER,
	snL4RealServerStatisticReassignmentLimit
		INTEGER,
	snL4RealServerStatisticFailedPortExists
		INTEGER,
	snL4RealServerStatisticFailTime
		INTEGER,
	snL4RealServerStatisticPeakConnections
		INTEGER
	}

snL4RealServerStatisticRealIP OBJECT-TYPE
	SYNTAX	IpAddress
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerStatisticEntry 1 }


snL4RealServerStatisticName OBJECT-TYPE
	SYNTAX	L4ServerName
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerStatisticEntry 2 }

snL4RealServerStatisticReceivePkts	  OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerStatisticEntry 3 }

snL4RealServerStatisticTransmitPkts  OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerStatisticEntry 4 }

snL4RealServerStatisticCurConnections   OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerStatisticEntry 5 }

snL4RealServerStatisticTotalConnections   OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerStatisticEntry 6 }

snL4RealServerStatisticAge  OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerStatisticEntry 7 }

snL4RealServerStatisticState  OBJECT-TYPE
	SYNTAX	INTEGER	{
	serverdisabled(0),
	serverenabled(1),
	serverfailed(2),
	servertesting(3),
	serversuspect(4),
	servershutdown(5),
	serveractive(6)
	}
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerStatisticEntry 8 }

snL4RealServerStatisticReassignments  OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerStatisticEntry 9 }

snL4RealServerStatisticReassignmentLimit  OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerStatisticEntry 10 }

snL4RealServerStatisticFailedPortExists  OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerStatisticEntry 11 }

snL4RealServerStatisticFailTime  OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerStatisticEntry 12 }


snL4RealServerStatisticPeakConnections   OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerStatisticEntry 13 }




-- Virtual Server Port Statistic table

snL4VirtualServerPortStatisticTable	       OBJECT-TYPE
	SYNTAX	SEQUENCE OF SnL4VirtualServerPortStatisticEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"Virtual Server Port Statistic table."
	::= { snL4VirtualServerPortStatistic 1 }

snL4VirtualServerPortStatisticEntry	       OBJECT-TYPE
	SYNTAX	SnL4VirtualServerPortStatisticEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"An entry in the Virtual Server Port Statistic table."
	INDEX	{ snL4VirtualServerPortStatisticIP,snL4VirtualServerPortStatisticPort }
	::= { snL4VirtualServerPortStatisticTable 1 }

SnL4VirtualServerPortStatisticEntry ::= SEQUENCE {
	snL4VirtualServerPortStatisticIP
		IpAddress,
	snL4VirtualServerPortStatisticPort
		INTEGER,
	snL4VirtualServerPortStatisticServerName
        L4ServerName,
	snL4VirtualServerPortStatisticCurrentConnection
		INTEGER,
	snL4VirtualServerPortStatisticTotalConnection
		Counter,
	snL4VirtualServerPortStatisticPeakConnection
		INTEGER
	}

snL4VirtualServerPortStatisticIP	       OBJECT-TYPE
	SYNTAX	IpAddress
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"The index for Virtual Server Port Statistic entry."
	::= { snL4VirtualServerPortStatisticEntry 1 }

snL4VirtualServerPortStatisticPort   OBJECT-TYPE
	SYNTAX	INTEGER	 (1..2048)
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerPortStatisticEntry 2 }

 snL4VirtualServerPortStatisticServerName 	       OBJECT-TYPE
	SYNTAX	L4ServerName
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerPortStatisticEntry 3 }

 snL4VirtualServerPortStatisticCurrentConnection 	       OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerPortStatisticEntry 4 }

 snL4VirtualServerPortStatisticTotalConnection		       OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerPortStatisticEntry 5 }

 snL4VirtualServerPortStatisticPeakConnection 	       OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerPortStatisticEntry 6 }

-- Real Server Port Statistic table

snL4RealServerPortStatisticTable	       OBJECT-TYPE
	SYNTAX	SEQUENCE OF SnL4RealServerPortStatisticEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"Real Server Port Statistic table."
	::= { snL4RealServerPortStatistic 1 }

snL4RealServerPortStatisticEntry	       OBJECT-TYPE
	SYNTAX	SnL4RealServerPortStatisticEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"An entry in the Real Server Port Statistic table."
	INDEX	{ snL4RealServerPortStatisticIP,snL4RealServerPortStatisticPort }
	::= { snL4RealServerPortStatisticTable 1 }

SnL4RealServerPortStatisticEntry ::= SEQUENCE {
	snL4RealServerPortStatisticIP
		IpAddress,
	snL4RealServerPortStatisticPort
		INTEGER,
	snL4RealServerPortStatisticServerName
        L4ServerName,
	snL4RealServerPortStatisticReassignCount
		INTEGER,
	snL4RealServerPortStatisticState
		INTEGER,
	snL4RealServerPortStatisticFailTime
		INTEGER,
	snL4RealServerPortStatisticCurrentConnection
		INTEGER,
	snL4RealServerPortStatisticTotalConnection
		Counter,
	snL4RealServerPortStatisticRxPkts
		Counter,
	snL4RealServerPortStatisticTxPkts
		Counter,
	snL4RealServerPortStatisticRxBytes
		Counter,
	snL4RealServerPortStatisticTxBytes
		Counter,
	snL4RealServerPortStatisticPeakConnection
		INTEGER
	}


snL4RealServerPortStatisticIP	       OBJECT-TYPE
	SYNTAX IpAddress
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"The index for Real Server Port Statistic entry."
	::= { snL4RealServerPortStatisticEntry 1 }

snL4RealServerPortStatisticPort	       OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerPortStatisticEntry 2 }

snL4RealServerPortStatisticServerName	       OBJECT-TYPE
	SYNTAX	L4ServerName
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerPortStatisticEntry 3 }

snL4RealServerPortStatisticReassignCount	       OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerPortStatisticEntry 4 }

 snL4RealServerPortStatisticState	       OBJECT-TYPE
	SYNTAX	INTEGER	{
		disabled(0),
		enabled(1),
		failed(2),
		testing(3),
		suspect(4),
	    shutdown(5),
		active(6),
		unbound(7),
		awaitUnbind(8),
		awaitDelete(9)
	}
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Real server port state"
	::= { snL4RealServerPortStatisticEntry 5 }

snL4RealServerPortStatisticFailTime 	       OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Only useful, if real server port state is failed.
		 Indicating how seconds has been elapsed from the last retry."
 	::= { snL4RealServerPortStatisticEntry 6 }

snL4RealServerPortStatisticCurrentConnection	       OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Real server port current connection"
	::= { snL4RealServerPortStatisticEntry 7 }

snL4RealServerPortStatisticTotalConnection	       OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Real server port total connection"
	::= { snL4RealServerPortStatisticEntry 8 }

snL4RealServerPortStatisticRxPkts	       OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Real server port receive packets."
	::= { snL4RealServerPortStatisticEntry 9 }


snL4RealServerPortStatisticTxPkts	       OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Real server port transmit packets."
	::= { snL4RealServerPortStatisticEntry 10 }


snL4RealServerPortStatisticRxBytes	       OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Real server port receive bytes."
	::= { snL4RealServerPortStatisticEntry 11 }

snL4RealServerPortStatisticTxBytes	       OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"Real server port transmit bytes."
	::= { snL4RealServerPortStatisticEntry 12 }


snL4RealServerPortStatisticPeakConnection	       OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"peak connection for real server port."
	::= { snL4RealServerPortStatisticEntry 13 }


-- GSLB Site Remote ServerIron Configuration table

snL4GslbSiteRemoteServerIronTable	       OBJECT-TYPE
	SYNTAX	SEQUENCE OF SnL4GslbSiteRemoteServerIronEntry
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"GSLB remote ServerIron configuration table."
	::= { snL4GslbSiteRemoteServerIrons 1 }

snL4GslbSiteRemoteServerIronEntry	       OBJECT-TYPE
	SYNTAX	SnL4GslbSiteRemoteServerIronEntry	
	ACCESS  not-accessible
	STATUS  mandatory
	DESCRIPTION
		"An entry of a GSLB remote ServerIron configuration."
	INDEX	{ snL4GslbSiteRemoteServerIronIP }
	::= { snL4GslbSiteRemoteServerIronTable 1 }

SnL4GslbSiteRemoteServerIronEntry ::= SEQUENCE {
	snL4GslbSiteRemoteServerIronIP
		IpAddress,
	snL4GslbSiteRemoteServerIronPreference
		INTEGER
	}


snL4GslbSiteRemoteServerIronIP	       OBJECT-TYPE
	SYNTAX IpAddress
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		"The index for each remote ServerIron in a site."
	::= { snL4GslbSiteRemoteServerIronEntry 1 }

snL4GslbSiteRemoteServerIronPreference 	OBJECT-TYPE
	SYNTAX	INTEGER	(0..255)
	ACCESS  read-write
	STATUS  mandatory
	DESCRIPTION
		"The preference of a remote ServerIron. The default value is 128."
    DEFVAL { 128 }
	::= { snL4GslbSiteRemoteServerIronEntry 2 }


-- Real Server Monitor Group

-- The Real Server History Control Group

-- The snL4History control group controls the periodic statistical
-- sampling of data from various types of data sources.  The
-- snL4RealServerHistoryControlTable stores configuration entries that each
-- define an interface, polling period, and other parameters.
-- Once samples are taken, their data is stored in an entry
-- in a media-specific table.  Each such entry defines one
-- sample, and is associated with the snL4RealServerHistoryControlEntry that
-- caused the sample to be taken.  Each counter in the
-- snL4HistoryEntry counts the same event as its
-- similarly-named counterpart in the Statistics Entry,
-- except that each value here is a cumulative sum during a
-- sampling period.
--
-- If the probe keeps track of the time of day, it should
-- start the first sample of the snL4History at a time such that
-- when the next hour of the day begins, a sample is
-- started at that instant.  This tends to make more
-- user-friendly reports, and enables comparison of reports
-- from different probes that have relatively accurate time
-- of day.
--
-- The probe is encouraged to add two snL4History control entries
-- per monitored interface upon initialization that describe
-- a short term and a long term polling period.  Suggested
-- parameters are 30 seconds for the short term polling period
-- and 30 minutes for the long term period.

snL4RealServerHistoryControlTable OBJECT-TYPE
	SYNTAX SEQUENCE OF SnL4RealServerHistoryControlEntry
	ACCESS not-accessible
	STATUS mandatory
	DESCRIPTION
		"A list of history control entries."
	::= { snL4History 1 }

snL4RealServerHistoryControlEntry OBJECT-TYPE
	SYNTAX SnL4RealServerHistoryControlEntry
	ACCESS not-accessible
	STATUS mandatory
	DESCRIPTION
		"A list of parameters that set up a periodic sampling
		of statistics.As an example, an instance of the
		snL4RealServerHistoryControlInterval object might be named
		snL4RealServerHistoryControlInterval.2"
	INDEX { snL4RealServerHistoryControlIndex }
	::= { snL4RealServerHistoryControlTable 1 }

	SnL4RealServerHistoryControlEntry ::= SEQUENCE {
		snL4RealServerHistoryControlIndex			 
			INTEGER (1..65535),
		snL4RealServerHistoryControlDataSource		
			OBJECT IDENTIFIER,
		snL4RealServerHistoryControlBucketsRequested
			INTEGER (1..65535),
		snL4RealServerHistoryControlBucketsGranted	
			INTEGER (1..65535),
		snL4RealServerHistoryControlInterval		
			INTEGER (1..3600),
		snL4RealServerHistoryControlOwner			 
			DisplayString,
		snL4RealServerHistoryControlStatus			
			INTEGER
	}

snL4RealServerHistoryControlIndex OBJECT-TYPE
	SYNTAX INTEGER (1..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION
		"An index that uniquely identifies an entry in the
		snL4RealServerHistoryControl table.Each such entry defines a
		set of samples at a particular interval for an
		interface on the device."
	::= { snL4RealServerHistoryControlEntry 1 }

snL4RealServerHistoryControlDataSource OBJECT-TYPE
	SYNTAX OBJECT IDENTIFIER
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"This object identifies the source of the data for
		which historical data was collected and
		placed in a media-specific table on behalf of this
		snL4RealServerHistoryControlEntry.This source can be any
		real/virtual server and real/virtual server port on 
		this ServerIron.  In order to identify
		a particular instance, this object shall identify
		the instance of the object, defined in the above 
		statistics tables.
	
		This object may not be modified if the associated
		snL4RealServerHistoryControlStatus object is equal to valid(1)."
	::= { snL4RealServerHistoryControlEntry 2 }

snL4RealServerHistoryControlBucketsRequested OBJECT-TYPE
	SYNTAX INTEGER (1..65535)
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"The requested number of discrete time intervals
		over which data is to be saved in the part of the
		media-specific table associated with this
		snL4RealServerHistoryControlEntry.
	
		When this object is created or modified, the probe
		should set snL4RealServerHistoryControlBucketsGranted as closely to
		this object as is possible for the particular probe
		implementation and available resources."
	DEFVAL { 50 }
	::= { snL4RealServerHistoryControlEntry 3 }

snL4RealServerHistoryControlBucketsGranted OBJECT-TYPE
	SYNTAX INTEGER (1..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION
		"The number of discrete sampling intervals
		over which data shall be saved in the part of
		the media-specific table associated with this
		snL4RealServerHistoryControlEntry.
	
		When the associated snL4RealServerHistoryControlBucketsRequested
		object is created or modified, the probe
		should set this object as closely to the requested
		value as is possible for the particular
		probe implementation and available resources.The
		probe must not lower this value except as a result
		of a modification to the associated
		snL4RealServerHistoryControlBucketsRequested object.
	
		There will be times when the actual number of
		buckets associated with this entry is less than
		the value of this object.In this case, at the
		end of each sampling interval, a new bucket will
		be added to the media-specific table.
	
		When the number of buckets reaches the value of
		this object and a new bucket is to be added to the
		media-specific table, the oldest bucket associated
		with this snL4RealServerHistoryControlEntry shall be deleted by
		the agent so that the new bucket can be added.
	
		When the value of this object changes to a value less
		than the current value, entries are deleted
		from the media-specific table associated with this
		snL4RealServerHistoryControlEntry.Enough of the oldest of these
		entries shall be deleted by the agent so that their
		number remains less than or equal to the new value of
		this object.
	
		When the value of this object changes to a value
		greater than the current value, the number of
		associated media- specific entries may be allowed to
		grow."
	::= { snL4RealServerHistoryControlEntry 4 }

snL4RealServerHistoryControlInterval OBJECT-TYPE
	SYNTAX INTEGER (1..3600)
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"The interval in seconds over which the data is
		sampled for each bucket in the part of the
		media-specific table associated with this
		snL4RealServerHistoryControlEntry.This interval can
		be set to any number of seconds between 1 and
		3600 (1 hour).
	
		Because the counters in a bucket may overflow at their
		maximum value with no indication, a prudent manager
		will take into account the possibility of overflow
		in any of the associated counters.It is important
		to consider the minimum time in which any counter
		could overflow on a particular media type and set
		the snL4RealServerHistoryControlInterval object to a value less
		than this interval.This is typically most
		important for the 'octets' counter in any
		media-specific table.	
		This object may not be modified if the associated
		snL4RealServerHistoryControlStatus object is equal to valid(1)."
	DEFVAL { 1800 }
	::= { snL4RealServerHistoryControlEntry 5 }

snL4RealServerHistoryControlOwner OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"The entity that configured this entry and is
		therefore using the resources assigned to it."
	::= { snL4RealServerHistoryControlEntry 6 }

snL4RealServerHistoryControlStatus OBJECT-TYPE
	SYNTAX INTEGER { 
				valid(1),
             	createRequest(2),
             	underCreation(3),
             	invalid(4)
           }
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"The status of this snL4RealServerHistoryControl entry.
		Each instance of the media-specific table associated
		with this snL4RealServerHistoryControlEntry will be deleted by the
		agent if this snL4RealServerHistoryControlEntry is not equal to
		valid(1)."
	::= { snL4RealServerHistoryControlEntry 7 }


-- The Real Server History Group


snL4RealServerHistoryTable OBJECT-TYPE
	SYNTAX SEQUENCE OF SnL4RealServerHistoryEntry
	ACCESS not-accessible
	STATUS mandatory
	DESCRIPTION
		"A list of Ethernet snL4History entries."
	::= { snL4History 2 }

snL4RealServerHistoryEntry OBJECT-TYPE
	SYNTAX SnL4RealServerHistoryEntry
	ACCESS not-accessible
	STATUS mandatory
	DESCRIPTION
		"An historical sample of Ethernet statistics on a
		particular Ethernet interface.  This sample is
		associated with the snL4RealServerHistoryControlEntry which set up
		the parameters for a regular collection of these
		samples.  As an example, an instance of the
		snL4RealServerHistoryReceivePkts object might be named
		snL4RealServerHistoryReceivePkts.2.89"
	INDEX { snL4RealServerHistoryIndex , snL4RealServerHistorySampleIndex }
	::= { snL4RealServerHistoryTable 1 }

SnL4RealServerHistoryEntry ::= SEQUENCE {
	snL4RealServerHistoryIndex                 
		INTEGER (1..65535),
	snL4RealServerHistorySampleIndex           
		INTEGER (1..2147483647),
	snL4RealServerHistoryIntervalStart         
		TimeTicks,
	snL4RealServerHistoryReceivePkts
		Counter,
	snL4RealServerHistoryTransmitPkts
		Counter,
	snL4RealServerHistoryTotalConnections
		Counter,
	snL4RealServerHistoryCurConnections
		INTEGER,
	snL4RealServerHistoryPeakConnections
		INTEGER,
	snL4RealServerHistoryReassignments
		INTEGER
    }

snL4RealServerHistoryIndex OBJECT-TYPE
	SYNTAX INTEGER (1..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION
		"The snL4RealServerHistory of which this entry is a part.The
		snL4RealServerHistory identified by a particular value of this
		index is the same snL4RealServerHistory as identified
		by the same value of snL4RealServerHistoryControlIndex."
	::= { snL4RealServerHistoryEntry 1 }

snL4RealServerHistorySampleIndex OBJECT-TYPE
	SYNTAX INTEGER (1..2147483647)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION
		"An index that uniquely identifies the particular
		sample this entry represents among all samples
		associated with the same snL4RealServerHistoryControlEntry.
		This index starts at 1 and increases by one
		as each new sample is taken."
	::= { snL4RealServerHistoryEntry 2 }

snL4RealServerHistoryIntervalStart OBJECT-TYPE
	SYNTAX TimeTicks
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION
		"The value of sysUpTime at the start of the interval
		over which this sample was measured.If the probe
		keeps track of the time of day, it should start
		the first sample of the snL4RealServerHistory at a time such that
		when the next hour of the day begins, a sample is
		started at that instant.Note that following this
		rule may require the probe to delay collecting the
		first sample of the snL4RealServerHistory, as each sample must be
		of the same interval.Also note that the sample which
		is currently being collected is not accessible in this
		table until the end of its interval."
	::= { snL4RealServerHistoryEntry 3 }


snL4RealServerHistoryReceivePkts	  OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerHistoryEntry 4 }

snL4RealServerHistoryTransmitPkts  OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerHistoryEntry 5 }

snL4RealServerHistoryTotalConnections   OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerHistoryEntry 6 }

snL4RealServerHistoryCurConnections   OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerHistoryEntry 7 }

snL4RealServerHistoryPeakConnections   OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerHistoryEntry 8 }

snL4RealServerHistoryReassignments   OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerHistoryEntry 9 }


-- Real Server Port Monitor Group

-- The Real Server Port History Control Group

snL4RealServerPortHistoryControlTable OBJECT-TYPE
	SYNTAX SEQUENCE OF SnL4RealServerPortHistoryControlEntry
	ACCESS not-accessible
	STATUS mandatory
	DESCRIPTION
		"A list of history control entries."
	::= { snL4History 3 }

snL4RealServerPortHistoryControlEntry OBJECT-TYPE
	SYNTAX SnL4RealServerPortHistoryControlEntry
	ACCESS not-accessible
	STATUS mandatory
	DESCRIPTION
		"A list of parameters that set up a periodic sampling
		of statistics.As an example, an instance of the
		snL4RealServerPortHistoryControlInterval object might be named
		snL4RealServerPortHistoryControlInterval.2"
	INDEX { snL4RealServerPortHistoryControlIndex }
	::= { snL4RealServerPortHistoryControlTable 1 }

	SnL4RealServerPortHistoryControlEntry ::= SEQUENCE {
		snL4RealServerPortHistoryControlIndex			 
			INTEGER (1..65535),
		snL4RealServerPortHistoryControlDataSource		
			OBJECT IDENTIFIER,
		snL4RealServerPortHistoryControlBucketsRequested
			INTEGER (1..65535),
		snL4RealServerPortHistoryControlBucketsGranted	
			INTEGER (1..65535),
		snL4RealServerPortHistoryControlInterval		
			INTEGER (1..3600),
		snL4RealServerPortHistoryControlOwner			 
			DisplayString,
		snL4RealServerPortHistoryControlStatus			
			INTEGER
	}

snL4RealServerPortHistoryControlIndex OBJECT-TYPE
	SYNTAX INTEGER (1..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION
		"An index that uniquely identifies an entry in the
		snL4RealServerPortHistoryControl table.Each such entry defines a
		set of samples at a particular interval for an
		interface on the device."
	::= { snL4RealServerPortHistoryControlEntry 1 }

snL4RealServerPortHistoryControlDataSource OBJECT-TYPE
	SYNTAX OBJECT IDENTIFIER
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"This object identifies the source of the data for
		which historical data was collected and
		placed in a media-specific table on behalf of this
		snL4RealServerPortHistoryControlEntry.This source can be any
		real/virtual server and real/virtual server port on 
		this ServerIron.  In order to identify
		a particular instance, this object shall identify
		the instance of the object, defined in the above 
		statistics tables.
	
		This object may not be modified if the associated
		snL4RealServerPortHistoryControlStatus object is equal to valid(1)."
	::= { snL4RealServerPortHistoryControlEntry 2 }

snL4RealServerPortHistoryControlBucketsRequested OBJECT-TYPE
	SYNTAX INTEGER (1..65535)
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"The requested number of discrete time intervals
		over which data is to be saved in the part of the
		media-specific table associated with this
		snL4RealServerPortHistoryControlEntry.
	
		When this object is created or modified, the probe
		should set snL4RealServerPortHistoryControlBucketsGranted as closely to
		this object as is possible for the particular probe
		implementation and available resources."
	DEFVAL { 50 }
	::= { snL4RealServerPortHistoryControlEntry 3 }

snL4RealServerPortHistoryControlBucketsGranted OBJECT-TYPE
	SYNTAX INTEGER (1..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION
		"The number of discrete sampling intervals
		over which data shall be saved in the part of
		the media-specific table associated with this
		snL4RealServerPortHistoryControlEntry.
	
		When the associated snL4RealServerPortHistoryControlBucketsRequested
		object is created or modified, the probe
		should set this object as closely to the requested
		value as is possible for the particular
		probe implementation and available resources.The
		probe must not lower this value except as a result
		of a modification to the associated
		snL4RealServerPortHistoryControlBucketsRequested object.
	
		There will be times when the actual number of
		buckets associated with this entry is less than
		the value of this object.In this case, at the
		end of each sampling interval, a new bucket will
		be added to the media-specific table.
	
		When the number of buckets reaches the value of
		this object and a new bucket is to be added to the
		media-specific table, the oldest bucket associated
		with this snL4RealServerPortHistoryControlEntry shall be deleted by
		the agent so that the new bucket can be added.
	
		When the value of this object changes to a value less
		than the current value, entries are deleted
		from the media-specific table associated with this
		snL4RealServerPortHistoryControlEntry.Enough of the oldest of these
		entries shall be deleted by the agent so that their
		number remains less than or equal to the new value of
		this object.
	
		When the value of this object changes to a value
		greater than the current value, the number of
		associated media- specific entries may be allowed to
		grow."
	::= { snL4RealServerPortHistoryControlEntry 4 }

snL4RealServerPortHistoryControlInterval OBJECT-TYPE
	SYNTAX INTEGER (1..3600)
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"The interval in seconds over which the data is
		sampled for each bucket in the part of the
		media-specific table associated with this
		snL4RealServerPortHistoryControlEntry.This interval can
		be set to any number of seconds between 1 and
		3600 (1 hour).
	
		Because the counters in a bucket may overflow at their
		maximum value with no indication, a prudent manager
		will take into account the possibility of overflow
		in any of the associated counters.It is important
		to consider the minimum time in which any counter
		could overflow on a particular media type and set
		the snL4RealServerPortHistoryControlInterval object to a value less
		than this interval.This is typically most
		important for the 'octets' counter in any
		media-specific table.	
		This object may not be modified if the associated
		snL4RealServerPortHistoryControlStatus object is equal to valid(1)."
	DEFVAL { 1800 }
	::= { snL4RealServerPortHistoryControlEntry 5 }

snL4RealServerPortHistoryControlOwner OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"The entity that configured this entry and is
		therefore using the resources assigned to it."
	::= { snL4RealServerPortHistoryControlEntry 6 }

snL4RealServerPortHistoryControlStatus OBJECT-TYPE
	SYNTAX INTEGER { 
				valid(1),
             	createRequest(2),
             	underCreation(3),
             	invalid(4)
           }
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"The status of this snL4RealServerPortHistoryControl entry.
		Each instance of the media-specific table associated
		with this snL4RealServerPortHistoryControlEntry will be deleted by the
		agent if this snL4RealServerPortHistoryControlEntry is not equal to
		valid(1)."
	::= { snL4RealServerPortHistoryControlEntry 7 }


-- The Real Server Port History Group


snL4RealServerPortHistoryTable OBJECT-TYPE
	SYNTAX SEQUENCE OF SnL4RealServerPortHistoryEntry
	ACCESS not-accessible
	STATUS mandatory
	DESCRIPTION
		"A list of Ethernet snL4History entries."
	::= { snL4History 4 }

snL4RealServerPortHistoryEntry OBJECT-TYPE
	SYNTAX SnL4RealServerPortHistoryEntry
	ACCESS not-accessible
	STATUS mandatory
	DESCRIPTION
		"An historical sample of Ethernet statistics on a
		particular Ethernet interface.  This sample is
		associated with the snL4RealServerPortHistoryControlEntry which set up
		the parameters for a regular collection of these
		samples.  As an example, an instance of the
		snL4RealServerPortHistoryReceivePkts object might be named
		snL4RealServerPortHistoryReceivePkts.2.89"
	INDEX { snL4RealServerPortHistoryIndex , snL4RealServerPortHistorySampleIndex }
	::= { snL4RealServerPortHistoryTable 1 }

SnL4RealServerPortHistoryEntry ::= SEQUENCE {
	snL4RealServerPortHistoryIndex                 
		INTEGER (1..65535),
	snL4RealServerPortHistorySampleIndex           
		INTEGER (1..2147483647),
	snL4RealServerPortHistoryIntervalStart         
		TimeTicks,
	snL4RealServerPortHistoryReceivePkts
		Counter,
	snL4RealServerPortHistoryTransmitPkts
		Counter,
	snL4RealServerPortHistoryTotalConnections
		Counter,
	snL4RealServerPortHistoryCurConnections
		INTEGER,
	snL4RealServerPortHistoryPeakConnections
		INTEGER,
	snL4RealServerPortHistoryResponseTime
		INTEGER
    }

snL4RealServerPortHistoryIndex OBJECT-TYPE
	SYNTAX INTEGER (1..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION
		"The snL4RealServerPortHistory of which this entry is a part.The
		snL4RealServerPortHistory identified by a particular value of this
		index is the same snL4RealServerPortHistory as identified
		by the same value of snL4RealServerPortHistoryControlIndex."
	::= { snL4RealServerPortHistoryEntry 1 }

snL4RealServerPortHistorySampleIndex OBJECT-TYPE
	SYNTAX INTEGER (1..2147483647)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION
		"An index that uniquely identifies the particular
		sample this entry represents among all samples
		associated with the same snL4RealServerPortHistoryControlEntry.
		This index starts at 1 and increases by one
		as each new sample is taken."
	::= { snL4RealServerPortHistoryEntry 2 }

snL4RealServerPortHistoryIntervalStart OBJECT-TYPE
	SYNTAX TimeTicks
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION
		"The value of sysUpTime at the start of the interval
		over which this sample was measured.If the probe
		keeps track of the time of day, it should start
		the first sample of the snL4RealServerPortHistory at a time such that
		when the next hour of the day begins, a sample is
		started at that instant.Note that following this
		rule may require the probe to delay collecting the
		first sample of the snL4RealServerPortHistory, as each sample must be
		of the same interval.Also note that the sample which
		is currently being collected is not accessible in this
		table until the end of its interval."
	::= { snL4RealServerPortHistoryEntry 3 }


snL4RealServerPortHistoryReceivePkts	  OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerPortHistoryEntry 4 }

snL4RealServerPortHistoryTransmitPkts  OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerPortHistoryEntry 5 }

snL4RealServerPortHistoryTotalConnections   OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerPortHistoryEntry 6 }

snL4RealServerPortHistoryCurConnections   OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerPortHistoryEntry 7 }

snL4RealServerPortHistoryPeakConnections   OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerPortHistoryEntry 8 }

snL4RealServerPortHistoryResponseTime   OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4RealServerPortHistoryEntry 9 }


-- Virtual Server Monitor Group
-- The Virtual Server History Control Group


snL4VirtualServerHistoryControlTable OBJECT-TYPE
	SYNTAX SEQUENCE OF SnL4VirtualServerHistoryControlEntry
	ACCESS not-accessible
	STATUS mandatory
	DESCRIPTION
		"A list of history control entries."
	::= { snL4History 5 }

snL4VirtualServerHistoryControlEntry OBJECT-TYPE
	SYNTAX SnL4VirtualServerHistoryControlEntry
	ACCESS not-accessible
	STATUS mandatory
	DESCRIPTION
		"A list of parameters that set up a periodic sampling
		of statistics.As an example, an instance of the
		snL4VirtualServerHistoryControlInterval object might be named
		snL4VirtualServerHistoryControlInterval.2"
	INDEX { snL4VirtualServerHistoryControlIndex }
	::= { snL4VirtualServerHistoryControlTable 1 }

	SnL4VirtualServerHistoryControlEntry ::= SEQUENCE {
		snL4VirtualServerHistoryControlIndex			 
			INTEGER (1..65535),
		snL4VirtualServerHistoryControlDataSource		
			OBJECT IDENTIFIER,
		snL4VirtualServerHistoryControlBucketsRequested
			INTEGER (1..65535),
		snL4VirtualServerHistoryControlBucketsGranted	
			INTEGER (1..65535),
		snL4VirtualServerHistoryControlInterval		
			INTEGER (1..3600),
		snL4VirtualServerHistoryControlOwner			 
			DisplayString,
		snL4VirtualServerHistoryControlStatus			
			INTEGER
	}

snL4VirtualServerHistoryControlIndex OBJECT-TYPE
	SYNTAX INTEGER (1..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION
		"An index that uniquely identifies an entry in the
		snL4VirtualServerHistoryControl table.Each such entry defines a
		set of samples at a particular interval for an
		interface on the device."
	::= { snL4VirtualServerHistoryControlEntry 1 }

snL4VirtualServerHistoryControlDataSource OBJECT-TYPE
	SYNTAX OBJECT IDENTIFIER
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"This object identifies the source of the data for
		which historical data was collected and
		placed in a media-specific table on behalf of this
		snL4VirtualServerHistoryControlEntry.This source can be any
		real/virtual server and real/virtual server port on 
		this ServerIron.  In order to identify
		a particular instance, this object shall identify
		the instance of the object, defined in the above 
		statistics tables.
	
		This object may not be modified if the associated
		snL4VirtualServerHistoryControlStatus object is equal to valid(1)."
	::= { snL4VirtualServerHistoryControlEntry 2 }

snL4VirtualServerHistoryControlBucketsRequested OBJECT-TYPE
	SYNTAX INTEGER (1..65535)
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"The requested number of discrete time intervals
		over which data is to be saved in the part of the
		media-specific table associated with this
		snL4VirtualServerHistoryControlEntry.
	
		When this object is created or modified, the probe
		should set snL4VirtualServerHistoryControlBucketsGranted as closely to
		this object as is possible for the particular probe
		implementation and available resources."
	DEFVAL { 50 }
	::= { snL4VirtualServerHistoryControlEntry 3 }

snL4VirtualServerHistoryControlBucketsGranted OBJECT-TYPE
	SYNTAX INTEGER (1..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION
		"The number of discrete sampling intervals
		over which data shall be saved in the part of
		the media-specific table associated with this
		snL4VirtualServerHistoryControlEntry.
	
		When the associated snL4VirtualServerHistoryControlBucketsRequested
		object is created or modified, the probe
		should set this object as closely to the requested
		value as is possible for the particular
		probe implementation and available resources.The
		probe must not lower this value except as a result
		of a modification to the associated
		snL4VirtualServerHistoryControlBucketsRequested object.
	
		There will be times when the actual number of
		buckets associated with this entry is less than
		the value of this object.In this case, at the
		end of each sampling interval, a new bucket will
		be added to the media-specific table.
	
		When the number of buckets reaches the value of
		this object and a new bucket is to be added to the
		media-specific table, the oldest bucket associated
		with this snL4VirtualServerHistoryControlEntry shall be deleted by
		the agent so that the new bucket can be added.
	
		When the value of this object changes to a value less
		than the current value, entries are deleted
		from the media-specific table associated with this
		snL4VirtualServerHistoryControlEntry.Enough of the oldest of these
		entries shall be deleted by the agent so that their
		number remains less than or equal to the new value of
		this object.
	
		When the value of this object changes to a value
		greater than the current value, the number of
		associated media- specific entries may be allowed to
		grow."
	::= { snL4VirtualServerHistoryControlEntry 4 }

snL4VirtualServerHistoryControlInterval OBJECT-TYPE
	SYNTAX INTEGER (1..3600)
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"The interval in seconds over which the data is
		sampled for each bucket in the part of the
		media-specific table associated with this
		snL4VirtualServerHistoryControlEntry.This interval can
		be set to any number of seconds between 1 and
		3600 (1 hour).
	
		Because the counters in a bucket may overflow at their
		maximum value with no indication, a prudent manager
		will take into account the possibility of overflow
		in any of the associated counters.It is important
		to consider the minimum time in which any counter
		could overflow on a particular media type and set
		the snL4VirtualServerHistoryControlInterval object to a value less
		than this interval.This is typically most
		important for the 'octets' counter in any
		media-specific table.	
		This object may not be modified if the associated
		snL4VirtualServerHistoryControlStatus object is equal to valid(1)."
	DEFVAL { 1800 }
	::= { snL4VirtualServerHistoryControlEntry 5 }

snL4VirtualServerHistoryControlOwner OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"The entity that configured this entry and is
		therefore using the resources assigned to it."
	::= { snL4VirtualServerHistoryControlEntry 6 }

snL4VirtualServerHistoryControlStatus OBJECT-TYPE
	SYNTAX INTEGER { 
				valid(1),
             	createRequest(2),
             	underCreation(3),
             	invalid(4)
           }
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"The status of this snL4VirtualServerHistoryControl entry.
		Each instance of the media-specific table associated
		with this snL4VirtualServerHistoryControlEntry will be deleted by the
		agent if this snL4VirtualServerHistoryControlEntry is not equal to
		valid(1)."
	::= { snL4VirtualServerHistoryControlEntry 7 }


-- The Virtual Server History Group


snL4VirtualServerHistoryTable OBJECT-TYPE
	SYNTAX SEQUENCE OF SnL4VirtualServerHistoryEntry
	ACCESS not-accessible
	STATUS mandatory
	DESCRIPTION
		"A list of Ethernet snL4History entries."
	::= { snL4History 6 }

snL4VirtualServerHistoryEntry OBJECT-TYPE
	SYNTAX SnL4VirtualServerHistoryEntry
	ACCESS not-accessible
	STATUS mandatory
	DESCRIPTION
		"An historical sample of Ethernet statistics on a
		particular Ethernet interface.  This sample is
		associated with the snL4VirtualServerHistoryControlEntry which set up
		the parameters for a regular collection of these
		samples.  As an example, an instance of the
		snL4VirtualServerHistoryReceivePkts object might be named
		snL4VirtualServerHistoryReceivePkts.2.89"
	INDEX { snL4VirtualServerHistoryIndex , snL4VirtualServerHistorySampleIndex }
	::= { snL4VirtualServerHistoryTable 1 }

SnL4VirtualServerHistoryEntry ::= SEQUENCE {
	snL4VirtualServerHistoryIndex                 
		INTEGER (1..65535),
	snL4VirtualServerHistorySampleIndex           
		INTEGER (1..2147483647),
	snL4VirtualServerHistoryIntervalStart         
		TimeTicks,
	snL4VirtualServerHistoryReceivePkts
		Counter,
	snL4VirtualServerHistoryTransmitPkts
		Counter,
	snL4VirtualServerHistoryTotalConnections
		Counter,
	snL4VirtualServerHistoryCurConnections
		INTEGER,
	snL4VirtualServerHistoryPeakConnections
		INTEGER
    }

snL4VirtualServerHistoryIndex OBJECT-TYPE
	SYNTAX INTEGER (1..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION
		"The snL4VirtualServerHistory of which this entry is a part.The
		snL4VirtualServerHistory identified by a particular value of this
		index is the same snL4VirtualServerHistory as identified
		by the same value of snL4VirtualServerHistoryControlIndex."
	::= { snL4VirtualServerHistoryEntry 1 }

snL4VirtualServerHistorySampleIndex OBJECT-TYPE
	SYNTAX INTEGER (1..2147483647)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION
		"An index that uniquely identifies the particular
		sample this entry represents among all samples
		associated with the same snL4VirtualServerHistoryControlEntry.
		This index starts at 1 and increases by one
		as each new sample is taken."
	::= { snL4VirtualServerHistoryEntry 2 }

snL4VirtualServerHistoryIntervalStart OBJECT-TYPE
	SYNTAX TimeTicks
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION
		"The value of sysUpTime at the start of the interval
		over which this sample was measured.If the probe
		keeps track of the time of day, it should start
		the first sample of the snL4VirtualServerHistory at a time such that
		when the next hour of the day begins, a sample is
		started at that instant.Note that following this
		rule may require the probe to delay collecting the
		first sample of the snL4VirtualServerHistory, as each sample must be
		of the same interval.Also note that the sample which
		is currently being collected is not accessible in this
		table until the end of its interval."
	::= { snL4VirtualServerHistoryEntry 3 }


snL4VirtualServerHistoryReceivePkts	  OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerHistoryEntry 4 }

snL4VirtualServerHistoryTransmitPkts  OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerHistoryEntry 5 }

snL4VirtualServerHistoryTotalConnections   OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerHistoryEntry 6 }

snL4VirtualServerHistoryCurConnections   OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerHistoryEntry 7 }

snL4VirtualServerHistoryPeakConnections   OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerHistoryEntry 8 }


-- Virtual Server Port Monitor Group

-- The Virtual Server Port History Control Group


snL4VirtualServerPortHistoryControlTable OBJECT-TYPE
	SYNTAX SEQUENCE OF SnL4VirtualServerPortHistoryControlEntry
	ACCESS not-accessible
	STATUS mandatory
	DESCRIPTION
		"A list of history control entries."
	::= { snL4History 7 }

snL4VirtualServerPortHistoryControlEntry OBJECT-TYPE
	SYNTAX SnL4VirtualServerPortHistoryControlEntry
	ACCESS not-accessible
	STATUS mandatory
	DESCRIPTION
		"A list of parameters that set up a periodic sampling
		of statistics.As an example, an instance of the
		snL4VirtualServerPortHistoryControlInterval object might be named
		snL4VirtualServerPortHistoryControlInterval.2"
	INDEX { snL4VirtualServerPortHistoryControlIndex }
	::= { snL4VirtualServerPortHistoryControlTable 1 }

	SnL4VirtualServerPortHistoryControlEntry ::= SEQUENCE {
		snL4VirtualServerPortHistoryControlIndex			 
			INTEGER (1..65535),
		snL4VirtualServerPortHistoryControlDataSource		
			OBJECT IDENTIFIER,
		snL4VirtualServerPortHistoryControlBucketsRequested
			INTEGER (1..65535),
		snL4VirtualServerPortHistoryControlBucketsGranted	
			INTEGER (1..65535),
		snL4VirtualServerPortHistoryControlInterval		
			INTEGER (1..3600),
		snL4VirtualServerPortHistoryControlOwner			 
			DisplayString,
		snL4VirtualServerPortHistoryControlStatus			
			INTEGER
	}

snL4VirtualServerPortHistoryControlIndex OBJECT-TYPE
	SYNTAX INTEGER (1..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION
		"An index that uniquely identifies an entry in the
		snL4VirtualServerPortHistoryControl table.Each such entry defines a
		set of samples at a particular interval for an
		interface on the device."
	::= { snL4VirtualServerPortHistoryControlEntry 1 }

snL4VirtualServerPortHistoryControlDataSource OBJECT-TYPE
	SYNTAX OBJECT IDENTIFIER
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"This object identifies the source of the data for
		which historical data was collected and
		placed in a media-specific table on behalf of this
		snL4VirtualServerPortHistoryControlEntry.This source can be any
		real/virtual server and real/virtual server port on 
		this ServerIron.  In order to identify
		a particular instance, this object shall identify
		the instance of the object, defined in the above 
		statistics tables.
	
		This object may not be modified if the associated
		snL4VirtualServerPortHistoryControlStatus object is equal to valid(1)."
	::= { snL4VirtualServerPortHistoryControlEntry 2 }

snL4VirtualServerPortHistoryControlBucketsRequested OBJECT-TYPE
	SYNTAX INTEGER (1..65535)
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"The requested number of discrete time intervals
		over which data is to be saved in the part of the
		media-specific table associated with this
		snL4VirtualServerPortHistoryControlEntry.
	
		When this object is created or modified, the probe
		should set snL4VirtualServerPortHistoryControlBucketsGranted as closely to
		this object as is possible for the particular probe
		implementation and available resources."
	DEFVAL { 50 }
	::= { snL4VirtualServerPortHistoryControlEntry 3 }

snL4VirtualServerPortHistoryControlBucketsGranted OBJECT-TYPE
	SYNTAX INTEGER (1..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION
		"The number of discrete sampling intervals
		over which data shall be saved in the part of
		the media-specific table associated with this
		snL4VirtualServerPortHistoryControlEntry.
	
		When the associated snL4VirtualServerPortHistoryControlBucketsRequested
		object is created or modified, the probe
		should set this object as closely to the requested
		value as is possible for the particular
		probe implementation and available resources.The
		probe must not lower this value except as a result
		of a modification to the associated
		snL4VirtualServerPortHistoryControlBucketsRequested object.
	
		There will be times when the actual number of
		buckets associated with this entry is less than
		the value of this object.In this case, at the
		end of each sampling interval, a new bucket will
		be added to the media-specific table.
	
		When the number of buckets reaches the value of
		this object and a new bucket is to be added to the
		media-specific table, the oldest bucket associated
		with this snL4VirtualServerPortHistoryControlEntry shall be deleted by
		the agent so that the new bucket can be added.
	
		When the value of this object changes to a value less
		than the current value, entries are deleted
		from the media-specific table associated with this
		snL4VirtualServerPortHistoryControlEntry.Enough of the oldest of these
		entries shall be deleted by the agent so that their
		number remains less than or equal to the new value of
		this object.
	
		When the value of this object changes to a value
		greater than the current value, the number of
		associated media- specific entries may be allowed to
		grow."
	::= { snL4VirtualServerPortHistoryControlEntry 4 }

snL4VirtualServerPortHistoryControlInterval OBJECT-TYPE
	SYNTAX INTEGER (1..3600)
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"The interval in seconds over which the data is
		sampled for each bucket in the part of the
		media-specific table associated with this
		snL4VirtualServerPortHistoryControlEntry.This interval can
		be set to any number of seconds between 1 and
		3600 (1 hour).
	
		Because the counters in a bucket may overflow at their
		maximum value with no indication, a prudent manager
		will take into account the possibility of overflow
		in any of the associated counters.It is important
		to consider the minimum time in which any counter
		could overflow on a particular media type and set
		the snL4VirtualServerPortHistoryControlInterval object to a value less
		than this interval.This is typically most
		important for the 'octets' counter in any
		media-specific table.	
		This object may not be modified if the associated
		snL4VirtualServerPortHistoryControlStatus object is equal to valid(1)."
	DEFVAL { 1800 }
	::= { snL4VirtualServerPortHistoryControlEntry 5 }

snL4VirtualServerPortHistoryControlOwner OBJECT-TYPE
	SYNTAX DisplayString
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"The entity that configured this entry and is
		therefore using the resources assigned to it."
	::= { snL4VirtualServerPortHistoryControlEntry 6 }

snL4VirtualServerPortHistoryControlStatus OBJECT-TYPE
	SYNTAX INTEGER { 
				valid(1),
             	createRequest(2),
             	underCreation(3),
             	invalid(4)
           }
	ACCESS read-write
	STATUS mandatory
	DESCRIPTION
		"The status of this snL4VirtualServerPortHistoryControl entry.
		Each instance of the media-specific table associated
		with this snL4VirtualServerPortHistoryControlEntry will be deleted by the
		agent if this snL4VirtualServerPortHistoryControlEntry is not equal to
		valid(1)."
	::= { snL4VirtualServerPortHistoryControlEntry 7 }


-- The Virtual Server Port History Group


snL4VirtualServerPortHistoryTable OBJECT-TYPE
	SYNTAX SEQUENCE OF SnL4VirtualServerPortHistoryEntry
	ACCESS not-accessible
	STATUS mandatory
	DESCRIPTION
		"A list of Ethernet snL4History entries."
	::= { snL4History 8 }

snL4VirtualServerPortHistoryEntry OBJECT-TYPE
	SYNTAX SnL4VirtualServerPortHistoryEntry
	ACCESS not-accessible
	STATUS mandatory
	DESCRIPTION
		"An historical sample of Ethernet statistics on a
		particular Ethernet interface.  This sample is
		associated with the snL4VirtualServerPortHistoryControlEntry which set up
		the parameters for a regular collection of these
		samples.  As an example, an instance of the
		snL4VirtualServerPortHistoryReceivePkts object might be named
		snL4VirtualServerPortHistoryReceivePkts.2.89"
	INDEX { snL4VirtualServerPortHistoryIndex , snL4VirtualServerPortHistorySampleIndex }
	::= { snL4VirtualServerPortHistoryTable 1 }

SnL4VirtualServerPortHistoryEntry ::= SEQUENCE {
	snL4VirtualServerPortHistoryIndex                 
		INTEGER (1..65535),
	snL4VirtualServerPortHistorySampleIndex           
		INTEGER (1..2147483647),
	snL4VirtualServerPortHistoryIntervalStart         
		TimeTicks,
	snL4VirtualServerPortHistoryReceivePkts
		Counter,
	snL4VirtualServerPortHistoryTransmitPkts
		Counter,
	snL4VirtualServerPortHistoryTotalConnections
		Counter,
	snL4VirtualServerPortHistoryCurConnections
		INTEGER,
	snL4VirtualServerPortHistoryPeakConnections
		INTEGER
    }

snL4VirtualServerPortHistoryIndex OBJECT-TYPE
	SYNTAX INTEGER (1..65535)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION
		"The snL4VirtualServerPortHistory of which this entry is a part.The
		snL4VirtualServerPortHistory identified by a particular value of this
		index is the same snL4VirtualServerPortHistory as identified
		by the same value of snL4VirtualServerPortHistoryControlIndex."
	::= { snL4VirtualServerPortHistoryEntry 1 }

snL4VirtualServerPortHistorySampleIndex OBJECT-TYPE
	SYNTAX INTEGER (1..2147483647)
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION
		"An index that uniquely identifies the particular
		sample this entry represents among all samples
		associated with the same snL4VirtualServerPortHistoryControlEntry.
		This index starts at 1 and increases by one
		as each new sample is taken."
	::= { snL4VirtualServerPortHistoryEntry 2 }

snL4VirtualServerPortHistoryIntervalStart OBJECT-TYPE
	SYNTAX TimeTicks
	ACCESS read-only
	STATUS mandatory
	DESCRIPTION
		"The value of sysUpTime at the start of the interval
		over which this sample was measured.If the probe
		keeps track of the time of day, it should start
		the first sample of the snL4VirtualServerPortHistory at a time such that
		when the next hour of the day begins, a sample is
		started at that instant.Note that following this
		rule may require the probe to delay collecting the
		first sample of the snL4VirtualServerPortHistory, as each sample must be
		of the same interval.Also note that the sample which
		is currently being collected is not accessible in this
		table until the end of its interval."
	::= { snL4VirtualServerPortHistoryEntry 3 }


snL4VirtualServerPortHistoryReceivePkts	  OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerPortHistoryEntry 4 }

snL4VirtualServerPortHistoryTransmitPkts  OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerPortHistoryEntry 5 }

snL4VirtualServerPortHistoryTotalConnections   OBJECT-TYPE
	SYNTAX	Counter
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerPortHistoryEntry 6 }

snL4VirtualServerPortHistoryCurConnections   OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerPortHistoryEntry 7 }

snL4VirtualServerPortHistoryPeakConnections   OBJECT-TYPE
	SYNTAX	INTEGER
	ACCESS  read-only
	STATUS  mandatory
	DESCRIPTION
		""
	::= { snL4VirtualServerPortHistoryEntry 8 }

END
