-- These MIBs were created on 1/9/2003
-- This module defines enterprise MIBs for virtual router
-- 
-- Copyright (c) 1999-2004, Juniper Networks, Inc.
-- All rights reserved.

NETSCREEN-VR-MIB DEFINITIONS ::= BEGIN

IMPORTS
   OBJECT-TYPE
       FROM SNMPv2-SMI
   netscreenVR
       FROM NETSCREEN-SMI;

netscreenVRMibModule MODULE-IDENTITY
    LAST-UPDATED  "200405032022Z" -- May 03, 2004
    ORGANIZATION
        "Juniper Networks, Inc."
    CONTACT-INFO
        "Customer Support

         1194 North Mathilda Avenue 
         Sunnyvale, California 94089-1206
         USA

         Tel: 1-800-638-8296
         E-mail: customerservice@juniper.net
         HTTP://www.juniper.net"
    DESCRIPTION
        "This module defines the object that are used to monitor VR
         info"
    REVISION      "200405030000Z" -- May 03, 2004
    DESCRIPTION
        "Modified copyright and contact information"
    REVISION      "200109010000Z" -- September 1, 2003
    DESCRIPTION
        "Creation Date"
    ::= { netscreenVR 0 }


vrTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF VrEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "VR table.  This table contains VR info."
    ::= { netscreenVR 1 }

vrEntry OBJECT-TYPE
    SYNTAX     VrEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "Entry containing information about the
         BGP's Version, LocalAs and Identifier"
    INDEX { vrId }
    ::= { vrTable 1 }

VrEntry ::= SEQUENCE {
        vrName
            OCTET STRING,
        vrId
            INTEGER,
        vrVsysName
            OCTET STRING,
        vrRouteId
            INTEGER,
        vrMaxRoutes
            INTEGER,
        vrNumRoutes
            INTEGER,
        vrSharable
            INTEGER,
        vrOspfRipBgpEnabled
            INTEGER,
        vrTrapPrivate
            INTEGER
}

vrName OBJECT-TYPE
    SYNTAX     OCTET STRING 
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "Name of the VR."
    ::= { vrEntry 1 }

vrId OBJECT-TYPE
    SYNTAX     INTEGER (0..65535)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "Id for the VR. It will be used in all other
         private MIBs so that cross reference can be made."
    ::= { vrEntry 2 }

vrVsysName OBJECT-TYPE
    SYNTAX     OCTET STRING
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "Id of the vsys which owns this VR."
    ::= { vrEntry 3 }

vrRouteId OBJECT-TYPE
    SYNTAX     INTEGER 
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "Router id, used by OSFP and BGP."
    ::= { vrEntry 4 }

vrMaxRoutes OBJECT-TYPE
    SYNTAX     INTEGER 
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "Maximum routes allowed for this VR."
    ::= { vrEntry 5 }

vrNumRoutes OBJECT-TYPE
    SYNTAX     INTEGER 
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The number of routes currently the VR has."
    ::= { vrEntry 6 }

vrSharable OBJECT-TYPE
    SYNTAX     INTEGER 
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "The VR is sharable or not."
    ::= { vrEntry 7 }

vrOspfRipBgpEnabled OBJECT-TYPE
    SYNTAX     INTEGER 
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "Enable OSPF, RIP, BGP."
    ::= { vrEntry 8 }

vrTrapPrivate OBJECT-TYPE
    SYNTAX     INTEGER 
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
        "0 private, 1 public. This only applies to 
         root system' default VR. If private trap is
         enabled, a private trap is sent, otherwise,
         the standard trap is sent. For other VRs, By
         default, the public trap is supported."
    ::= { vrEntry 9 }
END

