-- This module defines enterprise MIBs for ARP
-- 
-- Copyright (c) 1999-2004, Juniper Networks, Inc.
-- All rights reserved.

NETSCREEN-IP-ARP-MIB DEFINITIONS ::= BEGIN

IMPORTS
    netscreenIp
        FROM NETSCREEN-SMI
    Integer32, IpAddress, MODULE-IDENTITY, OBJECT-TYPE
        FROM SNMPv2-SMI
    DisplayString,PhysAddress
        FROM SNMPv2-TC
    ;

nsIpArp MODULE-IDENTITY
    LAST-UPDATED  "200405032022Z" -- May 03, 2004
    ORGANIZATION
        "Juniper Networks, Inc."
    CONTACT-INFO
        "Customer Support

         1194 North Mathilda Avenue 
         Sunnyvale, California 94089-1206
         USA

         Tel: 1-800-638-8296
         E-mail: customerservice@juniper.net
         HTTP://www.juniper.net"
    DESCRIPTION
        "This module defines NetScreen private MIBs for ARP"
    REVISION      "200405030000Z" -- May 03, 2004
    DESCRIPTION
        "Modified copyright and contact information"
    REVISION      "200403030000Z" -- March 03, 2004
    DESCRIPTION
        "Converted to SMIv2 by Longview Software"
    REVISION      "200311100000Z" -- November 10, 2003
    DESCRIPTION
        "Correct spelling mistake"
    REVISION      "200109280000Z" -- September 28, 2001
    DESCRIPTION
        "No Comment"
    REVISION      "200105020000Z" -- May 02, 2001
    DESCRIPTION
        "Creation Date"
    ::= { netscreenIp 1 }

NsIpArpEntry ::= SEQUENCE
{
    nsIpArpIndex  Integer32,
    nsIpArpIp     IpAddress,
    nsIpArpMac    PhysAddress,
    nsIpArpVsys   Integer32,
    nsIpArpIfIdx  Integer32,
    nsIpArpState  INTEGER,
    nsIpArpAge    Integer32,
    nsIpArpRetry  Integer32,
    nsIpArpPakQue Integer32
}

nsIpArpAOD OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "ARP always on destination."
    ::= { nsIpArp 1 }

nsIpArpCachUpdate OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enabled(1)
    }
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "ARP cache update."
    ::= { nsIpArp 2 }

nsIpArpTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF NsIpArpEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "This table collects all the ARP entries existing in NetScreen
         device."
    ::= { nsIpArp 3 }

nsIpArpEntry OBJECT-TYPE
    SYNTAX        NsIpArpEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "An entry containing attributes of arp info"
    INDEX
        { nsIpArpIndex }
    ::= { nsIpArpTable 1 }

nsIpArpIndex OBJECT-TYPE
    SYNTAX        Integer32 (0..2147483647)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "A unique value for arp table.  Its value ranges between 0 and
         65535 and may not be contiguous."
    ::= { nsIpArpEntry 1 }

nsIpArpIp OBJECT-TYPE
    SYNTAX        IpAddress
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "IP address."
    ::= { nsIpArpEntry 2 }

nsIpArpMac OBJECT-TYPE
    SYNTAX        PhysAddress
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "MAC address."
    ::= { nsIpArpEntry 3 }

nsIpArpVsys OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Virtual system id this entry belongs to."
    ::= { nsIpArpEntry 4 }

nsIpArpIfIdx OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Interface location."
    ::= { nsIpArpEntry 5 }

nsIpArpState OBJECT-TYPE
    SYNTAX        INTEGER {
        pending(1),
        valid(2),
        delete(3),
        static(4)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "ARP entry state."
    ::= { nsIpArpEntry 6 }

nsIpArpAge OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "ARP entry age."
    ::= { nsIpArpEntry 7 }

nsIpArpRetry OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "ARP entry retry time."
    ::= { nsIpArpEntry 8 }

nsIpArpPakQue OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "ARP entry package queue."
    ::= { nsIpArpEntry 9 }

END


