-- *****************************************************************************
-- Juniper-DOS-PROTECTION-MIB
--
-- Juniper Networks Enterprise MIB
--   DOS Protection MIB 
--
-- Copyright (c) 2005-2006 Juniper Networks, Inc.
-- Copyright (c) 2008 Juniper Networks, Inc.
--   All Rights Reserved.
-- *****************************************************************************

Juniper-DOS-PROTECTION-MIB  DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE,  Counter32,  
		Unsigned32
        FROM SNMPv2-SMI
	JuniEnable
		FROM Juniper-TC
    TEXTUAL-CONVENTION, TruthValue, DisplayString, RowStatus
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
        FROM SNMPv2-CONF
    InterfaceIndex
        FROM IF-MIB
    juniMibs
        FROM Juniper-MIBs;

juniDosProtectionMIB  MODULE-IDENTITY
    LAST-UPDATED "200805060000Z"  -- 06-May-2008 00:00
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
        "       Juniper Networks, Inc.
        Postal: 10 Technology Park Drive
                Westford, MA  01886-3146
                USA
        Tel:    +1 978 589 5800
        Email:  mib@Juniper.net"
    DESCRIPTION 
		"The DOS Protection MIB for the Juniper E-Series product family. 
		This MIB contains managed objects for the DOS Protection 
		application. Management objects are provided to control and
		monitor the DOS protection application."
    -- Revision History
	REVISION   "200805060000Z"  -- 06-May-2008 00:00   JUNOSe 8.1
    DESCRIPTION
        "Updated JuniDosProtectionProtocolType TEXTUAL-CONVENTION "
	REVISION   "200607010000Z"  -- 01-Jul-2006 00:00   JUNOSe 8.1
    DESCRIPTION
        "Added Dos-Protection-Group support"
    REVISION    "200608180400Z"  -- 18-Aug-2006 00:00 AM EDT - JUNOSe 8.0
    DESCRIPTION
        "Added MPLS Lsp Ping support."
    REVISION    "200608171926Z"  -- 17-Aug-2006 03:26 PM EDT - JUNOSe 7.3
    DESCRIPTION
        "Added new protocol type, atmDynamicIfPppData, to manage in 
	 JuniDosProtectionProtocolType."
    REVISION    "200601010500Z"  -- 01-Jan-2006 00:00 AM EST - JUNOSe 7.3
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { juniMibs 80 }                  

-- ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Textual conventions
-- ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++

JuniDosProtectionProtocolType ::= TEXTUAL-CONVENTION
	STATUS      current
    DESCRIPTION 
		"The control protocols that are supported by the DOS protection 
		application."

    SYNTAX	INTEGER {
        pppEchoRequest(0),
        ppEchoReply(1),
        pppEchoReplyFast(2),
        pppControl(3),
        atmControl(4),
        atmOam(5),
        atmDynamicIf(6),
        atmInverseArp(7),
        frameRelayControl(8),
        frameRelayArp(9),
        pppoeControl(10),
        pppoePppConfig(11),
        ethernetArpMiss(12),
        ethernetArp(13),
        ethernetFcBasedArp(14),
        ethernetLacp(15),
        ethernetDynamicIf(16),
        slepSlarp(17),
        slepSlarpReplyFast(18),
        mplsTtlOnReceive(19),
        mplsTtlOnTransmit(20),
        mplsMtuExceeded(21),
        itmL2tpControl(22),
        flisInPayload(23),
        flisInPayloadUpdateTable(24),
        dhcpExternal(25),
        ipOsi(26),
        ipTtlExpired(27),
        ipOptionsOther(28),
        ipOptionsRouterAlert(29),
        ipMulticastBroadcastOther(30),
        ipMulticastDhcpSc(31),
        ipMulticastControlSc(32),
        ipMulticastControlIc(33),
        ipMulticastVrrp(34),
        ipMulticastCacheMiss(35),
        ipMulticastCacheMissAutoReply(36),
        ipMulticastWrongIf(37),
        ipLocalDhcpSc(38),
        ipLocalDhcpIc(39),
        ipLocalIcmpEcho(40),
        ipLocalIcmpOther(41),
        ipLocalLDP(42),
        ipLocalBgp(43),
        ipLocalOspf(44),
        ipLocalRsvp(45),
        ipLocalPim(46),
        ipLocalCops(47),
        ipLocalL2tpControlSc(48),
        ipLocalL2tpControlIc(49),
        ipLocalOther(50),
        ipLocalDemuxMiss(51),
        ipRouteToSrpEthernet(52),
        ipRouteNoRoute(53),
        ipNormalPathMtu(54),
        ipNeighborDiscovery(55),
        ipNeighborDiscoveryMiss(56),
        ipSearchError(57),
        ipMld(58),
        ipLocalPimAssert(59),
        ipLocalBfd(60),
        ipFastBfd(61),
        ipLocalFastBfd(62),
        ipIke(63),
        ipReassembly(64),
        ipLocalIcmpFragment(65),
        ipLocalFragment(66),
        ipAppClassifierHttpRedirect(67),
        ipMulticastDhcpIc(68),
        dhcpTesterIc(69),
        atmDynamicIfPppData(70),
        ipLocalLspPing(71) }


JuniDosProtectionPriorityType ::= TEXTUAL-CONVENTION
	STATUS      current
    DESCRIPTION 
		"The control priorities that are supported by the DOS protection 
		application."

    SYNTAX	INTEGER {
		hiGreenFcIc(0),
		hiYellowFcIc(1),
		loGreenFcIc(2),
		loYellowFcIc(3),
        hiGreenFcSc(4),
		hiYellowFcSc(5),
		loGreenFcSc(6),
		loYellowFcSc(7) }

JuniDosProtectionProtocolState ::= TEXTUAL-CONVENTION
	STATUS      current
    DESCRIPTION 
		"The current state of a protocol."

    SYNTAX	INTEGER {
		ok(1),
		inTrouble(2) }

JuniDosProtectionScfdsTableOverflowState ::= TEXTUAL-CONVENTION
	STATUS      current
    DESCRIPTION 
		"The current state of the suspicious flow table."

	SYNTAX INTEGER {
		 notOverflowingOrGrouping(1),
		 grouping(2),
		 overflowing(3) }

JuniDosProtectionProtocolPriorityType ::= TEXTUAL-CONVENTION
	STATUS      current
    DESCRIPTION 
		"The control priorities that are supported by the DOS protection 
		application for each control processor"

    SYNTAX	INTEGER {
		hiGreen(0),
		hiYellow(1),
		loGreen(2),
		loYellow(3),
		dataPath(4) }

JuniDosProtectionProtocolCannedType ::= TEXTUAL-CONVENTION
	STATUS 		current
	DESCRIPTION
		"The available canned dos-protection-groups which can be used
		to set defaults into a user specified group."
	
	SYNTAX INTEGER {
		default(0),
        enetAccess(1),
        atmAccess(2),
        frame(3),
        uplink(4)
	}

JuniDosProtectionLayerId ::= TEXTUAL-CONVENTION
	STATUS 	current
	DESCRIPTION 
		"The available interface types for which a profile entry
		may be defined."
	
	SYNTAX INTEGER {
		ip(0),
		ppp(1),
		ethernet(6),
		atm1483(11),
		pppoe(17),
		bridge1483(19),
		vlan(35),
		ipv6(50)
	}
	
JuniDosProtectionControlProcessorDestination ::= TEXTUAL-CONVENTION
	STATUS 	current
	DESCRIPTION 
		"The available control processors to which a control
		protocol may be directed."
	
	SYNTAX INTEGER {
	    ic(0),
	    sc(1),
	    dataPath(2)
	}

-- ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Managed objects
-- ++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++

juniDosProtectionObjects    OBJECT IDENTIFIER ::= { juniDosProtectionMIB 1 }
juniDosProtectionScfdsGroup OBJECT IDENTIFIER ::= { juniDosProtectionObjects 1 }
juniDosProtectionDpgGroup   OBJECT IDENTIFIER ::= { juniDosProtectionObjects 2 }

--
-- scalars
--
juniDosProtectionScfdsGlobalState	OBJECT-TYPE
	SYNTAX		JuniEnable
	MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION 
		"Controls whether the suspicious control flow detection system is 
		enabled or disabled.  Setting the value to enable(1) enables the 
		suspicious control flow detection system. Setting the value to 
		disable(0) disables the system.  
		
		When read this object returns the current state of the system."		
    DEFVAL { enable }

	::= { juniDosProtectionScfdsGroup 1 }

juniDosProtectionScfdsGlobalGrouping	OBJECT-TYPE
	SYNTAX		JuniEnable
	MAX-ACCESS	read-write
	STATUS 		current
	DESCRIPTION 
		"When set to enable(1), the suspicious flow control system will 
		group flows when resources are unavailable to treat each 
		suspicious flow individually.  When set to disable(0), this feature 
		will be inhibited and the suspicious control flow system may not 
		recognize all suspicious flows during a resource shortage.

		When read this object will return the current state of the object."
	DEFVAL { enable }

	::= { juniDosProtectionScfdsGroup 2 }

juniDosProtectionScfdsGlobalClearAll OBJECT-TYPE
    SYNTAX      INTEGER {
					ok(0),
                    clear(1) }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "When set to clear(1), the suspicious control flow detection system
        is cleared.  When set to ok(0), there is no effect and the 
		suspicious control flow detection system is unchanged.
		
		By clearing the suspicious control flow detection system all flows 
		are removed from the suspicious flow table.

        When read, always returns a value of ok(0)."

	::= { juniDosProtectionScfdsGroup 3 }

juniDosProtectionScfdsGlobalDiscontinuityTime OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The sysUpTime at which the counters were last re-initialized on 
		any slot due to a restart."

	::= { juniDosProtectionScfdsGroup 4 }

juniDosProtectionScfdsGlobalTableOverflowState OBJECT-TYPE
	SYNTAX		JuniDosProtectionScfdsTableOverflowState
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION 
		"Indicates whether any module in the system is in under a resource 
		shortage situation. A value of notOverflowingOrGrouping(1) indicates
		that there is no resource shortage on any module. A value of 
		grouping(2) or overflowing(3) indicates that at least one module
		is suffering from a resource shortage, and has acted according to the
		state of the juniDosProtectionScfdsGlobalGrouping object."

	::= { juniDosProtectionScfdsGroup 5 } 

--
-- global counters
--

juniDosProtectionScfdsGlobalCurrentSuspiciousFlows OBJECT-TYPE
	SYNTAX		Counter32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION 
		"The number of flows currently marked as suspicious."

	::= { juniDosProtectionScfdsGroup 6 } 

juniDosProtectionScfdsGlobalNumberSuspiciousFlows	OBJECT-TYPE
	SYNTAX		Counter32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION 
		"The number of suspicious flows seen since system restart."

	::= { juniDosProtectionScfdsGroup 7 } 

juniDosProtectionScfdsGlobalCurrentSuspiciousFlowGroups OBJECT-TYPE
	SYNTAX		Counter32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION 
		"The number of flow groups currently marked as suspicious."

	::= { juniDosProtectionScfdsGroup 8 } 

juniDosProtectionScfdsGlobalNumberSuspiciousFlowGroups OBJECT-TYPE
	SYNTAX		Counter32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION 
		"The number of suspicius flow groups seen since system restart."

	::= { juniDosProtectionScfdsGroup 9 } 


juniDosProtectionScfdsGlobalCurrentFalseNegativeFlows OBJECT-TYPE
	SYNTAX		Counter32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION 
		"The number of flows currently falsely considered suspicious.
		A false negative indicates that the flow was seen as possibly
		suspicious, but did not pass all the tests to be considered
		suspicious. This is a normal condition of the system."

	::= { juniDosProtectionScfdsGroup 10 } 

juniDosProtectionScfdsGlobalNumberFalseNegativeFlows OBJECT-TYPE
	SYNTAX		Counter32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION 
		"The number of flows falsely considered possibly suspicious 
		seen since system restart."

	::= { juniDosProtectionScfdsGroup 11 } 

juniDosProtectionScfdsGlobalNumberTableOverflows OBJECT-TYPE
	SYNTAX		Counter32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION 
		"The total number of times the system had a table overflow on any slot."

	::= { juniDosProtectionScfdsGroup 12 } 


--
-- protocol table 
--

juniDosProtectionScfdsProtocolTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF JuniDosProtectionScfdsProtocolEntry
	MAX-ACCESS 	not-accessible
	STATUS		current
	DESCRIPTION 
		"The information for the DOS protection control protocols."

	::= { juniDosProtectionScfdsGroup 13 } 

juniDosProtectionScfdsProtocolEntry OBJECT-TYPE
	SYNTAX		JuniDosProtectionScfdsProtocolEntry
	MAX-ACCESS 	not-accessible
	STATUS		current
	DESCRIPTION
		"The information for an individual DOS protection control
		protocol."

	INDEX	{ juniDosProtectionScfdsProtocolIndex }

	::= { juniDosProtectionScfdsProtocolTable 1 } 
	
JuniDosProtectionScfdsProtocolEntry ::= SEQUENCE {
	juniDosProtectionScfdsProtocolIndex 		 JuniDosProtectionProtocolType,
	juniDosProtectionScfdsProtocolThreshold	 Unsigned32,
	juniDosProtectionScfdsProtocolLowThreshold Unsigned32,
	juniDosProtectionScfdsProtocolBackoffTime  Unsigned32,
	juniDosProtectionScfdsProtocolState        JuniDosProtectionProtocolState,
	juniDosProtectionScfdsProtocolTransitions  Counter32}

juniDosProtectionScfdsProtocolIndex OBJECT-TYPE
    SYNTAX      JuniDosProtectionProtocolType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The control protocol value for this entry."

    ::= { juniDosProtectionScfdsProtocolEntry 1 }

juniDosProtectionScfdsProtocolThreshold OBJECT-TYPE
	SYNTAX		Unsigned32(0|3..65535)
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION 
		"The threshold in packets per second for this control protocol.
		This is the rate at which a flow for this protocol is considered
		suspicious. Setting this object to zero will have the affect of
		excusing this protocol from suspicious control flow detection."

    ::= { juniDosProtectionScfdsProtocolEntry 2 }

juniDosProtectionScfdsProtocolLowThreshold OBJECT-TYPE
	SYNTAX		Unsigned32(0|1..32767)
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION 
		"The low threshold in packets per second for this control protocol .
		This is the rate at which a flow must fall below to in order return 
		to the normal state, after having been marked suspicious. A
		low threshold of zero disables this functionality."

    ::= { juniDosProtectionScfdsProtocolEntry 3 }

juniDosProtectionScfdsProtocolBackoffTime	OBJECT-TYPE
	SYNTAX      Unsigned32(0|10..1000)
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION 
		"The backoff time in seconds. A flow which is considered suspicious will
		be returned to normal after this amount of time regardless of the current
		rate of the flow.  A backoff time of 0 disables this functionality."
	DEFVAL  { 300 } 

    ::= { juniDosProtectionScfdsProtocolEntry 4 }

juniDosProtectionScfdsProtocolState OBJECT-TYPE
	SYNTAX		JuniDosProtectionProtocolState
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION 
		"The current state of the protocol.  This object will return inTrouble(2)
		if any module in the system has reported that the protocol is currently
		being watched for suspicious flows. If no module reports that this protocol
		is being watched this object will return ok(1). 

		A protocol is in trouble on a module when the sum of the rate for all 
		flows for the protocol is over the limit for that protocol."

    ::= { juniDosProtectionScfdsProtocolEntry 5 }

juniDosProtectionScfdsProtocolTransitions OBJECT-TYPE
	SYNTAX		Counter32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION 
		"The number of transitions to 'inTrouble' that this control protocol 
		has made."

    ::= { juniDosProtectionScfdsProtocolEntry 6 }

--
-- dos protection groups
-- 

juniDosProtectionDpgTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF JuniDosProtectionDpgEntry
	MAX-ACCESS 	not-accessible
	STATUS		current
	DESCRIPTION 
		"The information for a dos-protection-group. A 
		dos-protection-group defines a set of parameters that
		manage the handling of control protocols on the
		router."

	::= { juniDosProtectionDpgGroup 1 } 

juniDosProtectionDpgEntry OBJECT-TYPE
	SYNTAX		JuniDosProtectionDpgEntry
	MAX-ACCESS 	not-accessible
	STATUS		current
	DESCRIPTION
		"The information for an individual dos-protection-group."

	INDEX	{ juniDosProtectionDpgIndex }

	::= { juniDosProtectionDpgTable 1 } 

JuniDosProtectionDpgEntry ::= SEQUENCE {
	juniDosProtectionDpgIndex			 		 DisplayString,
	juniDosProtectionDpgRowStatus              RowStatus,
	juniDosProtectionDpgCanned                 
						JuniDosProtectionProtocolCannedType,
	juniDosProtectionDpgRevert                 INTEGER,
	juniDosProtectionDpgModified				 TruthValue,
	juniDosProtectionDpgReferences			 INTEGER}

juniDosProtectionDpgIndex OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The dos-protection-group-name for this entry."

    ::= { juniDosProtectionDpgEntry 1 }

juniDosProtectionDpgRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
		"Controls creation/deletion of entries in this table.  
		Only the values 'createAndGo' and 'destroy' may be SET. 
		When read this always returns a value of active"

    ::= { juniDosProtectionDpgEntry 2 }

juniDosProtectionDpgCanned OBJECT-TYPE
    SYNTAX      JuniDosProtectionProtocolCannedType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Sets the default values based for the dos-protection-group 
		based on the values from the canned group. Can only be used
		to set a different group. Using the current group will result
		in no changes to the dos-protection-group."
    DEFVAL { default }	

    ::= { juniDosProtectionDpgEntry 3 }

juniDosProtectionDpgRevert OBJECT-TYPE
    SYNTAX      INTEGER {
                    no-revert(0),
                    revert(1) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Revert this dos-protection-group to the canned values of the
		associated canned group by setting this object to
		revert(1). Reading this object will always return a value 
		of no-revert(1)"

    ::= { juniDosProtectionDpgEntry 4 }

juniDosProtectionDpgModified OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
		"When true is returned, some protocol or priority associated 
		with this dos-protection-group, has been modified from the 
		canned values associated with the group. When false is returned
		all settings associated with this dos-protection-group are 
		at the defaults for the associated canned group."

    ::= { juniDosProtectionDpgEntry 5 }

juniDosProtectionDpgReferences OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
		"The number of references for this dos-protection-group. 
		References include the number of interfaces currently 
		associated with the group, as well as the number of profile
		references."

    ::= { juniDosProtectionDpgEntry 6 }
--
-- dpg protocol information
--

juniDosProtectionDpgProtocolTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF JuniDosProtectionDpgProtocolEntry
	MAX-ACCESS 	not-accessible
	STATUS		current
	DESCRIPTION 
		"The information for the dos-protection-group control protocol 
		table."

	::= { juniDosProtectionDpgGroup 2 } 

juniDosProtectionDpgProtocolEntry OBJECT-TYPE
	SYNTAX		JuniDosProtectionDpgProtocolEntry
	MAX-ACCESS 	not-accessible
	STATUS		current
	DESCRIPTION
		"The information for an individual dos-protection-group control
		protocol entry."

	INDEX	{ juniDosProtectionDpgProtocolName,
	          juniDosProtectionDpgProtocolProtocol }

	::= { juniDosProtectionDpgProtocolTable 1 } 
	
JuniDosProtectionDpgProtocolEntry ::= SEQUENCE {
	juniDosProtectionDpgProtocolName			  DisplayString,
	juniDosProtectionDpgProtocolProtocol	      JuniDosProtectionProtocolType,
	juniDosProtectionDpgProtocolBurst			  Unsigned32,
	juniDosProtectionDpgProtocolDropProbability Unsigned32,
	juniDosProtectionDpgProtocolRate            Unsigned32,
	juniDosProtectionDpgProtocolSkipPriorityRateLimiter
											  JuniEnable,
	juniDosProtectionDpgProtocolWeight          Unsigned32,
	juniDosProtectionDpgProtocolPriority  
	                JuniDosProtectionProtocolPriorityType,
	juniDosProtectionDpgProtocolModified       TruthValue,
	juniDosProtectionDpgProtocolDestination    
					JuniDosProtectionControlProcessorDestination}


juniDosProtectionDpgProtocolName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The dos-protection-group name for this entry."

    ::= { juniDosProtectionDpgProtocolEntry 1 }	

juniDosProtectionDpgProtocolProtocol OBJECT-TYPE
    SYNTAX      JuniDosProtectionProtocolType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The dos-protection-group control protocol for this entry."

    ::= { juniDosProtectionDpgProtocolEntry 2 }	

juniDosProtectionDpgProtocolBurst OBJECT-TYPE
	SYNTAX		Unsigned32(0|32..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The burst in packets for this control protocol in this 
		dos-protection-group."

    ::= { juniDosProtectionDpgProtocolEntry 3 }	

juniDosProtectionDpgProtocolDropProbability OBJECT-TYPE
	SYNTAX		Unsigned32(10..100)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The drop probability for suspect packets for this
		control protocol in this dos-protection-group.  This is
		probability that a packet belonging to a suspicious
		flow will be dropped. A drop probability of less than
		100 indicates that the user wishes to have some 
		packets from a suspect flow reach the control
		processor."

    ::= { juniDosProtectionDpgProtocolEntry 4 }	

juniDosProtectionDpgProtocolRate OBJECT-TYPE
	SYNTAX		Unsigned32(0|64..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The rate in packets per second for this control protocol in 
		this dos-protection-group."

    ::= { juniDosProtectionDpgProtocolEntry 5 }

juniDosProtectionDpgProtocolSkipPriorityRateLimiter OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "When set to enable, this control protocol in this 
		dos-protection-group will skip the priority rate limiter. 
		When set to disable, the protocol will not skip the priority 
		rate-limiter."

    ::= { juniDosProtectionDpgProtocolEntry 6 }

juniDosProtectionDpgProtocolWeight OBJECT-TYPE
	SYNTAX		Unsigned32(100..500)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The weight of this control protocol against others of the
		same priority in this dos-protection-group. The weight
		is used to determine the minimum rate and burst 
		for the protocol within the priority group."
    DEFVAL { 100 } 

    ::= { juniDosProtectionDpgProtocolEntry 7 }	

juniDosProtectionDpgProtocolPriority  OBJECT-TYPE
	SYNTAX 		JuniDosProtectionProtocolPriorityType   
	MAX-ACCESS  read-write
	STATUS		current
	DESCRIPTION 
		"The priority for the control protocol. Packets of this control
		protocol on interfaces referencing this dos-protection-group will
		be categorized into the priority indicated."
	
    ::= { juniDosProtectionDpgProtocolEntry 8 }

juniDosProtectionDpgProtocolModified  OBJECT-TYPE
	SYNTAX 		TruthValue
	MAX-ACCESS  read-only
	STATUS		current
	DESCRIPTION 
		"When true is returned, the values for this control protocol
		in this dos-protection-group have been modified from the 
		canned values associated with the group. When false is returned
		all settings associated with this control protocol in this
		dos-protection-group are at the defaults for the associated 	
		canned group."
	
    ::= { juniDosProtectionDpgProtocolEntry 9 }

juniDosProtectionDpgProtocolDestination    OBJECT-TYPE
	SYNTAX 		JuniDosProtectionControlProcessorDestination
	MAX-ACCESS  read-only
	STATUS		current
	DESCRIPTION 
		"The destination processor for packets of this control protocol."
	
    ::= { juniDosProtectionDpgProtocolEntry 10 }

--
-- dpg priority information
--

juniDosProtectionDpgPriorityTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF JuniDosProtectionDpgPriorityEntry
	MAX-ACCESS 	not-accessible
	STATUS		current
	DESCRIPTION 
		"The information for a dos-protection-group priority table."

	::= { juniDosProtectionDpgGroup 3 } 

juniDosProtectionDpgPriorityEntry OBJECT-TYPE
	SYNTAX		JuniDosProtectionDpgPriorityEntry
	MAX-ACCESS 	not-accessible
	STATUS		current
	DESCRIPTION
		"The information for an individual dos-protection-group priority 
		table"

	INDEX	{ juniDosProtectionDpgPriorityName,
	          juniDosProtectionDpgPriorityPriority }

	::= { juniDosProtectionDpgPriorityTable 1 } 
	
JuniDosProtectionDpgPriorityEntry ::= SEQUENCE {
	juniDosProtectionDpgPriorityName			  DisplayString,
	juniDosProtectionDpgPriorityPriority	      JuniDosProtectionPriorityType,
	juniDosProtectionDpgPriorityBurst			  Unsigned32,
	juniDosProtectionDpgPriorityOverSubscriptionFactor
	                                          Unsigned32,
	juniDosProtectionDpgPriorityRate            Unsigned32,
	juniDosProtectionDpgPriorityModified        TruthValue}


juniDosProtectionDpgPriorityName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The dos-proteciton-group name for this entry."

    ::= { juniDosProtectionDpgPriorityEntry 1 }	

juniDosProtectionDpgPriorityPriority OBJECT-TYPE
    SYNTAX      JuniDosProtectionPriorityType
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The priority for this entry."

    ::= { juniDosProtectionDpgPriorityEntry 2 }	

juniDosProtectionDpgPriorityBurst OBJECT-TYPE
	SYNTAX		Unsigned32(0|32..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The burst in packets for this priority in this 
		dos-protection-group."

    ::= { juniDosProtectionDpgPriorityEntry 3 }	

juniDosProtectionDpgPriorityOverSubscriptionFactor OBJECT-TYPE
	SYNTAX		Unsigned32(100..1000)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The over-subscription factor for this priority in this 
		dos-protection-group. This is used when calculating 
		the minimum rates for control protocols that use this priority."

    ::= { juniDosProtectionDpgPriorityEntry 4 }	

juniDosProtectionDpgPriorityRate OBJECT-TYPE
	SYNTAX		Unsigned32(0|64..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The rate in packets per second for this priority in 
		this dos-protection-group."

    ::= { juniDosProtectionDpgPriorityEntry 5 }

juniDosProtectionDpgPriorityModified OBJECT-TYPE
	SYNTAX		TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "When true is returned, the values for this priority
		in this dos-protection-group have been modified from the 
		canned values associated with the group. When false is returned
		all settings associated with this priority in this
		dos-protection-group are at the defaults for the associated 	
		canned group."

    ::= { juniDosProtectionDpgPriorityEntry 6 }


--
--  attachment table
--

juniDosProtectionDpgAttachTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF JuniDosProtectionDpgAttachEntry
	MAX-ACCESS 	not-accessible
	STATUS		current
	DESCRIPTION 
		"The information for the DOS protection attachment table."

	::= { juniDosProtectionDpgGroup 4 } 

juniDosProtectionDpgAttachEntry OBJECT-TYPE
	SYNTAX		JuniDosProtectionDpgAttachEntry
	MAX-ACCESS 	not-accessible
	STATUS		current
	DESCRIPTION
		"The information for an individual DOS protection attachment entry."

	INDEX	{ juniDosProtectionDpgAttachIndex }

	::= { juniDosProtectionDpgAttachTable 1 } 
	
JuniDosProtectionDpgAttachEntry ::= SEQUENCE {
	juniDosProtectionDpgAttachIndex			  InterfaceIndex,
	juniDosProtectionDpgAttachRowStatus         RowStatus,
	juniDosProtectionDpgAttachName              DisplayString,
	juniDosProtectionDpgAttachConfigured        TruthValue}

juniDosProtectionDpgAttachIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex 
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The interface index for the attachment."

    ::= { juniDosProtectionDpgAttachEntry 1 }	

juniDosProtectionDpgAttachRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
		"Controls creation/deletion of entries in this table.  Only the 
		values 'createAndGo' and 'destroy' may be SET. 
		When read this always returns a value of active"

    ::= { juniDosProtectionDpgAttachEntry 2 }	

juniDosProtectionDpgAttachName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..32))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The dos-protection-group for this entry. This is the 
		dos-protection-group that is use by the interface."

    ::= { juniDosProtectionDpgAttachEntry 3 }	

juniDosProtectionDpgAttachConfigured         OBJECT-TYPE
	SYNTAX		TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the configured status of the attachment. This object
		returns true when the attachment was statically
		configured, and returns false when the attachment
		was made via a profile attachment."

    ::= { juniDosProtectionDpgAttachEntry 4 }	
--
--  profile table
--
juniDosProtectionDpgProfileTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF JuniDosProtectionDpgProfileEntry
	MAX-ACCESS 	not-accessible
	STATUS		current
	DESCRIPTION 
		"The information for the DOS protection profile table."

	::= { juniDosProtectionDpgGroup 5 } 

juniDosProtectionDpgProfileEntry OBJECT-TYPE
	SYNTAX		JuniDosProtectionDpgProfileEntry
	MAX-ACCESS 	not-accessible
	STATUS		current
	DESCRIPTION
		"The information for an individual DOS protection profile  entry."

	INDEX	{ juniDosProtectionDpgProfileProfileId,
			  juniDosProtectionDpgProfileLayerId}

	::= { juniDosProtectionDpgProfileTable 1 } 
	

JuniDosProtectionDpgProfileEntry ::= SEQUENCE {
	juniDosProtectionDpgProfileProfileId		   Unsigned32,
	juniDosProtectionDpgProfileLayerId		   JuniDosProtectionLayerId,
	juniDosProtectionDpgProfileRowStatus         RowStatus,
	juniDosProtectionDpgProfileName              DisplayString }

juniDosProtectionDpgProfileProfileId OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The profile ID for the profile entry. The profile ID 
		identifies which profile is being accessed. A value for this
        identifier is determined by locating or creating a profile name 
		in the juniProfileNameTable"

    ::= { juniDosProtectionDpgProfileEntry 1 }

juniDosProtectionDpgProfileLayerId OBJECT-TYPE
    SYNTAX      JuniDosProtectionLayerId
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The layer ID for the profile entry. The layer ID indicates
		which interface type is being accessed."

    ::= { juniDosProtectionDpgProfileEntry 2 }

juniDosProtectionDpgProfileRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
		"Controls creation/deletion of entries in this table.  Only the 
		values 'createAndGo' and 'destroy' may be SET. When read this 
		always returns a value of active"

    ::= { juniDosProtectionDpgProfileEntry 3 }	

juniDosProtectionDpgProfileName OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(1..32))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The dos-protection-group that is associated with this 
		profile/interface-type. This profile will be attached 
		when dynamic instances of the interface type are
		created that reference the specific profile."

    ::= { juniDosProtectionDpgProfileEntry 4 }	


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Notifications
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++

--juniDosProtectionTraps OBJECT IDENTIFIER ::= { juniDosProtectionMIB 0 }
--juniDosProtectionTrapControl OBJECT IDENTIFIER ::= { juniDosProtectionMIB 2 }
--juniDosProtectionScfdsTraps OBJECT IDENTIFIER ::= { juniDosProtectionTraps 0 }





-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Conformance information
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++

juniDosProtectionMIBConformance  OBJECT IDENTIFIER ::= { juniDosProtectionMIB 4 }
juniDosProtectionMIBCompliances  OBJECT IDENTIFIER ::= { juniDosProtectionMIBConformance 1 }
juniDosProtectionMIBGroups       OBJECT IDENTIFIER ::= { juniDosProtectionMIBConformance 2 }


juniDosProtectionCompliance  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for entities which implement the Juniper 
		Dos Protection MIB. This was made obsolete with the addition of
		dos-protection-groups."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniDosProtectionGroup }
    ::= { juniDosProtectionMIBCompliances 1 }  

juniDosProtectionCompliance2  MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for entities which implement the Juniper 
		Dos	Protection MIB."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniDosProtectionGroup2 }
    ::= { juniDosProtectionMIBCompliances 2 }   -- Junos x.y

--
-- units of conformance
--
juniDosProtectionGroup OBJECT-GROUP
	OBJECTS {juniDosProtectionScfdsGlobalState,	
			juniDosProtectionScfdsGlobalGrouping,	
			juniDosProtectionScfdsGlobalClearAll, 
			juniDosProtectionScfdsGlobalDiscontinuityTime, 
			juniDosProtectionScfdsGlobalTableOverflowState, 
			juniDosProtectionScfdsGlobalCurrentSuspiciousFlows, 
			juniDosProtectionScfdsGlobalNumberSuspiciousFlows,	
			juniDosProtectionScfdsGlobalCurrentSuspiciousFlowGroups, 
			juniDosProtectionScfdsGlobalNumberSuspiciousFlowGroups, 
			juniDosProtectionScfdsGlobalCurrentFalseNegativeFlows, 
			juniDosProtectionScfdsGlobalNumberFalseNegativeFlows, 
			juniDosProtectionScfdsGlobalNumberTableOverflows, 
			juniDosProtectionScfdsProtocolThreshold, 
			juniDosProtectionScfdsProtocolLowThreshold, 
			juniDosProtectionScfdsProtocolBackoffTime,	
			juniDosProtectionScfdsProtocolState, 
			juniDosProtectionScfdsProtocolTransitions }
    STATUS obsolete
	DESCRIPTION 
		"A collection of objects providing management of DOS protection 
		application in a Juniper product. This object became obsolete
		with the addition of dos-protection-groups."

	::= { juniDosProtectionMIBGroups 1 }

juniDosProtectionGroup2 OBJECT-GROUP
	OBJECTS {juniDosProtectionScfdsGlobalState,	
			juniDosProtectionScfdsGlobalGrouping,	
			juniDosProtectionScfdsGlobalClearAll, 
			juniDosProtectionScfdsGlobalDiscontinuityTime, 
			juniDosProtectionScfdsGlobalTableOverflowState, 
			juniDosProtectionScfdsGlobalCurrentSuspiciousFlows, 
			juniDosProtectionScfdsGlobalNumberSuspiciousFlows,	
			juniDosProtectionScfdsGlobalCurrentSuspiciousFlowGroups, 
			juniDosProtectionScfdsGlobalNumberSuspiciousFlowGroups, 
			juniDosProtectionScfdsGlobalCurrentFalseNegativeFlows, 
			juniDosProtectionScfdsGlobalNumberFalseNegativeFlows, 
			juniDosProtectionScfdsGlobalNumberTableOverflows, 
			juniDosProtectionScfdsProtocolThreshold, 
			juniDosProtectionScfdsProtocolLowThreshold, 
			juniDosProtectionScfdsProtocolBackoffTime,	
			juniDosProtectionScfdsProtocolState, 
			juniDosProtectionScfdsProtocolTransitions,
			juniDosProtectionDpgRowStatus,	
			juniDosProtectionDpgCanned,
			juniDosProtectionDpgRevert,
			juniDosProtectionDpgModified,
			juniDosProtectionDpgReferences,
			juniDosProtectionDpgProtocolBurst,
			juniDosProtectionDpgProtocolDropProbability,
			juniDosProtectionDpgProtocolRate,
			juniDosProtectionDpgProtocolSkipPriorityRateLimiter,
			juniDosProtectionDpgProtocolWeight,
			juniDosProtectionDpgProtocolModified,
			juniDosProtectionDpgPriorityBurst,
			juniDosProtectionDpgPriorityOverSubscriptionFactor,
			juniDosProtectionDpgPriorityRate,
			juniDosProtectionDpgPriorityModified,
			juniDosProtectionDpgAttachRowStatus,
			juniDosProtectionDpgAttachName,
			juniDosProtectionDpgProfileRowStatus,
			juniDosProtectionDpgProfileName	}
    STATUS current
	DESCRIPTION 
		"A collection of objects providing management of DOS protection 
		application in a Juniper product."

	::= { juniDosProtectionMIBGroups 2 }
END
