
Dell-Vendor-MIB DEFINITIONS ::= BEGIN

IMPORTS
        enterprises, TimeTicks
                FROM RFC1155-SMI
        MODULE-IDENTITY, OBJECT-TYPE, Unsigned32, Integer32, IpAddress,
        NOTIFICATION-TYPE
                FROM SNMPv2-SMI
        DisplayString, RowStatus, TEXTUAL-CONVENTION
                FROM SNMPv2-TC;


powerConnect3000MIB MODULE-IDENTITY
        LAST-UPDATED "200211250000Z"
        ORGANIZATION "Dell Computer Corporation"
        CONTACT-INFO
                "support.dell.com"
        DESCRIPTION
                "The private MIB module definition for the Dell powerConnect 3000 Devices."
        REVISION "200211250000Z"
        DESCRIPTION
                "Initial version of this MIB."
        ::= { enterprises dell(674) dellLan(10895) 3000 }

EnvMonState ::= TEXTUAL-CONVENTION
        STATUS  current
        DESCRIPTION
                "Represents the state of a device being monitored.
                 Valid values are:

                 normal(1):         the environment is good, such as low
                                    temperature.

                 warning(2):        the environment is bad, such as temperature
                                    above normal operation range but not too
                                    high.

                 critical(3):       the environment is very bad, such as
                                    temperature much higher than normal
                                    operation limit.

                 shutdown(4):       the environment is the worst, the system
                                    should be shutdown immediately.

                 notPresent(5):     the environmental monitor is not present,
                                    such as temperature sensors do not exist.

                 notFunctioning(6): the environmental monitor does not
                                    function properly, such as a temperature
                                    sensor generates a abnormal data like
                                    1000 C.
                "
        SYNTAX  INTEGER {
                        normal(1),
                        warning(2),
                        critical(3),
                        shutdown(4),
                        notPresent(5),
                        notFunctioning(6)
                }



dell-VendorMIBObjects       OBJECT IDENTIFIER ::= { powerConnect3000MIB 1 }
dellVendorNotifications     OBJECT IDENTIFIER ::= { powerConnect3000MIB 2 }



hardware              OBJECT IDENTIFIER ::= { dell-VendorMIBObjects 2 }
productIdentification OBJECT IDENTIFIER ::= { hardware 100 }
productStatus         OBJECT IDENTIFIER ::= { hardware 110 }

--

--
-- productIdentification
--


productIdentificationDisplayName OBJECT-TYPE
       SYNTAX      DisplayString
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION "Name of this product for display purposes."
       ::= { productIdentification 1}


productIdentificationDescription OBJECT-TYPE
       SYNTAX      DisplayString
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION "A short description of this product such as: Ethernet Router Switch."
       ::= { productIdentification 2}


productIdentificationVendor OBJECT-TYPE
       SYNTAX      DisplayString
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION "The name of the product manufacturer, such as: Dell Computer Corp."
       ::= { productIdentification 3 }

productIdentificationVersion OBJECT-TYPE
       SYNTAX      DisplayString
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION "The version of this product."
       ::= { productIdentification  4 }

productIdentificationBuildNumber OBJECT-TYPE
       SYNTAX      DisplayString
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION "The software build number of the product."
       ::= { productIdentification 5 }


productIdentificationURL  OBJECT-TYPE
       SYNTAX      DisplayString
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION "The URL of the web-based application to manage this device, should the device provide one.
                    The format of the value held by this object is: http://<device IP address>."
       ::= { productIdentification 6 }

productIdentificationDeviceNetworkName OBJECT-TYPE
       SYNTAX      DisplayString
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION "Device Name."
       ::= { productIdentification 7 }


productIdentificationPerUnitTable OBJECT-TYPE
   SYNTAX SEQUENCE OF ProductIdentificationPerBoxEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
        "Identification specific to product instance and, in case of stackable products, per unit. If the product is not stackable,
         it will be considered a stack of one unit and therefore this table will contain one conceptual row only."
     ::= { productIdentification 8 }

productIdentificationPerUnitEntry OBJECT-TYPE
   SYNTAX ProductIdentificationPerBoxEntry
   MAX-ACCESS not-accessible
   STATUS current
   DESCRIPTION
        "This row applies to a unit in a stackable product. "
   INDEX { productIdentificationPerBoxIndex }
     ::= { productIdentificationPerUnitTable 1 }



ProductIdentificationPerBoxEntry ::= SEQUENCE {

  productIdentificationPerBoxIndex   INTEGER,
  productIdentificationSerialNumber   DisplayString,
  productIdentificationAssetTag       DisplayString,
  productIdentificationServiceTag     DisplayString
}

productIdentificationPerBoxIndex OBJECT-TYPE
       SYNTAX      INTEGER (1..2147483647)
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION "The index of the stack unit to which this conceptual row corresponds.
                    Note that the index will be the same index as the index
                    of a 'chassis' physical entity in the entity MIB of the product."
       ::= { productIdentificationPerUnitEntry 1 }


productIdentificationSerialNumber OBJECT-TYPE
       SYNTAX      DisplayString
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION "Serial number of the product."
       ::= { productIdentificationPerUnitEntry 2 }

productIdentificationAssetTag OBJECT-TYPE
       SYNTAX      DisplayString
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION "Asset tag of the product."
       ::= { productIdentificationPerUnitEntry 3 }

productIdentificationServiceTag OBJECT-TYPE
       SYNTAX      DisplayString
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION "Service tag of the product."
       ::= { productIdentificationPerUnitEntry 4 }


--
-- productStatus
--

productStatusGlobalStatus  OBJECT-TYPE
       SYNTAX      INTEGER {
            ok(3),
            non-critical(4),
            critical(5)
       }
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION "Current status of the product.This is a rollup for the entire product.
                    The status is intended to give initiative to a snmp monitor to get further data when this status is abnormal.
                    This variable can take the following values:
                    3: OK
                       If fans and power supplies are functioning and the system did not reboot because of a HW watchdog failure
                       or a SW fatal error condition.
                    4: Non-critical
                       If at least one power supply is not functional or the system rebooted at least once because of a HW watchdog failure
                       or a SW fatal error condition.
                    5: Critical
                       If at least one fan is not functional, possibly causing a dangerous warming up of the device."
       ::= { productStatus 1 }

productStatusLastGlobalStatus OBJECT-TYPE
       SYNTAX      INTEGER {
            ok(3),
            non-critical(4),
            critical(5)
       }
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION "The status before the current status which induced an initiative to issue a global status change trap."
       ::= { productStatus 2 }

productStatusTimeStamp  OBJECT-TYPE
       SYNTAX      TimeTicks
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION "The last time that the product global status has been updated.
                    The time will be given in TimeTicks"
       ::= { productStatus 3 }

productStatusGetTimeOut  OBJECT-TYPE
       SYNTAX      INTEGER
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION "Suggested time out value in milliseconds for how long the SNMP getter
                    should wait while attempting to poll the product SNMP service."
       ::= { productStatus 4 }

productStatusRefreshRate  OBJECT-TYPE
       SYNTAX      INTEGER
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION "Rate in seconds at which the SNMP service cached data is being updated."
       ::= { productStatus 5 }

productStatusGeneratingTrapsFlag OBJECT-TYPE
       SYNTAX      INTEGER { true(1),
                             false(2),
                             disabled(3)
                            }
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION "Indicates if this SNMP service is generating SNMP Traps.
                    This variable can take the following values:
                         1: true     - The device is capable and currently configured to generate traps if necessary.
                         2: false    - The device is not capable of generating traps.
                         3: disabled - The device is capable but not configured to generate traps.
                   "
       ::= { productStatus 6 }

productStatusEnvironment OBJECT IDENTIFIER ::= { productStatus  7}

envMonFanStatusTable OBJECT-TYPE
        SYNTAX     SEQUENCE OF EnvMonFanStatusEntry
        MAX-ACCESS not-accessible
        STATUS     current
        DESCRIPTION
                "The table of fan status maintained by the environmental
                monitor."
        ::= { productStatusEnvironment 1 }

envMonFanStatusEntry OBJECT-TYPE
        SYNTAX     EnvMonFanStatusEntry
        MAX-ACCESS not-accessible
        STATUS     current
        DESCRIPTION
                "An entry in the fan status table, representing the status of
                the associated fan maintained by the environmental monitor."
        INDEX   { envMonFanStatusIndex }
        ::= { envMonFanStatusTable 1 }

EnvMonFanStatusEntry ::=
        SEQUENCE {
                envMonFanStatusIndex       INTEGER,
                envMonFanStatusDescr       DisplayString,
                envMonFanState             EnvMonState
        }

envMonFanStatusIndex OBJECT-TYPE
        SYNTAX     INTEGER (1..2147483647)
        MAX-ACCESS read-only
        STATUS     current
        DESCRIPTION
                "Unique index for the fan being instrumented.
                This index is for SNMP purposes only, and has no
                intrinsic meaning."
        ::= { envMonFanStatusEntry 1 }

envMonFanStatusDescr OBJECT-TYPE
        SYNTAX     DisplayString (SIZE (0..32))
        MAX-ACCESS read-only

        STATUS     current
        DESCRIPTION
                "Textual description of the fan being instrumented.
                This description is a short textual label, suitable as a
                human-sensible identification for the rest of the
                information in the entry."
        ::= { envMonFanStatusEntry 2 }

envMonFanState OBJECT-TYPE
        SYNTAX     EnvMonState
        MAX-ACCESS read-only

        STATUS     current
        DESCRIPTION
                "The mandatory  state of the fan being instrumented."
        ::= { envMonFanStatusEntry 3 }



envMonSupplyStatusTable OBJECT-TYPE
        SYNTAX     SEQUENCE OF EnvMonSupplyStatusEntry
        MAX-ACCESS not-accessible

        STATUS     current
        DESCRIPTION
                "The table of power supply status maintained by the
                environmental monitor card."
        ::= { productStatusEnvironment 2 }

envMonSupplyStatusEntry OBJECT-TYPE
        SYNTAX     EnvMonSupplyStatusEntry
        MAX-ACCESS not-accessible

        STATUS     current
        DESCRIPTION
                "An entry in the power supply status table, representing the
                status of the associated power supply maintained by the
                environmental monitor card."
        INDEX   { envMonSupplyStatusIndex }
        ::= { envMonSupplyStatusTable 1  }

EnvMonSupplyStatusEntry ::=
        SEQUENCE {
                envMonSupplyStatusIndex    INTEGER ,
                envMonSupplyStatusDescr    DisplayString,
                envMonSupplyState          EnvMonState,
                envMonSupplySource         INTEGER
        }

envMonSupplyStatusIndex OBJECT-TYPE
        SYNTAX     INTEGER (0..2147483647)
        MAX-ACCESS read-only

        STATUS     current
        DESCRIPTION
                "Unique index for the power supply being instrumented.
                This index is for SNMP purposes only, and has no
                intrinsic meaning."
        ::= { envMonSupplyStatusEntry 1 }

envMonSupplyStatusDescr OBJECT-TYPE
        SYNTAX     DisplayString (SIZE (0..32))
        MAX-ACCESS read-only

        STATUS     current
        DESCRIPTION
                "Textual description of the power supply being instrumented.
                This description is a short textual label, suitable as a
                human-sensible identification for the rest of the
                information in the entry."
        ::= { envMonSupplyStatusEntry 2 }

envMonSupplyState OBJECT-TYPE
        SYNTAX     EnvMonState
        MAX-ACCESS read-only

        STATUS     current
        DESCRIPTION
                "The mandatory  state of the power supply being instrumented."
        ::= { envMonSupplyStatusEntry 3 }

envMonSupplySource OBJECT-TYPE
        SYNTAX INTEGER {
                        unknown(1),
                        ac(2),
                        dc(3),
                        externalPowerSupply(4),
                        internalRedundant(5)
                }
        MAX-ACCESS read-only

        STATUS     current
        DESCRIPTION
                "The power supply source.
                 unknown - Power supply source unknown
                 ac      - AC power supply
                 dc      - DC power supply
                 externalPowerSupply - External power supply
                 internalRedundant - Internal redundant power supply
                "
        ::= { envMonSupplyStatusEntry 4 }




--
-- trap definitions
--


    dell-VendorTraps  OBJECT IDENTIFIER ::= { dellVendorNotifications  1 }
    dell-VendorTrapsPrefix OBJECT IDENTIFIER ::= { dell-VendorTraps 0 }

    productStatusGlobalStatusChange NOTIFICATION-TYPE

        OBJECTS     { productStatusGlobalStatus, productStatusLastGlobalStatus, productStatusTimeStamp }
        STATUS      current
        DESCRIPTION "This trap is sent when the product global status changes."
        --#TYPE "Product Global Status Change."
        --#SUMMARY "The product global status has changed from %d to %d at time %d."
        --#ARGUMENTS {1,0,2}


   ::= {dell-VendorTrapsPrefix 1 }


END
