-- This module defines enterprise MIBs for nsrp
-- 
-- Copyright (c) 1999-2004, Juniper Networks, Inc.
-- All rights reserved.

NETSCREEN-NSRP-MIB DEFINITIONS ::= BEGIN

IMPORTS
    netscreenNsrp
        FROM NETSCREEN-SMI
    Counter32, Integer32, IpAddress, MODULE-IDENTITY, OBJECT-TYPE
        FROM SNMPv2-SMI
    DisplayString,PhysAddress
        FROM SNMPv2-TC
    ;

netscreenNsrpMibModule MODULE-IDENTITY
    LAST-UPDATED  "200405032022Z" -- May 03, 2004
    ORGANIZATION
        "Juniper Networks, Inc."
    CONTACT-INFO
        "Customer Support

         1194 North Mathilda Avenue 
         Sunnyvale, California 94089-1206
         USA

         Tel: 1-800-638-8296
         E-mail: customerservice@juniper.net
         HTTP://www.juniper.net"
    DESCRIPTION
        "This module defines the object that are200 used for netscreen
         redundancy protocol"
    REVISION      "200405030000Z" -- May 03, 2004
    DESCRIPTION
        "Modified copyright and contact information"
    REVISION      "200403030000Z" -- March 03, 2004
    DESCRIPTION
        "Converted to SMIv2 by Longview Software"
    REVISION      "200311140000Z" -- November 14, 2003
    DESCRIPTION
        "no comment"
    REVISION      "200306040000Z" -- June 04, 2003
    DESCRIPTION
        "no comment"
    REVISION      "200101080000Z" -- January 08, 2001
    DESCRIPTION
        "Creation Date"
    ::= { netscreenNsrp 0 }

NsRpRtoCounterEntry ::= SEQUENCE
{
    nsrpRtoCounterIdx     Integer32,
    nsrpRtoCounterName    DisplayString,
    nsrpRtoCounterSend    Counter32,
    nsrpRtoCounterReceive Counter32,
    nsrpRtoCounterDrop    Counter32
}

NsRpRtoGroupEntry ::= SEQUENCE
{
    nsrpRtoGroupId   Integer32,
    nsrpRtoNumOfUnit Integer32
}

NsRpRtoUnitEntry ::= SEQUENCE
{
    nsrpRtoUnitGroupId       Integer32,
    nsrpRtoUnitId            Integer32,
    nsrpRtoUnitStatus        INTEGER,
    nsrpRtoUnitDirection     INTEGER,
    nsrpRtoUnitLostHeartbeat Counter32,
    nsrpRtoUnitToActive      Counter32,
    nsrpRtoUnitToSet         Counter32,
    nsrpRtoUnitLostPeer      Counter32,
    nsrpRtoUnitGroupDetach   Counter32
}

NsRpTrackEntry ::= SEQUENCE
{
    nsrpTrackIpIndex            Integer32,
    nsrpTrackIpAddr             IpAddress,
    nsrpTrackIpStatus           INTEGER,
    nsrpTrackIpTimestamp        Integer32,
    nsrpTrackIpInterval         Integer32,
    nsrpTrackIpThreshhold       Integer32,
    nsrpTrackIpMethod           INTEGER,
    nsrpTrackIpWeight           Integer32,
    nsrpTrackIpIfName           DisplayString,
    nsrpTrackIpTotalCheck       Integer32,
    nsrpTrackIpTotalFailedCheck Integer32
}

NsRpVsdInterfaceEntry ::= SEQUENCE
{
    nsrpVsdIfIndex         Integer32,
    nsrpVsdIfStatus        INTEGER,
    nsrpVsdIfGroupId       Integer32,
    nsrpVsdIfIp            IpAddress,
    nsrpVsdIfNetmask       IpAddress,
    nsrpVsdIfGateway       IpAddress,
    nsrpVsdIfName          DisplayString,
    nsrpVsdIfVLAN          Integer32,
    nsrpVsdIfMAC           PhysAddress,
    nsrpVsdIfVSys          DisplayString,
    nsrpVsdIfMngTelnet     INTEGER,
    nsrpVsdIfMngSCS        INTEGER,
    nsrpVsdIfMngWEB        INTEGER,
    nsrpVsdIfMngSSL        INTEGER,
    nsrpVsdIfMngSNMP       INTEGER,
    nsrpVsdIfMngGlobal     INTEGER,
    nsrpVsdIfMngGlobalPro  INTEGER,
    nsrpVsdIfMngPing       INTEGER,
    nsrpVsdIfMngIdentReset INTEGER
}

NsrpClusterEntry ::= SEQUENCE
{
    nsrpClusterTblIndex    Integer32,
    nsrpClusterUnitId      Integer32,
    nsrpClusterUnitCtrlMac PhysAddress,
    nsrpClusterUnitDataMac PhysAddress
}

NsrpLinkInfoEntry ::= SEQUENCE
{
    nsrpLinkInfoIndex    Integer32,
    nsrpLinkInfoLinkType INTEGER,
    nsrpLinkInfoChannel  DisplayString,
    nsrpLinkInfoMac      PhysAddress,
    nsrpLinkInfoState    INTEGER
}

NsrpVsdGroupEntry ::= SEQUENCE
{
    nsrpVsdGroupID                Integer32,
    nsrpVsdGroupPriority          Integer32,
    nsrpVsdGroupPreempt           Integer32,
    nsrpVsdGroupHoldDownTime      Integer32,
    nsrpVsdGroupNumberOfUnit      Integer32,
    nsrpVsdGroupCntStateChange    Integer32,
    nsrpVsdGroupCntToInit         Integer32,
    nsrpVsdGroupCntToMaster       Integer32,
    nsrpVsdGroupCntToPBackup      Integer32,
    nsrpVsdGroupCntToBackup       Integer32,
    nsrpVsdGroupCntToIneligible   Integer32,
    nsrpVsdGroupCntToInoperable   Integer32,
    nsrpVsdGroupCntMasterConflict Integer32,
    nsrpVsdGroupCntPbConfilict    Integer32,
    nsrpVsdGroupCntHeartbeatTx    Integer32,
    nsrpVsdGroupCntHeartbeatRx    Integer32
}

NsrpVsdMemberEntry ::= SEQUENCE
{
    nsrpVsdMemberGroupId  Integer32,
    nsrpVsdMemberUnitId   Integer32,
    nsrpVsdMemberStatus   INTEGER,
    nsrpVsdMemberPriority Integer32,
    nsrpVsdMemberPreempt  Integer32
}

netscreenNsrpGeneral OBJECT IDENTIFIER ::= { netscreenNsrp 1 }

nsrpGeneralClusterId OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "The cluster ID"
    ::= { netscreenNsrpGeneral 1 }

nsrpGeneralLocalUnitId OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "local device's unit ID"
    ::= { netscreenNsrpGeneral 2 }

nsrpGeneralEncrypEnable OBJECT-TYPE
    SYNTAX        INTEGER {
        disabled(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "NSRP encryption enabled"
    ::= { netscreenNsrpGeneral 3 }

nsrpGeneralAuthEnable OBJECT-TYPE
    SYNTAX        INTEGER {
        disabled(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "NSRP authentication enabled"
    ::= { netscreenNsrpGeneral 4 }

nsrpGeneralIfMonitor OBJECT-TYPE
    SYNTAX        DisplayString (SIZE(0..64))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "interface being monitored"
    ::= { netscreenNsrpGeneral 5 }

nsrpGeneralGratArps OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "number of gratuitious arps"
    ::= { netscreenNsrpGeneral 6 }

netscreenNsrpVSD OBJECT IDENTIFIER ::= { netscreenNsrp 2 }

nsrpVsdGroupTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF NsrpVsdGroupEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "A list of VSD groups on the device."
    ::= { netscreenNsrpVSD 1 }

nsrpVsdGroupEntry OBJECT-TYPE
    SYNTAX        NsrpVsdGroupEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "An entry containing attributes for a track ip"
    INDEX
        { nsrpVsdGroupID }
    ::= { nsrpVsdGroupTable 1 }

nsrpVsdGroupID OBJECT-TYPE
    SYNTAX        Integer32 (0..2147483647)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "one group ID the device belongs to."
    ::= { nsrpVsdGroupEntry 1 }

nsrpVsdGroupPriority OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "local unit in current group's priority."
    ::= { nsrpVsdGroupEntry 2 }

nsrpVsdGroupPreempt OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "local unit in current group's preempt."
    ::= { nsrpVsdGroupEntry 3 }

nsrpVsdGroupHoldDownTime OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "TBD"
    ::= { nsrpVsdGroupEntry 4 }

nsrpVsdGroupNumberOfUnit OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "unit quantity in this group."
    ::= { nsrpVsdGroupEntry 5 }

nsrpVsdGroupCntStateChange OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "total number of state transition events"
    ::= { nsrpVsdGroupEntry 6 }

nsrpVsdGroupCntToInit OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "number of state transition into init state, which is as out of
         ineligible state`"
    ::= { nsrpVsdGroupEntry 7 }

nsrpVsdGroupCntToMaster OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "number of state transition into master state"
    ::= { nsrpVsdGroupEntry 8 }

nsrpVsdGroupCntToPBackup OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "number of state transition into primary backup state"
    ::= { nsrpVsdGroupEntry 9 }

nsrpVsdGroupCntToBackup OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "number of state transition into backup state."
    ::= { nsrpVsdGroupEntry 10 }

nsrpVsdGroupCntToIneligible OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "number of state transition into ineligible  state."
    ::= { nsrpVsdGroupEntry 11 }

nsrpVsdGroupCntToInoperable OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "number of state transition into inoperable  state."
    ::= { nsrpVsdGroupEntry 12 }

nsrpVsdGroupCntMasterConflict OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "number of times multiple masters exist while the local unit is
         in master state."
    ::= { nsrpVsdGroupEntry 13 }

nsrpVsdGroupCntPbConfilict OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "number of times multiple primary backups exist while the local
         unit is in primary backup state."
    ::= { nsrpVsdGroupEntry 14 }

nsrpVsdGroupCntHeartbeatTx OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "number of heart beat transfered by a group."
    ::= { nsrpVsdGroupEntry 15 }

nsrpVsdGroupCntHeartbeatRx OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "number of heart beat received by a group."
    ::= { nsrpVsdGroupEntry 16 }

nsrpVsdMemberTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF NsrpVsdMemberEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "A list of devices within the VSD group."
    ::= { netscreenNsrpVSD 2 }

nsrpVsdMemberEntry OBJECT-TYPE
    SYNTAX        NsrpVsdMemberEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "A entry containing attributes of one device in a group"
    INDEX
        { nsrpVsdMemberGroupId, nsrpVsdMemberUnitId }
    ::= { nsrpVsdMemberTable 1 }

nsrpVsdMemberGroupId OBJECT-TYPE
    SYNTAX        Integer32 (0..2147483647)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "indicate the Group it belong to"
    ::= { nsrpVsdMemberEntry 1 }

nsrpVsdMemberUnitId OBJECT-TYPE
    SYNTAX        Integer32 (0..2147483647)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "VSD group member's unit id"
    ::= { nsrpVsdMemberEntry 2 }

nsrpVsdMemberStatus OBJECT-TYPE
    SYNTAX        INTEGER {
        undefined(0),
        init(1),
        master(2),
        primary-backup(3),
        backup(4),
        ineligible(5),
        inoperable(6)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "0 Undefined
         1 init
         2 Master
         3 Primary Backup
         4 Backup
         5 ineligible
         6 inoperable"
    ::= { nsrpVsdMemberEntry 3 }

nsrpVsdMemberPriority OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Priority of unit in this group"
    ::= { nsrpVsdMemberEntry 4 }

nsrpVsdMemberPreempt OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "unit in current group's preempt"
    ::= { nsrpVsdMemberEntry 5 }

nsrpVsdInterfaceTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF NsRpVsdInterfaceEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "A list of VSD interfaces on the device."
    ::= { netscreenNsrpVSD 3 }

nsrpVsdInterfaceEntry OBJECT-TYPE
    SYNTAX        NsRpVsdInterfaceEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "A track entry containing attributes for a track ip"
    INDEX
        { nsrpVsdIfIndex }
    ::= { nsrpVsdInterfaceTable 1 }

nsrpVsdIfIndex OBJECT-TYPE
    SYNTAX        Integer32 (0..2147483647)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "A index."
    ::= { nsrpVsdInterfaceEntry 1 }

nsrpVsdIfStatus OBJECT-TYPE
    SYNTAX        INTEGER {
        down(0),
        inactive(1),
        active(2)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "indicate the status of this vsi interface"
    ::= { nsrpVsdInterfaceEntry 2 }

nsrpVsdIfGroupId OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "indicate the group it belong to"
    ::= { nsrpVsdInterfaceEntry 3 }

nsrpVsdIfIp OBJECT-TYPE
    SYNTAX        IpAddress
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "ip ADDRESS"
    ::= { nsrpVsdInterfaceEntry 4 }

nsrpVsdIfNetmask OBJECT-TYPE
    SYNTAX        IpAddress
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "subnet mask"
    ::= { nsrpVsdInterfaceEntry 5 }

nsrpVsdIfGateway OBJECT-TYPE
    SYNTAX        IpAddress
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "gateway"
    ::= { nsrpVsdInterfaceEntry 6 }

nsrpVsdIfName OBJECT-TYPE
    SYNTAX        DisplayString (SIZE(0..32))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "trust/untrust/DMZ"
    ::= { nsrpVsdInterfaceEntry 7 }

nsrpVsdIfVLAN OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "vlan -1 means no vlan"
    ::= { nsrpVsdInterfaceEntry 8 }

nsrpVsdIfMAC OBJECT-TYPE
    SYNTAX        PhysAddress
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "mac address"
    ::= { nsrpVsdInterfaceEntry 9 }

nsrpVsdIfVSys OBJECT-TYPE
    SYNTAX        DisplayString (SIZE(0..32))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "virtual system"
    ::= { nsrpVsdInterfaceEntry 10 }

nsrpVsdIfMngTelnet OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enable(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "0 Disable
         1 Enable"
    ::= { nsrpVsdInterfaceEntry 11 }

nsrpVsdIfMngSCS OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enable(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "0 Disable
         1 Enable"
    ::= { nsrpVsdInterfaceEntry 12 }

nsrpVsdIfMngWEB OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enable(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "0 Disable
         1 Enable"
    ::= { nsrpVsdInterfaceEntry 13 }

nsrpVsdIfMngSSL OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enable(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "0 Disable
         1 Enable"
    ::= { nsrpVsdInterfaceEntry 14 }

nsrpVsdIfMngSNMP OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enable(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "0 Disable
         1 Enable"
    ::= { nsrpVsdInterfaceEntry 15 }

nsrpVsdIfMngGlobal OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enable(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "0 Disable
         1 Enable"
    ::= { nsrpVsdInterfaceEntry 16 }

nsrpVsdIfMngGlobalPro OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enable(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "0 Disable
         1 Enable"
    ::= { nsrpVsdInterfaceEntry 17 }

nsrpVsdIfMngPing OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enable(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "0 Disable
         1 Enable"
    ::= { nsrpVsdInterfaceEntry 18 }

nsrpVsdIfMngIdentReset OBJECT-TYPE
    SYNTAX        INTEGER {
        disable(0),
        enable(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "0 Disable
         1 Enable"
    ::= { nsrpVsdInterfaceEntry 19 }

nsrpVsdGeneral OBJECT IDENTIFIER ::= { netscreenNsrpVSD 4 }

nsrpVsdGeneralInitHoldTime OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "VSD group init hold time (in second)"
    ::= { nsrpVsdGeneral 1 }

nsrpVsdGeneralHbInterval OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "VSD heart beat interval.(in milisecond)"
    ::= { nsrpVsdGeneral 2 }

nsrpVsdGeneralHbLostThres OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "vsd heartbeat lost threshold"
    ::= { nsrpVsdGeneral 3 }

netscreenNsrpRTO OBJECT IDENTIFIER ::= { netscreenNsrp 3 }

nsrpRtoGroupTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF NsRpRtoGroupEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "A list of RTO groups on the device."
    ::= { netscreenNsrpRTO 1 }

nsrpRtoGroupEntry OBJECT-TYPE
    SYNTAX        NsRpRtoGroupEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "An entry containing attributes for RTO group"
    INDEX
        { nsrpRtoGroupId }
    ::= { nsrpRtoGroupTable 1 }

nsrpRtoGroupId OBJECT-TYPE
    SYNTAX        Integer32 (0..2147483647)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "A RTO group ID.also used as table index"
    ::= { nsrpRtoGroupEntry 1 }

nsrpRtoNumOfUnit OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "how many units in this RTO group"
    ::= { nsrpRtoGroupEntry 2 }

nsrpRtoUnitTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF NsRpRtoUnitEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "A list of device status within a RTO group."
    ::= { netscreenNsrpRTO 2 }

nsrpRtoUnitEntry OBJECT-TYPE
    SYNTAX        NsRpRtoUnitEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "A track entry containing attributes for a track ip"
    INDEX
        { nsrpRtoUnitGroupId, nsrpRtoUnitId }
    ::= { nsrpRtoUnitTable 1 }

nsrpRtoUnitGroupId OBJECT-TYPE
    SYNTAX        Integer32 (0..2147483647)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "The RTO group id, a unit belongs to"
    ::= { nsrpRtoUnitEntry 1 }

nsrpRtoUnitId OBJECT-TYPE
    SYNTAX        Integer32 (0..2147483647)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "device's unit id."
    ::= { nsrpRtoUnitEntry 2 }

nsrpRtoUnitStatus OBJECT-TYPE
    SYNTAX        INTEGER {
        undefined(0),
        set(1),
        active(2)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "The RTO group id, a unit belongs to"
    ::= { nsrpRtoUnitEntry 3 }

nsrpRtoUnitDirection OBJECT-TYPE
    SYNTAX        INTEGER {
        out(1),
        in(2)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "The RTO uint's dirction in the group"
    ::= { nsrpRtoUnitEntry 4 }

nsrpRtoUnitLostHeartbeat OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "counter of heartbeat"
    ::= { nsrpRtoUnitEntry 5 }

nsrpRtoUnitToActive OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "counter of active"
    ::= { nsrpRtoUnitEntry 6 }

nsrpRtoUnitToSet OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "counter of set"
    ::= { nsrpRtoUnitEntry 7 }

nsrpRtoUnitLostPeer OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "counter of lost peer"
    ::= { nsrpRtoUnitEntry 8 }

nsrpRtoUnitGroupDetach OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "counter of rto group detach"
    ::= { nsrpRtoUnitEntry 9 }

nsrpRtoCounter OBJECT IDENTIFIER ::= { netscreenNsrpRTO 3 }

nsrpRtoCounterPakForwarded OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "packets forwarded by rto."
    ::= { nsrpRtoCounter 1 }

nsrpRtoCounterPakReceived OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "packets received by rto."
    ::= { nsrpRtoCounter 2 }

nsrpRtoCounterTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF NsRpRtoCounterEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "A list of rto counter object entry."
    ::= { nsrpRtoCounter 3 }

nsrpRtoCounterEntry OBJECT-TYPE
    SYNTAX        NsRpRtoCounterEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "A rto counter entry containing attributes for a rto counter
         obj."
    INDEX
        { nsrpRtoCounterIdx }
    ::= { nsrpRtoCounterTable 1 }

nsrpRtoCounterIdx OBJECT-TYPE
    SYNTAX        Integer32 (0..2147483647)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "counter index."
    ::= { nsrpRtoCounterEntry 1 }

nsrpRtoCounterName OBJECT-TYPE
    SYNTAX        DisplayString (SIZE(0..32))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Name of a rto counter object."
    ::= { nsrpRtoCounterEntry 2 }

nsrpRtoCounterSend OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Total number of message sent."
    ::= { nsrpRtoCounterEntry 3 }

nsrpRtoCounterReceive OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Total number of message received."
    ::= { nsrpRtoCounterEntry 4 }

nsrpRtoCounterDrop OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Total number of message dropped."
    ::= { nsrpRtoCounterEntry 5 }

nsrpRtoGeneral OBJECT IDENTIFIER ::= { netscreenNsrpRTO 4 }

nsrpRtoGeneralHbInterval OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "rto heart beat interval."
    ::= { nsrpRtoGeneral 1 }

nsrpRtoGeneralHbLostThres OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "rto heartbeat lost threshold"
    ::= { nsrpRtoGeneral 2 }

nsrpRtoGeneralSessSyncEnable OBJECT-TYPE
    SYNTAX        INTEGER {
        disabled(0),
        enabled(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "session sync enabled."
    ::= { nsrpRtoGeneral 3 }

netscreenNsrpTrack OBJECT IDENTIFIER ::= { netscreenNsrp 4 }

nsrpTrackEnable OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "0 means disable, 1 meams enable"
    ::= { netscreenNsrpTrack 1 }

nsrpTrackThreshold OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Failover Threshold"
    ::= { netscreenNsrpTrack 2 }

nsrpTrackFailoverEnalble OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Failover enable switch"
    ::= { netscreenNsrpTrack 3 }

nsrpTrackTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF NsRpTrackEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "A list of track ip entries."
    ::= { netscreenNsrpTrack 4 }

nsrpTrackEntry OBJECT-TYPE
    SYNTAX        NsRpTrackEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "A track entry containing attributes for a track ip"
    INDEX
        { nsrpTrackIpIndex }
    ::= { nsrpTrackTable 1 }

nsrpTrackIpIndex OBJECT-TYPE
    SYNTAX        Integer32 (0..2147483647)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "A unique value for each track ip.  Its value ranges between 1
         and 65535 and may not be contigous.  It has no other meaning
         but a pure index."
    ::= { nsrpTrackEntry 1 }

nsrpTrackIpAddr OBJECT-TYPE
    SYNTAX        IpAddress
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "The IP address of the monitored device."
    ::= { nsrpTrackEntry 2 }

nsrpTrackIpStatus OBJECT-TYPE
    SYNTAX        INTEGER {
        success(0),
        fail(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Status"
    ::= { nsrpTrackEntry 3 }

nsrpTrackIpTimestamp OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Timestamp of status change. Reference 1970/1/1 0:0"
    ::= { nsrpTrackEntry 4 }

nsrpTrackIpInterval OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "A frequecy how the track ip is checked. It is in unit of
         seconds."
    ::= { nsrpTrackEntry 5 }

nsrpTrackIpThreshhold OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "A number of consective failures to regard the device has
         failed."
    ::= { nsrpTrackEntry 6 }

nsrpTrackIpMethod OBJECT-TYPE
    SYNTAX        INTEGER {
        ping(0),
        arp(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "The method to track the device."
    ::= { nsrpTrackEntry 7 }

nsrpTrackIpWeight OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "The weight of this failure contributing to the failover."
    ::= { nsrpTrackEntry 8 }

nsrpTrackIpIfName OBJECT-TYPE
    SYNTAX        DisplayString (SIZE(0..32))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "The interface the track messages are sent to. Auto means the
         actual interface is determined by the routing table."
    ::= { nsrpTrackEntry 9 }

nsrpTrackIpTotalCheck OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "The number of ping/arp attempts."
    ::= { nsrpTrackEntry 10 }

nsrpTrackIpTotalFailedCheck OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "The number of total failed attempts."
    ::= { nsrpTrackEntry 11 }

netscreenNsrpCluster OBJECT IDENTIFIER ::= { netscreenNsrp 5 }

nsrpClusterTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF NsrpClusterEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "A list of cluster on the device."
    ::= { netscreenNsrpCluster 1 }

nsrpClusterEntry OBJECT-TYPE
    SYNTAX        NsrpClusterEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "An entry containing attributes for nsrp cluster"
    INDEX
        { nsrpClusterTblIndex }
    ::= { nsrpClusterTable 1 }

nsrpClusterTblIndex OBJECT-TYPE
    SYNTAX        Integer32 (0..2147483647)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "table index"
    ::= { nsrpClusterEntry 1 }

nsrpClusterUnitId OBJECT-TYPE
    SYNTAX        Integer32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Unit id in this cluster"
    ::= { nsrpClusterEntry 2 }

nsrpClusterUnitCtrlMac OBJECT-TYPE
    SYNTAX        PhysAddress
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Unit id's control path mac address"
    ::= { nsrpClusterEntry 3 }

nsrpClusterUnitDataMac OBJECT-TYPE
    SYNTAX        PhysAddress
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Unit id's data path mac address"
    ::= { nsrpClusterEntry 4 }

netscreenNsrpLinkInfo OBJECT IDENTIFIER ::= { netscreenNsrp 6 }

nsrpLinkInfoTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF NsrpLinkInfoEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "A list of NSRP link info"
    ::= { netscreenNsrpLinkInfo 1 }

nsrpLinkInfoEntry OBJECT-TYPE
    SYNTAX        NsrpLinkInfoEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "An entry containing attributes for nsrp link info"
    INDEX
        { nsrpLinkInfoIndex }
    ::= { nsrpLinkInfoTable 1 }

nsrpLinkInfoIndex OBJECT-TYPE
    SYNTAX        Integer32 (0..2147483647)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "table index"
    ::= { nsrpLinkInfoEntry 1 }

nsrpLinkInfoLinkType OBJECT-TYPE
    SYNTAX        INTEGER {
        control(0),
        data(1),
        unused(2),
        hapath2(3)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "link type"
    ::= { nsrpLinkInfoEntry 2 }

nsrpLinkInfoChannel OBJECT-TYPE
    SYNTAX        DisplayString (SIZE(0..32))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "link channel's name"
    ::= { nsrpLinkInfoEntry 3 }

nsrpLinkInfoMac OBJECT-TYPE
    SYNTAX        PhysAddress
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "link channel's mac address"
    ::= { nsrpLinkInfoEntry 4 }

nsrpLinkInfoState OBJECT-TYPE
    SYNTAX        INTEGER {
        down(0),
        up(1)
    }
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "link channel's state"
    ::= { nsrpLinkInfoEntry 5 }

END


