
-- *****************************************************************************
-- Juniper-IP-PROFILE-MIB
--
-- Juniper Networks Enterprise MIB
--   IP Profile MIB
--
-- Copyright (c) 1999 Redstone Communications, Inc.
-- Copyright (c) 2000, 2001 Unisphere Networks, Inc.
-- Copyright (c) 2002 Juniper Networks, Inc.
--   All Rights Reserved.
-- *****************************************************************************

Juniper-IP-PROFILE-MIB  DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Integer32, Unsigned32, IpAddress
        FROM SNMPv2-SMI
    DisplayString, RowStatus
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF
    InterfaceIndexOrZero
        FROM IF-MIB
    juniMibs
        FROM Juniper-MIBs
    JuniEnable, JuniName, JuniSetMap
        FROM Juniper-TC;

juniIpProfileMIB  MODULE-IDENTITY
    LAST-UPDATED "200609081026Z"  -- 08-Sep-06 03:56 PM EST
    ORGANIZATION "Juniper Networks"
    CONTACT-INFO
        "       Juniper Networks, Inc.
        Postal: 10 Technology Park Drive
                Westford MA  01886-3146
                USA
        Tel:    +1 978 589 5800
        Email:  mib@Juniper.net"
    DESCRIPTION
        "The IP Profile MIB for the Juniper Networks enterprise."
    -- Revision History
    REVISION    "200609081026Z"  -- 08-Sep-06 03:56 PM EST  - JUNOSe 8.1 
    DESCRIPTION
        "Added support for Blocking multicast sources on IP Interfaces -
        juniIpProfileBlockMulticastSources."
    REVISION    "200509131721Z"  -- 13-Sep-05 01:21 PM EDT  - JUNOSe 7.2
    DESCRIPTION
        "Added support for Flow Stats a.k.a. J-Flow for IP Interfaces by 
        including juniIpProfileFlowStats."
    REVISION    "200410051404Z"  -- 05-Oct-04 10:04 AM EDT  - JUNOSe 7.0
    DESCRIPTION
        "Added support for IP filter options all for IP Interfaces by 
        including juniIpProfileFilterOptionsAll."
    REVISION    "200309241533Z"  -- 24-Sep-03 11:33 AM EDT  - JUNOSe 5.2
    DESCRIPTION
        "Added support for TCP MSS configuration for IP interfaces by 
        including juniIpProfileTcpMss."
    REVISION    "200210111320Z"  -- 11-Oct-02 09:20 AM EDT  - JUNOSe 5.0
    DESCRIPTION
        "Replaced Unisphere names with Juniper names.
        In juniIpProfileTable, to support unnumbered interfaces referencing
        numbered interfaces in addition to loopback interfaces, the
        following object is made obsolete:
          juniIpProfileLoopback
        and the following object is added:
          juniIpProfileInheritNumString"
    REVISION    "200101242006Z"  -- 24-Jan-01 03:06 PM EST  - JUNOSe 3.0
    DESCRIPTION
        "Deprecated juniIpProfileRowStatus; the table is now dense and populated
        as a side-effect of creation of an entry in the juniProfileNameTable in
        Juniper-PROFILE-MIB.  Also, added juniIpProfileSetMap and
        juniIpProfileSrcAddrValidEnable."
    REVISION    "200005080000Z"  --  8-May-00               - JUNOSe 2.0
    DESCRIPTION
        "Obsoleted juniIpProfileLoopbackIfIndex, replacing it with
        juniIpProfileLoopback."
    REVISION      "9908250000Z"  -- 25-Aug-99               - JUNOSe 1.1
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { juniMibs 26 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Managed object groups
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniIpProfileObjects  OBJECT IDENTIFIER ::= {juniIpProfileMIB 1}
juniIpProfile         OBJECT IDENTIFIER ::= {juniIpProfileObjects 1 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Managed objects for IP Profiles
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
--
-- This MIB defines configuration profile structure for IP interfaces.
-- The creation/deletion of profiles and mapping of profile names to profile
-- indices is coordinated in the Juniper-PROFILE-MIB.
--
--
-- The IP Profile Table
--
juniIpProfileTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIpProfileEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The entries in this table describe profiles for configuring IP
        interfaces.

        Entries in this table are created/deleted as a side-effect of
        corresponding operations to the juniProfileNameTable in the
        Juniper-PROFILE-MIB."
    ::= { juniIpProfile 1 }

juniIpProfileEntry OBJECT-TYPE
    SYNTAX      JuniIpProfileEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A profile describing configuration of an IP interface."
    INDEX     { juniIpProfileId }
    ::= { juniIpProfileTable 1 }

JuniIpProfileEntry ::= SEQUENCE {
    juniIpProfileId                  Unsigned32,
    juniIpProfileRowStatus           RowStatus,
    juniIpProfileRouterName          JuniName,
    juniIpProfileIpAddr              IpAddress,
    juniIpProfileIpMask              IpAddress,
    juniIpProfileDirectedBcastEnable JuniEnable,
    juniIpProfileIcmpRedirectEnable  JuniEnable,
    juniIpProfileAccessRoute         JuniEnable,
    juniIpProfileMtu                 Integer32,
    juniIpProfileLoopbackIfIndex     InterfaceIndexOrZero,
    juniIpProfileLoopback            Integer32,
    juniIpProfileSetMap              JuniSetMap,
    juniIpProfileSrcAddrValidEnable  JuniEnable,
    juniIpProfileInheritNumString    DisplayString,
    juniIpProfileTcpMss              Integer32,
    juniIpProfileFilterOptionsAll    JuniEnable, 
    juniIpProfileFlowStats           JuniEnable,
    juniIpProfileBlockMulticastSources JuniEnable }

juniIpProfileId OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The integer identifier associated with this profile.  A value for this
        identifier is determined by locating or creating a profile name in the
        juniProfileNameTable."
    ::= { juniIpProfileEntry 1 }

juniIpProfileRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      deprecated
    DESCRIPTION
        "Controls creation/deletion of entries in this table.  Only the values
        'createAndGo' and 'destroy' may be SET.

        The value of juniIpProfileId must match that of a profile name
        configured in juniProfileNameTable."
    ::= { juniIpProfileEntry 2 }

juniIpProfileRouterName OBJECT-TYPE
    SYNTAX      JuniName
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The virtual router to which an IP interface configured by this profile
        will be assigned, if other mechanisms do not otherwise specify a virtual
        router assignment."
    DEFVAL    { "" }
    ::= { juniIpProfileEntry 3 }

juniIpProfileIpAddr OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "An IP address to be used by an IP interface configured by this profile.
        This object will have a value of 0.0.0.0 for an unnumbered interface."
    DEFVAL    { 0 }
    ::= { juniIpProfileEntry 4 }

juniIpProfileIpMask OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "An IP address mask to be used by an IP interface configured by this
        profile.  This object will have a value of 0.0.0.0 for an unnumbered
        interface."
    DEFVAL    { 0 }
    ::= { juniIpProfileEntry 5 }

juniIpProfileDirectedBcastEnable OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enable/disable forwarding of directed broadcasts on this IP network
        interface."
    DEFVAL    { disable }
    ::= { juniIpProfileEntry 6 }

juniIpProfileIcmpRedirectEnable OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enable/disable transmission of ICMP Redirect messages on this IP
        network interface."
    DEFVAL    { disable }
    ::= { juniIpProfileEntry 7 }

juniIpProfileAccessRoute OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enable/disable whether a host route is automatically created for a
        remote host attached to an IP interface that is configured using this
        profile."
    DEFVAL    { enable }
    ::= { juniIpProfileEntry 8 }

juniIpProfileMtu OBJECT-TYPE
    SYNTAX      Integer32 (0|512..10240)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The configured MTU size for this IP network interface.  If set to zero,
        the default MTU size, as determined by the underlying network media, is
        used."
    DEFVAL    { 0 }
    ::= { juniIpProfileEntry 9 }

juniIpProfileLoopbackIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "For unnumbered interfaces, the IfIndex of the IP loopback interface
        whose IP address is used as the source address for transmitted IP
        packets.  A value of zero means the loopback interface is unspecified
        (e.g., when the interface is numbered)."
    DEFVAL    { 0 }
    ::= { juniIpProfileEntry 10 }

juniIpProfileLoopback OBJECT-TYPE
    SYNTAX      Integer32 (-1..2147483647)
    MAX-ACCESS  read-create
    STATUS      obsolete
    DESCRIPTION
        "The number of the loopback interface, associated with the specified
        virtual router, whose IP address is used as the source address when
        transmitting IP packets on unnumbered remote access user links.

        For example, if the loopback interface for the associated router was
        configured via the console as 'loopback 2', this object would contain
        the integer value 2.

        A value of -1 indicates the loopback interface is unspecified, e.g.,
        when the IP interface is numbered.

        This object has been replaced by juniIpProfileInheritNumString.
        This object is no longer represented in the juniIpProfileSetMap."
    DEFVAL    { -1 }
    ::= { juniIpProfileEntry 11 }

juniIpProfileSetMap OBJECT-TYPE
    SYNTAX      JuniSetMap
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "A bitmap representing which objects in this entry have been explicitly
        configured.  See the definition of the JuniSetMap TEXTUAL-CONVENTION for
        details of use.

        The INDEX object(s) and this object are excluded from representation
        (i.e. their bits are never set).

        When a SET request does not explicitly configure JuniSetMap, bits in
        JuniSetMap are set as a side-effect of configuring other profile
        attributes in the same entry.

        If, however, a SET request explicitly configures JuniSetMap, the
        explicitly configured value overrides 1) any previous bit settings, and
        2) any simultaneous 'side-effect' settings that would otherwise occur.

        Once set, bits can only be cleared by explicitly configuring
        JuniSetMap."
    ::= { juniIpProfileEntry 12 }

juniIpProfileSrcAddrValidEnable OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enable/disable whether source addresses in received IP packets are
        validated. Validation is performed by looking up the source IP address
        in the routing database and determining whether the packet arrived on
        the expected interface; if not, the packet is discarded."
    DEFVAL    { disable }
    ::= { juniIpProfileEntry 13 }

juniIpProfileInheritNumString OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..80))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The text identifier of the numbered interface, associated with the
        specified virtual router, whose IP address is used as the source address
        when transmitting IP packets on unnumbered remote access user links.
        Types/formats/examples for this string include:

            Loopback
            loopback <id>
            'loopback 0'

            ATM Virtual Circuit
            atm <slot>/<port>.<distinguisher>
            'atm 3/1.100'

            Ethernet
            { fastEthernet | gigabitEthernet } <slot>/<port>
            'fastEthernet 3/0'
            'gigabitEthernet 3/0'

            Ethernet VLAN
            { fastEthernet | gigabitEthernet } <slot>/<port>:<vlanID>
            'fastEthernet 3/0:1000'
            'gigabitEthernet 3/0:1000'

            Channelized Serial
            serial <slot>/<port>:<channelSpecifier>[/<channelSpecifier>]*
            'serial 3/0:4'            (T1/E1)
            'serial 3/0:2/4'          (T3/E3)
            'serial 3/0:2/1/1/4'      (OC3/OC12 - channelized DS3)
            'serial 3/0:2/1/1/1/4'    (OC3/OC12 - virtual tributaries)

        Other formats may be supported over time.

        An empty string indicates the referenced interface is unspecified, e.g.,
        when this IP interface is numbered."
    DEFVAL    { "" }
    ::= { juniIpProfileEntry 14 }

juniIpProfileTcpMss OBJECT-TYPE
    SYNTAX      Integer32 (0|160..10240)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Configures TCP MSS value for an IP interface.  When configured, 
        MSS value of TCP SYN packets received or transmitted on the 
        interface will be compared with the configured value and lowest 
        of the two will replace the value in the packet."
    DEFVAL    { 0 }
    ::= { juniIpProfileEntry 15 }

juniIpProfileFilterOptionsAll OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enable/disable whether IP packets containing options are to be discarded or sent
         to the control plane for processing."
    DEFVAL    { disable }
    ::= { juniIpProfileEntry 16 }

juniIpProfileFlowStats OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enable/disable whether J-Flow is enabled on the interface"
    DEFVAL    { disable }
    ::= { juniIpProfileEntry 17 }

juniIpProfileBlockMulticastSources OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enable/disable Blocking Multicast traffic"
    DEFVAL    { disable }
    ::= { juniIpProfileEntry 18 }

-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Notifications
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- No notifications are defined in this MIB.  Placeholders follow.
-- juniIpProfileTrapControl      OBJECT IDENTIFIER ::= { juniIpProfileMIB 2 }
-- juniIpProfileTraps            OBJECT IDENTIFIER ::= { juniIpProfileMIB 3 }
-- juniIpProfileTrapPrefix       OBJECT IDENTIFIER ::= { juniIpProfileTraps 0 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Conformance information
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniIpProfileMIBConformance
             OBJECT IDENTIFIER ::= { juniIpProfileMIB 4 }
juniIpProfileMIBCompliances
             OBJECT IDENTIFIER ::= { juniIpProfileMIBConformance 1 }
juniIpProfileMIBGroups
             OBJECT IDENTIFIER ::= { juniIpProfileMIBConformance 2 }


--
-- compliance statements
--
juniIpProfileCompliance  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for systems supporting IP configuration
        profiles.  This statement became obsolete when juniIpProfileLoopback
        replaced juniIpProfileLoopbackIfIndex."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpProfileGroup }
    ::= { juniIpProfileMIBCompliances 1 }                          -- JUNOSe 1.1

juniIpProfileCompliance1  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for systems supporting IP configuration
        profiles.  This statement became obsolete when juniIpProfileRowStatus
        was deprecate and the juniIpProfileSetMap and
        juniIpProfileSrcAddrValidEnable objects were added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpProfileGroup1 }
    ::= { juniIpProfileMIBCompliances 2 }                          -- JUNOSe 2.0

juniIpProfileCompliance2  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for systems supporting IP configuration
        profiles.  This statement became obsolete when juniIpProfileLoopback was
        obsoleted and the juniIpProfileInheritNumString object was added."
    MODULE  -- this module
        MANDATORY-GROUPS {
            juniIpProfileGroup2 }
    ::= { juniIpProfileMIBCompliances 3 }                          -- JUNOSe 3.0

juniIpProfileCompliance3  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for systems supporting IP configuration
        profiles.  This statement became obsolete when juniIpProfileTcpMss was
        added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpProfileGroup3 }
    ::= { juniIpProfileMIBCompliances 4 }                          -- JUNOSe 5.0

juniIpProfileCompliance4  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for systems supporting IP configuration
        profiles.  This statement became obsolete when juniIpProfileFilterOptionsAll
        was added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpProfileGroup4 }
    ::= { juniIpProfileMIBCompliances 5 }                          -- JUNOSe 5.2

juniIpProfileCompliance5  MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for systems supporting IP configuration
        profiles, incorporating juniIpProfileFilterOptionsAll."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpProfileGroup5 }
    ::= { juniIpProfileMIBCompliances 6 }                          -- JUNOSe 7.0

juniIpProfileCompliance6  MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for systems supporting IP configuration
        profiles, incorporating juniIpProfileFlowStats."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpProfileGroup6 }
    ::= { juniIpProfileMIBCompliances 7 }                          -- JUNOSe 7.2

juniIpProfileCompliance7  MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for systems supporting IP configuration
        profiles, incorporating juniIpProfileBlockMulticastSources."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpProfileGroup7 }
    ::= { juniIpProfileMIBCompliances 8 }                          -- JUNOSe 8.1
--
-- units of conformance
--
juniIpProfileGroup  OBJECT-GROUP
    OBJECTS {
        juniIpProfileRowStatus,
        juniIpProfileRouterName,
        juniIpProfileIpAddr,
        juniIpProfileIpMask,
        juniIpProfileDirectedBcastEnable,
        juniIpProfileIcmpRedirectEnable,
        juniIpProfileAccessRoute,
        juniIpProfileMtu,
        juniIpProfileLoopbackIfIndex }
    STATUS      obsolete
    DESCRIPTION
        "An obsolete collection of objects providing management of IP Profile
        functionality in a Juniper product.  This group became obsolete when
        juniIpProfileLoopback replaced juniIpProfileLoopbackIfIndex."
    ::= { juniIpProfileMIBGroups 1 }

juniIpProfileGroup1  OBJECT-GROUP
    OBJECTS {
        juniIpProfileRowStatus,
        juniIpProfileRouterName,
        juniIpProfileIpAddr,
        juniIpProfileIpMask,
        juniIpProfileDirectedBcastEnable,
        juniIpProfileIcmpRedirectEnable,
        juniIpProfileAccessRoute,
        juniIpProfileMtu,
        juniIpProfileLoopback }
    STATUS      obsolete
    DESCRIPTION
        "An obsolete collection of objects providing management of IP Profile
        functionality in a Juniper product.  This group became obsolete when
        juniIpProfileRowStatus was deprecate and the juniIpProfileSetMap and
        juniIpProfileSrcAddrValidEnable objects were added."
    ::= { juniIpProfileMIBGroups 2 }

juniIpProfileGroup2  OBJECT-GROUP
    OBJECTS {
        juniIpProfileRouterName,
        juniIpProfileIpAddr,
        juniIpProfileIpMask,
        juniIpProfileDirectedBcastEnable,
        juniIpProfileIcmpRedirectEnable,
        juniIpProfileAccessRoute,
        juniIpProfileMtu,
        juniIpProfileLoopback,
        juniIpProfileSetMap,
        juniIpProfileSrcAddrValidEnable }
    STATUS      obsolete
    DESCRIPTION
        "An obsolete collection of objects providing management of IP Profile
        functionality in a Juniper product.  This statement became obsolete
        when juniIpProfileLoopback was obsoleted and the
        juniIpProfileInheritNumString object was added."
    ::= { juniIpProfileMIBGroups 3 }

juniIpProfileDeprecatedGroup  OBJECT-GROUP
    OBJECTS {
        juniIpProfileRowStatus }
    STATUS      deprecated
    DESCRIPTION
        "Deprecated object providing management of IP Profile functionality in a
        Juniper product.  This group has been deprecated but may still be
        supported on some implementations."
    ::= { juniIpProfileMIBGroups 4 }

juniIpProfileGroup3  OBJECT-GROUP
    OBJECTS {
        juniIpProfileRouterName,
        juniIpProfileIpAddr,
        juniIpProfileIpMask,
        juniIpProfileDirectedBcastEnable,
        juniIpProfileIcmpRedirectEnable,
        juniIpProfileAccessRoute,
        juniIpProfileMtu,
        juniIpProfileSetMap,
        juniIpProfileSrcAddrValidEnable,
        juniIpProfileInheritNumString }
    STATUS      obsolete
    DESCRIPTION
        "An obsolete collection of objects providing management of IP Profile
        functionality in a Juniper product.  This statement became obsolete
        when juniIpProfileTcpMss was added."
    ::= { juniIpProfileMIBGroups 5 }

juniIpProfileGroup4  OBJECT-GROUP
    OBJECTS {
        juniIpProfileRouterName,
        juniIpProfileIpAddr,
        juniIpProfileIpMask,
        juniIpProfileDirectedBcastEnable,
        juniIpProfileIcmpRedirectEnable,
        juniIpProfileAccessRoute,
        juniIpProfileMtu,
        juniIpProfileSetMap,
        juniIpProfileSrcAddrValidEnable,
        juniIpProfileInheritNumString,
        juniIpProfileTcpMss }
    STATUS      obsolete
    DESCRIPTION
        "An obsolete collection of objects providing management of IP Profile
        functionality in a Juniper product. This statement became osolete
        when juniIpProfileFilterOptionsAll was added."
    ::= { juniIpProfileMIBGroups 6 }

juniIpProfileGroup5  OBJECT-GROUP
    OBJECTS {
        juniIpProfileRouterName,
        juniIpProfileIpAddr,
        juniIpProfileIpMask,
        juniIpProfileDirectedBcastEnable,
        juniIpProfileIcmpRedirectEnable,
        juniIpProfileAccessRoute,
        juniIpProfileMtu,
        juniIpProfileSetMap,
        juniIpProfileSrcAddrValidEnable,
        juniIpProfileInheritNumString,
        juniIpProfileTcpMss,
        juniIpProfileFilterOptionsAll }
    STATUS      obsolete
    DESCRIPTION
        "An obsolete collection of objects providing management of IP Profile
        functionality in a Juniper product. This statement became osolete
        when juniIpProfileFlowStats was added."
    ::= { juniIpProfileMIBGroups 7 }

juniIpProfileGroup6  OBJECT-GROUP
    OBJECTS {
        juniIpProfileRouterName,
        juniIpProfileIpAddr,
        juniIpProfileIpMask,
        juniIpProfileDirectedBcastEnable,
        juniIpProfileIcmpRedirectEnable,
        juniIpProfileAccessRoute,
        juniIpProfileMtu,
        juniIpProfileSetMap,
        juniIpProfileSrcAddrValidEnable,
        juniIpProfileInheritNumString,
        juniIpProfileTcpMss,
        juniIpProfileFilterOptionsAll,
        juniIpProfileFlowStats }
    STATUS      obsolete
    DESCRIPTION
        "An obsolete collection of objects providing management of IP Profile
        functionality in a Juniper product. This statement became obsolete
        when juniIpProfileBlockMulticastSources was added."
    ::= { juniIpProfileMIBGroups 8 }

juniIpProfileGroup7  OBJECT-GROUP
    OBJECTS {
        juniIpProfileRouterName,
        juniIpProfileIpAddr,
        juniIpProfileIpMask,
        juniIpProfileDirectedBcastEnable,
        juniIpProfileIcmpRedirectEnable,
        juniIpProfileAccessRoute,
        juniIpProfileMtu,
        juniIpProfileSetMap,
        juniIpProfileSrcAddrValidEnable,
        juniIpProfileInheritNumString,
        juniIpProfileTcpMss,
        juniIpProfileFilterOptionsAll,
        juniIpProfileFlowStats,
        juniIpProfileBlockMulticastSources }
    STATUS      current
    DESCRIPTION
        "The basic collection of objects providing management of IP Profile
        functionality in a Juniper product."
    ::= { juniIpProfileMIBGroups 9 }

END
