
-- *****************************************************************************
-- Juniper-PIM-MIB
--
-- Juniper Networks Enterprise MIB
--   Protocol Independent Multicast (PIM) MIB
--
-- Copyright (c) 2001 Unisphere Networks, Inc.
-- Copyright (c) 2002 Juniper Networks, Inc.
--   All Rights Reserved.
-- *****************************************************************************

Juniper-PIM-MIB  DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Integer32, IpAddress, TimeTicks
        FROM SNMPv2-SMI
    RowStatus, TruthValue, TEXTUAL-CONVENTION
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF
    pimInterfaceIfIndex, pimRPSetComponent, pimRPSetGroupAddress,
    pimRPSetGroupMask, pimRPSetAddress
        FROM PIM-MIB
    InterfaceIndex
        FROM IF-MIB
    juniMibs
        FROM Juniper-MIBs;

juniPimMIB  MODULE-IDENTITY
    LAST-UPDATED "200209162144Z"  -- 16-Sep-02 05:44 PM EDT
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
        "       Juniper Networks, Inc.
        Postal: 10 Technology Park Drive
                Westford, MA  01886-3146
                USA
        Tel:    +1 978 589 5800
        Email:  mib@Juniper.net"
    DESCRIPTION
        "The enterprise MIB module for management of PIM routers."
    -- Revision History
    REVISION    "200209162144Z"  -- 16-Sep-02 05:44 PM EDT  - JUNOSe 5.0
    DESCRIPTION
        "Replaced Unisphere names with Juniper names."
    REVISION    "200103191537Z"  -- 19-Mar-01 10:37 AM EST  - JUNOSe 3.0
    DESCRIPTION
        "Initial enterprise version."
    ::= { juniMibs 43 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Textual conventions
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
JuniPimType ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "This data type is used do identify Sparse mode and Dense mode PIM
        protocol."
    SYNTAX      INTEGER {
                    invalid(0),         -- not valid value
                    dense(1),           -- dense mode PIM
                    sparse(2),          -- sparse mode PIM
                    sparseAndDense(3) } -- both sparse and dense mode PIM


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Managed objects
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniPimMIBObjects OBJECT IDENTIFIER ::= { juniPimMIB 1 }
juniPimTraps      OBJECT IDENTIFIER ::= { juniPimMIBObjects 0 }
juniPimGlobal     OBJECT IDENTIFIER ::= { juniPimMIBObjects 1 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Pim General Group
--
-- NOTE: RowStatus rowStatus.  This needs to go into virtual-router
--       MIB table so that we can create/destroy PIM
--
-- PimPktStats: these actually augment the general group of standard MIB
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniPimNumHelloRcvd  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Total number of Hellos received by PIM on this router."
    ::= { juniPimGlobal 1 }

juniPimNumJoinPruneRcvd  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Total number of JoinPrunes received by PIM on this router."
    ::= { juniPimGlobal 2 }

juniPimNumAssertRcvd  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Total number of Asserts received by PIM on this router."
    ::= { juniPimGlobal 3 }

juniPimNumGraftRcvd  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Total number of Grafts received by PIM on this router."
    ::= { juniPimGlobal 4 }

juniPimNumGraftAckRcvd  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Total number of Graft Acks received by PIM on this router."
    ::= { juniPimGlobal 5 }

juniPimNumHelloSent  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Total number of Hellos sent by PIM on this router."
    ::= { juniPimGlobal 6 }

juniPimNumJoinPruneSent  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Total number of JoinPrunes sent by PIM on this router."
    ::= { juniPimGlobal 7 }

juniPimNumAssertSent  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Total number of Asserts sent by PIM on this router."
    ::= { juniPimGlobal 8 }

juniPimNumGraftSent  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Total number of Grafts sent by PIM on this router."
    ::= { juniPimGlobal 9 }

juniPimNumGraftAckSent  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Total number of Graft Acks sent by PIM on this router."
    ::= { juniPimGlobal 10 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Pim Interface Table
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniPimInterfaceTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniPimInterfaceEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table listing enterprise specific information on a
        subset of the rows of the pimInterfaceTable defined in the standard PIM
        MIB."
    ::= { juniPimGlobal 11 }

juniPimInterfaceEntry  OBJECT-TYPE
    SYNTAX      JuniPimInterfaceEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the juniPimInterfaceTable.  There is one
        entry per entry in the pimInterfaceTable."
    INDEX     { pimInterfaceIfIndex }
    ::= { juniPimInterfaceTable 1 }

JuniPimInterfaceEntry ::= SEQUENCE {
    juniPimIntfNumHelloRcvd         Integer32,
    juniPimIntfNumJoinPruneRcvd     Integer32,
    juniPimIntfNumAssertRcvd        Integer32,
    juniPimIntfNumGraftRcvd         Integer32,
    juniPimIntfNumGraftAckRcvd      Integer32,
    juniPimIntfNumHelloSent         Integer32,
    juniPimIntfNumJoinPruneSent     Integer32,
    juniPimIntfNumAssertSent        Integer32,
    juniPimIntfNumGraftSent         Integer32,
    juniPimIntfNumGraftAckSent      Integer32,
    juniPimIntfVersion              INTEGER,
    juniPimIntfNumNbrs              Integer32 }

juniPimIntfNumHelloRcvd  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Total number of Hellos received by PIM on this interface.  It can only
        be cleared to 0 when doing set.  Setting this also sets counters for
        other types of packets to 0."
    ::= { juniPimInterfaceEntry 1 }

juniPimIntfNumJoinPruneRcvd  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Total number of JoinPrunes received by PIM on this interface.  It can
        only be cleared to 0 when doing set.  Setting this also sets counters
        for other types of packets to 0."
    ::= { juniPimInterfaceEntry 2 }

juniPimIntfNumAssertRcvd  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Total number of Asserts received by PIM on this interface.  It can only
        be cleared to 0 when doing set.  Setting this also sets counters for
        other types of packets to 0."
    ::= { juniPimInterfaceEntry 3 }

juniPimIntfNumGraftRcvd  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Total number of Grafts received by PIM on this interface.  It can only
        be cleared to 0 when doing set.  Setting this also sets counters for
        other types of packets to 0."
    ::= { juniPimInterfaceEntry 4 }

juniPimIntfNumGraftAckRcvd  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Total number of Graft Acks received by PIM on this interface.  It can
        only be cleared to 0 when doing set.  Setting this also sets counters
        for other types of packets to 0."
    ::= { juniPimInterfaceEntry 5 }

juniPimIntfNumHelloSent  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Total number of Hellos sent by PIM on this interface.  It can only be
        cleared to 0 when doing set.  Setting this also sets counters for other
        types of packets to 0."
    ::= { juniPimInterfaceEntry 6 }

juniPimIntfNumJoinPruneSent  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Total number of JoinPrunes sent by PIM on this interface.  It can only
        be cleared to 0 when doing set.  Setting this also sets counters for
        other types of packets to 0."
    ::= { juniPimInterfaceEntry 7 }

juniPimIntfNumAssertSent  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Total number of Asserts sent by PIM on this interface.  It can only be
        cleared to 0 when doing set.  Setting this also sets counters for other
        types of packets to 0."
    ::= { juniPimInterfaceEntry 8 }

juniPimIntfNumGraftSent  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Total number of Grafts sent by PIM on this interface.  It can only be
        cleared to 0 when doing set.  Setting this also sets counters for other
        types of packets to 0."
    ::= { juniPimInterfaceEntry 9 }

juniPimIntfNumGraftAckSent  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Total number of Graft Acks sent by PIM on this interface.  It can only
        be cleared to 0 when doing set.  Setting this also sets counters for
        other types of packets to 0."
    ::= { juniPimInterfaceEntry 10 }

juniPimIntfVersion  OBJECT-TYPE
    SYNTAX      INTEGER (1..2147483647)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The version of PIM running on this interface."
    ::= { juniPimInterfaceEntry 11 }

juniPimIntfNumNbrs  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of PIM neighbors detected on this interface."
    ::= { juniPimInterfaceEntry 12 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- The PIM Multicast Route Table
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniPimMRouteTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniPimMRouteEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table listing PIM multicast routing information
        describing its <*, *, RP>/ <*, G>/ <S, G> states."
    ::= { juniPimGlobal 12 }

juniPimMRouteEntry  OBJECT-TYPE
    SYNTAX      JuniPimMRouteEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the juniPimMRouteTable."
    INDEX     { juniPimMRouteGroup,
                juniPimMRouteSource,
                juniPimMRouteSourceMask,
                juniPimMRouteRPAddress }
    ::= { juniPimMRouteTable 1 }

JuniPimMRouteEntry ::= SEQUENCE {
    juniPimMRouteGroup                         IpAddress,
    juniPimMRouteSource                        IpAddress,
    juniPimMRouteSourceMask                    IpAddress,
    juniPimMRouteRPAddress                     IpAddress,
    juniPimMRouteUpstreamAssertTimer           TimeTicks,
    juniPimMRouteAssertMetric                  Integer32,
    juniPimMRouteAssertPref                    Integer32,
    juniPimMRouteAssertRPTBit                  TruthValue,
    juniPimMRouteBits                          BITS,
    juniPimMRouteRPAddrInUse                   IpAddress,
    juniPimMRouteUpstreamNbr                   IpAddress,
    juniPimMRouteIifAddr                       IpAddress,
    juniPimMRouteIsWaitingToSwitchToSPT        TruthValue,
    juniPimMRouteEntryExpiryTimer              TimeTicks,
    juniPimMRouteSenderDRAddr                  IpAddress,
    juniPimMRouteRouteAddr                     IpAddress,
    juniPimMRouteRouteMask                     IpAddress,
    juniPimMRouteGRPAddr                       IpAddress,
    juniPimMRouteGRPMask                       IpAddress,
    juniPimMRouteOtherProtoOifJoinTypeAll      TruthValue,
    juniPimMRouteOtherProtoOifJoinTypeG        TruthValue,
    juniPimMRouteOtherProtoOifJoinTypeSG       TruthValue,
    juniPimMRoutePimType                       JuniPimType }

juniPimMRouteGroup  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The group address.  Specified as 224.0.0.0 for <*, *, RP> entries."
    ::= { juniPimMRouteEntry 1 }

juniPimMRouteSource  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The source address. Specified as 0.0.0.0 for <*, *, RP> and <*, G>
        entries."
    ::= { juniPimMRouteEntry 2 }

juniPimMRouteSourceMask  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The source address mask. Specified as 255.255.255.255 for <S, G>
        entries and 0.0.0.0 for <*, *, RP> and <*, G> entries."
    ::= { juniPimMRouteEntry 3 }

juniPimMRouteRPAddress  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The RP address used for <*, *, RP>.  Specified as 0.0.0.0 for <S, G>
        and <*, G> entries."
    ::= { juniPimMRouteEntry 4 }

juniPimMRouteUpstreamAssertTimer  OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The time remaining before the router changes its upstream neighbor back
        to its RPF neighbor.  This timer is called the Assert timer in the PIM
        Sparse and Dense mode specification.  A value of 0 indicates that no
        Assert has changed the upstream neighbor away from the RPF neighbor."
    ::= { juniPimMRouteEntry 5 }

juniPimMRouteAssertMetric  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The metric advertised by the assert winner on the upstream interface,
        or 0 if no such assert is in received."
    ::= { juniPimMRouteEntry 6 }

juniPimMRouteAssertPref  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The preference advertised by the assert winner on the upstream
        interface, or 0 if no such assert is in effect."
    ::= { juniPimMRouteEntry 7 }

juniPimMRouteAssertRPTBit  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the RPT-bit advertised by the assert winner on the
        upstream interface, or false if no such assert is in effect."
    ::= { juniPimMRouteEntry 8 }

juniPimMRouteBits  OBJECT-TYPE
    SYNTAX      BITS {
                    rpt(0),
                    spt(1) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object describes whether the entry is on shared tree (RPT) or
        shortest path tree (SPT)."
    ::= { juniPimMRouteEntry 9 }

juniPimMRouteRPAddrInUse  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The RP Address being used for the <S, G>RPT/<*, G>/<*, *, RP> entries.
        Set to 0.0.0.0 for <S, G> entries on shortest path tree."
    ::= { juniPimMRouteEntry 10 }

juniPimMRouteUpstreamNbr  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The address of upstream neighbor being used for the entry.  Its set to
        0.0.0.0 if the router is directly attached to source on one of its
        interface. "
    ::= { juniPimMRouteEntry 11 }

juniPimMRouteIifAddr  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The address of incoming interface for this entry."
    ::= { juniPimMRouteEntry 12 }

juniPimMRouteIsWaitingToSwitchToSPT  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION

        "This object describes whether the entry is still waiting to switch
        completely to shortest path tree in case of <S, G> entries.  It waits to
        do this till it receives first packet from incoming interface towards
        shortest path tree."
    ::= { juniPimMRouteEntry 13 }

juniPimMRouteEntryExpiryTimer  OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The time after which the entry timer expires for this entry.  Set to 0
        if entry timer is not active."
    ::= { juniPimMRouteEntry 14 }

juniPimMRouteSenderDRAddr  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The address of the designated router on the sender's subnet in case of
        <S, G> entries.  The sender designated router register encapsulates data
        to RP.  Set to 0.0.0.0 for <*, G> and <*, *, RP> entries."
    ::= { juniPimMRouteEntry 15 }

juniPimMRouteRouteAddr  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The address of the route being used to do RPF check for this entry.  It
        is set to 0.0.0.0 (with juniPimMRouteRouteMask set to 255.255.255.255)
        if there is no route available."
    ::= { juniPimMRouteEntry 16 }

juniPimMRouteRouteMask  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The mask of the route being used to do RPF check for this entry.  It is
        set to 255.255.255.255 (with juniPimMRouteRoute set to 0.0.0.0) if there
        is no route available."
    ::= { juniPimMRouteEntry 17 }

juniPimMRouteGRPAddr  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The address of the group-to-RP mapping being used to get the RP for
        this entry.  It is set to 0.0.0.0 (with juniPimMRouteGRPMask set to
        0.0.0.0) if there is no group-to-RP mapping available or if entry is <*,
        *, RP>."
    ::= { juniPimMRouteEntry 18 }

juniPimMRouteGRPMask  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The mask of the group-to-RP mapping being used to get the RP for this
        entry.  It is set to 255.255.255.255 (with juniPimMRouteGRPAddr set to
        0.0.0.0) if there is no group-to-RP mapping available or if entry is <*,
        *, RP>."
    ::= { juniPimMRouteEntry 19 }

juniPimMRouteOtherProtoOifJoinTypeAll  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates if some other multicast protocol is also
        interested in receiving data for this entry as a result of its interest
        in receiving all data.  This will be particularly true for dense mode
        protocols which would want all data (<*, *>) from PIM sparse mode
        protocol."
    ::= { juniPimMRouteEntry 20 }

juniPimMRouteOtherProtoOifJoinTypeG  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates if some other multicast protocol is also
        interested in receiving data for this entry as a result of its interest
        in receiving data for a given group.  This will be particularly true for
        IGMP which would want data for a given group (<*, G>) from PIM
        protocol."
    ::= { juniPimMRouteEntry 21 }

juniPimMRouteOtherProtoOifJoinTypeSG  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates if some other multicast protocol is also
        interested in receiving data for this entry as a result of its interest
        in receiving data for a given <source, group>.  This will be
        particularly true for IGMPv3 which would want data for a given <source,
        group (<S, G>) from PIM sparse-mode protocol."
    ::= { juniPimMRouteEntry 22 }

juniPimMRoutePimType  OBJECT-TYPE
    SYNTAX      JuniPimType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates if the owner of this entry is Sparse mode or
        Dense mode PIM.  Owner is usually determined by the protocol running on
        the incoming interface of the entry.  In case sparse-dense mode PIM is
        running on the incoming interface, sparse-mode is the owner if RP for
        the group is known, else dense mode is the owner."
    ::= { juniPimMRouteEntry 23 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- The PIM Next Hop Table
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniPimMRouteNextHopTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniPimMRouteNextHopEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table listing PIM multicast routing information
        describing its <*, *, RP>/ <*, G>/ <S, G> outgoing interfaces."
    ::= { juniPimGlobal 13 }

juniPimMRouteNextHopEntry  OBJECT-TYPE
    SYNTAX      JuniPimMRouteNextHopEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the juniPimMRouteNextHopTable."
    INDEX     { juniPimMRouteNextHopGroupAddr,
                juniPimMRouteNextHopSrcAddr,
                juniPimMRouteNextHopSrcMask,
                juniPimMRouteNextHopRPAddr,
                juniPimMRouteNextHopIfId,
                juniPimMRouteNextHopAddress }
    ::= { juniPimMRouteNextHopTable 1 }

JuniPimMRouteNextHopEntry ::= SEQUENCE {
    juniPimMRouteNextHopGroupAddr                   IpAddress,
    juniPimMRouteNextHopSrcAddr                     IpAddress,
    juniPimMRouteNextHopSrcMask                     IpAddress,
    juniPimMRouteNextHopRPAddr                      IpAddress,
    juniPimMRouteNextHopIfId                        InterfaceIndex,
    juniPimMRouteNextHopAddress                     IpAddress,
    juniPimMRouteNextHopPruneReason                 INTEGER,
    juniPimMRouteNextHopJoinTypeSSRP                TruthValue,
    juniPimMRouteNextHopJoinTypeG                   TruthValue,
    juniPimMRouteNextHopJoinTypeSG                  TruthValue,
    juniPimMRouteNextHopHasLGM                      TruthValue,
    juniPimMRouteNextHopHasOifAW                    TruthValue,
    juniPimMRouteNextHopHasOifSendAssert            TruthValue,
    juniPimMRouteNextHopHasOifRegister              TruthValue,
    juniPimMRouteNextHopHasOifBorderBit             TruthValue,
    juniPimMRouteNextHopHasOifNullEncapsBit         TruthValue,
    juniPimMRouteNextHopJoinEndTimer                TimeTicks,
    juniPimMRouteNextHopAssertEndTimer              TimeTicks,
    juniPimMRouteNextHopNextAssertTimer             TimeTicks,
    juniPimMRouteNextHopAssertSrcAddress            IpAddress,
    juniPimMRouteNextHopRegisterSuppressionTimer    TimeTicks,
    juniPimMRouteNextHopPimType                     JuniPimType,
    juniPimMRouteNextHopPruneTimeLeft               TimeTicks,
    juniPimMRouteNextHopsendingIpAddress            IpAddress }

juniPimMRouteNextHopGroupAddr  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The group address. Specified as 224.0.0.0 for <*, *, RP> entries."
    ::= { juniPimMRouteNextHopEntry 2 }

juniPimMRouteNextHopSrcAddr  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The source address. Specified as 0.0.0.0 for <*, *, RP> and <*, G>
        entries."
    ::= { juniPimMRouteNextHopEntry 3 }

juniPimMRouteNextHopSrcMask  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The source address mask. Specified as 255.255.255.255 for <S, G>
        entries and 0.0.0.0 for <*, *, RP> and <*, G> entries."
    ::= { juniPimMRouteNextHopEntry 4 }

juniPimMRouteNextHopRPAddr  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The RP address used for <*, *, RP>. Specified as 0.0.0.0 for <S, G> and
        <*, G> entries."
    ::= { juniPimMRouteNextHopEntry 5 }

juniPimMRouteNextHopIfId  OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The interface index of the outgoing interface (next hop).  Specified as
        0 for register outgoing interface.  Register outgoing interfaces are
        created by DR on the source subnet to send PIM register encapsulated
        data (as unicast) to RP.  It is also used by PIM boundary routers
        (PMBRs) to register data to RP."
    ::= { juniPimMRouteNextHopEntry 6 }

juniPimMRouteNextHopAddress  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This object takes following different values based on the type of next
        hop.  It should be set to the address of RP in case the next hop
        interface is register interface i.e. juniPimMRouteNextHopIfId object is
        set to 0.  It should be set to the address of neighbor in case the
        interface is an NBMA interface.  In all other cases it should be set to
        the group address itself."
    ::= { juniPimMRouteNextHopEntry 7 }

juniPimMRouteNextHopPruneReason  OBJECT-TYPE
    SYNTAX      INTEGER {
                    other(1),
                    prune(2),
                    assert(3) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates why the downstream interface was pruned, whether
        in response to a PIM prune message or due to PIM Assert processing."
    ::= { juniPimMRouteNextHopEntry 8 }

juniPimMRouteNextHopJoinTypeSSRP  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates whether or not the interface was added as a
        result of receiving <*, *, RP> join in case of <*, *, RP> entry OR
        inherited as outgoing interface from corresponding <*, *, RP> entry in
        case of <*, G> entry."
    ::= { juniPimMRouteNextHopEntry 9 }

juniPimMRouteNextHopJoinTypeG  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates whether or not the interface was added as a
        result of receiving <*, G> join in case of <*, G> entry OR inherited as
        outgoing interface from corresponding <*, G> entry in case of <S, G>
        entry."
    ::= { juniPimMRouteNextHopEntry 10 }

juniPimMRouteNextHopJoinTypeSG  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates whether or not the interface was added as a
        result of receiving <S, G> join in case of <S, G> entry."
    ::= { juniPimMRouteNextHopEntry 11 }

juniPimMRouteNextHopHasLGM  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates whether or not the interface has local group
        membership (as indicated by IGMP) in case of <*, G> and <S, G> entries."
    ::= { juniPimMRouteNextHopEntry 12 }

juniPimMRouteNextHopHasOifAW  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates whether or not this interface is the winner of
        assert for corresponding <*, G>/<S, G> entry."
    ::= { juniPimMRouteNextHopEntry 13 }

juniPimMRouteNextHopHasOifSendAssert  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates whether or not this interface is going to send an
        assert at the end of assert suppression interval.  Assert suppression is
        used to prevent a flood of assert to be generated in response to data or
        other asserts."
    ::= { juniPimMRouteNextHopEntry 14 }

juniPimMRouteNextHopHasOifRegister  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates whether or not this next hop is a register
        outgoing interface."
    ::= { juniPimMRouteNextHopEntry 15 }

juniPimMRouteNextHopHasOifBorderBit  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object is used to describe a register outgoing interface.  It
        indicates whether or not the border bit is set in the register packet
        when the packet is sent over the register interface.  For all other
        (non-register) interfaces its set to false."
    ::= { juniPimMRouteNextHopEntry 16 }

juniPimMRouteNextHopHasOifNullEncapsBit  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object is used to describe a register outgoing interface.  It
        indicates whether or not the NULL encapsulation bit is set
        (periodically) in the register packet when the packet is sent over the
        register interface.  For all other (non-register) interfaces its set to
        false."
    ::= { juniPimMRouteNextHopEntry 17 }

juniPimMRouteNextHopJoinEndTimer  OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates the time (in seconds) left when the join timer
        expires for the outgoing interface.  Join timer for an outgoing
        interface of <S, G> entry indicates when the <S, G> join expires, for a
        <*, G> entry indicates when the <*, G> join expires and for a <*, *, RP>
        entry indicates when the <*, *, RP> join expires.  Inherited joins (like
        <S, G> inheriting from <*, G> AND <*, G> inheriting from <*, *, RP>)
        expire when the corresponding parent join expires."
    ::= { juniPimMRouteNextHopEntry 18 }

juniPimMRouteNextHopAssertEndTimer  OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates the time (in seconds) left when the assert timer
        expires on this outgoing inteface."
    ::= { juniPimMRouteNextHopEntry 19 }

juniPimMRouteNextHopNextAssertTimer  OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates the duration (in seconds) left for which sending
        an assert has been suppressed on this outgoing interface."
    ::= { juniPimMRouteNextHopEntry 20 }

juniPimMRouteNextHopAssertSrcAddress  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates the source address which will be used in the
        assert packet to send an assert out for the entry on this outgoing
        interface.  For <S, G> entries it is the address of the source S itself.
        For <*, G> entries it is the address of the source whose data was
        forwarded using this <*, G> and caused the assert situation to happen."
    ::= { juniPimMRouteNextHopEntry 21 }

juniPimMRouteNextHopRegisterSuppressionTimer  OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object is used for register outgoing interfaces.  It indicates the
        duration (in seconds) left for which sending a register packet has been
        suppressed on the register outgoing interface as a result of receiving
        register-stop from the RP."
    ::= { juniPimMRouteNextHopEntry 22 }

juniPimMRouteNextHopPimType  OBJECT-TYPE
    SYNTAX      JuniPimType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates whether the outgoing interface was contributed by
        sparse-mode or dense-mode PIM."
    ::= { juniPimMRouteNextHopEntry 23 }

juniPimMRouteNextHopPruneTimeLeft  OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates the time (in seconds) left when the prune timer
        expires on an outgoing inteface.  Its used for pruned outgoing
        interfaces contributed by dense-mode PIM."
    ::= { juniPimMRouteNextHopEntry 24 }

juniPimMRouteNextHopsendingIpAddress  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object describes the source IP address used by this interface to
        send PIM packets out on this outgoing interface."
    ::= { juniPimMRouteNextHopEntry 25 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- The PIM RP-Set Table
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniPimRPSetTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniPimRPSetEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table listing enterprise specific information on a
        subset of the rows of the pimRPSetTable defined in the standard PIM
        MIB."
    ::= { juniPimGlobal 14 }

juniPimRPSetEntry  OBJECT-TYPE
    SYNTAX      JuniPimRPSetEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the juniPimRPSetTable."
    INDEX     { pimRPSetComponent,
                pimRPSetGroupAddress,
                pimRPSetGroupMask,
                pimRPSetAddress }
    ::= { juniPimRPSetTable 1 }

JuniPimRPSetEntry ::= SEQUENCE {
    juniPimRPSetPriority        Integer32,
    juniPimRPSetTypeInfo        INTEGER,
    juniPimRPSetAccessListName  OCTET STRING }

juniPimRPSetPriority  OBJECT-TYPE
    SYNTAX      Integer32 (1..'FFFF'h)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object describes the priority of the RP for this group-to-RP
        mapping."
    ::= { juniPimRPSetEntry 1 }

juniPimRPSetTypeInfo  OBJECT-TYPE
    SYNTAX      INTEGER {
                    pimRPTypeInvalid(0),
                    pimRPTypeStatic(1),
                    pimRPTypeStaticOverride(2),
                    pimRPTypeAutoRP(3),
                    pimRPTypeBSR(4),
                    pimRPTypeStaticNegative(5),
                    pimRPTypeStaticOverrideNegative(6),
                    pimRPTypeAutoRPNegative(7),
                    pimRPTypeBSRNegative(8) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object describes the mechanism by which this group to RP mapping
        has been learnt, i.e. whether its statically configured, AutoRP learnt
        or BSR learnt.  It also indicates whether the mapping is positive or
        negative.  Negative mappings force the groups in that range to fall into
        dense-mode category if sparse-dense mode is configured or no RP if its
        purely sparse mode configuration."
    ::= { juniPimRPSetEntry 2 }

juniPimRPSetAccessListName  OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(0..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object lists the name of the access list from which this
         group-to-RP mapping was picked up in case of statically configured
         RPs."
    ::= { juniPimRPSetEntry 3 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- The PIM Static RP configuration table
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniPimStaticRPConfTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniPimStaticRPConfEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table listing statically configured PIM RPs."
    ::= { juniPimGlobal 15 }

juniPimStaticRPConfEntry  OBJECT-TYPE
    SYNTAX      JuniPimStaticRPConfEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the juniPimStaticRPConfTable."
    INDEX     { juniPimStaticRPConfComponentIndex,
                juniPimStaticRPConfRPAddr,
                juniPimStaticRPConfAccessListName }
    ::= { juniPimStaticRPConfTable 1 }

JuniPimStaticRPConfEntry ::= SEQUENCE {
    juniPimStaticRPConfComponentIndex   Integer32,
    juniPimStaticRPConfRPAddr           IpAddress,
    juniPimStaticRPConfAccessListName   OCTET STRING,
    juniPimStaticRPConfRowStatus        RowStatus,
    juniPimStaticRPConfOverride         TruthValue }

juniPimStaticRPConfComponentIndex  OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A number uniquely identifying the component.  Each protocol instance
        connected to a separate domain should have a different index value."
    ::= { juniPimStaticRPConfEntry 1 }

juniPimStaticRPConfRPAddr  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Ip address of the RP which for the group-to-RP mapping being
        configured."
    ::= { juniPimStaticRPConfEntry 2 }

juniPimStaticRPConfAccessListName  OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(0..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Name of the access list from which group-ranges are picked up for this
        group-ro-RP mapping.  Every deny component in the list is added as
        negative group-ro-RP mapping."
    ::= { juniPimStaticRPConfEntry 3 }

juniPimStaticRPConfRowStatus  OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The status of this row, by which new entries may be created, or old
        entries deleted from this table."
    ::= { juniPimStaticRPConfEntry 4 }

juniPimStaticRPConfOverride  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The object indicates whether or not this statically configured
        group-to-RP mapping should override the group-to-RP mapping learnt via
        AutoRP for the component group-ranges in the access list.  By default
        AutoRP learnt group-to-RP mappings are preferred over statically
        configured ones.  While setting the rowStatus to create a static RP,
        this field should be assigned to true if the override property is
        desired."
    DEFVAL    { false }
    ::= { juniPimStaticRPConfEntry 5 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- The PIM AutoRP Candidate RP configuration table
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniPimAutoRPConfTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniPimAutoRPConfEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table allowing AutoRP configuration of candidate RPs
        (advertisement agents)."
    ::= { juniPimGlobal 16 }

juniPimAutoRPConfEntry  OBJECT-TYPE
    SYNTAX      JuniPimAutoRPConfEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the juniPimAutoRPConfTable."
    INDEX     { juniPimAutoRPConfComponentIndex,
                juniPimAutoRPConfCandRPAddr,
                juniPimAutoRPConfGroupAccessListName }
    ::= { juniPimAutoRPConfTable 1 }

JuniPimAutoRPConfEntry ::= SEQUENCE {
    juniPimAutoRPConfComponentIndex         Integer32,
    juniPimAutoRPConfCandRPAddr             IpAddress,
    juniPimAutoRPConfGroupAccessListName    OCTET STRING,
    juniPimAutoRPConfRowStatus              RowStatus,
    juniPimAutoRPConfTTL                    Integer32,
    juniPimAutoRPConfAncmntIntvl            TimeTicks,
    juniPimAutoRPConfifId                   InterfaceIndex }

juniPimAutoRPConfComponentIndex  OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A number uniquely identifying the component.  Each protocol instance
        connected to a separate domain should have a different index value."
    ::= { juniPimAutoRPConfEntry 1 }

juniPimAutoRPConfCandRPAddr  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The IP address of the candidate RP for this advertising agent
        configuration."
    ::= { juniPimAutoRPConfEntry 2 }

juniPimAutoRPConfGroupAccessListName  OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(0..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The access list name from which group ranges are picked up for
        advertising agent configuration."
    ::= { juniPimAutoRPConfEntry 3 }

juniPimAutoRPConfRowStatus  OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The status of this row, by which new entries may be created, or old
        entries deleted from this table."
    ::= { juniPimAutoRPConfEntry 4 }

juniPimAutoRPConfTTL  OBJECT-TYPE
    SYNTAX      Integer32 (1..'FFFF'h)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The time-to-live value used while sending AutoRP advertisement out for
        this group-to-RP mappings created as a result of this configuration.
        This should be set along with juniPimAutoRPConfRowStatus while creating
        an AutoRP advertising agent to denote the TTL value to be used."
    DEFVAL    { 64 }
    ::= { juniPimAutoRPConfEntry 5 }

juniPimAutoRPConfAncmntIntvl  OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The time interval at which AutoRP advertisements are sent out for the
        group-to-RP mappings created as a result of this configuration.  This
        should be set along with juniPimAutoRPConfRowStatus while creating an
        AutoRP advertising agent to denote the announcement interval to be
        used."
    DEFVAL    { 60 }
    ::= { juniPimAutoRPConfEntry 6 }

juniPimAutoRPConfifId  OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The interface index of the interface for the candidate RP if an
        interface with that address exists else it is set to 0."
    ::= { juniPimAutoRPConfEntry 7 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- The PIM AutoRP candidate RP table
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniPimAutoRPCandTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniPimAutoRPCandEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table listing AutoRP candidate RPS (advertising
        agents)."
    ::= { juniPimGlobal 17 }

juniPimAutoRPCandEntry  OBJECT-TYPE
    SYNTAX      JuniPimAutoRPCandEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the juniPimAutoRPCandTable."
    INDEX     { juniPimAutoRPCandComponentIndex,
                juniPimAutoRPCandRPAddr,
                juniPimAutoRPCandGroupAddr,
                juniPimAutoRPCandGroupMask }
    ::= { juniPimAutoRPCandTable 1 }

JuniPimAutoRPCandEntry ::= SEQUENCE {
    juniPimAutoRPCandComponentIndex     Integer32,
    juniPimAutoRPCandRPAddr             IpAddress,
    juniPimAutoRPCandGroupAddr          IpAddress,
    juniPimAutoRPCandGroupMask          IpAddress,
    juniPimAutoRPCandRowStatus          RowStatus,
    juniPimAutoRPCandAccessListName     OCTET STRING,
    juniPimAutoRPCandAutoRPTTL          Integer32,
    juniPimAutoRPCandAutoRPAncmntIntvl  TimeTicks,
    juniPimAutoRPCandIfId               InterfaceIndex }

juniPimAutoRPCandComponentIndex  OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A number uniquely identifying the component.  Each protocol instance
        connected to a separate domain should have a different index value."
    ::= { juniPimAutoRPCandEntry 1 }

juniPimAutoRPCandRPAddr  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The IP address of the candidate RP for this group-to-RP mapping."
    ::= { juniPimAutoRPCandEntry 2 }

juniPimAutoRPCandGroupAddr  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The group address of the candidate RP for this group-to-RP mapping."
    ::= { juniPimAutoRPCandEntry 3 }

juniPimAutoRPCandGroupMask  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The group mask of the candidate RP for this group-to-RP mapping."
    ::= { juniPimAutoRPCandEntry 4 }

juniPimAutoRPCandRowStatus  OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The current status of this row."
    ::= { juniPimAutoRPCandEntry 5 }

juniPimAutoRPCandAccessListName  OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(0..32))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The name of the group list using which this AutoRP group-to-RP
        candidate RP mapping was configured."
    ::= { juniPimAutoRPCandEntry 6 }

juniPimAutoRPCandAutoRPTTL  OBJECT-TYPE
    SYNTAX      Integer32(1..'FFFF'h)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The time-to-live value used while sending AutoRP advertisement out for
        this group-to-RP mapping."
    ::= { juniPimAutoRPCandEntry 7 }

juniPimAutoRPCandAutoRPAncmntIntvl  OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The time interval at which AutoRP advertisements are sent out for this
        group-to-RP mapping."
    ::= { juniPimAutoRPCandEntry 8 }

juniPimAutoRPCandIfId  OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The interface index of the interface for this AutoRP group-to-RP
        candidate RP mapping if an interface for RP address exists else it is
        set to 0."
    ::= { juniPimAutoRPCandEntry 9 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- The PIM Component Table
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniPimComponentTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniPimComponentEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table listing each component (domain) in PIM."
    ::= { juniPimGlobal 18 }

juniPimComponentEntry  OBJECT-TYPE
    SYNTAX      JuniPimComponentEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the juniPimComponentTable."
    INDEX     { juniPimComponentIndex }
    ::= { juniPimComponentTable 1 }

JuniPimComponentEntry ::= SEQUENCE {
    juniPimComponentIndex                               Integer32,
    juniPimComponentAutoRPMappingAgentRowStatus         RowStatus,
    juniPimComponentConfiguredAutoRPMappingAgentIfId    InterfaceIndex,
    juniPimComponentAutoRPMappingAgentInterval          TimeTicks,
    juniPimComponentAutoRPMappingTTL                    Integer32,
    juniPimComponentAutoRPMappingAgentIntfAddr          IpAddress,
    juniPimComponentAutoRPMappingAgentWinnerAddr        IpAddress,
    juniPimComponentAutoRPMappingAgentWinnerLastHeard   TimeTicks }

juniPimComponentIndex  OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A number uniquely identifying the component.  Each protocol instance
        connected to a separate domain should have a different index value."
    ::= { juniPimComponentEntry 1 }

juniPimComponentAutoRPMappingAgentRowStatus  OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The status of AutoRP mapping agent by which this router can be made an
        AutoRP mapping agent or removed from being an AutoRP mapping agent in
        this component."
    ::= { juniPimComponentEntry 2 }

juniPimComponentConfiguredAutoRPMappingAgentIfId  OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The interface index of the interface which mapping agent should use to
        send AutoRP mapping messages.  If not specified, the interface with
        highest IP address in this domain is picked up for this purpose."
    ::= { juniPimComponentEntry 3 }

juniPimComponentAutoRPMappingAgentInterval  OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The time interval at which AutoRP mapping messages are sent out in this
        component.  The default value is 60 seconds."
    DEFVAL    { 60 }
    ::= { juniPimComponentEntry 4 }

juniPimComponentAutoRPMappingTTL  OBJECT-TYPE
    SYNTAX      Integer32 (1..'FFFF'h)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The time-to-live value used while sending AutoRP mapping messages out
        in this component."
    DEFVAL    { 64 }
    ::= { juniPimComponentEntry 5 }

juniPimComponentAutoRPMappingAgentIntfAddr  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The IP address of the interface which mapping agent is using to send
        AutoRP mapping messages."
    ::= { juniPimComponentEntry 6 }

juniPimComponentAutoRPMappingAgentWinnerAddr  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The IP address of the winner AutoRP mapping agent.  There can be
        multiple mapping agents configured in a given PIM domain(component).
        The mapping agent with highest IP address is chosen as the winner and it
        continues to send AutoRP mapping messages.  If the router itself is the
        winner, then this is set to 0.0.0.0."
    ::= { juniPimComponentEntry 7 }

juniPimComponentAutoRPMappingAgentWinnerLastHeard  OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The time (in seconds) that has past since an AutoRP mapping message was
        receieved from the winner AutoRP mapping agent.  If the router itself is
        the winner, then this is set to 0."
    ::= { juniPimComponentEntry 8 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- The PIM Unicast Route Table
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniPimUnicastRouteTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniPimUnicastRouteEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table listing all the unicast routes currently in use
        by PIM for diong RPF checking."
    ::= { juniPimGlobal 19 }

juniPimUnicastRouteEntry  OBJECT-TYPE
    SYNTAX      JuniPimUnicastRouteEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the juniPimUnicastRouteTable."
    INDEX     { juniPimUnicastRouteEntryAddr,
                juniPimUnicastRouteEntryMask }
    ::= { juniPimUnicastRouteTable 1 }

JuniPimUnicastRouteEntry ::= SEQUENCE {
    juniPimUnicastRouteEntryAddr        IpAddress,
    juniPimUnicastRouteEntryMask        IpAddress,
    juniPimUnicastRouteEntryRpfNbr      IpAddress,
    juniPimUnicastRouteEntryIifId       InterfaceIndex,
    juniPimUnicastRouteEntryIifAddr     IpAddress,
    juniPimUnicastRouteEntryPref        Integer32,
    juniPimUnicastRouteEntryMetric      Integer32,
    juniPimUnicastRouteEntryPimType     JuniPimType }

juniPimUnicastRouteEntryAddr  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The address of route in use."
    ::= { juniPimUnicastRouteEntry 1 }

juniPimUnicastRouteEntryMask  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The mask of route in use."
    ::= { juniPimUnicastRouteEntry 2 }

juniPimUnicastRouteEntryRpfNbr  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The RPF neighbor (next-hop) to reach the route of this entry.  It is
        set to 0.0.0.0 for directly connected routes."
    ::= { juniPimUnicastRouteEntry 3 }

juniPimUnicastRouteEntryIifId  OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The interface index (next-hop) to reach the route of this entry."
    ::= { juniPimUnicastRouteEntry 4 }

juniPimUnicastRouteEntryIifAddr  OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The interface address (next-hop) to reach the route of this entry."
    ::= { juniPimUnicastRouteEntry 5 }

juniPimUnicastRouteEntryPref  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The preference of the route of this entry."
    ::= { juniPimUnicastRouteEntry 6 }

juniPimUnicastRouteEntryMetric  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The metric of the route of this entry."
    ::= { juniPimUnicastRouteEntry 7 }

juniPimUnicastRouteEntryPimType  OBJECT-TYPE
    SYNTAX      JuniPimType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This object indicates whether the route specified in this entry is
        being used by sparse-mode and/or dense-mode PIM."
    ::= { juniPimUnicastRouteEntry 8 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- The PIM Shortest Path Tree Threshold Table
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniPimSPTThresholdTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniPimSPTThresholdEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The (conceptual) table listing threshold values set for switching from
        shared tree to shortest path tree and vice versa for data forwarded by
        PIM sparse-mode."
    ::= { juniPimGlobal 20 }

juniPimSPTThresholdEntry  OBJECT-TYPE
    SYNTAX      JuniPimSPTThresholdEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry (conceptual row) in the juniPimSPTThresholdTable."
    INDEX     { juniPimSPTThresholdAccessListName }
    ::= { juniPimSPTThresholdTable 1 }

JuniPimSPTThresholdEntry ::= SEQUENCE {
    juniPimSPTThresholdAccessListName   OCTET STRING,
    juniPimSPTThresholdRowStatus        RowStatus,
    juniPimSPTThresholdKbps             Integer32 }

juniPimSPTThresholdAccessListName  OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(0..32))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The name of the access list from which group ranges are picked up for
        setting SPT threshold in this entry."
    ::= { juniPimSPTThresholdEntry 1 }

juniPimSPTThresholdRowStatus  OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The status of this row, by which new entries may be created, or old
        entries deleted from this table."
    ::= { juniPimSPTThresholdEntry 2 }

juniPimSPTThresholdKbps  OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of SPT threshold in kilobits per second.  Default value is
        0."
    DEFVAL    { 0 }
    ::= { juniPimSPTThresholdEntry 3 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Conformance information
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniPimConformance     OBJECT IDENTIFIER ::= { juniPimMIB 2 }
juniPimCompliances     OBJECT IDENTIFIER ::= { juniPimConformance 1 }
juniPimGroups          OBJECT IDENTIFIER ::= { juniPimConformance 2 }

--
-- compliance statements
--
juniPimCompliance  MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for entities which implement the Juniper PIM
        MIB."
    MODULE  -- this module
        MANDATORY-GROUPS {
            juniPimGeneralGroup,
            juniPimInterfaceGroup,
            juniPimMRouteConfGroup,
            juniPimMRouteNextHopGroup,
            juniPimRPSetGroup,
            juniPimStaticRPConfGroup,
            juniPimAutoRPConfGroup,
            juniPimAutoRPCandGroup,
            juniPimComponentGroup,
            juniPimUnicastRouteGroup,
            juniPimSPTThresholdGroup }
    ::= { juniPimCompliances 1 }

-- units of conformance

juniPimGeneralGroup OBJECT-GROUP
    OBJECTS {
        juniPimNumHelloRcvd,
        juniPimNumJoinPruneRcvd,
        juniPimNumAssertRcvd,
        juniPimNumGraftRcvd,
        juniPimNumGraftAckRcvd,
        juniPimNumHelloSent,
        juniPimNumJoinPruneSent,
        juniPimNumAssertSent,
        juniPimNumGraftSent,
        juniPimNumGraftAckSent }
    STATUS      current
    DESCRIPTION
        "A collection of objects for managing general PIM capabilities in a
        Juniper product."
    ::= { juniPimGroups 1 }                                        -- JUNOSe 3.0

juniPimInterfaceGroup OBJECT-GROUP
    OBJECTS {
        juniPimIntfNumHelloRcvd,
        juniPimIntfNumJoinPruneRcvd,
        juniPimIntfNumAssertRcvd,
        juniPimIntfNumGraftRcvd,
        juniPimIntfNumGraftAckRcvd,
        juniPimIntfNumHelloSent,
        juniPimIntfNumJoinPruneSent,
        juniPimIntfNumAssertSent,
        juniPimIntfNumGraftSent,
        juniPimIntfNumGraftAckSent,
        juniPimIntfVersion,
        juniPimIntfNumNbrs }
    STATUS      current
    DESCRIPTION
        "A collection of objects for managing PIM interface capabilities in a
        Juniper product."
    ::= { juniPimGroups 2 }

juniPimMRouteConfGroup OBJECT-GROUP
    OBJECTS {
        juniPimMRouteUpstreamAssertTimer,
        juniPimMRouteAssertMetric,
        juniPimMRouteAssertPref,
        juniPimMRouteAssertRPTBit,
        juniPimMRouteBits,
        juniPimMRouteRPAddrInUse,
        juniPimMRouteUpstreamNbr,
        juniPimMRouteIifAddr,
        juniPimMRouteIsWaitingToSwitchToSPT,
        juniPimMRouteEntryExpiryTimer,
        juniPimMRouteSenderDRAddr,
        juniPimMRouteRouteAddr,
        juniPimMRouteRouteMask,
        juniPimMRouteGRPAddr,
        juniPimMRouteGRPMask,
        juniPimMRouteOtherProtoOifJoinTypeAll,
        juniPimMRouteOtherProtoOifJoinTypeG,
        juniPimMRouteOtherProtoOifJoinTypeSG,
        juniPimMRoutePimType }
    STATUS      current
    DESCRIPTION
        "A collection of objects for managing PIM multicast route capabilities
        in a Juniper product."
    ::= { juniPimGroups 3 }

juniPimMRouteNextHopGroup OBJECT-GROUP
    OBJECTS {
        juniPimMRouteNextHopPruneReason,
        juniPimMRouteNextHopJoinTypeSSRP,
        juniPimMRouteNextHopJoinTypeG,
        juniPimMRouteNextHopJoinTypeSG,
        juniPimMRouteNextHopHasLGM,
        juniPimMRouteNextHopHasOifAW,
        juniPimMRouteNextHopHasOifSendAssert,
        juniPimMRouteNextHopHasOifRegister,
        juniPimMRouteNextHopHasOifBorderBit,
        juniPimMRouteNextHopHasOifNullEncapsBit,
        juniPimMRouteNextHopJoinEndTimer,
        juniPimMRouteNextHopAssertEndTimer,
        juniPimMRouteNextHopNextAssertTimer,
        juniPimMRouteNextHopAssertSrcAddress,
        juniPimMRouteNextHopRegisterSuppressionTimer,
        juniPimMRouteNextHopPimType,
        juniPimMRouteNextHopPruneTimeLeft,
        juniPimMRouteNextHopsendingIpAddress }
    STATUS      current
    DESCRIPTION
        "A collection of objects for managing PIM multicast route next hop
        capabilities in a Juniper product."
    ::= { juniPimGroups 4 }

juniPimRPSetGroup OBJECT-GROUP
    OBJECTS {
        juniPimRPSetPriority,
        juniPimRPSetTypeInfo,
        juniPimRPSetAccessListName }
    STATUS      current
    DESCRIPTION
        "A collection of objects for managing PIM RP-Set capabilities in a
        Juniper product."
    ::= { juniPimGroups 5 }

juniPimStaticRPConfGroup OBJECT-GROUP
    OBJECTS {
        juniPimStaticRPConfRowStatus,
        juniPimStaticRPConfOverride }
    STATUS      current
    DESCRIPTION
        "A collection of objects for managing statically configured PIM RPs
        capabilities in a Juniper product."
    ::= { juniPimGroups 6 }

juniPimAutoRPConfGroup OBJECT-GROUP
    OBJECTS {
        juniPimAutoRPConfRowStatus,
        juniPimAutoRPConfTTL,
        juniPimAutoRPConfAncmntIntvl,
        juniPimAutoRPConfifId }
    STATUS      current
    DESCRIPTION
        "A collection of objects for managing PIM AutoRP candidate advertisment
        agent RP capabilities in a Juniper product."
    ::= { juniPimGroups 7 }

juniPimAutoRPCandGroup OBJECT-GROUP
    OBJECTS {
        juniPimAutoRPCandRowStatus,
        juniPimAutoRPCandAccessListName,
        juniPimAutoRPCandAutoRPTTL,
        juniPimAutoRPCandAutoRPAncmntIntvl,
        juniPimAutoRPCandIfId }
    STATUS      current
    DESCRIPTION
        "A collection of objects for managing PIM AutoRP candidate advertising
        agent RP capabilities in a Juniper product."
    ::= { juniPimGroups 8 }

juniPimComponentGroup OBJECT-GROUP
    OBJECTS {
        juniPimComponentAutoRPMappingAgentRowStatus,
        juniPimComponentConfiguredAutoRPMappingAgentIfId,
        juniPimComponentAutoRPMappingAgentInterval,
        juniPimComponentAutoRPMappingTTL,
        juniPimComponentAutoRPMappingAgentIntfAddr,
        juniPimComponentAutoRPMappingAgentWinnerAddr,
        juniPimComponentAutoRPMappingAgentWinnerLastHeard }
    STATUS      current
    DESCRIPTION
        "A collection of objects for managing PIM component (domain)
        capabilities in a Juniper product."
    ::= { juniPimGroups 9 }

juniPimUnicastRouteGroup OBJECT-GROUP
    OBJECTS {
        juniPimUnicastRouteEntryRpfNbr,
        juniPimUnicastRouteEntryIifId,
        juniPimUnicastRouteEntryIifAddr,
        juniPimUnicastRouteEntryPref,
        juniPimUnicastRouteEntryMetric,
        juniPimUnicastRouteEntryPimType }
    STATUS      current
    DESCRIPTION
        "A collection of objects for managing PIM unicast route capabilities in
        a Juniper product."
    ::= { juniPimGroups 10 }

juniPimSPTThresholdGroup OBJECT-GROUP
    OBJECTS {
        juniPimSPTThresholdRowStatus,
        juniPimSPTThresholdKbps }
    STATUS      current
    DESCRIPTION
        "A collection of objects for managing PIM shortest path tree threshold
        capabilities in a Juniper product."
    ::= { juniPimGroups 11 }

END
