-- This module defines enterprise MIBs for Virtual Systems
-- 
-- Copyright (c) 1999-2004, Juniper Networks, Inc.
-- All rights reserved.

NETSCREEN-VSYS-MIB DEFINITIONS ::= BEGIN

IMPORTS
    netscreenVsys
        FROM NETSCREEN-SMI
    Integer32, MODULE-IDENTITY, OBJECT-TYPE
        FROM SNMPv2-SMI
    DisplayString
        FROM SNMPv2-TC
    ;

netscreenVsysMibModule MODULE-IDENTITY
    LAST-UPDATED  "200405032022Z" -- May 03, 2004
    ORGANIZATION
        "Juniper Networks, Inc."
    CONTACT-INFO
        "Customer Support

         1194 North Mathilda Avenue 
         Sunnyvale, California 94089-1206
         USA

         Tel: 1-800-638-8296
         E-mail: customerservice@juniper.net
         HTTP://www.juniper.net"
    DESCRIPTION
        "This module defines the object that are use to monitor all the
         virtual systems"
    REVISION      "200405030000Z" -- May 03, 2004
    DESCRIPTION
        "Modified copyright and contact information"
    REVISION      "200403030000Z" -- March 03, 2004
    DESCRIPTION
        "Converted to SMIv2 by Longview Software"
    REVISION      "200311130000Z" -- November 13, 2003
    DESCRIPTION
        "Correct spelling mistake"
    REVISION      "200109280000Z" -- September 28, 2001
    DESCRIPTION
        "no comment"
    REVISION      "200005080000Z" -- May 08, 2000
    DESCRIPTION
        "Creation Date"
    ::= { netscreenVsys 0 }

NsVsysCfgEntry ::= SEQUENCE
{
    nsVsysCfgId   Integer32,
    nsVsysCfgName DisplayString
}

nsVsysCfg OBJECT IDENTIFIER ::= { netscreenVsys 1 }

nsVsysCfgTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF NsVsysCfgEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "NetScreen-500, NetScreen-1000 and above series support virtual
         system. This table collects the vsys configuration in NetScreen
         device."
    ::= { nsVsysCfg 1 }

nsVsysCfgEntry OBJECT-TYPE
    SYNTAX        NsVsysCfgEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "Each entry in the table holds a set of configuration
         parameters associated  with an instance of virtual system."
    INDEX
        { nsVsysCfgId }
    ::= { nsVsysCfgTable 1 }

nsVsysCfgId OBJECT-TYPE
    SYNTAX        Integer32 (0..2147483647)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "A unique ID for each virtual system."
    ::= { nsVsysCfgEntry 1 }

nsVsysCfgName OBJECT-TYPE
    SYNTAX        DisplayString (SIZE(0..32))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "virtual system name."
    ::= { nsVsysCfgEntry 2 }

END


