
-- *****************************************************************************
-- Juniper-DS1-MIB
--
-- Juniper Networks Enterprise MIB
--   DS1/E1 MIB
--
-- Copyright (c) 1998, 1999 Redstone Communications, Inc.
-- Copyright (c) 1999, 2002 Unisphere Networks, Inc.
-- Copyright (c) 2002, 2003 Juniper Networks, Inc.
--   All Rights Reserved.
-- *****************************************************************************

Juniper-DS1-MIB  DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Integer32
        FROM SNMPv2-SMI
    RowStatus, DisplayString
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF
    ifIndex, InterfaceIndexOrZero
        FROM IF-MIB
    juniMibs
        FROM Juniper-MIBs
    JuniTimeSlotMap, JuniNextIfIndex
        FROM Juniper-TC;

juniDs1MIB  MODULE-IDENTITY
    LAST-UPDATED "200302101507Z"  -- 10-Feb-03 10:07 AM EST
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
        "       Juniper Networks, Inc.
        Postal: 10 Technology Park Drive
                Westford, MA  01886-3146
                USA
        Tel:    +1 978 589 5800
        Email:  mib@Juniper.net"
    DESCRIPTION
        "The DS1/E1 MIB for the Juniper enterprise.  This MIB contains managed
        objects to supplement those found in RFC1406 DS1/E1 MIB."
    -- Revision History
    REVISION    "200302101507Z"  -- 10-Feb-03 10:07 AM EST  - JUNOSe 5.0
    DESCRIPTION
        "Replaced Unisphere names with Juniper names."
    REVISION    "200209121659Z"  -- 12-Sep-02 12:59 PM EDT  - JUNOSe 4.1
    DESCRIPTION
        "Added support for FDL transmit mode, remote FDL strings and far end FDL
        carrier."
    REVISION    "200205131601Z"  -- 13-May-02 12:01 PM EDT  - JUNOSe 4.0
    DESCRIPTION
        "Added support for FDL."
    REVISION    "200107311825Z"  -- 31-Jul-01 02:25 PM EDT  - JUNOSe 3.2
    DESCRIPTION
        "Change access on juniDsx1Ds1ChannelNumber."
    REVISION    "200104041805Z"  -- 04-Apr-01 02:05 PM EDT  - JUNOSe 3.0
    DESCRIPTION
        "Added dynamic DS1 interface support."
    REVISION      "9906170000Z"  -- 17-Jun-99               - JUNOSe 1.1
    DESCRIPTION
        "Updated version of this MIB module."
    REVISION      "9811130000Z"  -- 13-Nov-98               - JUNOSe 1.0
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { juniMibs 5 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Managed objects
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniDs1Objects     OBJECT IDENTIFIER ::= { juniDs1MIB 1 }


-- /////////////////////////////////////////////////////////////////////////////
--
-- DS1 Interfaces
--
-- /////////////////////////////////////////////////////////////////////////////
--
-- The DS1 Configuration Table
--
juniDsx1ConfigTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniDsx1ConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for DS1/E1 interfaces present in the
        system."
    ::= { juniDs1Objects 1 }

juniDsx1ConfigEntry  OBJECT-TYPE
    SYNTAX      JuniDsx1ConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of an DS1/E1 interface."
    INDEX     { ifIndex }
    ::= { juniDsx1ConfigTable 1 }

JuniDsx1ConfigEntry ::= SEQUENCE {
        juniDsx1TimeSlotMap              JuniTimeSlotMap,
        juniDsx1Ds1ChannelNumber         Integer32,
        juniDsx1Capabilities             Integer32,
        juniDsx1Mode                     INTEGER,
        juniDsx1LineBuildOutCapabilities Integer32,
        juniDsx1LineBuildOutType         INTEGER,
        juniDsx1LineAttenuation          INTEGER,
        juniDsx1LineLength               Integer32,
        juniDsx1LowerIfIndex             InterfaceIndexOrZero,
        juniDsx1RowStatus                RowStatus,
        juniDsx1SendCode                 INTEGER,
        juniDsx1YellowAlarm              INTEGER,
        juniDsx1RemoteLoopback           INTEGER,
        juniDsx1FdlCarrier               INTEGER,
        juniDsx1FdlEic                   DisplayString,
        juniDsx1FdlLic                   DisplayString,
        juniDsx1FdlFic                   DisplayString,
        juniDsx1FdlUnit                  DisplayString,
        juniDsx1FdlPfi                   DisplayString,
        juniDsx1FdlPort                  DisplayString,
        juniDsx1FdlGenerator             DisplayString,
        juniDsx1FdlTransmit              BITS }

juniDsx1TimeSlotMap  OBJECT-TYPE
    SYNTAX      JuniTimeSlotMap
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A bitmap representing the timeslots on the DS1/E1 interface that have
        been allocated for service.

        For channelized DS1/E1, set bits reflect the union of timeslot
        allocations across all fractional arrangements operating over this
        DS1/E1 interface.

        For unchannelized DS1/E1, all relevant timeslot bits will be set."
    ::= { juniDsx1ConfigEntry 1 }

juniDsx1Ds1ChannelNumber  OBJECT-TYPE
    SYNTAX      Integer32 (0..28)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This variable represents the channel number of the DS1/E1 on its parent
        DS3/E3.  A value of 0 indicates this DS1/E1 does not have a parent
        DS3/E3."
    ::= { juniDsx1ConfigEntry 2 }

juniDsx1Capabilities  OBJECT-TYPE
    SYNTAX      Integer32 (0..7)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A value which indicates the set of capabilities of the DS1/E1
        interface.

        The value is a sum.  This sum initially takes the value zero.  Then, for
        each capability, C, in the range 1 through 3, that this interface
        supports, 2 raised to (C - 1) is added to the sum.  For example, an
        interface which is only E1 capable would have a value of 2 (2^(2-1)).
        In contrast, an interface which is both T1 and J1 capable would have a
        value of 5 (2^(1-1) + 2^(3-1)).  The values for DS1/E1 interface
        capabilities are as follows:
            capability  function
                1       T1
                2       E1
                3       J1 "
    ::= { juniDsx1ConfigEntry 3 }

juniDsx1Mode  OBJECT-TYPE
    SYNTAX      INTEGER {
                    t1(1),
                    e1(2),
                    j1(3) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This variable represents the DS1/E1 interface mode.  The value of the
        juniDsx1Capabilities object for the DS1/E1 interface indicates the valid
        set of values for this object."
    ::= { juniDsx1ConfigEntry 4 }

juniDsx1LineBuildOutCapabilities  OBJECT-TYPE
    SYNTAX      Integer32 (0..3)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A value which indicates the set of line build out capabilities of the
        DS1/E1 interface.

        The value is a sum.  This sum initially takes the value zero.  Then, for
        each line build out capability, C, in the range 1 or 2, that this
        interface supports, 2 raised to (C - 1) is added to the sum.  For
        example, an interface which is only short haul capable would have a
        value of 2 (2^(2-1)).  In contrast, an interface which is both short
        haul and long haul capable would have a value of 3 (2^(1-1) + 2^(2-1)).
        The values for DS1/E1 interface line build out capabilities are as
        follows:
            line build out capability   function
                1                       short haul
                2                       long haul"
    ::= { juniDsx1ConfigEntry 5 }

juniDsx1LineBuildOutType  OBJECT-TYPE
    SYNTAX      INTEGER {
                    shortHaul(1),
                    longHaul(2),
                    notSupported(3) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This variable represents the configured line build out type of the
        DS1/E1 interface.  The value of the juniDsx1LineBuildOutCapabilities
        object for the DS1/E1 interface indicates the valid set of values for
        this object."
    ::= { juniDsx1ConfigEntry 6 }

juniDsx1LineAttenuation  OBJECT-TYPE
    SYNTAX      INTEGER {
                    db0(1),
                    dbMinus7Point5(2),
                    dbMinus15(3),
                    dbMinus22Point5(4),
                    notSupported(5) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This variable represents the configured line attenuation of the DS1/E1
        interface.  Note that the value of this object only takes effect when
        the value of the juniDsx1LineBuildOutType for the DS1/E1 interface is
        set to longHaul(2)."
    ::= { juniDsx1ConfigEntry 7 }

juniDsx1LineLength  OBJECT-TYPE
    SYNTAX      Integer32 (0..64000)
    UNITS       "meters"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This variable represents the length of the DS1/E1 line in meters.  Note
        that the value of this object only takes effect when the value of the
        juniDsx1LineBuildOutType for the DS1/E1 interface is set to
        shortHaul(1)."
    ::= { juniDsx1ConfigEntry 8 }

juniDsx1LowerIfIndex  OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The ifIndex of the interface over which this Dsx1 interface is to be
        layered.  A value of zero indicates no layering.  An implementation may
        choose to require that a nonzero value be configured at entry creation."
    ::= { juniDsx1ConfigEntry 9 }

juniDsx1RowStatus  OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
            juniDsx1RowStatus
            juniDsx1LowerIfIndex

        In addition, when creating an entry the following conditions must hold:

            A value for ifIndex must have been determined previously, by reading
            juniDsx1NextIfIndex.

            The interface identified by juniDsx1hLowerIfIndex must exist.

        A corresponding entry in ifTable/ifXTable/juniIfTable is created/
        destroyed as a result of creating/destroying an entry in this table."
    ::= { juniDsx1ConfigEntry 10 }

juniDsx1SendCode  OBJECT-TYPE
    SYNTAX      INTEGER {
                    sendInbandLineCode(1),
                    sendBellcoreLineCode(2),
                    sendBellcoreInbandLineCode(3),
                    sendQRSPattern(4),
                    sendAllZerosPattern(5),
                    sendAllOnesPattern(6),
                    sendAltZeroOnePattern(7),
                    sendTwo11Pattern(8),
                    sendTwo15Pattern(9),
                    sendTwo20Pattern(10),
                    sendTwo23Pattern(11),
                    sendUnfrQRSPattern(12),
                    sendUnfrAllZerosPattern(13),
                    sendUnfrAllOnesPattern(14),
                    sendUnfrAltZeroOnePattern(15),
                    sendUnfrTwo11Pattern(16),
                    sendUnfrTwo15Pattern(17),
                    sendUnfrTwo20Pattern(18),
                    sendUnfrTwo23Pattern(19),
                    otherPattern(20) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This variable indicates what type of code is being sent across the DS1
        interface by the device."
    DEFVAL    { otherPattern }
    ::= { juniDsx1ConfigEntry 11 }

juniDsx1YellowAlarm  OBJECT-TYPE
    SYNTAX      INTEGER {
                    generate(1),
                    detect(2),
                    generateAndDetect(3),
                    none(4) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This bitmap indicates the yellow alarm settings, and is the sum of the
        capabilities."
    ::= { juniDsx1ConfigEntry 12 }

juniDsx1RemoteLoopback  OBJECT-TYPE
    SYNTAX      INTEGER {
                    disabled(0),
                    enabled(1) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This variable indicates the remote loopback setting."
    DEFVAL    { disabled }
    ::= { juniDsx1ConfigEntry 13 }

juniDsx1FdlCarrier  OBJECT-TYPE
    SYNTAX      INTEGER {
                    disabled(0),
                    enabled(1) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the interface is used in carrier environment."
    DEFVAL    { disabled }
    ::= { juniDsx1ConfigEntry 14 }

juniDsx1FdlEic  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..10))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This is the equipment identification code."
    DEFVAL    { "" }
    ::= { juniDsx1ConfigEntry 15 }

juniDsx1FdlLic  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..11))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This is the location identification code."
    DEFVAL    { "" }
    ::= { juniDsx1ConfigEntry 16 }

juniDsx1FdlFic  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..10))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This is the frame identification code."
    DEFVAL    { "" }
    ::= { juniDsx1ConfigEntry 17 }

juniDsx1FdlUnit  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..6))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This is the unit identification code."
    DEFVAL    { "" }
    ::= { juniDsx1ConfigEntry 18 }

juniDsx1FdlPfi  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..38))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This is the facility identification code."
    DEFVAL    { "" }
    ::= { juniDsx1ConfigEntry 19 }

juniDsx1FdlPort  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..4))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This is the equipment port number."
    ::= { juniDsx1ConfigEntry 20 }

juniDsx1FdlGenerator  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..38))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This is the generator number."
    ::= { juniDsx1ConfigEntry 21 }

juniDsx1FdlTransmit  OBJECT-TYPE
    SYNTAX      BITS {
                    path(0),
                    idlesignal(1),
                    testsignal(2) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies transmission enabling.
            path       - Bit 0 for path transmit.  When this bit is set
                         indicates path transmit is enabled; otherwise
                         path transmit disabled.
            idlesignal - Bit 1 for idlesignal transmit.  When this bit
                         is set idlesingal transmit is enabled; otherwise
                         idlesignal transmit disabled.
            testsignal - Bit 2 for testsignal transmit.  When this bit
                         is set testsignal transmit is enabled; otherwise
                         testsignal transmit disabled.

        The value of this object defaults to zero, indicating that none of FDL
        transmit methods are enabled."
    DEFVAL    { { } }
    ::= { juniDsx1ConfigEntry 22 }

juniDs1NextIfIndex  OBJECT-TYPE
    SYNTAX      JuniNextIfIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Coordinate ifIndex value allocation for entries in juniDsx1ConfigTable.

        A GET of this object returns the next available ifIndex value to be used
        to create an entry in the associated interface table; or zero, if no
        valid ifIndex value is available.  This object also returns a value of
        zero when it is the lexicographic successor of a varbind presented in an
        SNMP GETNEXT or GETBULK request, for which circumstance it is assumed
        that ifIndex allocation is unintended.

        Successive GETs will typically return different values, thus avoiding
        collisions among cooperating management clients seeking to create table
        entries simultaneously."
    ::= { juniDs1Objects 2 }


--
-- The DS1 Far End Configuration Table contains
-- configuration information reported from the remote end.
--
juniDsx1FarEndConfigTable  OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniDsx1FarEndConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The DS1 Far End Configuration table."
    ::= { juniDs1Objects 3 }

juniDsx1FarEndConfigEntry  OBJECT-TYPE
    SYNTAX      JuniDsx1FarEndConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry in the DS1 Far End Configuration table."
    INDEX     { juniDsx1FarEndLineIndex }
    ::= { juniDsx1FarEndConfigTable 1 }

JuniDsx1FarEndConfigEntry ::= SEQUENCE {
        juniDsx1FarEndLineIndex         INTEGER,
        juniDsx1FarEndEquipCode         DisplayString,
        juniDsx1FarEndLocationIDCode    DisplayString,
        juniDsx1FarEndFrameIDCode       DisplayString,
        juniDsx1FarEndUnitCode          DisplayString,
        juniDsx1FarEndFacilityIDCode    DisplayString,
        juniDsx1FarEndPortNumber        DisplayString,
        juniDsx1FarEndGeneratorNumber   DisplayString,
        juniDsx1FarEndCarrier           INTEGER }

juniDsx1FarEndLineIndex  OBJECT-TYPE
    SYNTAX      INTEGER (1..'7fffffff'h)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The index value which uniquely identifies the DS1 interface to which
        this entry is applicable.  The interface identified by a particular
        value of this index is the same interface as identified by the same
        value a dsx1LineIndex object instance."
    ::= { juniDsx1FarEndConfigEntry 1 }

juniDsx1FarEndEquipCode  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..10))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is the Far End Equipment Identification code that describes the
        specific piece of equipment.  It is sent within the Path Identification
        Message."
    ::= { juniDsx1FarEndConfigEntry 2 }

juniDsx1FarEndLocationIDCode  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..11))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is the Far End Location Identification code that describes the
        specific location of the equipment.  It is sent within the Path
        Identification Message."
    ::= { juniDsx1FarEndConfigEntry 3 }

juniDsx1FarEndFrameIDCode  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..10))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is the Far End Frame Identification code that identifies where the
        equipment is located within a building at a given location.  It is sent
        within the Path Identification Message."
    ::= { juniDsx1FarEndConfigEntry 4 }

juniDsx1FarEndUnitCode  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..6))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This is the Far End code that identifies the equipment location within
        a bay.  It is sent within the Path Identification Message."
    ::= { juniDsx1FarEndConfigEntry 5 }

juniDsx1FarEndFacilityIDCode  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..38))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This code identifies a specific Far End DS1 path.  It is sent within
        the Path Identification Message."
    ::= { juniDsx1FarEndConfigEntry 6 }

juniDsx1FarEndPortNumber  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..4))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This code identifies the port number of the Far End DS1.  It is sent
        within the Idle Signal Message."
    ::= { juniDsx1FarEndConfigEntry 7 }

juniDsx1FarEndGeneratorNumber  OBJECT-TYPE
    SYNTAX      DisplayString (SIZE (0..38))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "This code identifies the Far End DS1 Generator Number.  It is sent
        within the Test Signal Message."
    ::= { juniDsx1FarEndConfigEntry 8 }

juniDsx1FarEndCarrier  OBJECT-TYPE
    SYNTAX      INTEGER {
                    disabled(0),
                    enabled(1) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies the interface is used in carrier environment.  It is sent
        with all FDL messages."
    ::= { juniDsx1FarEndConfigEntry 9 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Notifications
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- No notifications are defined in this MIB.  Placeholders follow.
-- juniDs1TrapControl      OBJECT IDENTIFIER ::= { juniDs1MIB 2 }
-- juniDs1Traps            OBJECT IDENTIFIER ::= { juniDs1MIB 3 }
-- juniDs1TrapPrefix       OBJECT IDENTIFIER ::= { juniDs1Traps 0 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Conformance information
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniDs1Conformance OBJECT IDENTIFIER ::= { juniDs1MIB 4 }
juniDs1Compliances OBJECT IDENTIFIER ::= { juniDs1Conformance 1 }
juniDs1Groups      OBJECT IDENTIFIER ::= { juniDs1Conformance 2 }

--
-- compliance statements
--
juniDs1Compliance  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        DS1/E1 MIB.  This statement became obsolete when new objects were
        added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniDs1Group }
    ::= { juniDs1Compliances 1 }                                   -- JUNOSe 1.0

juniDs1Compliance2  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        DS1/E1 MIB.  This statement became obsolete when dynamic DS1 interface
        support was added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniDs1Group2 }
    ::= { juniDs1Compliances 2 }                                   -- JUNOSe 1.1

juniDs1Compliance3  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        DS1/E1 MIB.  This statement became obsolete when FDL support was added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniDs1Group3 }
    ::= { juniDs1Compliances 3 }                                   -- JUNOSe 3.0

juniDs1Compliance4  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        DS1/E1 MIB. This statement became obsolete when support for remote FDL
        strings and FDL transmit mode was added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniDs1Group4 }
    ::= { juniDs1Compliances 4 }                                   -- JUNOSe 4.0

juniDs1Compliance5  MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for entities which implement the Juniper
        DS1/E1 MIB."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniDs1Group5 }
    ::= { juniDs1Compliances 5 }                                   -- JUNOSe 4.1


--
-- units of conformance
--
juniDs1Group  OBJECT-GROUP
    OBJECTS {
        juniDsx1TimeSlotMap,
        juniDsx1Ds1ChannelNumber }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of DS1/E1
        interfaces in a Juniper product.  This group became obsolete when new
        objects where added to the MIB."
    ::= { juniDs1Groups 1 }

juniDs1Group2  OBJECT-GROUP
    OBJECTS {
        juniDsx1TimeSlotMap,
        juniDsx1Ds1ChannelNumber,
        juniDsx1Capabilities,
        juniDsx1Mode,
        juniDsx1LineBuildOutCapabilities,
        juniDsx1LineBuildOutType,
        juniDsx1LineAttenuation,
        juniDsx1LineLength }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of DS1/E1
        interfaces in a Juniper product.  This group became obsolete when
        dynamic DS1 interface support was added."
    ::= { juniDs1Groups 2 }

juniDs1Group3  OBJECT-GROUP
    OBJECTS {
        juniDsx1TimeSlotMap,
        juniDsx1Ds1ChannelNumber,
        juniDsx1Capabilities,
        juniDsx1Mode,
        juniDsx1LineBuildOutCapabilities,
        juniDsx1LineBuildOutType,
        juniDsx1LineAttenuation,
        juniDsx1LineLength,
        juniDsx1LowerIfIndex,
        juniDsx1RowStatus,

        juniDs1NextIfIndex }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of DS1/E1
        interfaces in a Juniper product.  This group became obsolete when FDL
        support was added."
    ::= { juniDs1Groups 3 }

juniDs1Group4  OBJECT-GROUP
    OBJECTS {
        juniDsx1TimeSlotMap,
        juniDsx1Ds1ChannelNumber,
        juniDsx1Capabilities,
        juniDsx1Mode,
        juniDsx1LineBuildOutCapabilities,
        juniDsx1LineBuildOutType,
        juniDsx1LineAttenuation,
        juniDsx1LineLength,
        juniDsx1LowerIfIndex,
        juniDsx1RowStatus,
        juniDsx1SendCode,
        juniDsx1YellowAlarm,
        juniDsx1RemoteLoopback,
        juniDsx1FdlCarrier,
        juniDsx1FdlEic,
        juniDsx1FdlLic,
        juniDsx1FdlFic,
        juniDsx1FdlUnit,
        juniDsx1FdlPfi,
        juniDsx1FdlPort,
        juniDsx1FdlGenerator,

        juniDs1NextIfIndex }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of DS1/E1
        interfaces in a Juniper product.  This group became obsolete when
        support for remote FDL strings and FDL transmit mode was added."
    ::= { juniDs1Groups 4 }

juniDs1Group5  OBJECT-GROUP
    OBJECTS {
        juniDsx1TimeSlotMap,
        juniDsx1Ds1ChannelNumber,
        juniDsx1Capabilities,
        juniDsx1Mode,
        juniDsx1LineBuildOutCapabilities,
        juniDsx1LineBuildOutType,
        juniDsx1LineAttenuation,
        juniDsx1LineLength,
        juniDsx1LowerIfIndex,
        juniDsx1RowStatus,
        juniDsx1SendCode,
        juniDsx1YellowAlarm,
        juniDsx1RemoteLoopback,
        juniDsx1FdlCarrier,
        juniDsx1FdlEic,
        juniDsx1FdlLic,
        juniDsx1FdlFic,
        juniDsx1FdlUnit,
        juniDsx1FdlPfi,
        juniDsx1FdlPort,
        juniDsx1FdlGenerator,
        juniDsx1FdlTransmit,
        juniDsx1FarEndEquipCode,
        juniDsx1FarEndLocationIDCode,
        juniDsx1FarEndFrameIDCode,
        juniDsx1FarEndUnitCode,
        juniDsx1FarEndFacilityIDCode,
        juniDsx1FarEndPortNumber,
        juniDsx1FarEndGeneratorNumber,
        juniDsx1FarEndCarrier,

        juniDs1NextIfIndex }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing management of DS1/E1 interfaces in a
        Juniper product."
    ::= { juniDs1Groups 5 }

END
