
-- *****************************************************************************
-- Juniper-LOG-MIB
--
-- Juniper Networks Enterprise MIB
--   Extensions for Logging Management
--
-- Copyright (c) 1999 Redstone Communications, Inc.
-- Copyright (c) 1999, 2001 Unisphere Networks, Inc.
-- Copyright (c) 2002 Juniper Networks, Inc.
--   All Rights Reserved.
-- *****************************************************************************

Juniper-LOG-MIB  DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, NOTIFICATION-TYPE, OBJECT-TYPE, Integer32, Counter32,
    Unsigned32, IpAddress
        FROM SNMPv2-SMI
    TEXTUAL-CONVENTION, DisplayString, RowStatus, TruthValue, TimeStamp,
    DateAndTime
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
        FROM SNMPv2-CONF
    juniMibs
        FROM Juniper-MIBs
    JuniLogSeverity
        FROM Juniper-TC;
    
juniLogMIB  MODULE-IDENTITY
    LAST-UPDATED "200209162144Z"  -- 16-Sep-02 05:44 PM EDT
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
        "       Juniper Networks, Inc.
        Postal: 10 Technology Park Drive
                Westford, MA  01886-3146
                USA
        Tel:    +1 978 589 5800
        Email:  mib@Juniper.net"
    DESCRIPTION
        "The Logging Facility MIB for the Juniper Networks enterprise."
    -- Revision History
    REVISION    "200209162144Z"  -- 16-Sep-02 05:44 PM EDT  - JUNOSe 5.0
    DESCRIPTION
        "Replaced Unisphere names with Juniper names."
    REVISION    "200103161902Z"  -- 16-Mar-01 02:02 PM EST  - JUNOSe 3.0
    DESCRIPTION
        "Make it SMIv2 conformant."
    REVISION    "200003270500Z"  -- 27-Mar-00               - JUNOSe 2.0
    DESCRIPTION
        "Replace single syslog destination with table of syslog destinations,
        and add syslog facility as an attribute for syslogs."
    REVISION    "9911080000Z"    --  8-Nov-99               - JUNOSe 1.3
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { juniMibs 28 }

--
-- Brief Description of Logging Facility Model
--
-- A system application may support one or more logging categories.  Each
-- category can be separately configured for severity and verbosity levels of
-- the logging messages it generates in reponse to category-specific events.
-- The severity level filters the generation of messages; the verbosity level
-- controls the content of each generated message.  Each category is resource-
-- limited in the rate of messages it can generate, thus high event volume in
-- one category will not exhaust common resources to the extent that other log
-- categories are starved.
-- 
-- Generated log messages are recorded into a central circular repository,
-- called the log message table.  Each such recorded message is examined and can
-- be sent to as many as three logging destinations:  network-based SYSLOG 
-- server; local console; and local nonvolatile log file.  Each of these
-- destinations is separately configurable for severity level of messages it
-- wishes to receive.
--

-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Textual conventions
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
JuniLogCatName ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "32a"
    STATUS      current
    DESCRIPTION
        "The name of a log category.  Represents textual information taken from
        the NVT ASCII character set."
    REFERENCE
        "RFC 854: NVT ASCII character set.  See SNMPv2-TC.DisplayString
        DESCRIPTION for a summary."
    SYNTAX      OCTET STRING (SIZE (1..32))

JuniLogVerbosity ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The log verbosity level. Not all event types
        offer medium- or high-verbosity levels of detail."
    SYNTAX      INTEGER {   
                    low(0),
                    medium(1),
                    high(2) }

JuniLogSyslogFacility ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The syslog daemon facility id."
    SYNTAX      INTEGER {
                    local0(0),
                    local1(1),
                    local2(2),
                    local3(3),
                    local4(4),
                    local5(5),
                    local6(6),
                    local7(7) }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Managed objects
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniLogObjects        OBJECT IDENTIFIER ::= { juniLogMIB 1 }

juniLogDestinations   OBJECT IDENTIFIER ::= { juniLogObjects 1 }
juniLogCategories     OBJECT IDENTIFIER ::= { juniLogObjects 2 }
juniLogMessages       OBJECT IDENTIFIER ::= { juniLogObjects 3 }

-- :::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::
-- Log Destinations
-- :::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::
juniLogDestSyslog         OBJECT IDENTIFIER ::= { juniLogDestinations 1 }
juniLogDestConsole        OBJECT IDENTIFIER ::= { juniLogDestinations 2 }
juniLogDestNvFile         OBJECT IDENTIFIER ::= { juniLogDestinations 3 }

--
-- SYSLOG server log destination
--
-- Scalar objects supporting a single syslog destination are obsoleted in favor
-- of a table of syslog destinations.
--
juniLogDestSyslogSeverity OBJECT-TYPE
    SYNTAX      JuniLogSeverity   
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "The minimum severity level of messages sent to the SYSLOG server.  A
        value of 'off' indicates no log messages are sent to this destination."
    ::= { juniLogDestSyslog 1 }

juniLogDestSyslogAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "The IP address of the SYSLOG server to which log messages are to be
        sent.  A value of 0.0.0.0 indicates no server address is configured."
    ::= { juniLogDestSyslog 2 }

juniLogSyslogTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniLogSyslogEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table describing the characteristics of each syslog destination."
    ::= { juniLogDestSyslog 3 }

juniLogSyslogEntry OBJECT-TYPE
    SYNTAX      JuniLogSyslogEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry describingthe characteristics of a syslog destination."
    INDEX     { juniLogSyslogIpAddress }
    ::= { juniLogSyslogTable 1 }

JuniLogSyslogEntry ::= SEQUENCE {
    juniLogSyslogIpAddress  IpAddress,
    juniLogSyslogRowStatus  RowStatus,
    juniLogSyslogSeverity   JuniLogSeverity,
    juniLogSyslogFacility   JuniLogSyslogFacility }

juniLogSyslogIpAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The IP address of this syslog destination.  This value must be a
        unicast IP address."
    ::= { juniLogSyslogEntry 1 }

juniLogSyslogRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table.  Only
        'createAndGo' and 'destroy' are supported."
    ::= { juniLogSyslogEntry 2 }

juniLogSyslogSeverity OBJECT-TYPE
    SYNTAX      JuniLogSeverity
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The severity level for this syslog destination.  Setting this value to
        'off' suppresses log messages from being sent to this syslog
        destination."
    DEFVAL    { off }
    ::= { juniLogSyslogEntry 3 }

juniLogSyslogFacility OBJECT-TYPE
    SYNTAX      JuniLogSyslogFacility
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The facility id attached to messages sent to this syslog destination."
    DEFVAL    { local7 }
    ::= { juniLogSyslogEntry 4 }


--
-- Local console log destination
--
juniLogDestConsoleSeverity OBJECT-TYPE
    SYNTAX      JuniLogSeverity   
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The minimum severity level of messages sent to the console.  A value of
        'off' indicates no log messages are sent to this destination."
    ::= { juniLogDestConsole 1 }


--
-- Local nonvolatile file log destination
--
juniLogDestNvFileSeverity OBJECT-TYPE
    SYNTAX      JuniLogSeverity   
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The minimum severity level of messages sent to the nonvolatile log
        file.  A value of 'off' indicates no log messages are to be sent to this
        destination."
    ::= { juniLogDestNvFile 1 }


-- :::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::
-- Log Categories
-- :::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::
juniLogCatScalars        OBJECT IDENTIFIER ::= { juniLogCategories 1 }
-- reserved for attributes pertaining to all logs

-- 
-- Log Category Table
-- 
juniLogCatTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniLogCatEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table describing the characteristics of each log category."
    ::= { juniLogCategories 2 }

juniLogCatEntry OBJECT-TYPE
    SYNTAX      JuniLogCatEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry describing the characteristics of a log category." 
    INDEX   { juniLogCatIndex }
    ::= { juniLogCatTable 1 }

JuniLogCatEntry ::= SEQUENCE {
    juniLogCatIndex         Integer32,
    juniLogCatName          JuniLogCatName,
    juniLogCatDescr         DisplayString,
    juniLogCatEngineering   TruthValue,
    juniLogCatDiscards      Counter32,
    juniLogCatSeverity      JuniLogSeverity,
    juniLogCatVerbosity     JuniLogVerbosity }

juniLogCatIndex OBJECT-TYPE
    SYNTAX      Integer32 (1..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An integer index uniquely associated with a log.

        Index values do not necessarily persist across system reboots.
        Following reboot, mappings of (reboot-invariant) log category names to
        log index values is available in the juniLogCatNameTable."
    ::= { juniLogCatEntry 1 }

juniLogCatName OBJECT-TYPE
    SYNTAX      JuniLogCatName
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The name of this log category."
    ::= { juniLogCatEntry 2 }

juniLogCatDescr OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A description of the functionality for which events are recorded by
        this log category."
    ::= { juniLogCatEntry 3 }

juniLogCatEngineering OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "An indication of whether this log is intended mainly for engineering
        development and debug purposes."
    ::= { juniLogCatEntry 4 }

juniLogCatDiscards OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of messages generated by this log category that were
        discarded because of resource limitations."
    ::= { juniLogCatEntry 5 }

juniLogCatSeverity OBJECT-TYPE
    SYNTAX      JuniLogSeverity
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The severity level for this log category. 

        The value 'off' disables recording of this log category's messages.  For
        other severity level values, only messages at or above this severity
        level will be logged in juniLogMsgTable."
    ::= { juniLogCatEntry 6 }

juniLogCatVerbosity OBJECT-TYPE
    SYNTAX      JuniLogVerbosity
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The verbosity level for this log category.

        Supplementary information may be available for certain event types.
        This object controls whether that additional information, if available
        for a given event, is recorded."
    ::= { juniLogCatEntry 7}


--
-- Log Category Name Table
--
juniLogCatNameTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniLogCatNameEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table mapping each log category's name to its index."
    ::= { juniLogCategories 3 }

juniLogCatNameEntry OBJECT-TYPE
    SYNTAX      JuniLogCatNameEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An entry mapping a log category's name to its index."
    INDEX     { IMPLIED juniLogCatNameName }
    ::= { juniLogCatNameTable 1 }

JuniLogCatNameEntry ::= SEQUENCE {
    juniLogCatNameName      JuniLogCatName,
    juniLogCatNameIndex     Integer32 }

juniLogCatNameName OBJECT-TYPE
    SYNTAX      JuniLogCatName
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The name of the log category."
    ::= { juniLogCatNameEntry 1 }

juniLogCatNameIndex OBJECT-TYPE
    SYNTAX      Integer32 (1..2147483647)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The log index associated with this log category."
    ::= { juniLogCatNameEntry 2 }


-- :::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::
-- Log Messages
-- :::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::::
--
-- Log Message Scalars
--
juniLogMsgScalars     OBJECT IDENTIFIER   ::= { juniLogMessages 1 }

juniLogMsgCapacity OBJECT-TYPE
    SYNTAX      Integer32
    UNITS       "messages"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The maximum capacity, in number of log messages, of the
        juniLogMsgTable."
    ::= { juniLogMsgScalars 1 }

juniLogMsgLastSeqNumber OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The sequence number of the most recent juniLogMsgTable entry.

        By monitoring this object's rate of change in relation to the
        juniLogMsgTable capacity, a management client can determine whether it
        is polling juniLogMsgTable frequently enough to avoid missing log
        messages."
    ::= { juniLogMsgScalars 2 }


--
-- Log Message Table
--
juniLogMsgTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniLogMsgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table of log messages generated by this device."
    ::= { juniLogMessages 2 }

juniLogMsgEntry OBJECT-TYPE
    SYNTAX      JuniLogMsgEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A log message generated by this device."
    INDEX     { juniLogMsgSysUpTimeStamp,
                juniLogMsgSequenceNumber }
    ::= { juniLogMsgTable 1 }

JuniLogMsgEntry ::= SEQUENCE {
    juniLogMsgSysUpTimeStamp    TimeStamp,
    juniLogMsgSequenceNumber    Unsigned32,
    juniLogMsgCatName           JuniLogCatName,
    juniLogMsgCatIndex          Integer32,
    juniLogMsgSeverity          JuniLogSeverity,
    juniLogMsgText              DisplayString,
    juniLogMsgDateAndTimeStamp  DateAndTime }

juniLogMsgSysUpTimeStamp OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of sysUpTime when this log message was recorded."
    ::= { juniLogMsgEntry 1 }

juniLogMsgSequenceNumber OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A sequence number that uniquely identifies this entry.  Sequence
        numbers are assigned consecutively beginning with 1.  More recent
        entries have higher sequence numbers."
    ::= { juniLogMsgEntry 2 }

juniLogMsgCatName OBJECT-TYPE
    SYNTAX      JuniLogCatName
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Name of the log category that contributed this message."
    ::= { juniLogMsgEntry 3 }

juniLogMsgCatIndex OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Index of the log category that contributed this message."
    ::= { juniLogMsgEntry 4 }

juniLogMsgSeverity OBJECT-TYPE
    SYNTAX      JuniLogSeverity
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The severity of the message."
    ::= { juniLogMsgEntry 5 }

juniLogMsgText  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The text of the log message.
        
        Truncation of log message text is indicated by n asterisk character
        ('*') in the last octet of a maximum-size string."
    ::= { juniLogMsgEntry 6 }

juniLogMsgDateAndTimeStamp  OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The date and time this message was generated."
    ::= { juniLogMsgEntry 7 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Notification control objects
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniLogTrapControl      OBJECT IDENTIFIER ::= { juniLogMIB 2 }

juniLogMsgThreshold OBJECT-TYPE
    SYNTAX      Integer32 (0..100)
    UNITS       "percent"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Number of log messages which, when added to juniLogMsgTable, cause a
        juniLogMsgThresholdTrap to be generated.
        
        This value is expressed as a percentage of the capacity of
        juniLogMsgTable.  A value of zero disables trap generation."
    ::= { juniLogTrapControl 1 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Notifications
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- The following OBJECT IDENTIFIERS is used to define SNMPv2 
-- Notifications that are easily translated into SNMPv1 Traps.
juniLogTrapPrefix         OBJECT IDENTIFIER ::= { juniLogMIB 0 }

juniLogMsgThresholdTrap NOTIFICATION-TYPE
    OBJECTS {
        juniLogMsgCapacity,
        juniLogMsgLastSeqNumber,
        juniLogMsgThreshold }
    STATUS      current
    DESCRIPTION
        "This trap is generated to report that an incremental number of log
        messages (described by the value of juniLogMsgThreshold) have been added
        to juniLogMsgTable."
    ::= { juniLogTrapPrefix 1 }

-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Conformance information
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniLogMIBConformance  OBJECT IDENTIFIER ::= { juniLogMIB 4 }
juniLogMIBCompliances  OBJECT IDENTIFIER ::= { juniLogMIBConformance 1 }
juniLogMIBGroups       OBJECT IDENTIFIER ::= { juniLogMIBConformance 2 }

--
-- compliance statements
--
juniLogCompliance  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION

        "Obsolete compliance statement for entities which implement the Juniper
        Networks Log MIB.  This statement became obsolete when support for
        multiple SYSLOGs was added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniLogGroup }
    ::= { juniLogMIBCompliances 1 }                                -- JUNOSe 1.3

juniLogCompliance2  MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for entities which implement the Juniper
        Networks Log MIB, including support for multiple SYSLOG destinations."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniLogGroup2,
            juniLogTrapGroup }
    ::= { juniLogMIBCompliances 2 }                                -- JUNOSe 2.0

--
-- units of conformance
--
juniLogGroup  OBJECT-GROUP
    OBJECTS {
        -- log destinations
        juniLogDestSyslogSeverity,
        juniLogDestSyslogAddress,
        juniLogDestConsoleSeverity,
        juniLogDestNvFileSeverity,

        -- log categories
        juniLogCatName,
        juniLogCatDescr,
        juniLogCatEngineering,
        juniLogCatDiscards,
        juniLogCatSeverity,
        juniLogCatVerbosity,

        -- log category names
        juniLogCatNameName,
        juniLogCatNameIndex,

        -- log message scalars
        juniLogMsgCapacity,
        juniLogMsgLastSeqNumber,

        -- log messages
        juniLogMsgCatName,
        juniLogMsgCatIndex,
        juniLogMsgSeverity,
        juniLogMsgText,
        juniLogMsgDateAndTimeStamp,

        -- trap control
        juniLogMsgThreshold }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of Juniper Networks
        logging capabilities.  This group became obsolete when support for
        multiple SYSLOGs was added."
    ::= { juniLogMIBGroups 1 }
    
juniLogGroup2  OBJECT-GROUP
    OBJECTS {
        -- log destinations
        juniLogSyslogRowStatus,
        juniLogSyslogSeverity,
        juniLogSyslogFacility,
        juniLogDestConsoleSeverity,
        juniLogDestNvFileSeverity,

        -- log categories
        juniLogCatName,
        juniLogCatDescr,
        juniLogCatEngineering,
        juniLogCatDiscards,
        juniLogCatSeverity,
        juniLogCatVerbosity,

        -- log category names
        juniLogCatNameName,
        juniLogCatNameIndex,

        -- log message scalars
        juniLogMsgCapacity,
        juniLogMsgLastSeqNumber,

        -- log messages
        juniLogMsgCatName,
        juniLogMsgCatIndex,
        juniLogMsgSeverity,
        juniLogMsgText,
        juniLogMsgDateAndTimeStamp,

        -- trap control
        juniLogMsgThreshold }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing management of Juniper Networks
        logging capabilities, including support for multiple SYSLOG
        destinations."
    ::= { juniLogMIBGroups 2 }
    
juniLogTrapGroup NOTIFICATION-GROUP
    NOTIFICATIONS {
        juniLogMsgThresholdTrap }
    STATUS      current
    DESCRIPTION
        "A management notification pertaining to logging operations."
    ::= { juniLogMIBGroups 3 }

END
