-- *****************************************************************
-- Cisco Switch Engine MIB
--
-- February 2000, Steven To 
-- July 2000, Edward Pham 
-- February 2002, Edward Pham
-- February 2003, Edward Pham
-- May 2003, Jayakumar Kadirvelu
-- August 2003, Edward Pham
--
-- Copyright (c) 2000-2008 
-- by cisco Systems, Inc.
-- All rights reserved.
-- *****************************************************************

CISCO-SWITCH-ENGINE-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE,
    Gauge32, Counter32, Counter64, IpAddress, Integer32,
    Unsigned32
        FROM SNMPv2-SMI
    ifIndex, OwnerString, InterfaceIndexOrZero 
        FROM IF-MIB
    CiscoNetworkProtocol, CiscoPort
        FROM CISCO-TC
    ciscoMgmt
        FROM CISCO-SMI
    VlanIndex
        FROM CISCO-VTP-MIB
    InetAddressType,
    InetAddress
        FROM INET-ADDRESS-MIB
    entPhysicalIndex
        FROM ENTITY-MIB
    TEXTUAL-CONVENTION, DisplayString, RowStatus, TimeInterval, 
                              MacAddress, TruthValue, TimeStamp
        FROM SNMPv2-TC
    SnmpAdminString
        FROM SNMP-FRAMEWORK-MIB
    MplsVpnId 
        FROM MPLS-VPN-MIB
    MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF;

ciscoSwitchEngineMIB MODULE-IDENTITY
  LAST-UPDATED "200801290000Z" 
  ORGANIZATION "Cisco Systems Inc. "
  CONTACT-INFO
            "Cisco Systems        
             Customer Service

             Postal: 170 W Tasman Drive
             San Jose, CA 95134
             USA

             Tel: +1 800 553-NETS

             E-mail: cs-lan-switch-snmp@cisco.com"
  DESCRIPTION
  "This MIB module defines management objects for Cisco Layer 2/3
   switches. These devices may either have a single (central) switching
   engine entity or may consist of multiple (distributed) switching
   engine entities which are inter-connected via a common 'switching
   fabric'. In the central switching engine model, all the physical
   ports in the system are handled by the only switching engine in the
   system.  In the distributed switching model, each switching engine
   will handle a set of 'local' physical ports and when necessary,
   packets are also switched between switching engines over the
   switching fabric.
 
   Cisco L2/L3 switching devices use regular routers to assist them
   in learning packet 'flows' by observing how a router routes a
   candidate flow. A flow is some combination of source network address,
   destination network address and the transport port numbers, as
   applicable.  Once a flow is established (learned), all traffic
   belonging to that flow will be switched at Layer 3 by the switch
   engine, effectively bypassing the router, until the flow has been
   'aged' out. Most Cisco L2/L3 switching devices employ built-in
   (internal) router module(s) for integrating Layer 3 switching with
   Layer 2 forwarding. However, they can also learn 'flows' through
   other physically-separate (external) Cisco routers that are
   connected to the switch-engine through the network."
  REVISION     "200801290000Z"
  DESCRIPTION
       "Add cseL3SwitchedPktsPerSecGroup.

        Add cseCacheStatisticsGroup.
        
        Add new enumerations to cseTcamResourceType.

       Add new enumerations to cseFlowIPFlowMask object."
  REVISION     "200509160000Z"
  DESCRIPTION
       "Add cseFlowMcastMgmtGroup2.
        
        Deprecate the objects:
        cseFlowMcastQuerySrc,
        cseFlowMcastQueryGrp,
        cseFlowMcastResultGrp,
        cseFlowMcastResultSrc.

        Add new enumerations to cseFlowMcastQueryMask."
  REVISION     "200504120000Z"
  DESCRIPTION
       "Add new enumerations to cseFlowIPFlowMask object.
        Add ingressInterfaceMapping and egressInterfaceMapping
        enumerations to cseTcamResourceType object."
  REVISION     "200411150000Z"
  DESCRIPTION
       "Add cseMetUsageGroup."
  REVISION     "200406090000Z"
  DESCRIPTION
       "Add the following Groups:
        cseNetflowASInfoExportGroup
        cseNetflowPerVlanIfGroup"
  REVISION     "200311070000Z"
  DESCRIPTION
       "Add cseErrorStatsLCTable."
  REVISION     "200308200000Z"
  DESCRIPTION
      "Add the following tables to support forwarding information base:
       cseCefFibTable,
       cseCefAdjacencyTable.

       Add the following table to support TCAM (Ternary Content
       Addressable Memory) resource usage:
       cseTcamUsageTable.

       Add default value for the following objects:
       cseFlowQuerySource,
       cseFlowQuerySourceMask,
       cseFlowQueryDestination,
       cseFlowQueryDestinationMask,
       cseFlowQueryOwner."
  REVISION     "200306100000Z"
  DESCRIPTION
       "Deprecated the objects:
        cseNetflowLSExportHost,
        cseNetflowLSExportTransportNumber"
  REVISION     "200305060000Z"
  DESCRIPTION
       "Added the object cseFlowQuerySkipNFlows"
  REVISION     "200302210000Z"
  DESCRIPTION
       "Added the following objects and table: 
        cseFlowLongAgingTime, 
        cseNetFlowIfIndexEnable,
        cseFlowStatsTable,
        cseFlowExcludeTable.
        Modified the description of the following objects:
        cseL2IpPkts,
        cseL2IpxPkts,
        cseL2AssignedProtoPkts,
        cseL2OtherProtoPkts,
        cseL2HCIpPkts,
        cseL2HCIpxPkts,
        cseL2HCAssignedProtoPkts,
        cseL2HCOtherProtoPkts." 
  REVISION     "200208050000Z"
  DESCRIPTION
       "Added the following objects: cseFlowIPFlowMask,
        cseFlowIPXFlowMask, cseProtocolFilterEnable."
  REVISION     "200202070000Z"
  DESCRIPTION
       "Added the objects in cseBridgedFlowStatsCtrlTable and 
        cseErrorStatsTable.

        Added the following objects:
        cseL3VlanInUnicastPkts
        cseL3VlanInUnicastOctets
        cseL3VlanOutUnicastPkts
        cseL3VlanOutUnicastOctets."
  REVISION     "200110260000Z"
  DESCRIPTION
       "Added the object cseFlowQueryTotalFlows"
  REVISION     "200109130000Z"
  DESCRIPTION
       "Added the follwowing objects
        o cseNetflowLSFilterSupport
        o cseNetflowLSFilterTable.
       Also created the new groups 
        o cseNDEMandatoryGroup
        o cseNDESingleFilterGroup
        o cseNDEMultipleFiltersGroup"
  REVISION     "200105160000Z"
  DESCRIPTION
   "Added 4k Vlan support"
  REVISION     "200103090000Z"
  DESCRIPTION
   "Update the range of cseFlowEstablishedAgingTime,
    cseFlowIPXEstablishedAgingTime, cseFlowOperEstablishedAgingTime,
    cseFlowOperIPXAgingTime.
    Replace cseFlowQueryResult with cseFlowQueryResultingRows."
  REVISION     "200006230000Z"
  DESCRIPTION
   "Added the following objects:
    o cseFlowOperEstablishedAgingTime.
    o cseFlowOperFastAgingTime.
    o cseFlowOperFastAgePktThreshold.
    o cseFlowOperIPXAgingTime."
  REVISION
   "200001311130Z"
  DESCRIPTION
   "Added  one High Capacity L2 Statistics table, an extension
    of cseL2StatsTable and new objects in NetflowLS group for
    new netflow export features. Also added a new enum type of 
    cseRouterFlowMask to support L3 multicast."
  REVISION
   "9912091130Z"
  DESCRIPTION
   "Added MIB objects to manage Switch Engine (SE) portion of
   Multicast MLS control protocol."
  REVISION
   "9806241130Z"
  DESCRIPTION   
    "Added 2 groups, for the purging (clearing) of layer 3 unicast and
    multicast flow entries stored in the cache. Also added new objects
    for layer 3 flow statistics."
  REVISION
    "9805281130Z"
  DESCRIPTION
    "Initial version of this MIB module."
  ::= { ciscoMgmt 97 }

-- Overview of MIB Objects:
--
-- Defines 9 groups of objects.
--
-- 1. cseL2Objects: Contains mainly Layer 2 statistics maintained by the
--    switching engine hardware.
--
-- 2. cseFlow: This group has all the important objects used in the 
--    management of switching engine hardware. It contains :
--    - Scalars for configuring aging times that determine how long 
--      certain learned flows, are used for L3 switching its traffic.
--    - A table of all routers whose "flows" are learned by the 
--      switching
--      engine.
--    - A table for adding external routers to the router table and 
--      enabling
--      the switching engine to learn of all the flows through those
--routers.
--    - A table listing the MAC address and VLAN number used for each
--router.
--    - A query/result table pair for monitoring the switching 
--      performance 
--      of the switching engine(s).
--    - A control table for enabling/disabling the flow switching 
--      feature
--      per protocol type (ip, ipx).
--
-- 3. cseNetflowLS: A group of objects used to manage 
--    the Netflow LAN Switching data export feature.
--
-- 4. cseL3Objects: Contains 
--    - L3 statistics maintained by the switching engine hardware.
--    - L3 packet/octets statistics (in/out) maintained per vlan.
--
-- 5. cseProtocolFilter: Contains 
--    - Table for configuring protocol filters per (non-trunking) port.
--
-- 6. cseUcastCache: Contains
--    - a MIB table to perform actions of purging IP/IPX
--      flows in switch engine cache pools.
--
-- 7. cseMcastCache:
--    - a MIB table to perform actions of purging IP
--      multicast flows in switch engine caches.
--
-- 8. cseCef: CEF (Cisco Express Forwarding) group. It contains:
--    - tables provide information on IP forwarding database
--      and statistics.
--
-- 9. cseTcamUsage: Contains
--    - table provides resource usage information on TCAM (Ternary
--      Content Addressable Memory) in the device.
--
-- 10. cseMet: MET group. It contains:
--    - table provides resource usage information on MET (Multicast
--      Expansion Table) in the device.


cseMIBObjects OBJECT IDENTIFIER   ::= { ciscoSwitchEngineMIB 1 }

-- object groups
cseL2Objects      OBJECT IDENTIFIER    ::= { cseMIBObjects 1 }
cseFlow           OBJECT IDENTIFIER    ::= { cseMIBObjects 2 }
cseNetflowLS      OBJECT IDENTIFIER    ::= { cseMIBObjects 3 }
cseL3Objects      OBJECT IDENTIFIER    ::= { cseMIBObjects 4 }
cseProtocolFilter OBJECT IDENTIFIER    ::= { cseMIBObjects 5 }
cseUcastCache     OBJECT IDENTIFIER    ::= { cseMIBObjects 6 }
cseMcastCache     OBJECT IDENTIFIER    ::= { cseMIBObjects 7 }
cseCef            OBJECT IDENTIFIER    ::= { cseMIBObjects 8 }
cseTcamUsage      OBJECT IDENTIFIER    ::= { cseMIBObjects 9 }
cseMet            OBJECT IDENTIFIER    ::= { cseMIBObjects 10 }

CiscoGauge64 ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
        "This TC describes an object with a nonnegative integer value
        that may increase or decrease, with a maximum value of 2^64-1. 
        "
    SYNTAX Counter64

ControlStatus ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
        "This TC describes the current status of a controlled object 
        value."
    SYNTAX INTEGER { enabled(1), disabled(2) }

McastGroupIp ::= TEXTUAL-CONVENTION
    DISPLAY-HINT        "1d.1d.1d.1d"
    STATUS      current
    DESCRIPTION
        "This TC specifies an multicast group IP address,
         a class D IP address with the first byte in the range of
         224 to 239."
    SYNTAX      IpAddress

FlowAddressComponent ::= TEXTUAL-CONVENTION
        DISPLAY-HINT    "1x:"
        STATUS          current
        DESCRIPTION
          "Represents a network layer address.  The length and format of
           the address is protocol dependent as follows:
           ip              6 octets
                           first 4 octets are the IP address in network
                           order
                           last 2 bytes is the transport's port number.
           ipx             10 octets
                           first 4 octets are the net number
                           last 6 octets are the host number"
        SYNTAX          OCTET STRING (SIZE (6 | 10))


-- Layer 2 statistics per switching engine
 
cseL2StatsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF CseL2StatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table containing switching engine's L2 statistics counters."
    ::= { cseL2Objects 1 }

cseL2StatsEntry OBJECT-TYPE
    SYNTAX      CseL2StatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A conceptual row containing L2 statistics maintained by a 
         switching engine (identified by entPhysicalIndex). 
         Each switching engine managed by this MIB module has an
         entry in this table."
    INDEX  { entPhysicalIndex }
    ::= { cseL2StatsTable 1 }
 
CseL2StatsEntry ::= SEQUENCE {
        cseL2ForwardedLocalPkts   Counter32,
        cseL2ForwardedLocalOctets Counter64,
        cseL2ForwardedTotalPkts   Counter32,
        cseL2NewAddressLearns     Counter32,
        cseL2AddrLearnFailures    Counter32,
        cseL2DstAddrLookupMisses  Counter32,
        cseL2IpPkts               Counter32,
        cseL2IpxPkts              Counter32,
        cseL2AssignedProtoPkts    Counter32,
        cseL2OtherProtoPkts       Counter32
}

cseL2ForwardedLocalPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of packets received from ports local to this switching 
       engine and forwarded at layer 2."
    ::= { cseL2StatsEntry 1 }

cseL2ForwardedLocalOctets OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of octets in the packets received from ports local to this 
       switching engine and forwarded at layer 2."
    ::= { cseL2StatsEntry 2 }

cseL2ForwardedTotalPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Total number of packets received from all sources (local and over 
       the fabric) and forwarded at layer 2 by this switching engine." 
    ::= { cseL2StatsEntry 3 }

cseL2NewAddressLearns OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of new MAC addresses learned by the switching engine.
      "
    ::= { cseL2StatsEntry 4 }

cseL2AddrLearnFailures OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of MAC addresses failed to be learned because the L2 
       forwarding address table was full. If the value keeps increasing,
       the network topology should be reconfigured." 
    ::= { cseL2StatsEntry 5 }

cseL2DstAddrLookupMisses OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of misses during destination MAC address table lookups.
       A few misses happen normally.  Large numbers of misses occur as
       a result of cseL2AddrLearnFailures.
      "
    ::= { cseL2StatsEntry 6 }

cseL2IpPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of packets belonging to the IP family received by this 
       switching engine from all sources.  This value includes L3 
       switched packets."
    ::= { cseL2StatsEntry 7 }

cseL2IpxPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of packets belonging to the IPX family received by this 
       switching engine from all sources.  This value includes L3 
       switched packets." 
    ::= { cseL2StatsEntry 8 }

cseL2AssignedProtoPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of packets belonging to an assigned group of network 
       protocols (typically AppleTalk, DecNet and Vines) received 
       by this switching engine from all sources. 
       This value includes L3 switched packets."
    ::= { cseL2StatsEntry 9 }

cseL2OtherProtoPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of packets belonging to all other protocol families, 
       received by this switching engine from all sources. 
       This value includes L3 switched packets." 
    ::= { cseL2StatsEntry 10 }

-- High Capacity extensions for cseL2StatsTable.

cseL2StatsHCTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF CseL2StatsHCEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Contains the High Capacity L2 Statistics extensions  to the
cseL2StatsTable."
    ::= { cseL2Objects 2 }

cseL2StatsHCEntry OBJECT-TYPE
    SYNTAX      CseL2StatsHCEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Contains the High Capacity L2 Statistics extensions to 
        cseL2StatsEntry. These objects will be created by the agent
        for all cseL2StatsEntries it deems appropriate."
    INDEX  { entPhysicalIndex }
    ::= { cseL2StatsHCTable 1 }
 
CseL2StatsHCEntry ::= SEQUENCE {
        cseL2HCOverflowForwardedLocalPkts       Counter32,
        cseL2HCForwardedLocalPkts               Counter64,
        cseL2HCOverflowForwardedTotalPkts       Counter32,
        cseL2HCForwardedTotalPkts               Counter64,
        cseL2HCOverflowIpPkts                   Counter32,
        cseL2HCIpPkts                           Counter64,
        cseL2HCOverflowIpxPkts          Counter32,
        cseL2HCIpxPkts                          Counter64,
        cseL2HCOverflowAssignedProtoPkts      Counter32,
        cseL2HCAssignedProtoPkts                Counter64,
        cseL2HCOverflowOtherProtoPkts         Counter32,
        cseL2HCOtherProtoPkts                   Counter64       
}

cseL2HCOverflowForwardedLocalPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "The number of times the associated cseL2ForwardedLocalPkts 
       counter has overflowed."
    ::= { cseL2StatsHCEntry 1 }

cseL2HCForwardedLocalPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of packets received from ports local to this switching 
       engine and forwarded at layer 2."
    ::= { cseL2StatsHCEntry 2 }

cseL2HCOverflowForwardedTotalPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "The number of times the associated cseL2ForwardeTotalPkts counter
       has overflowed." 
    ::= { cseL2StatsHCEntry 3 }

cseL2HCForwardedTotalPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Total number of packets received from all sources 
       (local and over the fabric) and forwarded at layer 2
       by this switching engine." 
    ::= { cseL2StatsHCEntry 4 }

cseL2HCOverflowIpPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "The number of times the associated cseL2IpPkts counter
       has overflowed."
    ::= { cseL2StatsHCEntry 5 }

cseL2HCIpPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of packets belonging to the IP family received by this 
       switching engine from all sources.  This value includes 
       L3 switched packets."
    ::= { cseL2StatsHCEntry 6 }

cseL2HCOverflowIpxPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "The number of times the associated cseL2IpxPkts counter
       has overflowed."
    ::= { cseL2StatsHCEntry 7 }

cseL2HCIpxPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of packets belonging to the IPX family received by this 
       switching engine from all sources.  
       This value includes L3 switched packets."
    ::= { cseL2StatsHCEntry 8 }

cseL2HCOverflowAssignedProtoPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "The number of times the associated cseL2HCAssignedProtoPkts
       counter has overflowed."
    ::= { cseL2StatsHCEntry 9 }

cseL2HCAssignedProtoPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of packets belonging to an assigned group of network
       protocols (typically AppleTalk, DecNet and Vines) received 
       by this switching engine from all sources.
       This value includes L3 switched packets." 
    ::= { cseL2StatsHCEntry 10 }

cseL2HCOverflowOtherProtoPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "The number of times the associated cseL2HCOtherProtoPkts
       counter has overflowed."
    ::= { cseL2StatsHCEntry 11 }

cseL2HCOtherProtoPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of packets belonging to all other protocol families,
        received by this switching engine from all sources.  This value 
        includes L3 switched packets."
    ::= { cseL2StatsHCEntry 12 }

-- Flow group of objects

-- Global aging times for the flows learned

cseFlowEstablishedAgingTime OBJECT-TYPE
    SYNTAX    Integer32 (1..65535) 
    UNITS     "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The adminstrative aging time for IP established flows.
        The default value for this object is implementation specific.
        If the cseFlowEstablishedAgingTime is not configured to the
        appropriate value, it will be adjusted to the closest value.
        The corresponding operational object, taken effect on the
        a device, is cseFlowOperIPEstablishedAgingTime."
    ::= { cseFlow 1 }

cseFlowFastAgingTime OBJECT-TYPE
    SYNTAX    Unsigned32
    UNITS     "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "The administrative fast aging time for the established flow 
       entries, that have less number of packets than the value set in 
       the cseFlowFastAgePktThreshold, switched within this time. 
       Setting to value of 0 turns off fast aging.

       The default value for this object is implementation specific.
       If the cseFlowFastAgingTime is not configured to the
       appropriate value, it will be adjusted to the closest value.
       The corresponding operational object, taken effect on the
       device, is cseFlowOperFastAgingTime."
    ::= { cseFlow 2 }

cseFlowFastAgePktThreshold OBJECT-TYPE
    SYNTAX    Unsigned32
    UNITS     "packets"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "The administrative packet threshold setting for the
       cseFlowFastAgingTime. The default for Fast Aging Packet
       Threshold is 0, i.e. no packets switched within the time
       set in cseFlowFastAgingTime, after an L3 flow was established.
       If the cseFlowFastAgingTime is not configured to the
       appropriate value, it will be adjusted to the closest value.
       The corresponding operational object, taken effect on the
       device,  is cseFlowOperFastAgePktThreshold."
    ::= { cseFlow 3 }

-- Router Table

cseRouterTable OBJECT-TYPE
       SYNTAX     SEQUENCE OF CseRouterEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
         "A table containing information about all routers that are 
          discovered by the switch, including internal and external
          routers."
       ::= { cseFlow 4 }
 
cseRouterEntry OBJECT-TYPE
       SYNTAX     CseRouterEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
         "A conceptual row in the cseRouterTable containing information 
          about a router. A row appears either directly through dynamic 
          learning or indirectly through management configuration 
          (via SNMP,by creating an entry in the
          cseStaticExtRouterTable or via CLI)."
       INDEX { cseRouterIndex }
       ::= { cseRouterTable 1 }

CseRouterEntry ::= SEQUENCE {
        cseRouterIndex             IpAddress, 
        cseRouterFlowMask          INTEGER,
        cseRouterName              DisplayString,
        cseRouterStatic            TruthValue,
        cseRouterIpxFlowMask       INTEGER
}
 
cseRouterIndex    OBJECT-TYPE
       SYNTAX     IpAddress
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
         "The router's IP address which is used to uniquely identify 
          it for L3 flows."
        ::= { cseRouterEntry 1 }

cseRouterFlowMask     OBJECT-TYPE
       SYNTAX         INTEGER { dstOnly(1), srcDst(2), fullFlow(3),
                                   notApplicable(4), srcDstVlan(5) }
     
       MAX-ACCESS     read-only
       STATUS         current
       DESCRIPTION
         "The IP type of mask configured for the router represented by
         this row.  Each flow known to the switching engine has a mask
         which is applied to all packets in order to compare them to
         that flow.  Each hardware-learned flow has the mask configured
         for the router which logically forwards that flow."
       ::= { cseRouterEntry 2 }

cseRouterName     OBJECT-TYPE
       SYNTAX     DisplayString
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
         "DNS name (if available) of the router."
       ::= { cseRouterEntry 3 }

cseRouterStatic   OBJECT-TYPE
       SYNTAX     TruthValue
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "If the value of the object is true, this router was
            configured via SNMP or CLI. Otherwise, this router was
            learned automatically."
       ::= { cseRouterEntry 4 }

cseRouterIpxFlowMask     OBJECT-TYPE
      SYNTAX         INTEGER { dstOnly(1), srcDst(2), fullFlow(3),
                                   notApplicable(4) }
     
       MAX-ACCESS     read-only
       STATUS         current
       DESCRIPTION
         "The IPX type of mask configured for the router represented by
         this row.  Each flow known to the switching engine has a mask
         which is applied to all packets in order to compare them to
         that flow.  Each hardware-learned flow has the mask configured
         for the router which logically forwards that flow."
       ::= { cseRouterEntry 5 }

-- Table of external routers that are enabled. 

cseStaticExtRouterTable OBJECT-TYPE
        SYNTAX       SEQUENCE OF CseStaticExtRouterEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
          "A table of external routers which are enabled for Layer 3 IP
           switching by the switching engine. This table may contain 
           routers that have not yet been discovered by the device."
        ::= { cseFlow 5 }
 
cseStaticExtRouterEntry OBJECT-TYPE
        SYNTAX       CseStaticExtRouterEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
          "A conceptual row in the cseStaticExtRouterTable for 
           enabling an external router to be installed in the switch's 
           router table. The entry is created and deleted by using
           cseStaticRouterStatus."
        INDEX { cseRouterIndex }

        ::= { cseStaticExtRouterTable 1 }

CseStaticExtRouterEntry ::= SEQUENCE {
        cseStaticRouterName              DisplayString,
        cseStaticRouterOwner             OwnerString,
        cseStaticRouterStatus            RowStatus,
        cseStaticRouterType              BITS
--        cseStaticRouterType              OCTET STRING 
}
 
cseStaticRouterName  OBJECT-TYPE
       SYNTAX        DisplayString
       MAX-ACCESS    read-only
       STATUS        current
       DESCRIPTION
         "DNS name (if available) of the external router."
        ::= { cseStaticExtRouterEntry 1 }

cseStaticRouterOwner  OBJECT-TYPE
       SYNTAX         OwnerString
       MAX-ACCESS     read-create
       STATUS         current
       DESCRIPTION
         "String indicating the owner who created the static entry."
        ::= { cseStaticExtRouterEntry 2 }

cseStaticRouterStatus  OBJECT-TYPE
       SYNTAX          RowStatus
       MAX-ACCESS      read-create
       STATUS          current
       DESCRIPTION
         "Used to manage creation and deletion of rows in this table.
          Once a row becomes active, values within that row cannot be
          modified except by deleting and creating the row."
        ::= { cseStaticExtRouterEntry 3 }

-- per Router, per VLAN MAC address table for the flows
cseStaticRouterType  OBJECT-TYPE
       SYNTAX         BITS { unicast(0), multicast(1) }
--       SYNTAX         OCTET STRING (SIZE(1)) 
       MAX-ACCESS     read-create
       STATUS         current
       DESCRIPTION
         "Indicates if the router is included for unicast switching,
         or multicast switching, or both."
       DEFVAL         { { unicast } }
        ::= { cseStaticExtRouterEntry 4 }


cseRouterVlanTable OBJECT-TYPE
        SYNTAX        SEQUENCE OF CseRouterVlanEntry
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION
          "The table listing the MAC address used by routers on 
           particular VLANs."
        ::= { cseFlow 6 }
 
cseRouterVlanEntry OBJECT-TYPE
        SYNTAX        CseRouterVlanEntry
        MAX-ACCESS    not-accessible
        STATUS        current
        DESCRIPTION
          "A conceptual row of the cseRouterVlanTable. 
           An entry exists for each known VLAN of each known router.
          " 
        INDEX { cseRouterIndex, cseRouterMac, cseRouterVlan }
        ::= { cseRouterVlanTable 1 }

CseRouterVlanEntry ::= SEQUENCE {
        cseRouterMac      MacAddress,
        cseRouterVlan     VlanIndex,
        cseRouterProtocol BITS
--        cseRouterProtocol OCTET STRING 
}
 
cseRouterMac       OBJECT-TYPE
       SYNTAX      MacAddress
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
         "Mac address used by the router for this VLAN number."
        ::= { cseRouterVlanEntry 1 }

cseRouterVlan     OBJECT-TYPE
       SYNTAX     VlanIndex
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
          "The Vlan number associated with the router's MAC address."
        ::= { cseRouterVlanEntry 2 }

cseRouterProtocol     OBJECT-TYPE
       SYNTAX     BITS { ip(0), ipx(1) }
--       SYNTAX     OCTET STRING (SIZE(1)) 
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
          "Indicates which protocols are routed by this router on this 
           VLAN using this Mac address."
        ::= { cseRouterVlanEntry 3 }

-- Unicast Flow Query table

cseFlowMaxQueries  OBJECT-TYPE
       SYNTAX      Unsigned32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
         "Maximum number of query entries allowed to be outstanding at 
          any time, in the cseFlowQueryTable. The typical value for 
          this object is 5."
        ::= { cseFlow 7 }

cseFlowQueryTable OBJECT-TYPE
        SYNTAX     SEQUENCE OF CseFlowQueryEntry
        MAX-ACCESS not-accessible
        STATUS     current
        DESCRIPTION
          "A control table used to query the switching engine by 
           specifying retrieval criteria for L3 flows.
           The resulting data for each instance of a query in this
           table is returned in the cseFlowDataTable. 
           The maximum number of entries (rows) in this table
           cannot exceed the value returned by cseFlowMaxQueries."
        ::= { cseFlow 8 }
 
cseFlowQueryEntry OBJECT-TYPE
        SYNTAX     CseFlowQueryEntry
        MAX-ACCESS not-accessible
        STATUS     current
        DESCRIPTION
          "A conceptual row of the cesFlowQueryTable used to setup 
           retrieval criteria to search for L3 flows on a particular 
           switching engine entity identified by entPhysicalIndex.
           The actual search is started by setting the value of 
           cseFlowQueryStatus to 'active'. Once a row becomes active,
           values within the row cannot be modified, except by
           deleting and re-creating the row."
        INDEX { entPhysicalIndex, cseFlowQueryIndex }
        ::= { cseFlowQueryTable 1 }

CseFlowQueryEntry ::= SEQUENCE {
        cseFlowQueryIndex             Unsigned32, 
        cseFlowQueryMask              INTEGER, 
        cseFlowQueryTransport         BITS,
--        cseFlowQueryTransport         OCTET STRING,
        cseFlowQuerySource            FlowAddressComponent,
        cseFlowQuerySourceMask        FlowAddressComponent,
        cseFlowQueryDestination       FlowAddressComponent,
        cseFlowQueryDestinationMask   FlowAddressComponent,
        cseFlowQueryRouterIndex       IpAddress,
        cseFlowQueryOwner             OwnerString,
        cseFlowQueryResultingRows     Integer32, 
        cseFlowQueryResultTotalPkts   CiscoGauge64,
        cseFlowQueryResultTotalOctets CiscoGauge64,
        cseFlowQueryResultAvgDuration TimeInterval,
        cseFlowQueryResultAvgIdle     TimeInterval,
        cseFlowQueryStatus            RowStatus,
        cseFlowQueryCreateTime        TimeStamp,
        cseFlowQueryTotalFlows        Unsigned32,
        cseFlowQuerySkipNFlows        Integer32
}

cseFlowQueryIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
      "An arbitrary integer which uniquely identifies the control
      query among all those specified for the switching engine
      indicated by entPhysicalIndex."
    ::= { cseFlowQueryEntry 1 }

cseFlowQueryMask OBJECT-TYPE
    SYNTAX     INTEGER { dstOnly(1), 
                         srcOrDst(2),
                         srcAndDst(3),
                         fullFlow(4),
                         ipxDstOnly(5),
                         ipxSrcAndDst(6),
                         any(7)
                       }
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
          "Setting each value causes the appropriate action:

           'dstOnly' - causes the creation of rows in the
          cseFlowDataTable corresponding to the current L3 flow 
          information for the absolute destination IP address 
          set in the cseFlowQueryDestination object in this table. 
          If cseFlowQueryDestinationMask is also specified at the 
          same time, it will be applied to the address part of
          cseFlowQueryDestination.

           'srcOrDst' -  causes the creation of rows in the
          cseFlowDataTable corresponding to the current L3 flow 
          information for EITHER of the absolute IP addresses set in 
          the cseFlowQueryDestination or cseFlowQuerySource objects. 
          If either of cseFlowQueryDestinationMask and
          cseFlowQuerySourceMask
          objects are also specified at the same time, 
          they will be applied to the respective address parts 
          of cseFlowQueryDestination and cseFlowQuerySource
          objects. This option is typically used to 
          setup queries for flows on traffic in either directions.

           'srcAndDst' -  causes the creation of rows in the
          cseFlowDataTable corresponding to the current L3 flow 
          information for BOTH the absolute IP addresses set in 
          the cseFlowQueryDestination and cseFlowQuerySource objects. 
          If either of cseFlowQueryDestinationMask and
          cseFlowQuerySourceMask objects are also specified
          at the same time, they will be applied to the 
          respective address parts of cseFlowQueryDestination and 
          cseFlowQuerySource objects. This option is typically used to 
          setup queries for flows on traffic in one direction only.


           'fullFlow' -  causes the creation of row(s) in the
          cseFlowDataTable exactly corresponding to the current
          L3 flow information for the complete IP flow (including the 
          transport port numbers) set in the cseFlowQueryDestination and 
          cseFlowQuerySource objects. If either of
          cseFlowQueryDestinationMask and cseFlowQuerySourceMask
          objects are also specified at the same
          time, they will be applied to the respective address parts of 
          cseFlowQueryDestination and cseFlowQuerySource objects. 
          This option is typically used to setup queries for flows
          on traffic for specific (TCP/UDP) port numbers
          corresponding to standard protocols such as FTP, 
          WWW, TELNET, etc.

           'ipxDstOnly' - causes the creation of rows in the
          cseFlowDataTable corresponding to the current L3 flow
          information for the absolute destination IPX address
          set in the cseFlowQueryDestination object in this table.
          If cseFlowQueryDestinationMask is also specified at 
          the same time, it will be applied to the address part
          of cseFlowQueryDestination.

           'ipxSrcAndDst' - causes the creation of rows in the
          cseFlowDataTable corresponding to the current L3 flow
          information for BOTH the absolute IPX addresses set in
          the cseFlowQueryDestination and cseFlowQuerySource objects.
          If either of cseFlowQueryDestinationMask and
          cseFlowQuerySourceMask objects are also specified at the 
          same time, they will be applied to the respective address
          parts of cseFlowQueryDestination and
          cseFlowQuerySource objects. 

           'any' - returns all rows corresponding to all established 
          flow entries in the cseFlowDataTable.

           Note: 
           1. The type FlowAddressComponent used for objects 
              cseFlowQuerySource and cseFlowQueryDestination, has the
              network address part and also the transport port 
              number part, if applicable.
           2. The value of this object cannot be modified when the 
              corresponding instance of cseFlowQueryStatus is 'active'."
  DEFVAL { any }
  ::= { cseFlowQueryEntry 2 }

cseFlowQueryTransport OBJECT-TYPE
    SYNTAX      BITS { udp(0), tcp(1) }
--    SYNTAX      OCTET STRING (SIZE(1)) 
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
      "The IP transport protocol type specified for this query. Ignored
       for IPX flow queries. The value of this object cannot be 
       modified when the corresponding instance of cseFlowQueryStatus 
       is 'active'."
    DEFVAL {{ udp, tcp }}
    ::= { cseFlowQueryEntry 3 }
 
cseFlowQuerySource OBJECT-TYPE
    SYNTAX      FlowAddressComponent
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
      "The source network address and port (if applicable). The 
       value of this object cannot be modified when the 
       corresponding instance of 
       cseFlowQueryStatus is 'active'."
    DEFVAL { '000000000000'H }
    ::= { cseFlowQueryEntry 4 }
 
cseFlowQuerySourceMask OBJECT-TYPE
    SYNTAX      FlowAddressComponent
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
      "The source address mask to be applied to the corresponding 
       instance of cseFlowQuerySource. The value of this object
       cannot be modified  when the corresponding instance of 
       cseFlowQueryStatus is 'active'."
    DEFVAL  { 'FFFFFFFFFFFF'H }
    ::= { cseFlowQueryEntry 5 }

 
cseFlowQueryDestination OBJECT-TYPE
    SYNTAX      FlowAddressComponent
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
      "The destination network address and port (if applicable). 
       The value of this object cannot be modified when the
       corresponding instance of cseFlowQueryStatus is 'active'."
    DEFVAL { '000000000000'H }
    ::= { cseFlowQueryEntry 6 }
 
cseFlowQueryDestinationMask OBJECT-TYPE
    SYNTAX      FlowAddressComponent
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
      "The destination address mask to be applied to the corresponding 
       instance of cseFlowQueryDestination. The value of this object 
       cannot be modified when the corresponding instance of 
       cseFlowQueryStatus is 'active'."
    DEFVAL  { 'FFFFFFFFFFFF'H }
    ::= { cseFlowQueryEntry 7 }
 
cseFlowQueryRouterIndex     OBJECT-TYPE
    SYNTAX     IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
      "Index of the router for which the flows are available. 
       An 'all-zero' IP address indicates that the query is for 
       any router. The value of this object cannot be modified
       when the corresponding instance of cseFlowQueryStatus
       is 'active'."
    ::= { cseFlowQueryEntry 8 }
 
cseFlowQueryOwner OBJECT-TYPE
    SYNTAX      OwnerString
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
      "The manager entity that configured this entry and is therefore 
       using the resources assigned to it."
    DEFVAL { "" }
    ::= { cseFlowQueryEntry 9 }

cseFlowQueryResultingRows OBJECT-TYPE
    SYNTAX     Integer32 (-1..2147483647 )
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "The result status of the query. Possible values are:

   -1            - Either the query has not been initiated or 
                   the agent is busy processing this query instance.
                   Time to completion of the query processing
                   depends on the complexity of the query and
                   the number of matches that satisfy this query.

   0..2147483647 - The search has ended and this is the number of 
                   rows in the cseFlowDataTable, resulting 
                   from this query."
    ::= { cseFlowQueryEntry 10 }

cseFlowQueryResultTotalPkts    OBJECT-TYPE
    SYNTAX      CiscoGauge64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "The aggregate number of total packets switched by the system on 
       all the flows matching this query. This is a snapshot value and 
       is valid only when the corresponding instance of
       cseFlowQueryResultingRows is greater than  or equal to 0." 
    ::= { cseFlowQueryEntry 11 }

cseFlowQueryResultTotalOctets  OBJECT-TYPE
    SYNTAX      CiscoGauge64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "The aggregate number of total octets switched by the system on 
        all the flows matching this query. This is a snapshot value 
        and is valid only when the corresponding instance of
        cseFlowQueryResultingRows is greater than or equal to 0." 
    ::= { cseFlowQueryEntry 12 }

cseFlowQueryResultAvgDuration  OBJECT-TYPE
    SYNTAX      TimeInterval
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "The average duration of the flows matching this query. This is 
        a snapshot value and is valid only when the corresponding 
        instance of cseFlowQueryResultingRows is greater
        than or equal to 0." 
    ::= { cseFlowQueryEntry 13 }

cseFlowQueryResultAvgIdle  OBJECT-TYPE
    SYNTAX      TimeInterval
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
       "The elapsed time since the flows were last used, averaged over 
        all flows matching this query. This is a snapshot value 
        and is valid only when the corresponding instance of
        cseFlowQueryResultingRows is greater than or equal to 0." 
    ::= { cseFlowQueryEntry 14 }

cseFlowQueryStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The status object used to manage rows in this table. 
         When set to active(1), the query is initiated. 
         Once initiated, the value may 
         not be modified until the value of cseFlowQueryResultingRows is
         greater than or equal to 0. However, this object can be set to
         active(1) only after all the appropriate objects for this query
         as defined by the value set in the cseFlowQueryMask object,
         have also been set.
         Once a row becomes active, values within the row cannot
         be modified, except by deleting and re-creating it."
    ::= { cseFlowQueryEntry 15 }

cseFlowQueryCreateTime OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Time when this query was created."
    ::= { cseFlowQueryEntry 16 }

cseFlowQueryTotalFlows OBJECT-TYPE
    SYNTAX      Unsigned32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of L3 flows matching the query criterion."
    ::= { cseFlowQueryEntry 17 }

cseFlowQuerySkipNFlows OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The number of searched flows to be skipped before storing
        any L3 flows in cseFlowDataTable.

        This object can be used along with cseFloQueryTotalFlows
        object to skip previously found flows by setting the variable
        equal to the number of the associated rows in
        cseFlowDataTable, and only query the remaining flows
        in the table.

        Note that due to the dynamical nature of the L3 flows, the
        queried flows may be missed or repeated by setting this object.

        The value of this object cannot be modified
        when the corresponding instance of cseFlowQueryStatus
        is 'active'."
    DEFVAL      { 0 }
    ::= { cseFlowQueryEntry 18 }



-- The Unicast Flow query results data table 

cseFlowDataTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF CseFlowDataEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table containing L3 flow information corresponding to all 
         the completed queries setup in the cseFlowQueryTable, that were 
         initiated on the switch engine(s)."
    ::= { cseFlow 9 }


cseFlowDataEntry OBJECT-TYPE
        SYNTAX     CseFlowDataEntry
        MAX-ACCESS not-accessible
        STATUS     current
        DESCRIPTION
            "A conceptual row of the cseFlowDataTable used to return 
             information about one of the L3 flows which matched the 
             search criteria set by the cseFlowQueryMask object in the 
             corresponding instance of the cseFlowQueryTable."
        INDEX { entPhysicalIndex, cseFlowQueryIndex, cseFlowDataIndex }
        ::= { cseFlowDataTable 1 }
 
CseFlowDataEntry ::= SEQUENCE {
        cseFlowDataIndex          Unsigned32,
        cseFlowDataSrcMac         MacAddress,
        cseFlowDataDstMac         MacAddress,
        cseFlowDataStaticFlow     TruthValue,
        cseFlowDataEncapType      INTEGER,
        cseFlowDataSource         FlowAddressComponent,
        cseFlowDataDestination    FlowAddressComponent,
        cseFlowDataDestVlan       VlanIndex,
        cseFlowDataIpQOS          Integer32, 
        cseFlowDataIpQOSPolicy    Integer32, 
        cseFlowDataWhenCreated    TimeStamp,
        cseFlowDataLastUsed       TimeStamp,
        cseFlowDataPkts           Gauge32,
        cseFlowDataOctets         CiscoGauge64
}

cseFlowDataIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
      "A number to uniquely identify a result entry that matches a 
       particular query for a specific switching engine." 
    ::= { cseFlowDataEntry 1 }
 
cseFlowDataSrcMac OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Source Mac Address of the router's outgoing interface."
    ::= { cseFlowDataEntry 2 }
 
cseFlowDataDstMac OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Destination Mac Address used to forward the packets in 
       this flow."
    ::= { cseFlowDataEntry 3 }
 
cseFlowDataStaticFlow OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Indicates whether this flow was software-installed."
    ::= { cseFlowDataEntry 4 }
 
cseFlowDataEncapType OBJECT-TYPE
    SYNTAX      INTEGER { ipArpa(1), ipxEthernet(2), ipx802raw(3), 
                          ipx802sap(4), ipx802snap(5), other(6) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Protocol encapsulation type used to forward packets in this flow
       to their destination."
    ::= { cseFlowDataEntry 5 }
 
cseFlowDataSource OBJECT-TYPE
    SYNTAX      FlowAddressComponent
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "The source network address and the port (if appropriate) of this
       flow."
    ::= { cseFlowDataEntry 6 }
 
cseFlowDataDestination OBJECT-TYPE
    SYNTAX      FlowAddressComponent
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "The destination network address and port (if appropriate) of this
       flow."
    ::= { cseFlowDataEntry 7 }

cseFlowDataDestVlan OBJECT-TYPE
    SYNTAX      VlanIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "The vlan number on which packets belonging to this flow are
forwarded."
    ::= { cseFlowDataEntry 8 }
 
cseFlowDataIpQOS OBJECT-TYPE
    SYNTAX      Integer32 (0..7)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      " Level of Quality of service for this IP flow.
        If it is not an IP flow, this object will not be instantiated."
    ::= { cseFlowDataEntry 9 }
 
cseFlowDataIpQOSPolicy OBJECT-TYPE
    SYNTAX      Integer32 (0..7)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Level of the Quality of service policy for this IP flow.
       If it is not an IP flow, this object will not be instantiated."
    ::= { cseFlowDataEntry 10 }
 
cseFlowDataWhenCreated OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Time when this flow was created in the switching engine."
    ::= { cseFlowDataEntry 11 }
 
cseFlowDataLastUsed OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Time since this flow was last used to forward a packet by the 
       switching engine."
    ::= { cseFlowDataEntry 12 }
 
cseFlowDataPkts OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "A snapshot value of the number of packets forwarded on this flow 
       at the time of corresponding query."
    ::= { cseFlowDataEntry 13 }
 
cseFlowDataOctets OBJECT-TYPE
    SYNTAX      CiscoGauge64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "A snapshot value of octets forwarded on this flow at the time of 
       corresponding query."
    ::= { cseFlowDataEntry 14 }
 
cseFlowSwitchControlTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF CseFlowSwitchControlEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
      "A table used to control the L3 flow switching operation, per 
       protocol type."
    ::= { cseFlow 10 }

cseFlowSwitchControlEntry OBJECT-TYPE
    SYNTAX     CseFlowSwitchControlEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
      "A conceptual row for the configuration of Flow switching
       feature for an L3 protocol type."
    INDEX     { cseFlowSwitchProtocol }
    ::= { cseFlowSwitchControlTable 1 }

CseFlowSwitchControlEntry ::= SEQUENCE {
        cseFlowSwitchProtocol     CiscoNetworkProtocol,
        cseFlowSwitchStatus       ControlStatus
}

cseFlowSwitchProtocol OBJECT-TYPE
    SYNTAX     CiscoNetworkProtocol
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
      "Protocol type for which this row instance. Only ip(1) and ipx(14)
       values are currently supported."
    ::= { cseFlowSwitchControlEntry 1 }

cseFlowSwitchStatus OBJECT-TYPE
    SYNTAX     ControlStatus
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
      "The current status of the global flow switching capability for
       the specified L3 protocol type."
    ::= { cseFlowSwitchControlEntry 2 }

-- Multicast Flow Query table

cseFlowMcastMaxQueries OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Maximum number of query entries allowed to be outstanding
        at any time, in the cseFlowMcastQueryTable.  The typical value
        for this object is 5."
    ::= { cseFlow 11 }

cseFlowMcastQueryTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF CseFlowMcastQueryEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A control table used to query the switching engine by
        specifying retrieval criteria for IP multicast L3 flows.
        Each row instance in the table represents a query with
        its parameters.  The resulting data for each instance of
        a query in this table is returned in the 
        cseFlowMcastResultTable.
        The maximum number of entries (rows) in this table cannot
        exceed the value of cseFlowMcastMaxQueries object.

        Unlike unicast switched layer 3 flows, an IP multicast
        switched flow is created and installed by software, and
        is uniquely identified by flow's source IP address, and
        multicast group IP address.  It is stored with input Vlan
        ID in the cache entry, so that the packets in the flow
        will not be replicated and forwarded to the receivers on the
        same (input) Vlan.
        Another difference is that all IP multicast hardware
        switched flows belonging to the same (source, group) are
        stored only on one switch engine on a Cisco L3 switch with
        distributed switch engines, whereas unicast flows identified
        by certain criterion may resident on multiple switch engines 
        in the system."
    ::= {  cseFlow 12 }

cseFlowMcastQueryEntry OBJECT-TYPE
    SYNTAX      CseFlowMcastQueryEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A conceptual row of the cesMcastFlowQueryTable used to
        setup retrieval criteria to search for IP multicast L3
        flows on all switching engine entities in the device.
        The actual search is started by setting the value of
        cseFlowMcastQueryStatus to 'active'.  Once a row becomes
        active, values within the row cannot be modified, without
        setting the associated RowStatus object to 'notInService'
        first, or deleting and re-creating the row."
    INDEX { cseFlowMcastQueryIndex }
    ::= { cseFlowMcastQueryTable 1 }

CseFlowMcastQueryEntry ::= SEQUENCE {
        cseFlowMcastQueryIndex      Unsigned32,
        cseFlowMcastQueryMask       BITS,
        cseFlowMcastQuerySrc        IpAddress,
        cseFlowMcastQueryGrp        McastGroupIp,
        cseFlowMcastQuerySrcVlan    VlanIndex,
        cseFlowMcastQueryRtrIndex   IpAddress,
        cseFlowMcastQuerySkipNFlows Integer32,
        cseFlowMcastQueryOwner      OwnerString,
        cseFlowMcastQueryTotalFlows Integer32,
        cseFlowMcastQueryRows       Integer32,
        cseFlowMcastQueryStatus     RowStatus,
        cseFlowMcastQueryCreateTime TimeStamp,
        cseFlowMcastQueryMvrf       MplsVpnId,
        cseFlowMcastQueryAddrType   InetAddressType,
        cseFlowMcastQuerySource     InetAddress,
        cseFlowMcastQueryGroup      InetAddress
}

cseFlowMcastQueryIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An arbitrary integer in the range of 1 to 
         cseFlowMcastMaxQueries to identify this control query."
    ::= { cseFlowMcastQueryEntry 1 }

cseFlowMcastQueryMask OBJECT-TYPE
    SYNTAX      BITS { source(0), group(1), vlan(2), router(3),
                       mvrf(4) , sourceip(5), groupip(6) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This object is used to set up the query criterion for
        the multicast flows of interest.  If any one of the
        defined BITs is set, then the value of the corresponding
        object in the same row instance will be used for the search.
        
        Specifically, if the 'source(0)' BIT is set, then the 
        cseFlowMcastQuerySrc object will be included in the
        search criterion.

        If the group(1) BIT is set, then the 
        cseFlowMcastQueryGrp object will be included in the
        search criterion.

        If the vlan(2) BIT is set, then the 
        cseFlowMcastQuerySrcVlan object will be included in the 
        search criterion.

        If the router(3) BIT is set, then the
        cseFlowMcastQueryRtrIndex object will be included in the
        search criterion.

        If the mvrf(4) BIT is set, then the
        cseFlowMcastQueryMvrf object will be included in the 
        search criterion; 

        If the sourceip(5) BIT is set, then the
        cseFlowMcastQueryAddrType and cseFlowMcastQuerySource
        objects will be included in the search criterion.

        If the groupip(6) BIT is set, then the
        cseFlowMcastQueryAddrType and cseFlowMcastQueryGroup
        objects will be included in the search criterion.

        If the source(0) or group(1) BIT is set, then the
        sourceip(5) or groupip(6) cannot be set, and vice-versa.

        If any of the BITs in this variable is cleared, the 
        corresponding parameter object in the same row is 
        treated as a wildcard.  When the row is instantiated,
        the BITs in the variable will be cleared, and none of
        query parameter objects in this row will be instantiated.
        This will be considered as a wildcard search for flows
        on the default Multicast Virtual Private Network (MVPN)
        routing/forwarding (MVRF) instance. 
        i.e. it will return all rows corresponding 
        to all established multicast flow entries in the default
        MVRF, in cseFlowMcastResultTable. The address type of this
        wildcard search will be specified be cseFlowMcastQueryAddrType.
        It is SNMP managers' responsibility to set certain
        bits on in this object instance, if necessary,
        and the corresponding flow parameter variables to the 
        appropriate values in order to setup the desired
        query criteria.
        The value of this object can not be altered when the 
        corresponding instance of cseFlowMcastQueryStatus is 'active'."
       DEFVAL      { {} }
    ::= { cseFlowMcastQueryEntry 2 }
    
cseFlowMcastQuerySrc OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      deprecated
    DESCRIPTION
        "The source address of the IP multicast layer 3 flows.
        This object should be instantiated and assigned a
        proper IP address whenever the 'source' bit of
        cseFlowMcastQueryMask object in the same row is on.
        If the 'source' bit is set, and an appropriate IP address
        is assigned to this object, then only flows with the
        specified source address will be containing in the 
        result table.
        If the 'source' bit in the associated cseFlowMcastQueryMask
        is cleared, this object is ignored during the query, and all
        flows will be considered regardless of their source IP address.

        This object is deprecated and replaced by
        cseFlowMcastQueryAddrType and cseFlowMcastQuerySource."
    ::= { cseFlowMcastQueryEntry 3 }

cseFlowMcastQueryGrp OBJECT-TYPE
    SYNTAX      McastGroupIp
    MAX-ACCESS  read-create
    STATUS      deprecated
    DESCRIPTION
        "The IP multicast group address of the queried flows.
        This object should be instantiated and set whenever
        the 'group' bit of the associated cseFlowMcastQueryMask object
        is on.
        If the 'group' bit is set, and a multicast group address is 
        assigned to the object, only flows with the specified group
        address will be contained in the result table.
        If the 'group' bit in the associated cseFlowMcastQueryMask
        is cleared, this object is ignored during the query, and all
        flows will be considered regardless of their group address.

        This object is deprecated and replaced by 
        cseFlowMcastQueryAddrType and cseFlowMcastQueryGroup."
    ::= { cseFlowMcastQueryEntry 4 }

cseFlowMcastQuerySrcVlan OBJECT-TYPE
    SYNTAX      VlanIndex
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The source Vlan ID of the IP multicast layer 3 flows.
        This object should be instantiated and set whenever
        the 'vlan' bit of the associated cseFlowMcastQueryMask object
        is on.
        If the 'vlan' bit is set, and a Vlan ID is assigned to this
        object, only flows belonging to that vlan will be contained
        in the result table.
        If the 'vlan' bit in the associated cseFlowMcastQueryMask object
        is cleared, this object is ignored during the query, and all
        flows will be considered regardless of their vlan IDs."
    ::= { cseFlowMcastQueryEntry 5 }

cseFlowMcastQueryRtrIndex OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Index of the router for which the multicast flows are 
        available, that is the flows would be replicated
        and routed by the specified
        router, should the flows did not get switched.
        This object should be instantiated and set whenever the 'router'
        bit of the asociated cseFlowMcastQueryMask object is on.
        If the 'router' bit is set, and a router's IP address 
        is assigned to this object, then only flows associated with
        that router will be contained in the result table.
        If the 'router' bit in the cseFlowMcastQueryMask object
        is cleared, this object is ignored during the query, and all
        flows will be considered regardless of the routers 
        being switched."
    ::= { cseFlowMcastQueryEntry 6 }

cseFlowMcastQuerySkipNFlows OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The number of searched flows to be skipped before storing
        any multicast flows in cseFlowMcastResultTable.
        This object can be used along with cseFlowMcastQueryTotalFlows
        object to skip previously found flows by setting the variable
        equal to the number of the associated rows in 
        cseFlowMcastResultTable, and only query the remaining flows
        in the table.
        Note that due to the dynamical nature of the L3 flows, the
        queried flows may be missed or repeated by setting this object."
    DEFVAL      { 0 }
    ::= { cseFlowMcastQueryEntry 7 }

cseFlowMcastQueryOwner OBJECT-TYPE
    SYNTAX      OwnerString
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
      "The manager entity that configured this entry and is therefore
       using the resources assigned to it.  It is used to model an
       administratively assigned name of the owner of a resource.
       It is recommended that this object have one or more the following
       information: IP address, management station name, network
       manager's name, location, or phone number."
    ::= { cseFlowMcastQueryEntry 8 }

cseFlowMcastQueryTotalFlows OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of flows matching the query criterion."
    ::= { cseFlowMcastQueryEntry 9 }

cseFlowMcastQueryRows OBJECT-TYPE
    SYNTAX      Integer32 (-1..2147483647)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicating the status of the query by following values:
        -1 - Either the query has not been started or the
             agent is still processing this query instance.
             It is the default value when the row is instantiated.

        0..2147483647 - The search has ended and this is the
                        number of rows in the cseFlowMcastResultTable,
                        resulting from this query."
    ::= { cseFlowMcastQueryEntry 10 }

cseFlowMcastQueryStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The status object used to manage rows in this table.
        When set to 'active', the query of flows is initiated.
        This object can be set to active only after all the
        appropriate objects for this query as defined by the
        bits in the cseFlowMcastQueryMask object, have also been
        instantiated.  The completion of the query is indicated
        by the value of cseFlowMcastQueryRows as soon as it
        becomes greater than or equal to 0.
        Once a row becomes active, values within the row cannot be
        modified without setting it to 'notInService' first, or just
        deleting and re-creating it.
        To abort a lengthy on-going query, setting this object to
        'notInService', or 'destroy' will terminate a search
        if one is in progress, and cause the associated rows in
        cseFlowMcastResultTable, if any, to be deleted."
    ::= { cseFlowMcastQueryEntry 11 }

cseFlowMcastQueryCreateTime OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Time when this query was last set to active."
    ::= { cseFlowMcastQueryEntry 12 }

cseFlowMcastQueryMvrf OBJECT-TYPE
    SYNTAX      MplsVpnId
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The human-readable name of the Multicast 
        Virtual Private Network (MVPN) routing/forwarding
        instance (MVRF). When the 'mvrf' bit of
        cseFlowMcastQueryMask object in the same row is on,
        an appropriate value should be specified and only flows
        with the specified MVRF name will be contained in the
        result table. If the 'mvrf' bit in the associated
        cseFlowMcastQueryMask is cleared, this object is ignored
        during the query, and all the flows corresponding to the
        default MVRF will be considered."
    ::= { cseFlowMcastQueryEntry 13 }

cseFlowMcastQueryAddrType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The Internet address type for this multicast search
         query."
    DEFVAL      { ipv4 }
   ::= { cseFlowMcastQueryEntry 14 }

cseFlowMcastQuerySource OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The source Internet address of the IP multicast layer 3 
        flows. When the 'sourceip' bit of cseFlowMcastQueryMask
        cseFlowMcastQueryMask object in the same row is on,
        an appropriate value should be specified and only flows
        with the specified source address will be contained in the
        result table. If the 'sourceip' bit in the associated
        cseFlowMcastQueryMask is cleared, this object is ignored
        during the query, and all flows will be considered regardless
        of their source address.

        The type of this address is determined by the value of the 
        cseFlowMcastQueryAddrType object.
        
        The default value of this object is all zeros."
    DEFVAL { '00000000'H } -- 0.0.0.0
    ::= { cseFlowMcastQueryEntry 15 }

cseFlowMcastQueryGroup OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The multicast group Internet address of the queried flows.
        When the 'mvrf' bit of cseFlowMcastQueryMask object 
        in the same row is on, an appropriate value should be 
        specified and only flows with the specified group address
        will be contained in the result table. If the 'groupip' bit 
        in the associated cseFlowMcastQueryMask is cleared, this 
        object is ignored during the query, and all flows will
        be considered regardless of their group address.

        The type of this address is determined by the value of the
        cseFlowMcastQueryAddrType object.

        The default value of this object is all zeros."
    DEFVAL { '00000000'H } -- 0.0.0.0
    ::= { cseFlowMcastQueryEntry 16 }
    
-- The multicast flow query result data table

cseFlowMcastResultTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF CseFlowMcastResultEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A table containing current IP multicast flow information
        corresponding to all the completed queries set up in
        the cseFlowMcastQueryTable, that were initiated on the switch
        engine(s).  The query result will not become available until
        the current search completes."
    ::= { cseFlow 13 }

cseFlowMcastResultEntry OBJECT-TYPE
    SYNTAX      CseFlowMcastResultEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A conceptual row of cseFlowMcastResultTable, containing
        information about an IP multicast layer 3 flow that matchs
        the search criteria set in the corresponding row of
        cseFlowMcastQueryTable.  This row instance is indexed by
        the query index (cseFlowMcastQueryIndex), the switch engine
        entity (entPhysicalIndex), and data entry index
        (cseFlowMcastResultIndex).  The value of entPhysicalIndex
        object is assigned by Entity-MIB, and uniquely identifies
        a switching engine on which the IP multicast flow is stored."
    INDEX { cseFlowMcastQueryIndex, entPhysicalIndex,
            cseFlowMcastResultIndex }
    ::= { cseFlowMcastResultTable 1 }

CseFlowMcastResultEntry ::= SEQUENCE {
        cseFlowMcastResultIndex      Integer32,
        cseFlowMcastResultGrp        McastGroupIp,
        cseFlowMcastResultSrc        IpAddress,
        cseFlowMcastResultSrcVlan    VlanIndex,
        cseFlowMcastResultRtrIp      IpAddress,
        cseFlowMcastResultRtrMac     MacAddress,
        cseFlowMcastResultCreatedTS  TimeStamp,
        cseFlowMcastResultLastUsedTS TimeStamp,
        cseFlowMcastResultPkts       Counter64,
        cseFlowMcastResultOctets     Counter64,
        cseFlowMcastResultDstVlans   OCTET STRING,
        cseFlowMcastResultDstVlans2k OCTET STRING,
        cseFlowMcastResultDstVlans3k OCTET STRING,
        cseFlowMcastResultDstVlans4k OCTET STRING,
        cseFlowMcastResultMvrf       MplsVpnId,
        cseFlowMcastResultAddrType   InetAddressType,
        cseFlowMcastResultGroup      InetAddress,
        cseFlowMcastResultSource     InetAddress,
        cseFlowMcastResultFlowType   INTEGER,
        cseFlowMcastResultHFlag1k2k  OCTET STRING,
        cseFlowMcastResultHFlag3k4k  OCTET STRING
}

cseFlowMcastResultIndex OBJECT-TYPE
    SYNTAX      Integer32 (1..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A positive integer which uniquely identify a result entry
        on a specific switching engine matching a particular query."
    ::= { cseFlowMcastResultEntry 1 }

cseFlowMcastResultGrp OBJECT-TYPE
    SYNTAX      McastGroupIp
    MAX-ACCESS  read-only
    STATUS      deprecated
    DESCRIPTION
        "The multicast group IP address of the multicast layer 3 flow.

         This object is deprecated and replaced by 
         cseFlowMcastResultAddrType and cseFlowMcastResultGroup."
    ::= { cseFlowMcastResultEntry 2 }

cseFlowMcastResultSrc OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      deprecated
    DESCRIPTION
        "The source address of the multicast layer 3 flow.

         This object is deprecated and replaced by 
         cseFlowMcastResultAddrType and cseFlowMcastResultSource."
    ::= { cseFlowMcastResultEntry 3 }

cseFlowMcastResultSrcVlan OBJECT-TYPE
    SYNTAX      VlanIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The source Vlan ID of the IP multicast layer 3 flow."
    ::= { cseFlowMcastResultEntry 4 }

cseFlowMcastResultRtrIp OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The interface IP address of the router this multicast flow
        is switching for.  Since IP multicast flows can only be
        established for a router's trunk ports, it is the primary
        IP address of the router's trunk link that connects to the
        switch."
    ::= { cseFlowMcastResultEntry 5 }

cseFlowMcastResultRtrMac OBJECT-TYPE
    SYNTAX      MacAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The default MAC address of the router the multicast flow is
        switching for.  Different multicast flows switching different
        ports of the same router will have the identical value of this
        object."
    ::= { cseFlowMcastResultEntry 6 }

cseFlowMcastResultCreatedTS OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Time when the IP multicast flow was created."
    ::= { cseFlowMcastResultEntry 7 }

cseFlowMcastResultLastUsedTS OBJECT-TYPE
    SYNTAX      TimeStamp
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Time when this IP multicast flow was last used."
    ::= { cseFlowMcastResultEntry 8 }

cseFlowMcastResultPkts OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of multicast traffic packets forwarded
        for this flow (replicated packets are not counted)."
    ::= { cseFlowMcastResultEntry 9 }

cseFlowMcastResultOctets OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of multicast traffic octets forwarded
        for this flow (replicated packets are not counted)."
    ::= { cseFlowMcastResultEntry 10 }

cseFlowMcastResultDstVlans OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A string of octets containing one bit per VLAN.
        Each octet within the value of this object specifies a
        set of eight VLANs, e.g. the first octet corresponding to
        VLANs with VlanIndex values of 0 through 7, the second
        octet to VLANs 8 through 15, etc.  Within each octet,
        the most significant bit represents the lowest numbered
        VLAN, and the least significant bit represents the highest
        numbered VLAN, thus each vlan is represented by a single bit
        within the octet.  The bits in this object will be set
        to '1' if the corresponding Vlans are in the out-going
        interface (vlan) list of the IP multicast flow described
        by this row instance."
    ::= { cseFlowMcastResultEntry 11 }
 
cseFlowMcastResultDstVlans2k OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A string of octets containing one bit per VLAN,
        with VlanIndex values of 1024 through 2047,with
        each octet within the value of this object specifies a
        set of eight VLANs, e.g. the first octet corresponding to
        VLANs with VlanIndex values of 1024 through 1031, the second
        octet to VLANs 1032 through 1039 etc.  Within each octet,
        the most significant bit represents the lowest numbered
        VLAN, and the least significant bit represents the highest
        numbered VLAN, thus each vlan is represented by a single bit
        within the octet.  The bits in this object will be set
        to '1' if the corresponding Vlans are in the out-going    
        interface (vlan) list of the IP multicast flow described    
        by this row instance."
    ::= { cseFlowMcastResultEntry 12 }

cseFlowMcastResultDstVlans3k OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A string of octets containing one bit per VLAN.
        With VlanIndex values of 2048 through 3071 with
        each octet within the value of this object specifies a
        set of eight VLANs, e.g. the first octet corresponding to
        VLANs with VlanIndex values of 2048 through 2055, the second
        octet to VLANs 2056 through 2063 etc.  Within each octet,
        the most significant bit represents the lowest numbered
        VLAN, and the least significant bit represents the highest
        numbered VLAN, thus each vlan is represented by a single bit
        within the octet.  The bits in this object will be set   
        to '1' if the corresponding Vlans are in the out-going 
        interface (vlan) list of the IP multicast flow described  
        by this row instance."
    ::= { cseFlowMcastResultEntry 13 }

cseFlowMcastResultDstVlans4k OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..128))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A string of octets containing one bit per VLAN.
        With VlanIndex values of 3072 through 4095, with
        each octet within the value of this object specifies a
        set of eight VLANs, e.g. the first octet corresponding to
        VLANs with VlanIndex values of 3072 through 3079 the second
        octet to VLANs 3080 through 3087 etc.  Within each octet,
        the most significant bit represents the lowest numbered
        VLAN, and the least significant bit represents the highest
        numbered VLAN, thus each vlan is represented by a single bit
        within the octet.  The bits in this object will be set   
        to '1' if the corresponding Vlans are in the out-going 
        interface (vlan) list of the IP multicast flow described  
        by this row instance."
    ::= { cseFlowMcastResultEntry 14 }

cseFlowMcastResultMvrf OBJECT-TYPE
    SYNTAX      MplsVpnId 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The MVRF to which this flow belongs to."
    ::= { cseFlowMcastResultEntry 15 }

cseFlowMcastResultAddrType OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The Internet address type of cseFlowMcastResultGroup
         and cseFlowMcastResultSource."
    ::= { cseFlowMcastResultEntry 16 }

cseFlowMcastResultGroup OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The multicast group IP address of the multicast layer 
         3 flow."
    ::= { cseFlowMcastResultEntry 17 }

cseFlowMcastResultSource OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The source address of the multicast layer 3 flow."
    ::= { cseFlowMcastResultEntry 18 }

cseFlowMcastResultFlowType OBJECT-TYPE
    SYNTAX      INTEGER { other(1),
                          rpfMfd(2), 
                          partialSC(3) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the type of multicast layer 3 flow.

         other       - Multicast flow type is none of the followoing. 

         rpfMfd      - This flow is a RPF MFD flow.

         partial     - This flow is a partial shortcut flow."
    ::= { cseFlowMcastResultEntry 19 }

cseFlowMcastResultHFlag1k2k  OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..256))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A string of octets containing one bit per out-going 
        interface (VLAN) with VlanIndex values of 0 through 2047.
        Each octet within the value of this object specifies
        a set of eight VLANs, e.g. the first octet
        corresponding to VLANs with VlanIndex values of 
        0 through 7, the second octet to VLANs 8 through 15, 
        etc. Within each octet, the most significant bit 
        represents the lowest numbered VLAN, and the least
        significant bit represents the highest numbered VLAN,
        thus each vlan is represented by a single bit within the
        octet.

        The bits in this object will be set to '1' if the 
        multicast layer 3 flow described by this row instance
        is hardware switched on the corresponding VLAN.
        If the length of this string is less than 256 octets,
        any 'missing' octets are assumed to contain the value 
        of zero."

    ::= { cseFlowMcastResultEntry 20 }

cseFlowMcastResultHFlag3k4k OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..256))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "A string of octets containing one bit per out-going
         interface (VLAN) with VlanIndex values of 2048 through
         4095. Each octet within the value of this object 
         specifies a set of eight VLANs, e.g. the first octet 
         corresponding to VLANs with VlanIndex values of 2048
         through 2055, the second octet to VLANs 2056 through
         2063 etc. Within each octet, the most significant
         bit represents the lowest numbered VLAN, and the least
         significant bit represents the highest numbered VLAN,
         thus each vlan is represented by a single bit within 
         the octet.

         The bits in this object will be set to '1' if the 
         multicast layer 3 flow described by this row instance
         is hardware switched on the corresponding VLAN.
         If the length of this string is less than 256 octets,
         any 'missing' octets are assumed to contain the value
         of zero."
    ::= { cseFlowMcastResultEntry 21 }


-- Multicast MLS-SE global configuration
cseFlowMcastSwitchStatus OBJECT-TYPE
    SYNTAX      ControlStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "The current status of the global IP multicast flow switching
      capability.  When enabled, the switch engine will be able to
      install multicast flow entries in its L3 forwarding table,
      and perform hardware assisted switching for the flows."
    ::= { cseFlow 14 }

-- Now that our hardware can L3 switch IPX traffic

cseFlowIPXEstablishedAgingTime OBJECT-TYPE
    SYNTAX    Integer32 (1..2147483647)
    UNITS     "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "The administrative aging time for established IPX flows. The
       default value for this object is implementation specific.
       The corresponding operational object is
       cseFlowOperIPXAgingTime."
    ::= { cseFlow 15 }

cseStaticIpxExtRouterTable OBJECT-TYPE
        SYNTAX       SEQUENCE OF CseStaticIpxExtRouterEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
          "A table of external routers which are enabled for 
           Layer 3 IPX switching by the switching engine.
           This table may contain routers
           that have not yet been discovered by the device."
        ::= { cseFlow 16 }
 
cseStaticIpxExtRouterEntry OBJECT-TYPE
        SYNTAX       CseStaticIpxExtRouterEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
          "A conceptual row in the cseStaticIpxExtRouterTable for 
           enabling an external router to be installed in the
           switch's router table. The entry is created and deleted
           by using cseStaticIpxRouterStatus."
        INDEX { cseRouterIndex }

        ::= { cseStaticIpxExtRouterTable 1 }

CseStaticIpxExtRouterEntry ::= SEQUENCE {
        cseStaticIpxRouterName              DisplayString,
        cseStaticIpxRouterOwner             OwnerString,
        cseStaticIpxRouterStatus            RowStatus
}
 
cseStaticIpxRouterName  OBJECT-TYPE
       SYNTAX        DisplayString
       MAX-ACCESS    read-only
       STATUS        current
       DESCRIPTION
         "DNS name (if available) of the external router."
        ::= { cseStaticIpxExtRouterEntry 1 }

cseStaticIpxRouterOwner  OBJECT-TYPE
       SYNTAX         OwnerString
       MAX-ACCESS     read-create
       STATUS         current
       DESCRIPTION
         "String indicating the owner who created the static entry."
        ::= { cseStaticIpxExtRouterEntry 2 }

cseStaticIpxRouterStatus  OBJECT-TYPE
       SYNTAX          RowStatus
       MAX-ACCESS      read-create
       STATUS          current
       DESCRIPTION
         "Used to manage creation and deletion of rows in this table.
          Once a row becomes active, values within that row cannot be
          modified except by deleting and creating the row."
        ::= { cseStaticIpxExtRouterEntry 3 }

cseFlowOperEstablishedAgingTime OBJECT-TYPE
    SYNTAX       Integer32 (1..2147483647)
    UNITS        "seconds"
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The operational aging time for IP established flows."
    ::= { cseFlow 17 }

cseFlowOperFastAgingTime OBJECT-TYPE
    SYNTAX       Unsigned32
    UNITS        "seconds"
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
        "The operational fast aging time for the established flow 
        entries, that have less number of packets than the value set 
        in the cseFlowOperFastAgePktThreshold,switched within this
        time."
    ::= { cseFlow 18 }

cseFlowOperFastAgePktThreshold OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The operational packet threshold for the 
         cseFlowOperFastAgingTime."
    ::= { cseFlow 19 }


cseFlowOperIPXAgingTime OBJECT-TYPE
    SYNTAX      Integer32 (1..2147483647) 
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The operational aging time for established IPX flows."
    ::= { cseFlow 20 }

--
--  The bridged flow statistics control table
--

cseBridgedFlowStatsCtrlTable OBJECT-TYPE
        SYNTAX       SEQUENCE OF CseBridgedFlowStatsCtrlEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
          "A table controls the reporting of intra-vlan statistics
          for bridged flow per vlan. When a vlan is created in
          a device supporting this table, a corresponding entry
          of this table will be added." 
        ::= { cseFlow 21 }
 
cseBridgedFlowStatsCtrlEntry OBJECT-TYPE
        SYNTAX       CseBridgedFlowStatsCtrlEntry 
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
          "A row instance contains the configuration to enable
           or disable the reporting of intra-vlan statistics for
           bridged flow per vlan."  
        INDEX { cseBridgedFlowVlan }
        ::= { cseBridgedFlowStatsCtrlTable 1 }

CseBridgedFlowStatsCtrlEntry ::= SEQUENCE {
        cseBridgedFlowVlan                  VlanIndex,
        cseFlowBridgedFlowStatsEnable       TruthValue
}
 
cseBridgedFlowVlan    OBJECT-TYPE
    SYNTAX      VlanIndex 
    MAX-ACCESS  not-accessible 
    STATUS      current
    DESCRIPTION
        "Indicates the Vlan number on which the reporting of
         intra-vlan bridged flow statistics is configured." 
    ::= { cseBridgedFlowStatsCtrlEntry 1 }

cseFlowBridgedFlowStatsEnable OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Indicates whether intra-vlan bridged flow statistics is
         enabled. If this object is set to 'true', intra-vlan
         bridged flow statistics is reported in cseFlowDataTable
         when a corresponding query is set up in cseFlowQueryTable.
         If this object is set to 'false', intra-vlan bridged flow
         statistics is not reported. The default is false."
    DEFVAL { false }
    ::= { cseBridgedFlowStatsCtrlEntry 2 }

cseFlowIPFlowMask   OBJECT-TYPE
    SYNTAX    INTEGER { 
                        dstOnly(1),
                        srcDst(2),
                        fullFlow(3),
                        srcOnly(4),
                        intDstSrc(5),
                        intFull(6),
                        null(7),
                        intDstOnly(8),
                        intSrcOnly(9)
                      } 
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "Indicates the flow mask for IP flows.
 
      If dstOnly(1) is used, it enables flows based on Layer 3
      destination addresses only.
 
      If srcDst(2) is used, it enables flows based on both Layer 3
      source and destination addresses only.
 
      If fullFlow(3) is used, it enables flows based on Layer 4 port 
      numbers in addition to source and destination addresses.

      If srcOnly(4) is used, it enables flows based on Layer 3
      source addresses only.

      If intDstSrc(5) is used, it enables flows based on source
      interface in addition to source and destination addresses. 

      If intFull(6) is used, it enables flows based on source 
      interface in addition to Layer 4 port numbers, source and 
      destination addresses.

      If null(7) is used, no flow will be enabled.

      If intDstOnly(8) is used, it enables flows based on source
      interface in addition to the destination addresses.

      If intSrcOnly(9) is used, it enables flows based on source
      interface in addition to the source addresses."
    ::= { cseFlow 22 }

cseFlowIPXFlowMask   OBJECT-TYPE
    SYNTAX    INTEGER { 
                        dstOnly(1),
                        srcDst(2)
                      } 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Indicates the flow mask for IPX flows.

      If dstOnly(1) is used, it enables flows based on Layer 3
      destination addresses only.
 
      If srcDst(2) is used, it enables flows based on both Layer 3
      source and destination addresses only."
    ::= { cseFlow 23 }

cseFlowLongAgingTime OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The administrative long aging time for the established
        flow entries. Setting to value of 0 turns off long aging."
    ::= { cseFlow 24 }


--
--  The protocol exclude table 
--

cseFlowExcludeTable OBJECT-TYPE
        SYNTAX       SEQUENCE OF CseFlowExcludeEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
          "A table controls the flow creation based on protocol
          and port number. If a packet matches the protocol and
          port number specified in this table entries, a flow
          entry will not be established."
        ::= { cseFlow 25 }
 
cseFlowExcludeEntry OBJECT-TYPE
        SYNTAX       CseFlowExcludeEntry 
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
          "A row instance contains the configuration to enable or
          disable the establishment of flow entry for matching
          traffic." 
        INDEX { cseFlowExcludePort }
        ::= { cseFlowExcludeTable 1 }

CseFlowExcludeEntry ::= SEQUENCE {
        cseFlowExcludePort            CiscoPort,
        cseFlowExcludeProtocol        INTEGER,
        cseFlowExcludeStatus          RowStatus      
}
 
cseFlowExcludePort    OBJECT-TYPE
    SYNTAX      CiscoPort 
    MAX-ACCESS  not-accessible 
    STATUS      current
    DESCRIPTION
        "Indicates the TCP or UDP port number that matching
        traffic will be excluded from flow establishment.
        The value of 0 is not allowed."  
    ::= { cseFlowExcludeEntry 1 }

cseFlowExcludeProtocol OBJECT-TYPE
    SYNTAX      INTEGER {
                    udp(1),
                    tcp(2),
                    both(3)
                }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the protocol that matching traffic will be
         excluded from flow establishment." 
    ::= { cseFlowExcludeEntry 2 }

cseFlowExcludeStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The status of this conceptual row. New rows are created
         using 'createAndGo' and deleted using 'destroy'.
 
         Once 'active' this object may be set to only 'destroy'.
         cseFlowExcludeProtocol may be modified at any time (even
         while the row is active)."  
    ::= { cseFlowExcludeEntry 3 }

--
-- The flow statistics table 
-- 
cseFlowStatsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF CseFlowStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
      "A table containing flow statistics information on each switching 
       engine."
    ::= { cseFlow 26 }
 
cseFlowStatsEntry OBJECT-TYPE
    SYNTAX      CseFlowStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
      "A conceptual row of cseFlowStatsTable, containing flow 
       statistics maintained by a switching engine entity
       (identified by entPhysicalIndex). Each switching engine
       managed by this MIB module has an entry in this table."
    INDEX  { entPhysicalIndex }
    ::= { cseFlowStatsTable 1 }

CseFlowStatsEntry ::= SEQUENCE {
        cseFlowTotalFlows           Gauge32
}

cseFlowTotalFlows   OBJECT-TYPE
    SYNTAX      Gauge32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Indicates the total number of flow entries installed in
       this switching engine." 
    ::= { cseFlowStatsEntry 1 }


-- Optional NetFlow Lan Switching group

cseNetflowLSExportStatus  OBJECT-TYPE
    SYNTAX      ControlStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
      "Status of the Netflow LAN Switching data export feature."
    ::= { cseNetflowLS 1 }

cseNetflowLSExportHost  OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-write
    STATUS      deprecated
    DESCRIPTION
      "Network(IP) address in dotted decimal format or the DNS hostname 
       of the host to which Netflow LAN switching statistics are 
       exported."
    ::= { cseNetflowLS 2 }
 
cseNetflowLSExportTransportNumber  OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      deprecated
    DESCRIPTION
      "The transport(UDP) port number to be used for the Netflow LAN 
       switching statistics being exported."
    ::= { cseNetflowLS 3 }

cseNetflowLSExportDataSource OBJECT-TYPE
     SYNTAX        FlowAddressComponent 
     MAX-ACCESS    read-write
     STATUS        current
     DESCRIPTION   
       "The source network address used as a filter for selecting 
        the flows to which the netflow LAN switching data export 
        feature is applied."
        ::= { cseNetflowLS 4 }
 
cseNetflowLSExportDataSourceMask OBJECT-TYPE
     SYNTAX        FlowAddressComponent 
     MAX-ACCESS    read-write
     STATUS        current
     DESCRIPTION  
       "The mask to be applied to the corresponding instance of 
        cseNetflowExportDataSource."
     ::= { cseNetflowLS 5 }
 
cseNetflowLSExportDataDest OBJECT-TYPE
     SYNTAX        FlowAddressComponent 
     MAX-ACCESS    read-write
     STATUS        current
     DESCRIPTION   
       "The destination network address used as a filter for 
        selecting the flows to which the netflow LAN switching
        data export feature is applied."
     ::= { cseNetflowLS 6 }
 
cseNetflowLSExportDataDestMask OBJECT-TYPE
     SYNTAX        FlowAddressComponent 
     MAX-ACCESS    read-write
     STATUS        current
     DESCRIPTION   
       "The mask to be applied to its corresponding instance 
        of cseNetflowExportDataDest." 
     ::= { cseNetflowLS 7 }

cseNetflowLSExportDataProtocol   OBJECT-TYPE
       SYNTAX         Integer32 (0..255)  
       MAX-ACCESS     read-write
       STATUS         current
       DESCRIPTION
         "The protocol used as a filter for selecting the
        flows to which the netflow LAN switching data export feature
        is applied."
       REFERENCE
         "The protocol value is defined in the RFC 1700."
       ::= { cseNetflowLS 8 }

cseNetflowLSExportDataFilterSelection OBJECT-TYPE
       SYNTAX         INTEGER { included(1), excluded(2) }
       MAX-ACCESS     read-write
       STATUS         current
       DESCRIPTION
         "The filter set can be chosen either included(1) or 
          excluded(2) mutually exclusive.  If this object is set to
                included(1) -   exports the flows that match
                                cseNetflowLSExportDataSource, 
                                cseNetflowLSExportDataSourceMask, 
                                cseNetflowLSExportDataDest,
                                cseNetflowLSExportDataDestMask and 
                                cseNetflowLSExportDataProtocol.

                excluded(2) -   exports the flows that don't match
                                cseNetflowLSExportDataSource, 
                                cseNetflowLSExportDataSourceMask, 
                                cseNetflowLSExportDataDest,
                                cseNetflowLSExportDataDestMask and 
                                cseNetflowLSExportDataProtocol.
              
         "
       ::= { cseNetflowLS 9 }

cseNetflowLSExportNDEVersionNumber OBJECT-TYPE
       SYNTAX         Integer32 (1..65535)
       MAX-ACCESS     read-write
       STATUS         current
       DESCRIPTION 
            "The netflow data export version number which is 
             supported by the device.
             The typical value of this object can be 1, 7 or 8." 
      ::= { cseNetflowLS 10 }

cseNetflowLSFilterSupport OBJECT-TYPE
     SYNTAX      INTEGER { single(1), multiple(2) }
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
          "Indicates whether this device supports single filter or
           multiple filters.

           single   - use objects in cseNDESingleFilterGroupRev1 to
                      configure NDE filtering paramaters.

           multiple - use objects in cseNDEMultipleFiltersGroup to
                      configure NDE filtering paramaters."
     ::= { cseNetflowLS 11 }

cseNetflowLSFilterTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF CseNetflowLSFilterEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
          "A Table containing Netflow Data Export filtering 
           configuration."
     ::= { cseNetflowLS 12 }

cseNetflowLSFilterEntry OBJECT-TYPE
     SYNTAX     CseNetflowLSFilterEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
          "A conceptutal row in the cseNetflowLSFilterTable, 
          representing a NDE filter configuration."
     INDEX  { cseNetflowLSFilterIndex }
     ::= { cseNetflowLSFilterTable 1 }
 
CseNetflowLSFilterEntry ::= SEQUENCE {
     cseNetflowLSFilterIndex             Unsigned32,
     cseNetflowLSFilterDataSource        FlowAddressComponent,
     cseNetflowLSFilterDataSourceMask    FlowAddressComponent,
     cseNetflowLSFilterDataDest          FlowAddressComponent,
     cseNetflowLSFilterDataDestMask      FlowAddressComponent,
     cseNetflowLSFilterDataProtocol      Integer32 ,
     cseNetflowLSFilterSelection         INTEGER,
     cseNetflowLSFilterStatus            RowStatus
     } 

cseNetflowLSFilterIndex OBJECT-TYPE
     SYNTAX      Unsigned32
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION
          "An arbitrary integer which uniquely identifies the filter"
     ::= { cseNetflowLSFilterEntry 1 }

cseNetflowLSFilterDataSource OBJECT-TYPE
     SYNTAX      FlowAddressComponent
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
          "The source network address used as a filter for selecting 
           the flows to which the netflow LAN switching data export
           feature is applied. If cseNetflowLSNDEFilterDataSource 
           contains all zeros, then the 
           cseNetflowLSNDEFilterDataSource object will not be 
           included in the filtering criterion."
     DEFVAL      { '000000000000'H }  -- 00 00 00 00 00 00
     ::= { cseNetflowLSFilterEntry 2 }

cseNetflowLSFilterDataSourceMask OBJECT-TYPE
     SYNTAX      FlowAddressComponent
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
          "The mask to be applied to the corresponding instance of
           cseNetflowExportDataSource.
           If cseNetflowLSFilterDataSourceMask contains all zeros, 
           then the cseNetflowLSFilterDataSourceMask object will
           not be included in the filtering criterion."
     DEFVAL      { '000000000000'H }  -- 00 00 00 00 00 00
     ::= { cseNetflowLSFilterEntry 3 }

cseNetflowLSFilterDataDest OBJECT-TYPE
     SYNTAX      FlowAddressComponent
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
          "The destination network address used as a filter for 
           selecting the flows to which the netflow LAN switching data
           export feature is applied.
           If cseNetflowLSFilterDataDest contains all zeros, then the
           cseNetflowLSFilterDataDest object will not be included in
           the filtering criterion."
     DEFVAL      { '000000000000'H }  -- 00 00 00 00 00 00
     ::= { cseNetflowLSFilterEntry 4 }
 
cseNetflowLSFilterDataDestMask OBJECT-TYPE
     SYNTAX      FlowAddressComponent
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
          "The mask to be applied to its corresponding instance
           of cseNetflowExportDataDest.
           If cseNetflowLSFilterDataDestMask contains all zeros, 
           then the cseNetflowLSFilterDataDestMask object will not be
           included in the filtering criterion."
     DEFVAL      { '000000000000'H }  -- 00 00 00 00 00 00
     ::= { cseNetflowLSFilterEntry 5 }

cseNetflowLSFilterDataProtocol OBJECT-TYPE
     SYNTAX      Integer32 (0..255)
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
          "The protocol used as a filter for selecting the
           flows to which the netflow LAN switching data export
           feature is applied.
           The default value is set to 0, to specify that no value
           has been set.
           If cseNetflowLSFilterDataProtocol is set to 0, then the
           cseNetflowLSFilterDataProtocol object will not be included in
           the filtering criterion."
     DEFVAL      { 0 }
     ::= { cseNetflowLSFilterEntry 6 }

cseNetflowLSFilterSelection OBJECT-TYPE
     SYNTAX      INTEGER { included(1), excluded(2) }
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
          "The filter set can be chosen either included(1) or 
           excluded(2).
           If this object is set to
           included(1) -   exports the flows that match
                           cseNetflowLSFilterDataSource,
                           cseNetflowLSFilterDataSourceMask,
                           cseNetflowLSFilterDataDest,
                           cseNetflowLSFilterDataDestMask and 
                           cseNetflowLSFilterDataProtocol.

           excluded(2) -   exports the flows that don't match
                           cseNetflowLSFilterDataSource,
                           cseNetflowLSFilterDataSourceMask,
                           cseNetflowLSFilterDataDest,
                           cseNetflowLSFilterDataDestMask and 
                           cseNetflowLSFilterDataProtocol." 

     ::= { cseNetflowLSFilterEntry 7 }
  
cseNetflowLSFilterStatus OBJECT-TYPE
     SYNTAX      RowStatus
     MAX-ACCESS  read-create
     STATUS      current
     DESCRIPTION
          "The status object used to manage the rows in this table.
           Once a row becomes active, values within that row cannot be
           modified except by deleting and creating the row."
     ::= { cseNetflowLSFilterEntry 8 }

cseNetFlowIfIndexEnable OBJECT-TYPE
     SYNTAX     BITS {
                  destIfIndex(0),
                  srcIfIndex(1)
                }
     MAX-ACCESS read-write
     STATUS     current
     DESCRIPTION
         "Indicates whether ifIndex reporting in NDE (Netflow
          Data Export) is enabled.

          if bit destIfIndex(0) is on, destination ifIndex reporting
          in NDE is enabled.

          if bit srcIfIndex(1) is on, source ifIndex reporting in NDE
          is enabled." 
     ::= { cseNetflowLS 13 }

cseNetflowASInfoExportCtrl OBJECT-TYPE
     SYNTAX     INTEGER { disable(1),
                          originate(2),
                          peer(3)
                        }
     MAX-ACCESS read-write
     STATUS     current
     DESCRIPTION
         "Indicates whether export of Autonomous System(AS) number
          information, in the NDE records, is enabled.

          disable   - Disables the export of AS number information.

          originate - Enables the export of origination AS numbers of
                      source and destination IP addresses.

          peer      - Enables the export of peer AS numbers of
                      source and destination IP addresses.
         "
     ::= { cseNetflowLS 14 }

cseNetflowPerVlanIfGlobalEnable OBJECT-TYPE
     SYNTAX     TruthValue
     MAX-ACCESS read-write
     STATUS     current
     DESCRIPTION
         "Indicates whether 'creation of Netflow entries per
          VLAN interface' feature is enabled at the device level. 

          If this object is set to 'false',
          netflow entries will be created for all VLANs.

          If this object is set to 'true', creation of netflow   
          entries can be controlled by cseNetflowPerVlanIfCtrlTable."
     ::= { cseNetflowLS 15 }

cseNetflowPerVlanIfCtrlTable OBJECT-TYPE
        SYNTAX       SEQUENCE OF CseNetflowPerVlanIfCtrlEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
          "A table to control netflow entry creation for each VLAN.
           When a VLAN is created, a corresponding entry is added 
           to this table."
     ::= { cseNetflowLS 16 }

cseNetflowPerVlanIfCtrlEntry OBJECT-TYPE
        SYNTAX       CseNetflowPerVlanIfCtrlEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
          "An entry containing the configuration to enable or
           disable netflow entry creation for each VLAN."
        INDEX { cseNetflowPerVlanIfCtrlVlan }
        ::= { cseNetflowPerVlanIfCtrlTable 1 }

CseNetflowPerVlanIfCtrlEntry ::= SEQUENCE {
        cseNetflowPerVlanIfCtrlVlan                  VlanIndex,
        cseNetflowPerVlanIfEnable                    TruthValue 
}

cseNetflowPerVlanIfCtrlVlan OBJECT-TYPE
    SYNTAX      VlanIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Indicates the VLAN number on which creation of netflow 
         entries is configured."
    ::= { cseNetflowPerVlanIfCtrlEntry 1 }

cseNetflowPerVlanIfEnable OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Specifies whether creation of netflow entries is enabled
         on this VLAN.

         If this object is set to 'true', the system will create 
         netflow entries for this VLAN.

         If this object is set to 'false', the system will not create
         any netflow entries for this VLAN.

         When the value of cseNetflowPerVlanIfGlobalEnable is 'false',
         this object will not take effect." 
    ::= { cseNetflowPerVlanIfCtrlEntry 2 } 
 
-- L3 switching statistics

cseL3StatsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF CseL3StatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
      "A table containing L3 statistics information on each switching 
       engine."
    ::= { cseL3Objects 1 }
 
cseL3StatsEntry OBJECT-TYPE
    SYNTAX      CseL3StatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
      "A conceptual row of cseL3StatsTable, containing L3 statistics 
       maintained by a switching engine entity (identified by
       entPhysicalIndex).  Each switching engine managed by this
       MIB module has an entry in this table."
    INDEX  { entPhysicalIndex }
    ::= { cseL3StatsTable 1 }

CseL3StatsEntry ::= SEQUENCE {
        cseL3SwitchedTotalPkts     Counter32,
        cseL3SwitchedTotalOctets   Counter64,
        cseL3CandidateFlowHits     Counter32,
        cseL3EstablishedFlowHits   Counter32,
        cseL3ActiveFlows           Gauge32,
        cseL3FlowLearnFailures     Counter32,
        cseL3IntFlowInvalids       Counter32,
        cseL3ExtFlowInvalids       Counter32,
        cseL3SwitchedPktsPerSec    Counter32
}

cseL3SwitchedTotalPkts OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Total number of packets switched at Layer 3 by this switching
engine." 
    ::= { cseL3StatsEntry 1 }

cseL3SwitchedTotalOctets OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of octets in the total packets switched at Layer 3 by this
       switching engine."
    ::= { cseL3StatsEntry 2 }

cseL3CandidateFlowHits OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of L3 Cache hits for the candidate flow entries in this 
       switching engine."
    ::= { cseL3StatsEntry 3 }

cseL3EstablishedFlowHits OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Number of L3 Cache hits for established flow entries in this
       switching engine."
    ::= { cseL3StatsEntry 4 }

cseL3ActiveFlows OBJECT-TYPE
    SYNTAX      Gauge32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
     "Number of active flows in the Layer 3 flow table of this switching 
      engine."
    ::= { cseL3StatsEntry 5 }

cseL3FlowLearnFailures OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
     "Number of flows that failed to be learned because the Layer 3 
      flow table in this switching engine was full."
    ::= { cseL3StatsEntry 6 }

cseL3IntFlowInvalids OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
     "Number of flow invalidation events received by this switching 
      engine from the internal router(s)."
    ::= { cseL3StatsEntry 7 }

cseL3ExtFlowInvalids OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
     "Number of flow invalidation events received by this switching 
      engine from external routers."
    ::= { cseL3StatsEntry 8 }
 
cseL3SwitchedPktsPerSec OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
     "Number of packets switched per second at Layer 3 by this
      switching engine."
    ::= { cseL3StatsEntry 9 }


-- Per-VLAN L3 statistics

cseL3VlanStatsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF CseL3VlanStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
      "A table containing per-VLAN, Layer 3 statistics information per 
       switching engine."
    ::= { cseL3Objects 2 }
 
cseL3VlanStatsEntry OBJECT-TYPE
    SYNTAX      CseL3VlanStatsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
      "A conceptual row of cseL3VlanStatsTable, containing per-VLAN 
       Layer 3 statistics maintained by a switching engine (identified
       by entPhysicalIndex).  An entry exists for each known VLAN for
       each switching engine."
    INDEX  { entPhysicalIndex, cseL3VlanIndex }
    ::= { cseL3VlanStatsTable 1 }
 
CseL3VlanStatsEntry ::= SEQUENCE {
        cseL3VlanIndex         VlanIndex,
        cseL3VlanInPkts        Counter64,
        cseL3VlanInOctets      Counter64,
        cseL3VlanOutPkts       Counter64,
        cseL3VlanOutOctets     Counter64,
        cseL3VlanInUnicastPkts      Counter64,
        cseL3VlanInUnicastOctets    Counter64,
        cseL3VlanOutUnicastPkts     Counter64,
        cseL3VlanOutUnicastOctets   Counter64
}

cseL3VlanIndex    OBJECT-TYPE
       SYNTAX     VlanIndex
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
         "Vlan number for which the statistics are maintained by this 
          entry."
        ::= { cseL3VlanStatsEntry 1 }
 
cseL3VlanInPkts   OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
         "Number of packets Layer 3 forwarded from this Vlan to some
          other VLAN by this switching engine."
        ::= { cseL3VlanStatsEntry 2 }
 
cseL3VlanInOctets  OBJECT-TYPE
       SYNTAX      Counter64
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
         "Number of octets in packets Layer-3 forwarded from this Vlan
          to some other VLAN by this switching engine."
        ::= { cseL3VlanStatsEntry 3 }
 
cseL3VlanOutPkts  OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
         "Number of packets Layer-3 forwarded to this Vlan by this
          switching engine."
        ::= { cseL3VlanStatsEntry 4 }
 
cseL3VlanOutOctets  OBJECT-TYPE
       SYNTAX       Counter64
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
         "Number of octets in packets Layer-3 forwarded to this Vlan
          by this switching engine."
        ::= { cseL3VlanStatsEntry 5 }
 
cseL3VlanInUnicastPkts   OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
         "Number of unicast packets Layer 3 forwarded from this Vlan
          to some other VLAN by this switching engine."
        ::= { cseL3VlanStatsEntry 6 }
 
cseL3VlanInUnicastOctets  OBJECT-TYPE
       SYNTAX      Counter64
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
         "Number of octets in unicast packets Layer-3 forwarded from
          this Vlan to some other VLAN by this switching engine."
        ::= { cseL3VlanStatsEntry 7 }

cseL3VlanOutUnicastPkts   OBJECT-TYPE
       SYNTAX     Counter64
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
         "Number of unicast packets Layer 3 forwarded to this
          Vlan by this switching engine."
        ::= { cseL3VlanStatsEntry 8 }
 
cseL3VlanOutUnicastOctets  OBJECT-TYPE
       SYNTAX      Counter64
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
         "Number of octets in unicast packets Layer-3 forwarded
          to this Vlan by this switching engine."
        ::= { cseL3VlanStatsEntry 9 }

-- Switch Engine based layer 3 flow statistics; it is protocol
-- independent, i.e. IP and IPX statistics are not separated
-- This group is an augmentation of cseL3StatsTable
cseStatsFlowTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF CseStatsFlowEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
      "A table of flow statistics per switch engine that is
      not covered in cseL3StatsTable."
    ::= { cseL3Objects 3 }

cseStatsFlowEntry OBJECT-TYPE
    SYNTAX     CseStatsFlowEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
      "A conceptual row about slot based L3 flow statistics."
    AUGMENTS   { cseL3StatsEntry }
    ::= { cseStatsFlowTable 1 }

CseStatsFlowEntry ::= SEQUENCE {
        cseStatsFlowAged       Counter32,
        cseStatsFlowPurged     Counter32,
        cseStatsFlowParityFail Counter32
}

cseStatsFlowAged OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Total number of layer 3 flows aged out by hardware.  Management
      applications can control flow aging by setting the value of
      cseFlowEstablishedAgingTime object."
    ::= { cseStatsFlowEntry 1 }

cseStatsFlowPurged OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Total number of layer 3 flows purged by software; it may happen
      because a router invalidates certain flows, or a router for which
      flows are being switched has been excluded from cseRouterTable, or
      access-list has changed, or certain features have been enabled
      that would purge certain flows (TCP interception, Web cache are
      examples of such features)."
    ::= { cseStatsFlowEntry 2 }

cseStatsFlowParityFail OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Total number of memory parity errors on accessing flows in
      the cache pools.  It may be due to the internal RAM reading
      error, not necessarily the corrupted flow data."
    ::= { cseStatsFlowEntry 3 }

-- Utilization level of flow cache pool per Switch Engine
-- Flows are combined for IP and IPX
cseCacheUtilTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF CseCacheUtilEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
      "A table of utilization levels in percentage of cache
      capacity per switch engine.  Each row instance is the
      current flow utilization information in the cache pool
      of the corresponding switching engine."
    ::= { cseL3Objects 4 }

cseCacheUtilEntry OBJECT-TYPE
    SYNTAX     CseCacheUtilEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
      "A row instance represents layer 3 flow utilization of
      a particular cache pool on a switching engine."
    INDEX      { entPhysicalIndex }
    ::= { cseCacheUtilTable 1 }

CseCacheUtilEntry ::= SEQUENCE {
        cseCacheUtilization     Gauge32,
        cseCacheEntriesCreated  Unsigned32,
        cseCacheEntriesFailed   Unsigned32
}

cseCacheUtilization OBJECT-TYPE
    SYNTAX      Gauge32 (0..100)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "Flow utilization level in percentage in this switching engine.
       It includes the flow entries for both unicast and multicast.
       The lighter the utilization level, the less risk of dropping
       flows, i.e. the higher success-rate of flow insertion."
    ::= { cseCacheUtilEntry 1 }

cseCacheEntriesCreated   OBJECT-TYPE
    SYNTAX        Unsigned32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "This object indicates the total number of flow entries 
         successfully created in this switching engine."
    ::= { cseCacheUtilEntry 2 }

cseCacheEntriesFailed    OBJECT-TYPE
    SYNTAX        Unsigned32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "This object indicates the number of flow entries
         which were failed to be created in this switching engine."
    ::= { cseCacheUtilEntry 3 }


--
--  L3 error counters table.
-- 
cseErrorStatsTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF CseErrorStatsEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A table of IP and IPX error counters per switch engine."
    ::= { cseL3Objects 5 }

cseErrorStatsEntry OBJECT-TYPE
    SYNTAX     CseErrorStatsEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A row instance represents layer-3 IP and IPX error counters
        on a switching engine."
    INDEX { entPhysicalIndex }
    ::= { cseErrorStatsTable 1 }

CseErrorStatsEntry ::= SEQUENCE {
    cseIpPlenErrors        Counter64,
    cseIpTooShortErrors    Counter64,
    cseIpCheckSumErrors    Counter64,
    cseIpxPlenErrors       Counter64,
    cseIpxTooShortErrors   Counter64
}

cseIpPlenErrors OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of IP length against physical length
        errors." 
    ::= { cseErrorStatsEntry 1 }

cseIpTooShortErrors OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of IP length too short errors." 
    ::= { cseErrorStatsEntry 2 }

cseIpCheckSumErrors OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of IP checksum errors." 
    ::= { cseErrorStatsEntry 3 }

cseIpxPlenErrors OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of IPX length against physical length
        errors." 
    ::= { cseErrorStatsEntry 4 }

cseIpxTooShortErrors OBJECT-TYPE
    SYNTAX      Counter64 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of IPX length too short errors." 
    ::= { cseErrorStatsEntry 5 }

--
--  L3 error counters table.
-- 
cseErrorStatsLCTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF CseErrorStatsLCEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A table of IP and IPX error counters per switch engine."
    ::= { cseL3Objects 6 }

cseErrorStatsLCEntry OBJECT-TYPE
    SYNTAX     CseErrorStatsLCEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
        "A row instance represents layer-3 IP and IPX error counters
        on a switching engine."
    INDEX { entPhysicalIndex }
    ::= { cseErrorStatsLCTable 1 }

CseErrorStatsLCEntry ::= SEQUENCE {
    cseLCIpPlenErrors        Counter32,
    cseLCIpTooShortErrors    Counter32,
    cseLCIpCheckSumErrors    Counter32,
    cseLCIpxPlenErrors       Counter32,
    cseLCIpxTooShortErrors   Counter32
}

cseLCIpPlenErrors OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of IP length against physical length
        errors." 
    ::= { cseErrorStatsLCEntry 1 }

cseLCIpTooShortErrors OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of IP length too short errors." 
    ::= { cseErrorStatsLCEntry 2 }

cseLCIpCheckSumErrors OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of IP checksum errors." 
    ::= { cseErrorStatsLCEntry 3 }

cseLCIpxPlenErrors OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of IPX length against physical length
        errors." 
    ::= { cseErrorStatsLCEntry 4 }

cseLCIpxTooShortErrors OBJECT-TYPE
    SYNTAX      Counter32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the number of IPX length too short errors." 
    ::= { cseErrorStatsLCEntry 5 }

-- Packets Switched Per Second

cseL3SwitchedAggrPktsPerSec OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of packets switched per second at Layer 3 by the
        entire system."
    ::= { cseL3Objects 7 } 

-- Protocol Filter capability

cseProtocolFilterEnable OBJECT-TYPE
    SYNTAX      TruthValue 
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Indicates if protocol filtering is enabled in the device."
    ::= { cseProtocolFilter 1 }

cseProtocolFilterPortTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF CseProtocolFilterPortEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
     "A table containing the protocol filtering configuration and status
      information on ports."
    ::= { cseProtocolFilter 2 }
 
cseProtocolFilterPortEntry OBJECT-TYPE
    SYNTAX     CseProtocolFilterPortEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
      "A conceptual row in the cseProtocolFilterPortTable, 
       representing a Protocol filter configuration
       status information for a particular
       port (identified by ifIndex) and protocol type."
    INDEX { ifIndex, cseProtocolFilterPortProtocol }
    ::= { cseProtocolFilterPortTable 1 }
 
CseProtocolFilterPortEntry ::= SEQUENCE {
        cseProtocolFilterPortProtocol       INTEGER,
        cseProtocolFilterPortAdminStatus    INTEGER,
        cseProtocolFilterPortOperStatus     INTEGER
}

cseProtocolFilterPortProtocol      OBJECT-TYPE
        SYNTAX      INTEGER { ip(1),
                              ipx(2),
                              grpProtocols(3) -- Appletalk/Decnet/Vines
                    }
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
        "The protocol (group) to filter, used here as the secondary 
         index."
        ::= { cseProtocolFilterPortEntry 1 }

cseProtocolFilterPortAdminStatus      OBJECT-TYPE
        SYNTAX      INTEGER { on(1),
                              off(2),
                              auto(3)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
        "An indication of the administrative status of the protocol
         filtering on this interface.
         
         - on(1) indicates that the interface will send and receive the 
           traffic for protocol specified in 
           cseProtocolFilterPortProtocol.
         - off(2) indicates that the interface will not receive 
           traffic for this protocol, or if this feature is not 
           supported.
         - auto(3) indicates that the corresponding 
           cseProtocolFilterPortOperStatus will transit to 'on' after 
           receiving one packet of this protocol type."
        ::= { cseProtocolFilterPortEntry 2 }

cseProtocolFilterPortOperStatus      OBJECT-TYPE
        SYNTAX      INTEGER { on(1),
                              off(2),
                              notSupported(3)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
        "An indication of the operational status of filtering for
         this protocol on this interface.
         - on(1) indicates that the interface will send and receive the 
           protocol traffic.
         - off(2) indicates that the interface will drop all traffic 
           belonging to this protocol.
         - notSupported(3) indicates the hardware does not support 
           protocol filtering."
        ::= { cseProtocolFilterPortEntry 3 }

-- This MIB group/table is designed for control of purging flow caches
-- The caches are distributed in the switching engines across the system
 
cseUcastCacheTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF CseUcastCacheEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
     "A control table used to purge certain types of IP/IPX layer 3
     unicast flows stored in the cache pool."
    ::= { cseUcastCache 1 }
 
cseUcastCacheEntry OBJECT-TYPE
    SYNTAX     CseUcastCacheEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
      "A conceptual row in the cseUcastCacheTable, used to set up
      flow clearing criteria.  The actual purging is started by setting
      the value of cseUcastCacheStatus to 'active'.  Once a row becomes
      active, values within the row cannot be modified, except by
      setting it to 'notInService' first or deleting and re-creating
      the row."
    INDEX { cseUcastCacheIndex }
    ::= { cseUcastCacheTable 1 }
 
CseUcastCacheEntry ::= SEQUENCE {
        cseUcastCacheIndex      Unsigned32,
        cseUcastCacheFlowType   INTEGER,
        cseUcastCacheTransport  INTEGER,
        cseUcastCacheDest       FlowAddressComponent,
        cseUcastCacheDestMask   FlowAddressComponent,
        cseUcastCacheSource     FlowAddressComponent,
        cseUcastCacheSrcMask    FlowAddressComponent,
        cseUcastCacheRtrIp      IpAddress,
        cseUcastCacheOwner      OwnerString,
        cseUcastCacheResult     INTEGER,
        cseUcastCacheStatus     RowStatus
}

cseUcastCacheIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
      "An arbitrary integer which uniquely identifies the flow
      purge contained in this row instance."
    ::= { cseUcastCacheEntry 1 }

cseUcastCacheFlowType OBJECT-TYPE
    SYNTAX      INTEGER {
                         any(1),
                         dstOnly(2),
                         srcOrDst(3),
                         srcAndDst(4),
                         fullFlow(5),
                         ipxDstOnly(6),
                         ipxSrcAndDst(7)
                        }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
      "Setting each value causes the appropriate action:
 
      'dstOnly' - causes purge of flows in the cache whose absolute
      destination IP addresses match the address part of the value set
      in the cseUcastCacheDest object.  If cseUcastCacheDestMask is also
      specified at the same time, it will be applied to the address part
      of cseUcastCacheDest.
 
      'srcOrDst' - causes purge of flows in the cache whose either
      absolute source or destination IP addresses match the address
      parts of the values set in cseUcastCacheSource or 
      cseUcastCacheDest.
      If cseUcastCacheDestMask/cseUcastCacheSrcMask also specified,
      they will be applied to the address parts of cseUcastCacheSource/
      cseUcastCacheDest appropriately.
 
      'srcAndDst' - causes purge of flows in the cache whose both
      absolute source and destination IP addresses match the address
      parts of values set in cseUcastCacheSource and cseUcastCacheDest
      objects.  If cseUcastCacheSrcMask and cseUcastCacheDestMask also
      specified, they will be applied to the address parts of
      cseUcastCacheSource and cseUcastCacheDest.
 
      'fullFlow' - causes purge of IP flows whose IP addresses and
      transport port numbers match the values set in cseUcastCacheDest
      and cseUcastCacheSource objects.
      If either cseUcastCacheDestMask or cseUcastCacheSrcMask objects
      have valid values, they will be applied to the respective address
      parts of cseUcastCacheDest and cseUcastCacheSource objects.
      This option is typically used to purge flows relevant to specific
      applications such as FTP, WWW, TELNET, etc.
 
      'ipxDstOnly' - causes purge of IPX flows in the cache whose
      absolute destination IPX address match the address part of
      the value set in cseUcastCacheDest object.
      if cseUcastCacheDestMask holds valid value at the same time,
      it will be applied to the address part of cseUcastCacheDest.
 
      'ipxSrcAndDst' - causes purge of IPX flows in the cache whose
      both absolute source and destination IPX addresses match the
      address parts of the values set in cseUcastCacheSource and
      cseUcastCacheDest objects.
      If either of cseUcastCacheSrcMask or cseUcastCacheDestMask
      have valid values at the same time, they will be applied to
      the respective address parts of cseUcastCacheSource and
      cseUcastCacheDest objects.
 
      'any' - causes purge of all established flows currently in
      the cache.  The values of cseUcastCacheDest, cseUcastCacheSource,
      cseUcastCacheDestMask, cseUcastCacheSrcMask, and
      cseUcastCacheTransport should be ignored in this case.
 
      Note:
        1. When the row instance is initialized, the value of this 
           object instance will be set to 'any'.
        2. The rest flow parameter variables will not be instantiated
           until they get set by management applications based on
           the value of cseUcastCacheFlowType object."
    DEFVAL      { any }
    ::= { cseUcastCacheEntry 2 }
 
cseUcastCacheTransport OBJECT-TYPE
    SYNTAX      INTEGER { udp(1), tcp(2) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
      "The IP transport protocol type (if applicable) of the specified
      switched flows to be purged; it will be instantiated if and only
      if it gets set by the management applications and the value of
      cseUcastCacheFlowMask is equal to 'fullFlow'.
      Its value can not be modified when the corresponding instance
      of cseUcastCacheStatus is 'active'."
    ::= { cseUcastCacheEntry 3 }
 
cseUcastCacheDest OBJECT-TYPE
    SYNTAX      FlowAddressComponent
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
      "Destination network address and port number (if applicable).
      The port field is ignored for IPX flows and IP flows if the
      value of cseUcastCacheFlowMask is not equal to 'fullFlow'.
      Its value can not be modified when the corresponding instance
      of cseUcastCacheStatus is 'active'."
    ::= { cseUcastCacheEntry 4 }
 
cseUcastCacheDestMask OBJECT-TYPE
    SYNTAX      FlowAddressComponent
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
      "If instantiated, specified and applicable, the destination 
      address mask will be applied to the value of
      cseUcastCacheDest in the same row instance.
      Its value can not be modified when the corresponding instance
      of cseUcastCacheStatus is 'active'."
    ::= { cseUcastCacheEntry 5 }
 
cseUcastCacheSource OBJECT-TYPE
    SYNTAX      FlowAddressComponent
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
      "Source network address and port number (if applicable).
      The port field is ignored for IPX flows and IP flows if the
      value of cseUcastCacheFlowMask is not equal to 'fullFlow'.
      Its value can not be modified when the corresponding instance
      of cseUcastCacheStatus is 'active'."
    ::= { cseUcastCacheEntry 6 }
 
cseUcastCacheSrcMask OBJECT-TYPE
    SYNTAX      FlowAddressComponent
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
      "If instantiated, specified and applicable, the source address
      mask will be applied to the  value of cseUcastCacheSource
      in the same row instance.
      Its value can not be modified when the corresponding instance
      of cseUcastCacheStatus is 'active'."
    ::= { cseUcastCacheEntry 7 }
 
cseUcastCacheRtrIp OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
      "IP address of the router (internal or external) for which the
      flows are being switched, and need to be purged.  An 'all-zero'
      value is a wildcard IP address for any router.
      Its value can not be modified when the corresponding instance
      of cseUcastCacheStatus is 'active'."
    ::= { cseUcastCacheEntry 8 }

cseUcastCacheOwner OBJECT-TYPE
    SYNTAX      OwnerString
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
      "The manager entity that configured this entry and is therefore 
       using the resources assigned to it."
    ::= { cseUcastCacheEntry 9 }
 
cseUcastCacheResult OBJECT-TYPE
    SYNTAX      INTEGER { purging(1), notPurging(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "state of the flow purging operation.
 
      'purging' - purging operation is proceeding
 
      'notPurging' - the purging operation completed, or not 
       started yet."
    DEFVAL      { notPurging }
    ::= { cseUcastCacheEntry 11 }
 
cseUcastCacheStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
      "The status object used to manage rows in this table.
      When set to active(1), the flow purge is initiated, and
      the value of cseUcastCacheResult object becomes 'purging'.
      However, this object can be set to active(1) only after
      all the appropriate objects for this query as defined 
      by the value set in the cseUcastCacheFlowType object,
      have also been set.  Upon the completion of flow purge,
      the value of cseUcastCacheResult object changes to
      'notPurging'.
      Once a row becomes active, values within the row cannot
      be modified, except by setting it to 'notInService' first,
      or deleting and re-creating it."
    ::= { cseUcastCacheEntry 10 }
 

-- This MIB group/table is designed for purging IP multicast
-- flows.  For a multicast switch, a row instance can be used to clear
-- specified multicast L3 flows from its cache pools

cseMcastCacheTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF CseMcastCacheEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
     "A control table used to purge specified IP multicast flows
     from the switch engine."
    ::= { cseMcastCache 1 }
 
cseMcastCacheEntry OBJECT-TYPE
    SYNTAX     CseMcastCacheEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
      "A conceptual row in the cseMcastCacheTable, used to set up
      flow clearing criteria.  The actual purging is started by setting
      the value of cseMcastCacheStatus to 'active'.  Once a row becomes
      active, values within the row cannot be modified, except by
      setting it to 'notInService' first, or deleting and re-creating
      the row."
    INDEX { cseMcastCacheIndex }
    ::= { cseMcastCacheTable 1 }
 
CseMcastCacheEntry ::= SEQUENCE {
        cseMcastCacheIndex      Unsigned32,
        cseMcastCacheFlowType   INTEGER,
        cseMcastCacheGrp        McastGroupIp,
        cseMcastCacheSrc        IpAddress,
        cseMcastCacheRtrIp      IpAddress,
        cseMcastCacheOwner      OwnerString,
        cseMcastCacheResult     INTEGER,
        cseMcastCacheStatus     RowStatus
}

cseMcastCacheIndex OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
      "An arbitrary integer which uniquely identifies the flow
      purge contained in the current row instance."
    ::= { cseMcastCacheEntry 1 }

cseMcastCacheFlowType OBJECT-TYPE
    SYNTAX      INTEGER { any(1), group(2), grpAndSrc(3) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Setting each value causes the appropriate action:
 
        'any' - causes purge of all established IP multicast
        layer 3 flows in the cache.  The value of cseMcastCacheGrp,
        and cseMcastCacheSrc will be ignored in this case.
 
        'group' - causes purge of flows whose multicast
        group IP address match the values of cseMcastCacheGrp.
 
        'grpAndSrc' - causes purge of multicast flows whose both
        group IP address and source Ip address match the
        values of cseMcastCacheGrp and cseMcastCacheSrc.
 
        Note:
          1. The instance of this object is initialized to
             'any' when the corresponding row instance is
             being instantiated.
          2. Flow parameter variables, cseMcastCacheGrp, 
             cseMcastCacheSrc, cseMcastCacheRtrIp will not
             be instantiated until they get set by management
             applications (in such cases, cseMcastCacheFlowType
             object should be set to a value other than 'any')."
    DEFVAL      { any }
    ::= { cseMcastCacheEntry 2 }
 
cseMcastCacheGrp OBJECT-TYPE
    SYNTAX      McastGroupIp
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifying multicast group IP address of the flows to be
        cleared.  Its value can not be modified when the corresponding
        instance of cseMcastCacheStatus is 'active'."
    ::= { cseMcastCacheEntry 3 }
 
cseMcastCacheSrc OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The source address of the IP multicast flows to be purged.
        Its value can not be modified when the corresponding instance
        of cseMcastCacheStatus is 'active'."
    ::= { cseMcastCacheEntry 4 }
 
cseMcastCacheRtrIp OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The IP address of the router whose flows are currently
        being switched, and will be purged.  An 'all-zero' value is
        a wildcard IP address for any router.
        Its value can not be modified when the corresponding instance
        of cseMcastCacheStatus is 'active'."
    ::= { cseMcastCacheEntry 5 }
 
cseMcastCacheOwner OBJECT-TYPE
    SYNTAX      OwnerString
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
      "The manager entity that configured this entry and is therefore 
       using the resources assigned to it."
    ::= { cseMcastCacheEntry 6 }

cseMcastCacheResult OBJECT-TYPE
    SYNTAX      INTEGER { purging(1), notPurging(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
      "state of the flow purging operation.
 
      'purging' - purging operation is proceeding
 
      'notPurging' - the purging operation completed, or not 
       started yet."
    DEFVAL      { notPurging }
    ::= { cseMcastCacheEntry 7 }

cseMcastCacheStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The status object used to manage rows in this table.
        When set to active(1), the flow purge is initiated, and
        the value of cseMcastCacheResult object becomes 'purging'.
        However, this object can be set to active(1) only after
        all the appropriate objects for this query as defined 
        by the value set in the cseMcastCacheFlowType object,
        have also been set.  Upon the completion of flow purge,
        the value of cseMcastCacheResult object changes to
        'notPurging'.
        Once a row becomes active, values within the row cannot
        be modified, except by setting it to 'notInService' first,
        or deleting and re-creating it."
    ::= { cseMcastCacheEntry 8 }

--
--  cseCef Group 
--

--
-- The cseCefFibTable
--
cseCefFibTable    OBJECT-TYPE
    SYNTAX        SEQUENCE OF CseCefFibEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "This table contains the information stored in the device's 
         forwarding information base (FIB). 

         FIB is a forwarding scheme that utilizes matching pattern
         to provide optimized lookup for efficient packet forwarding.
         It contains a forwarding table which consist of matching
         criteria for incoming traffic as well as information to
         forward traffic that matched defined criteria." 
    ::= { cseCef 1 }

cseCefFibEntry    OBJECT-TYPE
    SYNTAX        CseCefFibEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "Each row contains the IP address type, the final destination
         IP address, the final destination IP address mask as well as
         the FIB entry type."
    INDEX { cseCefFibIndex }
    ::= { cseCefFibTable 1 }

CseCefFibEntry ::= SEQUENCE {
    cseCefFibIndex           Unsigned32, 
    cseCefFibAddrType        InetAddressType,
    cseCefFibDestIp          InetAddress,
    cseCefFibDestIpMask      InetAddress,
    cseCefFibType            INTEGER
}

cseCefFibIndex     OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The index of this table entry."
    ::= { cseCefFibEntry 1 }

cseCefFibAddrType  OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The type of IP address denoted in cseCefFibDestIp and
         cseCefFibDestIpMask object." 
    ::= { cseCefFibEntry 2 }

cseCefFibDestIp    OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The destination IP address specified in IP packet header."
    ::= { cseCefFibEntry 3 }

cseCefFibDestIpMask  OBJECT-TYPE
    SYNTAX        InetAddress
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "The specified destination IP address mask."
    ::= { cseCefFibEntry 4 }

cseCefFibType        OBJECT-TYPE
    SYNTAX        INTEGER {
                      other(1),
                      resolved(2),
                      bridge(3),
                      drop(4),
                      connected(5),
                      receive(6),
                      wildcard(7),
                      tunnel(8),
                      default(9)
                  } 
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Indicates the FIB entry type.
         
         other(1) indicates that this FIB entry type is none
         of the following.
         
         resolved(2) indicates that IP traffic matched the
         destination prefix of this entry is associated with a
         valid next-hop address. 
 
         bridge(3) indicates that IP traffic matched the destination
         prefix of this entry will be forwarded using Layer 2
         look up result. 

         drop(4) indicates that IP traffic matched the destination
         prefix of this entry will be dropped.

         connected(5) indicates that IP traffic matched the destination
         prefix of this entry is associated with a connected network. 

         receive(6) indicates that IP traffic matched the destination
         prefix of this entry will be sent to a router interface.

         wildcard(7) indicates this FIB entry will match all traffic. 

         tunnel(8) indicates this FIB entry applied to tunneling
         traffic. 

         default(9) indicates that IP traffic matched the destination
         prefix of this entry will be forwarded using a default route." 
    ::= { cseCefFibEntry 5 }

--
-- The cseCefAdjacencyTable
--

cseCefAdjacencyTable    OBJECT-TYPE
    SYNTAX        SEQUENCE OF CseCefAdjacencyEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "This table contains information stored in the device's 
         adjacency table. Entry in this table is linked to entry
         of cseCefFibTable by its cseCefFibIndex object." 
    ::= { cseCef 3 }

cseCefAdjacencyEntry    OBJECT-TYPE
    SYNTAX        CseCefAdjacencyEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "Each row contains next hop IP address, next-hop Ethernet
         address, adjacency type, and number of bytes and packets
         transmitted to each adjacency entry. Next hop encapsulation
         type and MTU value are also available if supported by the
         device."  
    INDEX { cseCefFibIndex, cseCefAdjacencyIndex }
    ::= { cseCefAdjacencyTable 1 }

CseCefAdjacencyEntry ::= SEQUENCE {
    cseCefAdjacencyIndex           Unsigned32, 
    cseCefAdjacencyAddrType        InetAddressType,
    cseCefAdjacencyNextHopIp       InetAddress,
    cseCefAdjacencyNextHopMac      MacAddress,
    cseCefAdjacencyNextHopIfIndex  InterfaceIndexOrZero, 
    cseCefAdjacencyType            INTEGER,
    cseCefAdjacencyPkts            Counter64,
    cseCefAdjacencyOctets          Counter64,
    cseCefAdjacencyEncap           INTEGER,
    cseCefAdjacencyMTU             Unsigned32
}

cseCefAdjacencyIndex     OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The adjacency index of this table entry."
    ::= { cseCefAdjacencyEntry 1 }

cseCefAdjacencyAddrType  OBJECT-TYPE
    SYNTAX      InetAddressType
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The type of IP address denoted in cseCefAdjacencyNextHopIp
         object." 
    ::= { cseCefAdjacencyEntry 2 }

cseCefAdjacencyNextHopIp    OBJECT-TYPE
    SYNTAX      InetAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The next hop IP address."
    ::= { cseCefAdjacencyEntry 3 }

cseCefAdjacencyNextHopMac  OBJECT-TYPE
    SYNTAX        MacAddress  
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "The next hop Ethernet address." 
    ::= { cseCefAdjacencyEntry 4 }

cseCefAdjacencyNextHopIfIndex    OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the next hop interface ifIndex." 
    ::= { cseCefAdjacencyEntry 5 }

cseCefAdjacencyType        OBJECT-TYPE
    SYNTAX        INTEGER {
                      other(1),
                      punt(2),
                      glean(3),
                      drop(4),
                      null(5),
                      noRewrite(6),
                      forceDrop(7),
                      connect(8),
                      unresolved(9),
                      loopback(10),
                      tunnel(11)
                  } 
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
        "Indicates this adjacency entry type.
        
         other(1) indicates the adjacency entry type is none of
         the following.

         punt(2) indicates entry that sends traffic to the router.

         glean(3) indicates entry that needs to be gleaned for incoming
         traffic.

         drop(4) indicates entry that drops packets.

         null(5) indicates entry that drops packets destined 
         for the Null0 interface.

         noRewrite(6) indicates entry that sends traffic to the router
         when rewrite information is incomplete. 

         forceDrop(7) indicates entry that drop packets due to ARP
         throttling. 

         connect(8) indicates entry that contains complete rewrite
         information.

         unresolved(9) indicates entry that next hop traffic is 
         unresolved. 

         loopback(10) indicates entry that drops packets destined 
         for loopback interface.

         tunnel(11) indicates entry that next hop traffic is 
         through a tunnel."
    ::= { cseCefAdjacencyEntry 6 }

cseCefAdjacencyPkts   OBJECT-TYPE
     SYNTAX        Counter64
     MAX-ACCESS    read-only
     STATUS        current
     DESCRIPTION
         "Indicates the number of Layer 3 packets transmitted to 
          this adjacency entry."
     ::= { cseCefAdjacencyEntry 7 }

cseCefAdjacencyOctets   OBJECT-TYPE
     SYNTAX        Counter64
     MAX-ACCESS    read-only
     STATUS        current
     DESCRIPTION
         "Indicates the number of Layer 3 octets transmitted to 
          this adjacency entry."
     ::= { cseCefAdjacencyEntry 8 }

cseCefAdjacencyEncap    OBJECT-TYPE
    SYNTAX      INTEGER {
                   arpa(1),
                   raw(2),
                   sap(3),
                   snap(4)
                } 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the next hop destination encapsulation type.

         arpa(1) indicates that next hop destination used ARPA
         encapsulation type to forward packets.

         raw(2) indicates that next hop destination used RAW
         encapsulation type to forward packets.

         sap(3) indicates that next hop destination used SAP 
         encapsulation type to forward packets.

         snap(4) indicates that next hop destination used SNAP
         encapsulation type to forward packets." 
    ::= { cseCefAdjacencyEntry 9 }

cseCefAdjacencyMTU    OBJECT-TYPE
    SYNTAX      Unsigned32 
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the next hop destination MTU value." 
    ::= { cseCefAdjacencyEntry 10 }

--
--  cseTcamUsage group
--

--
-- The cseTcamUsageTable 
--

cseTcamUsageTable    OBJECT-TYPE
    SYNTAX        SEQUENCE OF CseTcamUsageEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "This table contains the resource usage of TCAM (Ternary
         Content Addressable Memory) in the device.  Not all the
         resource types denoted by cseTcamResourceType object
         are supported. If that is the case, the corresponding row
         for that type will not be instantiated in this table."
    ::= { cseTcamUsage 1 }

cseTcamUsageEntry    OBJECT-TYPE
    SYNTAX        CseTcamUsageEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "Each row contains a short description of the resource type,
        the total amount of TCAM allocated for that type as well
        as the amount of allocated resource has been used up."  
    INDEX { entPhysicalIndex, cseTcamResourceType }
    ::= { cseTcamUsageTable 1 }

CseTcamUsageEntry ::= SEQUENCE {
    cseTcamResourceType     INTEGER,
    cseTcamResourceDescr    SnmpAdminString,
    cseTcamResourceUsed     Unsigned32,
    cseTcamResourceTotal    Unsigned32 
}

cseTcamResourceType        OBJECT-TYPE
    SYNTAX        INTEGER {
                      aclStorageMask(1),
                      aclStorageValue(2),
                      aclDynamicStorageMask(3),
                      aclDynamicStorageValue(4),
                      qosStorageMask(5),
                      qosStorageValue(6),
                      qosDynamicStorageMask(7),
                      qosDynamicStorageValue(8),
                      l4PortOperator(9),
                      interfaceMapping(10),
                      ingressInterfaceMapping(11),
                      egressInterfaceMapping(12),
                      louSource(13),
                      louDestination(14),
                      andOr(15),
                      orAnd(16),
                      aclAdjacency(17)
                   } 
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "The resource type which take up TCAM space.

         aclStorageMask(1) indicates that TCAM space is allocated
         to store ACL masks.

         aclStorageValue(2) indicates that TCAM space is allocated
         to store ACL value.

         aclDynamicStorageMask(3) indicates that TCAM space is
         allocated to dynamically store ACL masks.

         aclDynamicStorageValue(4) indicates that TCAM space is
         allocated to dynamically store ACL values.

         qosStorageMask(5) indicates that TCAM space is allocated
         to store QoS masks.

         qosStorageValue(6) indicates that TCAM space is allocated
         to store QoS value.

         qosDynamicStorageMask(7) indicates that TCAM space is
         allocated to dynamically store QoS masks.

         qosDynamicStorageValue(8) indicates that TCAM space is
         allocated to dynamically store QoS values.

         l4PortOperator(9) indicates that TCAM space is allocated
         for layer 4 port operators purpose.

         interfaceMapping(10) indicates that TCAM space is allocated
         for interface mapping purpose.
       
         ingressInterfaceMapping(11) indicates that TCAM space is
         allocated for ingress interface mapping purpose.

         egressInterfaceMapping(12) indicates that TCAM space is
         allocated for egress interface mapping purpose.

         louSource(13) indicates that TCAM space is allocated
         as source LOUs (Logical Operation Unit).
 
         louDestination(14) indicates that TCAM space is allocated
         as destination LOUs.

         andOr(15) indicates that TCAM space is allocated for 
         ANDOR purpose.

         orAnd(16) indicates that TCAM space is allocated for
         ORAND purpose.

         aclAdjacency(17) indicates that TCAM space is allocated
         for ACL adjacency purpose." 
    ::= { cseTcamUsageEntry 1 }

cseTcamResourceDescr     OBJECT-TYPE
    SYNTAX        SnmpAdminString 
    MAX-ACCESS    read-only 
    STATUS        current
    DESCRIPTION
        "The short description of the resource type." 
    ::= { cseTcamUsageEntry 2 }

cseTcamResourceUsed     OBJECT-TYPE
    SYNTAX        Unsigned32 
    MAX-ACCESS    read-only 
    STATUS        current
    DESCRIPTION
        "The amount of TCAM resource has been used up for this resource
        type." 
    ::= { cseTcamUsageEntry 3 }

cseTcamResourceTotal     OBJECT-TYPE
    SYNTAX        Unsigned32 
    MAX-ACCESS    read-only 
    STATUS        current
    DESCRIPTION
        "The total amount of TCAM resource is allocated for this
        resource type." 
    ::= { cseTcamUsageEntry 4 }


--
--  cseMet group
--

--
-- The cseMetUsageTable 
--

cseMetUsageTable    OBJECT-TYPE
    SYNTAX        SEQUENCE OF CseMetUsageEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "This table contains the resource usage of MET (Multicast
         Expansion Table) in the device."
    ::= { cseMet 1 }

cseMetUsageEntry    OBJECT-TYPE
    SYNTAX        CseMetUsageEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "Each row contains the total number of entries in each MET,
         the number of free entries in unallocated as well as
         allocated space of the MET. Each row represents MET data 
         maintained by each module (identified by its entPhysicalIndex)
         which is capable of this feature."   
    INDEX { entPhysicalIndex, cseMetIndex }
    ::= { cseMetUsageTable 1 }

CseMetUsageEntry ::= SEQUENCE {
    cseMetIndex                        Unsigned32, 
    cseMetTotalEntries                 Unsigned32,
    cseMetUnallocatedSpcFreeEntries    Unsigned32,
    cseMetAllocatedSpcFreeEntries      Unsigned32
}

cseMetIndex       OBJECT-TYPE
    SYNTAX        Unsigned32 
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "A value uniquely identifies a MET in a module."
    ::= { cseMetUsageEntry 1 }

cseMetTotalEntries     OBJECT-TYPE
    SYNTAX        Unsigned32 
    MAX-ACCESS    read-only 
    STATUS        current
    DESCRIPTION
        "The total number of entries in this MET."
    ::= { cseMetUsageEntry 2 }

cseMetUnallocatedSpcFreeEntries OBJECT-TYPE
    SYNTAX        Unsigned32 
    MAX-ACCESS    read-only 
    STATUS        current
    DESCRIPTION
        "The number of free entries reside in unallocated
         space of this MET." 
    ::= { cseMetUsageEntry 3 }

cseMetAllocatedSpcFreeEntries   OBJECT-TYPE
    SYNTAX        Unsigned32 
    MAX-ACCESS    read-only 
    STATUS        current
    DESCRIPTION
        "The number of free entries reside in allocated 
        space of this MET." 
    ::= { cseMetUsageEntry 4 }
 
 
-- Notifications

cseMIBNotifications   OBJECT IDENTIFIER ::= { ciscoSwitchEngineMIB 2 }

-- no notifications defined

-- Conformance

cseMIBConformance   OBJECT IDENTIFIER   ::= { ciscoSwitchEngineMIB 3 }

cseMIBCompliances   OBJECT IDENTIFIER   ::= { cseMIBConformance 1 }

cseMIBGroups        OBJECT IDENTIFIER   ::= { cseMIBConformance 2 }

-- compliance statements

cseMIBCompliance MODULE-COMPLIANCE
        STATUS deprecated
        DESCRIPTION
          "The compliance statement for 
           the CISCO-SWITCH_ENGINE-MIB MIB."
        MODULE
        MANDATORY-GROUPS { cseStatisticsGroup }

        GROUP  cseRouterGroup 
        DESCRIPTION
        "This group is mandatory only for those switches which
         support layer 3 switching in the system." 

        GROUP  cseVlanStatisticsGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         can provide per-vlan statistics."

        GROUP  cseFlowMgmtGroup 
        DESCRIPTION
        "This group is mandatory only for those switches which
         support layer 3 switching in the system." 

        GROUP  cseFlowMcastMgmtGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         support layer 3 IP multicast switching in the system."

        GROUP  cseUcastCachePurgeGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         supports IP/IPX unicast flow cache purging in the system."

        GROUP  cseMcastCachePurgeGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         supports IP multicast flow cache purging in the system."

        ::= { cseMIBCompliances 1 }

cseMIBCompliance2 MODULE-COMPLIANCE
        STATUS deprecated
        DESCRIPTION
          "The compliance statement for 
           the CISCO-SWITCH-ENGINE-MIB MIB."
        MODULE
        MANDATORY-GROUPS { cseStatisticsGroup }

        GROUP  cseRouterGroup 
        DESCRIPTION
        "This group is mandatory only for those switches which
         support layer 3 switching in the system." 

        GROUP  cseVlanStatisticsGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         can provide per-vlan statistics."

        GROUP  cseFlowMgmtGroup 
        DESCRIPTION
        "This group is mandatory only for those switches which
         support layer 3 switching in the system." 

        GROUP  cseFlowMcastMgmtGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         support layer 3 IP multicast switching in the system."

        GROUP  cseUcastCachePurgeGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         supports IP/IPX unicast flow cache purging in the system."

        GROUP  cseMcastCachePurgeGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         supports IP multicast flow cache purging in the system."

        GROUP  cseFlowMgmtOperStatusGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         support operating status on aging time for flows used
         in L3 switching."

        ::= { cseMIBCompliances 2 }

cseMIBCompliance3 MODULE-COMPLIANCE
        STATUS deprecated
        DESCRIPTION
          "The compliance statement for
           the CISCO-SWITCH-ENGINE-MIB MIB."
        MODULE
        MANDATORY-GROUPS { cseStatisticsGroup }
         
        GROUP  cseRouterGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         support layer 3 switching in the system."
        
        GROUP  cseVlanStatisticsGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         can provide per-vlan statistics."

        GROUP  cseFlowMgmtGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         support layer 3 switching in the system."
               
        GROUP  cseFlowMcastMgmtGroup
        DESCRIPTION
        "This group is mandatory only for those switches which  
         support layer 3 IP multicast switching in the system."
               
        GROUP  cseUcastCachePurgeGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         supports IP/IPX unicast flow cache purging in the system."
               
        GROUP  cseFlowMgmtOperStatusGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         support operating status on aging time for flows used
         in L3 switching."
               
        GROUP  cse4kVlanGroup
        DESCRIPTION
        "This group must be implemented by the devices which
         support the range of VlanIndex between 1024 and 4095 "
         
        ::= { cseMIBCompliances 3 }

cseMIBCompliance4 MODULE-COMPLIANCE
        STATUS deprecated
        DESCRIPTION
          "The compliance statement for
           the CISCO-SWITCH-ENGINE-MIB MIB."
        MODULE
        MANDATORY-GROUPS { cseStatisticsGroup }

        GROUP  cseRouterGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         support layer 3 switching in the system."

        GROUP  cseVlanStatisticsGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         can provide per-vlan statistics."

        GROUP  cseFlowMgmtGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         support layer 3 switching in the system."

        GROUP  cseFlowMcastMgmtGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         support layer 3 IP multicast switching in the system."

        GROUP  cseUcastCachePurgeGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         supports IP/IPX unicast flow cache purging in the system."

        GROUP  cseMcastCachePurgeGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         supports IP multicast flow cache purging in the system."

        GROUP  cseFlowMgmtOperStatusGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         support operating status on aging time for flows used
         in L3 switching."

        GROUP  cse4kVlanGroup
        DESCRIPTION
        "This group must be implemented by the devices which
         support the range of VlanIndex between 1024 and 4095 "

        GROUP cseNDEMandatoryGroup
        DESCRIPTION
        "This group is mandatory for those switched which
         support Netflow Data Export"

        GROUP cseNDESingleFilterGroup
        DESCRIPTION
        "This group is mandatory in agents for which the value of
         cseNetflowLSFilterSupport is single."
   
        GROUP cseNDEMultipleFiltersGroup
        DESCRIPTION
        "This group is mandatory in agents for which the value of
         cseNetflowLSFilterSupport is multiple."

        OBJECT cseNetflowLSFilterSelection
        MIN-ACCESS read-only
        DESCRIPTION
        "Write access is not required, for systems which 
         support just one include and one exclude filter."

        OBJECT cseNetflowLSFilterStatus
        MIN-ACCESS read-only
        DESCRIPTION
        "Write access is not required, for systems which 
         support just one include and one exclude filter"

        GROUP cseProtocolFilterGroup
        DESCRIPTION
        "Implementation of this group is optional."

        GROUP cseStatisticsGroup2
        DESCRIPTION 
        "Implementation of this group is optional."
 
        ::= { cseMIBCompliances 4 }

cseMIBCompliance5 MODULE-COMPLIANCE
        STATUS deprecated
        DESCRIPTION
          "The compliance statement for
           the CISCO-SWITCH-ENGINE-MIB MIB."
        MODULE
        MANDATORY-GROUPS { cseStatisticsGroup }

        GROUP  cseRouterGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         support layer 3 switching in the system."

        GROUP  cseVlanStatisticsGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         can provide per-vlan statistics."

        GROUP  cseFlowMgmtGroupRev1
        DESCRIPTION
        "This group is mandatory only for those switches which
         support layer 3 switching in the system."

        GROUP  cseFlowMcastMgmtGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         support layer 3 IP multicast switching in the system."

        GROUP  cseUcastCachePurgeGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         supports IP/IPX unicast flow cache purging in the system."

        GROUP  cseMcastCachePurgeGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         supports IP multicast flow cache purging in the system."

        GROUP  cseFlowMgmtOperStatusGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         support operating status on aging time for flows used
         in L3 switching."

        GROUP  cse4kVlanGroup
        DESCRIPTION
        "This group must be implemented by the devices which
         support the range of VlanIndex between 1024 and 4095 "

        GROUP cseNDEMandatoryGroup
        DESCRIPTION
        "This group is mandatory for those switched which
         support Netflow Data Export"

        GROUP cseNDESingleFilterGroup
        DESCRIPTION
        "This group is mandatory in agents for which the value of
         cseNetflowLSFilterSupport is single."
   
        GROUP cseNDEMultipleFiltersGroup
        DESCRIPTION
        "This group is mandatory in agents for which the value of
         cseNetflowLSFilterSupport is multiple."

        OBJECT cseNetflowLSFilterSelection
        MIN-ACCESS read-only
        DESCRIPTION
        "Write access is not required, for systems which 
         support just one include and one exclude filter."

        OBJECT cseNetflowLSFilterStatus
        MIN-ACCESS read-only
        DESCRIPTION
        "Write access is not required, for systems which 
         support just one include and one exclude filter"

        GROUP cseProtocolFilterGroup
        DESCRIPTION
        "Implementation of this group is optional."

        GROUP cseStatisticsGroup2
        DESCRIPTION 
        "Implementation of this group is optional."
 
        ::= { cseMIBCompliances 5 }     

cseMIBCompliance6 MODULE-COMPLIANCE
        STATUS deprecated
        DESCRIPTION
          "The compliance statement for
           the CISCO-SWITCH-ENGINE-MIB MIB."
        MODULE
        MANDATORY-GROUPS { cseStatisticsGroup }

        GROUP  cseRouterGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         support layer 3 switching in the system."

        GROUP  cseVlanStatisticsGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         can provide per-vlan statistics."

        GROUP  cseFlowMgmtGroupRev1
        DESCRIPTION
        "This group is mandatory only for those switches which
         support layer 3 switching in the system."

        GROUP  cseFlowMcastMgmtGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         support layer 3 IP multicast switching in the system."

        GROUP  cseUcastCachePurgeGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         supports IP/IPX unicast flow cache purging in the system."

        GROUP  cseMcastCachePurgeGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         supports IP multicast flow cache purging in the system."

        GROUP  cseFlowMgmtOperStatusGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         support operating status on aging time for flows used
         in L3 switching."

        GROUP  cse4kVlanGroup
        DESCRIPTION
        "This group must be implemented by the devices which
         support the range of VlanIndex between 1024 and 4095 "

        GROUP cseNDEMandatoryGroup
        DESCRIPTION
        "This group is mandatory for those switched which
         support Netflow Data Export"

        GROUP cseNDESingleFilterGroupRev1
        DESCRIPTION
        "This group is mandatory in agents for which the value of
         cseNetflowLSFilterSupport is single."
   
        GROUP cseNDEMultipleFiltersGroup
        DESCRIPTION
        "This group is mandatory in agents for which the value of
         cseNetflowLSFilterSupport is multiple."

        OBJECT cseNetflowLSFilterSelection
        MIN-ACCESS read-only
        DESCRIPTION
        "Write access is not required, for systems which 
         support just one include and one exclude filter."

        OBJECT cseNetflowLSFilterStatus
        MIN-ACCESS read-only
        DESCRIPTION
        "Write access is not required, for systems which 
         support just one include and one exclude filter"

        GROUP cseProtocolFilterGroup
        DESCRIPTION
        "Implementation of this group is optional."

        GROUP cseStatisticsGroup2
        DESCRIPTION 
        "Implementation of this group is optional."
        
        GROUP cseFlowMgmtExtGroup2
        DESCRIPTION
        "This group is mandatory only for those switches which
         support layer 3 switching in the system."
         
        ::= { cseMIBCompliances 6 }     

cseMIBCompliance7 MODULE-COMPLIANCE
        STATUS current
        DESCRIPTION
          "The compliance statement for
           the CISCO-SWITCH-ENGINE-MIB MIB."
        MODULE
        MANDATORY-GROUPS { cseStatisticsGroup }

        GROUP  cseRouterGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         support layer 3 switching in the system."

        GROUP  cseVlanStatisticsGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         can provide per-vlan statistics."

        GROUP  cseFlowMgmtGroupRev1
        DESCRIPTION
        "This group is mandatory only for those switches which
         support layer 3 switching in the system."
  
        GROUP  cseFlowMcastMgmtGroup1
        DESCRIPTION
        "This group is mandatory only for those switches which
         support layer 3 IP multicast switching in the system."

        GROUP  cseUcastCachePurgeGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         supports IP/IPX unicast flow cache purging in the system."

        GROUP  cseMcastCachePurgeGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         supports IP multicast flow cache purging in the system."

        GROUP  cseFlowMgmtOperStatusGroup
        DESCRIPTION
        "This group is mandatory only for those switches which
         support operating status on aging time for flows used
         in L3 switching."

        GROUP  cse4kVlanGroup
        DESCRIPTION
        "This group must be implemented by the devices which
         support the range of VlanIndex between 1024 and 4095 "

        GROUP cseNDEMandatoryGroup
        DESCRIPTION
        "This group is mandatory for those switched which
         support Netflow Data Export"

        GROUP cseNDESingleFilterGroupRev1
        DESCRIPTION
        "This group is mandatory in agents for which the value of
         cseNetflowLSFilterSupport is single."

        GROUP cseNDEMultipleFiltersGroup
        DESCRIPTION
        "This group is mandatory in agents for which the value of
         cseNetflowLSFilterSupport is multiple."

        OBJECT cseNetflowLSFilterSelection
        MIN-ACCESS read-only
        DESCRIPTION
        "Write access is not required, for systems which 
         support just one include and one exclude filter."

        OBJECT cseNetflowLSFilterStatus
        MIN-ACCESS read-only
        DESCRIPTION
        "Write access is not required, for systems which 
         support just one include and one exclude filter"

        GROUP cseProtocolFilterGroup
        DESCRIPTION
        "Implementation of this group is optional."

        GROUP cseStatisticsGroup2
        DESCRIPTION
        "Implementation of this group is optional."

        GROUP cseFlowMgmtExtGroup2
        DESCRIPTION
        "This group is mandatory only for those switches which
         support layer 3 switching in the system."

        GROUP cseFlowMcastRtrMgmtGroup
        DESCRIPTION
        "Implementation of this group is optional."

        GROUP cseFlowMcastMgmtGroup2
        DESCRIPTION
        "This group is mandatory only for those switches which
         support layer 3 IP multicast switching in the system."

        ::= { cseMIBCompliances 7 }

-- units of conformance

cseStatisticsGroup OBJECT-GROUP
    OBJECTS  { cseL2ForwardedLocalPkts, cseL2ForwardedLocalOctets,
               cseL2ForwardedTotalPkts,
               cseL2NewAddressLearns, cseL2AddrLearnFailures,
               cseL2DstAddrLookupMisses, cseL3SwitchedTotalPkts,
               cseL3SwitchedTotalOctets, cseL3CandidateFlowHits,
               cseL3EstablishedFlowHits, cseL3ActiveFlows, 
               cseL3FlowLearnFailures, cseL3IntFlowInvalids, 
               cseL3ExtFlowInvalids,
               cseL2HCOverflowForwardedLocalPkts,
               cseL2HCForwardedLocalPkts,
               cseL2HCOverflowForwardedTotalPkts,
               cseL2HCForwardedTotalPkts,
               cseL2HCOverflowIpPkts,
               cseL2HCIpPkts,
               cseL2HCOverflowIpxPkts,
               cseL2HCIpxPkts,
               cseL2HCOverflowAssignedProtoPkts,
               cseL2HCAssignedProtoPkts,
               cseL2HCOverflowOtherProtoPkts,
               cseL2HCOtherProtoPkts  }
    STATUS  current
    DESCRIPTION
      "A collection of objects providing switch engine statistics." 
    ::= { cseMIBGroups 1 }

cseStatisticsGroup2 OBJECT-GROUP
    OBJECTS  { cseStatsFlowAged, cseStatsFlowPurged,
               cseStatsFlowParityFail, cseCacheUtilization }
    STATUS  current
    DESCRIPTION
      "A collection of objects providing switch engine statistics
      on aged/purged flows, and the cache utilizations."
    ::= { cseMIBGroups 2 }

cseVlanStatisticsGroup OBJECT-GROUP
    OBJECTS  { cseL3VlanInPkts, cseL3VlanInOctets, cseL3VlanOutPkts, 
               cseL3VlanOutOctets }
    STATUS  current
    DESCRIPTION
      "A collection of objects providing per-vlan switch engine 
       statistics, if supported."
    ::= { cseMIBGroups 3 }

cseRouterGroup OBJECT-GROUP
    OBJECTS { cseRouterFlowMask, cseRouterName, cseRouterStatic, 
              cseStaticRouterOwner, cseStaticRouterName, 
              cseStaticRouterType, cseStaticRouterStatus, 
              cseRouterIpxFlowMask, cseStaticIpxRouterOwner,
              cseStaticIpxRouterName,  cseStaticIpxRouterStatus,
              cseRouterMac, cseRouterProtocol }
    STATUS  current
    DESCRIPTION
      "A collection of objects providing information on routers which
       are used to support layer 3 switching in the system."
    ::= { cseMIBGroups 4 }

cseFlowMgmtGroup OBJECT-GROUP
    OBJECTS { cseFlowEstablishedAgingTime, cseFlowFastAgingTime, 
              cseFlowFastAgePktThreshold, 
              cseFlowIPXEstablishedAgingTime,
              cseFlowMaxQueries,
              cseFlowQueryMask, cseFlowQueryTransport,
              cseFlowQuerySource, cseFlowQuerySourceMask,
              cseFlowQueryDestination, cseFlowQueryDestinationMask, 
              cseFlowQueryRouterIndex, cseFlowQueryOwner, 
              cseFlowQueryResultingRows,
              cseFlowQueryResultTotalPkts, 
              cseFlowQueryResultTotalOctets,
              cseFlowQueryResultAvgDuration, cseFlowQueryResultAvgIdle,
              cseFlowQueryStatus, cseFlowQueryCreateTime, 
              cseFlowDataSrcMac,
              cseFlowDataDstMac, cseFlowDataEncapType, 
              cseFlowDataSource,
              cseFlowDataStaticFlow, 
              cseFlowDataDestination, cseFlowDataDestVlan, 
              cseFlowDataIpQOS, cseFlowDataIpQOSPolicy,
              cseFlowDataWhenCreated, cseFlowDataLastUsed, 
              cseFlowDataPkts,
              cseFlowDataOctets, cseFlowSwitchStatus }
    STATUS  deprecated
    DESCRIPTION
      "A collection of objects providing information for determining the
       L3 flow switching performance in the switching engine. There may
       be some platform specific limitations when performing a SET 
       on some of these objects.

       The following are valid for Catalyst 5000 platforms:

       - cseFlowEstablishedAgingTime has a default value of 256.

       - cseFlowFastAgePktThreshold can only be set to 1, 3, 7, 15, 31 
       or 63 packets. If the packet threshold is not configured to one 
       of these values, it will be adjusted to the closest value.

       - cseFlowFastAgingTime can be set to only values that are 
       multiples  of 8 in the range (0..128).
       If it is set to a value that is not 
       multiple of 8, then the closest value that is a multiple of 8
       will take effect. The default value for fast aging time is 32
       seconds. (i.e. less than cseFlowFastAgePktThreshold number of
       packets were switched within 32 seconds after the an L3
       flow entry was established).

       - cseFlowIPXEstablishedAgingTime has a default value of 256."
    ::= { cseMIBGroups 5 }

cseNetflowLSGroup OBJECT-GROUP
    OBJECTS { cseNetflowLSExportHost, cseNetflowLSExportTransportNumber,
              cseNetflowLSExportStatus,
              cseNetflowLSExportDataSource,
              cseNetflowLSExportDataSourceMask,
              cseNetflowLSExportDataDest, 
              cseNetflowLSExportDataDestMask,
              cseNetflowLSExportDataProtocol,
              cseNetflowLSExportDataFilterSelection,
              cseNetflowLSExportNDEVersionNumber
           }
    STATUS  deprecated
    DESCRIPTION
      "A collection of objects providing information on the Netflow LAN
       switching Data Export feature, if supported."
    ::= { cseMIBGroups 6 }

cseProtocolFilterGroup OBJECT-GROUP
    OBJECTS { cseProtocolFilterPortAdminStatus, 
              cseProtocolFilterPortOperStatus, cseL2IpPkts, 
              cseL2IpxPkts,
              cseL2AssignedProtoPkts, cseL2OtherProtoPkts }
    STATUS  current
    DESCRIPTION
      "A collection of objects providing information on the Protocol
       filter feature, if supported."
    ::= { cseMIBGroups 7 }

cseFlowMcastMgmtGroup OBJECT-GROUP
    OBJECTS     { cseFlowMcastMaxQueries, cseFlowMcastQueryMask,
                  cseFlowMcastQuerySrc, cseFlowMcastQueryGrp,
                  cseFlowMcastQuerySrcVlan, cseFlowMcastQueryRtrIndex,
                  cseFlowMcastQuerySkipNFlows, cseFlowMcastQueryOwner,
                  cseFlowMcastQueryTotalFlows, cseFlowMcastQueryRows,
                  cseFlowMcastQueryStatus, cseFlowMcastQueryCreateTime,
                  cseFlowMcastResultSrc, cseFlowMcastResultGrp,
                  cseFlowMcastResultSrcVlan, cseFlowMcastResultRtrIp,
                  cseFlowMcastResultRtrMac, cseFlowMcastResultCreatedTS,
                  cseFlowMcastResultLastUsedTS, cseFlowMcastResultPkts,
                  cseFlowMcastResultOctets, cseFlowMcastResultDstVlans,
                  cseFlowMcastSwitchStatus }
    STATUS      deprecated
    DESCRIPTION
      "A collection of objects for querying IP multicast flows
      stored in hardware switching cache."
    ::= { cseMIBGroups 8 }

cseUcastCachePurgeGroup OBJECT-GROUP
    OBJECTS     { cseUcastCacheFlowType, cseUcastCacheTransport,
                  cseUcastCacheDest, cseUcastCacheDestMask,
                  cseUcastCacheSource, cseUcastCacheSrcMask,
                  cseUcastCacheRtrIp, cseUcastCacheOwner,
                  cseUcastCacheStatus, cseUcastCacheResult }
    STATUS      current
    DESCRIPTION
      "A collection of objects providing IP/IPX unicast flow cache
       purging function."
    ::= { cseMIBGroups 9 }

cseMcastCachePurgeGroup OBJECT-GROUP
    OBJECTS     { cseMcastCacheFlowType, cseMcastCacheGrp,
                  cseMcastCacheSrc, cseMcastCacheRtrIp,
                  cseMcastCacheOwner, cseMcastCacheStatus,
                  cseMcastCacheResult }
    STATUS      current
    DESCRIPTION
      "A collection of objects providing IP multicast flow cache purge
       function."
    ::= { cseMIBGroups 10 }

cseFlowMgmtOperStatusGroup OBJECT-GROUP
    OBJECTS { cseFlowOperEstablishedAgingTime,
              cseFlowOperFastAgingTime, cseFlowOperFastAgePktThreshold,
              cseFlowOperIPXAgingTime
            }
    STATUS  current
    DESCRIPTION
      "A collection of objects providing operating status information 
       on aging time for flows used in L3 switching."
    ::= { cseMIBGroups 11 }

cse4kVlanGroup OBJECT-GROUP
    OBJECTS { cseFlowMcastResultDstVlans2k,
              cseFlowMcastResultDstVlans3k,
              cseFlowMcastResultDstVlans4k
            }
    STATUS  current
    DESCRIPTION
      "A collection of objects providing information
       for VLANS with VlanIndex from 1024 to 4095."
    ::= { cseMIBGroups 12 }

cseNDEMandatoryGroup OBJECT-GROUP
    OBJECTS { cseNetflowLSFilterSupport,
              cseNetflowLSExportStatus,
              cseNetflowLSExportNDEVersionNumber
            }
   STATUS  current
   DESCRIPTION
     "A collection of objects providing information on the type
      of filter support, status and the version of NDE used."
   ::= { cseMIBGroups 13 }

cseNDESingleFilterGroup OBJECT-GROUP
    OBJECTS { cseNetflowLSExportHost, 
              cseNetflowLSExportTransportNumber,
              cseNetflowLSExportDataSource,
              cseNetflowLSExportDataSourceMask,
              cseNetflowLSExportDataDest, 
              cseNetflowLSExportDataDestMask,
              cseNetflowLSExportDataProtocol,
              cseNetflowLSExportDataFilterSelection
           }
    STATUS  deprecated
    DESCRIPTION
      "A collection of objects providing information on the Netflow LAN
       switching Data Export feature, with a single host and a
       single filter support."
    ::= { cseMIBGroups 14 }

cseNDEMultipleFiltersGroup OBJECT-GROUP
    OBJECTS { cseNetflowLSFilterDataSource,
              cseNetflowLSFilterDataSourceMask,
              cseNetflowLSFilterDataDest,
              cseNetflowLSFilterDataDestMask,
              cseNetflowLSFilterDataProtocol,
              cseNetflowLSFilterSelection,
              cseNetflowLSFilterStatus
           }
    STATUS  current
    DESCRIPTION
      "A collection of objects providing information on the Netflow LAN
       switching Data Export feature, with multiple filter support."
   ::= { cseMIBGroups 15 }

cseFlowMgmtGroupRev1 OBJECT-GROUP
    OBJECTS { cseFlowEstablishedAgingTime, cseFlowFastAgingTime, 
              cseFlowFastAgePktThreshold, 
              cseFlowIPXEstablishedAgingTime,
              cseFlowMaxQueries,
              cseFlowQueryMask, cseFlowQueryTransport,
              cseFlowQuerySource, cseFlowQuerySourceMask,
              cseFlowQueryDestination, cseFlowQueryDestinationMask, 
              cseFlowQueryRouterIndex, cseFlowQueryOwner, 
              cseFlowQueryResultingRows,
              cseFlowQueryResultTotalPkts, 
              cseFlowQueryResultTotalOctets,
              cseFlowQueryResultAvgDuration, cseFlowQueryResultAvgIdle,
              cseFlowQueryStatus, cseFlowQueryCreateTime,
              cseFlowQueryTotalFlows,
              cseFlowDataSrcMac,
              cseFlowDataDstMac, cseFlowDataEncapType, 
              cseFlowDataSource,
              cseFlowDataStaticFlow, 
              cseFlowDataDestination, cseFlowDataDestVlan, 
              cseFlowDataIpQOS, cseFlowDataIpQOSPolicy,
              cseFlowDataWhenCreated, cseFlowDataLastUsed, 
              cseFlowDataPkts,
              cseFlowDataOctets, cseFlowSwitchStatus }
    STATUS  current
    DESCRIPTION
      "A collection of objects providing information for determining the
       L3 flow switching performance in the switching engine. There may
       be some platform specific limitations when performing a SET 
       on some of these objects.

       The following are valid for Catalyst 5000 platforms:

       - cseFlowEstablishedAgingTime has a default value of 256.

       - cseFlowFastAgePktThreshold can only be set to 1, 3, 7, 15, 31 
       or 63 packets. If the packet threshold is not configured to one 
       of these values, it will be adjusted to the closest value.

       - cseFlowFastAgingTime can be set to only values that are 
       multiples  of 8 in the range (0..128).
       If it is set to a value that is not 
       multiple of 8, then the closest value that is a multiple of 8
       will take effect. The default value for fast aging time is 32
       seconds. (i.e. less than cseFlowFastAgePktThreshold number of
       packets were switched within 32 seconds after the an L3
       flow entry was established).

       - cseFlowIPXEstablishedAgingTime has a default value of 256."
    ::= { cseMIBGroups 16 }

cseL3ErrorsGroup  OBJECT-GROUP
    OBJECTS {
      cseIpPlenErrors,
      cseIpTooShortErrors,
      cseIpCheckSumErrors,
      cseIpxPlenErrors,
      cseIpxTooShortErrors
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the IP and IPX error 
        statistics."
    ::= { cseMIBGroups 17 }

cseBridgedFlowGroup  OBJECT-GROUP
    OBJECTS {
      cseFlowBridgedFlowStatsEnable
    }
    STATUS current
    DESCRIPTION
        "A collection of objects control the reporting of intra-vlan
         bridged flow statistics."
    ::= { cseMIBGroups 18 }

cseVlanStatisticsExtGroup OBJECT-GROUP
    OBJECTS  { 
      cseL3VlanInUnicastPkts,
      cseL3VlanInUnicastOctets,
      cseL3VlanOutUnicastPkts,
      cseL3VlanOutUnicastOctets
    }
    STATUS  current
    DESCRIPTION
      "A collection of objects providing additional per-vlan switch
       engine statistics, if supported."
    ::= { cseMIBGroups 19 }

cseProtocolFilterExtGroup OBJECT-GROUP
    OBJECTS { cseProtocolFilterEnable }
    STATUS  current
    DESCRIPTION
      "A collection of objects providing additional information on the
       Protocol filter feature, if supported."
    ::= { cseMIBGroups 20 }

cseFlowMgmtExtGroup OBJECT-GROUP
    OBJECTS { cseFlowIPFlowMask, cseFlowIPXFlowMask}
    STATUS  current
    DESCRIPTION
      "A collection of objects providing additional information on the
       L3 flow switching in the switching engine."
    ::= { cseMIBGroups 21 }

cseFlowMgmtExtGroup1 OBJECT-GROUP
    OBJECTS { 
         cseFlowLongAgingTime,
         cseFlowExcludeProtocol,
         cseFlowExcludeStatus
    }
    STATUS  current
    DESCRIPTION
      "A collection of objects providing additional information on the
       L3 flow switching in the switching engine."
    ::= { cseMIBGroups 22 }

cseNDEReportGroup OBJECT-GROUP
     OBJECTS { cseNetFlowIfIndexEnable }
     STATUS  current
     DESCRIPTION
       "A collection of objects providing the configuration
        on NDE ifIndex report feature."
     ::= { cseMIBGroups 23 }

cseStatisticsFlowGroup OBJECT-GROUP
    OBJECTS  { cseFlowTotalFlows  }
    STATUS  current
    DESCRIPTION
      "A collection of object providing switch engine statistics
      on total number of installed flows."
    ::= { cseMIBGroups 24 }

cseFlowMgmtExtGroup2 OBJECT-GROUP
    OBJECTS { cseFlowQuerySkipNFlows }
    STATUS  current
    DESCRIPTION
      "A collection of objects providing additional information on the
       L3 flow switching in the switching engine."
    ::= { cseMIBGroups 25 }

cseNDESingleFilterGroupRev1 OBJECT-GROUP
    OBJECTS { cseNetflowLSExportDataSource, 
              cseNetflowLSExportDataSourceMask,
              cseNetflowLSExportDataDest,
              cseNetflowLSExportDataDestMask,
              cseNetflowLSExportDataProtocol,
              cseNetflowLSExportDataFilterSelection
           }
    STATUS  current
    DESCRIPTION
      "A collection of objects providing information on the Netflow LAN
       switching Data Export feature, with a single filter support." 
    ::= { cseMIBGroups 26 }

cseCefFibAdjacencyGroup OBJECT-GROUP
    OBJECTS  {
         cseCefFibAddrType,
         cseCefFibDestIp,
         cseCefFibDestIpMask,
         cseCefFibType,
         cseCefAdjacencyAddrType,
         cseCefAdjacencyNextHopIp,
         cseCefAdjacencyNextHopMac,
         cseCefAdjacencyNextHopIfIndex,
         cseCefAdjacencyType,
         cseCefAdjacencyPkts,
         cseCefAdjacencyOctets
    }
    STATUS  current
    DESCRIPTION
      "A collection of objects providing FIB and adjacency
       information available in the device."
    ::= { cseMIBGroups 27 }

cseCefAdjacencyEncapGroup OBJECT-GROUP
    OBJECTS { cseCefAdjacencyEncap }
    STATUS  current
    DESCRIPTION
      "A collection of object providing adjacency next hop 
       encapsulation information available in the device."
    ::= { cseMIBGroups 28 }

cseCefAdjacencyMTUGroup OBJECT-GROUP
    OBJECTS { cseCefAdjacencyMTU }
    STATUS  current
    DESCRIPTION
      "A collection of object providing adjacency next hop
       MTU information available in the device."
    ::= { cseMIBGroups 29 }

cseTcamUsageGroup OBJECT-GROUP
    OBJECTS {
      cseTcamResourceDescr,
      cseTcamResourceUsed,
      cseTcamResourceTotal
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the resource usage
        information on TCAM available in the device."
    ::= { cseMIBGroups 30 }

cseL3ErrorsLCGroup  OBJECT-GROUP
    OBJECTS {
      cseLCIpPlenErrors,
      cseLCIpTooShortErrors,
      cseLCIpCheckSumErrors,
      cseLCIpxPlenErrors,
      cseLCIpxTooShortErrors
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing the IP and IPX error 
        statistics."
    ::= { cseMIBGroups 31 }

cseNetflowASInfoExportGroup OBJECT-GROUP
    OBJECTS {
      cseNetflowASInfoExportCtrl
    }
    STATUS current
    DESCRIPTION
        "A collection of object providing AS number information
         export control."
    ::= { cseMIBGroups 32 }

cseNetflowPerVlanIfGroup OBJECT-GROUP
    OBJECTS {
      cseNetflowPerVlanIfGlobalEnable,
      cseNetflowPerVlanIfEnable
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing control of netflow entry 
         creation per vlan."
    ::= { cseMIBGroups 33 }

cseMetUsageGroup OBJECT-GROUP
    OBJECTS {
      cseMetTotalEntries,
      cseMetUnallocatedSpcFreeEntries,
      cseMetAllocatedSpcFreeEntries 
    }
    STATUS current
    DESCRIPTION
        "A collection of objects providing MET utilization 
         information." 
    ::= { cseMIBGroups 34 }

cseFlowMcastMgmtGroup1 OBJECT-GROUP
    OBJECTS     { cseFlowMcastMaxQueries, 
                  cseFlowMcastQueryMask,
                  cseFlowMcastQuerySrcVlan, 
                  cseFlowMcastQuerySkipNFlows, 
                  cseFlowMcastQueryOwner,
                  cseFlowMcastQueryTotalFlows, 
                  cseFlowMcastQueryRows,
                  cseFlowMcastQueryStatus, 
                  cseFlowMcastQueryCreateTime,
                  cseFlowMcastResultSrcVlan,
                  cseFlowMcastResultCreatedTS,
                  cseFlowMcastResultLastUsedTS, 
                  cseFlowMcastResultPkts,
                  cseFlowMcastResultOctets, 
                  cseFlowMcastResultDstVlans,
                  cseFlowMcastSwitchStatus }
    STATUS      current
    DESCRIPTION
      "A collection of objects for querying IP multicast flows
      stored in hardware switching cache."
    ::= { cseMIBGroups 35 }

cseFlowMcastRtrMgmtGroup OBJECT-GROUP
    OBJECTS     { 
      cseFlowMcastQueryRtrIndex,
      cseFlowMcastResultRtrIp,
      cseFlowMcastResultRtrMac
    }
    STATUS      current
    DESCRIPTION
      "A collection of objects for specifying the router based 
      information while IP multicast flows stored in the hardware 
      switching cache are queried."
    ::= { cseMIBGroups 36 }

cseFlowMcastMgmtGroup2 OBJECT-GROUP
    OBJECTS {
      cseFlowMcastQueryMvrf,
      cseFlowMcastQueryAddrType,
      cseFlowMcastQuerySource,
      cseFlowMcastQueryGroup,
      cseFlowMcastResultMvrf,
      cseFlowMcastResultAddrType,
      cseFlowMcastResultGroup,
      cseFlowMcastResultSource,
      cseFlowMcastResultFlowType,
      cseFlowMcastResultHFlag1k2k,
      cseFlowMcastResultHFlag3k4k
    }
    STATUS      current
    DESCRIPTION
      "A collection of objects for enhanced querying of
      IP multicast flows stored in hardware switching cache."
    ::= { cseMIBGroups 37 }

cseCacheStatisticsGroup OBJECT-GROUP
    OBJECTS  { cseCacheEntriesCreated, cseCacheEntriesFailed }
    STATUS  current
    DESCRIPTION
      "A collection of objects providing switch engine statistics
      on the flow cache entries."
    ::= { cseMIBGroups 38 }

cseL3SwitchedPktsPerSecGroup OBJECT-GROUP
    OBJECTS {
      cseL3SwitchedPktsPerSec,
      cseL3SwitchedAggrPktsPerSec
    }
    STATUS current
    DESCRIPTION
      "A collection of objects providing switch engine
       statistics on total number of packets switched per
       second."
    ::= { cseMIBGroups 39 }
END
