
-- *****************************************************************************
-- Juniper-ISIS-MIB
--
-- Juniper Networks Enterprise MIB
-- Integrated IS-IS MIB
--
-- Copyright (c) 1997 The Internet Society.
-- Copyright (c) 2000, 2001 Unisphere Networks, Inc.
-- Copyright (c) 2002 Juniper Networks, Inc.
--   All Rights Reserved.
-- *****************************************************************************
                               
Juniper-ISIS-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Integer32, Counter32, Gauge32, IpAddress, Unsigned32
        FROM SNMPv2-SMI
    MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF
    InterfaceIndexOrZero
        FROM IF-MIB
    TEXTUAL-CONVENTION, DisplayString, RowStatus, TruthValue
        FROM SNMPv2-TC
    juniMibs
        FROM Juniper-MIBs;

juniIsisMIB  MODULE-IDENTITY
    LAST-UPDATED "200603131430Z"  -- 13-Mar-06 02:30 PM EST
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
        "       Juniper Networks, Inc.
        Postal: 10 Technology Park Drive
                Westford, MA  01886-3146
                USA
        Tel:    +1 978 589 5800
        Email:  mib@Juniper.net"
    DESCRIPTION
        "The intermediate system to intermediate system (IS-IS) routing protocol
        MIB for Juniper Networks E-series products.  This MIB provides
        objects for management of the IS-IS Routing protocol, as described in
        ISO 10589, when it is used to construct routing tables for IP networks,
        as described in RFC 1195."
    -- Revision History
    REVISION    "200612131330Z"  -- 13-Dec-06 01:30 PM EST  - JUNOSe 8.0
    DESCRIPTION
	"Modifiled width of juniIsisMplsTeTunnelName from 32 to 40"
    REVISION    "200603011430Z"  -- 13-Mar-06 02:30 PM EST  - JUNOSe 7.4
    DESCRIPTION
	"Added juniIsisSysReferenceBandwidth and juniIsisSysHighReferenceBandwidth
         to juniIsisSysEntry"
    REVISION    "200603011430Z"  -- 01-Mar-06 02:30 PM EST  - JUNOSe 7.4
    DESCRIPTION
	"Added juniIsisSysMplsTeSpfUseAnyBestPath to juniIsisSysEntry.
	 Added juniIsisMplsTeTunnelTable to juniIsisSystemGroup"
    REVISION    "200512261430Z"  -- 26-Dec-05 09:30 AM EST  - JUNOSe 7.0
    DESCRIPTION
	"Default value for juniIsisSysLSPIgnoreErrors is changed from false to true.
	Default value for juniIsisCircMeshGroup =1 is removed"
    REVISION    "200510210810Z"  -- 21-Oct-05 03:10 AM EST  - RX 6.1.0
    DESCRIPTION
	"L2 Buffer Size is added and is made obsolete."
	REVISION    "200503291430Z"  -- 29-Mar-05 09:30 AM EST  - JUNOSe 7.0
    DESCRIPTION
	"Updated the SystemID TEXTUAL-CONVENTION to be inline with standard
         - SystemID should now be exactly 6 bytes.
         - SystemID description modified. All zeros are invalid."
    REVISION    "200501170810Z"  -- 17-Jan-05 03:10 AM EST  - RX 6.1.0
    DESCRIPTION
	"Updated the upper bound for Max Split Paths and removed the 
	 L2 Buffer Size"
    REVISION    "200501060504Z"  -- 06-Jan-05 01:04 AM EST  - JUNOSe 7.0
    DESCRIPTION
	"Modified the default value for the juniIsisSysSetOverloadBitStartupDuration 
         object. This object has a meaning only if the ISIS overload bit 
		 is set."
    REVISION    "200411020504Z"  -- 02-Nov-04 01:04 AM EST  - RX 5.2.2
    DESCRIPTION
	"Updated the upper bound for Authentication Key Id in Area 
         Authentication, Domain Authentication, L1 Circuit and L2 Circuit 
	 Tables."
    REVISION    "200410181414Z"  -- 18-Oct-04 09:14 AM EST  - RX 5.0.4
    DESCRIPTION
        "Changed the lower bound value & default value of juniIsisSysSetOverloadBitStartupDuration
         from 0 to 5."
    REVISION    "200209162144Z"  -- 16-Sep-02 05:44 PM EDT  - JUNOSe 5.0
    DESCRIPTION
        "Replaced Unisphere names with Juniper names."
    REVISION    "200112102129Z"  -- 10-Dec-01 04:29 PM EST  - JUNOSe 4.0
    DESCRIPTION
        "Added MPLS support."
    REVISION    "200112071522Z"  -- 07-Dec-01 10:22 AM EST  - JUNOSe 3.3
    DESCRIPTION
        "Added support for simple password protection."
    REVISION    "200104172126Z"  -- 17-Apr-01 05:26 PM EDT  - JUNOSe 3.0
    DESCRIPTION
        "Add circuit state object."
    REVISION    "200002220000Z"  -- 22-Feb-00               - JUNOSe 2.0
    DESCRIPTION
        "Initial version of this MIB module, based on draft-ietf-isis-wg-mib."
    ::= { juniMibs 38 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Textual conventions
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
--
-- Type definitions
--
OSINSAddress ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "OSI Network Service Address, e.g. NSAP, Network Entity Title"
    SYNTAX      OCTET STRING (SIZE(0..20))

SystemID ::= TEXTUAL-CONVENTION
    STATUS      current
	DESCRIPTION
		 "A system ID of exactly six bytes. 
         Must not be all zeros."
    SYNTAX      OCTET STRING (SIZE(6))
    
OperState ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Type used in enabling and disabling a row."
    SYNTAX      INTEGER {
                    off(1),
                    on(2) }

AuthTime ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Then number of seconds since Jan. 1 1970."
    SYNTAX      Integer32

LSPBuffSize ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Integer sub range for LSP size."
    SYNTAX      Integer32 (512..9180)

LevelState ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "States of the ISIS protocol."
    SYNTAX      INTEGER {
                    off(1),
                    on(2),
                    waiting(3) }

SupportedProtocol ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Types of network protocol supported by Integrated ISIS.  The values for
        ISO8473 and IP are those registered for these protocols in ISO TR9577."
    SYNTAX      INTEGER {
                    iso8473(129),
                    ip(204),
                    ipV6(205) }

JuniDefaultMetric ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Integer sub-range for default metric for single hop.  The value is
        truncated to 63 when the juniIsisSysL1MetricStyle or
        juniIsisSysL2MetricStyle is set to juniIsisMetricStyleNarrow "
    SYNTAX      Integer32 (0..16777215)

OtherMetric ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Integer sub-range for metrics other than the default metric for single
        hop."
    SYNTAX      Integer32 (0..63)

CircuitID ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "ID for a circuit."
    SYNTAX      OCTET STRING (SIZE(2..9))

ISPriority ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Integer sub-range for ISIS priority."
    SYNTAX      Integer32 (1..127)


-- Behaviour Definitions

-- ResettingTimer behaviour definition
-- "This object specifies the interval between certain events in
-- the operation of the protocol state machine.  If the value of
-- this object is set to a new value while the protocol state
-- machine is in operation, the implementation shall take the
-- necessary steps to ensure that for any time interval which
-- was in progress when the value of the corresponding object
-- was changed, the next expiration of that interval takes place
-- the specified time after the original start of that interval,
-- or immediately, whichever is later.  The precision with which
-- this time shall be implemented shall be the same as that
-- associated with the basic operation of the timer object."

-- OperationalState behaviour definition
-- "This object controls the enabling and disabling of the
-- corresponding table row.  Setting this object to the value
-- off has the effect of disabling the corresponding row.
-- Setting this object to the value on has the effect of
-- enabling the corresponding row.  Setting the value of this
-- object to the same value as its current value has no effect.
-- If the table entry also contains an object controlling the
-- RowStatus then the object following the operationalState
-- behaviour shall not be set to on when the object following
-- the RowStatus behaviour has value off.  An attempt to do
-- so is rejected."


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Managed objects
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniIsisObjects      OBJECT IDENTIFIER ::= { juniIsisMIB 1 }
juniIsisTrapGroup    OBJECT IDENTIFIER ::= { juniIsisMIB 2 }
juniIsisConformance  OBJECT IDENTIFIER ::= { juniIsisMIB 3 }

juniIsisSystemGroup  OBJECT IDENTIFIER ::= { juniIsisObjects 1}
juniIsisCircuitGroup OBJECT IDENTIFIER ::= { juniIsisObjects 2 }

juniIsisSysTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIsisSysEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The set of instances of the Integrated IS-IS protocol existing on the
        system."
    ::= { juniIsisSystemGroup 1 }

juniIsisSysEntry OBJECT-TYPE
    SYNTAX      JuniIsisSysEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row defines information specific to a single instance of the
        protocol existing on the system."
    REFERENCE
        "ISIS.poi cLNSISISBasic-P (1)"
    INDEX     { juniIsisSysInstance }
    ::= { juniIsisSysTable 1 }

JuniIsisSysEntry ::= SEQUENCE {
    juniIsisSysInstance                      Integer32,
    juniIsisSysVersion                       DisplayString,
    juniIsisSysType                          INTEGER,
    juniIsisSysID                            SystemID,
    juniIsisSysMaxPathSplits                 Integer32,
    juniIsisSysMaxLSPGenInt                  Integer32,
    juniIsisSysOrigLSPBuffSize               LSPBuffSize,
    juniIsisSysMaxAreaAddresses              Integer32,
    juniIsisSysMinL1LSPGenInt                Integer32,
    juniIsisSysMinL2LSPGenInt                Integer32,
    juniIsisSysPollESHelloRate               Integer32,
    juniIsisSysWaitTime                      Integer32,
    juniIsisSysOperState                     OperState,
    juniIsisSysL1State                       LevelState,
    juniIsisSysCorrLSPs                      Counter32,
    juniIsisSysLSPL1DbaseOloads              Counter32,
    juniIsisSysManAddrDropFromAreas          Counter32,
    juniIsisSysAttmptToExMaxSeqNums          Counter32,
    juniIsisSysSeqNumSkips                   Counter32,
    juniIsisSysOwnLSPPurges                  Counter32,
    juniIsisSysIDFieldLenMismatches          Counter32,
    juniIsisSysMaxAreaAddrMismatches         Counter32,
    juniIsisSysOrigL2LSPBuffSize             LSPBuffSize,
    juniIsisSysL2State                       LevelState,
    juniIsisSysLSPL2DbaseOloads              Counter32,
    juniIsisSysAuthFails                     Counter32,
    juniIsisSysLSPIgnoreErrors               TruthValue,
    juniIsisSysMaxAreaCheck                  TruthValue,
    juniIsisSysSetOverloadBit                TruthValue,
    juniIsisSysSetOverloadBitStartupDuration Integer32,
    juniIsisSysMaxLspLifetime                Integer32,
    juniIsisSysL1SpfInterval                 Integer32,
    juniIsisSysL2SpfInterval                 Integer32,
    juniIsisSysIshHoldTime                   Integer32,
    juniIsisSysIshConfigTimer                Integer32,
    juniIsisSysDistributeDomainWide          TruthValue,
    juniIsisSysDistance                      Integer32,
    juniIsisSysL1MetricStyle                 INTEGER,
    juniIsisSysL2MetricStyle                 INTEGER,
    juniIsisSysIsoRouteTag                   OCTET STRING,
    juniIsisSysMplsTeLevel                   INTEGER,
    juniIsisSysMplsTeRtrIdIfIndex            InterfaceIndexOrZero,
    juniIsisSysMplsTeSpfUseAnyBestPath       TruthValue,
    juniIsisSysReferenceBandwidth            Gauge32,
    juniIsisSysHighReferenceBandwidth        Gauge32 }

juniIsisSysInstance OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The unique identifier of the Integrated IS-IS instance to which this
        row corresponds.  This object follows the index behaviour."
    ::= { juniIsisSysEntry 1 }

juniIsisSysVersion OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..24))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The version number of the IS-IS protocol to which this instance
        conforms.  This value must be set by the implementation when the row is
        valid."
    REFERENCE
        "ISIS.aoi version (1)"
    ::= { juniIsisSysEntry 2 }

juniIsisSysType OBJECT-TYPE
    SYNTAX      INTEGER {
                    level1IS(1),
                    level1l2IS(2),
                    level2Only(3) }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The type of this instance of the Integrated IS-IS protocol.  This
        object follows the replaceOnlyWhileDisabled behaviour."
    REFERENCE
        "ISIS.aoi iSType (2)"
    ::= { juniIsisSysEntry 3 }

juniIsisSysID OBJECT-TYPE
    SYNTAX      SystemID
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The ID for this instance of the Integrated IS-IS protocol.  This value
        is appended to each of the instance's area addresses to form the Network
        Entity Titles valid for this instance.  The derivation of a value for
        this object is implementation-specific.  Some implementations may assign
        values and not permit write MAX-ACCESS, others may require the value to
        be set manually."
    REFERENCE
        "ISIS.aoi systemId (119)"
    ::= { juniIsisSysEntry 4 }

juniIsisSysMaxPathSplits OBJECT-TYPE
    SYNTAX      Integer32 (1..16)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Maximum number of paths with equal routing metric value which it is
        permitted to split between.  This object follows the
        replaceOnlyWhileDisabled behaviour."
    REFERENCE
        "ISIS.aoi maximumPathSplits (3)"
    DEFVAL    { 4 }
    ::= { juniIsisSysEntry 5 }

juniIsisSysMaxLSPGenInt OBJECT-TYPE
    SYNTAX      Integer32 (1..65535)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Maximum interval, in seconds, between generated LSPs by this instance.
        This object follows the resettingTimer behaviour."
    REFERENCE
        "ISIS.aoi maximumLSPGenerationInterval (6)"
    DEFVAL    { 900 }
    ::= { juniIsisSysEntry 6 }

juniIsisSysOrigLSPBuffSize OBJECT-TYPE
    SYNTAX      LSPBuffSize
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The maximum size of LSPs and SNPs originated by this instance.
        This object follows the replaceOnlyWhileDisabled behaviour."
    REFERENCE
        "ISIS.aoi originatingLSPBufferSize (9)"
    DEFVAL    { 1497 }
    ::= { juniIsisSysEntry 7 }

juniIsisSysMaxAreaAddresses OBJECT-TYPE
    SYNTAX      Integer32 (0..254)
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The maximum number of area addresses to be permitted for the area in
        which this instance exists.  Note that all Intermediate Systems in the
        same area must have the same value configured for this attribute if
        correct operation is to be assumed.  This object follows the
        replaceOnlyWhileDisabled behaviour."
    REFERENCE
        "ISIS.aoi maximumAreaAddresses (4)"
    DEFVAL    { 3 }
    ::= { juniIsisSysEntry 8 }

juniIsisSysMinL1LSPGenInt OBJECT-TYPE
    SYNTAX      Integer32 (0..120)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Minimum interval, in seconds, between successive generation of L1 LSPs
        with the same LSPID by this instance.  This object follows the
        resettingTimer behaviour."
    REFERENCE
        "ISIS.aoi minimumLSPGenerationInterval (11)"
    DEFVAL    { 5 }
    ::= { juniIsisSysEntry 9 }

juniIsisSysMinL2LSPGenInt OBJECT-TYPE
    SYNTAX      Integer32 (0..120)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Minimum interval, in seconds, between successive generation of L2 LSPs
        with the same LSPID by this instance.  This object follows the
        resettingTimer behaviour."
    REFERENCE
        "ISIS.aoi minimumLSPGenerationInterval (11)"
    DEFVAL    { 5 }
    ::= { juniIsisSysEntry 10 }

juniIsisSysPollESHelloRate OBJECT-TYPE
    SYNTAX      Integer32 (1..65535)
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value, in seconds, to be used for the suggested ES configuration
        timer in ISH PDUs when soliciting the ES configuration."
    REFERENCE
        "ISIS.aoi pollESHelloRate (13)"
    DEFVAL    { 10 }
    ::= { juniIsisSysEntry 11 }

juniIsisSysWaitTime OBJECT-TYPE
    SYNTAX      Integer32 (1..65535)
    UNITS       "seconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of seconds to delay in waiting state before entering on state.
        This object follows the resettingTimer behaviour."
    REFERENCE
        "ISIS.aoi waitingTime (15)"
    DEFVAL    { 60 }
    ::= { juniIsisSysEntry 12 }

juniIsisSysOperState OBJECT-TYPE
    SYNTAX      OperState
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The operational state of this instance of the Integrated IS-IS
        protocol.  Setting this object to the value on when its current value is
        off enables operation of this instance of the Integrated IS-IS
        protocol."
    DEFVAL    { off }
    ::= { juniIsisSysEntry 13 }

juniIsisSysL1State OBJECT-TYPE
    SYNTAX      LevelState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The state of the Level 1 database."
    REFERENCE
        "ISIS.aoi l1State (17)"
    ::= { juniIsisSysEntry 14 }

juniIsisSysCorrLSPs OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of corrupted LSPs detected."
    REFERENCE
        "ISIS.aoi corruptedLSPsDetected (19)"
    ::= { juniIsisSysEntry 15 }

juniIsisSysLSPL1DbaseOloads OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of times the LSP L1 database has become overloaded."
    REFERENCE
        "ISIS.aoi lSPL1DatabaseOverloads (20)"
    ::= { juniIsisSysEntry 16 }

juniIsisSysManAddrDropFromAreas OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of times a manual address has been dropped from the area."
    REFERENCE
        "ISIS.aoi manualAddressesDroppedFromArea (21)"
    ::= { juniIsisSysEntry 17 }

juniIsisSysAttmptToExMaxSeqNums OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of times the IS has attempted to exceed the maximum sequence
        number."
    REFERENCE
        "ISIS.aoi attemptsToExceedmaximumSequenceNumber (22)"
    ::= { juniIsisSysEntry 18 }

juniIsisSysSeqNumSkips OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of times a sequence number skip has occurred."
    REFERENCE
        "ISIS.aoi sequenceNumberSkips (23)"
    ::= { juniIsisSysEntry 19 }

juniIsisSysOwnLSPPurges OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of times a zero-aged copy of the system's own LSP is received
        from some other node."
    REFERENCE
        "ISIS.aoi ownLSPPurges (24)"
    ::= { juniIsisSysEntry 20 }

juniIsisSysIDFieldLenMismatches OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of times a PDU is received with a different value for ID field
        length to that of the receiving system."
    REFERENCE
        "ISIS.aoi iDFieldLengthMismatches (25)"
    ::= { juniIsisSysEntry 21 }

juniIsisSysMaxAreaAddrMismatches OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of times a PDU is received with a different value for
        MaximumAreaAddresses from that of the receiving system."
    REFERENCE
        "ISIS.aoi MaximumAreaAddressesMismatches (118)"
    ::= { juniIsisSysEntry 22 }

-- The following objects map those from the cLNSISISLevel2-P Package

juniIsisSysOrigL2LSPBuffSize OBJECT-TYPE
    SYNTAX      LSPBuffSize
    MAX-ACCESS  read-write
    STATUS      obsolete
    DESCRIPTION
        "The maximum size of Level 2 LSPs and SNPs originated by this system.
        This object follows the replaceOnlyWhileDisabled behaviour."
    REFERENCE
        "ISIS.aoi originatingL2LSPBufferSize (26)"
    DEFVAL    { 1497 }
    ::= { juniIsisSysEntry 23 }
    
juniIsisSysL2State OBJECT-TYPE
    SYNTAX      LevelState
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The state of the Level 2 database."
    REFERENCE
        "ISIS.aoi l2State (28)"
    ::= { juniIsisSysEntry 24 }

juniIsisSysLSPL2DbaseOloads OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of times the Level 2 LSP database has become overloaded."
    REFERENCE
        "ISIS.aoi lSPL2DatabaseOverloads (32)"
    ::= { juniIsisSysEntry 25 }

juniIsisSysAuthFails OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of authentication failures recognized by this instance of
        the protocol."
    ::= { juniIsisSysEntry 26 }

juniIsisSysLSPIgnoreErrors OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "If true, allow the router to ignore IS-IS link state packets (LSPs)
        that are received with internal checksum errors rather than purging the
        LSPs."
    DEFVAL    { true }
    ::= { juniIsisSysEntry 27 }

juniIsisSysMaxAreaCheck OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "When on, enables checking of maximum area addresses per IS version of
        ISO10589."
    DEFVAL    { true }
    ::= { juniIsisSysEntry 28 }

juniIsisSysSetOverloadBit OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Isis overload bit"
    DEFVAL    { false }
    ::= { juniIsisSysEntry 29 }

juniIsisSysSetOverloadBitStartupDuration OBJECT-TYPE
    SYNTAX      Integer32 (0|5..86400)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION

        "Specifies the length in time of seconds to set the overload bit from
        startup.  This object must be set together with
        juniIsisSysSetOverloadBit, otherwise the agent will return zero.
		Zero value for this object implies that the overload bit is not set.
		Zero value does not have any meaning for this object."
    DEFVAL    { 0 }
    ::= { juniIsisSysEntry 30 }

juniIsisSysMaxLspLifetime  OBJECT-TYPE
    SYNTAX      Integer32 (1..65535)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Specifies the maximum time (in seconds) a LSP will remain in the box
        without being refreshed before being considered invalid."
    DEFVAL    { 1200 }
    ::= { juniIsisSysEntry 31 }

juniIsisSysL1SpfInterval OBJECT-TYPE
    SYNTAX      Integer32 (0..120)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Minimum interval, in seconds, between level 1 SPF calculations."
    DEFVAL    { 5 }
    ::= { juniIsisSysEntry 32 }

juniIsisSysL2SpfInterval OBJECT-TYPE
    SYNTAX      Integer32 (0..120)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Minimum interval, in seconds, between level 2 SPF calculations."
    DEFVAL    { 5 }
    ::= { juniIsisSysEntry 33 }

juniIsisSysIshHoldTime OBJECT-TYPE
    SYNTAX      Integer32 (1..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Specify a holdtime advertised in ESH/ISH PDUs."
    DEFVAL    { 30 }
    ::= { juniIsisSysEntry 34 }

juniIsisSysIshConfigTimer OBJECT-TYPE
    SYNTAX      Integer32 (1..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Specify the rate of transmission for ESH and ISH packets."
    DEFVAL    { 10 }
    ::= { juniIsisSysEntry 35 }

juniIsisSysDistributeDomainWide OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "When on, enables distribution of prefixes throughout a multi-level
        domain."
    DEFVAL    { false }
    ::= { juniIsisSysEntry 36 }

juniIsisSysDistance OBJECT-TYPE
    SYNTAX      Integer32 (1..255)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The weight applied to IS-IS routes."
    DEFVAL    { 115 }
    ::= { juniIsisSysEntry 37 }

juniIsisSysL1MetricStyle OBJECT-TYPE
    SYNTAX      INTEGER {
                    juniIsisMetricStyleNarrow(2),
                    juniIsisMetricStyleNarrowTransition(3),
                    juniIsisMetricStyleTransition(4),
                    juniIsisMetricStyleWide(5),
                    juniIsisMetricStyleWideTransition(6) }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Specifies the type of IP reachability TLV to advertise in level 1
        LSPs."
    DEFVAL    { juniIsisMetricStyleNarrow }
    ::= { juniIsisSysEntry 38 }

juniIsisSysL2MetricStyle OBJECT-TYPE
    SYNTAX      INTEGER {
                    juniIsisMetricStyleNarrow(2),
                    juniIsisMetricStyleNarrowTransition(3),
                    juniIsisMetricStyleTransition(4),
                    juniIsisMetricStyleWide(5),
                    juniIsisMetricStyleWideTransition(6) }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Specifies the type of IP reachability TLV to advertise in level 2
        LSPs."
    DEFVAL    { juniIsisMetricStyleNarrow }
    ::= { juniIsisSysEntry 39 }

juniIsisSysIsoRouteTag OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(1..19))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
         "The ISO routing area tag."
    DEFVAL    { "" }
    ::= { juniIsisSysEntry 40 }

juniIsisSysMplsTeLevel OBJECT-TYPE
    SYNTAX      INTEGER {
                    levelNone(0),
                    level1(1),
                    level2(2) }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Select flooding of MPLS traffic engineering link information into the
        specified ISIS level."
    ::= { juniIsisSysEntry 41 }

juniIsisSysMplsTeRtrIdIfIndex OBJECT-TYPE
    SYNTAX       InterfaceIndexOrZero
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
        "Configure the stable router interface ID to designate it as TE capable.
        A value of zero is used to remove any configured router interface ID."
    ::= { juniIsisSysEntry 42 }  
    
juniIsisSysMplsTeSpfUseAnyBestPath OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
        "Configure whether or not to consider spf paths when alternate 
         tunnel path exists"
    ::= { juniIsisSysEntry 43 }

juniIsisSysReferenceBandwidth OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
        "Configure the reference bandwitdth used to calculate the link cost in 
         bits per second.If the reference bandwidth is greater than the maximum 
         value reportable by this object then this object should report its 
         maximum value (4,294,967,295) and juniIsisSysHighReferenceBandwidth must 
         be used to report the reference bandwidth. "
    ::= { juniIsisSysEntry 44 }

juniIsisSysHighReferenceBandwidth OBJECT-TYPE
    SYNTAX       Gauge32(1..1000000)
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
        "Configure the reference bandwitdth in mega bits per second.
         It is used to calculate the link cost."
    ::= { juniIsisSysEntry 45 }

--
-- The Level 1 Manual Area Address Table contains the set of area addresses
-- manually configured for each instance of the Integrated IS-IS protocol.
-- At least one row in which the value of juniIsisManAreaAddRowStatus is on
-- must be present for each instance of the protocol when juniIsisSysOperState
-- is also on for that instance.  The maximum number of rows in this table for
-- each instance of the protocol for which the object
-- juniIsisManAreaAddrRowStatus has the value on is the value of
-- maximumAreaAddresses (as defined in ISO 10589) for that instance.
-- An Attempt to create a new row such that the number of rows with
-- juniIsisManAreaAddrRowStatus set to on for that protocol instance exceeds
-- maximumAreaAddresses is rejected.
--
juniIsisManAreaAddrTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIsisManAreaAddrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The set of manual area addresses configured on this Intermediate
        System."
    REFERENCE
        "ISIS.aoi manualAreaAddresses (10)"
    ::= { juniIsisSystemGroup 2 }

juniIsisManAreaAddrEntry OBJECT-TYPE
    SYNTAX      JuniIsisManAreaAddrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry contains one area address manually configured on this
        system."
    INDEX     { juniIsisManAreaAddrSysInstance,
                juniIsisManAreaAddr }
    ::= { juniIsisManAreaAddrTable 1 }

JuniIsisManAreaAddrEntry ::= SEQUENCE {
    juniIsisManAreaAddrSysInstance   Integer32,
    juniIsisManAreaAddr              OSINSAddress,
    juniIsisManAreaAddrRowStatus     RowStatus }

juniIsisManAreaAddrSysInstance OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The unique identifier of the Integrated IS-IS instance to which this
        row corresponds.  This object follows the index behaviour."
    ::= { juniIsisManAreaAddrEntry 1 }

juniIsisManAreaAddr OBJECT-TYPE
    SYNTAX      OSINSAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A manually configured area address for this system.  This object
        follows the index behaviour.

        Note:  an index for the entry {1, {49.0001} active} in this table would
        be the ordered pair (1, (0x03 0x49 0x00 0x01)), as the length of an
        octet string is part of the OID."
    ::= { juniIsisManAreaAddrEntry 2 }

juniIsisManAreaAddrRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The state of the juniIsisManAreaAddrEntry.  This object follows the
        RowStatus behaviour.  If an attempt is made to set this object to the
        value off when the corresponding juniIsisManAreaAddrEntry is the only
        valid entry for this instance and when the corresponding IS-IS instance
        has juniIsisSysOperState set to on then the attempt is rejected."
    DEFVAL    { active }
    ::= { juniIsisManAreaAddrEntry 3 }


--
-- The System Integrated Group
--
-- The System Integrated Group is present if the system supports Integrated ISIS
-- at Level 1.
--
-- The System Protocol Supported Table
--
-- The System Protocol Supported Table contains the manually configured set of
-- protocols supported by each instance of the Integrated ISIS protocol.
--
juniIsisSysProtSuppTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIsisSysProtSuppEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains the manually configured set of protocols supported
        by each instance of the Integrated ISIS protocol."
    ::= { juniIsisSystemGroup 3 }

juniIsisSysProtSuppEntry OBJECT-TYPE
    SYNTAX      JuniIsisSysProtSuppEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry contains one protocol supported by an instance of the
        Integrated ISIS protocol."
    INDEX     { juniIsisSysProtSuppSysInstance,
                juniIsisSysProtSuppProtocol }
    ::= { juniIsisSysProtSuppTable 1 }

JuniIsisSysProtSuppEntry ::= SEQUENCE {
    juniIsisSysProtSuppSysInstance   Integer32,
    juniIsisSysProtSuppProtocol      SupportedProtocol,
    juniIsisSysProtSuppRowStatus     RowStatus }

juniIsisSysProtSuppSysInstance OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The unique identifier of the Integrated IS-IS instance to which this
        row corresponds.  This object follows the index behaviour."
    ::= { juniIsisSysProtSuppEntry 1 }

juniIsisSysProtSuppProtocol OBJECT-TYPE
    SYNTAX      SupportedProtocol
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "One supported protocol.  This object follows the index behaviour."
    ::= { juniIsisSysProtSuppEntry 2 }

juniIsisSysProtSuppRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The state of the juniIsisSysProtSuppEntry.  This object follows the
        RowStatus behavior."
    DEFVAL    { active }
    ::= { juniIsisSysProtSuppEntry 3 }


--
-- The Summary Address Table
--
-- The Summary Address Table contains the set of summary addresses manually
-- configured for each instance of IP Integrated ISIS on the system.
--
juniIsisSummAddrTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIsisSummAddrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The set of IP summary addresses to use in forming the contents of Level
        2 LSPs originated by this level 2 Intermediate System."
    ::= { juniIsisSystemGroup 4 }

juniIsisSummAddrEntry OBJECT-TYPE
    SYNTAX      JuniIsisSummAddrEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry contains one IP summary address."
    INDEX     { juniIsisSummAddrSysInstance,
                juniIsisSummAddress,
                juniIsisSummAddrMask }
    ::= { juniIsisSummAddrTable 1 }

JuniIsisSummAddrEntry ::= SEQUENCE {
    juniIsisSummAddrSysInstance      Integer32,
    juniIsisSummAddress              IpAddress,
    juniIsisSummAddrMask             IpAddress,
    juniIsisSummAddrRowStatus        RowStatus,
    juniIsisSummAddrOperState        OperState,
    juniIsisSummAddrDefaultMetric    Integer32,
    juniIsisSummAddrDelayMetric      OtherMetric,
    juniIsisSummAddrExpenseMetric    OtherMetric,
    juniIsisSummAddrErrorMetric      OtherMetric,
    juniIsisSummLevel                INTEGER }

juniIsisSummAddrSysInstance OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The unique identifier of the Integrated IS-IS instance to which this
        row corresponds.  This object follows the index behaviours."
    ::= { juniIsisSummAddrEntry 1 }

juniIsisSummAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The IP Address value for this summary address.  This object follows the
        index behaviour."
    ::= { juniIsisSummAddrEntry 2 }

juniIsisSummAddrMask OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The mask value for this summary address.  This object follows the index
        behaviour."
    ::= { juniIsisSummAddrEntry 3 }

juniIsisSummAddrRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The existence state of this summary address.  This object follows the
        RowStatus behaviour."
    ::= { juniIsisSummAddrEntry 4 }

juniIsisSummAddrOperState OBJECT-TYPE
    SYNTAX      OperState
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The operational state of this entry.  This object follows the
        operationalState behaviour.  When the operational state changes if this
        would cause the contents of LSPs originated by the system to change then
        those new LSPs must be generated and sent as soon as is permitted by the
        ISIS protocol."
    ::= { juniIsisSummAddrEntry 5 }

juniIsisSummAddrDefaultMetric OBJECT-TYPE
    SYNTAX      Integer32 (0..16777214)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION

        "The default metric value to announce this summary address with in Level
        1 or 2 LSPs generated by this system.  A Metric value of 0 indicates to
        use the lowest metric value amongst the routes being summarized.  When
        advertising a metric value into a narrow domain
        (juniIsisSysL1MetricStyle or juniIsisSysL2MetricStyle is set to
        juniIsisMetricStyleNarrow) the value will be truncated to 63."
    ::= { juniIsisSummAddrEntry 6 }

juniIsisSummAddrDelayMetric OBJECT-TYPE
    SYNTAX      OtherMetric
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The delay metric value to announce this summary address with in Level 2
        LSPs generated by this system.  The value of zero is reserved to
        indicate that this metric is not supported."
    ::= { juniIsisSummAddrEntry 7 }

juniIsisSummAddrExpenseMetric OBJECT-TYPE
    SYNTAX      OtherMetric
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The expense metric value to announce this summary address with in Level
        2 LSPs generated by this system.  The value of zero is reserved to
        indicate that this metric is not supported."
    ::= { juniIsisSummAddrEntry 8 }

juniIsisSummAddrErrorMetric OBJECT-TYPE
    SYNTAX      OtherMetric
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The error metric value to announce this summary address with in Level n
        LSPs generated by this system.  The value of zero is reserved to
        indicate that this metric is not supported."
    ::= { juniIsisSummAddrEntry 9 }

juniIsisSummLevel OBJECT-TYPE
    SYNTAX      INTEGER {
                    level1IS(1),
                    level2IS(2),
                    level1l2IS(3) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The level of database at which to annouce this summary."
    ::= { juniIsisSummAddrEntry 10 }

--
-- The Circuit Group
--
-- The Circuit Group is current
--
-- The Circuit Table
-- Each broadcast or point-to-point interface on the system corresponds to one
-- entry in the Circuit table.
--
juniIsisCircTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIsisCircEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The table of circuits used by each instance of Integrated IS-IS on this
        system."
    ::= { juniIsisCircuitGroup 1 }

juniIsisCircEntry OBJECT-TYPE
    SYNTAX      JuniIsisCircEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An juniIsisCircEntry exists for each circuit used by Integrated IS-IS
        on this system."
    INDEX     { juniIsisCircSysInstance,
                juniIsisCircIfIndex }
    ::= { juniIsisCircTable 1 }

JuniIsisCircEntry ::= SEQUENCE {
    juniIsisCircSysInstance          Integer32,
    juniIsisCircIfIndex              Integer32,
    juniIsisCircLocalID              Integer32,
    juniIsisCircOperState            OperState,
    juniIsisCircRowStatus            RowStatus,
    juniIsisCircType                 INTEGER,
    juniIsisCircL1DefaultMetric      JuniDefaultMetric,
    juniIsisCircL1DelayMetric        OtherMetric,
    juniIsisCircL1ExpenseMetric      OtherMetric,
    juniIsisCircL1ErrorMetric        OtherMetric,
    juniIsisCircExtDomain            TruthValue,
    juniIsisCircAdjChanges           Counter32,
    juniIsisCircInitFails            Counter32,
    juniIsisCircRejAdjs              Counter32,
    juniIsisCircOutCtrlPDUs          Counter32,
    juniIsisCircInCtrlPDUs           Counter32,
    juniIsisCircIDFieldLenMismatches Counter32,
    juniIsisCircL2DefaultMetric      JuniDefaultMetric,
    juniIsisCircL2DelayMetric        OtherMetric,
    juniIsisCircL2ExpenseMetric      OtherMetric,
    juniIsisCircL2ErrorMetric        OtherMetric,
    juniIsisCircManL2Only            TruthValue,
    juniIsisCircL1ISPriority         ISPriority,
    juniIsisCircL1CircID             CircuitID,
    juniIsisCircL1DesIS              SystemID,
    juniIsisCircLANL1DesISChanges    Counter32,
    juniIsisCircL2ISPriority         ISPriority,
    juniIsisCircL2CircID             CircuitID,
    juniIsisCircL2DesIS              SystemID,
    juniIsisCircLANL2DesISChanges    Counter32,
    juniIsisCircMCAddr               INTEGER,
    juniIsisCircPtToPtCircID         CircuitID,
    juniIsisCircL1HelloTimer         Integer32,
    juniIsisCircL2HelloTimer         Integer32,
    juniIsisCircL1HelloMultiplier    Integer32,
    juniIsisCircL2HelloMultiplier    Integer32,
    juniIsisCircMinLSPTransInt       Unsigned32,
    juniIsisCircMinLSPReTransInt     Integer32,
    juniIsisCircL1CSNPInterval       Integer32,
    juniIsisCircL2CSNPInterval       Integer32,
    juniIsisCircLSPThrottle          Integer32,
    juniIsisCircMeshGroupEnabled     INTEGER,
    juniIsisCircMeshGroup            Unsigned32,
    juniIsisCircLevel                INTEGER,
    juniIsisCircState                INTEGER }

juniIsisCircSysInstance OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The unique identifier of the Integrated IS-IS instance to which this
        row corresponds.  This object follows the index behaviour."
    ::= { juniIsisCircEntry 1 }

juniIsisCircIfIndex OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of ifIndex for the interface to which this circuit
        corresponds."
    ::= { juniIsisCircEntry 2 }

juniIsisCircLocalID OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "An identification that can be used in protocol packets to identify a
        circuit.  Implementations may devise ways to assure that this value is
        suitable for the circuit it is used on.  LAN packets only have space for
        8 bits.

        Values of juniIsisCircLocalID do not need to be unique.  They are only
        required to differ on LANs where the Intermediate System is the
        Designated Intermediate System."
    ::= { juniIsisCircEntry 3 }

juniIsisCircOperState OBJECT-TYPE
    SYNTAX      OperState
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The operational state of the circuit.  This object follows the
        operationalState behaviour."
    DEFVAL    { off }
    ::= { juniIsisCircEntry 4 }

juniIsisCircRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The existence state of this circuit.  This object follows the RowStatus
        behaviour."
    DEFVAL    { active }
    ::= { juniIsisCircEntry 5 }

juniIsisCircType OBJECT-TYPE
    SYNTAX      INTEGER {
                    broadcast(1),
                    ptToPt(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The type of the circuit.  This object follows the
        replaceOnlyWhileDisabled behaviour.  The type specified must be
        compatible with the type of the interface defined by the value of
        juniIsisCircIfIndex."
    REFERENCE
        "ISIS.aoi type (33)"
    ::= { juniIsisCircEntry 6 }

juniIsisCircL1DefaultMetric OBJECT-TYPE
    SYNTAX      JuniDefaultMetric
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The default metric value of this circuit for Level 1 traffic."
    REFERENCE
        "ISIS.aoi l1DefaultMetric (35)"
    DEFVAL    { 10 }
    ::= { juniIsisCircEntry 7 }

juniIsisCircL1DelayMetric OBJECT-TYPE
    SYNTAX      OtherMetric
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The delay metric value of this circuit for Level 1 traffic.  The value
        of zero is reserved to indicate that this metric is not supported."
    REFERENCE
        "ISIS.aoi l1DelayMetric (36)"
    DEFVAL    { 0 }
    ::= { juniIsisCircEntry 8 }

juniIsisCircL1ExpenseMetric OBJECT-TYPE
    SYNTAX      OtherMetric
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The expense metric value of this circuit for Level 1 traffic.  The
        value of zero is reserved to indicate that this metric is not
        supported."
    REFERENCE
        "ISIS.aoi l1ExpenseMetric (37)"
    DEFVAL    { 0 }
    ::= { juniIsisCircEntry 9 }

juniIsisCircL1ErrorMetric OBJECT-TYPE
    SYNTAX      OtherMetric
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The error metric value of this circuit for Level 1 traffic.  The value
        of zero is reserved to indicate that this metric is not supported."
    REFERENCE
        "ISIS.aoi l1ErrorMetric (38)"
    DEFVAL    { 0 }
    ::= { juniIsisCircEntry 10 }

juniIsisCircExtDomain OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "If true, suppress normal transmission of and interpretation of
        Intra-domain ISIS PDUs on this circuit."
    REFERENCE
        "ISIS.aoi externalDomain (46)"
    DEFVAL    { false }
    ::= { juniIsisCircEntry 11 }

juniIsisCircAdjChanges OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of times an adjacency state change has occurred on this
        circuit."
    REFERENCE
        "ISIS.aoi changesInAdjacencyState (40)"
    ::= { juniIsisCircEntry 12 }

juniIsisCircInitFails OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of times initialization of this circuit has failed."
    REFERENCE
        "ISIS.aoi initializationFailures (41)"
    ::= { juniIsisCircEntry 13 }

juniIsisCircRejAdjs OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of times an adjacency has been rejected on this circuit."
    REFERENCE
        "ISIS.aoi rejectedAdjacencies (42)"
    ::= { juniIsisCircEntry 14 }

juniIsisCircOutCtrlPDUs OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of IS-IS control PDUs sent on this circuit."
    REFERENCE
        "ISIS.aoi iSISControlPDUsSent (43)"
    ::= { juniIsisCircEntry 15 }

juniIsisCircInCtrlPDUs OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of IS-IS control PDUs received on this circuit."
    REFERENCE
        "ISIS.aoi controlPDUsReceived (44)"
    ::= { juniIsisCircEntry 16 }

juniIsisCircIDFieldLenMismatches OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of times an IS-IS control PDU with an ID field length
        different to that for this system has been received."
    REFERENCE
        "ISIS.aoi iDFieldLengthMismatches (25)"
    ::= { juniIsisCircEntry 17 }


--
-- The following objects map those from the linkageISISLevel2-P package
--
juniIsisCircL2DefaultMetric OBJECT-TYPE
    SYNTAX      JuniDefaultMetric
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The default metric value of this circuit for level 2 traffic."
    REFERENCE
        "ISIS.aoi l2DefaultMetric (68)"
    DEFVAL    { 10 }
    ::= { juniIsisCircEntry 18 }

juniIsisCircL2DelayMetric OBJECT-TYPE
    SYNTAX      OtherMetric
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The delay metric value of this circuit for level 2 traffic.  The value
        of zero is reserved to indicate that this metric is not supported."
    REFERENCE
        "ISIS.aoi l2DelayMetric (69)"
    DEFVAL    { 0 }
    ::= { juniIsisCircEntry 19 }

juniIsisCircL2ExpenseMetric OBJECT-TYPE
    SYNTAX      OtherMetric
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The expense metric value of this circuit for level 2 traffic.  The
        value of zero is reserved to indicate that this metric is not
        supported."
    REFERENCE
        "ISIS.aoi l2ExpenseMetric (70)"
    DEFVAL    { 0 }
    ::= { juniIsisCircEntry 20 }

juniIsisCircL2ErrorMetric OBJECT-TYPE
    SYNTAX      OtherMetric
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The error metric value of this circuit for level 2 traffic.  The value
        of zero is reserved to indicate that this metric is not supported."
    REFERENCE
        "ISIS.aoi l2ErrorMetric (71)"
    DEFVAL    { 0 }
    ::= { juniIsisCircEntry 21 }

juniIsisCircManL2Only OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "When true, indicates that this circuit is to be used only for level 2.
        This object follows the replaceOnlyWhileDisabled behaviour."
    REFERENCE
        "ISIS.aoi manualL2OnlyMode (72)"
    DEFVAL    { false }
    ::= { juniIsisCircEntry 22 }


--
-- The following objects map those from the linkageISISBroadcast-P package
--
juniIsisCircL1ISPriority OBJECT-TYPE
    SYNTAX      ISPriority
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The priority for becoming LAN Level 1 Deignated Intermediate System on
        a broadcast circuit."
    REFERENCE
        "ISIS.aoi l1IntermediateSystemPriority (47)"
    DEFVAL    { 64 }
    ::= { juniIsisCircEntry 23 }

juniIsisCircL1CircID OBJECT-TYPE
    SYNTAX      CircuitID
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The LAN ID allocated by the LAN Level 1 Designated Intermediate System.
        Where this system is not aware of the value (because it is not
        participating in the Level 1 Designated Intermediate System election),
        this object has the value which would be proposed for this circuit (i.e.
        the concatenation of the local system ID and the one octet local Circuit
        ID for this circuit."
    REFERENCE
        "ISIS.aoi l1CircuitID (48)"
    ::= { juniIsisCircEntry 24 }

juniIsisCircL1DesIS OBJECT-TYPE
    SYNTAX      SystemID
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The ID of the LAN Level 1 Designated Intermediate System on this
        circuit.  If, for any reason this system is not partaking in the
        relevant Designated Intermediate System election process, then the value
        returned is the zero length OCTET STRING."
    REFERENCE
        "ISIS.aoi l1DesignatedIntermediateSystem (49)"
    ::= { juniIsisCircEntry 25 }

juniIsisCircLANL1DesISChanges OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of times the LAN Level 1 Designated Intermediate System has
        changed."
    REFERENCE
        "ISIS.aoi lanL1DesignatedIntermediateSystemChanges (50)"
    ::= { juniIsisCircEntry 26 }

-- The following objects map those from the linkageISISLevel2Broadcast-P package

juniIsisCircL2ISPriority OBJECT-TYPE
    SYNTAX      ISPriority
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The priority for becoming LAN level 2 Designated Intermediate System."
    REFERENCE
        "ISIS.aoi l2IntermediateSystemPriority (73)"
    DEFVAL    { 64 }
    ::= { juniIsisCircEntry 27 }

juniIsisCircL2CircID OBJECT-TYPE
    SYNTAX      CircuitID
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The LAN ID allocated by the LAN Level 2 Designated Intermediate System.
        Where this system is not aware of this value (because it is not
        participating in the Level 2 Designated Intermediate System election),
        this object has the value which would be proposed for this circuit
        (i.e. the concatenation of the local system ID and the one octet local
        Circuit ID for this circuit."
    REFERENCE
        "ISIS.aoi l2CircuitID (74)"
    ::= { juniIsisCircEntry 28 }

juniIsisCircL2DesIS OBJECT-TYPE
    SYNTAX      SystemID
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The ID of the LAN Level 2 Designated Intermediate System on this
        circuit.  If, for any reason, this system is not partaking in the
        relevant Designated Intermediate System election process, then the value
        returned is the zero length OCTET STRING."
    REFERENCE
        "ISIS.aoi l2DesignatedIntermediateSystem (75)"
    ::= { juniIsisCircEntry 29 }

juniIsisCircLANL2DesISChanges OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of times the LAN Level 2 Designated Intermediate System has
        changed."
    REFERENCE
        "ISIS.aoi lanL2DesignatedIntermediateSystemChanges (76)"
    ::= { juniIsisCircEntry 30 }

juniIsisCircMCAddr OBJECT-TYPE
    SYNTAX      INTEGER {
                    group(1),
                    functional(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Specifies which type of multicast address will be used for sending
        HELLO PDUs on this circuit."
    DEFVAL    { group }
    ::= { juniIsisCircEntry 31 }

juniIsisCircPtToPtCircID OBJECT-TYPE
    SYNTAX      CircuitID
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The ID of the circuit allocated during initialization.  If no value has
        been negotiated (either because the adjacency is to an End System, or
        because initialization has not yet successfully completed), this object
        has the value which would be proposed for this circuit (i.e. the
        concatenation of the local system ID and the one octet local Circuit ID
        for this circuit."
    REFERENCE
        "ISIS.aoi ptPtCircuitID (51)"
    ::= { juniIsisCircEntry 32 }

juniIsisCircL1HelloTimer OBJECT-TYPE
    SYNTAX      Integer32 (1..65535)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Maximum period, in seconds, between Level 1 IIH PDUs on multiaccess
        networks.  It is also used as the period between Hellos on point to
        point circuits.  This object follows the resettingTimer behaviour."
    REFERENCE
        "ISIS.aoi iSISHelloTimer (45)"
    DEFVAL    { 10 }
    ::= { juniIsisCircEntry 33 }

juniIsisCircL2HelloTimer OBJECT-TYPE
    SYNTAX      Integer32 (1..65535)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Maximum period, in seconds, between Level 1 IIH PDUs on multiaccess
        networks.  This object follows the resettingTimer behaviour."
    REFERENCE
        "ISIS.aoi iSISHelloTimer (45)"
    DEFVAL    { 10 }
    ::= { juniIsisCircEntry 34 }

juniIsisCircL1HelloMultiplier OBJECT-TYPE
    SYNTAX      Integer32 (3..1000)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This value is multiplied by the corresponding HelloTimer and the result
        in seconds (rounded up) is used as the holding time in transmitted
        hellos, to be used by receivers of hello packets from this IS."
    REFERENCE
        "ISIS.aoi iSISHelloTimer (45)"
    DEFVAL    { 3 }
    ::= { juniIsisCircEntry 35 }

juniIsisCircL2HelloMultiplier OBJECT-TYPE
    SYNTAX      Integer32 (3..1000)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "This value is multiplied by the corresponding HelloTimer and the result
        in seconds (rounded up) is used as the holding time in transmitted
        hellos, to be used by receivers of hello packets from this IS"
    REFERENCE
        "ISIS.aoi iSISHelloTimer (45)"
    DEFVAL    { 3 }
    ::= { juniIsisCircEntry 36 }

juniIsisCircMinLSPTransInt OBJECT-TYPE
    SYNTAX      Unsigned32
    UNITS       "milliseconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Minimum interval, in milliseconds, between transmission of LSPs on a
        circuit.  This object follows the resettingTimer behaviour.  This timer
        shall be capable of a resolution not coarser than 10 milliseconds."
    REFERENCE
        "ISIS.aoi minimumBroadcastLSPTransmissionInterval (7)"
    DEFVAL    { 33 }
    ::= { juniIsisCircEntry 37 }

juniIsisCircMinLSPReTransInt OBJECT-TYPE
    SYNTAX      Integer32 (1..65535)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Minimum interval, in seconds, between re-transmission of an Level 1 or
        2 LSP.  This object follows the resettingTimer behaviour."
    REFERENCE
        "ISIS.aoi minimumLSPTransmissionInterval (5)"
    DEFVAL    { 5 }
    ::= { juniIsisCircEntry 38 }

juniIsisCircL1CSNPInterval OBJECT-TYPE
    SYNTAX      Integer32 (1..65535)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Interval of time, in seconds, between transmission of Level 1 CSNPs on
        multiaccess networks if this router is the designated router.  On
        point-to-point networks the default is to not transmit CSNPs. Hence CSNP 
        interval will be 0 for point-to-point networks."
    DEFVAL    { 10 }
    ::= { juniIsisCircEntry 39 }

juniIsisCircL2CSNPInterval OBJECT-TYPE
    SYNTAX      Integer32 (1..65535)
    UNITS       "seconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Interval of time, in seconds, between transmission of Level 2 CSNPs on
        multiaccess networks if this router is the designated router. On
        point-to-point networks the default is to not transmit CSNPs. Hence CSNP 
        interval will be 0 for point-to-point networks."
    DEFVAL    { 10 }
    ::= { juniIsisCircEntry 40 }

juniIsisCircLSPThrottle OBJECT-TYPE
    SYNTAX      Integer32 (0..65535)
    UNITS       "milliseconds"
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Minimal interval of time, in milliseconds, between retransmissions of
        LSPs on a point to point interface."
    DEFVAL    { 33 }
    ::= { juniIsisCircEntry 41 }

juniIsisCircMeshGroupEnabled OBJECT-TYPE
    SYNTAX      INTEGER {
                    inactive(1),
                    blocked(2),
                    set(3) }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Is this port a member of a mesh group, or blocked?  Circuits in the
        same mesh group act as a virtual multiaccess network.  LSPs seen on one
        circuit in a mesh group will not be flooded to another circuit in the
        same mesh group."
    DEFVAL    { inactive }
    ::= { juniIsisCircEntry 42 }

juniIsisCircMeshGroup OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Circuits in the same mesh group act as a virtual multiaccess network.
        LSPs seen on one circuit in a mesh group will not be flooded to another
        circuit in the same mesh group.  If juniIsisCircMeshGroupEnabled is
        false, this value is ignored. Default value returned as 0 has no significance
        for this variable."
    ::= { juniIsisCircEntry 43 }

juniIsisCircLevel OBJECT-TYPE
    SYNTAX      INTEGER {
                    level1IS(0),
                    level1l2IS(1),
                    level2Only(2) }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The type of this circuit.  This object follows the
        replaceOnlyWhileDisabled behavior."
    REFERENCE
        "ISIS.aoi iSType(2)"
    ::= { juniIsisCircEntry 44 }

juniIsisCircState OBJECT-TYPE
    SYNTAX      INTEGER {
                   isisCircuitDown(1),
                   isisCircuitUp(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The operational state of the circuit."
    ::= { juniIsisCircEntry 45 }


juniIsisCircBFDTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIsisCircBFDEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The Juniper ISIS circuit table describes the BFD-specific
        characteristics of interfaces."
    ::= { juniIsisCircuitGroup 4 }

juniIsisCircBFDEntry OBJECT-TYPE
    SYNTAX      JuniIsisCircBFDEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The Juniper ISIS circuit table describes the BFD-specific
        characteristics of one interface."
    AUGMENTS  { juniIsisCircEntry }
    ::= { juniIsisCircBFDTable 1 }

JuniIsisCircBFDEntry ::= SEQUENCE {
    juniIsisCircBfdEnable	TruthValue,
    juniIsisCircBfdMinRxInterval	Integer32,
    juniIsisCircBfdMinTxInterval	Integer32,
    juniIsisCircBfdMultiplier	Integer32
}

juniIsisCircBfdEnable OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This variable indicates whether BFD session on the interface is active or not"
    DEFVAL    { false }
    ::= { juniIsisCircBFDEntry 1 }
    
juniIsisCircBfdMinRxInterval OBJECT-TYPE
    SYNTAX      Integer32 (100..65535)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This variable specifies upper-limit on rate local-system requires remote-system to
         transmit bfd control-packets [milliseconds]"
    DEFVAL    { 300 }
    ::= { juniIsisCircBFDEntry 2 }

juniIsisCircBfdMinTxInterval OBJECT-TYPE
    SYNTAX      Integer32 (100..65535)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This variable specifies lower-limit on rate local-system requires remote-system to 
         transmit bfd control-packets [milliseconds]"
    DEFVAL    { 300 }                 
    ::= { juniIsisCircBFDEntry 3 }

juniIsisCircBfdMultiplier OBJECT-TYPE
    SYNTAX      Integer32 (1..255)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This variable specifies detection-multiplier "
    DEFVAL    { 3 }                         
    ::= { juniIsisCircBFDEntry 4 }    
--
-- The System Host Name Table
--
-- The System Host Name Table contains a manually configured set of host to
-- system ID aliases supported by each instance of the Integrated ISIS protocol.
--
juniIsisSysHostNameTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIsisSysHostNameEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains the manually configured set of host name to system
        ID aliases supported by each instance of the Integrated ISIS protocol."
    ::= { juniIsisSystemGroup 5 }

juniIsisSysHostNameEntry OBJECT-TYPE
    SYNTAX      JuniIsisSysHostNameEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry contains one name to system ID alias supported by an
        instance of the Integrated ISIS protocol."
    INDEX     { juniIsisSysHostNameSysInstance,
                juniIsisSysHostNameSysId }
    ::= { juniIsisSysHostNameTable 1 }

JuniIsisSysHostNameEntry ::= SEQUENCE {
    juniIsisSysHostNameSysInstance   Integer32,
    juniIsisSysHostNameSysId         SystemID,
    juniIsisSysHostNameAreaAddr      OSINSAddress,
    juniIsisSysHostNameName          OCTET STRING,
    juniIsisSysHostNameType          INTEGER,
    juniIsisSysHostNameRowStatus     RowStatus }

juniIsisSysHostNameSysInstance OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The unique identifier of the Integrated IS-IS instance to which this
        row corresponds.  This object follows the index behaviour."
    ::= { juniIsisSysHostNameEntry 1 }

juniIsisSysHostNameSysId OBJECT-TYPE
    SYNTAX      SystemID
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ID for the system which this name will be assigned."
    ::= { juniIsisSysHostNameEntry 2 }

juniIsisSysHostNameAreaAddr OBJECT-TYPE
    SYNTAX      OSINSAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "A configured area address for the system which this name will be
        assigned.  This object follows the index behaviour.

        Note: an index for the entry {1, {49.0001} active} in this table would
        be the ordered pair (1, (0x03 0x49 0x00 0x01)), as the length of an
        Octet string is part of the OID."
    ::= { juniIsisSysHostNameEntry 3 }

juniIsisSysHostNameName OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(0..32))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "A string to use when displaying system data with this system ID."
    ::= { juniIsisSysHostNameEntry 4 }

juniIsisSysHostNameType OBJECT-TYPE
    SYNTAX      INTEGER {
                    hostNameTypeStatic(1),
                    hostNameTypeDynamic(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The type of host name entry."
    ::= { juniIsisSysHostNameEntry 5 }

juniIsisSysHostNameRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The status of this host name entry.  This object follows the RowStatus
        behaviour."
    ::= { juniIsisSysHostNameEntry 6 }


--
-- The Area Authentication Table
--
-- The Area Authentication Table contains the manually configured set of
-- authentication keys used to authenticate Level 1 LSPs and SNPs in each
-- instance of the Integrated ISIS protocol.
--
juniIsisSysAreaAuthenticationTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIsisSysAreaAuthenticationEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains the manually configured set of area authentication
        keys supported by each instance of the Integrated ISIS protocol."
    ::= { juniIsisSystemGroup 6 }

juniIsisSysAreaAuthenticationEntry OBJECT-TYPE
    SYNTAX      JuniIsisSysAreaAuthenticationEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry contains one area authentication key supported by an
        instance of the Integrated ISIS protocol."
    INDEX     { juniIsisSysAreaAuthenticationSysInstance,
                juniIsisSysAreaAuthenticationKeyId }
    ::= { juniIsisSysAreaAuthenticationTable 1 }

JuniIsisSysAreaAuthenticationEntry ::= SEQUENCE {
    juniIsisSysAreaAuthenticationSysInstance         Integer32,
    juniIsisSysAreaAuthenticationKeyId               Integer32,
    juniIsisSysAreaAuthenticationPwd                 OCTET STRING,
    juniIsisSysAreaAuthenticationKeyType             INTEGER,
    juniIsisSysAreaAuthenticationStartAcceptTime     AuthTime,
    juniIsisSysAreaAuthenticationStartGenerateTime   AuthTime,
    juniIsisSysAreaAuthenticationStopAcceptTime      AuthTime,
    juniIsisSysAreaAuthenticationStopGenerateTime    AuthTime,
    juniIsisSysAreaAuthenticationRowStatus           RowStatus }

juniIsisSysAreaAuthenticationSysInstance OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The unique identifier of the Integrated IS-IS instance to which this
        row corresponds.  This object follows the index behaviour."
    ::= { juniIsisSysAreaAuthenticationEntry 1 }

juniIsisSysAreaAuthenticationKeyId OBJECT-TYPE
    SYNTAX      Integer32 (0..255)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The unique identifier of the instance to which this row corresponds.
        This object follows the index behaviour."
    ::= { juniIsisSysAreaAuthenticationEntry 2 }

juniIsisSysAreaAuthenticationPwd OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..20))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value to be used as the Authentication Key in Level 1 Link State
        Packets whenever the value of juniIsisSysAreaAuthenticationKeyType has a
        value of plaintext or hmacMd5.  A modification of
        juniIsisSysAreaAuthenticationKeyType does not modify the
        juniIsisSysAreaAuthenticationPwd value.

        Reading this object always results in an OCTET STRING of length zero;
        authentication may not be bypassed by reading the MIB object."
    DEFVAL    { "" }
    ::= { juniIsisSysAreaAuthenticationEntry 3 }

juniIsisSysAreaAuthenticationKeyType OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    plaintext(1),
                    hmacMd5(2) }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "What authentication scheme, if any, is used to protect Level 1 Link
        State packets and sequence number packets"
    DEFVAL    { hmacMd5 }
    ::= { juniIsisSysAreaAuthenticationEntry 4 }

juniIsisSysAreaAuthenticationStartAcceptTime OBJECT-TYPE
    SYNTAX      AuthTime
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The date and time when this authentication key will start to be used to
        validate level 1 LSPs and SNPs received.  The Default value the start
        accept time will be the current time when the key was created"
    ::= { juniIsisSysAreaAuthenticationEntry 5 }

juniIsisSysAreaAuthenticationStartGenerateTime OBJECT-TYPE
    SYNTAX      AuthTime
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The date and time when this authentication key will start to be used to
        authenticate level 1 LSPs and SNPs transmitted.  The Default value the
        start accept time will be the current time when the key was created + 2
        minutes"
    ::= { juniIsisSysAreaAuthenticationEntry 6 }

juniIsisSysAreaAuthenticationStopAcceptTime OBJECT-TYPE
    SYNTAX      AuthTime
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The date and time when this authentication key will stop being accepted
        as a valid level 1 LSP and SNP key received.  A value of zero indicates
        the key will never stop being used to authenticate packets."
    DEFVAL    { 0 }
    ::= { juniIsisSysAreaAuthenticationEntry 7 }

juniIsisSysAreaAuthenticationStopGenerateTime OBJECT-TYPE
    SYNTAX      AuthTime
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The date and time when this authentication key will stop being used to
        authenticate level 1 LSPs and SNPs transmitted.  A value of zero
        indicates the key will never stop being used to authenticate packets."
    DEFVAL    { 0 }
    ::= { juniIsisSysAreaAuthenticationEntry 8 }

juniIsisSysAreaAuthenticationRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The existence state of this authentication key.  This object follows
        the RowStatus behaviour."
    ::= { juniIsisSysAreaAuthenticationEntry 9 }

-- The Domain Authentication Table

-- The Domain Authentication Table contains the manually configured set of
-- authentication keys used to authenticate Level 2 LSPs and SNPs in each
-- instance of the Integrated ISIS protocol.
--
juniIsisSysDomainAuthenticationTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIsisSysDomainAuthenticationEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains the manually configured set of domain
        authentication keys supported by each instance of the Integrated ISIS
        protocol."
    ::= { juniIsisSystemGroup 7 }

juniIsisSysDomainAuthenticationEntry OBJECT-TYPE
    SYNTAX      JuniIsisSysDomainAuthenticationEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry contains one domain authentication key supported by an
        instance of the Integrated ISIS protocol."
    INDEX     { juniIsisSysDomainAuthenticationSysInstance,
                juniIsisSysDomainAuthenticationKeyId }
    ::= { juniIsisSysDomainAuthenticationTable 1 }

JuniIsisSysDomainAuthenticationEntry ::= SEQUENCE {
    juniIsisSysDomainAuthenticationSysInstance       Integer32,
    juniIsisSysDomainAuthenticationKeyId             Integer32,
    juniIsisSysDomainAuthenticationPwd               OCTET STRING,
    juniIsisSysDomainAuthenticationKeyType           INTEGER,
    juniIsisSysDomainAuthenticationStartAcceptTime   AuthTime,
    juniIsisSysDomainAuthenticationStartGenerateTime AuthTime,
    juniIsisSysDomainAuthenticationStopAcceptTime    AuthTime,
    juniIsisSysDomainAuthenticationStopGenerateTime  AuthTime,
    juniIsisSysDomainAuthenticationRowStatus         RowStatus }

juniIsisSysDomainAuthenticationSysInstance OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The unique identifier of the Integrated IS-IS instance to which this
        row corresponds.  This object follows the index behaviour."
    ::= { juniIsisSysDomainAuthenticationEntry 1 }

juniIsisSysDomainAuthenticationKeyId OBJECT-TYPE
    SYNTAX      Integer32 (0..255)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The unique identifier of the instance to which this row corresponds.
        This object follows the index behaviour."
    ::= { juniIsisSysDomainAuthenticationEntry 2 }

juniIsisSysDomainAuthenticationPwd OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE (0..20))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value to be used as the Authentication Key in Level 2 Link State
        Packets whenever the value of juniIsisSysDomainAuthenticationKeyType has
        a value of plaintext or hmacMd5.  A modification of
        juniIsisSysDomainAuthenticationKeyType does not modify the
        juniIsisSysDomainAuthenticationPwd value.

        Reading this object always results in an OCTET STRING of length zero;
        authentication may not be bypassed by reading the MIB object."
    DEFVAL    { "" }
    ::= { juniIsisSysDomainAuthenticationEntry 3 }

juniIsisSysDomainAuthenticationKeyType OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    plaintext(1),
                    hmacMd5(2) }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "What authentication scheme, if any, is used to protect Level 2 Link
        State packets and Sequence Number packets"
    DEFVAL    { hmacMd5 }
    ::= { juniIsisSysDomainAuthenticationEntry 4 }

juniIsisSysDomainAuthenticationStartAcceptTime OBJECT-TYPE
    SYNTAX      AuthTime
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The date and time when this authentication key will start to be used to
        validate level 2 LSPs and SNPs received.  The Default value the start
        accept time will be the current time when the key was created"
    ::= { juniIsisSysDomainAuthenticationEntry 5 }

juniIsisSysDomainAuthenticationStartGenerateTime OBJECT-TYPE
    SYNTAX      AuthTime
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The date and time when this authentication key will start to be used to
        authenticate level 2 LSPs and SNPs transmitted.  The Default value the
        start accept time will be the current time when the key was created + 2
        minutes"
    ::= { juniIsisSysDomainAuthenticationEntry 6 }

juniIsisSysDomainAuthenticationStopAcceptTime OBJECT-TYPE
    SYNTAX      AuthTime
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The date and time when this authentication key will stop being accepted
        as a valid level 2 LSP and SNP key received.  A value of zero indicates
        the key will never stop being used to authenticate packets."
    DEFVAL    { 0 }
    ::= { juniIsisSysDomainAuthenticationEntry 7 }

juniIsisSysDomainAuthenticationStopGenerateTime OBJECT-TYPE
    SYNTAX      AuthTime
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The date and time when this authentication key will stop being used to
        authenticate level 2 LSPs and SNPs transmitted.  A value of zero
        indicates the key will never stop being used to authenticate packets."
    DEFVAL    { 0 }
    ::= { juniIsisSysDomainAuthenticationEntry 8 }

juniIsisSysDomainAuthenticationRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The existence state of this authentication key.  This object follows
        the RowStatus behaviour."
    ::= { juniIsisSysDomainAuthenticationEntry 9 }


--
-- The Level 1 Circuit Authentication Table
--
-- The Level 1 Circuit Authentication Table contains the manually configured
-- set of authentication keys used to authenticate Level 1 hello packets in each
-- instance of the Integrated ISIS protocol.
--
juniIsisSysL1CircAuthenticationTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIsisSysL1CircAuthenticationEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains the manually configured set of Level 1 Circuit
        authentication keys supported by each instance of the Integrated ISIS
        protocol."
    ::= { juniIsisCircuitGroup 2 }

juniIsisSysL1CircAuthenticationEntry OBJECT-TYPE
    SYNTAX      JuniIsisSysL1CircAuthenticationEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry contains one Level 1 circuit authentication key supported by
        an instance of the Integrated ISIS protocol."
    INDEX     { juniIsisSysL1CircAuthenticationSysInstance,
                juniIsisSysL1CircAuthenticationIfIndex,
                juniIsisSysL1CircAuthenticationKeyId }
    ::= { juniIsisSysL1CircAuthenticationTable 1 }

JuniIsisSysL1CircAuthenticationEntry ::= SEQUENCE {
    juniIsisSysL1CircAuthenticationSysInstance       Integer32,
    juniIsisSysL1CircAuthenticationIfIndex           Integer32,
    juniIsisSysL1CircAuthenticationKeyId             Integer32,
    juniIsisSysL1CircAuthenticationPwd               OCTET STRING,
    juniIsisSysL1CircAuthenticationKeyType           INTEGER,
    juniIsisSysL1CircAuthenticationStartAcceptTime   AuthTime,
    juniIsisSysL1CircAuthenticationStartGenerateTime AuthTime,
    juniIsisSysL1CircAuthenticationStopAcceptTime    AuthTime,
    juniIsisSysL1CircAuthenticationStopGenerateTime  AuthTime,
    juniIsisSysL1CircAuthenticationRowStatus         RowStatus }

juniIsisSysL1CircAuthenticationSysInstance OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The unique identifier of the Integrated IS-IS instance to which this
        row corresponds.  This object follows the index behaviour."
    ::= { juniIsisSysL1CircAuthenticationEntry 1 }

juniIsisSysL1CircAuthenticationIfIndex OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of ifIndex for the interface to which this circuit
        corresponds."
    ::= { juniIsisSysL1CircAuthenticationEntry 2 }

juniIsisSysL1CircAuthenticationKeyId OBJECT-TYPE
    SYNTAX      Integer32 (0..255)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The unique identifier of the instance to which this row corresponds.
        This object follows the index behaviour."
    ::= { juniIsisSysL1CircAuthenticationEntry 3 }

juniIsisSysL1CircAuthenticationPwd OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(0..20))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value to be used as the Authentication Key in Level 1 Hello Packets
        whenever the value of juniIsisSysL1CircAuthenticationKeyType has a value
        of hmacMd5.  A modification of juniIsisSysL1CircAuthenticationKeyType
        does not modify the juniIsisSysL1CircAuthenticationPwd value.

        Reading this object always results in an OCTET STRING of length zero;
        authentication may not be bypassed by reading the MIB object."
    DEFVAL    { "" }
    ::= { juniIsisSysL1CircAuthenticationEntry 4 }

juniIsisSysL1CircAuthenticationKeyType OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    plaintext(1),
                    hmacMd5(2) }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "What authentication scheme, if any, is used to protect Level 1 hello
        packets."
    DEFVAL    { hmacMd5 }
    ::= { juniIsisSysL1CircAuthenticationEntry 5 }

juniIsisSysL1CircAuthenticationStartAcceptTime OBJECT-TYPE
    SYNTAX      AuthTime
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The date and time when this authentication key will start to be used to
        validate level 1 IIH packets received.  The Default value the start
        accept time will be the current time when the key was created."
    ::= { juniIsisSysL1CircAuthenticationEntry 6 }

juniIsisSysL1CircAuthenticationStartGenerateTime OBJECT-TYPE
    SYNTAX      AuthTime
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The date and time when this authentication key will start to be used to
        authenticate level 1 IIH packets transmitted.  The Default value the
        start accept time will be the current time when the key was created + 2
        minutes."
    ::= { juniIsisSysL1CircAuthenticationEntry 7 }

juniIsisSysL1CircAuthenticationStopAcceptTime OBJECT-TYPE
    SYNTAX      AuthTime
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The date and time when this authentication key will stop being accepted
        as a valid level 1 IIH packets key received.  A value of zero indicates
        the key will never stop being used to authenticate packets."
    DEFVAL    { 0 }
    ::= { juniIsisSysL1CircAuthenticationEntry 8 }

juniIsisSysL1CircAuthenticationStopGenerateTime OBJECT-TYPE
    SYNTAX      AuthTime
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The date and time when this authentication key will stop being used to
        authenticate level 1 IIH packets transmitted.  A value of zero indicates
        the key will never stop being used to authenticate packets."
    DEFVAL    { 0 }
    ::= { juniIsisSysL1CircAuthenticationEntry 9 }

juniIsisSysL1CircAuthenticationRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The existence state of this authentication key.  This object follows
        the RowStatus behaviour."
    ::= { juniIsisSysL1CircAuthenticationEntry 10 }


--
-- The Level 2 Circuit Authentication Table
--
-- The Level 2 Circuit Authentication Table contains the manually configured set
-- of authentication keys used to authenticate Level 2 hello packets in each
-- instance of the Integrated ISIS protocol.
--
juniIsisSysL2CircAuthenticationTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIsisSysL2CircAuthenticationEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains the manually configured set of Level 2 Circuit
        authentication keys supported by each instance of the Integrated ISIS
        protocol."
    ::= { juniIsisCircuitGroup 3 }

juniIsisSysL2CircAuthenticationEntry OBJECT-TYPE
    SYNTAX      JuniIsisSysL2CircAuthenticationEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry contains one Level 2 circuit authentication key supported by
        an instance of the Integrated ISIS protocol."
    INDEX     { juniIsisSysL2CircAuthenticationSysInstance,
                juniIsisSysL2CircAuthenticationIfIndex,
                juniIsisSysL2CircAuthenticationKeyId }
    ::= { juniIsisSysL2CircAuthenticationTable 1 }

JuniIsisSysL2CircAuthenticationEntry ::= SEQUENCE {
    juniIsisSysL2CircAuthenticationSysInstance       Integer32,
    juniIsisSysL2CircAuthenticationIfIndex           Integer32,
    juniIsisSysL2CircAuthenticationKeyId             Integer32,
    juniIsisSysL2CircAuthenticationPwd               OCTET STRING,
    juniIsisSysL2CircAuthenticationKeyType           INTEGER,
    juniIsisSysL2CircAuthenticationStartAcceptTime   AuthTime,
    juniIsisSysL2CircAuthenticationStartGenerateTime AuthTime,
    juniIsisSysL2CircAuthenticationStopAcceptTime    AuthTime,
    juniIsisSysL2CircAuthenticationStopGenerateTime  AuthTime,
    juniIsisSysL2CircAuthenticationRowStatus         RowStatus }

juniIsisSysL2CircAuthenticationSysInstance OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The unique identifier of the Integrated IS-IS instance to which this
        row corresponds.  This object follows the index behaviour."
    ::= { juniIsisSysL2CircAuthenticationEntry 1 }

juniIsisSysL2CircAuthenticationIfIndex OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of ifIndex for the interface to which this circuit
        corresponds."
    ::= { juniIsisSysL2CircAuthenticationEntry 2 }

juniIsisSysL2CircAuthenticationKeyId OBJECT-TYPE
    SYNTAX      Integer32 (0..255)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The unique identifier of the instance to which this row corresponds.
        This object follows the index behaviour."
    ::= { juniIsisSysL2CircAuthenticationEntry 3 }
juniIsisSysL2CircAuthenticationPwd OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(0..20))
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value to be used as the Authentication Key in Level 2 Hello Packets
        whenever the value of juniIsisSysL2CircAuthenticationKeyType has a value
        of hmacMd5.  A modification of juniIsisSysL2CircAuthenticationKeyType
        does not modify the juniIsisSysL2CircAuthenticationPwd value.

        Reading this object always results in an OCTET STRING of length zero;
        authentication may not be bypassed by reading the MIB object."
    DEFVAL    { "" }
    ::= { juniIsisSysL2CircAuthenticationEntry 4 }

juniIsisSysL2CircAuthenticationKeyType OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    plaintext(1),
                    hmacMd5(2) }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "What authentication scheme, if any, is used to protect Level 2 hello
        packets."
    DEFVAL    { hmacMd5 }
    ::= { juniIsisSysL2CircAuthenticationEntry 5 }

juniIsisSysL2CircAuthenticationStartAcceptTime OBJECT-TYPE
    SYNTAX      AuthTime
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The date and time when this authentication key will start to be used to
        validate level 2 IIH packets received.  The Default value the start
        accept time will be the current time when the key was created."
    ::= { juniIsisSysL2CircAuthenticationEntry 6 }

juniIsisSysL2CircAuthenticationStartGenerateTime OBJECT-TYPE
    SYNTAX      AuthTime
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The date and time when this authentication key will start to be used to
        authenticate level 2 IIH packets transmitted.  The Default value the
        start accept time will be the current time when the key was created + 2
        minutes."
    ::= { juniIsisSysL2CircAuthenticationEntry 7 }

juniIsisSysL2CircAuthenticationStopAcceptTime OBJECT-TYPE
    SYNTAX      AuthTime
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The date and time when this authentication key will stop being accepted
        as a valid level 2 IIH packets key received.  A value of zero indicates
        the key will never stop being used to authenticate packets."
    DEFVAL    { 0 }
    ::= { juniIsisSysL2CircAuthenticationEntry 8 }

juniIsisSysL2CircAuthenticationStopGenerateTime OBJECT-TYPE
    SYNTAX      AuthTime
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The date and time when this authentication key will stop being used to
        authenticate level 2 IIH packets transmitted.  A value of zero indicates
        the key will never stop being used to authenticate packets."
    DEFVAL    { 0 }
    ::= { juniIsisSysL2CircAuthenticationEntry 9 }

juniIsisSysL2CircAuthenticationRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The existence state of this authentication key.  This object follows
        the RowStatus behaviour."
    DEFVAL    { active }
    ::= { juniIsisSysL2CircAuthenticationEntry 10 }    

-- 
-- The MPLS TE tunnel table contains the set of tunnels exported by MPLS into
-- ISIS. 

juniIsisMplsTeTunnelTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIsisMplsTeTunnelEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The set of tunnels imported from MPLS."
    REFERENCE
        "ISIS.aoi mplsTeTunnels(6)"
    ::= { juniIsisSystemGroup 8 }

juniIsisMplsTeTunnelEntry OBJECT-TYPE
    SYNTAX      JuniIsisMplsTeTunnelEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry contains metric details of an MPLS LSP"
    INDEX     { juniIsisMplsTeTunnelSysInstance,
                juniIsisMplsNextHopIndex }
    ::= { juniIsisMplsTeTunnelTable 1 }

JuniIsisMplsTeTunnelEntry ::= SEQUENCE {
    juniIsisMplsTeTunnelSysInstance       Integer32,
    juniIsisMplsNextHopIndex             Integer32,
    juniIsisMplsTeSystemId               SystemID,
    juniIsisMplsTeRouterId               IpAddress,
    juniIsisMplsTeTunnelMetric           Integer32,
    juniIsisMplsTeTunnelRelMetric        Integer32,
    juniIsisMplsTeTunnelName             OCTET STRING
 }
 

juniIsisMplsTeTunnelSysInstance OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The unique identifier of the Integrated IS-IS instance to which this
        row corresponds.  This object follows the index behaviour."
    ::= { juniIsisMplsTeTunnelEntry 1 }

juniIsisMplsNextHopIndex OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "An index to uniquely identify the tunnels."
    ::= { juniIsisMplsTeTunnelEntry 2 }

juniIsisMplsTeSystemId OBJECT-TYPE
    SYNTAX      SystemID
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The ID for the instance of the Integrated IS-IS protocol 
     running in the tunnel's end point."
    ::= { juniIsisMplsTeTunnelEntry 3 }

juniIsisMplsTeRouterId OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The router ID of the tunnel's end point."
    ::= { juniIsisMplsTeTunnelEntry 4 }

juniIsisMplsTeTunnelMetric OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The metric associated with the tunnel."
    ::= { juniIsisMplsTeTunnelEntry 5 }

juniIsisMplsTeTunnelRelMetric OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The metric associated with the tunnel relative to the spf path."
    ::= { juniIsisMplsTeTunnelEntry 6 }

juniIsisMplsTeTunnelName OBJECT-TYPE
    SYNTAX      OCTET STRING ( SIZE (1..40))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The name associated with the tunnel."
    ::= { juniIsisMplsTeTunnelEntry 7 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Conformance information
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniIsisCompliances  OBJECT IDENTIFIER ::= { juniIsisConformance 1 }
juniIsisMIBGroups    OBJECT IDENTIFIER ::= { juniIsisConformance 2 }

--
-- Compliance Statements
--
juniIsisCompliance  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for systems supporting ISIS
        functionality.  This statement became obsolete when the
        juniIsisCircState object was added."
    MODULE   -- juniIsisMIB
        MANDATORY-GROUPS {
            juniIsisSystemMgmtGroup,
            juniIsisCircuitMgmtGroup }
    ::= { juniIsisCompliances 1 }                                  -- JUNOSe 2.0

juniIsisCompliance2  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for systems supporting ISIS
        functionality.  This statement became obsolete when MPSL support was
        added."
    MODULE   -- juniIsisMIB
        MANDATORY-GROUPS {
            juniIsisSystemMgmtGroup,
            juniIsisCircuitMgmtGroup2 }
    ::= { juniIsisCompliances 2 }                                  -- JUNOSe 3.0

juniIsisCompliance3  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for systems supporting ISIS functionality. This 
        statement became obsolete when juniIsisCircBFDTable is implemented."

    MODULE   -- juniIsisMIB
        MANDATORY-GROUPS {
            juniIsisSystemMgmtGroup2,
            juniIsisCircuitMgmtGroup2 }
    ::= { juniIsisCompliances 3 }                                  -- JUNOSe 4.0

juniIsisCompliance4  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for systems supporting ISIS functionality."
    MODULE   -- juniIsisMIB
        MANDATORY-GROUPS {
            juniIsisSystemMgmtGroup2,
            juniIsisCircuitMgmtGroup2,
            juniIsisCircBFDGroup }
    ::= { juniIsisCompliances 4 } 
juniIsisCompliance5  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for systems supporting ISIS functionality."
    MODULE   -- juniIsisMIB
        MANDATORY-GROUPS {
            juniIsisSystemMgmtGroup3,
            juniIsisCircuitMgmtGroup2,
            juniIsisCircBFDGroup }
    ::= { juniIsisCompliances 5 } 

juniIsisCompliance6  MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for systems supporting ISIS functionality."
    MODULE   -- juniIsisMIB
        MANDATORY-GROUPS {
            juniIsisSystemMgmtGroup4,
            juniIsisCircuitMgmtGroup2,
            juniIsisCircBFDGroup }
    ::= { juniIsisCompliances 6 } 

--
-- Units of Conformance
--
juniIsisSystemMgmtGroup  OBJECT-GROUP
    OBJECTS {
        juniIsisSysVersion,
        juniIsisSysType,
        juniIsisSysID,
        juniIsisSysMaxPathSplits,
        juniIsisSysMaxLSPGenInt,
        juniIsisSysOrigLSPBuffSize,
        juniIsisSysMaxAreaAddresses,
        juniIsisSysMinL1LSPGenInt,
        juniIsisSysMinL2LSPGenInt,
        juniIsisSysPollESHelloRate,
        juniIsisSysWaitTime,
        juniIsisSysOperState,
        juniIsisSysL1State,
        juniIsisSysCorrLSPs,
        juniIsisSysLSPL1DbaseOloads,
        juniIsisSysManAddrDropFromAreas,
        juniIsisSysAttmptToExMaxSeqNums,
        juniIsisSysSeqNumSkips,
        juniIsisSysOwnLSPPurges,
        juniIsisSysIDFieldLenMismatches,
        juniIsisSysMaxAreaAddrMismatches,
        juniIsisSysL2State,
        juniIsisSysLSPL2DbaseOloads,
        juniIsisSysAuthFails,
        juniIsisSysLSPIgnoreErrors,
        juniIsisSysMaxAreaCheck,
        juniIsisSysSetOverloadBit,
        juniIsisSysSetOverloadBitStartupDuration,
        juniIsisSysMaxLspLifetime ,
        juniIsisSysL1SpfInterval,
        juniIsisSysL2SpfInterval,
        juniIsisSysIshHoldTime,
        juniIsisSysIshConfigTimer,
        juniIsisSysDistributeDomainWide,
        juniIsisSysDistance,
        juniIsisSysL1MetricStyle,
        juniIsisSysL2MetricStyle,
        juniIsisSysIsoRouteTag,
        juniIsisManAreaAddrRowStatus,
        juniIsisSysProtSuppRowStatus,
        juniIsisSummAddrRowStatus,
        juniIsisSummAddrOperState,
        juniIsisSummAddrDefaultMetric,
        juniIsisSummAddrDelayMetric,
        juniIsisSummAddrExpenseMetric,
        juniIsisSummAddrErrorMetric,
        juniIsisSummLevel,
        juniIsisSysHostNameAreaAddr,
        juniIsisSysHostNameName,
        juniIsisSysHostNameType,
        juniIsisSysHostNameRowStatus,
        juniIsisSysAreaAuthenticationPwd,
        juniIsisSysAreaAuthenticationKeyType,
        juniIsisSysAreaAuthenticationStartAcceptTime,
        juniIsisSysAreaAuthenticationStartGenerateTime,
        juniIsisSysAreaAuthenticationStopAcceptTime,
        juniIsisSysAreaAuthenticationStopGenerateTime,
        juniIsisSysAreaAuthenticationRowStatus,
        juniIsisSysDomainAuthenticationPwd,
        juniIsisSysDomainAuthenticationKeyType,
        juniIsisSysDomainAuthenticationStartAcceptTime,
        juniIsisSysDomainAuthenticationStartGenerateTime,
        juniIsisSysDomainAuthenticationStopAcceptTime,
        juniIsisSysDomainAuthenticationStopGenerateTime,
        juniIsisSysDomainAuthenticationRowStatus }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete system level objects for ISIS management functionality.  This
        group became obsolete when the MPLS management objects were added."
    ::= { juniIsisMIBGroups 1 }

juniIsisCircuitMgmtGroup  OBJECT-GROUP
    OBJECTS {
        juniIsisCircLocalID,
        juniIsisCircOperState,
        juniIsisCircRowStatus,
        juniIsisCircType,
        juniIsisCircL1DefaultMetric,
        juniIsisCircL1DelayMetric,
        juniIsisCircL1ExpenseMetric,
        juniIsisCircL1ErrorMetric,
        juniIsisCircExtDomain,
        juniIsisCircAdjChanges,
        juniIsisCircInitFails,
        juniIsisCircRejAdjs,
        juniIsisCircOutCtrlPDUs,
        juniIsisCircInCtrlPDUs,
        juniIsisCircIDFieldLenMismatches,
        juniIsisCircL2DefaultMetric,
        juniIsisCircL2DelayMetric,
        juniIsisCircL2ExpenseMetric,
        juniIsisCircL2ErrorMetric,
        juniIsisCircManL2Only,
        juniIsisCircL1ISPriority,
        juniIsisCircL1CircID,
        juniIsisCircL1DesIS,
        juniIsisCircLANL1DesISChanges,
        juniIsisCircL2ISPriority,
        juniIsisCircL2CircID,
        juniIsisCircL2DesIS,
        juniIsisCircLANL2DesISChanges,
        juniIsisCircMCAddr,
        juniIsisCircPtToPtCircID,
        juniIsisCircL1HelloTimer,
        juniIsisCircL2HelloTimer,
        juniIsisCircL1HelloMultiplier,
        juniIsisCircL2HelloMultiplier,
        juniIsisCircMinLSPTransInt,
        juniIsisCircMinLSPReTransInt,
        juniIsisCircL1CSNPInterval,
        juniIsisCircL2CSNPInterval,
        juniIsisCircLSPThrottle,
        juniIsisCircMeshGroupEnabled,
        juniIsisCircMeshGroup,
        juniIsisCircLevel,
        juniIsisSysL1CircAuthenticationPwd,
        juniIsisSysL1CircAuthenticationKeyType,
        juniIsisSysL1CircAuthenticationStartAcceptTime,
        juniIsisSysL1CircAuthenticationStartGenerateTime,
        juniIsisSysL1CircAuthenticationStopAcceptTime,
        juniIsisSysL1CircAuthenticationStopGenerateTime,
        juniIsisSysL1CircAuthenticationRowStatus,
        juniIsisSysL2CircAuthenticationPwd,
        juniIsisSysL2CircAuthenticationKeyType,
        juniIsisSysL2CircAuthenticationStartAcceptTime,
        juniIsisSysL2CircAuthenticationStartGenerateTime,
        juniIsisSysL2CircAuthenticationStopAcceptTime,
        juniIsisSysL2CircAuthenticationStopGenerateTime,
        juniIsisSysL2CircAuthenticationRowStatus }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete circuit management objects.  This group became obsolete when
        the juniIsisCircState object was added."
    ::= { juniIsisMIBGroups 2 }

juniIsisCircuitMgmtGroup2  OBJECT-GROUP
    OBJECTS {
        juniIsisCircLocalID,
        juniIsisCircOperState,
        juniIsisCircRowStatus,
        juniIsisCircType,
        juniIsisCircL1DefaultMetric,
        juniIsisCircL1DelayMetric,
        juniIsisCircL1ExpenseMetric,
        juniIsisCircL1ErrorMetric,
        juniIsisCircExtDomain,
        juniIsisCircAdjChanges,
        juniIsisCircInitFails,
        juniIsisCircRejAdjs,
        juniIsisCircOutCtrlPDUs,
        juniIsisCircInCtrlPDUs,
        juniIsisCircIDFieldLenMismatches,
        juniIsisCircL2DefaultMetric,
        juniIsisCircL2DelayMetric,
        juniIsisCircL2ExpenseMetric,
        juniIsisCircL2ErrorMetric,
        juniIsisCircManL2Only,
        juniIsisCircL1ISPriority,
        juniIsisCircL1CircID,
        juniIsisCircL1DesIS,
        juniIsisCircLANL1DesISChanges,
        juniIsisCircL2ISPriority,
        juniIsisCircL2CircID,
        juniIsisCircL2DesIS,
        juniIsisCircLANL2DesISChanges,
        juniIsisCircMCAddr,
        juniIsisCircPtToPtCircID,
        juniIsisCircL1HelloTimer,
        juniIsisCircL2HelloTimer,
        juniIsisCircL1HelloMultiplier,
        juniIsisCircL2HelloMultiplier,
        juniIsisCircMinLSPTransInt,
        juniIsisCircMinLSPReTransInt,
        juniIsisCircL1CSNPInterval,
        juniIsisCircL2CSNPInterval,
        juniIsisCircLSPThrottle,
        juniIsisCircMeshGroupEnabled,
        juniIsisCircMeshGroup,
        juniIsisCircLevel,
        juniIsisCircState,
        juniIsisSysL1CircAuthenticationPwd,
        juniIsisSysL1CircAuthenticationKeyType,
        juniIsisSysL1CircAuthenticationStartAcceptTime,
        juniIsisSysL1CircAuthenticationStartGenerateTime,
        juniIsisSysL1CircAuthenticationStopAcceptTime,
        juniIsisSysL1CircAuthenticationStopGenerateTime,
        juniIsisSysL1CircAuthenticationRowStatus,
        juniIsisSysL2CircAuthenticationPwd,
        juniIsisSysL2CircAuthenticationKeyType,
        juniIsisSysL2CircAuthenticationStartAcceptTime,
        juniIsisSysL2CircAuthenticationStartGenerateTime,
        juniIsisSysL2CircAuthenticationStopAcceptTime,
        juniIsisSysL2CircAuthenticationStopGenerateTime,
        juniIsisSysL2CircAuthenticationRowStatus }
    STATUS      current
    DESCRIPTION
        "The circuit management objects."
    ::= { juniIsisMIBGroups 3 }

juniIsisSystemMgmtGroup2  OBJECT-GROUP
    OBJECTS {
        juniIsisSysVersion,
        juniIsisSysType,
        juniIsisSysID,
        juniIsisSysMaxPathSplits,
        juniIsisSysMaxLSPGenInt,
        juniIsisSysOrigLSPBuffSize,
        juniIsisSysMaxAreaAddresses,
        juniIsisSysMinL1LSPGenInt,
        juniIsisSysMinL2LSPGenInt,
        juniIsisSysPollESHelloRate,
        juniIsisSysWaitTime,
        juniIsisSysOperState,
        juniIsisSysL1State,
        juniIsisSysCorrLSPs,
        juniIsisSysLSPL1DbaseOloads,
        juniIsisSysManAddrDropFromAreas,
        juniIsisSysAttmptToExMaxSeqNums,
        juniIsisSysSeqNumSkips,
        juniIsisSysOwnLSPPurges,
        juniIsisSysIDFieldLenMismatches,
        juniIsisSysMaxAreaAddrMismatches,
        juniIsisSysOrigL2LSPBuffSize,
        juniIsisSysL2State,
        juniIsisSysLSPL2DbaseOloads,
        juniIsisSysAuthFails,
        juniIsisSysLSPIgnoreErrors,
        juniIsisSysMaxAreaCheck,
        juniIsisSysSetOverloadBit,
        juniIsisSysSetOverloadBitStartupDuration,
        juniIsisSysMaxLspLifetime ,
        juniIsisSysL1SpfInterval,
        juniIsisSysL2SpfInterval,
        juniIsisSysIshHoldTime,
        juniIsisSysIshConfigTimer,
        juniIsisSysDistributeDomainWide,
        juniIsisSysDistance,
        juniIsisSysL1MetricStyle,
        juniIsisSysL2MetricStyle,
        juniIsisSysIsoRouteTag,
        juniIsisSysMplsTeLevel,
        juniIsisSysMplsTeRtrIdIfIndex,
        juniIsisManAreaAddrRowStatus,
        juniIsisSysProtSuppRowStatus,
        juniIsisSummAddrRowStatus,
        juniIsisSummAddrOperState,
        juniIsisSummAddrDefaultMetric,
        juniIsisSummAddrDelayMetric,
        juniIsisSummAddrExpenseMetric,
        juniIsisSummAddrErrorMetric,
        juniIsisSummLevel,
        juniIsisSysHostNameAreaAddr,
        juniIsisSysHostNameName,
        juniIsisSysHostNameType,
        juniIsisSysHostNameRowStatus,
        juniIsisSysAreaAuthenticationPwd,
        juniIsisSysAreaAuthenticationKeyType,
        juniIsisSysAreaAuthenticationStartAcceptTime,
        juniIsisSysAreaAuthenticationStartGenerateTime,
        juniIsisSysAreaAuthenticationStopAcceptTime,
        juniIsisSysAreaAuthenticationStopGenerateTime,
        juniIsisSysAreaAuthenticationRowStatus,
        juniIsisSysDomainAuthenticationPwd,
        juniIsisSysDomainAuthenticationKeyType,
        juniIsisSysDomainAuthenticationStartAcceptTime,
        juniIsisSysDomainAuthenticationStartGenerateTime,
        juniIsisSysDomainAuthenticationStopAcceptTime,
        juniIsisSysDomainAuthenticationStopGenerateTime,
        juniIsisSysDomainAuthenticationRowStatus }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete system level objects for ISIS management functionality.  This
        group became obsolete when the MPLS tunnel table was added."
    ::= { juniIsisMIBGroups 4 }

juniIsisCircBFDGroup  OBJECT-GROUP
    OBJECTS {
         juniIsisCircBfdEnable,
         juniIsisCircBfdMinRxInterval,
    	 juniIsisCircBfdMinTxInterval,
    	 juniIsisCircBfdMultiplier
 }
    STATUS      current
    DESCRIPTION
        "The circuit level ISIS BFD configuration parameters."
    ::= { juniIsisMIBGroups 5 }
    
juniIsisSystemMgmtGroup3  OBJECT-GROUP
    OBJECTS {
        juniIsisSysVersion,
        juniIsisSysType,
        juniIsisSysID,
        juniIsisSysMaxPathSplits,
        juniIsisSysMaxLSPGenInt,
        juniIsisSysOrigLSPBuffSize,
        juniIsisSysMaxAreaAddresses,
        juniIsisSysMinL1LSPGenInt,
        juniIsisSysMinL2LSPGenInt,
        juniIsisSysPollESHelloRate,
        juniIsisSysWaitTime,
        juniIsisSysOperState,
        juniIsisSysL1State,
        juniIsisSysCorrLSPs,
        juniIsisSysLSPL1DbaseOloads,
        juniIsisSysManAddrDropFromAreas,
        juniIsisSysAttmptToExMaxSeqNums,
        juniIsisSysSeqNumSkips,
        juniIsisSysOwnLSPPurges,
        juniIsisSysIDFieldLenMismatches,
        juniIsisSysMaxAreaAddrMismatches,
        juniIsisSysOrigL2LSPBuffSize,
        juniIsisSysL2State,
        juniIsisSysLSPL2DbaseOloads,
        juniIsisSysAuthFails,
        juniIsisSysLSPIgnoreErrors,
        juniIsisSysMaxAreaCheck,
        juniIsisSysSetOverloadBit,
        juniIsisSysSetOverloadBitStartupDuration,
        juniIsisSysMaxLspLifetime ,
        juniIsisSysL1SpfInterval,
        juniIsisSysL2SpfInterval,
        juniIsisSysIshHoldTime,
        juniIsisSysIshConfigTimer,
        juniIsisSysDistributeDomainWide,
        juniIsisSysDistance,
        juniIsisSysL1MetricStyle,
        juniIsisSysL2MetricStyle,
        juniIsisSysIsoRouteTag,
        juniIsisSysMplsTeLevel,
        juniIsisSysMplsTeRtrIdIfIndex,
        juniIsisSysMplsTeSpfUseAnyBestPath,
        juniIsisManAreaAddrRowStatus,
        juniIsisSysProtSuppRowStatus,
        juniIsisSummAddrRowStatus,
        juniIsisSummAddrOperState,
        juniIsisSummAddrDefaultMetric,
        juniIsisSummAddrDelayMetric,
        juniIsisSummAddrExpenseMetric,
        juniIsisSummAddrErrorMetric,
        juniIsisSummLevel,
        juniIsisSysHostNameAreaAddr,
        juniIsisSysHostNameName,
        juniIsisSysHostNameType,
        juniIsisSysHostNameRowStatus,
        juniIsisSysAreaAuthenticationPwd,
        juniIsisSysAreaAuthenticationKeyType,
        juniIsisSysAreaAuthenticationStartAcceptTime,
        juniIsisSysAreaAuthenticationStartGenerateTime,
        juniIsisSysAreaAuthenticationStopAcceptTime,
        juniIsisSysAreaAuthenticationStopGenerateTime,
        juniIsisSysAreaAuthenticationRowStatus,
        juniIsisSysDomainAuthenticationPwd,
        juniIsisSysDomainAuthenticationKeyType,
        juniIsisSysDomainAuthenticationStartAcceptTime,
        juniIsisSysDomainAuthenticationStartGenerateTime,
        juniIsisSysDomainAuthenticationStopAcceptTime,
        juniIsisSysDomainAuthenticationStopGenerateTime,
        juniIsisSysDomainAuthenticationRowStatus,
        juniIsisMplsTeSystemId,
        juniIsisMplsTeRouterId,
        juniIsisMplsTeTunnelMetric,
        juniIsisMplsTeTunnelRelMetric,
        juniIsisMplsTeTunnelName }
        
    STATUS      obsolete
    DESCRIPTION
        "Obsolete system level objects for ISIS management functionality.  This
        group became obsolete when the reference bandwidth related variables were added."
    ::= { juniIsisMIBGroups 6 }

    juniIsisSystemMgmtGroup4  OBJECT-GROUP
    OBJECTS {
        juniIsisSysVersion,
        juniIsisSysType,
        juniIsisSysID,
        juniIsisSysMaxPathSplits,
        juniIsisSysMaxLSPGenInt,
        juniIsisSysOrigLSPBuffSize,
        juniIsisSysMaxAreaAddresses,
        juniIsisSysMinL1LSPGenInt,
        juniIsisSysMinL2LSPGenInt,
        juniIsisSysPollESHelloRate,
        juniIsisSysWaitTime,
        juniIsisSysOperState,
        juniIsisSysL1State,
        juniIsisSysCorrLSPs,
        juniIsisSysLSPL1DbaseOloads,
        juniIsisSysManAddrDropFromAreas,
        juniIsisSysAttmptToExMaxSeqNums,
        juniIsisSysSeqNumSkips,
        juniIsisSysOwnLSPPurges,
        juniIsisSysIDFieldLenMismatches,
        juniIsisSysMaxAreaAddrMismatches,
        juniIsisSysOrigL2LSPBuffSize,
        juniIsisSysL2State,
        juniIsisSysLSPL2DbaseOloads,
        juniIsisSysAuthFails,
        juniIsisSysLSPIgnoreErrors,
        juniIsisSysMaxAreaCheck,
        juniIsisSysSetOverloadBit,
        juniIsisSysSetOverloadBitStartupDuration,
        juniIsisSysMaxLspLifetime ,
        juniIsisSysL1SpfInterval,
        juniIsisSysL2SpfInterval,
        juniIsisSysIshHoldTime,
        juniIsisSysIshConfigTimer,
        juniIsisSysDistributeDomainWide,
        juniIsisSysDistance,
        juniIsisSysL1MetricStyle,
        juniIsisSysL2MetricStyle,
        juniIsisSysIsoRouteTag,
        juniIsisSysMplsTeLevel,
        juniIsisSysMplsTeRtrIdIfIndex,
        juniIsisSysMplsTeSpfUseAnyBestPath,
        juniIsisSysReferenceBandwidth,
        juniIsisSysHighReferenceBandwidth,
        juniIsisManAreaAddrRowStatus,
        juniIsisSysProtSuppRowStatus,
        juniIsisSummAddrRowStatus,
        juniIsisSummAddrOperState,
        juniIsisSummAddrDefaultMetric,
        juniIsisSummAddrDelayMetric,
        juniIsisSummAddrExpenseMetric,
        juniIsisSummAddrErrorMetric,
        juniIsisSummLevel,
        juniIsisSysHostNameAreaAddr,
        juniIsisSysHostNameName,
        juniIsisSysHostNameType,
        juniIsisSysHostNameRowStatus,
        juniIsisSysAreaAuthenticationPwd,
        juniIsisSysAreaAuthenticationKeyType,
        juniIsisSysAreaAuthenticationStartAcceptTime,
        juniIsisSysAreaAuthenticationStartGenerateTime,
        juniIsisSysAreaAuthenticationStopAcceptTime,
        juniIsisSysAreaAuthenticationStopGenerateTime,
        juniIsisSysAreaAuthenticationRowStatus,
        juniIsisSysDomainAuthenticationPwd,
        juniIsisSysDomainAuthenticationKeyType,
        juniIsisSysDomainAuthenticationStartAcceptTime,
        juniIsisSysDomainAuthenticationStartGenerateTime,
        juniIsisSysDomainAuthenticationStopAcceptTime,
        juniIsisSysDomainAuthenticationStopGenerateTime,
        juniIsisSysDomainAuthenticationRowStatus,
        juniIsisMplsTeSystemId,
        juniIsisMplsTeRouterId,
        juniIsisMplsTeTunnelMetric,
        juniIsisMplsTeTunnelRelMetric,
        juniIsisMplsTeTunnelName }
        
    STATUS      current
    DESCRIPTION
        "The system level objects for ISIS management functionality."
    ::= { juniIsisMIBGroups 7 }
END

