OSPFV3-MIB DEFINITIONS ::= BEGIN 
 
    IMPORTS 
-- **********************************************************
-- > > >  Use Alcatel Branch Until IANA Assigns Number  < < <
-- **********************************************************
						routingIND1Ospf3		FROM ALCATEL-IND1-BASE
-- **********************************************************
-- > > >  Use Alcatel Branch Until IANA Assigns Number  < < <
-- **********************************************************

--            MODULE-IDENTITY, OBJECT-TYPE, mib-2, 
            MODULE-IDENTITY, OBJECT-TYPE,
            Counter32, Gauge32, Integer32, Unsigned32 
                    FROM SNMPv2-SMI 
            TEXTUAL-CONVENTION, TruthValue, StorageType, RowStatus 
                    FROM SNMPv2-TC 
            MODULE-COMPLIANCE, OBJECT-GROUP 
                    FROM SNMPv2-CONF 
            InterfaceIndex 
                    FROM IF-MIB 
            InetAddressType, InetAddress, InetAddressPrefixLength 
            				FROM INET-ADDRESS-MIB
            Metric, BigMetric, Status,  
            HelloRange, DesignatedRouterPriority 
                    FROM OSPF-MIB; 
    
    ospfv3MIB MODULE-IDENTITY 
  
            LAST-UPDATED "200505021200Z" 
            ORGANIZATION "IETF OSPF Working Group" 
            CONTACT-INFO 
                "WG E-Mail: ospf@peach.ease.lsoft.com 
                 WG Chairs: acee@cisco.com 
                            rohit@utstar.com 
 
                 Dan Joyal 
                 Nortel Networks 
                 600 Technology Park Drive 
                 Billerica, MA  01821, USA 
                 djoyal@nortel.com 
 
                 Vishwas Manral 
                 SiNett Corporation 
                 2/1, First Floor 
                 Embassy Icon Annex 
                 Infantry Road 
                 Bangalore 560001 
                 vishwas@sinett.com" 
 
             DESCRIPTION 
                 "The MIB module to describe OSPF version 3. 
 
                  Copyright (C) The Internet Society (2005). 
                  This version of this MIB module is part of 
                  RFC XXXX;  see the RFC itself for full legal 
                  notices." 
    
             REVISION "200505021200Z" 
             DESCRIPTION -- RFC Editor assigns RFC xxxx 
                 "Initial version, published as RFC xxxx" 
 
--             ::= { mib-2 XXX } 
-- **********************************************************
-- > > >  Use Alcatel Branch Until IANA Assigns Number  < < <
-- **********************************************************
    ::= { routingIND1Ospf3 999 }
-- **********************************************************
-- > > >  Use Alcatel Branch Until IANA Assigns Number  < < <
-- **********************************************************

 
    -- Texual conventions 
 
    Ospfv3UpToRefreshIntervalTc ::= TEXTUAL-CONVENTION 
             DISPLAY-HINT "d" 
             STATUS        current 
             DESCRIPTION 
                "The values one might be able to configure for                  
                variables bounded by the Refresh Interval" 
             SYNTAX      Integer32 (1..1800) 
 
    Ospfv3DeadIntRangeTc ::= TEXTUAL-CONVENTION 
             DISPLAY-HINT "d" 
             STATUS        current 
             DESCRIPTION 
                "The range, in seconds, of dead interval value." 
             SYNTAX      Integer32 (1..'FFFF'h) 
    
    Ospfv3RouterIdTc ::= TEXTUAL-CONVENTION 
  
             DISPLAY-HINT "d" 
             STATUS      current 
             DESCRIPTION 
                "A 32-bit, unsigned integer uniquely identifying the 
                router in the Autonomous System. To ensure uniqueness, 
                this may default to the value of one of the router's 
                IPv4 host addresses if IPv4 is configured on the 
                router." 
             SYNTAX      Unsigned32 (0..'FFFFFFFF'h) 
 
    Ospfv3AreaIdTc ::= TEXTUAL-CONVENTION 
             DISPLAY-HINT "d" 
             STATUS      current 
             DESCRIPTION 
                "An OSPFv3 Area Identifier" 
             SYNTAX      Unsigned32 (0..'FFFFFFFF'h) 
 
    Ospfv3IfInstIdTc ::= TEXTUAL-CONVENTION 
             DISPLAY-HINT "d" 
             STATUS      current 
             DESCRIPTION 
                "An OSPFv3 interface instance ID" 
             SYNTAX      Integer32 (0..255) 
    
 
    -- Top-level structure of MIB 
    ospfv3Objects        OBJECT IDENTIFIER ::= { ospfv3MIB 1 } 
    ospfv3Conformance    OBJECT IDENTIFIER ::= { ospfv3MIB 2 } 
 
    -- OSPFv3 General Variables 
 
    -- These parameters apply globally to the Router's 
    -- OSPFv3 Process. 
 
    ospfv3GeneralGroup OBJECT IDENTIFIER ::= { ospfv3Objects 1 } 
 
    ospfv3RouterId OBJECT-TYPE 
            SYNTAX         Ospfv3RouterIdTc 
            MAX-ACCESS     read-write 
            STATUS         current 
            DESCRIPTION 
                "A 32-bit integer uniquely identifying the 
                router in the Autonomous System. To ensure 
                uniqueness, this may default to the value of 
                one of the router's IPv4 host addresses, 
                represented as a 32-bit unsigned integer, 
                if IPv4 is configured on the router." 
            ::= { ospfv3GeneralGroup 1 } 
 
    ospfv3AdminStat OBJECT-TYPE 
            SYNTAX          Status 
            MAX-ACCESS      read-write 
            STATUS          current 
  
            DESCRIPTION 
                "The administrative status of OSPFv3 in the 
                router. The value 'enabled' denotes that the 
                OSPFv3 Process is active on at least one 
                interface; 'disabled' disables it on all 
                interfaces." 
            ::= { ospfv3GeneralGroup 2 } 
 
    ospfv3VersionNumber OBJECT-TYPE 
            SYNTAX          INTEGER { version3 (3) } 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The version number of OSPF for IPv6 is 3." 
            ::= { ospfv3GeneralGroup 3 } 
 
    ospfv3AreaBdrRtrStatus OBJECT-TYPE 
            SYNTAX          TruthValue 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "A flag to note whether this router is an area 
                border router." 
            REFERENCE 
                "OSPF Version 2, Section 3 Splitting the AS into 
                Areas" 
            ::= { ospfv3GeneralGroup 4 } 
 
    ospfv3ASBdrRtrStatus OBJECT-TYPE 
            SYNTAX          TruthValue 
            MAX-ACCESS      read-write 
            STATUS          current 
            DESCRIPTION 
                "A flag to note whether this router is  
                configured as an Autonomous System border router." 
            REFERENCE 
                "OSPF Version 2, Section 3.3 Classification of 
                routers" 
            ::= { ospfv3GeneralGroup 5 } 
 
    ospfv3AsScopeLsaCount OBJECT-TYPE 
            SYNTAX          Gauge32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The number of AS-Scope (e.g. AS-External) link state 
                advertisements in the link state database." 
            ::= { ospfv3GeneralGroup 6 } 
 
    ospfv3AsScopeLsaCksumSum OBJECT-TYPE 
            SYNTAX          Integer32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The 32-bit unsigned sum of the LS checksums of 
                the AS-scoped link state advertisements  
                contained in the link state database. This sum 
                can be  used  to determine if there has been a 
                change in a router's link state database, and 
                to compare the link state database of two 
                routers." 
            ::= { ospfv3GeneralGroup 7 } 
 
    ospfv3OriginateNewLsas OBJECT-TYPE 
            SYNTAX          Counter32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The number of new link-state advertisements 
                that have been originated.  This number is 
                incremented each time the router originates a new 
                LSA." 
            ::= { ospfv3GeneralGroup 8 } 
 
    ospfv3RxNewLsas OBJECT-TYPE 
            SYNTAX          Counter32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The number of link state advertisements  
                received determined to be new instantiations. 
                This number does not include newer  
                instantiations of self-originated link state 
                advertisements." 
            ::= { ospfv3GeneralGroup 9 } 
 
    ospfv3ExtLsaCount OBJECT-TYPE 
            SYNTAX          Gauge32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The number of External(LS type 0x4005) in the  
                link state database" 
            ::= { ospfv3GeneralGroup 10 } 
 
 
    ospfv3ExtAreaLsdbLimit OBJECT-TYPE 
            SYNTAX          Integer32 (-1..'7FFFFFFF'h) 
            MAX-ACCESS      read-write 
            STATUS          current 
            DESCRIPTION 
                "The maximum number of non-default  
                AS-external-LSAs entries that can be stored in the 
                link state database. If the value is -1, then 
                there is no limit. 
 
                When the number of non-default AS-external-LSAs 
                in a router's link-state database reaches 
                ospfv3ExtAreaLsdbLimit, the router enters Overflow 
                state. The router never holds more than 
                ospfv3ExtAreaLsdbLimit non-default AS-external-LSAs 
                in its database. OspfExtAreaLsdbLimit MUST be set 
                identically in all routers attached to the OSPFv3 
                backbone and/or any regular OSPFv3 area. (i.e., 
                OSPFv3 stub areas and NSSAs are excluded)." 
            ::= { ospfv3GeneralGroup 11 } 
 
    ospfv3MulticastExtensions OBJECT-TYPE 
            SYNTAX          BITS { 
                                     intraAreaMulticast(0), 
                                     interAreaMulticast(1), 
                                     interAsMulticast(2) 
                                 } 
                                         
            MAX-ACCESS      read-write 
            STATUS          current 
            DESCRIPTION 
                "A Bit Mask indicating whether the router is 
                forwarding IPv6 multicast datagrams based on 
                the algorithms defined in the  Multicast 
                Extensions to OSPF. 
 
                If intraAreaMulticast set, indicates that the router 
                can forward IPv6 multicast datagrams in the router's 
                directly attached areas (called intra-area 
                multicast routing). 
 
                If interAreaMulticast set, indicates that the router 
                can forward IPv6 multicast datagrams between OSPFv3 
                areas (called inter-area multicast routing). 
 
                If interAsMulticast set, indicates that the router can 
                forward  IPv6  multicast datagrams between 
                Autonomous Systems (called inter-AS multicast 
                routing). 
 
                Only certain combinations of bit settings are 
                allowed, namely: 
                        - All bits cleared (no multicasting) 
                        - intraAreaMulticast only, 
                        - intraAreaMulticast and interAreaMulticast, 
                        - intraAreaMulticast and interAsMulticast 
                        - intraAreaMulticast, interAreaMulticast and 
                                interAsMulticast 
                By default, all bits are cleared." 
            ::= { ospfv3GeneralGroup 12 } 
 
    ospfv3ExitOverflowInterval OBJECT-TYPE 
            SYNTAX          Unsigned32 
            UNITS           "seconds" 
            MAX-ACCESS      read-write 
            STATUS          current 
            DESCRIPTION 
                "The number of seconds that, after entering 
                Overflow State, a router will attempt to leave 
                Overflow State. This allows the router to again 
                originate non-default, AS-External-LSAs. When 
                set to 0, the router will not leave Overflow 
                State until restarted." 
            ::= { ospfv3GeneralGroup 13 } 
 
    ospfv3DemandExtensions OBJECT-TYPE 
            SYNTAX         TruthValue 
            MAX-ACCESS     read-write 
            STATUS         current 
            DESCRIPTION 
                "The router's support for demand routing." 
            REFERENCE 
                "OSPF Version 2, Appendix on Demand Routing" 
            ::= { ospfv3GeneralGroup 14 } 
 
    ospfv3ReferenceBandwidth OBJECT-TYPE  
           SYNTAX       Unsigned32  
           MAX-ACCESS   read-write  
           STATUS       current  
           DESCRIPTION  
              "Reference bandwidth in kilobits/second for  
              calculating default interface metrics. The  
              default value is 100,000 KBPS (100 MBPS)"  
        ::= { ospfv3GeneralGroup 15 } 
 
    ospfv3RestartSupport OBJECT-TYPE  
           SYNTAX       INTEGER { none (1),  
                                  plannedOnly (2),  
                                  plannedAndUnplanned (3)  
                             } 
           MAX-ACCESS   read-write  
           STATUS       current  
           DESCRIPTION  
              "The router's support for OSPF Graceful restart.  
              Options include: no restart support, only planned  
              restarts or both planned and unplanned restarts."  
           ::= { ospfv3GeneralGroup 16 }  
        
    ospfv3RestartInterval OBJECT-TYPE  
           SYNTAX       Ospfv3UpToRefreshIntervalTc 
           UNITS        "seconds"  
           MAX-ACCESS   read-write  
           STATUS       current  
           DESCRIPTION  
              "Configured OSPF Graceful restart timeout interval."  
           ::= { ospfv3GeneralGroup 17 }  
        
    ospfv3RestartStatus OBJECT-TYPE  
           SYNTAX       INTEGER { notRestarting (1),  
                                  plannedRestart (2),  
                                  unplannedRestart (3)  
                                }  
           MAX-ACCESS   read-only  
           STATUS       current  
           DESCRIPTION  
              "The current status of OSPF Graceful restart capability."  
           ::= { ospfv3GeneralGroup 18 }  
        
    ospfv3RestartAge OBJECT-TYPE  
           SYNTAX       Ospfv3UpToRefreshIntervalTc 
           UNITS        "seconds"  
           MAX-ACCESS   read-only  
           STATUS       current  
           DESCRIPTION  
              "Remaining time in current OSPF Graceful restart  
              interval."  
           ::= { ospfv3GeneralGroup 19 }  
        
    ospfv3RestartExitRc OBJECT-TYPE  
           SYNTAX       INTEGER { none (1),  
                                  inProgress (2),  
                                  completed (3), 
                                  timedOut (4), 
                                  topologyChanged (5) 
                                }  
           MAX-ACCESS   read-only  
           STATUS       current  
           DESCRIPTION  
              "Describes the outcome of the last attempt at a  
              Graceful restart. 
     
              none:............no restart has yet been attempted. 
              inProgress:......a restart attempt is currently underway. 
              completed:.......the last restart completed successfully. 
              timedOut:........the last restart timed out. 
              topologyChanged:.the last restart was aborted due to 
                               a topology change."  
        ::= { ospfv3GeneralGroup 20 } 
 
 
    -- The OSPFv3 Area Data Structure contains information 
    -- regarding the various areas. The interfaces and 
    -- virtual links are configured as part of these areas. 
    -- Area 0, by definition, is the Backbone Area 
 
    ospfv3AreaTable OBJECT-TYPE 
            SYNTAX          SEQUENCE OF Ospfv3AreaEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "Information describing the configured  
                parameters and cumulative statistics of the router's 
                attached areas." 
            REFERENCE 
                "OSPF Version 2, Section 6 The Area Data  
                Structure" 
            ::= { ospfv3Objects 2 } 
 
    ospfv3AreaEntry OBJECT-TYPE 
            SYNTAX          Ospfv3AreaEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "Information describing the configured  
                parameters and cumulative statistics of one of the 
                router's attached areas." 
            INDEX           { ospfv3AreaId } 
            ::= { ospfv3AreaTable 1 } 
 
    Ospfv3AreaEntry ::= SEQUENCE { 
            ospfv3AreaId 
                    Ospfv3AreaIdTc, 
            ospfv3ImportAsExtern 
                    INTEGER, 
            ospfv3AreaSpfRuns 
                    Counter32, 
            ospfv3AreaBdrRtrCount 
                    Gauge32, 
            ospfv3AreaAsBdrRtrCount 
                    Gauge32, 
            ospfv3AreaScopeLsaCount 
                    Gauge32, 
            ospfv3AreaScopeLsaCksumSum 
                    Integer32, 
            ospfv3AreaSummary 
                    INTEGER, 
            ospfv3AreaStatus 
                    RowStatus, 
            ospfv3StubMetric 
                    BigMetric, 
            ospfv3AreaNssaTranslatorRole 
                    INTEGER, 
            ospfv3AreaNssaTranslatorState 
                    INTEGER, 
            ospfv3AreaNssaTranslatorStabInt 
                    Unsigned32, 
            ospfv3AreaNssaTranslatorEvents 
                    Counter32, 
            ospfv3AreaStubMetricType 
                    INTEGER 
            } 
 
    ospfv3AreaId OBJECT-TYPE 
            SYNTAX          Ospfv3AreaIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "A 32-bit integer uniquely identifying an area. 
                Area ID 0 is used for the OSPFv3 backbone." 
            REFERENCE 
                "OSPF Version 2, Appendix C.2 Area parameters" 
            ::= { ospfv3AreaEntry 1 } 
 
    ospfv3ImportAsExtern OBJECT-TYPE 
            SYNTAX          INTEGER { 
                            importExternal(1),   -- normal area 
                            importNoExternal(2), -- stub area 
                            importNssa(3)        -- not-so-stubby-area 
                            } 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "Indicates whether an area is a Stub area, NSSA, or 
                standard area. AS-scope LSAs are not imported into Stub 
                Areas or NSSAs. NSSAs import AS-External data as NSSA 
                LSAs which have Area-scope" 
            REFERENCE 
                "OSPF Version 2, Appendix C.2 Area parameters" 
            DEFVAL { importExternal } 
            ::= { ospfv3AreaEntry 2 } 
 
    ospfv3AreaSpfRuns OBJECT-TYPE 
            SYNTAX          Counter32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The number of times that the intra-area route 
                table has  been  calculated  using this area's 
                link state database. This is typically done 
                using Dijkstra's algorithm." 
            ::= { ospfv3AreaEntry 3 } 
 
    ospfv3AreaBdrRtrCount OBJECT-TYPE 
            SYNTAX          Gauge32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The total number of area border routers 
                reachable within this area. This is initially zero, 
                and is calculated in each SPF Pass." 
            ::= { ospfv3AreaEntry 4 } 
 
    ospfv3AreaAsBdrRtrCount OBJECT-TYPE 
            SYNTAX          Gauge32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The total number of Autonomous System border 
                routers reachable within this area. This is 
                initially zero, and is calculated in each SPF 
                Pass." 
            ::= { ospfv3AreaEntry 5 } 
 
    ospfv3AreaScopeLsaCount OBJECT-TYPE 
            SYNTAX          Gauge32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The total number of Area-Scope link state  
                advertisements in  this  area's link state  
                database." 
            ::= { ospfv3AreaEntry 6 } 
 
    ospfv3AreaScopeLsaCksumSum OBJECT-TYPE 
            SYNTAX          Integer32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The 32-bit unsigned sum of the Area-Scope link state 
                advertisements' LS checksums contained in this 
                area's link state database. The sum can be used 
                to determine if there has been a change in a 
                router's link state database, and to compare the 
                link-state database of two routers." 
            ::= { ospfv3AreaEntry 7 } 
 
    ospfv3AreaSummary OBJECT-TYPE 
            SYNTAX          INTEGER { 
                            noAreaSummary(1), 
                            sendAreaSummary(2) 
                            } 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The variable ospfv3AreaSummary controls the 
                import of Inter-Area LSAs into stub areas. It 
                has no effect on other areas. 
 
                If it is noAreaSummary, the router will neither 
                originate nor propagate Inter-Area LSAs into the 
                stub area. It will rely entirely on its default 
                route. 
 
                If it is sendAreaSummary, the router will both 
                summarize and propagate Inter-Area LSAs." 
            DEFVAL   { sendAreaSummary } 
            ::= { ospfv3AreaEntry 8 } 
 
    ospfv3AreaStatus OBJECT-TYPE 
            SYNTAX          RowStatus 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "This variable controls the status of the  
                entry. The use of RowStatus is covered in more detail 
                in [6]." 
            ::= { ospfv3AreaEntry 9 } 
 
    ospfv3StubMetric OBJECT-TYPE 
            SYNTAX          BigMetric 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The metric value advertised for the default route 
                 into Stub and NSSA areas." 
            ::= { ospfv3AreaEntry 10 } 
 
    ospfv3AreaNssaTranslatorRole OBJECT-TYPE 
            SYNTAX          INTEGER { always(1), candidate(2) } 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "Indicates an NSSA Border router's ability to 
                perform NSSA translation of NSSA-LSAs into 
                AS-External-LSAs." 
            DEFVAL { candidate } 
            ::= { ospfv3AreaEntry 11 } 
 
    ospfv3AreaNssaTranslatorState OBJECT-TYPE 
            SYNTAX          INTEGER { 
                            enabled(1), 
                            elected(2), 
                            disabled(3) 
                            } 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "Indicates if and how an NSSA Border router is 
                 performing NSSA translation of NSSA-LSAs into  
                AS-External-LSAÆs. When this object is set to enabled, 
                the NSSA Border router's ospfv3AreaNssTranslatorRole 
                has been set to always. When this object is set to 
                elected, a candidate NSSA Border router is translating 
                NSSA-LSAÆs into AS-External-LSAÆs. When this object is 
                set to disabled, a candidate NSSA Border router is NOT 
                translating NSSA-LSAÆs into AS-External-LSAÆs." 
            ::= { ospfv3AreaEntry 12 } 
 
    ospfv3AreaNssaTranslatorStabInt OBJECT-TYPE 
            SYNTAX          Unsigned32 
            UNITS           "seconds" 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The number of seconds after an elected translator 
                determines its services are no longer required, that 
                it should continue to perform its translation duties." 
            DEFVAL { 40 } 
            ::= { ospfv3AreaEntry 13 } 
 
    ospfv3AreaNssaTranslatorEvents OBJECT-TYPE 
            SYNTAX          Counter32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "Indicates the number of Translator State changes 
                that have occurred since the last boot-up." 
            ::= { ospfv3AreaEntry 14 } 
    
    ospfv3AreaStubMetricType OBJECT-TYPE 
            SYNTAX       INTEGER { 
                            ospfv3Metric (1),   -- OSPF Metric 
                            comparableCost (2), -- external type 1 
                            nonComparable (3)   -- external type 2 
                            } 
            MAX-ACCESS   read-create 
            STATUS       current 
            DESCRIPTION 
               "This variable displays the type of metric 
               advertised as a default route." 
            DEFVAL { ospfv3Metric } 
            ::= { ospfv3AreaEntry 15 } 
    
    -- OSPFv3 AS-Scope Link State Database 
 
    -- The Link State Database contains the AS-Scope Link State 
    -- Advertisements from throughout the areas that the 
    -- device is attached to. 
 
    ospfv3AsLsdbTable OBJECT-TYPE 
            SYNTAX          SEQUENCE OF Ospfv3AsLsdbEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The OSPFv3 Process's AS-Scope Link State Database." 
            ::= { ospfv3Objects 3 } 
 
    ospfv3AsLsdbEntry OBJECT-TYPE 
            SYNTAX          Ospfv3AsLsdbEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "A single AS-Scope Link State Advertisement." 
            INDEX           { ospfv3AsLsdbType, 
                              ospfv3AsLsdbRouterId, 
                              ospfv3AsLsdbLsid } 
            ::= { ospfv3AsLsdbTable 1 } 
 
    Ospfv3AsLsdbEntry ::= SEQUENCE { 
            ospfv3AsLsdbType 
                    Unsigned32, 
            ospfv3AsLsdbRouterId 
                    Ospfv3RouterIdTc, 
            ospfv3AsLsdbLsid 
                    Unsigned32, 
            ospfv3AsLsdbSequence 
                    Integer32, 
            ospfv3AsLsdbAge 
                    Integer32, 
            ospfv3AsLsdbChecksum 
                    Integer32, 
            ospfv3AsLsdbAdvertisement 
                    OCTET STRING, 
            ospfv3AsLsdbTypeKnown 
                    TruthValue 
            } 
 
    ospfv3AsLsdbType OBJECT-TYPE 
            SYNTAX          Unsigned32(0..'FFFFFFFF'h) 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The type of the link state advertisement. 
                Each link state type has a separate  
                advertisement format. AS-Scope LSAs not recognized 
                by the router may be stored in the database." 
            ::= { ospfv3AsLsdbEntry 1 } 
 
    ospfv3AsLsdbRouterId OBJECT-TYPE 
            SYNTAX          Ospfv3RouterIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The 32 bit number that uniquely identifies the 
                originating router in the Autonomous System." 
            REFERENCE 
                "OSPF Version 2, Appendix C.1 Global parameters" 
            ::= { ospfv3AsLsdbEntry 2 } 
 
    ospfv3AsLsdbLsid OBJECT-TYPE 
            SYNTAX          Unsigned32 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The Link State ID is an LS Type Specific field 
                containing a unique identifier; 
                it identifies the piece of the  routing  domain 
                that is being described by the advertisement. 
                In contrast to OSPFv2, the LSID has no 
                addressing semantics." 
            ::= { ospfv3AsLsdbEntry 3 } 
 
    -- Note that the OSPF Sequence Number is a 32 bit signed 
    -- integer.  It starts with the value '80000001'h, 
    -- or -'7FFFFFFF'h, and increments until '7FFFFFFF'h 
    -- Thus, a typical sequence number will be very negative. 
 
    ospfv3AsLsdbSequence OBJECT-TYPE 
            SYNTAX          Integer32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The sequence number field is a signed 32-bit 
                integer. It is used to detect old and duplicate 
                link state advertisements. The space of 
                sequence numbers is linearly ordered. The 
                larger the sequence number the more recent the 
                advertisement." 
            REFERENCE 
                "OSPF Version  2,  Section  12.1.6  LS  sequence 
                number" 
            ::= { ospfv3AsLsdbEntry 4 } 
 
    ospfv3AsLsdbAge OBJECT-TYPE 
            SYNTAX          Integer32 -- Should be 0..MaxAge 
                                      -- unless DoNotAge bit is set 
            UNITS           "seconds" 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "This field is the age of the link state  
                advertisement in seconds." 
            REFERENCE 
                "OSPF Version 2, Section 12.1.1 LS age" 
            ::= { ospfv3AsLsdbEntry 5 } 
 
    ospfv3AsLsdbChecksum OBJECT-TYPE 
            SYNTAX          Integer32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "This field is the checksum of the complete 
                contents of the advertisement, excepting the 
                age field. The age field is excepted so that 
                an advertisement's age can be incremented 
                without updating the checksum. The checksum 
                used is the same that is used for ISO 
                connectionless datagrams; it is commonly referred 
                to as the Fletcher checksum." 
            REFERENCE 
                "OSPF Version 2, Section 12.1.7 LS checksum" 
            ::= { ospfv3AsLsdbEntry 6 } 
 
    ospfv3AsLsdbAdvertisement OBJECT-TYPE 
            SYNTAX          OCTET STRING (SIZE (1..65535)) 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The entire Link State Advertisement, including 
                its header." 
            ::= { ospfv3AsLsdbEntry 7 } 
 
    ospfv3AsLsdbTypeKnown OBJECT-TYPE 
            SYNTAX          TruthValue 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "Indicates whether the LSA type is recognized by 
                this Router." 
            ::= { ospfv3AsLsdbEntry 8 } 
 
 
    -- OSPFv3 Area-Scope Link State Database 
 
    -- The Link State Database contains the Area-Scope Link State 
    -- Advertisements from throughout the area that the 
    -- device is attached to. 
 
    ospfv3AreaLsdbTable OBJECT-TYPE 
            SYNTAX          SEQUENCE OF Ospfv3AreaLsdbEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The OSPFv3 Process's Area-Scope Link State Database." 
            ::= { ospfv3Objects 4 } 
 
    ospfv3AreaLsdbEntry OBJECT-TYPE 
            SYNTAX          Ospfv3AreaLsdbEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "A single Area-Scope Link State Advertisement." 
            INDEX           { ospfv3AreaLsdbAreaId, 
                              ospfv3AreaLsdbType, 
                              ospfv3AreaLsdbRouterId, 
                              ospfv3AreaLsdbLsid } 
            ::= { ospfv3AreaLsdbTable 1 } 
 
    Ospfv3AreaLsdbEntry ::= SEQUENCE { 
            ospfv3AreaLsdbAreaId 
                    Ospfv3AreaIdTc, 
            ospfv3AreaLsdbType 
                    Unsigned32, 
            ospfv3AreaLsdbRouterId 
                    Ospfv3RouterIdTc, 
            ospfv3AreaLsdbLsid 
                    Unsigned32, 
            ospfv3AreaLsdbSequence 
                    Integer32, 
            ospfv3AreaLsdbAge 
                    Integer32, 
            ospfv3AreaLsdbChecksum 
                    Integer32, 
            ospfv3AreaLsdbAdvertisement 
                    OCTET STRING, 
            ospfv3AreaLsdbTypeKnown 
                    TruthValue 
            } 
 
    ospfv3AreaLsdbAreaId OBJECT-TYPE 
            SYNTAX          Ospfv3AreaIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The 32-bit identifier of the Area from which the 
                LSA was received." 
            REFERENCE 
                "OSPF Version 2, Appendix C.2 Area parameters" 
            ::= { ospfv3AreaLsdbEntry 1 } 
 
    ospfv3AreaLsdbType OBJECT-TYPE 
            SYNTAX          Unsigned32(0..'FFFFFFFF'h) 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The type of the link state advertisement. 
                Each link state type has a separate 
                advertisement format. Area-Scope LSAs unrecognized 
                by the router are also stored in this database." 
            ::= { ospfv3AreaLsdbEntry 2 } 
 
    ospfv3AreaLsdbRouterId OBJECT-TYPE 
            SYNTAX          Ospfv3RouterIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The 32-bit number that uniquely identifies the 
                originating router in the Autonomous System." 
            REFERENCE 
                "OSPF Version 2, Appendix C.1 Global parameters" 
            ::= { ospfv3AreaLsdbEntry 3 } 
 
    ospfv3AreaLsdbLsid OBJECT-TYPE 
            SYNTAX          Unsigned32 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The Link State ID is an LS Type Specific field 
                containing a unique identifier; 
                it identifies the piece of the  routing  domain 
                that is being described by the advertisement. 
                In contrast to OSPFv2, the LSID has no 
                addressing semantics." 
            ::= { ospfv3AreaLsdbEntry 4 } 
 
    -- Note that the OSPF Sequence Number is a 32 bit signed 
    -- integer.  It starts with the value '80000001'h, 
    -- or -'7FFFFFFF'h, and increments until '7FFFFFFF'h 
    -- Thus, a typical sequence number will be very negative. 
 
    ospfv3AreaLsdbSequence OBJECT-TYPE 
            SYNTAX          Integer32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The sequence number field is a  signed  32-bit 
                integer.   It  is used to detect old and dupli- 
                cate link state advertisements.  The  space  of 
                sequence  numbers  is  linearly  ordered.   The 
                larger the sequence number the more recent  the 
                advertisement." 
            REFERENCE 
                "OSPF Version  2,  Section  12.1.6  LS  sequence 
                number" 
            ::= { ospfv3AreaLsdbEntry 5 } 
 
    ospfv3AreaLsdbAge OBJECT-TYPE 
            SYNTAX          Integer32 -- Should be 0..MaxAge 
                                      -- unless DoNotAge bit is set 
            UNITS           "seconds" 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "This field is the age of the link state 
                advertisement in seconds." 
            REFERENCE 
                "OSPF Version 2, Section 12.1.1 LS age" 
            ::= { ospfv3AreaLsdbEntry 6 } 
 
    ospfv3AreaLsdbChecksum OBJECT-TYPE 
            SYNTAX          Integer32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "This field is the checksum of the complete 
                contents of the advertisement, excepting the 
                age field. The age field is excepted so that 
                an advertisement's age can be incremented 
                without updating the checksum. The checksum 
                used is the same that is used for ISO  
                connectionless datagrams; it is commonly referred 
                to as the Fletcher checksum." 
            REFERENCE 
                "OSPF Version 2, Section 12.1.7 LS checksum" 
            ::= { ospfv3AreaLsdbEntry 7 } 
 
    ospfv3AreaLsdbAdvertisement OBJECT-TYPE 
            SYNTAX          OCTET STRING (SIZE (1..65535)) 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The entire Link State Advertisement, including 
                its header." 
            ::= { ospfv3AreaLsdbEntry 8 } 
 
    ospfv3AreaLsdbTypeKnown OBJECT-TYPE 
            SYNTAX          TruthValue 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "Indicates whether the LSA type is recognized 
                by this Router." 
            ::= { ospfv3AreaLsdbEntry 9 } 
 
    -- OSPFv3 Link-Scope Link State Database 
 
    -- The Link State Database contains the Link-Scope Link State 
    -- Advertisements from the links that the 
    -- device is attached to. 
 
    ospfv3LinkLsdbTable OBJECT-TYPE 
            SYNTAX          SEQUENCE OF Ospfv3LinkLsdbEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The OSPFv3 Process's Link-Scope Link State Database." 
            ::= { ospfv3Objects 5 } 
 
    ospfv3LinkLsdbEntry OBJECT-TYPE 
            SYNTAX          Ospfv3LinkLsdbEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "A single Link-Scope Link State Advertisement." 
            INDEX           { ospfv3LinkLsdbIfIndex, 
                              ospfv3LinkLsdbIfInstId, 
                              ospfv3LinkLsdbType, 
                              ospfv3LinkLsdbRouterId, 
                              ospfv3LinkLsdbLsid } 
            ::= { ospfv3LinkLsdbTable 1 } 
 
    Ospfv3LinkLsdbEntry ::= SEQUENCE { 
            ospfv3LinkLsdbIfIndex 
                    InterfaceIndex, 
            ospfv3LinkLsdbIfInstId 
                    Ospfv3IfInstIdTc, 
            ospfv3LinkLsdbType 
                    Unsigned32, 
            ospfv3LinkLsdbRouterId 
                    Ospfv3RouterIdTc, 
            ospfv3LinkLsdbLsid 
                    Unsigned32, 
            ospfv3LinkLsdbSequence 
                    Integer32, 
            ospfv3LinkLsdbAge 
                    Integer32, 
            ospfv3LinkLsdbChecksum 
                    Integer32, 
            ospfv3LinkLsdbAdvertisement 
                    OCTET STRING, 
            ospfv3LinkLsdbTypeKnown 
                    TruthValue 
            } 
 
    ospfv3LinkLsdbIfIndex OBJECT-TYPE 
            SYNTAX         InterfaceIndex 
            MAX-ACCESS     not-accessible 
            STATUS         current 
            DESCRIPTION 
                "The identifier of the link from which the LSA 
                was received." 
            ::= { ospfv3LinkLsdbEntry 1 } 
 
    ospfv3LinkLsdbIfInstId OBJECT-TYPE 
            SYNTAX         Ospfv3IfInstIdTc 
            MAX-ACCESS     not-accessible 
            STATUS         current 
            DESCRIPTION 
                "The identifier of the interface instance from 
                which the LSA was received." 
            ::= { ospfv3LinkLsdbEntry 2 } 
 
    ospfv3LinkLsdbType OBJECT-TYPE 
            SYNTAX          Unsigned32(0..'FFFFFFFF'h) 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The type of the link state advertisement. 
                Each link state type has a separate 
                advertisement format. Link-Scope LSAs unrecognized 
                by the router are also stored in this database." 
            ::= { ospfv3LinkLsdbEntry 3 } 
 
    ospfv3LinkLsdbRouterId OBJECT-TYPE 
            SYNTAX          Ospfv3RouterIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The 32 bit number that uniquely identifies the 
                originating router in the Autonomous System." 
            REFERENCE 
                "OSPF Version 2, Appendix C.1 Global parameters" 
            ::= { ospfv3LinkLsdbEntry 4 } 
 
    ospfv3LinkLsdbLsid OBJECT-TYPE 
            SYNTAX        Unsigned32 
            MAX-ACCESS    not-accessible 
            STATUS        current 
            DESCRIPTION 
                "The Link State ID is an LS Type Specific field 
                containing a unique identifier; 
                it identifies the piece of the  routing  domain 
                that is being described by the advertisement. 
                In contrast to OSPFv2, the LSID has no 
                addressing semantics." 
            ::= { ospfv3LinkLsdbEntry 5 } 
 
    -- Note that the OSPF Sequence Number is a 32 bit signed 
    -- integer.  It starts with the value '80000001'h, 
    -- or -'7FFFFFFF'h, and increments until '7FFFFFFF'h 
    -- Thus, a typical sequence number will be very negative. 
 
    ospfv3LinkLsdbSequence OBJECT-TYPE 
            SYNTAX          Integer32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The sequence number field is a signed 32-bit 
                integer. It is used to detect old and duplicate 
                link state advertisements. The space of 
                sequence numbers is linearly ordered. The 
                larger the sequence number the more recent the 
                advertisement." 
            REFERENCE 
                "OSPF Version  2,  Section  12.1.6  LS  sequence 
                number" 
            ::= { ospfv3LinkLsdbEntry 6 } 
 
    ospfv3LinkLsdbAge OBJECT-TYPE 
            SYNTAX          Integer32 -- Should be 0..MaxAge 
                                      -- unless DoNotAge bit is set 
            UNITS           "seconds" 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "This field is the age of the link state 
                advertisement in seconds." 
            REFERENCE 
                "OSPF Version 2, Section 12.1.1 LS age" 
            ::= { ospfv3LinkLsdbEntry 7 } 
 
    ospfv3LinkLsdbChecksum OBJECT-TYPE 
            SYNTAX          Integer32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "This field is the checksum of the complete 
                contents of the advertisement, excepting the 
                age field. The age field is excepted so that 
                an advertisement's age can be incremented 
                without updating the  checksum. The checksum 
                used is the same that is used for ISO 
                connectionless datagrams; it is commonly 
                referred to as the Fletcher checksum." 
            REFERENCE 
                "OSPF Version 2, Section 12.1.7 LS checksum" 
            ::= { ospfv3LinkLsdbEntry 8 } 
 
    ospfv3LinkLsdbAdvertisement OBJECT-TYPE 
            SYNTAX          OCTET STRING (SIZE (1..65535)) 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The entire Link State Advertisement, including 
                its header." 
            ::= { ospfv3LinkLsdbEntry 9 } 
 
    ospfv3LinkLsdbTypeKnown OBJECT-TYPE 
            SYNTAX          TruthValue 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "Indicates whether the LSA type is recognized by this 
                 Router." 
            ::= { ospfv3LinkLsdbEntry 10 } 
 
 
    -- OSPF Host Table 
 
    -- The Host/Metric Table indicates what hosts are directly 
    -- attached to the Router, and what metrics and types of 
    -- service should be advertised for them. 
 
    ospfv3HostTable OBJECT-TYPE 
            SYNTAX          SEQUENCE OF Ospfv3HostEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The list of Hosts, and their metrics, that the 
                router will advertise as host routes." 
            REFERENCE 
                "OSPF Version 2, Appendix C.6  Host route 
                parameters" 
            ::= { ospfv3Objects 6 } 
 
    ospfv3HostEntry OBJECT-TYPE 
            SYNTAX          Ospfv3HostEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "A metric to be advertised when a given host is 
                reachable." 
            INDEX           { ospfv3HostAddressType, 
                              ospfv3HostAddress } 
            ::= { ospfv3HostTable 1 } 
 
    Ospfv3HostEntry ::= SEQUENCE { 
            ospfv3HostAddressType 
                    InetAddressType, 
            ospfv3HostAddress 
                    InetAddress, 
            ospfv3HostMetric 
                    Metric, 
            ospfv3HostStatus 
                    RowStatus, 
            ospfv3HostAreaID 
                    Ospfv3AreaIdTc 
            } 
 
    ospfv3HostAddressType OBJECT-TYPE 
            SYNTAX          InetAddressType 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The address type of ospfv3HostAddress. Only IPv6 
                addresses without zone index are expected." 
            REFERENCE 
                "OSPF Version 2, Appendix C.6 Host route  
                parameters" 
            ::= { ospfv3HostEntry 1 } 
 
 
    ospfv3HostAddress OBJECT-TYPE 
            SYNTAX          InetAddress (SIZE (16)) 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The IPv6 Address of the Host. Must be a Global 
                 address." 
            REFERENCE 
                "OSPF Version 2, Appendix C.6 Host route 
                parameters" 
            ::= { ospfv3HostEntry 2 } 
 
    ospfv3HostMetric OBJECT-TYPE 
            SYNTAX          Metric 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The Metric to be advertised." 
            REFERENCE 
                "OSPF Version 2, Appendix C.6 Host route 
                parameters" 
            ::= { ospfv3HostEntry 3 } 
 
    ospfv3HostStatus OBJECT-TYPE 
            SYNTAX          RowStatus 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "This variable controls the status of the 
                entry. The use of RowStatus is covered in 
                more detail in [6]." 
            ::= { ospfv3HostEntry 4 } 
 
    ospfv3HostAreaID OBJECT-TYPE 
            SYNTAX          Ospfv3AreaIdTc 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The Area the Host Entry is to be found within. 
                By default, the area that a subsuming OSPFv3 
                interface is in, or Area 0" 
            REFERENCE 
                "OSPF Version 2, Appendix C.2 Area parameters" 
            ::= { ospfv3HostEntry 5 } 
 
    -- OSPFv3 Interface Table 
 
    ospfv3IfTable OBJECT-TYPE 
            SYNTAX          SEQUENCE OF Ospfv3IfEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The OSPFv3 Interface Table describes the  
                interfaces from the viewpoint of OSPFv3." 
            REFERENCE 
                "OSPF Version 2, Appendix C.3 Router interface 
                parameters" 
            ::= { ospfv3Objects 7 } 
 
    ospfv3IfEntry OBJECT-TYPE 
            SYNTAX          Ospfv3IfEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The OSPFv3 Interface Entry describes one 
                interface from the viewpoint of OSPFv3." 
            INDEX           { ospfv3IfIndex, 
                              ospfv3IfInstId } 
            ::= { ospfv3IfTable 1 } 
 
 
    Ospfv3IfEntry ::= SEQUENCE { 
            ospfv3IfIndex 
                    InterfaceIndex, 
            ospfv3IfInstId 
                    Ospfv3IfInstIdTc, 
            ospfv3IfAreaId 
                    Ospfv3AreaIdTc, 
            ospfv3IfType 
                    INTEGER, 
            ospfv3IfAdminStat 
                    Status, 
            ospfv3IfRtrPriority 
                    DesignatedRouterPriority, 
            ospfv3IfTransitDelay 
                    Ospfv3UpToRefreshIntervalTc, 
            ospfv3IfRetransInterval 
                    Ospfv3UpToRefreshIntervalTc, 
            ospfv3IfHelloInterval 
                    HelloRange, 
            ospfv3IfRtrDeadInterval 
                     Ospfv3DeadIntRangeTc, 
            ospfv3IfPollInterval 
                    Unsigned32, 
            ospfv3IfState 
                    INTEGER, 
            ospfv3IfDesignatedRouter 
                    Ospfv3RouterIdTc, 
            ospfv3IfBackupDesignatedRouter 
                    Ospfv3RouterIdTc, 
            ospfv3IfEvents 
                    Counter32, 
            ospfv3IfStatus 
                    RowStatus, 
            ospfv3IfMulticastForwarding 
                    INTEGER, 
            ospfv3IfDemand 
                    TruthValue, 
            ospfv3IfMetricValue 
                    Metric, 
            ospfv3IfLinkScopeLsaCount 
                    Gauge32, 
            ospfv3IfLinkLsaCksumSum 
                    Integer32, 
            ospfv3IfDemandNbrProbe 
                    TruthValue, 
            ospfv3IfDemandNbrProbeRetxLimit  
                    Unsigned32, 
            ospfv3IfDemandNbrProbeInterval  
                    Unsigned32 
            } 
 
    ospfv3IfIndex OBJECT-TYPE 
            SYNTAX          InterfaceIndex 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The interface index of this OSPFv3 interface. 
                 It corresponds to the interface index of the 
                 IPv6 interface on which OSPFv3 is configured." 
            ::= { ospfv3IfEntry 1 } 
 
    ospfv3IfInstId OBJECT-TYPE 
            SYNTAX          Ospfv3IfInstIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "Enables multiple interface instances of OSPFv3 
                to be run over a single link. Each protocol 
                instance would be assigned a separate ID. This ID 
                has local link significance only." 
            ::= { ospfv3IfEntry 2 } 
 
    ospfv3IfAreaId OBJECT-TYPE 
            SYNTAX          Ospfv3AreaIdTc 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "A 32-bit integer uniquely identifying the area 
                to which the interface connects. Area ID 
                0 is used for the OSPFv3 backbone." 
            DEFVAL          { 0 } 
            ::= { ospfv3IfEntry 3 } 
 
    ospfv3IfType OBJECT-TYPE 
            SYNTAX          INTEGER { 
                            broadcast(1), 
                            nbma(2), 
                            pointToPoint(3), 
                            pointToMultipoint(5) 
                            } 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The OSPFv3 interface type." 
            ::= { ospfv3IfEntry 4 } 
 
    ospfv3IfAdminStat OBJECT-TYPE 
            SYNTAX          Status 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The OSPFv3 interface's administrative status. 
                The value formed on the interface, and the 
                interface will be advertised as an internal route 
                to some area. The value 'disabled' denotes 
                that the interface is external to OSPFv3." 
            DEFVAL          { enabled } 
            ::= { ospfv3IfEntry 5 } 
 
    ospfv3IfRtrPriority OBJECT-TYPE 
            SYNTAX          DesignatedRouterPriority 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The priority of this interface. Used in 
                multi-access networks, this field is used in 
                the designated router election algorithm. The 
                value 0 signifies that the router is not  
                eligible to become the designated router on this 
                particular network. In the event of a tie in 
                this value, routers will use their Router ID as 
                a tie breaker." 
            DEFVAL          { 1 } 
            ::= { ospfv3IfEntry 6 } 
 
    ospfv3IfTransitDelay OBJECT-TYPE 
            SYNTAX          Ospfv3UpToRefreshIntervalTc 
            UNITS           "seconds" 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The estimated number of seconds it takes to 
                transmit a link state update packet over this 
                interface." 
            DEFVAL          { 1 } 
            ::= { ospfv3IfEntry 7 } 
 
    ospfv3IfRetransInterval OBJECT-TYPE 
            SYNTAX          Ospfv3UpToRefreshIntervalTc 
            UNITS           "seconds" 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The number of seconds between link state 
                advertisement retransmissions, for adjacencies 
                belonging to this interface. This value is 
                also used when retransmitting database  
                description and link state request packets." 
            DEFVAL          { 5 } 
            ::= { ospfv3IfEntry 8 } 
 
    ospfv3IfHelloInterval OBJECT-TYPE 
            SYNTAX          HelloRange 
            UNITS           "seconds" 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The length of time, in seconds, between the 
                Hello packets that the router sends on the 
                interface. This value must be the same for all 
                routers attached to a common network." 
            DEFVAL          { 10 } 
            ::= { ospfv3IfEntry 9 } 
 
    ospfv3IfRtrDeadInterval OBJECT-TYPE 
            SYNTAX          Ospfv3DeadIntRangeTc 
            UNITS           "seconds" 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The number of seconds that a router's Hello 
                packets have not been seen before its  
                neighbors declare the router down on the interface. 
                This should be some multiple of the Hello interval. 
                This value must be the same for all routers attached 
                to a common network." 
            DEFVAL          { 40 } 
            ::= { ospfv3IfEntry 10 } 
 
    ospfv3IfPollInterval OBJECT-TYPE 
            SYNTAX          Unsigned32 
            UNITS           "seconds" 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The larger time interval, in seconds, between 
                the Hello packets sent to an inactive  
                non-broadcast multi-access neighbor." 
            DEFVAL          { 120 } 
            ::= { ospfv3IfEntry 11 } 
 
    ospfv3IfState OBJECT-TYPE 
            SYNTAX          INTEGER { 
                            down(1), 
                            loopback(2), 
                            waiting(3), 
                            pointToPoint(4), 
                            designatedRouter(5), 
                            backupDesignatedRouter(6), 
                            otherDesignatedRouter(7) 
                            } 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The OSPFv3 Interface State." 
            ::= { ospfv3IfEntry 12 } 
 
    ospfv3IfDesignatedRouter OBJECT-TYPE 
            SYNTAX          Ospfv3RouterIdTc 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The Router ID of the Designated Router." 
            ::= { ospfv3IfEntry 13 } 
 
    ospfv3IfBackupDesignatedRouter OBJECT-TYPE 
            SYNTAX          Ospfv3RouterIdTc 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The Router ID of the Backup Designated 
                Router." 
            ::= { ospfv3IfEntry 14 } 
 
    ospfv3IfEvents OBJECT-TYPE 
            SYNTAX          Counter32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The number of times this OSPF interface has 
                changed its state, or an error has occurred." 
            ::= { ospfv3IfEntry 15 } 
 
     ospfv3IfStatus OBJECT-TYPE 
            SYNTAX          RowStatus 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "This variable controls the status of the 
                entry. The use of RowStatus is covered in more 
                detail in [6]." 
            ::= { ospfv3IfEntry 16 } 
 
    ospfv3IfMulticastForwarding OBJECT-TYPE 
            SYNTAX          INTEGER { 
                            blocked(1),   -- no multicast forwarding 
                            multicast(2), -- using multicast address 
                            unicast(3)    -- to each OSPFv3 neighbor 
                            } 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The way multicasts should forwarded on this 
                interface; not forwarded, forwarded as data 
                link multicasts, or forwarded as data link  
                unicasts. Data link multicasting is not  
                meaningful on point to point and NBMA interfaces, 
                and setting ospfv3MulticastForwarding to 0 
                effectively disables all multicast forwarding." 
            DEFVAL { blocked } 
            ::= { ospfv3IfEntry 17 } 
 
    ospfv3IfDemand OBJECT-TYPE 
            SYNTAX          TruthValue 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "Indicates whether Demand OSPFv3 procedures 
                (hello suppression to FULL neighbors and 
                setting the DoNotAge flag on propagated LSAs) 
                should be performed on this interface." 
            DEFVAL { false } 
            ::= { ospfv3IfEntry 18 } 
 
    ospfv3IfMetricValue OBJECT-TYPE 
            SYNTAX          Metric 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The metric assigned to this interface. 
                 The default value of the Metric is 
                Reference Bandwidth / ifSpeed. The value of the   
                reference bandwidth is configured by the 
                ospfv3ReferenceBandwidth object." 
            ::= { ospfv3IfEntry 19 } 
 
     ospfv3IfLinkScopeLsaCount OBJECT-TYPE 
            SYNTAX          Gauge32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The total number of Link-Scope link state 
                advertisements in  this  link's link state 
                database." 
            ::= { ospfv3IfEntry 20 } 
 
     ospfv3IfLinkLsaCksumSum OBJECT-TYPE 
            SYNTAX          Integer32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The 32-bit unsigned sum of the Link-Scope link state 
                advertisements' LS checksums contained in this 
                link's link state database. The sum can be used 
                to determine if  there has been a change in a 
                router's link state database, and to compare the 
                link state database of two routers." 
            ::= { ospfv3IfEntry 21 } 
 
    ospfv3IfDemandNbrProbe OBJECT-TYPE 
            SYNTAX          TruthValue 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                   "Indicates whether or not neighbor probing is 
                   enabled to determine whether or not the neighbor  
                   is inactive. Neighbor probing is disabled by  
                   default." 
            DEFVAL { false } 
            ::= { ospfv3IfEntry 22 } 
 
   ospfv3IfDemandNbrProbeRetxLimit OBJECT-TYPE  
           SYNTAX       Unsigned32  
           UNITS        "seconds"  
           MAX-ACCESS   read-create 
           STATUS       current  
           DESCRIPTION  
              "The number of consecutive LSA retransmissions before 
              the neighbor is deemed inactive and the neighbor  
              adjacency is brought down."  
           DEFVAL          { 10 } 
           ::= { ospfv3IfEntry 23}  
 
 
   ospfv3IfDemandNbrProbeInterval OBJECT-TYPE  
           SYNTAX       Unsigned32  
           UNITS        "seconds"  
           MAX-ACCESS   read-create 
           STATUS       current  
           DESCRIPTION  
              "Defines how often the neighbor will be probed."  
           DEFVAL          { 120 } 
           ::= { ospfv3IfEntry 24 }  
 
 
    -- OSPFv3 Virtual Interface Table 
 
    -- The Virtual Interface Table describes the virtual 
    -- links that the OSPFv3 Process is configured to 
    -- carry on. 
 
    ospfv3VirtIfTable OBJECT-TYPE 
            SYNTAX          SEQUENCE OF Ospfv3VirtIfEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "Information about this router's virtual 
                interfaces." 
            REFERENCE 
                "OSPF Version 2, Appendix C.4 Virtual link 
                parameters" 
            ::= { ospfv3Objects 8 } 
 
    ospfv3VirtIfEntry OBJECT-TYPE 
            SYNTAX          Ospfv3VirtIfEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "Information about a single Virtual Interface." 
            INDEX           { ospfv3VirtIfAreaId, 
                              ospfv3VirtIfNeighbor } 
            ::= { ospfv3VirtIfTable 1 } 
 
    Ospfv3VirtIfEntry ::= SEQUENCE { 
            ospfv3VirtIfAreaId 
                    Ospfv3AreaIdTc, 
            ospfv3VirtIfNeighbor 
                    Ospfv3RouterIdTc, 
            ospfv3VirtIfIndex 
                    InterfaceIndex, 
            ospfv3VirtIfInstId 
                    Ospfv3IfInstIdTc, 
            ospfv3VirtIfTransitDelay 
                    Ospfv3UpToRefreshIntervalTc, 
            ospfv3VirtIfRetransInterval 
                    Ospfv3UpToRefreshIntervalTc, 
            ospfv3VirtIfHelloInterval 
                    HelloRange, 
            ospfv3VirtIfRtrDeadInterval 
                    Ospfv3DeadIntRangeTc, 
            ospfv3VirtIfState 
                    INTEGER, 
            ospfv3VirtIfEvents 
                    Counter32, 
            ospfv3VirtIfStatus 
                    RowStatus, 
            ospfv3VirtIfLinkScopeLsaCount 
                    Gauge32, 
            ospfv3VirtIfLinkLsaCksumSum 
                    Integer32 
            } 
 
    ospfv3VirtIfAreaId OBJECT-TYPE 
            SYNTAX          Ospfv3AreaIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The Transit Area that the Virtual Link 
                traverses. By definition, this is not 
                Area 0" 
            ::= { ospfv3VirtIfEntry 1 } 
 
    ospfv3VirtIfNeighbor OBJECT-TYPE 
            SYNTAX          Ospfv3RouterIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The Router ID of the Virtual Neighbor." 
            ::= { ospfv3VirtIfEntry 2 } 
 
    ospfv3VirtIfIndex OBJECT-TYPE 
            SYNTAX          InterfaceIndex 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The interface index assigned to this OSPFv3 virtual 
                interface. It is advertised in Hello's sent over 
                the virtal link and in the router's router-LSAs." 
            ::= { ospfv3VirtIfEntry 3 } 
 
    ospfv3VirtIfInstId OBJECT-TYPE 
            SYNTAX          Ospfv3IfInstIdTc 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "Specifies the interface instance ID to be used 
                for the virtual interface. This ID has local link 
                significance only." 
            DEFVAL          { 0 } 
            ::= { ospfv3VirtIfEntry 4 } 
 
    ospfv3VirtIfTransitDelay OBJECT-TYPE 
            SYNTAX          Ospfv3UpToRefreshIntervalTc 
            UNITS           "seconds" 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The estimated number of seconds it takes to 
                transmit a link state update packet over this 
                interface." 
            DEFVAL          { 1 } 
            ::= { ospfv3VirtIfEntry 5 } 
 
    ospfv3VirtIfRetransInterval OBJECT-TYPE 
            SYNTAX          Ospfv3UpToRefreshIntervalTc 
            UNITS           "seconds" 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The number of seconds between link state 
                advertisement retransmissions, for adjacencies 
                belonging to this  interface. This value is 
                also used when retransmitting database 
                description and link state request packets. This 
                value should be well over the expected 
                round-trip time." 
            DEFVAL          { 5 } 
            ::= { ospfv3VirtIfEntry 6 } 
 
    ospfv3VirtIfHelloInterval OBJECT-TYPE 
            SYNTAX          HelloRange 
            UNITS           "seconds" 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The length of time, in seconds, between the 
                Hello packets that the router sends on the 
                interface.  This value must be the same for the 
                virtual neighbor." 
            DEFVAL          { 10 } 
            ::= { ospfv3VirtIfEntry 7 } 
 
    ospfv3VirtIfRtrDeadInterval OBJECT-TYPE 
            SYNTAX          Ospfv3DeadIntRangeTc 
            UNITS           "seconds" 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The number of seconds that a router's Hello 
                packets have not been seen before its 
                neighbors declare the router down. This should 
                be some multiple of the Hello interval. This 
                value must be the same for the virtual 
                neighbor." 
            DEFVAL          { 60 } 
            ::= { ospfv3VirtIfEntry 8 } 
 
    ospfv3VirtIfState OBJECT-TYPE 
            SYNTAX          INTEGER { 
                            down(1), 
                            pointToPoint(4) 
                            } 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "OSPF virtual interface states. The same encoding 
                as the ospfV3IfTable is used." 
            ::= { ospfv3VirtIfEntry 9 } 
 
    ospfv3VirtIfEvents OBJECT-TYPE 
            SYNTAX          Counter32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The number of state changes or error events on 
                this Virtual Link" 
            ::= { ospfv3VirtIfEntry 10 } 
 
    ospfv3VirtIfStatus OBJECT-TYPE 
            SYNTAX          RowStatus 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "This variable controls the status of the entry. 
                The use of RowStatus is covered in more detail 
                in [6]." 
            ::= { ospfv3VirtIfEntry 11 } 
 
    ospfv3VirtIfLinkScopeLsaCount OBJECT-TYPE 
            SYNTAX          Gauge32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The total number of Link-Scope link state 
                advertisements in  this  virtual link's link state 
                database." 
            ::= { ospfv3VirtIfEntry 12 } 
 
    ospfv3VirtIfLinkLsaCksumSum OBJECT-TYPE 
            SYNTAX          Integer32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The 32-bit unsigned sum of the Link-Scope link-state 
                advertisements'  LS  checksums  contained in this 
                virtual link's link-state database.  The sum can be used 
                to determine if  there  has been  a  change  in a 
                router's link state database, and to compare the 
                link state database of two routers." 
            ::= { ospfv3VirtIfEntry 13 } 
 
 
    -- OSPFv3 Neighbor Table 
 
    -- The OSPFv3 Neighbor Table describes all neighbors in 
    -- the locality of the subject router. 
 
    ospfv3NbrTable OBJECT-TYPE 
            SYNTAX          SEQUENCE OF Ospfv3NbrEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "A table of non-virtual neighbor information." 
            REFERENCE 
                "OSPF Version 2, Section 10 The Neighbor Data 
                Structure" 
            ::= { ospfv3Objects 9 } 
 
    ospfv3NbrEntry OBJECT-TYPE 
            SYNTAX          Ospfv3NbrEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The information regarding a single neighbor." 
            REFERENCE 
                "OSPF Version 2, Section 10 The Neighbor Data 
                Structure" 
            INDEX           { ospfv3NbrIfIndex, 
                              ospfv3NbrIfInstId, 
                              ospfv3NbrRtrId } 
            ::= { ospfv3NbrTable 1 } 
 
    Ospfv3NbrEntry ::= SEQUENCE { 
            ospfv3NbrIfIndex 
                    InterfaceIndex, 
            ospfv3NbrIfInstId 
                    Ospfv3IfInstIdTc, 
            ospfv3NbrRtrId 
                    Ospfv3RouterIdTc, 
            ospfv3NbrAddressType 
                    InetAddressType, 
            ospfv3NbrAddress 
                    InetAddress,             
            ospfv3NbrOptions 
                    Integer32, 
            ospfv3NbrPriority 
                    DesignatedRouterPriority, 
            ospfv3NbrState 
                    INTEGER, 
            ospfv3NbrEvents 
                    Counter32, 
            ospfv3NbrLsRetransQLen 
                    Gauge32, 
            ospfv3NbrHelloSuppressed 
                    TruthValue, 
            ospfv3NbrIfId 
                    InterfaceIndex, 
            ospfv3NbrRestartHelperStatus  
                    INTEGER,  
            ospfv3NbrRestartHelperAge  
                    Ospfv3UpToRefreshIntervalTc,  
            ospfv3NbrRestartHelperExitRc  
                    INTEGER 
            } 
 
    ospfv3NbrIfIndex OBJECT-TYPE 
            SYNTAX          InterfaceIndex 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The local link ID of the link over which the 
                 neighbor can be reached." 
            ::= { ospfv3NbrEntry 1 } 
 
    ospfv3NbrIfInstId OBJECT-TYPE 
            SYNTAX          Ospfv3IfInstIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "Interface instance over which the neighbor 
                can be reached. This ID has local link 
                significance only." 
            ::= { ospfv3NbrEntry 2 } 
 
    ospfv3NbrRtrId OBJECT-TYPE 
            SYNTAX          Ospfv3RouterIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
               "A 32-bit integer uniquely identifying the neighboring 
               router in the Autonomous System." 
            ::= { ospfv3NbrEntry 3 } 
 
    ospfv3NbrAddressType OBJECT-TYPE 
            SYNTAX          InetAddressType 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The address type of ospfv3NbrAddress. Only IPv6 
                addresses without zone index are expected." 
            ::= { ospfv3NbrEntry 4 } 
 
    ospfv3NbrAddress OBJECT-TYPE 
            SYNTAX          InetAddress (SIZE (16)) 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The IPv6 address of the neighbor associated with 
                the local link." 
            ::= { ospfv3NbrEntry 5 } 
 
    ospfv3NbrOptions OBJECT-TYPE 
            SYNTAX          Integer32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "A Bit Mask corresponding to the neighbor's 
                options field." 
            REFERENCE 
                "OSPF Version 3, Appendix A.2 the Options field" 
            ::= { ospfv3NbrEntry 6 } 
 
    ospfv3NbrPriority OBJECT-TYPE 
            SYNTAX          DesignatedRouterPriority 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The priority of this neighbor in the designated 
                router election algorithm. The value 0 signifies 
                that the neighbor is not eligible to become the 
                designated router on this particular network." 
            ::= { ospfv3NbrEntry 7 } 
 
    ospfv3NbrState OBJECT-TYPE 
            SYNTAX          INTEGER { 
                            down(1), 
                            attempt(2), 
                            init(3), 
                            twoWay(4), 
                            exchangeStart(5), 
                            exchange(6), 
                            loading(7), 
                            full(8) 
                            } 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The State of the relationship with this 
                Neighbor." 
            REFERENCE 
                "OSPF Version 2, Section 10.1 Neighbor States" 
            ::= { ospfv3NbrEntry 8 } 
 
    ospfv3NbrEvents OBJECT-TYPE 
            SYNTAX          Counter32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The number of times this neighbor relationship 
                has changed state, or an error has occurred." 
            ::= { ospfv3NbrEntry 9 } 
 
    ospfv3NbrLsRetransQLen OBJECT-TYPE 
            SYNTAX          Gauge32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The current length of the retransmission 
                queue." 
            ::= { ospfv3NbrEntry 10 } 
 
    ospfv3NbrHelloSuppressed OBJECT-TYPE 
            SYNTAX          TruthValue 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "Indicates whether Hellos are being suppressed 
                to the neighbor" 
            ::= { ospfv3NbrEntry 11 } 
 
    ospfv3NbrIfId OBJECT-TYPE 
            SYNTAX          InterfaceIndex 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The interface ID that the neighbor advertises 
                in its Hello Packets on this link, that is, the 
                neighbor's local interface index." 
            ::= { ospfv3NbrEntry 12 } 
 
    ospfv3NbrRestartHelperStatus OBJECT-TYPE  
           SYNTAX       INTEGER { notHelping (1),  
                                  helping (2)  
                                }  
           MAX-ACCESS   read-only  
           STATUS       current  
           DESCRIPTION  
              "Indicates whether the router is acting  
              as a Graceful restart helper for the neighbor."  
              ::= { ospfv3NbrEntry 13 }  
        
    ospfv3NbrRestartHelperAge OBJECT-TYPE  
           SYNTAX       Ospfv3UpToRefreshIntervalTc 
           UNITS        "seconds"  
           MAX-ACCESS   read-only  
           STATUS       current  
           DESCRIPTION  
              "Remaining time in current OSPF Graceful restart  
              interval, if the router is acting as a restart  
              helper for the neighbor."  
           ::= { ospfv3NbrEntry 14 }  
        
    ospfv3NbrRestartHelperExitRc OBJECT-TYPE  
           SYNTAX       INTEGER { none (1), 
                                  inProgress (2),  
                                  completed (3),  
                                  timedOut (4),  
                                  topologyChanged (5) 
                                }  
           MAX-ACCESS   read-only  
           STATUS       current  
           DESCRIPTION  
              "Describes the outcome of the last attempt at acting  
              as a Graceful restart helper for the neighbor. 
    
              none:............no restart has yet been attempted. 
              inProgress:......a restart attempt is currently underway. 
              completed:.......the last restart completed successfully. 
              timedOut:........the last restart timed out. 
              topologyChanged:.the last restart was aborted due to 
                               a topology change."  
        ::= { ospfv3NbrEntry 15 } 
 
 
    -- OSPFv3 Configured Neighbor Table 
 
    -- The OSPFv3 Configured Neighbor Table describes all configured 
    -- neighbors and neighbors dynamically discovered by 
    -- lower-level protocols such as Inverse Neighbor Discovery. 
 
    ospfv3CfgNbrTable OBJECT-TYPE 
            SYNTAX          SEQUENCE OF Ospfv3CfgNbrEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "A table of configured non-virtual neighbor 
                information and neighbors dynamically discovered 
                by lower-level protocols such as Inverse Neighbor 
                Discovery." 
            REFERENCE 
                "OSPF Version 2, Section 10 The Neighbor Data 
                Structure" 
            ::= { ospfv3Objects 10 } 
 
    ospfv3CfgNbrEntry OBJECT-TYPE 
            SYNTAX          Ospfv3CfgNbrEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The information regarding a single configured 
                neighbor or neighbor discovered by lower-level 
                protocols such as Inverse Neighbor Discovery." 
            REFERENCE 
                "OSPF Version 2, Section 10 The Neighbor Data 
                Structure" 
            INDEX           { ospfv3CfgNbrIfIndex, 
                              ospfv3CfgNbrIfInstId, 
                              ospfv3CfgNbrAddressType, 
                              ospfv3CfgNbrAddress } 
            ::= { ospfv3CfgNbrTable 1 } 
 
    Ospfv3CfgNbrEntry ::= SEQUENCE { 
            ospfv3CfgNbrIfIndex 
                    InterfaceIndex, 
            ospfv3CfgNbrIfInstId 
                    Ospfv3IfInstIdTc, 
            ospfv3CfgNbrAddressType 
                    InetAddressType, 
            ospfv3CfgNbrAddress 
                    InetAddress, 
            ospfv3CfgNbrPriority 
                    DesignatedRouterPriority, 
            ospfv3CfgNbrRtrId 
                    Ospfv3RouterIdTc, 
            ospfv3CfgNbrState 
                    INTEGER, 
            ospfv3CfgNbrStorageType 
                    StorageType, 
            ospfv3CfgNbrStatus 
                    RowStatus 
            } 
 
    ospfv3CfgNbrIfIndex OBJECT-TYPE 
            SYNTAX          InterfaceIndex 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The local link ID of the link over which the 
                 neighbor can be reached." 
            ::= { ospfv3CfgNbrEntry 1 } 
 
    ospfv3CfgNbrIfInstId OBJECT-TYPE 
            SYNTAX          Ospfv3IfInstIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "Interface instance over which the neighbor 
                can be reached. This ID has local link 
                significance only." 
            ::= { ospfv3CfgNbrEntry 2 } 
 
    ospfv3CfgNbrAddressType OBJECT-TYPE 
            SYNTAX          InetAddressType 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The address type of ospfv3NbrAddress. Only IPv6 
                addresses without zone index are expected." 
            ::= { ospfv3CfgNbrEntry 3 } 
 
    ospfv3CfgNbrAddress OBJECT-TYPE 
            SYNTAX          InetAddress (SIZE (16)) 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The IPv6 address of the neighbor associated with 
                the local link." 
            ::= { ospfv3CfgNbrEntry 4 } 
 
    ospfv3CfgNbrPriority OBJECT-TYPE 
            SYNTAX          DesignatedRouterPriority 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The priority of this neighbor in the designated 
                router election algorithm. The value 0 signifies 
                that the neighbor is not eligible to become the 
                designated router on this particular network." 
            DEFVAL          { 1 } 
            ::= { ospfv3CfgNbrEntry 5 } 
 
    ospfv3CfgNbrRtrId OBJECT-TYPE 
            SYNTAX          Ospfv3RouterIdTc 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "A 32-bit integer uniquely identifying the neighboring 
                router in the Autonomous System. A value of 0 
                is returned until a Hello is received 
                from the configured neighbor." 
            ::= { ospfv3CfgNbrEntry 6 } 
 
    ospfv3CfgNbrState OBJECT-TYPE 
            SYNTAX          INTEGER { 
                            down(1), 
                            attempt(2), 
                            init(3), 
                            twoWay(4), 
                            exchangeStart(5), 
                            exchange(6), 
                            loading(7), 
                            full(8) 
                            } 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The State of the relationship with this Neighbor." 
            REFERENCE 
                "OSPF Version 2, Section 10.1 Neighbor States" 
            ::= { ospfv3CfgNbrEntry 7 } 
 
    ospfv3CfgNbrStorageType OBJECT-TYPE 
            SYNTAX          StorageType 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "The storage type for this conceptual row. 
                Conceptual rows having the value 'permanent' need not 
                allow write-access to any columnar objects in the row. 
                Manually configured entries will have a storage type 
                of nonVolatile while entries dynamically created as a 
                result of a lower-level protocol such as Inverse 
                Neighbor Discovery will have a storage type of 
                volatile." 
            DEFVAL          { nonVolatile } 
            ::= { ospfv3CfgNbrEntry 8 } 
 
    ospfv3CfgNbrStatus OBJECT-TYPE 
            SYNTAX          RowStatus 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "This variable controls the status of the entry. 
                The use of RowStatus is covered in more detail 
                in [6]." 
            ::= { ospfv3CfgNbrEntry 9 } 
 
    -- OSPFv3 Virtual Neighbor Table 
 
    -- This table describes all virtual neighbors. 
    -- Since Virtual Links are configured in the 
    -- virtual interface table, this table is read-only. 
 
    ospfv3VirtNbrTable OBJECT-TYPE 
            SYNTAX          SEQUENCE OF Ospfv3VirtNbrEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "A table of virtual neighbor information." 
            REFERENCE 
                "OSPF Version 2, Section 15 Virtual Links" 
            ::= { ospfv3Objects 11 } 
 
    ospfv3VirtNbrEntry OBJECT-TYPE 
            SYNTAX          Ospfv3VirtNbrEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "Virtual neighbor information." 
            INDEX           { ospfv3VirtNbrArea, 
                              ospfv3VirtNbrRtrId } 
            ::= { ospfv3VirtNbrTable 1 } 
 
    Ospfv3VirtNbrEntry ::= SEQUENCE { 
            ospfv3VirtNbrArea 
                    Ospfv3AreaIdTc, 
            ospfv3VirtNbrRtrId 
                    Ospfv3RouterIdTc, 
            ospfv3VirtNbrIfIndex 
                    InterfaceIndex, 
            ospfv3VirtNbrIfInstId 
                    Ospfv3IfInstIdTc, 
            ospfv3VirtNbrAddressType 
                    InetAddressType, 
            ospfv3VirtNbrAddress 
                    InetAddress, 
            ospfv3VirtNbrOptions 
                    Integer32, 
            ospfv3VirtNbrState 
                    INTEGER, 
            ospfv3VirtNbrEvents 
                    Counter32, 
            ospfv3VirtNbrLsRetransQLen 
                    Gauge32, 
            ospfv3VirtNbrHelloSuppressed 
                    TruthValue, 
            ospfv3VirtNbrIfId 
                    InterfaceIndex, 
            ospfv3VirtNbrRestartHelperStatus  
                    INTEGER,  
            ospfv3VirtNbrRestartHelperAge  
                    Ospfv3UpToRefreshIntervalTc,  
            ospfv3VirtNbrRestartHelperExitRc  
                    INTEGER 
            } 
 
    ospfv3VirtNbrArea OBJECT-TYPE 
            SYNTAX          Ospfv3AreaIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The Transit Area Identifier." 
            ::= { ospfv3VirtNbrEntry 1 } 
 
    ospfv3VirtNbrRtrId OBJECT-TYPE 
            SYNTAX          Ospfv3RouterIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "A 32-bit integer uniquely identifying the 
                neighboring router in the Autonomous System." 
            ::= { ospfv3VirtNbrEntry 2 } 
 
    ospfv3VirtNbrIfIndex OBJECT-TYPE 
            SYNTAX          InterfaceIndex 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The local interface ID for the virtual link over 
                which the neighbor can be reached." 
            ::= { ospfv3VirtNbrEntry 3 } 
 
    ospfv3VirtNbrIfInstId OBJECT-TYPE 
            SYNTAX          Ospfv3IfInstIdTc 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The interface instance for the virtual link over 
                which the neighbor can be reached." 
            ::= { ospfv3VirtNbrEntry 4 } 
 
    ospfv3VirtNbrAddressType OBJECT-TYPE 
            SYNTAX          InetAddressType 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The address type of ospfv3VirtNbrAddress. Only IPv6 
                addresses without zone index are expected." 
            ::= { ospfv3VirtNbrEntry 5 } 
 
    ospfv3VirtNbrAddress OBJECT-TYPE 
            SYNTAX          InetAddress (SIZE (16)) 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The IPv6 address advertised by this Virtual Neighbor. 
                It must be a Global scope address." 
            ::= { ospfv3VirtNbrEntry 6 } 
 
    ospfv3VirtNbrOptions OBJECT-TYPE 
            SYNTAX          Integer32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "A Bit Mask corresponding to the neighbor's options 
                field." 
            REFERENCE 
                "OSPF Version 3, Appendix A.2 the Options field" 
            ::= { ospfv3VirtNbrEntry 7 } 
 
    ospfv3VirtNbrState OBJECT-TYPE 
            SYNTAX          INTEGER { 
                            down(1), 
                            attempt(2), 
                            init(3), 
                            twoWay(4), 
                            exchangeStart(5), 
                            exchange(6), 
                            loading(7), 
                            full(8) 
                            } 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The state of the Virtual Neighbor Relationship." 
            ::= { ospfv3VirtNbrEntry 8 } 
 
    ospfv3VirtNbrEvents OBJECT-TYPE 
            SYNTAX          Counter32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The number of times this virtual link has 
                changed its state, or an error has occurred." 
            ::= { ospfv3VirtNbrEntry 9 } 
 
    ospfv3VirtNbrLsRetransQLen OBJECT-TYPE 
            SYNTAX          Gauge32 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The current length of the retransmission 
                queue." 
            ::= { ospfv3VirtNbrEntry 10 } 
 
    ospfv3VirtNbrHelloSuppressed OBJECT-TYPE 
            SYNTAX          TruthValue 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "Indicates whether Hellos are being suppressed 
                to the neighbor" 
            ::= { ospfv3VirtNbrEntry 11 } 
 
    ospfv3VirtNbrIfId OBJECT-TYPE 
            SYNTAX          InterfaceIndex 
            MAX-ACCESS      read-only 
            STATUS          current 
            DESCRIPTION 
                "The interface ID that the neighbor advertises 
                in its Hello Packets on this virtual link, that is, 
                the neighbor's local interface ID." 
            ::= { ospfv3VirtNbrEntry 12 } 
 
   ospfv3VirtNbrRestartHelperStatus OBJECT-TYPE  
           SYNTAX       INTEGER { notHelping (1),  
                                  helping (2)  
                                }  
           MAX-ACCESS   read-only  
           STATUS       current  
           DESCRIPTION  
              "Indicates whether the router is acting  
              as a Graceful restart helper for the neighbor."  
              ::= { ospfv3VirtNbrEntry 13 }  
        
    ospfv3VirtNbrRestartHelperAge OBJECT-TYPE  
           SYNTAX       Ospfv3UpToRefreshIntervalTc 
           UNITS        "seconds"  
           MAX-ACCESS   read-only  
           STATUS       current  
           DESCRIPTION  
              "Remaining time in current OSPF Graceful restart  
              interval, if the router is acting as a restart  
              helper for the neighbor."  
           ::= { ospfv3VirtNbrEntry 14 }  
        
    ospfv3VirtNbrRestartHelperExitRc OBJECT-TYPE  
           SYNTAX       INTEGER { none (1),  
                                  inProgress (2),  
                                  completed (3),  
                                  timedOut (4),  
                                  topologyChanged (5)  
                                }  
           MAX-ACCESS   read-only  
           STATUS       current  
           DESCRIPTION  
              "Describes the outcome of the last attempt at acting  
               as a Graceful restart helper for the neighbor. 
    
              none:............no restart has yet been attempted. 
              inProgress:......a restart attempt is currently underway. 
              completed:.......the last restart completed successfully. 
              timedOut:........the last restart timed out. 
              topologyChanged:.the last restart was aborted due to 
                               a topology change."  
        ::= { ospfv3VirtNbrEntry 15 } 
 
 
    -- 
    -- The OSPFv3 Area Aggregate Table 
    -- 
 
    ospfv3AreaAggregateTable OBJECT-TYPE 
            SYNTAX          SEQUENCE OF Ospfv3AreaAggregateEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "A range of IPv6 prefixes specified by a 
                prefix/prefix length pair. Note that if 
                ranges are configured such that one range 
                subsumes another range the most specific 
                match is the preferred one." 
            ::= { ospfv3Objects 12 } 
 
    ospfv3AreaAggregateEntry OBJECT-TYPE 
            SYNTAX          Ospfv3AreaAggregateEntry 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "A range of IPv6 prefixes specified by a 
                prefix/prefix length  pair. Note that if 
                ranges are configured such that one range 
                subsumes another range the most specific match is 
                the preferred one." 
            REFERENCE 
                "OSPF Version 2, Appendix C.2  Area parameters" 
            INDEX           { ospfv3AreaAggregateAreaID,  
                              ospfv3AreaAggregateAreaLsdbType, 
                              ospfv3AreaAggregatePrefixType, 
                              ospfv3AreaAggregatePrefix, 
                              ospfv3AreaAggregatePrefixLength } 
            ::= { ospfv3AreaAggregateTable 1 } 
 
    Ospfv3AreaAggregateEntry ::= SEQUENCE { 
            ospfv3AreaAggregateAreaID 
                    Ospfv3AreaIdTc, 
            ospfv3AreaAggregateAreaLsdbType 
                    INTEGER, 
            ospfv3AreaAggregatePrefixType 
                    InetAddressType, 
            ospfv3AreaAggregatePrefix 
                    InetAddress, 
            ospfv3AreaAggregatePrefixLength 
                    InetAddressPrefixLength, 
            ospfv3AreaAggregateStatus 
                    RowStatus, 
            ospfv3AreaAggregateEffect 
                    INTEGER, 
            ospfv3AreaAggregateRouteTag 
                    Integer32
--                    INTEGER 
            } 
 
    ospfv3AreaAggregateAreaID OBJECT-TYPE 
            SYNTAX          Ospfv3AreaIdTc 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The Area the Address Aggregate is to be found 
                within." 
            REFERENCE 
                "OSPF Version 2, Appendix C.2 Area parameters" 
            ::= { ospfv3AreaAggregateEntry 1 } 
 
    ospfv3AreaAggregateAreaLsdbType OBJECT-TYPE 
            SYNTAX          INTEGER { 
                            interAreaPrefixLsa(8195), -- 0x2003 
                            nssaExternalLsa(8199)     -- 0x2007 
                            } 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The type of the Address Aggregate.  This field 
                specifies  the  Area Lsdb type that this Address 
                Aggregate applies to." 
            REFERENCE 
                "OSPF Version 2, Appendix A.4.1 The Link State 
                Advertisement header" 
            ::= { ospfv3AreaAggregateEntry 2 } 
 
    ospfv3AreaAggregatePrefixType OBJECT-TYPE 
            SYNTAX          InetAddressType 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The prefix type of ospfv3AreaAggregatePrefix. Only 
                IPv6 addresses are expected." 
            ::= { ospfv3AreaAggregateEntry 4 } 
 
    ospfv3AreaAggregatePrefix OBJECT-TYPE 
            SYNTAX          InetAddress (SIZE (0..16)) 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The IPv6 Prefix." 
            REFERENCE 
                "OSPF Version 2, Appendix C.2 Area parameters" 
            ::= { ospfv3AreaAggregateEntry 5 } 
 
    ospfv3AreaAggregatePrefixLength OBJECT-TYPE 
            SYNTAX          InetAddressPrefixLength (3..128) 
            UNITS           "bits" 
            MAX-ACCESS      not-accessible 
            STATUS          current 
            DESCRIPTION 
                "The length of the prefix (in bits). A prefix can 
                not be shorter than 3 bits." 
            REFERENCE 
                "OSPF Version 2, Appendix C.2 Area parameters" 
            ::= { ospfv3AreaAggregateEntry 6 } 
 
    ospfv3AreaAggregateStatus OBJECT-TYPE 
            SYNTAX          RowStatus 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "This variable controls the status of the entry 
                The use of RowStatus is covered in more detail 
                in [6]." 
            ::= { ospfv3AreaAggregateEntry 7 } 
 
    ospfv3AreaAggregateEffect OBJECT-TYPE 
            SYNTAX          INTEGER { 
                            advertiseMatching(1), 
                            doNotAdvertiseMatching(2) 
                            } 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "Prefixes subsumed by ranges either trigger the 
                advertisement of the indicated aggregate 
                (advertiseMatching), or result in the prefix not 
                being advertised at all outside the area." 
            DEFVAL          { advertiseMatching } 
            ::= { ospfv3AreaAggregateEntry 8 } 
 
    ospfv3AreaAggregateRouteTag OBJECT-TYPE 
            SYNTAX          Integer32 
            MAX-ACCESS      read-create 
            STATUS          current 
            DESCRIPTION 
                "This tag is advertised only in the summarized 
                 As-External LSA when summarizing from NSSA-LSAÆs to  
                 AS-External-LSAÆs." 
            DEFVAL         { 0 } 
            ::= { ospfv3AreaAggregateEntry 9 } 
             
    
    -- conformance information 
 
    ospfv3Groups      OBJECT IDENTIFIER ::= { ospfv3Conformance 1 } 
    ospfv3Compliances OBJECT IDENTIFIER ::= { ospfv3Conformance 2 } 
 
    -- compliance statements 
 
    ospfv3Compliance MODULE-COMPLIANCE 
            STATUS          current 
            DESCRIPTION     "The compliance statement" 
            MODULE          -- this module 
            MANDATORY-GROUPS { 
                            ospfv3BasicGroup, 
                            ospfv3AreaGroup, 
                            ospfv3IfGroup, 
                            ospfv3VirtIfGroup, 
                            ospfv3NbrGroup, 
                            ospfv3CfgNbrGroup, 
                            ospfv3VirtNbrGroup, 
                            ospfv3AreaAggregateGroup 
                            } 
 
            GROUP           ospfv3AsLsdbGroup 
            DESCRIPTION 
                "This group is required for OSPFv3 systems that 
                display their AS-scope link state database." 
 
            GROUP           ospfv3AreaLsdbGroup 
            DESCRIPTION 
                "This group is required for OSPFv3 systems that 
                display their Area-scope link state database." 
 
            GROUP           ospfv3LinkLsdbGroup 
            DESCRIPTION 
                "This group is required for OSPFv3 systems that 
                display their Link-scope link state database." 
 
            GROUP           ospfv3HostGroup 
            DESCRIPTION 
                "This group is required for OSPFv3 systems that 
                support attached hosts." 
 
            OBJECT          ospfv3NbrAddressType 
--            SYNTAX          InetAddressType { ipv6(2) } 
            DESCRIPTION 
                "An implementation is only required to support IPv6 
                address without zone index." 
 
            OBJECT          ospfv3VirtNbrAddressType 
--           SYNTAX          InetAddressType { ipv6(2) } 
            DESCRIPTION 
                "An implementation is only required to support IPv6 
                address without zone index." 
 
            ::= { ospfv3Compliances 1 } 
 
    -- units of conformance 
 
    ospfv3BasicGroup OBJECT-GROUP 
            OBJECTS         { 
                            ospfv3RouterId, 
                            ospfv3AdminStat, 
                            ospfv3VersionNumber, 
                            ospfv3AreaBdrRtrStatus, 
                            ospfv3ASBdrRtrStatus, 
                            ospfv3AsScopeLsaCount, 
                            ospfv3AsScopeLsaCksumSum, 
                            ospfv3OriginateNewLsas, 
                            ospfv3RxNewLsas, 
                            ospfv3ExtLsaCount, 
                            ospfv3ExtAreaLsdbLimit, 
                            ospfv3MulticastExtensions, 
                            ospfv3ExitOverflowInterval, 
                            ospfv3DemandExtensions, 
                            ospfv3ReferenceBandwidth, 
                            ospfv3RestartSupport, 
                            ospfv3RestartInterval, 
                            ospfv3RestartStatus, 
                            ospfv3RestartAge, 
                            ospfv3RestartExitRc 
                            } 
            STATUS          current 
            DESCRIPTION 
                "These objects are required for OSPFv3 systems." 
            ::= { ospfv3Groups 1 } 
 
 
    ospfv3AreaGroup OBJECT-GROUP 
            OBJECTS         {                       
                            ospfv3ImportAsExtern, 
                            ospfv3AreaSpfRuns, 
                            ospfv3AreaBdrRtrCount, 
                            ospfv3AreaAsBdrRtrCount, 
                            ospfv3AreaScopeLsaCount, 
                            ospfv3AreaScopeLsaCksumSum, 
                            ospfv3AreaSummary, 
                            ospfv3AreaStatus, 
                            ospfv3StubMetric, 
                            ospfv3AreaNssaTranslatorRole, 
                            ospfv3AreaNssaTranslatorState, 
                            ospfv3AreaNssaTranslatorStabInt, 
                            ospfv3AreaNssaTranslatorEvents, 
                            ospfv3AreaStubMetricType 
                            } 
            STATUS          current 
            DESCRIPTION 
                "These objects are required for OSPFv3 systems 
                supporting areas." 
            ::= { ospfv3Groups 2 } 
 
    ospfv3AsLsdbGroup OBJECT-GROUP 
            OBJECTS         { 
                            ospfv3AsLsdbSequence, 
                            ospfv3AsLsdbAge, 
                            ospfv3AsLsdbChecksum, 
                            ospfv3AsLsdbAdvertisement, 
                            ospfv3AsLsdbTypeKnown 
                            } 
            STATUS          current 
            DESCRIPTION 
                "These objects are required for OSPFv3 systems 
                that display their AS-scope link state database." 
            ::= { ospfv3Groups 3 } 
 
    ospfv3AreaLsdbGroup OBJECT-GROUP 
            OBJECTS         { 
                            ospfv3AreaLsdbSequence, 
                            ospfv3AreaLsdbAge, 
                            ospfv3AreaLsdbChecksum, 
                            ospfv3AreaLsdbAdvertisement, 
                            ospfv3AreaLsdbTypeKnown 
                            } 
            STATUS          current 
            DESCRIPTION 
                "These objects are required for OSPFv3 systems 
                that display their Area-scope link state database." 
            ::= { ospfv3Groups 4 } 
 
    ospfv3LinkLsdbGroup OBJECT-GROUP 
            OBJECTS         { 
                            ospfv3LinkLsdbSequence, 
                            ospfv3LinkLsdbAge, 
                            ospfv3LinkLsdbChecksum, 
                            ospfv3LinkLsdbAdvertisement, 
                            ospfv3LinkLsdbTypeKnown 
                            } 
            STATUS          current 
            DESCRIPTION 
                "These objects are required for OSPFv3 systems 
                that display their Link-scope link state database." 
            ::= { ospfv3Groups 5 } 
 
    ospfv3HostGroup OBJECT-GROUP 
            OBJECTS         { 
                            ospfv3HostMetric, 
                            ospfv3HostStatus, 
                            ospfv3HostAreaID 
                            } 
            STATUS          current 
            DESCRIPTION 
                "These objects are required for OSPFv3 systems 
                that support attached hosts." 
            ::= { ospfv3Groups 6 } 
 
    ospfv3IfGroup OBJECT-GROUP 
            OBJECTS         { 
                            ospfv3IfAreaId, 
                            ospfv3IfType, 
                            ospfv3IfAdminStat, 
                            ospfv3IfRtrPriority, 
                            ospfv3IfTransitDelay, 
                            ospfv3IfRetransInterval, 
                            ospfv3IfHelloInterval, 
                            ospfv3IfRtrDeadInterval, 
                            ospfv3IfPollInterval, 
                            ospfv3IfState, 
                            ospfv3IfDesignatedRouter, 
                            ospfv3IfBackupDesignatedRouter, 
                            ospfv3IfEvents, 
                            ospfv3IfStatus, 
                            ospfv3IfMulticastForwarding, 
                            ospfv3IfDemand, 
                            ospfv3IfMetricValue, 
                            ospfv3IfLinkScopeLsaCount, 
                            ospfv3IfLinkLsaCksumSum, 
                            ospfv3IfDemandNbrProbe, 
                            ospfv3IfDemandNbrProbeRetxLimit,  
                            ospfv3IfDemandNbrProbeInterval  
                            } 
            STATUS          current 
            DESCRIPTION 
                "These interface objects are required for  
                OSPFv3 systems." 
            ::= { ospfv3Groups 7 } 
 
    ospfv3VirtIfGroup OBJECT-GROUP 
            OBJECTS         { 
                            ospfv3VirtIfIndex, 
                            ospfv3VirtIfInstId, 
                            ospfv3VirtIfTransitDelay, 
                            ospfv3VirtIfRetransInterval, 
                            ospfv3VirtIfHelloInterval, 
                            ospfv3VirtIfRtrDeadInterval, 
                            ospfv3VirtIfState, 
                            ospfv3VirtIfEvents, 
                            ospfv3VirtIfStatus, 
                            ospfv3VirtIfLinkScopeLsaCount, 
                            ospfv3VirtIfLinkLsaCksumSum  
                            } 
            STATUS          current 
            DESCRIPTION 
                "These virtual interface objects are required for  
                OSPFv3 systems." 
            ::= { ospfv3Groups 8 } 
 
    ospfv3NbrGroup OBJECT-GROUP 
            OBJECTS         { 
                            ospfv3NbrAddressType, 
                            ospfv3NbrAddress, 
                            ospfv3NbrOptions, 
                            ospfv3NbrPriority, 
                            ospfv3NbrState, 
                            ospfv3NbrEvents, 
                            ospfv3NbrLsRetransQLen, 
                            ospfv3NbrHelloSuppressed, 
                            ospfv3NbrIfId, 
                            ospfv3NbrRestartHelperStatus,  
                            ospfv3NbrRestartHelperAge,  
                            ospfv3NbrRestartHelperExitRc 
                            } 
            STATUS          current 
            DESCRIPTION 
                "These neighbor objects are required for 
                OSPFv3 systems." 
            ::= { ospfv3Groups 9 } 
 
    ospfv3CfgNbrGroup OBJECT-GROUP 
            OBJECTS         { 
                            ospfv3CfgNbrPriority, 
                            ospfv3CfgNbrRtrId, 
                            ospfv3CfgNbrState, 
                            ospfv3CfgNbrStorageType, 
                            ospfv3CfgNbrStatus 
                            } 
            STATUS          current 
            DESCRIPTION 
                "These Configured neighbor objects are required for 
                OSPFv3 systems." 
            ::= { ospfv3Groups 10 } 
 
    ospfv3VirtNbrGroup OBJECT-GROUP 
            OBJECTS         { 
                            ospfv3VirtNbrIfIndex, 
                            ospfv3VirtNbrIfInstId, 
                            ospfv3VirtNbrAddressType,  
                            ospfv3VirtNbrAddress, 
                            ospfv3VirtNbrOptions, 
                            ospfv3VirtNbrState, 
                            ospfv3VirtNbrEvents, 
                            ospfv3VirtNbrLsRetransQLen, 
                            ospfv3VirtNbrHelloSuppressed, 
                            ospfv3VirtNbrIfId, 
                            ospfv3VirtNbrRestartHelperStatus,  
                            ospfv3VirtNbrRestartHelperAge,  
                            ospfv3VirtNbrRestartHelperExitRc 
                            } 
            STATUS          current 
            DESCRIPTION 
                "These virtual neighbor objects are required for 
                OSPFv3 systems." 
            ::= { ospfv3Groups 11 } 
 
    ospfv3AreaAggregateGroup OBJECT-GROUP 
            OBJECTS         { 
                            ospfv3AreaAggregateStatus, 
                            ospfv3AreaAggregateEffect, 
                            ospfv3AreaAggregateRouteTag 
                            } 
            STATUS          current 
            DESCRIPTION 
                "These area aggregate objects are required for 
                OSPFv3 systems." 
            ::= { ospfv3Groups 12 } 
 
    END 
