--  MPLS Static Fast Reroute Management Information Base Using SMIv2
--                                
--                   draft-alcatel-static-frr-mib-00.txt
ALCATEL-STATIC-FRR-MIB DEFINITIONS ::= BEGIN

IMPORTS
        MODULE-IDENTITY, OBJECT-TYPE,
        Integer32,
        Unsigned32, IpAddress                  FROM SNMPv2-SMI

        softentIND1MplsFrr                     FROM ALCATEL-IND1-BASE

        DisplayString, RowStatus,
        TruthValue                             FROM SNMPv2-TC
                                                        
	InterfaceIndexOrZero		       FROM IF-MIB	

	InetAddressType,InetAddressIPv4        FROM INET-ADDRESS-MIB

        MplsLabel, MplsObjectOwner             FROM MPLS-LSR-MIB

        TmnxOperState                          FROM TIMETRA-TC-MIB;


alcatelStaticFrrMIBModule MODULE-IDENTITY
        LAST-UPDATED    "0801010000Z"
        ORGANIZATION    "Alcatel-Lucent Inc"
	CONTACT-INFO
	    "Please consult with Customer Service to ensure the most appropriate
	     version of this document is used with the products in question:
 
			Alcatel-Lucent, Enterprise Solutions Division
		       (Formerly Alcatel Internetworking, Incorporated)
			       26801 West Agoura Road
			    Agoura Hills, CA  91301-5122
			      United States Of America
	
	    Telephone:               North America  +1 800 995 2696
				     Latin America  +1 877 919 9526
				     Europe         +31 23 556 0100
				     Asia           +65 394 7933
				     All Other      +1 818 878 4507
	
	    Electronic Mail:         support@ind.alcatel.com
	    World Wide Web:          http://alcatel-lucent.com/wps/portal/enterprise
	    File Transfer Protocol:  ftp://ftp.ind.alcatel.com/pub/products/mibs"

        DESCRIPTION
        "This document is the SNMP MIB module to manage and provision 
        Static FRR extensions for the Alcatel 9x00 device.

        Copyright 2000-2009 Alcatel-Lucent. All rights reserved.
        Reproduction of this document is authorized on the condition that
        the foregoing copyright notice is included.

        This SNMP MIB module (Specification) embodies Alcatel's
        proprietary intellectual property.  Alcatel retains 
        all title and ownership in the Specification, including any 
        revisions.

        Alcatel grants all interested parties a non-exclusive 
        license to use and distribute an unmodified copy of this 
        Specification in connection with management of Alcatel 
        products, and without fee, provided this copyright notice and 
        license appear on all copies.

        This Specification is supplied 'as is', and Alcatel 
        makes no warranty, either express or implied, as to the use, 
        operation, condition, or performance of the Specification."
--
--  Revision History
--
        REVISION        "0902020000Z"   
        DESCRIPTION     "Rev 1.0                28 Mar 2009 00:00
                         1.0 release of the ALCATEL-STATIC-FRR-MIB."


        ::= { softentIND1MplsFrr 1 }


--%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
alcatelStaticFrrMIBModuleObjs  OBJECT-IDENTITY
STATUS current
DESCRIPTION
     "Branch for ALU FRR  Managed Objects."
     ::= {alcatelStaticFrrMIBModule 1}

--
-- Protected Static FRR InSegment Table
--

vRtrStaticFrrMplsInSegmentTable  OBJECT-TYPE

   SYNTAX        SEQUENCE OF VRtrStaticFrrMplsInSegmentEntry
   MAX-ACCESS    not-accessible
   STATUS        current
   DESCRIPTION
       "This table contains a collection of incoming
        segments to an LSR."
   ::= { alcatelStaticFrrMIBModuleObjs 1 }

vRtrStaticFrrMplsInSegmentEntry  OBJECT-TYPE
   SYNTAX        VRtrStaticFrrMplsInSegmentEntry
   MAX-ACCESS    not-accessible
   STATUS        current
   DESCRIPTION
       "An entry in this table represents one incoming
        segment.  An entry can be created by a network
            administrator or an SNMP agent. The creator of the entry is 
        denoted by vRtrStaticFrrMplsInSegmentOwner.  An entry in this table is
        indexed by the ifIndex of the incoming interface and
        the (top) label."
   INDEX         { vRtrStaticFrrMplsInSegmentIfIndex, vRtrStaticFrrMplsInSegmentLabel }
   ::= { vRtrStaticFrrMplsInSegmentTable 1 }

VRtrStaticFrrMplsInSegmentEntry ::= SEQUENCE {
  vRtrStaticFrrMplsInSegmentIfIndex              InterfaceIndexOrZero,
  vRtrStaticFrrMplsInSegmentLabel                MplsLabel,
  vRtrStaticFrrMplsInSegmentNPop                 Integer32,
  vRtrStaticFrrMplsInSegmentXCIndex              Integer32,
  vRtrStaticFrrMplsInSegmentOwner                MplsObjectOwner,
  vRtrStaticFrrMplsInSegmentRowStatus            RowStatus
}

vRtrStaticFrrMplsInSegmentIfIndex OBJECT-TYPE
   SYNTAX        InterfaceIndexOrZero
   MAX-ACCESS    accessible-for-notify
   STATUS        current
   DESCRIPTION
       "This is a unique index for an entry in the
        StaticFrrMplsInSegmentTable.  This value represents the
        interface index for the incoming MPLS interface.  A
        value of zero represents an incoming label from the
        per-platform label space.  In this case, the
        vRtrStaticFrrMplsInSegmentLabel is interpreted to be an MPLS-type
        label."
   ::= { vRtrStaticFrrMplsInSegmentEntry 1 }

vRtrStaticFrrMplsInSegmentLabel OBJECT-TYPE
   SYNTAX        MplsLabel
   MAX-ACCESS    accessible-for-notify
   STATUS        current
   DESCRIPTION
       "The incoming label for this protected ingress segment."
   ::= { vRtrStaticFrrMplsInSegmentEntry 2 }

vRtrStaticFrrMplsInSegmentNPop OBJECT-TYPE
   SYNTAX        Integer32 (1..2147483647)
   MAX-ACCESS    read-create
   STATUS        current
   DESCRIPTION
       "The number of labels to pop from the incoming
        packet.  Normally only the top label is popped from
        the packet and used for all switching decisions for
        that packet. "
   DEFVAL        { 1 }
   ::= { vRtrStaticFrrMplsInSegmentEntry 3 }

vRtrStaticFrrMplsInSegmentXCIndex OBJECT-TYPE
SYNTAX        Integer32 (0..2147483647)
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION
       "Index into vRtrStaticFrrMplsXCTable which identifies which cross-
        connect entry this segment is part of.  A value of
        zero indicates that this entry is not referred to by
        any cross-connect entry.  When a cross-connect entry
        is created which this in-segment is a part of, this
        object is automatically updated to reflect the value
        of vRtrStaticFrrMplsXCIndex of that cross-connect entry."
   DEFVAL        { 0 }
   ::= { vRtrStaticFrrMplsInSegmentEntry 4 }
   
vRtrStaticFrrMplsInSegmentOwner OBJECT-TYPE
   SYNTAX        MplsObjectOwner
   MAX-ACCESS    read-create
   STATUS        current
   DESCRIPTION
       "Denotes the entity that created and is responsible
        for managing this segment."
   DEFVAL { unknown }
   ::= { vRtrStaticFrrMplsInSegmentEntry 5 }

vRtrStaticFrrMplsInSegmentRowStatus OBJECT-TYPE
   SYNTAX        RowStatus
   MAX-ACCESS    read-create
   STATUS        current
   DESCRIPTION
       "This variable is used to create, modify, and/or
        delete a row in this table."
   ::= { vRtrStaticFrrMplsInSegmentEntry 6 }
   
-- End of vRtrStaticFrrMplsInSegmentTable

--
-- Protecting Static FRR Out-segment table
--

vRtrStaticFrrMplsOutSegmentIndexNext OBJECT-TYPE
   SYNTAX        Integer32 (0..2147483647)
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION
       "This object contains the next appropriate value to
        be used for vRtrStaticFrrMplsOutSegmentIndex when creating
        entries in the vRtrStaticFrrMplsOutSegmentTable.  If the number
        of unassigned entries is exhausted, this object will
        take on the value of 0.  To obtain the
        vRtrStaticFrrMplsOutSegmentIndex value for a new entry, the
        manager must first issue a management protocol
        retrieval operation to obtain the current value of
        this object.  The agent should modify the value to
        reflect the next unassigned index after each
        retrieval operation.  After a manager retrieves a
        value the agent will determine through its local
        policy when this index value will be made available
        for reuse."
   ::= { alcatelStaticFrrMIBModuleObjs 2 }


vRtrStaticFrrMplsOutSegmentTable  OBJECT-TYPE
   SYNTAX        SEQUENCE OF StaticFrrMplsOutSegmentEntry
   MAX-ACCESS    not-accessible
   STATUS        current
   DESCRIPTION
       "This table contains a representation of the outgoing
        segments from an LSR."
   ::= { alcatelStaticFrrMIBModuleObjs 3 }

vRtrStaticFrrMplsOutSegmentEntry  OBJECT-TYPE
   SYNTAX        StaticFrrMplsOutSegmentEntry
   MAX-ACCESS    not-accessible
   STATUS        current
   DESCRIPTION
       "An entry in this table represents one outgoing
        segment.  An entry can be created by a network
             administrator or an SNMP agent.  The object 
        vRtrStaticFrrMplsOutSegmentOwner indicates
        the creator of this entry."
   INDEX         { vRtrStaticFrrMplsOutSegmentIndex }
   ::= { vRtrStaticFrrMplsOutSegmentTable 1 }

StaticFrrMplsOutSegmentEntry ::= SEQUENCE {
  vRtrStaticFrrMplsOutSegmentIndex                Integer32,
  vRtrStaticFrrMplsOutSegmentIfIndex              InterfaceIndexOrZero,
  vRtrStaticFrrMplsOutSegmentPushTopLabel         TruthValue,
  vRtrStaticFrrMplsOutSegmentTopLabel             MplsLabel,
  vRtrStaticFrrMplsOutSegmentNextHopIpAddrType    InetAddressType,
--  vRtrStaticFrrMplsOutSegmentNextHopIpv4Addr      InetAddressIPv4,
  vRtrStaticFrrMplsOutSegmentNextHopIpv4Addr      IpAddress,
  vRtrStaticFrrMplsOutSegmentXCIndex              Integer32,
  vRtrStaticFrrMplsOutSegmentOwner                MplsObjectOwner,
  vRtrStaticFrrMplsOutSegmentRowStatus            RowStatus
}

vRtrStaticFrrMplsOutSegmentIndex                OBJECT-TYPE
   SYNTAX        Integer32 (0..2147483647)
   MAX-ACCESS    accessible-for-notify
   STATUS        current
   DESCRIPTION
       "This value contains a unique index for this row.
        While a value of 0 is not valid as an index for this
        row it can be supplied as a valid value to index
        vRtrStaticFrrMplsXCTable to access entries for 
        which no out-segment has been configured."
   ::= { vRtrStaticFrrMplsOutSegmentEntry  1 }

-- mplsOutSegmentIfIndex can take a value of 0. 
vRtrStaticFrrMplsOutSegmentIfIndex              OBJECT-TYPE
   SYNTAX        InterfaceIndexOrZero
   MAX-ACCESS    read-create
   STATUS        current
   DESCRIPTION
       "This value contains the interface index of the
        outgoing protecting interface."
   ::= { vRtrStaticFrrMplsOutSegmentEntry  2 }

vRtrStaticFrrMplsOutSegmentPushTopLabel       OBJECT-TYPE
   SYNTAX        TruthValue
   MAX-ACCESS    read-create
   STATUS        current
   DESCRIPTION
       "This value indicates whether or not a top label
        should be pushed onto the outgoing packet's label
        stack. "
   ::= { vRtrStaticFrrMplsOutSegmentEntry  3 }

vRtrStaticFrrMplsOutSegmentTopLabel            OBJECT-TYPE
   SYNTAX        MplsLabel
   MAX-ACCESS    read-create
   STATUS        current
   DESCRIPTION
       "If mplsOutSegmentPushTopLabel is true then this
        represents the label that should be pushed onto the
        top of the outgoing packet's label stack."
   ::= { vRtrStaticFrrMplsOutSegmentEntry  4 }

vRtrStaticFrrMplsOutSegmentNextHopIpAddrType      OBJECT-TYPE
   SYNTAX        InetAddressType
   MAX-ACCESS    read-create
   STATUS        current
   DESCRIPTION
       "Indicates whether the protecting next hop address is IPv4 or
        IPv6.  Note that a value of unknown (0) is valid
        only when the outgoing interface is of type point-to-
        point."
   DEFVAL        { unknown }
   ::= { vRtrStaticFrrMplsOutSegmentEntry  5 }

vRtrStaticFrrMplsOutSegmentNextHopIpv4Addr      OBJECT-TYPE
   SYNTAX        IpAddress
   MAX-ACCESS    read-create
   STATUS        current
   DESCRIPTION
       "IPv4 Address of the protecting next hop.  Its value is
        significant only when  mplsOutSegmentNextHopIpAddrType is ipV4 (1),
        otherwise it should return a value of 0."
   ::= { vRtrStaticFrrMplsOutSegmentEntry  6 }

vRtrStaticFrrMplsOutSegmentXCIndex              OBJECT-TYPE
   SYNTAX        Integer32 (0..2147483647)
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION
       "Index into vRtrStaticFrrMplsXCTable which identifies which 
        cross-connect entry this segment is part of.  A value of
        zero indicates that this entry is not referred to by
        any cross-connect entry.  When a cross-connect entry
        is created which this out-segment is a part of, this
        object is automatically updated to reflect the value
        of vRtrStaticFrrMplsXCIndex of that cross-connect entry."
   DEFVAL        { 0 }
   ::= { vRtrStaticFrrMplsOutSegmentEntry  7 }

vRtrStaticFrrMplsOutSegmentOwner               OBJECT-TYPE
   SYNTAX        MplsObjectOwner
   MAX-ACCESS    read-create
   STATUS        current
   DESCRIPTION
       "Denotes the entity which created and is responsible
        for managing this segment."
   DEFVAL { unknown }
   ::= { vRtrStaticFrrMplsOutSegmentEntry  8 }

vRtrStaticFrrMplsOutSegmentRowStatus          OBJECT-TYPE
   SYNTAX        RowStatus
   MAX-ACCESS    read-create
   STATUS        current
   DESCRIPTION
       "For creating, modifying, and deleting this row."
   ::= { vRtrStaticFrrMplsOutSegmentEntry  9 }

-- End of vRtrStaticFrrMplsOutSegmentTable

--
-- Protected Static FRR Cross-connect table.
--

vRtrStaticFrrMplsXCIndexNext OBJECT-TYPE
   SYNTAX        Integer32 (0..2147483647)
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION
       "This object contains an appropriate value to be used
        for vRtrStaticFrrMplsXCIndex when creating entries in the
        vRtrStaticFrrMplsXCTable on a Transit LSR.  The value 0 
        indicates that no unassigned entries are available.  To obtain the
        value of vRtrStaticFrrMplsXCIndex for a new entry in the
        vRtrStaticFrrMplsXCTable, the manager issues a management
        protocol retrieval operation to obtain the current
        value of vRtrStaticFrrMplsXCIndex.  After each retrieval
        operation, the agent should modify the value to
        reflect the next unassigned index.  After a manager
        retrieves a value the agent will determine through
        its local policy when this index value will be made
        available for reuse."
   ::= { alcatelStaticFrrMIBModuleObjs 4 }

vRtrStaticFrrMplsXCTable  OBJECT-TYPE
   SYNTAX        SEQUENCE OF VRtrStaticFrrMplsXCEntry
   MAX-ACCESS    not-accessible
   STATUS        current
   DESCRIPTION
       "This table specifies information for switching
        between LSP segments.  It supports point-to-point
        connections.  mplsLabelStackTable specifies the
        label stack information for a cross-connect LSR and
        is referred to from vRtrStaticFrrMplsXCTable."
   ::= { alcatelStaticFrrMIBModuleObjs 5 }

vRtrStaticFrrMplsXCEntry  OBJECT-TYPE
   SYNTAX        VRtrStaticFrrMplsXCEntry
   MAX-ACCESS    not-accessible
   STATUS        current
   DESCRIPTION
       "A row in this table represents one backup cross-connect
        entry.  The following objects index it:
       
        - cross-connect index vRtrStaticFrrMplsXCIndex that uniquely
          identifies a backup cross-connect entry
        - interface index of the in-segment,  vRtrStaticFrrMplsInSegmentIfIndex
        - incoming label(s), vRtrStaticFrrMplsInSegmentLabel
        - out-segment index, vRtrStaticFrrMplsOutSegmentIndex
       
       Originating LSPs and Terminating LSPs are unsupported in this Table.

       Special labels are not allowed in this Table.
       
        An entry can be created by a network administrator
        or by an SNMP agent."
   INDEX  { vRtrStaticFrrMplsXCIndex, vRtrStaticFrrMplsInSegmentIfIndex,
            vRtrStaticFrrMplsInSegmentLabel,
            vRtrStaticFrrMplsOutSegmentIndex }
      ::= { vRtrStaticFrrMplsXCTable 1 }

VRtrStaticFrrMplsXCEntry ::= SEQUENCE {
      vRtrStaticFrrMplsXCIndex           Integer32,
      vRtrStaticFrrMplsXCOwner           MplsObjectOwner,
      vRtrStaticFrrMplsXCRowStatus       RowStatus,
      vRtrStaticFrrMplsXCAdminStatus     INTEGER,
      vRtrStaticFrrMplsXCOperStatus      INTEGER
   }

vRtrStaticFrrMplsXCIndex OBJECT-TYPE
   SYNTAX        Integer32 (1..2147483647)
   MAX-ACCESS    accessible-for-notify
   STATUS        current
   DESCRIPTION
       "Primary index for the conceptual row identifying 
        a backing cross-connect segment on a transit LSR. "
   ::= { vRtrStaticFrrMplsXCEntry 1 }

vRtrStaticFrrMplsXCOwner OBJECT-TYPE
   SYNTAX    MplsObjectOwner
   MAX-ACCESS    read-create
   STATUS        current
   DESCRIPTION
       "Denotes the entity that created and is responsible
        for managing this cross-connect."
   ::= { vRtrStaticFrrMplsXCEntry 2 }

vRtrStaticFrrMplsXCRowStatus OBJECT-TYPE
   SYNTAX        RowStatus
   MAX-ACCESS    read-create
   STATUS        current
   DESCRIPTION
       "For creating, modifying, and deleting this row."
   ::= { vRtrStaticFrrMplsXCEntry 3 }
   
vRtrStaticFrrMplsXCAdminStatus OBJECT-TYPE
   SYNTAX   INTEGER {
                up(1),  -- ready to pass packets
                down(2)
                }
   MAX-ACCESS    read-create
   STATUS        current
   DESCRIPTION
       "The desired operational status of this backup segment."
   ::= { vRtrStaticFrrMplsXCEntry 4 }

vRtrStaticFrrMplsXCOperStatus OBJECT-TYPE
   SYNTAX   INTEGER {
         up(1),        -- ready to pass packets
         down(2),
         unknown(4)    -- status cannot be determined
                       -- for some reason.
      }
   MAX-ACCESS    read-only
   STATUS        current
   DESCRIPTION
       "The actual operational status of this backup cross-connect."
   ::= { vRtrStaticFrrMplsXCEntry 5 }

-- End of vRtrStaticFrrMplsXCTable

END
--  End of MPLS Static Fast Reroute Management Information Base Using SMIv2
--                                
