--/*
-- *  Copyright (c) 2000-2004 Accton Technology Corp.,  All Rights Reserved.
--    2005 July 14  Add the Mesh table by Loonng, using the mesh material from Ming.
--    This private mib is modified for the WA6102X-2-38 project based on MIPS platform, Sep 21, 2005
-- */

    AP80-PRIVATE-MIB

    DEFINITIONS ::= BEGIN
  
    IMPORTS
        ifIndex                                 FROM RFC1213-MIB
        mgmt,Counter,IpAddress, enterprises     FROM RFC1155-SMI
        Integer32                               FROM SNMPv2-SMI
    ;

    MacAddress  
        ::= OCTET STRING(SIZE (6))
    DisplayString  
        ::= OCTET STRING
    TruthValue  ::=
        INTEGER { false(2), true(1) }
        
--iso(1).org(3).dod(6).internet(1).private(4).enterprises(1).aruba(14823).arubaEnterpriseMibModules(2).arubaAp(3).wlsrOutDoorApMibModules(2)

   aruba			                OBJECT IDENTIFIER ::= { enterprises 14823 }
   arubaEnterpriseMibModules     	OBJECT IDENTIFIER ::= { aruba 2 }
   arubaAp			                OBJECT IDENTIFIER ::= { arubaEnterpriseMibModules 3 }
   wlsrOutDoorApMibModules   		OBJECT IDENTIFIER ::= { arubaAp 2 } 
   enterpriseApSys		   	        OBJECT IDENTIFIER ::= { wlsrOutDoorApMibModules 1 }
   enterpriseApLineMgnt		    	OBJECT IDENTIFIER ::= { wlsrOutDoorApMibModules 2 }
   enterpriseApPortMgnt		    	OBJECT IDENTIFIER ::= { wlsrOutDoorApMibModules 3 }
   enterpriseApFileTransferMgt  	OBJECT IDENTIFIER ::= { wlsrOutDoorApMibModules 4 }
   enterpriseApResetMgt		    	OBJECT IDENTIFIER ::= { wlsrOutDoorApMibModules 5 }
   enterpriseApIpMgt		    	OBJECT IDENTIFIER ::= { wlsrOutDoorApMibModules 6 }
   enterpriseAPdot11		    	OBJECT IDENTIFIER ::= { wlsrOutDoorApMibModules 7 }
   enterpriseApAdmin		    	OBJECT IDENTIFIER ::= { wlsrOutDoorApMibModules 8 }
   enterpriseApVLAN		         	OBJECT IDENTIFIER ::= { wlsrOutDoorApMibModules 9 }
   enterpriseApFilterControl		OBJECT IDENTIFIER ::= { wlsrOutDoorApMibModules 10 }
   enterpriseApSNTP			    	OBJECT IDENTIFIER ::= { wlsrOutDoorApMibModules 11 }
   enterpriseApDNS			  	    OBJECT IDENTIFIER ::= { wlsrOutDoorApMibModules 12 }
   enterpriseApSyslog				OBJECT IDENTIFIER ::= { wlsrOutDoorApMibModules 13 }
   enterpriseApSecurity	        	OBJECT IDENTIFIER ::= { wlsrOutDoorApMibModules 14 }
   enterpriseApRadio	        	OBJECT IDENTIFIER ::= { wlsrOutDoorApMibModules 15 }
   enterpriseApSNMP		       		OBJECT IDENTIFIER ::= { wlsrOutDoorApMibModules 16 }
   enterpriseApSession				OBJECT IDENTIFIER ::= { wlsrOutDoorApMibModules 17 }
   --enterpriseApIapp                 OBJECT IDENTIFIER ::= { wlsrOutDoorApMibModules 18 }
   --enterpriseApEventLog             OBJECT IDENTIFIER ::= { wlsrOutDoorApMibModules 19 }
   enterpriseAPVapRadio             OBJECT IDENTIFIER ::= { wlsrOutDoorApMibModules 20 }
   --enterpriseApMesh                 OBJECT IDENTIFIER ::= { wlsrOutDoorApMibModules 21 }
   enterpriseApRadioWds             OBJECT IDENTIFIER ::= { wlsrOutDoorApMibModules 22 }
   enterpriseApWMM                  OBJECT IDENTIFIER ::= { wlsrOutDoorApMibModules 24 }
   enterpriseApSTP                  OBJECT IDENTIFIER ::= { wlsrOutDoorApMibModules 25 }   

-- ****************************************************************************************
--  enterpriseApSys - Standard Mib elements
-- ****************************************************************************************
swHardwareVer OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..20))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Hardware version of the main board."
        ::= { enterpriseApSys 1 }

swBootRomVer OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..20))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Boot ROM code version of the main board."
        ::= { enterpriseApSys 2 }

swOpCodeVer OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..20))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Operation code version of the main board."
        ::= { enterpriseApSys 3 }

swSerialNumber OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..20))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Serial Number of the Access Point."
        ::= { enterpriseApSys 4 }

-- ****************************************
-- anilg:09/22/2003 added for traps
-- ****************************************
sysNotificationTree	  OBJECT IDENTIFIER ::= { enterpriseApSys 5 }

sysNotificationObjects  OBJECT IDENTIFIER ::= { sysNotificationTree 1 }

-- no objects for now (but just to keep consistent with the overall system design

sysNotifications        OBJECT IDENTIFIER ::= { sysNotificationTree 2 }

sysSystemUp NOTIFICATION-TYPE
--        OBJECTS { }
        STATUS current
        DESCRIPTION
        
		"The system up notification shall be sent when the AP 
		is fully up and running."

    ::= { sysNotifications 1 }

sysSystemDown NOTIFICATION-TYPE
--        OBJECTS { }
        STATUS current
        DESCRIPTION
        
		"The system down notification shall be sent before the AP 
		is about to reboot."

    ::= { sysNotifications 2 }

sysRadiusServerChanged NOTIFICATION-TYPE
--        OBJECTS { }
        STATUS current
        DESCRIPTION
        
		"The RADIUS server changed notification shall be sent when
		 the RADIUS server has changed from Primary / Secondary to 
		 Secondary / Primary."

    ::= { sysNotifications 3 }

sysConfigFileVersionChanged NOTIFICATION-TYPE
--        OBJECTS { }
        STATUS current
        DESCRIPTION
        
		"The Config file version changed notification shall be sent when
		 the version of the AP's configuration file has changed."

    ::= { sysNotifications 4 }


-- ****************************************************************************************

-- ****************************************************************************************
--  enterpriseApLine  AP Line elements
-- ****************************************************************************************
lineTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF LineEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table of descriptive and status information about
                     configuration of each RS-232 line in this system"
        ::= { enterpriseApLineMgnt 1 }

lineEntry OBJECT-TYPE
        SYNTAX      LineEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An entry in the table, containing information
                     about configuration in one RS232 line of the Access Point."
        INDEX       { lineIndex }
        ::= { lineTable 1 }

LineEntry ::= SEQUENCE
{
    lineIndex                Integer32,
    lineDataBits             Integer32,
    lineParity               INTEGER,
    lineSpeed                Integer32,
    lineStopBits             Integer32
}

lineIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "This is defined as RS-232 index."
        ::= { lineEntry 1 }

lineDataBits OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "This is defined as number of data bits for the RS232 interface."
        ::= { lineEntry 2 }


lineParity OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        none(99),
                        odd(1),
                        even(2)
                    }
        MAX-ACCESS      read-only
        STATUS      current
        DESCRIPTION "This is defined as parity of the RS232 interface."
        ::= { lineEntry 3 }

lineSpeed OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "This is defined as the speed of the RS-232 interface."
        ::= { lineEntry 4 }

lineStopBits OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "This is defined as the number of stop bits for the RS-232 interface."
        ::= { lineEntry 5 }


-- ****************************************************************************************
--  enterpriseApPortMgnt - Port Mib elements
-- ****************************************************************************************
portTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF PortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table of descriptive and status information about
                     configuration of each switch port (including expansion slot)
                     in this system. This table also contains information
                     about each trunk (similar to Cisco's EtherChannel)."
        ::= { enterpriseApPortMgnt 1 }

portEntry OBJECT-TYPE
        SYNTAX      PortEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An entry in the table, containing information
                     about configuration in one switch port of the switch."
        INDEX       { portIndex }
        ::= { portTable 1 }

PortEntry ::= SEQUENCE
{
    portIndex                Integer32,
    portName                 DisplayString,
    portType                 INTEGER,
    portSpeedDpxCfg          INTEGER,
    portFlowCtrlCfg          INTEGER,
    portCapabilities         INTEGER,
    portAutonegotiation      INTEGER,
    portSpeedDpxStatus       INTEGER,
    portFlowCtrlStatus       INTEGER
}

portIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "This is defined as ifIndex in the IF-MIB."
        ::= { portEntry 1 }

portName OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..64))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Indicates the port name. This is same as 
                     ifAlias in the IF-MIB (RFC2863 or later)."
        ::= { portEntry 2 }

portType OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        other(1),
                        hundredBaseTX(2),
                        hundredBaseFX(3),
                        thousandBaseSX(4),
                        thousandBaseLX(5),
                        thousandBaseT(6),
                        thousandBaseGBIC(7),
                        thousandBaseMiniGBIC(8)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Indicates the port type."
        ::= { portEntry 3 }

portSpeedDpxCfg OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        reserved(1),
                        halfDuplex10(2),
                        fullDuplex10(3),
                        halfDuplex100(4),
                        fullDuplex100(5),
                        halfDuplex1000(6),
                        fullDuplex1000(7)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Indicates the port speed and duplex mode as follows:
                         halfDuplex10(2)    - 10Mbps and half duplex mode
                         fullDuplex10(3)    - 10Mbps and full duplex mode
                         halfDuplex100(4)   - 100Mbps and half duplex mode
                         fullDuplex100(5)   - 100Mbps and full duplex mode
                         halfDuplex1000(6)  - 1000Mbps and half duplex mode
                         fullDuplex1000(7)  - 1000Mbps and full duplex mode
                     hundredBaseTX port can be set as
                         halfDuplex10(2)
                         fullDuplex10(3)
                         halfDuplex100(4)
                         fullDuplex100(5)
                     hundredBaseFX port can be set as
                         halfDuplex100(4)
                         fullDuplex100(5)
                     thousandBaseSX port can be set as
                         halfDuplex1000(6)
                         fullDuplex1000(7)
                     The actual operating speed and duplex of the port
                     is given by portSpeedDpxStatus."
        DEFVAL      { halfDuplex10 }
        ::= { portEntry 4 }

portFlowCtrlCfg OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        enabled(1),
                        disabled(2),
                        backPressure(3),
                        dot3xFlowControl(4)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "(1) Flow control mechanism is enabled.
                         If the port type is hundredBaseTX or thousandBaseSX:
                         When the port is operating in halfDuplex mode, the
                         port uses backPressure flow control mechanism. When
                         the port is operating in fullDuplex mode, the port
                         uses IEEE 802.3x flow control mechanism.
                         If the port type is hundredBaseFX:
                         When the port is operating in halfDuplex mode, the
                         port uses backPressure flow control mechanism. When
                         the port is operating in fullDuplex mode, Flow
                         control mechanism will not function.
                     (2) Flow control mechanism is disabled.
                     (3) Flow control mechanism is backPressure.
                         when the port is in fullDuplex mode.This flow control
                         mechanism will not function.
                     (4) Flow control mechanism is IEEE 802.3x flow control.
                         when the port is in halfDuplex mode.This flow control
                         mechanism will not function.
                     hundredBaseTX and thousandBaseSX port can be set as:
                         enabled(1),
                         disabled(2),
                         backPressure(3),
                         dot3xFlowControl(4).
                     hundredBaseFX port can be set as:
                         enabled(1),
                         disabled(2),
                         backPressure(3).
                     The actual flow control mechanism is used given by
                     portFlowCtrlStatus."
        DEFVAL      { enabled }
        ::= { portEntry 5 }

portCapabilities OBJECT-TYPE
-- INTEGER should be bits
        SYNTAX      INTEGER
                    {
                        portCap10half(99),
                        portCap10full(1),
                        portCap100half(2),
                        portCap100full(3),
                        portCap1000half(4),
                        portCap1000full(5),
                        reserved6(6),
                        reserved7(7),
                        reserved8(8),
                        reserved9(9),
                        reserved10(10),
                        reserved11(11),
                        reserved12(12),
                        reserved13(13),
                        portCapSym(14),
                        portCapFlowCtrl(15)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Port capabilities."
        ::= { portEntry 6 }

portAutonegotiation OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        enabled(1),
                        disabled(2)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "Whether autonegotiation is enabled."
        ::= { portEntry 7 }
                        
portSpeedDpxStatus OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        error(1),
                        halfDuplex10(2),
                        fullDuplex10(3),
                        halfDuplex100(4),
                        fullDuplex100(5),
                        halfDuplex1000(6),
                        fullDuplex1000(7)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The operating speed and duplex mode of the
                     switched port. If this index is a trunk,
                     the speed is the speed of its individual members.
                     If this index is a trunk and the result
                     is inconsistent among its member ports, this value is
                     error(1)."
        ::= { portEntry 8 }

portFlowCtrlStatus OBJECT-TYPE
        SYNTAX      INTEGER
                    {
                        error(1),
                        backPressure(2),
                        dot3xFlowControl(3),
                        none(4)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "(2) BackPressure flow control machanism is used.
                     (3) IEEE 802.3 flow control machanism is used.
                     (4) Flow control mechanism is disabled.
                     If this index is a trunk and the result
                     is inconsistent among its member ports, this value is
                     error(1)."
        ::= { portEntry 9 }

-- ****************************************************************************************
--  enterpriseApTftpMgt - File Transfer Mib elements
-- ****************************************************************************************

transferType  OBJECT-TYPE
    SYNTAX     INTEGER {
                  ftp(1),
                  tftp(2)
               }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION "Type of file to transfer."
    ::= { enterpriseApFileTransferMgt 1 }

fileType  OBJECT-TYPE
    SYNTAX     INTEGER {
                  application(1),
                  config(2),
                  bootcode(3)
               }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION "Type of file to transfer."
    ::= { enterpriseApFileTransferMgt 2 }

srcFile  OBJECT-TYPE
    SYNTAX     DisplayString (SIZE(0..127))
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION "The source file name for TFTP transfer when a
	        	transfer is next requested via this MIB.  This value is set to
		        the zero length string when no file name has been specified."
    ::= { enterpriseApFileTransferMgt 3 }

destFile  OBJECT-TYPE
    SYNTAX     DisplayString (SIZE(0..127))
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION "The destination file name for TFTP transfer when a
		        transfer is next requested via this MIB.  This value is set to
		        the zero length string when no file name has been specified."
    ::= { enterpriseApFileTransferMgt 4 }

fileServer  OBJECT-TYPE
    SYNTAX     IpAddress
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION "The IP address of the TFTP server for transfer
		        when a download is next requested via this MIB.
		        This value is set to `0.0.0.0' when no IP address has been
		        specified."
    ::= { enterpriseApFileTransferMgt 5 }

userName  OBJECT-TYPE
    SYNTAX     DisplayString (SIZE(0..127))
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION "The username specified for an FTP Transfer."
    ::= { enterpriseApFileTransferMgt 6 }

password  OBJECT-TYPE
    SYNTAX     DisplayString (SIZE(0..127))
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION "The password specified for an FTP Transfer."
    ::= { enterpriseApFileTransferMgt 7 }

status    OBJECT-TYPE
    SYNTAX     INTEGER {
			running(1),
        	success(2),
            failureGeneric(3),
			flashOpenError(10),
			flashMallocError(11),
			flashReadError(12),
			flashFtypeError(13),
			socketWriteError(20),
			protocolError(30)
	}
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION "The status of the transfer."
    ::= { enterpriseApFileTransferMgt 8 }

transferStart  OBJECT-TYPE
    SYNTAX     INTEGER {
                  nothing(0),
                  download(1),
                  upload(2)
               }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION "Set to go(1) to start a transfer."
    ::= { enterpriseApFileTransferMgt 9 }

-- ****************************************************************************************
--  enterpriseApResetMgt - Reset Mib elements
-- ****************************************************************************************

restartOpCodeFile OBJECT-TYPE
        SYNTAX      DisplayString (SIZE(0..127))
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Name of op-code file for start-up."
        ::= { enterpriseApResetMgt 1 }

restartControl  OBJECT-TYPE
	    SYNTAX     INTEGER {
			running(1),
        	warmBoot(2),
            coldBoot(3)
        }
	    MAX-ACCESS read-write
	    STATUS     current
	    DESCRIPTION "Setting this object to warmBoot(2) causes the device to
			        restart the application software with current configuration
			        parameters saved in non-volatile memory.  Setting this
			        object to coldBoot(3) causes the device to reinitialize
			        configuration parameters in non-volatile memory to default
			        values and restart the application software.  When the device
			        is running normally, this variable has a value of running(1)."
		::= { enterpriseApResetMgt 2 }


-- ****************************************************************************************
--  enterpriseApIpMgnt - Ip Mib elements
-- ****************************************************************************************

netConfigIPAddress  OBJECT-TYPE
    SYNTAX     IpAddress
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION "The IP address of this Net interface.  The default value
		        for this object is 0.0.0.0.  If either the netConfigIPAddress
		        or netConfigSubnetMask are 0.0.0.0, then when the device
		        boots, it may use DHCP to try to figure out what these
		        values should be. If DHCP fails, before the device
		        can talk on the network, this value must be configured
		        (e.g., through a terminal attached to the device)."
    ::= { enterpriseApIpMgt 1 }

netConfigSubnetMask  OBJECT-TYPE
    SYNTAX     IpAddress
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION "The subnet mask of this Net interface.  The default value
		        for this object is 0.0.0.0.  If either the netConfigIPAddress
		        or netConfigSubnetMask are 0.0.0.0, then when the device
		        boots, it may use DHCP to try to figure out what these
		        values should be. If DHCP fails, before the device
		        can talk on the network, this value must be configured
		        (e.g., through a terminal attached to the device)."
    ::= { enterpriseApIpMgt 2 }

netConfigDefaultGateway  OBJECT-TYPE
    SYNTAX     IpAddress
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION "The IP Address of the default gateway.  If this value is
		        undefined or unknown, it shall have the value 0.0.0.0."
    ::= { enterpriseApIpMgt 3 }

netConfigHttpState OBJECT-TYPE
    SYNTAX     INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION "Whether HTTP is enabled."
    ::= { enterpriseApIpMgt 4 }

netConfigHttpPort OBJECT-TYPE
	SYNTAX     INTEGER (1024..65535)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION "The port number for HTTP. Default port number is 80."
    ::= { enterpriseApIpMgt 5 }

netConfigHttpsState OBJECT-TYPE
    SYNTAX     INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION "Whether Secure HTTP is enabled."
    ::= { enterpriseApIpMgt 6 }

netConfigHttpsPort OBJECT-TYPE
	SYNTAX     INTEGER (1024..65535)
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION "The port number for Secure HTTP. Default port number is 443."
    ::= { enterpriseApIpMgt 7 }

netConfigDHCPState OBJECT-TYPE
    SYNTAX     INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION "Whether DHCP is enabled."
    ::= { enterpriseApIpMgt 8 }

-- ****************************************************************************************
--  enterpriseAPdot11 - 802.11 MIB elements 
-- ****************************************************************************************

-- **********************************************************************
-- * dot11AuthenticationEntry TABLE
-- **********************************************************************
dot11AuthenticationEntry                      OBJECT IDENTIFIER ::= { enterpriseAPdot11 1 }

dot118021xState OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   disabled(0),
                   supported(1),
                   required(2)
               }
        MAX-ACCESS read-write
        STATUS obsolete
        DESCRIPTION
            "This attribute indicates that the Enterprise the state
            of the 802.1x authentication algorithm."

    ::= { dot11AuthenticationEntry 1 }

dot118021xBroadcastKeyRefreshRate OBJECT-TYPE
        SYNTAX INTEGER (0..1440)
        MAX-ACCESS read-write
        STATUS obsolete
        DESCRIPTION
            "The number (in minutes) between changing the broadcast key for 
			802.1x and WPA clients"

    ::= { dot11AuthenticationEntry 2 }

dot118021xSessionKeyRefreshRate OBJECT-TYPE
        SYNTAX INTEGER (0..1440)
        MAX-ACCESS read-write
        STATUS obsolete
        DESCRIPTION
            "The number (in minutes) between changing session keys for 
			802.1x and WPA clients"

    ::= { dot11AuthenticationEntry 3 }

dot118021xReauthenticationTimeout OBJECT-TYPE
        SYNTAX INTEGER (0..1440)
        MAX-ACCESS read-write
        STATUS obsolete
        DESCRIPTION
            "The number (in minutes) between forcing 802.1x clients to 
			reauthenticate"

    ::= { dot11AuthenticationEntry 4 }

dot11MACAuthenticationType OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   disabled(0),
                   local(1),
                   radius(2)
               }
        ACCESS read-write
        STATUS obsolete
        DESCRIPTION
            "This value indicates the type of mac authentication in use."

	    ::= { dot11AuthenticationEntry 5 }

-- **********************************************************************
-- * End of dot11Authentication TABLE
-- **********************************************************************


-- **********************************************************************
-- * dot11AuthenticationServer TABLE
-- **********************************************************************

dot11AuthenticationServerTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF Dot11AuthenticationServerEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table of descriptive and status information about
                     configuration of each authentication server."
        ::= { enterpriseAPdot11 2 }

dot11AuthenticationServerEntry OBJECT-TYPE
        SYNTAX      Dot11AuthenticationServerEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An entry in the table, containing information
                     about configuration of one authentication server of the AP."
        INDEX       { dot11AuthenticationServerIndex }
        ::= { dot11AuthenticationServerTable 1 }

Dot11AuthenticationServerEntry ::= SEQUENCE
{
    dot11AuthenticationServerIndex        Integer32,
    dot11AuthenticationServer             IpAddress,
    dot11AuthenticationPort               INTEGER,
    dot11AuthenticationKey                DisplayString,
    dot11AuthenticationRetransmit         INTEGER,
    dot11AuthenticationTimeout            INTEGER,
    dot11AuthenticationAcctPort           INTEGER,
    dot11AuthenticationAcctInterimUpdate	INTEGER,
    dot11AuthenticationMACAddressFormat		INTEGER,
    dot11AuthenticationVLANIDFormat	    	INTEGER    
}

dot11AuthenticationServerIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Index of the Authentication Server"
        ::= { dot11AuthenticationServerEntry 1 }


dot11AuthenticationServer OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the IP address of the authentication server."

    ::= { dot11AuthenticationServerEntry 2 }

dot11AuthenticationPort OBJECT-TYPE
        SYNTAX INTEGER (1024..65535)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the UDP Port used by the authentication server."

    ::= { dot11AuthenticationServerEntry 3 }

dot11AuthenticationKey OBJECT-TYPE
        SYNTAX DisplayString (SIZE(0..20))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the shared key used by the authentication server."

    ::= { dot11AuthenticationServerEntry 4 }

dot11AuthenticationRetransmit OBJECT-TYPE
        SYNTAX INTEGER (1..30)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the retransmit timer length used by the 
            authentication server."

    ::= { dot11AuthenticationServerEntry 5 }

dot11AuthenticationTimeout OBJECT-TYPE
        SYNTAX INTEGER (1..60)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the Timeout value(sec) used by the 
			authentication server."

    ::= { dot11AuthenticationServerEntry 6 }

dot11AuthenticationAcctPort OBJECT-TYPE
        SYNTAX INTEGER (1024..65535)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The port number for radius server accounting."
        DEFVAL { 1813 }
    ::= { dot11AuthenticationServerEntry 7 }
    
dot11AuthenticationAcctInterimUpdate OBJECT-TYPE
        SYNTAX INTEGER (60..86400)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the Timeout value(sec) used by the 
			radius server interim update."
        DEFVAL { 3600 }
    ::= { dot11AuthenticationServerEntry 8 }
    
dot11AuthenticationMACAddressFormat OBJECT-TYPE
	SYNTAX     INTEGER
               {
                   no-delimiter(1),
                   single-dash(2),
                   multi-dash(3),
                   multi-colon(4)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the MAC address format from Radius 
            		MAC authentication.
		no-delimiter  format: aabbccddeeff
		single-dash   format: aabbcc-ddeeff
		multi-dash    format: aa-bb-cc-dd-ee-ff
		multi-colon   format: aa:bb:cc:dd:ee:ff"
    ::= { dot11AuthenticationServerEntry 9 }

dot11AuthenticationVLANIDFormat OBJECT-TYPE
	SYNTAX     INTEGER
               {
                   hex(1),
                   ascii(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the VLAN ID format from Radius server."
    ::= { dot11AuthenticationServerEntry 10 }
    
-- **********************************************************************
-- * End of dot11AuthenticationServer TABLE
-- **********************************************************************

-- **********************************************************************
-- * dot11FilteringTable TABLE
-- **********************************************************************

dot11MACAuthenticationFilter	  OBJECT IDENTIFIER ::= { enterpriseAPdot11 3 }

dot11FilterDefault OBJECT-TYPE
 	    SYNTAX     INTEGER
               {
                   allow(1),
                   deny(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the default access for local mac filters."
        ::= { dot11MACAuthenticationFilter 1 }

dot11FilterTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF Dot11FilterEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table of status information about
                     each configured MAC Address Filtering Entry."
        ::= { dot11MACAuthenticationFilter 2 }

dot11FilterEntry OBJECT-TYPE
        SYNTAX      Dot11FilterEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An entry in the table, containing information
                     about configuration in one radio of the AP."
        INDEX       { dot11FilterAddress }
        ::= { dot11FilterTable 1 }

Dot11FilterEntry ::= SEQUENCE
{
    dot11FilterAddress                      MacAddress,
    dot11FilterStatus                       INTEGER
}

dot11FilterAddress OBJECT-TYPE
        SYNTAX MacAddress
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "This value indicates the MAC address of the 
            filter entry."
    ::= { dot11FilterEntry 1 }

dot11FilterStatus OBJECT-TYPE
        SYNTAX INTEGER
         {
                allowed(30),
                denied(31),
                delete(32)
         }

        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the Status of the filter entry.
             Ifallowed, the client is allowed access to the network.
             If disallowed, the no frames will be forwarded to the 
             network from the client."

    ::= { dot11FilterEntry 2 }


-- *********************************************************
-- anilg: 09/22/03 :notifications used for dot11 management
-- *********************************************************
dot11NotificationTree	  OBJECT IDENTIFIER ::= { enterpriseAPdot11 4 }

dot11NotificationObjects  OBJECT IDENTIFIER ::= { dot11NotificationTree 1 }

dot11MacAddr OBJECT-TYPE
        SYNTAX MacAddress
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Mac Address of the affected interface, returned with traps only." 
        ::= { dot11NotificationObjects 1 }

dot11Station OBJECT-TYPE
		SYNTAX MacAddress
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"This attribute holds the MAC address of the wireless station"
	::= { dot11NotificationObjects 2 }

dot11RequestType OBJECT-TYPE
		SYNTAX INTEGER
		{
		unknown(1),
		association(2),
		reAssociation(3),
		authentication(4)
		}
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"This attribute defines the request type sent by the station.
                Value = 1: Unknown request type
                Value = 2: Association Request
                Value = 3: Re-association Request
		Value = 4: Authentication"
	::= { dot11NotificationObjects 3 }

dot11ReasonCode OBJECT-TYPE
		SYNTAX INTEGER
		{
		invalidModeOrState(1),
		unAuthenticatedStation(2),
		internalError(3),
		outOfSequenceFrame(4),
		unsupportedAlgorithm(5),
		invalidFrameLngth(6),
		wepRequiredOnAP(7),
		wepNotAllowed(8),
		challengeTextMismatch(9)
		}
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"This attribute defines the reason for the failure of an operation.
                Value = 1: Invalid mode/state
                Value = 2: Station not authenticated.
				Value = 3: Internal error
				Value = 4: Out of sequence frame
				Value = 5: Un-supportd algorithm
				Value = 6: Invalid frame length
				Value = 7: WEP is required on the AP
				Value = 8: WEP not allowed
				Value = 9: Challenge text mismatch"
	::= { dot11NotificationObjects 4 }

dot11ApIpAddress OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "This value indicates the IP address of the Access Point"
        ::= { dot11NotificationObjects 5 }

dot1xAuthenticatorMacAddr OBJECT-TYPE
		SYNTAX MacAddress
		MAX-ACCESS not-accessible
		STATUS current
		DESCRIPTION
			"This attribute holds the MAC address of the authenticator for the AP."
	::= { dot11NotificationObjects 6 }


dot11Notifications        OBJECT IDENTIFIER ::= { dot11NotificationTree 2 }

dot11StationAssociation NOTIFICATION-TYPE
        OBJECTS { dot11Station }
        STATUS current
        DESCRIPTION
        
		"The associate notification shall be sent when a station successfully 
		associates with the Access Point. The value of the notification shall 
		include the MAC address of the station that has associated."

    ::= { dot11Notifications 1 }

dot11StationReAssociation NOTIFICATION-TYPE
        OBJECTS { dot11Station }
        STATUS current
        DESCRIPTION
        
		"The re-associate notification shall be sent when a station 
		successfully re-associates with the Access Point. The value of the 
		notification shall include the MAC address of the station 
		that has associated."

    ::= { dot11Notifications 2 }

dot11StationAuthentication NOTIFICATION-TYPE
        OBJECTS { dot11Station }
        STATUS current
        DESCRIPTION
        
		"The authentication notification shall be sent when a station 
		successfully authenticates with the Access Point. The value of the 
		notification shall include the MAC address of the station 
		that has authenticated."

    ::= { dot11Notifications 3 }

-- Note that the following is different from the standard 802.11 mib dot11AuthenticateFail Notification
-- This one also has a reason code within the trap.

dot11StationRequestFail NOTIFICATION-TYPE
        OBJECTS { dot11Station, dot11RequestType, dot11ReasonCode }
        STATUS current
        DESCRIPTION
        
		"The station request fail shall be sent out when a station 
		fails to associate / re-associate / authenticate with the 
		Access Point. The notification shall include the MAC address 
		of the station and the reason code for the failure."

    ::= { dot11Notifications 4 }

dot11InterfaceBFail NOTIFICATION-TYPE
--        OBJECTS { }
        STATUS current
        DESCRIPTION
        
		"The InterfaceBFail notification shall be sent out when 
		802.11b wireless interface has failed."

    ::= { dot11Notifications 5 }

dot11InterfaceAGFail NOTIFICATION-TYPE
--        OBJECTS { }
        STATUS current
        DESCRIPTION
        
		"The InterfaceAGFail notification shall be sent out when 
		802.11a/802.11g wireless interface has failed."

    ::= { dot11Notifications 6 }

dot1xMacAddrAuthSuccess NOTIFICATION-TYPE
        OBJECTS { dot11Station }
        STATUS current
        DESCRIPTION
        
		"The 802.1x MAC address authentication success notification shall 
		be sent when a station successfully authenticates the MAC address
		with the RADIUS server. The value of the notification shall 
		include the MAC address of the station that has authenticated."

    ::= { dot11Notifications 7 }

dot1xMacAddrAuthFail NOTIFICATION-TYPE
        OBJECTS { dot11Station }
        STATUS current
        DESCRIPTION
        
		"The 802.1x MAC address authentication failure notification shall 
		be sent when a station fails to authenticate the MAC address
		with the RADIUS server. The value of the notification shall 
		include the MAC address of the station that failed to authenticate."

    ::= { dot11Notifications 8 }

dot1xAuthNotInitiated NOTIFICATION-TYPE
        OBJECTS { dot11Station }
        STATUS current
        DESCRIPTION
        
		"The 802.1x authentication not initiated notification shall 
		be sent when a station did not initiate 802.1x authentication
		with the RADIUS server. The value of the notification shall 
		include the MAC address of the station that did not initiate 
		802.1x authentication."

    ::= { dot11Notifications 9 }

dot1xAuthSuccess NOTIFICATION-TYPE
        OBJECTS { dot11Station }
        STATUS current
        DESCRIPTION
        
		"The 802.1x authentication success notification shall 
		be sent when a station successfully authenticates with the 
		RADIUS server. The value of the notification shall include 
		the MAC address of the station that has authenticated."

    ::= { dot11Notifications 10 }

dot1xAuthFail NOTIFICATION-TYPE
        OBJECTS { dot11Station }
        STATUS current
        DESCRIPTION
        
		"The 802.1x authentication failure notification shall 
		be sent when a station fails to authenticate with the 
		RADIUS server. The value of the notification shall include 
		the MAC address of the station that failed to authenticate."

    ::= { dot11Notifications 11 }

localMacAddrAuthSuccess NOTIFICATION-TYPE
        OBJECTS { dot11Station }
        STATUS current
        DESCRIPTION
        
		"The Local MAC address authentication success notification shall 
		be sent when a station successfully authenticates the MAC address
		with the database stored locally within the AP. The value of the 
		notification shall include the MAC address of the station that 
		has authenticated."

    ::= { dot11Notifications 12 }

localMacAddrAuthFail NOTIFICATION-TYPE
        OBJECTS { dot11Station }
        STATUS current
        DESCRIPTION
        
		"The Local MAC address authentication failure notification shall 
		be sent when a station fails to authenticate the MAC address
		with the database stored locally within the AP. The value of the 
		notification shall include the MAC address of the station that 
		has authenticated."

    ::= { dot11Notifications 13 }

pppLogonFail NOTIFICATION-TYPE
--        OBJECTS { }
        STATUS current
        DESCRIPTION
        
		"The PPP Logon failure notification shall be sent out when 
		the AP fails to login successfully to the PPP peer using the 
		supplied username and password."

    ::= { dot11Notifications 14 }

iappStationRoamedFrom NOTIFICATION-TYPE
        OBJECTS { dot11Station, dot11ApIpAddress}
        STATUS current
        DESCRIPTION
        
		"The IAPP Station Roamed-From Notification shall be sent out
		 whenever a station roams from another Access Point (AP) to 
		 this AP. The notification shall include the MAC address of 
		 the station and the IP address of the old AP."

    ::= { dot11Notifications 15 }

iappStationRoamedTo NOTIFICATION-TYPE
        OBJECTS { dot11Station, dot11ApIpAddress}
        STATUS current
        DESCRIPTION
        
		"The IAPP Station Roamed-To Notification shall be sent out
		 whenever a station roams to another Access Point (AP) from 
		 this AP. The notification shall include the MAC address of 
		 the station and the IP address of the new AP."

    ::= { dot11Notifications 16 }


iappContextDataSent NOTIFICATION-TYPE
        OBJECTS { dot11Station, dot11ApIpAddress}
        STATUS current
        DESCRIPTION
        
		"The IAPP Context Data Sent notification shall be sent out
		 whenever the context data for a station has been sent to 
		 the new AP with which the station has associated. The 
		 notification shall include the MAC address of 
		 the station and the IP address of the new AP."

    ::= { dot11Notifications 17 }
    
dot1xSupplicantAuthenticated NOTIFICATION-TYPE
        OBJECTS { dot11AuthenticatorMacAddr }
        STATUS current
        DESCRIPTION
        
		"The notification shall be sent when the AP has successfully authenticated 
		 with the switch.  The value of the notification shall include the MAC
		 address of the switch (authenticator) that the AP has authenticated with."

    ::= { dot11Notifications 18 }

-- ****************************************************************************************
--  dot11AuthenticationSupplicantTable
-- ****************************************************************************************
  
dot11AuthenticationSupplicantTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF Dot11AuthenticationSupplicantEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table of descriptive and status information about
                     configuration of supplicant"
        ::= { enterpriseAPdot11 5 }


dot11AuthenticationSupplicantEntry OBJECT-TYPE
        SYNTAX      Dot11AuthenticationSupplicantEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An entry in the table, containing information
                     about configuration of one supplicant."
        INDEX       { dot11AuthenticationSuppIndex }
        ::= { dot11AuthenticationSupplicantTable 1 }


Dot11AuthenticationSupplicantEntry ::= SEQUENCE
{
    dot118021xSuppIndex          Integer32,
    dot118021xSuppState          INTEGER,
    dot118021xSuppUser           DisplayString,
    dot118021xSuppPasswd         DisplayString
}

dot118021xSuppIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Index of the interface for which this supplicant is
		             running.  Currently only the ethernet interface."
        ::= { dot11AuthenticationSupplicantEntry 1 }


dot118021xSuppState OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   disabled(0),
                   enabled(1)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This object is used to enable or disable the 802.1x supplicant."

    ::= { dot11AuthenticationSupplicantEntry 2 }

dot118021xSuppUser OBJECT-TYPE
        SYNTAX DisplayString (SIZE(1..32))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the username for supplicant. If value is
			 configured, will display ****.  Else will display EMPTY."
        ::= { dot11AuthenticationSupplicantEntry 3 }
		
dot118021xSuppPasswd OBJECT-TYPE
        SYNTAX DisplayString (SIZE(1..32))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the password for supplicant. If value is
			 configured, will display ****.  Else will display EMPTY."
        ::= { dot11AuthenticationSupplicantEntry 4 }

-- **********************************************************************
-- * dot11VapAuthenticationEntry TABLE
-- **********************************************************************

dot11VapAuthenticationTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF Dot11VapAuthenticationEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table of descriptive and status information about
                     configuration of 8021x for each Vap."
        ::= { enterpriseAPdot11 6 }

dot11VapAuthenticationEntry OBJECT-TYPE
        SYNTAX      Dot11VapAuthenticationEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An entry in the table, containing information
                     about configuration of 8021x for each Vap of the AP."
        INDEX       { dot11Vap8021xIndex }
        ::= { dot11VapAuthenticationTable 1 }

Dot11VapAuthenticationEntry ::= SEQUENCE
{
    dot11Vap8021xIndex        	       	  Integer32,
    dot11Vap8021xState        	          INTEGER,
    dot11Vap8021xBroadcastKeyRefreshRate  INTEGER,
    dot11Vap8021xSessionKeyRefreshRate    INTEGER,
    dot11Vap8021xReauthenticationTimeout  INTEGER,
    dot11VapAuthMACAuthenticationType     INTEGER,
    dot11VapAuthMACAuthenticationTimeout  INTEGER
}

dot11Vap8021xIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Index for configuration."
        ::= { dot11VapAuthenticationEntry 1 }


dot11Vap8021xState OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   disabled(0),
                   supported(1),
                   required(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This attribute indicates that the Enterprise the state
            of the 802.1x authentication algorithm."

    ::= { dot11VapAuthenticationEntry 2 }

dot11Vap8021xBroadcastKeyRefreshRate OBJECT-TYPE
        SYNTAX INTEGER (0..1440)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The number (in minutes) between changing the broadcast key for 
			802.1x and WPA clients"

    ::= { dot11VapAuthenticationEntry 3 }

dot11Vap8021xSessionKeyRefreshRate OBJECT-TYPE
        SYNTAX INTEGER (0..1440)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The number (in minutes) between changing session keys for 
			802.1x and WPA clients"

    ::= { dot11VapAuthenticationEntry 4 }

dot11Vap8021xReauthenticationTimeout OBJECT-TYPE
        SYNTAX INTEGER (0..1440)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The number (in minutes) between forcing 802.1x clients to 
			reauthenticate"

    ::= { dot11VapAuthenticationEntry 5 }

dot11VapAuthMACAuthenticationType OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   disabled(0),
                   local(1),
                   remote(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the type of mac authentication in use."
	    DEFVAL { disabled }
	::= { dot11VapAuthenticationEntry 6 }

dot11VapAuthMACAuthenticationTimeout OBJECT-TYPE
        SYNTAX INTEGER (0..1440)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The number (in minutes) between forcing Radius MAC to authenticate."
	::= { dot11VapAuthenticationEntry 7 }

-- ****************************************************************************************
--  enterpriseApAdmin - Admin Mib elements
-- ****************************************************************************************

enterpriseApAdminUser OBJECT-TYPE
        SYNTAX DisplayString (SIZE(3..16))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the username for management login."
        ::= { enterpriseApAdmin 1 }

enterpriseApAdminPassword OBJECT-TYPE
        SYNTAX DisplayString (SIZE(0..16))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the password for management login.
             The password length is betwen 3 and 16. 'Zero-length'
             indicates 'no password'."
        ::= { enterpriseApAdmin 2 }

-- ****************************************************************************************
--  enterpriseApVLAN - VLAN Mib elements
-- ****************************************************************************************

enterpriseApVLANNativeId OBJECT-TYPE
        SYNTAX INTEGER
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the native VLAN id."
        ::= { enterpriseApVLAN 1 }

enterpriseApVLANState OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether VLANs are enabled or disabled."
        ::= { enterpriseApVLAN 2 }


enterpriseApNativeVlanTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF EnterpriseApNativeVlanEntry
        ACCESS      not-accessible
        STATUS      mandatory
        DESCRIPTION "Table used to manage the Vlans for each
                     wireless interface."
        ::= { enterpriseApVLAN 3 }

enterpriseApNativeVlanEntry OBJECT-TYPE
        SYNTAX      EnterpriseApNativeVlanEntry
        ACCESS      not-accessible
        STATUS      mandatory
        DESCRIPTION "An entry in the table, containing information
                     about vlan configuration of one wireless interface."
        INDEX       { nativeVlanIfIndex, 
		              nativeVlanSsidNumber }
        ::= { enterpriseApNativeVlanTable 1 }


EnterpriseApNativeVlanEntry ::= SEQUENCE
{
    nativeVlanIfIndex          Integer32,
    nativeVlanSsidNumber       Integer32,
    nativeVlanVlanId           Integer32
}


nativeVlanIfIndex OBJECT-TYPE
        SYNTAX      Integer32
        ACCESS      not-accessible
        STATUS      mandatory
        DESCRIPTION "Interface Index of the wireless interface for which
		             the vlan is assigned to."
        ::= { enterpriseApNativeVlanEntry 1 }

nativeVlanSsidNumber OBJECT-TYPE
        SYNTAX      Integer32
        ACCESS      not-accessible
        STATUS      mandatory
        DESCRIPTION "Associated Number for Service Set Id (SSID) of the 
		             wireless interface for which the vlan is assigned to.  
					 Note: This is for future support of multiple SSIDs 
					 per radio interface."
        ::= { enterpriseApNativeVlanEntry 2 }

nativeVlanVlanId OBJECT-TYPE
        SYNTAX Integer32
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION
            "This value indicates the native VLAN id of the wireless interface associated
			  with the if index and the SSID number(if it is not 0)."
        ::= { enterpriseApNativeVlanEntry 3 }

-- ****************************************************************************************
--  enterpriseApFilterControl - Filter Control Mib elements
-- ****************************************************************************************

enterpriseApFilterControlInterClientSTAsCommun OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   disabled                     (1),
                   PreventIntraVAPClient        (2),
                   PreventInterAndIntraVAPClient(3)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the Inter Client STAs Communication Filter setting.
               disabled                     (1) To disable the Inter Client STAs Communication Filter
               PreventIntraVAPClient        (2) To set filter to prevent intra VAP client communication
               PreventInterAndIntraVAPClient(3) To set filter to prevent inter and intra VAP client communication"
        ::= { enterpriseApFilterControl 1 }

enterpriseApFilterControlAPManage OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the AP management filter setting."
        ::= { enterpriseApFilterControl 2 }

enterpriseApFilterControlEthernet OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the ethernet filter setting."
        ::= { enterpriseApFilterControl 3 }

enterpriseApFilterProtocolTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF EnterpriseApFilterProtocolEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table of descriptive and status information about
                     configuration of the filter protocol table."
        ::= { enterpriseApFilterControl 4 }

enterpriseApFilterProtocolEntry OBJECT-TYPE
        SYNTAX      EnterpriseApFilterProtocolEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An entry in the filter protocol table, containing information
                     about configuration of one filter table entry."
        INDEX       { enterpriseApFilterProtocolIndex }
        ::= { enterpriseApFilterProtocolTable 1 }

EnterpriseApFilterProtocolEntry ::= SEQUENCE
{
    enterpriseApFilterProtocolIndex          Integer32,
    enterpriseApFilterProtocolName           DisplayString,
    enterpriseApFilterProtocolISODesignator  DisplayString,
    enterpriseApFilterProtocolState          INTEGER
}

enterpriseApFilterProtocolIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Index of the Protocol Filters."
        ::= { enterpriseApFilterProtocolEntry 1 }

enterpriseApFilterProtocolName OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This value indicates the name of the protocol filter.  One of 
			 the following:
			 Aironet_DDP, Appletalk_ARP, ARP, Banyan, Berkeley_Trailer_Negotiation, 
			 CDP, DEC_LAT, DEC_MOP, DEC_MOP_Dump_Load, DEC_XNS, EAPOL, 
			 Enet_Config_Test, Ethertalk, IP, LAN_Test, NetBEUI, Novell_IPX(new),
			 Novell_IPX(old), RARP, Telxon_TXP, X.25_Level3
			"
    ::= { enterpriseApFilterProtocolEntry 2 }

enterpriseApFilterProtocolISODesignator OBJECT-TYPE
        SYNTAX DisplayString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This value indicates the name of the protocol filter."
    ::= { enterpriseApFilterProtocolEntry 3 }

enterpriseApFilterProtocolState OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the protocol filter is enabled."
    ::= { enterpriseApFilterProtocolEntry 4 }

--***********************************************************************************************
--enterpriseApFilterUplinkPortMACAddrFilter
--***********************************************************************************************

enterpriseApFilterUplinkPortMACAddrFilter OBJECT IDENTIFIER ::= { enterpriseApFilterControl 5 }

uplinkPortMACAddrFilterStatus OBJECT-TYPE
    SYNTAX INTEGER
    {
        enable   (1),    
        disabled (2)
    }             
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This value indicates whether the Uplink Port MAC Address Filter Table is enabled or not."
    ::= { enterpriseApFilterUplinkPortMACAddrFilter 1 }

uplinkPortMACAddrFilterAddMac OBJECT-TYPE
    SYNTAX MacAddress
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "To add mac address to Uplink Port MAC Address Filter Table.
        (Mac Address format: xx-xx-xx-xx-xx-xx or xx:xx:xx:xx:xx:xx)"
    ::= { enterpriseApFilterUplinkPortMACAddrFilter 2 } 

uplinkPortMACAddrFilteringTable OBJECT-TYPE
    SYNTAX SEQUENCE OF UplinkPortMACAddrFilteringEntry
    MAX-ACCESS not-accessible 
    STATUS current
    DESCRIPTION
            "Table of descriptive and status information about
              configuration of the Uplink Port MAC Address Filter Table. "
    ::= { enterpriseApFilterUplinkPortMACAddrFilter 3 }

uplinkPortMACAddrFilteringEntry OBJECT-TYPE           
    SYNTAX UplinkPortMACAddrFilteringEntry
    MAX-ACCESS not-accessible 
    STATUS current
    DESCRIPTION
            "An entry in Uplink Port MAC Address Filter Table." 
    INDEX { uplinkPortMacAddrIndex }
    ::= { uplinkPortMACAddrFilteringTable 1 }        

UplinkPortMACAddrFilteringEntry ::=  SEQUENCE
{
    uplinkPortMacAddrIndex  Integer32,
    uplinkPortMACAddr       MacAddress, 
    deleteMacAddr           INTEGER
}      

uplinkPortMacAddrIndex OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The index for Uplink Port MAC Address Filter Table." 
        ::= { uplinkPortMACAddrFilteringEntry 1 }

uplinkPortMACAddr OBJECT-TYPE
        SYNTAX MacAddress
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION                  
            "The MAC Address of wireless clients which allowed to communicate on subnet."
        ::= { uplinkPortMACAddrFilteringEntry 2 }

deleteMacAddr OBJECT-TYPE
        SYNTAX INTEGER
        {
            Delete(1),
            Nothing (2)
        }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "To delete the MAC Address from Uplink Port MAC Address Filter Table.
                Delete(1)   To start delete MAC address.
                Nothing(2)  Nothing occur." 
        ::= { uplinkPortMACAddrFilteringEntry 3 }

-- newMACAddress OBJECT-TYPE
--    SYNTAX MacAddress
--    MAX-ACCESS read-write
--    STATUS current
--    DESCRIPTION
--        "To add mac address to Uplink Port MAC Address Filter Table."
--    ::= { addUplinkPortMACAddress 1 }
--***********************************************************************************************
--enterpriseApFilterUplinkPortMACAddrFilter Table
--***********************************************************************************************


-- ****************************************************************************************
--  enterpriseApSNTP - SNTP Mib elements
-- ****************************************************************************************

enterpriseApSNTPState OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether SNTP is enabled or not. At least one of the 
			 SNTP servers must have a valid IP address before SNTP can be enabled."
        ::= { enterpriseApSNTP 1 }

enterpriseApSNTPPrimaryServer OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the IP address of the primary SNTP server."
        ::= { enterpriseApSNTP 2 }

enterpriseApSNTPSecondaryServer OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the IP address of the secondary SNTP server."
        ::= { enterpriseApSNTP 3 }

enterpriseApSNTPTimezone OBJECT-TYPE
	    SYNTAX     INTEGER
               {
					enewetakKwajalein(0),
					midwayIsland(1),
					hawaii(2),
					alaska(3),
					pacific(4),
					arizona(5),
					mountain(6),
					central(7),
					mexicoCity(8),
					saskatchewan(9),
					bogota(10),
					eastern(11),
					indiana(12),
					atlantic(13),
					caracas(14),
					santiago(15),
					newfoundland(16),
					brasilia(17),
					buenos(18),
					midAtlantic(19),
					azores(20),
					casablanca(21),
					greenwichMeanTimeDublin(22),
					greenwichMeanTimeLisbon(23),
					amsterdam(24),
					stockhoim(25),
					bratislava(26),
					prague(27),
					paris(28),
					sofija(29),
					athens(30),
					bucharest(31),
					cairo(32),
					harare(33),
					helsinki(34),
					israel(35),
					baghdad(36),
					moscow(37),
					tehran(38),
					abuDhabi(39),
					vogograd(40),
					islamabad(41),
					almaty(42),
					bangkok(43),
					beijing(44),
					taipei(45),
					tokyo(46),
					brisbane(47),
					canberra(48),
					guam(49),
					hobart(50),
					magadan(51),
					fiji(52),
					wellington(53)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates which timezone to use."
        ::= { enterpriseApSNTP 4 }

enterpriseApSNTPDST OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether Daylight Savings Time is enabled or not."
        ::= { enterpriseApSNTP 5 }

enterpriseApSNTPDSTStartMonth OBJECT-TYPE
        SYNTAX INTEGER (1..12)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the starting month for Daylight Savings Time."
        ::= { enterpriseApSNTP 6 }

enterpriseApSNTPDSTStartDay OBJECT-TYPE
        SYNTAX INTEGER (1..31)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the starting day for Daylight Savings Time."
        ::= { enterpriseApSNTP 7 }

enterpriseApSNTPDSTEndMonth OBJECT-TYPE
        SYNTAX INTEGER (1..12)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the ending month for Daylight Savings Time."
        ::= { enterpriseApSNTP 8 }

enterpriseApSNTPDSTEndDay OBJECT-TYPE
        SYNTAX INTEGER (1..31)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the ending day for Daylight Savings Time."
        ::= { enterpriseApSNTP 9 }

-- ****************************************
-- anilg:09/19/2003 added for traps
-- ****************************************
sntpNotificationTree	  OBJECT IDENTIFIER ::= { enterpriseApSNTP 10 }


sntpNotificationObjects  OBJECT IDENTIFIER ::= { sntpNotificationTree 1 }

-- no objects for now (but just to keep consistent with the overall system design

sntpNotifications        OBJECT IDENTIFIER ::= { sntpNotificationTree 2 }

sntpServerFail NOTIFICATION-TYPE
--        OBJECTS { }
        STATUS current
        DESCRIPTION
        
		"The sntpServerFail notification shall be sent when the AP 
		fails to get time from the configured SNTP server."

    ::= { sntpNotifications 1 }

-- ****************************************************************************************
--  enterpriseApDNS - DNS Mib elements
-- ****************************************************************************************

enterpriseApDNSPrimaryServer OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the IP address of the primary DNS server."
        ::= { enterpriseApDNS 1 }

enterpriseApDNSSecondaryServer OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the IP address of the secondary DNS server."
        ::= { enterpriseApDNS 2 }


-- ****************************************************************************************
--  enterpriseApSyslog - Syslog Mib elements
-- ****************************************************************************************

enterpriseApSyslogState OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION "This value indicates whether syslog is enabled."
        ::= { enterpriseApSyslog 1 }

enterpriseApSyslogConsoleState OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION "This value indicates whether syslog console logging is enabled."
        ::= { enterpriseApSyslog 2 }

enterpriseApSyslogLevel OBJECT-TYPE
        SYNTAX INTEGER
               {
                   emergency(0),
                   alert(1),
                   critical(2),
                   error(3),
                   warning(4),
                   notice(5),
                   info(6),
                   debug(7)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION "This value indicates the syslog logging level."
        ::= { enterpriseApSyslog 3 }

-- **********************************************************************
-- * EnterpriseApSyslogServer TABLE
-- **********************************************************************

enterpriseApSyslogServerTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF EnterpriseApSyslogServerEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table of descriptive and status information about
                     configuration of each syslog server."
        ::= { enterpriseApSyslog 4 }

enterpriseApSyslogServerEntry OBJECT-TYPE
        SYNTAX      EnterpriseApSyslogServerEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An entry in the table, containing information
                     about configuration of one syslog server of the AP."
        INDEX       { enterpriseApSyslogServerIndex }
        ::= { enterpriseApSyslogServerTable 1 }

EnterpriseApSyslogServerEntry ::= SEQUENCE
{
    enterpriseApSyslogServerIndex        Integer32,
    enterpriseApSyslogServerState        INTEGER,
    enterpriseApSyslogServerIPAddress    IpAddress,
    enterpriseApSyslogServerPort         INTEGER
}

enterpriseApSyslogServerIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Index of the Syslog Server"
        ::= { enterpriseApSyslogServerEntry 1 }


enterpriseApSyslogServerState OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the syslog server is enabled."
    ::= { enterpriseApSyslogServerEntry 2 }

enterpriseApSyslogServerIPAddress OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the IP address of the syslog server."
    ::= { enterpriseApSyslogServerEntry 3 }

enterpriseApSyslogServerPort OBJECT-TYPE
        SYNTAX INTEGER (1024..65535)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the UDP Port used by the syslog server."
    ::= { enterpriseApSyslogServerEntry 4 }


-- **********************************************************************
-- * EnterpriseApSecurity TABLE
-- **********************************************************************

enterpriseApSecurityTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF EnterpriseApSecurityEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table of descriptive and status information about
                     configuration of each radio in terms of security settings."
        ::= { enterpriseApSecurity 1 }

enterpriseApSecurityEntry OBJECT-TYPE
        SYNTAX      EnterpriseApSecurityEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An entry in the table, containing information
                     about configuration of one radio of the AP."
        INDEX       { enterpriseApSecurityIndex }
        ::= { enterpriseApSecurityTable 1 }

EnterpriseApSecurityEntry ::= SEQUENCE
{
    enterpriseApSecurityIndex             Integer32,
    enterpriseApSecurityAuthType          INTEGER,
    enterpriseApSecuritySharedKeyLen      INTEGER,
    enterpriseApSecurityWPAMode           INTEGER,
    enterpriseApSecurityWPAKeyType        INTEGER,
    enterpriseApSecurityWPACipher         INTEGER,
    enterpriseApSecurityWPAPSKType        INTEGER,
    enterpriseApSecurityWPAPSK            DisplayString,
    enterpriseApSecurityWEPKeyType        INTEGER,
    enterpriseApSecurityWEPEnabled        TruthValue,
    enterpriseApSecurityWPACipherSuite      INTEGER,
    enterpriseApSecurityWPAPreAuthentication	INTEGER,
    enterpriseApSecurityWPAPmksaLifetime INTEGER
}

enterpriseApSecurityIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Radio Index for security settings."
        ::= { enterpriseApSecurityEntry 1 }

enterpriseApSecurityAuthType OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   opensystem(0),
                   sharedkey(1)
                   wpa(2)
                   wpapsk(3)
                   wpawpa2mixed(4)
                   wpawpa2pskmixed(5)
                   wpa2(6)
                   wpa2psk(7)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the type of authentication in use for this radio interface.
							opensystem(0)         Set authentication open
 							sharedkey(1)          Set authentication shared
 							wpa(2)                Set WPA Mode
 							wpapsk(3)             Set WPA-PSK Mode
 							wpa-wpa2-mixed(4)     Set WPA-WPA2-Mixed Mode
 							wpawpa2pskmixed(5)    Set WPA-WPA2 PSK Mixed Mode
 							wpa2(6)               Set WPA2 Mode
 							wpa2psk(7)            Set WPA2-PSK Mode
            "
        ::= { enterpriseApSecurityEntry 2 }

enterpriseApSecuritySharedKeyLen OBJECT-TYPE
	    SYNTAX     INTEGER
               {
				   none(0),
				   sixtyFour(1),
				   oneHundredTwentyEight(2),	
				   oneHundredFiftyTwo(3)	
               }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This value indicates the shared key length for this radio interface."
        ::= { enterpriseApSecurityEntry 3 }

enterpriseApSecurityWPAMode OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   supported(0),
                   required(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the state of WPA for this radio interface."
        ::= { enterpriseApSecurityEntry 4 }

enterpriseApSecurityWPAKeyType OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   dot1x(0),
                   presharedkey(1)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the type of WPA Key Management in use for this radio interface."
        ::= { enterpriseApSecurityEntry 5 }

enterpriseApSecurityWPACipher OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   wep(0),
                   tkip(1),
                   aes(2)
               }
        MAX-ACCESS read-write
        STATUS obsolete
        DESCRIPTION
            "This value indicates the type of WPA Cipher in use for this radio interface."
        ::= { enterpriseApSecurityEntry 6 }

enterpriseApSecurityWPAPSKType OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   hex(0),
                   alphanumeric(1)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the type of WPA Pre Shared Key in use for this radio interface."
        ::= { enterpriseApSecurityEntry 7 }

enterpriseApSecurityWPAPSK OBJECT-TYPE
        SYNTAX DisplayString (SIZE(0..80))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates WPA Pre Shared Key in use for this radio interface."
        ::= { enterpriseApSecurityEntry 8 }

enterpriseApSecurityWEPKeyType OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   hexadecimal(0),
                   alphanumeric(1)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the type of WEP Key in use for this radio interface."
        ::= { enterpriseApSecurityEntry 9 }

enterpriseApSecurityWEPEnabled OBJECT-TYPE
        SYNTAX TruthValue 
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether WEP is enabled."
        ::= { enterpriseApSecurityEntry 10 }

enterpriseApSecurityWPACipherSuite OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   aes-ccmp(0),
                   tkip(1),
                   wep(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the type of WPA Cipher Suite in use for this radio interface."
        ::= { enterpriseApSecurityEntry 11 }
        
enterpriseApSecurityWPAPreAuthentication OBJECT-TYPE
	SYNTAX     INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
	MAX-ACCESS     read-write
        STATUS current
        DESCRIPTION
            "Whether Pre-Authentication is enabled."
        DEFVAL { disabled }
        ::= { enterpriseApSecurityEntry 12 }
        
enterpriseApSecurityWPAPmksaLifetime OBJECT-TYPE
	SYNTAX INTEGER (0..14400)
	MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The number (in minutes) for Pmksa-Lifetime."
        ::= { enterpriseApSecurityEntry 13 }


enterpriseApSsh	        OBJECT IDENTIFIER ::= { enterpriseApSecurity 2 }

enterpriseApSshServerEnabled OBJECT-TYPE
        SYNTAX TruthValue 
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION
            "This value indicates whether SSH server is enabled."
        ::= { enterpriseApSsh 1 }
        
enterpriseApSshServerPort OBJECT-TYPE
        SYNTAX Integer32
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION
            "This value indicates SSH server's port number."
        DEFVAL      { 22 }
        ::= { enterpriseApSsh 2 }

enterpriseApSshTelnetServerEnabled OBJECT-TYPE
        SYNTAX TruthValue 
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION
            "This value indicates whether telnet server is enabled."
        ::= { enterpriseApSsh 3 }
        

-- **********************************************************************
-- * EnterpriseApRadio TABLE
-- **********************************************************************

enterpriseApRadioTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF EnterpriseApRadioEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table of descriptive and status information about
                     configuration of each radio."
        ::= { enterpriseApRadio 1 }

enterpriseApRadioEntry OBJECT-TYPE
        SYNTAX      EnterpriseApRadioEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An entry in the table, containing information
                     about configuration of one radio of the AP."
        INDEX       { enterpriseApRadioIndex }
        ::= { enterpriseApRadioTable 1 }

EnterpriseApRadioEntry ::= SEQUENCE
{
    enterpriseApRadioIndex          Integer32,
    enterpriseApRadioState          INTEGER,
    enterpriseApRadioAutoChannel    INTEGER,
    enterpriseApRadioTransmitPower  INTEGER,
    enterpriseApRadioClosedSystem   INTEGER,
    enterpriseApRadioMaxAssoc       INTEGER,
    enterpriseApRadioTransmitKey    INTEGER,
	enterpriseApRadioTurboMode      INTEGER,
    enterpriseApRadioDescription    DisplayString,
    enterpriseApRadioDataRate       INTEGER,
    enterpriseApRadioGMode          INTEGER,
	enterpriseApRadioAntennaMode   INTEGER,
    enterpriseApRadioAntennaId            DisplayString,
    enterpriseApRadioAntennaControlMethod INTEGER,
    enterpriseApRadioAntennaLocation      INTEGER,
    enterpriseApRadioRogueApDetection     INTEGER,
    enterpriseApRadioRogueApScanInterval  Integer32,
    enterpriseApRadioRogueApScanDuration  Integer32,
    enterpriseApRadioRogueApScanNow       INTEGER, 
    enterpriseApRadioMICMode              INTEGER,
    enterpriseApRadioSuperMode            INTEGER,
    enterpriseApRadioBeaconInterval       Integer32,
    enterpriseApRadioDataBeaconRate       Integer32,
    enterpriseApRadioChannel              Integer32,
    enterpriseApRadioFragmentLength       Integer32,
    enterpriseApRadioRTSThreshold         Integer32,
    enterpriseApRadioAntennaGainReduction Integer32
}

enterpriseApRadioIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Radio Index for configuration."
        ::= { enterpriseApRadioEntry 1 }

enterpriseApRadioState OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS obsolete
        DESCRIPTION
            "This value indicates the state of the radio interface."
        ::= { enterpriseApRadioEntry 2 }

enterpriseApRadioAutoChannel OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether auto channel selection is enabled or not
			 for this radio interface"
        ::= { enterpriseApRadioEntry 3 }

enterpriseApRadioTransmitPower OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   min(0),
				   eighth(1),
				   quarter(2),
				   half(3),
				   full(4)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the transmit power for this radio interface."
        ::= { enterpriseApRadioEntry 4 }

enterpriseApRadioClosedSystem OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS obsolete
        DESCRIPTION
            "This value indicates whether closed system is enabled for this radio interface."
        ::= { enterpriseApRadioEntry 5 }

enterpriseApRadioMaxAssoc OBJECT-TYPE
        SYNTAX INTEGER (1..64)
        MAX-ACCESS read-write
        STATUS obsolete
        DESCRIPTION
            "This value indicates the max number of clients allowed on this radio interface."
        ::= { enterpriseApRadioEntry 6 }

enterpriseApRadioTransmitKey OBJECT-TYPE
        SYNTAX INTEGER (1..4)
        MAX-ACCESS read-write
        STATUS obsolete
        DESCRIPTION
            "This value indicates default transmit key in use for this radio interface."
        ::= { enterpriseApRadioEntry 7 }

enterpriseApRadioTurboMode OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   disabled(1),
                   static-turbo(2),
                   dynamic-turbo(3)                  
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether turbo mode is enabled for this radio interface."
        ::= { enterpriseApRadioEntry 8 }

enterpriseApRadioDescription OBJECT-TYPE
        SYNTAX DisplayString (SIZE(0..80))
        MAX-ACCESS read-write
        STATUS obsolete
        DESCRIPTION
            "This value indicates the description for this radio interface."
        ::= { enterpriseApRadioEntry 9 }

enterpriseApRadioDataRate OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   oneMbps(1),
                   twoMbps(2),
                   fiveAndHalfMbps(5), 
                   sixMbps(6), 
                   nineMbps(9), 
                   elevenMbps(11), 
                   twelveMbps(12), 
                   eighteenMbps(18), 
                   twentyFourMbps(24), 
                   thirtySixMbps(36), 
                   fourtyEightMbps(48), 
                   fiftyFourMbps(54),
				   auto(255)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the data rate for this radio interface.
			Radio interface A operates at 6, 9, 12, 18, 24, 36, 48, 54.
            Radio interface G operates all listed data rates.   The auto
			setting will attempt to set the best data rate for the interface" 
        ::= { enterpriseApRadioEntry 10 }

enterpriseApRadioGMode OBJECT-TYPE
	    SYNTAX     INTEGER
               {
					bOnly(1),
					gOnly(2),
					bg(3)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the radio mode for the 802.11g radio.
			This setting is only valid for the 802.11g interface."
        ::= { enterpriseApRadioEntry 11 }

enterpriseApRadioAntennaMode OBJECT-TYPE
	    SYNTAX     INTEGER
               {
					fixed(1),
					external(2)
               }
        ACCESS read-write
        STATUS mandatory
        DESCRIPTION
            "This value indicates the antenna mode in use for the G-radio. 
			 The values are interpreted as follows:
				fixed(1)	means use both built-in antennas,
				external(2) means use one external antenna on the right side.
			This setting is only valid for the 802.11g interface."
        ::= { enterpriseApRadioEntry 12 }

enterpriseApRadioAntennaId OBJECT-TYPE
    SYNTAX DisplayString
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        " " 
    ::= { enterpriseApRadioEntry 13 }
   
enterpriseApRadioAntennaControlMethod OBJECT-TYPE
        SYNTAX INTEGER
        {
            Diversity (1),
            Left      (2),
            Right     (3)
        }               
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
             "This value indicates the antenna control method for the radio index.
                 Diversity(1)  AP select the antenna automatically.
                 Left     (2)  Use the left antenna.
                 Right    (3)  Use the right antenna."  
        ::= { enterpriseApRadioEntry 14 }

enterpriseApRadioAntennaLocation OBJECT-TYPE
        SYNTAX INTEGER
        {
            Indoor (1)
            Outdoor(2),
        }               
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
             "This value indicates the location of antenna for each radio index."  
        ::= { enterpriseApRadioEntry 15 }

enterpriseApRadioRogueApDetection OBJECT-TYPE
    SYNTAX INTEGER
    {
        enabled  (1),
        disabled (2)
    }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION 
        "The status of Rogue AP detection for each index.
            enabled(1)  To set rogue Ap detection enabled.
            disabled(2) To set rogue Ap detection disabled." 
    ::= { enterpriseApRadioEntry 16 }

enterpriseApRadioRogueApScanInterval OBJECT-TYPE
    SYNTAX Integer32(30..10080)
    MAX-ACCESS read-write    
    STATUS current
    DESCRIPTION 
        "This value indicates the interval between each rogue AP scan.(unit: minutes)" 
    ::= { enterpriseApRadioEntry 17 }

enterpriseApRadioRogueApScanDuration OBJECT-TYPE
    SYNTAX Integer32(100..1000)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION 
        "This value indicates the rogue AP scan duratoin.(unit: minutes)" 
    ::= { enterpriseApRadioEntry 18 }


enterpriseApRadioRogueApScanNow OBJECT-TYPE
    SYNTAX INTEGER
    {
        enabled  (1),
        disabled (2)
    }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION 
        "To force Ap to do rogue AP scan right away.
            enabled(1)  To do Rogue AP scan right now.
            disabled(2) To set rogue Ap." 
    ::= { enterpriseApRadioEntry 19 }


enterpriseApRadioMICMode OBJECT-TYPE
        SYNTAX INTEGER
        {
            software(1),
            hardware(2)
        }               
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
             "This value indicates the MIC mode status for this radio index.
                 software(1) To set MIC mode to software.
                 hardware(2) To set MIC mode to hardware."  
        ::= { enterpriseApRadioEntry 21 }

enterpriseApRadioSuperMode OBJECT-TYPE
        SYNTAX INTEGER
        {
            enabled(1),
            disabled(2)
        }               
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
             "This value indicates the super mode status for this radio index.
                 enabled (1) To set super mode enabled.
                 disabled(2) To set super mode disabled."  
        ::= { enterpriseApRadioEntry 22 }

enterpriseApRadioBeaconInterval OBJECT-TYPE
        SYNTAX Integer32(20..1000)              
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
             "This value indicates the beacon interval for this radio index."  
        ::= { enterpriseApRadioEntry 23 }

enterpriseApRadioDataBeaconRate OBJECT-TYPE
        SYNTAX Integer32         
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
             "This value indicates the data beacon rate for the radio index."  
        ::= { enterpriseApRadioEntry 24 }

enterpriseApRadioChannel OBJECT-TYPE
        SYNTAX Integer32         
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
             "This valud indicates the radio channel for the radio index.
             set channel 42/50/58/152/160 for static turbo mode,
             set channel 40/48/56/153/161 for dynamic turbo mode,
             set channel 36/40/44/48/52/56/60/64/149/153/157/161/165 when turbo mode is disabled.
             The value '0' indicates the radio interface cannot be enable in current country code."  
        ::= { enterpriseApRadioEntry 25 }      

enterpriseApRadioFragmentLength OBJECT-TYPE
    SYNTAX Integer32(256..2346)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This value indicates the fragment length for the radio index.(unit: Byte)"
    ::= { enterpriseApRadioEntry 26 } 

enterpriseApRadioRTSThreshold OBJECT-TYPE
    SYNTAX Integer32(0..2347)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This value indicates the RTS Threshold for the radio index.(unit: Byte)"
    ::= { enterpriseApRadioEntry 27 }
-- 20070330, Eva Hsieh, added for ARUBA
enterpriseApRadioAntennaGainReduction OBJECT-TYPE
    SYNTAX Integer32(0..29)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This value indicates the antenna gain reduction for the radio index.(unit: dB)"
    ::= { enterpriseApRadioEntry 28 }

-- ****************************************************************************************
--  enterpriseApSNMP - SNMP MIB
-- ****************************************************************************************


enterpriseApSNMPCommunityReadOnly OBJECT-TYPE
    SYNTAX     DisplayString (SIZE(0..32))
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION "The SNMP Read Only Community.  The value if read,
	             will only show ******."
    ::= { enterpriseApSNMP 1 }

enterpriseApSNMPCommunityReadWrite OBJECT-TYPE
    SYNTAX     DisplayString (SIZE(0..32))
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION "The SNMP Read Write Community.  The value if read,
	             will only show *****."
    ::= { enterpriseApSNMP 2 }

enterpriseApSNMPTrapDestinationTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF EnterpriseApSNMPTrapDestinationEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table of descriptive and status information about
                     configuration of each trap receiving server."
    ::= { enterpriseApSNMP 3 }

enterpriseApSNMPTrapDestinationEntry OBJECT-TYPE
        SYNTAX      EnterpriseApSNMPTrapDestinationEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An entry in the table, containing information
                     about configuration of one trap receiving server."
        INDEX       { enterpriseApSNMPTrapDestinationIndex }
        ::= { enterpriseApSNMPTrapDestinationTable 1 }

EnterpriseApSNMPTrapDestinationEntry ::= SEQUENCE
{
    enterpriseApSNMPTrapDestinationIndex        INTEGER,
    enterpriseApSNMPTrapDestinationCommunity    DisplayString,
    enterpriseApSNMPTrapDestinationIP           IpAddress,
    enterpriseApSNMPTrapDestinationState        INTEGER
}

enterpriseApSNMPTrapDestinationIndex OBJECT-TYPE
        SYNTAX      INTEGER (1..4) 
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Index of the Trap Destination Table."
        ::= { enterpriseApSNMPTrapDestinationEntry 1 }

enterpriseApSNMPTrapDestinationCommunity OBJECT-TYPE
        SYNTAX     DisplayString (SIZE(0..32))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The SNMP Trap Community"
        ::= { enterpriseApSNMPTrapDestinationEntry 2 }

enterpriseApSNMPTrapDestinationIP OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The IP address of the trap receiving server."
        ::= { enterpriseApSNMPTrapDestinationEntry 3 }

enterpriseApSNMPTrapDestinationState OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the trap receiving server is enabled."
        ::= { enterpriseApSNMPTrapDestinationEntry 4 }


enterpriseApSNMPTrapFilters	OBJECT IDENTIFIER ::= { enterpriseApSNMP 4 }

sysSystemUpTrapEnabled OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the sysSystemUp trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 1 }

sysSystemDownTrapEnabled OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the sysSystemDowntrap is enabled."
        ::= { enterpriseApSNMPTrapFilters 2 }

sysRadiusServerChangedTrapEnabled OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the sysRadiusServerChanged trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 3 }

sysConfigFileVersionChangedTrapEnabled OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the sysConfigFileVersionChanged trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 4 }
        
dot11StationAssociationTrapEnabled OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the dot11StationAssociation trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 5 }

dot11StationReAssociationTrapEnabled OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the dot11StationReAssociation trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 6 }

dot11StationAuthenticationTrapEnabled OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the dot11StationAuthentication trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 7 }

dot11StationRequestFailTrapEnabled OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the dot11StationRequestFail trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 8 }

dot11InterfaceBFailTrapEnabled OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the dot11InterfaceBFail trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 9 }

dot11InterfaceAGFailTrapEnabled OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the dot11InterfaceAGFail trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 10 }

dot1xMacAddrAuthSuccessTrapEnabled OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the dot1xMacAddrAuthSuccess trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 11 }

dot1xMacAddrAuthFailTrapEnabled OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the dot1xMacAddrAuthFail trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 12 }

dot1xAuthNotInitiatedTrapEnabled OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the dot1xAuthNotInitiated trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 13 }
        
dot1xAuthSuccessTrapEnabled OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the dot1xAuthSuccess trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 14 }

dot1xAuthFailTrapEnabled OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the dot1xAuthFail trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 15 }

localMacAddrAuthSuccessTrapEnabled OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the localMacAddrAuthSuccess trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 16 }

localMacAddrAuthFailTrapEnabled OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the localMacAddrAuthFail trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 17 }

pppLogonFailTrapEnabled OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the pppLogonFail trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 18 }

iappStationRoamedFromTrapEnabled OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the iappStationRoamedFrom trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 19 }

iappStationRoamedToTrapEnabled OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the iappStationRoamedTo trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 20 }

iappContextDataSentTrapEnabled OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the iappContextDataSent trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 21 }

sntpServerFailTrapEnabled OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the sntpServerFail trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 22 }

dot1xSuppAuthenticatedTrapEnabled OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the dot1xSupplicantAuthenticated 
			 trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 23 }
                                                    
dot11FailedTransmitsTrapEnabled OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the dot11FailedTransmitsTrapEnabled 
			 trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 24 } 


dot11AckFailuresTrapEnabled OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the dot11AckFailuresTrapEnabled 
			 trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 25 }   
        
dot11FcsErrorsTrapEnabled  OBJECT-TYPE
	SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the dot11FcsErrorsTrapEnabled 
			 trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 26 }       

rogueAPDetectedTrapEnabled OBJECT-TYPE
	   SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the RogueAPDetectedTrapEnabled 
			 trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 27 }   

  
 possibleRogueAPDetectedTrapEnabled OBJECT-TYPE
	   SYNTAX INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether the RogueAPDetectedTrapEnabled 
			 trap is enabled."
        ::= { enterpriseApSNMPTrapFilters 28 }       
-- ***************************************************************
--                     EAP Wireless Session Table
-- ***************************************************************

enterpriseApSessionTable OBJECT-TYPE
	SYNTAX		SEQUENCE OF EnterpriseApSessionEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"This table list all sessions (wireless stations) status"
	::= { enterpriseApSession 1 }
	
enterpriseApSessionEntry OBJECT-TYPE
	SYNTAX		EnterpriseApSessionEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"An entry in the table, containing information
		about status and statistics of the wireless station."
    INDEX { enterpriseApSessionIfIndex, enterpriseApSessionStationAddres } 
	::= { enterpriseApSessionTable 1 }

EnterpriseApSessionEntry ::= SEQUENCE 
{
	enterpriseApSessionIfIndex					Integer32,
	enterpriseApSessionStationAddres 			MacAddress,
	enterpriseApSessionAuthenticated			TruthValue,
	enterpriseApSessionAssociated				TruthValue,
	enterpriseApSessionIsForwarding				TruthValue,
	enterpriseApSessionKeyType					INTEGER,
	enterpriseApSessionAssociationId			Integer32,
	enterpriseApSessionLastAuthenticatedTime	TimeTicks,
	enterpriseApSessionAssociatedTime			TimeTicks,
	enterpriseApSessionLastAssociatedTime 		TimeTicks,
	enterpriseApSessionLastDisassociatedTime	TimeTicks,
	enterpriseApSessionTxPacketCount			Counter32,
	enterpriseApSessionRxPacketCount			Counter32,
	enterpriseApSessionTxByteCount				Counter32,
	enterpriseApSessionRxByteCount				Counter32
}

enterpriseApSessionIfIndex OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS	not-accessible
    STATUS      current
    DESCRIPTION 
    	"Interface index for the radio this session is associated
		 with."
    ::= { enterpriseApSessionEntry 1 }
        
enterpriseApSessionStationAddres OBJECT-TYPE 
    SYNTAX		MacAddress 
    MAX-ACCESS	not-accessible 
    STATUS		current 
    DESCRIPTION 
    	"The unique MAC Address of the station for this session." 
    ::= { enterpriseApSessionEntry 2 }

enterpriseApSessionAuthenticated OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"Whether the session is authenticated or not."
	::= { enterpriseApSessionEntry 3 }

enterpriseApSessionAssociated OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"Whether the session is associated or not. It is rare case that 
		not associated stations show up in the table."
	::= { enterpriseApSessionEntry 4 }
	
enterpriseApSessionIsForwarding OBJECT-TYPE
	SYNTAX TruthValue
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"Whether the AP is forwarding the client station traffic (higher level authentication)"
	::= { enterpriseApSessionEntry 5 }
	
enterpriseApSessionKeyType OBJECT-TYPE
	SYNTAX INTEGER
	{
		none(1),
		staticWep(2),
		dynamicWep(3),
		wpaWep(4),
		wpaTkip(5),
		wpaAes(6)
	}	
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The encryption key type used by the station. Note that wpa-wep is not supported"
	::= { enterpriseApSessionEntry 6 }
	
enterpriseApSessionAssociationId OBJECT-TYPE
	SYNTAX Integer32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"The internal association identify number"
	::= { enterpriseApSessionEntry 7 }

enterpriseApSessionLastAuthenticatedTime OBJECT-TYPE
	SYNTAX		TimeTicks
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"This is the time in hundredths of a second last time the client
		is authenticated. Note that a session may be authenticated multiple times. 
		The value is related to the system startup"
	::= { enterpriseApSessionEntry 8 }

enterpriseApSessionAssociatedTime OBJECT-TYPE
	SYNTAX		TimeTicks
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"This is the time in hundredths of a second since the client 
		associated. The value is related to the system startup"
	::= { enterpriseApSessionEntry 9 }
	
enterpriseApSessionLastAssociatedTime OBJECT-TYPE
	SYNTAX		TimeTicks
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"This is the time in hundredths of a second when the client 
		associated in last session. The value is related to the system startup"
	::= { enterpriseApSessionEntry 10 }
	
enterpriseApSessionLastDisassociatedTime OBJECT-TYPE
	SYNTAX		TimeTicks
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION
		"This is the time in hundredths of a second when the client 
		disassociated in last session. The value is related to the system startup"
	::= { enterpriseApSessionEntry 11 }

enterpriseApSessionTxPacketCount OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"This is the number of packets transmitted from the client to the AP. It includes 
         data, control and management packets."
	::= { enterpriseApSessionEntry 12 }

enterpriseApSessionRxPacketCount OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"This is the number of unicast packets transmitted from the AP to the client. 
         It includes data, control and management packets."
	::= { enterpriseApSessionEntry 13 }

enterpriseApSessionTxByteCount OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"This is the number of bytes transmitted from the client to the AP. It 
         includes the bytes of data, control and management packets."
	::= { enterpriseApSessionEntry 14 }

enterpriseApSessionRxByteCount OBJECT-TYPE
	SYNTAX	Counter32
	MAX-ACCESS	read-only
	STATUS	current
	DESCRIPTION
		"This is the number of unicast bytes transmitted from the AP to 
         the client. It includes the bytes of data, control and management 
         packets."
	::= { enterpriseApSessionEntry 15 }


-- **********************************************************************
-- * EnterpriseAPVapRadio TABLE
-- **********************************************************************

enterpriseAPVapRadioTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF EnterpriseAPVapRadioEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table of descriptive and status information about
                     configuration of each radio."
        ::= { enterpriseAPVapRadio 1 }

enterpriseAPVapRadioEntry OBJECT-TYPE
        SYNTAX      EnterpriseAPVapRadioEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An entry in the table, containing information
                     about configuration of one radio of the AP."
        INDEX       { enterpriseAPVapRadioIndex }
        ::= { enterpriseAPVapRadioTable 1 }

EnterpriseAPVapRadioEntry ::= SEQUENCE
{
    enterpriseAPVapRadioIndex          Integer32,
    enterpriseAPVapRadioState          INTEGER,
    enterpriseAPVapRadioClosedSystem   INTEGER,
    enterpriseAPVapRadioMaxAssoc       INTEGER,
    enterpriseAPVapRadioTransmitKey    INTEGER,
	enterpriseAPVapRadioDescription    DisplayString ,
-- 20070307, Eva Hsieh, added 
    enterpriseAPVapRadioAuthTimeoutInterval  Integer32,
    enterpriseAPVapRadioAssocTimeoutInterval Integer32,
    enterpriseAPVapRadioWPA2PMKSALifeTime    Integer32
}

enterpriseAPVapRadioIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Radio Index for configuration."
        ::= { enterpriseAPVapRadioEntry 1 }

enterpriseAPVapRadioState OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the state of the radio interface."
        ::= { enterpriseAPVapRadioEntry 2 }

enterpriseAPVapRadioClosedSystem OBJECT-TYPE
	    SYNTAX     INTEGER
               {
                   enabled(1),
                   disabled(2)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates whether closed system is enabled for this radio interface."
        ::= { enterpriseAPVapRadioEntry 3 }

enterpriseAPVapRadioMaxAssoc OBJECT-TYPE
        SYNTAX INTEGER (1..64)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the max number of clients allowed on this radio interface."
        ::= { enterpriseAPVapRadioEntry 4 }

enterpriseAPVapRadioTransmitKey OBJECT-TYPE
        SYNTAX INTEGER (1..4)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates default transmit key in use for this radio interface."
        ::= { enterpriseAPVapRadioEntry 5 }

enterpriseAPVapRadioDescription OBJECT-TYPE
        SYNTAX DisplayString (SIZE(0..80))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the description for this radio interface."
        ::= { enterpriseAPVapRadioEntry 6 }
 --20070307, Eva Hsieh, added 
    enterpriseAPVapRadioAuthTimeoutInterval  OBJECT-TYPE
        SYNTAX Integer32 (5..60)
        MAX-ACCESS read-write 
        STATUS current
        DESCRIPTION
            "This value indicates the Authentication Timeout interval for this radio interface."
        ::= { enterpriseAPVapRadioEntry 8 }

    enterpriseAPVapRadioAssocTimeoutInterval OBJECT-TYPE
        SYNTAX Integer32 (5..60)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the Association Timeout interval for this radio interface."
        ::= { enterpriseAPVapRadioEntry 9 }

    enterpriseAPVapRadioWPA2PMKSALifeTime OBJECT-TYPE
        SYNTAX Integer32 (1..1440)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the WPA2 PMSA Life Time for this radio interface."
        ::= { enterpriseAPVapRadioEntry 10 }

-- ****************************************************************************************
--  enterpriseApWds Table 
-- ****************************************************************************************


enterpriseApRadioWdsTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF EnterpriseApRadioWdsEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table of configuration information for Wds for each
		Radio interface."
        ::= { enterpriseApRadioWds 1 }

enterpriseApRadioWdsEntry OBJECT-TYPE
        SYNTAX      EnterpriseApRadioWdsEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An entry in the table, containing information
                     about configuration of peer Bridging
		     for one radio of the AP.  The table is indexed by radio 
		     Index (corresponding to enterpriseApRadioTable).  The table does not contain the radio index as
		     a member of the table."
        INDEX       { enterpriseApRadioIndex }
        ::= { enterpriseApRadioWdsTable 1 }

EnterpriseApRadioWdsEntry ::= SEQUENCE
{
	wdsApRole			INTEGER,
    wdsChannelAutoSync  INTEGER,
    wdsMasterSlaveMode  INTEGER
}

wdsApRole OBJECT-TYPE
	    SYNTAX     INTEGER
               {
					roleAp(1),
					roleBridgeMaster(2),
--					roleRepeater(3),
					roleBridge(4)
               }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "This value indicates the role of the Ap for this radio, 
                  roleAp(1):			AP operation.
			      roleBridgeMaster(2): 	Root-Bridge mode.
			      roleBridge(4): 		Bridge Mode. 
			 relay wireless traffic."
        ::= { enterpriseApRadioWdsEntry 1 }

wdsChannelAutoSync OBJECT-TYPE
    SYNTAX INTEGER
    {
        enabled  (1),
        disabled (2)
    }            
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This value indicates the states of channel auto synchronize for this radio."
    ::= { enterpriseApRadioWdsEntry 3 }

wdsMasterSlaveMode OBJECT-TYPE
    SYNTAX INTEGER
    {
        master  (1),
        slave   (2)
    }            
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This value indicates the Master/Slave mode for this radio.
            master (1) To set to master mode.
            slave  (2) To set to slave mode."
    ::= { enterpriseApRadioWdsEntry 4 }
-- ****************************************************************************************
--  enterpriseApRadioWdsPeer Table 
-- ****************************************************************************************
enterpriseApRadioWdsPeerTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF EnterpriseApRadioWdsPeerEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Table of configuration information for Wds Peers for each
		Radio interface."
        ::= { enterpriseApRadioWds 2 }
        
enterpriseApRadioWdsPeerEntry OBJECT-TYPE
        SYNTAX      EnterpriseApRadioWdsPeerEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An entry in the table, containing information
                     about configuration of peer Bridging
					 for one radio of the AP.  The table is indexed by radio 
					 Index (corresponding to enterpriseApRadioTable) and the peer
					 index (Up to 8).  The table does not contain the radio index as
					 a member of the table."
        INDEX       { enterpriseApRadioIndex, wdsPeerIndex }
        ::= { enterpriseApRadioWdsPeerTable 1 }

EnterpriseApRadioWdsPeerEntry ::= SEQUENCE
{
    wdsPeerIndex                    Integer32,
    wdsPeerBssid                    DisplayString
}

wdsPeerIndex OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Peer Index for the radio interface."
        ::= { enterpriseApRadioWdsPeerEntry 1 }

wdsPeerBssid OBJECT-TYPE
	SYNTAX     DisplayString (SIZE(1..6))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The BSSID for this peer."
        ::= { enterpriseApRadioWdsPeerEntry 2 }    

--************************************************************************************************
-- enterpriseApWMMTable
--************************************************************************************************
enterpriseApWMMTable OBJECT-TYPE
    SYNTAX SEQUENCE OF EnterpriseApWMMEntry
    MAX-ACCESS not-accessible
    STATUS current 
    DESCRIPTION 
        "The table of WMM information for each radio interface."
    ::= { enterpriseApWMM 1 }

enterpriseApWMMEntry OBJECT-TYPE
    SYNTAX EnterpriseApWMMEntry   
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "An entry of table, contains the WMM information." 
    INDEX  { enterpriseApWMMModeIndex }
    ::= { enterpriseApWMMTable 1 }
    
EnterpriseApWMMEntry ::= SEQUENCE
{
    enterpriseApWMMModeIndex Integer32,
    enterpriseApWMMMode      INTEGER,
}

enterpriseApWMMModeIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS not-accessible
    STATUS current 
    DESCRIPTION 
        "Peer Index for the radio interface."
    ::= { enterpriseApWMMEntry 1 }

enterpriseApWMMMode  OBJECT-TYPE
    SYNTAX INTEGER
    {
        disabled(1),
        support (2),
        required(3)
    } 
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This value indicates the WMM mode for the radio interface.
             disabled(1)  To set WMM mode disabled.
             support (2)  To set WMM mode supported.
             required(3)  To set WMM mode required." 
    ::= { enterpriseApWMMEntry 2 } 

--************************************************************************************************
-- enterpriseApWMMAckPolicyTable 
--************************************************************************************************
enterpriseApWMMAckPolicyTable OBJECT-TYPE
    SYNTAX SEQUENCE OF EnterpriseApWMMAckPolicyEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION 
        "The table of WMM Ack Policy information for each ac number on the radio interface."
    ::= { enterpriseApWMM 2 } 

enterpriseApWMMAckPolicyEntry OBJECT-TYPE
    SYNTAX EnterpriseApWMMAckPolicyEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION 
        "An entry of table, contains the WMM Ack Policy information."
    INDEX { enterpriseApWMMAckPolicyIndex }
    ::= { enterpriseApWMMAckPolicyTable 1 } 

EnterpriseApWMMAckPolicyEntry ::= SEQUENCE
{
    enterpriseApWMMAckPolicyIndex Integer32,
    enterpriseApWMMACKPolicy INTEGER,
}

enterpriseApWMMAckPolicyIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current 
    DESCRIPTION 
      "The value indicates the AC number for each radio interface.
        0 --> AC0 (Best Effect)
        1 --> AC1 (Background)
        2 --> AC2 (Video)
        3 --> AC3 (Voice)"
     ::= { enterpriseApWMMAckPolicyEntry 1 }
   
enterpriseApWMMACKPolicy OBJECT-TYPE
    SYNTAX INTEGER
    {
        acknowledge(1),
        NoAcknowledge(2)
    }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This value indicates WMM Ack Policy state of each ac number for the radio interface."
    ::= { enterpriseApWMMAckPolicyEntry 2 }

--************************************************************************************************
-- enterpriseApWMMBSSParameterTable 
--************************************************************************************************
enterpriseApWMMBSSParamTable OBJECT-TYPE
    SYNTAX SEQUENCE OF EnterpriseApWMMBSSParamEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of WMM BSS parameter information."
    ::= { enterpriseApWMM 3 }

enterpriseApWMMBSSParamEntry OBJECT-TYPE
    SYNTAX EnterpriseApWMMBSSParamEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "An entry of table, contains the WMM BSS parameter information for each ac number on the radio interface."
    INDEX { enterpriseApWMMBSSParamIndex }
    ::= { enterpriseApWMMBSSParamTable 1 }

EnterpriseApWMMBSSParamEntry ::= SEQUENCE
{
    enterpriseApWMMBSSParamIndex      Integer32,
    enterpriseApWMMBSSParamLogCwMin   Integer32,
    enterpriseApWMMBSSParamLogCwMax   Integer32,
    enterpriseApWMMBSSParamAIFSN      Integer32,
    enterpriseApWMMBSSParamTXOPLimit  Integer32,
    enterpriseApWMMBSSParamAdmissionCtrl INTEGER
}

enterpriseApWMMBSSParamIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
      "The value indicates the AC number for each radio interface.
        0 --> AC0 (Best Effort)
        1 --> AC1 (Background)
        2 --> AC2 (Video)
        3 --> AC3 (Voice)"
     ::= { enterpriseApWMMBSSParamEntry 1 } 

enterpriseApWMMBSSParamLogCwMin OBJECT-TYPE
    SYNTAX Integer32(1..15)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This value indicates the WMM BSS parameter logCwMin of AC number for the radio interface."
    ::= { enterpriseApWMMBSSParamEntry 2 } 
    
enterpriseApWMMBSSParamLogCwMax OBJECT-TYPE
    SYNTAX Integer32(1..15)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This value indicates the WMM BSS parameter logCwMax of each AC number for the radio interface."
    ::= { enterpriseApWMMBSSParamEntry 3 } 

enterpriseApWMMBSSParamAIFSN OBJECT-TYPE
    SYNTAX Integer32(1..15)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This value indicates the WMM BSS parameters AIFSN of each AC number for the radio interface."
    ::= { enterpriseApWMMBSSParamEntry 4 }

enterpriseApWMMBSSParamTXOPLimit OBJECT-TYPE
    SYNTAX Integer32(0..65535)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This value indicates the WMM BSS parameters TXOP Limit of each AC number for the radio interface."
    ::= { enterpriseApWMMBSSParamEntry 5 }

enterpriseApWMMBSSParamAdmissionCtrl OBJECT-TYPE
    SYNTAX INTEGER
    {
        ebabled (1),
        disabled(2)
    }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This value indicates the BSS parameters Admission Control of each AC number for the radio interface."
    ::= { enterpriseApWMMBSSParamEntry 6 }

--************************************************************************************************
-- enterpriseApWMMAPParameterTable 
--************************************************************************************************
enterpriseApWMMAPParamTable OBJECT-TYPE
    SYNTAX SEQUENCE OF EnterpriseApWMMAPParamEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of configuration information for WMM AP parameters for each ac number on the radio interface."
    ::= { enterpriseApWMM 4 }

enterpriseApWMMAPParamEntry OBJECT-TYPE
    SYNTAX EnterpriseApWMMAPParamEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "An entry table, include the Ap parameter information for each ac numbers."
    INDEX { enterpriseApWMMAPParamIndex }
    ::= { enterpriseApWMMAPParamTable 1 }

EnterpriseApWMMAPParamEntry ::= SEQUENCE
{
    enterpriseApWMMAPParamIndex      Integer32,
    enterpriseApWMMAPParamLogCwMin   Integer32,
    enterpriseApWMMAPParamLogCwMax   Integer32,
    enterpriseApWMMAPParamAIFSN      Integer32,
    enterpriseApWMMAPParamTXOPLimit  Integer32,
    enterpriseApWMMAPParamAdmissionCtrl INTEGER
}

enterpriseApWMMAPParamIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
      "The value indicates the AC number for each radio interface.
        0 --> AC0 (Best Effort)
        1 --> AC1 (Background)
        2 --> AC2 (Video)
        3 --> AC3 (Voice)"
    ::= { enterpriseApWMMAPParamEntry 1 } 

enterpriseApWMMAPParamLogCwMin OBJECT-TYPE
    SYNTAX Integer32(1..15)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This value indicates the LogCwMin of AP parameter for each AC number on the radio interface."
    ::= { enterpriseApWMMAPParamEntry 2 } 
    
enterpriseApWMMAPParamLogCwMax OBJECT-TYPE
    SYNTAX Integer32(1..15)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This value indicates the LogCwMax of AP parameter for each AC number on the radio interface."
    ::= { enterpriseApWMMAPParamEntry 3 } 

enterpriseApWMMAPParamAIFSN OBJECT-TYPE
    SYNTAX Integer32(1..15)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This value indicates the AIFSN of AP parameter for each AC number on the radio interface."
    ::= { enterpriseApWMMAPParamEntry 4 }

enterpriseApWMMAPParamTXOPLimit OBJECT-TYPE
    SYNTAX Integer32(0..65535)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This value indicates the TXOP Limit of AP parameter for each AC number on the radio interface."
    ::= { enterpriseApWMMAPParamEntry 5 }

enterpriseApWMMAPParamAdmissionCtrl OBJECT-TYPE
    SYNTAX INTEGER
    {
        ebabled (1),
        disabled(2)
    }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This value indicates the admission control of AP parameter for each AC number on the radio interface."
    ::= { enterpriseApWMMAPParamEntry 6 }

                   
-- ****************************************************************************************
--  enterpriseApSpanningTreeProtocol Table 
-- ****************************************************************************************

enterpriseApSTPBridgeStatus OBJECT-TYPE
    SYNTAX INTEGER
    {
        enabled  (1),
        disabled (2)
    }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION 
        "This value indicates the STP bridge status for the radio interface."    
    ::= { enterpriseApSTP 1 } 
    
enterpriseApSTPBridgePriority OBJECT-TYPE 
    SYNTAX Integer32(0..65535)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This value indicates the STP bridge priority for the radio interface."
    ::= { enterpriseApSTP 2 }

enterpriseApSTPBridgeMaxAge OBJECT-TYPE
    SYNTAX Integer32(6..40)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This value indicates the STP bridge max age for the radio interface.(unit: second)"
    ::= { enterpriseApSTP 3 }

enterpriseApSTPHelloTime OBJECT-TYPE
    SYNTAX Integer32(1..10)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This value indicates the STP hello time for the radio interface.(unit: second)"
    ::= { enterpriseApSTP 4 }

enterpriseApSTPBridgeForwardingDelay OBJECT-TYPE
    SYNTAX Integer32(4..30)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This value indicates the STP forwarding delay for the radio interface.(unit: second)"
    ::= { enterpriseApSTP 5 }

--************************************************************************************************
-- enterpriseApSTP
--************************************************************************************************
enterpriseApSTPRadioInterface OBJECT IDENTIFIER ::= { enterpriseApSTP 6 }

enterpriseApSTPNodeTable OBJECT-TYPE
    SYNTAX SEQUENCE OF EnterpriseApSTPNodeEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of STP link Path Cost and link port priority information for each nodes on radio interface."
    ::= { enterpriseApSTPRadioInterface 1 }   

enterpriseApSTPNodeEntry OBJECT-TYPE
    SYNTAX EnterpriseApSTPNodeEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "An entry in a table, contain the link path cost and link port priroity information."
    INDEX { enterpriseApSTPNodeIndex }
    ::= { enterpriseApSTPNodeTable 1 }

EnterpriseApSTPNodeEntry  ::= SEQUENCE
{
    enterpriseApSTPNodeIndex            Integer32,
    enterpriseApSTPNodeLinkPathCost     Integer32,
    enterpriseApSTPNodeLinkPortPriority Integer32
}

enterpriseApSTPNodeIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Peer Index for the nodes on the radio interface."
    ::= { enterpriseApSTPNodeEntry 1 }

enterpriseApSTPNodeLinkPathCost OBJECT-TYPE
    SYNTAX Integer32(1..65535)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This value indicates the link path cost for the node on this radio interface."
    ::= { enterpriseApSTPNodeEntry 2 }

enterpriseApSTPNodeLinkPortPriority OBJECT-TYPE
    SYNTAX Integer32(0..255)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This value indicates the link path cost for the node on this radio interface."
    ::= { enterpriseApSTPNodeEntry 3 }


--************************************************************************************************
-- enterpriseApSTPEthernetInterface
--************************************************************************************************

enterpriseApSTPEthernetInterface OBJECT IDENTIFIER ::= { enterpriseApSTP 7 }

enterpriseApSTPEthernetLinkPathCost OBJECT-TYPE
    SYNTAX Integer32(1..65535)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This value indicates link path cost for ethernet interface."   
    ::= { enterpriseApSTPEthernetInterface 1 } 
    
enterpriseApSTPEthernetLinkPortPriority OBJECT-TYPE
    SYNTAX Integer32(0..255)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "This value indicates link port prirorty for ethernet interface."   
    ::= { enterpriseApSTPEthernetInterface 2 }

--************************************************************************************************
-- enterpriseApSTP end
--************************************************************************************************
END

