-- COPYRIGHT NOTICE
-- Copyright (c) Nortel Networks, 2004
-- All rights reserved
-- 
-- HISTORY
-- $Log: aosphysical.mib,v $
-- Revision 1.1  2007/10/17 01:09:54  jeneric
-- 10/07 mib updates
--
-- Revision submit_cheetah_18020/1 2006/04/08 13:51:32 rvakkala
-- Fixed Q01310786 Adde support for /i/l2/team.
-- 
-- Revision submit_cheetah_16636/1 2006/01/10 04:46:36 rvakkala
-- Deleted flag which is bounded to stpInfoPortState discard vlaue.
-- 
-- Revision submit_cheetah_16394/1 2005/12/05 18:37:27 bshao
-- CR 1223294: Dynamically compile out MIB objects that are 
-- not applicable to the product.
-- 
-- Revision submit_cheetah_15706/2 2005/11/22 06:59:53 rvakkala
-- Fixed CRQ01218971 stpInfoPortState MIB does not have
-- discarding value.
-- 
-- Revision submit_cheetah_15676/1 2005/11/11 13:53:06 rvakkala
-- Fixed CRQ01242511 stgNewCfgPortPathCost MIB cannot set value
-- more than 65535.
-- 
-- Revision submit_cheetah_15706/1 2005/11/22 06:47:22 rvakkala
-- Fixed CRQ01218971 stpInfoPortState MIB does not
-- have discarding value
-- 
-- Revision submit_cheetah_13965/1 2005/09/20 05:34:53 angamuth
-- Added MIBs port role, link type and edge type in stpInfo
-- for RSTP mode.
-- 
-- Revision submit_cheetah_13814/1 2005/08/17 04:43:58 joju
-- Revert fixes for Q01011874-01,Q01011868-01.
-- 
-- Revision submit_cheetah_13639/2 2005/08/12 07:24:25 joju
-- Merged with others.
-- 
-- Revision submit_cheetah_13685/1 2005/08/11 19:08:50 rrekha
-- More cleanup of excludes from the Makefile. Moved them
-- to #if defines in the corresponding *.ctl_raw and *.mib_raw files.
-- 
-- Revision submit_cheetah_13639/1 2005/08/12 07:15:15 joju
-- SUBMIT DESCRIPTION: Change range from (1..65535) to (0..65535) for commands
-- /cfg/l2/lacp/sysprio
-- /cfg/l2/lacp/port/prio
-- /c/l2/mrst/version
-- 
-- Revision submit_cheetah_13563/1 2005/08/05 17:39:30 rrekha
-- Moved all the BWM related flags into the raw files.
-- 
-- Revision submit_cheetah_11345/1 2005/03/30 02:30:15 rrekha
-- Remove the range for the VlanID since it defers in 
-- Cheetah/Elmo/Zoe. Added a new MIB variable vlanMaxVlanID which
-- will give the max. value for the VLAN ID.
-- 
-- Revision submit_cheetah_11335/1 2005/03/29 21:28:59 yatsze
-- Add MIB for PORT_TEAM
-- 
-- Revision submit_cheetah_11294/1 2005/03/28 20:37:30 yatsze
-- Add portTeamCfg objects
-- 
-- Revision submit_cheetah_10834/1 2005/02/08 11:51:23 dillibab
-- Added SNMP support for VLAN Info.
-- 
-- Revision submit_cheetah_10393/1 2005/01/05 21:01:32 mmacnt
-- code reorg - moved from lib/agent
-- 
-- Revision submit_cheetah_10219/1 2004/11/16 18:45:44 dillibab
-- Added SNMP objects to configure STP Port Link Type and Edge State.
-- 
-- Revision submit_cheetah_10162/1 2004/11/10 18:49:52 bshao
-- CR 1016054: Changed VLAN range to 0..4095.
-- 
-- Revision submit_cheetah_10075/1 2004/11/04 18:53:25 bshao
-- CR 1016467: Changed CIST port priority in SNMP/BBI to
-- 0 - 240.
-- 
-- Revision submit_cheetah_10051/1 2004/11/03 01:29:32 bshao
-- Cr 1016469: Changed mst___CfgMaxHopCount to range from
-- 4 .. 60
-- 
-- Revision submit_cheetah_9239/1 2004/09/08 00:44:56 rrekha
-- Cleanup L2 related flags.
-- 
-- Revision submit_cheetah_9196/1 2004/09/01 21:43:12 rrekha
-- Minor changes for SMIv2 compliance.
-- 
-- Revision submit_cheetah_8623/1 2004/08/03 18:43:22 rrekha
-- Moved QOS configuration to a new mib.
-- 
-- Revision submit_cheetah_8578/1 2004/07/30 00:36:28 rrekha
-- Update the copyright header.
-- 
-- Revision submit_cheetah_8500/1 2004/07/26 21:40:38 rrekha
-- Added ZOE related mibs from /src/bert/lib/agent directory.
-- 
-- Revision submit_cheetah_8441/1 2004/07/20 23:36:24 vprayaga
-- Added description for lacpInfoPortTable MIB objects.
-- 
-- Revision submit_cheetah_8294/1 2004/07/13 22:47:08 rrekha
-- Obsoleted stgCurCfgVlanBmap1, stgCurCfgVlanBmap2, stgNewCfgVlanBmap1
-- and stgNewCfgVlanBmap2.
-- Obosleted pmCurCfgPmirrPortVlansBmap1, pmCurCfgPmirrPortVlansBmap2,
-- pmNewCfgPmirrPortVlansBmap1 and pmNewCfgPmirrPortVlansBmap2.
-- 
-- Revision submit_cheetah_8277/1 2004/07/12 14:57:33 rrekha
-- Fixed Q00944149: Add lacpPortInfoTable for missing information.
-- 
-- Revision submit_cheetah_7777/2 2004/06/15 15:08:48 dillibab
-- Merged with previous changes.
-- 
-- Revision submit_cheetah_7748/1 2004/06/10 17:35:41 rrekha
-- Fixed Q00923538: Correct range for lacpur/NewCfgSystemPriority.
-- Fixed Q00923594: Correct range for lacpCur/NewCfgPortActorAdminKey.
-- Fixed Q00923600: Correct range for lacpCur/NewCfgPortActorPortPriority.
-- 
-- Revision submit_cheetah_7777/1 2004/06/15 09:16:21 dillibab
-- Added SNMP object for STP Statistics.
-- 
-- Revision submit_cheetah_7576/1 2004/05/27 10:16:49 dillibab
-- Added new vlan bitmap object to represent splitted vlan bitmaps into single object.
-- 
-- Revision submit_cheetah_5917/1 2003/12/12 21:55:35 rmundhra
-- Porting SNMP/BBI support for Elmo Trunk Hash from 
-- elmof_1.0.0.0int branch.
-- 
-- Revision submit_cheetah_5822/1 2003/12/09 03:03:21 dleu
-- Q00789469: changed the term "Teaming" to "Failover". 
-- For Elmo only.
-- 
-- Revision submit_cheetah_5841/1 2003/12/05 22:58:08 rrekha
-- Converted MIBs to SMIv2.
-- 
-- Revision submit_cheetah_5311/1 2003/10/17 00:03:02 dleu
-- Added SNMP/WebUI support for ELMO_TEAMING_TRUNK.
-- 
-- Revision submit_cheetah_5363/1 2003/10/16 02:01:47 vprayaga
-- Added Cur and New MIBs for lacp group.
-- 
-- Revision submit_cheetah_5342/1 2003/10/15 03:28:55 vprayaga
-- Added private MIBs for LACP feature.
-- 
-- Revision submit_cheetah_4435/1 2003/08/12 22:59:54 rrekha
-- Changed name of mib file for cheetah*.mib to aos*.mib.
-- 
-- Revision submit_cheetah_3099/1 2003/05/13 14:17:49 yatsze
-- Add new object fdbSrcTrunk
-- 
-- Revision submit_cheetah_2843/1 2003/04/29 00:26:51 vprayaga
-- Corrected description of port mirroring features mib elements.
-- 
-- Revision submit_cheetah_2825/1 2003/04/28 22:07:24 vprayaga
-- Updated CFG_STATIC_ARP/port mirroring mibs as per
-- wendell suggestions.
-- 
-- Revision submit_cheetah_2813/1 2003/04/26 02:47:30 vprayaga
-- Added SNMP support for VLAN traffic mirroring per port.
-- 
-- Revision submit_cheetah_2784/1 2003/04/24 20:33:09 yuhuang
-- Added MIB objects vlanCurCfgLearn and vlanNewCfgLearn for the 
-- VLAN source mac learning control.
-- 
-- Revision submit_cheetah_2695/1 2003/04/18 21:36:16 rrekha
-- Added object stpInfoPortPathCost.
-- 
-- Revision submit_cheetah_2494/3 2003/04/02 21:56:10 mp1
-- added Jumbo access
-- 
-- Revision submit_cheetah_2488/1 2003/04/02 20:00:42 rrekha
-- Added stpInfoTable and stpInfoPortTable in private MIB since
-- with SNMPv3 the standard mibs cannot be used as they do not support
-- multiple STPs.
-- 
-- Revision submit_cheetah_2476/1 2003/04/02 00:29:31 rrekha
-- Since SNMPv3 does not use community strings which was used
-- to specify the STP number previously added private mibs for 
-- STP configuration as RFC 1493 does not provide for configuration
-- of multiple STPs. With this change using SNMPv3 the RFC mibs 
-- will always return only the STP 1 configuration.
-- 
-- Revision submit_cheetah_1919/1 2003/02/05 20:05:58 rrekha
-- Changed the include paths for integrating support
-- for SNMP V3 Windmanage Stack.
-- 
-- Revision submit_cheetah_1583/1 2002/11/27 00:14:04 rmundhra
-- Fixed CR Q00570451: EMS: Monitor>Bridge>Fwd database
-- shows different SP than telnet.
-- 
-- Revision submit_cheetah_1573/1 2002/11/26 18:15:22 rmundhra
-- Modified the range for vlan entries to be 4090
-- for Cheetah switches as the other 4 entries are 
-- going to be used internally.
-- 
-- Revision submit_cheetah_1546/1 2002/11/21 01:04:10 rrekha
-- Fixed Q00546520 : Added FDB table in the private mib since
-- the standard mib table dot1dTpFdbTable does not have all the 
-- columns.
-- 
-- Revision submit_cheetah_1109/1 2002/10/02 23:32:30 rrekha
-- Fixed Q00533514: Added MIB object fdbClear to clear the 
-- FDB.
-- 
-- Revision submit_cheetah_217/1 2002/06/26 20:27:30 rrekha
-- Modified some of the incorrect ranges. Also removed ranges
-- for table indices as these should be obtained from the max
-- table sizes. Fixed typos in BGP mibs.
-- 
-- Revision submit_cheetah_20/1 2002/06/06 23:11:02 mmacnt
-- testing submit
-- 
-- Revision submit_cheetah_13/1 2002/06/06 22:56:43 rrekha
-- Correct description for fdbStatsFinds.
-- 
-- Revision ch_1_0_0_dev/4 2002/06/04 21:48:06 rrekha
-- Added MIB objects for FDB statistics.
-- 
-- Revision ch_1_0_0_dev/3 2002/04/23 21:47:11 smiao
-- Renamed node cheetah to aws-switches.
-- 
-- Revision ch_1_0_0_dev/2 2002/03/19 04:51:30 smiao
-- Removed port mirroring operation for SNMP and webUI.
-- 
-- Revision ch_1_0_0_dev/1 2002/03/07 19:01:55 smiao
-- Removed unnecssary MIB objects for CHEEATH.
-- 
-- Revision ch10latest_smiao/2 2002/02/13 01:41:24 smiao
-- 	Initial checked in for cheetah MIB files.
-- 
-- $EndLog$
--

ALTEON-CS-PHYSICAL-MIB DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Integer32, Counter32, Gauge32, TimeTicks
        FROM SNMPv2-SMI
    DisplayString, PhysAddress
        FROM SNMPv2-TC
    aws-switch 
        FROM ALTEON-ROOT-MIB;

layer2 MODULE-IDENTITY
    LAST-UPDATED "200409010000Z" --  1 September, 2004
    ORGANIZATION "Nortel Networks"
    CONTACT-INFO "Rekha Singamsetty
                  Suresh Batchu

                  Nortel Networks
                  4655 Great America Parkway
                  Santa Clara CA 95054

                  +1 408 495 2400
                  rrekha@nortelnetworks.com
                  sbatchu@nortelnetworks.com"
    DESCRIPTION
        "The MIB module for the Alteon OS Layer2 configuration, statistics and 
         information ."
    REVISION "200409010000Z"     -- 1 September, 2004
    DESCRIPTION
        "Added revision clause for SMIv2 compliance."
    ::= { aws-switch 2 }


    BridgeId ::= OCTET STRING (SIZE (8))
    
    
layer2Configs     OBJECT IDENTIFIER ::= { layer2 1 }
layer2Stats       OBJECT IDENTIFIER ::= { layer2 2 }
layer2Info        OBJECT IDENTIFIER ::= { layer2 3 }
layer2Oper        OBJECT IDENTIFIER ::= { layer2 4 }

vlan              OBJECT IDENTIFIER ::= { layer2Configs 1 }
trunkgroup        OBJECT IDENTIFIER ::= { layer2Configs 2 }
stgCfg            OBJECT IDENTIFIER ::= { layer2Configs 3 }
mirroring         OBJECT IDENTIFIER ::= { layer2Configs 4 }
lacp              OBJECT IDENTIFIER ::= { layer2Configs 5 }
mstCfg            OBJECT IDENTIFIER ::= { layer2Configs 7 }
portTeamCfg       OBJECT IDENTIFIER ::= { layer2Configs 9 }


mirrPortMirr      OBJECT IDENTIFIER ::= { mirroring 1 }

mstGeneralCfg     OBJECT IDENTIFIER ::= { mstCfg 1 }
mstCistCfg        OBJECT IDENTIFIER ::= { mstCfg 2 }

fdbStats	  OBJECT IDENTIFIER ::= { layer2Stats 1 }
stpStats	  OBJECT IDENTIFIER ::= { layer2Stats 2 }

fdbInfo 	  OBJECT IDENTIFIER ::= { layer2Info 1 }
stpInfo           OBJECT IDENTIFIER ::= { layer2Info 2 }
lacpInfo          OBJECT IDENTIFIER ::= { layer2Info 3 }
cistInfo          OBJECT IDENTIFIER ::= { layer2Info 4 }
vlanInfo          OBJECT IDENTIFIER ::= { layer2Info 5 }

cistGeneralInfo   OBJECT IDENTIFIER ::= { cistInfo 1 }

portTeamInfo      OBJECT IDENTIFIER ::= { layer2Info 6  }

-- VLAN group
vlanMaxEnt OBJECT-TYPE
    SYNTAX  Integer32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The maximum number of rows in the VLAN configuration table."
    ::= { vlan 1 }

vlanMaxVlanID OBJECT-TYPE
    SYNTAX  Integer32 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The maximum allowed VLAN ID."
    ::= { vlan 4 }

vlanCurCfgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF VlanCurCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of VLAN configuration."
    ::= { vlan 2 }

vlanCurCfgTableEntry OBJECT-TYPE
    SYNTAX  VlanCurCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the VLAN configuration table."
    INDEX  { vlanCurCfgVlanId }
    ::= { vlanCurCfgTable 1 }

VlanCurCfgTableEntry ::= SEQUENCE {
    vlanCurCfgVlanId 		Integer32,
    vlanCurCfgPorts 		OCTET STRING,
    vlanCurCfgState 		INTEGER,
    vlanCurCfgBwmContract	Integer32,
    vlanCurCfgStg  	        Integer32,
    vlanCurCfgJumbo  	        INTEGER,
    vlanCurCfgLearn             INTEGER, 
    vlanCurCfgVlanName 		DisplayString
    }

vlanCurCfgVlanId OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The VLAN identifier."
    ::= { vlanCurCfgTableEntry 1 }

vlanCurCfgVlanName OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..32))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The VLAN name."
    ::= { vlanCurCfgTableEntry 2 }

vlanCurCfgPorts	OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port list in the VLAN. The ports are presented in bitmap format.
	 in receiving order:

	     OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx ..... 
             ||    || |_ port 8
             ||    ||  
             ||    ||___ port 7
             ||    |____ port 6
             ||      .    .   .
             ||_________ port 1
             |__________ reserved

         where x : 1 - The represented port belongs to the VLAN
		   0 - The represented port does not belong to the VLAN"
    ::= { vlanCurCfgTableEntry 3 }

vlanCurCfgState	OBJECT-TYPE
    SYNTAX  INTEGER  {
	enabled(2),
	disabled(3)
	}
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable a VLAN"
    ::= { vlanCurCfgTableEntry 4 }

vlanCurCfgBwmContract OBJECT-TYPE
    SYNTAX  Integer32  
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Default contract number the VLAN "
    ::= { vlanCurCfgTableEntry 5 }

vlanCurCfgStg OBJECT-TYPE
    SYNTAX  Integer32  
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Spanning Tree Group for the VLAN."
    ::= { vlanCurCfgTableEntry 6 }

vlanCurCfgJumbo	OBJECT-TYPE
    SYNTAX  INTEGER  {
	enabled(2),
	disabled(3)
	}
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable Jumbo frames on a VLAN"
    ::= { vlanCurCfgTableEntry 7 }

vlanCurCfgLearn OBJECT-TYPE
    SYNTAX  INTEGER  {
        enabled(2),
        disabled(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable source MAC address learning on a VLAN"
    ::= { vlanCurCfgTableEntry 8 }

vlanNewCfgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF VlanNewCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of VLAN configuration."
    ::= { vlan 3 }

vlanNewCfgTableEntry OBJECT-TYPE
    SYNTAX  VlanNewCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the VLAN configuration table."
    INDEX  { vlanNewCfgVlanId }
    ::= { vlanNewCfgTable 1 }

VlanNewCfgTableEntry ::= SEQUENCE {
    vlanNewCfgVlanId 		Integer32,
    vlanNewCfgVlanName 		DisplayString,
    vlanNewCfgPorts 		OCTET STRING,
    vlanNewCfgState 		INTEGER,
    vlanNewCfgAddPort 		Integer32,
    vlanNewCfgRemovePort	Integer32,
    vlanNewCfgBwmContract	Integer32,
    vlanNewCfgStg  	        Integer32,
    vlanNewCfgJumbo	        INTEGER,
    vlanNewCfgLearn             INTEGER,
    vlanNewCfgDelete 		INTEGER
    }

vlanNewCfgVlanId OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The VLAN identifier."
    ::= { vlanNewCfgTableEntry 1 }

vlanNewCfgVlanName OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..32))
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The VLAN name."
    ::= { vlanNewCfgTableEntry 2 }

vlanNewCfgPorts	OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port list in the VLAN.  The ports are presented in bitmap format.
         in receiving order:

	     OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx ..... 
             ||    || |_ port 8
             ||    ||  
             ||    ||___ port 7
             ||    |____ port 6
             ||      .    .   .
             ||_________ port 1
             |__________ reserved

         where x : 1 - The represented port belongs to the VLAN
	           0 - The represented port does not belong to the VLAN"
    ::= { vlanNewCfgTableEntry 3 }

vlanNewCfgState	OBJECT-TYPE
    SYNTAX  INTEGER  {
	enabled(2),
	disabled(3)
	}
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Enable or disable a VLAN"
    ::= { vlanNewCfgTableEntry 4 }

vlanNewCfgAddPort OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The port to be added to the specified VLAN.  A '0' value is 
         returned when read."
    ::= { vlanNewCfgTableEntry 5 }

vlanNewCfgRemovePort OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The port to be removed from the specified VLAN.  A '0'
         value is returned when read."
    ::= { vlanNewCfgTableEntry 6 }

vlanNewCfgDelete OBJECT-TYPE
    SYNTAX  INTEGER  {
        other(1),
        delete(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "This is an action object to create or delete a VLAN.
         other(1) is returned always when read.
         The following values are writable: delete(2)...to delete a VLAN"
    ::= { vlanNewCfgTableEntry 7 }

vlanNewCfgBwmContract OBJECT-TYPE
    SYNTAX  Integer32  
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Default contract number for the VLAN."
    ::= { vlanNewCfgTableEntry 8 }

vlanNewCfgStg OBJECT-TYPE
    SYNTAX  Integer32  
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The Spanning Tree Group for the VLAN."
    ::= { vlanNewCfgTableEntry 9 }

vlanNewCfgJumbo	OBJECT-TYPE
    SYNTAX  INTEGER  {
	enabled(2),
	disabled(3)
	}
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Enable or disable Jumbo frames on a VLAN"
    ::= { vlanNewCfgTableEntry 10 }

vlanNewCfgLearn OBJECT-TYPE
    SYNTAX  INTEGER  {
        enabled(2),
        disabled(3)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Enable or disable source mac address learning on a VLAN"
    ::= { vlanNewCfgTableEntry 11 }

-- Link Aggregation Control Protocol Group
lacpCurSystemPriority OBJECT-TYPE
    SYNTAX  INTEGER (1..65535)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
       "A 2-octet read-write value indicating the priority
        value associated with the Actor's System ID."
    ::= { lacp 1 }

lacpNewSystemPriority OBJECT-TYPE
    SYNTAX  INTEGER (1..65535)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "A 2-octet read-write value indicating the priority
        value associated with the Actor's System ID."
    ::= { lacp 2 }

lacpCurSystemTimeoutTime OBJECT-TYPE
    SYNTAX  INTEGER  {
        short(3),
        long(90)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "If a port does not receive LACPDUs for Timeout time LACP 
         information pertaining to the port is invalidated.
         Its every 3 sec (short) and every 90 sec (long 3)."
    ::= { lacp 5 }

lacpNewSystemTimeoutTime OBJECT-TYPE
    SYNTAX  INTEGER  {
        short(3),
        long(90)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "If a port does not receive LACPDUs for Timeout time LACP 
         information pertaining to the port is invalidated.
         Its every 3 sec (short) and every 90 sec (long 3)."
    ::= { lacp 6 }

lacpCurPortCfgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF LacpCurPortCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of LACP port configuration."
    ::= { lacp 7 }

lacpCurPortCfgTableEntry OBJECT-TYPE
    SYNTAX  LacpCurPortCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the LACP port configuration table."
    INDEX  { lacpCurPortCfgTableId }
    ::= { lacpCurPortCfgTable 1 }

LacpCurPortCfgTableEntry ::= SEQUENCE {
    lacpCurPortCfgTableId 	    Integer32,
    lacpCurPortState                INTEGER, 
    lacpCurPortActorPortPriority    INTEGER, 
    lacpCurPortActorAdminKey        INTEGER 
    }

lacpCurPortCfgTableId OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
          " LACP port number."
    ::= { lacpCurPortCfgTableEntry 1 }

lacpCurPortState OBJECT-TYPE
    SYNTAX  INTEGER  {
        off(1),
        active(2),
        passive(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "LACP port state can be one of three states 
         off (Not participating in LACP) 
         Active (Initiates LACPDU updates)
         Passive (Does not initiate LACPDU updates but responds to peer."
    ::= { lacpCurPortCfgTableEntry 2 }

lacpCurPortActorPortPriority OBJECT-TYPE
    SYNTAX       INTEGER (1..65535)
    MAX-ACCESS       read-only
    STATUS       current
    DESCRIPTION
        "The priority value assigned to this Aggregation Port.
        This 16-bit value is read-only."
    ::= { lacpCurPortCfgTableEntry 3 }

lacpCurPortActorAdminKey OBJECT-TYPE
    SYNTAX       INTEGER (1..65535)
    MAX-ACCESS       read-only
    STATUS       current
    DESCRIPTION
        "The current administrative value of the Key for the
        Aggregation Port. This is a 16-bit read-only value.
        The meaning of particular Key values is of local
        significance."
    ::= { lacpCurPortCfgTableEntry 4 }

lacpNewPortCfgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF LacpNewPortCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of LACP port configuration."
    ::= { lacp 8 }

lacpNewPortCfgTableEntry OBJECT-TYPE
    SYNTAX  LacpNewPortCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the LACP port configuration table."
    INDEX  { lacpNewPortCfgTableId }
    ::= { lacpNewPortCfgTable 1 }

LacpNewPortCfgTableEntry ::= SEQUENCE {
    lacpNewPortCfgTableId 	    Integer32,
    lacpNewPortState                INTEGER, 
    lacpNewPortActorPortPriority    INTEGER, 
    lacpNewPortActorAdminKey        INTEGER 
    }

lacpNewPortCfgTableId OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
          " LACP port number."
    ::= { lacpNewPortCfgTableEntry 1 }

lacpNewPortState OBJECT-TYPE
    SYNTAX  INTEGER  {
        off(1),
        active(2),
        passive(3)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "LACP port state can be one of three states 
         off (Not participating in LACP) 
         Active (Initiates LACPDU updates)
         Passive (Does not initiate LACPDU updates but responds to peer."
    ::= { lacpNewPortCfgTableEntry 2 }

lacpNewPortActorPortPriority OBJECT-TYPE
    SYNTAX       INTEGER (1..65535)
    MAX-ACCESS       read-write
    STATUS       current
    DESCRIPTION
        "The priority value assigned to this Aggregation Port.
        This 16-bit value is read-write."
    ::= { lacpNewPortCfgTableEntry 3 }

lacpNewPortActorAdminKey OBJECT-TYPE
    SYNTAX       INTEGER (1..65535)
    MAX-ACCESS       read-write
    STATUS       current
    DESCRIPTION
        "The current administrative value of the Key for the
        Aggregation Port. This is a 16-bit read-write value.
        The meaning of particular Key values is of local
        significance."
    ::= { lacpNewPortCfgTableEntry 4 }

-- Trunk Group Group
trunkGroupTableMaxSize OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The maximum number of entries in trunk group table."
    ::= { trunkgroup 1 }

trunkGroupCurCfgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF TrunkGroupCurCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of trunk group configuration."
    ::= { trunkgroup 2 }

trunkGroupCurCfgTableEntry OBJECT-TYPE
    SYNTAX  TrunkGroupCurCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the trunk group configuration table."
    INDEX   { trunkGroupCurCfgIndex }
    ::= { trunkGroupCurCfgTable 1 }

TrunkGroupCurCfgTableEntry ::= SEQUENCE {
    trunkGroupCurCfgIndex         Integer32,
    trunkGroupCurCfgPorts         OCTET STRING,
    trunkGroupCurCfgBwmContract   Integer32,
    trunkGroupCurCfgState         INTEGER
    }
 
trunkGroupCurCfgIndex OBJECT-TYPE
    SYNTAX  Integer32  
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The identifier of the trunk group."
    ::= { trunkGroupCurCfgTableEntry 1 }
 
trunkGroupCurCfgPorts OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port list in the trunk group. The ports are presented in 
         bitmap format.
 
         in receiving order:
 
             OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx ..... 
             ||    || |_ port 8
             ||    ||  
             ||    ||___ port 7
             ||    |____ port 6
             ||      .    .   .
             ||_________ port 1
             |__________ reserved

         where x : 1 - The represented port belongs to the trunk group
                   0 - The represented port does not belong to the trunk group"
    ::= { trunkGroupCurCfgTableEntry 2 }
 
trunkGroupCurCfgState OBJECT-TYPE
    SYNTAX  INTEGER  {
        enable(1),
        disable(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable a trunk group."
    ::= { trunkGroupCurCfgTableEntry 3 }
 
trunkGroupCurCfgBwmContract OBJECT-TYPE
    SYNTAX  Integer32  
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Default BW contract of a trunk group."
    ::= { trunkGroupCurCfgTableEntry 4 }
 

trunkGroupNewCfgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF TrunkGroupNewCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of trunk group configuration."
    ::= { trunkgroup 3 }

trunkGroupNewCfgTableEntry OBJECT-TYPE
    SYNTAX  TrunkGroupNewCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the trunk group configuration table."
    INDEX   { trunkGroupNewCfgIndex }
    ::= { trunkGroupNewCfgTable 1 }

TrunkGroupNewCfgTableEntry ::= SEQUENCE {
    trunkGroupNewCfgIndex          Integer32,
    trunkGroupNewCfgPorts          OCTET STRING,
    trunkGroupNewCfgAddPort        Integer32,
    trunkGroupNewCfgRemovePort     Integer32,
    trunkGroupNewCfgState          INTEGER,
    trunkGroupNewCfgBwmContract    Integer32,
    trunkGroupNewCfgDelete         INTEGER
    }
 
trunkGroupNewCfgIndex OBJECT-TYPE
    SYNTAX  Integer32  
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The identifier of the trunk group."
    ::= { trunkGroupNewCfgTableEntry 1 }
 
trunkGroupNewCfgPorts OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port list in the trunk group.  The ports are presented
         in bitmap format.

         in receiving order:

             OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx ..... 
             ||    || |_ port 8
             ||    ||  
             ||    ||___ port 7
             ||    |____ port 6
             ||      .    .   .
             ||_________ port 1
             |__________ reserved
 
         where x : 1 - The represented port belongs to the trunk group
                   0 - The represented port does not belong to the trunk group"
    ::= { trunkGroupNewCfgTableEntry 2 }
 
trunkGroupNewCfgAddPort OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The port to be added in the trunk group. When read, 0 is returned."
    ::= { trunkGroupNewCfgTableEntry 3 }

trunkGroupNewCfgRemovePort OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The port to be deleted from the trunk group. when read, 0
	 is returned."
    ::= { trunkGroupNewCfgTableEntry 4 }

trunkGroupNewCfgState OBJECT-TYPE
    SYNTAX  INTEGER  {
        enable(1),
        disable(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Enable or disable a trunk group."
    ::= { trunkGroupNewCfgTableEntry 5 }
 
trunkGroupNewCfgDelete OBJECT-TYPE
    SYNTAX  INTEGER  {
        other(1),
        delete(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Setting the value to delete(2) will delete the entire
         row. When read, other(1) is returned."
    ::= { trunkGroupNewCfgTableEntry 6 }

trunkGroupNewCfgBwmContract OBJECT-TYPE
    SYNTAX  Integer32  
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Default BW contract of a trunk group."
    ::= { trunkGroupNewCfgTableEntry 7 }



-- Spanning Tree Group Configuration
-- This group specifies the additional configurations that are not
-- covered by the Bridge MIB (RFC 1493).
-- The relative Spanning Tree information can be retrieved or configured
-- using Bridge MIB with an unique community string for each group specified
-- in entLogicalTable of Entity MIB (RFC 2037).
--
stgCurCfgTable OBJECT-TYPE
    SYNTAX SEQUENCE OF StgCurCfgTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of Spanning Tree Group configuration."
    ::= { stgCfg 1 }

stgCurCfgTableEntry OBJECT-TYPE
    SYNTAX StgCurCfgTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about a particular Spanning Tree Group configuration."
    INDEX { stgCurCfgIndex }
    ::= { stgCurCfgTable 1 }

StgCurCfgTableEntry ::= SEQUENCE {
    stgCurCfgIndex           Integer32,
    stgCurCfgState           INTEGER,
    stgCurCfgPriority        INTEGER,
    stgCurCfgBrgHelloTime    INTEGER,
    stgCurCfgBrgForwardDelay INTEGER,
    stgCurCfgBrgMaxAge       INTEGER,
    stgCurCfgAgingTime       INTEGER,
    stgCurCfgVlanBmap        OCTET STRING
    }

stgCurCfgIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The identifier of a particular Spanning Tree Group.  This is also
         index to the entLogicalTable of Entity MIB."
    ::= { stgCurCfgTableEntry 1 }

stgCurCfgState OBJECT-TYPE
    SYNTAX INTEGER {
        on(1),
        off(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Turn on of off Spanning Tree operation of a particular Spanning
         Tree Group."
    ::= { stgCurCfgTableEntry 2 }


stgCurCfgPriority OBJECT-TYPE
    SYNTAX  INTEGER (0..65535)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The value of the write-able portion of the Bridge ID, i.e., the first
         two octets of the (8 octet long) Bridge ID."
    ::= { stgCurCfgTableEntry 5 }

stgCurCfgBrgHelloTime OBJECT-TYPE
    SYNTAX  INTEGER (1..10)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for HelloTime when this 
         bridge is acting as the root."
    ::= { stgCurCfgTableEntry 6 }

stgCurCfgBrgForwardDelay OBJECT-TYPE
    SYNTAX  INTEGER (4..30)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for ForwardDelay when this 
         bridge is acting as the root."
    ::= { stgCurCfgTableEntry 7 }

stgCurCfgBrgMaxAge OBJECT-TYPE
    SYNTAX  INTEGER (6..40)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for MaxAge when this bridge
         is acting as the root."
    ::= { stgCurCfgTableEntry 8 }

stgCurCfgAgingTime OBJECT-TYPE
    SYNTAX  INTEGER (0..65535)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The timeout period in seconds for aging out dynamically learned 
         forwarding information."
    ::= { stgCurCfgTableEntry 9 }

stgCurCfgVlanBmap OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE(0..512)) 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	"The vlans applied to the spanning tree group.  The vlans are 
         presented in bitmap format. This string displays vlan number
	 from 1 to 4096.

	 in receiving order:

	     OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx ..... 
             ||    || |_ vlan 9
             ||    ||  
             ||    ||___ vlan 8
             ||    |____ vlan 7
             ||      .    .   .
             ||_________ vlan 2
             |__________ vlan 1 (as index to stgCurCfgTable)

         where x : 1 - The represented vlan applied to the spanning tree. 
		   0 - The represented vlan not applied to the spanning tree"
    ::= { stgCurCfgTableEntry 10 }


stgNewCfgTable OBJECT-TYPE
    SYNTAX SEQUENCE OF StgNewCfgTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of Spanning Tree Groups configuration in the new_config."
    ::= { stgCfg 2 }

stgNewCfgTableEntry OBJECT-TYPE
    SYNTAX StgNewCfgTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about a particular Spanning Tree Group configuration."
    INDEX { stgNewCfgIndex }
    ::= { stgNewCfgTable 1 }

StgNewCfgTableEntry ::= SEQUENCE {
    stgNewCfgIndex           Integer32,
    stgNewCfgState           INTEGER,
    stgNewCfgDefaultCfg      INTEGER,
    stgNewCfgAddVlan         Integer32,
    stgNewCfgRemoveVlan      Integer32,
    stgNewCfgPriority        INTEGER,
    stgNewCfgBrgHelloTime    INTEGER,
    stgNewCfgBrgForwardDelay INTEGER,
    stgNewCfgBrgMaxAge       INTEGER,
    stgNewCfgAgingTime       INTEGER,
    stgNewCfgVlanBmap        OCTET STRING
    }

stgNewCfgIndex  OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The identifier of a particular Spanning Tree Group.  This is also
         index to the entLogicalTable of Entity MIB."
    ::= { stgNewCfgTableEntry 1 }

stgNewCfgState OBJECT-TYPE
    SYNTAX INTEGER {
        on(1),
        off(2)
        }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Turn on of off Spanning Tree operation of a particular Spanning
         Tree Group."
    ::= { stgNewCfgTableEntry 2 }

stgNewCfgDefaultCfg OBJECT-TYPE
    SYNTAX INTEGER {
        default-config(1)
        }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Setting the value to default-config(1) will set the default
         configuration as recommended by IEEE 802.1D for a particular
         Spanning Tree Group.  default-config (1) is always returned 
	 When read, but it does not mean anything."
    ::= { stgNewCfgTableEntry 3 }

stgNewCfgAddVlan OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The vlan to be added to the specified Spanning Tree Group.  A 
         '0' value is returned when read." 
    ::= {stgNewCfgTableEntry 4 }

stgNewCfgRemoveVlan OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The vlan to be removed from the specified Spanning Tree Group.
         A '0' value is returned when read."
    ::= { stgNewCfgTableEntry 5 }


stgNewCfgPriority OBJECT-TYPE
    SYNTAX  INTEGER (0..65535)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The value of the write-able portion of the Bridge ID, i.e., the first
         two octets of the (8 octet long) Bridge ID."
    ::= { stgNewCfgTableEntry 8 }

stgNewCfgBrgHelloTime OBJECT-TYPE
    SYNTAX  INTEGER (1..10)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for HelloTime when this 
         bridge is acting as the root."
    ::= { stgNewCfgTableEntry 9 }

stgNewCfgBrgForwardDelay OBJECT-TYPE
    SYNTAX  INTEGER (4..30)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for ForwardDelay when this 
         bridge is acting as the root."
    ::= { stgNewCfgTableEntry 10 }

stgNewCfgBrgMaxAge OBJECT-TYPE
    SYNTAX  INTEGER (6..40)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for MaxAge when this bridge
         is acting as the root."
    ::= { stgNewCfgTableEntry 11 }

stgNewCfgAgingTime OBJECT-TYPE
    SYNTAX  INTEGER (0..65535)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The timeout period in seconds for aging out dynamically learned 
         forwarding information."
    ::= { stgNewCfgTableEntry 12 }

stgNewCfgVlanBmap OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE(0..512)) 
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
	"The vlans applied to the spanning tree group.  The vlans are 
         presented in bitmap format. This string displays vlan number
	 from 1 to 4096.

	 in receiving order:

	     OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx ..... 
             ||    || |_ vlan 9
             ||    ||  
             ||    ||___ vlan 8
             ||    |____ vlan 7
             ||      .    .   .
             ||_________ vlan 2
             |__________ vlan 1 (as index to stgCurCfgTable)

         where x : 1 - The represented vlan applied to the spanning tree. 
		   0 - The represented vlan not applied to the spanning tree"
    ::= { stgNewCfgTableEntry 13 }


stgCurCfgPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF StgCurCfgPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of Spanning Tree Group port configuration in the
         current_config."
    ::= { stgCfg 3 }

stgCurCfgPortTableEntry OBJECT-TYPE
    SYNTAX StgCurCfgPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about port configuration of a particular Spanning Tree
         Group."
    INDEX { stgCurCfgStgIndex, stgCurCfgPortIndex }
    ::= { stgCurCfgPortTable 1 }

StgCurCfgPortTableEntry ::= SEQUENCE {
    stgCurCfgStgIndex      Integer32,
    stgCurCfgPortIndex     Integer32,
    stgCurCfgPortPriority  INTEGER,
    stgCurCfgPortPathCost  Integer32,
    stgCurCfgPortLink      INTEGER,
    stgCurCfgPortEdge      INTEGER,
    stgCurCfgPortState     INTEGER
    }

stgCurCfgStgIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The identifier of a particular Spanning Tree Group.  This is also
         index to the entLogicalTable of Entity MIB."
    ::= { stgCurCfgPortTableEntry 1 }

stgCurCfgPortIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The port identifier of a particular Spanning Tree Group."
    ::= { stgCurCfgPortTableEntry 2 }

stgCurCfgPortState OBJECT-TYPE
    SYNTAX INTEGER {
        on(1),
        off(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Turn on of off Spanning Tree operation of a particular port of a
         Spanning Tree Group."
    ::= { stgCurCfgPortTableEntry 3 }

stgCurCfgPortPriority OBJECT-TYPE
    SYNTAX INTEGER (0..255)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The value of the priority field which is contained in the first 
         (in network byte order) octet of the (2 octet long) Port ID."
    ::= { stgCurCfgPortTableEntry 4 }

stgCurCfgPortPathCost OBJECT-TYPE
    SYNTAX Integer32 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
       "The contribution of this port to the path cost of paths towards the 
        spanning tree root which include this port (if MSTP/RSTP is enabled
        range is (0..200000000) else range is (0..65535) )."
    ::= { stgCurCfgPortTableEntry 5 }

stgCurCfgPortLink OBJECT-TYPE
    SYNTAX INTEGER {
        auto(1),
        p2p(2),
        shared(3)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The type of the port link."
    ::= { stgCurCfgPortTableEntry 6 }

stgCurCfgPortEdge OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The state of port edge."
    ::= { stgCurCfgPortTableEntry 7 }

stgNewCfgPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF StgNewCfgPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of Spanning Tree Group port configuration in the
         new_config."
    ::= { stgCfg 4 }

stgNewCfgPortTableEntry OBJECT-TYPE
    SYNTAX StgNewCfgPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about port configuration of a particular Spanning Tree
         Group."
    INDEX { stgNewCfgStgIndex, stgNewCfgPortIndex }
    ::= { stgNewCfgPortTable 1 }

StgNewCfgPortTableEntry ::= SEQUENCE {
    stgNewCfgStgIndex      Integer32,
    stgNewCfgPortIndex     Integer32,
    stgNewCfgPortPriority  INTEGER,
    stgNewCfgPortPathCost  Integer32,
    stgNewCfgPortLink      INTEGER,
    stgNewCfgPortEdge      INTEGER,
    stgNewCfgPortState     INTEGER
    }

stgNewCfgStgIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The identifier of a particular Spanning Tree Group.  This is also
         index to the entLogicalTable of Entity MIB."
    ::= { stgNewCfgPortTableEntry 1 }

stgNewCfgPortIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The port identifier of a particular Spanning Tree Group."
    ::= { stgNewCfgPortTableEntry 2 }

stgNewCfgPortState OBJECT-TYPE
    SYNTAX INTEGER {
        on(1),
        off(2)
        }
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "Turn on of off Spanning Tree operation of a particular port of a
         Spanning Tree Group."
    ::= { stgNewCfgPortTableEntry 3 }

stgNewCfgPortPriority OBJECT-TYPE
    SYNTAX INTEGER (0..255)
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
        "The value of the priority field which is contained in the first 
         (in network byte order) octet of the (2 octet long) Port ID."
    ::= { stgNewCfgPortTableEntry 4 }

stgNewCfgPortPathCost OBJECT-TYPE
    SYNTAX  Integer32 
    MAX-ACCESS read-create
    STATUS current
    DESCRIPTION
       "The contribution of this port to the path cost of paths towards the 
        spanning tree root which include this port (if MSTP/RSTP is enabled
        range is (0..200000000) else range is (0..65535) )."
    ::= { stgNewCfgPortTableEntry 5 }

stgNewCfgPortLink OBJECT-TYPE
    SYNTAX INTEGER {
        auto(1),
        p2p(2),
        shared(3)
        }
    MAX-ACCESS read-create 
    STATUS current
    DESCRIPTION
        "The type of the port link."
    ::= { stgNewCfgPortTableEntry 6 }

stgNewCfgPortEdge OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-create 
    STATUS current
    DESCRIPTION
        "The state of port edge."
    ::= { stgNewCfgPortTableEntry 7 }

-- Complete Port Mirroring 
pmCurCfgPortMirrState OBJECT-TYPE
    SYNTAX  INTEGER {
	enabled(1),
	disabled(2)
	}
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The state of port-based port mirroring."
    ::= { mirrPortMirr 1 }
 
pmNewCfgPortMirrState OBJECT-TYPE
    SYNTAX  INTEGER {
	enabled(1),
	disabled(2)
        }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The state of port-based port mirroring."
    ::= { mirrPortMirr 2 }

pmCurCfgPortMonitorTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF PmCurCfgPortMonitorEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of monitoring ports."
    ::= { mirrPortMirr 3 }

pmCurCfgPortMonitorEntry OBJECT-TYPE
    SYNTAX  PmCurCfgPortMonitorEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the monitoring port table."
    INDEX   { pmCurCfgPmirrMoniPortIndex, pmCurCfgPmirrMirrPortIndex }
    ::= { pmCurCfgPortMonitorTable 1 }

PmCurCfgPortMonitorEntry ::= SEQUENCE {
    pmCurCfgPmirrMoniPortIndex       Integer32,
    pmCurCfgPmirrMirrPortIndex       Integer32,
    pmCurCfgPmirrDirection           INTEGER,
    pmCurCfgPmirrPortVlansBmap       OCTET STRING
    }

pmCurCfgPmirrMoniPortIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The monitoring port number." 
    ::= { pmCurCfgPortMonitorEntry 1 }

pmCurCfgPmirrMirrPortIndex OBJECT-TYPE 
    SYNTAX  Integer32 
    MAX-ACCESS  read-only 
    STATUS  current 
    DESCRIPTION 
        "The mirrored port number" 
    ::= { pmCurCfgPortMonitorEntry 2 }

pmCurCfgPmirrDirection OBJECT-TYPE
    SYNTAX  INTEGER {
	in(1),
	out(2),
	both(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The type of traffic to be monitored with respect to the
         mirrored port."
    ::= { pmCurCfgPortMonitorEntry 3 }


pmCurCfgPmirrPortVlansBmap	OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The mirrored VLANs (1-4096) list for the port. The VLANs are presented in bitmap format.
	 in receiving order:

	     OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx ..... 
             ||    || |_ vlan 9
             ||    ||  
             ||    ||___ vlan 8
             ||    |____ vlan 7
             ||      .    .   .
             ||_________ vlan 2
             |__________ vlan 1

         where x : 1 - The represented VLAN is being mirrored.
		   0 - The represented VLAN is not being mirrored.
         Note: When all octets are zero - all vlan(s) traffic is 
               being for the port"
    ::= { pmCurCfgPortMonitorEntry 6 }

pmNewCfgPortMonitorTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF PmNewCfgPortMonitorEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of monitoring ports."
    ::= { mirrPortMirr 4 }

pmNewCfgPortMonitorEntry OBJECT-TYPE
    SYNTAX  PmNewCfgPortMonitorEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the monitoring port table."
    INDEX   { pmNewCfgPmirrMoniPortIndex, pmNewCfgPmirrMirrPortIndex }
    ::= { pmNewCfgPortMonitorTable 1 }

PmNewCfgPortMonitorEntry ::= SEQUENCE {
    pmNewCfgPmirrMoniPortIndex          Integer32,
    pmNewCfgPmirrMirrPortIndex          Integer32,
    pmNewCfgPmirrDirection              INTEGER,
    pmNewCfgPmirrDelete                 INTEGER,
    pmNewCfgAddVlan 			Integer32,
    pmNewCfgRemoveVlan			Integer32,
    pmNewCfgPmirrPortVlansBmap         OCTET STRING
    }

pmNewCfgPmirrMoniPortIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The monitoring port number." 
    ::= { pmNewCfgPortMonitorEntry 1 }

pmNewCfgPmirrMirrPortIndex OBJECT-TYPE 
    SYNTAX  Integer32 
    MAX-ACCESS  read-only 
    STATUS  current 
    DESCRIPTION 
        "The mirrored port number" 
    ::= { pmNewCfgPortMonitorEntry 2 }

pmNewCfgPmirrDirection OBJECT-TYPE
    SYNTAX  INTEGER {
	in(1),
	out(2),
	both(3)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The type of traffic to be monitored with respect to the
         mirrored port."
    ::= { pmNewCfgPortMonitorEntry 3 }

pmNewCfgPmirrDelete OBJECT-TYPE
    SYNTAX  INTEGER  {
        other(1),
        delete(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Setting the value to delete(2) will delete the entire
         row. When read, other(1) is returned."
    ::= { pmNewCfgPortMonitorEntry 4 }


pmNewCfgAddVlan OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The VLAN whose traffic is to be mirrored for this port. 
         A '0' value is returned when read."
    ::= { pmNewCfgPortMonitorEntry 7 }

pmNewCfgRemoveVlan OBJECT-TYPE		
    SYNTAX  Integer32
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The VLAN whose traffic will no longer to be mirrored. 
         A '0' value is returned when read."
    ::= { pmNewCfgPortMonitorEntry 8 }

pmNewCfgPmirrPortVlansBmap	OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The mirrored VLANs(1-4096) list for the port. The VLANs are presented in bitmap format.
	 in receiving order:

	     OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx ..... 
             ||    || |_ vlan 9
             ||    ||  
             ||    ||___ vlan 8
             ||    |____ vlan 7
             ||      .    .   .
             ||_________ vlan 2
             |__________ vlan 1

         where x : 1 - The represented VLAN is being mirrored.
		   0 - The represented VLAN is not being mirrored.
         Note: All octets are zero means all vlan(s) traffic is 
               being mirrored for the port"
    ::= { pmNewCfgPortMonitorEntry 9 }

-- MST Configuration 

mstCurCfgState	OBJECT-TYPE
    SYNTAX  INTEGER  {
	enabled(2),
	disabled(3)
	}
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable MSTP/RSTP"
    ::= { mstGeneralCfg 1 }

mstNewCfgState	OBJECT-TYPE
    SYNTAX  INTEGER  {
	enabled(2),
	disabled(3)
	}
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Enable or disable MSTP/RSTP"
    ::= { mstGeneralCfg 2 }

mstCurCfgRegionName OBJECT-TYPE
   SYNTAX  DisplayString (SIZE (0..32))
   MAX-ACCESS  read-only
   STATUS  current
   DESCRIPTION
      "The Name for the Region's configuration."
   ::= { mstGeneralCfg 3 } 

mstNewCfgRegionName OBJECT-TYPE
   SYNTAX  DisplayString (SIZE (0..32))
   MAX-ACCESS  read-write
   STATUS  current
   DESCRIPTION
      "The Name for the Region's configuration."
   ::= { mstGeneralCfg 4 } 

mstCurCfgRegionVersion OBJECT-TYPE
    SYNTAX  INTEGER  (0..65535)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Version of the MST Region."
    ::= { mstGeneralCfg 5 }

mstNewCfgRegionVersion OBJECT-TYPE
    SYNTAX  INTEGER  (0..65535)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Version of the MST Region."
    ::= { mstGeneralCfg 6 }

mstCurCfgMaxHopCount OBJECT-TYPE
    SYNTAX  INTEGER  (4..60)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Indicates the maximum hop count value."
    ::= { mstGeneralCfg 7 }

mstNewCfgMaxHopCount OBJECT-TYPE
    SYNTAX  INTEGER  (4..60)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "Indicates the maximum hop count value."
    ::= { mstGeneralCfg 8 }

mstCurCfgStpMode OBJECT-TYPE
    SYNTAX  INTEGER  {
	mstp(1),
	rstp(2)
	}
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The version of Spanning Tree Protocal the bridge is currently 
         running."
    ::= { mstGeneralCfg 9 }

mstNewCfgStpMode OBJECT-TYPE
    SYNTAX  INTEGER  {
	mstp(1),
	rstp(2)
	}
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The version of Spanning Tree Protocal the bridge is currently 
         running."
    ::= { mstGeneralCfg 10 }

mstCistDefaultCfg OBJECT-TYPE
    SYNTAX INTEGER {
        default(1)
        }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Setting the value to default(1) will set the Multiple
         Spanning Tree and member parameters to default.  default(1) is 
         always returned when read, but it does not mean anything."
    ::= { mstCistCfg 1 }

-- CIST Brige Configuration
mstCistBridgeCfg  OBJECT IDENTIFIER ::= { mstCistCfg 2 }

mstCistCurCfgBridgePriority OBJECT-TYPE
    SYNTAX  INTEGER  (0..65535)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The value of the writable portion of the Brigde Identifier comprising
         of the first two octets."
    ::= { mstCistBridgeCfg 1 }

mstCistNewCfgBridgePriority OBJECT-TYPE
    SYNTAX  INTEGER  (0..65535)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The value of the writable portion of the Brigde Identifier comprising
         of the first two octets."
    ::= { mstCistBridgeCfg 2 }


mstCistCurCfgBridgeMaxAge OBJECT-TYPE
    SYNTAX  INTEGER  (6..40)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for MaxAge when this bridge
         is acting as the root."
    ::= { mstCistBridgeCfg 5 }

mstCistNewCfgBridgeMaxAge OBJECT-TYPE
    SYNTAX  INTEGER  (6..40)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for MaxAge when this bridge
         is acting as the root."
    ::= { mstCistBridgeCfg 6 }

mstCistCurCfgBridgeForwardDelay OBJECT-TYPE
    SYNTAX  INTEGER  (4..30)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for ForwardDelay when this 
         bridge is acting as the root."
    ::= { mstCistBridgeCfg 7 }

mstCistNewCfgBridgeForwardDelay OBJECT-TYPE
    SYNTAX  INTEGER  (4..30)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for ForwardDelay when this 
         bridge is acting as the root."
    ::= { mstCistBridgeCfg 8 }

-- CIST Port Configuration

mstCistCurCfgPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MstCistCurCfgPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of CIST Port configuration."
    ::= { mstCistCfg 3 }

mstCistCurCfgPortTableEntry OBJECT-TYPE
    SYNTAX MstCistCurCfgPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about a particular CIST Port configuration."
    INDEX { mstCistCurCfgPortIndex }
    ::= { mstCistCurCfgPortTable 1 }

MstCistCurCfgPortTableEntry ::= SEQUENCE {
    mstCistCurCfgPortIndex      Integer32,
    mstCistCurCfgPortPriority   INTEGER,
    mstCistCurCfgPortPathCost   INTEGER,
    mstCistCurCfgPortLinkType   INTEGER,
    mstCistCurCfgPortEdge       INTEGER,
    mstCistCurCfgPortStpState   INTEGER,
    mstCistCurCfgPortHelloTime  INTEGER
    }

mstCistCurCfgPortIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The port number of the port for which this entry contains spanning
         tree configuration."
    ::= { mstCistCurCfgPortTableEntry 1 }

mstCistCurCfgPortPriority OBJECT-TYPE
    SYNTAX INTEGER (0..240)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The four most significant bits of the Port Identifier of the 
         Spanning Tree instance can be modified by setting this value."
    ::= { mstCistCurCfgPortTableEntry 2 }

mstCistCurCfgPortPathCost OBJECT-TYPE
    SYNTAX INTEGER (1..200000000)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The contribution of this port to the path cost of paths towards 
         the CIST Root which include this port."
    ::= { mstCistCurCfgPortTableEntry 3 }

mstCistCurCfgPortLinkType OBJECT-TYPE
    SYNTAX INTEGER {
        auto(1),
        p2p(2),
        shared(3)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The administrative point-to-point status of the LAN segment attached 
         to this port.  A value of p2p (2) indicates that this port should 
         always be treated as if it is connected to a point-to-point link. 
         A value of shared(3) indicates that this port should be treated as 
         having a shared media connection.  A value of auto(1) indicates that 
         this port is considered to have a point-to-point link if it is an 
         Aggregator and all of its members are aggregatable, or if the MAC 
         entity is configured for full duplex operation, either through
         auto-negotiation or by management means."    
    ::= { mstCistCurCfgPortTableEntry 4 }

mstCistCurCfgPortEdge OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The value of the Edge Port parameter."
    ::= { mstCistCurCfgPortTableEntry 5 }

mstCistCurCfgPortStpState OBJECT-TYPE
    SYNTAX INTEGER {
        on(1),
        off(2)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Turn port's Spanning Tree on/off."
    ::= { mstCistCurCfgPortTableEntry 6 }

mstCistCurCfgPortHelloTime OBJECT-TYPE
    SYNTAX  INTEGER (1..10)
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The amount of time between the transmission of Configuration Port 
         PDUs in seconds."
    ::= { mstCistCurCfgPortTableEntry 7 } 

mstCistNewCfgPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF MstCistNewCfgPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of CIST Port configuration."
    ::= { mstCistCfg 4 }

mstCistNewCfgPortTableEntry OBJECT-TYPE
    SYNTAX MstCistNewCfgPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about a particular CIST Port configuration."
    INDEX { mstCistNewCfgPortIndex }
    ::= { mstCistNewCfgPortTable 1 }

MstCistNewCfgPortTableEntry ::= SEQUENCE {
    mstCistNewCfgPortIndex      Integer32,
    mstCistNewCfgPortPriority   INTEGER,
    mstCistNewCfgPortPathCost   INTEGER,
    mstCistNewCfgPortLinkType   INTEGER,
    mstCistNewCfgPortEdge       INTEGER,
    mstCistNewCfgPortStpState   INTEGER,
    mstCistNewCfgPortHelloTime  INTEGER
    }

mstCistNewCfgPortIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The port number of the port for which this entry contains spanning
         tree configuration."
    ::= { mstCistNewCfgPortTableEntry 1 }

mstCistNewCfgPortPriority OBJECT-TYPE
    SYNTAX INTEGER (0..240)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "The four most significant bits of the Port Identifier of the 
         Spanning Tree instance can be modified by setting this value."
    ::= { mstCistNewCfgPortTableEntry 2 }

mstCistNewCfgPortPathCost OBJECT-TYPE
    SYNTAX INTEGER (1..200000000)
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "The contribution of this port to the path cost of paths towards 
         the CIST Root which include this port."
    ::= { mstCistNewCfgPortTableEntry 3 }

mstCistNewCfgPortLinkType OBJECT-TYPE
    SYNTAX INTEGER {
        auto(1),
        p2p(2),
        shared(3)
        }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "The administrative point-to-point status of the LAN segment attached 
         to this port.  A value of p2p (2) indicates that this port should 
         always be treated as if it is connected to a point-to-point link. 
         A value of shared(3) indicates that this port should be treated as 
         having a shared media connection.  A value of auto(1) indicates that 
         this port is considered to have a point-to-point link if it is an 
         Aggregator and all of its members are aggregatable, or if the MAC 
         entity is configured for full duplex operation, either through
         auto-negotiation or by management means."    
    ::= { mstCistNewCfgPortTableEntry 4 }

mstCistNewCfgPortEdge OBJECT-TYPE
    SYNTAX INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "The value of the Edge Port parameter."
    ::= { mstCistNewCfgPortTableEntry 5 }

mstCistNewCfgPortStpState OBJECT-TYPE
    SYNTAX INTEGER {
        on(1),
        off(2)
        }
    MAX-ACCESS read-write
    STATUS current
    DESCRIPTION
        "Turn port's Spanning Tree on/off."
    ::= { mstCistNewCfgPortTableEntry 6 }

mstCistNewCfgPortHelloTime OBJECT-TYPE
    SYNTAX  INTEGER (1..10)
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
        "The amount of time between the transmission of Configuration Port 
         PDUs in seconds."
    ::= { mstCistNewCfgPortTableEntry 7 } 


-- Port Team

portTeamTableMaxSize OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The maximum number of port teams."
    ::= { portTeamCfg 1 }

portTeamCurCfgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF PortTeamCurCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The port team current configuration."
    ::= { portTeamCfg 2 }

portTeamCurCfgTableEntry OBJECT-TYPE
    SYNTAX  PortTeamCurCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the port team configuration table."
    INDEX   { portTeamCurCfgIndex }
    ::= { portTeamCurCfgTable 1 }

PortTeamCurCfgTableEntry ::= SEQUENCE {
    portTeamCurCfgIndex         Integer32,
    portTeamCurCfgState         INTEGER,
    portTeamCurCfgPorts         OCTET STRING,
    portTeamCurCfgTrunks        OCTET STRING
    }

portTeamCurCfgIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The identifier of the port team."
    ::= { portTeamCurCfgTableEntry 1 }

portTeamCurCfgState OBJECT-TYPE
    SYNTAX  INTEGER  {
        enable(1),
        disable(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable a port team."
    ::= { portTeamCurCfgTableEntry 2 }

portTeamCurCfgPorts OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port list in the port team. The ports are presented in
         bitmap format.

         in receiving order:

             OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx .....
             |    |||_ port 8
             |    ||
             |    ||___ port 7
             |    |____ port 6
             |      .    .   .
             |_________ port 1

         where x : 1 - The represented port belongs to the port team
                   0 - The represented port does not belong to the port team"
    ::= { portTeamCurCfgTableEntry 3 }

portTeamCurCfgTrunks OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The trunk list in the port team. The trunks are presented in
         bitmap format.

         in receiving order:

             OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx .....
             |    |||_ trunk 8
             |    ||
             |    ||___ trunk 7
             |    |____ trunk 6
             |      .    .   .
             |_________ trunk 1

         where x : 1 - The represented trunk belongs to the port team
                   0 - The represented trunk does not belong to the port team"
    ::= { portTeamCurCfgTableEntry 4 }

portTeamNewCfgTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF PortTeamNewCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The port team new configuration."
    ::= { portTeamCfg 3 }

portTeamNewCfgTableEntry OBJECT-TYPE
    SYNTAX  PortTeamNewCfgTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the port team configuration table."
    INDEX   { portTeamNewCfgIndex }
    ::= { portTeamNewCfgTable 1 }

PortTeamNewCfgTableEntry ::= SEQUENCE {
    portTeamNewCfgIndex         Integer32,
    portTeamNewCfgState         INTEGER,
    portTeamNewCfgPorts         OCTET STRING,
    portTeamNewCfgAddPort       Integer32,
    portTeamNewCfgRemovePort    Integer32,
    portTeamNewCfgTrunks        OCTET STRING,
    portTeamNewCfgAddTrunk      Integer32,
    portTeamNewCfgRemoveTrunk   Integer32,
    portTeamNewCfgDelete        INTEGER
    }

portTeamNewCfgIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The identifier of the port team."
    ::= { portTeamNewCfgTableEntry 1 }

portTeamNewCfgState OBJECT-TYPE
    SYNTAX  INTEGER  {
        enable(1),
        disable(2)
        }
    MAX-ACCESS  read-create 
    STATUS  current
    DESCRIPTION
        "Enable or disable a port team."
    ::= { portTeamNewCfgTableEntry 2 }

portTeamNewCfgPorts OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port list in the port team. The ports are presented in
         bitmap format.

         in receiving order:

             OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx .....
             |    |||_ port 8
             |    ||
             |    ||___ port 7
             |    |____ port 6
             |      .    .   .
             |_________ port 1

         where x : 1 - The represented port belongs to the port team
                   0 - The represented port does not belong to the port team"
    ::= { portTeamNewCfgTableEntry 3 }

portTeamNewCfgAddPort OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The port to be added in the port team. When read, 0 is returned."
    ::= { portTeamNewCfgTableEntry 4 }

portTeamNewCfgRemovePort OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The port to be deleted from the port team. When read, 0is returned."
    ::= { portTeamNewCfgTableEntry 5 }

portTeamNewCfgTrunks OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The trunk list in the port team. The trunks are presented in
         bitmap format.

         in receiving order:

             OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx .....
             |    |||_ trunk 8
             |    ||
             |    ||___ trunk 7
             |    |____ trunk 6
             |      .    .   .
             |_________ trunk 1

         where x : 1 - The represented trunk belongs to the port team
                   0 - The represented trunk does not belong to the port team"
    ::= { portTeamNewCfgTableEntry 6 }

portTeamNewCfgAddTrunk OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The trunk to be added in the port team. When read, 0 is returned."
    ::= { portTeamNewCfgTableEntry 7 }

portTeamNewCfgRemoveTrunk OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "The trunk to be deleted from the port team. When read, 0is returned."
    ::= { portTeamNewCfgTableEntry 8 }

portTeamNewCfgDelete OBJECT-TYPE
    SYNTAX  INTEGER  {
        other(1),
        delete(2)
        }
    MAX-ACCESS  read-create
    STATUS  current
    DESCRIPTION
        "Setting the value to delete(2) will delete the entire
         row. When read, other(1) is returned."
    ::= { portTeamNewCfgTableEntry 9 }

portTeamInfoTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF PortTeamInfoTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The port team information table."
    ::= { portTeamInfo 1 }
 
portTeamInfoTableEntry OBJECT-TYPE
    SYNTAX  PortTeamInfoTableEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the port team information table."
    INDEX   { portTeamInfoIndex }
    ::= { portTeamInfoTable 1 }
 
PortTeamInfoTableEntry ::= SEQUENCE {
    portTeamInfoIndex          Integer32,
    portTeamInfoState          INTEGER,
    portTeamInfoPorts          OCTET STRING,
    portTeamInfoPortsState     OCTET STRING,
    portTeamInfoTrunks         OCTET STRING,
    portTeamInfoTrunksState    OCTET STRING
    }

portTeamInfoIndex OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The identifier of the port team."
    ::= { portTeamInfoTableEntry 1 }
 
portTeamInfoState OBJECT-TYPE
    SYNTAX  INTEGER  {
        off(1),
        passive(2),
        active(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "State of a port team."
    ::= { portTeamInfoTableEntry 2 }
 
portTeamInfoPorts OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port list in the port team. The ports are presented in
         bitmap format.
 
         in receiving order:

             OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx .....
             |    |||_ port 8
             |    ||
             |    ||___ port 7
             |    |____ port 6
             |      .    .   .
             |_________ port 1

         where x : 1 - The represented port is added to the port team
                   0 - The represented port is not added to the port team"
    ::= { portTeamInfoTableEntry 3 }
 
portTeamInfoPortsState OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port state list in the port team. The ports states are presented in
         bitmap format.
 
         in receiving order:

             OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx .....
             |    |||_ port 8 state
             |    ||
             |    ||___ port 7 state
             |    |____ port 6 state
             |      .    .   .
             |_________ port 1 state

         where x : 1 - The represented port in that team is up
                   0 - If the represented port is added in that team then
                       the port state is down otherwise the port is not 
                       added into that team( check whether port is added 
                       to the team or not through the mib portTeamInfoPorts)."
    ::= { portTeamInfoTableEntry 4 }
 
portTeamInfoTrunks OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The trunk list in the port team. The trunks are presented in
         bitmap format.
 
         in receiving order:

             OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx .....
             |    |||_ trunk 8
             |    ||
             |    ||___ trunk 7
             |    |____ trunk 6
             |      .    .   .
             |_________ trunk 1

         where x : 1 - The represented trunk belongs to the port team
                   0 - The represented trunk does not belong to the port team"
    ::= { portTeamInfoTableEntry 5 }

portTeamInfoTrunksState OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The trunk state list in the trunk team. The trunks states are presented in
         bitmap format.

         in receiving order:

             OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx .....
             |    |||_ trunk 8 state
             |    ||
             |    ||___ trunk 7 state
             |    |____ trunk 6 state
             |      .    .   .
             |_________ trunk 1 state

         where x : 1 - The represented trunk in that team is up
                   0 - If the represented trunk is added in that team then
                       the trunk state is down otherwise the port is
                       not added into that team( check whether it is added
                       to the team or not through the mib portTeamInfoTrunks)."
    ::= { portTeamInfoTableEntry 6 }


-- FDB Statistics
 
fdbStatsCreates OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Number of entries created in the Forwarding Database."
    ::= { fdbStats 1 }

fdbStatsDeletes OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Number of entries deleted from the Forwarding Database."
    ::= { fdbStats 2 }

fdbStatsCurrent OBJECT-TYPE
    SYNTAX  Gauge32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Current number of entries in the Forwarding Database."
    ::= { fdbStats 3 }

fdbStatsHiwat OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Highest number of entries recorded at any given time in the 
         Forwarding Database."
    ::= { fdbStats 4 }

fdbStatsLookups OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Number of entry lookups in the Forwarding Database."
    ::= { fdbStats 5 }

fdbStatsLookupFails OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Number of unsuccessful searches made in the Forwarding Database."
    ::= { fdbStats 6 }

fdbStatsFinds OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Number of searches in the Forwarding Database."
    ::= { fdbStats 7 }

fdbStatsFindFails OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Number of search failures in the Forwarding Database."
    ::= { fdbStats 8 }

fdbStatsFindOrCreates OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Number of entries found or created in the Forwarding Database."
    ::= { fdbStats 9 }

fdbStatsOverflows OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Number of entries overflowing the Forwarding Database."
    ::= { fdbStats 10 }

-- STP Statistics

stgStatsPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF StgStatsPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of Spanning Tree Group port statistics."
    ::= { stpStats 1 }

stgStatsPortTableEntry OBJECT-TYPE
    SYNTAX StgStatsPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Statistics about port of a particular Spanning Tree Group."
    INDEX { stgStatsStpIndex, stgStatsPortIndex }
    ::= { stgStatsPortTable 1 }

StgStatsPortTableEntry ::= SEQUENCE {
    stgStatsStpIndex            Integer32,
    stgStatsPortIndex	        Integer32,
    stgStatsPortRcvCfgBpdus     Counter32,
    stgStatsPortRcvTcnBpdus     Counter32,
    stgStatsPortXmtCfgBpdus     Counter32,
    stgStatsPortXmtTcnBpdus     Counter32 
    }

stgStatsStpIndex OBJECT-TYPE
    SYNTAX Integer32  
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The identifier of a particular Spanning Tree Group."
    ::= { stgStatsPortTableEntry 1 }

stgStatsPortIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The port identifier of a particular Spanning Tree Group."
    ::= { stgStatsPortTableEntry 2 }

stgStatsPortRcvCfgBpdus OBJECT-TYPE
    SYNTAX Counter32 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Number of Configuration BPDU's received on this port."
    ::= { stgStatsPortTableEntry 3 }

stgStatsPortRcvTcnBpdus OBJECT-TYPE
    SYNTAX Counter32 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Number of TCN BPDU's received on this port."
    ::= { stgStatsPortTableEntry 4 }

stgStatsPortXmtCfgBpdus OBJECT-TYPE
    SYNTAX Counter32 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Number of Configuration BPDU's trasmitted from the port."
    ::= { stgStatsPortTableEntry 5 }

stgStatsPortXmtTcnBpdus OBJECT-TYPE
    SYNTAX Counter32 
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Number of TCN BPDU's trasmitted from the port."
    ::= { stgStatsPortTableEntry 6 }

fdbClear OBJECT-TYPE
    SYNTAX  INTEGER {
        ok(1),
        clear(2)
        }
    MAX-ACCESS  read-write
    STATUS  current 
    DESCRIPTION
        "Setting this value to clear(2) clears the entire master FDB."
    ::= { fdbInfo 1 }

--  FDB table
fdbTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF FdbEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "The table of FDB entries."
    ::= { fdbInfo 2 }

fdbEntry OBJECT-TYPE
    SYNTAX  FdbEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
        "A row in the FDB table"
    INDEX   { fdbMacAddr }
    ::= { fdbTable 1 }

FdbEntry ::= SEQUENCE {
    fdbMacAddr            PhysAddress,
    fdbVlan       	  Integer32,
    fdbSrcPort            Integer32,
    fdbSrcTrunk           Integer32,
    fdbState              INTEGER,
    fdbRefSps             DisplayString,
    fdbLearnedPort        Integer32
    }

fdbMacAddr OBJECT-TYPE
    SYNTAX  PhysAddress
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The MAC address for the FDB entry."
    ::= { fdbEntry 1 }

fdbVlan OBJECT-TYPE 
    SYNTAX  Integer32 
    MAX-ACCESS  read-only 
    STATUS  current 
    DESCRIPTION 
        "The VLAN ID for the FDB entry." 
    ::= { fdbEntry 2 }

fdbSrcPort OBJECT-TYPE  
    SYNTAX  Integer32 
    MAX-ACCESS  read-only  
    STATUS  current  
    DESCRIPTION  
       "Either the value '0', or the port number of the port on which a frame 
        having a source address equal to the value of the corresponding 
        instance has been seen.  A value of '0' indicates that the port 
        number has not been learned but that the bridge does have some
        forwarding/filtering information about this address."
    ::= { fdbEntry 3 }

fdbState OBJECT-TYPE  
    SYNTAX  INTEGER {
        unknown(1),
        ignore(2),
        forward(3),
        flood(4),
        ffd(5),
        trunk(6),
        vir(7),
        vsr(8),
        vpr(9),
        other(10)
        }
    MAX-ACCESS  read-only  
    STATUS  current  
    DESCRIPTION  
        "The state of the FDB entry. The meanings of the values are :
         unknown(1) : the MAC address has not yet been learned by the switch
                      but has only been seen as a destination address
         forward(3) : the MAC address has been learned by the switch
         flood(4)   : the MAC address is a multicast destination address 
         trunk(6)   : frames with this MAC address are forwarded to trunk
                      group
         vir(7)     : frames with this MAC address are forwarded for L3 
                      processing"
    ::= { fdbEntry 4 }

fdbRefSps OBJECT-TYPE   
    SYNTAX  DisplayString (SIZE(0..32))
    MAX-ACCESS  read-only   
    STATUS  current   
    DESCRIPTION   
        "The referenced SPs associated with this FDB entry."   
    ::= { fdbEntry 5 }

fdbLearnedPort OBJECT-TYPE   
    SYNTAX  Integer32  
    MAX-ACCESS  read-only   
    STATUS  current   
    DESCRIPTION   
        "The learned port associated with this FDB entry."   
    ::= { fdbEntry 6 }

fdbSrcTrunk OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
       "Either the value '0', or the trunk number of the trunk on which a frame
        having a source address equal to the value of the corresponding
        instance has been seen.  A value of '0' indicates that the source
        address is not associated with a trunk."
    ::= { fdbEntry 7 }

-- STP information

stpInfoTable OBJECT-TYPE
    SYNTAX SEQUENCE OF StpInfoTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of Spanning Tree Group information."
    ::= { stpInfo 1 }

stpInfoTableEntry OBJECT-TYPE
    SYNTAX StpInfoTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about a particular Spanning Tree Group."
    INDEX { stpInfoIndex }
    ::= { stpInfoTable 1 }

StpInfoTableEntry ::= SEQUENCE {
    stpInfoIndex              Integer32,
    stpInfoTimeSinceTopChange TimeTicks,
    stpInfoTopChanges         Counter32,
    stpInfoDesignatedRoot     BridgeId,
    stpInfoRootCost           Integer32,
    stpInfoRootPort           Integer32,
    stpInfoMaxAge             Integer32,
    stpInfoHelloTime          Integer32,
    stpInfoForwardDelay       Integer32,
    stpInfoHoldTime           Integer32
    }

stpInfoIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The identifier of a particular Spanning Tree Group.  This is also
         index to the entLogicalTable of Entity MIB."
    ::= { stpInfoTableEntry 1 }

stpInfoTimeSinceTopChange OBJECT-TYPE
    SYNTAX  TimeTicks
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The time (in hundredths of a second) since the last time a topology 
         change was detected by the bridge entity."
    ::= { stpInfoTableEntry 2 }

stpInfoTopChanges OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The total number of topology changes detected by this bridge since 
         the management entity was last reset or initialized."
    ::= { stpInfoTableEntry 3 }

stpInfoDesignatedRoot OBJECT-TYPE
    SYNTAX  BridgeId
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The bridge identifier of the root of the spanning tree as determined 
         by the Spanning Tree Protocol as executed by this node.  This value 
         is used as the Root Identifier parameter in all Configuration Bridge 
         PDUs originated by this node."
    ::= { stpInfoTableEntry 4 }

stpInfoRootCost OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The cost of the path to the root as seen from this bridge."
    ::= { stpInfoTableEntry 5 }

stpInfoRootPort OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port number of the port which offers the lowest cost path from 
         this bridge to the root bridge."
    ::= { stpInfoTableEntry 6 }

stpInfoMaxAge OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The maximum age of Spanning Tree Protocol information learned from 
         the network on any port before it is discarded, in units of 
         hundredths of a second.  This is the actual value that this bridge is
         currently using."
    ::= { stpInfoTableEntry 7 }

stpInfoHelloTime OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The amount of time between the transmission of Configuration bridge 
         PDUs by this node on any port when it is the root of the spanning 
         tree or trying to become so, in units of hundredths of a second.
         This is the actual value that this bridge is currently using."
    ::= { stpInfoTableEntry 8 }

stpInfoForwardDelay OBJECT-TYPE
     SYNTAX  Integer32
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
         "This time value, measured in units of hundredths of a second, 
          controls how fast a port changes its spanning state when moving 
          towards the Forwarding state.  The value determines how long the port
          stays in each of the Listening and Learning states, which precede 
          the Forwarding state.  This value is also used, when a topology 
          change has been detected and is underway, to age all dynamic entries
          in the Forwarding Database."
    ::= { stpInfoTableEntry 9 }

stpInfoHoldTime OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "This time value determines the interval length during which no more 
         than two Configuration bridge PDUs shall be transmitted by this node,
         in units of hundredths of a second."
    ::= { stpInfoTableEntry 10 }

stpInfoPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF StpInfoPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of Spanning Tree Group port information."
    ::= { stpInfo 2 }

stpInfoPortTableEntry OBJECT-TYPE
    SYNTAX StpInfoPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about port configuration for a particular Spanning Tree
         Group."
    INDEX { stpInfoPortStpIndex, stpInfoPortIndex }
    ::= { stpInfoPortTable 1 }

StpInfoPortTableEntry ::= SEQUENCE {
    stpInfoPortStpIndex           Integer32,
    stpInfoPortIndex              Integer32,
    stpInfoPortState              INTEGER,
    stpInfoPortDesignatedRoot     BridgeId,
    stpInfoPortDesignatedCost     Integer32,
    stpInfoPortDesignatedBridge   BridgeId,
    stpInfoPortDesignatedPort     OCTET STRING,
    stpInfoPortForwardTransitions Counter32,
    stpInfoPortRole               INTEGER,
    stpInfoPortLinkType           INTEGER,
    stpInfoPortEdge               INTEGER,
    stpInfoPortPathCost           Integer32
   }

stpInfoPortStpIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The identifier of a particular Spanning Tree Group."
    ::= { stpInfoPortTableEntry 1 }

stpInfoPortIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The port identifier of a particular Spanning Tree Group."
    ::= { stpInfoPortTableEntry 2 }

stpInfoPortState OBJECT-TYPE
    SYNTAX  INTEGER {
        disabled(1),
        blocking(2),
        listening(3),
        learning(4),
        forwarding(5),
        broken(6),
        discarding(7)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port's current state as defined by application of the Spanning 
         Tree Protocol.  This state controls what action a port takes on
         reception of a frame.  If the bridge has detected a port that is 
         malfunctioning it will place that port into the broken(6) state.  
         For ports which are disabled, this object will have a value of 
         disabled(1)."
    ::= { stpInfoPortTableEntry 3 }

stpInfoPortDesignatedRoot OBJECT-TYPE
    SYNTAX  BridgeId
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The unique Bridge Identifier of the Bridge recorded as the Root in 
         the Configuration BPDUs transmitted by the Designated Bridge for the
         segment to which the port is attached."
    ::= { stpInfoPortTableEntry 4 }

stpInfoPortDesignatedCost OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The path cost of the Designated Port of the segment connected to this
         port.  This value is compared to the Root Path Cost field in received
         bridge PDUs."
    ::= { stpInfoPortTableEntry 5 }

stpInfoPortDesignatedBridge OBJECT-TYPE
    SYNTAX  BridgeId
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Bridge Identifier of the bridge which this port considers to be 
         the Designated Bridge for this port's segment."
    ::= { stpInfoPortTableEntry 6 }

stpInfoPortDesignatedPort OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE (2))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Port Identifier of the port on the Designated Bridge for this 
         port's segment."
    ::= { stpInfoPortTableEntry 7 }

stpInfoPortForwardTransitions OBJECT-TYPE
    SYNTAX  Counter32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The number of times this port has transitioned from the Learning 
         state to the Forwarding state."
    ::= { stpInfoPortTableEntry 8 }

stpInfoPortPathCost OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The path cost of the port."
    ::= { stpInfoPortTableEntry 9 }

stpInfoPortRole OBJECT-TYPE
    SYNTAX  INTEGER {
        disabled(1),
        alternate(2),
        backup(3),
        root(4),
        designated(5),
        master(6),
        unknown(7)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port role. Returns unknown(7) when MSTP/RSTP is not enabled,
         otherwise returns appropriate port role."
    ::= { stpInfoPortTableEntry 10 }

stpInfoPortLinkType OBJECT-TYPE
    SYNTAX  INTEGER {
        p2p(1),
        shared(2),
        unknown(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The point-to-point status of the LAN segment attached
         to this port.  A value of p2p (1) indicates that this port is being
         treated as if it is connected to a point-to-point link.
         A value of shared(2) indicates that this port is being treated as
         having a shared media connection."
    ::= { stpInfoPortTableEntry 11 }

stpInfoPortEdge OBJECT-TYPE
    SYNTAX  INTEGER {
        enabled(1),
        disabled(2)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port is an edge port or not. Returns disabled(2) when the port is
	 not an edge port and returns enabled(1) when it is an edge port."
    ::= { stpInfoPortTableEntry 12 }

-- LACP information 
lacpInfoPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF LacpInfoPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of LACP port information."
    ::= { lacpInfo 1 }

lacpInfoPortTableEntry OBJECT-TYPE
    SYNTAX LacpInfoPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about a LACP port."
    INDEX { lacpInfoPortIndex }
    ::= { lacpInfoPortTable 1 }

LacpInfoPortTableEntry ::= SEQUENCE {
    lacpInfoPortIndex           Integer32,
    lacpInfoPortSelected        INTEGER,
    lacpInfoPortNtt             INTEGER,
    lacpInfoPortReadyN          INTEGER,
    lacpInfoPortMoved           INTEGER
    }

lacpInfoPortIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The port identifier."
    ::= { lacpInfoPortTableEntry 1 }

lacpInfoPortSelected OBJECT-TYPE
    SYNTAX  INTEGER {
        selected(1),
        unselected(2),
        standby(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Selected flag value indicates that the selection logic has selected
         an appropriate Aggregator. A value of unselected indicates that no 
         aggregator is currently selected. A value of standby indicates that
         although the selection logic has selected an appropriate Aggregator,
         aggregation restrictions currently precent the port from being 
         enabled as part of the aggregation, and so the port is being held
         in standby condition." 
    ::= { lacpInfoPortTableEntry 2 }

lacpInfoPortNtt OBJECT-TYPE
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS read-only
    STATUS  current
    DESCRIPTION
        "Need to transmit flag. True indicates that there is new protocol 
         information that should be transmitted on the link."
    ::= { lacpInfoPortTableEntry 3 }

lacpInfoPortReadyN OBJECT-TYPE
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS read-only
    STATUS  current
    DESCRIPTION
        "True value for Ready_N flag indicates that the wait while timer 
         has expired and it is waiting to attach to an aggregator. 
         There is one Ready_N value for each port."
    ::= { lacpInfoPortTableEntry 4 }

lacpInfoPortMoved OBJECT-TYPE
    SYNTAX  INTEGER {
        true(1),
        false(2)
        }
    MAX-ACCESS read-only
    STATUS  current
    DESCRIPTION
        "Port Moved flag is set to true if the receive machine for a port 
         is in the port_disabled state, and the combination of partner oper
         system and partner oper port number in use by the port has been 
         used by received in an incoming LACPDU on a different port."
    ::= { lacpInfoPortTableEntry 5 }

-- CIST Information

cistRoot OBJECT-TYPE
    SYNTAX  BridgeId
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The bridge identifier of the Root of the common spanning
         tree as determined by the Spanning Tree Protocol
         as executed by this node.  This value is used as
         the CIST Root Identifier parameter in all Configuration
         Bridge PDUs originated by this node."
    ::= { cistGeneralInfo 1 } 

cistRootPathCost OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The cost of the path to the CIST Root as seen from this bridge."
    ::= { cistGeneralInfo 2 } 

cistRootPort OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION 
        "The Port Number of the Port which offers the lowest path cost from 
        this bridge to the CIST Root Bridge."
    ::= { cistGeneralInfo 3 } 

cistBridgeHelloTime OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The amount of time between the transmission of Configuration bridge
         PDUs in seconds."
    ::= { cistGeneralInfo 4 } 

cistBridgeMaxAge OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for MaxAge when this bridge
         is acting as the root."
    ::= { cistGeneralInfo 5 } 

cistBridgeForwardDelay OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The value in seconds that all bridges use for ForwardDelay when this 
         bridge is acting as the root."
    ::= { cistGeneralInfo 6 } 

cistRegionalRoot OBJECT-TYPE
    SYNTAX  BridgeId
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The bridge identifier of the Root of the Multiple
         spanning tree region as determined by the Spanning Tree
         Protocol as executed by this node.  This value is used as
         the CIST Regional Root Identifier parameter in all Configuration
         Bridge PDUs originated by this node."
   ::= { cistGeneralInfo 7 } 

cistRegionalPathCost OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The Cost of the path to the CIST Regional Root as seen from this 
         bridge."
   ::= { cistGeneralInfo 8 } 


-- CIST Port Information Table
cistInfoPortTable OBJECT-TYPE
    SYNTAX SEQUENCE OF CistInfoPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of CIST Port information."
    ::= { cistInfo 2 }

cistInfoPortTableEntry OBJECT-TYPE
    SYNTAX CistInfoPortTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about a particular CIST Port."
    INDEX { cistInfoPortIndex }
    ::= { cistInfoPortTable 1 }

CistInfoPortTableEntry ::= SEQUENCE {
    cistInfoPortIndex            Integer32,
    cistInfoPortPriority         Integer32,
    cistInfoPortPathCost         Integer32,
    cistInfoPortState            INTEGER,
    cistInfoPortRole             INTEGER,
    cistInfoPortDesignatedBridge BridgeId,
    cistInfoPortDesignatedPort   OCTET STRING,
    cistInfoPortLinkType         INTEGER
    }

cistInfoPortIndex OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The port number of the port for which this entry contains spanning
         tree configuration."
    ::= { cistInfoPortTableEntry 1 }

cistInfoPortPriority OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The four most significant bits of the Port Identifier of the 
         Spanning Tree instance can be modified by setting this value."
    ::= { cistInfoPortTableEntry 2 }

cistInfoPortPathCost OBJECT-TYPE
    SYNTAX Integer32
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The contribution of this port to the path cost of paths towards 
         the CIST Root which include this port."
    ::= { cistInfoPortTableEntry 3 }

cistInfoPortState OBJECT-TYPE
    SYNTAX INTEGER {
        disabled (1),
        discarding (2),
        learning (4),
        forwarding (5)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "Current state of the Port as defined by the Common    
         spanning tree protocol." 
    ::= { cistInfoPortTableEntry 4 }

cistInfoPortRole OBJECT-TYPE
    SYNTAX INTEGER {
        disabled(1),
        alternate(2),
        backup(3),
        root(4),
        designated(5),
        master(6),
        unknown(7)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
          "Selected Port Role of the port for this spanning tree instance."
    ::= { cistInfoPortTableEntry 5 }

cistInfoPortDesignatedBridge OBJECT-TYPE
    SYNTAX  BridgeId
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The unique Bridge Identifier of the bridge which this port  
         considers to be the Designated Bridge for the port's segment."   
    ::= { cistInfoPortTableEntry 6 }

cistInfoPortDesignatedPort OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE (2))
    MAX-ACCESS  read-only
    STATUS  current
      DESCRIPTION
          "The Port identifier of the port on the Designated Bridge    
           for this port's segment."                                           
    ::= { cistInfoPortTableEntry 7 }

cistInfoPortLinkType OBJECT-TYPE
    SYNTAX INTEGER {
        p2p(1),
        shared(2),
        unknown(3)
        }
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The point-to-point status of the LAN segment attached 
         to this port.  A value of p2p (2) indicates that this port is being
         treated as if it is connected to a point-to-point link. 
         A value of shared(3) indicates that this port is being treated as 
         having a shared media connection."
    ::= { cistInfoPortTableEntry 8 }

-- VLAN information

vlanInfoTable OBJECT-TYPE
    SYNTAX SEQUENCE OF VlanInfoTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "The table of VLAN information."
    ::= { vlanInfo 1 }

vlanInfoTableEntry OBJECT-TYPE
    SYNTAX VlanInfoTableEntry
    MAX-ACCESS not-accessible
    STATUS current
    DESCRIPTION
        "Information about a particular VLAN."
    INDEX { vlanInfoId }
    ::= { vlanInfoTable 1 }

VlanInfoTableEntry ::= SEQUENCE {
    vlanInfoId                INTEGER,
    vlanInfoName 	      DisplayString,
    vlanInfoStatus            INTEGER,
    vlanInfoJumbo             INTEGER,
    vlanInfoBwmContract       Integer32,
    vlanInfoLearn             INTEGER,
    vlanInfoPorts             OCTET STRING
    }

vlanInfoId OBJECT-TYPE
    SYNTAX  INTEGER  (1..4090)
    MAX-ACCESS read-only
    STATUS current
    DESCRIPTION
        "The VLAN identifier."
    ::= { vlanInfoTableEntry 1 }

vlanInfoName OBJECT-TYPE
    SYNTAX  DisplayString (SIZE(0..32))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The VLAN name."
    ::= { vlanInfoTableEntry 2 }

vlanInfoStatus OBJECT-TYPE
    SYNTAX  INTEGER  {
	enabled(2),
	disabled(3)
	}
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable, VLAN state information"
    ::= { vlanInfoTableEntry 3 }

vlanInfoJumbo OBJECT-TYPE
    SYNTAX  INTEGER  {
	enabled(2),
	disabled(3)
	}
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable Jumbo frames, Jumbo frames state 
         information of a VLAN"
    ::= { vlanInfoTableEntry 4 }

vlanInfoBwmContract OBJECT-TYPE
    SYNTAX  Integer32
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Default BWM contract number information of a VLAN "
    ::= { vlanInfoTableEntry 5 }

vlanInfoLearn OBJECT-TYPE
    SYNTAX  INTEGER  {
        enabled(2),
        disabled(3)
        }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "Enable or disable source MAC address learning, MAC address
         learning information of a VLAN"
    ::= { vlanInfoTableEntry 6 }

vlanInfoPorts OBJECT-TYPE
    SYNTAX  OCTET STRING
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
        "The port list information in the VLAN. The ports are presented 
         in bitmap format.
	 in receiving order:

	     OCTET 1  OCTET 2  .....
             xxxxxxxx xxxxxxxx ..... 
             ||    || |_ port 8
             ||    ||  
             ||    ||___ port 7
             ||    |____ port 6
             ||      .    .   .
             ||_________ port 1
             |__________ reserved

         where x : 1 - The represented port belongs to the VLAN
		   0 - The represented port does not belong to the VLAN"
    ::= { vlanInfoTableEntry 7 }
END

