RADLAN-LLDP-MIB DEFINITIONS ::= BEGIN

-- Title:                RADLAN LLDP ROS
--                       Private LLDP MIB
-- Version:              7.42
-- Date:                 12 Dec 2005

IMPORTS
    rnd                                     FROM RADLAN-MIB
    OBJECT-TYPE, MODULE-IDENTITY            FROM SNMPv2-SMI
    TruthValue                              FROM RADLAN-SNMPv2;

rlLldp MODULE-IDENTITY
         LAST-UPDATED "200506200000Z"
         ORGANIZATION "Radlan Computer Communications Ltd."
         CONTACT-INFO
                "radlan.com"
         DESCRIPTION
                "This private MIB module adds MIBs to LLDP (Link Layer Discovery Protocol)."
         REVISION "200506200000Z"
         DESCRIPTION
                "Initial revision."
        ::= { rnd 110 }

rlLldpEnabled OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "Setting this variable to 'true' will globally enable the LLDP feature
             (both transmit and receive functionalities). Setting this variable
             to 'false' will globally disable the LLDP feature. Thus, the
             administratively desired status of a local port is determined by
             both this variable and the MIB lldpPortConfigAdminStatus."
    ::= { rlLldp 1 }

--rlLldpLocChassisId  OBJECT-TYPE
--    SYNTAX      OCTET STRING(SIZE(1..20))
--    MAX-ACCESS  read-write
--    STATUS      current
--    DESCRIPTION
--            "The string value used to identify the chassis component associated
--             with the local system. As a result of updating this variable,
--             lldpLocChassisid will have the same value, and the MIB
--             lldpLocChassisIdSubtype will have the value local(7). "
--    ::= { rlLldp 2}

END

