HP-USER-AUTH DEFINITIONS ::= BEGIN

    IMPORTS
        hpSwitch            
            FROM HP-ICF-OID            
        InterfaceIndex            
            FROM IF-MIB            
        VlanIndex            
            FROM Q-BRIDGE-MIB            
        SnmpAdminString            
            FROM SNMP-FRAMEWORK-MIB            
        OBJECT-GROUP, MODULE-COMPLIANCE, NOTIFICATION-GROUP            
            FROM SNMPv2-CONF            
        IpAddress, Integer32, Unsigned32, OBJECT-TYPE, 
        MODULE-IDENTITY, NOTIFICATION-TYPE            
            FROM SNMPv2-SMI            
        RowStatus
            FROM SNMPv2-TC
        TruthValue, MacAddress            
            FROM SNMPv2-TC
        InetAddressType, InetAddress
            FROM INET-ADDRESS-MIB;


    -- 1.3.6.1.4.1.11.2.14.11.5.1.19
    hpicfUsrAuthMIB MODULE-IDENTITY 
        LAST-UPDATED "200708290000Z"      -- August 29, 2007 at 00:00 GMT
        ORGANIZATION 
            "Hewlett-Packard Company
            ProCurve Networking Business"
        CONTACT-INFO 
            "Hewlett-Packard Company
            8000 Foothills Blvd.
            Roseville, CA 95747
            www.ProCurve.com"
        DESCRIPTION 
            "This MIB module contains the definitions of Managed
            Objects for various subsystems that perform 
            user authentication. The subsystems under control
            by this MIB are:
            'WebAuth' - Web-based login authentication
            'MacAuth' - MAC addresss-based authentication
            'CLI Password' - CLI-based login authentication"
        REVISION "200708290000Z"      -- August 29, 2007 at 00:00 GMT
        DESCRIPTION 
            "Added hpicfUsrAuthWMA failure notification and objects"
        REVISION "200305231020Z"      -- May 23, 2003 at 10:20 GMT
        DESCRIPTION 
            "Initial revision."
        REVISION "200508050000Z"      -- August 05, 2005 at 00:00 GMT
        DESCRIPTION 
            "Added import objects."
        REVISION "200706221200Z"      -- June 22, 2007 at 12:00 GMT
        DESCRIPTION 
            "Added hpicfUsrAuthNotifyConformance group and objects."
        ::= { hpSwitch 19 }

    
--
-- Node definitions
--

    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.0
    hpicfUsrAuthNotifications OBJECT IDENTIFIER ::= { hpicfUsrAuthMIB 0 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.0.1
    hpicfUsrAuthCLIAuthFail NOTIFICATION-TYPE
        OBJECTS { hpicfUsrAuthCLIFailCnt, hpicfUsrAuthCLIInterface }
        STATUS current
        DESCRIPTION 
            "An hpicfUsrAuthCLIPasswd notification signifies that
            CLI password authentication has failed.
            Operational control of this notification is provided
            using hpicfUsrAuthCliNotifyEnable.
            "
        ::= { hpicfUsrAuthNotifications 1 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.0.2
    hpicfUsrAuthPasswdChng NOTIFICATION-TYPE
        OBJECTS { hpicfUsrAuthCLIPasswdSet, hpicfUsrAuthCLIPwdNotifyCnt }
        STATUS current
        DESCRIPTION 
            "An hpicfUsrAuthPasswdChng notification signifies that
                         the manager password has been changed.  The value of 
                         hpicfUsrAuthCLIPasswdSet can be used to determine
                         whether the password has been set or cleared by this action.
            "
        ::= { hpicfUsrAuthNotifications 2 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.0.3
    hpicfPortSecAuthFailure NOTIFICATION-TYPE
        OBJECTS { hpicfUsrAuthWMAFailCnt, 
            hpicfUsrAuthWMAFailVlan, 
            hpicfUsrAuthWMAFailPort, 
            hpicfUsrAuthWMAFailMAC }
        STATUS current
        DESCRIPTION 
            "This notification indicates a failed Port Security
            (network access) authentication event."
        ::= { hpicfUsrAuthNotifications 3 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.1
    hpicfUsrAuthSystem OBJECT IDENTIFIER ::= { hpicfUsrAuthMIB 1 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.1.1
    hpicfUsrAuthWebAuthDhcpBaseAddress OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "For all ports running with web authentication 
            enabled: Specifies the base address that should 
            be used by the switch DHCP server for web-based 
            authentication purposes."
        ::= { hpicfUsrAuthSystem 1 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.1.2
    hpicfUsrAuthWebAuthDhcpMask OBJECT-TYPE
        SYNTAX IpAddress
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "For all ports running with web authentication
            enabled: Specifies the subnet mask to be used in 
            conjunction with the DHCP base address when 
            servicing DHCP requests.
            
            Allowable mask range is 255.255.240.0 (20) to 
            255.255.255.0 (24)."
        ::= { hpicfUsrAuthSystem 2 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.1.3
    hpicfUsrAuthWebAuthDhcpLease OBJECT-TYPE
        SYNTAX Integer32 (1..30)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "For all ports running with web authentication
            enabled: Specifies the DHCP lease length in 
            seconds."
        ::= { hpicfUsrAuthSystem 3 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.1.4
    hpicfUsrAuthMacAuthAddrFormat OBJECT-TYPE
        SYNTAX INTEGER
            {
            noDelimiter(1),
            singleDash(2),
            multiDash(3),
            multiColon(4),
            noDelimiterUppercase(5),
            singleDashUppercase(6),
            multiDashUppercase(7),
            multiColonUppercase(8)
            }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "For all ports running with MAC authentication
            enabled: Specifies the MAC address format to use
            in the RADIUS access-request, as follows:
                    'noDelimiter'  - Sends MAC address in  aabbccddeeff format
                    'singleDash'   - Sends MAC address in aabbcc-ddeeff format
                    'multiDash'    - Sends MAC address in aa-bb-cc-dd-ee-ff format
                    'multiColon'   - Sends MAC address in aa:bb:cc:dd:ee:ff format
                    'noDelimiterUppercase'  - Sends MAC address in AABBCCDDEEFF format
                    'singleDashUppercase'   - Sends MAC address in AABBCC-DDEEFF format
                    'multiDashUppercase'    - Sends MAC address in AA-BB-CC-DD-EE-FF format
                    'multiColonUppercase'   - Sends MAC address in AA:BB:CC:DD:EE:FF format
            The default value is noDelimiter(1)."
        ::= { hpicfUsrAuthSystem 4 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.1.5
    hpicfUsrAuthCliNotifyEnable OBJECT-TYPE
        SYNTAX INTEGER
            {
            enabled(1),
            disabled(2)
            }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The operational status of hpicfUsrAuthCliAuthFail notifications.
            The default value is ‘1’ (Enabled).  A value of ‘2’ represents 
            Disabled.  Writing this object requires authentication, such 
            as provided by SNMPv3.
            "
        ::= { hpicfUsrAuthSystem 5 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.1.6
    hpicfUsrAuthCLIInterface OBJECT-TYPE
        SYNTAX INTEGER
            {
            serial(1),
            telnet(2),
            ssh(3),
            other(9)
            }
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
            "Denotes the interface that is generating the notification.
            "
        ::= { hpicfUsrAuthSystem 6 }

    
--  
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.1.7
    hpicfUsrAuthCLIPasswdSet OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
            "Indicates whether the CLI manager password
            is set.  ‘1’ indicates True while ‘2’
            indicates False.
            "
        ::= { hpicfUsrAuthSystem 7 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.1.8
    hpicfUsrAuthCLIFailCnt OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
            "The count of hpicfUsrAuthPasswdFail notifications sent by the hpicfUsrAuth
            entity to the SNMP entity.  The actual count of notifications sent by SNMP
            may be lower due to rate limiting or configuration."
        ::= { hpicfUsrAuthSystem 8 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.1.9
    hpicfUsrAuthCLIPwdNotifyCnt OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
            "A count of CLI password change notifications
            sent from the Auth entity to the SNMP entity
            within the switch.  This count may therefore differ from
            the count of notifications actually sent by the SNMP
            entity due to switch configuration (e.g., the value
            of hpicfUsrAuthNotifyEnable.)"
        ::= { hpicfUsrAuthSystem 9 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.1.10
    hpicfUsrAuthWMAFailCnt OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
            "The count of hpicfUsrAuthWMAFail notifications sent by the hpicfUsrAuth
            entity to the SNMP entity.  The actual count of notifications sent by SNMP
            may be lower due to rate limiting or configuration."
        ::= { hpicfUsrAuthSystem 10 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.1.11
    hpicfUsrAuthWMAFailMAC OBJECT-TYPE
        SYNTAX MacAddress
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
            "The MAC address supplied in the failed authentication request."
        ::= { hpicfUsrAuthSystem 11 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.1.12
    hpicfUsrAuthWMAFailPort OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
            "The port index of the failed authentication request."
        ::= { hpicfUsrAuthSystem 12 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.1.13
    hpicfUsrAuthWMAFailVlan OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
            "The VLAN ID associated with the failed authentication request."
        ::= { hpicfUsrAuthSystem 13 }


    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.1.14
    hpicfUsrAuthPortSecNotifyEnable OBJECT-TYPE
        SYNTAX INTEGER
            {
            enabled(1),
            disabled(2)
            }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Provides operational control of hpicfPortSecAuthFailure 
            notification.  When enabled (1), the notification will
            be sent.  When disabled (2), the notification will not 
            be sent.  Setting this object requires authentication,
            such as provided by SNMPv3.
            "
        ::= { hpicfUsrAuthSystem 14 }

   
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.1.15
    hpicfUsrAuthPasswdNotifyEnable OBJECT-TYPE
        SYNTAX INTEGER
            {
            enabled(1),
            disabled(2)
            }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Provides operational control of hpicfUsrAuthPasswdChng notification.  
            When enabled (1), the notification will be sent.  
            When disabled (2), the notification will not be sent.
            Setting this object requires authentication, such
            as provided by SNMPv3."
        ::= { hpicfUsrAuthSystem 15 }


    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.1.16
    --
    -- EWA Server Table
    -- 
    hpicfUsrAuthWMAEWAServerTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HpicfUsrAuthWMAEWAServerEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A table of the Enhanced Web Auth servers." 
        ::= { hpicfUsrAuthSystem 16 } 


    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.1.16.1
    hpicfUsrAuthWMAEWAServerEntry OBJECT-TYPE
              SYNTAX      HpicfUsrAuthWMAEWAServerEntry
              MAX-ACCESS  not-accessible
              STATUS      current
              DESCRIPTION
                "Addresses for an Enhanced Web Auth server."
              INDEX { hpicfUsrAuthWMAeWAServerIndex }
              ::= { hpicfUsrAuthWMAEWAServerTable 1 }


    HpicfUsrAuthWMAEWAServerEntry ::= SEQUENCE {
              hpicfUsrAuthWMAeWAServerIndex                  Integer32,
              hpicfUsrAuthWMAeWAServerIPAddressType          InetAddressType,
              hpicfUsrAuthWMAeWAServerIPAddress              InetAddress,
              hpicfUsrAuthWMAeWAServerPath                   OCTET STRING,           
              hpicfUsrAUthWMAeWAServerRowStatus              RowStatus
      }


    hpicfUsrAuthWMAeWAServerIndex OBJECT-TYPE
              SYNTAX      Integer32 
              MAX-ACCESS  not-accessible
              STATUS      current
              DESCRIPTION
                "Index into hpicfUsrAuthWMAEWAServerTable."
              ::= { hpicfUsrAuthWMAEWAServerEntry 1 }


    hpicfUsrAuthWMAeWAServerIPAddressType OBJECT-TYPE
              SYNTAX      InetAddressType
              MAX-ACCESS  read-create
              STATUS      current
              DESCRIPTION
                "The type of Enhanced Web Auth Server Address."
              DEFVAL { unknown }
              ::= { hpicfUsrAuthWMAEWAServerEntry 2 }


    hpicfUsrAuthWMAeWAServerIPAddress OBJECT-TYPE
              SYNTAX      InetAddress
              MAX-ACCESS  read-create
              STATUS      current
              DESCRIPTION
                "The IP address of the Enhanced Web Auth Server.
                 If set to 0.0.0.0 or URL not configured
                 no Enhanced Web Auth Server will run."
              ::= { hpicfUsrAuthWMAEWAServerEntry 3 }


    hpicfUsrAuthWMAeWAServerPath    OBJECT-TYPE
              SYNTAX       OCTET STRING 
              MAX-ACCESS   read-create
              STATUS       current
              DESCRIPTION 
                "The Enhanced Web Auth Server Path for the location
                 of the Enhanced Web Auth Pages.  If not configured 
                 the default path will be used." 
              ::= { hpicfUsrAuthWMAEWAServerEntry 4 }


    hpicfUsrAUthWMAeWAServerRowStatus OBJECT-TYPE
              SYNTAX       RowStatus
              MAX-ACCESS   read-create
              STATUS       current
              DESCRIPTION 
                "This marks the row as active/inactive." 
              ::= { hpicfUsrAuthWMAEWAServerEntry 5 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.2
    hpicfUsrAuthPorts OBJECT IDENTIFIER ::= { hpicfUsrAuthMIB 2 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.2.1
    hpicfUsrAuthPortTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HpicfUsrAuthPortEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A table of system level information about Web-
            MAC-based authentication for each port in the 
            switch."
        ::= { hpicfUsrAuthPorts 1 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.2.1.1
    hpicfUsrAuthPortEntry OBJECT-TYPE
        SYNTAX HpicfUsrAuthPortEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The port number, operational mode and 
            re-authentication control for each switch port."
        INDEX { hpicfUsrAuthPortNumber }
        ::= { hpicfUsrAuthPortTable 1 }

    
    HpicfUsrAuthPortEntry ::=
        SEQUENCE { 
            hpicfUsrAuthPortNumber
                InterfaceIndex,
            hpicfUsrAuthWebAuthAdminStatus
                TruthValue,
            hpicfUsrAuthMacAuthAdminStatus
                TruthValue,
            hpicfUsrAuthPortReauthenticate
                TruthValue
         }

    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.2.1.1.1
    hpicfUsrAuthPortNumber OBJECT-TYPE
        SYNTAX InterfaceIndex
        MAX-ACCESS accessible-for-notify
        STATUS current
        DESCRIPTION
            "The port number associated with this switch port."
        ::= { hpicfUsrAuthPortEntry 1 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.2.1.1.2
    hpicfUsrAuthWebAuthAdminStatus OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Setting this attribute TRUE enables web-based
            authentication services.  A value of FALSE
            disabled web-based authentication.  This attribute
            cannot be set TRUE concurrently with 
            hpicfUsrAuthMacAuthAdminStatus."
        ::= { hpicfUsrAuthPortEntry 2 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.2.1.1.3
    hpicfUsrAuthMacAuthAdminStatus OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Setting this attribute TRUE enables MAC-based
            authentication services.  A value of FALSE
            disabled MAC-based authentication.  This attribute
            cannot be set TRUE concurrently with 
            hpicfUsrAuthWebAuthAdminStatus."
        ::= { hpicfUsrAuthPortEntry 3 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.2.1.1.4
    hpicfUsrAuthPortReauthenticate OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The reauthentication control for this port. Setting this 
            attribute TRUE forces all authenticated clients to 
            re-authenticate themselves. Setting this attribute FALSE
            has no effect. This attribute always returns FALSE
            when read."
        ::= { hpicfUsrAuthPortEntry 4 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.3
    hpicfUsrAuthWebAuthConfig OBJECT IDENTIFIER ::= { hpicfUsrAuthMIB 3 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.3.1
    hpicfUsrAuthWebAuthConfigTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HpicfUsrAuthWebAuthConfigEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A table that contains the configuration objects for 
            Web-based Authentication associated with each port. An entry
            appears in this table for each port that may authenticate
            access to itself."
        ::= { hpicfUsrAuthWebAuthConfig 1 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.3.1.1
    hpicfUsrAuthWebAuthConfigEntry OBJECT-TYPE
        SYNTAX HpicfUsrAuthWebAuthConfigEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The configuration information for Web-based authentication."
        INDEX { hpicfUsrAuthPortNumber }
        ::= { hpicfUsrAuthWebAuthConfigTable 1 }

    
    HpicfUsrAuthWebAuthConfigEntry ::=
        SEQUENCE { 
            hpicfUsrAuthWebAuthClientLimit
                Integer32,
            hpicfUsrAuthWebAuthClientMoves
                INTEGER,
            hpicfUsrAuthWebAuthSSLState
                INTEGER,
            hpicfUsrAuthWebAuthRedirectUrl
                OCTET STRING,
            hpicfUsrAuthWebAuthQuietPeriod
                Integer32,
            hpicfUsrAuthWebAuthServerTimeout
                Integer32,
            hpicfUsrAuthWebAuthServerMaxReq
                Integer32,
            hpicfUsrAuthWebAuthMaxRetries
                Integer32,
            hpicfUsrAuthWebAuthLogoffPeriod
                Integer32,
            hpicfUsrAuthWebAuthReAuthPeriod
                Integer32,
            hpicfUsrAuthWebAuthAuthVid
                VlanIndex,
            hpicfUsrAuthWebAuthUnauthVid
                VlanIndex
         }

    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.3.1.1.1
    hpicfUsrAuthWebAuthClientLimit OBJECT-TYPE
        SYNTAX Integer32 (1..32)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The maximum number of authenticated clients to allow on 
            the port."
        DEFVAL { 1 }
        ::= { hpicfUsrAuthWebAuthConfigEntry 1 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.3.1.1.2
    hpicfUsrAuthWebAuthClientMoves OBJECT-TYPE
        SYNTAX INTEGER
            {
            disabled(1),
            enabled(2)
            }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Specifies whether client may roam across ports under
            web authentication control. Setting this attribute 
            'enabled'allows authenticated clients to roam to other 
            ports under web authentication control (that also have 
            this attribute set to 'enabled') without requiring a 
            re-authentication.  
            
            Setting this attribute 'disabled' disallows authenticated
            clients from roaming to other ports (regardless of that 
            port's attribute value).  The client has to re-
            authenticate, if it attempts to roam."
        DEFVAL { 1 }
        ::= { hpicfUsrAuthWebAuthConfigEntry 2 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.3.1.1.3
    hpicfUsrAuthWebAuthSSLState OBJECT-TYPE
        SYNTAX INTEGER
            {
            disabled(1),
            enabled(2)
            }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Specifies whether web-based authentication should use an 
            SSL connection (i.e. https://) to switch to collect client  
            credentials.
            Note: A valid certificate must be configured on switch
            before SSL connections are enabled."
        DEFVAL { 1 }
        ::= { hpicfUsrAuthWebAuthConfigEntry 3 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.3.1.1.4
    hpicfUsrAuthWebAuthRedirectUrl OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE (0..127))
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Specifies the URL, to which an authenticated client should
            be re-directed, after successful authentication."
        ::= { hpicfUsrAuthWebAuthConfigEntry 4 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.3.1.1.5
    hpicfUsrAuthWebAuthQuietPeriod OBJECT-TYPE
        SYNTAX Integer32 (1..65535)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Specifies the time, in seconds, that the switch should 
            refrain from re-attempting an authentication request for
            a client whose credentials were rejected."
        DEFVAL { 60 }
        ::= { hpicfUsrAuthWebAuthConfigEntry 5 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.3.1.1.6
    hpicfUsrAuthWebAuthServerTimeout OBJECT-TYPE
        SYNTAX Integer32 (1..300)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Specifies the time, in seconds, that the switch should 
            wait for an authentication reply to return before 
            considering it as timed out."
        DEFVAL { 30 }
        ::= { hpicfUsrAuthWebAuthConfigEntry 6 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.3.1.1.7
    hpicfUsrAuthWebAuthServerMaxReq OBJECT-TYPE
        SYNTAX Integer32 (1..10)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Specifies the number of authentication requests that 
            must time out before failing authentication."
        DEFVAL { 3 }
        ::= { hpicfUsrAuthWebAuthConfigEntry 7 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.3.1.1.8
    hpicfUsrAuthWebAuthMaxRetries OBJECT-TYPE
        SYNTAX Integer32 (1..10)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Specifies the number of authentication requests that
            must fail (i.e. invalid credentials) before failing 
            authentication."
        DEFVAL { 3 }
        ::= { hpicfUsrAuthWebAuthConfigEntry 8 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.3.1.1.9
    hpicfUsrAuthWebAuthLogoffPeriod OBJECT-TYPE
        SYNTAX Integer32 (1..999999999)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Specifies the period, in seconds, at which an 
            authenticated client will be considered unauthenticated
            for a lack of activity (i.e. traffic originating 
            from client)."
        DEFVAL { 300 }
        ::= { hpicfUsrAuthWebAuthConfigEntry 9 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.3.1.1.10
    hpicfUsrAuthWebAuthReAuthPeriod OBJECT-TYPE
        SYNTAX Integer32 (0..999999999)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Specifies the period, in seconds, at which an 
            authenticated client must re-authenticate. A value of 
            0 signifies that an authenticated client will never have 
            to re-authenticate."
        DEFVAL { 0 }
        ::= { hpicfUsrAuthWebAuthConfigEntry 10 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.3.1.1.11
    hpicfUsrAuthWebAuthAuthVid OBJECT-TYPE
        SYNTAX VlanIndex
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Specifies the port VID (PVID) that should be used for 
            an authenticated client."
        ::= { hpicfUsrAuthWebAuthConfigEntry 11 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.3.1.1.12
    hpicfUsrAuthWebAuthUnauthVid OBJECT-TYPE
        SYNTAX VlanIndex
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Specifies the port VID (PVID) that should be used for 
            an unauthenticated client."
        ::= { hpicfUsrAuthWebAuthConfigEntry 12 }

    
-- 
-- 
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.4
    hpicfUsrAuthMacAuthConfig OBJECT IDENTIFIER ::= { hpicfUsrAuthMIB 4 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.4.1
    hpicfUsrAuthMacAuthConfigTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HpicfUsrAuthMacAuthConfigEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A table that contains the configuration objects for 
            Mac-based Authentication associated with each port. An entry
            appears in this table for each port that may authenticate
            access to itself."
        ::= { hpicfUsrAuthMacAuthConfig 1 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.4.1.1
    hpicfUsrAuthMacAuthConfigEntry OBJECT-TYPE
        SYNTAX HpicfUsrAuthMacAuthConfigEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The configuration information for Mac-based authentication."
        INDEX { hpicfUsrAuthPortNumber }
        ::= { hpicfUsrAuthMacAuthConfigTable 1 }

    
    HpicfUsrAuthMacAuthConfigEntry ::=
        SEQUENCE { 
            hpicfUsrAuthMacAuthClientLimit
                Integer32,
            hpicfUsrAuthMacAuthClientMoves
                INTEGER,
            hpicfUsrAuthMacAuthQuietPeriod
                Integer32,
            hpicfUsrAuthMacAuthServerTimeout
                Integer32,
            hpicfUsrAuthMacAuthServerMaxReq
                Integer32,
            hpicfUsrAuthMacAuthLogoffPeriod
                Integer32,
            hpicfUsrAuthMacAuthReAuthPeriod
                Integer32,
            hpicfUsrAuthMacAuthAuthVid
                VlanIndex,
            hpicfUsrAuthMacAuthUnauthVid
                VlanIndex
         }

    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.4.1.1.1
    hpicfUsrAuthMacAuthClientLimit OBJECT-TYPE
        SYNTAX Integer32 (1..32)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The maximum number of authenticated clients to allow on 
            the port."
        DEFVAL { 1 }
        ::= { hpicfUsrAuthMacAuthConfigEntry 1 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.4.1.1.2
    hpicfUsrAuthMacAuthClientMoves OBJECT-TYPE
        SYNTAX INTEGER
            {
            disabled(1),
            enabled(2)
            }
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Specifies whether client may roam across ports under
            web authentication control. Setting this attribute 
            'enabled'allows authenticated clients to roam to other 
            ports under web authentication control (that also have 
            this attribute set to 'enabled') without requiring a 
            re-authentication.  
            
            Setting this attribute 'disabled' disallows authenticated
            clients from roaming to other ports (regardless of that 
            port's attribute value).  The client has to re-
            authenticate, if it attempts to roam."
        DEFVAL { 1 }
        ::= { hpicfUsrAuthMacAuthConfigEntry 2 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.4.1.1.3
    hpicfUsrAuthMacAuthQuietPeriod OBJECT-TYPE
        SYNTAX Integer32 (1..65535)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Specifies the time, in seconds, that the switch should 
            refrain from re-attempting an authentication request for
            a client whose credentials were rejected."
        DEFVAL { 60 }
        ::= { hpicfUsrAuthMacAuthConfigEntry 3 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.4.1.1.4
    hpicfUsrAuthMacAuthServerTimeout OBJECT-TYPE
        SYNTAX Integer32 (1..300)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Specifies the time, in seconds, that the switch should 
            wait for an authentication reply to return before 
            considering it as timed out."
        DEFVAL { 30 }
        ::= { hpicfUsrAuthMacAuthConfigEntry 4 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.4.1.1.5
    hpicfUsrAuthMacAuthServerMaxReq OBJECT-TYPE
        SYNTAX Integer32 (1..10)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Specifies the number of authentication requests that 
            must time out before failing authentication."
        DEFVAL { 3 }
        ::= { hpicfUsrAuthMacAuthConfigEntry 5 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.4.1.1.6
    hpicfUsrAuthMacAuthLogoffPeriod OBJECT-TYPE
        SYNTAX Integer32 (1..999999999)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Specifies the period, in seconds, at which an 
            authenticated client will be considered unauthenticated
            for a lack of activity (i.e. traffic originating 
            from client)."
        DEFVAL { 300 }
        ::= { hpicfUsrAuthMacAuthConfigEntry 6 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.4.1.1.7
    hpicfUsrAuthMacAuthReAuthPeriod OBJECT-TYPE
        SYNTAX Integer32 (0..999999999)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Specifies the period, in seconds, at which an 
            authenticated client must re-authenticate. A value of 
            0 signifies that an authenticated client will never have 
            to re-authenticate."
        DEFVAL { 0 }
        ::= { hpicfUsrAuthMacAuthConfigEntry 7 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.4.1.1.8
    hpicfUsrAuthMacAuthAuthVid OBJECT-TYPE
        SYNTAX VlanIndex
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Specifies the port VID (PVID) that should be used for 
            an authenticated client."
        ::= { hpicfUsrAuthMacAuthConfigEntry 8 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.4.1.1.9
    hpicfUsrAuthMacAuthUnauthVid OBJECT-TYPE
        SYNTAX VlanIndex
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "Specifies the port VID (PVID) that should be used for 
            an unauthenticated client."
        ::= { hpicfUsrAuthMacAuthConfigEntry 9 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.5
    hpicfUsrAuthWebAuthStats OBJECT IDENTIFIER ::= { hpicfUsrAuthMIB 5 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.5.1
    hpicfUsrAuthWebAuthSessionStatsTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HpicfUsrAuthWebAuthSessionStatsEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A table that contains session statistic objects
            for each client (i.e. user) attempting to 
            authenticate to a port with Web-authentication 
            enabled. An entry appears in this table for each 
            port in the switch."
        ::= { hpicfUsrAuthWebAuthStats 1 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.5.1.1
    hpicfUsrAuthWebAuthSessionStatsEntry OBJECT-TYPE
        SYNTAX HpicfUsrAuthWebAuthSessionStatsEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The session statistics information for a port with
            Web-based authentication enabled. This shows
            the current values being collected for active sessions."
        INDEX { hpicfUsrAuthPortNumber, hpicfUsrAuthWebAuthSessionMacAddr }
        ::= { hpicfUsrAuthWebAuthSessionStatsTable 1 }

    
    HpicfUsrAuthWebAuthSessionStatsEntry ::=
        SEQUENCE { 
            hpicfUsrAuthWebAuthSessionMacAddr
                MacAddress,
            hpicfUsrAuthWebAuthSessionName
                SnmpAdminString,
            hpicfUsrAuthWebAuthSessionState
                INTEGER,
            hpicfUsrAuthWebAuthSessionStateTime
                Unsigned32,
            hpicfUsrAuthWebAuthSessionAuthVid
                VlanIndex,
            hpicfUsrAuthWebAuthSessionUnauthVid
                VlanIndex
         }

    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.5.1.1.1
    hpicfUsrAuthWebAuthSessionMacAddr OBJECT-TYPE
        SYNTAX MacAddress
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Specifies the MAC address of the client."
        ::= { hpicfUsrAuthWebAuthSessionStatsEntry 1 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.5.1.1.2
    hpicfUsrAuthWebAuthSessionName OBJECT-TYPE
        SYNTAX SnmpAdminString
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Specifies the username of the client."
        ::= { hpicfUsrAuthWebAuthSessionStatsEntry 2 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.5.1.1.3
    hpicfUsrAuthWebAuthSessionState OBJECT-TYPE
        SYNTAX INTEGER
            {
            authenticated(1),
            unauthenticated(2),
            authenticating(3),
            authReqRejectNoVlan(4),
            authReqRejectUnauthVlan(5),
            authReqTimeoutNoVlan(6),
            authReqTimeoutUnauthVlan(7)
            }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Specifies the state of the client as follows:
            'authenticated'            - authenticated client
            'unauthenticated'          - unauthenticated client,  
                                         waiting for credentials
            'authenticating'           - credentials have been sent
                                         for verification, waiting for
                                         response
            'authReqRejectNoVlan'      - credentials invalid; client
                                         does not have access to 
                                         unauthenticated VLAN
            'authReqRejectUnauthVlan   - credentials invalid; client
                                         does have access to 
                                         unauthenticated VLAN
            'authReqTimeoutNoVlan'     - credentials could not be 
                                         verified; client is still 
                                         unauthenticated and does 
                                         not have access to 
                                         unauthenticated VLAN
            'authReqTimeoutUnauthVlan' - credentials could not be 
                                         verified; client is still 
                                         unauthenticated, but has 
                                         access to unauthenticated
                                         VLAN"
        ::= { hpicfUsrAuthWebAuthSessionStatsEntry 3 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.5.1.1.4
    hpicfUsrAuthWebAuthSessionStateTime OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The duration, in seconds, a client has spent in the
            state specified by hpicfUsrAuthSessionState."
        ::= { hpicfUsrAuthWebAuthSessionStatsEntry 4 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.5.1.1.5
    hpicfUsrAuthWebAuthSessionAuthVid OBJECT-TYPE
        SYNTAX VlanIndex
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Specifies the PVID that the authenticated client is
            utilizing. If client is unauthenticated, this object 
            has no meaning."
        ::= { hpicfUsrAuthWebAuthSessionStatsEntry 5 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.5.1.1.6
    hpicfUsrAuthWebAuthSessionUnauthVid OBJECT-TYPE
        SYNTAX VlanIndex
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Specifies the PVID that the unauthenticated client is
            utilizing. If client is authenticated, this object 
            has no meaning."
        ::= { hpicfUsrAuthWebAuthSessionStatsEntry 6 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.6
    hpicfUsrAuthMacAuthStats OBJECT IDENTIFIER ::= { hpicfUsrAuthMIB 6 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.6.1
    hpicfUsrAuthMacAuthSessionStatsTable OBJECT-TYPE
        SYNTAX SEQUENCE OF HpicfUsrAuthMacAuthSessionStatsEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "A table that contains session statistic objects
            for each client (i.e. user) attempting to 
            authenticate to a port with MAC-authentication 
            enabled. An entry appears in this table for each 
            port in the switch."
        ::= { hpicfUsrAuthMacAuthStats 1 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.6.1.1
    hpicfUsrAuthMacAuthSessionStatsEntry OBJECT-TYPE
        SYNTAX HpicfUsrAuthMacAuthSessionStatsEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The session statistics information for a port with
            Mac-based authentication enabled. This shows
            the current values being collected for active sessions."
        INDEX { hpicfUsrAuthPortNumber, hpicfUsrAuthMacAuthSessionMacAddr }
        ::= { hpicfUsrAuthMacAuthSessionStatsTable 1 }

    
    HpicfUsrAuthMacAuthSessionStatsEntry ::=
        SEQUENCE { 
            hpicfUsrAuthMacAuthSessionMacAddr
                MacAddress,
            hpicfUsrAuthMacAuthSessionState
                INTEGER,
            hpicfUsrAuthMacAuthSessionStateTime
                Unsigned32,
            hpicfUsrAuthMacAuthSessionAuthVid
                VlanIndex,
            hpicfUsrAuthMacAuthSessionUnauthVid
                VlanIndex
         }

    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.6.1.1.1
    hpicfUsrAuthMacAuthSessionMacAddr OBJECT-TYPE
        SYNTAX MacAddress
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Specifies the MAC address of the client."
        ::= { hpicfUsrAuthMacAuthSessionStatsEntry 1 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.6.1.1.2
    hpicfUsrAuthMacAuthSessionState OBJECT-TYPE
        SYNTAX INTEGER
            {
            authenticated(1),
            unauthenticated(2),
            authenticating(3),
            authReqRejectNoVlan(4),
            authReqRejectUnauthVlan(5),
            authReqTimeoutNoVlan(6),
            authReqTimeoutUnauthVlan(7)
            }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Specifies the state of the client as follows:
            'authenticated'            - authenticated client
            'unauthenticated'          - unauthenticated client,  
                                         waiting for credentials
            'authenticating'           - credentials have been sent
                                         for verification, waiting for
                                         response
            'authReqRejectNoVlan'      - credentials invalid; client
                                         does not have access to 
                                         unauthenticated VLAN
            'authReqRejectUnauthVlan   - credentials invalid; client
                                         does have access to 
                                         unauthenticated VLAN
            'authReqTimeoutNoVlan'     - credentials could not be 
                                         verified; client is still 
                                         unauthenticated and does 
                                         not have access to 
                                         unauthenticated VLAN
            'authReqTimeoutUnauthVlan' - credentials could not be 
                                         verified; client is still 
                                         unauthenticated, but has 
                                         access to unauthenticated
                                         VLAN"
        ::= { hpicfUsrAuthMacAuthSessionStatsEntry 2 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.6.1.1.3
    hpicfUsrAuthMacAuthSessionStateTime OBJECT-TYPE
        SYNTAX Unsigned32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The duration, in seconds, a client has spent in the
            state specified by hpicfUsrAuthSessionState."
        ::= { hpicfUsrAuthMacAuthSessionStatsEntry 3 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.6.1.1.4
    hpicfUsrAuthMacAuthSessionAuthVid OBJECT-TYPE
        SYNTAX VlanIndex
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Specifies the PVID that the authenticated client is
            utilizing. If client is unauthenticated, this object 
            has no meaning."
        ::= { hpicfUsrAuthMacAuthSessionStatsEntry 4 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.6.1.1.5
    hpicfUsrAuthMacAuthSessionUnauthVid OBJECT-TYPE
        SYNTAX VlanIndex
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Specifies the PVID that the unauthenticated client is
            utilizing. If client is authenticated, this object 
            has no meaning."
        ::= { hpicfUsrAuthMacAuthSessionStatsEntry 5 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.7
    hpicfUsrAuthConformance OBJECT IDENTIFIER ::= { hpicfUsrAuthMIB 7 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.7.2
    hpicfUsrAuthGroups OBJECT IDENTIFIER ::= { hpicfUsrAuthConformance 2 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.7.2.1
    hpicfUsrAuthSystemGroup OBJECT-GROUP
        OBJECTS { hpicfUsrAuthWebAuthDhcpBaseAddress, 
            hpicfUsrAuthWebAuthDhcpMask, 
            hpicfUsrAuthWebAuthDhcpLease, 
            hpicfUsrAuthMacAuthAddrFormat, 
            hpicfUsrAuthCLIPasswdSet, 
            hpicfUsrAuthCLIInterface }
        STATUS current
        DESCRIPTION 
            "A collection of objects providing system 
            information about, and control over, Web- and 
            MAC-based authentication."
        ::= { hpicfUsrAuthGroups 1 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.7.2.2
    hpicfUsrAuthPortsGroup OBJECT-GROUP
        OBJECTS { hpicfUsrAuthPortNumber, 
            hpicfUsrAuthWebAuthAdminStatus, 
            hpicfUsrAuthMacAuthAdminStatus, 
            hpicfUsrAuthPortReauthenticate }
        STATUS current
        DESCRIPTION 
            "A collection of objects providing system level
            information about Web and MAC based authentication
            for each port in the switch."
        ::= { hpicfUsrAuthGroups 2 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.7.2.3
    hpicfUsrAuthWebAuthConfigGroup OBJECT-GROUP
        OBJECTS { hpicfUsrAuthWebAuthClientLimit, 
            hpicfUsrAuthWebAuthClientMoves, 
            hpicfUsrAuthWebAuthSSLState, 
            hpicfUsrAuthWebAuthRedirectUrl, 
            hpicfUsrAuthWebAuthQuietPeriod, 
            hpicfUsrAuthWebAuthServerTimeout, 
            hpicfUsrAuthWebAuthServerMaxReq, 
            hpicfUsrAuthWebAuthMaxRetries, 
            hpicfUsrAuthWebAuthLogoffPeriod, 
            hpicfUsrAuthWebAuthReAuthPeriod, 
            hpicfUsrAuthWebAuthAuthVid, 
            hpicfUsrAuthWebAuthUnauthVid }
        STATUS current
        DESCRIPTION 
            "A collection of objects providing configuration
            objects for Web-based authentication associated with 
            each port."
        ::= { hpicfUsrAuthGroups 3 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.7.2.4
    hpicfUsrAuthMacAuthConfigGroup OBJECT-GROUP
        OBJECTS { hpicfUsrAuthMacAuthClientLimit, 
            hpicfUsrAuthMacAuthClientMoves, 
            hpicfUsrAuthMacAuthQuietPeriod, 
            hpicfUsrAuthMacAuthServerTimeout, 
            hpicfUsrAuthMacAuthServerMaxReq, 
            hpicfUsrAuthMacAuthLogoffPeriod, 
            hpicfUsrAuthMacAuthReAuthPeriod, 
            hpicfUsrAuthMacAuthAuthVid, 
            hpicfUsrAuthMacAuthUnauthVid }
        STATUS current
        DESCRIPTION 
            "A collection of objects providing configuration
            objects for MAC-based authentication associated with 
            each port."
        ::= { hpicfUsrAuthGroups 4 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.7.2.5
    hpicfUsrAuthWebAuthSessionStatsGroup OBJECT-GROUP
        OBJECTS { hpicfUsrAuthWebAuthSessionMacAddr, 
            hpicfUsrAuthWebAuthSessionName, 
            hpicfUsrAuthWebAuthSessionState, 
            hpicfUsrAuthWebAuthSessionStateTime, 
            hpicfUsrAuthWebAuthSessionAuthVid, 
            hpicfUsrAuthWebAuthSessionUnauthVid }
        STATUS current
        DESCRIPTION 
            "A collection of objects providing statistics about 
            current sessions for Web-based authentication."
        ::= { hpicfUsrAuthGroups 5 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.7.2.6
    hpicfUsrAuthMacAuthSessionStatsGroup OBJECT-GROUP
        OBJECTS { hpicfUsrAuthMacAuthSessionMacAddr, 
            hpicfUsrAuthMacAuthSessionState, 
            hpicfUsrAuthMacAuthSessionStateTime, 
            hpicfUsrAuthMacAuthSessionAuthVid, 
            hpicfUsrAuthMacAuthSessionUnauthVid
             }
        STATUS current
        DESCRIPTION 
            "A collection of objects providing statistics about 
            current sessions for MAC-based authentication."
        ::= { hpicfUsrAuthGroups 6 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.7.4
    hpicfUsrAuthCompliances OBJECT IDENTIFIER ::= { hpicfUsrAuthConformance 4 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.7.4.1
    hpicfUsrAuthCompliance MODULE-COMPLIANCE
        STATUS current
        DESCRIPTION 
            "The compliance statement for devices support of
            HP-USER-AUTH MIB."
        MODULE -- this module
            MANDATORY-GROUPS { hpicfUsrAuthSystemGroup, 
                hpicfUsrAuthPortsGroup, 
                hpicfUsrAuthWebAuthConfigGroup, 
                hpicfUsrAuthMacAuthConfigGroup, 
                hpicfUsrAuthWebAuthSessionStatsGroup, 
                hpicfUsrAuthMacAuthSessionStatsGroup }
        ::= { hpicfUsrAuthCompliances 1 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.8
    hpicfUsrAuthNotifyConformance OBJECT IDENTIFIER ::= { hpicfUsrAuthMIB 8 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.8.1
    hpicfUsrAuthNotificationGroup NOTIFICATION-GROUP
        NOTIFICATIONS { hpicfUsrAuthCLIAuthFail, 
            hpicfUsrAuthPasswdChng, 
            hpicfPortSecAuthFailure }
        STATUS current
        DESCRIPTION 
            "A group of authorization notifications."
        ::= { hpicfUsrAuthNotifyConformance 1 }

    
    -- 1.3.6.1.4.1.11.2.14.11.5.1.19.8.2
    hpicfNotifcationConfigDataGroup OBJECT-GROUP
        OBJECTS { hpicfUsrAuthCLIFailCnt, 
            hpicfUsrAuthCLIPwdNotifyCnt, 
            hpicfUsrAuthWMAFailCnt, 
            hpicfUsrAuthWMAFailMAC, 
            hpicfUsrAuthWMAFailPort, 
            hpicfUsrAuthWMAFailVlan, 
            hpicfUsrAuthPasswdNotifyEnable, 
            hpicfUsrAuthCliNotifyEnable, 
            hpicfUsrAuthPortSecNotifyEnable }
        STATUS current
        DESCRIPTION 
            "A group of notification data and configuration objects."
        ::= { hpicfUsrAuthNotifyConformance 2 }

    

END
