
-- *****************************************************************************
-- Juniper-PPP-MIB
--
-- Juniper Networks Enterprise MIB
--   PPP MIB
--
-- Copyright (c) 1998, 1999 Redstone Communications, Inc.
-- Copyright (c) 1999, 2002 Unisphere Networks, Inc.
-- Copyright (c) 2002-2007 Juniper Networks, Inc.
-- Copyright (c) 2008 Juniper Networks, Inc.
--   All Rights Reserved.
-- *****************************************************************************

Juniper-PPP-MIB  DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, Integer32, Counter32, IpAddress, TimeTicks
        FROM SNMPv2-SMI
    TEXTUAL-CONVENTION, TruthValue, RowStatus
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF
    ifIndex, InterfaceIndex, InterfaceIndexOrZero
        FROM IF-MIB
    Ipv6AddressIfIdentifier
        FROM IPV6-TC
    juniMibs
        FROM Juniper-MIBs
    JuniEnable, JuniNextIfIndex, JuniName, JuniNibbleConfig
        FROM Juniper-TC;

juniPppMIB  MODULE-IDENTITY
    LAST-UPDATED "200909180724Z"  -- 18-Sep-09 03:24 AM EDT
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
        "       Juniper Networks, Inc.
        Postal: 10 Technology Park Drive
                Westford, MA  01886-3146
                USA
        Tel:    +1 978 589 5800
        Email:  mib@Juniper.net"
    
    DESCRIPTION
        "The Point-to-Point Protocol (PPP) MIB for the Juniper enterprise."
    -- Revision History  
    REVISION    "200909180724Z"  -- 18-Sep-09 03:24 AM EDT  - JUNOSe 11.1
    DESCRIPTION
		"Added new multiclass multilink objects. Added new traffic class 
		mapping for multiclasses."
    REVISION    "200908101423Z"  -- 10-Aug-09 07:53 PM EST  - JUNOSe 11.0
    DESCRIPTION
        "Added new variables for prompting IPCP DNS options and IPCP 
         lockout options."

    REVISION    "200808271120Z"  -- 08-Sep-08 04:50 PM EST  - JUNOSe 10.1
    DESCRIPTION
        "Added new variables for configuring Maximum negotiation attempts
         allowed for any client in LCP , IPCP and IPv6CP config. Also
         added statistics for lcp, ip and ipv6 for renegotiation attempts
         terminated due to exceeding the configured attempts. RLI 4138."
    REVISION    "200707121215Z"  -- 12-Jul-07 08:15 AM EDT  - JUNOSe 7.3
    DESCRIPTION
        "Added new ignore magic number mismatch element.
         Added new authentication elements to use JuniNibbleConfig."
    REVISION    "200510191626Z"  -- 19-Oct-05 12:26 PM EDT  - JUNOSe 7.2
    DESCRIPTION
	"Added new object to the multi-link group." 
    REVISION    "200410052217Z"  -- 05-Oct-04 06:17 PM EDT -  JUNOSe 6.2
    DESCRIPTION
        "Added support for short keepalives in juniPppLinkConfigKeepalive."
    REVISION    "200410012141Z"  -- 01-Oct-04 05:41 PM EDT -  JUNOSe 6.0
    DESCRIPTION
        "Updated the juniPppSummary table"
    REVISION    "200408251212Z"  -- 25-Aug-04 08:12 AM EDT -  JUNOSe 5.3
    DESCRIPTION
        "Added new objects to the multi-link group."
    REVISION    "200408251212Z"  -- 25-Aug-04 08:12 AM EDT -  JUNOSe 5.2 
    DESCRIPTION
        "Increased max keepalive timer."
    REVISION    "200408251212Z"  -- 25-Aug-04 08:12 AM EDT -  JUNOSe 5.1
    DESCRIPTION
        "Added IPv6 support."
    REVISION    "200408251212Z"  -- 25-Aug-04 08:12 AM EDT -  JUNOSe 5.0
    DESCRIPTION
        "Replaced Unisphere names with Juniper names.
         Added new objects to the multi-link group.
         Reduced min keepalive timer."
    REVISION    "200208302036Z"  -- 30-Aug-02 04:36 PM EDT  - JUNOSe 4.1
    DESCRIPTION
        "Added new objects to the link and multi-link groups."
    REVISION    "200205092031Z"  -- 09-May-02 04:31 PM EDT  - JUNOSe 4.0
    DESCRIPTION
        "Added new objects to the IP, LCP and multi-link groups."
    REVISION    "200112122147Z"  -- 12-Dec-01 04:47 PM EST  - JUNOSe 3.3
    DESCRIPTION
        "Revised the conformance statements."
    REVISION    "200010091610Z"  --  9-Oct-00 12:10 PM EDT  - JUNOSe 2.4
    DESCRIPTION
        "Added juniPppLinkConfigStandardIfIndex object for cross referencing
        with standard PPP MIBs."
    REVISION    "200002151200Z"  -- 15-Feb-00               - JUNOSe 2.0
    DESCRIPTION
        "Added juniPppLinkStatusTunnelIfIndex, Multi-Link PPP support, and PPP
        Interface Summary counts.
        Modified Terminate reasons to include tunnel-related events."
    REVISION    "9907010000Z"    --  1-Jul-99               - JUNOSe 1.1
    DESCRIPTION
        "Additional objects added to support remote access capabilities,
        including termination reason, authentication protocol, option
        negotiation status."
    REVISION    "9811130000Z"    -- 13-Nov-98               - JUNOSe 1.0
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { juniMibs 11 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Textual conventions
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
JuniPppAuthentication ::= TEXTUAL-CONVENTION
    STATUS      deprecated
    DESCRIPTION
        "Specifies the type(s) of PPP authentication used, if any:
          none      No authentication is negotiated.
          pap       PAP negotiation only.
          chap      CHAP negotiation only.
          papChap   PAP negotiation is attempted first; if fails, attempt CHAP.
          chapPap   CHAP negotiation is attempted first; if fails, attempt PAP."
    SYNTAX      INTEGER {
                    none(0),
                    pap(1),
                    chap(2),
                    papChap(3),
                    chapPap(4) }

JuniPppAuthentication2 ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Specifies the type(s) of PPP authentication used, if any:
          none      No authentication is negotiated.
          pap       PAP negotiation.
          chap      CHAP negotiation.
          eap       EAP negotiation." 

    SYNTAX      INTEGER {
                    none(0),
                    pap(1),
                    chap(2),
                    eap(3) }

JuniPppMlPppBundleName ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "MLPPP Bundle name.  The bundle name is a characteristic of a MLPPP
        network interface."
    SYNTAX OCTET STRING (SIZE(0..32))


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Managed objects
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniPppObjects     OBJECT IDENTIFIER ::= { juniPppMIB 1 }

--
-- This MIB contains managed objects for PPP interfaces.
-- Management objects are provided to query for an available
-- interface index, and to create/delete interfaces of this type.
-- Creating/deleting this interface type using this MIB has
-- the side effect of creating/deleting corresponding entries
-- in the Interface MIB ifTable/ifXTable, and in the Juniper
-- Enterprise Interface MIB juniIfTable.
--
-- This MIB acts as a supplement to IETF MIBs RFC1471 PPP-LCP-MIB
-- and RFC1473 PPP-IP-NCP-MIB.
--

--
-- MIB object definitions are organized into the following
-- functional sections:
--
juniPppLcp        OBJECT IDENTIFIER   ::= { juniPppObjects 1 }
juniPppSec        OBJECT IDENTIFIER   ::= { juniPppObjects 2 }     -- reserved
juniPppIp         OBJECT IDENTIFIER   ::= { juniPppObjects 3 }
juniPppOsi        OBJECT IDENTIFIER   ::= { juniPppObjects 4 }
juniPppSession    OBJECT IDENTIFIER   ::= { juniPppObjects 5 }
juniPppMlPpp      OBJECT IDENTIFIER   ::= { juniPppObjects 6 }
juniPppSummary    OBJECT IDENTIFIER   ::= { juniPppObjects 7 }
juniPppIpv6       OBJECT IDENTIFIER   ::= { juniPppObjects 8 }


-- /////////////////////////////////////////////////////////////////////////////
--
-- PPP LCP
--
-- This section defines objects used to manage the PPP Link / LCP
-- layer of PPP.
--
-- The juniPppLinkStatusTable complements RFC1471 pppLinkStatusTable,
-- providing status indications regarding the operation
-- of network protocols over each link. The addition/removal of a
-- network protocol service is accomplished outside this MIB.
--
-- The juniPppLinkConfigTable complements RFC1471 pppLinkConfigTable,
-- providing the ability to create/delete instances of PPP links
-- and providing for configuration of option parameter values (if any)
-- not found in the standard MIB, to be used during LCP negotiation.
--
-- /////////////////////////////////////////////////////////////////////////////
--
-- The PPP Link Status Table
--
juniPppLinkStatusTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniPppLinkStatusEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for PPP interfaces present in the system."
    ::= { juniPppLcp 1 }

juniPppLinkStatusEntry OBJECT-TYPE
    SYNTAX      JuniPppLinkStatusEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of a PPP interface."
    INDEX     { ifIndex }
    ::= { juniPppLinkStatusTable 1 }

JuniPppLinkStatusEntry ::= SEQUENCE {
    juniPppLinkStatusTerminateReason         INTEGER,
    juniPppLinkStatusTerminateNegFailOption  INTEGER,
    juniPppLinkStatusInKeepaliveRequests     Counter32,
    juniPppLinkStatusOutKeepaliveRequests    Counter32,
    juniPppLinkStatusInKeepaliveReplies      Counter32,
    juniPppLinkStatusOutKeepaliveReplies     Counter32,
    juniPppLinkStatusKeepaliveFailures       Counter32,
    juniPppLinkStatusLocalMagicNumber        Integer32,
    juniPppLinkStatusRemoteMagicNumber       Integer32,
    juniPppLinkStatusLocalAuthentication     JuniPppAuthentication2,
    juniPppLinkStatusTunnelIfIndex           InterfaceIndexOrZero,
    juniPppLinkStatuslcpRenegoTerminates     Counter32}

juniPppLinkStatusTerminateReason OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    other(1),
                    adminDisable(2),
                    lowerLayerDown(3),
                    noUpperInterface(4),
                    authenticationFailure(5),
                    peerTerminated(6),
                    peerRenegotiated(7),
                    maxRetriesExceeded(8),
                    negotiationFailure(9),
                    keepaliveFailure(10),
                    sessionTimeout(11),
                    inactivityTimeout(12),
                    addressLeaseExpired(13),
                    adminLogout(14),
                    tunnelFailed(15),
                    tunnelDisconnected(16),
                    loopback(17) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Reason the PPP link was terminated:
            none                    None.
            other                   Not specified.
            adminDisable            Interface administratively disabled.
            lowerLayerDown          Underlying interface is down.
            noUpperInterface        No interface above PPP.
            authenticationFailure   Authentication failed.
            peerTerminated          Peer initiated termination.
            peerRenegotiated        Peer initiated renegotiation.
            maxRetriesExceeded      Maximum number of config retries exceeded.
            negotiationFailure      Failed to negotiate LCP option.  See
                                    juniPppLinkStatusTerminateNegFailOption.
            keepaliveFailure        Keepalive failed.
            sessionTimeout          Maximum session period expired.
            inactivityTimeout       Maximum inactivity period expired.
            addressLeaseExpired     Lease for network address expired.
            adminLogout             Session administratively terminated.
            tunnelFailed            Associated tunnel failed.
            tunnelDisconnected      Associated tunnel disconnected.
            loopback                Loopback detected."
    ::= { juniPppLinkStatusEntry 1 }

juniPppLinkStatusTerminateNegFailOption OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    other(1),
                    localMru(2),
                    remoteMru(3),
                    localMagicNumber(4),
                    remoteMagicNumber(5),
                    localAuthentication(6),
                    localToRemoteProtocolCompression(7),
                    localToRemoteACCompression(8) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Reports the PPP LCP option for which negotiation failed, when
        juniPppLinkStatusTerminateReason has the value 'negotiationFailure'."
    ::= { juniPppLinkStatusEntry 2 }

juniPppLinkStatusInKeepaliveRequests OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of keepalive requests received."
    ::= { juniPppLinkStatusEntry 3 }

juniPppLinkStatusOutKeepaliveRequests OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of keepalive requests transmitted."
    ::= { juniPppLinkStatusEntry 4 }

juniPppLinkStatusInKeepaliveReplies OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of keepalive replies received."
    ::= { juniPppLinkStatusEntry 5 }

juniPppLinkStatusOutKeepaliveReplies OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of keepalive replies transmitted."
    ::= { juniPppLinkStatusEntry 6 }

juniPppLinkStatusKeepaliveFailures OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of keepalive failures detected."
    ::= { juniPppLinkStatusEntry 7 }

juniPppLinkStatusLocalMagicNumber OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Magic number negotiated for the local side."
    ::= { juniPppLinkStatusEntry 8 }

juniPppLinkStatusRemoteMagicNumber OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Magic number negotiated for the remote side."
    ::= { juniPppLinkStatusEntry 9 }

juniPppLinkStatusLocalAuthentication OBJECT-TYPE
    SYNTAX      JuniPppAuthentication2
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Authentication protocol negotiated for the local side."
    ::= { juniPppLinkStatusEntry 10 }

juniPppLinkStatusTunnelIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The ifIndex of an associated interface pertaining to a tunneling
        protocol, or zero if no such interface exists.

        The type of tunneling interface can be identified from information in
        the entries in ifTable and juniIfTable for this tunnel interface."
    ::= { juniPppLinkStatusEntry 11 }

juniPppLinkStatuslcpRenegoTerminates OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of times lcp terminated due to peer exceeding max renegotiation
        attempts."
    ::= { juniPppLinkStatusEntry 12 }

--
-- The PPP Link Configuration Table
--
juniPppLinkConfigTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniPppLinkConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for PPP interfaces present in the system."
    ::= { juniPppLcp 2 }

juniPppLinkConfigEntry OBJECT-TYPE
    SYNTAX      JuniPppLinkConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of a PPP interface.
        Creating/deleting entries in this table causes corresponding entries for
        be created/deleted in ifTable/ifXTable/juniIfTable."
    INDEX     { juniPppLinkConfigIfIndex }
    ::= { juniPppLinkConfigTable 1 }

JuniPppLinkConfigEntry ::= SEQUENCE {
    juniPppLinkConfigIfIndex                    InterfaceIndex,
    juniPppLinkConfigRowStatus                  RowStatus,
    juniPppLinkConfigLowerIfIndex               InterfaceIndexOrZero,
    juniPppLinkConfigKeepalive                  Integer32,
    juniPppLinkConfigAuthentication             JuniPppAuthentication,
    juniPppLinkConfigMaxAuthenRetries           Integer32,
    juniPppLinkConfigStandardIfIndex            InterfaceIndex,
    juniPppLinkConfigChapMinChallengeLength     Integer32,
    juniPppLinkConfigChapMaxChallengeLength     Integer32,
    juniPppLinkConfigPassiveMode                JuniEnable,
    juniPppLinkConfigAuthenticatorVirtualRouter JuniName,
    juniPppLinkConfigAaaProfile                 JuniName,
    juniPppLinkConfigAuthentication2            JuniNibbleConfig,
    juniPppLinkConfigIgnoreMagicNumberMismatch  JuniEnable,
    juniPppLinkConfigMaxLcpRenegotiation        Integer32}

juniPppLinkConfigIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ifIndex of the PPP interface.  When creating entries in this table,
        suitable values for this object are determined by reading
        juniPppNextIfIndex."
    ::= { juniPppLinkConfigEntry 1 }

juniPppLinkConfigRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
            juniPppLinkConfigRowStatus
            juniPppLinkConfigLowerIfIndex

        In addition, when creating an entry the following conditions must hold:

            A value for juniPppLinkConfigIndex must have been determined
            previously, by reading juniPppNextIfIndex.

            The interface identified by juniPppLinkConfigLowerIfIndex must
            exist.

        A corresponding entry in ifTable/ifXTable/juniIfTable is created/
        destroyed as a result of creating/destroying an entry in this table."
    ::= { juniPppLinkConfigEntry 2 }

juniPppLinkConfigLowerIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The ifIndex of an interface over which this PPP interface is to be
        layered.  A value of zero indicates no layering.  An implementation may
        choose to require that a non-zero value be configured at entry
        creation."
    ::= { juniPppLinkConfigEntry 3 }

juniPppLinkConfigKeepalive OBJECT-TYPE
    SYNTAX      Integer32 (0..64800)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Keepalive interval in seconds.  A value of zero disables keepalive.
        Keepalive is performed using LCP Echo."
    DEFVAL    { 30 }
    ::= { juniPppLinkConfigEntry 4 }

juniPppLinkConfigAuthentication OBJECT-TYPE
    SYNTAX      JuniPppAuthentication
    MAX-ACCESS  read-create
    STATUS      deprecated
    DESCRIPTION
        "Specifies the type(s) of authentication, if any, to be negotiated with
        the peer:
          none      No authentication is negotiated.
          pap       PAP negotiation only.
          chap      CHAP negotiation only.
          papChap   PAP negotiation is attempted first; if fails, attempt CHAP.
          chapPap   CHAP negotiation is attempted first; if fails, attempt PAP.

        If authentication negotiation is not supported for this PPP interface,
        then any attempt to explicitely set this object will result in a
        notWritable error and it will be implicitily set to the DEFVAL on row
        creation.

        Setting this object to none(0) will set
        juniPppLinkConfigAuthenticatorVirtualRouter object to an empty string.

        This object returns a null(0) value on the get operation. New object
        juniPppLinkConfigAuthentication2 will reflect the configured values.

        Setting this object along with the juniPppLinkConfigAuthentication2 object
        will return an inconsistentValue error."
    DEFVAL    { none }
    ::= { juniPppLinkConfigEntry 5 }

juniPppLinkConfigMaxAuthenRetries OBJECT-TYPE
    SYNTAX      Integer32 (0..7)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The number of authentication retries permitted, in addition to a failed
        initial attempt.  If all retries fail, the link is reset.

        If authentication negotiation is not supported for this PPP interface,
        then any attempt to explicitely set this object will result in a
        notWritable error and it will be implicitily set to the DEFVAL on row
        creation."
    DEFVAL    { 0 }
    ::= { juniPppLinkConfigEntry 6 }

juniPppLinkConfigStandardIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The ifIndex value for this interface in the standard PPP MIBs.  The
        ifIndex value for PPP interfaces is not the same for both proprietary
        and standard MIB tables pertaining to PPP interface.  Therefore this
        value is provide to simply cross referencing standard PPP and
        proprietary PPP MIB information."
    ::= { juniPppLinkConfigEntry 7 }

juniPppLinkConfigChapMinChallengeLength OBJECT-TYPE
    SYNTAX      Integer32 (8..63)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Minimum value of the CHAP authenticator challenge length value.  This
        value is never allowed to be set to a value greater than
        juniPppLinkConfigChapMaxChallengeLength."
    DEFVAL    { 16 }
    ::= { juniPppLinkConfigEntry 8 }

juniPppLinkConfigChapMaxChallengeLength OBJECT-TYPE
    SYNTAX      Integer32 (8..63)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Maximum value of the CHAP authenticator challenge length value. This
        value is never allowed to be set to a value less than
        juniPppLinkConfigChapMinChallengeLength."
    DEFVAL    { 32 }
    ::= { juniPppLinkConfigEntry 9 }

juniPppLinkConfigPassiveMode OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "When enabled, LCP state machine is forced into passive mode on lower
        layer UP message.  It adds compatibility with slow and buggy clients."
    DEFVAL    { disable }
    ::= { juniPppLinkConfigEntry 10 }

juniPppLinkConfigAuthenticatorVirtualRouter OBJECT-TYPE
    SYNTAX      JuniName
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The name of the virtual router (Juniper-ROUTER-MIB.juniRouterName) to
        be used for authentication on the PPP interface.  Setting this object
        statically binds the authenticating virtual router with the PPP
        interface.  If this object is not explicitly set or it is set to null
        string, then this object is ignored and the virtual router used for
        authentication is determined by other means.  On a Set operation, if the
        value of this object is not null and does not correspond to an existing
        virtual router, then an inconsistentValue error is returned.

        Setting this object to a non-null string returns inconsistentValue error
        if juniPppLinkConfigAuthentication object is none(0) or not configured."
    ::= { juniPppLinkConfigEntry 11 }

juniPppLinkConfigAaaProfile OBJECT-TYPE
    SYNTAX      JuniName
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The name of the AAA profile to be used for authentication on the PPP
        interface.  Setting this object statically binds the AAA profile with
        the PPP interface.  If this object is not explicitly set or it is set to
        null string, then this object is ignored.  On a Set operation, if the
        value of this object is not null and does not correspond to an existing
        AAA profile, then an inconsistentValue error is returned."
    ::= { juniPppLinkConfigEntry 12 }

juniPppLinkConfigAuthentication2 OBJECT-TYPE
    SYNTAX      JuniNibbleConfig
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "A configuration variable comprised of nibbles i.e. 4 bits, such that 
         a client can supply a list of 0 to 8 selections.  The least 
         significant nibble is the first value of the list, and the most 
         significant nibble is the last value.  The value in each field 
         ranges from 0 to 15, however the first nibble with value 0 indicates
         the end of the list.  Repetition of values is not allowed. 
         Segregation of values is not allowed.

         Valid Values are:
         none - 0
         pap  - 1
         chap - 2
         eap  - 3

         Example valid encoding:
         0x00000321
         0x00000012

         Not a valid encoding:
         0x00000121
         0x01002001

         If authentication negotiation is not supported for this PPP interface,
         then any attempt to explicitly set this object will result in a
         notWritable error and it will be implicitly set to the DEFVAL on row
         creation.

         Setting this object to null will set
         juniPppLinkConfigAuthenticatorVirtualRouter object to an empty string.

         Setting this object along with the juniPppLinkConfigAuthentication object
         will return an inconsistentValue error."
    DEFVAL    { 0 }
    ::= { juniPppLinkConfigEntry 13 }
    
juniPppLinkConfigIgnoreMagicNumberMismatch OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The ignore magic number mismatch option of the PPP interface 
        determines the action to be taken, when the peer has not negotiated 
        any value yet sent null or invalid magic number in the LCP echo 
        packets. The two actions that can be configured are:
            1)	Ignore the mismatch and retain connection
            2)	Disallow the mismatch and terminate connection"
    DEFVAL    { disable }
    ::= { juniPppLinkConfigEntry 14 }

juniPppLinkConfigMaxLcpRenegotiation OBJECT-TYPE
    SYNTAX      Integer32 (1..65535)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Maximum number of allowed lcp renegotiation attempts from peer."
    DEFVAL    { 30 }
    ::= { juniPppLinkConfigEntry 15 }


--
-- IfIndex selection for creating new PPP interfaces in juniPppLinkConfigTable.
--
-- NOTE: This object is placed after juniPppLinkConfigTable so
-- that juniPppLinkStatusTable and juniPppLinkConfigTable have the
-- same relative MIB node positions below the juniPppLcp node
-- (juniPppLcp.1 and juniPppLcp.2, respectively) as their counterpart
-- Status and Config tables in RFC1471.
--
juniPppNextIfIndex OBJECT-TYPE
    SYNTAX      JuniNextIfIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Coordinate ifIndex value allocation for entries in the
        juniPppLinkConfigTable.

        A GET of this object returns the next available ifIndex value to be used
        to create an entry in the associated interface table; or zero, if no
        valid ifIndex value is available.  This object also returns a value of
        zero when it is the lexicographic successor of a varbind presented in an
        SNMP GETNEXT or GETBULK request, for which circumstance it is assumed
        that ifIndex allocation is unintended.

        Successive GETs will typically return different values, thus avoiding
        collisions among cooperating management clients seeking to create table
        entries simultaneously."
    ::= { juniPppLcp 3 }

-- /////////////////////////////////////////////////////////////////////////////
--
-- PPP Security
--
-- This section defines objects used to manage the PPP Security
-- functionality of PPP.
--
-- /////////////////////////////////////////////////////////////////////////////

-- No objects are currently defined.


-- /////////////////////////////////////////////////////////////////////////////
--
-- PPP IP NCP
--
-- This section defines objects used to manage the PPP Network
-- Control Protocol for IP protocol operation (IPCP).
--
-- /////////////////////////////////////////////////////////////////////////////

--
-- The PPP IP Table
--
juniPppIpTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniPppIpEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table containing the IP parameters for the local PPP entity."
    ::= { juniPppIp 1 }

juniPppIpEntry OBJECT-TYPE
    SYNTAX      JuniPppIpEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "IPCP status information for a particular PPP link."
    INDEX     { ifIndex }
    ::= { juniPppIpTable 1 }

JuniPppIpEntry ::= SEQUENCE {
    juniPppIpServiceStatus                      JuniEnable,
    juniPppIpTerminateReason                    INTEGER,
    juniPppIpTerminateNegFailOption             INTEGER,
    juniPppIpLocalIpAddress                     IpAddress,
    juniPppIpRemoteIpAddress                    IpAddress,
    juniPppIpRemotePrimaryDnsAddress            IpAddress,
    juniPppIpRemoteSecondaryDnsAddress          IpAddress,
    juniPppIpRemotePrimaryWinsAddress           IpAddress,
    juniPppIpRemoteSecondaryWinsAddress         IpAddress,
    juniPppIpNetworkStatusIpcpRenegoTerminates  Counter32}

juniPppIpServiceStatus OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates whether IP protocol service is operating over this PPP link.
        Service is established on this link through means outside this MIB."
    ::= { juniPppIpEntry 1 }

juniPppIpTerminateReason OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    other(1),
                    noService(2),
                    admin(3),
                    linkDown(4),
                    peerTerminated(5),
                    peerRenegotiated(6),
                    maxRetriesExceeded(7),
                    negotiationFailure(8) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Reason the IPCP link was terminated:
            none                    None.
            other                   Not specified.
            noService               No IP service configured on this PPP link.
            admin                   Administratively disabled.
            linkDown                Underlying link is down.
            peerTerminated          Peer initiated termination.
            peerRenegotiated        Peer initiated renegotiation.
            maxRetriesExceeded      Maximum number of config retries exceeded.
            negotiationFailure      Failed to negotiate IPCP option.  See
                                    juniPppIpTerminateNegFailOption."
    ::= { juniPppIpEntry 2 }

juniPppIpTerminateNegFailOption OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    other(1),
                    localIpAddress(2),
                    remoteIpAddress(3),
                    remotePrimaryDnsAddress(4),
                    remoteSecondaryDnsAddress(5),
                    remotePrimaryWinsAddress(6),
                    remoteSecondaryWinsAddress(7),
                    localIpAddressMask(8),
                    remoteIpAddressMask(9) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Reports the PPP IPCP option for which negotiation failed, when
        juniPppIpTerminateReason has the value 'negotiationFailure'."
    ::= { juniPppIpEntry 3 }

juniPppIpLocalIpAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "IP Address used by the local side."
    ::= { juniPppIpEntry 4 }

juniPppIpRemoteIpAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "IP Address used by the remote side."
    ::= { juniPppIpEntry 5 }

juniPppIpRemotePrimaryDnsAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Primary DNS server used by the remote side."
    ::= { juniPppIpEntry 6 }

juniPppIpRemoteSecondaryDnsAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Secondary DNS server used by the remote side."
    ::= { juniPppIpEntry 7 }

juniPppIpRemotePrimaryWinsAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Primary WINS server used by the remote side."
    ::= { juniPppIpEntry 8 }

juniPppIpRemoteSecondaryWinsAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Secondary WINS server used by the remote side."
    ::= { juniPppIpEntry 9 }

juniPppIpNetworkStatusIpcpRenegoTerminates OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of times ipcp terminated due to peer exceeding max
        renegotiation attempts."
    ::= { juniPppIpEntry 10 }

--
-- The PPP IP Config Table
--
juniPppIpConfigTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniPppIpConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table containing the IP parameters for the local PPP entity."
    ::= { juniPppIp 2 }

juniPppIpConfigEntry OBJECT-TYPE
    SYNTAX      JuniPppIpConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "IPCP configuration information for a particular PPP link."
    INDEX     { ifIndex }
    ::= { juniPppIpConfigTable 1 }

JuniPppIpConfigEntry ::= SEQUENCE {
    juniPppIpConfigPeerDnsPriority      JuniEnable,
    juniPppIpConfigPeerWinsPriority     JuniEnable,
    juniPppIpConfigIpcpNetmask          JuniEnable,
    juniPppIpConfigInitiateIp           JuniEnable,
    juniPppIpConfigMaxIpcpRenegotiation Integer32,
    juniPppIpConfigPromptIpcpDnsOption  JuniEnable,
    juniPppIpConfigIpcpLockout          JuniEnable}

juniPppIpConfigPeerDnsPriority OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "When enabled, allows peer's DNS address to prevail in the event of a
        negotiation conflict; when disabled, the local PPP interface's DNS
        address prevails."
    ::= { juniPppIpConfigEntry 1 }

juniPppIpConfigPeerWinsPriority OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "When enabled, allows peer's WINS address to prevail in the event of a
        negotiation conflict; when disabled, the local PPP interface's WINS
        address prevails."
    ::= { juniPppIpConfigEntry 2 }

juniPppIpConfigIpcpNetmask OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Enables the negotiation of the IPCP option netmask (0x90) during IPCP
        negotiation."
    DEFVAL    { disable }
    ::= { juniPppIpConfigEntry 3 }

juniPppIpConfigInitiateIp OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Enables the initiation of negotiation of the IPCP."
    DEFVAL    { disable }
    ::= { juniPppIpConfigEntry 4 }

juniPppIpConfigMaxIpcpRenegotiation OBJECT-TYPE
    SYNTAX      Integer32 (1..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Maximum number of allowed ipcp renegotiation attempts from peer."
    DEFVAL    { 30 }
    ::= { juniPppIpConfigEntry 5 }

juniPppIpConfigPromptIpcpDnsOption OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Control prompting of IPCP DNS option to remote peer."
    DEFVAL    { disable }
    ::= { juniPppIpConfigEntry 6 }

juniPppIpConfigIpcpLockout OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Enables IPCP lockout. It determines whether this NCP can be negotiated
         when the interface is already running a different NCP. On enabling this
         option, the IPCP negotiation will be blocked after a different NCP
         service is up and waited for 10 seconds for IPCP initiation from peer."
    DEFVAL    { disable }
    ::= { juniPppIpConfigEntry 7 }

-- /////////////////////////////////////////////////////////////////////////////
--
-- PPP OSI NCP
--
-- This section defines objects used to manage the PPP Network
-- Control Protocol for OSI protocol operation (OSICP).
--
-- The IETF does not define a standard MIB for managing an OSI NCP.
-- For consistency, this MIB follows the model of RFC1473 for IP NCP:
-- A status table reports the condition of the NCP state machine, and
-- the outcome of option parameter negotiation (if any) when the
-- OperStatus object has the value 'opened(1)'; a configuration table
-- provides administrative control over the NCP state machine, and
-- permits configuration of proposed option parameter values (if any)
-- to be used during NCP negotiation.
--
-- /////////////////////////////////////////////////////////////////////////////
--
-- PPP OSI Status Table
--
juniPppOsiTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniPppOsiEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table containing the OSI parameters for the local PPP entity."
    ::= { juniPppOsi 1 }

juniPppOsiEntry OBJECT-TYPE
    SYNTAX      JuniPppOsiEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "OSICP status information for a particular PPP link."
    INDEX     { ifIndex }
    ::= { juniPppOsiTable 1 }

JuniPppOsiEntry ::= SEQUENCE {
    juniPppOsiServiceStatus          JuniEnable,
    juniPppOsiOperStatus             INTEGER,
    juniPppOsiTerminateReason        INTEGER,
    juniPppOsiTerminateNegFailOption INTEGER,
    juniPppOsiLocalAlignNpdu         INTEGER,
    juniPppOsiRemoteAlignNpdu        INTEGER }

juniPppOsiServiceStatus OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates whether OSI protocol service is operating over this PPP link.
        Service is established on this link through means outside this MIB."
    ::= { juniPppOsiEntry 1 }

juniPppOsiOperStatus OBJECT-TYPE
    SYNTAX      INTEGER {
                    opened(1),
                    notOpened(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The operational status of the OSI network protocol.  If the value of
        this object is up then the finite state machine for the OSI network
        protocol has reached the Opened state."
    ::= { juniPppOsiEntry 2 }

juniPppOsiTerminateReason OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    other(1),
                    noService(2),
                    admin(3),
                    linkDown(4),
                    peerTerminated(5),
                    peerRenegotiated(6),
                    maxRetriesExceeded(7),
                    negotiationFailure(8) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Reason the OSICP link was terminated:
            none                    None.
            other                   Not specified.
            noService               No OSI service configured on this PPP link.
            admin                   Administratively disabled.
            linkDown                Underlying link is down.
            peerTerminated          Peer initiated termination.
            peerRenegotiated        Peer initiated renegotiation.
            maxRetriesExceeded      Maximum number of config retries exceeded.
            negotiationFailure      Failed to negotiate IPCP option.  See
                                    juniPppOsiTerminateNegFailOption."
    ::= { juniPppOsiEntry 3 }

juniPppOsiTerminateNegFailOption OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    other(1),
                    localAlignNpdu(2),
                    remoteAlignNpdu(3) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Reports the PPP OSICP option for which negotiation failed, when
        juniPppOsiTerminateReason has the value 'negotiationFailure'."
    ::= { juniPppOsiEntry 4 }

juniPppOsiLocalAlignNpdu OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    oneModulo4(1),
                    twoModulo4(2),
                    threeModulo4(3),
                    fourModulo4(4),
                    even(254),
                    odd(255) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Local alignment of network PDU:
            none            No alignment specified.
            oneModulo4      Alignment on first octet (out of four).
            twoModulo4      Alignment on second octet (out of four).
            threeModulo4    Alignment on third octet (out of four).
            fourModulo4     Alignment on fourth octet (out of four).
            even            Alignment on even-octet boundary.
            odd             Alignment on odd-octet boundary."
    ::= { juniPppOsiEntry 5 }

juniPppOsiRemoteAlignNpdu OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    oneModulo4(1),
                    twoModulo4(2),
                    threeModulo4(3),
                    fourModulo4(4),
                    even(254),
                    odd(255) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Remote alignment of network PDU.
            none            No alignment specified.
            oneModulo4      Alignment on first octet (out of four).
            twoModulo4      Alignment on second octet (out of four).
            threeModulo4    Alignment on third octet (out of four).
            fourModulo4     Alignment on fourth octet (out of four).
            even            Alignment on even-octet boundary.
            odd             Alignment on odd-octet boundary."
    ::= { juniPppOsiEntry 6 }


--
-- The PPP OSI Configuration Table
--
juniPppOsiConfigTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniPppOsiConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table containing configuration variables for the OSICP for the local
        PPP entity."
    ::= { juniPppOsi 2 }

juniPppOsiConfigEntry   OBJECT-TYPE
    SYNTAX      JuniPppOsiConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "OSICP information for a particular PPP link."
    INDEX     { ifIndex }
    ::= { juniPppOsiConfigTable 1 }

JuniPppOsiConfigEntry ::= SEQUENCE {
    juniPppOsiConfigAdminStatus  INTEGER }

juniPppOsiConfigAdminStatus   OBJECT-TYPE
    SYNTAX      INTEGER {
                    open(1),
                    close(2) }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The immediate desired status of the OSI network protocol.  Setting this
        object to open will inject an administrative open event into the OSI
        network protocol's finite state machine.  Setting this object to close
        will inject an administrative close event into the OSI network
        protocol's finite state machine."
    ::= { juniPppOsiConfigEntry 1 }


-- /////////////////////////////////////////////////////////////////////////////
--
-- PPP Session
--
-- This section defines objects used to manage the PPP sessions.
--
-- The juniPppSessionTable provides status of each PPP session.
--
-- /////////////////////////////////////////////////////////////////////////////
--
-- The PPP Session Table
--
juniPppSessionTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniPppSessionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for PPP interfaces present in the system."
    ::= { juniPppSession 1 }

juniPppSessionEntry OBJECT-TYPE
    SYNTAX      JuniPppSessionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of a PPP interface."
    INDEX     { ifIndex }
    ::= { juniPppSessionTable 1 }

JuniPppSessionEntry ::= SEQUENCE {
    juniPppSessionGrant                         TruthValue,
    juniPppSessionTerminateReason               INTEGER,
    juniPppSessionStartTime                     TimeTicks,
    juniPppSessionInOctets                      Counter32,
    juniPppSessionOutOctets                     Counter32,
    juniPppSessionInPackets                     Counter32,
    juniPppSessionOutPackets                    Counter32,
    juniPppSessionSessionTimeout                Integer32,
    juniPppSessionInactivityTimeout             Integer32,
    juniPppSessionAccountingInterval            Integer32,
    juniPppSessionRemoteIpAddress               IpAddress,
    juniPppSessionRemotePrimaryDnsAddress       IpAddress,
    juniPppSessionRemoteSecondaryDnsAddress     IpAddress,
    juniPppSessionRemotePrimaryWinsAddress      IpAddress,
    juniPppSessionRemoteSecondaryWinsAddress    IpAddress,
    juniPppSessionRemoteIpv6AddressIfIdentifier Ipv6AddressIfIdentifier,
    juniPppSessionInhibitIp                     TruthValue,
    juniPppSessionInhibitIpv6                   TruthValue }

juniPppSessionGrant OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates whether a session has been granted via the authentication
        mechanism."
    ::= { juniPppSessionEntry 1 }

juniPppSessionTerminateReason OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    unknown(1),
                    userRequest(2),
                    keepaliveFailure(3),
                    sessionTimeout(4),
                    inactivityTimeout(5),
                    adminDisable(6),
                    lowerLayerDown(7),
                    noUpperInterface(8),
                    deny(9),
                    noHardware(10),
                    noResources(11),
                    noInterface(12),
                    challengeTimeout(13),
                    requestTimeout(14),
                    authenticatorTimeout(15),
                    addressLeaseExpired(16),
                    adminLogout(17),
                    tunnelFailed(18) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The reason the session was terminated."
    ::= { juniPppSessionEntry 2 }

juniPppSessionStartTime OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of sysUpTime when this session last became active."
    ::= { juniPppSessionEntry 3 }

juniPppSessionInOctets OBJECT-TYPE
    SYNTAX      Counter32
    UNITS       "octets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of octets received since this session last became active, as
        denoted by juniPppSessionStartTime."
    ::= { juniPppSessionEntry 4 }

juniPppSessionOutOctets OBJECT-TYPE
    SYNTAX      Counter32
    UNITS       "octets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of octets sent since this session last became active, as denoted
        by juniPppSessionStartTime."
    ::= { juniPppSessionEntry 5 }

juniPppSessionInPackets OBJECT-TYPE
    SYNTAX      Counter32
    UNITS       "packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of packets received since this session last became active, as
        denoted by juniPppSessionStartTime."
    ::= { juniPppSessionEntry 6 }

juniPppSessionOutPackets OBJECT-TYPE
    SYNTAX      Counter32
    UNITS       "packets"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of packets sent since this session last became active, as
        denoted by juniPppSessionStartTime."
    ::= { juniPppSessionEntry 7 }

juniPppSessionSessionTimeout OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Maximum duration for the session, after which the session terminates
        automatically."
    ::= { juniPppSessionEntry 8 }

juniPppSessionInactivityTimeout OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Maximum inactivity duration for the session, after which the session
        terminates automatically."
    ::= { juniPppSessionEntry 9 }

juniPppSessionAccountingInterval OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    UNITS       "milliseconds"
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Interval that must elapse between generation of accounting records for
        this session."
    ::= { juniPppSessionEntry 10 }

juniPppSessionRemoteIpAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Remote IP address, obtained from the authentication service, to be used
        during IPCP negotiation with the remote side."
    ::= { juniPppSessionEntry 11 }

juniPppSessionRemotePrimaryDnsAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Remote primary DNS IP address, obtained from the authentication
        service, to be used during IPCP negotiation with the remote side."
    ::= { juniPppSessionEntry 12 }

juniPppSessionRemoteSecondaryDnsAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Remote secondary DNS IP address, obtained from the authentication
        service, to be used during IPCP negotiation with the remote side."
    ::= { juniPppSessionEntry 13 }

juniPppSessionRemotePrimaryWinsAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Remote primary WINS IP address, obtained from the authentication
        service, to be used during IPCP negotiation with the remote side."
    ::= { juniPppSessionEntry 14 }

juniPppSessionRemoteSecondaryWinsAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Remote secondary WINS IP address, obtained from the authentication
        service, to be used during IPCP negotiation with the remote side."
    ::= { juniPppSessionEntry 15 }

juniPppSessionRemoteIpv6AddressIfIdentifier OBJECT-TYPE
    SYNTAX      Ipv6AddressIfIdentifier
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "IPV6 Address Interface Identifier obtained from the authentication
        service, to be used during IPCP negotiation with the remote side."
    ::= { juniPppSessionEntry 16 }

juniPppSessionInhibitIp OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates whether a session has had its IP service inhibited by the
        authentication mechanism."
    ::= { juniPppSessionEntry 17 }

juniPppSessionInhibitIpv6 OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates whether a session has had its IPv6 service inhibited by the
        authentication mechanism."
    ::= { juniPppSessionEntry 18 }


-- /////////////////////////////////////////////////////////////////////////////
--
-- Multi-Link PPP  (MLPPP)
--
-- This section defines objects used to manage the MLPPP.
--
-- /////////////////////////////////////////////////////////////////////////////
--
-- The MLPPP BundleTable
--
juniPppMlPppBundleTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniPppMlPppBundleEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for MLPPP bundles present in the system."
    ::= { juniPppMlPpp 1 }

juniPppMlPppBundleEntry OBJECT-TYPE
    SYNTAX      JuniPppMlPppBundleEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of a MLPPP bundle."
    INDEX     { juniPppMlPppBundleName }
    ::= { juniPppMlPppBundleTable 1 }

JuniPppMlPppBundleEntry ::= SEQUENCE {
    juniPppMlPppBundleName           JuniPppMlPppBundleName,
    juniPppMlPppBundleRowStatus      RowStatus,
    juniPppMlPppBundleNetworkIfIndex InterfaceIndex }

juniPppMlPppBundleName OBJECT-TYPE
    SYNTAX      JuniPppMlPppBundleName
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The administrative name of the MLPPP bundle associated with this MLPPP
        network interface."
    ::= { juniPppMlPppBundleEntry 1 }

juniPppMlPppBundleRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The rowStatus for this entry.  The following sets are supported:
             createAndGo(4),
             destroy(6)

         The following values can be read from this object:
             active(1) "
    ::= { juniPppMlPppBundleEntry 2 }

juniPppMlPppBundleNetworkIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The ifIndex of this MLPPP network interface.  It is a valid ifIndex
        even if there is no corresponding network interface instance in the
        juniPppMlPppLinkConfigTable."
    ::= { juniPppMlPppBundleEntry 3 }

--
-- IfIndex selection for creating new MLPPP Link interfaces
-- in juniPppLinkConfigTable.
--
-- NOTE: This object is placed after juniPppLinkConfigTable so
-- that juniPppLinkStatusTable and juniPppLinkConfigTable have the
-- same relative MIB node positions below the juniPppLcp node
-- (juniPppLcp.1 and juniPppLcp.2, respectively) as their counterpart
-- Status and Config tables in RFC1471.
--
juniPppMlPppNextLinkIfIndex OBJECT-TYPE
    SYNTAX      JuniNextIfIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Coordinate ifIndex value allocation for entries in
        juniPppMlPppLinkConfigTable.

        A GET of this object returns the next available ifIndex value to be used
        to create an entry in the associated interface table; or zero, if no
        valid ifIndex value is available.  This object also returns a value of
        zero when it is the lexicographic successor of a varbind presented in an
        SNMP GETNEXT or GETBULK request, for which circumstance it is assumed
        that ifIndex allocation is unintended.

        Successive GETs will typically return different values, thus avoiding
        collisions among cooperating management clients seeking to create table
        entries simultaneously."
    ::= { juniPppMlPpp 2 }

--
-- The MLPPP Link Configuration Table
--
juniPppMlPppLinkConfigTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniPppMlPppLinkConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for MLPPP interfaces present in the
        system."
    ::= { juniPppMlPpp 3 }

juniPppMlPppLinkConfigEntry OBJECT-TYPE
    SYNTAX      JuniPppMlPppLinkConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of MLPPP interface.
        Creating/deleting entries in this table causes corresponding entries for
        be created/deleted in ifTable/ifXTable/juniIfTable."
    INDEX     { juniPppMlPppLinkConfigIfIndex }
    ::= { juniPppMlPppLinkConfigTable 1 }

JuniPppMlPppLinkConfigEntry ::= SEQUENCE {
    juniPppMlPppLinkConfigIfIndex                      InterfaceIndex,
    juniPppMlPppLinkConfigLowerIfIndex                 InterfaceIndexOrZero,
    juniPppMlPppLinkConfigKeepalive                    Integer32,
    juniPppMlPppLinkConfigAuthentication               JuniPppAuthentication,
    juniPppMlPppLinkConfigMaxAuthenRetries             Integer32,
    juniPppMlPppLinkConfigRowStatus                    RowStatus,
    juniPppMlPppLinkConfigAaaProfile                   JuniName,
    juniPppMlPppLinkConfigChapMinChallengeLength       Integer32,
    juniPppMlPppLinkConfigChapMaxChallengeLength       Integer32,
    juniPppMlPppLinkConfigPassiveMode                  JuniEnable,
    juniPppMlPppLinkConfigAuthenticatorVirtualRouter   JuniName,
    juniPppMlPppLinkConfigFragmentation                JuniEnable,
    juniPppMlPppLinkConfigReassembly                   JuniEnable,
    juniPppMlPppLinkConfigMaxReceiveReconstructedUnit  Integer32,
    juniPppMlPppLinkConfigFragmentSize                 Integer32,
    juniPppMlPppLinkConfigHashLinkSelection            JuniEnable,
    juniPppMlPppLinkConfigAuthentication2              JuniNibbleConfig,
    juniPppMlPppLinkConfigIgnoreMagicNumberMismatch    JuniEnable,
    juniPppMlPppLinkConfigMultilinkMulticlass          JuniEnable,
    juniPppMlPppLinkConfigMultilinkMaxMultiClasses     INTEGER}

juniPppMlPppLinkConfigIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ifIndex of the MLPPP interface.  When creating entries in this
        table, suitable values for this object are determined by reading
        juniPppMlPppNextLinkIfIndex."
    ::= { juniPppMlPppLinkConfigEntry 1 }

juniPppMlPppLinkConfigLowerIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndexOrZero
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The ifIndex of an interface over which this PPP interface is to be
        layered.  A value of zero indicates no layering.  An implementation may
        choose to require that a non-zero value be configured at entry
        creation."
    ::= { juniPppMlPppLinkConfigEntry 2 }

juniPppMlPppLinkConfigKeepalive OBJECT-TYPE
    SYNTAX      Integer32 (0|10..64800)
    UNITS       "seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Keepalive interval in seconds.  A value of zero disables keepalive.
        Keepalive is performed using LCP Echo."
    DEFVAL    { 30 }
    ::= { juniPppMlPppLinkConfigEntry 4 }

juniPppMlPppLinkConfigAuthentication OBJECT-TYPE
    SYNTAX      JuniPppAuthentication
    MAX-ACCESS  read-create
    STATUS      deprecated
    DESCRIPTION
        "Specifies the type(s) of authentication, if any, to be negotiated with
        the peer:
          none      No authentication is negotiated.
          pap       PAP negotiation only.
          chap      CHAP negotiation only.
          papChap   PAP negotiation is attempted first; if fails, attempt CHAP.
          chapPap   CHAP negotiation is attempted first; if fails, attempt PAP.

        If authentication negotiation is not supported for this MLPPP interface,
        then any attempt to explicitely set this object will result in a
        notWritable error and it will be implicitily set to the DEFVAL on row
        creation.

        Setting this object to none(0) will set
        juniPppMlPppLinkConfigAuthenticatorVirtualRouter object to an empty 
        string.

        This object returns a none (0) value on the get operation. New object
        juniPppMlPppLinkConfigAuthentication2 will reflect the configured values.

        Setting this object along with the juniPppMlPppLinkConfigAuthentication2 
        object will return an inconsistentValue error."
    DEFVAL    { none }
    ::= { juniPppMlPppLinkConfigEntry 5 }

juniPppMlPppLinkConfigMaxAuthenRetries OBJECT-TYPE
    SYNTAX      Integer32 (0..7)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The number of authentication retries permitted, in addition to a failed
        initial attempt.  If all retries fail, the link is reset."
    DEFVAL    { 0 }
    ::= { juniPppMlPppLinkConfigEntry 6 }

juniPppMlPppLinkConfigRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
            juniPppMlPppLinkConfigRowStatus
            juniPppMlPppLinkConfigLowerIfIndex

        In addition, when creating an entry the following conditions must hold:

            A value for juniPppMlPppLinkConfigIndex must have been determined
            previously, by reading juniPppMlPppNextIfIndex.

            The interface identified by juniPppMlPppLinkConfigLowerIfIndex
            must exist.

        A corresponding entry in ifTable/ifXTable/juniIfTable is created/
        destroyed as a result of creating/destroying an entry in this table."
    ::= { juniPppMlPppLinkConfigEntry 7 }

juniPppMlPppLinkConfigAaaProfile OBJECT-TYPE
    SYNTAX      JuniName
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The name of the AAA profile to be used for authentication on the PPP
        interface.  Setting this object statically binds the AAA profile with
        the PPP interface.  If this object is not explicitly set or it is set to
        null string, then this object is ignored.  On a Set operation, if the
        value of this object is not null and does not correspond to an existing
        AAA profile, then an inconsistentValue error is returned."
    ::= { juniPppMlPppLinkConfigEntry 8 }

juniPppMlPppLinkConfigChapMinChallengeLength OBJECT-TYPE
    SYNTAX      Integer32 (8..63)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Minimum value of the CHAP authenticator challenge length value.  This
        value is never allowed to be set to a value greater than
        juniPppMlPppLinkConfigChapMaxChallengeLength."
    DEFVAL    { 16 }
    ::= { juniPppMlPppLinkConfigEntry 9 }

juniPppMlPppLinkConfigChapMaxChallengeLength OBJECT-TYPE
    SYNTAX      Integer32 (8..63)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Maximum value of the CHAP authenticator challenge length value."
    DEFVAL    { 32 }
    ::= { juniPppMlPppLinkConfigEntry 10 }

juniPppMlPppLinkConfigPassiveMode OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "When enabled, LCP state machine is forced into passive mode on lower
        layer UP message.  It adds compatibility with slow and buggy clients."
    DEFVAL    { disable }
    ::= { juniPppMlPppLinkConfigEntry 11 }

juniPppMlPppLinkConfigAuthenticatorVirtualRouter OBJECT-TYPE
    SYNTAX      JuniName
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The name of the virtual router (Juniper-ROUTER-MIB.juniRouterName) to
        be used for authentication on the PPP interface.  Setting this object
        statically binds the authenticating virtual router with the link
        interface.  If this object is not explicitly set or it is set to null
        string, then this object is ignored and the virtual router used for
        authentication is determined by other means.  On a Set operation, if the
        value of this object is not null and does not correspond to an existing
        virtual router, then an inconsistentValue error is returned."
    ::= { juniPppMlPppLinkConfigEntry 12 }

juniPppMlPppLinkConfigFragmentation OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enables MLPPP fragmentation.  Changing this object has an effect when
        the link is next restarted."
    DEFVAL    { disable }
    ::= { juniPppMlPppLinkConfigEntry 13 }

juniPppMlPppLinkConfigReassembly OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enables MLPPP reassembly.  Changing this object has an effect when the
        link is next restarted."
    DEFVAL    { disable }
    ::= { juniPppMlPppLinkConfigEntry 14 }

juniPppMlPppLinkConfigMaxReceiveReconstructedUnit OBJECT-TYPE
    SYNTAX      Integer32 (1|64..65535)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The Maximum Receive Reconstructed Unit (MRRU) that the local PPP entity
        will advertise to the remote entity.  If the value of this variable is
        1, then the MRRU is set to the local MRU value.  Changing this object
        has an effect when the link is next restarted."
    DEFVAL    { 1 }
    ::= { juniPppMlPppLinkConfigEntry 15 }

juniPppMlPppLinkConfigFragmentSize OBJECT-TYPE
    SYNTAX      Integer32 (1|128..65535)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The size of fragments transmitted by the local PPP entity.  If the
        value of this variable is 1, then the fragment size is set to the link's
        MTU value.  Changing this object has an effect when the link is next
        restarted."
    DEFVAL    { 1 }
    ::= { juniPppMlPppLinkConfigEntry 16 }

juniPppMlPppLinkConfigHashLinkSelection OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enables MLPPP hash-based link selection for non-best-effort traffic.
	Changing this object has an effect when the link is next restarted."
    DEFVAL    { disable }
    ::= { juniPppMlPppLinkConfigEntry 17 }

juniPppMlPppLinkConfigAuthentication2 OBJECT-TYPE
    SYNTAX      JuniNibbleConfig
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "A configuration variable comprised of nibbles i.e. 4 bits, such that 
         a client can supply a list of 0 to 8 selections.  The least 
         significant nibble is the first value of the list, and the most 
         significant nibble is the last value.  The value in each field 
         ranges from 0 to 15, however the first nibble with value 0 indicates
         the end of the list.  Repetition of values is not allowed. 
         Segregation of values is not allowed.

         Valid Values are:
         none - 0
         pap  - 1
         chap - 2
         eap  - 3

         Example valid encoding:
         0x00000321
         0x00000012

         Not a valid encoding:
         0x00000121
         0x01002001

         If authentication negotiation is not supported for this PPP interface,
         then any attempt to explicitly set this object will result in a
         notWritable error and it will be implicitly set to the DEFVAL on row
         creation.

         Setting this object to null will set
         juniPppMlPppLinkConfigAuthenticatorVirtualRouter object to an empty 
         string.

         Setting this object along with the juniPppMlPppLinkConfigAuthentication
         object will return an inconsistentValue error."
    DEFVAL    { 0 }
    ::= { juniPppMlPppLinkConfigEntry 18 }
    
juniPppMlPppLinkConfigIgnoreMagicNumberMismatch OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The ignore magic number mismatch option of the PPP interface 
        determines the action to be taken, when the peer has not negotiated
        any value yet sent null or invalid magic number in the LCP echo 
        packets. The two actions that can be configured are:
            1)	Ignore the mismatch and retain connection
            2)	Disallow the mismatch and terminate connection"
    DEFVAL    { disable }
    ::= { juniPppMlPppLinkConfigEntry 19 }

juniPppMlPppLinkConfigMultilinkMulticlass OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Enables Multiclass Multilink PPP (MCML). Changing this object has an 
		effect when the link is next restarted."
    DEFVAL    {disable}
    ::= { juniPppMlPppLinkConfigEntry 20 }

juniPppMlPppLinkConfigMultilinkMaxMultiClasses OBJECT-TYPE
    SYNTAX      INTEGER (0..8)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Maximum number of MCML classes to be negotiated. Changing this object
		 has an effect when the link is next restarted."
    DEFVAL    {0}
    ::= { juniPppMlPppLinkConfigEntry 21 }

juniPppMlPppNextNetworkIfIndex OBJECT-TYPE
    SYNTAX      JuniNextIfIndex
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Coordinate ifIndex value allocation for entries in
        juniPppMlPppNetworkConfigTable.

        A GET of this object returns the next available ifIndex value to be used
        to create an entry in the associated interface table; or zero, if no
        valid ifIndex value is available.  This object also returns a value of
        zero when it is the lexicographic successor of a varbind presented in an
        SNMP GETNEXT or GETBULK request, for which circumstance it is assumed
        that ifIndex allocation is unintended.

        Successive GETs will typically return different values, thus avoiding
        collisions among cooperating management clients seeking to create table
        entries simultaneously."
    ::= { juniPppMlPpp 4 }


--
-- The MLPPP Network Configuration Table
--
juniPppMlPppNetworkConfigTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniPppMlPppNetworkConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for MLPPP network interfaces present in the
        system."
    ::= { juniPppMlPpp 5 }

juniPppMlPppNetworkConfigEntry OBJECT-TYPE
    SYNTAX      JuniPppMlPppNetworkConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of MLPPP interface.
        Creating/deleting entries in this table causes corresponding entries for
        be created/deleted in ifTable/ifXTable/juniIfTable."
    INDEX     { juniPppMlPppNetworkConfigIfIndex }
    ::= { juniPppMlPppNetworkConfigTable 1 }

JuniPppMlPppNetworkConfigEntry ::= SEQUENCE {
    juniPppMlPppNetworkConfigIfIndex         InterfaceIndex,
    juniPppMlPppNetworkConfigLowerIfIndex    InterfaceIndex,
    juniPppMlPppNetworkBundleName            JuniPppMlPppBundleName,
    juniPppMlPppNetworkRowStatus             RowStatus }

juniPppMlPppNetworkConfigIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ifIndex of the MLPPP network interface.  When creating entries in
        this table, suitable values for this object are determined by reading
        juniPppMlPppNextNetworkIfIndex."
    ::= { juniPppMlPppNetworkConfigEntry 1 }

juniPppMlPppNetworkConfigLowerIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The ifIndex of a PPP link interface over which this PPP network
        interface is to be layered.  On sets, the value of this object must
        equal on of the previously created PPP link interfaces created in the
        juniPppMlPppLinkConfigTable.  On gets, the value of this object is the
        lexicographically least PPP link interface in a potential bundle of PPP
        link interfaces."
    ::= { juniPppMlPppNetworkConfigEntry 2 }

juniPppMlPppNetworkBundleName OBJECT-TYPE
    SYNTAX     JuniPppMlPppBundleName
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
        "The MLPPP bundle name administratively assigned."
    ::= { juniPppMlPppNetworkConfigEntry 3 }

juniPppMlPppNetworkRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
            juniPppMlPppNetworkConfigLowerIfIndex
            juniPppMlPppNetworkBundleName
            juniPppMlPppNetworkConfigRowStatus

        In addition, when creating an entry the following conditions must hold:

            A value for juniPppMlPppNetworkConfigIndex must have been determined
            previously, by reading juniPppMlPppNextNetworkIfIndex.

            The interface identified by juniPppMlPppNetworkConfigLowerIfIndex
            must exist by a creation request to the juniPppMlPppLinkConfigTable.

            The bundleName specified in juniPppMlPppNetworkBundleName must have
            been created first in the juniPppMlPppBundleTable.

        A corresponding entry in ifTable/ifXTable/juniIfTable is created/
        destroyed as a result of creating/destroying an entry in this table.  "
    ::= { juniPppMlPppNetworkConfigEntry 4 }


--
-- The MLPPP Link Bind Table
--
juniPppMlPppLinkBindTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniPppMlPppLinkBindEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for MLPPP Link interface to MLPPP network
        interfaces bindings."
    ::= { juniPppMlPpp 6 }

juniPppMlPppLinkBindEntry OBJECT-TYPE
    SYNTAX      JuniPppMlPppLinkBindEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the MLPPP link interface to MLPPP network
        interface bindings."
    INDEX     { juniPppMlPppBindNetworkIfIndex,
                juniPppMlPppBindLinkIfIndex }
    ::= { juniPppMlPppLinkBindTable 1 }

JuniPppMlPppLinkBindEntry ::= SEQUENCE {
    juniPppMlPppBindNetworkIfIndex   InterfaceIndex,
    juniPppMlPppBindLinkIfIndex      InterfaceIndex,
    juniPppMlPppBindRowStatus        RowStatus }

juniPppMlPppBindNetworkIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ifIndex of the MLPPP network interface."
    ::= { juniPppMlPppLinkBindEntry 1 }

juniPppMlPppBindLinkIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ifIndex of a MLPPP link interface bound by the MLPPP network
        interface defined by juniPppMlPppBindNetworkIfIndex."
    ::= { juniPppMlPppLinkBindEntry 2 }

juniPppMlPppBindRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
            juniPppMlPppBindRowStatus

        In addition, when creating an entry the following conditions must hold:

            The interfaces identified by juniPppMlPppBindNetworkIfIndex and
            juniPppMlPppBindLinkIfIndex must be created in the
            juniPppMlPppNetworkConfigTable and juniPppMlPppLinkConfigTable
            respectively.

            A MLPPP bundle must be associated with the
            juniPppMlPppNetworkIfIndex and exist in the
            juniPppMibPppBundleTable.

        A corresponding entry in ifStackTable is created/destroyed as a result
        of creating/destroying an entry in this table."
    ::= { juniPppMlPppLinkBindEntry 3 }


--
-- The MLPPP Multiclass Traffic class Configuration Table
--

JuniPppMlPppMulticlassTcName ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "Name of the Traffic class.  The bundle name is a characteristic of a MLPPP
        Multiclass."
    SYNTAX OCTET STRING (SIZE(0..64))
    
juniPppMlPppMulticlassTraffiClassTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniPppMlPppMulticlassTrafficClassEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for MLPPP Multiclass to traffic class
         mapping of interfaces present in the system."
    ::= { juniPppMlPpp 7 }
 
juniPppMlPppMulticlassTrafficClassEntry OBJECT-TYPE
    SYNTAX      JuniPppMlPppMulticlassTrafficClassEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the MLPPP multiclass to traffic class mapping of
         interfaces.Other characteristics like fragmentation and reassembly
         for a particular traffic class can be configured."
    INDEX     { juniPppMlPppMulticlassIfIndex,
                juniPppMlPppMulticlassIndex }
    ::= { juniPppMlPppMulticlassTraffiClassTable  1 }

JuniPppMlPppMulticlassTrafficClassEntry ::= SEQUENCE {
	juniPppMlPppMulticlassIfIndex						InterfaceIndex,
    juniPppMlPppMulticlassIndex                       INTEGER,
    juniPppMlPppMulticlassTcName            			JuniPppMlPppMulticlassTcName,
    juniPppMlPppMulticlassFragmentation               JuniEnable,
    juniPppMlPppMulticlassReassembly                  JuniEnable }

juniPppMlPppMulticlassIfIndex OBJECT-TYPE
    SYNTAX      InterfaceIndex
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The ifIndex of the MLPPP interface.  When creating entries in this
        table, suitable values for this object are determined by reading
        juniPppMlPppMulticlassIfIndex."
    ::= { juniPppMlPppMulticlassTrafficClassEntry 1 }

juniPppMlPppMulticlassIndex OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION
		"The multiclass index of a particular traffic class type. This can be
		 configured only when MCMP is enabled on the link interface."
	DEFVAL	{ 15 }
	::= { juniPppMlPppMulticlassTrafficClassEntry 2 }
	
juniPppMlPppMulticlassTcName OBJECT-TYPE
	SYNTAX		JuniPppMlPppMulticlassTcName
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"The traffic class index mapped to the MCMP multiclass index. This can be
		 configured only when MCMP is enabled on the link interface."
	::= { juniPppMlPppMulticlassTrafficClassEntry 3 }
	
juniPppMlPppMulticlassFragmentation  OBJECT-TYPE
	SYNTAX		JuniEnable
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"Enable or disable fragmentation for a particular multiclass. This can be
		 configured only when MCMP is enaled on the link interface."
	DEFVAL  { disable }
	::= { juniPppMlPppMulticlassTrafficClassEntry 4 }

juniPppMlPppMulticlassReassembly  OBJECT-TYPE
	SYNTAX		JuniEnable
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION
		"Enable or disable rassembly for a particular multiclass. This can be
		 configured only when MCMP is enaled on the link interface."
	DEFVAL  { disable }
	::= { juniPppMlPppMulticlassTrafficClassEntry 5 }

-- /////////////////////////////////////////////////////////////////////////////
--
-- PPP Interface Summary Counts
--
-- /////////////////////////////////////////////////////////////////////////////

juniPppSummaryPppInterfaceCount OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP interfaces configured in the system."
    ::= { juniPppSummary 1 }

juniPppSummaryPppIpNCPs OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number IP NCPs configured in the system."
    ::= { juniPppSummary 2 }

juniPppSummaryPppOsiNCPs OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of OSI NCPs configured in the system."
    ::= { juniPppSummary 3 }

juniPppSummaryPppIfAdminUp OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP interfaces in the system that are
        administratively configured to up(1)."
    REFERENCE
        "IF-MIB.ifAdminStatus"
    ::= { juniPppSummary 4 }

juniPppSummaryPppIfAdminDown OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP interfaces in the system that are
        administrateively configued to down(2)."
    REFERENCE
        "IF-MIB.ifAdminStatus"
    ::= { juniPppSummary 5 }

juniPppSummaryPppIfOperUp OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP interfaces in the system with an operational
        state of up(1)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { juniPppSummary 7 }

juniPppSummaryPppIfOperDown OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP interfaces in the system with an operational
        state of down(2)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { juniPppSummary 8 }

juniPppSummaryPppIfOperDormant OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP interfaces in the system with an operational
        state of dormant(5)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { juniPppSummary 9 }

juniPppSummaryPppIfNotPresent OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP interfaces in the system with an operational
        state of notPresent(6)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { juniPppSummary 10 }

juniPppSummaryPppIfLowerLayerDown OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP interfaces in the system with an operational
        state of lowerLayerDown(7)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { juniPppSummary 11 }

juniPppSummaryPppIpNcpOpened OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP IP NCPs in the system with an operational state
        of opened(1)."
    REFERENCE
        "PPP-IP-NCP-MIB.pppIpOperStatus"
    ::= { juniPppSummary 12 }

juniPppSummaryPppIpNcpClosed OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP IP NCPs in the system with an operational
        state of not-opened(2)."
    REFERENCE
        "PPP-IP-NCP-MIB.pppIpOperStatus"
    ::= { juniPppSummary 13 }

juniPppSummaryPppOsiNcpOpened OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP OSI NCPs in the system with an operational
        state of opened."
    ::= { juniPppSummary 14 }

juniPppSummaryPppOsiNcpClosed OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP OSI NCPs in the system with an operational
        state of closed."
    ::= { juniPppSummary 15 }

juniPppSummaryPppIfLastChangeTime OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the sysUpTime at the time of the last PPP interface
        creation or deletion in the system.  If the number of PPP interfaces has
        been unchanged since the last re-initialization of the system, then this
        object contains a zero value. "
    ::= { juniPppSummary 16 }

juniPppSummaryPppLinkInterfaceCount OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP Link interfaces configured in the system."
    ::= { juniPppSummary 17 }

juniPppSummaryPppLinkIfAdminUp OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP Link interfaces in the system that are
        administratively configured to up(1)."
    REFERENCE
        "IF-MIB.ifAdminStatus"
    ::= { juniPppSummary 18 }

juniPppSummaryPppLinkIfAdminDown OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP Link interfaces in the system that are
        administrateively configued to down(2)."
    REFERENCE
        "IF-MIB.ifAdminStatus"
    ::= { juniPppSummary 19 }

juniPppSummaryPppLinkIfOperUp OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP Link interfaces in the system with an
        operational state of up(1)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { juniPppSummary 20 }

juniPppSummaryPppLinkIfOperDown OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP Link interfaces in the system with an
        operational state of down(2)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { juniPppSummary 21 }

juniPppSummaryPppLinkIfOperDormant OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP Link interfaces in the system with an
        operational state of dormant(5)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { juniPppSummary 22 }

juniPppSummaryPppLinkIfNotPresent OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP link interfaces in the system with an
        operational state of notPresent(6)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { juniPppSummary 23 }

juniPppSummaryPppLinkIfLowerLayerDown OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP Link interfaces in the system with an
        operational state of lowerLayerDown(7)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { juniPppSummary 24 }

juniPppSummaryPppLinkIfLastChangeTime OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the sysUpTime at the time of the last PPP Link interface
        creation or deletion in the system.  If the number of PPP interfaces has
        been unchanged since the last re-initialization of the system, then this
        object contains a zero value. "
    ::= { juniPppSummary 25 }

juniPppSummaryPppNetworkInterfaceCount OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP network interfaces configured in the system."
    ::= { juniPppSummary 26 }

juniPppSummaryPppNetworkIpNCPs OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number IP NCPs in the system configured on PPP network
        interfaces."
    ::= { juniPppSummary 27 }

juniPppSummaryPppNetworkOsiNCPs OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of OSI NCPs in the system configured on PPP network
        interfaces."
    ::= { juniPppSummary 28 }

juniPppSummaryPppNetworkIfAdminUp OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP network interfaces in the system that are
        administratively configured to up(1)."
    REFERENCE
        "IF-MIB.ifAdminStatus"
    ::= { juniPppSummary 29 }

juniPppSummaryPppNetworkIfAdminDown OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP network interfaces in the system that are
        administrateively configued to down(2)."
    REFERENCE
        "IF-MIB.ifAdminStatus"
    ::= { juniPppSummary 30 }

juniPppSummaryPppNetworkIfOperUp OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP network interfaces in the system with an
        operational state of up(1)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { juniPppSummary 31 }

juniPppSummaryPppNetworkIfOperDown OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP network interfaces in the system with an
        operational state of down(2)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { juniPppSummary 32 }

juniPppSummaryPppNetworkIfOperDormant OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP network interfaces in the system with an
        operational state of dormant(5)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { juniPppSummary 33 }

juniPppSummaryPppNetworkIfNotPresent OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP network interfaces in the system with an
        operational state of notPresent(6)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { juniPppSummary 34 }

juniPppSummaryPppNetworkIfLowerLayerDown OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP network interfaces in the system with an
        operational state of lowerLayerDown(7)."
    REFERENCE
        "IF-MIB.ifOperStatus"
    ::= { juniPppSummary 35 }

juniPppSummaryPppNetworkIpNcpOpened OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP IP NCPs in the system with an operational state
        of opened(1)."
    REFERENCE
        "PPP-IP-NCP-MIB.pppIpOperStatus"
    ::= { juniPppSummary 36 }

juniPppSummaryPppNetworkIpNcpClosed OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP IP NCPs in the system with an operational state
        of not-opened(2)."
    REFERENCE
        "PPP-IP-NCP-MIB.pppIpOperStatus"
    ::= { juniPppSummary 37 }

juniPppSummaryPppNetworkOsiNcpOpened OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP OSI NCPs in the system with an operational
        state of opened."
    ::= { juniPppSummary 38 }

juniPppSummaryPppNetworkOsiNcpClosed OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP OSI NCPs in the system with an operational
        state of closed."
    ::= { juniPppSummary 39 }

juniPppSummaryPppNetworkIfLastChangeTime OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the sysUpTime at the time of the last PPP network
        interface creation or deletion in the system.  If the number of PPP
        network interfaces has been unchanged since the last re-initialization
        of the system, then this object contains a zero value. "
    ::= { juniPppSummary 40 }

juniPppSummaryPppIpv6NCPs OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number IPv6 NCPs configured in the system."
    ::= { juniPppSummary 41 }

juniPppSummaryPppIpv6NcpOpened OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP IPv6 NCPs in the system with an operational
        state of opened(1)."
    REFERENCE
        "PPP-IP-NCP-MIB.pppIpOperStatus"
    ::= { juniPppSummary 42 }

juniPppSummaryPppIpv6NcpClosed OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP IPv6 NCPs in the system with an operational
        state of not-opened(2)."
    REFERENCE
        "PPP-IP-NCP-MIB.pppIpOperStatus"
    ::= { juniPppSummary 43 }

juniPppSummaryPppNetworkIpv6NCPs OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number IPv6 NCPs configured in the system."
    ::= { juniPppSummary 44 }

juniPppSummaryPppNetworkIpv6NcpOpened OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP IPv6 NCPs in the system with an operational
        state of opened(1)."
    REFERENCE
        "PPP-IP-NCP-MIB.pppIpOperStatus"
    ::= { juniPppSummary 45 }

juniPppSummaryPppNetworkIpv6NcpClosed OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP IPv6 NCPs in the system with an operational
        state of not-opened(2)."
    REFERENCE
        "PPP-IP-NCP-MIB.pppIpOperStatus"
    ::= { juniPppSummary 46 }

juniPppSummaryPppStaticInterfaceCount OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of static PPP interfaces configured in the system."
    ::= { juniPppSummary 47 }

juniPppSummaryPppMplsNCPs OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number MPLS NCPs configured in the system."
    ::= { juniPppSummary 48 }

juniPppSummaryPppIpAdminOpen OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IP NCPs in the system that are
        administratively configured to open(1)."
    ::= { juniPppSummary 49 }

juniPppSummaryPppIpAdminClose OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IP NCPs in the system that are
        administratively configured to close(2)."
    ::= { juniPppSummary 50 }

juniPppSummaryPppIpv6AdminOpen OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IPV6 NCPs in the system that are
        administratively configured to open(1)."
    ::= { juniPppSummary 51 }

juniPppSummaryPppIpv6AdminClose OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IPV6 NCPs in the system that are
        administratively configured to close(2)."
    ::= { juniPppSummary 52 }

juniPppSummaryPppOsiAdminOpen OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of OSI NCPs in the system that are
        administratively configured to open(1)."
    ::= { juniPppSummary 53 }

juniPppSummaryPppOsiAdminClose OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of OSI NCPs in the system that are
        administratively configured to close(2)."
    ::= { juniPppSummary 54 }

juniPppSummaryPppMplsAdminOpen OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of MPLS NCPs in the system that are
        administratively configured to open(1)."
    ::= { juniPppSummary 55 }

juniPppSummaryPppMplsAdminClose OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of MPLS NCPs in the system that are
        administratively configured to close(2)."
    ::= { juniPppSummary 56 }

juniPppSummaryPppIpNcpNotPresent OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP IP NCPs in the system with an operational state
        of notPresent(3)."
    REFERENCE
        "PPP-IP-NCP-MIB.pppIpOperStatus"
    ::= { juniPppSummary 57}

juniPppSummaryPppIpNcpNoResources OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP IP NCPs in the system with an operational
        state of noResources(4)."
    REFERENCE
        "PPP-IP-NCP-MIB.pppIpOperStatus"
    ::= { juniPppSummary 58 }

juniPppSummaryPppIpv6NcpNotPresent OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP IPV6 NCPs in the system with an operational state
        of notPresent(3)."
    ::= { juniPppSummary 59 }

juniPppSummaryPppIpv6NcpNoResources OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP IPV6 NCPs in the system with an operational
        state of noResources(4)."
    ::= { juniPppSummary 60 }

juniPppSummaryPppOsiNcpNotPresent OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP OSI NCPs in the system with an operational state
        of notPresent(3)."
    ::= { juniPppSummary 61 }

juniPppSummaryPppOsiNcpNoResources OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP OSI NCPs in the system with an operational
        state of noResources(4)."
    ::= { juniPppSummary 62 }

juniPppSummaryPppMplsNcpOpened OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP MPLS NCPs in the system with an operational state
        of opened(1)."
    ::= { juniPppSummary 63 }

juniPppSummaryPppMplsNcpClosed OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP MPLS NCPs in the system with an operational
        state of not-opened(2)."
    ::= { juniPppSummary 64 }

juniPppSummaryPppMplsNcpNotPresent OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP MPLS NCPs in the system with an operational state
        of notPresent(3)."
    ::= { juniPppSummary 65 }

juniPppSummaryPppMplsNcpNoResources OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of PPP MPLS NCPs in the system with an operational
        state of noResources(4)."
    ::= { juniPppSummary 66 }

juniPppSummaryPppLinkStaticInterfaceCount OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of static PPP Link interfaces configured in the system."
    ::= { juniPppSummary 67 }

juniPppSummaryPppNetworkStaticInterfaceCount OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of static PPP network interfaces configured in the system."
    ::= { juniPppSummary 68 }

juniPppSummaryPppNetworkMplsNCPs OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of MPLS NCPs in the system configured on PPP network
        interfaces."
    ::= { juniPppSummary 69 }

juniPppSummaryPppNetworkIpAdminOpen OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IP NCPs in the system configured on PPP network
         interfaces that are administratively configured to open(1)."
    ::= { juniPppSummary 70 }

juniPppSummaryPppNetworkIpAdminClose OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IP NCPs in the system configured on PPP network
         interfaces that are administratively configured to close(2)."
    ::= { juniPppSummary 71 }

juniPppSummaryPppNetworkIpv6AdminOpen OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IPV6 NCPs in the system configured on PPP network
         interfaces that are administratively configured to open(1)."
    ::= { juniPppSummary 72 }

juniPppSummaryPppNetworkIpv6AdminClose OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IPV6 NCPs in the system configured on PPP network
         interfaces that are administratively configured to close(2)."
    ::= { juniPppSummary 73 }

juniPppSummaryPppNetworkOsiAdminOpen OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of OSI NCPs in the system configured on PPP network
         interfaces that are administratively configured to open(1)."
    ::= { juniPppSummary 74 }

juniPppSummaryPppNetworkOsiAdminClose OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of OSI NCPs in the system configured on PPP network
         interfaces that are administratively configured to close(2)."
    ::= { juniPppSummary 75 }

juniPppSummaryPppNetworkMplsAdminOpen OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of MPLS NCPs in the system configured on PPP network
         interfaces that are administratively configured to open(1)."
    ::= { juniPppSummary 76 }

juniPppSummaryPppNetworkMplsAdminClose OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of MPLS NCPs in the system configured on PPP network
         interfaces that are administratively configured to close(2)."
    ::= { juniPppSummary 77 }

juniPppSummaryPppNetworkIpNcpNotPresent OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IP NCPs in the system configured on PPP network
        interfaces with an operational state of notPresent(3)."
    REFERENCE
        "PPP-IP-NCP-MIB.pppIpOperStatus"
    ::= { juniPppSummary 78 }

juniPppSummaryPppNetworkIpNcpNoResources OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IP NCPs in the system configured on PPP network
        interfaces with an operational state of noResources(4)."
    REFERENCE
        "PPP-IP-NCP-MIB.pppIpOperStatus"
    ::= { juniPppSummary 79 }

juniPppSummaryPppNetworkIpv6NcpNotPresent OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IPV6 NCPs in the system configured on PPP network
        interfaces with an operational state of notPresent(3)."
    ::= { juniPppSummary 80 }

juniPppSummaryPppNetworkIpv6NcpNoResources OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of IPV6 NCPs in the system configured on PPP network
        interfaces with an operational state of noResources(4)."
    ::= { juniPppSummary 81 }

juniPppSummaryPppNetworkOsiNcpNotPresent OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of OSI NCPs in the system configured on PPP network
        interfaces with an operational state of notPresent(3)."
    ::= { juniPppSummary 82 }

juniPppSummaryPppNetworkOsiNcpNoResources OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of OSI NCPs in the system configured on PPP network
        interfaces with an operational state of noResources(4)."
    ::= { juniPppSummary 83 }

juniPppSummaryPppNetworkMplsNcpOpened OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of MPLS NCPs in the system configured on PPP network
        interfaces with an operational state of opened(1)."
    ::= { juniPppSummary 84 }

juniPppSummaryPppNetworkMplsNcpClosed OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of MPLS NCPs in the system configured on PPP network
        interfaces with an operational state of not-opened(2)."
    ::= { juniPppSummary 85 }

juniPppSummaryPppNetworkMplsNcpNotPresent OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of MPLS NCPs in the system configured on PPP network
        interfaces with an operational state of notPresent(3)."
    ::= { juniPppSummary 86 }

juniPppSummaryPppNetworkMplsNcpNoResources OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The total number of MPLS NCPs in the system configured on PPP network
        interfaces with an operational state of noResources(4)."
    ::= { juniPppSummary 87 }

-- /////////////////////////////////////////////////////////////////////////////
--
-- PPP IPv6 NCP
--
-- This section defines objects used to manage the PPP Network
-- Control Protocol for IPv6 protocol operation (IPV6CP).
--
-- /////////////////////////////////////////////////////////////////////////////
--
-- The PPP IPv6 Table
--
juniPppIpv6Table OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniPppIpv6Entry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table containing the IPv6 parameters for the local PPP entity."
    ::= { juniPppIpv6 1 }

juniPppIpv6Entry OBJECT-TYPE
    SYNTAX      JuniPppIpv6Entry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "IPV6CP status information for a particular PPP link."
    INDEX     { ifIndex }
    ::= { juniPppIpv6Table 1 }

JuniPppIpv6Entry ::= SEQUENCE {
    juniPppIpv6ServiceStatus                       JuniEnable,
    juniPppIpv6OperStatus                          INTEGER,
    juniPppIpv6TerminateReason                     INTEGER,
    juniPppIpv6TerminateNegFailOption              INTEGER,
    juniPppIpv6LocalIpv6AddressIfIdentifier        Ipv6AddressIfIdentifier,
    juniPppIpv6RemoteIpv6AddressIfIdentifier       Ipv6AddressIfIdentifier,
    juniPppIpv6NetworkStatusIpv6cpRenegoTerminates Counter32}

juniPppIpv6ServiceStatus OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates whether IPv6 protocol service is operating over this PPP
        link.  Service is established on this link through means outside this
        MIB."
    ::= { juniPppIpv6Entry 1 }

juniPppIpv6OperStatus OBJECT-TYPE
    SYNTAX      INTEGER {
                    opened(1),
                    notOpened(2) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The operational status of the IPv6 network protocol.  If the value of
        this object is up then the finite state machine for the IPv6 network
        protocol has reached the Opened state."
    ::= { juniPppIpv6Entry 2 }

juniPppIpv6TerminateReason OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    other(1),
                    noService(2),
                    admin(3),
                    linkDown(4),
                    peerTerminated(5),
                    peerRenegotiated(6),
                    maxRetriesExceeded(7),
                    negotiationFailure(8) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Reason the IPV6CP link was terminated:
            none                    None.
            other                   Not specified.
            noService               No IPv6 service configured on this PPP link.
            admin                   Administratively disabled.
            linkDown                Underlying link is down.
            peerTerminated          Peer initiated termination.
            peerRenegotiated        Peer initiated renegotiation.
            maxRetriesExceeded      Maximum number of config retries exceeded.
            negotiationFailure      Failed to negotiate IPV6CP option.  See
                                    juniPppIpv6TerminateNegFailOption."
    ::= { juniPppIpv6Entry 3 }

juniPppIpv6TerminateNegFailOption OBJECT-TYPE
    SYNTAX      INTEGER {
                    none(0),
                    other(1),
                    localIpv6AddressIfIdentifier(2),
                    remoteIpv6AddressIfIdentifier(3) }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Reports the PPP IPV6CP option for which negotiation failed, when
        juniPppIpv6TerminateReason has the value 'negotiationFailure'."
    ::= { juniPppIpv6Entry 4 }

juniPppIpv6LocalIpv6AddressIfIdentifier OBJECT-TYPE
    SYNTAX      Ipv6AddressIfIdentifier
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "IPv6 Address Interface Identifier used by the local side."
    ::= { juniPppIpv6Entry 5 }

juniPppIpv6RemoteIpv6AddressIfIdentifier OBJECT-TYPE
    SYNTAX      Ipv6AddressIfIdentifier
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "IPv6 Address Interface Identifier used by the remote side."
    ::= { juniPppIpv6Entry 6 }

juniPppIpv6NetworkStatusIpv6cpRenegoTerminates OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Number of times ipv6cp terminated due to peer exceeding max
        renegotiation attempts."
    ::= { juniPppIpv6Entry 7 }

--
-- The PPP IPv6 Config Table
--
juniPppIpv6ConfigTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniPppIpv6ConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Table containing the IPv6 parameters for the local PPP entity."
    ::= { juniPppIpv6 2 }

juniPppIpv6ConfigEntry OBJECT-TYPE
    SYNTAX      JuniPppIpv6ConfigEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "IPV6CP configuration information for a particular PPP link."
    INDEX     { ifIndex }
    ::= { juniPppIpv6ConfigTable 1 }

JuniPppIpv6ConfigEntry ::= SEQUENCE {
    juniPppIpv6ConfigAdminStatus            INTEGER,
    juniPppIpv6ConfigInitiateIpv6           JuniEnable,
    juniPppIpv6ConfigMaxIpv6cpRenegotiation Integer32 }

juniPppIpv6ConfigAdminStatus OBJECT-TYPE
    SYNTAX      INTEGER {
                    open(1),
                    close(2) }
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The immediate desired status of the IPv6 network protocol.  Setting
        this object to open will inject an administrative open event into the
        IPv6 network protocol's finite state machine.  Setting this object to
        close will inject an administrative close event into the IPv6 network
        protocol's finite state machine."
    ::= { juniPppIpv6ConfigEntry 1 }

juniPppIpv6ConfigInitiateIpv6 OBJECT-TYPE
    SYNTAX      JuniEnable
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Enables the initiation of negotiation of the IPv6CP."
    DEFVAL { disable }
    ::= { juniPppIpv6ConfigEntry 2 }

juniPppIpv6ConfigMaxIpv6cpRenegotiation OBJECT-TYPE
    SYNTAX      Integer32 (1..65535)
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "Maximum number of allowed ipv6cp renegotiation attempts from peer."
    DEFVAL { 30 }
    ::= { juniPppIpv6ConfigEntry 3 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Notifications
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- No notifications are defined in this MIB.  Placeholders follow.
-- juniPppTrapControl      OBJECT IDENTIFIER ::= { juniPppMIB 2 }
-- juniPppTraps            OBJECT IDENTIFIER ::= { juniPppMIB 3 }
-- juniPppTrapPrefix       OBJECT IDENTIFIER ::= { juniPppTraps 0 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Conformance information
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniPppConformance OBJECT IDENTIFIER ::= { juniPppMIB 4 }
juniPppCompliances OBJECT IDENTIFIER ::= { juniPppConformance 1 }
juniPppGroups      OBJECT IDENTIFIER ::= { juniPppConformance 2 }

--
-- compliance statements
--
juniPppCompliance  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        PPP MIB.  This statement became obsolete when additional objects were
        added to the MIB."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniPppLcpGroup,
            juniPppIpGroup,
            juniPppOsiGroup }
    ::= { juniPppCompliances 1 }                                   -- JUNOSe 1.0

juniPppCompliance2  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION

        "Obsolete compliance statement for entities which implement the Juniper
        PPP MIB.  This statement became obsolete when the juniPppMlPppGroup and
        juniPppSummaryGroup objects were added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniPppLcpGroup2,
            juniPppIpGroup2,
            juniPppOsiGroup2,
            juniPppSessionGroup }
    ::= { juniPppCompliances 2 }                                   -- JUNOSe 1.1

juniPppCompliance3  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        PPP MIB.  This statement became obsolete when the
        juniPppLinkConfigStandardIfIndex object was added to the MIB."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniPppLcpGroup2,
            juniPppIpGroup2,
            juniPppOsiGroup2,
            juniPppSessionGroup,
            juniPppMlPppGroup,
            juniPppSummaryGroup }
    ::= { juniPppCompliances 3 }                                   -- JUNOSe 2.0

juniPppCompliance4  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        PPP MIB.  This statement became obsolete when the juniPppMlPppGroup,
        juniPppSummaryLinkGroup and juniPppSummaryNetworkGroup were moved from
        the list of mandatory groups."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniPppLcpGroup3,
            juniPppIpGroup2,
            juniPppOsiGroup2,
            juniPppSessionGroup,
            juniPppMlPppGroup,
            juniPppSummaryGroup }
    ::= { juniPppCompliances 4 }                                   -- JUNOSe 2.4

juniPppCompliance5  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        PPP MIB.  This statement became obsolete when new IP, LCP and multi-link
        objects were added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniPppLcpGroup3,
            juniPppIpGroup2,
            juniPppOsiGroup2,
            juniPppSessionGroup,
            juniPppSummaryBasicGroup }
        GROUP       juniPppMlPppGroup
            DESCRIPTION
                "The multi-link PPP group is mandatory only for PPP entities
                that support multi-link functionality."
        GROUP       juniPppSummaryLinkGroup
            DESCRIPTION
                "The link summary group is mandatory only for PPP entities that
                support multi-link functionality."
        GROUP       juniPppSummaryNetworkGroup
            DESCRIPTION
                "The network summary group is mandatory only for PPP entities
                that support multi-link functionality."
    ::= { juniPppCompliances 5 }                                   -- JUNOSe 3.3

juniPppCompliance6  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        PPP MIB.  This statement became obsolete when new juniPppLcpGroup and
        juniPppMlPppGroup objects were added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniPppLcpGroup4,
            juniPppIpGroup3,
            juniPppOsiGroup2,
            juniPppSessionGroup,
            juniPppSummaryBasicGroup }
        GROUP       juniPppMlPppGroup2
            DESCRIPTION
                "The multi-link PPP group is mandatory only for PPP entities
                that support multi-link functionality."
        GROUP       juniPppSummaryLinkGroup
            DESCRIPTION
                "The link summary group is mandatory only for PPP entities that
                support multi-link functionality."
        GROUP       juniPppSummaryNetworkGroup
            DESCRIPTION
                "The network summary group is mandatory only for PPP entities
                that support multi-link functionality."
    ::= { juniPppCompliances 6 }                                   -- JUNOSe 4.0

juniPppCompliance7  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        PPP MIB.  This statement became obsolete when more new multi-link
        objects were added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniPppLcpGroup5,
            juniPppIpGroup3,
            juniPppOsiGroup2,
            juniPppSessionGroup,
            juniPppSummaryBasicGroup }
        GROUP       juniPppMlPppGroup3
            DESCRIPTION
                "The multi-link PPP group is mandatory only for PPP entities
                that support multi-link functionality."
        GROUP       juniPppSummaryLinkGroup
            DESCRIPTION
                "The link summary group is mandatory only for PPP entities that
                support multi-link functionality."
        GROUP       juniPppSummaryNetworkGroup
            DESCRIPTION
                "The network summary group is mandatory only for PPP entities
                that support multi-link functionality."
    ::= { juniPppCompliances 7 }                                   -- JUNOSe 4.1

juniPppCompliance8  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        PPP MIB.  This statement became obsolete when IPv6 support was added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniPppLcpGroup5,
            juniPppIpGroup3,
            juniPppOsiGroup2,
            juniPppSessionGroup,
            juniPppSummaryBasicGroup }
        GROUP       juniPppMlPppGroup4
            DESCRIPTION
                "The multi-link PPP group is mandatory only for PPP entities
                that support multi-link functionality."
        GROUP       juniPppSummaryLinkGroup
             DESCRIPTION
                "The link summary group is mandatory only for PPP entities that
                support multi-link functionality."
        GROUP       juniPppSummaryNetworkGroup
            DESCRIPTION
                "The network summary group is mandatory only for PPP entities
                that support multi-link functionality."
    ::= { juniPppCompliances 8 }                                   -- JUNOSe 5.0

juniPppCompliance9  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        PPP MIB.  This statement became obsolete when more new multi-link
        objects were added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniPppLcpGroup5,
            juniPppIpGroup4,
            juniPppOsiGroup2,
            juniPppSessionGroup2,
            juniPppSummaryBasicGroup2,
            juniPppIpv6Group }
        GROUP       juniPppMlPppGroup4
            DESCRIPTION
                "The multi-link PPP group is mandatory only for PPP entities
                that support multi-link functionality."
        GROUP       juniPppSummaryLinkGroup
            DESCRIPTION
                "The link summary group is mandatory only for PPP entities that
                support multi-link functionality."
        GROUP       juniPppSummaryNetworkGroup2
            DESCRIPTION
                "The network summary group is mandatory only for PPP entities
                that support multi-link functionality."
    ::= { juniPppCompliances 9 }                                  -- JUNOSe 5.1

juniPppCompliance10  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        PPP MIB.  This statement became obsolete when more new juniPppSummary
        objects were added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniPppLcpGroup5,
            juniPppIpGroup4,
            juniPppOsiGroup2,
            juniPppSessionGroup2,
            juniPppSummaryBasicGroup2,
            juniPppIpv6Group }
        GROUP       juniPppMlPppGroup5
            DESCRIPTION
                "The multi-link PPP group is mandatory only for PPP entities
                that support multi-link functionality."
        GROUP       juniPppSummaryLinkGroup
            DESCRIPTION
                "The link summary group is mandatory only for PPP entities that
                support multi-link functionality."
        GROUP       juniPppSummaryNetworkGroup2
            DESCRIPTION
                "The network summary group is mandatory only for PPP entities
                that support multi-link functionality."
    ::= { juniPppCompliances 10 }                                  -- JUNOSe 5.3

juniPppCompliance11  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
	"Obsolete compliance statement for entities which implement the Juniper
        PPP MIB.  This statement became obsolete when a new multi-link
        object was added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniPppLcpGroup5,
            juniPppIpGroup4,
            juniPppOsiGroup2,
            juniPppSessionGroup2,
            juniPppSummaryBasicGroup3,
            juniPppIpv6Group }
        GROUP       juniPppMlPppGroup5
            DESCRIPTION
                "The multi-link PPP group is mandatory only for PPP entities
                that support multi-link functionality."
        GROUP       juniPppSummaryLinkGroup2
            DESCRIPTION
                "The link summary group is mandatory only for PPP entities that
                support multi-link functionality."
        GROUP       juniPppSummaryNetworkGroup3
            DESCRIPTION
                "The network summary group is mandatory only for PPP entities
                that support multi-link functionality."
    ::= { juniPppCompliances 11 }                                  -- JUNOSe 6.0

juniPppCompliance12  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "Obsolete compliance statement for entities which implement the Juniper
        PPP MIB.  This statement became obsolete when more new juniPppLcpGroup
        and juniPppMlPppGroup objects were added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniPppLcpGroup5,
            juniPppIpGroup4,
            juniPppOsiGroup2,
            juniPppSessionGroup2,
            juniPppSummaryBasicGroup3,
            juniPppIpv6Group }
        GROUP       juniPppMlPppGroup6
            DESCRIPTION
                "The multi-link PPP group is mandatory only for PPP entities
                that support multi-link functionality."
        GROUP       juniPppSummaryLinkGroup2
            DESCRIPTION
                "The link summary group is mandatory only for PPP entities that
                support multi-link functionality."
        GROUP       juniPppSummaryNetworkGroup3
            DESCRIPTION
                "The network summary group is mandatory only for PPP entities
                that support multi-link functionality."
    ::= { juniPppCompliances 12 }                                  -- JUNOSe 7.2

juniPppCompliance13  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for entities which implement the Juniper PPP
        MIB. This statement became obsolete when more new juniPppLcpGroup,
        juniPppIpGroup and juniPppIpv6Group objects were added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniPppLcpGroup7,
            juniPppIpGroup4,
            juniPppOsiGroup2,
            juniPppSessionGroup2,
            juniPppSummaryBasicGroup3,
            juniPppIpv6Group }
        GROUP       juniPppMlPppGroup8
            DESCRIPTION
                "The multi-link PPP group is mandatory only for PPP entities
                that support multi-link functionality."
        GROUP       juniPppSummaryLinkGroup2
            DESCRIPTION
                "The link summary group is mandatory only for PPP entities that
                support multi-link functionality."
        GROUP       juniPppSummaryNetworkGroup3
            DESCRIPTION
                "The network summary group is mandatory only for PPP entities
                that support multi-link functionality."
    ::= { juniPppCompliances 13 }                                  -- JUNOSe 7.3

juniPppCompliance14  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "The compliance statement for entities which implement the Juniper PPP
        MIB."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniPppLcpGroup8,
            juniPppIpGroup5,
            juniPppOsiGroup2,
            juniPppSessionGroup2,
            juniPppSummaryBasicGroup3,
            juniPppIpv6Group2 }
        GROUP       juniPppMlPppGroup8
            DESCRIPTION
                "The multi-link PPP group is mandatory only for PPP entities
                that support multi-link functionality."
        GROUP       juniPppSummaryLinkGroup2
            DESCRIPTION
                "The link summary group is mandatory only for PPP entities that
                support multi-link functionality."
        GROUP       juniPppSummaryNetworkGroup3
            DESCRIPTION
                "The network summary group is mandatory only for PPP entities
                that support multi-link functionality."
    ::= { juniPppCompliances 14 }                                  -- JUNOSe 10.1

juniPppCompliance15  MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for entities which implement the Juniper PPP
        MIB."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniPppLcpGroup8,
            juniPppIpGroup6,
            juniPppOsiGroup2,
            juniPppSessionGroup2,
            juniPppSummaryBasicGroup3,
            juniPppIpv6Group2 }
        GROUP       juniPppMlPppGroup8
            DESCRIPTION
                "The multi-link PPP group is mandatory only for PPP entities
                that support multi-link functionality."
        GROUP       juniPppSummaryLinkGroup2
            DESCRIPTION
                "The link summary group is mandatory only for PPP entities that
                support multi-link functionality."
        GROUP       juniPppSummaryNetworkGroup3
            DESCRIPTION
                "The network summary group is mandatory only for PPP entities
                that support multi-link functionality."
    ::= { juniPppCompliances 15 }                                  -- JUNOSe 11.0

juniPppCompliance16  MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for entities which implement the Juniper PPP
        MIB. This statement was obsoleted when MCMP traffic class mapping was
		added. New group juniPppMlPppMulticlassTcGroup1 was added."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniPppLcpGroup8,
            juniPppIpGroup5,
            juniPppOsiGroup2,
            juniPppSessionGroup2,
            juniPppSummaryBasicGroup3,
            juniPppIpv6Group2 }
        GROUP       juniPppMlPppGroup9
            DESCRIPTION
                "The multi-link PPP group is mandatory only for PPP entities
                that support multi-link functionality."
        GROUP       juniPppSummaryLinkGroup2
            DESCRIPTION
                "The link summary group is mandatory only for PPP entities that
                support multi-link functionality."
        GROUP       juniPppSummaryNetworkGroup3
            DESCRIPTION
                "The network summary group is mandatory only for PPP entities
                that support multi-link functionality."
        GROUP		juniPppMlPppMulticlassTcGroup1
        	DESCRIPTION
        		"The Multilink multiclass traffic class group is mandatory only 
				for PPP entities that support multi-link functionality."
    ::= { juniPppCompliances 16 }                                  -- JUNOSe 11.1
    
--
-- units of conformance
--
juniPppLcpGroup  OBJECT-GROUP
    OBJECTS {
        juniPppLinkConfigRowStatus,
        juniPppLinkConfigLowerIfIndex,
        juniPppNextIfIndex }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of link-layer
        functionality (LCP) of PPP interfaces in a Juniper product.  This group
        became obsolete when additional objects were added."
    ::= { juniPppGroups 1 }                                        -- JUNOSe 1.0

juniPppIpGroup  OBJECT-GROUP
    OBJECTS {
        juniPppIpServiceStatus }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of IP network
        control protocol functionality (IPCP) of PPP interfaces in a Juniper
        product.  This group became obsolete when additional objects were
        added."
    ::= { juniPppGroups 2 }                                        -- JUNOSe 1.0

juniPppOsiGroup  OBJECT-GROUP
    OBJECTS {
        juniPppOsiServiceStatus,
        juniPppOsiOperStatus,

        juniPppOsiConfigAdminStatus }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of OSI network
        control protocol functionality (OSICP) of PPP interfaces in a Juniper
        product.  This group became obsolete when additional objects were
        added."
    ::= { juniPppGroups 3 }                                        -- JUNOSe 1.0

juniPppLcpGroup2  OBJECT-GROUP
    OBJECTS {
        juniPppLinkStatusTerminateReason,
        juniPppLinkStatusTerminateNegFailOption,
        juniPppLinkStatusInKeepaliveRequests,
        juniPppLinkStatusOutKeepaliveRequests,
        juniPppLinkStatusInKeepaliveReplies,
        juniPppLinkStatusOutKeepaliveReplies,
        juniPppLinkStatusKeepaliveFailures,
        juniPppLinkStatusLocalMagicNumber,
        juniPppLinkStatusRemoteMagicNumber,
        juniPppLinkStatusLocalAuthentication,
        juniPppLinkStatusTunnelIfIndex,
        juniPppLinkConfigRowStatus,
        juniPppLinkConfigLowerIfIndex,
        juniPppLinkConfigKeepalive,
        juniPppLinkConfigAuthentication,
        juniPppLinkConfigMaxAuthenRetries,
        juniPppNextIfIndex }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of link-layer
        functionality (LCP) of PPP interfaces in a Juniper product.  This group
        became obsolete when the juniPppLinkConfigStandardIfIndex object was
        added."
    ::= { juniPppGroups 4 }                                        -- JUNOSe 1.1

juniPppIpGroup2  OBJECT-GROUP
    OBJECTS {
        juniPppIpServiceStatus,
        juniPppIpTerminateReason,
        juniPppIpTerminateNegFailOption,
        juniPppIpLocalIpAddress,
        juniPppIpRemoteIpAddress,
        juniPppIpRemotePrimaryDnsAddress,
        juniPppIpRemoteSecondaryDnsAddress,
        juniPppIpRemotePrimaryWinsAddress,
        juniPppIpRemoteSecondaryWinsAddress,
        juniPppIpConfigPeerDnsPriority,
        juniPppIpConfigPeerWinsPriority }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of IP network
        control protocol functionality (IPCP) of PPP interfaces in a Juniper
        product.  This group became obsolete when additional objects were
        added."
    ::= { juniPppGroups 5 }                                        -- JUNOSe 1.1

juniPppOsiGroup2  OBJECT-GROUP
    OBJECTS {
        juniPppOsiServiceStatus,
        juniPppOsiOperStatus,
        juniPppOsiTerminateReason,
        juniPppOsiTerminateNegFailOption,
        juniPppOsiLocalAlignNpdu,
        juniPppOsiRemoteAlignNpdu,
        juniPppOsiConfigAdminStatus }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing management of OSI network control
        protocol functionality (OSICP) of PPP interfaces in a Juniper product."
    ::= { juniPppGroups 6 }                                        -- JUNOSe 1.1

juniPppSessionGroup  OBJECT-GROUP
    OBJECTS {
        juniPppSessionGrant,
        juniPppSessionTerminateReason,
        juniPppSessionStartTime,
        juniPppSessionInOctets,
        juniPppSessionOutOctets,
        juniPppSessionInPackets,
        juniPppSessionOutPackets,
        juniPppSessionSessionTimeout,
        juniPppSessionInactivityTimeout,
        juniPppSessionAccountingInterval,
        juniPppSessionRemoteIpAddress,
        juniPppSessionRemotePrimaryDnsAddress,
        juniPppSessionRemoteSecondaryDnsAddress,
        juniPppSessionRemotePrimaryWinsAddress,
        juniPppSessionRemoteSecondaryWinsAddress }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of PPP session
        functionality of PPP interfaces in a Juniper product.  This group became
        obsolete when IPv6 support was added."
    ::= { juniPppGroups 7 }                                        -- JUNOSe 1.1

juniPppMlPppGroup  OBJECT-GROUP
    OBJECTS {
        juniPppMlPppBundleRowStatus,
        juniPppMlPppNextLinkIfIndex,
        juniPppMlPppLinkConfigLowerIfIndex,
        juniPppMlPppLinkConfigKeepalive,
        juniPppMlPppLinkConfigAuthentication,
        juniPppMlPppLinkConfigMaxAuthenRetries,
        juniPppMlPppLinkConfigRowStatus,
        juniPppMlPppNextNetworkIfIndex,
        juniPppMlPppNetworkConfigLowerIfIndex,
        juniPppMlPppNetworkBundleName,
        juniPppMlPppNetworkRowStatus,
        juniPppMlPppBindRowStatus }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing multi link PPP management
        support in a Juniper product.  This group became obsolete when
        additional objects were added."
    ::= { juniPppGroups 8 }                                        -- JUNOSe 2.0

juniPppSummaryGroup  OBJECT-GROUP
    OBJECTS {
        juniPppSummaryPppInterfaceCount,
        juniPppSummaryPppIpNCPs,
        juniPppSummaryPppOsiNCPs,
        juniPppSummaryPppIfAdminUp,
        juniPppSummaryPppIfAdminDown,
        juniPppSummaryPppIfOperUp,
        juniPppSummaryPppIfOperDown,
        juniPppSummaryPppIfOperDormant,
        juniPppSummaryPppIfNotPresent,
        juniPppSummaryPppIfLowerLayerDown,
        juniPppSummaryPppIfLastChangeTime,
        juniPppSummaryPppLinkInterfaceCount,
        juniPppSummaryPppLinkIfAdminUp,
        juniPppSummaryPppLinkIfAdminDown,
        juniPppSummaryPppLinkIfOperUp,
        juniPppSummaryPppLinkIfOperDown,
        juniPppSummaryPppLinkIfOperDormant,
        juniPppSummaryPppLinkIfNotPresent,
        juniPppSummaryPppLinkIfLowerLayerDown,
        juniPppSummaryPppLinkIfLastChangeTime,
        juniPppSummaryPppNetworkInterfaceCount,
        juniPppSummaryPppNetworkIpNCPs,
        juniPppSummaryPppNetworkOsiNCPs,
        juniPppSummaryPppNetworkIfAdminUp,
        juniPppSummaryPppNetworkIfAdminDown,
        juniPppSummaryPppNetworkIfOperUp,
        juniPppSummaryPppNetworkIfOperDown,
        juniPppSummaryPppNetworkIfOperDormant,
        juniPppSummaryPppNetworkIfNotPresent,
        juniPppSummaryPppNetworkIfLowerLayerDown,
        juniPppSummaryPppNetworkIfLastChangeTime,
        juniPppSummaryPppIpNcpOpened,
        juniPppSummaryPppIpNcpClosed,
        juniPppSummaryPppOsiNcpOpened,
        juniPppSummaryPppOsiNcpClosed,
        juniPppSummaryPppNetworkIpNcpOpened,
        juniPppSummaryPppNetworkIpNcpClosed,
        juniPppSummaryPppNetworkOsiNcpOpened,
        juniPppSummaryPppNetworkOsiNcpClosed }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing PPP interface summary
        information in a Juniper product.  This group became obsolete when it
        was divided into three groups so that the link and network object would
        not be manditory."
    ::= { juniPppGroups 9 }                                        -- JUNOSe 2.0

juniPppLcpGroup3  OBJECT-GROUP
    OBJECTS {
        juniPppLinkStatusTerminateReason,
        juniPppLinkStatusTerminateNegFailOption,
        juniPppLinkStatusInKeepaliveRequests,
        juniPppLinkStatusOutKeepaliveRequests,
        juniPppLinkStatusInKeepaliveReplies,
        juniPppLinkStatusOutKeepaliveReplies,
        juniPppLinkStatusKeepaliveFailures,
        juniPppLinkStatusLocalMagicNumber,
        juniPppLinkStatusRemoteMagicNumber,
        juniPppLinkStatusLocalAuthentication,
        juniPppLinkStatusTunnelIfIndex,
        juniPppLinkConfigRowStatus,
        juniPppLinkConfigLowerIfIndex,
        juniPppLinkConfigKeepalive,
        juniPppLinkConfigAuthentication,
        juniPppLinkConfigMaxAuthenRetries,
        juniPppLinkConfigStandardIfIndex,
        juniPppNextIfIndex }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of link-layer
        functionality (LCP) of PPP interfaces in a Juniper product.  This group
        became obsolete when additional objects were added."
    ::= { juniPppGroups 10 }                                       -- JUNOSe 2.4

juniPppSummaryBasicGroup  OBJECT-GROUP
    OBJECTS {
        juniPppSummaryPppInterfaceCount,
        juniPppSummaryPppIpNCPs,
        juniPppSummaryPppOsiNCPs,
        juniPppSummaryPppIfAdminUp,
        juniPppSummaryPppIfAdminDown,
        juniPppSummaryPppIfOperUp,
        juniPppSummaryPppIfOperDown,
        juniPppSummaryPppIfOperDormant,
        juniPppSummaryPppIfNotPresent,
        juniPppSummaryPppIfLowerLayerDown,
        juniPppSummaryPppIfLastChangeTime,
        juniPppSummaryPppIpNcpOpened,
        juniPppSummaryPppIpNcpClosed,
        juniPppSummaryPppOsiNcpOpened,
        juniPppSummaryPppOsiNcpClosed }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing PPP interface basic summary
        information in a Juniper product.  This group became obsolete when IPv6
        support was added."
    ::= { juniPppGroups 11 }                                       -- JUNOSe 3.3

juniPppSummaryLinkGroup  OBJECT-GROUP
    OBJECTS {
        juniPppSummaryPppLinkInterfaceCount,
        juniPppSummaryPppLinkIfAdminUp,
        juniPppSummaryPppLinkIfAdminDown,
        juniPppSummaryPppLinkIfOperUp,
        juniPppSummaryPppLinkIfOperDown,
        juniPppSummaryPppLinkIfOperDormant,
        juniPppSummaryPppLinkIfNotPresent,
        juniPppSummaryPppLinkIfLowerLayerDown,
        juniPppSummaryPppLinkIfLastChangeTime }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing PPP interface basic summary
        information in a Juniper product.  This group became obsolete when 
        new objects were added."
    ::= { juniPppGroups 12 }                                       -- JUNOSe 3.3

juniPppSummaryNetworkGroup  OBJECT-GROUP
    OBJECTS {
        juniPppSummaryPppNetworkInterfaceCount,
        juniPppSummaryPppNetworkIpNCPs,
        juniPppSummaryPppNetworkOsiNCPs,
        juniPppSummaryPppNetworkIfAdminUp,
        juniPppSummaryPppNetworkIfAdminDown,
        juniPppSummaryPppNetworkIfOperUp,
        juniPppSummaryPppNetworkIfOperDown,
        juniPppSummaryPppNetworkIfOperDormant,
        juniPppSummaryPppNetworkIfNotPresent,
        juniPppSummaryPppNetworkIfLowerLayerDown,
        juniPppSummaryPppNetworkIfLastChangeTime,
        juniPppSummaryPppNetworkIpNcpOpened,
        juniPppSummaryPppNetworkIpNcpClosed,
        juniPppSummaryPppNetworkOsiNcpOpened,
        juniPppSummaryPppNetworkOsiNcpClosed }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing PPP interface network summary
        information in a Juniper product.  This group became obsolete when IPv6
        support was added."
    ::= { juniPppGroups 13 }                                       -- JUNOSe 3.3

juniPppLcpGroup4  OBJECT-GROUP
    OBJECTS {
        juniPppLinkStatusTerminateReason,
        juniPppLinkStatusTerminateNegFailOption,
        juniPppLinkStatusInKeepaliveRequests,
        juniPppLinkStatusOutKeepaliveRequests,
        juniPppLinkStatusInKeepaliveReplies,
        juniPppLinkStatusOutKeepaliveReplies,
        juniPppLinkStatusKeepaliveFailures,
        juniPppLinkStatusLocalMagicNumber,
        juniPppLinkStatusRemoteMagicNumber,
        juniPppLinkStatusLocalAuthentication,
        juniPppLinkStatusTunnelIfIndex,
        juniPppLinkConfigRowStatus,
        juniPppLinkConfigLowerIfIndex,
        juniPppLinkConfigKeepalive,
        juniPppLinkConfigAuthentication,
        juniPppLinkConfigMaxAuthenRetries,
        juniPppLinkConfigStandardIfIndex,
        juniPppLinkConfigChapMinChallengeLength,
        juniPppLinkConfigChapMaxChallengeLength,
        juniPppLinkConfigPassiveMode,
        juniPppLinkConfigAuthenticatorVirtualRouter,
        juniPppNextIfIndex }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of link-layer
        functionality (LCP) of PPP interfaces in a Juniper product.  This group
        became obsolete when additional objects were added."
    ::= { juniPppGroups 14 }                                       -- JUNOSe 4.0

juniPppIpGroup3  OBJECT-GROUP
    OBJECTS {
        juniPppIpServiceStatus,
        juniPppIpTerminateReason,
        juniPppIpTerminateNegFailOption,
        juniPppIpLocalIpAddress,
        juniPppIpRemoteIpAddress,
        juniPppIpRemotePrimaryDnsAddress,
        juniPppIpRemoteSecondaryDnsAddress,
        juniPppIpRemotePrimaryWinsAddress,
        juniPppIpRemoteSecondaryWinsAddress,
        juniPppIpConfigPeerDnsPriority,
        juniPppIpConfigPeerWinsPriority,
        juniPppIpConfigIpcpNetmask }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of IP network
        control protocol functionality (IPCP) of PPP interfaces in a Juniper
        product.  This group became obsolete when IPv6 support was added."
    ::= { juniPppGroups 15 }                                       -- JUNOSe 4.0

juniPppMlPppGroup2  OBJECT-GROUP
    OBJECTS {
        juniPppMlPppBundleRowStatus,
        juniPppMlPppBundleNetworkIfIndex,
        juniPppMlPppNextLinkIfIndex,
        juniPppMlPppLinkConfigLowerIfIndex,
        juniPppMlPppLinkConfigKeepalive,
        juniPppMlPppLinkConfigAuthentication,
        juniPppMlPppLinkConfigMaxAuthenRetries,
        juniPppMlPppLinkConfigRowStatus,
        juniPppMlPppNetworkConfigLowerIfIndex,
        juniPppMlPppNetworkBundleName,
        juniPppMlPppNetworkRowStatus,
        juniPppMlPppBindRowStatus }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing multi link PPP management
        support in a Juniper product.  This group became obsolete when
        additional objects were added."
    ::= { juniPppGroups 16 }                                       -- JUNOSe 4.0

juniPppMlPppGroup3  OBJECT-GROUP
    OBJECTS {
        juniPppMlPppBundleRowStatus,
        juniPppMlPppBundleNetworkIfIndex,
        juniPppMlPppNextLinkIfIndex,
        juniPppMlPppLinkConfigLowerIfIndex,
        juniPppMlPppLinkConfigKeepalive,
        juniPppMlPppLinkConfigAuthentication,
        juniPppMlPppLinkConfigMaxAuthenRetries,
        juniPppMlPppLinkConfigRowStatus,
        juniPppMlPppLinkConfigAaaProfile,
        juniPppMlPppNetworkConfigLowerIfIndex,
        juniPppMlPppNetworkBundleName,
        juniPppMlPppNetworkRowStatus,
        juniPppMlPppBindRowStatus }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing multi link PPP management
        support in a Juniper product.  This group became obsolete when
        additional objects were added."
    ::= { juniPppGroups 17 }                                       -- JUNOSe 4.1

juniPppLcpGroup5  OBJECT-GROUP
    OBJECTS {
        juniPppLinkStatusTerminateReason,
        juniPppLinkStatusTerminateNegFailOption,
        juniPppLinkStatusInKeepaliveRequests,
        juniPppLinkStatusOutKeepaliveRequests,
        juniPppLinkStatusInKeepaliveReplies,
        juniPppLinkStatusOutKeepaliveReplies,
        juniPppLinkStatusKeepaliveFailures,
        juniPppLinkStatusLocalMagicNumber,
        juniPppLinkStatusRemoteMagicNumber,
        juniPppLinkStatusLocalAuthentication,
        juniPppLinkStatusTunnelIfIndex,
        juniPppLinkConfigRowStatus,
        juniPppLinkConfigLowerIfIndex,
        juniPppLinkConfigKeepalive,
        juniPppLinkConfigAuthentication,
        juniPppLinkConfigMaxAuthenRetries,
        juniPppLinkConfigStandardIfIndex,
        juniPppLinkConfigChapMinChallengeLength,
        juniPppLinkConfigChapMaxChallengeLength,
        juniPppLinkConfigPassiveMode,
        juniPppLinkConfigAuthenticatorVirtualRouter,
        juniPppLinkConfigAaaProfile,
        juniPppNextIfIndex }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of link-layer
        functionality (LCP) of PPP interfaces in a Juniper product.  This group
        became obsolete when additional objects were added."
    ::= { juniPppGroups 18 }                                       -- JUNOSe 4.1

juniPppMlPppGroup4  OBJECT-GROUP
    OBJECTS {
        juniPppMlPppBundleRowStatus,
        juniPppMlPppBundleNetworkIfIndex,
        juniPppMlPppNextLinkIfIndex,
        juniPppMlPppLinkConfigLowerIfIndex,
        juniPppMlPppLinkConfigKeepalive,
        juniPppMlPppLinkConfigAuthentication,
        juniPppMlPppLinkConfigMaxAuthenRetries,
        juniPppMlPppLinkConfigRowStatus,
        juniPppMlPppLinkConfigChapMinChallengeLength,
        juniPppMlPppLinkConfigChapMaxChallengeLength,
        juniPppMlPppLinkConfigPassiveMode,
        juniPppMlPppLinkConfigAuthenticatorVirtualRouter,
        juniPppMlPppLinkConfigAaaProfile,
        juniPppMlPppNextNetworkIfIndex,
        juniPppMlPppNetworkConfigLowerIfIndex,
        juniPppMlPppNetworkBundleName,
        juniPppMlPppNetworkRowStatus,
        juniPppMlPppBindRowStatus }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing multi link PPP management
        support in a Juniper product.  This group became obsolete when
        additional objects were added."
    ::= { juniPppGroups 19 }                                       -- JUNOSe 5.0

juniPppSummaryBasicGroup2  OBJECT-GROUP
    OBJECTS {
        juniPppSummaryPppInterfaceCount,
        juniPppSummaryPppIpNCPs,
        juniPppSummaryPppOsiNCPs,
        juniPppSummaryPppIfAdminUp,
        juniPppSummaryPppIfAdminDown,
        juniPppSummaryPppIfOperUp,
        juniPppSummaryPppIfOperDown,
        juniPppSummaryPppIfOperDormant,
        juniPppSummaryPppIfNotPresent,
        juniPppSummaryPppIfLowerLayerDown,
        juniPppSummaryPppIfLastChangeTime,
        juniPppSummaryPppIpNcpOpened,
        juniPppSummaryPppIpNcpClosed,
        juniPppSummaryPppOsiNcpOpened,
        juniPppSummaryPppOsiNcpClosed,
        juniPppSummaryPppIpv6NCPs,
        juniPppSummaryPppIpv6NcpOpened,
        juniPppSummaryPppIpv6NcpClosed }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing PPP interface basic summary
        information in a Juniper product.  This group became obsolete when 
        new objects were added."
    ::= { juniPppGroups 20 }                                       -- JUNOSe 5.1

juniPppSummaryNetworkGroup2  OBJECT-GROUP
    OBJECTS {
        juniPppSummaryPppNetworkInterfaceCount,
        juniPppSummaryPppNetworkIpNCPs,
        juniPppSummaryPppNetworkOsiNCPs,
        juniPppSummaryPppNetworkIfAdminUp,
        juniPppSummaryPppNetworkIfAdminDown,
        juniPppSummaryPppNetworkIfOperUp,
        juniPppSummaryPppNetworkIfOperDown,
        juniPppSummaryPppNetworkIfOperDormant,
        juniPppSummaryPppNetworkIfNotPresent,
        juniPppSummaryPppNetworkIfLowerLayerDown,
        juniPppSummaryPppNetworkIfLastChangeTime,
        juniPppSummaryPppNetworkIpNcpOpened,
        juniPppSummaryPppNetworkIpNcpClosed,
        juniPppSummaryPppNetworkOsiNcpOpened,
        juniPppSummaryPppNetworkOsiNcpClosed,
        juniPppSummaryPppNetworkIpv6NCPs,
        juniPppSummaryPppNetworkIpv6NcpOpened,
        juniPppSummaryPppNetworkIpv6NcpClosed }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing PPP interface basic summary
        information in a Juniper product.  This group became obsolete when 
        new objects were added."
    ::= { juniPppGroups 21 }                                       -- JUNOSe 5.1

juniPppIpGroup4  OBJECT-GROUP
    OBJECTS {
        juniPppIpServiceStatus,
        juniPppIpTerminateReason,
        juniPppIpTerminateNegFailOption,
        juniPppIpLocalIpAddress,
        juniPppIpRemoteIpAddress,
        juniPppIpRemotePrimaryDnsAddress,
        juniPppIpRemoteSecondaryDnsAddress,
        juniPppIpRemotePrimaryWinsAddress,
        juniPppIpRemoteSecondaryWinsAddress,
        juniPppIpConfigPeerDnsPriority,
        juniPppIpConfigPeerWinsPriority,
        juniPppIpConfigIpcpNetmask,
        juniPppIpConfigInitiateIp }
    STATUS      obsolete
    DESCRIPTION
        "A collection of objects providing management of IP network control
        protocol functionality (IPCP) of PPP interfaces in a Juniper product.
        This group became obsolete when additional objects were added"
    ::= { juniPppGroups 22 }                                       -- JUNOSe 5.1

juniPppIpv6Group  OBJECT-GROUP
    OBJECTS {
        juniPppIpv6ServiceStatus,
        juniPppIpv6OperStatus,
        juniPppIpv6TerminateReason,
        juniPppIpv6TerminateNegFailOption,
        juniPppIpv6LocalIpv6AddressIfIdentifier,
        juniPppIpv6RemoteIpv6AddressIfIdentifier,
        juniPppIpv6ConfigAdminStatus,
        juniPppIpv6ConfigInitiateIpv6 }
    STATUS      obsolete 
    DESCRIPTION
        "A collection of objects providing management of IPV6 network control
        protocol functionality (IPV6CP) of PPP interfaces in a Juniper product.
        This group became obsolete when additional objects were added."
    ::= { juniPppGroups 23 }                                       -- JUNOSe 5.1

juniPppSessionGroup2  OBJECT-GROUP
    OBJECTS {
        juniPppSessionGrant,
        juniPppSessionTerminateReason,
        juniPppSessionStartTime,
        juniPppSessionInOctets,
        juniPppSessionOutOctets,
        juniPppSessionInPackets,
        juniPppSessionOutPackets,
        juniPppSessionSessionTimeout,
        juniPppSessionInactivityTimeout,
        juniPppSessionAccountingInterval,
        juniPppSessionRemoteIpAddress,
        juniPppSessionRemotePrimaryDnsAddress,
        juniPppSessionRemoteSecondaryDnsAddress,
        juniPppSessionRemotePrimaryWinsAddress,
        juniPppSessionRemoteSecondaryWinsAddress,
        juniPppSessionRemoteIpv6AddressIfIdentifier,
        juniPppSessionInhibitIp,
        juniPppSessionInhibitIpv6 }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing management of PPP session
        functionality of PPP interfaces in a Juniper product."
    ::= { juniPppGroups 24 }                                       -- JUNOSe 5.1

juniPppMlPppGroup5  OBJECT-GROUP
    OBJECTS {
        juniPppMlPppBundleRowStatus,
        juniPppMlPppBundleNetworkIfIndex,
        juniPppMlPppNextLinkIfIndex,
        juniPppMlPppLinkConfigLowerIfIndex,
        juniPppMlPppLinkConfigKeepalive,
        juniPppMlPppLinkConfigAuthentication,
        juniPppMlPppLinkConfigMaxAuthenRetries,
        juniPppMlPppLinkConfigRowStatus,
        juniPppMlPppLinkConfigChapMinChallengeLength,
        juniPppMlPppLinkConfigChapMaxChallengeLength,
        juniPppMlPppLinkConfigPassiveMode,
        juniPppMlPppLinkConfigAuthenticatorVirtualRouter,
        juniPppMlPppLinkConfigAaaProfile,
        juniPppMlPppLinkConfigFragmentation,
        juniPppMlPppLinkConfigReassembly,
        juniPppMlPppLinkConfigMaxReceiveReconstructedUnit,
        juniPppMlPppLinkConfigFragmentSize,
        juniPppMlPppNextNetworkIfIndex,
        juniPppMlPppNetworkConfigLowerIfIndex,
        juniPppMlPppNetworkBundleName,
        juniPppMlPppNetworkRowStatus,
        juniPppMlPppBindRowStatus }
    STATUS      obsolete
    DESCRIPTION
	"Obsolete collection of objects providing multi link PPP management
        support in a Juniper product.  This group became obsolete when
        additional objects were added."
    ::= { juniPppGroups 25 }                                       -- JUNOSe 5.3

juniPppSummaryBasicGroup3  OBJECT-GROUP
    OBJECTS {
        juniPppSummaryPppInterfaceCount,
        juniPppSummaryPppStaticInterfaceCount,
        juniPppSummaryPppIpNCPs,
        juniPppSummaryPppIpv6NCPs,
        juniPppSummaryPppOsiNCPs,
        juniPppSummaryPppMplsNCPs,
        juniPppSummaryPppIfAdminUp,
        juniPppSummaryPppIfAdminDown,
        juniPppSummaryPppIpAdminOpen,
        juniPppSummaryPppIpAdminClose,
        juniPppSummaryPppIpv6AdminOpen,
        juniPppSummaryPppIpv6AdminClose,
        juniPppSummaryPppOsiAdminOpen,
        juniPppSummaryPppOsiAdminClose,
        juniPppSummaryPppMplsAdminOpen,
        juniPppSummaryPppMplsAdminClose,
        juniPppSummaryPppIfOperUp,
        juniPppSummaryPppIfOperDown,
        juniPppSummaryPppIfOperDormant,
        juniPppSummaryPppIfNotPresent,
        juniPppSummaryPppIfLowerLayerDown,
        juniPppSummaryPppIpNcpOpened,
        juniPppSummaryPppIpNcpClosed,
        juniPppSummaryPppIpNcpNotPresent,
        juniPppSummaryPppIpNcpNoResources,
        juniPppSummaryPppIpv6NcpOpened,
        juniPppSummaryPppIpv6NcpClosed,
        juniPppSummaryPppIpv6NcpNotPresent,
        juniPppSummaryPppIpv6NcpNoResources,
        juniPppSummaryPppOsiNcpOpened,
        juniPppSummaryPppOsiNcpClosed,
        juniPppSummaryPppOsiNcpNotPresent,
        juniPppSummaryPppOsiNcpNoResources,
        juniPppSummaryPppMplsNcpOpened,
        juniPppSummaryPppMplsNcpClosed,
        juniPppSummaryPppMplsNcpNotPresent,
        juniPppSummaryPppMplsNcpNoResources,
        juniPppSummaryPppIfLastChangeTime }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing PPP interface basic summary
        information in a Juniper product."
    ::= { juniPppGroups 26 }                                       -- JUNOSe 6.0

juniPppSummaryLinkGroup2 OBJECT-GROUP
    OBJECTS {
        juniPppSummaryPppLinkInterfaceCount,
        juniPppSummaryPppLinkStaticInterfaceCount,
        juniPppSummaryPppLinkIfAdminUp,
        juniPppSummaryPppLinkIfAdminDown,
        juniPppSummaryPppLinkIfOperUp,
        juniPppSummaryPppLinkIfOperDown,
        juniPppSummaryPppLinkIfOperDormant,
        juniPppSummaryPppLinkIfNotPresent,
        juniPppSummaryPppLinkIfLowerLayerDown,
        juniPppSummaryPppLinkIfLastChangeTime }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing PPP interface link summary
        information in a Juniper product."
    ::= { juniPppGroups 27 }                                       -- JUNOSe 6.0

juniPppSummaryNetworkGroup3  OBJECT-GROUP
    OBJECTS {
        juniPppSummaryPppNetworkInterfaceCount,
        juniPppSummaryPppNetworkStaticInterfaceCount,
        juniPppSummaryPppNetworkIpNCPs,
        juniPppSummaryPppNetworkIpv6NCPs,
        juniPppSummaryPppNetworkOsiNCPs,
        juniPppSummaryPppNetworkMplsNCPs,
        juniPppSummaryPppNetworkIfAdminUp,
        juniPppSummaryPppNetworkIfAdminDown,
        juniPppSummaryPppNetworkIpAdminOpen,
        juniPppSummaryPppNetworkIpAdminClose,
        juniPppSummaryPppNetworkIpv6AdminOpen,
        juniPppSummaryPppNetworkIpv6AdminClose,
        juniPppSummaryPppNetworkOsiAdminOpen,
        juniPppSummaryPppNetworkOsiAdminClose,
        juniPppSummaryPppNetworkMplsAdminOpen,
        juniPppSummaryPppNetworkMplsAdminClose,
        juniPppSummaryPppNetworkIfOperUp,
        juniPppSummaryPppNetworkIfOperDown,
        juniPppSummaryPppNetworkIfOperDormant,
        juniPppSummaryPppNetworkIfNotPresent,
        juniPppSummaryPppNetworkIfLowerLayerDown,
        juniPppSummaryPppNetworkIpNcpOpened,
        juniPppSummaryPppNetworkIpNcpClosed,
        juniPppSummaryPppNetworkIpNcpNotPresent,
        juniPppSummaryPppNetworkIpNcpNoResources,
        juniPppSummaryPppNetworkIpv6NcpOpened,
        juniPppSummaryPppNetworkIpv6NcpClosed,
        juniPppSummaryPppNetworkIpv6NcpNotPresent,
        juniPppSummaryPppNetworkIpv6NcpNoResources,
        juniPppSummaryPppNetworkOsiNcpOpened,
        juniPppSummaryPppNetworkOsiNcpClosed,
        juniPppSummaryPppNetworkOsiNcpNotPresent,
        juniPppSummaryPppNetworkOsiNcpNoResources,
        juniPppSummaryPppNetworkMplsNcpOpened,
        juniPppSummaryPppNetworkMplsNcpClosed,
        juniPppSummaryPppNetworkMplsNcpNotPresent,
        juniPppSummaryPppNetworkMplsNcpNoResources,
        juniPppSummaryPppNetworkIfLastChangeTime }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing PPP interface network summary
        information in a Juniper product."
    ::= { juniPppGroups 28 }                                       -- JUNOSe 6.0

juniPppMlPppGroup6  OBJECT-GROUP
    OBJECTS {
        juniPppMlPppBundleRowStatus,
        juniPppMlPppBundleNetworkIfIndex,
        juniPppMlPppNextLinkIfIndex,
        juniPppMlPppLinkConfigLowerIfIndex,
        juniPppMlPppLinkConfigKeepalive,
        juniPppMlPppLinkConfigAuthentication,
        juniPppMlPppLinkConfigMaxAuthenRetries,
        juniPppMlPppLinkConfigRowStatus,
        juniPppMlPppLinkConfigChapMinChallengeLength,
        juniPppMlPppLinkConfigChapMaxChallengeLength,
        juniPppMlPppLinkConfigPassiveMode,
        juniPppMlPppLinkConfigAuthenticatorVirtualRouter,
        juniPppMlPppLinkConfigAaaProfile,
        juniPppMlPppLinkConfigFragmentation,
        juniPppMlPppLinkConfigReassembly,
        juniPppMlPppLinkConfigMaxReceiveReconstructedUnit,
        juniPppMlPppLinkConfigFragmentSize,
	juniPppMlPppLinkConfigHashLinkSelection,
        juniPppMlPppNextNetworkIfIndex,
        juniPppMlPppNetworkConfigLowerIfIndex,
        juniPppMlPppNetworkBundleName,
        juniPppMlPppNetworkRowStatus,
        juniPppMlPppBindRowStatus }
    STATUS      obsolete
    DESCRIPTION
	"Obsolete collection of objects providing multi link PPP management
        support in a Juniper product.  This group became obsolete when
        additional objects were added."
    ::= { juniPppGroups 29 }                                       -- JUNOSe 7.2

juniPppLcpGroup6  OBJECT-GROUP
    OBJECTS {
        juniPppLinkStatusTerminateReason,
        juniPppLinkStatusTerminateNegFailOption,
        juniPppLinkStatusInKeepaliveRequests,
        juniPppLinkStatusOutKeepaliveRequests,
        juniPppLinkStatusInKeepaliveReplies,
        juniPppLinkStatusOutKeepaliveReplies,
        juniPppLinkStatusKeepaliveFailures,
        juniPppLinkStatusLocalMagicNumber,
        juniPppLinkStatusRemoteMagicNumber,
        juniPppLinkStatusLocalAuthentication,
        juniPppLinkStatusTunnelIfIndex,
        juniPppLinkConfigRowStatus,
        juniPppLinkConfigLowerIfIndex,
        juniPppLinkConfigKeepalive,
        juniPppLinkConfigAuthentication,
        juniPppLinkConfigMaxAuthenRetries,
        juniPppLinkConfigStandardIfIndex,
        juniPppLinkConfigChapMinChallengeLength,
        juniPppLinkConfigChapMaxChallengeLength,
        juniPppLinkConfigPassiveMode,
        juniPppLinkConfigAuthenticatorVirtualRouter,
        juniPppLinkConfigAaaProfile,
        juniPppLinkConfigAuthentication2,
        juniPppNextIfIndex }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing management of link-layer
        functionality (LCP) of PPP interfaces in a Juniper product. This group
        became obsolete when additional objects were added."
    ::= { juniPppGroups 30 }                                       -- JUNOSe 7.3

juniPppMlPppGroup7  OBJECT-GROUP
    OBJECTS {
        juniPppMlPppBundleRowStatus,
        juniPppMlPppBundleNetworkIfIndex,
        juniPppMlPppNextLinkIfIndex,
        juniPppMlPppLinkConfigLowerIfIndex,
        juniPppMlPppLinkConfigKeepalive,
        juniPppMlPppLinkConfigAuthentication,
        juniPppMlPppLinkConfigMaxAuthenRetries,
        juniPppMlPppLinkConfigRowStatus,
        juniPppMlPppLinkConfigChapMinChallengeLength,
        juniPppMlPppLinkConfigChapMaxChallengeLength,
        juniPppMlPppLinkConfigPassiveMode,
        juniPppMlPppLinkConfigAuthenticatorVirtualRouter,
        juniPppMlPppLinkConfigAaaProfile,
        juniPppMlPppLinkConfigFragmentation,
        juniPppMlPppLinkConfigReassembly,
        juniPppMlPppLinkConfigMaxReceiveReconstructedUnit,
        juniPppMlPppLinkConfigFragmentSize,
        juniPppMlPppLinkConfigHashLinkSelection,
        juniPppMlPppLinkConfigAuthentication2,
        juniPppMlPppNextNetworkIfIndex,
        juniPppMlPppNetworkConfigLowerIfIndex,
        juniPppMlPppNetworkBundleName,
        juniPppMlPppNetworkRowStatus }
    STATUS      obsolete
    DESCRIPTION
        "Obsolete collection of objects providing multi link PPP management support in
        a Juniper product. This group became obsolete when additional objects were added"
    ::= { juniPppGroups 31 }                                       -- JUNOSe 7.3
    
juniPppLcpGroup7  OBJECT-GROUP
    OBJECTS {
        juniPppLinkStatusTerminateReason,
        juniPppLinkStatusTerminateNegFailOption,
        juniPppLinkStatusInKeepaliveRequests,
        juniPppLinkStatusOutKeepaliveRequests,
        juniPppLinkStatusInKeepaliveReplies,
        juniPppLinkStatusOutKeepaliveReplies,
        juniPppLinkStatusKeepaliveFailures,
        juniPppLinkStatusLocalMagicNumber,
        juniPppLinkStatusRemoteMagicNumber,
        juniPppLinkStatusLocalAuthentication,
        juniPppLinkStatusTunnelIfIndex,
        juniPppLinkConfigRowStatus,
        juniPppLinkConfigLowerIfIndex,
        juniPppLinkConfigKeepalive,
        juniPppLinkConfigAuthentication,
        juniPppLinkConfigMaxAuthenRetries,
        juniPppLinkConfigStandardIfIndex,
        juniPppLinkConfigChapMinChallengeLength,
        juniPppLinkConfigChapMaxChallengeLength,
        juniPppLinkConfigPassiveMode,
        juniPppLinkConfigAuthenticatorVirtualRouter,
        juniPppLinkConfigAaaProfile,
        juniPppLinkConfigAuthentication2,
        juniPppLinkConfigIgnoreMagicNumberMismatch,
        juniPppNextIfIndex }
    STATUS      obsolete
    DESCRIPTION
        "A collection of objects providing management of link-layer
        functionality (LCP) of PPP interfaces in a Juniper product. This group
        became obsolete when additional objects were added."
    ::= { juniPppGroups 32 }                                       -- JUNOSe 7.3

juniPppMlPppGroup8  OBJECT-GROUP
    OBJECTS {
        juniPppMlPppBundleRowStatus,
        juniPppMlPppBundleNetworkIfIndex,
        juniPppMlPppNextLinkIfIndex,
        juniPppMlPppLinkConfigLowerIfIndex,
        juniPppMlPppLinkConfigKeepalive,
        juniPppMlPppLinkConfigAuthentication,
        juniPppMlPppLinkConfigMaxAuthenRetries,
        juniPppMlPppLinkConfigRowStatus,
        juniPppMlPppLinkConfigChapMinChallengeLength,
        juniPppMlPppLinkConfigChapMaxChallengeLength,
        juniPppMlPppLinkConfigPassiveMode,
        juniPppMlPppLinkConfigAuthenticatorVirtualRouter,
        juniPppMlPppLinkConfigAaaProfile,
        juniPppMlPppLinkConfigFragmentation,
        juniPppMlPppLinkConfigReassembly,
        juniPppMlPppLinkConfigMaxReceiveReconstructedUnit,
        juniPppMlPppLinkConfigFragmentSize,
        juniPppMlPppLinkConfigHashLinkSelection,
        juniPppMlPppLinkConfigAuthentication2,
        juniPppMlPppLinkConfigIgnoreMagicNumberMismatch,
        juniPppMlPppNextNetworkIfIndex,
        juniPppMlPppNetworkConfigLowerIfIndex,
        juniPppMlPppNetworkBundleName,
        juniPppMlPppNetworkRowStatus,
        juniPppMlPppBindRowStatus }
    STATUS      obsolete
    DESCRIPTION
        "A collection of objects providing multi link PPP management support in
        a Juniper product. This was obsoleted when multiclass multilink support
		was added."
    ::= { juniPppGroups 33 }                                       -- JUNOSe 7.3

juniPppLcpGroup8  OBJECT-GROUP
    OBJECTS {
        juniPppLinkStatusTerminateReason,
        juniPppLinkStatusTerminateNegFailOption,
        juniPppLinkStatusInKeepaliveRequests,
        juniPppLinkStatusOutKeepaliveRequests,
        juniPppLinkStatusInKeepaliveReplies,
        juniPppLinkStatusOutKeepaliveReplies,
        juniPppLinkStatusKeepaliveFailures,
        juniPppLinkStatusLocalMagicNumber,
        juniPppLinkStatusRemoteMagicNumber,
        juniPppLinkStatusLocalAuthentication,
        juniPppLinkStatusTunnelIfIndex,
        juniPppLinkStatuslcpRenegoTerminates,
        juniPppLinkConfigRowStatus,
        juniPppLinkConfigLowerIfIndex,
        juniPppLinkConfigKeepalive,
        juniPppLinkConfigAuthentication,
        juniPppLinkConfigMaxAuthenRetries,
        juniPppLinkConfigStandardIfIndex,
        juniPppLinkConfigChapMinChallengeLength,
        juniPppLinkConfigChapMaxChallengeLength,
        juniPppLinkConfigPassiveMode,
        juniPppLinkConfigAuthenticatorVirtualRouter,
        juniPppLinkConfigAaaProfile,
        juniPppLinkConfigAuthentication2,
        juniPppLinkConfigIgnoreMagicNumberMismatch,
        juniPppLinkConfigMaxLcpRenegotiation,
        juniPppNextIfIndex }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing management of link-layer
		functionality (LCP) of PPP interfaces in a Juniper product."
    ::= { juniPppGroups 34 }                                       -- JUNOSe 10.1

juniPppIpGroup5  OBJECT-GROUP
    OBJECTS {
        juniPppIpServiceStatus,
        juniPppIpTerminateReason,
        juniPppIpTerminateNegFailOption,
        juniPppIpLocalIpAddress,
        juniPppIpRemoteIpAddress,
        juniPppIpRemotePrimaryDnsAddress,
        juniPppIpRemoteSecondaryDnsAddress,
        juniPppIpRemotePrimaryWinsAddress,
        juniPppIpRemoteSecondaryWinsAddress,
        juniPppIpNetworkStatusIpcpRenegoTerminates,
        juniPppIpConfigPeerDnsPriority,
        juniPppIpConfigPeerWinsPriority,
        juniPppIpConfigIpcpNetmask,
        juniPppIpConfigInitiateIp,
        juniPppIpConfigMaxIpcpRenegotiation }
    STATUS      obsolete
    DESCRIPTION
        "A collection of objects providing management of IP network 
         control protocol functionality (IPCP) of PPP interfaces in a Juniper 
         product.This group became obsolete when additional objects were added."
    ::= { juniPppGroups 35 }                                       -- JUNOSe 10.1

juniPppIpv6Group2  OBJECT-GROUP
    OBJECTS {
        juniPppIpv6ServiceStatus,
        juniPppIpv6OperStatus,
        juniPppIpv6TerminateReason,
        juniPppIpv6TerminateNegFailOption,
        juniPppIpv6LocalIpv6AddressIfIdentifier,
        juniPppIpv6RemoteIpv6AddressIfIdentifier,
        juniPppIpv6NetworkStatusIpv6cpRenegoTerminates,
        juniPppIpv6ConfigAdminStatus,
        juniPppIpv6ConfigInitiateIpv6,
        juniPppIpv6ConfigMaxIpv6cpRenegotiation }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing management of IPV6 network control
        protocol functionality (IPV6CP) of PPP interfaces in a Juniper product."
    ::= { juniPppGroups 36 }                                       -- JUNOSe 10.1

juniPppIpGroup6  OBJECT-GROUP
    OBJECTS {
        juniPppIpServiceStatus,
        juniPppIpTerminateReason,
        juniPppIpTerminateNegFailOption,
        juniPppIpLocalIpAddress,
        juniPppIpRemoteIpAddress,
        juniPppIpRemotePrimaryDnsAddress,
        juniPppIpRemoteSecondaryDnsAddress,
        juniPppIpRemotePrimaryWinsAddress,
        juniPppIpRemoteSecondaryWinsAddress,
        juniPppIpNetworkStatusIpcpRenegoTerminates,
        juniPppIpConfigPeerDnsPriority,
        juniPppIpConfigPeerWinsPriority,
        juniPppIpConfigIpcpNetmask,
        juniPppIpConfigInitiateIp,
        juniPppIpConfigMaxIpcpRenegotiation,
        juniPppIpConfigPromptIpcpDnsOption,
        juniPppIpConfigIpcpLockout }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing management of IP network control
        protocol functionality (IPCP) of PPP interfaces in a Juniper product."
    ::= { juniPppGroups 37 }                                        --JUNOSe 11.0

juniPppMlPppGroup9  OBJECT-GROUP
    OBJECTS {
        juniPppMlPppBundleRowStatus,
        juniPppMlPppBundleNetworkIfIndex,
        juniPppMlPppNextLinkIfIndex,
        juniPppMlPppLinkConfigLowerIfIndex,
        juniPppMlPppLinkConfigKeepalive,
        juniPppMlPppLinkConfigAuthentication,
        juniPppMlPppLinkConfigMaxAuthenRetries,
        juniPppMlPppLinkConfigRowStatus,
        juniPppMlPppLinkConfigChapMinChallengeLength,
        juniPppMlPppLinkConfigChapMaxChallengeLength,
        juniPppMlPppLinkConfigPassiveMode,
        juniPppMlPppLinkConfigAuthenticatorVirtualRouter,
        juniPppMlPppLinkConfigAaaProfile,
        juniPppMlPppLinkConfigFragmentation,
        juniPppMlPppLinkConfigReassembly,
        juniPppMlPppLinkConfigMaxReceiveReconstructedUnit,
        juniPppMlPppLinkConfigFragmentSize,
        juniPppMlPppLinkConfigHashLinkSelection,
        juniPppMlPppLinkConfigAuthentication2,
        juniPppMlPppLinkConfigIgnoreMagicNumberMismatch,
        juniPppMlPppNextNetworkIfIndex,
        juniPppMlPppNetworkConfigLowerIfIndex,
        juniPppMlPppNetworkBundleName,
        juniPppMlPppNetworkRowStatus,
        juniPppMlPppBindRowStatus,
		juniPppMlPppLinkConfigMultilinkMulticlass,
    	juniPppMlPppLinkConfigMultilinkMaxMultiClasses }
    STATUS      current
    DESCRIPTION
        "A collection of objects providing multi link PPP management support in
        a Juniper product."
    ::= { juniPppGroups 38 }                                       -- JUNOSe 11.1
    
juniPppMlPppMulticlassTcGroup1  OBJECT-GROUP
	OBJECTS {
	  	juniPppMlPppMulticlassTcName,
    	juniPppMlPppMulticlassFragmentation,
    	juniPppMlPppMulticlassReassembly  }
    STATUS		current
    DESCRIPTION
    	" A collection of object providing management of MCMP traffic class
		mapping functionality of PPP link interfaces in a Juniper product."
	::= { juniPppGroups 39 }										-- JUNOSe 11.1

END

