ATM-FORUM-M4-MIB DEFINITIONS ::= BEGIN

IMPORTS
          MODULE-IDENTITY, OBJECT-TYPE,
          NOTIFICATION-TYPE, OBJECT-IDENTITY,
          Counter32, Integer32, IpAddress,
          Unsigned32                                                             FROM SNMPv2-SMI
          TEXTUAL-CONVENTION, DisplayString,
          AutonomousType, RowStatus, TestAndIncr,
          RowPointer, TruthValue, TimeStamp,
          DateAndTime, TimeInterval                      FROM SNMPv2-TC
          MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP           FROM SNMPv2-CONF
          ifIndex, OwnerString                                   FROM IF-MIB
          atmForum                                                                       FROM ATM-FORUM-TC-MIB
          atmVplEntry, atmVclEntry, atmVpCrossConnectEntry,
          atmVcCrossConnectEntry, atmVplVpi,
          atmVclVpi, atmVclVci,
          atmVpCrossConnectIndex, atmVpCrossConnectLowIfIndex,
          atmVpCrossConnectLowVpi, atmVpCrossConnectHighIfIndex,
          atmVpCrossConnectHighVpi, atmVcCrossConnectIndex,
          atmVcCrossConnectLowIfIndex, atmVcCrossConnectLowVpi,
          atmVcCrossConnectLowVci, atmVcCrossConnectHighIfIndex,
          atmVcCrossConnectHighVpi, atmVcCrossConnectHighVci
                                                                                                         FROM ATM-MIB
          entPhysicalIndex, entPhysicalClass, entPhysicalContainedIn,
          entPhysicalParentRelPos
                                                                                                         FROM ENTITY-MIB
          hrSWInstalledIndex,
          hrSWInstalledName                                              FROM HOST-RESOURCES-MIB;


atmfM4MIB MODULE-IDENTITY
          LAST-UPDATED    "9701210000Z"
          ORGANIZATION    "ATM Forum"
          CONTACT-INFO
                        "          Andrew G. Malis
          Postal:   Ascend Communications, Inc.
                    5 Carlisle Road
                    Westford MA  01886
                    USA
          Tel:      +1 508 952 7414
          Fax:      +1 508 392 9250
          E-Mail:   malis@ascend.com"
         DESCRIPTION
                         "This MIB module is the SNMP version of the ATM Forum's
          M4 interface (network element view)."
         ::= { atmForum 100 }

atmfM4MIBObjects          OBJECT IDENTIFIER ::= { atmfM4MIB 1 }
atmfM4MIBTraps            OBJECT IDENTIFIER ::= { atmfM4MIB 2 }
atmfM4MIBCompliance OBJECT IDENTIFIER ::= { atmfM4MIB 3 }


--        This MIB module consists of the following groups:
--                       (1)     ATM NE High-Level Objects
--                       (2)     Interfaces: Physical Path Termination Point Table
--                       (3)     TC Adaptor Table
--                       (4)     ATM Cell Layer Interface Table
--                       (5)     VPL Termination Point Table Extensions
--                       (6)     VCL Termination Point Table Extensions
--                       (7)     VP Cross-Connect Table Extensions
--                       (8)     VC Cross-Connect Table Extensions
--                       (9)     VP 'next VPI' Table
--                       (10)    VC 'next VCI' Table
--                       (11)    ATM Cell Protocol Monitoring Current Data Table
--                       (12)    ATM Cell Protocol Monitoring History Data Table
--                       (13)    ATM Cell Protocol Monitoring Error Log Table
--                       (14)    TC Adaptor Protocol Monitoring Current Data Table
--                       (15)    TC Adaptor Protocol Monitoring History Data Table
--                       (16)    VPL UPC/NPC Disagreement Monitoring Current Data Table
--                       (17)    VPL UPC/NPC Disagreement Monitoring History Data Table
--                       (18)    VCL UPC/NPC Disagreement Monitoring Current Data Table
--                       (19)    VCL UPC/NPC Disagreement Monitoring History Data Table
--                       (20)    OAM Loopback Test Definitions
--                       (21)    VPL/VPC Termination Point Test Table
--                       (22)    VCL/VCC Termination Point Test Table
--                       (23)    Equipment Table extension
--                       (24)    Equipment Holder Table extension
--                       (25)    Plug-In Unit Table extension
--                       (26)    Hardware Unit/Running Software Relationship Table
--                       (27)    Hardware Unit/Installed Software Relationship Table
--                       (28)    Alarm Forwarding Discriminator Table
--                       (29)    Trap Log Table
--                       (30)    Trap Log Entry Table
--                       (31)    Alarm Trap Log Entry Table extension
--                       (32)    Notifications (traps)
--                       (33)    Conformance statements


-- ATM Forum M4 ATM network element (NE) high-level objects

atmfM4NeVendor OBJECT-TYPE
          SYNTAX                DisplayString
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "The vendor of the ATM network element."
          ::= { atmfM4MIBObjects 1 }

atmfM4NeVersion OBJECT-TYPE
          SYNTAX                AutonomousType
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "The version of the ATM network element."
          ::= { atmfM4MIBObjects 2 }

atmfM4NeStartTime OBJECT-TYPE
          SYNTAX                DateAndTime
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "The time at which the agent was last started; in other
          words, the time at which sysUpTime was zero."
          ::= { atmfM4MIBObjects 3 }

atmfM4NeAlarmSeverityIndex OBJECT-TYPE
          SYNTAX                Integer32
          MAX-ACCESS      read-write
          STATUS                current
          DESCRIPTION
                         "An index into the alarm severity profile table, specifying
          the severity assignments for M4 alarms reported for the
          ATM network element."
          DEFVAL                { 0 }
          ::= { atmfM4MIBObjects 4 }

atmfM4NeSuppressZeroStats OBJECT-TYPE
          SYNTAX                TruthValue
          MAX-ACCESS      read-write
          STATUS                current
          DESCRIPTION
                         "When the value of this object is true, no entry will be
          created in any of the the historical statistics tables for
          intervals in which all counts are zero."
          DEFVAL                { true }
          ::= { atmfM4MIBObjects 5 }


-- ATM Forum M4 Interface Configuration Table Extensions
-- Physical Path Termination Point Layer

atmfM4PhysPathTpTable OBJECT-TYPE
          SYNTAX                SEQUENCE OF             AtmfM4PhysPathTpEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "The ATM Forum M4 interface Configuration table extensions
          for the physical path termination point."
          ::= { atmfM4MIBObjects 6 }

atmfM4PhysPathTpEntry OBJECT-TYPE
          SYNTAX                AtmfM4PhysPathTpEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "Columns conceptually added to the interface table
          entry for an ATM interface to model the physical path
          termination point.

          The row of the interface table modeling this object should
          also include columns for the TC Adaptor object and the ATM
          interface table defined in RFC 1695.

          The interface table entry for the physical path TP
          fields of an ATM interface are set up without management
          system control (or else that setup is outside the
          scope of M4)."
          INDEX                   { ifIndex }
          ::= { atmfM4PhysPathTpTable 1 }

AtmfM4PhysPathTpEntry ::= SEQUENCE {
          atmfM4PhysPathTpHwUnitIndex                     Integer32,
          atmfM4PhysPathTpPortID                                  Integer32,
          atmfM4PhysPathTpAlarmSeverityIndex  Integer32
                         }

atmfM4PhysPathTpHwUnitIndex OBJECT-TYPE
          SYNTAX                Integer32 (1..2147483647)
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "Specifies the index of the entry in the entPhysicalTable
          that represents the device (i.e., card) on which the
          physical path terminates."
          ::= { atmfM4PhysPathTpEntry 1 }

atmfM4PhysPathTpPortID OBJECT-TYPE
          SYNTAX                Integer32 (1..2147483647)
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "Identifies the port (within the card identified by the
          hardware unit index) on which the physical path terminates."
          ::= { atmfM4PhysPathTpEntry 2 }

atmfM4PhysPathTpAlarmSeverityIndex OBJECT-TYPE
          SYNTAX                Integer32
          MAX-ACCESS      read-write
          STATUS                current
          DESCRIPTION
                         "Specifies the index of the entry in the communications
          alarm severity profile table that should be used."
          DEFVAL                { 0 }
          ::= { atmfM4PhysPathTpEntry 3 }


-- ATM Forum M4 Interface Configuration Table Extensions
-- TC Adaptor Layer

atmfM4TcAdaptorTable OBJECT-TYPE
          SYNTAX                SEQUENCE OF             AtmfM4TcAdaptorEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "The ATM Forum M4 interface Configuration table extensions
          for the TC Adaptor."
          ::= { atmfM4MIBObjects 7 }

atmfM4TcAdaptorEntry OBJECT-TYPE
          SYNTAX                AtmfM4TcAdaptorEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "Columns conceptually added to the interface table
          entry for an ATM interface to model the TC Adaptor.

          The row of the interface table modeling this object should
          also include columns for the physical path TP and the ATM
          interface table defined in RFC 1695.

          The interface table entry for the TC Adaptor
          fields of an ATM interface are set up without management
          system control (or else that setup is outside the
          scope of M4)."
          INDEX                   { ifIndex }
          ::= { atmfM4TcAdaptorTable 1 }

AtmfM4TcAdaptorEntry ::= SEQUENCE {
          atmfM4TcACellScrambling                 TruthValue,
          atmfM4TcAlarmSeverityIndex      Integer32
                         }

atmfM4TcACellScrambling OBJECT-TYPE
          SYNTAX                TruthValue
          MAX-ACCESS      read-write
          STATUS                current
          DESCRIPTION
                         "This attribute is used by the management system to
          activate and deactivate the ATM cell scrambling function.
          When the value of this attribute is TRUE, cell scrambling
          on the interface is activated.

          This attribute shall be present only for interfaces that
          support the deactivation of cell scrambling.  The ATM Forum
          UNI specification requires cell scrambling for ATM/SONET
          interfaces but allows cell scrambling to be controlled
          (i.e., turned on and off) for ATM/DS3 interfaces."
          DEFVAL                { true }
          ::= { atmfM4TcAdaptorEntry 1 }

atmfM4TcAlarmSeverityIndex OBJECT-TYPE
          SYNTAX                Integer32
          MAX-ACCESS      read-write
          STATUS                current
          DESCRIPTION
                         "Specifies the index of the entry in the communications
          alarm severity profile table that should be used."
          DEFVAL                { 0 }
          ::= { atmfM4TcAdaptorEntry 2 }


-- ATM Forum M4 Interface Configuration Table Extensions
-- ATM Cell Layer

atmfM4AtmLayerTable OBJECT-TYPE
          SYNTAX                SEQUENCE OF             AtmfM4AtmLayerEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "The ATM Forum M4 interface Configuration table extensions
          for the ATM cell layer."
          ::= { atmfM4MIBObjects 8 }

atmfM4AtmLayerEntry OBJECT-TYPE
          SYNTAX                AtmfM4AtmLayerEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "Columns conceptually added to the interface table
          entry for an ATM interface to model the ATM cell layer.
          The row of the interface table modeling this object should
          also include columns for the physical path TP and TC Adaptor
          object, as well as the ATM interface table defined in
          RFC 1695.

          The default configuration of an entry in this table is
          used whenever the entries for the physical path TP, etc.,
          are created.  The management system configures a UNI,
          B-ICI, or B-ISSI on the interface by first modifying the
          atmfM4IfType column (this can be done in the same SNMP
          set-request that sets up the other necessary variables."
          INDEX                   { ifIndex }
          ::= { atmfM4AtmLayerTable 1 }

AtmfM4AtmLayerEntry ::= SEQUENCE {
          atmfM4IfType                                            INTEGER,
          atmfM4IfLoopbackLocationCode  Integer32,
          atmfM4IfSubscriberAddress       DisplayString,
          atmfM4IfPreferredCarrier                DisplayString,
          atmfM4IfFarEndCarrierNetwork  DisplayString
                         }

atmfM4IfType OBJECT-TYPE
          SYNTAX                INTEGER {
                                                  none(0),
                                                  uni(1),
                                                  bici(2),
                                                  bissi(3)
                                                                 }
          MAX-ACCESS      read-write
          STATUS                current
          DESCRIPTION
                         "Specifies the type of ATM cell-layer interface defined
          on the physical path termination point modeled by this
          entry in the interface table."
          DEFVAL                { none }
          ::= { atmfM4AtmLayerEntry 1 }

atmfM4IfLoopbackLocationCode OBJECT-TYPE
          SYNTAX                Integer32
          MAX-ACCESS      read-write
          STATUS                current
          DESCRIPTION
                         "Specifies the code that shall exist in incoming OAM
          Loopback cells that are to be looped back at this
          interface.

          A value of zero shall indicate that the management system
          has not set any loopback location code for this interface.
          Therefore, zero should not be used as the actual loopback
          location code for any interface.

          This object shall be present only for table entries that
          represent an actual ATM cell layer interface (i.e., the
          atmM4IfType is not none(0))."
          DEFVAL                { 0 }
          ::= { atmfM4AtmLayerEntry 2 }

atmfM4IfSubscriberAddress OBJECT-TYPE
          SYNTAX                DisplayString
          MAX-ACCESS      read-write
          STATUS                current
          DESCRIPTION
                         "Specifies the address or newline-delimited list of
          addresses assigned to the UNI.

          This object shall be present only for table entries that
          represent an UNI interface."
          DEFVAL                { "" }
          ::= { atmfM4AtmLayerEntry 3 }

atmfM4IfPreferredCarrier OBJECT-TYPE
          SYNTAX                DisplayString
          MAX-ACCESS      read-write
          STATUS                current
          DESCRIPTION
                         "Specifies the name of the default carrier to use when one
          is not explicitly identified in the call set-up message.

          This object shall be present only for table entries that
          represent an UNI interface and only when SVC services are
          supported."
          DEFVAL                { "" }
          ::= { atmfM4AtmLayerEntry 4 }

atmfM4IfFarEndCarrierNetwork OBJECT-TYPE
          SYNTAX                DisplayString
          MAX-ACCESS      read-write
          STATUS                current
          DESCRIPTION
                         "Specifies the adjacent carrier to which the B-ICI
          transmission path is connected.

          This object shall be present only for table entries that
          represent an B-ICI interface and only when SVC services are
          supported."
          DEFVAL                { "" }
          ::= { atmfM4AtmLayerEntry 5 }




-- ATM Forum M4 VPL Termination Point Configuration Table Extensions

atmfM4VplTable OBJECT-TYPE
          SYNTAX                SEQUENCE OF             AtmfM4VplEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "The ATM Forum M4 VPL Termination Point Configuration
          table extensions.  This table augments the VPL
          configuration table in RFC 1695."
          ::= { atmfM4MIBObjects 9 }

atmfM4VplEntry OBJECT-TYPE
          SYNTAX                AtmfM4VplEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "Additional columns for the VPL configuration table entry."
          AUGMENTS { atmVplEntry }
          ::= { atmfM4VplTable 1 }

AtmfM4VplEntry ::= SEQUENCE {
          atmfM4VplSegEndPt                     TruthValue
                         }

atmfM4VplSegEndPt OBJECT-TYPE
          SYNTAX                TruthValue
          MAX-ACCESS      read-create
          STATUS                current
          DESCRIPTION
                         "Specifies whether the VPL termination point is a segment
          end-point."
          ::= { atmfM4VplEntry 1 }


-- ATM Forum M4 VCL Termination Point Configuration Table Extensions

atmfM4VclTable OBJECT-TYPE
          SYNTAX                SEQUENCE OF             AtmfM4VclEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "The ATM Forum M4 VCL Termination Point Configuration
                         table extensions.  This table augments the VCL
                         configuration table in RFC 1695."
     ::= { atmfM4MIBObjects 10 }

atmfM4VclEntry OBJECT-TYPE
     SYNTAX    AtmfM4VclEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "Additional columns for the VCL configuration table entry."
     AUGMENTS { atmVclEntry }
     ::= { atmfM4VclTable 1 }

AtmfM4VclEntry ::= SEQUENCE {
     atmfM4VclSegEndPt        TruthValue
          }

atmfM4VclSegEndPt OBJECT-TYPE
     SYNTAX    TruthValue
     MAX-ACCESS     read-create
     STATUS    current
     DESCRIPTION
          "Specifies whether the VCL termination point is a segment
                         end-point."
     ::= { atmfM4VclEntry 1 }


-- ATM Forum M4 VP Cross-Connect Table Extensions

atmfM4VpXConnTable OBJECT-TYPE
     SYNTAX    SEQUENCE OF    AtmfM4VpXConnEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "The ATM Forum M4 VP Cross-Connect Configuration
                         table extensions.  This table augments the VP Cross-Connect
                         configuration table in RFC 1695."
     ::= { atmfM4MIBObjects 11 }

atmfM4VpXConnEntry OBJECT-TYPE
     SYNTAX    AtmfM4VpXConnEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "Additional columns for the VP Cross-Connect table entry."
     AUGMENTS { atmVpCrossConnectEntry }
     ::= { atmfM4VpXConnTable 1 }

AtmfM4VpXConnEntry ::= SEQUENCE {
     atmfM4VpXConnRecover     TruthValue
          }

atmfM4VpXConnRecover OBJECT-TYPE
     SYNTAX    TruthValue
     MAX-ACCESS     read-create
     STATUS    current
     DESCRIPTION
          "If FALSE, this cross-connection will be removed on
                         failure."
     ::= { atmfM4VpXConnEntry 1 }


-- ATM Forum M4 VC Cross-Connect Table Extensions

atmfM4VcXConnTable OBJECT-TYPE
     SYNTAX    SEQUENCE OF    AtmfM4VcXConnEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "The ATM Forum M4 VC Cross-Connect Configuration
                         table extensions.  This table augments the VC Cross-Connect
                         configuration table in RFC 1695."
     ::= { atmfM4MIBObjects 12 }

atmfM4VcXConnEntry OBJECT-TYPE
     SYNTAX    AtmfM4VcXConnEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "Additional columns for the VC Cross-Connect table entry."
     AUGMENTS { atmVcCrossConnectEntry }
     ::= { atmfM4VcXConnTable 1 }

AtmfM4VcXConnEntry ::= SEQUENCE {
     atmfM4VcXConnRecover     TruthValue
          }

atmfM4VcXConnRecover OBJECT-TYPE
     SYNTAX    TruthValue
     MAX-ACCESS     read-create
     STATUS    current
     DESCRIPTION
          "If FALSE, this cross-connection will be removed on
                         failure."
     ::= { atmfM4VcXConnEntry 1 }


-- ATM Forum M4 VP "Next VPI" Table

atmfM4VpNextVpiTable OBJECT-TYPE
     SYNTAX    SEQUENCE OF    AtmfM4VpNextVpiEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "The ATM Forum M4 VP Next-VPI value
                         table. This optional table supplied unused VPI values
                         for use in creating entries in the atmVplTable."
     ::= { atmfM4MIBObjects 13 }

atmfM4VpNextVpiEntry OBJECT-TYPE
     SYNTAX    AtmfM4VpNextVpiEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "Each entry in this table represents the 'next' VPI
                         value available for a given ATM interface.

                         Each ATM interface (UNI, BICI, BISSI) automatically has
                         an entry in this table associated with it."
     INDEX          { ifIndex }
     ::= { atmfM4VpNextVpiTable 1 }

AtmfM4VpNextVpiEntry ::= SEQUENCE {
     atmfM4VpNextVpiValue     INTEGER
          }

atmfM4VpNextVpiValue OBJECT-TYPE
     SYNTAX    INTEGER (-1..4095)
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "This object contains an appropriate value to be used for
                         atmVplVpi when creating entries in the atmVplTable.    The
                         value -1 indicates that no unassigned entries are available.
                         To obtain the atmVplVpi value for a new entry, the manager
                         issues a management protocol retrieval operation to obtain
                         the current value of this object.      After each retrieval, the
                         agent should modify the value to the next unassigned index
                         (or -1)."
     ::= { atmfM4VpNextVpiEntry 1 }


-- ATM Forum M4 VC "Next VCI" Table

atmfM4VcNextVciTable OBJECT-TYPE
     SYNTAX    SEQUENCE OF    AtmfM4VcNextVciEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "The ATM Forum M4 VC Next-VCI value
                         table. This optional table supplied unused VCI values
                         for use in creating entries in the atmVclTable."
     ::= { atmfM4MIBObjects 14 }

atmfM4VcNextVciEntry OBJECT-TYPE
     SYNTAX    AtmfM4VcNextVciEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "Each entry in this table represents the 'next' VCI
                         value available for a given ATM interface.

                         Each VPL Termination Point automatically has
                         an entry in this table associated with it."
     INDEX          { ifIndex,
                      atmVplVpi }
     ::= { atmfM4VcNextVciTable 1 }

AtmfM4VcNextVciEntry ::= SEQUENCE {
     atmfM4VcNextVciValue     INTEGER
          }

atmfM4VcNextVciValue OBJECT-TYPE
     SYNTAX    INTEGER (-1..65535)
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "This object contains an appropriate value to be used for
                         atmVclVci when creating entries in the atmVclTable.    The
                         value -1 indicates that no unassigned entries are available.
                         To obtain the atmVclVci value for a new entry, the manager
                         issues a management protocol retrieval operation to obtain
                         the current value of this object.      After each retrieval, the
                         agent should modify the value to the next unassigned index
                         (or -1)."
     ::= { atmfM4VcNextVciEntry 1 }


-- ATM Cell Protocol Monitoring Current Data (per interface)

atmfM4CellProtoCurrTable OBJECT-TYPE
     SYNTAX    SEQUENCE OF    AtmfM4CellProtoCurrEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "The ATM Forum M4 Cell Protocol Monitoring Current Data
                         table.

                         This table maintains per-interface statistics for the
                         fifteen-minute interval currently being collected."
     ::= { atmfM4MIBObjects 15 }

atmfM4CellProtoCurrEntry OBJECT-TYPE
     SYNTAX    AtmfM4CellProtoCurrEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "An entry in the ATM Forum M4 Cell Protocol Monitoring
                         Current Data table.

                         Each ATM interface (UNI, BICI, BISSI) automatically has
                         an entry in this table associated with it."
     INDEX          { ifIndex }
     ::= { atmfM4CellProtoCurrTable 1 }

AtmfM4CellProtoCurrEntry ::= SEQUENCE {
     atmfM4CellProtoCurrSuspect         TruthValue,
     atmfM4CellProtoCurrElapsedTime     TimeInterval,
     atmfM4CellProtoCurrSupprIntvls     Counter32,
     atmfM4CellProtoCurrProtoErrors     Counter32,
     atmfM4CellProtoCurrInOAMCells      Counter32
          }

atmfM4CellProtoCurrSuspect OBJECT-TYPE
     SYNTAX    TruthValue
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "If true, the statistics in this entry may be unreliable."
     ::= { atmfM4CellProtoCurrEntry 1 }

atmfM4CellProtoCurrElapsedTime OBJECT-TYPE
     SYNTAX    TimeInterval
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "Amount of time, measured in units of 0.01 second, that
                         statistics for this entry (the current interval) have been
                         counted."
     ::= { atmfM4CellProtoCurrEntry 2 }

atmfM4CellProtoCurrSupprIntvls OBJECT-TYPE
     SYNTAX    Counter32
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "This attribute is non-zero only if the ATM NE is
                         suppressing ATM Cell Protocol Monitoring History Data
                         entry creation when the current interval terminates with
                         'all-zeroes' performance measurements."
     ::= { atmfM4CellProtoCurrEntry 3 }

atmfM4CellProtoCurrProtoErrors OBJECT-TYPE
     SYNTAX    Counter32
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "The number of ATM cells dropped on this interface, due to
                         an unrecognized field or set of fields in the ATM cell
                         header, since the start of this interval."
     ::= { atmfM4CellProtoCurrEntry 4 }

atmfM4CellProtoCurrInOAMCells OBJECT-TYPE
     SYNTAX    Counter32
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "The number of OAM cells received at this interface since
                         the start of this interval."
     ::= { atmfM4CellProtoCurrEntry 5 }


-- ATM Cell Protocol Monitoring History Data (per interface and time
-- interval)

atmfM4CellProtoHistTable OBJECT-TYPE
     SYNTAX    SEQUENCE OF    AtmfM4CellProtoHistEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "The ATM Forum M4 Cell Protocol Monitoring History Data
                         table.

                         This table maintains per-interface statistics for previous
                         fifteen-minute intervals."
     ::= { atmfM4MIBObjects 16 }

atmfM4CellProtoHistEntry OBJECT-TYPE
     SYNTAX    AtmfM4CellProtoHistEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "An entry in the ATM Forum M4 Cell Protocol Monitoring
                         History Data table.

                         Each ATM interface (UNI, BICI, BISSI) automatically has
                         an entry in this table associated with it for each fifteen-
                         minute interval in which statistics are collected for it."
     INDEX          { ifIndex,
                    atmfM4CellProtoHistIndex }
     ::= { atmfM4CellProtoHistTable 1 }


AtmfM4CellProtoHistEntry ::= SEQUENCE {
     atmfM4CellProtoHistIndex           INTEGER,
     atmfM4CellProtoHistSuspect         TruthValue,
     atmfM4CellProtoHistElapsedTime     TimeInterval,
     atmfM4CellProtoHistSupprIntvls     Counter32,
     atmfM4CellProtoHistProtoErrors     Counter32,
     atmfM4CellProtoHistInOAMCells      Counter32
          }

atmfM4CellProtoHistIndex OBJECT-TYPE
     SYNTAX    INTEGER (1..96)
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "A number between 1 and 96, which identifies the interval
                         for which the set of statistics in this entry was
                         collected.

                         The interval identified by 1 is the most recently completed
                         15 minute interval, and the interval identified by N is the
                         interval immediately preceding the one identified by N-1."
     ::= { atmfM4CellProtoHistEntry 1 }

atmfM4CellProtoHistSuspect OBJECT-TYPE
     SYNTAX    TruthValue
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "If true, the statistics in this entry may be unreliable."
     ::= { atmfM4CellProtoHistEntry 2 }

atmfM4CellProtoHistElapsedTime OBJECT-TYPE
     SYNTAX    TimeInterval
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "Amount of time, measured in units of 0.01 second, that
                         statistics for this entry (the current interval) have been
                         counted."
     ::= { atmfM4CellProtoHistEntry 3 }

atmfM4CellProtoHistSupprIntvls OBJECT-TYPE
     SYNTAX    Counter32
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "This attribute is non-zero only if the ATM NE is
                         suppressing ATM Cell Protocol Monitoring History Data
                         entry creation when the current interval terminates with
                         'all-zeroes' performance measurements."
     ::= { atmfM4CellProtoHistEntry 4 }

atmfM4CellProtoHistProtoErrors OBJECT-TYPE
     SYNTAX    Counter32
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "The number of ATM cells dropped on this interface, due to
                         an unrecognized field or set of fields in the ATM cell
                         header, since the start of this interval."
     ::= { atmfM4CellProtoHistEntry 5 }

atmfM4CellProtoHistInOAMCells OBJECT-TYPE
     SYNTAX    Counter32
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "The number of OAM cells received at this interface since
                         the start of this interval."
     ::= { atmfM4CellProtoHistEntry 6 }


-- ATM Cell Protocol Monitoring Error Log (per interface, error code)

atmfM4CellProtoErrorTable OBJECT-TYPE
     SYNTAX    SEQUENCE OF    AtmfM4CellProtoErrorEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "The ATM Forum M4 Cell Protocol Monitoring Error Log
                         table.

                         This table maintains a record of the last error of each
                         type encountered on each interface, as a result of ATM
                         Cell Protocol Monitoring."
     ::= { atmfM4MIBObjects 17 }

atmfM4CellProtoErrorEntry OBJECT-TYPE
     SYNTAX    AtmfM4CellProtoErrorEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "An entry in the ATM Forum M4 Cell Protocol Monitoring
                         Error Log table.

                         Each ATM interface (UNI, BICI, BISSI) automatically has
                         an entry in this table associated with it for each error
                         that has occurred since agent start-up."
     INDEX          { ifIndex,
                    atmfM4CellProtoErrorCode }
     ::= { atmfM4CellProtoErrorTable 1 }

AtmfM4CellProtoErrorEntry ::= SEQUENCE {
     atmfM4CellProtoErrorCode      Integer32,
     atmfM4CellProtoErrorTime      TimeStamp,
     atmfM4CellProtoErrorReason    Integer32,
     atmfM4CellProtoErrorVpi       INTEGER,
     atmfM4CellProtoErrorVci       INTEGER
          }

atmfM4CellProtoErrorCode OBJECT-TYPE
     SYNTAX    Integer32
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "Indicates the type of error for which this entry contains
                         information."
     ::= { atmfM4CellProtoErrorEntry 1 }

atmfM4CellProtoErrorTime OBJECT-TYPE
     SYNTAX    TimeStamp
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "Value of sysUpTime when the error occurred."
     ::= { atmfM4CellProtoErrorEntry 2 }

atmfM4CellProtoErrorReason OBJECT-TYPE
     SYNTAX    Integer32
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "The cell header abnormality type: the reason for
                         discarding the ATM cell (i.e., unassigned VPI/VCI value or
                         VPI/VCI value out of range."
     ::= { atmfM4CellProtoErrorEntry 3 }

atmfM4CellProtoErrorVpi OBJECT-TYPE
     SYNTAX    INTEGER (0..4096)
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "The VPI value of the discarded cell."
     ::= { atmfM4CellProtoErrorEntry 4 }

atmfM4CellProtoErrorVci OBJECT-TYPE
     SYNTAX    INTEGER (0..65535)
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "The VCI value of the discarded cell."
     ::= { atmfM4CellProtoErrorEntry 5 }


-- TC Adaptor Protocol Monitoring Current Data (per interface)

atmfM4TcProtoCurrTable OBJECT-TYPE
     SYNTAX    SEQUENCE OF    AtmfM4TcProtoCurrEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "The ATM Forum M4 TC Adaptor Protocol Monitoring Current
                         Data table.

                         This table maintains per-interface statistics for the
                         fifteen-minute interval currently being collected."
          ::= { atmfM4MIBObjects 18 }

atmfM4TcProtoCurrEntry OBJECT-TYPE
          SYNTAX                AtmfM4TcProtoCurrEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "An entry in the ATM Forum M4 TC Adaptor Protocol Monitoring
          Current Data table.

          Each ATM interface (UNI, BICI, BISSI) automatically has
          an entry in this table associated with it."
          INDEX                   { ifIndex }
          ::= { atmfM4TcProtoCurrTable 1 }

AtmfM4TcProtoCurrEntry ::= SEQUENCE {
          atmfM4TcProtoCurrSuspect                               TruthValue,
          atmfM4TcProtoCurrElapsedTime           TimeInterval,
          atmfM4TcProtoCurrSupprIntvls           Counter32,
          atmfM4TcProtoCurrDiscardHECViol        Counter32
                         }

atmfM4TcProtoCurrSuspect OBJECT-TYPE
          SYNTAX                TruthValue
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "If true, the statistics in this entry may be unreliable."
          ::= { atmfM4TcProtoCurrEntry 1 }

atmfM4TcProtoCurrElapsedTime OBJECT-TYPE
          SYNTAX                TimeInterval
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "Amount of time, measured in units of 0.01 second, that
          statistics for this entry (the current interval) have been
          counted."
          ::= { atmfM4TcProtoCurrEntry 2 }

atmfM4TcProtoCurrSupprIntvls OBJECT-TYPE
          SYNTAX                Counter32
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "This attribute is non-zero only if the ATM NE is
          suppressing ATM TC Adaptor Protocol Monitoring History Data
          entry creation when the current interval terminates with
          'all-zeroes' performance measurements."
          ::= { atmfM4TcProtoCurrEntry 3 }

atmfM4TcProtoCurrDiscardHECViol OBJECT-TYPE
          SYNTAX                Counter32
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "The number of ATM cells discarded on this interface, due to
          an HEC violation, since the start of this interval."
          ::= { atmfM4TcProtoCurrEntry 4 }


-- ATM TC Adaptor Protocol Monitoring History Data (per interface and
-- time interval)

atmfM4TcProtoHistTable OBJECT-TYPE
          SYNTAX                SEQUENCE OF             AtmfM4TcProtoHistEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "The ATM Forum M4 TC Adaptor Protocol Monitoring History
          Data table.

          This table maintains per-interface statistics for previous
          fifteen-minute intervals."
          ::= { atmfM4MIBObjects 19 }

atmfM4TcProtoHistEntry OBJECT-TYPE
          SYNTAX                AtmfM4TcProtoHistEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "An entry in the ATM Forum M4 TC Adaptor Protocol Monitoring
          History Data table.

          Each ATM interface (UNI, BICI, BISSI) automatically has
          an entry in this table associated with it for each fifteen-
          minute interval in which statistics are collected for it."
          INDEX                   { ifIndex,
                                                  atmfM4TcProtoHistIndex }
          ::= { atmfM4TcProtoHistTable 1 }

AtmfM4TcProtoHistEntry ::= SEQUENCE {
          atmfM4TcProtoHistIndex                                 INTEGER,
          atmfM4TcProtoHistSuspect                               TruthValue,
          atmfM4TcProtoHistElapsedTime           TimeInterval,
          atmfM4TcProtoHistSupprIntvls           Unsigned32,
          atmfM4TcProtoHistDiscardHECViol        Unsigned32
                         }

atmfM4TcProtoHistIndex OBJECT-TYPE
          SYNTAX                INTEGER (1..96)
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "A number between 1 and 96, which identifies the interval
          for which the set of statistics in this entry was
          collected.

          The interval identified by 1 is the most recently completed
          15 minute interval, and the interval identified by N is the
          interval immediately preceding the one identified by N-1."
          ::= { atmfM4TcProtoHistEntry 1 }

atmfM4TcProtoHistSuspect OBJECT-TYPE
          SYNTAX                TruthValue
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "If true, the statistics in this entry may be unreliable."
          ::= { atmfM4TcProtoHistEntry 2 }

atmfM4TcProtoHistElapsedTime OBJECT-TYPE
          SYNTAX                TimeInterval
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "Amount of time, measured in units of 0.01 second, that
          statistics for this entry (the current interval) have been
          counted."
          ::= { atmfM4TcProtoHistEntry 3 }

atmfM4TcProtoHistSupprIntvls OBJECT-TYPE
          SYNTAX                Unsigned32
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "This attribute is non-zero only if the ATM NE is
          suppressing ATM Cell Protocol Monitoring History Data
          entry creation when the current interval terminates with
          'all-zeroes' performance measurements."
          ::= { atmfM4TcProtoHistEntry 4 }

atmfM4TcProtoHistDiscardHECViol OBJECT-TYPE
          SYNTAX                Unsigned32
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "The number of ATM cells discarded on this interface, due to
          an HEC violation, since the start of this interval."
          ::= { atmfM4TcProtoHistEntry 5 }


-- UPC/NPC Disagreement Monitoring Current Data (per VPL
-- termination point)

atmfM4VpUpcNpcCurrTable OBJECT-TYPE
          SYNTAX                SEQUENCE OF             AtmfM4VpUpcNpcCurrEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "The ATM Forum M4 UPC/NPC Disagreement Monitoring Current
          Data table for VPL termination points.

          This table maintains per-TP statistics for the
          fifteen-minute interval currently being collected."
          ::= { atmfM4MIBObjects 20 }

atmfM4VpUpcNpcCurrEntry OBJECT-TYPE
          SYNTAX                AtmfM4VpUpcNpcCurrEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "An entry in the ATM Forum M4 UPC/NPC Disagreement
          Monitoring Current Data table for VPL termination points.

          Each VPL Termination Point automatically has
          an entry in this table associated with it."
          INDEX                   { ifIndex,
                                                  atmVplVpi }
          ::= { atmfM4VpUpcNpcCurrTable 1 }

AtmfM4VpUpcNpcCurrEntry ::= SEQUENCE {
          atmfM4VpUpcNpcCurrSuspect                      TruthValue,
          atmfM4VpUpcNpcCurrElapsedTime          TimeInterval,
          atmfM4VpUpcNpcCurrSupprIntvls          Counter32,
          atmfM4VpUpcNpcCurrDiscardedCells       Counter32,
          atmfM4VpUpcNpcCurrDiscardedClp0        Counter32,
          atmfM4VpUpcNpcCurrPassedCells          Counter32,
          atmfM4VpUpcNpcCurrPassedClp0           Counter32
                         }

atmfM4VpUpcNpcCurrSuspect OBJECT-TYPE
          SYNTAX                TruthValue
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "If true, the statistics in this entry may be unreliable."
          ::= { atmfM4VpUpcNpcCurrEntry 1 }

atmfM4VpUpcNpcCurrElapsedTime OBJECT-TYPE
          SYNTAX                TimeInterval
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "Amount of time, measured in units of 0.01 second, that
          statistics for this entry (the current interval) have been
          counted."
          ::= { atmfM4VpUpcNpcCurrEntry 2 }

atmfM4VpUpcNpcCurrSupprIntvls OBJECT-TYPE
          SYNTAX                Counter32
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "This attribute is non-zero only if the ATM NE is
          suppressing UPC/NPC Disagreement Monitoring History Data
          entry creation when the current interval terminates with
          'all-zeroes' performance measurements."
          ::= { atmfM4VpUpcNpcCurrEntry 3 }

atmfM4VpUpcNpcCurrDiscardedCells OBJECT-TYPE
          SYNTAX                Counter32
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "The number of discarded cells due to combined CLP=0 and
          CLP=1 UPC/NPC policing."
          ::= { atmfM4VpUpcNpcCurrEntry 4 }

atmfM4VpUpcNpcCurrDiscardedClp0 OBJECT-TYPE
          SYNTAX                Counter32
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "The number of discarded cells due to CLP=0 only
          UPC/NPC policing.

          This object shall be present only if CLP=0 traffic is
          separately policed."
          ::= { atmfM4VpUpcNpcCurrEntry 5 }

atmfM4VpUpcNpcCurrPassedCells OBJECT-TYPE
          SYNTAX                Counter32
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "The number of cells that have been successfully passed by
          the combined CLP=0 and CLP=1 UPC/NPC policing."
          ::= { atmfM4VpUpcNpcCurrEntry 6 }

atmfM4VpUpcNpcCurrPassedClp0 OBJECT-TYPE
          SYNTAX                Counter32
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "The number of cells that have been successfully passed by
          the CLP=0 UPC/NPC policing.

          This object shall be present only if CLP=0 traffic is
          separately policed."
          ::= { atmfM4VpUpcNpcCurrEntry 7 }


-- UPC/NPC Disagreement Monitoring History (per VPL termination
-- point and time interval)

atmfM4VpUpcNpcHistTable OBJECT-TYPE
          SYNTAX                SEQUENCE OF             AtmfM4VpUpcNpcHistEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "The ATM Forum M4 UPC/NPC Disagreement Monitoring History
          Data table for VPL termination points.

          This table maintains per-interface statistics for previous
          fifteen-minute intervals."
          ::= { atmfM4MIBObjects 21 }

atmfM4VpUpcNpcHistEntry OBJECT-TYPE
          SYNTAX                AtmfM4VpUpcNpcHistEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "An entry in the ATM Forum M4 UPC/NPC Disagreement
          Monitoring History Data table for VPL termination points.

          Each VPL Termination Point automatically has
          an entry in this table associated with it."
          INDEX                   { ifIndex,
                                                  atmVplVpi,
                                                  atmfM4VpUpcNpcHistIndex }
          ::= { atmfM4VpUpcNpcHistTable 1 }

AtmfM4VpUpcNpcHistEntry ::= SEQUENCE {
          atmfM4VpUpcNpcHistIndex                                INTEGER,
          atmfM4VpUpcNpcHistSuspect                      TruthValue,
          atmfM4VpUpcNpcHistElapsedTime          TimeInterval,
          atmfM4VpUpcNpcHistSupprIntvls          Unsigned32,
          atmfM4VpUpcNpcHistDiscardedCells       Unsigned32,
          atmfM4VpUpcNpcHistDiscardedClp0        Unsigned32,
          atmfM4VpUpcNpcHistPassedCells          Unsigned32,
          atmfM4VpUpcNpcHistPassedClp0           Unsigned32
                         }

atmfM4VpUpcNpcHistIndex OBJECT-TYPE
          SYNTAX                INTEGER (1..96)
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "A number between 1 and 96, which identifies the interval
          for which the set of statistics in this entry was
          collected.

          The interval identified by 1 is the most recently completed
          15 minute interval, and the interval identified by N is the
          interval immediately preceding the one identified by N-1."
          ::= { atmfM4VpUpcNpcHistEntry 1 }

atmfM4VpUpcNpcHistSuspect OBJECT-TYPE
          SYNTAX                TruthValue
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "If true, the statistics in this entry may be unreliable."
          ::= { atmfM4VpUpcNpcHistEntry 2 }

atmfM4VpUpcNpcHistElapsedTime OBJECT-TYPE
          SYNTAX                TimeInterval
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "Amount of time, measured in units of 0.01 second, that
          statistics for this entry (the current interval) have been
          counted."
          ::= { atmfM4VpUpcNpcHistEntry 3 }

atmfM4VpUpcNpcHistSupprIntvls OBJECT-TYPE
          SYNTAX                Unsigned32
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "This attribute is non-zero only if the ATM NE is
          suppressing UPC/NPC Disagreement Monitoring History Data
          entry creation when the current interval terminates with
          'all-zeroes' performance measurements."
          ::= { atmfM4VpUpcNpcHistEntry 4 }

atmfM4VpUpcNpcHistDiscardedCells OBJECT-TYPE
          SYNTAX                Unsigned32
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "The number of discarded cells due to combined CLP=0 and
          CLP=1 UPC/NPC policing."
          ::= { atmfM4VpUpcNpcHistEntry 5 }

atmfM4VpUpcNpcHistDiscardedClp0 OBJECT-TYPE
          SYNTAX                Unsigned32
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "The number of discarded cells due to CLP=0 only
          UPC/NPC policing.

          This object shall be present only if CLP=0 traffic is
          separately policed."
          ::= { atmfM4VpUpcNpcHistEntry 6 }

atmfM4VpUpcNpcHistPassedCells OBJECT-TYPE
          SYNTAX                Unsigned32
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "The number of cells that have been successfully passed by
          the combined CLP=0 and CLP=1 UPC/NPC policing."
          ::= { atmfM4VpUpcNpcHistEntry 7 }

atmfM4VpUpcNpcHistPassedClp0 OBJECT-TYPE
          SYNTAX                Unsigned32
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "The number of cells that have been successfully passed by
          the CLP=0 UPC/NPC policing.

          This object shall be present only if CLP=0 traffic is
          separately policed."
          ::= { atmfM4VpUpcNpcHistEntry 8 }



-- UPC/NPC Disagreement Monitoring Current Data (per VCL
-- termination point)

atmfM4VcUpcNpcCurrTable OBJECT-TYPE
          SYNTAX                SEQUENCE OF             AtmfM4VcUpcNpcCurrEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "The ATM Forum M4 UPC/NPC Disagreement Monitoring Current
          Data table for VCL termination points.

          This table maintains per-TP statistics for the
          fifteen-minute interval currently being collected."
          ::= { atmfM4MIBObjects 22 }

atmfM4VcUpcNpcCurrEntry OBJECT-TYPE
          SYNTAX                AtmfM4VcUpcNpcCurrEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "An entry in the ATM Forum M4 UPC/NPC Disagreement
          Monitoring Current Data table for VCL termination points.

          Each VCL Termination Point automatically has
          an entry in this table associated with it."
          INDEX                   { ifIndex,
                                                  atmVclVpi,
                                                  atmVclVci }
          ::= { atmfM4VcUpcNpcCurrTable 1 }

AtmfM4VcUpcNpcCurrEntry ::= SEQUENCE {
          atmfM4VcUpcNpcCurrSuspect                      TruthValue,
          atmfM4VcUpcNpcCurrElapsedTime          TimeInterval,
          atmfM4VcUpcNpcCurrSupprIntvls          Counter32,
          atmfM4VcUpcNpcCurrDiscardedCells       Counter32,
          atmfM4VcUpcNpcCurrDiscardedClp0        Counter32,
          atmfM4VcUpcNpcCurrPassedCells          Counter32,
          atmfM4VcUpcNpcCurrPassedClp0           Counter32
                         }

atmfM4VcUpcNpcCurrSuspect OBJECT-TYPE
          SYNTAX                TruthValue
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "If true, the statistics in this entry may be unreliable."
          ::= { atmfM4VcUpcNpcCurrEntry 1 }

atmfM4VcUpcNpcCurrElapsedTime OBJECT-TYPE
          SYNTAX                TimeInterval
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "Amount of time, measured in units of 0.01 second, that
          statistics for this entry (the current interval) have been
          counted."
          ::= { atmfM4VcUpcNpcCurrEntry 2 }

atmfM4VcUpcNpcCurrSupprIntvls OBJECT-TYPE
          SYNTAX                Counter32
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "This attribute is non-zero only if the ATM NE is
                         suppressing UPC/NPC Disagreement Monitoring History Data
                         entry creation when the current interval terminates with
                         'all-zeroes' performance measurements."
     ::= { atmfM4VcUpcNpcCurrEntry 3 }

atmfM4VcUpcNpcCurrDiscardedCells OBJECT-TYPE
     SYNTAX    Counter32
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "The number of discarded cells due to combined CLP=0 and
                         CLP=1 UPC/NPC policing."
     ::= { atmfM4VcUpcNpcCurrEntry 4 }

atmfM4VcUpcNpcCurrDiscardedClp0 OBJECT-TYPE
     SYNTAX    Counter32
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "The number of discarded cells due to CLP=0 only
                         UPC/NPC policing.

                         This object shall be present only if CLP=0 traffic is
                         separately policed."
     ::= { atmfM4VcUpcNpcCurrEntry 5 }

atmfM4VcUpcNpcCurrPassedCells OBJECT-TYPE
     SYNTAX    Counter32
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "The number of cells that have been successfully passed by
                         the combined CLP=0 and CLP=1 UPC/NPC policing."
     ::= { atmfM4VcUpcNpcCurrEntry 6 }

atmfM4VcUpcNpcCurrPassedClp0 OBJECT-TYPE
     SYNTAX    Counter32
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "The number of cells that have been successfully passed by
                         the CLP=0 UPC/NPC policing.

                         This object shall be present only if CLP=0 traffic is
                         separately policed."
     ::= { atmfM4VcUpcNpcCurrEntry 7 }


-- UPC/NPC Disagreement Monitoring History (per VCL termination
-- point and time interval)

atmfM4VcUpcNpcHistTable OBJECT-TYPE
     SYNTAX    SEQUENCE OF    AtmfM4VcUpcNpcHistEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "The ATM Forum M4 UPC/NPC Disagreement Monitoring History
                         Data table for VCL termination points.

                         This table maintains per-interface statistics for previous
                         fifteen-minute intervals."
     ::= { atmfM4MIBObjects 23 }

atmfM4VcUpcNpcHistEntry OBJECT-TYPE
     SYNTAX    AtmfM4VcUpcNpcHistEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "An entry in the ATM Forum M4 UPC/NPC Disagreement
                         Monitoring History Data table for VCL termination points.

                         Each VCL Termination Point automatically has
                         an entry in this table associated with it."
     INDEX          { ifIndex,
                    atmVclVpi,
                    atmVclVci,
                    atmfM4VcUpcNpcHistIndex }
     ::= { atmfM4VcUpcNpcHistTable 1 }

AtmfM4VcUpcNpcHistEntry ::= SEQUENCE {
     atmfM4VcUpcNpcHistIndex            INTEGER,
     atmfM4VcUpcNpcHistSuspect          TruthValue,
     atmfM4VcUpcNpcHistElapsedTime      TimeInterval,
     atmfM4VcUpcNpcHistSupprIntvls      Unsigned32,
     atmfM4VcUpcNpcHistDiscardedCells   Unsigned32,
     atmfM4VcUpcNpcHistDiscardedClp0    Unsigned32,
     atmfM4VcUpcNpcHistPassedCells      Unsigned32,
     atmfM4VcUpcNpcHistPassedClp0       Unsigned32
          }

atmfM4VcUpcNpcHistIndex OBJECT-TYPE
     SYNTAX    INTEGER (1..96)
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "A number between 1 and 96, which identifies the interval
                         for which the set of statistics in this entry was
                         collected.

                         The interval identified by 1 is the most recently completed
                         15 minute interval, and the interval identified by N is the
                         interval immediately preceding the one identified by N-1."
     ::= { atmfM4VcUpcNpcHistEntry 1 }

atmfM4VcUpcNpcHistSuspect OBJECT-TYPE
     SYNTAX    TruthValue
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "If true, the statistics in this entry may be unreliable."
     ::= { atmfM4VcUpcNpcHistEntry 2 }

atmfM4VcUpcNpcHistElapsedTime OBJECT-TYPE
     SYNTAX    TimeInterval
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "Amount of time, measured in units of 0.01 second, that
                         statistics for this entry (the current interval) have been
                         counted."
     ::= { atmfM4VcUpcNpcHistEntry 3 }

atmfM4VcUpcNpcHistSupprIntvls OBJECT-TYPE
     SYNTAX    Unsigned32
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "This attribute is non-zero only if the ATM NE is
                         suppressing UPC/NPC Disagreement Monitoring History Data
                         entry creation when the current interval terminates with
                         'all-zeroes' performance measurements."
     ::= { atmfM4VcUpcNpcHistEntry 4 }

atmfM4VcUpcNpcHistDiscardedCells OBJECT-TYPE
     SYNTAX    Unsigned32
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "The number of discarded cells due to combined CLP=0 and
                         CLP=1 UPC/NPC policing."
     ::= { atmfM4VcUpcNpcHistEntry 5 }

atmfM4VcUpcNpcHistDiscardedClp0 OBJECT-TYPE
     SYNTAX    Unsigned32
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "The number of discarded cells due to CLP=0 only
                         UPC/NPC policing.

                         This object shall be present only if CLP=0 traffic is
                         separately policed."
     ::= { atmfM4VcUpcNpcHistEntry 6 }

atmfM4VcUpcNpcHistPassedCells OBJECT-TYPE
     SYNTAX    Unsigned32
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "The number of cells that have been successfully passed by
                         the combined CLP=0 and CLP=1 UPC/NPC policing."
     ::= { atmfM4VcUpcNpcHistEntry 7 }

atmfM4VcUpcNpcHistPassedClp0 OBJECT-TYPE
     SYNTAX    Unsigned32
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "The number of cells that have been successfully passed by
                         the CLP=0 UPC/NPC policing.

                         This object shall be present only if CLP=0 traffic is
                         separately policed."
     ::= { atmfM4VcUpcNpcHistEntry 8 }


-- ATM Forum M4 Test Types

atmfM4TestTypes     OBJECT IDENTIFIER
     ::= { atmfM4MIBObjects 24 }


-- OAM Loopback Tests (VPL, VPC, VCL, anc VCC termination points):

atmfM4TestOAMLoopbackSeg OBJECT-IDENTITY
     STATUS    current
     DESCRIPTION
          "This identifies an OAM Loopback Test on a VPL, VPC,
                         VCL, or VCC termination point, using a segment OAM
                         cell.

                         The test type must have appended to it a code that uniquely
                         identifies an intermediate point responsible for looping
                         back the cell.  If this is absent, the loopback is performed
                         at the end of the segment or connection.

                         E.g., the OID { atmfM4TestOAMLoopbackSeg 5 } identifies
                         that the loopback should be performed at the intermediate
                         point labeled 5."
     ::= { atmfM4TestTypes 1 }

atmfM4TestOAMLoopbackE2E OBJECT-IDENTITY
     STATUS    current
     DESCRIPTION
          "This identifies an OAM Loopback Test on a VPL, VPC,
                         VCL, or VCC termination point, using an end-to-end OAM
                         cell."
     ::= { atmfM4TestTypes 2 }


-- ATM Forum M4 VP Termination Point Test Table

atmfM4VpTestTable OBJECT-TYPE
     SYNTAX    SEQUENCE OF    AtmfM4VpTestEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "The ATM Forum M4 VP Termination Point Test table.
                         This table allows tests to be run on VPL and VPC
                         termination points.

                         The operation of this table is entirely analogous
                         to that of the ifTestTable in RFC 1573, except that
                         the indexes into this table are different."
     ::= { atmfM4MIBObjects 25 }

atmfM4VpTestEntry OBJECT-TYPE
     SYNTAX    AtmfM4VpTestEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "An entry containing objects for invoking tests on a
                         VPL or VPC termination point."
     INDEX          { ifIndex,
                    atmVplVpi,
                    atmfM4VpTestObject }
     ::= { atmfM4VpTestTable 1 }

AtmfM4VpTestEntry ::= SEQUENCE {
     atmfM4VpTestObject  INTEGER,
     atmfM4VpTestId      TestAndIncr,
     atmfM4VpTestStatus  INTEGER,
     atmfM4VpTestType    AutonomousType,
     atmfM4VpTestResult  INTEGER,
     atmfM4VpTestCode    OBJECT IDENTIFIER,
     atmfM4VpTestOwner   OwnerString
          }

atmfM4VpTestObject OBJECT-TYPE
     SYNTAX    INTEGER {
                    vplTp(1),
                    vpcTp(2)
                         }
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "Specifies whether the test applies to the VPL termination
                         point with the specified VPI, or the VPC termination point."
     ::= { atmfM4VpTestEntry 1 }

atmfM4VpTestId         OBJECT-TYPE
     SYNTAX       TestAndIncr
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
           "This object identifies the current invocation of the
                          interface's test."
     ::= { atmfM4VpTestEntry 2 }

atmfM4VpTestStatus     OBJECT-TYPE
     SYNTAX       INTEGER { notInUse(1), inUse(2) }
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
           "This object indicates whether or not some manager
           currently has the necessary 'ownership' required to
           invoke a test on this interface.  A write to this
           object is only successful when it changes its value
           from 'notInUse(1)' to 'inUse(2)'.  After completion of
           a test, the agent resets the value back to
           'notInUse(1)'."
     ::= { atmfM4VpTestEntry 3 }

atmfM4VpTestType       OBJECT-TYPE
     SYNTAX       AutonomousType
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
           "A control variable used to start and stop operator-
           initiated interface tests.  Most OBJECT IDENTIFIER
           values assigned to tests are defined elsewhere, in
           association with specific types of interface.
           However, this document assigns a value for a full-
           duplex loopback test, and defines the special meanings
           of the subject identifier:

               noTest  OBJECT IDENTIFIER ::= { 0 0 }

           When the value noTest is written to this object, no
           action is taken unless a test is in progress, in which
           case the test is aborted.  Writing any other value to
           this object is only valid when no test is currently in
           progress, in which case the indicated test is
           initiated.

           When read, this object always returns the most recent
           value that atmfM4VpTestType was set to.  If it has not been
           set since the last initialization of the network
           management subsystem on the agent, a value of noTest
           is returned."
     ::= { atmfM4VpTestEntry 4 }

atmfM4VpTestResult  OBJECT-TYPE
     SYNTAX       INTEGER {
                      none(1),          -- no test yet requested
                      success(2),
                      inProgress(3),
                      notSupported(4),
                      unAbleToRun(5),   -- due to state of system
                      aborted(6),
                      failed(7)
                  }
     MAX-ACCESS   read-only
     STATUS       current
     DESCRIPTION
           "This object contains the result of the most recently
           requested test, or the value none(1) if no tests have
           been requested since the last reset.  Note that this
           facility provides no provision for saving the results
           of one test when starting another, as could be
           required if used by multiple managers concurrently."
     ::= { atmfM4VpTestEntry 5 }

atmfM4VpTestCode  OBJECT-TYPE
     SYNTAX       OBJECT IDENTIFIER
     MAX-ACCESS   read-only
     STATUS       current
     DESCRIPTION
           "This object contains a code which contains more
           specific information on the test result, for example
           an error-code after a failed test.  Error codes and
           other values this object may take are specific to the
           type of interface and/or test.  The value may have the
           semantics of either the AutonomousType or
           RowPointer textual conventions as defined in RFC
           1903 [15].  The identifier:

               testCodeUnknown  OBJECT IDENTIFIER ::= { 0 0 }

           is defined for use if no additional result code is
           available."
     ::= { atmfM4VpTestEntry 6 }

atmfM4VpTestOwner      OBJECT-TYPE
     SYNTAX       OwnerString
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
           "The entity which currently has the 'ownership'
           required to invoke a test on this interface."
     ::= { atmfM4VpTestEntry 7 }



-- ATM Forum M4 VC Termination Point Test Table

atmfM4VcTestTable OBJECT-TYPE
     SYNTAX    SEQUENCE OF    AtmfM4VcTestEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "The ATM Forum M4 VC Termination Point Test table.
          This table allows tests to be run on VCL and VCC
          termination points.

          The operation of this table is entirely analogous
          to that of the ifTestTable in RFC 1573, except that
          the indexes into this table are different."
     ::= { atmfM4MIBObjects 26 }

atmfM4VcTestEntry OBJECT-TYPE
     SYNTAX    AtmfM4VcTestEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "An entry containing objects for invoking tests on a
          VCL or VCC termination point."
     INDEX          { ifIndex,
                    atmVclVpi,
                    atmVclVci,
                    atmfM4VcTestObject }
     ::= { atmfM4VcTestTable 1 }

AtmfM4VcTestEntry ::= SEQUENCE {
     atmfM4VcTestObject  INTEGER,
     atmfM4VcTestId      TestAndIncr,
     atmfM4VcTestStatus  INTEGER,
     atmfM4VcTestType    AutonomousType,
     atmfM4VcTestResult  INTEGER,
     atmfM4VcTestCode    OBJECT IDENTIFIER,
     atmfM4VcTestOwner   OwnerString
          }

atmfM4VcTestObject OBJECT-TYPE
     SYNTAX    INTEGER {
                    vclTp(1),
                    vccTp(2)
                         }
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "Specifies whether the test applies to the VCL termination
          point with the specified VPI and VCI values, or to the VCC
          termination point."
     ::= { atmfM4VcTestEntry 1 }

atmfM4VcTestId         OBJECT-TYPE
     SYNTAX       TestAndIncr
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
          "This object identifies the current invocation of the
          interface's test."
     ::= { atmfM4VcTestEntry 2 }

atmfM4VcTestStatus     OBJECT-TYPE
     SYNTAX       INTEGER { notInUse(1), inUse(2) }
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
          "This object indicates whether or not some manager
                         currently has the necessary 'ownership' required to
                         invoke a test on this interface.  A write to this
                         object is only successful when it changes its value
                         from 'notInUse(1)' to 'inUse(2)'.      After completion of
                         a test, the agent resets the value back to
                         'notInUse(1)'."
     ::= { atmfM4VcTestEntry 3 }

atmfM4VcTestType       OBJECT-TYPE
     SYNTAX       AutonomousType
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
          "A control variable used to start and stop operator-
                         initiated interface tests.  Most OBJECT IDENTIFIER
                         values assigned to tests are defined elsewhere, in
                         association with specific types of interface.
                         However, this document assigns a value for a full-
                         duplex loopback test, and defines the special meanings
                         of the subject identifier:

                                  noTest         OBJECT IDENTIFIER ::= { 0 0 }

                         When the value noTest is written to this object, no
                         action is taken unless a test is in progress, in which
                         case the test is aborted.       Writing any other value to
                         this object is only valid when no test is currently in
                         progress, in which case the indicated test is
                         initiated.

                         When read, this object always returns the most recent
                         value that atmfM4VcTestType was set to.        If it has not been
                         set since the last initialization of the network
                         management subsystem on the agent, a value of noTest
                         is returned."
     ::= { atmfM4VcTestEntry 4 }

atmfM4VcTestResult  OBJECT-TYPE
     SYNTAX       INTEGER {
                      none(1),          -- no test yet requested
                      success(2),
                      inProgress(3),
                      notSupported(4),
                      unAbleToRun(5),   -- due to state of system
                      aborted(6),
                      failed(7)
                  }
     MAX-ACCESS   read-only
     STATUS       current
     DESCRIPTION
          "This object contains the result of the most recently
                         requested test, or the value none(1) if no tests have
                         been requested since the last reset.   Note that this
                         facility provides no provision for saving the results
                         of one test when starting another, as could be
                         required if used by multiple managers concurrently."
     ::= { atmfM4VcTestEntry 5 }

atmfM4VcTestCode  OBJECT-TYPE
     SYNTAX       OBJECT IDENTIFIER
     MAX-ACCESS   read-only
     STATUS       current
     DESCRIPTION
          "This object contains a code which contains more
                         specific information on the test result, for example
                         an error-code after a failed test.      Error codes and
                         other values this object may take are specific to the
                         type of interface and/or test. The value may have the
                         semantics of either the AutonomousType or
                         RowPointer textual conventions as defined in RFC
                         1903 [15].      The identifier:

                                  testCodeUnknown        OBJECT IDENTIFIER ::= { 0 0 }

                         is defined for use if no additional result code is
                         available."
     ::= { atmfM4VcTestEntry 6 }

atmfM4VcTestOwner      OBJECT-TYPE
     SYNTAX       OwnerString
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
          "The entity which currently has the 'ownership'
                         required to invoke a test on this termination point."
     ::= { atmfM4VcTestEntry 7 }


-- ATM Forum M4 Equipment Table

atmfM4EquipTable OBJECT-TYPE
     SYNTAX    SEQUENCE OF    AtmfM4EquipEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "The ATM Forum M4 Equipment table.     This table augments the
                         physical entity table."
     ::= { atmfM4MIBObjects 28 }

atmfM4EquipEntry OBJECT-TYPE
     SYNTAX    AtmfM4EquipEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "An entry in the ATM Forum M4 Equipment table. Each entry
                         of this type represents a piece of equipment within the ATM
                         NE that neither is nor accepts a replaceable plug- in unit."
     INDEX          { entPhysicalIndex }
     ::= { atmfM4EquipTable 1 }

AtmfM4EquipEntry ::= SEQUENCE {
     atmfM4EquipAdminStatus   INTEGER,
     atmfM4EquipLocation      DisplayString,
     atmfM4EquipOperStatus    INTEGER,
     atmfM4EquipVendor        DisplayString,
     atmfM4EquipVersion       AutonomousType,
     atmfM4EquipUserLabel     DisplayString,
     atmfM4EquipAlarmSeverityIndex Integer32
          }

atmfM4EquipAdminStatus OBJECT-TYPE
     SYNTAX    INTEGER {
                    up(1),
                    down(2)
                        }
     MAX-ACCESS     read-write
     STATUS    current
     DESCRIPTION
          "Used by the adminstrator to lock and unlock the object."
     ::= { atmfM4EquipEntry 1 }

atmfM4EquipLocation OBJECT-TYPE
     SYNTAX    DisplayString
     MAX-ACCESS     read-write
     STATUS    current
     DESCRIPTION
          "The specific or general location of the component."
     ::= { atmfM4EquipEntry 2 }

atmfM4EquipOperStatus OBJECT-TYPE
     SYNTAX    INTEGER {
                    up(1),
                    down(2),
                    unknown(3)
                         }
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "This attributes identifies whether or not the component is
                         capable of performing its normal functions."
     ::= { atmfM4EquipEntry 3 }

atmfM4EquipVendor OBJECT-TYPE
     SYNTAX    DisplayString
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "The vendor of the component."
     ::= { atmfM4EquipEntry 4 }

atmfM4EquipVersion OBJECT-TYPE
     SYNTAX    AutonomousType
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "The version of the component."
     ::= { atmfM4EquipEntry 5 }

atmfM4EquipUserLabel OBJECT-TYPE
     SYNTAX    DisplayString
     MAX-ACCESS     read-write
     STATUS    current
     DESCRIPTION
          "A user-friendly name for the piece of equipment."
     DEFVAL    { "" }
     ::= { atmfM4EquipEntry 6 }

atmfM4EquipAlarmSeverityIndex OBJECT-TYPE
     SYNTAX    Integer32
     MAX-ACCESS     read-write
     STATUS    current
     DESCRIPTION
          "An index into the alarm severity profile table, specifying
                         the severity assignments for M4 alarms reported for this
                         component."
     DEFVAL    { 0 }
     ::= { atmfM4EquipEntry 7 }


-- ATM Forum M4 Equipment Holder Table

atmfM4EquipHolderTable OBJECT-TYPE
     SYNTAX    SEQUENCE OF    AtmfM4EquipHolderEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "The ATM Forum M4 Equipment Holder table.     This table
                         augments the physical table."
     ::= { atmfM4MIBObjects 29 }

atmfM4EquipHolderEntry OBJECT-TYPE
     SYNTAX    AtmfM4EquipHolderEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "An entry in the ATM Forum M4 Equipment Holder table.  Each
                         entry of this type represents a component within the ATM NE
                         that accepts a replaceable plug-in unit."
     INDEX          { entPhysicalIndex }
     ::= { atmfM4EquipHolderTable 1 }

AtmfM4EquipHolderEntry ::= SEQUENCE {
     atmfM4EquipHolderType              INTEGER,
     atmfM4EquipHolderAcceptableTypes   DisplayString,
     atmfM4EquipHolderSlotStatus        INTEGER,
     atmfM4EquipHolderSwLoad            INTEGER
          }

atmfM4EquipHolderType OBJECT-TYPE
     SYNTAX    INTEGER {
                    rack(1),
                    shelf(2),
                    drawer(3),
                    slot(4)
                         }
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "The type of the component."
     ::= { atmfM4EquipHolderEntry 1 }

atmfM4EquipHolderAcceptableTypes OBJECT-TYPE
     SYNTAX    DisplayString
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "The types of plug-in units that can be supported by the
                         slot, separated by newline characters.

                         This attribute shall be present only when the Equipment
                         Holder represents a slot."
     ::= { atmfM4EquipHolderEntry 2 }

atmfM4EquipHolderSlotStatus OBJECT-TYPE
     SYNTAX    INTEGER {
                    empty(1),
                    full(2)
                         }
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "This attributes identifies whether or not a plug-in unit is
                         present in the slot.

                         This attribute shall be present only when the Equipment
                         Holder represents a slot."
     ::= { atmfM4EquipHolderEntry 3 }

atmfM4EquipHolderSwLoad OBJECT-TYPE
     SYNTAX    INTEGER (1..2147483647)
     MAX-ACCESS     read-write
     STATUS    current
     DESCRIPTION
          "An index into the installed software table, specifying
                         the software that is to be loaded into the plug-in unit
                         whenever an automatic reload of software is needed.

                         This attribute shall be present only when the Equipment
                         Holder represents a slot."
     ::= { atmfM4EquipHolderEntry 4 }


-- ATM Forum M4 Plug-In Unit Table

atmfM4PlugInUnitTable OBJECT-TYPE
     SYNTAX    SEQUENCE OF    AtmfM4PlugInUnitEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "The ATM Forum M4 Plug-In Unittable.  This table augments
                         the physical entity table."
     ::= { atmfM4MIBObjects 30 }

atmfM4PlugInUnitEntry OBJECT-TYPE
     SYNTAX    AtmfM4PlugInUnitEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "An entry in the ATM Forum M4 Plug-In Unit table. Each
                         entry    of this type represents a piece of equipment within
                         the ATM NE that is inserted into and removed from an
                         Equipment Holder."
     INDEX          { entPhysicalIndex }
     ::= { atmfM4PlugInUnitTable 1 }

AtmfM4PlugInUnitEntry ::= SEQUENCE {
     atmfM4PlugInUnitAdminStatus   INTEGER,
     atmfM4PlugInUnitAvailStatus   INTEGER,
     atmfM4PlugInUnitOperStatus    INTEGER,
     atmfM4PlugInUnitVendor        DisplayString,
     atmfM4PlugInUnitVersion       AutonomousType,
     atmfM4PlugInUnitAlarmSeverityIndex Integer32
          }

atmfM4PlugInUnitAdminStatus OBJECT-TYPE
     SYNTAX    INTEGER {
                    up(1),
                    down(2)
                         }
     MAX-ACCESS     read-write
     STATUS    current
     DESCRIPTION
          "Used by the adminstrator to lock and unlock the object."
     ::= { atmfM4PlugInUnitEntry 1 }

atmfM4PlugInUnitAvailStatus OBJECT-TYPE
     SYNTAX    INTEGER {
                    available(1),
                    inTest(2),
                    failed(3),
                    powerOff(4),
                    notInstalled(5),
                    offLine(6),
                    dependency(7)
                         }
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "Provides further information regarding the state of the
                         component."
     ::= { atmfM4PlugInUnitEntry 2 }

atmfM4PlugInUnitOperStatus OBJECT-TYPE
     SYNTAX    INTEGER {
                    up(1),
                    down(2),
                    unknown(3)
                         }
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "This attributes identifies whether or not the component is
                         capable of performing its normal functions."
     ::= { atmfM4PlugInUnitEntry 3 }

atmfM4PlugInUnitVendor OBJECT-TYPE
     SYNTAX    DisplayString
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "The vendor of the component."
     ::= { atmfM4PlugInUnitEntry 4 }

atmfM4PlugInUnitVersion OBJECT-TYPE
     SYNTAX    AutonomousType
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "The version of the component."
     ::= { atmfM4PlugInUnitEntry 5 }

atmfM4PlugInUnitAlarmSeverityIndex OBJECT-TYPE
     SYNTAX    Integer32
     MAX-ACCESS     read-write
     STATUS    current
     DESCRIPTION
          "An index into the alarm severity profile table, specifying
                         the severity assignments for M4 alarms reported for this
                         component."
     DEFVAL    { 0 }
     ::= { atmfM4PlugInUnitEntry 6 }

-- ATM Forum M4 Hardware Unit/Running Software Relationship Table

atmfM4HwRunningSwTable OBJECT-TYPE
     SYNTAX    SEQUENCE OF    AtmfM4HwRunningSwEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "The ATM Forum M4 Hardware Unit/Running Software
                         relationship.   This table describes the software that is
                         running on each hardware unit in the ATM NE."
     ::= { atmfM4MIBObjects 32 }

atmfM4HwRunningSwEntry OBJECT-TYPE
     SYNTAX    AtmfM4HwRunningSwEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "An entry in the ATM Forum M4 Hardware Unit/Running Software
                         relationship table.     Each entry of this type identifies an
                         entry in the entPhysicalTable and one in the
                         hrRunningSoftwareTable."
     INDEX          { atmfM4HwRunningSwHwIndex,
                    atmfM4HwRunningSwIndex }
     ::= { atmfM4HwRunningSwTable 1 }

AtmfM4HwRunningSwEntry ::= SEQUENCE {
     atmfM4HwRunningSwHwIndex INTEGER,
     atmfM4HwRunningSwIndex        INTEGER,
     atmfM4HwRunningSwSwIndex INTEGER
          }

atmfM4HwRunningSwHwIndex OBJECT-TYPE
     SYNTAX    INTEGER (1..2147483647)
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "The index, in the entPhysicalTable, of the containing
                         hardware unit in this pair."
     ::= { atmfM4HwRunningSwEntry 1 }

atmfM4HwRunningSwIndex OBJECT-TYPE
     SYNTAX    INTEGER (1..2147483647)
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "A unique number within the context of the containing
                         hardware unit."
     ::= { atmfM4HwRunningSwEntry 2 }

atmfM4HwRunningSwSwIndex OBJECT-TYPE
     SYNTAX    INTEGER (1..2147483647)
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "The index, in the hrRunningSwTable, of the software product
                         represented by this entry."
     ::= { atmfM4HwRunningSwEntry 3 }


-- ATM Forum M4 Hardware Unit/Installed Software Relationship Table

atmfM4HwInstalledSwTable OBJECT-TYPE
     SYNTAX    SEQUENCE OF    AtmfM4HwInstalledSwEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "The ATM Forum M4 Hardware Unit/Installed Software
                         relationship.   This table describes the software that is
                         Installed on each hardware unit in the ATM NE."
     ::= { atmfM4MIBObjects 33 }

atmfM4HwInstalledSwEntry OBJECT-TYPE
     SYNTAX    AtmfM4HwInstalledSwEntry
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "An entry in the ATM Forum M4 Hardware Unit/Installed
                         Software relationship table.    Each entry of this type
                         identifies an entry in the physical entity table and one in the
                         hrInstalledSoftwareTable."
     INDEX          { atmfM4HwInstalledSwHwIndex,
                    atmfM4HwInstalledSwIndex }
     ::= { atmfM4HwInstalledSwTable 1 }

AtmfM4HwInstalledSwEntry ::= SEQUENCE {
     atmfM4HwInstalledSwHwIndex    INTEGER,
     atmfM4HwInstalledSwIndex      INTEGER,
     atmfM4HwInstalledSwSwIndex    INTEGER,
     atmfM4HwSwAlarmSeverityIndex  Integer32
          }

atmfM4HwInstalledSwHwIndex OBJECT-TYPE
     SYNTAX    INTEGER (1..2147483647)
     MAX-ACCESS     not-accessible
     STATUS    current
     DESCRIPTION
          "The index, in the entPhysical table, of the containing
                         physical entity in this pair."
     ::= { atmfM4HwInstalledSwEntry 1 }

atmfM4HwInstalledSwIndex OBJECT-TYPE
     SYNTAX    INTEGER (1..2147483647)
     MAX-ACCESS     read-only
     STATUS    current
     DESCRIPTION
          "A unique number within the context of the containing
                         hardware unit."
          ::= { atmfM4HwInstalledSwEntry 2 }

atmfM4HwInstalledSwSwIndex OBJECT-TYPE
          SYNTAX                INTEGER (1..2147483647)
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "The index, in the hrInstalledSwTable, of the software
          product represented by this entry."
          ::= { atmfM4HwInstalledSwEntry 3 }

atmfM4HwSwAlarmSeverityIndex OBJECT-TYPE
          SYNTAX                Integer32
          MAX-ACCESS      read-write
          STATUS                current
          DESCRIPTION
                         "An index into the alarm severity profile table, specifying
          the severity assignments for M4 alarms reported for this
          piece of software installed on the hardware unit."
          DEFVAL                { 0 }
          ::= { atmfM4HwInstalledSwEntry 4 }



-- ATM Forum M4 Alarm Severity Identifier Textual Convention

AtmfM4AlarmLogSeverity ::= TEXTUAL-CONVENTION
          STATUS                current
          DESCRIPTION
                         "The value of this object identifies the severity of
          an alarm in the log, including 'cleared'."
          SYNTAX                INTEGER {
                                                  cleared(-1),
                                                  indeterminate(0),
                                                  critical(1),
                                                  major(2),
                                                  minor(3),
                                                  warning(4)
                                                                 }

AtmfM4AlarmSeverity ::= TEXTUAL-CONVENTION
          STATUS                current
          DESCRIPTION
                         "The value of this object identifies the severity of
          an alarm that has occurred.  (Note that there is no
          value corresponding to 'cleared'.)"
          SYNTAX                INTEGER {
                                                  indeterminate(0),
                                                  critical(1),
                                                  major(2),
                                                  minor(3),
                                                  warning(4)
                                                                 }

-- ATM Forum M4 Alarm Severity Profile Table

atmfM4AlarmSevDefault OBJECT-TYPE
          SYNTAX                AtmfM4AlarmSeverity
          MAX-ACCESS      read-write
          STATUS                current
          DESCRIPTION
                         "The default severity value used for new profile
          index/trap ID pairs that have not yet been modified.
          This value is also used whenever an object's alarm
          severity profile index is set to 0."
          DEFVAL                { minor }
          ::= { atmfM4MIBObjects 34 }

atmfM4AlarmSevProfileIndexNext OBJECT-TYPE
          SYNTAX                Integer32
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "This object contains an appropriate value to be used for
          atmfM4AlarmSevProfileIndex when creating entries in the
          atmfM4AlarmSevProfileTable.
          The value -1 indicates that no unassigned entries are
          available.
          To obtain the index value for a new entry, the manager
          issues a management protocol retrieval operation to obtain
          the current value of this object.  After each retrieval, the
          agent should modify the value to the next unassigned index
          (or -1)."
          ::= { atmfM4MIBObjects 35 }

atmfM4AlarmSevProfileTable OBJECT-TYPE
          SYNTAX                SEQUENCE OF             AtmfM4AlarmSevProfileEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "The ATM Forum M4 alarm severity profile table.
          This table specifies which profiles exist. Creating
          or deleting an entry in this table automatically
          creates or deletes the corresponding entries in the
          atmfM4AlarmSeverityTable."
          ::= { atmfM4MIBObjects 36 }

atmfM4AlarmSevProfileEntry OBJECT-TYPE
          SYNTAX                AtmfM4AlarmSevProfileEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "A group of severities, one for each alarm type in
          the communications alarm group."
          INDEX                   { atmfM4AlarmSevProfileIndex }
          ::= { atmfM4AlarmSevProfileTable 1 }

AtmfM4AlarmSevProfileEntry ::= SEQUENCE {
          atmfM4AlarmSevProfileIndex                     Integer32,
          atmfM4AlarmSevProfileRowStatus                 RowStatus
                         }

atmfM4AlarmSevProfileIndex OBJECT-TYPE
          SYNTAX                Integer32
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "A number identifying this alarm severity profile."
          ::= { atmfM4AlarmSevProfileEntry 1 }

atmfM4AlarmSevProfileRowStatus OBJECT-TYPE
          SYNTAX                RowStatus
          MAX-ACCESS      read-create
          STATUS                current
          DESCRIPTION
                         "This object is used to create a new row or to delete
          an existing row in the table."
          ::= { atmfM4AlarmSevProfileEntry 2 }


-- ATM Forum M4 Alarm Severity Table

atmfM4AlarmSevTable OBJECT-TYPE
          SYNTAX                SEQUENCE OF             AtmfM4AlarmSevEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "The ATM Forum M4 alarm severity table.
          This table associates profile index and trap
          ID pairs with severities to be used for
          M4 alarm traps that have occurred.
          (Note that this table does not apply to cleared alarms.)"
          ::= { atmfM4MIBObjects 37 }

atmfM4AlarmSevEntry OBJECT-TYPE
          SYNTAX                AtmfM4AlarmSevEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "An entry in this table associates an alarm severity
          profile index/trap ID pair with a severity.
          Deleting a particular profile's row in the alarm severity
          profile table deletes all rows in this table with the
          same profile index.
          Conceptually, rows corresponding to all possible trap ID's
          are created in this table when a new alarm severity profile
          is created, but the agent will return a default value
          except for those few traps for which values have been set."
          INDEX                   { atmfM4AlarmSevProfileIndex,
                                                  atmfM4AlarmSevTrapId }
          ::= { atmfM4AlarmSevTable 1 }

AtmfM4AlarmSevEntry ::= SEQUENCE {
          atmfM4AlarmSevTrapId          Integer32,
          atmfM4AlarmSeverity           AtmfM4AlarmSeverity
                         }

atmfM4AlarmSevTrapId OBJECT-TYPE
          SYNTAX                Integer32
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "The ID of the trap type to which this entry applies."
          ::= { atmfM4AlarmSevEntry 1 }

atmfM4AlarmSeverity OBJECT-TYPE
          SYNTAX                AtmfM4AlarmSeverity
          MAX-ACCESS      read-create
          STATUS                current
          DESCRIPTION
                         "The severity to be used for this trap type when the
          is selected.
          If no value for this object has ever been set since
          the corresponding profile was created, the agent should
          return the value of the object atmfM4AlarmSevDefault"
          ::= { atmfM4AlarmSevEntry 2 }


-- ATM Forum M4 Alarm Forwarding Discriminator Table

atmfM4ForwardAllTraps OBJECT-IDENTITY
          STATUS                current
          DESCRIPTION
                         "This is used as the value of the object
          atmfM4ForwardedTrapObject when traps from all objects
          are to be forwarded, or when there is only one
          object of the type that forwards the specified
          trap type."
          ::= { atmfM4MIBObjects 38 }


atmfM4TrapForwardingTable OBJECT-TYPE
          SYNTAX                SEQUENCE OF             AtmfM4TrapForwardingEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "The ATM Forum M4 Trap forwarding discriminator
          table.
          This table specifies which traps will be sent to
          which management system."
          ::= { atmfM4MIBObjects 39 }

atmfM4TrapForwardingEntry OBJECT-TYPE
          SYNTAX                AtmfM4TrapForwardingEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "Information about a group of traps to be sent to
          a particular IP address.

          A new entry must have values for all attributes that
          do not have default values before its RowStatus column
          can be set to active(1)."
          INDEX                   { atmfM4TrapForwardingIndex }
          ::= { atmfM4TrapForwardingTable 1 }

AtmfM4TrapForwardingEntry ::= SEQUENCE {
          atmfM4TrapForwardingIndex       Integer32,
          atmfM4TrapForwardingDest                IpAddress,
          atmfM4ForwardedTrapId                   Integer32,
          atmfM4ForwardedTrapObject       RowPointer,
          atmfM4TrapForwardingPort                Integer32,
          atmfM4LowestForwardedSeverity AtmfM4AlarmSeverity,
          atmfM4ForwardedIndeterminate  TruthValue,
          atmfM4TrapForwardingRowStatus RowStatus
                         }

atmfM4TrapForwardingIndex OBJECT-TYPE
          SYNTAX                Integer32
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "A unique number identifying the table entry."
          ::= { atmfM4TrapForwardingEntry 1 }

atmfM4TrapForwardingDest OBJECT-TYPE
          SYNTAX                IpAddress
          MAX-ACCESS      read-create
          STATUS                current
          DESCRIPTION
                         "The IP address to which traps identified by this
          table entry should be sent."
          ::= { atmfM4TrapForwardingEntry 2 }

atmfM4ForwardedTrapId OBJECT-TYPE
          SYNTAX                Integer32
          MAX-ACCESS      read-create
          STATUS                current
          DESCRIPTION
                         "The ID of the trap type to which this entry applies."
          ::= { atmfM4TrapForwardingEntry 3 }

atmfM4ForwardedTrapObject OBJECT-TYPE
          SYNTAX                RowPointer
          MAX-ACCESS      read-create
          STATUS                current
          DESCRIPTION
                         "The object to which this entry applies.
          By convention, this is the name of the first object in
          the row in the table referenced.

          The special value { 0 0 } indicates that
          traps of this type from all objects of the type that can
          generate it.  It should also be used when traps from the
          ATM NE are to be specified."
          ::= { atmfM4TrapForwardingEntry 4 }

atmfM4TrapForwardingPort OBJECT-TYPE
          SYNTAX                Integer32
          MAX-ACCESS      read-create
          STATUS                current
          DESCRIPTION
                         "The UDP port on the specified management system to
          which traps identified by this entry should be sent."
          DEFVAL                { 161 }
          ::= { atmfM4TrapForwardingEntry 5 }

atmfM4LowestForwardedSeverity OBJECT-TYPE
          SYNTAX                AtmfM4AlarmSeverity
          MAX-ACCESS      read-create
          STATUS                current
          DESCRIPTION
                         "The lowest severity of traps of this type from
          the specified object that should be sent to this
          address.
          This object has significance only if the trap type
          specified has a severity associated with it"
          DEFVAL                { minor }
          ::= { atmfM4TrapForwardingEntry 6 }

atmfM4ForwardedIndeterminate OBJECT-TYPE
          SYNTAX                TruthValue
          MAX-ACCESS      read-create
          STATUS                current
          DESCRIPTION
                         "When this object has the value TRUE, traps with
          indeterminate severity will be forwarded to the
          specified event.
          This object has significance only if the trap type
          specified has a severity associated with it"
          DEFVAL                { false }
          ::= { atmfM4TrapForwardingEntry 7 }

atmfM4TrapForwardingRowStatus OBJECT-TYPE
          SYNTAX                RowStatus
          MAX-ACCESS      read-create
          STATUS                current
          DESCRIPTION
                         "This object is used to create a new row or to delete
          an existing row in the table."
          ::= { atmfM4TrapForwardingEntry 8 }


-- ATM Forum M4 Trap Agent MIB Log Table

atmfM4TrapLogTable OBJECT-TYPE
          SYNTAX                SEQUENCE OF             AtmfM4TrapLogEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "The ATM Forum M4 Trap Agent log table.
          This table defines the trap logs currently maintained
          by the agent.
          The management system creates entries in this table to
          specify which types of traps, from which ATM network
          elements, should be logged.
          Deleting an entry in this table deletes all entries in
          the corresponding log."
          ::= { atmfM4MIBObjects 40 }

atmfM4TrapLogEntry OBJECT-TYPE
          SYNTAX                AtmfM4TrapLogEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "Information about a single trap log."
          INDEX                   { atmfM4TrapLogSrc,
                                                  atmfM4TrapLogType }
          ::= { atmfM4TrapLogTable 1 }

AtmfM4TrapLogEntry ::= SEQUENCE {
          atmfM4TrapLogSrc                                IpAddress,
          atmfM4TrapLogType                               INTEGER,
          atmfM4TrapLogAdminStatus                INTEGER,
          atmfM4TrapLogOperStatus                 INTEGER,
          atmfM4TrapLogFullAction                 INTEGER,
          atmfM4TrapLogRowStatus                  RowStatus
                         }

atmfM4TrapLogSrc OBJECT-TYPE
          SYNTAX                IpAddress
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "The IP address of the SNMP agent whose traps are
          stored in this log."
          ::= { atmfM4TrapLogEntry 1 }

atmfM4TrapLogType OBJECT-TYPE
          SYNTAX                INTEGER {
                                                  objectCreated(1),
                                                  objectDeleted(2),
                                                  configChange(3),
                                                  stateChange(4),
                                                  alarm(5)
                                                                 }
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "The type of traps stored in this log."
          ::= { atmfM4TrapLogEntry 2 }

atmfM4TrapLogAdminStatus OBJECT-TYPE
          SYNTAX                INTEGER {
                                                  up(1),
                                                  down(2)
                                                                 }
          MAX-ACCESS      read-create
          STATUS                current
          DESCRIPTION
                         "The management system uses this object to stop and
          start the operations of this object."
          DEFVAL                { up }
          ::= { atmfM4TrapLogEntry 3 }

atmfM4TrapLogOperStatus OBJECT-TYPE
          SYNTAX                INTEGER {
                                                  up(1),
                                                  down(2),
                                                  logFull(3)
                                                                 }
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "Indicates whether or not the log is capable of
          performing its normal operations."
          DEFVAL                { up }
          ::= { atmfM4TrapLogEntry 4 }

atmfM4TrapLogFullAction OBJECT-TYPE
          SYNTAX                INTEGER {
                                                  halt(1),
                                                  wrap(2)
                                                                 }
          MAX-ACCESS      read-create
          STATUS                current
          DESCRIPTION
                         "Indicates the action that should be performed when no
          more log entries can be created due to a log-full
          condition.  If the value of this object is wrap(2),
          each new log entry will cause the deletion of the oldest
          entry still in the log, for as long as the log is still
          full."
          DEFVAL                { wrap }
          ::= { atmfM4TrapLogEntry 5 }

atmfM4TrapLogRowStatus OBJECT-TYPE
          SYNTAX                RowStatus
          MAX-ACCESS      read-create
          STATUS                current
          DESCRIPTION
                         "This object is used to create a new row or to delete
          an existing row in the table."
          ::= { atmfM4TrapLogEntry 6 }


-- ATM Forum M4 Trap Agent MIB Logged Trap Table

atmfM4LoggedTrapTable OBJECT-TYPE
          SYNTAX                SEQUENCE OF             AtmfM4LoggedTrapEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "The ATM Forum M4 Trap Agent logged trap table.
          This table is used to maintain the traps logged."
          ::= { atmfM4MIBObjects 41 }

atmfM4LoggedTrapEntry OBJECT-TYPE
          SYNTAX                AtmfM4LoggedTrapEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "Information about a single trap in the log.
          Entries in this table are created automatically but
          can be deleted by the management system.
          Entries that represent 'alarm' log types are augmented
          by the atmfM4LoggedAlarmEntry table."
          INDEX                   { atmfM4TrapLogSrc,
                                                  atmfM4TrapLogType,
                                                  atmfM4LoggedTrapIndex }
          ::= { atmfM4LoggedTrapTable 1 }

AtmfM4LoggedTrapEntry ::= SEQUENCE {
          atmfM4LoggedTrapIndex                   Unsigned32,
          atmfM4LoggedTrapTime                    DateAndTime,
          atmfM4LoggedTrapID                              Integer32,
          atmfM4LoggedTrapObject                  RowPointer,
          atmfM4LoggedTrapRowStatus       RowStatus
                         }

atmfM4LoggedTrapIndex OBJECT-TYPE
          SYNTAX                Unsigned32
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "A unique number identifying this entry in the log.
          When the maximum value for this object has been reached,
          it will wrap around to 0."
          ::= { atmfM4LoggedTrapEntry 1 }

atmfM4LoggedTrapTime OBJECT-TYPE
          SYNTAX                DateAndTime
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "The time at which this trap was logged."
          ::= { atmfM4LoggedTrapEntry 2 }

atmfM4LoggedTrapID OBJECT-TYPE
          SYNTAX                Integer32
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "The type of trap to which this entry applies.
          Together with the logged trap ID object, this object
          specifies the entity to which this logged trap referred."
          ::= { atmfM4LoggedTrapEntry 3 }

atmfM4LoggedTrapObject OBJECT-TYPE
          SYNTAX                RowPointer
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "The object to which this entry applies.
          By convention, this is the name of the first object in
          the row in the table referenced.
          Together with the logged trap ID object, this object
          specifies the entity to which this logged trap referred.

          The special value { 0 0 } indicates that the trap refers
          to the ATM NE entity itself."
          ::= { atmfM4LoggedTrapEntry 4 }

atmfM4LoggedTrapRowStatus OBJECT-TYPE
          SYNTAX                RowStatus
          MAX-ACCESS      read-write
          STATUS                current
          DESCRIPTION
                         "This object is used to delete an existing row in the
          table.  Note that the only value to which a management
          system can set this object is destroy(6)."
          ::= { atmfM4LoggedTrapEntry 5 }


-- ATM Forum M4 Trap Agent MIB Logged Alarm Table

atmfM4LoggedAlarmTable OBJECT-TYPE
          SYNTAX                SEQUENCE OF             AtmfM4LoggedAlarmEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "The ATM Forum M4 Trap Agent logged alarm trap table.
          This table is used to maintain extra information for
          logged traps that represent alarm types."
          ::= { atmfM4MIBObjects 42 }

atmfM4LoggedAlarmEntry OBJECT-TYPE
          SYNTAX                AtmfM4LoggedAlarmEntry
          MAX-ACCESS      not-accessible
          STATUS                current
          DESCRIPTION
                         "Information about the alarm-specific attributes of
          a single trap in the log."
          INDEX                   { atmfM4TrapLogSrc,
                                                  atmfM4TrapLogType,
                                                  atmfM4LoggedTrapIndex }
          ::= { atmfM4LoggedAlarmTable 1 }

AtmfM4LoggedAlarmEntry ::= SEQUENCE {
          atmfM4LoggedAlarmSeverity       AtmfM4AlarmLogSeverity,
          atmfM4LoggedAlarmBackedUp       TruthValue,
          atmfM4LoggedAlarmBUObject       RowPointer,
          atmfM4LoggedAlarmSpecificProb DisplayString,
          atmfM4LoggedAlarmRepairAct      DisplayString
                         }

atmfM4LoggedAlarmSeverity OBJECT-TYPE
          SYNTAX                AtmfM4AlarmLogSeverity
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "The perceived severity of the alarm, as specified by
          the agent that generated it."
          ::= { atmfM4LoggedAlarmEntry 1 }

atmfM4LoggedAlarmBackedUp OBJECT-TYPE
          SYNTAX                TruthValue
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "If the value of this object is true, the agent reported
          in this trap that the failed object had been backed up.

          This object is only present if it was included in the
          alarm trap corresponding to this log entry."
          ::= { atmfM4LoggedAlarmEntry 2 }

atmfM4LoggedAlarmBUObject OBJECT-TYPE
          SYNTAX                RowPointer
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "Indicates the object that provided back-up services to
          the failed object.

          This object is only present if it was included in the
          alarm trap corresponding to this log entry."
          ::= { atmfM4LoggedAlarmEntry 3 }

atmfM4LoggedAlarmSpecificProb OBJECT-TYPE
          SYNTAX                DisplayString
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "Indicates further refinements to the problem identified
          by the alarm type.  If more than one specific problem
          is described in this object, the problem descriptions are
          separated by newline characters.

          This object is only present if it was included in the
          alarm trap corresponding to this log entry."
          ::= { atmfM4LoggedAlarmEntry 4 }

atmfM4LoggedAlarmRepairAct OBJECT-TYPE
          SYNTAX                DisplayString
          MAX-ACCESS      read-only
          STATUS                current
          DESCRIPTION
                         "Indicates proposed repair actions reported by the agent
          for the the problem identified by the alarm.  If more than
          one action is described in this object, the problem
          descriptions are separated by newline characters.

          This object is only present if it was included in the
          alarm trap corresponding to this log entry."
          ::= { atmfM4LoggedAlarmEntry 5 }


-- ATM M4 MIB Notification types

-- Auxiliary definitions for alarms

-- Except for perceived severity, the following objects may be
-- optionally appended to any alarm notification.

atmfM4TrapAlarmSeverity OBJECT-TYPE
          SYNTAX                AtmfM4AlarmLogSeverity
          MAX-ACCESS      accessible-for-notify
          STATUS                current
          DESCRIPTION
                         "The perceived severity of the alarm, as specified by
          the agent that generated it."
          ::= { atmfM4MIBObjects 43 }

atmfM4TrapAlarmBackedUp OBJECT-TYPE
          SYNTAX                TruthValue
          MAX-ACCESS      accessible-for-notify
          STATUS                current
          DESCRIPTION
                         "If the value of this object is true, the failed object
          has been backed up."
          ::= { atmfM4MIBObjects 44 }

atmfM4TrapAlarmBUObject OBJECT-TYPE
          SYNTAX                RowPointer
          MAX-ACCESS      accessible-for-notify
          STATUS                current
          DESCRIPTION
                         "Indicates the object that provided back-up services to
          the failed object."
          ::= { atmfM4MIBObjects 45 }

atmfM4TrapAlarmSpecificProb OBJECT-TYPE
          SYNTAX                DisplayString
          MAX-ACCESS      accessible-for-notify
          STATUS                current
          DESCRIPTION
                         "Indicates further refinements to the problem identified
          by the alarm type.  If more than one specific problem
          is described in this object, the problem descriptions are
          separated by newline characters."
          ::= { atmfM4MIBObjects 46 }

atmfM4TrapAlarmRepairAct OBJECT-TYPE
          SYNTAX                Unsigned32
          MAX-ACCESS      accessible-for-notify
          STATUS                current
          DESCRIPTION
                         "Indicates proposed repair actions reported by the agent
          for the the problem identified by the alarm.  If more than
          one action is described in this object, the problem
          descriptions are separated by newline characters."
          ::= { atmfM4MIBObjects 47 }


-- Comunications Alarms (interface)

atmfM4IfAisAlarm NOTIFICATION-TYPE
          OBJECTS       { ifIndex, atmfM4TrapAlarmSeverity }
          STATUS                current
          DESCRIPTION
                         "Indicates that an AIS alarm condition has occurred
          on the physical path TP associated with the specified
          interface."
          ::= { atmfM4MIBTraps 1 }

atmfM4IfLcdAlarm NOTIFICATION-TYPE
          OBJECTS       { ifIndex, atmfM4TrapAlarmSeverity }
          STATUS                current
          DESCRIPTION
                         "Indicates that an LCD (Loss of Cell Delineation)
          condition has occurred on the TC Adatpr associated
          with the specified interface."
          ::= { atmfM4MIBTraps 2 }

atmfM4IfLofAlarm NOTIFICATION-TYPE
          OBJECTS       { ifIndex, atmfM4TrapAlarmSeverity }
          STATUS                current
          DESCRIPTION
                         "Indicates that an LOF (Loss of Frame)
          condition has occurred on the physical path TP associated
          with the specified interface."
          ::= { atmfM4MIBTraps 3 }

atmfM4IfLopAlarm NOTIFICATION-TYPE
          OBJECTS       { ifIndex, atmfM4TrapAlarmSeverity }
          STATUS                current
          DESCRIPTION
                         "Indicates that an LOP (Loss of Pointer)
          condition has occurred on the physical path TP associated
          with the specified interface."
          ::= { atmfM4MIBTraps 4 }

atmfM4IfLosAlarm NOTIFICATION-TYPE
          OBJECTS       { ifIndex, atmfM4TrapAlarmSeverity }
          STATUS                current
          DESCRIPTION
                         "Indicates that an LOS (Loss of Signal)
          condition has occurred on the physical path TP associated
          with the specified interface."
          ::= { atmfM4MIBTraps 5 }

atmfM4IfPayloadMismatchAlarm NOTIFICATION-TYPE
          OBJECTS       { ifIndex, atmfM4TrapAlarmSeverity }
          STATUS                current
          DESCRIPTION
                         "Indicates that a payload type mismatch condition has
          occurred
          on the physical path TP associated with the specified
          interface."
          ::= { atmfM4MIBTraps 6 }

atmfM4IfXmissionErrAlarm NOTIFICATION-TYPE
          OBJECTS       { ifIndex, atmfM4TrapAlarmSeverity }
          STATUS                current
          DESCRIPTION
                         "Indicates that an transmission error condition has occurred
          on the physical path TP associated with the specified
          interface."
          ::= { atmfM4MIBTraps 7 }

atmfM4IfPathTraceMismatchAlarm NOTIFICATION-TYPE
          OBJECTS       { ifIndex, atmfM4TrapAlarmSeverity }
          STATUS                current
          DESCRIPTION
                         "Indicates that path trace mismatch condition has occurred
          on the physical path TP associated with the specified
          interface."
          ::= { atmfM4MIBTraps 8 }

atmfM4IfRdiAlarm NOTIFICATION-TYPE
          OBJECTS       { ifIndex, atmfM4TrapAlarmSeverity }
          STATUS                current
          DESCRIPTION
                         "Indicates that an RDI (Remote Defect Indication)
          condition has occurred on the physical path TP associated
          with the specified interface."
          ::= { atmfM4MIBTraps 9 }

atmfM4IfSignalLabelMismatchAlarm NOTIFICATION-TYPE
          OBJECTS       { ifIndex, atmfM4TrapAlarmSeverity }
          STATUS                current
          DESCRIPTION
                         "Indicates that a signal label mismatch has occurred
          on the physical path TP associated with the specified
          interface."
          ::= { atmfM4MIBTraps 10 }


--Start of commenting out to get MIB to compile (fah@salix.com)
-- Communications alarms (VPL termination point)
--
--atmfM4VplTpAisAlarm NOTIFICATION-TYPE
--               OBJECTS          { ifIndex, atmVplVpi, atmfM4TrapAlarmSeverity }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that an AIS alarm condition has occurred
--          on the VPL TP associated with the specified
--          interface and VPI."
--               ::= { atmfM4MIBTraps 11 }
--
--atmfM4VplTpRdiAlarm NOTIFICATION-TYPE
--               OBJECTS          { ifIndex, atmVplVpi, atmfM4TrapAlarmSeverity }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that an RDI (Remote Defect Indication)
--          condition has occurred on the VPL TP associated
--          with the specified interface."
--               ::= { atmfM4MIBTraps 12 }
--
--
-- Communications alarms (VPC termination point)
--
--atmfM4VpcTpAisAlarm NOTIFICATION-TYPE
--               OBJECTS          { ifIndex, atmVplVpi, atmfM4TrapAlarmSeverity }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that an AIS alarm condition has occurred
--          on the VPC TP associated with the specified
--          interface and VPI."
--               ::= { atmfM4MIBTraps 13 }
--
--atmfM4VpcTpRdiAlarm NOTIFICATION-TYPE
--               OBJECTS          { ifIndex, atmVplVpi, atmfM4TrapAlarmSeverity }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that an RDI (Remote Defect Indication)
--          condition has occurred on the VPC TP associated
--          with the specified interface."
--               ::= { atmfM4MIBTraps 14 }
--
--
-- Communications alarms (VCL termination point)
--
--atmfM4VclTpAisAlarm NOTIFICATION-TYPE
--               OBJECTS          { ifIndex, atmVclVpi, atmVclVci,
--                                                       atmfM4TrapAlarmSeverity }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that an AIS alarm condition has occurred
--          on the VCL TP associated with the specified
--          interface and VCI."
--               ::= { atmfM4MIBTraps 15 }
--
--atmfM4VclTpRdiAlarm NOTIFICATION-TYPE
--               OBJECTS          { ifIndex, atmVclVpi, atmVclVci,
--                                                       atmfM4TrapAlarmSeverity }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that an RDI (Remote Defect Indication)
--          condition has occurred on the VCL TP associated
--          with the specified interface."
--               ::= { atmfM4MIBTraps 16 }
--
--
-- Communications alarms (VCC termination point)
--
--atmfM4VccTpAisAlarm NOTIFICATION-TYPE
--               OBJECTS          { ifIndex, atmVclVpi, atmVclVci,
--                                                       atmfM4TrapAlarmSeverity }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that an AIS alarm condition has occurred
--          on the VCC TP associated with the specified
--          interface and VCI."
--               ::= { atmfM4MIBTraps 17 }
--
--atmfM4VccTpRdiAlarm NOTIFICATION-TYPE
--               OBJECTS          { ifIndex, atmVclVpi, atmVclVci,
--                                                       atmfM4TrapAlarmSeverity }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that an RDI (Remote Defect Indication)
--          condition has occurred on the VCC TP associated
--          with the specified interface."
--               ::= { atmfM4MIBTraps 18 }
--
--
-- ATM NE and Hardware Unit Alarms
--
--atmfM4HwBackPlaneAlarm NOTIFICATION-TYPE
--               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that a back-plane failure condition
--          has occurred on the hardware unit associated
--          with the specified index.
--          A hardware index of 0 indicates that the error
--          occurred in the ATM NE but not in any one hardware
--          unit maintained in the MIB table."
--               ::= { atmfM4MIBTraps 19 }
--
--atmfM4HwCallEstErrAlarm NOTIFICATION-TYPE
--               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that a call establishment error condition
--          has occurred on the hardware unit associated
--          with the specified index.
--          A hardware index of 0 indicates that the error
--          occurred in the ATM NE but not in any one hardware
--          unit maintained in the MIB table."
--               ::= { atmfM4MIBTraps 20 }
--
--atmfM4HwCongestionAlarm NOTIFICATION-TYPE
--               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that a congestion condition
--          has occurred on the hardware unit associated
--          with the specified index.
--          A hardware index of 0 indicates that the error
--          occurred in the ATM NE but not in any one hardware
--          unit maintained in the MIB table."
--               ::= { atmfM4MIBTraps 21 }
--
--atmfM4HwExtIfDevProbAlarm NOTIFICATION-TYPE
--               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that an external interface device problem
--          has occurred on the hardware unit associated
--          with the specified index.
--          A hardware index of 0 indicates that the error
--          occurred in the ATM NE but not in any one hardware
--          unit maintained in the MIB table."
--               ::= { atmfM4MIBTraps 22 }
--
atmfM4HwLineCardAlarm NOTIFICATION-TYPE
               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
               STATUS   current
               DESCRIPTION
                              "Indicates that a line-card problem condition
          has occurred on the hardware unit associated
          with the specified index.
          A hardware index of 0 indicates that the error
          occurred in the ATM NE but not in any one hardware
          unit maintained in the MIB table."
               ::= { atmfM4MIBTraps 23 }

--atmfM4HwMultiplexerAlarm NOTIFICATION-TYPE
--               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that a multiplexer problem condition
--          has occurred on the hardware unit associated
--          with the specified index.
--          A hardware index of 0 indicates that the error
--          occurred in the ATM NE but not in any one hardware
--          unit maintained in the MIB table."
--               ::= { atmfM4MIBTraps 24 }
--
atmfM4HwPowerAlarm NOTIFICATION-TYPE
               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
               STATUS   current
               DESCRIPTION
                              "Indicates that a power problem alarm condition
          has occurred on the hardware unit associated
          with the specified index.
          A hardware index of 0 indicates that the error
          occurred in the ATM NE but not in any one hardware
          unit maintained in the MIB table."
               ::= { atmfM4MIBTraps 25 }

--atmfM4HwProcessorAlarm NOTIFICATION-TYPE
--               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that a processor problem alarm condition
--          has occurred on the hardware unit associated
--          with the specified index.
--          A hardware index of 0 indicates that the error
--          occurred in the ATM NE but not in any one hardware
--          unit maintained in the MIB table."
--               ::= { atmfM4MIBTraps 26 }
--
--atmfM4HwProtectionPathAlarm NOTIFICATION-TYPE
--               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that a protection path problem condition
--          has occurred on the hardware unit associated
--          with the specified index.
--          A hardware index of 0 indicates that the error
--          occurred in the ATM NE but not in any one hardware
--          unit maintained in the MIB table."
--               ::= { atmfM4MIBTraps 27 }
--
--atmfM4HwReceiverFailAlarm NOTIFICATION-TYPE
--               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that a receiver failure condition
--          has occurred on the hardware unit associated
--          with the specified index.
--          A hardware index of 0 indicates that the error
--          occurred in the ATM NE but not in any one hardware
--          unit maintained in the MIB table."
--               ::= { atmfM4MIBTraps 28 }
--
atmfM4HwPIUnitMissingAlarm NOTIFICATION-TYPE
               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
               STATUS   current
               DESCRIPTION
                              "Indicates that a plug-in unit missing condition
          has occurred on the hardware unit associated
          with the specified index.
          A hardware index of 0 indicates that the error
          occurred in the ATM NE but not in any one hardware
          unit maintained in the MIB table."
               ::= { atmfM4MIBTraps 29 }

atmfM4HwPIUnitProbAlarm NOTIFICATION-TYPE
               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
               STATUS   current
               DESCRIPTION
                              "Indicates that a plug-in unit problem condition
          has occurred on the hardware unit associated
          with the specified index.
          A hardware index of 0 indicates that the error
          occurred in the ATM NE but not in any one hardware
          unit maintained in the MIB table."
               ::= { atmfM4MIBTraps 30 }

atmfM4HwPIUnitMismatchAlarm NOTIFICATION-TYPE
               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
               STATUS   current
               DESCRIPTION
                              "Indicates that a plug-in unit type mismatch condition
          has occurred on the hardware unit associated
          with the specified index.
          A hardware index of 0 indicates that the error
          occurred in the ATM NE but not in any one hardware
          unit maintained in the MIB table."
               ::= { atmfM4MIBTraps 31 }

atmfM4HwTimingProbAlarm NOTIFICATION-TYPE
               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
               STATUS   current
               DESCRIPTION
                              "Indicates that a timing problem alarm condition
          has occurred on the hardware unit associated
          with the specified index.
          A hardware index of 0 indicates that the error
          occurred in the ATM NE but not in any one hardware
          unit maintained in the MIB table."
               ::= { atmfM4MIBTraps 32 }

--atmfM4HwXmitterFailAlarm NOTIFICATION-TYPE
--               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that a transmitter failure condition
--          has occurred on the hardware unit associated
--          with the specified index.
--          A hardware index of 0 indicates that the error
--          occurred in the ATM NE but not in any one hardware
--          unit maintained in the MIB table."
--               ::= { atmfM4MIBTraps 33 }
--
--atmfM4HwTrunkCardAlarm NOTIFICATION-TYPE
--               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that a trunk-card problem condition
--          has occurred on the hardware unit associated
--          with the specified index.
--          A hardware index of 0 indicates that the error
--          occurred in the ATM NE but not in any one hardware
--          unit maintained in the MIB table."
--               ::= { atmfM4MIBTraps 34 }
--
--atmfM4HwStorageCapacityAlarm NOTIFICATION-TYPE
--               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that a storage capacity problem condition
--          has occurred on the hardware unit associated
--          with the specified index.
--          A hardware index of 0 indicates that the error
--          occurred in the ATM NE but not in any one hardware
--          unit maintained in the MIB table."
--               ::= { atmfM4MIBTraps 35 }
--
--atmfM4HwMemoryMismatchAlarm NOTIFICATION-TYPE
--               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that a memory mismatch alarm condition
--          has occurred on the hardware unit associated
--          with the specified index.
--          A hardware index of 0 indicates that the error
--          occurred in the ATM NE but not in any one hardware
--          unit maintained in the MIB table."
--               ::= { atmfM4MIBTraps 36 }
--
--atmfM4HwCorruptDataAlarm NOTIFICATION-TYPE
--               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that a corrupt data alarm condition
--          has occurred on the hardware unit associated
--          with the specified index.
--          A hardware index of 0 indicates that the error
--          occurred in the ATM NE but not in any one hardware
--          unit maintained in the MIB table."
--               ::= { atmfM4MIBTraps 37 }
--
--atmfM4HwSwEnvironAlarm NOTIFICATION-TYPE
--               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that a software environment problem
--          has occurred on the hardware unit associated
--          with the specified index.
--          A hardware index of 0 indicates that the error
--          occurred in the ATM NE but not in any one hardware
--          unit maintained in the MIB table."
--               ::= { atmfM4MIBTraps 38 }
--
atmfM4HwSwDownloadFailAlarm NOTIFICATION-TYPE
               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
               STATUS   current
               DESCRIPTION
                              "Indicates that a software download failure
          has occurred on the hardware unit associated
          with the specified index.
          A hardware index of 0 indicates that the error
          occurred in the ATM NE but not in any one hardware
          unit maintained in the MIB table."
               ::= { atmfM4MIBTraps 39 }

atmfM4HwVersionMismatchAlarm NOTIFICATION-TYPE
               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
               STATUS   current
               DESCRIPTION
                              "Indicates that a version mismatch condition
          has occurred on the hardware unit associated
          with the specified index.
          A hardware index of 0 indicates that the error
          occurred in the ATM NE but not in any one hardware
          unit maintained in the MIB table."
               ::= { atmfM4MIBTraps 40 }

atmfM4HwFanFailAlarm NOTIFICATION-TYPE
               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
               STATUS   current
               DESCRIPTION
                              "Indicates that a cooling fan failure condition
          has occurred on the hardware unit associated
          with the specified index.
          A hardware index of 0 indicates that the error
          occurred in the ATM NE but not in any one hardware
          unit maintained in the MIB table."
               ::= { atmfM4MIBTraps 41 }

--atmfM4HwDoorOpenAlarm NOTIFICATION-TYPE
--               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that an enclosure door open condition
--          has occurred on the hardware unit associated
--          with the specified index.
--          A hardware index of 0 indicates that the error
--          occurred in the ATM NE but not in any one hardware
--          unit maintained in the MIB table."
--               ::= { atmfM4MIBTraps 42 }
--
--atmfM4HwFuseFailAlarm NOTIFICATION-TYPE
--               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that a fuse failure alarm condition
--          has occurred on the hardware unit associated
--          with the specified index.
--          A hardware index of 0 indicates that the error
--          occurred in the ATM NE but not in any one hardware
--          unit maintained in the MIB table."
--               ::= { atmfM4MIBTraps 43 }
--
atmfM4HwHighTempAlarm NOTIFICATION-TYPE
               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
               STATUS   current
               DESCRIPTION
                              "Indicates that a high temperature condition
          has occurred on the hardware unit associated
          with the specified index.
          A hardware index of 0 indicates that the error
          occurred in the ATM NE but not in any one hardware
          unit maintained in the MIB table."
               ::= { atmfM4MIBTraps 44 }

--
-- Software alarms
--
atmfM4SwVersionMismatchAlarm NOTIFICATION-TYPE
               OBJECTS          { entPhysicalIndex, atmfM4HwInstalledSwIndex,
                                                       atmfM4TrapAlarmSeverity }
               STATUS   current
               DESCRIPTION
                              "Indicates that a version mismatch condition
          has occurred on the hardware unit associated
          with the specified index.
          A hardware index of 0 indicates that the error
          occurred in the ATM NE but not in any one hardware
          unit maintained in the MIB table."
               ::= { atmfM4MIBTraps 45 }

--       State change notification traps:

--atmfM4VplTpUp NOTIFICATION-TYPE
--               OBJECTS          { ifIndex, atmVplVpi }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that the operational state of the specified
--          VPL termination point has transitioned to 'up'."
--               ::= { atmfM4MIBTraps 46 }
--
--atmfM4VplTpDown NOTIFICATION-TYPE
--               OBJECTS          { ifIndex, atmVplVpi }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that the operational state of the specified
--          VPL termination point has transitioned to 'down'."
--               ::= { atmfM4MIBTraps 47 }
--
--atmfM4VclTpUp NOTIFICATION-TYPE
--               OBJECTS          { ifIndex, atmVclVpi, atmVclVci }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that the operational state of the specified
--          VCL termination point has transitioned to 'up'."
--               ::= { atmfM4MIBTraps 48 }
--
--atmfM4VclTpDown NOTIFICATION-TYPE
--               OBJECTS          { ifIndex, atmVclVpi, atmVclVci }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that the operational state of the specified
--          VCL termination point has transitioned to 'down'."
--               ::= { atmfM4MIBTraps 49 }
--
--atmfM4VplXConnUp NOTIFICATION-TYPE
--               OBJECTS          { atmVpCrossConnectIndex,
--                                                       atmVpCrossConnectLowIfIndex,
--                                                       atmVpCrossConnectLowVpi,
--                                                       atmVpCrossConnectHighIfIndex,
--                                                       atmVpCrossConnectHighVpi }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that the operational state of the specified
--          VPL cross-connection has transitioned to 'up'."
--               ::= { atmfM4MIBTraps 50 }
--
--atmfM4VplXConnDown NOTIFICATION-TYPE
--               OBJECTS          { atmVpCrossConnectIndex,
--                                                       atmVpCrossConnectLowIfIndex,
--                                                       atmVpCrossConnectLowVpi,
--                                                       atmVpCrossConnectHighIfIndex,
--                                                       atmVpCrossConnectHighVpi }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that the operational state of the specified
--          VPL cross-connection has transitioned to 'down'."
--               ::= { atmfM4MIBTraps 51 }
--
--atmfM4VclXConnUp NOTIFICATION-TYPE
--               OBJECTS          { atmVcCrossConnectIndex,
--                                                       atmVcCrossConnectLowIfIndex,
--                                                       atmVcCrossConnectLowVpi,
--                                                       atmVcCrossConnectLowVci,
--                                                       atmVcCrossConnectHighIfIndex,
--                                                       atmVcCrossConnectHighVpi,
--                                                       atmVcCrossConnectHighVci }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that the operational state of the specified
--          VCL cross-connection has transitioned to 'up'."
--               ::= { atmfM4MIBTraps 52 }
--
--atmfM4VclXConnDown NOTIFICATION-TYPE
--               OBJECTS          { atmVcCrossConnectIndex,
--                                                       atmVcCrossConnectLowIfIndex,
--                                                       atmVcCrossConnectLowVpi,
--                                                       atmVcCrossConnectLowVci,
--                                                       atmVcCrossConnectHighIfIndex,
--                                                       atmVcCrossConnectHighVpi,
--                                                       atmVcCrossConnectHighVci }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that the operational state of the specified
--          VCL cross-connection has transitioned to 'down'."
--               ::= { atmfM4MIBTraps 53 }
--
atmfM4HwUnitUp NOTIFICATION-TYPE
               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
               STATUS   current
               DESCRIPTION
                              "Indicates that the operational state of the specified
          hardware unit has transitioned to 'up'."
               ::= { atmfM4MIBTraps 54 }

atmfM4HwUnitDown NOTIFICATION-TYPE
               OBJECTS          { entPhysicalIndex, atmfM4TrapAlarmSeverity }
               STATUS   current
               DESCRIPTION
                              "Indicates that the operational state of the specified
          hardware unit has transitioned to 'down'."
               ::= { atmfM4MIBTraps 55 }

--
-- Object creation and deletion notification traps:

atmfM4AtmCellIfCreated NOTIFICATION-TYPE
          OBJECTS       { ifIndex, atmfM4IfType }
          STATUS                current
          DESCRIPTION
                         "Indicates that an ATM cell layer interface has just
          been created on the interface."
          ::= { atmfM4MIBTraps 56 }

atmfM4AtmCellIfDeleted NOTIFICATION-TYPE
          OBJECTS       { ifIndex }
          STATUS                current
          DESCRIPTION
                         "Indicates that the ATM cell layer interface has just
          been deleted."
          ::= { atmfM4MIBTraps 57 }

--atmfM4VpcTpCreated NOTIFICATION-TYPE
--               OBJECTS          { ifIndex, atmVplVpi }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that the VPC termination point has just
--          been created."
--               ::= { atmfM4MIBTraps 58 }
--
--atmfM4VpcTpDeleted NOTIFICATION-TYPE
--               OBJECTS          { ifIndex, atmVplVpi }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that the VPC termination point has just
--          been deleted."
--               ::= { atmfM4MIBTraps 59 }
--
--atmfM4VccTpCreated NOTIFICATION-TYPE
--               OBJECTS          { ifIndex, atmVclVpi, atmVclVci }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that the VCC termination point has just
--          been created."
--               ::= { atmfM4MIBTraps 60 }
--
--atmfM4VccTpDeleted NOTIFICATION-TYPE
--               OBJECTS          { ifIndex, atmVclVpi, atmVclVci }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that the VCC termination point has just
--          been deleted."
--               ::= { atmfM4MIBTraps 61 }
--
--atmfM4VplXConnCreated NOTIFICATION-TYPE
--               OBJECTS          { atmVpCrossConnectIndex,
--                                                       atmVpCrossConnectLowIfIndex,
--                                                       atmVpCrossConnectLowVpi,
--                                                       atmVpCrossConnectHighIfIndex,
--                                                       atmVpCrossConnectHighVpi }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that the VPL cross-connection has just
--          been created.  When a cross-connection is created along
--          with its VPL endpoints, this trap should be emitted
--          to indicate the creation of the entire group of objects."
--               ::= { atmfM4MIBTraps 62 }
--
--atmfM4VplXConnDeleted NOTIFICATION-TYPE
--               OBJECTS          { atmVpCrossConnectIndex,
--                                                       atmVpCrossConnectLowIfIndex,
--                                                       atmVpCrossConnectLowVpi,
--                                                       atmVpCrossConnectHighIfIndex,
--                                                       atmVpCrossConnectHighVpi }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that the VPL cross-connection has just
--          been deleted.  When a cross-connection is deleted along
--          with its VPL endpoints, this trap should be emitted
--          to indicate the deletion of the entire group of objects."
--               ::= { atmfM4MIBTraps 63 }
--
--atmfM4VclXConnCreated NOTIFICATION-TYPE
--               OBJECTS          { atmVcCrossConnectIndex,
--                                                       atmVcCrossConnectLowIfIndex,
--                                                       atmVcCrossConnectLowVpi,
--                                                       atmVcCrossConnectLowVci,
--                                                       atmVcCrossConnectHighIfIndex,
--                                                       atmVcCrossConnectHighVpi,
--                                                       atmVcCrossConnectHighVci }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that the VCL cross-connection has just
--          been created.  When a cross-connection is created along
--          with its VCL endpoints, this trap should be emitted
--          to indicate the creation of the entire group of objects."
--               ::= { atmfM4MIBTraps 64 }
--
--atmfM4VclXConnDeleted NOTIFICATION-TYPE
--               OBJECTS          { atmVcCrossConnectIndex,
--                                                       atmVcCrossConnectLowIfIndex,
--                                                       atmVcCrossConnectLowVpi,
--                                                       atmVcCrossConnectLowVci,
--                                                       atmVcCrossConnectHighIfIndex,
--                                                       atmVcCrossConnectHighVpi,
--                                                       atmVcCrossConnectHighVci }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that the VCL cross-connection has just
--          been deleted.  When a cross-connection is deleted along
--          with its VCL endpoints, this trap should be emitted
--          to indicate the deletion of the entire group of objects."
--               ::= { atmfM4MIBTraps 65 }
--
atmfM4HwUnitCreated NOTIFICATION-TYPE
               OBJECTS          { entPhysicalContainedIn,
                                                       entPhysicalParentRelPos,
                                                       entPhysicalClass,
                                                       atmfM4TrapAlarmSeverity}
               STATUS   current
               DESCRIPTION
                              "Indicates that the specified hardware unit has been
          installed at the specified location."
               ::= { atmfM4MIBTraps 66 }

atmfM4HwUnitDeleted NOTIFICATION-TYPE
               OBJECTS          { entPhysicalContainedIn,
                                                       entPhysicalParentRelPos,
                                                       entPhysicalClass,
                                                       atmfM4TrapAlarmSeverity}
               STATUS   current
               DESCRIPTION
                              "Indicates that the specified hardware unit has been
          removed or de-instaleld from the specified location."
               ::= { atmfM4MIBTraps 67 }
--
--atmfM4InstalledSwCreated NOTIFICATION-TYPE
--               OBJECTS          { atmfM4HwInstalledSwHwIndex,
--                                                       hrSWInstalledIndex,
--                                                       hrSWInstalledName }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that the specified software package has been
--          installed."
--               ::= { atmfM4MIBTraps 68 }
--
--atmfM4InstalledSwDeleted NOTIFICATION-TYPE
--               OBJECTS          { atmfM4HwInstalledSwHwIndex,
--                                                       hrSWInstalledIndex,
--                                                       hrSWInstalledName }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that the specified software package has been
--          removed."
--               ::= { atmfM4MIBTraps 69 }
--
--
--       Configuration change notification traps.

atmfM4IfChanged NOTIFICATION-TYPE
          OBJECTS       { ifIndex }
          STATUS                current
          DESCRIPTION
                         "Indicates that the configuration of the interface has
          been changed."
          ::= { atmfM4MIBTraps 70 }

--atmfM4VplTpChanged NOTIFICATION-TYPE
--               OBJECTS          { ifIndex, atmVplVpi }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that the VPL termination point config. has
--          been changed."
--               ::= { atmfM4MIBTraps 71 }
--
--atmfM4VclTpChanged NOTIFICATION-TYPE
--               OBJECTS          { ifIndex, atmVclVpi, atmVclVci }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that the VCL termination point config. has
--          been changed."
--               ::= { atmfM4MIBTraps 72 }
--
--atmfM4VplXConnChanged NOTIFICATION-TYPE
--               OBJECTS          { atmVpCrossConnectIndex,
--                                                       atmVpCrossConnectLowIfIndex,
--                                                       atmVpCrossConnectLowVpi,
--                                                       atmVpCrossConnectHighIfIndex,
--                                                       atmVpCrossConnectHighVpi }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that the VPL cross-connection config. has
--          been changed."
--               ::= { atmfM4MIBTraps 73 }
--
--atmfM4VclXConnChanged NOTIFICATION-TYPE
--               OBJECTS          { atmVcCrossConnectIndex,
--                                                       atmVcCrossConnectLowIfIndex,
--                                                       atmVcCrossConnectLowVpi,
--                                                       atmVcCrossConnectLowVci,
--                                                       atmVcCrossConnectHighIfIndex,
--                                                       atmVcCrossConnectHighVpi,
--                                                       atmVcCrossConnectHighVci }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that the VCL cross-connection config. has
--          been changed."
--               ::= { atmfM4MIBTraps 74 }
--
--atmfM4HwUnitChanged NOTIFICATION-TYPE
--               OBJECTS          { entPhysicalIndex }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that the specified hardware unit config.
--          has changed."
--               ::= { atmfM4MIBTraps 75 }
--
--atmfM4InstalledSwChanged NOTIFICATION-TYPE
--               OBJECTS          { hrSWInstalledIndex }
--               STATUS   current
--               DESCRIPTION
--                              "Indicates that the specified software package config.
--          has changed."
--               ::= { atmfM4MIBTraps 76 }
--
--
-- Conformance statements


atmfM4Groups                            OBJECT IDENTIFIER ::= { atmfM4MIBCompliance 1 }
atmfM4Compliances                       OBJECT IDENTIFIER ::= { atmfM4MIBCompliance 2 }

-- compliance statements

atmfM4Compliance                        MODULE-COMPLIANCE
                  STATUS         current
                  DESCRIPTION
                                         "The compliance statements are listed as a set up conformance units
                that correspond to each table. Support for all tables is mandatory."
                  MODULE         -- this module
                                         MANDATORY-GROUPS {atmfM4General, atmfM4PhysPathTpGroup, atmfM4TcAdaptorGroup,
                                         atmfM4AtmLayerGroup, atmfM4VplGroup, atmfM4VclGroup, atmfM4VpXConnGroup,
                                         atmfM4VcXConnGroup, atmfM4VpNextVpiGroup, atmfM4VcNextVciGroup,
                                         atmfM4CellProtoCurrGroup, atmfM4CellProtoHistGroup, atmfM4CellProtoErrorGroup,
                                         atmfM4TcProtoCurrGroup, atmfM4TcProtoHistGroup, atmfM4VpUpcNpcCurrGroup,
                                         atmfM4VpUpcNpcHistGroup, atmfM4VcUpcNpcCurrGroup, atmfM4VcUpcNpcHistGroup,
                                         atmfM4VpTestGroup, atmfM4VcTestGroup, atmfM4EquipGroup, atmfM4EquipHolderGroup,
                                         atmfM4PlugInUnitGroup, atmfM4HwRunningSwGroup, atmfM4HwInstalledSwGroup,
                                         atmfM4AlarmSevGroup, atmfM4TrapForwardingGroup,
                                         atmfM4TrapLogGroup, atmfM4LoggedTrapGroup, atmfM4LoggedAlarmGroup}
                  ::= { atmfM4Compliances 1 }
-- Replace 3 lines below with line 2 lines above
--                                       atmfM4TrapLogGroup, atmfM4LoggedTrapGroup, atmfM4LoggedAlarmGroup,
--                                       atmfM4NotificationsGroup}
--                ::= { atmfM4Compliances 1 }

-- units of conformance

atmfM4General    OBJECT-GROUP
                  OBJECTS {atmfM4NeVendor, atmfM4NeVersion, atmfM4NeStartTime, atmfM4NeAlarmSeverityIndex, atmfM4NeSuppressZeroStats}
                  STATUS         current
                  DESCRIPTION
                                         "NE high level objects"
                  ::= { atmfM4Groups 1}

atmfM4PhysPathTpGroup   OBJECT-GROUP
                  OBJECTS {atmfM4PhysPathTpHwUnitIndex, atmfM4PhysPathTpPortID,
                                          atmfM4PhysPathTpAlarmSeverityIndex}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 interface Configuration table extensions
                for the physical path termination point"
                  ::= { atmfM4Groups 2 }

atmfM4TcAdaptorGroup            OBJECT-GROUP
                  OBJECTS {atmfM4TcACellScrambling, atmfM4TcAlarmSeverityIndex}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 interface Configuration table extensions
                for the TC Adaptor."
                  ::= { atmfM4Groups 3 }

atmfM4AtmLayerGroup             OBJECT-GROUP
                  OBJECTS {atmfM4IfType, atmfM4IfLoopbackLocationCode, atmfM4IfSubscriberAddress,
                                          atmfM4IfPreferredCarrier, atmfM4IfFarEndCarrierNetwork}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 interface Configuration table extensions
                for the ATM cell layer."
                  ::= { atmfM4Groups 4 }

atmfM4VplGroup   OBJECT-GROUP
                  OBJECTS {atmfM4VplSegEndPt}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 VPL Termination Point Configuration
                 table extensions. "
                  ::= { atmfM4Groups 5 }

atmfM4VclGroup   OBJECT-GROUP
                  OBJECTS {atmfM4VclSegEndPt}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 VCL Termination Point Configuration
                table extensions."
                  ::= { atmfM4Groups 6 }

atmfM4VpXConnGroup              OBJECT-GROUP
                  OBJECTS {atmfM4VpXConnRecover}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 VP Cross-Connect Configuration
                table extensions."
                  ::= { atmfM4Groups 7 }

atmfM4VcXConnGroup              OBJECT-GROUP
                  OBJECTS {atmfM4VcXConnRecover}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 VC Cross-Connect Configuration
                table extensions."
                  ::= { atmfM4Groups 8 }

atmfM4VpNextVpiGroup            OBJECT-GROUP
                  OBJECTS {atmfM4VpNextVpiValue}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 VP Next-VPI value table."
                  ::= { atmfM4Groups 9 }

atmfM4VcNextVciGroup            OBJECT-GROUP
                  OBJECTS {atmfM4VcNextVciValue}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 VC Next-VCI value table."
                  ::= { atmfM4Groups 10 }

atmfM4CellProtoCurrGroup                  OBJECT-GROUP
                  OBJECTS {atmfM4CellProtoCurrSuspect, atmfM4CellProtoCurrElapsedTime,
                                          atmfM4CellProtoCurrSupprIntvls, atmfM4CellProtoCurrProtoErrors,
                                          atmfM4CellProtoCurrInOAMCells}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 Cell Protocol Monitoring Current Data
                 table."
                  ::= { atmfM4Groups 11 }

atmfM4CellProtoHistGroup                  OBJECT-GROUP
                  OBJECTS {atmfM4CellProtoHistSuspect, atmfM4CellProtoHistElapsedTime,
                                          atmfM4CellProtoHistSupprIntvls, atmfM4CellProtoHistProtoErrors,
                                          atmfM4CellProtoHistInOAMCells}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 Cell Protocol Monitoring History Data
                table."
                  ::= { atmfM4Groups 12 }

atmfM4CellProtoErrorGroup                 OBJECT-GROUP
                  OBJECTS {atmfM4CellProtoErrorTime, atmfM4CellProtoErrorReason,
                                          atmfM4CellProtoErrorVpi, atmfM4CellProtoErrorVci}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 Cell Protocol Monitoring Error Log
                table."
                  ::= { atmfM4Groups 13 }

atmfM4TcProtoCurrGroup  OBJECT-GROUP
                  OBJECTS {atmfM4TcProtoCurrSuspect, atmfM4TcProtoCurrElapsedTime,
                                          atmfM4TcProtoCurrSupprIntvls, atmfM4TcProtoCurrDiscardHECViol}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 TC Adaptor Protocol Monitoring Current
                Data table."
                  ::= { atmfM4Groups 14 }

atmfM4TcProtoHistGroup  OBJECT-GROUP
                  OBJECTS {atmfM4TcProtoHistSuspect, atmfM4TcProtoHistElapsedTime,
                                          atmfM4TcProtoHistSupprIntvls, atmfM4TcProtoHistDiscardHECViol}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 TC Adaptor Protocol Monitoring History
                Data table."
                  ::= { atmfM4Groups 15 }

atmfM4VpUpcNpcCurrGroup OBJECT-GROUP
                  OBJECTS {atmfM4VpUpcNpcCurrSuspect, atmfM4VpUpcNpcCurrElapsedTime,
                                          atmfM4VpUpcNpcCurrSupprIntvls, atmfM4VpUpcNpcCurrDiscardedCells,
                                          atmfM4VpUpcNpcCurrDiscardedClp0, atmfM4VpUpcNpcCurrPassedCells,
                                          atmfM4VpUpcNpcCurrPassedClp0}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 UPC/NPC Disagreement Monitoring Current
                Data table for VPL termination points."
                  ::= { atmfM4Groups 16 }

atmfM4VpUpcNpcHistGroup OBJECT-GROUP
                  OBJECTS {atmfM4VpUpcNpcHistSuspect, atmfM4VpUpcNpcHistElapsedTime,
                                          atmfM4VpUpcNpcHistSupprIntvls, atmfM4VpUpcNpcHistDiscardedCells,
                                          atmfM4VpUpcNpcHistDiscardedClp0, atmfM4VpUpcNpcHistPassedCells,
                                          atmfM4VpUpcNpcHistPassedClp0}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 UPC/NPC Disagreement Monitoring History
                Data table for VPL termination points."
                  ::= { atmfM4Groups 17 }

atmfM4VcUpcNpcCurrGroup OBJECT-GROUP
                  OBJECTS {atmfM4VcUpcNpcCurrSuspect, atmfM4VcUpcNpcCurrElapsedTime,
                                          atmfM4VcUpcNpcCurrSupprIntvls, atmfM4VcUpcNpcCurrDiscardedCells,
                                          atmfM4VcUpcNpcCurrDiscardedClp0, atmfM4VcUpcNpcCurrPassedCells,
                                          atmfM4VcUpcNpcCurrPassedClp0}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 UPC/NPC Disagreement Monitoring Current
                Data table for VCL termination points"
                  ::= { atmfM4Groups 18 }

atmfM4VcUpcNpcHistGroup OBJECT-GROUP
                  OBJECTS {atmfM4VcUpcNpcHistSuspect, atmfM4VcUpcNpcHistElapsedTime,
                                          atmfM4VcUpcNpcHistSupprIntvls, atmfM4VcUpcNpcHistDiscardedCells,
                                          atmfM4VcUpcNpcHistDiscardedClp0, atmfM4VcUpcNpcHistPassedCells,
                                          atmfM4VcUpcNpcHistPassedClp0}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 UPC/NPC Disagreement Monitoring History
                Data table for VCL termination points."
                  ::= { atmfM4Groups 19 }

atmfM4VpTestGroup                       OBJECT-GROUP
                  OBJECTS {atmfM4VpTestId, atmfM4VpTestStatus, atmfM4VpTestType,
                                          atmfM4VpTestResult, atmfM4VpTestCode, atmfM4VpTestOwner}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 VP Termination Point Test table."
                  ::= { atmfM4Groups 20 }

atmfM4VcTestGroup                       OBJECT-GROUP
                  OBJECTS {atmfM4VcTestId, atmfM4VcTestStatus, atmfM4VcTestType,
                                          atmfM4VcTestResult, atmfM4VcTestCode, atmfM4VcTestOwner}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 VC Termination Point Test table."
                  ::= { atmfM4Groups 21 }

atmfM4EquipGroup                        OBJECT-GROUP
                  OBJECTS {atmfM4EquipAdminStatus, atmfM4EquipLocation, atmfM4EquipOperStatus,
                                          atmfM4EquipVendor, atmfM4EquipVersion, atmfM4EquipUserLabel,
                                          atmfM4EquipAlarmSeverityIndex}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 Equipment table."
                  ::= { atmfM4Groups 22 }

atmfM4EquipHolderGroup  OBJECT-GROUP
                  OBJECTS {atmfM4EquipHolderType, atmfM4EquipHolderAcceptableTypes,
                                          atmfM4EquipHolderSlotStatus, atmfM4EquipHolderSwLoad}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 Equipment Holder table."
                  ::= { atmfM4Groups 23 }

atmfM4PlugInUnitGroup   OBJECT-GROUP
                  OBJECTS {atmfM4PlugInUnitAdminStatus, atmfM4PlugInUnitAvailStatus,
                                          atmfM4PlugInUnitOperStatus, atmfM4PlugInUnitVendor, atmfM4PlugInUnitVersion,
                                          atmfM4PlugInUnitAlarmSeverityIndex}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 Plug-In Unit table."
                  ::= { atmfM4Groups 24 }

atmfM4HwRunningSwGroup  OBJECT-GROUP
                  OBJECTS {atmfM4HwRunningSwSwIndex}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 Hardware Unit/Running Software
                table."
                  ::= { atmfM4Groups 25 }

atmfM4HwInstalledSwGroup                  OBJECT-GROUP
                  OBJECTS {atmfM4HwInstalledSwSwIndex, atmfM4HwSwAlarmSeverityIndex}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 Hardware Unit/Installed Software
                table"
                  ::= { atmfM4Groups 26 }

atmfM4AlarmSevGroup             OBJECT-GROUP
                  OBJECTS {atmfM4AlarmSevProfileRowStatus, atmfM4AlarmSeverity, atmfM4AlarmSevDefault,
                                          atmfM4AlarmSevProfileIndexNext }
                  STATUS         current
                  DESCRIPTION
                                         "Alarm handling objects"
                  ::= { atmfM4Groups 27 }

atmfM4TrapForwardingGroup                 OBJECT-GROUP
                  OBJECTS {atmfM4TrapForwardingDest, atmfM4ForwardedTrapId, atmfM4ForwardedTrapObject,
                                          atmfM4TrapForwardingPort, atmfM4LowestForwardedSeverity,
                                          atmfM4ForwardedIndeterminate, atmfM4TrapForwardingRowStatus}
                  STATUS         current
                  DESCRIPTION
                                         "Trap forwarding table"
                  ::= { atmfM4Groups 28 }

atmfM4TrapLogGroup              OBJECT-GROUP
                  OBJECTS {atmfM4TrapLogAdminStatus, atmfM4TrapLogOperStatus, atmfM4TrapLogFullAction,
                                          atmfM4TrapLogRowStatus}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 Trap Agent log table."
                  ::= { atmfM4Groups 29 }

atmfM4LoggedTrapGroup   OBJECT-GROUP
                  OBJECTS {atmfM4LoggedTrapTime, atmfM4LoggedTrapID, atmfM4LoggedTrapObject,
                                          atmfM4LoggedTrapRowStatus}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 Trap Agent logged trap table."
                  ::= { atmfM4Groups 30 }

atmfM4LoggedAlarmGroup  OBJECT-GROUP
                  OBJECTS {atmfM4LoggedAlarmSeverity, atmfM4LoggedAlarmBackedUp, atmfM4LoggedAlarmBUObject,
                                          atmfM4LoggedAlarmSpecificProb, atmfM4LoggedAlarmRepairAct,
                                          atmfM4TrapAlarmSeverity, atmfM4TrapAlarmBackedUp, atmfM4TrapAlarmBUObject,
                                          atmfM4TrapAlarmSpecificProb, atmfM4TrapAlarmRepairAct}
                  STATUS         current
                  DESCRIPTION
                                         "The ATM Forum M4 Trap Agent logged alarm trap table."
                  ::= { atmfM4Groups 31 }

--atmfM4NotificationsGroup                       NOTIFICATION-GROUP
--                       NOTIFICATIONS {atmfM4IfAisAlarm, atmfM4IfLcdAlarm, atmfM4IfLofAlarm, atmfM4IfLopAlarm,
--                                               atmfM4IfLosAlarm, atmfM4IfPayloadMismatchAlarm, atmfM4IfXmissionErrAlarm,
--                                               atmfM4IfPathTraceMismatchAlarm, atmfM4IfRdiAlarm,
--                                               atmfM4IfSignalLabelMismatchAlarm, atmfM4VplTpAisAlarm, atmfM4VplTpRdiAlarm,
--                                               atmfM4VpcTpAisAlarm, atmfM4VpcTpRdiAlarm, atmfM4VclTpAisAlarm,
--                                               atmfM4VclTpRdiAlarm, atmfM4VccTpAisAlarm, atmfM4VccTpRdiAlarm,
--                                               atmfM4HwBackPlaneAlarm, atmfM4HwCallEstErrAlarm, atmfM4HwCongestionAlarm,
--                                               atmfM4HwExtIfDevProbAlarm, atmfM4HwLineCardAlarm, atmfM4HwMultiplexerAlarm,
--                                               atmfM4HwPowerAlarm, atmfM4HwProcessorAlarm, atmfM4HwProtectionPathAlarm,
--                                               atmfM4HwReceiverFailAlarm, atmfM4HwPIUnitMissingAlarm, atmfM4HwPIUnitProbAlarm,
--                                               atmfM4HwPIUnitMismatchAlarm, atmfM4HwTimingProbAlarm, atmfM4HwXmitterFailAlarm,
--                                               atmfM4HwTrunkCardAlarm, atmfM4HwStorageCapacityAlarm,
--                                               atmfM4HwMemoryMismatchAlarm, atmfM4HwCorruptDataAlarm, atmfM4HwSwEnvironAlarm,
--                                               atmfM4HwSwDowloadFailAlarm, atmfM4HwVersionMismatchAlarm, atmfM4HwFanFailAlarm,
--                                               atmfM4HwDoorOpenAlarm, atmfM4HwFuseFailAlarm, atmfM4HwHighTempAlarm,
--                                               atmfM4SwVersionMismatchAlarm, atmfM4VplTpUp, atmfM4VplTpDown, atmfM4VclTpUp,
--                                               atmfM4VclTpDown, atmfM4VplXConnUp, atmfM4VplXConnDown, atmfM4VclXConnUp,
--                                               atmfM4VclXConnDown, atmfM4HwUnitUp, atmfM4HwUnitDown, atmfM4AtmCellIfCreated,
--                                               atmfM4AtmCellIfDeleted, atmfM4VpcTpCreated, atmfM4VpcTpDeleted,
--                                               atmfM4VccTpCreated, atmfM4VccTpDeleted, atmfM4VplXConnCreated,
--                                               atmfM4VplXConnDeleted, atmfM4VclXConnCreated, atmfM4VclXConnDeleted,
--                                               atmfM4HwUnitCreated, atmfM4HwUnitDeleted, atmfM4InstalledSwCreated,
--                                               atmfM4InstalledSwDeleted, atmfM4IfChanged, atmfM4VplTpChanged,
--                                               atmfM4VclTpChanged, atmfM4VplXConnChanged, atmfM4VclXConnChanged,
--                                               atmfM4HwUnitChanged, atmfM4InstalledSwChanged }
--                       STATUS current
--                       DESCRIPTION
--                                              "The ATM Forum M4 notification list."
--                       ::= { atmfM4Groups 32 }

END

