	DEVBASE-MIB DEFINITIONS ::= BEGIN

	IMPORTS
		OBJECT-TYPE, MODULE-IDENTITY, IpAddress
			FROM SNMPv2-SMI
		DisplayString, MacAddress
			FROM SNMPv2-TC
		device
			FROM ANIROOT-MIB;

-- Device Mib (Common to BSU/SU)

aniDevBase  MODULE-IDENTITY
	LAST-UPDATED "0105091130Z"      -- Wed May 9 11:30:00 PDT 2001
	ORGANIZATION "Aperto Networks"
	CONTACT-INFO
	  "       
	  Postal:  Aperto Networks Inc
		   1637 S Main Street 
		   Milpitas, California 95035
	  Tel:	   +1 408 719 9977
	  "       
	DESCRIPTION
	"This group gives some basic information about the device 
	 (BSU or SU). 
	 All objects within this group are applicable to both the devices. 
	"
	::= { device 1 }

aniDevProductName OBJECT-TYPE
	SYNTAX      DisplayString (SIZE (0..64))
	MAX-ACCESS  read-only
	STATUS      current
	DESCRIPTION
	   "The model number of the device.
	   "
	--DEFAULT next-function-async     std_next_async
	::= { aniDevBase 1 }

aniDevLanIpAddr OBJECT-TYPE 
	SYNTAX      IpAddress
	MAX-ACCESS  read-only
	STATUS      current
	DESCRIPTION
	   "The Lan IP Address of the device."
	--DEFAULT next-function-async     std_next_async
	::= { aniDevBase 2 }

aniDevLanSubnetMask  OBJECT-TYPE 
	SYNTAX      IpAddress
	MAX-ACCESS  read-only
	STATUS      current
	DESCRIPTION
	   "The subnet mask of the device."
	--DEFAULT next-function-async     std_next_async
	::= { aniDevBase 3 }

aniDevDefaultGateway  OBJECT-TYPE	
	SYNTAX      IpAddress
	MAX-ACCESS  read-only
	STATUS      current
	DESCRIPTION
	   "The Gateway IP address.
	    On BSU, this refers to the Lan Gateway address.
	    On SU, this refers to the Wireless Gateway address.
	   "
	--DEFAULT next-function-async     std_next_async
	::= { aniDevBase 4 }

aniDevMacAddr OBJECT-TYPE 
	SYNTAX      MacAddress
	MAX-ACCESS  read-only
	STATUS      current
	DESCRIPTION
	   "The Mac Address of the device."
	--DEFAULT next-function-async     std_next_async
	::= { aniDevBase 5 }

END


