	F10-LINK-AGGREGATION-MIB DEFINITIONS ::= BEGIN

	--  Force10 Networks, Inc.
	--  1440 McCarthy Blvd
	--  Milpitas, CA 95035-7438

	--  This module provides authoritative definitions for Force10
	--  enterprise Link Aggregation Mib.
	--
	--  This module will be extended, as needed.
	--

	IMPORTS
		MODULE-IDENTITY, OBJECT-TYPE, 
		Integer32 
			FROM SNMPv2-SMI
		MacAddress
			FROM SNMPv2-TC
		MODULE-COMPLIANCE, OBJECT-GROUP
			FROM SNMPv2-CONF
		f10Mgmt
			FROM FORCE10-SMI
		PortList		
			FROM FORCE10-TC;
		
	
	f10LinkAggMib MODULE-IDENTITY
	LAST-UPDATED "0308010000Z"  -- Auguest 1, 2003
	ORGANIZATION
	  "Force10 Networks, Inc."
	CONTACT-INFO
	  "Force10 Networks, Inc
	   1440 McCarthy Blvd
	   Milpitas, CA 95035
	   (408) 571-3500
	   support@force10networks.com
	   http://www.force10networks.com"

	DESCRIPTION
	   "Force10 Enterprise Link Aggregation MIB. "

	REVISION     "0308010000Z"
	DESCRIPTION
		"Force10 Link Aggreagation MIB version 1.3.
		  - Add FDB common table for configured or negotiated link aggregation"

	REVISION     "0308010000Z"
	DESCRIPTION
		"1. Move textual conventions to the Textual-Convention MIB f10-tc.mib.
		 2. Rename dot3aClearCurAggFdb to dot3aClearFdb."

	REVISION     "0203120000Z"
	DESCRIPTION
		"Force10 Link Aggreagation MIB version 1.1.
		Deprecated dot3aAggStaticTable & dot3aAggFdbTable
		Added dot3aCurAggStaticTable & dot3aCurAggFdbTable
		because of indexing changes"

	REVISION     "0011210000Z"
	DESCRIPTION
          "Force10 Link Aggreagation MIB version 1.0."

	REVISION     "0103010000Z"
	DESCRIPTION
          "First revision of Force10 link aggregation mib."

           ::= { f10Mgmt 2 }   


	-- ### Groups ###

	f10LinkAggObjects OBJECT IDENTIFIER ::={ f10LinkAggMib 1 }

        f10dot3dAgg	OBJECT IDENTIFIER ::={ f10LinkAggObjects 1 }
        f10LinkAggMgmt	OBJECT IDENTIFIER ::={ f10LinkAggObjects 2 }


	-- ### Aggregation Configuration Port List Table 

	   dot3aAggConfigTable	OBJECT-TYPE
		SYNTAX		SEQUENCE OF Dot3aAggConfigEntry
		MAX-ACCESS	not-accessible
		STATUS		current
		DESCRIPTION
			"A list of all aggregated links configured."
		::= { f10dot3dAgg 1 }

	  dot3aAggConfigEntry	OBJECT-TYPE 
		SYNTAX		Dot3aAggConfigEntry
		MAX-ACCESS	not-accessible
		STATUS		current
		DESCRIPTION
			"A list of all aggregated links configured 
			in the system"
		INDEX	{ dot3aAggCfgId }
		::= { dot3aAggConfigTable 1 }

	  Dot3aAggConfigEntry	::=
		SEQUENCE {
		   dot3aAggCfgId			    Integer32,
		   dot3aAggCfgMacAddr		    MacAddress,		
		   dot3aAggCfgIfIndex		    Integer32,
		   dot3aAggCfgNumPorts		    Integer32,
		   dot3aAggCfgPortList		    PortList,
		   dot3aAggCfgPortListString    OCTET STRING
		}

	   dot3aAggCfgId	OBJECT-TYPE
		SYNTAX		Integer32
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
		"The link aggregation id or port channel id."
		::= { dot3aAggConfigEntry 1 }

	   dot3aAggCfgMacAddr	OBJECT-TYPE
		SYNTAX		MacAddress
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
		"A 6-octet read only value MAC Address assigned 
		 to this link aggregation or user-defined MAC address
		 if a static user-defined MAC address is configured."
		::= { dot3aAggConfigEntry 2 }

	   dot3aAggCfgIfIndex	OBJECT-TYPE
		SYNTAX		Integer32
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
		"The logical interface index assigned to this 
		 link aggregation."
		::= { dot3aAggConfigEntry 3 }

	   dot3aAggCfgNumPorts	OBJECT-TYPE
		SYNTAX		Integer32
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
		"The number of physical ports configured to this 
		 link aggregation. Maximum is 16 ports"
		::= { dot3aAggConfigEntry 4 }

	   dot3aAggCfgPortList	OBJECT-TYPE
		SYNTAX		PortList
		MAX-ACCESS	read-only
		STATUS		current
		DESCRIPTION
        	"The bitmask of ports configured for this link aggregation.
            This object is deprecated and no longer in use. Please use the new
            dot3aAggCfgPortListString object instead.
            " 
		::= { dot3aAggConfigEntry 5 }

	   dot3aAggCfgPortListString	OBJECT-TYPE
		SYNTAX		OCTET STRING 
		MAX-ACCESS  read-only
		STATUS		deprecated
		DESCRIPTION
        "The list of ports configured for this link aggregation.
		 The format of this output is as follows:
		 <interface type> <slot/port>, or 
		 <port channel> <number>"
		::= { dot3aAggConfigEntry 6 }




        -- ### Aggregation MAC Addr Table

           dot3aAggStaticTable  OBJECT-TYPE
            SYNTAX          SEQUENCE OF Dot3aAggStaticEntry
            MAX-ACCESS      not-accessible
		STATUS          current
		DESCRIPTION
		"A list of statically configured MAC Address on the aggregated links."
            ::= { f10dot3dAgg 2 }

          dot3aAggStaticEntry   OBJECT-TYPE
            SYNTAX          Dot3aAggStaticEntry
            MAX-ACCESS      not-accessible
            STATUS          deprecated
            DESCRIPTION
            "A list of statically configured MAC Address on the aggregated links in the system"
            INDEX   { dot3aAggIndex, dot3aAggVlanId, dot3aAggMacAddr }
            ::= { dot3aAggStaticTable 1 }

          Dot3aAggStaticEntry   ::=
            SEQUENCE {
               dot3aAggIndex              Integer32,
               dot3aAggVlanId             Integer32,
		   dot3aAggMacAddr	      MacAddress,		
		   dot3aAggStatus			INTEGER,		
		   dot3aAggDistributedPort	OCTET STRING	
            }

	   dot3aAggIndex	OBJECT-TYPE
		SYNTAX		Integer32
		MAX-ACCESS      read-only
		STATUS		deprecated
		DESCRIPTION
		"The link aggregation id or port channel id."
		::= { dot3aAggStaticEntry 1 }

	   dot3aAggVlanId	OBJECT-TYPE
		SYNTAX		Integer32 
		MAX-ACCESS      read-only
		STATUS		deprecated
		DESCRIPTION
		"VLAN id that this ports configured to ."
		::= { dot3aAggStaticEntry 2 }

	   dot3aAggMacAddr	OBJECT-TYPE
		SYNTAX		MacAddress
		MAX-ACCESS      read-only
		STATUS		deprecated
		DESCRIPTION
		"A 6-octet read only value MAC Address assigned 
		 to this link aggregation or user-defined MAC address
		 if a static user-defined MAC address is configured."
		::= { dot3aAggStaticEntry 3 }

	   dot3aAggStatus	OBJECT-TYPE
		SYNTAX		INTEGER {
				   	active(1),
				   	inactive(2)
					}	  
		MAX-ACCESS	read-only
		STATUS		deprecated
		DESCRIPTION
		"The status of this aggregation link .
		 active - this aggregation link is active.
		 inactive  - this aggregation link is no active." 
		::= { dot3aAggStaticEntry 4 }

	   dot3aAggDistributedPort	OBJECT-TYPE
		SYNTAX		OCTET STRING 
		MAX-ACCESS      read-only
		STATUS		deprecated
		DESCRIPTION
		"The interface of the MAC address.
		 The format of this output is as follows:
		 <interface type> <slot/port>, or 
		 <port channel> <number>"
		::= { dot3aAggStaticEntry 5 }


        -- ### Aggregation Dynamic FDB Table

           dot3aAggFdbTable  OBJECT-TYPE
            SYNTAX          SEQUENCE OF Dot3aAggFdbEntry
            MAX-ACCESS      not-accessible
		STATUS          current
		DESCRIPTION
		"A list of dynamically learned Mac Address on the aggregated links"
                ::= { f10dot3dAgg 3 }

          dot3aAggFdbEntry   OBJECT-TYPE
            SYNTAX          Dot3aAggFdbEntry
            MAX-ACCESS      not-accessible
            STATUS          deprecated
            DESCRIPTION
            "A list of dynamically learned Mac Address on the aggregated links in the system"
            INDEX   { dot3aAggFdbIndex, dot3aAggFdbVlanId, dot3aAggFdbMacAddr }
            ::= { dot3aAggFdbTable 1 }

          Dot3aAggFdbEntry   ::=
            SEQUENCE {
             dot3aAggFdbIndex        	Integer32,
             dot3aAggFdbVlanId       	Integer32,
	       dot3aAggFdbMacAddr      	MacAddress,		
	       dot3aAggFdbStatus       	INTEGER,		
	       dot3aAggFdbDistributedPort	OCTET STRING	
            }

	   dot3aAggFdbIndex	OBJECT-TYPE
		SYNTAX		Integer32
		MAX-ACCESS      read-only
		STATUS		deprecated
		DESCRIPTION
		"The FDB link aggregation id or port channel id."
		::= { dot3aAggFdbEntry 1 }

	   dot3aAggFdbVlanId	OBJECT-TYPE
		SYNTAX		Integer32
		MAX-ACCESS      read-only
		STATUS		deprecated
		DESCRIPTION
		"The forwarding table VLAN id that this ports configured to ."
		::= { dot3aAggFdbEntry 2 }

	   dot3aAggFdbMacAddr	OBJECT-TYPE
		SYNTAX		MacAddress
		MAX-ACCESS      read-only
		STATUS		deprecated
		DESCRIPTION
		"A 6-octet read only value MAC Address assigned 
		 to this link aggregation or user-defined MAC address
		 if a static user-defined MAC address is configured."
		::= { dot3aAggFdbEntry 3 }

	   dot3aAggFdbStatus	OBJECT-TYPE
		SYNTAX		INTEGER {
				   	active(1),
				   	inactive(2)
					}	  
		MAX-ACCESS	read-only
		STATUS		deprecated
		DESCRIPTION
		"The status of this aggregation link .
		 active - this aggregation link is active.
		 inactive  - this aggregation link is no active." 
		::= { dot3aAggFdbEntry 4 }

	   dot3aAggFdbDistributedPort	OBJECT-TYPE
		SYNTAX		OCTET STRING 
		MAX-ACCESS      read-only
		STATUS		deprecated
		DESCRIPTION
		"The interface of the MAC address.
		 The format of this output is as follows:
		 <interface type> <slot/port>,  
		 <port channel> <number>,
                 or NULL if it is not available"
		::= { dot3aAggFdbEntry 5 }

        -- ### Current Aggregation MAC Addr Table

           dot3aCurAggStaticTable  OBJECT-TYPE
            SYNTAX          SEQUENCE OF Dot3aCurAggStaticEntry
            MAX-ACCESS      not-accessible
                STATUS      current
                DESCRIPTION
                "A list of statically configured MAC Address on the aggregated links."
                ::= { f10dot3dAgg 4 }

          dot3aCurAggStaticEntry   OBJECT-TYPE
            SYNTAX          Dot3aCurAggStaticEntry
            MAX-ACCESS      not-accessible
            STATUS          current
            DESCRIPTION
            "A list of statically configured MAC Address on the aggregated links in the system"
            INDEX   { dot3aCurAggVlanId, dot3aCurAggMacAddr, dot3aCurAggIndex }
            ::= { dot3aCurAggStaticTable 1 }

          Dot3aCurAggStaticEntry   ::=
            SEQUENCE {
                   dot3aCurAggVlanId               Integer32,
                   dot3aCurAggMacAddr              MacAddress,
                   dot3aCurAggIndex                Integer32,
                   dot3aCurAggStatus               INTEGER
            }

           dot3aCurAggVlanId    OBJECT-TYPE
                SYNTAX          Integer32
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                "VLAN id that this ports configured to ."
                ::= { dot3aCurAggStaticEntry 1 }

           dot3aCurAggMacAddr   OBJECT-TYPE
                SYNTAX          MacAddress
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                "A 6-octet read only value MAC Address assigned 
                 to this link aggregation or user-defined MAC address
                 if a static user-defined MAC address is configured."
                ::= { dot3aCurAggStaticEntry 2 }

           dot3aCurAggIndex     OBJECT-TYPE
                SYNTAX          Integer32
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                "The link aggregation id or port channel id."
                ::= { dot3aCurAggStaticEntry 3 }

           dot3aCurAggStatus    OBJECT-TYPE
                SYNTAX          INTEGER {
                                        active(1),
                                        inactive(2)
                                        }
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                "The status of this aggregation link .
                 active - this aggregation link is active.
                 inactive  - this aggregation link is no active."
                ::= { dot3aCurAggStaticEntry 4 }

        -- ### Current Aggregation Dynamic FDB Table

           dot3aCurAggFdbTable  OBJECT-TYPE
            SYNTAX          SEQUENCE OF Dot3aCurAggFdbEntry
            MAX-ACCESS      not-accessible
                STATUS      current
                DESCRIPTION
                "A list of dynamically learned Mac Address on the aggregated links"
                ::= { f10dot3dAgg 5 }

          dot3aCurAggFdbEntry   OBJECT-TYPE
            SYNTAX          Dot3aCurAggFdbEntry
            MAX-ACCESS      not-accessible
            STATUS          current
            DESCRIPTION
            "A list of dynamically learned Mac Address on the aggregated links in the system"
            INDEX   { dot3aCurAggFdbVlanId, dot3aCurAggFdbMacAddr, dot3aCurAggFdbIndex }
            ::= { dot3aCurAggFdbTable 1 }

          Dot3aCurAggFdbEntry   ::=
            SEQUENCE {
               dot3aCurAggFdbVlanId       Integer32,
               dot3aCurAggFdbMacAddr      MacAddress,
               dot3aCurAggFdbIndex        Integer32,
               dot3aCurAggFdbStatus       INTEGER
            }

           dot3aCurAggFdbVlanId    OBJECT-TYPE
                SYNTAX          Integer32
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                "The forwarding table VLAN id that this ports configured to ."
                ::= { dot3aCurAggFdbEntry 1 }

           dot3aCurAggFdbMacAddr   OBJECT-TYPE
                SYNTAX          MacAddress
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                "A 6-octet read only value MAC Address assigned 
                 to this link aggregation or user-defined MAC address
                 if a static user-defined MAC address is configured."
                ::= { dot3aCurAggFdbEntry 2 }

           dot3aCurAggFdbIndex     OBJECT-TYPE
                SYNTAX          Integer32
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                "The FDB link aggregation id or port channel id."
                ::= { dot3aCurAggFdbEntry 3 }

           dot3aCurAggFdbStatus    OBJECT-TYPE
                SYNTAX          INTEGER {
                                        active(1),
                                        inactive(2)
                                        }
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                "The status of this aggregation link .
                 active - this aggregation link is active.
                 inactive  - this aggregation link is not active."
                ::= { dot3aCurAggFdbEntry 4 }

        -- ### Common Aggregation FDB Table

           dot3aCommonAggFdbTable  OBJECT-TYPE
            SYNTAX          SEQUENCE OF Dot3aCommonAggFdbEntry
            MAX-ACCESS      not-accessible
                STATUS      current
                DESCRIPTION
                "A list of configured and dynamically negotiated aggregated links"
                ::= { f10dot3dAgg 6 }

          dot3aCommonAggFdbEntry   OBJECT-TYPE
            SYNTAX          Dot3aCommonAggFdbEntry
            MAX-ACCESS      not-accessible
            STATUS          current
            DESCRIPTION
            "A list of configured and dynamically negotiated aggregated links in the system"
            INDEX   { dot3aCommonAggFdbIndex, dot3aCommonAggFdbVlanId }
            ::= { dot3aCommonAggFdbTable 1 }

          Dot3aCommonAggFdbEntry   ::=
            SEQUENCE {
               dot3aCommonAggFdbIndex     Integer32,
               dot3aCommonAggFdbVlanId    Integer32,
               dot3aCommonAggFdbTagConfig INTEGER,
               dot3aCommonAggFdbStatus    INTEGER
            }

           dot3aCommonAggFdbIndex     OBJECT-TYPE
                SYNTAX          Integer32
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                "The FDB link aggregation id or port channel id."
                ::= { dot3aCommonAggFdbEntry 1 }

           dot3aCommonAggFdbVlanId    OBJECT-TYPE
                SYNTAX          Integer32
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                "The VLAN id belongs to this port channel."
                ::= { dot3aCommonAggFdbEntry 2 }

           dot3aCommonAggFdbTagConfig    OBJECT-TYPE
                SYNTAX          INTEGER {
                                        tagged(1),
                                        untagged(2)
                                        }
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                "The status if the aggregation link is tagged, untagged, or not configured.
                 tagged    - this aggregation link is tagged.
                 untagged  - this aggregation link is untagged.
                 notConfigured  - this aggregation link is not tagged or untagged."
                 
                ::= { dot3aCommonAggFdbEntry 3 }

           dot3aCommonAggFdbStatus    OBJECT-TYPE
                SYNTAX          INTEGER {
                                        active(1),
                                        inactive(2)
                                        }
                MAX-ACCESS      read-only
                STATUS          current
                DESCRIPTION
                "The status of this aggregation link .
                 active - this aggregation link is active.
                 inactive  - this aggregation link is not active."
                ::= { dot3aCommonAggFdbEntry 4 }

           dot3aClearFdb		OBJECT-TYPE
                SYNTAX          INTEGER {
                                        yes(1),
                                        no(2)
                                        }
                MAX-ACCESS      read-write
                STATUS          current
                DESCRIPTION
				"Write yes(1) to this object will clear all fdb entries.
				The value will be changed to no(2) once the fdb is cleared.
					yes(1) - clear fdb aggregation links.
					no(2)  - do not clear fdb aggregation links"
				DEFVAL {2}
                ::= { f10LinkAggMgmt 1 }

        -- ### conformance information ###

        f10LinkAggMibConformance        OBJECT IDENTIFIER       ::=     { f10LinkAggMib 2 }
        f10LinkAggMibCompliances        OBJECT IDENTIFIER       ::=     { f10LinkAggMibConformance 1 }
        f10LinkAggMibGroups             OBJECT IDENTIFIER       ::=     { f10LinkAggMibConformance 2 }


        -- ## compliance statements

        f10LinkAggMibCompliance MODULE-COMPLIANCE
                STATUS          current
                DESCRIPTION
                    "The compliance statement for Force10
                    product which implement the f10
                    Link Aggregation MIB."
                MODULE  -- this module
                MANDATORY-GROUPS {
                        f10CommonGroup
                }
                ::= { f10LinkAggMibCompliances 1 }

        -- ## units of conformance

        f10CommonGroup  OBJECT-GROUP
                OBJECTS {

                dot3aAggCfgMacAddr,
                dot3aAggCfgIfIndex,
                dot3aAggCfgNumPorts,
                dot3aAggCfgPortList,
                dot3aAggStatus,
                dot3aAggDistributedPort,
                dot3aAggFdbStatus,
                dot3aAggFdbDistributedPort,
                dot3aCurAggStatus,
                dot3aCurAggFdbStatus,
				dot3aClearFdb
                }
                STATUS  current
                DESCRIPTION
                        "A collection of objects providing the
                        overall chassis information."
                ::= { f10LinkAggMibGroups 1 }

	END
