HP-ICF-IPCONFIG DEFINITIONS ::= BEGIN

    IMPORTS
        OBJECT-TYPE, MODULE-IDENTITY
            FROM SNMPv2-SMI
        RowStatus
            FROM SNMPv2-TC
        MODULE-COMPLIANCE, OBJECT-GROUP
            FROM SNMPv2-CONF
        InetAddress, InetAddressType, InetAddressPrefixLength, InetAddressIPv4, 
        InetPortNumber
            FROM INET-ADDRESS-MIB
        ipNetToPhysicalEntry
            FROM IP-MIB
        ifIndex
            FROM IF-MIB
        hpicfCommon
            FROM HP-ICF-OID
        ipv4InterfaceEntry, ipv6InterfaceEntry, IpAddressOriginTC, 
	    IpAddressStatusTC
            FROM IP-MIB
        tunnelInetConfigEntry
            FROM TUNNEL-MIB;
        
    hpicfIpConfig MODULE-IDENTITY
        LAST-UPDATED "200702020000Z"  -- JUNE 06,2007
        ORGANIZATION "Hewlett Packard Company,
                      ProCurve Networking Business"
        CONTACT-INFO "Hewlett Packard Company
                      8000 Foothills Blvd.
                      Roseville, CA 95747"
        DESCRIPTION  "This MIB module describes objects for basic
                      IP address configuration and interface configuration
                      for devices in the HP Integrated Communication Facility
                      product line."

        REVISION     "200702020000Z"  -- JUNE 06, 2007
        DESCRIPTION  "Added hpicfIpv6NDDadAttempts to augment the 
                      hpicfIpv6GlobalConfigObjects."

        REVISION     "200705300000Z"  -- MAY 30, 2007
        DESCRIPTION  "Added hpicfIpv4InterfaceLocalProxyArp on to the
                      hpicfIpv4InterfaceEntry."

        REVISION     "200702020000Z"  -- FEBRUARY 02, 2007
        DESCRIPTION  "Added hpicfIpv6InterfaceTable to augment the 
                      Ipv6InterfaceTable."

        REVISION     "200612030000Z"  -- DECEMBER 03, 2006
        DESCRIPTION  "Added hpicfUdpTunnelMirrorSessionID to augment the 
                      tunnelInetConfigEntry object in RFC4087."

        REVISION     "200607070000Z"  -- JULY 07, 2006
        DESCRIPTION  "Added hpicfUdpTunnelSrcPort to augment the 
                      tunnelInetConfigEntry object in RFC4087."

        REVISION     "200508081600Z"  -- August 08, 2005
        DESCRIPTION  "Initial version."

        ::= { hpicfCommon 10 }


    -- The HP ICF IP configuration group

    hpicfIpConfigObjects        OBJECT IDENTIFIER ::= {hpicfIpConfig 1}

    -- The HP ICF Address group

    hpicfIpAddressObjects        OBJECT IDENTIFIER ::= {hpicfIpConfigObjects 1}

    -- The HP ICF IPV4 interface group

    hpicfIpv4InterfaceObjects    OBJECT IDENTIFIER ::= {hpicfIpConfigObjects 2}

    -- The HP ICF IPV6 config group

    hpicfIpv6ConfigObjects    OBJECT IDENTIFIER ::= {hpicfIpConfig 3}

    -- The HP ICF IPV6 global config group

    hpicfIpv6GlobalConfigObjects    OBJECT IDENTIFIER ::= {hpicfIpv6ConfigObjects 1}
    
    
    hpicfIpv6NDObjects                OBJECT IDENTIFIER ::= {hpicfIpv6GlobalConfigObjects 1}
    
    
    -- The HP ICF IPV6 ICMP group
    
    hpicfIpv6IcmpObjects              OBJECT IDENTIFIER ::= {hpicfIpv6GlobalConfigObjects 2}
    
    
    -- The HP ICF IPV6 interface group

    hpicfIpv6InterfaceObjects    OBJECT IDENTIFIER ::= {hpicfIpv6ConfigObjects 2}

    


    hpicfIpAddressTable  OBJECT-TYPE
        SYNTAX      SEQUENCE OF HpicfIpAddressEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "This table contains manually configured IPv4 and IPv6 
                     addresses for each interface. An entry in this table
                     may not exist in the active state unless all objects
                     in the entry are consistent. In particular, the value of
                     hpicfIpAddressPrefixLength."
        ::= { hpicfIpAddressObjects 1 }


    hpicfIpAddressEntry OBJECT-TYPE
        SYNTAX      HpicfIpAddressEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An entry in the hpicfIpAddressEntry contains a single 
                     manually configured IP address."
        INDEX       { ifIndex,
                      hpicfIpAddressAddrType,
                      hpicfIpAddressAddr }
        ::= { hpicfIpAddressTable 1 }

    HpicfIpAddressEntry ::=
        SEQUENCE {
            hpicfIpAddressAddrType          InetAddressType,
            hpicfIpAddressAddr              InetAddress,
            hpicfIpAddressPrefixLength      InetAddressPrefixLength,
            hpicfIpAddressType              INTEGER,
            hpicfIpAddressRowStatus         RowStatus,
            hpicfIpAddressExtendedType      INTEGER
        }


    hpicfIpAddressAddrType OBJECT-TYPE
        SYNTAX      InetAddressType
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Type of IP address"
        ::= { hpicfIpAddressEntry 1 }


    hpicfIpAddressAddr OBJECT-TYPE
        SYNTAX      InetAddress
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The IP address to which this entry's addressing
                     information pertains.
                     hpicfIpAddressAddr is always interpreted within the 
                     context of hpicfIpAddressAddrType."
        ::= { hpicfIpAddressEntry 2 }


    hpicfIpAddressPrefixLength OBJECT-TYPE
        SYNTAX      InetAddressPrefixLength
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "The prefix length associated with IP address."
        ::= { hpicfIpAddressEntry 3 }


    hpicfIpAddressType OBJECT-TYPE
        SYNTAX      INTEGER {
                        unicast(1),
                        anycast(2)
                    }
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "IP address type. For V4 addresses the value will be 
                     unicast."
        DEFVAL { unicast }
        ::= { hpicfIpAddressEntry 4 }


    hpicfIpAddressRowStatus OBJECT-TYPE
        SYNTAX      RowStatus
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "The status of the IP address entry."
        ::= { hpicfIpAddressEntry 5 }

    hpicfIpAddressExtendedType OBJECT-TYPE
        SYNTAX      INTEGER {
                        none(0),
                        eui64(1),
                        linkLocal(2)
                    }
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "IP address type. For V4 addresses the value will be 
                     none. For V6 address it can be eui64 and linkLocal also."
        DEFVAL { none }
        ::= { hpicfIpAddressEntry 6 }


    -- Switch IP Address Table

    hpicfSwitchIpAddressTable  OBJECT-TYPE
        SYNTAX      SEQUENCE OF HpicfSwitchIpAddressEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "This read only table contains IPV4 and/or IPV6 addresses
                     for each interface.

                     These IP Addresses are either manually configured or 
                     obtained by a dynamic meathod (such as DHCP).

                     This table will hold all manually configured IP Addresses
                     that exist in hpicfIpAddressTable except for those entries
                     that are not in active state (hpicfIpAddressRowStatus)."
        ::= { hpicfIpAddressObjects 2 }


    hpicfSwitchIpAddressEntry OBJECT-TYPE
        SYNTAX      HpicfSwitchIpAddressEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An entry in the hpicfSwitchIpAddressEntry contains a single 
                     IP address."
        INDEX       { ifIndex,
                      hpicfSwitchIpAddressAddrType,
                      hpicfSwitchIpAddressAddr }
        ::= { hpicfSwitchIpAddressTable 1 }

    HpicfSwitchIpAddressEntry ::=
        SEQUENCE {
            hpicfSwitchIpAddressAddrType            InetAddressType,
            hpicfSwitchIpAddressAddr                InetAddress,
            hpicfSwitchIpAddressPrefixLength        InetAddressPrefixLength,
            hpicfSwitchIpAddressType                INTEGER,
            hpicfSwitchIpAddressOrigin              IpAddressOriginTC,
            hpicfSwitchIpAddressStatus              IpAddressStatusTC,
            hpicfSwitchIpAddressPreferredLifetime   Unsigned32,
            hpicfSwitchIpAddressValidLifetime       Unsigned32,
            hpicfSwitchIpAddressExtendedType        INTEGER
        }


    hpicfSwitchIpAddressAddrType OBJECT-TYPE
        SYNTAX      InetAddressType
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "Type of IP address."
        ::= { hpicfSwitchIpAddressEntry 1 }


    hpicfSwitchIpAddressAddr OBJECT-TYPE
        SYNTAX      InetAddress
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "The IP address to which this entry's addressing
                     information pertains.
                     hpicfSwitchIpAddressAddr is always interpreted within the
                     context of hpicfSwitchIpAddressAddrType."
        ::= { hpicfSwitchIpAddressEntry 2 }


    hpicfSwitchIpAddressPrefixLength OBJECT-TYPE
        SYNTAX      InetAddressPrefixLength
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "The prefix length associated with IP address."
        ::= { hpicfSwitchIpAddressEntry 3 }


    hpicfSwitchIpAddressType OBJECT-TYPE
        SYNTAX      INTEGER {
                        unicast(1),
                        anycast(2)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION "IP address type. For V4 addresses the value will be 
                     unicast."
        ::= { hpicfSwitchIpAddressEntry 4 }

   hpicfSwitchIpAddressOrigin OBJECT-TYPE
    SYNTAX     IpAddressOriginTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "The origin of the address."
    ::= { hpicfSwitchIpAddressEntry 5 }
    
   hpicfSwitchIpAddressStatus OBJECT-TYPE
    SYNTAX     IpAddressStatusTC
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "The status of the address, describing if the address can be
            used for communication.
            In the absence of other information, an IPv4 address is
            always preferred(1)."
    DEFVAL { preferred }
    ::= { hpicfSwitchIpAddressEntry 6 }

   hpicfSwitchIpAddressPreferredLifetime OBJECT-TYPE
    SYNTAX     Unsigned32
    UNITS       "seconds"
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "The remaining length of time in seconds that this address
            will continue to be preferred, i.e. time until deprecation.
            A value of 4,294,967,295 represents infinity.
            The address generated from a deprecated address should no
            longer be used as a source address in new communications,
            but packets received on such an interface are processed as
            expected.
            The default for IPv4 addresses is 4,294,967,295 (infinity)."
    REFERENCE "For IPv6 RFC2461, especially sections 2 and 4.6.2 and RFC2462"
    ::= { hpicfSwitchIpAddressEntry 7 }
    

   hpicfSwitchIpAddressValidLifetime OBJECT-TYPE
    SYNTAX     Unsigned32
    UNITS       "seconds"
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
           "The remaining length of time, in seconds, that this address
            will continue to be valid, i.e. time until invalidation.  A
            value of 4,294,967,295 represents infinity.
            The address generated from an invalidated address should not
            appear as the destination or source address of a packet.
            The default for IPv4 addresses is 4,294,967,295 (infinity)."
    REFERENCE "For IPv6 RFC2461, especially sections 2 and 4.6.2 and RFC2462"
    ::= { hpicfSwitchIpAddressEntry 8 }   

    hpicfSwitchIpAddressExtendedType OBJECT-TYPE
    SYNTAX      INTEGER {
                     none(0),
                     eui64(1),
                     linkLocal(2)
                 }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION "IP address type. For V4 addresses the value will be 
                  none. For V6 address it can be eui64 and linkLocal also."
    DEFVAL { none }
    ::= { hpicfSwitchIpAddressEntry 9 }

    hpicfIpNetToPhysicalTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF HpicfIpNetToPhysicalEntry

    MAX-ACCESS not-accessible

    STATUS     current

    DESCRIPTION 
    "This table augments ipNeTtoPhysicalTable"
    
    ::= {hpicfIpAddressObjects 3 }

   hpicfIpNetToPhysicalEntry OBJECT-TYPE
         SYNTAX      HpicfIpNetToPhysicalEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION "This table augments ipNeTtoPhysicalTable" 
         AUGMENTS { ipNetToPhysicalEntry }
    ::= { hpicfIpNetToPhysicalTable 1 }
    
    HpicfIpNetToPhysicalEntry ::=
    SEQUENCE {
            hpicfIpNetToPhysicalPort Integer32
         }

    hpicfIpNetToPhysicalPort OBJECT-TYPE
    SYNTAX     Integer32
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
            "This object gives the port through which the
	     physical address was learnt"
    ::= { hpicfIpNetToPhysicalEntry 1}



    -- V4 Interface Table

    hpicfIpv4InterfaceTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF HpicfIpv4InterfaceEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "This table contains per-interface IPV4 configuration
                     information."
        ::= { hpicfIpv4InterfaceObjects 1 }


    hpicfIpv4InterfaceEntry OBJECT-TYPE
        SYNTAX      HpicfIpv4InterfaceEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An entry in the hpicfIpv4InterfaceEntry contains IPV4 
                     interface specific configuration information. This table
                     is indexed by ipv4InterfaceIfIndex."
        AUGMENTS    { ipv4InterfaceEntry }
        ::= { hpicfIpv4InterfaceTable 1 }


    HpicfIpv4InterfaceEntry ::=
        SEQUENCE {
            hpicfIpv4InterfaceDhcpEnable         INTEGER,
            hpicfIpv4InterfaceForwarding         INTEGER,
            hpicfIpv4InterfaceProxyArp           INTEGER,
            hpicfIpv4InterfaceLocalProxyArp      INTEGER,
            hpicfIpv4InterfaceBootpGateway       InetAddressIPv4 
        }

    hpicfIpv4InterfaceDhcpEnable OBJECT-TYPE
        SYNTAX      INTEGER {
                        full(1),
                        off(2),
                        inform(3)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Changing this flag to 'full' will clear any existing
                     IP address configuration for this interface and
                     will cause the device to use a dynamic method
                     (e.g. DHCP) to obtain its IP configuration and
                     other configuration parameter (such as gateway,
                     time of day, etc...) for this interface.

                     Setting this flag to 'inform' will allow manual IP
                     address configuration and yet permit other configuration
                     parameters (such as gateway, time of day, etc...) to
                     be obtained from a DHCP server.

                     Setting this flag to 'off' will allow manual IP
                     configuration but disallow any DHCP configuration."
        DEFVAL { full }
        ::= { hpicfIpv4InterfaceEntry 1 }


    hpicfIpv4InterfaceForwarding OBJECT-TYPE
        SYNTAX      INTEGER {
                        enabled (1),
                        disabled(2)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "This flag indicates whether this interface is forwarding
                     the datagrams that were not addressed to this interface.

                     Setting this flag to 'enabled' (the default) results 
                     in forwarding the datagrams that were not addressed to 
                     this interface.

                     Setting this flag to 'disabled' results in ignoring
                     datagrams that were not addressed to this entity."
        DEFVAL { enabled }
        ::= { hpicfIpv4InterfaceEntry 2 }


    hpicfIpv4InterfaceProxyArp OBJECT-TYPE
        SYNTAX      INTEGER {
                        enabled(1),
                        disabled(2)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Enables/disables ARP proxy on the interface. If set
                     to 'enabled', the switch will respond on ARP request
                     for IP addresses from other subnets.
                     If set to disabled (the default), the switch will not
                     respond on ARP request for IP addresses from other 
                     subnets."
        DEFVAL { disabled }
        ::= { hpicfIpv4InterfaceEntry 3 }

    hpicfIpv4InterfaceLocalProxyArp OBJECT-TYPE
        SYNTAX      INTEGER {
                        enabled(1),
                        disabled(2)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Enables/disables local ARP proxy on the interface. If set
                     to 'enabled', the switch will respond on ARP request
                     for IP addresses within the local subnet.
                     If set to disabled (the default), the switch will not
                     respond on ARP request for IP addresses within the 
                     local subnet."
        DEFVAL { disabled }
        ::= { hpicfIpv4InterfaceEntry 4 }

    hpicfIpv4InterfaceBootpGateway OBJECT-TYPE
        SYNTAX      InetAddressIPv4
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "This entry will contain the IP address of the 
                     BOOTP gateway for the interface."
        ::= { hpicfIpv4InterfaceEntry 5 }

    -- V6 Global Objects 
    hpicfIpv6NDDadAttempts OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The value in this object indicates the maximum number of
                     neighbour solicitation requests that will be sent while
                     performing duplicate address detection." 

        ::= { hpicfIpv6NDObjects 1 }

    -- V6 Global Icmp Objects 
    hpicfIpv6IcmpErrorInterval OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The value in this object indicates the error interval
                     in which the token bucket algorithm places one token
                     in the bucket for ICMPV6 rate limiting.Each token
                     represents the right to send one ICMP error message.
                     Each time an error is sent, it takes a token from the bucket. 
                     ICMP will not be allowed to originate an error 
                     message if the bucket is empty." 
        ::= { hpicfIpv6IcmpObjects 1 }

     hpicfIpv6IcmpBucketsize OBJECT-TYPE
        SYNTAX      Integer32
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "The value in this object indicates the maximum number of
                     tokens that can be in the bucket."
        ::= { hpicfIpv6IcmpObjects 2 }

    -- V6 Interface Table

    hpicfIpv6InterfaceTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF HpicfIpv6InterfaceEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "This table contains per-interface IPV6 configuration
                     information."
        ::= { hpicfIpv6InterfaceObjects 1 }


    hpicfIpv6InterfaceEntry OBJECT-TYPE
        SYNTAX      HpicfIpv6InterfaceEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An entry in the hpicfIpv6InterfaceEntry contains IPV6 
                     interface specific configuration information. This table
                     is indexed by ipv6InterfaceIfIndex."
        AUGMENTS    { ipv6InterfaceEntry }
        ::= { hpicfIpv6InterfaceTable 1 }


    HpicfIpv6InterfaceEntry ::=
        SEQUENCE {
            hpicfIpv6InterfaceDhcpMode          INTEGER,
            hpicfIpv6InterfaceManual            INTEGER,
            hpicfIpv6InterfaceAutoConfig        INTEGER,
            hpicfIpv6InterfaceDhcpRapidCommit   INTEGER,
            hpicfIpv6InterfaceDhcpRelay         INTEGER,
            hpicfIpv6InterfaceCfgEnableStatus   INTEGER
        }


    hpicfIpv6InterfaceDhcpMode OBJECT-TYPE
        SYNTAX      INTEGER {
                        disabled(0),
                        dhcpFull(1),
                        dhcpInform(2)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Setting this flag to 'dhcpFull' will clear any existing
                     IP address configuration for this interface and
                     will cause the device to use a dynamic method
                     (e.g. DHCP) to obtain its IP configuration and
                     other configuration parameter (such as gateway,
                     time of day, etc...) for this interface.

                     Setting this flag to 'dhcpInform' will allow manual IP
                     address configuration and yet permit other configuration
                     parameters (such as gateway, time of day, etc...) to
                     be obtained from a DHCP server.

                     Setting this flag to 'disabled' will not allow any of the
                     above mentioned two configuration, but interface can
                     have link-local, auto-config and manual ip-address."
        DEFVAL { disabled }
        ::= { hpicfIpv6InterfaceEntry 1 }

    hpicfIpv6InterfaceManual OBJECT-TYPE
        SYNTAX      INTEGER {
                        enabled(1),
                        disabled(2)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Setting this flag to 'enabled' will allow manual IP
                     address configuration but disallow any DHCP configuration."
        DEFVAL { disabled }
        ::= { hpicfIpv6InterfaceEntry 2 }

    hpicfIpv6InterfaceAutoConfig OBJECT-TYPE
        SYNTAX      INTEGER {
                        enabled(1),
                        disabled(2)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Setting this flag to 'enabled' will allow host to
                     configure automatically from default router.
                     There may be multiple routers and in that scenario switch will
                     add the addresses from all these routers"
        DEFVAL { disabled }
        ::= { hpicfIpv6InterfaceEntry 3 }

    hpicfIpv6InterfaceDhcpRapidCommit OBJECT-TYPE
        SYNTAX      INTEGER {
                        enabled(1),
                        disabled(2)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "Setting this flag to 'enabled' will allow the host to get
                     address and configuration information from the dhcp server
                     rapidly. This flag can be enabled only if the 
                     hpicfIpv6InterfaceDhcpMode object is set as dhcpFull.
                     By default this flag is set to disabled."
        DEFVAL { disabled }
        ::= { hpicfIpv6InterfaceEntry 4 }

    hpicfIpv6InterfaceDhcpRelay OBJECT-TYPE
        SYNTAX      INTEGER {
                        enabled (1),
                        disabled(2)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION "This flag indicates whether this interface is dhcp-relay
                     enabled. By default this flag is set to disabled."
        DEFVAL { enabled }
        ::= { hpicfIpv6InterfaceEntry 5 }

   hpicfIpv6InterfaceCfgEnableStatus OBJECT-TYPE
    SYNTAX     INTEGER {
                 up(1),
                 down(2)
              }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
           "The indication of whether IPv6 is enabled (up) or disabled
            (down) on this interface.  
            Setting this object to up(1) will enable ipv6 for the given
            interface.Setting this object to down(2) will disable the ipv6
            for the interface only if hpicfIpv6InterfaceDhcpMode,
            hpicfIpv6InterfaceManual and hpicfIpv6InterfaceAutoConfig are 
            disabled.A get on this object reflects the data saved in a 
            non-volatile storage.
            Note:To get the current ipv6 status for an interface refer to 
                 ipv6InterfaceEnableStatus."
    ::= { hpicfIpv6InterfaceEntry 6 }        

-- **********************************************************************
-- Remote mirroring tunnel Objects
-- **********************************************************************

    hpicfUdpTunnelTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF HpicfUdpTunnelEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "This table contains per interface IPV4
                     Udp encapsulated tunnel specific configuration
                     information."
        ::= { hpicfIpv4InterfaceObjects 3 }


    hpicfUdpTunnelEntry OBJECT-TYPE
        SYNTAX      HpicfUdpTunnelEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION "An entry in the hpicfUdpTunnelEntry contains
                     Udp encapsulated tunnel specific configuration
                     information."
        AUGMENTS    { tunnelInetConfigEntry }
        ::= { hpicfUdpTunnelTable 1 }


    HpicfUdpTunnelEntry ::=
        SEQUENCE {
            hpicfUdpTunnelSrcPort                InetPortNumber,
            hpicfUdpTunnelMirrorSessionID        Integer32
        }

    hpicfUdpTunnelSrcPort OBJECT-TYPE
        SYNTAX      InetPortNumber
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "This variable is valid only for the remote
                        mirroring source or destination switch.  
                        The value will be ignored otherwise. A 
                        value of 0 means that the UDP port
                        is irrelevant for the tunnel type. If this
                        value is non-zero it must be duplicated
                        in the tunnelInetConfigID value (this
                        will ensure that a given UDP port can
                        only be associated once with a given 
                        tunnelInetConfigAddressType, 
                        tunnelInetConfigLocalAddress,
                        tunnelInetConfigRemoteAddress,
                        tunnelInetConfigEncapsMethod combination)."
        DEFVAL { 0 }
        ::= { hpicfUdpTunnelEntry 1 }

    hpicfUdpTunnelMirrorSessionID OBJECT-TYPE
        SYNTAX      Integer32(0..512)   
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION "This variable is valid only for a remote
                        mirroring switch which interfaces with the
                        source end of the tunnel.  
                        The value will be ignored otherwise. A 
                        value of 0 means that the mirror session ID
                        is irrelevant for the tunnel type. "
        DEFVAL { 0 }
        ::= { hpicfUdpTunnelEntry 2 }


-- **********************************************************************
-- Conformance information
-- **********************************************************************

    hpicfIpConfigConformance OBJECT IDENTIFIER ::= {hpicfIpConfig  2}

    hpicfIpConfigCompliances OBJECT IDENTIFIER ::= {hpicfIpConfigConformance 1}
    hpicfIpConfigGroups      OBJECT IDENTIFIER ::= {hpicfIpConfigConformance 2}


-- **********************************************************************
-- Compliance statements
-- **********************************************************************


    hpicfIpConfigCompliance MODULE-COMPLIANCE
        STATUS      deprecated
        DESCRIPTION "
                A compliance statement for HP Routing switches with IP 
                Configuration"
        MODULE
        MANDATORY-GROUPS {  hpicfIpAddressTableGroup,
                            hpicfIpv4InterfaceTableGroup,
                            hpicfSwitchIpAddressTableGroup }

        OBJECT      hpicfIpv4InterfaceDhcpEnable
        MIN-ACCESS  read-write
        DESCRIPTION "An agent is not required to implement inform (3) 
                     state."

        ::= { hpicfIpConfigCompliances 1 }

    hpicfIpConfigCompliance2 MODULE-COMPLIANCE
        STATUS      current 
        DESCRIPTION "
                A compliance statement for HP Routing switches with IP 
                Configuration"
        MODULE
        MANDATORY-GROUPS {  hpicfIpAddressTableGroup,
                            hpicfIpv4InterfaceTableGroup,
                            hpicfSwitchIpAddressTableGroup }
        
        GROUP       hpicfUdpTunnelTableGroup
        DESCRIPTION "This group is valid only for the remote
                        mirroring source or destination switch.  
                        The value will be ignored otherwise."
        OBJECT      hpicfIpv4InterfaceDhcpEnable
        MIN-ACCESS  read-write        
        DESCRIPTION "An agent is not required to implement inform (3) 
                     state."
        ::= { hpicfIpConfigCompliances 2 }


    hpicfIpConfigCompliance4 MODULE-COMPLIANCE
        STATUS      current
        DESCRIPTION "
                A compliance statement for HP Routing switches with IP 
                Configuration"
        MODULE
        MANDATORY-GROUPS {  hpicfIpAddressTableGroup,
                            hpicfIpv4InterfaceTableGroup2,
                            hpicfSwitchIpAddressTableGroup,
                            hpicfIpv6InterfaceTableGroup }
        
        GROUP       hpicfUdpTunnelTableGroup
        DESCRIPTION "This group is valid only for the remote
                        mirroring source or destination switch.  
                        The value will be ignored otherwise."
        OBJECT      hpicfIpv4InterfaceDhcpEnable
        MIN-ACCESS  read-write        
        DESCRIPTION "An agent is not required to implement inform (3) 
                     state."
        ::= { hpicfIpConfigCompliances 4 }

    hpicfIpAddressTableGroup OBJECT-GROUP
        OBJECTS { 
                    hpicfIpAddressPrefixLength,
                    hpicfIpAddressType,
                    hpicfIpAddressRowStatus,
                    hpicfIpAddressExtendedType }
        STATUS      current
        DESCRIPTION "A Collection of objects allowing configuration of
                     an IP address for an interface."
        ::= { hpicfIpConfigGroups 1 }

    hpicfSwitchIpAddressTableGroup OBJECT-GROUP
        OBJECTS { 
                    hpicfSwitchIpAddressAddrType,
                    hpicfSwitchIpAddressAddr}
        STATUS      current
        DESCRIPTION "A Collection of objects providing interfaces addressing
                     information."
        ::= { hpicfIpConfigGroups 2 }


    hpicfIpv4InterfaceTableGroup  OBJECT-GROUP
        OBJECTS {
                    hpicfIpv4InterfaceDhcpEnable,
                    hpicfIpv4InterfaceForwarding,
                    hpicfIpv4InterfaceProxyArp }
        STATUS      deprecated
        DESCRIPTION "Deprecated - see hpicfIpv4InterfaceTableGroup2"
        ::= { hpicfIpConfigGroups 3 }

 
    hpicfUdpTunnelTableGroup  OBJECT-GROUP
        OBJECTS {
                    hpicfUdpTunnelSrcPort,
                    hpicfUdpTunnelMirrorSessionID }
        STATUS      current
        DESCRIPTION "A Collection of objects that allows IPV4 interface 
                     configuration for remote mirroring"
        ::= { hpicfIpConfigGroups 4 }

                              
    hpicfIpv6InterfaceTableGroup  OBJECT-GROUP
        OBJECTS {
                    hpicfIpv6InterfaceDhcpMode,
                    hpicfIpv6InterfaceManual,
                    hpicfIpv6InterfaceAutoConfig,
                    hpicfIpv6InterfaceDhcpRapidCommit,
                    hpicfIpv6InterfaceDhcpRelay }
        STATUS      current
        DESCRIPTION "A Collection of objects that allows IPV6 interface 
                     configuration"
        ::= { hpicfIpConfigGroups 5 }

    hpicfIpv4InterfaceTableGroup2  OBJECT-GROUP
        OBJECTS {
                    hpicfIpv4InterfaceDhcpEnable,
                    hpicfIpv4InterfaceForwarding,
                    hpicfIpv4InterfaceProxyArp,
                    hpicfIpv4InterfaceLocalProxyArp }
        STATUS      current
        DESCRIPTION "A Collection of objects that allows IPV4 interface 
                     configuration"
        ::= { hpicfIpConfigGroups 6 }

 
 
END
