IPX DEFINITIONS ::= BEGIN

-- This MIB defines the management information for a system using the IPX
-- protocol.  The MIB consists of four groups:
--
--    1.  System Group - contains general information about all instances
--                       of IPX on the system
--
--    2.  Circuit Group - contains information about all circuits used by
--                        IPX on the system
--
--    3.  Forwarding Group - contains generic routing information that
--                           must be provided by any IPX routing protocol.
--
--    4.  Services Group - contains information about all known services.
--
-- The MIB is designed to support multiple instances of the IPX
-- protocol on one system via a system instance identifier which is the
-- primary index for every table in this MIB.
--
-- This MIB is designed to provide a basic framework for the management
-- of systems implementing the IPX protocol.  Additional MIBs may be
-- created (especially in the area of IPX routing protocols) to contain
-- more specific information.  Whenever possible, these additional MIBs
-- should follow the format of this IPX MIB.  Information in these MIBs
-- should be linked to this MIB via the use of the system instance 
-- identifier mentioned above.


IMPORTS
        enterprises, Counter
                FROM RFC1155-SMI
        OBJECT-TYPE
                FROM RFC-1212
        TRAP-TYPE
                FROM RFC-1215
        PhysAddress
                FROM RFC1213-MIB;

novell  OBJECT IDENTIFIER ::= { enterprises 23 }
mibDoc  OBJECT IDENTIFIER ::= { novell 2 }
ipx     OBJECT IDENTIFIER ::= { mibDoc 5 }


-- Groups

ipxSystem OBJECT IDENTIFIER ::= {ipx 1}
ipxCircuit OBJECT IDENTIFIER ::= {ipx 2}
ipxForwarding OBJECT IDENTIFIER ::= {ipx 3}
ipxServices OBJECT IDENTIFIER ::= {ipx 4}
ipxTraps OBJECT IDENTIFIER ::= {ipx 5}

-- Types

NetNumber ::= OCTET STRING (SIZE(4))

-- System Group
--   This group contains global information about each instance of IPX
--   running on one system.

-- Basic System Table
--   This table contains one entry for each instance of IPX running on
--   the system.  It contains the management information that should
--   be made available by all implementations of the IPX protocol.

ipxBasicSysTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF IPXBasicSysEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "The IPX System table - basic information."
   ::= {ipxSystem 1}

ipxBasicSysEntry OBJECT-TYPE
   SYNTAX      IPXBasicSysEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "Each entry corresponds to one instance of IPX running
                on the system."
   INDEX       {ipxBasicSysInstance}
   ::= {ipxBasicSysTable 1}

IPXBasicSysEntry ::= SEQUENCE {
                        ipxBasicSysInstance
                           INTEGER,
                        ipxBasicSysExistState
                           INTEGER,
                        ipxBasicSysNetNumber
                           NetNumber,
                        ipxBasicSysNode
                           OCTET STRING,
                        ipxBasicSysName
                           OCTET STRING,
                        ipxBasicSysInReceives
                           Counter,
                        ipxBasicSysInHdrErrors
                           Counter,
                        ipxBasicSysInUnknownSockets
                           Counter,
                        ipxBasicSysInDiscards
                           Counter,
                        ipxBasicSysInBadChecksums
                           Counter,
                        ipxBasicSysInDelivers
                           Counter,
                        ipxBasicSysNoRoutes
                           Counter,
                        ipxBasicSysOutRequests
                           Counter,
                        ipxBasicSysOutMalformedRequests
                           Counter,
                        ipxBasicSysOutDiscards
                           Counter,
                        ipxBasicSysOutPackets
                           Counter,
                        ipxBasicSysConfigSockets
                           INTEGER,
                        ipxBasicSysOpenSocketFails
                           Counter
                    }
                           
ipxBasicSysInstance OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the instance of IPX to which this
                row corresponds.  This value may be written only when
                creating a new entry in the table."
   ::= {ipxBasicSysEntry 1}

ipxBasicSysExistState OBJECT-TYPE
   SYNTAX      INTEGER {
                        off(1),
                        on(2)
                       }
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The validity of this entry in the IPX system table.
                Setting this field to off indicates that this entry may be
                deleted from the system table at the IPX implementation's
                discretion."
   ::= {ipxBasicSysEntry 2}

ipxBasicSysNetNumber OBJECT-TYPE
   SYNTAX      NetNumber
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The network number portion of the IPX address of this
                system."
   ::= {ipxBasicSysEntry 3}

ipxBasicSysNode OBJECT-TYPE
   SYNTAX      OCTET STRING (SIZE(6))
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The node number portion of the IPX address of this
                system."
   ::= {ipxBasicSysEntry 4}

ipxBasicSysName OBJECT-TYPE
   SYNTAX      OCTET STRING (SIZE(0..48))
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The readable name for this system."
   ::= {ipxBasicSysEntry 5}

ipxBasicSysInReceives OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The total number of IPX packets received, including
                those received in error."
   ::= {ipxBasicSysEntry 6}

ipxBasicSysInHdrErrors OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of IPX packets discarded due to errors in
                their headers, including any IPX packet with a size less
                than the minimum of 30 bytes."
   ::= {ipxBasicSysEntry 7}

ipxBasicSysInUnknownSockets OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of IPX packets discarded because the
                destination socket was not open."
   ::= {ipxBasicSysEntry 8}

ipxBasicSysInDiscards OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of IPX packets received but discarded due to
                reasons other than those accounted for by 
                ipxBasicSysInHdrErrors, ipxBasicSysInUnknownSockets,
                ipxAdvSysInDiscards, and ipxAdvSysInCompressDiscards."
   ::= {ipxBasicSysEntry 9}

ipxBasicSysInBadChecksums OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of IPX packets received with incorrect
                checksums."
   ::= {ipxBasicSysEntry 10}

ipxBasicSysInDelivers OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The total number of IPX packets delivered locally,
                including packets from local applications."
   ::= {ipxBasicSysEntry 11}

ipxBasicSysNoRoutes OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of times no route to a destination was
                found."
   ::= {ipxBasicSysEntry 12}

ipxBasicSysOutRequests OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of IPX packets supplied locally for
                transmission, not including any packets counted in
                ipxAdvForwPackets."
   ::= {ipxBasicSysEntry 13}

ipxBasicSysOutMalformedRequests OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of IPX packets supplied locally that contained
                errors in their structure."
   ::= {ipxBasicSysEntry 14}

ipxBasicSysOutDiscards OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of outgoing IPX packets discarded due to
                reasons other than those accounted for in
                ipxBasicSysOutMalformedRequests, ipxAdvSysOutFiltered,
                and ipxAdvSysOutCompressDiscards."
   ::= {ipxBasicSysEntry 15}

ipxBasicSysOutPackets OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The total number of IPX packets transmitted."
   ::= {ipxBasicSysEntry 16}

ipxBasicSysConfigSockets OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The configured maximum number of IPX sockets that may be
                open at one time."
   ::= {ipxBasicSysEntry 17}

ipxBasicSysOpenSocketFails OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of IPX socket open calls which failed."
   ::= {ipxBasicSysEntry 18}


-- Advanced System Table
--   This table contains one entry for each instance of IPX running on
--   the system.  It contains the advanced management information that
--   may not be available from all implementations of the IPX protocol.

ipxAdvSysTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF IPXAdvSysEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "The IPX System table - advanced information."
   ::= {ipxSystem 2}

ipxAdvSysEntry OBJECT-TYPE
   SYNTAX      IPXAdvSysEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "Each entry corresponds to one instance of IPX running
                on the system."
   INDEX       {ipxAdvSysInstance}
   ::= {ipxAdvSysTable 1}

IPXAdvSysEntry ::= SEQUENCE {
                     ipxAdvSysInstance
                        INTEGER,
                     ipxAdvSysMaxPathSplits
                        INTEGER,
                     ipxAdvSysMaxHops
                        INTEGER,
                     ipxAdvSysInTooManyHops
                        Counter,
                     ipxAdvSysInFiltered
                        Counter,
                     ipxAdvSysInCompressDiscards
                        Counter,
                     ipxAdvSysNETBIOSPackets
                        Counter,
                     ipxAdvSysForwPackets
                        Counter,
                     ipxAdvSysOutFiltered
                        Counter,
                     ipxAdvSysOutCompressDiscards
                        Counter,
                     ipxAdvSysCircCount
                        INTEGER,
                     ipxAdvSysDestCount
                        INTEGER,
                     ipxAdvSysServCount
                        INTEGER
                    }
                           
ipxAdvSysInstance OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the instance of IPX to which this
                row corresponds.  This value may be written only when
                creating a new entry in the table."
   ::= {ipxAdvSysEntry 1}

ipxAdvSysMaxPathSplits OBJECT-TYPE
   SYNTAX      INTEGER (1..32)
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The maximum number of paths with equal routing metric
                value which this instance of the IPX may split
                between when forwarding packets."
   DEFVAL      { 1 }
   ::= {ipxAdvSysEntry 2}

ipxAdvSysMaxHops OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The maximum number of hops a packet may take."
   DEFVAL      { 64 }
   ::= {ipxAdvSysEntry 3}

ipxAdvSysInTooManyHops OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of IPX packets discarded due to exceeding the
                maximum hop count."
   ::= {ipxAdvSysEntry 4}

ipxAdvSysInFiltered OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of incoming IPX packets discarded due to
                filtering."
   ::= {ipxAdvSysEntry 5}

ipxAdvSysInCompressDiscards OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of incoming IPX packets discarded due to
                decompression errors."
   ::= {ipxAdvSysEntry 6}

ipxAdvSysNETBIOSPackets OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of NETBIOS packets received."
   ::= {ipxAdvSysEntry 7}

ipxAdvSysForwPackets OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of IPX packets forwarded."
   ::= {ipxAdvSysEntry 8}

ipxAdvSysOutFiltered OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of outgoing IPX packets discarded due to
                filtering."
   ::= {ipxAdvSysEntry 9}

ipxAdvSysOutCompressDiscards OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of outgoing IPX packets discarded due to
                compression errors."
   ::= {ipxAdvSysEntry 10}

ipxAdvSysCircCount OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of circuits known to this instance of IPX."
   ::= {ipxAdvSysEntry 11}

ipxAdvSysDestCount OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of currently reachable destinations known to
                this instance of IPX."
   ::= {ipxAdvSysEntry 12}

ipxAdvSysServCount OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of services known to this instance of IPX."
   ::= {ipxAdvSysEntry 13}


-- Circuit Group
--   This group contains management information for each circuit known
--   to this system.

-- Circuit Table
--   The Circuit table contains an entry for each circuit known to the
--   system.

ipxCircTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF IPXCircEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "The Circuit table."
   ::= {ipxCircuit 1}

ipxCircEntry OBJECT-TYPE
   SYNTAX      IPXCircEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "Each entry corresponds to one circuit known to the
                system."
   INDEX       {
                ipxCircSysInstance,
                ipxCircIndex
               }
   ::= {ipxCircTable 1}

IPXCircEntry ::= SEQUENCE {
                     ipxCircSysInstance
                        INTEGER,
                     ipxCircIndex
                        INTEGER,
                     ipxCircExistState
                        INTEGER,
                     ipxCircOperState
                        INTEGER,
                     ipxCircIfIndex
                        INTEGER,
                     ipxCircName
                        OCTET STRING,
                     ipxCircType
                        INTEGER,
                     ipxCircDialName
                        OCTET STRING,
                     ipxCircLocalMaxPacketSize
                        INTEGER,
                     ipxCircCompressState
                        INTEGER,
                     ipxCircCompressSlots
                        INTEGER,
                     ipxCircStaticStatus
                        INTEGER,
                     ipxCircCompressedSent
                        Counter,
                     ipxCircCompressedInitSent
                        Counter,
                     ipxCircCompressedRejectsSent
                        Counter,
                     ipxCircUncompressedSent
                        Counter,
                     ipxCircCompressedReceived
                        Counter,
                     ipxCircCompressedInitReceived
                        Counter,
                     ipxCircCompressedRejectsReceived
                        Counter,
                     ipxCircUncompressedReceived
                        Counter,
                     ipxCircMediaType
                        OCTET STRING,
                     ipxCircNetNumber
                        NetNumber,
                     ipxCircStateChanges
                        Counter,
                     ipxCircInitFails
                        Counter,
                     ipxCircDelay
                        INTEGER,
                     ipxCircThroughput
                        INTEGER,
                     ipxCircNeighRouterName
                        OCTET STRING,
                     ipxCircNeighInternalNetNum
                        NetNumber
                    }

ipxCircSysInstance OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the instance of IPX
                to which this entry corresponds.  This value may be 
                written only when creating a new entry in the table."
   ::= {ipxCircEntry 1}

ipxCircIndex OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The identifier of this circuit, unique within the
                instance of IPX.  This value may be written
                only when creating a new entry in the table."
   ::= {ipxCircEntry 2}

ipxCircExistState OBJECT-TYPE
   SYNTAX      INTEGER {
                        off(1),
                        on(2)
                       }
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The validity of this circuit entry.  A circuit with this
                value set to off may be deleted from the table at the
                IPX implementation's discretion."
   ::= {ipxCircEntry 3}

ipxCircOperState OBJECT-TYPE
   SYNTAX      INTEGER {
                        down(1),
                        up(2),
                        sleeping(3)
                       }
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The operational state of the circuit."
   ::= {ipxCircEntry 4}

ipxCircIfIndex OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The value of ifIndex for the interface used by this
                circuit.  This value may be written only when creating
                a new entry in the table."
   ::= {ipxCircEntry 5}

ipxCircName OBJECT-TYPE
   SYNTAX      OCTET STRING (SIZE(0..48))
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The readable name for the circuit."
   ::= {ipxCircEntry 6}

ipxCircType OBJECT-TYPE
   SYNTAX      INTEGER {
                        other(1),
                        broadcast(2),
                        ptToPt(3),
                        wanRIP(4),
                        unnumberedRIP(5),
                        dynamic(6),
                        wanWS(7)
                       }
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The type of the circuit."
   ::= {ipxCircEntry 7}

ipxCircDialName OBJECT-TYPE
   SYNTAX      OCTET STRING (SIZE(0..48))
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The symbolic name used to refernce the dialing information
                used to create this circuit.  This value may be written 
                only when creating a new entry in the table."
   ::= {ipxCircEntry 8}

ipxCircLocalMaxPacketSize OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The maximum size (including header), in bytes, that the
                system supports locally on this circuit."
   ::= {ipxCircEntry 9}

ipxCircCompressState OBJECT-TYPE
   SYNTAX      INTEGER {
                        off(1),
                        on(2)
                       }
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The compression state on this circuit.  This value may 
                be written only when creating a new entry in the table."
   DEFVAL      { off }
   ::= {ipxCircEntry 10}

ipxCircCompressSlots OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of compression slots available on this 
                circuit.  This value may be written only when creating a
                new entry in the table."
   DEFVAL      { 16 }
   ::= {ipxCircEntry 11}

ipxCircStaticStatus OBJECT-TYPE
   SYNTAX      INTEGER {
                        unknown(1),
                        current(2),
                        changed(3),
                        read(4),
                        reading(5),
                        write(6),
                        writing(7)
                       }
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "Indicates whether the information about static routes
                and services reached via this circuit matches that
                saved in permanent storage (current).  Setting the
                value to write when it had the value changed will write
                the currently in use information to permanent storage, 
                if supported.  Setting the value to read when it had
                the value changed will replace any routes and services
                currently defined for the circuit with those read from
                permanent storage, if supported."
   ::= {ipxCircEntry 12}

ipxCircCompressedSent OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of compressed packets sent."
   ::= {ipxCircEntry 13}

ipxCircCompressedInitSent OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of compression initialization packets sent."
   ::= {ipxCircEntry 14}

ipxCircCompressedRejectsSent OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of compressed packet rejected packets sent."
   ::= {ipxCircEntry 15}

ipxCircUncompressedSent OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of packets sent without being compressed
                even though compression was turned on for this circuit."
   ::= {ipxCircEntry 16}

ipxCircCompressedReceived OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of compressed packets received."
   ::= {ipxCircEntry 17}

ipxCircCompressedInitReceived OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of compression initialization packets received."
   ::= {ipxCircEntry 18}

ipxCircCompressedRejectsReceived OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of compressed packet rejected packets received."
   ::= {ipxCircEntry 19}

ipxCircUncompressedReceived OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of packets received without having been
                compressed even though compression was turned on for
                this circuit."
   ::= {ipxCircEntry 20}

ipxCircMediaType OBJECT-TYPE
   SYNTAX      OCTET STRING (SIZE(2))
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The media type used on this circuit."
   ::= {ipxCircEntry 21}

ipxCircNetNumber OBJECT-TYPE
   SYNTAX      NetNumber
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The IPX network number of this circuit.  This value may
                be written only when creating a new entry in the table."
   ::= {ipxCircEntry 22}

ipxCircStateChanges OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of times the circuit has changed state."
   ::= {ipxCircEntry 23}

ipxCircInitFails OBJECT-TYPE
   SYNTAX      Counter
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of times that initialization of this
                circuit has failed."
   ::= {ipxCircEntry 24}

ipxCircDelay OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The period of time, in milliseconds, that it takes to
                transmit one byte of data, excluding protocol headers,
                to a destination on the other end of the circuit, if 
                the circuit is free of other traffic."
   ::= {ipxCircEntry 25}

ipxCircThroughput OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The amount of data, in bits per second, that may flow
                through the circuit if there is no other traffic."
   ::= {ipxCircEntry 26}

ipxCircNeighRouterName OBJECT-TYPE
   SYNTAX      OCTET STRING (SIZE(0..48))
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The name of the neighboring router on a WAN circuit."
   ::= {ipxCircEntry 27}

ipxCircNeighInternalNetNum OBJECT-TYPE
   SYNTAX      NetNumber
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The internal network number of the neighboring router
                on a WAN circuit."
   ::= {ipxCircEntry 28}


-- Forwarding Group
--   This group provides a representation of the forwarding database used
--   by all instances of IPX on the system.

-- Destination Table
--   The Destination table contains information about all known
--   destinations.  The routing information shown in this table represents
--   the path currently being used to reach the destination.

ipxDestTable OBJECT-TYPE
   SYNTAX      SEQUENCE OF IPXDestEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "The Destination table contains information about all
                known destinations."
   ::= {ipxForwarding 1}

ipxDestEntry OBJECT-TYPE
   SYNTAX      IPXDestEntry
   ACCESS      not-accessible
   STATUS      mandatory
   DESCRIPTION "Each entry corresponds to one destination."
   INDEX       {
                ipxDestSysInstance,
                ipxDestNetNum
               }
   ::= {ipxDestTable 1}

IPXDestEntry ::= SEQUENCE {
                     ipxDestSysInstance
                        INTEGER,
                     ipxDestNetNum
                        NetNumber,
                     ipxDestProtocol
                        INTEGER,
                     ipxDestTicks
                        INTEGER,
                     ipxDestHopCount
                        INTEGER,
                     ipxDestNextHopCircIndex
                        INTEGER,
                     ipxDestNextHopNICAddress
                        PhysAddress,
                     ipxDestNextHopNetNum
                        NetNumber
                    }

ipxDestSysInstance OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the instance of IPX
                to which this row corresponds."
   ::= {ipxDestEntry 1}

ipxDestNetNum OBJECT-TYPE
   SYNTAX      NetNumber
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The IPX network number of the destination."
   ::= {ipxDestEntry 2}

ipxDestProtocol OBJECT-TYPE
   SYNTAX      INTEGER {
                        other(1),
                        local(2),
                        rip(3),
                        nlsp(4),
                        static(5)
                       }
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The routing protocol from which knowledge of this
                destination was obtained."
   ::= {ipxDestEntry 3}

ipxDestTicks OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The delay in ticks to reach this destination."
   ::= {ipxDestEntry 4}

ipxDestHopCount OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The number of hops necessary to reach the destination."
   ::= {ipxDestEntry 5}

ipxDestNextHopCircIndex OBJECT-TYPE
   SYNTAX      INTEGER
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The unique identifier of the circuit used to reach the 
                next hop."
   ::= {ipxDestEntry 6}

ipxDestNextHopNICAddress OBJECT-TYPE
   SYNTAX      PhysAddress
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The NIC address of the next hop."
   ::= {ipxDestEntry 7}

ipxDestNextHopNetNum OBJECT-TYPE
   SYNTAX      NetNumber
   ACCESS      read-only
   STATUS      mandatory
   DESCRIPTION "The IPX network number of the next hop."
   ::= {ipxDestEntry 8}


-- Static Routes Table
--   This table contains the information about all the static routes
--   defined.  There may be more than one static route to any given
--   destination.  Only the route currently being used will also be
--   present in the Destination Table defined above.

-- ipxStaticRouteTable OBJECT-TYPE
--    SYNTAX      SEQUENCE OF IPXStaticRouteEntry
--    ACCESS      not-accessible
--    STATUS      mandatory
--    DESCRIPTION "The Static Routes table contains information about all
--                 destinations reached via statically configured routes."
--    ::= {ipxForwarding 2}
-- 
-- ipxStaticRouteEntry OBJECT-TYPE
--    SYNTAX      IPXStaticRouteEntry
--    ACCESS      not-accessible
--    STATUS      mandatory
--    DESCRIPTION "Each entry corresponds to one static route."
--    INDEX       {
--                 ipxStaticRouteSysInstance,
--                 ipxStaticRouteCircIndex,
--                 ipxStaticRouteNetNum
--                }
--    ::= {ipxStaticRouteTable 1}
-- 
-- IPXStaticRouteEntry ::= SEQUENCE {
--                            ipxStaticRouteSysInstance
--                               INTEGER,
--                            ipxStaticRouteCircIndex
--                               INTEGER,
--                            ipxStaticRouteNetNum
--                               NetNumber,
--                            ipxStaticRouteExistState
--                               INTEGER,
--                            ipxStaticRouteTicks
--                               INTEGER,
--                            ipxStaticRouteHopCount
--                               INTEGER
--                           }
-- 
-- ipxStaticRouteSysInstance OBJECT-TYPE
--    SYNTAX      INTEGER
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The unique identifier of the instance of IPX to
--                 which this row corresponds."
--    ::= {ipxStaticRouteEntry 1}
-- 
-- ipxStaticRouteCircIndex OBJECT-TYPE
--    SYNTAX      INTEGER
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The unique identifier of the circuit used to
--                 reach the first hop in the static route."
--    ::= {ipxStaticRouteEntry 2}
-- 
-- ipxStaticRouteNetNum OBJECT-TYPE
--    SYNTAX      NetNumber
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The IPX network number of the route's destination."
--    ::= {ipxStaticRouteEntry 3}
-- 
-- ipxStaticRouteExistState OBJECT-TYPE
--    SYNTAX      INTEGER {
--                         off(1),
--                         on(2)
--                        }
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The validity of this static route.  Entries with the
--                 value set to off may be deleted from the table at the
--                 implementation's discretion."
--    ::= {ipxStaticRouteEntry 4}
-- 
-- ipxStaticRouteTicks OBJECT-TYPE
--    SYNTAX      INTEGER
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The delay, in ticks, to reach the route's destination."
--    ::= {ipxStaticRouteEntry 5}
-- 
-- ipxStaticRouteHopCount OBJECT-TYPE
--    SYNTAX      INTEGER
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The number of hops necessary to reach the destination."
--    ::= {ipxStaticRouteEntry 6}


-- Services Group
--    The Services group contains management information for all known
--    services.
-- 
-- Services Table
--    This table contains the services information indexed by service
--    name and type.

-- ipxServTable OBJECT-TYPE
--    SYNTAX      SEQUENCE OF IPXServEntry
--    ACCESS      not-accessible
--    STATUS      mandatory
--    DESCRIPTION "The table of services, indexed by name and type."
--    ::= {ipxServices 1}
-- 
-- ipxServEntry OBJECT-TYPE
--    SYNTAX      IPXServEntry
--    ACCESS      not-accessible
--    STATUS      mandatory
--    DESCRIPTION "Each entry corresponds to one service."
--    INDEX       {
--                 ipxServSysInstance,
--                 ipxServType,
--                 ipxServName
--                }
--    ::= {ipxServTable 1}
-- 
-- IPXServEntry ::= SEQUENCE {
--                      ipxServSysInstance
--                         INTEGER,
--                      ipxServType
--                         OCTET STRING,
--                      ipxServName
--                         OCTET STRING,
--                      ipxServProtocol
--                         INTEGER,
--                      ipxServNetNum
--                         NetNumber,
--                      ipxServNode
--                         OCTET STRING,
--                      ipxServSocket
--                         OCTET STRING,
--                      ipxServHopCount
--                         INTEGER
--                     }
-- 
-- ipxServSysInstance OBJECT-TYPE
--    SYNTAX      INTEGER
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The unique identifier of the instance of IPX
--                 to which this entry corresponds."
--    ::= {ipxServEntry 1}
-- 
-- ipxServType OBJECT-TYPE
--    SYNTAX      OCTET STRING (SIZE(2))
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The service type."
--    ::= {ipxServEntry 2}
-- 
-- ipxServName OBJECT-TYPE
--    SYNTAX      OCTET STRING (SIZE(1..48))
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The service name."
--    ::= {ipxServEntry 3}
-- 
-- ipxServProtocol OBJECT-TYPE
--    SYNTAX      INTEGER {
--                         other(1),
--                         local(2),
--                         nlsp(4),
--                         static(5),
--                         sap(6)
--                        }
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The protocol from which knowledge of this service was
--                 obtained."
--    ::= {ipxServEntry 4}
-- 
-- ipxServNetNum OBJECT-TYPE
--    SYNTAX      NetNumber
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The IPX network number portion of the IPX address of the
--                 service."
--    ::= {ipxServEntry 5}
-- 
-- ipxServNode OBJECT-TYPE
--    SYNTAX      OCTET STRING (SIZE(6))
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The node portion of the IPX address of the service."
--    ::= {ipxServEntry 6}
-- 
-- ipxServSocket OBJECT-TYPE
--    SYNTAX      OCTET STRING (SIZE(2))
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The socket portion of the IPX address of the service."
--    ::= {ipxServEntry 7}
-- 
-- ipxServHopCount OBJECT-TYPE
--    SYNTAX      INTEGER
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The number of hops to the service."
--    ::= {ipxServEntry 8}
 
 
-- Destination Services Table
--   This table contains the services information indexed by address, 
--   name, and type.

-- ipxDestServTable OBJECT-TYPE
--    SYNTAX      SEQUENCE OF IPXDestServEntry
--    ACCESS      not-accessible
--    STATUS      mandatory
--    DESCRIPTION "The table of services, indexed by address, name,
--                 and type."
--    ::= {ipxServices 2}
-- 
-- ipxDestServEntry OBJECT-TYPE
--    SYNTAX      IPXDestServEntry
--    ACCESS      not-accessible
--    STATUS      mandatory
--    DESCRIPTION "Each entry corresponds to one service."
--    INDEX       {
--                 ipxDestServSysInstance,
--                 ipxDestServNetNum,
--                 ipxDestServNode,
--                 ipxDestServSocket,
--                 ipxDestServName,
--                 ipxDestServType
--                }
--    ::= {ipxDestServTable 1}
-- 
-- IPXDestServEntry ::= SEQUENCE {
--                         ipxDestServSysInstance
--                            INTEGER,
--                         ipxDestServNetNum
--                            NetNumber,
--                         ipxDestServNode
--                            OCTET STRING,
--                         ipxDestServSocket
--                            OCTET STRING,
--                         ipxDestServName
--                            OCTET STRING,
--                         ipxDestServType
--                            OCTET STRING,
--                         ipxDestServProtocol
--                            INTEGER,
--                         ipxDestServHopCount
--                            INTEGER
--                        }
-- 
-- ipxDestServSysInstance OBJECT-TYPE
--    SYNTAX      INTEGER
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The unique identifier of the instance of IPX
--                 to which this entry corresponds."
--    ::= {ipxDestServEntry 1}
-- 
-- ipxDestServNetNum OBJECT-TYPE
--    SYNTAX      NetNumber
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The IPX network number portion of the IPX address of the
--                 service."
--    ::= {ipxDestServEntry 2}
-- 
-- ipxDestServNode OBJECT-TYPE
--    SYNTAX      OCTET STRING (SIZE(6))
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The node portion of the IPX address of the service."
--    ::= {ipxDestServEntry 3}
-- 
-- ipxDestServSocket OBJECT-TYPE
--    SYNTAX      OCTET STRING (SIZE(2))
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The socket portion of the IPX address of the service."
--    ::= {ipxDestServEntry 4}
-- 
-- ipxDestServName OBJECT-TYPE
--    SYNTAX      OCTET STRING (SIZE(1..48))
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The service name."
--    ::= {ipxDestServEntry 5}
-- 
-- ipxDestServType OBJECT-TYPE
--    SYNTAX      OCTET STRING (SIZE(2))
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The service type."
--    ::= {ipxDestServEntry 6}
-- 
-- ipxDestServProtocol OBJECT-TYPE
--    SYNTAX      INTEGER {
--                         other(1),
--                         local(2),
--                         nlsp(4),
--                         static(5),
--                         sap(6)
--                        }
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The protocol from which knowledge of this service was
--                 obtained."
--    ::= {ipxDestServEntry 7}
-- 
-- ipxDestServHopCount OBJECT-TYPE
--    SYNTAX      INTEGER
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The number of hops to the service."
--    ::= {ipxDestServEntry 8}


-- Static Services Table
--   This table contains information for all services reached via a
--   static route.

-- ipxStaticServTable OBJECT-TYPE
--    SYNTAX      SEQUENCE OF IPXStaticServEntry
--    ACCESS      not-accessible
--    STATUS      mandatory
--    DESCRIPTION "The Static Services table contains information about
--                 all services reached via statically configured routes."
--    ::= {ipxServices 3}
-- 
-- ipxStaticServEntry OBJECT-TYPE
--    SYNTAX      IPXStaticServEntry
--    ACCESS      not-accessible
--    STATUS      mandatory
--    DESCRIPTION "Each entry corresponds to one service."
--    INDEX       {
--                 ipxStaticServSysInstance,
--                 ipxStaticServCircIndex,
--                 ipxStaticServName,
--                 ipxStaticServType
--                }
--    ::= {ipxStaticServTable 1}
-- 
-- IPXStaticServEntry ::= SEQUENCE {
--                            ipxStaticServSysInstance
--                               INTEGER,
--                            ipxStaticServCircIndex
--                               INTEGER,
--                            ipxStaticServName
--                               OCTET STRING,
--                            ipxStaticServType
--                               OCTET STRING,
--                            ipxStaticServExistState
--                               INTEGER,
--                            ipxStaticServNetNum
--                               NetNumber,
--                            ipxStaticServNode
--                               OCTET STRING,
--                            ipxStaticServSocket
--                               OCTET STRING,
--                            ipxStaticServHopCount
--                               INTEGER
--                           }
-- 
-- ipxStaticServSysInstance OBJECT-TYPE
--    SYNTAX      INTEGER
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The unique identifier of the instance of IPX to which
--                 this entry corresponds."
--    ::= {ipxStaticServEntry 1}
-- 
-- ipxStaticServCircIndex OBJECT-TYPE
--    SYNTAX      INTEGER
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The circuit used to reach this service."
--    ::= {ipxStaticServEntry 2}
-- 
-- ipxStaticServName OBJECT-TYPE
--    SYNTAX      OCTET STRING (SIZE(1..48))
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The service name."
--    ::= {ipxStaticServEntry 3}
-- 
-- ipxStaticServType OBJECT-TYPE
--    SYNTAX      OCTET STRING (SIZE(2))
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The service type."
--    ::= {ipxStaticServEntry 4}
-- 
-- ipxStaticServExistState OBJECT-TYPE
--    SYNTAX      INTEGER {
--                         off(1),
--                         on(2)
--                        }
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The validity of this static service.  Entries with the
--                 value set to off may be deleted from the table at the
--                 implementation's discretion."
--    ::= {ipxStaticServEntry 5}
-- 
-- ipxStaticServNetNum OBJECT-TYPE
--    SYNTAX      NetNumber
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The IPX network number portion of the IPX address of the
--                 service."
--    ::= {ipxStaticServEntry 6}
-- 
-- ipxStaticServNode OBJECT-TYPE
--    SYNTAX      OCTET STRING (SIZE(6))
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The node portion of the IPX address of the service."
--    ::= {ipxStaticServEntry 7}
-- 
-- ipxStaticServSocket OBJECT-TYPE
--    SYNTAX      OCTET STRING (SIZE(2))
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The socket portion of the IPX address of the service."
--    ::= {ipxStaticServEntry 8}
-- 
-- ipxStaticServHopCount OBJECT-TYPE
--    SYNTAX      INTEGER
--    ACCESS      read-only
--    STATUS      mandatory
--    DESCRIPTION "The number of hops to the service."
--    ::= {ipxStaticServEntry 9}


-- Traps
--   The section describes the traps defined for IPX.

-- ipxTrapCircuitDown TRAP-TYPE
--    ENTERPRISE    ipxTraps
--    VARIABLES     {
--                   ipxCircSysInstance,
--                   ipxCircIndex
--                  }
--    DESCRIPTION   "This trap signifies that the specified circuit has
--                   gone down."
--    ::= 1
-- 
-- ipxTrapCircuitUp TRAP-TYPE
--    ENTERPRISE    ipxTraps
--    VARIABLES     {
--                   ipxCircSysInstance,
--                   ipxCircIndex
--                  }
--    DESCRIPTION   "This trap signifies that the specified circuit has
--                   come up."
--    ::= 2
-- 

END
