
-- *****************************************************************************
-- Juniper-Interfaces-CONF
--
-- SNMP Agent Capabilities definitions for the Interfaces MIBs.
--
-- Copyright (c) 2001 Unisphere Networks, Inc.
-- Copyright (c) 2002, 2003 Juniper Networks, Inc.
-- Copyright (c) 2004 Juniper Networks, Inc.
--   All rights reserved.
-- *****************************************************************************

Juniper-Interfaces-CONF  DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY
        FROM SNMPv2-SMI
    AGENT-CAPABILITIES
        FROM SNMPv2-CONF
    juniAgents
        FROM Juniper-Agents;

juniInterfacesAgent  MODULE-IDENTITY
    LAST-UPDATED "200307162138Z"  -- 16-Jul-03 05:38 PM EDT
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
        "       Juniper Networks, Inc.
        Postal: 10 Technology Park Drive
                Westford, MA  01886-3146
                USA
        Tel:    +1 978 589 5800
        E-mail: mib@Juniper.net"
    DESCRIPTION
        "The agent capabilities definitions for the Interfaces component of the
        SNMP agent in the Juniper E-series family of products."
    -- Revision History
    REVISION    "200402042138Z"  -- 04-Feb-04 05:38 PM EDT  - JUNOSe 6.1
    DESCRIPTION
        "Added mib table rsIfCountTable to count systemwide interfaces by if type."
    REVISION    "200307162138Z"  -- 16-Jul-03 05:38 PM EDT  - JUNOSe 5.1
    DESCRIPTION
        "IF-INVERTED-STACK-MIB:
         Added support for RFC 2864, the Inverted Stack Table."
    REVISION    "200212161443Z"  -- 16-Dec-02 09:43 AM EST  - JUNOSe 5.0
    DESCRIPTION
        "Juniper-UNI-IF-MIB:
         Replaced Unisphere names with Juniper names."
    REVISION    "200104271424Z"  -- 27-Apr-01 10:24 AM EDT  - JUNOSe 3.2
    DESCRIPTION
        "The initial release of this management information module."
    ::= { juniAgents 20 }


-- *****************************************************************************
-- Interfaces SNMP Agent Capabilities definitions
-- *****************************************************************************
juniInterfacesAgentV1  AGENT-CAPABILITIES
    PRODUCT-RELEASE
        "Version 1 of the Interfaces component of the JUNOSe SNMP agent.  This
        version of the Interfaces component was supported in JUNOSe 1.0 thru 5.0
        system releases."
    STATUS      current
    DESCRIPTION
        "The MIBs supported by the SNMP agent for the Interfaces application in
        JUNOSe.  These capabilities became obsolete when support was added for
        the IF-INVERTED-STACK-MIB."
    SUPPORTS    IF-MIB
        INCLUDES {
            ifGeneralInformationGroup,
            ifFixedLengthGroup,
            ifHCFixedLengthGroup,
            ifPacketGroup,
            ifHCPacketGroup,
            ifVHCPacketGroup,
            ifStackGroup2,
            ifCounterDiscontinuityGroup,
            linkUpDownNotificationsGroup }
        VARIATION   ifAlias
            DESCRIPTION
                "This Agent limits the lenght of an alias to 15 octets excect
                for IP, ATM and ATM 1483 interfaces, which may have a length of
                up to 255 octets."
        VARIATION   ifStackStatus
            ACCESS      read-only
            DESCRIPTION
                "The ifStackTable cannot be modified with this Agent."
    SUPPORTS    Juniper-UNI-IF-MIB
        INCLUDES {
            juniIfGroup,
            juniIfInvStackGroup }
    ::= { juniInterfacesAgent 1 }

juniInterfacesAgentV2  AGENT-CAPABILITIES
    PRODUCT-RELEASE
        "Version 2 of the Interfaces component of the JUNOSe SNMP agent.  This
        version of the Interfaces component is supported in JUNOSe 1.0 and
        subsequent 2.0, 3.x, 4.x and 5.x system releases."
    STATUS      obsolete
    DESCRIPTION
       "The MIBs supported by the SNMP agent for the Interfaces application in
       JUNOSe.  These capabilities became obsolete when support was added for
       the ifCountTable."
    SUPPORTS    IF-MIB
        INCLUDES {
            ifGeneralInformationGroup,
            ifFixedLengthGroup,
            ifHCFixedLengthGroup,
            ifPacketGroup,
            ifHCPacketGroup,
            ifVHCPacketGroup,
            ifStackGroup2,
            ifCounterDiscontinuityGroup,
            linkUpDownNotificationsGroup }
        VARIATION   ifAlias
            DESCRIPTION
                "This Agent limits the lenght of an alias to 15 octets excect
                for IP, ATM and ATM 1483 interfaces, which may have a length of
                up to 255 octets."
        VARIATION   ifStackStatus
            ACCESS      read-only
            DESCRIPTION
                "The ifStackTable cannot be modified with this Agent."
    SUPPORTS    IF-INVERTED-STACK-MIB
        INCLUDES {
            ifInvStackGroup }
    SUPPORTS    Juniper-UNI-IF-MIB
        INCLUDES {
            juniIfGroup,
            juniIfInvStackGroup }
    ::= { juniInterfacesAgent 2 }

juniInterfacesAgentV3  AGENT-CAPABILITIES
    PRODUCT-RELEASE
        "Version 3 of the Interfaces component of the JUNOSe SNMP agent.  This
        version of the Interfaces component is supported in JUNOSe 1.0 and
        subsequent system releases."
    STATUS      current
    DESCRIPTION
        "The MIBs supported by the SNMP agent for the Interfaces application in
        JUNOSe."
    SUPPORTS    IF-MIB
        INCLUDES {
            ifGeneralInformationGroup,
            ifFixedLengthGroup,
            ifHCFixedLengthGroup,
            ifPacketGroup,
            ifHCPacketGroup,
            ifVHCPacketGroup,
            ifStackGroup2,
            ifCounterDiscontinuityGroup,
            linkUpDownNotificationsGroup }
        VARIATION   ifAlias
            DESCRIPTION
                "This Agent limits the lenght of an alias to 15 octets excect
                for IP, ATM and ATM 1483 interfaces, which may have a length of
                up to 255 octets."
        VARIATION   ifStackStatus
            ACCESS      read-only
            DESCRIPTION
                "The ifStackTable cannot be modified with this Agent."
    SUPPORTS    IF-INVERTED-STACK-MIB
        INCLUDES {
            ifInvStackGroup }
    SUPPORTS    Juniper-UNI-IF-MIB
        INCLUDES {
            juniIfGroup,
            juniIfInvStackGroup,
            juniIfCountGroup }
    ::= { juniInterfacesAgent 3 }

END
