
ALCATEL-IND1-SERVICE-MGR-MIB DEFINITIONS ::= BEGIN

        IMPORTS
                MODULE-IDENTITY, OBJECT-IDENTITY, OBJECT-TYPE, Integer32, Counter32, Unsigned32, TimeTicks
			FROM SNMPv2-SMI
		OBJECT-GROUP, MODULE-COMPLIANCE	        
			FROM SNMPv2-CONF
		softentIND1serviceMgr    	
			FROM ALCATEL-IND1-BASE
		RowStatus, TEXTUAL-CONVENTION, DisplayString, TruthValue, MacAddress				
			FROM SNMPv2-TC
		InterfaceIndex 			
			FROM IF-MIB
		AlaEServiceUNIProfileProtocolTreatment	
			FROM ALCATEL-IND1-E-SERVICE-MIB
		svcId, SdpId
			FROM TIMETRA-SERV-MIB
		sapPortId, sapEncapValue 	
			FROM TIMETRA-SAP-MIB
		sdpBindId                       
			FROM TIMETRA-SDP-MIB
		TmnxPortID, TmnxEncapVal, TmnxServId, TmnxVcIdOrNone, SdpBindId	
			FROM TIMETRA-TC-MIB
		InetAddress, InetAddressType
			FROM INET-ADDRESS-MIB
		MplsLdpIdentifier
			FROM MPLS-LDP-MIB
		vRtrID
			FROM TIMETRA-VRTR-MIB
		;
		

        alcatelIND1ServiceMgrMIB MODULE-IDENTITY
		LAST-UPDATED "200901290000Z"
		ORGANIZATION "Alcatel-Lucent"
		CONTACT-INFO
                "Please consult with Customer Service to ensure the most appropriate
                version of this document is used with the products in question:
 	
				                   Alcatel-Lucent, Enterprise Solutions Division
			                    (Formerly Alcatel Internetworking, Incorporated)
				                         26801 West Agoura Road
			 	                       Agoura Hills, CA  91301-5122
			      		                United States Of America
	
                Telephone:	    North America	+1 800 995 2696
				                        Latin America 	+1 877 919 9526
                                Europe		+31 23 556 0100
                                Asia		+65 394 7933
                                All Other	+1 818 878 4507
	
                Electronic Mail:	support@ind.alcatel.com
                World Wide Web:		http://alcatel-lucent.com/wps/portal/enterprise
                File Transfer Protocol:	ftp://ftp.ind.alcatel.com/pub/products/mibs"
                DESCRIPTION
                "The parameters for configuration of the service manager feature.

                The right to make changes in specification and other information
                contained in this document without prior notice is reserved.

                No liability shall be assumed for any incidental, indirect, special, or
                consequential damages whatsoever arising from or related to this 
                document or the information contained herein.

                Vendors, end-users, and other interested parties are granted
                non-exclusive license to use this specification in connection with 
                management of the products for which it is intended to be used.

                               Copyright (C) 1995-2006 Alcatel-Lucent
	                                 ALL RIGHTS RESERVED WORLDWIDE"
		::= { softentIND1serviceMgr 1}

-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx
--  Textual Conventions   (alphabetical)
-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx


AluLocation ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
        "The data type AluLocation represents the
         type of the local 'interface':
         - 'sap(1)': sap interface
         - 'sdp(2)': mesh-sdp or spoke-sdp interface."
    SYNTAX  INTEGER {
                sap(1),
                sdp(2)
            }

-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

alcatelIND1ServiceMgrMIBObjects OBJECT-IDENTITY
        STATUS current
        DESCRIPTION
            "Branch For Service Manager Managed Objects."
     	::= { alcatelIND1ServiceMgrMIB 1 }

alcatelIND1ServiceMgrMIBConformance OBJECT-IDENTITY
        STATUS current
        DESCRIPTION
            "Branch For Service Manager Conformance Information."
    	::= { alcatelIND1ServiceMgrMIB 2 }

alcatelIND1ServiceMgrMIBGroups OBJECT-IDENTITY
        STATUS current
        DESCRIPTION
            "Branch For Service Manager Units Of Conformance."
     	::= { alcatelIND1ServiceMgrMIBConformance 1 }

alcatelIND1ServiceMgrMIBCompliances OBJECT-IDENTITY
        STATUS current
        DESCRIPTION
            "Branch For Service Manager Compliance Statements."
    	 ::= { alcatelIND1ServiceMgrMIBConformance 2 }


-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

--  The Service Manager Group 

     alaServiceMgr OBJECT IDENTIFIER ::= { alcatelIND1ServiceMgrMIBObjects 1 }

-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx


-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

--   The Service Manager Port Profile Table

-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

alaServiceMgrPortProfileTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF  AlaServiceMgrPortProfileEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
        "A table that contains service profiles containing performance and control attributes. 
        An entry in this table is created when a new service profile is defined."
        ::= { alaServiceMgr 1 }

alaServiceMgrPortProfileEntry  OBJECT-TYPE
        SYNTAX  AlaServiceMgrPortProfileEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
        "A Service Manager Port Profile entry."
        INDEX   { alaServiceMgrPortProfileID }
        ::= { alaServiceMgrPortProfileTable 1 }

AlaServiceMgrPortProfileEntry ::= SEQUENCE 
        {
                alaServiceMgrPortProfileID		        DisplayString, 
		alaServiceMgrPortProfileStpBpduTreatment	AlaEServiceUNIProfileProtocolTreatment,
		alaServiceMgrPortProfile8021xTreatment		AlaEServiceUNIProfileProtocolTreatment,
		alaServiceMgrPortProfile8021ABTreatment		AlaEServiceUNIProfileProtocolTreatment,
		alaServiceMgrPortProfile8023adTreatment		AlaEServiceUNIProfileProtocolTreatment,
		alaServiceMgrPortProfileGvrpTreatment		AlaEServiceUNIProfileProtocolTreatment,
		alaServiceMgrPortProfileAmapTreatment		AlaEServiceUNIProfileProtocolTreatment,
		alaServiceMgrPortProfileRowStatus               RowStatus,
		alaServiceMgrPortProfileMvrpTreatment		AlaEServiceUNIProfileProtocolTreatment
        }

alaServiceMgrPortProfileID OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (1..31))
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
        "A label given to uniquely identify this port profile. Must be at least one character long."
        ::= { alaServiceMgrPortProfileEntry 1 }

alaServiceMgrPortProfileStpBpduTreatment  OBJECT-TYPE
        SYNTAX  AlaEServiceUNIProfileProtocolTreatment
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
        "This object describes the behavior of the bridge in regards to the spanning tree 
        protocol BPDU received on the Access Port. Tunnel (1) enables the PDU to be tunneled across 
        the provider network.  Discard (2) causes the PDU of the protocol to be discarded 
        and not enter the provider network. Peer (3) means that on this port the bridge 
        is to participate in the protocol.  Currnetly Peer is not supported for Spanning Tree"
        DEFVAL { tunnel }
        ::= { alaServiceMgrPortProfileEntry 2 }

alaServiceMgrPortProfile8021xTreatment  OBJECT-TYPE
        SYNTAX  AlaEServiceUNIProfileProtocolTreatment
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
        "This object describes the behavior of the bridge in regards to the IEEE 802.1x PDU 
        frames received on the Access Port. Tunnel (1) enables the PDU to be tunneled across 
        the provider network.  Discard (2) causes the PDU of the protocol to be discarded 
        and not enter the provider network. Peer (3) means that on this port the bridge 
        is to participate in the protocol.  Currnetly only drop is supported"
        DEFVAL { drop }
        ::= { alaServiceMgrPortProfileEntry 3 }

alaServiceMgrPortProfile8021ABTreatment  OBJECT-TYPE
        SYNTAX  AlaEServiceUNIProfileProtocolTreatment
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
        "This object describes the behavior of the bridge in regards to the IEEE 802.1AB PDU 
        frames received on the Access Port. Tunnel (1) enables the PDU to be tunneled across 
        the provider network.  Discard (2) causes the PDU of the protocol to be discarded 
        and not enter the provider network. Peer (3) means that on this port the bridge 
        is to participate in the protocol.  Currently drop and tunnel are supported"
        DEFVAL { drop }
        ::= { alaServiceMgrPortProfileEntry 4 }

alaServiceMgrPortProfile8023adTreatment  OBJECT-TYPE
        SYNTAX  AlaEServiceUNIProfileProtocolTreatment
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
        "This object describes the behavior of the bridge in regards to the IEEE 802.1ad PDU 
        frames received on the Access Port. Tunnel (1) enables the PDU to be tunneled across 
        the provider network.  Discard (2) causes the PDU of the protocol to be discarded 
        and not enter the provider network. Peer (3) means that on this port the bridge 
        is to participate in the protocol.  Currently peer and drop are supported"
        DEFVAL { peer }
        ::= { alaServiceMgrPortProfileEntry 5 }

alaServiceMgrPortProfileGvrpTreatment  OBJECT-TYPE
        SYNTAX  AlaEServiceUNIProfileProtocolTreatment
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
        "This object describes the behavior of the bridge in regards to the GVRP PDU 
        frames received on the Access Port. Tunnel (1) enables the PDU to be tunneled across 
        the provider network.  Discard (2) causes the PDU of the protocol to be discarded 
        and not enter the provider network. Peer (3) means that on this port the bridge 
        is to participate in the protocol.  Currently peer is not supported for GVRP"
        DEFVAL { tunnel }
        ::= { alaServiceMgrPortProfileEntry 6 }

alaServiceMgrPortProfileAmapTreatment  OBJECT-TYPE
        SYNTAX  AlaEServiceUNIProfileProtocolTreatment
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
        "This object describes the behavior of the bridge in regards to the Alcatel
        propietary AMAP PDU frames received on the Access Port. Tunnel (1) enables the PDU to 
        be tunneled across the provider network.  Discard (2) causes the PDU of the 
        protocol to be discarded and not enter the provider network. Peer (3) means 
        that on this port the bridge is to participate in the protocol.  Currently 
        drop is only supported"
        DEFVAL { drop }
        ::= { alaServiceMgrPortProfileEntry 7 }

alaServiceMgrPortProfileRowStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS  read-create
        STATUS  current
        DESCRIPTION
        "The status of this table entry."
        ::= { alaServiceMgrPortProfileEntry 8 }	

alaServiceMgrPortProfileMvrpTreatment  OBJECT-TYPE
        SYNTAX  AlaEServiceUNIProfileProtocolTreatment
        MAX-ACCESS  read-create
        STATUS  current
        DESCRIPTION
        "This object describes the behavior of the bridge in regards to the MVRP PDU 
        frames received on the Access Port. Tunnel (1) enables the PDU to be tunneled across 
        the provider network.  Discard (2) causes the PDU of the protocol to be discarded 
        and not enter the provider network. Peer (3) means that on this port the bridge 
        is to participate in the protocol.  Currently peer is not supported for MVRP"
        DEFVAL { tunnel }
        ::= { alaServiceMgrPortProfileEntry 9 }

-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

--   The Service Manager Port Table

-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

alaServiceMgrPortTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF  AlaServiceMgrPortEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
        "The port table has an entry for each port."
        ::= { alaServiceMgr 2 }

alaServiceMgrPortEntry  OBJECT-TYPE
        SYNTAX  AlaServiceMgrPortEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
        "A Service Manager Port entry."
        INDEX   {  alaServiceMgrPortID }
        ::= { alaServiceMgrPortTable 1 }

AlaServiceMgrPortEntry ::= SEQUENCE 
        {
                alaServiceMgrPortID			InterfaceIndex,
		alaServiceMgrPortMode			INTEGER,
		alaServiceMgrPortEncapType              INTEGER,
		alaServiceMgrPortPortProfileID		DisplayString,
		alaServiceMgrPortRowStatus		RowStatus
        }

alaServiceMgrPortID OBJECT-TYPE
        SYNTAX  InterfaceIndex 
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
         "IfIndex uniquely identify this port table."
        ::= { alaServiceMgrPortEntry 1 }

alaServiceMgrPortMode  OBJECT-TYPE
        SYNTAX      INTEGER {
                    undefined (0),
                    access (1),
                    network (2)
                }
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
        "The alaServiceMgrPortMode variable indicates if the interface on this port
         is configured as a service access port or a network access
         port.  

         If port mode equals 'access', alaServiceMgrPortEncapType must also
         be configured to 'qEncap' (For Ethernet MDAs) or to
         'bcpNullEncap' for Sonet/SDH MDAs.  

         Once the port's operation mode has been configured 
         for 'access' mode, multiple services may be configured 
         on the port.  

         If the port mode equals 'network', alaServiceMgrPortEncapType must also
         be configured to 'nullEncap' (Ethernet MDAs), or 'pppAutoEncap'
         (Sonet/SDH MDAs) and tmnxPortEncapType is defaulted to those
         values on the mode change."
        DEFVAL { 2 }
        ::= { alaServiceMgrPortEntry 2 }

alaServiceMgrPortEncapType  OBJECT-TYPE
	SYNTAX      INTEGER {
		    unknown (0),
		    nullEncap (1),
		    qEncap (2)
		    
		}
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
        "The type of encapsulation protocol configured on this
         port's network interface.  If alaServiceMgrPortEncapType has a value
         of 'nullEncap', frames received will not carry any tags
         or labels and as a result only one service can be
         configured on this port.  Sometimes this is referred to
         as raw Ethernet packets. 
                 
         If alaServiceMgrPortEncapType has a value of 'qEncap', ingress frames 
         carry 802.1q tags where each different tag can signify a 
         different service. This is not a valid value if
         Port Class has a value of 'sonetPath'. 
                 
         If alaServiceMgrPortEncapType has a value of 'bcpNullEncap',
         Bcp is used on the sonet path as the NCP control protocol.
         The BCP IEEE 802 Tagged Frame Configuration Option (type 8)
         is negotiated to 'enabled'.  VLAN tagged frames are
         allowed into the sonet path.  Only a single SAP can
         be associated with the sonet path.  'bcpNullEncap' is 
         valid only if Port Class has a value of 'sonetPath'.
                 
         If alaServiceMgrPortEncapType has a value of 'bcpDot1qEncap',
         BCP is used as the NCP control protocol.  The BCP IEEE 802
         Tagged Frame Configuration Option (type 8) is negotiated to
         'enabled'.  VLAN tagged frames are allowed on the sonet path.
         This encapsulation type is required when multiple SAPs are
         defined on the sonet path where each one is service
         delimited by a provisioned Dot1q tag.  When 'bcpDot1qEncap'
         is specified, BCP does not enter the 'open' state unless
         the far end peer also supports 'bcpDot1qEncap'.  This allows
         a LCP negotiation to transmit configuration request and
         confirmation messages to enable this feature.  'bcpDot1qEncap'
         is a valid value only if Port Classhas a value of 'sonetPath'.
 
         If alaServiceMgrPortEncapType has a value of 'ipcpEncap',
         BCP will not be used on this sonet path.  IPCP NCP is used
         instead.  'ipcpEncap' is a valid only if Port Class has
         a value of 'sonetPath'.
         
         If alaServiceMgrPortEncapType has a value of 'frEncap', Frame Relay is
         the expected encapsulation.

         If alaServiceMgrPortEncapType has a value of 'pppAutoEncap', IPCP is 
         automatically enabled. This encap type is only valid on 
         ports/paths in network mode.

         If alaServiceMgrPortEncapType has a value of 'atmEncap', the encapsulation
         on the port is ATM. The 'atmEncap' is also used when mirroring
         ATM ports.

         If alaServiceMgrPortEncapType has a value of 'wanMirrorEncap', the 
         port is used for mirroring of frame-relay and POS ports. On such 
         ports no link management protocol would run.

         If alaServiceMgrPortEncapType has a value of 'ciscoHDLCEncap', the Cisco HDLC
         encapsulation is applied. This encap type is only valid if 
         Port Class has a value of 'tdm' or 'sonet'.
         
         If alaServiceMgrPortEncapType has a value of 'cemEncap', encapsulation of
         frames will be circuit emulation.  This is used to support transparent
         transmission of frames.  This encap type is only valid
         if Port Class has a value of 'tdm' or 'sonet' in access mode.

         alaServiceMgrPortEncapType is set to 'unknown' for physical SONET/SDH and
         TDM ports.
         "
        DEFVAL { 1 }
        ::= { alaServiceMgrPortEntry 3 }

alaServiceMgrPortPortProfileID OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (1..31))
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
        "This labels which Port Profile this port matched to."
        ::= { alaServiceMgrPortEntry 4 }

alaServiceMgrPortRowStatus OBJECT-TYPE
        SYNTAX  RowStatus
        MAX-ACCESS  read-create
        STATUS  current
        DESCRIPTION
        "The status of this table entry."
        ::= { alaServiceMgrPortEntry 5 }	

-- ---------------------------------------------------------------------
--  SAP Extra Information Table
--
--  This is an extension of the sapBaseInfoTable.
--
--  Deletion of a row in the sapBaseInfoTable results in the
--  same fate for the row in the alaSapExtraInfoTable.
-- ---------------------------------------------------------------------

alaSapExtraInfoTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF ASapExtraInfoEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION     "A table that contains SAP information."
    ::= { alaServiceMgr 3 }

alaSapExtraInfoEntry OBJECT-TYPE
    SYNTAX          ASapExtraInfoEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION     "Information about a specific SAP."
    INDEX           { svcId, sapPortId, sapEncapValue }
    ::= { alaSapExtraInfoTable 1 }

ASapExtraInfoEntry ::=
    SEQUENCE {
        alaSapInfoTrusted      	             INTEGER,
        alaSapInfoPriority                   INTEGER
    }

alaSapInfoTrusted  OBJECT-TYPE
	SYNTAX      INTEGER {
		    true (1),
		    false (2)
		}
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
	 "Indicates whether the SAP is trusted.
         "
        DEFVAL { false }
        ::= { alaSapExtraInfoEntry 1 }

alaSapInfoPriority  OBJECT-TYPE
	SYNTAX      INTEGER (0..7)
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
	 "Priority for this SAP.
         "
        DEFVAL { 0 }
        ::= { alaSapExtraInfoEntry 2 }

--
--  Service IGMP Configuration Table
--

alaServiceMgrIgmp OBJECT IDENTIFIER ::= { alcatelIND1ServiceMgrMIBObjects 2 }

alaIgmpServiceTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF IgmpServiceEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The Service table contains the information on which IPv4 multicast
         switching and routing is configured."
    ::= { alaServiceMgrIgmp 1 }

alaIgmpServiceEntry OBJECT-TYPE
    SYNTAX          IgmpServiceEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponds to a service on which IPv4 multicast switching
         and routing is configured."
    INDEX         { 
                    svcId
                  }
    ::= { alaIgmpServiceTable 1 }

IgmpServiceEntry ::= SEQUENCE {
    alaIgmpServiceStatus                     INTEGER,
    alaIgmpServiceQuerying                   INTEGER,
    alaIgmpServiceSpoofing                   INTEGER,
    alaIgmpServiceZapping                    INTEGER,
    alaIgmpServiceVersion                    Unsigned32,
    alaIgmpServiceRobustness                 Unsigned32,
    alaIgmpServiceQueryInterval              Unsigned32,
    alaIgmpServiceQueryResponseInterval      Unsigned32,
    alaIgmpServiceLastMemberQueryInterval    Unsigned32,
    alaIgmpServiceRouterTimeout              Unsigned32,
    alaIgmpServiceSourceTimeout              Unsigned32,
    alaIgmpServiceProxying                   INTEGER,
    alaIgmpServiceUnsolicitedReportInterval  Unsigned32,
    alaIgmpServiceQuerierForwarding          INTEGER,
    alaIgmpServiceMaxGroupLimit  		  Unsigned32,
    alaIgmpServiceMaxGroupExceedAction       INTEGER
}


alaIgmpServiceStatus OBJECT-TYPE
    SYNTAX          INTEGER { none(0), enable(1), disable(2) }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Administratively enable IPv4 multicast switching and routing 
         on the Service."
    ::= { alaIgmpServiceEntry 1 }

alaIgmpServiceQuerying OBJECT-TYPE
    SYNTAX          INTEGER { none(0), enable(1), disable(2) }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Administratively enable IGMP Querying on the Service."
    ::= { alaIgmpServiceEntry 2 }

alaIgmpServiceSpoofing OBJECT-TYPE
    SYNTAX          INTEGER { none(0), enable(1), disable(2) }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Administratively enable IGMP Spoofing on the Service."
    ::= { alaIgmpServiceEntry 3 }

alaIgmpServiceZapping OBJECT-TYPE
    SYNTAX          INTEGER { none(0), enable(1), disable(2) }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Administratively enable IGMP Zapping on the Service."
    ::= { alaIgmpServiceEntry 4 }

alaIgmpServiceVersion OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Set the default IGMP protocol Version running on the Service."
    ::= { alaIgmpServiceEntry 5 }

alaIgmpServiceRobustness OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Set the IGMP Robustness variable used on the Service."
    ::= { alaIgmpServiceEntry 6 }

alaIgmpServiceQueryInterval OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Set the IGMP Query Interval used on the Service."
    ::= { alaIgmpServiceEntry 7 }

alaIgmpServiceQueryResponseInterval OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "tenths of seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Set the IGMP Query Response Interval on the Service."
    ::= { alaIgmpServiceEntry 8 }

alaIgmpServiceLastMemberQueryInterval OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "tenths of seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Set the IGMP Last Member Query Interval on the Service."
    ::= { alaIgmpServiceEntry 9 }

alaIgmpServiceRouterTimeout OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Set the IGMP Router Timeout on the Service."
    ::= { alaIgmpServiceEntry 10 }

alaIgmpServiceSourceTimeout OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Set the IGMP Source Timeout on the Service."
    ::= { alaIgmpServiceEntry 11 }

alaIgmpServiceProxying OBJECT-TYPE
    SYNTAX          INTEGER { none(0), enable(1), disable(2) }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Administratively enable IGMP Proxying on the Service."
    ::= { alaIgmpServiceEntry 12 }

alaIgmpServiceUnsolicitedReportInterval OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Set the IGMP Unsolicited Report Interval on the Service."
    ::= { alaIgmpServiceEntry 13 }

alaIgmpServiceQuerierForwarding OBJECT-TYPE
    SYNTAX          INTEGER { none(0), enable(1), disable(2) }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Administratively enable IGMP Querier Forwarding on the Service."
    ::= { alaIgmpServiceEntry 14 }

alaIgmpServiceMaxGroupLimit OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The maximum number of IGMP Group memberships that can be learnt on the Service."
    DEFVAL 		{0}
    ::= { alaIgmpServiceEntry 15 }

alaIgmpServiceMaxGroupExceedAction OBJECT-TYPE
    SYNTAX          INTEGER { none(0), drop(1), replace(2) }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The action to be taken when the IGMP group membership limit is exceeded on the Service."
    DEFVAL        { none }
    ::= { alaIgmpServiceEntry 16 }


--
--  Service Group Membership Table
--


alaIgmpMemberServiceSapTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF IgmpMemberServiceSapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the IGMP group membership information for SAPs."
    ::= { alaServiceMgrIgmp 2 }

alaIgmpMemberServiceSapEntry OBJECT-TYPE
    SYNTAX          IgmpMemberServiceSapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to an IGMP group membership request."
    INDEX         { 
                    svcId,
                    sapPortId,
                    sapEncapValue,
		    alaIgmpMemberServiceSapGroupAddressType,
                    alaIgmpMemberServiceSapGroupAddress,
                    alaIgmpMemberServiceSapSourceAddressType,
		    alaIgmpMemberServiceSapSourceAddress
                  }
    ::= { alaIgmpMemberServiceSapTable 1 }

IgmpMemberServiceSapEntry ::= SEQUENCE {
    alaIgmpMemberServiceSapGroupAddressType         InetAddressType,
    alaIgmpMemberServiceSapGroupAddress             InetAddress,
    alaIgmpMemberServiceSapSourceAddressType        InetAddressType,
    alaIgmpMemberServiceSapSourceAddress            InetAddress,
    alaIgmpMemberServiceSapMode                     INTEGER,
    alaIgmpMemberServiceSapCount                    Counter32,
    alaIgmpMemberServiceSapTimeout                  TimeTicks
   
}

alaIgmpMemberServiceSapGroupAddressType OBJECT-TYPE
        SYNTAX InetAddressType (1)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv4."
        ::= { alaIgmpMemberServiceSapEntry 1 }

alaIgmpMemberServiceSapGroupAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The group membership request's IPv4 group address."
    ::= { alaIgmpMemberServiceSapEntry 2 }

alaIgmpMemberServiceSapSourceAddressType OBJECT-TYPE
        SYNTAX InetAddressType (1)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv4."
        ::= { alaIgmpMemberServiceSapEntry 3 }

alaIgmpMemberServiceSapSourceAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The group membership request's IPv4 source address."
    ::= { alaIgmpMemberServiceSapEntry 4 }

alaIgmpMemberServiceSapMode OBJECT-TYPE
    SYNTAX          INTEGER { include(1), exclude(2) }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The group membership request's IGMP source filter mode."
    ::= { alaIgmpMemberServiceSapEntry 5 }

alaIgmpMemberServiceSapCount OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The group membership request's counter."
    ::= { alaIgmpMemberServiceSapEntry 6 }

alaIgmpMemberServiceSapTimeout OBJECT-TYPE
    SYNTAX          TimeTicks
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The group membership request's timeout."
    ::= { alaIgmpMemberServiceSapEntry 7}


alaIgmpMemberServiceSdpBindTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF IgmpMemberServiceSdpBindEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the IGMP group membership information for SDP bindings."
    ::= { alaServiceMgrIgmp 3 }

alaIgmpMemberServiceSdpBindEntry OBJECT-TYPE
    SYNTAX          IgmpMemberServiceSdpBindEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to an IGMP group membership request."
    INDEX         { 
                    svcId,
                    sdpBindId,
		    alaIgmpMemberServiceSdpBindGroupAddressType,
                    alaIgmpMemberServiceSdpBindGroupAddress,
                    alaIgmpMemberServiceSdpBindSourceAddressType,
		    alaIgmpMemberServiceSdpBindSourceAddress
                  }
    ::= { alaIgmpMemberServiceSdpBindTable 1 }

IgmpMemberServiceSdpBindEntry ::= SEQUENCE {
    alaIgmpMemberServiceSdpBindGroupAddressType         InetAddressType,
    alaIgmpMemberServiceSdpBindGroupAddress             InetAddress,
    alaIgmpMemberServiceSdpBindSourceAddressType        InetAddressType,
    alaIgmpMemberServiceSdpBindSourceAddress            InetAddress,
    alaIgmpMemberServiceSdpBindMode                     INTEGER,
    alaIgmpMemberServiceSdpBindCount                    Counter32,
    alaIgmpMemberServiceSdpBindTimeout                  TimeTicks
}

alaIgmpMemberServiceSdpBindGroupAddressType OBJECT-TYPE
        SYNTAX InetAddressType (1)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv4."
        ::= { alaIgmpMemberServiceSdpBindEntry 1 }

alaIgmpMemberServiceSdpBindGroupAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The group membership request's IPv4 group address."
    ::= { alaIgmpMemberServiceSdpBindEntry 2 }

alaIgmpMemberServiceSdpBindSourceAddressType OBJECT-TYPE
        SYNTAX InetAddressType (1)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv4."
        ::= { alaIgmpMemberServiceSdpBindEntry 3 }

alaIgmpMemberServiceSdpBindSourceAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The group membership request's IPv4 source address."
    ::= { alaIgmpMemberServiceSdpBindEntry 4 }

alaIgmpMemberServiceSdpBindMode OBJECT-TYPE
    SYNTAX          INTEGER { include(1), exclude(2) }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The group membership request's IGMP source filter mode."
    ::= { alaIgmpMemberServiceSdpBindEntry 5 }

alaIgmpMemberServiceSdpBindCount OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The group membership request's counter."
    ::= { alaIgmpMemberServiceSdpBindEntry 6 }

alaIgmpMemberServiceSdpBindTimeout OBJECT-TYPE
    SYNTAX          TimeTicks
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The group membership request's timeout."
    ::= { alaIgmpMemberServiceSdpBindEntry 7 }

--
--  Static Group Membership Table
--

alaIgmpStaticMemberServiceSapTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF IgmpStaticMemberServiceSapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the service sap static IGMP group membership information."
    ::= { alaServiceMgrIgmp 4 }

alaIgmpStaticMemberServiceSapEntry OBJECT-TYPE
    SYNTAX          IgmpStaticMemberServiceSapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to a ervice sap static IGMP group membership request."
    INDEX         { 
                    svcId,
                    sapPortId,
                    sapEncapValue,
		    alaIgmpStaticMemberServiceSapGroupAddressType,
                    alaIgmpStaticMemberServiceSapGroupAddress
                  }
    ::= { alaIgmpStaticMemberServiceSapTable 1 }

IgmpStaticMemberServiceSapEntry ::= SEQUENCE {
    alaIgmpStaticMemberServiceSapGroupAddressType   InetAddressType,
    alaIgmpStaticMemberServiceSapGroupAddress       InetAddress,
    alaIgmpStaticMemberServiceSapRowStatus          RowStatus
}

alaIgmpStaticMemberServiceSapGroupAddressType OBJECT-TYPE
        SYNTAX InetAddressType (1)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv4."
        ::= { alaIgmpStaticMemberServiceSapEntry 1 }

alaIgmpStaticMemberServiceSapGroupAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The service sap static group membership request's IPv4 group address."
    ::= { alaIgmpStaticMemberServiceSapEntry 2 }

alaIgmpStaticMemberServiceSapRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Used in accordance with installation and removal conventions
         for conceptual rows."
    ::= { alaIgmpStaticMemberServiceSapEntry 3}


alaIgmpStaticMemberServiceSdpBindTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF IgmpStaticMemberServiceSdpBindEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the service sdp binding static IGMP group membership information."
    ::= { alaServiceMgrIgmp 5 }

alaIgmpStaticMemberServiceSdpBindEntry OBJECT-TYPE
    SYNTAX          IgmpStaticMemberServiceSdpBindEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to a service sdp binding static IGMP group membership request."
    INDEX         { 
                    svcId,
                    sdpBindId,
		    alaIgmpStaticMemberServiceSdpBindGroupAddressType,
                    alaIgmpStaticMemberServiceSdpBindGroupAddress
                  }
    ::= { alaIgmpStaticMemberServiceSdpBindTable 1 }

IgmpStaticMemberServiceSdpBindEntry ::= SEQUENCE {
    alaIgmpStaticMemberServiceSdpBindGroupAddressType   InetAddressType,
    alaIgmpStaticMemberServiceSdpBindGroupAddress       InetAddress,
    alaIgmpStaticMemberServiceSdpBindRowStatus          RowStatus
}

alaIgmpStaticMemberServiceSdpBindGroupAddressType OBJECT-TYPE
        SYNTAX InetAddressType (1)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv4."
        ::= { alaIgmpStaticMemberServiceSdpBindEntry 1 }

alaIgmpStaticMemberServiceSdpBindGroupAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The service sdp binding static group membership request's IPv4 group address."
    ::= { alaIgmpStaticMemberServiceSdpBindEntry 2 }

alaIgmpStaticMemberServiceSdpBindRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Used in accordance with installation and removal conventions
         for conceptual rows."
    ::= { alaIgmpStaticMemberServiceSdpBindEntry 3}


--
--  Neighbor Table
--

alaIgmpNeighborServiceSapTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF IgmpNeighborServiceSapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the service sap neighboring IP multicast routers."
    ::= { alaServiceMgrIgmp 6 }

alaIgmpNeighborServiceSapEntry OBJECT-TYPE
    SYNTAX          IgmpNeighborServiceSapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to an IP multicast router."
    INDEX         { 
		    svcId,
                    sapPortId,
                    sapEncapValue,
		    alaIgmpNeighborServiceSapHostAddressType,
                    alaIgmpNeighborServiceSapHostAddress
                  }
    ::= { alaIgmpNeighborServiceSapTable 1 }

IgmpNeighborServiceSapEntry ::= SEQUENCE {
    alaIgmpNeighborServiceSapHostAddressType	    InetAddressType,
    alaIgmpNeighborServiceSapHostAddress            InetAddress,
    alaIgmpNeighborServiceSapCount                  Counter32,
    alaIgmpNeighborServiceSapTimeout                TimeTicks
}


alaIgmpNeighborServiceSapHostAddressType OBJECT-TYPE
        SYNTAX InetAddressType (1)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv4."
        ::= { alaIgmpNeighborServiceSapEntry 1 }

alaIgmpNeighborServiceSapHostAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast router's IPv4 host address."
    ::= { alaIgmpNeighborServiceSapEntry 2 }

alaIgmpNeighborServiceSapCount OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The IP multicast router's counter."
    ::= { alaIgmpNeighborServiceSapEntry 3 }

alaIgmpNeighborServiceSapTimeout OBJECT-TYPE
    SYNTAX          TimeTicks
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The IP multicast router's timeout."
    ::= { alaIgmpNeighborServiceSapEntry 4 }

alaIgmpNeighborServiceSdpBindTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF IgmpNeighborServiceSdpBindEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the service SdpBind neighboring IP multicast routers."
    ::= { alaServiceMgrIgmp 7 }

alaIgmpNeighborServiceSdpBindEntry OBJECT-TYPE
    SYNTAX          IgmpNeighborServiceSdpBindEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to an IP multicast router."
    INDEX         { 
		    svcId,
                    sdpBindId,
		    alaIgmpNeighborServiceSdpBindHostAddressType,
                    alaIgmpNeighborServiceSdpBindHostAddress
                  }
    ::= { alaIgmpNeighborServiceSdpBindTable 1 }

IgmpNeighborServiceSdpBindEntry ::= SEQUENCE {
    alaIgmpNeighborServiceSdpBindHostAddressType	InetAddressType,
    alaIgmpNeighborServiceSdpBindHostAddress            InetAddress,
    alaIgmpNeighborServiceSdpBindCount                  Counter32,
    alaIgmpNeighborServiceSdpBindTimeout                TimeTicks
}

alaIgmpNeighborServiceSdpBindHostAddressType OBJECT-TYPE
        SYNTAX InetAddressType (1)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv4."
        ::= { alaIgmpNeighborServiceSdpBindEntry 1 }

alaIgmpNeighborServiceSdpBindHostAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast router's IPv4 host address."
    ::= { alaIgmpNeighborServiceSdpBindEntry 2 }

alaIgmpNeighborServiceSdpBindCount OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The IP multicast router's counter."
    ::= { alaIgmpNeighborServiceSdpBindEntry 3 }

alaIgmpNeighborServiceSdpBindTimeout OBJECT-TYPE
    SYNTAX          TimeTicks
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The IP multicast router's timeout."
    ::= { alaIgmpNeighborServiceSdpBindEntry 4 }


--
--  Static Neighbor Table
--


alaIgmpStaticNeighborServiceSapTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF IgmpStaticNeighborServiceSapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the service sap static IP multicast routers."
    ::= { alaServiceMgrIgmp 8 }

alaIgmpStaticNeighborServiceSapEntry OBJECT-TYPE
    SYNTAX          IgmpStaticNeighborServiceSapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to a service sap static IP multicast router."
    INDEX         { 
		    svcId,
                    sapPortId,
                    sapEncapValue

                  }
    ::= { alaIgmpStaticNeighborServiceSapTable 1 }

IgmpStaticNeighborServiceSapEntry ::= SEQUENCE {
    alaIgmpStaticNeighborServiceSapRowStatus        RowStatus
}

alaIgmpStaticNeighborServiceSapRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Used in accordance with installation and removal conventions
         for conceptual rows."
    ::= { alaIgmpStaticNeighborServiceSapEntry 1 }


alaIgmpStaticNeighborServiceSdpBindTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF IgmpStaticNeighborServiceSdpBindEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the service SdpBind static IP multicast routers."
    ::= { alaServiceMgrIgmp 9 }

alaIgmpStaticNeighborServiceSdpBindEntry OBJECT-TYPE
    SYNTAX          IgmpStaticNeighborServiceSdpBindEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to a service SdpBind static IP multicast router."
    INDEX         { 
		    svcId,
                    sdpBindId
                  }
    ::= { alaIgmpStaticNeighborServiceSdpBindTable 1 }

IgmpStaticNeighborServiceSdpBindEntry ::= SEQUENCE {
    alaIgmpStaticNeighborServiceSdpBindRowStatus        RowStatus
}

alaIgmpStaticNeighborServiceSdpBindRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Used in accordance with installation and removal conventions
         for conceptual rows."
    ::= { alaIgmpStaticNeighborServiceSdpBindEntry 1 }


--
--  Querier Table
--


alaIgmpQuerierServiceSapTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF IgmpQuerierServiceSapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the service sap neighboring IGMP queriers."
    ::= { alaServiceMgrIgmp 10 }

alaIgmpQuerierServiceSapEntry OBJECT-TYPE
    SYNTAX          IgmpQuerierServiceSapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to an IGMP querier."
    INDEX         { 
                    svcId,
                    sapPortId,
                    sapEncapValue,
		    alaIgmpQuerierServiceSapHostAddressType,
                    alaIgmpQuerierServiceSapHostAddress
                  }
    ::= { alaIgmpQuerierServiceSapTable 1 }

IgmpQuerierServiceSapEntry ::= SEQUENCE {
    alaIgmpQuerierServiceSapHostAddressType	    InetAddressType,
    alaIgmpQuerierServiceSapHostAddress             InetAddress,
    alaIgmpQuerierServiceSapCount                   Counter32,
    alaIgmpQuerierServiceSapTimeout                 TimeTicks
}
alaIgmpQuerierServiceSapHostAddressType OBJECT-TYPE
        SYNTAX InetAddressType (1)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv4."
        ::= { alaIgmpQuerierServiceSapEntry 1 }

alaIgmpQuerierServiceSapHostAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IGMP querier's IPv4 host address."
    ::= { alaIgmpQuerierServiceSapEntry 2 }

alaIgmpQuerierServiceSapCount OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The IGMP querier's counter."
    ::= { alaIgmpQuerierServiceSapEntry 3 }

alaIgmpQuerierServiceSapTimeout OBJECT-TYPE
    SYNTAX          TimeTicks
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The IGMP querier's timeout."
    ::= { alaIgmpQuerierServiceSapEntry 4 }

alaIgmpQuerierServiceSdpBindTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF IgmpQuerierServiceSdpBindEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the service SdpBind neighboring IGMP queriers."
    ::= { alaServiceMgrIgmp 11 }

alaIgmpQuerierServiceSdpBindEntry OBJECT-TYPE
    SYNTAX          IgmpQuerierServiceSdpBindEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to an IGMP querier."
    INDEX         { 
                   
		    svcId,
                    sdpBindId,
		    alaIgmpQuerierServiceSdpBindHostAddressType,
                    alaIgmpQuerierServiceSdpBindHostAddress
                  }
    ::= { alaIgmpQuerierServiceSdpBindTable 1 }

IgmpQuerierServiceSdpBindEntry ::= SEQUENCE {
    alaIgmpQuerierServiceSdpBindHostAddressType		InetAddressType,
    alaIgmpQuerierServiceSdpBindHostAddress             InetAddress,
    alaIgmpQuerierServiceSdpBindCount                   Counter32,
    alaIgmpQuerierServiceSdpBindTimeout                 TimeTicks
}

alaIgmpQuerierServiceSdpBindHostAddressType OBJECT-TYPE
        SYNTAX InetAddressType (1)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv4."
        ::= { alaIgmpQuerierServiceSdpBindEntry 1 }

alaIgmpQuerierServiceSdpBindHostAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IGMP querier's IPv4 host address."
    ::= { alaIgmpQuerierServiceSdpBindEntry 2 }

alaIgmpQuerierServiceSdpBindCount OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The IGMP querier's counter."
    ::= { alaIgmpQuerierServiceSdpBindEntry 3 }

alaIgmpQuerierServiceSdpBindTimeout OBJECT-TYPE
    SYNTAX          TimeTicks
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The IGMP querier's timeout."
    ::= { alaIgmpQuerierServiceSdpBindEntry 4 }


--
--  Static Querier Table
--


alaIgmpStaticQuerierServiceSapTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF IgmpStaticQuerierServiceSapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the service sap static IGMP queriers."
    ::= { alaServiceMgrIgmp 12 }

alaIgmpStaticQuerierServiceSapEntry OBJECT-TYPE
    SYNTAX          IgmpStaticQuerierServiceSapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to a static IGMP querier."
    INDEX         { 
                    svcId,
                    sapPortId,
                    sapEncapValue
                  }
    ::= { alaIgmpStaticQuerierServiceSapTable 1 }

IgmpStaticQuerierServiceSapEntry ::= SEQUENCE {
    alaIgmpStaticQuerierServiceSapRowStatus         RowStatus
}


alaIgmpStaticQuerierServiceSapRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Used in accordance with installation and removal conventions
         for conceptual rows."
    ::= { alaIgmpStaticQuerierServiceSapEntry 1 }


alaIgmpStaticQuerierServiceSdpBindTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF IgmpStaticQuerierServiceSdpBindEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the service SdpBind static IGMP queriers."
    ::= { alaServiceMgrIgmp 13 }

alaIgmpStaticQuerierServiceSdpBindEntry OBJECT-TYPE
    SYNTAX          IgmpStaticQuerierServiceSdpBindEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to a static IGMP querier."
    INDEX         { 
                    
		    svcId,
                    sdpBindId
                  }
    ::= { alaIgmpStaticQuerierServiceSdpBindTable 1 }

IgmpStaticQuerierServiceSdpBindEntry ::= SEQUENCE {
    alaIgmpStaticQuerierServiceSdpBindRowStatus         RowStatus
}


alaIgmpStaticQuerierServiceSdpBindRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Used in accordance with installation and removal conventions
         for conceptual rows."
    ::= { alaIgmpStaticQuerierServiceSdpBindEntry 1 }



--
--  Source Table
--


alaIgmpServiceSourceTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF IgmpServiceSourceEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the Service IP multicast source information."
    ::= { alaServiceMgrIgmp 14 }

alaIgmpServiceSourceEntry OBJECT-TYPE
    SYNTAX          IgmpServiceSourceEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to an IP multicast source flow."
    INDEX         { 
                    svcId,
		    alaIgmpServiceSourceGroupAddressType,
                    alaIgmpServiceSourceGroupAddress,
                    alaIgmpServiceSourceHostAddressType,
		    alaIgmpServiceSourceHostAddress,
                    alaIgmpServiceSourceDestAddressType,
		    alaIgmpServiceSourceDestAddress,
                    alaIgmpServiceSourceOrigAddressType,
		    alaIgmpServiceSourceOrigAddress
                  }
    ::= { alaIgmpServiceSourceTable 1 }

IgmpServiceSourceEntry ::= SEQUENCE {
    alaIgmpServiceSourceGroupAddressType	 InetAddressType,
    alaIgmpServiceSourceGroupAddress             InetAddress,
    alaIgmpServiceSourceHostAddressType		 InetAddressType,
    alaIgmpServiceSourceHostAddress              InetAddress,
    alaIgmpServiceSourceDestAddressType		 InetAddressType,
    alaIgmpServiceSourceDestAddress              InetAddress,
    alaIgmpServiceSourceOrigAddressType		 InetAddressType,
    alaIgmpServiceSourceOrigAddress              InetAddress,
    alaIgmpServiceSourceLocale			  AluLocation,
    alaIgmpServiceSourcePortId                   TmnxPortID,
    alaIgmpServiceSourceEncapValue               TmnxEncapVal,
    alaIgmpServiceSourceSdpId                    SdpId,
    alaIgmpServiceSourceVcId                     TmnxVcIdOrNone,
    alaIgmpServiceSourceType                     INTEGER
}

alaIgmpServiceSourceGroupAddressType OBJECT-TYPE
        SYNTAX InetAddressType (1)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv4."
        ::= { alaIgmpServiceSourceEntry 1 }

alaIgmpServiceSourceGroupAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast source flow's IPv4 group address."
    ::= { alaIgmpServiceSourceEntry 2 }

alaIgmpServiceSourceHostAddressType OBJECT-TYPE
        SYNTAX InetAddressType (1)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv4."
        ::= { alaIgmpServiceSourceEntry 3 }

alaIgmpServiceSourceHostAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast source flow's IPv4 host address."
    ::= { alaIgmpServiceSourceEntry 4 }

alaIgmpServiceSourceDestAddressType OBJECT-TYPE
        SYNTAX InetAddressType (1)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv4."
        ::= { alaIgmpServiceSourceEntry 5 }

alaIgmpServiceSourceDestAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast source flow's IPv4 tunnel destination address."
    ::= { alaIgmpServiceSourceEntry 6 }

alaIgmpServiceSourceOrigAddressType OBJECT-TYPE
        SYNTAX InetAddressType (1)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv4."
        ::= { alaIgmpServiceSourceEntry 7 }

alaIgmpServiceSourceOrigAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast source flow's IPv4 tunnel source address."
    ::= { alaIgmpServiceSourceEntry 8 }

alaIgmpServiceSourceLocale OBJECT-TYPE
    SYNTAX      AluLocation
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaIgmpServiceSourceLocale indicates
         where this multicast router was detected.

         A multicast router found on a local SAP has the value 'sap(1)'.
         A multicast router detected on an SDP has the value 'sdp(2)'."
    ::= { alaIgmpServiceSourceEntry 9 }

alaIgmpServiceSourcePortId OBJECT-TYPE
    SYNTAX      TmnxPortID
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaIgmpServiceSourcePortId indicates,
         together with the object alaIgmpServiceSourceEncapValue, the SAP
         on which this multicast router is detected.

         The value of this object is only meaningful when the value of
         tlsIgmpSnpgMRouterLocale is 'sap(1)'."
    ::= { alaIgmpServiceSourceEntry 10 }

alaIgmpServiceSourceEncapValue OBJECT-TYPE
    SYNTAX      TmnxEncapVal
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaIgmpServiceSourceEncapValue indicates,
         together with the objectalaIgmpServiceSourcePortId, the SAP
         on which this multicast router is detected.

         The value of this object is only meaningful when the value of
         alaIgmpServiceSourceLocale is 'sap(1)'."
    ::= { alaIgmpServiceSourceEntry 11 }

alaIgmpServiceSourceSdpId OBJECT-TYPE
    SYNTAX      SdpId
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaIgmpServiceSourceSdpId indicates,
         together with the object alaIgmpServiceSourceVcId, the SDP Bind
         on which this multicast router is detected.

         The value of this object is only meaningful when the value of
         alaIgmpServiceSourceLocale is 'sdp(2)'."
    ::= { alaIgmpServiceSourceEntry 12 }

alaIgmpServiceSourceVcId OBJECT-TYPE
    SYNTAX      TmnxVcIdOrNone
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaIgmpServiceSourceVcId indicates,
         together with the object alaIgmpServiceSourceSdpId, the SDP Bind
         on which this multicast router is detected.

         The value of this object is only meaningful when the value of
         alaIgmpServiceSourceLocale is 'sdp(2)'."
    ::= { alaIgmpServiceSourceEntry 13 }

alaIgmpServiceSourceType OBJECT-TYPE
    SYNTAX          INTEGER { mcast(1), pim(2), ipip(3) }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The IP multicast source flow's encapsulation type."
    ::= { alaIgmpServiceSourceEntry 14 }

--
--  Forward Table
--

alaIgmpServiceSapForwardTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF IgmpServiceSapForwardEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the IP multicast forward information."
    ::= { alaServiceMgrIgmp 15 }

alaIgmpServiceSapForwardEntry OBJECT-TYPE
    SYNTAX          IgmpServiceSapForwardEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to an IP multicast forwarded flow."
    INDEX         { 
                    svcId,
                    alaIgmpServiceSapForwardGroupAddress,
                    alaIgmpServiceSapForwardHostAddress,
                    alaIgmpServiceSapForwardDestAddress,
                    alaIgmpServiceSapForwardOrigAddress,
                    alaIgmpServiceSapForwardNextSapPortId,
		    alaIgmpServiceSapForwardNextSapEncapValue

                  }
    ::= { alaIgmpServiceSapForwardTable 1 }

IgmpServiceSapForwardEntry ::= SEQUENCE {

    alaIgmpServiceSapForwardLocale		    AluLocation,
    alaIgmpServiceSapForwardPortId                  TmnxPortID,
    alaIgmpServiceSapForwardEncapValue              TmnxEncapVal,
    alaIgmpServiceSapForwardSdpId                   SdpId,
    alaIgmpServiceSapForwardVcId                    TmnxVcIdOrNone,
    alaIgmpServiceSapForwardGroupAddress            MacAddress,
    alaIgmpServiceSapForwardHostAddress             MacAddress,
    alaIgmpServiceSapForwardDestAddress             MacAddress,
    alaIgmpServiceSapForwardOrigAddress             MacAddress,
    alaIgmpServiceSapForwardType                    INTEGER,
    alaIgmpServiceSapForwardNextSapPortId           TmnxPortID,
    alaIgmpServiceSapForwardNextSapEncapValue       TmnxEncapVal,
    alaIgmpServiceSapForwardNextType                    INTEGER

  
}

alaIgmpServiceSapForwardLocale OBJECT-TYPE
    SYNTAX      AluLocation
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaIgmpServiceSapForwardLocale indicates
         where this multicast router was detected.

         A multicast router found on a local SAP has the value 'sap(1)'.
         A multicast router detected on an SDP has the value 'sdp(2)'."
    ::= { alaIgmpServiceSapForwardEntry 1 }

alaIgmpServiceSapForwardPortId OBJECT-TYPE
    SYNTAX      TmnxPortID
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaIgmpServiceSapForwardPortId indicates,
         together with the object alaIgmpServiceSapForwardEncapValue, the SAP
         on which this multicast router is detected.

         The value of this object is only meaningful when the value of
         tlsIgmpSnpgMRouterLocale is 'sap(1)'."
    ::= { alaIgmpServiceSapForwardEntry 2 }

alaIgmpServiceSapForwardEncapValue OBJECT-TYPE
    SYNTAX      TmnxEncapVal
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaIgmpServiceSapForwardEncapValue indicates,
         together with the objectalaIgmpServiceSapForwardPortId, the SAP
         on which this multicast router is detected.

         The value of this object is only meaningful when the value of
         alaIgmpServiceSapForwardLocale is 'sap(1)'."
    ::= { alaIgmpServiceSapForwardEntry 3 }

alaIgmpServiceSapForwardSdpId OBJECT-TYPE
    SYNTAX      SdpId
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaIgmpServiceSapForwardSdpId indicates,
         together with the object alaIgmpServiceSapForwardVcId, the SDP Bind
         on which this multicast router is detected.

         The value of this object is only meaningful when the value of
         alaIgmpServiceSapForwardLocale is 'sdp(2)'."
    ::= { alaIgmpServiceSapForwardEntry 4 }

alaIgmpServiceSapForwardVcId OBJECT-TYPE
    SYNTAX      TmnxVcIdOrNone
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaIgmpServiceSapForwardVcId indicates,
         together with the object alaIgmpServiceSapForwardSdpId, the SDP Bind
         on which this multicast router is detected.

         The value of this object is only meaningful when the value of
         alaIgmpServiceSapForwardLocale is 'sdp(2)'."
    ::= { alaIgmpServiceSapForwardEntry 5 }


alaIgmpServiceSapForwardGroupAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast forwarded flow's IPv4 group address."
    ::= { alaIgmpServiceSapForwardEntry 6 }

alaIgmpServiceSapForwardHostAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast forwarded flow's IPv4 host address."
    ::= { alaIgmpServiceSapForwardEntry 7 }

alaIgmpServiceSapForwardDestAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast forwarded flow's IPv4 tunnel destination address."
    ::= { alaIgmpServiceSapForwardEntry 8 }

alaIgmpServiceSapForwardOrigAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast forwarded flow's IPv4 tunnel source address."
    ::= { alaIgmpServiceSapForwardEntry 9 }

alaIgmpServiceSapForwardType OBJECT-TYPE
    SYNTAX          INTEGER { mcast(1), pim(2), ipip(3) }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The IP multicast forwarded flow's encapsulation type."
    ::= { alaIgmpServiceSapForwardEntry 10 }


alaIgmpServiceSapForwardNextSapPortId OBJECT-TYPE
    SYNTAX          TmnxPortID
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION     "The IP multicast forwarded flow's next SAP. The ID of the access port where this SAP
                     is defined."
    ::= { alaIgmpServiceSapForwardEntry 11 }

alaIgmpServiceSapForwardNextSapEncapValue OBJECT-TYPE
    SYNTAX          TmnxEncapVal
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION     "The IP multicast forwarded flow's next SAP. The value of the label used to identify this
                     SAP on the access port specified by sapPortId."
    ::= { alaIgmpServiceSapForwardEntry 12 }

alaIgmpServiceSapForwardNextType OBJECT-TYPE
    SYNTAX          INTEGER { mcast(1), pim(2), ipip(3) }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The IP multicast forwarded flow's next encapsulation type."
    ::= { alaIgmpServiceSapForwardEntry 13 }

alaIgmpServiceSdpBindForwardTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF IgmpServiceSdpBindForwardEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the IP multicast forward information."
    ::= { alaServiceMgrIgmp 16 }

alaIgmpServiceSdpBindForwardEntry OBJECT-TYPE
    SYNTAX          IgmpServiceSdpBindForwardEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to an IP multicast forwarded flow."
    INDEX         { 
                    svcId,
                    alaIgmpServiceSdpBindForwardGroupAddress,
                    alaIgmpServiceSdpBindForwardHostAddress,
                    alaIgmpServiceSdpBindForwardDestAddress,
                    alaIgmpServiceSdpBindForwardOrigAddress,
                    alaIgmpServiceSdpBindForwardNextSdpBindId

                  }
    ::= { alaIgmpServiceSdpBindForwardTable 1 }

IgmpServiceSdpBindForwardEntry ::= SEQUENCE {

    alaIgmpServiceSdpBindForwardLocale		    AluLocation,
    alaIgmpServiceSdpBindForwardPortId                  TmnxPortID,
    alaIgmpServiceSdpBindForwardEncapValue              TmnxEncapVal,
    alaIgmpServiceSdpBindForwardSdpId                   SdpId,
    alaIgmpServiceSdpBindForwardVcId                    TmnxVcIdOrNone,
    alaIgmpServiceSdpBindForwardGroupAddress            MacAddress,
    alaIgmpServiceSdpBindForwardHostAddress             MacAddress,
    alaIgmpServiceSdpBindForwardDestAddress             MacAddress,
    alaIgmpServiceSdpBindForwardOrigAddress             MacAddress,
    alaIgmpServiceSdpBindForwardType                    INTEGER,
    alaIgmpServiceSdpBindForwardNextSdpBindId          SdpBindId,
    alaIgmpServiceSdpBindForwardNextType                    INTEGER

  
}

alaIgmpServiceSdpBindForwardLocale OBJECT-TYPE
    SYNTAX      AluLocation
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaIgmpServiceSdpBindForwardLocale indicates
         where this multicast router was detected.

         A multicast router found on a local SAP has the value 'sap(1)'.
         A multicast router detected on an SDP has the value 'sdp(2)'."
    ::= { alaIgmpServiceSdpBindForwardEntry 1 }

alaIgmpServiceSdpBindForwardPortId OBJECT-TYPE
    SYNTAX      TmnxPortID
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaIgmpServiceSdpBindForwardPortId indicates,
         together with the object alaIgmpServiceSdpBindForwardEncapValue, the SdpBind
         on which this multicast router is detected.

         The value of this object is only meaningful when the value of
         tlsIgmpSnpgMRouterLocale is 'sap(1)'."
    ::= { alaIgmpServiceSdpBindForwardEntry 2 }

alaIgmpServiceSdpBindForwardEncapValue OBJECT-TYPE
    SYNTAX      TmnxEncapVal
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaIgmpServiceSdpBindForwardEncapValue indicates,
         together with the object alaIgmpServiceSdpBindForwardPortId, the SAP
         on which this multicast router is detected.

         The value of this object is only meaningful when the value of
         alaIgmpServiceSdpBindForwardLocale is 'sap(1)'."
    ::= { alaIgmpServiceSdpBindForwardEntry 3 }

alaIgmpServiceSdpBindForwardSdpId OBJECT-TYPE
    SYNTAX      SdpId
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaIgmpServiceSdpBindForwardSdpId indicates,
         together with the object alaIgmpServiceSdpBindForwardVcId, the SDP Bind
         on which this multicast router is detected.

         The value of this object is only meaningful when the value of
         alaIgmpServiceSdpBindForwardLocale is 'sdp(2)'."
    ::= { alaIgmpServiceSdpBindForwardEntry 4 }

alaIgmpServiceSdpBindForwardVcId OBJECT-TYPE
    SYNTAX      TmnxVcIdOrNone
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaIgmpServiceSdpBindForwardVcId indicates,
         together with the object alaIgmpServiceSdpBindForwardSdpId, the SDP Bind
         on which this multicast router is detected.

         The value of this object is only meaningful when the value of
         alaIgmpServiceSdpBindForwardLocale is 'sdp(2)'."
    ::= { alaIgmpServiceSdpBindForwardEntry 5 }


alaIgmpServiceSdpBindForwardGroupAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast forwarded flow's IPv4 group address."
    ::= { alaIgmpServiceSdpBindForwardEntry 6 }

alaIgmpServiceSdpBindForwardHostAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast forwarded flow's IPv4 host address."
    ::= { alaIgmpServiceSdpBindForwardEntry 7 }

alaIgmpServiceSdpBindForwardDestAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast forwarded flow's IPv4 tunnel destination address."
    ::= { alaIgmpServiceSdpBindForwardEntry 8 }

alaIgmpServiceSdpBindForwardOrigAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast forwarded flow's IPv4 tunnel source address."
    ::= { alaIgmpServiceSdpBindForwardEntry 9 }

alaIgmpServiceSdpBindForwardType OBJECT-TYPE
    SYNTAX          INTEGER { mcast(1), pim(2), ipip(3) }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The IP multicast forwarded flow's encapsulation type."
    ::= { alaIgmpServiceSdpBindForwardEntry 10 }



alaIgmpServiceSdpBindForwardNextSdpBindId OBJECT-TYPE
    SYNTAX          SdpBindId
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION     "The IP multicast forwarded flow's next sdpBind."
    ::= { alaIgmpServiceSdpBindForwardEntry 11 }



alaIgmpServiceSdpBindForwardNextType OBJECT-TYPE
    SYNTAX          INTEGER { mcast(1), pim(2), ipip(3) }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The IP multicast forwarded flow's next encapsulation type."
    ::= { alaIgmpServiceSdpBindForwardEntry 12 }


--
--  SAP/SDPBIND Table for IP Multicast objects managed per  SAP/SDPBIND 
--
		
alaIgmpServiceSapTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF AlaIgmpServiceSapEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION 
       "The table listing the IP multicast port information."   
     ::= { alaServiceMgrIgmp 17 }
   
alaIgmpServiceSapEntry OBJECT-TYPE
     SYNTAX     AlaIgmpServiceSapEntry
     MAX-ACCESS not-accessible
     STATUS     current
     DESCRIPTION 
       "An entry corresponding to IP multicast Service SAP information."
     INDEX        { 
		    svcId,
                    sapPortId,
                    sapEncapValue
                  }
    ::= { alaIgmpServiceSapTable 1 }
   
AlaIgmpServiceSapEntry ::=
     SEQUENCE {
       alaIgmpServiceSapMaxGroupLimit   		Unsigned32,
       alaIgmpServiceSapMaxGroupExceedAction    	INTEGER,
       alaIgmpServiceSapCurrentGroupCount     		Unsigned32
     }
 

alaIgmpServiceSapMaxGroupLimit OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The maximum number of IGMP Group memberships that can be learnt 
	on the sap."
    DEFVAL 		{0}
    ::= { alaIgmpServiceSapEntry 1 }

alaIgmpServiceSapMaxGroupExceedAction OBJECT-TYPE
    SYNTAX          INTEGER { none(0), drop(1), replace(2) }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The action to be taken when IGMP group membership limit is 
	exceeded for the sap."
    DEFVAL        { none }
    ::= { alaIgmpServiceSapEntry 2 }


alaIgmpServiceSapCurrentGroupCount OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The current IP multicast group memberships on a sap. 
	instance."
    ::= { alaIgmpServiceSapEntry 3 }

alaIgmpServiceSdpBindTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF AlaIgmpServiceSdpBindEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION 
       "The table listing the IP multicast port information."   
     ::= { alaServiceMgrIgmp 18 }
   
alaIgmpServiceSdpBindEntry OBJECT-TYPE
     SYNTAX     AlaIgmpServiceSdpBindEntry
     MAX-ACCESS not-accessible
     STATUS     current
     DESCRIPTION 
       "An entry corresponding to IP multicast Service SdpBind information."
     INDEX        { 
		    svcId,
                    sdpBindId
                  }
    ::= { alaIgmpServiceSdpBindTable 1 }
   
AlaIgmpServiceSdpBindEntry ::=
     SEQUENCE {
       alaIgmpServiceSdpBindMaxGroupLimit   		Unsigned32,
       alaIgmpServiceSdpBindMaxGroupExceedAction    	INTEGER,
       alaIgmpServiceSdpBindCurrentGroupCount     		Unsigned32
     }
 

alaIgmpServiceSdpBindMaxGroupLimit OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The maximum number of IGMP Group memberships that can be learnt 
	on the SdpBind."
    DEFVAL 		{0}
    ::= { alaIgmpServiceSdpBindEntry 1 }

alaIgmpServiceSdpBindMaxGroupExceedAction OBJECT-TYPE
    SYNTAX          INTEGER { none(0), drop(1), replace(2) }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The action to be taken when IGMP group membership limit is 
	exceeded for the SdpBind."
    DEFVAL        { none }
    ::= { alaIgmpServiceSdpBindEntry 2 }

alaIgmpServiceSdpBindCurrentGroupCount OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The current IP multicast group memberships on a SdpBind. 
	instance."
    ::= { alaIgmpServiceSdpBindEntry 3 }

--
--  Service MLD Configuration Table
--

alaServiceMgrMld OBJECT IDENTIFIER ::= { alcatelIND1ServiceMgrMIBObjects 3 }

alaMldServiceTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF MldServiceEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The Service table contains the information on which IPv6 multicast
         switching and routing is configured."
    ::= { alaServiceMgrMld 1 }

alaMldServiceEntry OBJECT-TYPE
    SYNTAX          MldServiceEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponds to a service on which IPv6 multicast switching
         and routing is configured."
    INDEX         { 
                    svcId
                  }
    ::= { alaMldServiceTable 1 }

MldServiceEntry ::= SEQUENCE {
    alaMldServiceStatus                     INTEGER,
    alaMldServiceQuerying                   INTEGER,
    alaMldServiceSpoofing                   INTEGER,
    alaMldServiceZapping                    INTEGER,
    alaMldServiceVersion                    Unsigned32,
    alaMldServiceRobustness                 Unsigned32,
    alaMldServiceQueryInterval              Unsigned32,
    alaMldServiceQueryResponseInterval      Unsigned32,
    alaMldServiceLastMemberQueryInterval    Unsigned32,
    alaMldServiceRouterTimeout              Unsigned32,
    alaMldServiceSourceTimeout              Unsigned32,
    alaMldServiceProxying                   INTEGER,
    alaMldServiceUnsolicitedReportInterval  Unsigned32,
    alaMldServiceQuerierForwarding          INTEGER,
    alaMldServiceMaxGroupLimit  		  Unsigned32,
    alaMldServiceMaxGroupExceedAction       INTEGER
}


alaMldServiceStatus OBJECT-TYPE
    SYNTAX          INTEGER { none(0), enable(1), disable(2) }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Administratively enable IPv6 multicast switching and routing 
         on the Service."
    ::= { alaMldServiceEntry 1 }

alaMldServiceQuerying OBJECT-TYPE
    SYNTAX          INTEGER { none(0), enable(1), disable(2) }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Administratively enable MLD Querying on the Service."
    ::= { alaMldServiceEntry 2 }

alaMldServiceSpoofing OBJECT-TYPE
    SYNTAX          INTEGER { none(0), enable(1), disable(2) }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Administratively enable MLD Spoofing on the Service."
    ::= { alaMldServiceEntry 3 }

alaMldServiceZapping OBJECT-TYPE
    SYNTAX          INTEGER { none(0), enable(1), disable(2) }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Administratively enable MLD Zapping on the Service."
    ::= { alaMldServiceEntry 4 }

alaMldServiceVersion OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Set the default MLD protocol Version running on the Service."
    ::= { alaMldServiceEntry 5 }

alaMldServiceRobustness OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Set the MLD Robustness variable used on the Service."
    ::= { alaMldServiceEntry 6 }

alaMldServiceQueryInterval OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Set the MLD Query Interval used on the Service."
    ::= { alaMldServiceEntry 7 }

alaMldServiceQueryResponseInterval OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "tenths of seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Set the MLD Query Response Interval on the Service."
    ::= { alaMldServiceEntry 8 }

alaMldServiceLastMemberQueryInterval OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "tenths of seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Set the MLD Last Member Query Interval on the Service."
    ::= { alaMldServiceEntry 9 }

alaMldServiceRouterTimeout OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Set the MLD Router Timeout on the Service."
    ::= { alaMldServiceEntry 10 }

alaMldServiceSourceTimeout OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Set the MLD Source Timeout on the Service."
    ::= { alaMldServiceEntry 11 }

alaMldServiceProxying OBJECT-TYPE
    SYNTAX          INTEGER { none(0), enable(1), disable(2) }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Administratively enable MLD Proxying on the Service."
    ::= { alaMldServiceEntry 12 }

alaMldServiceUnsolicitedReportInterval OBJECT-TYPE
    SYNTAX          Unsigned32
    UNITS           "seconds"
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Set the MLD Unsolicited Report Interval on the Service."
    ::= { alaMldServiceEntry 13 }

alaMldServiceQuerierForwarding OBJECT-TYPE
    SYNTAX          INTEGER { none(0), enable(1), disable(2) }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "Administratively enable MLD Querier Forwarding on the Service."
    ::= { alaMldServiceEntry 14 }

alaMldServiceMaxGroupLimit OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The maximum number of MLD Group memberships that can be learnt on the Service."
    DEFVAL 		{0}
    ::= { alaMldServiceEntry 15 }

alaMldServiceMaxGroupExceedAction OBJECT-TYPE
    SYNTAX          INTEGER { none(0), drop(1), replace(2) }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The action to be taken when the MLD group membership limit is exceeded on the Service."
    DEFVAL        { none }
    ::= { alaMldServiceEntry 16 }


--
--  Service Group Membership Table
--


alaMldMemberServiceSapTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF MldMemberServiceSapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the MLD group membership information for SAPs."
    ::= { alaServiceMgrMld 2 }

alaMldMemberServiceSapEntry OBJECT-TYPE
    SYNTAX          MldMemberServiceSapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to an MLD group membership request."
    INDEX         { 
                    svcId,
                    sapPortId,
                    sapEncapValue,
		    alaMldMemberServiceSapGroupAddressType,
                    alaMldMemberServiceSapGroupAddress,
                    alaMldMemberServiceSapSourceAddressType,
		    alaMldMemberServiceSapSourceAddress
                  }
    ::= { alaMldMemberServiceSapTable 1 }

MldMemberServiceSapEntry ::= SEQUENCE {
    alaMldMemberServiceSapGroupAddressType         InetAddressType,
    alaMldMemberServiceSapGroupAddress             InetAddress,
    alaMldMemberServiceSapSourceAddressType        InetAddressType,
    alaMldMemberServiceSapSourceAddress            InetAddress,
    alaMldMemberServiceSapMode                     INTEGER,
    alaMldMemberServiceSapCount                    Counter32,
    alaMldMemberServiceSapTimeout                  TimeTicks
}

alaMldMemberServiceSapGroupAddressType OBJECT-TYPE
        SYNTAX InetAddressType (2)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv6."
        ::= { alaMldMemberServiceSapEntry 1 }

alaMldMemberServiceSapGroupAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The group membership request's IPv6 group address."
    ::= { alaMldMemberServiceSapEntry 2 }

alaMldMemberServiceSapSourceAddressType OBJECT-TYPE
        SYNTAX InetAddressType (2)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv6."
        ::= { alaMldMemberServiceSapEntry 3 }

alaMldMemberServiceSapSourceAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The group membership request's IPv6 source address."
    ::= { alaMldMemberServiceSapEntry 4 }

alaMldMemberServiceSapMode OBJECT-TYPE
    SYNTAX          INTEGER { include(1), exclude(2) }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The group membership request's MLD source filter mode."
    ::= { alaMldMemberServiceSapEntry 5 }

alaMldMemberServiceSapCount OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The group membership request's counter."
    ::= { alaMldMemberServiceSapEntry 6 }

alaMldMemberServiceSapTimeout OBJECT-TYPE
    SYNTAX          TimeTicks
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The group membership request's timeout."
    ::= { alaMldMemberServiceSapEntry 7 }


alaMldMemberServiceSdpBindTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF MldMemberServiceSdpBindEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the MLD group membership information for SDP bindings."
    ::= { alaServiceMgrMld 3 }

alaMldMemberServiceSdpBindEntry OBJECT-TYPE
    SYNTAX          MldMemberServiceSdpBindEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to an MLD group membership request."
    INDEX         { 
                    svcId,
                    sdpBindId,
		    alaMldMemberServiceSdpBindGroupAddressType,
                    alaMldMemberServiceSdpBindGroupAddress,
                    alaMldMemberServiceSdpBindSourceAddressType,
		    alaMldMemberServiceSdpBindSourceAddress
                  }
    ::= { alaMldMemberServiceSdpBindTable 1 }

MldMemberServiceSdpBindEntry ::= SEQUENCE {
    alaMldMemberServiceSdpBindGroupAddressType         InetAddressType,
    alaMldMemberServiceSdpBindGroupAddress             InetAddress,
    alaMldMemberServiceSdpBindSourceAddressType        InetAddressType,
    alaMldMemberServiceSdpBindSourceAddress            InetAddress,
    alaMldMemberServiceSdpBindMode                     INTEGER,
    alaMldMemberServiceSdpBindCount                    Counter32,
    alaMldMemberServiceSdpBindTimeout                  TimeTicks
}

alaMldMemberServiceSdpBindGroupAddressType OBJECT-TYPE
        SYNTAX InetAddressType (2)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv6."
        ::= { alaMldMemberServiceSdpBindEntry 1 }

alaMldMemberServiceSdpBindGroupAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The group membership request's IPv6 group address."
    ::= { alaMldMemberServiceSdpBindEntry 2 }

alaMldMemberServiceSdpBindSourceAddressType OBJECT-TYPE
        SYNTAX InetAddressType (2)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv6."
        ::= { alaMldMemberServiceSdpBindEntry 3 }

alaMldMemberServiceSdpBindSourceAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The group membership request's IPv6 source address."
    ::= { alaMldMemberServiceSdpBindEntry 4 }

alaMldMemberServiceSdpBindMode OBJECT-TYPE
    SYNTAX          INTEGER { include(1), exclude(2) }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The group membership request's MLD source filter mode."
    ::= { alaMldMemberServiceSdpBindEntry 5 }

alaMldMemberServiceSdpBindCount OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The group membership request's counter."
    ::= { alaMldMemberServiceSdpBindEntry 6 }

alaMldMemberServiceSdpBindTimeout OBJECT-TYPE
    SYNTAX          TimeTicks
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The group membership request's timeout."
    ::= { alaMldMemberServiceSdpBindEntry 7 }

--
--  Static Group Membership Table
--

alaMldStaticMemberServiceSapTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF MldStaticMemberServiceSapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the service sap static MLD group membership information."
    ::= { alaServiceMgrMld 4 }

alaMldStaticMemberServiceSapEntry OBJECT-TYPE
    SYNTAX          MldStaticMemberServiceSapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to a ervice sap static MLD group membership request."
    INDEX         { 
                    svcId,
                    sapPortId,
                    sapEncapValue,
		    alaMldStaticMemberServiceSapGroupAddressType,
                    alaMldStaticMemberServiceSapGroupAddress
                  }
    ::= { alaMldStaticMemberServiceSapTable 1 }

MldStaticMemberServiceSapEntry ::= SEQUENCE {
    alaMldStaticMemberServiceSapGroupAddressType   InetAddressType,
    alaMldStaticMemberServiceSapGroupAddress       InetAddress,
    alaMldStaticMemberServiceSapRowStatus          RowStatus
}

alaMldStaticMemberServiceSapGroupAddressType OBJECT-TYPE
        SYNTAX InetAddressType (2)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv6."
        ::= { alaMldStaticMemberServiceSapEntry 1 }

alaMldStaticMemberServiceSapGroupAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The service sap static group membership request's IPv6 group address."
    ::= { alaMldStaticMemberServiceSapEntry 2 }

alaMldStaticMemberServiceSapRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Used in accordance with installation and removal conventions
         for conceptual rows."
    ::= { alaMldStaticMemberServiceSapEntry 3}


alaMldStaticMemberServiceSdpBindTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF MldStaticMemberServiceSdpBindEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the service sdp binding static MLD group membership information."
    ::= { alaServiceMgrMld 5 }

alaMldStaticMemberServiceSdpBindEntry OBJECT-TYPE
    SYNTAX          MldStaticMemberServiceSdpBindEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to a service sdp binding static MLD group membership request."
    INDEX         { 
                    svcId,
                    sdpBindId,
		    alaMldStaticMemberServiceSapGroupAddressType,
                    alaMldStaticMemberServiceSapGroupAddress
                  }
    ::= { alaMldStaticMemberServiceSdpBindTable 1 }

MldStaticMemberServiceSdpBindEntry ::= SEQUENCE {
    alaMldStaticMemberServiceSdpBindGroupAddressType   InetAddressType,
    alaMldStaticMemberServiceSdpBindGroupAddress       InetAddress,
    alaMldStaticMemberServiceSdpBindRowStatus          RowStatus
}

alaMldStaticMemberServiceSdpBindGroupAddressType OBJECT-TYPE
        SYNTAX InetAddressType (2)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv6."
        ::= { alaMldStaticMemberServiceSdpBindEntry 1 }

alaMldStaticMemberServiceSdpBindGroupAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The service sdp binding static group membership request's IPv6 group address."
    ::= { alaMldStaticMemberServiceSdpBindEntry 2 }

alaMldStaticMemberServiceSdpBindRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Used in accordance with installation and removal conventions
         for conceptual rows."
    ::= { alaMldStaticMemberServiceSdpBindEntry 3}


--
--  Neighbor Table
--

alaMldNeighborServiceSapTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF MldNeighborServiceSapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the service sap neighboring IP multicast routers."
    ::= { alaServiceMgrMld 6 }

alaMldNeighborServiceSapEntry OBJECT-TYPE
    SYNTAX          MldNeighborServiceSapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to an IP multicast router."
    INDEX         { 
		    svcId,
                    sapPortId,
                    sapEncapValue,
		    alaMldNeighborServiceSapHostAddressType,
                    alaMldNeighborServiceSapHostAddress
                  }
    ::= { alaMldNeighborServiceSapTable 1 }

MldNeighborServiceSapEntry ::= SEQUENCE {
    alaMldNeighborServiceSapHostAddressType        InetAddressType,
    alaMldNeighborServiceSapHostAddress            InetAddress,
    alaMldNeighborServiceSapCount                  Counter32,
    alaMldNeighborServiceSapTimeout                TimeTicks
}

alaMldNeighborServiceSapHostAddressType OBJECT-TYPE
        SYNTAX InetAddressType (2)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv6."
        ::= { alaMldNeighborServiceSapEntry 1 }

alaMldNeighborServiceSapHostAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast router's IPv6 host address."
    ::= { alaMldNeighborServiceSapEntry 2 }

alaMldNeighborServiceSapCount OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The IP multicast router's counter."
    ::= { alaMldNeighborServiceSapEntry 3 }

alaMldNeighborServiceSapTimeout OBJECT-TYPE
    SYNTAX          TimeTicks
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The IP multicast router's timeout."
    ::= { alaMldNeighborServiceSapEntry 4 }

alaMldNeighborServiceSdpBindTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF MldNeighborServiceSdpBindEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the service SdpBind neighboring IP multicast routers."
    ::= { alaServiceMgrMld 7 }

alaMldNeighborServiceSdpBindEntry OBJECT-TYPE
    SYNTAX          MldNeighborServiceSdpBindEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to an IP multicast router."
    INDEX         { 
		    svcId,
                    sdpBindId,
		    alaMldNeighborServiceSdpBindHostAddressType,
                    alaMldNeighborServiceSdpBindHostAddress
                  }
    ::= { alaMldNeighborServiceSdpBindTable 1 }

MldNeighborServiceSdpBindEntry ::= SEQUENCE {
    alaMldNeighborServiceSdpBindHostAddressType        InetAddressType,
    alaMldNeighborServiceSdpBindHostAddress            InetAddress,
    alaMldNeighborServiceSdpBindCount                  Counter32,
    alaMldNeighborServiceSdpBindTimeout                TimeTicks
}


alaMldNeighborServiceSdpBindHostAddressType OBJECT-TYPE
        SYNTAX InetAddressType (2)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv6."
        ::= { alaMldNeighborServiceSdpBindEntry 1 }

alaMldNeighborServiceSdpBindHostAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast router's IPv6 host address."
    ::= { alaMldNeighborServiceSdpBindEntry 2 }

alaMldNeighborServiceSdpBindCount OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The IP multicast router's counter."
    ::= { alaMldNeighborServiceSdpBindEntry 3 }

alaMldNeighborServiceSdpBindTimeout OBJECT-TYPE
    SYNTAX          TimeTicks
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The IP multicast router's timeout."
    ::= { alaMldNeighborServiceSdpBindEntry 4 }


--
--  Static Neighbor Table
--


alaMldStaticNeighborServiceSapTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF MldStaticNeighborServiceSapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the service sap static IP multicast routers."
    ::= { alaServiceMgrMld 8 }

alaMldStaticNeighborServiceSapEntry OBJECT-TYPE
    SYNTAX          MldStaticNeighborServiceSapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to a service sap static IP multicast router."
    INDEX         { 
		    svcId,
                    sapPortId,
                    sapEncapValue

                  }
    ::= { alaMldStaticNeighborServiceSapTable 1 }

MldStaticNeighborServiceSapEntry ::= SEQUENCE {
    alaMldStaticNeighborServiceSapRowStatus        RowStatus
}

alaMldStaticNeighborServiceSapRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Used in accordance with installation and removal conventions
         for conceptual rows."
    ::= { alaMldStaticNeighborServiceSapEntry 1 }


alaMldStaticNeighborServiceSdpBindTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF MldStaticNeighborServiceSdpBindEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the service SdpBind static IP multicast routers."
    ::= { alaServiceMgrMld 9 }

alaMldStaticNeighborServiceSdpBindEntry OBJECT-TYPE
    SYNTAX          MldStaticNeighborServiceSdpBindEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to a service SdpBind static IP multicast router."
    INDEX         { 
		    svcId,
                    sdpBindId
                  }
    ::= { alaMldStaticNeighborServiceSdpBindTable 1 }

MldStaticNeighborServiceSdpBindEntry ::= SEQUENCE {
    alaMldStaticNeighborServiceSdpBindRowStatus        RowStatus
}

alaMldStaticNeighborServiceSdpBindRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Used in accordance with installation and removal conventions
         for conceptual rows."
    ::= { alaMldStaticNeighborServiceSdpBindEntry 1 }


--
--  Querier Table
--


alaMldQuerierServiceSapTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF MldQuerierServiceSapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the service sap neighboring MLD queriers."
    ::= { alaServiceMgrMld 10 }

alaMldQuerierServiceSapEntry OBJECT-TYPE
    SYNTAX          MldQuerierServiceSapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to an MLD querier."
    INDEX         { 
                    svcId,
                    sapPortId,
                    sapEncapValue,
		    alaMldQuerierServiceSapHostAddressType,
                    alaMldQuerierServiceSapHostAddress
                  }
    ::= { alaMldQuerierServiceSapTable 1 }

MldQuerierServiceSapEntry ::= SEQUENCE {
    alaMldQuerierServiceSapHostAddressType         InetAddressType,
    alaMldQuerierServiceSapHostAddress             InetAddress,
    alaMldQuerierServiceSapCount                   Counter32,
    alaMldQuerierServiceSapTimeout                 TimeTicks
}

alaMldQuerierServiceSapHostAddressType OBJECT-TYPE
        SYNTAX InetAddressType (2)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv6."
        ::= { alaMldQuerierServiceSapEntry 1 }

alaMldQuerierServiceSapHostAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The MLD querier's IPv6 host address."
    ::= { alaMldQuerierServiceSapEntry 2 }

alaMldQuerierServiceSapCount OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The MLD querier's counter."
    ::= { alaMldQuerierServiceSapEntry 3 }

alaMldQuerierServiceSapTimeout OBJECT-TYPE
    SYNTAX          TimeTicks
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The MLD querier's timeout."
    ::= { alaMldQuerierServiceSapEntry 4 }

alaMldQuerierServiceSdpBindTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF MldQuerierServiceSdpBindEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the service SdpBind neighboring MLD queriers."
    ::= { alaServiceMgrMld 11 }

alaMldQuerierServiceSdpBindEntry OBJECT-TYPE
    SYNTAX          MldQuerierServiceSdpBindEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to an MLD querier."
    INDEX         { 
                   
		    svcId,
                    sdpBindId,
		    alaMldQuerierServiceSdpBindHostAddressType,
                    alaMldQuerierServiceSdpBindHostAddress
                  }
    ::= { alaMldQuerierServiceSdpBindTable 1 }

MldQuerierServiceSdpBindEntry ::= SEQUENCE {
    alaMldQuerierServiceSdpBindHostAddressType         InetAddressType,
    alaMldQuerierServiceSdpBindHostAddress             InetAddress,
    alaMldQuerierServiceSdpBindCount                   Counter32,
    alaMldQuerierServiceSdpBindTimeout                 TimeTicks
}

alaMldQuerierServiceSdpBindHostAddressType OBJECT-TYPE
        SYNTAX InetAddressType (2)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv6."
        ::= { alaMldQuerierServiceSdpBindEntry 1 }

alaMldQuerierServiceSdpBindHostAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The MLD querier's IPv6 host address."
    ::= { alaMldQuerierServiceSdpBindEntry 2 }

alaMldQuerierServiceSdpBindCount OBJECT-TYPE
    SYNTAX          Counter32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The MLD querier's counter."
    ::= { alaMldQuerierServiceSdpBindEntry 3 }

alaMldQuerierServiceSdpBindTimeout OBJECT-TYPE
    SYNTAX          TimeTicks
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The MLD querier's timeout."
    ::= { alaMldQuerierServiceSdpBindEntry 4 }


--
--  Static Querier Table
--


alaMldStaticQuerierServiceSapTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF MldStaticQuerierServiceSapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the service sap static MLD queriers."
    ::= { alaServiceMgrMld 12 }

alaMldStaticQuerierServiceSapEntry OBJECT-TYPE
    SYNTAX          MldStaticQuerierServiceSapEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to a static MLD querier."
    INDEX         { 
                    svcId,
                    sapPortId,
                    sapEncapValue
                  }
    ::= { alaMldStaticQuerierServiceSapTable 1 }

MldStaticQuerierServiceSapEntry ::= SEQUENCE {
    alaMldStaticQuerierServiceSapRowStatus         RowStatus
}


alaMldStaticQuerierServiceSapRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Used in accordance with installation and removal conventions
         for conceptual rows."
    ::= { alaMldStaticQuerierServiceSapEntry 1 }


alaMldStaticQuerierServiceSdpBindTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF MldStaticQuerierServiceSdpBindEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the service SdpBind static MLD queriers."
    ::= { alaServiceMgrMld 13 }

alaMldStaticQuerierServiceSdpBindEntry OBJECT-TYPE
    SYNTAX          MldStaticQuerierServiceSdpBindEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to a static MLD querier."
    INDEX         { 
                    
		    svcId,
                    sdpBindId
                  }
    ::= { alaMldStaticQuerierServiceSdpBindTable 1 }

MldStaticQuerierServiceSdpBindEntry ::= SEQUENCE {
    alaMldStaticQuerierServiceSdpBindRowStatus         RowStatus
}


alaMldStaticQuerierServiceSdpBindRowStatus OBJECT-TYPE
    SYNTAX          RowStatus
    MAX-ACCESS      read-create
    STATUS          current
    DESCRIPTION
        "Used in accordance with installation and removal conventions
         for conceptual rows."
    ::= { alaMldStaticQuerierServiceSdpBindEntry 1 }



--
--  Source Table
--


alaMldServiceSourceTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF MldServiceSourceEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the Service IP multicast source information."
    ::= { alaServiceMgrMld 14 }

alaMldServiceSourceEntry OBJECT-TYPE
    SYNTAX          MldServiceSourceEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to an IP multicast source flow."
    INDEX         { 
                    svcId,
		    alaMldServiceSourceGroupAddressType,
                    alaMldServiceSourceGroupAddress,
		    alaMldServiceSourceHostAddressType,
                    alaMldServiceSourceHostAddress,
		    alaMldServiceSourceDestAddressType,
                    alaMldServiceSourceDestAddress,
		    alaMldServiceSourceOrigAddressType,
                    alaMldServiceSourceOrigAddress
                  }
    ::= { alaMldServiceSourceTable 1 }

MldServiceSourceEntry ::= SEQUENCE {
    alaMldServiceSourceGroupAddressType         InetAddressType,
    alaMldServiceSourceGroupAddress             InetAddress,
    alaMldServiceSourceHostAddressType          InetAddressType,
    alaMldServiceSourceHostAddress              InetAddress,
    alaMldServiceSourceDestAddressType          InetAddressType,
    alaMldServiceSourceDestAddress              InetAddress,
    alaMldServiceSourceOrigAddressType          InetAddressType,
    alaMldServiceSourceOrigAddress              InetAddress,
    alaMldServiceSourceLocale			  AluLocation,
    alaMldServiceSourcePortId                   TmnxPortID,
    alaMldServiceSourceEncapValue               TmnxEncapVal,
    alaMldServiceSourceSdpId                    SdpId,
    alaMldServiceSourceVcId                     TmnxVcIdOrNone,
    alaMldServiceSourceType                     INTEGER
}


alaMldServiceSourceGroupAddressType OBJECT-TYPE
        SYNTAX InetAddressType (2)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv6."
        ::= { alaMldServiceSourceEntry 1 }

alaMldServiceSourceGroupAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast source flow's IPv6 group address."
    ::= { alaMldServiceSourceEntry 2 }

alaMldServiceSourceHostAddressType OBJECT-TYPE
        SYNTAX InetAddressType (2)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv6."
        ::= { alaMldServiceSourceEntry 3 }

alaMldServiceSourceHostAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast source flow's IPv6 host address."
    ::= { alaMldServiceSourceEntry 4 }

alaMldServiceSourceDestAddressType OBJECT-TYPE
        SYNTAX InetAddressType (2)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv6."
        ::= { alaMldServiceSourceEntry 5 }

alaMldServiceSourceDestAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast source flow's IPv6 tunnel destination address."
    ::= { alaMldServiceSourceEntry 6 }

alaMldServiceSourceOrigAddressType OBJECT-TYPE
        SYNTAX InetAddressType (2)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
        "The IP address type. This release only supports IPv6."
        ::= { alaMldServiceSourceEntry 7 }

alaMldServiceSourceOrigAddress OBJECT-TYPE
    SYNTAX       InetAddress(SIZE(4|16))
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast source flow's IPv6 tunnel source address."
    ::= { alaMldServiceSourceEntry 8 }

alaMldServiceSourceLocale OBJECT-TYPE
    SYNTAX      AluLocation
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaMldServiceSourceLocale indicates
         where this multicast router was detected.

         A multicast router found on a local SAP has the value 'sap(1)'.
         A multicast router detected on an SDP has the value 'sdp(2)'."
    ::= { alaMldServiceSourceEntry 9 }

alaMldServiceSourcePortId OBJECT-TYPE
    SYNTAX      TmnxPortID
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaMldServiceSourcePortId indicates,
         together with the object alaMldServiceSourceEncapValue, the SAP
         on which this multicast router is detected.

         The value of this object is only meaningful when the value of
         tlsMldSnpgMRouterLocale is 'sap(1)'."
    ::= { alaMldServiceSourceEntry 10 }

alaMldServiceSourceEncapValue OBJECT-TYPE
    SYNTAX      TmnxEncapVal
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaMldServiceSourceEncapValue indicates,
         together with the objectalaMldServiceSourcePortId, the SAP
         on which this multicast router is detected.

         The value of this object is only meaningful when the value of
         alaMldServiceSourceLocale is 'sap(1)'."
    ::= { alaMldServiceSourceEntry 11 }

alaMldServiceSourceSdpId OBJECT-TYPE
    SYNTAX      SdpId
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaMldServiceSourceSdpId indicates,
         together with the object alaMldServiceSourceVcId, the SDP Bind
         on which this multicast router is detected.

         The value of this object is only meaningful when the value of
         alaMldServiceSourceLocale is 'sdp(2)'."
    ::= { alaMldServiceSourceEntry 12 }

alaMldServiceSourceVcId OBJECT-TYPE
    SYNTAX      TmnxVcIdOrNone
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaMldServiceSourceVcId indicates,
         together with the object alaMldServiceSourceSdpId, the SDP Bind
         on which this multicast router is detected.

         The value of this object is only meaningful when the value of
         alaMldServiceSourceLocale is 'sdp(2)'."
    ::= { alaMldServiceSourceEntry 13 }

alaMldServiceSourceType OBJECT-TYPE
    SYNTAX          INTEGER { mcast(1), pim(2), ipip(3) }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The IP multicast source flow's encapsulation type."
    ::= { alaMldServiceSourceEntry 14 }

--
--  Forward Table
--

alaMldServiceSapForwardTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF MldServiceSapForwardEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the IP multicast forward information."
    ::= { alaServiceMgrMld 15 }

alaMldServiceSapForwardEntry OBJECT-TYPE
    SYNTAX          MldServiceSapForwardEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to an IP multicast forwarded flow."
    INDEX         { 
                    svcId,
                    alaMldServiceSapForwardGroupAddress,
                    alaMldServiceSapForwardHostAddress,
                    alaMldServiceSapForwardDestAddress,
                    alaMldServiceSapForwardOrigAddress,
                    alaMldServiceSapForwardNextSapPortId,
		    alaMldServiceSapForwardNextSapEncapValue

                  }
    ::= { alaMldServiceSapForwardTable 1 }

MldServiceSapForwardEntry ::= SEQUENCE {

    alaMldServiceSapForwardLocale		    AluLocation,
    alaMldServiceSapForwardPortId                  TmnxPortID,
    alaMldServiceSapForwardEncapValue              TmnxEncapVal,
    alaMldServiceSapForwardSdpId                   SdpId,
    alaMldServiceSapForwardVcId                    TmnxVcIdOrNone,
    alaMldServiceSapForwardGroupAddress            MacAddress,
    alaMldServiceSapForwardHostAddress             MacAddress,
    alaMldServiceSapForwardDestAddress             MacAddress,
    alaMldServiceSapForwardOrigAddress             MacAddress,
    alaMldServiceSapForwardType                    INTEGER,
    alaMldServiceSapForwardNextSapPortId           TmnxPortID,
    alaMldServiceSapForwardNextSapEncapValue       TmnxEncapVal,
    alaMldServiceSapForwardNextType                    INTEGER

  
}

alaMldServiceSapForwardLocale OBJECT-TYPE
    SYNTAX      AluLocation
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaMldServiceSapForwardLocale indicates
         where this multicast router was detected.

         A multicast router found on a local SAP has the value 'sap(1)'.
         A multicast router detected on an SDP has the value 'sdp(2)'."
    ::= { alaMldServiceSapForwardEntry 1 }

alaMldServiceSapForwardPortId OBJECT-TYPE
    SYNTAX      TmnxPortID
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaMldServiceSapForwardPortId indicates,
         together with the object alaMldServiceSapForwardEncapValue, the SAP
         on which this multicast router is detected.

         The value of this object is only meaningful when the value of
         tlsMldSnpgMRouterLocale is 'sap(1)'."
    ::= { alaMldServiceSapForwardEntry 2 }

alaMldServiceSapForwardEncapValue OBJECT-TYPE
    SYNTAX      TmnxEncapVal
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaMldServiceSapForwardEncapValue indicates,
         together with the objectalaMldServiceSapForwardPortId, the SAP
         on which this multicast router is detected.

         The value of this object is only meaningful when the value of
         alaMldServiceSapForwardLocale is 'sap(1)'."
    ::= { alaMldServiceSapForwardEntry 3 }

alaMldServiceSapForwardSdpId OBJECT-TYPE
    SYNTAX      SdpId
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaMldServiceSapForwardSdpId indicates,
         together with the object alaMldServiceSapForwardVcId, the SDP Bind
         on which this multicast router is detected.

         The value of this object is only meaningful when the value of
         alaMldServiceSapForwardLocale is 'sdp(2)'."
    ::= { alaMldServiceSapForwardEntry 4 }

alaMldServiceSapForwardVcId OBJECT-TYPE
    SYNTAX      TmnxVcIdOrNone
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaMldServiceSapForwardVcId indicates,
         together with the object alaMldServiceSapForwardSdpId, the SDP Bind
         on which this multicast router is detected.

         The value of this object is only meaningful when the value of
         alaMldServiceSapForwardLocale is 'sdp(2)'."
    ::= { alaMldServiceSapForwardEntry 5 }


alaMldServiceSapForwardGroupAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast forwarded flow's IPv6 group address."
    ::= { alaMldServiceSapForwardEntry 6 }

alaMldServiceSapForwardHostAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast forwarded flow's IPv6 host address."
    ::= { alaMldServiceSapForwardEntry 7 }

alaMldServiceSapForwardDestAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast forwarded flow's IPv6 tunnel destination address."
    ::= { alaMldServiceSapForwardEntry 8 }

alaMldServiceSapForwardOrigAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast forwarded flow's IPv6 tunnel source address."
    ::= { alaMldServiceSapForwardEntry 9 }

alaMldServiceSapForwardType OBJECT-TYPE
    SYNTAX          INTEGER { mcast(1), pim(2), ipip(3) }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The IP multicast forwarded flow's encapsulation type."
    ::= { alaMldServiceSapForwardEntry 10 }


alaMldServiceSapForwardNextSapPortId OBJECT-TYPE
    SYNTAX          TmnxPortID
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION     "The IP multicast forwarded flow's next SAP. The ID of the access port where this SAP
                     is defined."
    ::= { alaMldServiceSapForwardEntry 11 }

alaMldServiceSapForwardNextSapEncapValue OBJECT-TYPE
    SYNTAX          TmnxEncapVal
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION     "The IP multicast forwarded flow's next SAP. The value of the label used to identify this
                     SAP on the access port specified by sapPortId."
    ::= { alaMldServiceSapForwardEntry 12 }

alaMldServiceSapForwardNextType OBJECT-TYPE
    SYNTAX          INTEGER { mcast(1), pim(2), ipip(3) }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The IP multicast forwarded flow's next encapsulation type."
    ::= { alaMldServiceSapForwardEntry 13 }

alaMldServiceSdpBindForwardTable OBJECT-TYPE
    SYNTAX          SEQUENCE OF MldServiceSdpBindForwardEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The table listing the IP multicast forward information."
    ::= { alaServiceMgrMld 16 }

alaMldServiceSdpBindForwardEntry OBJECT-TYPE
    SYNTAX          MldServiceSdpBindForwardEntry
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "An entry corresponding to an IP multicast forwarded flow."
    INDEX         { 
                    svcId,
                    alaMldServiceSdpBindForwardGroupAddress,
                    alaMldServiceSdpBindForwardHostAddress,
                    alaMldServiceSdpBindForwardDestAddress,
                    alaMldServiceSdpBindForwardOrigAddress,
                    alaMldServiceSdpBindForwardNextSdpBindId

                  }
    ::= { alaMldServiceSdpBindForwardTable 1 }

MldServiceSdpBindForwardEntry ::= SEQUENCE {

    alaMldServiceSdpBindForwardLocale		    AluLocation,
    alaMldServiceSdpBindForwardPortId                  TmnxPortID,
    alaMldServiceSdpBindForwardEncapValue              TmnxEncapVal,
    alaMldServiceSdpBindForwardSdpId                   SdpId,
    alaMldServiceSdpBindForwardVcId                    TmnxVcIdOrNone,
    alaMldServiceSdpBindForwardGroupAddress            MacAddress,
    alaMldServiceSdpBindForwardHostAddress             MacAddress,
    alaMldServiceSdpBindForwardDestAddress             MacAddress,
    alaMldServiceSdpBindForwardOrigAddress             MacAddress,
    alaMldServiceSdpBindForwardType                    INTEGER,
    alaMldServiceSdpBindForwardNextSdpBindId          SdpBindId,
    alaMldServiceSdpBindForwardNextType                    INTEGER

  
}

alaMldServiceSdpBindForwardLocale OBJECT-TYPE
    SYNTAX      AluLocation
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaMldServiceSdpBindForwardLocale indicates
         where this multicast router was detected.

         A multicast router found on a local SAP has the value 'sap(1)'.
         A multicast router detected on an SDP has the value 'sdp(2)'."
    ::= { alaMldServiceSdpBindForwardEntry 1 }

alaMldServiceSdpBindForwardPortId OBJECT-TYPE
    SYNTAX      TmnxPortID
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaMldServiceSdpBindForwardPortId indicates,
         together with the object alaMldServiceSdpBindForwardEncapValue, the SdpBind
         on which this multicast router is detected.

         The value of this object is only meaningful when the value of
         tlsMldSnpgMRouterLocale is 'sap(1)'."
    ::= { alaMldServiceSdpBindForwardEntry 2 }

alaMldServiceSdpBindForwardEncapValue OBJECT-TYPE
    SYNTAX      TmnxEncapVal
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaMldServiceSdpBindForwardEncapValue indicates,
         together with the object alaMldServiceSdpBindForwardPortId, the SAP
         on which this multicast router is detected.

         The value of this object is only meaningful when the value of
         alaMldServiceSdpBindForwardLocale is 'sap(1)'."
    ::= { alaMldServiceSdpBindForwardEntry 3 }

alaMldServiceSdpBindForwardSdpId OBJECT-TYPE
    SYNTAX      SdpId
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaMldServiceSdpBindForwardSdpId indicates,
         together with the object alaMldServiceSdpBindForwardVcId, the SDP Bind
         on which this multicast router is detected.

         The value of this object is only meaningful when the value of
         alaMldServiceSdpBindForwardLocale is 'sdp(2)'."
    ::= { alaMldServiceSdpBindForwardEntry 4 }

alaMldServiceSdpBindForwardVcId OBJECT-TYPE
    SYNTAX      TmnxVcIdOrNone
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of the object alaMldServiceSdpBindForwardVcId indicates,
         together with the object alaMldServiceSdpBindForwardSdpId, the SDP Bind
         on which this multicast router is detected.

         The value of this object is only meaningful when the value of
         alaMldServiceSdpBindForwardLocale is 'sdp(2)'."
    ::= { alaMldServiceSdpBindForwardEntry 5 }


alaMldServiceSdpBindForwardGroupAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast forwarded flow's IPv6 group address."
    ::= { alaMldServiceSdpBindForwardEntry 6 }

alaMldServiceSdpBindForwardHostAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast forwarded flow's IPv6 host address."
    ::= { alaMldServiceSdpBindForwardEntry 7 }

alaMldServiceSdpBindForwardDestAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast forwarded flow's IPv6 tunnel destination address."
    ::= { alaMldServiceSdpBindForwardEntry 8 }

alaMldServiceSdpBindForwardOrigAddress OBJECT-TYPE
    SYNTAX          MacAddress
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
        "The IP multicast forwarded flow's IPv6 tunnel source address."
    ::= { alaMldServiceSdpBindForwardEntry 9 }

alaMldServiceSdpBindForwardType OBJECT-TYPE
    SYNTAX          INTEGER { mcast(1), pim(2), ipip(3) }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The IP multicast forwarded flow's encapsulation type."
    ::= { alaMldServiceSdpBindForwardEntry 10 }



alaMldServiceSdpBindForwardNextSdpBindId OBJECT-TYPE
    SYNTAX          SdpBindId
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION     "The IP multicast forwarded flow's next sdpBind."
    ::= { alaMldServiceSdpBindForwardEntry 11 }



alaMldServiceSdpBindForwardNextType OBJECT-TYPE
    SYNTAX          INTEGER { mcast(1), pim(2), ipip(3) }
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The IP multicast forwarded flow's next encapsulation type."
    ::= { alaMldServiceSdpBindForwardEntry 12 }


--
--  SAP/SDPBIND Table for IP Multicast objects managed per  SAP/SDPBIND 
--
		
alaMldServiceSapTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF AlaMldServiceSapEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION 
       "The table listing the IP multicast port information."   
     ::= { alaServiceMgrMld 17 }
   
alaMldServiceSapEntry OBJECT-TYPE
     SYNTAX     AlaMldServiceSapEntry
     MAX-ACCESS not-accessible
     STATUS     current
     DESCRIPTION 
       "An entry corresponding to IP multicast Service SAP information."
     INDEX        { 
		    svcId,
                    sapPortId,
                    sapEncapValue
                  }
    ::= { alaMldServiceSapTable 1 }
   
AlaMldServiceSapEntry ::=
     SEQUENCE {
       alaMldServiceSapMaxGroupLimit   		Unsigned32,
       alaMldServiceSapMaxGroupExceedAction    	INTEGER,
       alaMldServiceSapCurrentGroupCount     		Unsigned32
     }
 

alaMldServiceSapMaxGroupLimit OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The maximum number of MLD Group memberships that can be learnt 
	on the sap."
    DEFVAL 		{0}
    ::= { alaMldServiceSapEntry 1 }

alaMldServiceSapMaxGroupExceedAction OBJECT-TYPE
    SYNTAX          INTEGER { none(0), drop(1), replace(2) }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The action to be taken when MLD group membership limit is 
	exceeded for the sap."
    DEFVAL        { none }
    ::= { alaMldServiceSapEntry 2 }


alaMldServiceSapCurrentGroupCount OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The current IP multicast group memberships on a sap. 
	instance."
    ::= { alaMldServiceSapEntry 3 }

alaMldServiceSdpBindTable OBJECT-TYPE
     SYNTAX      SEQUENCE OF AlaMldServiceSdpBindEntry
     MAX-ACCESS  not-accessible
     STATUS      current
     DESCRIPTION 
       "The table listing the IP multicast port information."   
     ::= { alaServiceMgrMld 18 }
   
alaMldServiceSdpBindEntry OBJECT-TYPE
     SYNTAX     AlaMldServiceSdpBindEntry
     MAX-ACCESS not-accessible
     STATUS     current
     DESCRIPTION 
       "An entry corresponding to IP multicast Service SdpBind information."
     INDEX        { 
		    svcId,
                    sdpBindId
                  }
    ::= { alaMldServiceSdpBindTable 1 }
   
AlaMldServiceSdpBindEntry ::=
     SEQUENCE {
       alaMldServiceSdpBindMaxGroupLimit   		Unsigned32,
       alaMldServiceSdpBindMaxGroupExceedAction    	INTEGER,
       alaMldServiceSdpBindCurrentGroupCount     		Unsigned32
     }
 

alaMldServiceSdpBindMaxGroupLimit OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The maximum number of MLD Group memberships that can be learnt 
	on the SdpBind."
    DEFVAL 		{0}
    ::= { alaMldServiceSdpBindEntry 1 }

alaMldServiceSdpBindMaxGroupExceedAction OBJECT-TYPE
    SYNTAX          INTEGER { none(0), drop(1), replace(2) }
    MAX-ACCESS      read-write
    STATUS          current
    DESCRIPTION
        "The action to be taken when MLD group membership limit is 
	exceeded for the SdpBind."
    DEFVAL        { none }
    ::= { alaMldServiceSdpBindEntry 2 }

alaMldServiceSdpBindCurrentGroupCount OBJECT-TYPE
    SYNTAX          Unsigned32
    MAX-ACCESS      read-only
    STATUS          current
    DESCRIPTION
        "The current IP multicast group memberships on a SdpBind. 
	instance."
    ::= { alaMldServiceSdpBindEntry 3 }

-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx
-- AOS LDP related MIB
-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

alaExtraLdp OBJECT IDENTIFIER ::= { alcatelIND1ServiceMgrMIBObjects 4 }



 alaVRtrExtendedLdpGeneralTable    OBJECT-TYPE
    SYNTAX      SEQUENCE OF AlaVRtrExtendedLdpGeneralEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        " alaVRtrExtendedLdpGeneralTable  is an extension to vRtrLdpGeneralTable 	   
	and it has an entry for each virtual router 
         in the system capable of supporting an instance of the
         Label Distribution Protocol (LDP)."
    ::= { alaExtraLdp 1 }

alaVRtrExtendedLdpGeneralEntry   OBJECT-TYPE
    SYNTAX      AlaVRtrExtendedLdpGeneralEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each row entry represents an instance of the Label Distribution
         Protocol (LDP) for a virtual router in the system.

         An entry in this table is created by the agent when vRtrLdpStatus
         in the vRtrConfTable is set to 'create'.
         The entry is destroyed when vRtrLdpStatus is set to 'delete' but
         only if vRtrLdpGenAdminState has a value of 'outOfService'."
    INDEX { vRtrID }
::= { alaVRtrExtendedLdpGeneralTable  1 }

AlaVRtrExtendedLdpGeneralEntry ::= SEQUENCE {
    alaVRtrLdpGenGracefulRestartSupport   TruthValue,
    alaVRtrLdpGenGRReconnectTime           Unsigned32,
    alaVRtrLdpGenGRFwdStateHoldTime        Unsigned32
}

  alaVRtrLdpGenGracefulRestartSupport  OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
        "The value of alaVRtrLdpGenGracefulRestartSupport specifies whether
	 restarting the LSR gracefully during a control plane restart is 	     	   
	 allowed. When this object has a value of 'true',
         graceful restart procedures are  enabled.  When its value is 'false', 	   
	 graceful restart procedures are disabled."
    DEFVAL { false }
    ::= { alaVRtrExtendedLdpGeneralEntry 1 }

alaVRtrLdpGenGRReconnectTime  OBJECT-TYPE
    SYNTAX       Unsigned32 (5..300)
    UNITS        "seconds"
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
	"The value of alaVRtrLdpGenGRReconnectTime  
	specifies the value of FT Reconnect timer. 
	The FT Reconnect timeout is the time that the sender of the TLV would like the receiver 
	of that TLV to wait after the receiver detects the failure of LDP communication with the sender. 
	This object has meaning only when alaVRtrLdpGenGracefulRestartSupport is ‘true’." 
    DEFVAL { 120 }
    ::= { alaVRtrExtendedLdpGeneralEntry 2 }

alaVRtrLdpGenGRFwdStateHoldTime   OBJECT-TYPE
    SYNTAX       Unsigned32 (15..1800)
    UNITS        "seconds"
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
	  "The value of vRtrLdpGenGRFwdStateHoldTime specifies the MPLS 	   	      	  
	  ‘forwarding state hold’timer. If the forwarding state has been 	   	   
	  preserved during a control plane restart, then the LSR starts this 		   
	  timer and marks all forwarding entries as stale. At the expiration of 	   
	  the timer all the entries that are still marked as stale are deleted.     	   
	  The value of Recovery Time advertised to the neighbors in the FT 	   	   
	  session TLV is set to the current value of the timer at the point in 	   
	  which the Initialization message carrying the FT session TLV is sent"
    DEFVAL { 120 }
    ::= { alaVRtrExtendedLdpGeneralEntry 3}


  alaVRtrLdpExtendedSessionTable    OBJECT-TYPE
    SYNTAX      SEQUENCE OF AlaVRtrLdpExtendedSessionEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "alaVRtrLdpExtendedSessionTable is an extension to vRtrLdpSessionTable.
	 This isa read-only table which parallels the
          mplsLdpSessionTable in the MPLS-LDP-MIB. The purpose of this
          table is to keep information about a single session between
          an LDP entity and an LDP Peer"
    ::= { alaExtraLdp 2 }

alaVRtrLdpExtendedSessionEntry OBJECT-TYPE
    SYNTAX      AlaVRtrLdpExtendedSessionEntry 
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "A row in this table represents information about a single
         session between an LDP entity and an LDP Peer."
    INDEX  { vRtrID,
             alaVRtrLdpPeerLdpId }
    ::= { alaVRtrLdpExtendedSessionTable    1 }

AlaVRtrLdpExtendedSessionEntry ::= SEQUENCE {
    alaVRtrLdpPeerLdpId                    MplsLdpIdentifier,
    alaVRtrLdpSessRestartInProgress		TruthValue,
    alaVRtrLdpSessFtReconTimeAdvertised         Unsigned32,
    alaVRtrLdpSessFtRecoveryTimeAdvertised      Unsigned32
}


alaVRtrLdpPeerLdpId    OBJECT-TYPE
    SYNTAX      MplsLdpIdentifier
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The value of alaVRtrLdpSessLocalLdpId specifies the local LDP
         identifier for this LDP session." 
    ::= { alaVRtrLdpExtendedSessionEntry 1 }

alaVRtrLdpSessRestartInProgress OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The value of alaVRtrLdpSessRestartInProgress  indicates whether 
	   graceful restart is in progress for this session"
    ::= { alaVRtrLdpExtendedSessionEntry 2 }

alaVRtrLdpSessFtReconTimeAdvertised OBJECT-TYPE
	SYNTAX      Unsigned32
	UNITS        "seconds"
	MAX-ACCESS  read-only
	STATUS      current
	DESCRIPTION
	"The value of alaVRtrLdpSessFtReconTimeAdvertised  indicates the session's
	Fault Tolerant(FT) Reconnect Timeout advertised to the peer"
	::= { alaVRtrLdpExtendedSessionEntry 3 }

alaVRtrLdpSessFtRecoveryTimeAdvertised       OBJECT-TYPE
	SYNTAX      Unsigned32
	UNITS        "seconds"
	MAX-ACCESS  read-only
	STATUS      current
	DESCRIPTION
	"The value of alaVRtrLdpSessFtRecoveryTimeAdvertised  indicates the session's
	Fault Tolerant(FT) recovery timeout that was advertised to the peer."
	::= { alaVRtrLdpExtendedSessionEntry 4 }



-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx
-- COMPLIANCE
-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx

alcatelIND1ServiceMgrMIBCompliance MODULE-COMPLIANCE
        STATUS  current
        DESCRIPTION
        "Compliance statement for service manager."
        MODULE  MANDATORY-GROUPS
                {
                alaServiceMgrPortProfileGroup ,
		alaServiceMgrPortGroup,
		alaSapExtraInfoGroup,
		alaIgmpServiceGroup,
		alaIgmpMemberServiceSapGroup,
		alaIgmpMemberServiceSdpBindGroup,
		alaIgmpStaticMemberServiceSapGroup,
		alaIgmpStaticMemberServiceSdpBindGroup,
		alaIgmpNeighborServiceSapGroup,
		alaIgmpNeighborServiceSdpBindGroup,
		alaIgmpStaticNeighborServiceSapGroup,
		alaIgmpStaticNeighborServiceSdpBindGroup,
		alaIgmpQuerierServiceSapGroup,
		alaIgmpQuerierServiceSdpBindGroup,
		alaIgmpStaticQuerierServiceSapGroup,
		alaIgmpStaticQuerierServiceSdpBindGroup,
		alaIgmpServiceSourceGroup,
		alaIgmpServiceSapForwardGroup,
		alaIgmpServiceSdpBindForwardGroup,
		alaIgmpServiceSapGroup,
		alaIgmpServiceSdpBindGroup,
		alaMldServiceGroup,
		alaMldMemberServiceSapGroup,
		alaMldMemberServiceSdpBindGroup,
		alaMldStaticMemberServiceSapGroup,
		alaMldStaticMemberServiceSdpBindGroup,
		alaMldNeighborServiceSapGroup,
		alaMldNeighborServiceSdpBindGroup,
		alaMldStaticNeighborServiceSapGroup,
		alaMldStaticNeighborServiceSdpBindGroup,
		alaMldQuerierServiceSapGroup,
		alaMldQuerierServiceSdpBindGroup,
		alaMldStaticQuerierServiceSapGroup,
		alaMldStaticQuerierServiceSdpBindGroup,
		alaMldServiceSourceGroup,
		alaMldServiceSapForwardGroup,
		alaMldServiceSdpBindForwardGroup,
		alaMldServiceSapGroup,
		alaMldServiceSdpBindGroup
                }
        ::= { alcatelIND1ServiceMgrMIBCompliances 1 }


-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx
-- UNITS OF CONFORMANCE
-- xxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxxx



alaServiceMgrPortProfileGroup OBJECT-GROUP
        OBJECTS
        { 
		alaServiceMgrPortProfileStpBpduTreatment,
		alaServiceMgrPortProfile8021xTreatment,
		alaServiceMgrPortProfile8021ABTreatment,
		alaServiceMgrPortProfile8023adTreatment,
		alaServiceMgrPortProfileGvrpTreatment,
		alaServiceMgrPortProfileAmapTreatment,
		alaServiceMgrPortProfileRowStatus,
		alaServiceMgrPortProfileMvrpTreatment
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of Service Manager Port Profiles."
        ::= { alcatelIND1ServiceMgrMIBGroups 1 }

alaServiceMgrPortGroup OBJECT-GROUP
        OBJECTS
        { 
		alaServiceMgrPortMode,
		alaServiceMgrPortEncapType,
		alaServiceMgrPortPortProfileID,
		alaServiceMgrPortRowStatus		
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of Service Manager Port."
	::= { alcatelIND1ServiceMgrMIBGroups 2 }

alaSapExtraInfoGroup OBJECT-GROUP
        OBJECTS
        { 
		alaSapInfoTrusted,
		alaSapInfoPriority	
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of Sap extra info."
	::= { alcatelIND1ServiceMgrMIBGroups 3 }

alaIgmpServiceGroup OBJECT-GROUP
        OBJECTS
        { 
		alaIgmpServiceStatus,
		alaIgmpServiceQuerying,
		alaIgmpServiceSpoofing,
		alaIgmpServiceZapping,
		alaIgmpServiceVersion,
		alaIgmpServiceRobustness,
		alaIgmpServiceQueryInterval,
		alaIgmpServiceQueryResponseInterval,
		alaIgmpServiceLastMemberQueryInterval,
		alaIgmpServiceRouterTimeout,
		alaIgmpServiceSourceTimeout,
		alaIgmpServiceProxying,
		alaIgmpServiceUnsolicitedReportInterval,
		alaIgmpServiceQuerierForwarding,
		alaIgmpServiceMaxGroupLimit,
		alaIgmpServiceMaxGroupExceedAction
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of service igmp object."
	::= { alcatelIND1ServiceMgrMIBGroups 4 }

alaIgmpMemberServiceSapGroup OBJECT-GROUP
        OBJECTS
        { 
		alaIgmpMemberServiceSapMode,
		alaIgmpMemberServiceSapCount,
		alaIgmpMemberServiceSapTimeout
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of service igmp member sap object."
	::= { alcatelIND1ServiceMgrMIBGroups 5 }

alaIgmpMemberServiceSdpBindGroup OBJECT-GROUP
        OBJECTS
        { 
		alaIgmpMemberServiceSdpBindMode,
		alaIgmpMemberServiceSdpBindCount,
		alaIgmpMemberServiceSdpBindTimeout	
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of service igmp member sdp binding object."
	::= { alcatelIND1ServiceMgrMIBGroups 6 }

alaIgmpStaticMemberServiceSapGroup OBJECT-GROUP
        OBJECTS
        { 
		alaIgmpStaticMemberServiceSapRowStatus	
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of service igmp static member sap object."
	::= { alcatelIND1ServiceMgrMIBGroups 7 }

alaIgmpStaticMemberServiceSdpBindGroup OBJECT-GROUP
        OBJECTS
        { 
		alaIgmpStaticMemberServiceSdpBindRowStatus	
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of service igmp static member sdp binding object."
	::= { alcatelIND1ServiceMgrMIBGroups 8 }

alaIgmpNeighborServiceSapGroup OBJECT-GROUP
        OBJECTS
        { 
		alaIgmpNeighborServiceSapCount,
		alaIgmpNeighborServiceSapTimeout	
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of service igmp sap neighbor object."
	::= { alcatelIND1ServiceMgrMIBGroups 9 }

alaIgmpNeighborServiceSdpBindGroup OBJECT-GROUP
        OBJECTS
        { 
		alaIgmpNeighborServiceSdpBindCount,
		alaIgmpNeighborServiceSdpBindTimeout	
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of service igmp SdpBind neighbor object."
	::= { alcatelIND1ServiceMgrMIBGroups 10 }

alaIgmpStaticNeighborServiceSapGroup OBJECT-GROUP
        OBJECTS
        { 
		alaIgmpStaticNeighborServiceSapRowStatus	
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of service igmp sap static neighbor object."
	::= { alcatelIND1ServiceMgrMIBGroups 11 }

alaIgmpStaticNeighborServiceSdpBindGroup OBJECT-GROUP
        OBJECTS
        { 
		alaIgmpStaticNeighborServiceSdpBindRowStatus	
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of service igmp SdpBind static neighbor object."
	::= { alcatelIND1ServiceMgrMIBGroups 12 }

alaIgmpQuerierServiceSapGroup OBJECT-GROUP
        OBJECTS
        { 
		alaIgmpQuerierServiceSapCount,
		alaIgmpQuerierServiceSapTimeout	
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of service sap igmp querier object."
	::= { alcatelIND1ServiceMgrMIBGroups 13 }

alaIgmpQuerierServiceSdpBindGroup OBJECT-GROUP
        OBJECTS
        { 
		alaIgmpQuerierServiceSdpBindCount,
		alaIgmpQuerierServiceSdpBindTimeout	
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of service SdpBind igmp querier object."
	::= { alcatelIND1ServiceMgrMIBGroups 14 }

alaIgmpStaticQuerierServiceSapGroup OBJECT-GROUP
        OBJECTS
        { 
		alaIgmpStaticQuerierServiceSapRowStatus
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of service sap igmp static querier object."
	::= { alcatelIND1ServiceMgrMIBGroups 15 }

alaIgmpStaticQuerierServiceSdpBindGroup OBJECT-GROUP
        OBJECTS
        { 
		alaIgmpStaticQuerierServiceSdpBindRowStatus
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of service SdpBind igmp static querier object."
	::= { alcatelIND1ServiceMgrMIBGroups 16 }

alaIgmpServiceSourceGroup OBJECT-GROUP
        OBJECTS
        { 
		alaIgmpServiceSourceLocale,
		alaIgmpServiceSourcePortId,
		alaIgmpServiceSourceEncapValue,
		alaIgmpServiceSourceSdpId,
		alaIgmpServiceSourceVcId,
		alaIgmpServiceSourceType
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of igmp service source object."
	::= { alcatelIND1ServiceMgrMIBGroups 17 }

alaIgmpServiceSapForwardGroup OBJECT-GROUP
        OBJECTS
        { 
		alaIgmpServiceSapForwardLocale,
		alaIgmpServiceSapForwardPortId,
		alaIgmpServiceSapForwardEncapValue,
		alaIgmpServiceSapForwardSdpId,
		alaIgmpServiceSapForwardVcId,
		alaIgmpServiceSapForwardType,
		alaIgmpServiceSapForwardNextType
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of igmp service sap forward object."
	::= { alcatelIND1ServiceMgrMIBGroups 18 }

alaIgmpServiceSdpBindForwardGroup OBJECT-GROUP
        OBJECTS
        { 
		alaIgmpServiceSdpBindForwardLocale,
		alaIgmpServiceSdpBindForwardPortId,
		alaIgmpServiceSdpBindForwardEncapValue,
		alaIgmpServiceSdpBindForwardSdpId,
		alaIgmpServiceSdpBindForwardVcId,
		alaIgmpServiceSdpBindForwardType,
		alaIgmpServiceSdpBindForwardNextType
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of igmp service SdpBind forward object."
	::= { alcatelIND1ServiceMgrMIBGroups 19 }


alaIgmpServiceSapGroup OBJECT-GROUP
        OBJECTS
        { 
		alaIgmpServiceSapMaxGroupLimit,
		alaIgmpServiceSapMaxGroupExceedAction,
		alaIgmpServiceSapCurrentGroupCount
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of igmp service sap object."
	::= { alcatelIND1ServiceMgrMIBGroups 20 }

alaIgmpServiceSdpBindGroup OBJECT-GROUP
        OBJECTS
        { 
		alaIgmpServiceSdpBindMaxGroupLimit,
		alaIgmpServiceSdpBindMaxGroupExceedAction,
		alaIgmpServiceSdpBindCurrentGroupCount
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of igmp service SdpBind object."
	::= { alcatelIND1ServiceMgrMIBGroups 21 }
alaMldServiceGroup OBJECT-GROUP
        OBJECTS
        { 
		alaMldServiceStatus,
		alaMldServiceQuerying,
		alaMldServiceSpoofing,
		alaMldServiceZapping,
		alaMldServiceVersion,
		alaMldServiceRobustness,
		alaMldServiceQueryInterval,
		alaMldServiceQueryResponseInterval,
		alaMldServiceLastMemberQueryInterval,
		alaMldServiceRouterTimeout,
		alaMldServiceSourceTimeout,
		alaMldServiceProxying,
		alaMldServiceUnsolicitedReportInterval,
		alaMldServiceQuerierForwarding,
		alaMldServiceMaxGroupLimit,
		alaMldServiceMaxGroupExceedAction
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of service MLD object."
	::= { alcatelIND1ServiceMgrMIBGroups 22 }

alaMldMemberServiceSapGroup OBJECT-GROUP
        OBJECTS
        { 
		alaMldMemberServiceSapMode,
		alaMldMemberServiceSapCount,
		alaMldMemberServiceSapTimeout
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of service MLD member sap object."
	::= { alcatelIND1ServiceMgrMIBGroups 23 }

alaMldMemberServiceSdpBindGroup OBJECT-GROUP
        OBJECTS
        { 
		alaMldMemberServiceSdpBindMode,
		alaMldMemberServiceSdpBindCount,
		alaMldMemberServiceSdpBindTimeout	
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of service MLD member sdp binding object."
	::= { alcatelIND1ServiceMgrMIBGroups 24 }

alaMldStaticMemberServiceSapGroup OBJECT-GROUP
        OBJECTS
        { 
		alaMldStaticMemberServiceSapRowStatus	
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of service MLD static member sap object."
	::= { alcatelIND1ServiceMgrMIBGroups 25 }

alaMldStaticMemberServiceSdpBindGroup OBJECT-GROUP
        OBJECTS
        { 
		alaMldStaticMemberServiceSdpBindRowStatus	
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of service MLD static member sdp binding object."
	::= { alcatelIND1ServiceMgrMIBGroups 26 }

alaMldNeighborServiceSapGroup OBJECT-GROUP
        OBJECTS
        { 
		alaMldNeighborServiceSapCount,
		alaMldNeighborServiceSapTimeout	
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of service MLD sap neighbor object."
	::= { alcatelIND1ServiceMgrMIBGroups 27 }

alaMldNeighborServiceSdpBindGroup OBJECT-GROUP
        OBJECTS
        { 
		alaMldNeighborServiceSdpBindCount,
		alaMldNeighborServiceSdpBindTimeout	
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of service MLD SdpBind neighbor object."
	::= { alcatelIND1ServiceMgrMIBGroups 28 }

alaMldStaticNeighborServiceSapGroup OBJECT-GROUP
        OBJECTS
        { 
		alaMldStaticNeighborServiceSapRowStatus	
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of service MLD sap static neighbor object."
	::= { alcatelIND1ServiceMgrMIBGroups 29 }

alaMldStaticNeighborServiceSdpBindGroup OBJECT-GROUP
        OBJECTS
        { 
		alaMldStaticNeighborServiceSdpBindRowStatus	
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of service MLD SdpBind static neighbor object."
	::= { alcatelIND1ServiceMgrMIBGroups 30 }

alaMldQuerierServiceSapGroup OBJECT-GROUP
        OBJECTS
        { 
		alaMldQuerierServiceSapCount,
		alaMldQuerierServiceSapTimeout	
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of service sap MLD querier object."
	::= { alcatelIND1ServiceMgrMIBGroups 31 }

alaMldQuerierServiceSdpBindGroup OBJECT-GROUP
        OBJECTS
        { 
		alaMldQuerierServiceSdpBindCount,
		alaMldQuerierServiceSdpBindTimeout	
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of service SdpBind MLD querier object."
	::= { alcatelIND1ServiceMgrMIBGroups 32 }

alaMldStaticQuerierServiceSapGroup OBJECT-GROUP
        OBJECTS
        { 
		alaMldStaticQuerierServiceSapRowStatus
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of service sap MLD static querier object."
	::= { alcatelIND1ServiceMgrMIBGroups 33 }

alaMldStaticQuerierServiceSdpBindGroup OBJECT-GROUP
        OBJECTS
        { 
		alaMldStaticQuerierServiceSdpBindRowStatus
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of service SdpBind MLD static querier object."
	::= { alcatelIND1ServiceMgrMIBGroups 34 }

alaMldServiceSourceGroup OBJECT-GROUP
        OBJECTS
        { 
		alaMldServiceSourceLocale,
		alaMldServiceSourcePortId,
		alaMldServiceSourceEncapValue,
		alaMldServiceSourceSdpId,
		alaMldServiceSourceVcId,
		alaMldServiceSourceType
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of MLD service source object."
	::= { alcatelIND1ServiceMgrMIBGroups 35 }

alaMldServiceSapForwardGroup OBJECT-GROUP
        OBJECTS
        { 
		alaMldServiceSapForwardLocale,
		alaMldServiceSapForwardPortId,
		alaMldServiceSapForwardEncapValue,
		alaMldServiceSapForwardSdpId,
		alaMldServiceSapForwardVcId,
		alaMldServiceSapForwardType,
		alaMldServiceSapForwardNextType
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of MLD service sap forward object."
	::= { alcatelIND1ServiceMgrMIBGroups 36 }

alaMldServiceSdpBindForwardGroup OBJECT-GROUP
        OBJECTS
        { 
		alaMldServiceSdpBindForwardLocale,
		alaMldServiceSdpBindForwardPortId,
		alaMldServiceSdpBindForwardEncapValue,
		alaMldServiceSdpBindForwardSdpId,
		alaMldServiceSdpBindForwardVcId,
		alaMldServiceSdpBindForwardType,
		alaMldServiceSdpBindForwardNextType
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of MLD service SdpBind forward object."
	::= { alcatelIND1ServiceMgrMIBGroups 37 }


alaMldServiceSapGroup OBJECT-GROUP
        OBJECTS
        { 
		alaMldServiceSapMaxGroupLimit,
		alaMldServiceSapMaxGroupExceedAction,
		alaMldServiceSapCurrentGroupCount
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of MLD service sap object."
	::= { alcatelIND1ServiceMgrMIBGroups 38 }

alaMldServiceSdpBindGroup OBJECT-GROUP
        OBJECTS
        { 
		alaMldServiceSdpBindMaxGroupLimit,
		alaMldServiceSdpBindMaxGroupExceedAction,
		alaMldServiceSdpBindCurrentGroupCount
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of MLD service SdpBind object."
	::= { alcatelIND1ServiceMgrMIBGroups 39 }

alaVRtrExtendedLdpGeneralGroup OBJECT-GROUP
        OBJECTS
        { 
		alaVRtrLdpGenGracefulRestartSupport,
		alaVRtrLdpGenGRReconnectTime,
		alaVRtrLdpGenGRFwdStateHoldTime
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of MLD service SdpBind object."
	::= { alcatelIND1ServiceMgrMIBGroups 40 }

alaVRtrLdpExtendedSessionGroup OBJECT-GROUP
        OBJECTS
        { 
		alaVRtrLdpSessRestartInProgress,
		alaVRtrLdpSessFtReconTimeAdvertised,
		alaVRtrLdpSessFtRecoveryTimeAdvertised
        }
        STATUS current
        DESCRIPTION
        "Collection of objects for management of MLD service SdpBind object."
	::= { alcatelIND1ServiceMgrMIBGroups 41 }

END

