
-- *****************************************************************************
-- Juniper-IP-POLICY-MIB
--
-- Juniper Networks Enterprise MIB
--   Extensions for IP Policy management
--
-- Copyright (c) 1998 Redstone Communications, Inc.
-- Copyright (c) 2000, 2002 Unisphere Networks, Inc.
-- Copyright (c) 2003 Juniper Networks, Inc.
-- Copyright (c) 2006 Juniper Networks, Inc.
--   All Rights Reserved.
-- *****************************************************************************


Juniper-IP-POLICY-MIB  DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, IpAddress, Counter32, Integer32
        FROM SNMPv2-SMI
    TEXTUAL-CONVENTION, RowStatus, DisplayString, TruthValue
        FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF
    juniMibs
        FROM Juniper-MIBs;

juniIpPolicyMIB  MODULE-IDENTITY
    LAST-UPDATED "200701250824Z"  -- 25-Jan-07 03:24 AM EST
    ORGANIZATION "Juniper Networks, Inc."
    CONTACT-INFO
        "       Juniper Networks, Inc.
        Postal: 10 Technology Park Drive
                Westford, MA  01886-3146
                USA
        Tel:    +1 978 589 5800
        Email:  mib@Juniper.net"
    DESCRIPTION
        "The IP Policy MIB for the Juniper Networks enterprise."
    -- Revision History
    REVISION    "200701250834Z"  -- 25-Jan-07 03:34 AM EST  - JUNOSe 7.0
    DESCRIPTION
        "Changed the length of octet string for juniIpAspAccessExpression to
         vary from 1 to 256."
    REVISION    "200607250413Z"  -- 24-Jul-06 11:13 PM EST  - JUNOSe 6.0
    DESCRIPTION
        "Changed the length of octet string for juniIpCommunityListExpression to
         vary from 1 to 256." 
    REVISION    "200601101421Z"  -- 10-Jan-06 09:21 AM EST  - JUNOSe 7.1
    DESCRIPTION
        "Added two more protocols to JuniIpRedistributeProtocol."
    REVISION    "200402051421Z"  -- 05-Feb-04 09:21 AM EST  - JUNOSe 5.3
    DESCRIPTION
        "Added Policy-List under juniIpRouteMapClauseElemId."
    REVISION    "200302051421Z"  -- 05-Feb-03 09:21 AM EST  - JUNOSe 5.1
    DESCRIPTION
        "Added IP route maps config support."
    REVISION    "200302042230Z"  -- 04-Feb-03 05:30 PM EST  - JUNOSe 5.0
    DESCRIPTION
        "Replaced Unisphere names with Juniper names.
         Fixed the index for the juniIpDynRedistributeTable."
    REVISION    "200201031506Z"  -- 03-Jan-02 11:06 AM EDT  - JUNOSe 3.0
    DESCRIPTION
        "Expanded MIB to include following tables:
                     JuniIpAspAccessListTable
                     JuniIpPrefixListTable
                     JuniIpPrefixTreeTable
                     JuniIpCommunityListTable
                     JuniIpExtCommunityListTable
                     JuniIpRedistributeTable
                     JuniIpRouteMapTable
         Expanded MIB to include a new textual convention:
                     JuniIpPolicyExtendedCommunity"
    REVISION    "200007200000Z"  -- 20-Jul-00               - JUNOSe 2.0
    DESCRIPTION
        "Added Named Access List support."
    REVISION    "9811190000Z"    -- 19-Nov-98               - JUNOSe 1.0
    DESCRIPTION
        "Initial version of this MIB module."
    ::= { juniMibs 13 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Textual conventions
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
JuniIpPolicyName ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "32a"
    STATUS      current
    DESCRIPTION
        "IP access list name.  Represents textual information taken from the NVT
        ASCII character set."
    REFERENCE
        "RFC 854: NVT ASCII character set.  See SNMPv2-TC.DisplayString
        DESCRIPTION for a summary."
    SYNTAX      OCTET STRING (SIZE(0..32))

JuniIpPolicyPolicy ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The set of IP policy actions."
    SYNTAX      INTEGER {
                    permit(0),
                    deny(1) }

JuniIpDynRedistributeProtocol ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The set of protocols choices used to configure to/from settings in an
        IP Dynamic Route Redistribution element."
    SYNTAX      INTEGER {
                    ipRedistrProtocolIsis(1),
                    ipRedistrProtocolRip(2),
                    ipRedistrProtocolOspf(3),
                    ipRedistrProtocolStatic(4),
                    ipRedistrProtocolConnected(5),
                    ipRedistrProtocolBgp(6),
                    ipRedistrProtocolMBgp(7),
                    ipRedistrProtocolStaticLow(8),
                    ipRedistrProtocolOspfIntern(9),
                    ipRedistrProtocolOspfExtern(10),
                    ipRedistrProtocolDvmrp(11),
                    ipRedistrProtocolDvmrpAggregate(12),
                    ipRedistrProtocolHidden(13),
                    ipRedistrProtocolOwnerAccess(14),
                    ipRedistrProtocolOwnerAccessInternal(15),
                    ipRedistrProtocolOwnerDialout(16),
                    ipRedistrProtocolDefaultRoute(17) }

JuniIpRedistributeProtocol ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The set of protocols choices used to configure to/from settings in an
        IP Redistribution element."
    SYNTAX      INTEGER {
                    ipRedistrProtocolStatic(1),
                    ipRedistrProtocolBgp(2),
                    ipRedistrProtocolMBgp(3),
                    ipRedistrProtocolOspf(4),
                    ipRedistrProtocolIsis(5),
                    ipRedistrProtocolRip(6),
                    ipRedistrProtocolConnected(7),
                    ipRedistrProtocolDefaultRoute(8),
                    ipRedistrProtocolAccess(9),
                    ipRedistrProtocolAccessInternal(10),
                    ipRedistrProtocolDvmrp(11),
                    ipRedistrProtocolDialout(12),
  			  ipRedistrProtocolOspfM(13),
                    ipRedistrProtocolStaticMcast(14),
			  ipRedistrProtocolLdpUcast(15) }

JuniIpPolicyAdminStatus ::= TEXTUAL-CONVENTION
    STATUS      current
    DESCRIPTION
        "The administratively assigned management state for an IP route policy."
    SYNTAX      INTEGER {
                    ipPolicyAdminStateDisable(0),
                    ipPolicyAdminStateEnable(1) }

JuniIpPolicyExtendedCommunity ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "22a"
    STATUS      current
    DESCRIPTION
        "The extended community specification.  Represents textual information
        taken from the NVT ASCII character set.  The format of the text string
        is defined by either one of these choices:

         In:
             ASN::nn          where ASN is a 16 bit decimal number and
                              nn is a 32 bit decimal number

         Or:
             IP-address::nn   where IP-address is in dotted decimal format
                              and nn is a 16 bit decimal number
         "
    REFERENCE
        "RFC 854: NVT ASCII character set."
    SYNTAX      OCTET STRING (SIZE(0..22))


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Managed objects
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniIpPolicyObjects    OBJECT IDENTIFIER ::= { juniIpPolicyMIB 1 }

juniIpAccessList       OBJECT IDENTIFIER ::= { juniIpPolicyObjects 1 }
juniIpNamedAccessList  OBJECT IDENTIFIER ::= { juniIpPolicyObjects 2 }
juniIpAspAccessList    OBJECT IDENTIFIER ::= { juniIpPolicyObjects 3 }
juniIpPrefixList       OBJECT IDENTIFIER ::= { juniIpPolicyObjects 4 }
juniIpPrefixTree       OBJECT IDENTIFIER ::= { juniIpPolicyObjects 5 }
juniIpCommunityList    OBJECT IDENTIFIER ::= { juniIpPolicyObjects 6 }
juniIpRedistributeList OBJECT IDENTIFIER ::= { juniIpPolicyObjects 7 }
juniIpRouteMapTree     OBJECT IDENTIFIER ::= { juniIpPolicyObjects 8 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- IP Access Lists
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
--
-- The IP Access List Table
--
juniIpAccessListTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIpAccessListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for elements of IP access lists.  Entries
        belonging to the same access list are ordered, and comparisons to those
        entries are performed in that order until a match is detected.  If no
        match is found, the default action is to 'deny'."
    ::= { juniIpAccessList 1 }

juniIpAccessListEntry OBJECT-TYPE
    SYNTAX      JuniIpAccessListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of an IP access list element."
    INDEX     { juniIpAccessListId,
                juniIpAccessListElemId }
    ::= { juniIpAccessListTable 1 }

JuniIpAccessListEntry ::= SEQUENCE {
    juniIpAccessListId        Integer32,
    juniIpAccessListElemId    Integer32,
    juniIpAccessListRowStatus RowStatus,
    juniIpAccessListAction    JuniIpPolicyPolicy,
    juniIpAccessListSrc       IpAddress,
    juniIpAccessListSrcMask   IpAddress,
    juniIpAccessListDst       IpAddress,
    juniIpAccessListDstMask   IpAddress,
    juniIpAccessListProtocol  Integer32 }

juniIpAccessListId OBJECT-TYPE
    SYNTAX      Integer32 (1..10000)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The number of the access list to which this entry belongs."
    ::= { juniIpAccessListEntry 1 }

juniIpAccessListElemId OBJECT-TYPE
    SYNTAX      Integer32 (0..10000)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The relative position of this entry within its access list.  Access
        list entries are searched in this sequence (low to high values) until a
        match is found.

        NOTE:  The value zero is reserved for use with SET operations to perform
        special-purpose table entry creations/deletions; see the DESCRIPTION of
        juniIpAccessListRowStatus for details.

        Get/GetNext/GetBulk retrievals never return an entry for which this
        object is zero-valued."
    ::= { juniIpAccessListEntry 2 }

juniIpAccessListRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        Two configuration levels are defined, limited and full.  EARLY
        IMPLEMENTATIONS MIGHT PROVIDE ONLY THE LIMITED LEVEL OF CONFIGURATION
        CAPABILITY.

        *** LIMITED ACCESS LIST CONFIGURATION LEVEL ***

         1) RowStatus createAndGo/destroy operations directed to a target table
            entry for which juniIpAccessListElemId is ZERO, have the following
            special-purpose semantics:
                createAndGo     Create an entry having the specified
                                configuration and append it to the target list,
                                i.e. assign it a value of juniIpAccessListElemId
                                that is one greater than the current last
                                element in the list.
                destroy         Destroy the specified list and all of its
                                constituent elements.

         2) RowStatus createAndGo/destroy operations directed to a target table
            entry for which juniIpAccessListElemId is NONZERO are disallowed.

        *** FULL ACCESS LIST CONFIGURATION LEVEL ***

        Permit conventional RowStatus-based management of table entries having a
        nonzero value for juniIpAccessListElemId, IN ADDITION TO the special
        RowStatus semantics applied to entries having a zero value for
        juniIpAccessListElemId.

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
                juniIpAccessListRowStatus

        In addition, when creating an entry the following conditions must hold:

                The value of juniIpAccessListElemId is nonzero.

        Once created, element attributes cannot be modified except by a
        RowStatus destroy operation to delete the list element."
    ::= { juniIpAccessListEntry 3 }

juniIpAccessListAction OBJECT-TYPE
    SYNTAX      JuniIpPolicyPolicy
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the disposition of an item that matches the comparison
        criteria described by this entry."
    DEFVAL    { permit }
    ::= { juniIpAccessListEntry 4 }

juniIpAccessListSrc OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "A source IP address.  A subject IP address is first masked with the
        value of juniIpAccessListSrcMask, then the result is compared to this
        value.  Setting both this object and its corresponding mask to 0.0.0.0
        acts as a wildcard, matching any source IP address."
    DEFVAL    { '00000000'H }    -- 0.0.0.0
    ::= { juniIpAccessListEntry 5 }

juniIpAccessListSrcMask OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The IP address mask to be applied to a subject source IP address before
        comparing it to juniIpAccessListSrc.  Ones in the mask identify which
        bits in the subject IP address are significant for the comparison.

        To be considered valid, a nonzero value for this object must contain a
        single contiguous string of ones, beginning with the most significant
        bit of the mask."
    DEFVAL    { '00000000'H }    -- 0.0.0.0
    ::= { juniIpAccessListEntry 6 }

juniIpAccessListDst OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "A destination IP address.  A subject IP address is first masked with
        the value of juniIpAccessListDstMask, then the result is compared to
        this value.  Setting both this object and its corresponding mask to
        0.0.0.0 acts as a wildcard, matching any destination IP address."
    DEFVAL    { '00000000'H }    -- 0.0.0.0
    ::= { juniIpAccessListEntry 7 }

juniIpAccessListDstMask OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The IP address mask to be applied to a subject destination IP address
        before comparing it to juniIpAccessListDst.  Ones in the mask identify
        which bits in the IP address are significant for the comparison.

        To be considered valid, a nonzero value for this object must contain a
        single contiguous string of ones, beginning with the most significant
        bit of the mask."
    DEFVAL    { '00000000'H }    -- 0.0.0.0
    ::= { juniIpAccessListEntry 8 }

juniIpAccessListProtocol OBJECT-TYPE
    SYNTAX      Integer32 (0..255)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "An IP Protocol value.  Nonzero values match a specific IP Protocol
        value (e.g. 6 for TCP) carried in an IP packet; a value of zero acts as
        a wildcard, matching any IP Protocol."
    DEFVAL    { 0 }
    ::= { juniIpAccessListEntry 9 }


--
-- The IP Named Access List Table
--
juniIpNamedAccessListTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIpNamedAccessListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for elements of IP access lists.  Entries
        belonging to the same access list are ordered, and comparisons to those
        entries are performed in that order until a match is detected.  If no
        match is found, the default action is to 'deny'."
    ::= { juniIpNamedAccessList 1 }

juniIpNamedAccessListEntry OBJECT-TYPE
    SYNTAX      JuniIpNamedAccessListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of an IP access list element."
    INDEX     { juniIpNamedAccessListName,
                juniIpNamedAccessListElemId }
    ::= { juniIpNamedAccessListTable 1 }

JuniIpNamedAccessListEntry ::= SEQUENCE {
    juniIpNamedAccessListName         JuniIpPolicyName,
    juniIpNamedAccessListElemId       Integer32,
    juniIpNamedAccessListRowStatus    RowStatus,
    juniIpNamedAccessListAction       JuniIpPolicyPolicy,
    juniIpNamedAccessListSrc          IpAddress,
    juniIpNamedAccessListSrcMask      IpAddress,
    juniIpNamedAccessListDst          IpAddress,
    juniIpNamedAccessListDstMask      IpAddress,
    juniIpNamedAccessListProtocol     Integer32 }

juniIpNamedAccessListName OBJECT-TYPE
    SYNTAX      JuniIpPolicyName
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The name of the access list to which this entry belongs."
    ::= { juniIpNamedAccessListEntry 1 }

juniIpNamedAccessListElemId OBJECT-TYPE
    SYNTAX      Integer32 (0..10000)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The relative position of this entry within its access list.  Access
        list entries are searched in this sequence (low to high values) until a
        match is found.

        NOTE:  The value zero is reserved for use with SET operations to perform
        special-purpose table entry creations/deletions; see the DESCRIPTION of
        juniIpNamedAccessListRowStatus for details.

        Get/GetNext/GetBulk retrievals never return an entry for which this
        object is zero-valued."
    ::= { juniIpNamedAccessListEntry 2 }

juniIpNamedAccessListRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        Two configuration levels are defined, limited and full.  EARLY
        IMPLEMENTATIONS MIGHT PROVIDE ONLY THE LIMITED LEVEL OF CONFIGURATION
        CAPABILITY.

        *** LIMITED ACCESS LIST CONFIGURATION LEVEL ***

         1) RowStatus createAndGo/destroy operations directed to a target table
            entry for which juniIpNamedAccessListElemId is ZERO, have the
            following special-purpose semantics:
                createAndGo     Create an entry having the specified
                                configuration and append it to the target list,
                                i.e. assign it a value of
                                juniIpNamedAccessListElemId that is one greater
                                than the current last element in the list.
                destroy         Destroy the specified list and all of its
                                constituent elements.

         2) RowStatus createAndGo/destroy operations directed to a target table
            entry for which juniIpNamedAccessListElemId is NONZERO are
            disallowed.

        *** FULL ACCESS LIST CONFIGURATION LEVEL ***

        Permit conventional RowStatus-based management of table entries having a
        nonzero value for juniIpNamedAccessListElemId, IN ADDITION TO the
        special RowStatus semantics applied to entries having a zero value for
        juniIpNamedAccessListElemId.

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
                juniIpNamedAccessListRowStatus

        In addition, when creating an entry the following conditions must hold:

                The value of juniIpNamedAccessListElemId is nonzero.

        Once created, element attributes cannot be modified except by a
        RowStatus destroy operation to delete the list element."
    ::= { juniIpNamedAccessListEntry 3 }

juniIpNamedAccessListAction OBJECT-TYPE
    SYNTAX      JuniIpPolicyPolicy
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Specifies the disposition of an item that matches the comparison
        criteria described by this entry."
    DEFVAL    { permit }
    ::= { juniIpNamedAccessListEntry 4 }

juniIpNamedAccessListSrc OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "A source IP address.  A subject IP address is first masked with the
        value of juniIpNamedAccessListSrcMask, then the result is compared to
        this value.  Setting both this object and its corresponding mask to
        0.0.0.0 acts as a wildcard, matching any source IP address."
    DEFVAL    { '00000000'H }    -- 0.0.0.0
    ::= { juniIpNamedAccessListEntry 5 }

juniIpNamedAccessListSrcMask OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The IP address mask to be applied to a subject source IP address before
        comparing it to juniIpNamedAccessListSrc.  Ones in the mask identify
        which bits in the subject IP address are significant for the comparison.

        To be considered valid, a nonzero value for this object must contain a
        single contiguous string of ones, beginning with the most significant
        bit of the mask."
    DEFVAL    { '00000000'H }    -- 0.0.0.0
    ::= { juniIpNamedAccessListEntry 6 }

juniIpNamedAccessListDst OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "A destination IP address.  A subject IP address is first masked with
        the value of juniIpNamedAccessListDstMask, then the result is compared
        to this value.  Setting both this object and its corresponding mask to
        0.0.0.0 acts as a wildcard, matching any destination IP address."
    DEFVAL    { '00000000'H }    -- 0.0.0.0
    ::= { juniIpNamedAccessListEntry 7 }

juniIpNamedAccessListDstMask OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The IP address mask to be applied to a subject destination IP address
        before comparing it to juniIpNamedAccessListDst.  Ones in the mask
        identify which bits in the IP address are significant for the
        comparison.

        To be considered valid, a nonzero value for this object must contain a
        single contiguous string of ones, beginning with the most significant
        bit of the mask."
    DEFVAL    { '00000000'H }    -- 0.0.0.0
    ::= { juniIpNamedAccessListEntry 8 }

juniIpNamedAccessListProtocol OBJECT-TYPE
    SYNTAX      Integer32 (0..255)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "An IP Protocol value.  Nonzero values match a specific IP Protocol
        value (e.g. 6 for TCP) carried in an IP packet; a value of zero acts as
        a wildcard, matching any IP Protocol."
    DEFVAL    { 0 }
    ::= { juniIpNamedAccessListEntry 9 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- IP AS-Path Access List
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
--
-- The IP AS-Path Access Table
--
juniIpAspAccessTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIpAspAccessEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for elements of IP AS-Path access entries."
    ::= { juniIpAspAccessList 1 }

juniIpAspAccessEntry OBJECT-TYPE
    SYNTAX      JuniIpAspAccessEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of an IP AS-Path access
        element."
    INDEX     { juniIpAspAccessName,
                juniIpAspAccessElemId }
    ::= { juniIpAspAccessTable 1 }

JuniIpAspAccessEntry ::= SEQUENCE {
    juniIpAspAccessName               JuniIpPolicyName,
    juniIpAspAccessElemId             Integer32,
    juniIpAspAccessCreatedInternally  TruthValue,
    juniIpAspAccessPolicy             JuniIpPolicyPolicy,
    juniIpAspAccessExpression         OCTET STRING,
    juniIpAspAccessRowStatus          RowStatus }

juniIpAspAccessName OBJECT-TYPE
    SYNTAX      JuniIpPolicyName
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The name of the AS-Path Access List to which this entry belongs."
    ::= { juniIpAspAccessEntry 1 }

juniIpAspAccessElemId OBJECT-TYPE
    SYNTAX      Integer32 (0..10000)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The element ID portion of the IP AS-Path for this entry."
    ::= { juniIpAspAccessEntry 2 }

juniIpAspAccessCreatedInternally OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicated whether this entry was created internally by the system, or
        dynamically via a management interface.  A true value for this object
        indicates that this entry was created internally; false indicates
        externally."
    ::= { juniIpAspAccessEntry 3 }

juniIpAspAccessPolicy OBJECT-TYPE
    SYNTAX      JuniIpPolicyPolicy
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the action to take for this AS-Path access list."
    ::= { juniIpAspAccessEntry 4 }

juniIpAspAccessExpression OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(1..256))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The AS-Path access list expression for this entry."
    ::= { juniIpAspAccessEntry 5 }

juniIpAspAccessRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
            juniIpCommunityRowStatus

        In addition, when creating an entry the following conditions must hold:

            Once created, only certain attributes can be modified."
    ::= { juniIpAspAccessEntry 6 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- IP Prefix Lists
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
--
-- The IP Prefix List Table
--
juniIpPrefixListTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIpPrefixListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for elements of IP prefix lists.  Entries
        belonging to the same prefix list are ordered, and comparisons to those
        entries are performed in that order until a match is detected.  If no
        match is found, the default action is to 'deny'."
    ::= { juniIpPrefixList 1 }

juniIpPrefixListEntry OBJECT-TYPE
    SYNTAX      JuniIpPrefixListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of an IP prefix list element."
    INDEX     { juniIpPrefixListName,
                juniIpPrefixListElemId,
                juniIpPrefixListIpAddress,
                juniIpPrefixListLength }
    ::= { juniIpPrefixListTable 1 }

JuniIpPrefixListEntry ::= SEQUENCE {
    juniIpPrefixListName          JuniIpPolicyName,
    juniIpPrefixListElemId        Integer32,
    juniIpPrefixListIpAddress     IpAddress,
    juniIpPrefixListLength        Integer32,
    juniIpPrefixListPolicy        JuniIpPolicyPolicy,
    juniIpPrefixListGeValue       Integer32,
    juniIpPrefixListLeValue       Integer32,
    juniIpPrefixListDescription   DisplayString,
    juniIpPrefixListHitCount      Counter32,
    juniIpPrefixListRowStatus     RowStatus }

juniIpPrefixListName OBJECT-TYPE
    SYNTAX      JuniIpPolicyName
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The name of the prefix list to which this entry belongs."
    ::= { juniIpPrefixListEntry 1 }

juniIpPrefixListElemId OBJECT-TYPE
    SYNTAX      Integer32 (0..10000)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The relative position of this entry within its prefix list.  Access
        list entries are searched in this sequence (low to high values) until a
        match is found."
    ::= { juniIpPrefixListEntry 2 }

juniIpPrefixListIpAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The IP Address portion of the IP List value for this entry."
    ::= { juniIpPrefixListEntry 3 }

juniIpPrefixListLength OBJECT-TYPE
    SYNTAX      Integer32 (0..32)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The length portion of the IP List value for this entry."
    ::= { juniIpPrefixListEntry 4 }

juniIpPrefixListPolicy OBJECT-TYPE
    SYNTAX      JuniIpPolicyPolicy
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The IP Prefix list action to perform for this entry."
    ::= { juniIpPrefixListEntry 5 }

juniIpPrefixListGeValue OBJECT-TYPE
    SYNTAX      Integer32 (0..32)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The minimum prefix length to apply to address."
    ::= { juniIpPrefixListEntry 6 }

juniIpPrefixListLeValue OBJECT-TYPE
    SYNTAX      Integer32 (0..32)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The maximum prefix length to apply to address."
    ::= { juniIpPrefixListEntry 7 }

juniIpPrefixListDescription OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The administratively assigned description for this entry."
    ::= { juniIpPrefixListEntry 8 }

juniIpPrefixListHitCount OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of hits for this entry."
    ::= { juniIpPrefixListEntry 9 }

juniIpPrefixListRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table according to the
        RowStatus textual convention, constrained to support the following
        values only:

            createAndGo
            destroy

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:

            juniIpPrefixListRowStatus

        In addition, when creating an entry the following conditions must hold:

            The value of juniIpPrefixListElemId is nonzero.

        Once created, only certain attributes can be modified."
    ::= { juniIpPrefixListEntry 10 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- IP Prefix Tree
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
--
-- The IP Prefix Tree Table
--
juniIpPrefixTreeTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIpPrefixTreeEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for elements of IP prefix trees.  Entries
        belonging to the same prefix tree are ordered, and comparisons to those
        entries are performed in that order until a match is detected.  If no
        match is found, the default action is to 'deny'."
    ::= { juniIpPrefixTree 1 }

juniIpPrefixTreeEntry OBJECT-TYPE
    SYNTAX      JuniIpPrefixTreeEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of an IP prefix tree element."
    INDEX     { juniIpPrefixTreeName,
                juniIpPrefixTreeIpAddress,
                juniIpPrefixTreeLength }
    ::= { juniIpPrefixTreeTable 1 }

JuniIpPrefixTreeEntry ::= SEQUENCE {
    juniIpPrefixTreeName          JuniIpPolicyName,
    juniIpPrefixTreeIpAddress     IpAddress,
    juniIpPrefixTreeLength        Integer32,
    juniIpPrefixTreePolicy        JuniIpPolicyPolicy,
    juniIpPrefixTreeDescription   DisplayString,
    juniIpPrefixTreeHitCount      Counter32,
    juniIpPrefixTreeRowStatus     RowStatus }

juniIpPrefixTreeName OBJECT-TYPE
    SYNTAX      JuniIpPolicyName
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The name of the prefix tree to which this entry belongs."
    ::= { juniIpPrefixTreeEntry 1 }

juniIpPrefixTreeIpAddress OBJECT-TYPE
    SYNTAX      IpAddress
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The IP Address portion of the IP Prefix value for this entry."
    ::= { juniIpPrefixTreeEntry 2 }

juniIpPrefixTreeLength OBJECT-TYPE
    SYNTAX      Integer32 (0..32)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The length portion of the IP Prefix value for this entry."
    ::= { juniIpPrefixTreeEntry 3 }

juniIpPrefixTreePolicy OBJECT-TYPE
    SYNTAX      JuniIpPolicyPolicy
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The IP Prefix tree policy perform for this entry."
    ::= { juniIpPrefixTreeEntry 4 }

juniIpPrefixTreeDescription OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The administratively assigned description for this entry."
    ::= { juniIpPrefixTreeEntry 5 }

juniIpPrefixTreeHitCount OBJECT-TYPE
    SYNTAX      Counter32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "The number of hits for this entry."
    ::= { juniIpPrefixTreeEntry 6 }

juniIpPrefixTreeRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
            juniIpPrefixTreeRowStatus

        In addition, when creating an entry the following conditions must hold:

            The value of juniIpPrefixTreeIpAddress and juniIpPrefixTreeLength
            are nonzero.

        Once created, only certain attributes can be modified."
    ::= { juniIpPrefixTreeEntry 7 }

-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- IP Community List Tables
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++

--
-- The IP Community List Table
--
juniIpCommunityListTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIpCommunityListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for elements of IP Community Lists.
        Entries belonging to the same Community List are ordered.  The table
        supports standard and extended community lists."
    ::= { juniIpCommunityList 1 }

juniIpCommunityListEntry OBJECT-TYPE
    SYNTAX      JuniIpCommunityListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of an IP Community List
        element."
    INDEX     { juniIpCommunityListName,
                juniIpCommunityListElemId }
    ::= { juniIpCommunityListTable 1 }

JuniIpCommunityListEntry ::= SEQUENCE {
    juniIpCommunityListName               JuniIpPolicyName,
    juniIpCommunityListElemId             Integer32,
    juniIpCommunityListCreatedInternally  TruthValue,
    juniIpCommunityListExtended           TruthValue,
    juniIpCommunityListPolicy             JuniIpPolicyPolicy,
    juniIpCommunityListExpression         OCTET STRING,
    juniIpCommunityListRowStatus          RowStatus }

juniIpCommunityListName OBJECT-TYPE
    SYNTAX      JuniIpPolicyName
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The name of the Community List to which this entry belongs."
    ::= { juniIpCommunityListEntry 1 }

juniIpCommunityListElemId OBJECT-TYPE
    SYNTAX      Integer32 (0..10000)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The IP Address portion of the IP Prefix value for this entry."
    ::= { juniIpCommunityListEntry 2 }

juniIpCommunityListCreatedInternally OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicated whether this entry was created internally by the system, or
        dynamically via a management interface.  A true value for this object
        indicates that this entry was created internally; false indicates
        externally."
    ::= { juniIpCommunityListEntry 3 }

juniIpCommunityListExtended OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates whether this entry is a standard or extended Community List.
        True indicates extended, false indicates standard"
    ::= { juniIpCommunityListEntry 4 }

juniIpCommunityListPolicy OBJECT-TYPE
    SYNTAX      JuniIpPolicyPolicy
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the policy action to perform for this list."
    ::= { juniIpCommunityListEntry 5 }

juniIpCommunityListExpression OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(1..256))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The community list expression for this entry."
    ::= { juniIpCommunityListEntry 6 }

juniIpCommunityListRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
            juniIpCommunityRowStatus

        In addition, when creating an entry the following conditions must hold:

            Once created, only certain attributes can be modified."
    ::= { juniIpCommunityListEntry 7 }


--
-- The IP Extended Community List Table
--
juniIpExtCommunityListTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIpExtCommunityListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for Extended IP Community Lists.  Entries
        belonging to the same Extended Community List are ordered."
    ::= { juniIpCommunityList 2 }

juniIpExtCommunityListEntry OBJECT-TYPE
    SYNTAX      JuniIpExtCommunityListEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of an Extended IP Community
        List element."
    INDEX     { juniIpExtCommunityListName,
                juniIpExtCommunityListElemId }
    ::= { juniIpExtCommunityListTable 1 }

JuniIpExtCommunityListEntry ::= SEQUENCE {
    juniIpExtCommunityListName                JuniIpPolicyName,
    juniIpExtCommunityListElemId              Integer32,
    juniIpExtCommunityListCreatedInternally   TruthValue,
    juniIpExtCommunityListPolicy              JuniIpPolicyPolicy,
    juniIpExtCommunityListExpression          OCTET STRING,
    juniIpExtCommunityListRowStatus           RowStatus }

juniIpExtCommunityListName OBJECT-TYPE
    SYNTAX      JuniIpPolicyName
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The name of the Extended Community List to which this entry belongs."
    ::= { juniIpExtCommunityListEntry 1 }

juniIpExtCommunityListElemId OBJECT-TYPE
    SYNTAX      Integer32 (0..10000)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The element ID value for this entry."
    ::= { juniIpExtCommunityListEntry 2 }

juniIpExtCommunityListCreatedInternally OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicated whether this entry was created internally by the system, or
        dynamically via a management interface.  A true value for this object
        indicates that this entry was created internally; false indicates
        externally."
    ::= { juniIpExtCommunityListEntry 3 }

juniIpExtCommunityListPolicy OBJECT-TYPE
    SYNTAX      JuniIpPolicyPolicy
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the policy action to perform for this list."
    ::= { juniIpExtCommunityListEntry 4 }

juniIpExtCommunityListExpression OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(8..256))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "The extended community list expression for this entry."
    ::= { juniIpExtCommunityListEntry 5 }

juniIpExtCommunityListRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
            juniIpExtCommunityRowStatus

        In addition, when creating an entry the following conditions must hold:

            The value of juniIpExtCommunityListElemId is included in this table
            as a key for future use.  It must be the value zero.

        Once created, only certain attributes can be modified."
    ::= { juniIpExtCommunityListEntry 6 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- IP Redistribute Tables
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
--
-- The IP Dynamic Route Redistribution Table
--
juniIpDynRedistributeTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIpDynRedistributeEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for elements of IP Dynamic Route
        Redistribution elements."
    ::= { juniIpRedistributeList 1 }

juniIpDynRedistributeEntry OBJECT-TYPE
    SYNTAX      JuniIpDynRedistributeEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of a dynamic IP Route
        Redistribute element."
    INDEX     { juniIpDynRedistributeToProtocol }
    ::= { juniIpDynRedistributeTable 1 }

JuniIpDynRedistributeEntry ::= SEQUENCE {
    juniIpDynRedistributeToProtocol   JuniIpDynRedistributeProtocol,
    juniIpDynRedistributeState        JuniIpPolicyAdminStatus,
    juniIpDynRedistributeRowStatus    RowStatus }

juniIpDynRedistributeToProtocol OBJECT-TYPE
    SYNTAX      JuniIpDynRedistributeProtocol
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Identifies the protocol associated with this Dynamic Route
        Redistribution element that routes are redistributed to."
    ::= { juniIpDynRedistributeEntry 1 }

juniIpDynRedistributeState OBJECT-TYPE
    SYNTAX      JuniIpPolicyAdminStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the enable/disable state of this redistribution element."
    DEFVAL    { ipPolicyAdminStateEnable }
    ::= { juniIpDynRedistributeEntry 2 }

juniIpDynRedistributeRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
            juniIpDynRedistributeRowStatus

        Once created, only the juniIpDynRedistributeState object can be
        modified."
    ::= { juniIpDynRedistributeEntry 3 }


--
-- The IP Route Redistribution Table
--
juniIpRedistributeTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIpRedistributeEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for elements of IP Route Redistribution
        elements."
    ::= { juniIpRedistributeList 2 }

juniIpRedistributeEntry OBJECT-TYPE
    SYNTAX      JuniIpRedistributeEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of an IP Route Redistribution
        element."
    INDEX     { juniIpRedistributeToProtocol,
                juniIpRedistributeFromProtocol }
    ::= { juniIpRedistributeTable 1 }

JuniIpRedistributeEntry ::= SEQUENCE {
    juniIpRedistributeToProtocol      JuniIpRedistributeProtocol,
    juniIpRedistributeFromProtocol    JuniIpRedistributeProtocol,
    juniIpRedistributeState           JuniIpPolicyAdminStatus,
    juniIpRedistributeRouteMapName    JuniIpPolicyName,
    juniIpRedistributeRowStatus       RowStatus }

juniIpRedistributeToProtocol OBJECT-TYPE
    SYNTAX      JuniIpRedistributeProtocol
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Identifies the protocol for this element that routes are redistributed
        to."
    ::= { juniIpRedistributeEntry 1 }

juniIpRedistributeFromProtocol OBJECT-TYPE
    SYNTAX      JuniIpRedistributeProtocol
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Identifies the protocol for this element that routes are redistributed
        from."
    ::= { juniIpRedistributeEntry 2 }

juniIpRedistributeState OBJECT-TYPE
    SYNTAX      JuniIpPolicyAdminStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the enable/disable state of this redistribution element."
    DEFVAL    { ipPolicyAdminStateEnable }
    ::= { juniIpRedistributeEntry 3 }

juniIpRedistributeRouteMapName OBJECT-TYPE
    SYNTAX      JuniIpPolicyName
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Identifies the IP route-map associated with this IP Route
        Redistribution element."
    ::= { juniIpRedistributeEntry 4 }

juniIpRedistributeRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
            juniIpRedistributeRowStatus
            juniIpRedistributeRouteMapName

        Once created, only the juniIpRedistributeState object can be modified."
    ::= { juniIpRedistributeEntry 5 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- IP Route-Map Tables
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
--
-- The IP Route-Map Table
--
juniIpRouteMapTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIpRouteMapEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for elements of IP Route Maps."
    ::= { juniIpRouteMapTree 1 }

juniIpRouteMapEntry OBJECT-TYPE
    SYNTAX      JuniIpRouteMapEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of an IP Route Map element."
    INDEX     { juniIpRouteMapName,
                juniIpRouteMapSequenceNum,
                juniIpRouteMapElemId,
                juniIpRouteMapSubElemId }
    ::= { juniIpRouteMapTable 1 }

JuniIpRouteMapEntry ::= SEQUENCE {
    juniIpRouteMapName                JuniIpPolicyName,
    juniIpRouteMapSequenceNum         Integer32,
    juniIpRouteMapElemId              Integer32,
    juniIpRouteMapSubElemId           Integer32,
    juniIpRouteMapCreatedInternally   TruthValue,
    juniIpRouteMapPolicy              JuniIpPolicyPolicy,
    juniIpRouteMapDisplay             OCTET STRING }

juniIpRouteMapName OBJECT-TYPE
    SYNTAX      JuniIpPolicyName
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The name of the route map to which this entry belongs."
    ::= { juniIpRouteMapEntry 1 }

juniIpRouteMapSequenceNum OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The element ID value for this entry."
    ::= { juniIpRouteMapEntry 2 }

juniIpRouteMapElemId OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The element ID to which this entry belongs."
    ::= { juniIpRouteMapEntry 3 }

juniIpRouteMapSubElemId OBJECT-TYPE
    SYNTAX      Integer32 (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The sub-element ID to which this entry belongs."
    ::= { juniIpRouteMapEntry 4 }

juniIpRouteMapCreatedInternally OBJECT-TYPE
    SYNTAX      TruthValue
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicated whether this entry was created internally by the system, or
        dynamically via a management interface.  A true value for this object
        indicates that this entry was created internally; false indicates
        externally."
    ::= { juniIpRouteMapEntry 5 }

juniIpRouteMapPolicy OBJECT-TYPE
    SYNTAX      JuniIpPolicyPolicy
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Indicates the policy action performed by this element."
    ::= { juniIpRouteMapEntry 6 }

juniIpRouteMapDisplay OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(0..2048))
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
        "Textual information taken from the NVT ASCII character set
        (i.e. RFC1903 DisplayString), but with increased length.  The
        information in this object is the series of set, match, and/or match &
        set clauses for this route map.

        It is assumed that the information conveyed in this object is used for
        display purposes and in general, is not parsed.  The information in this
        string is a concatentation of routemap clauses configured via the
        systems non SNMP interface."
    ::= { juniIpRouteMapEntry 7 }

--
-- The IP Route-Map version 2 Table
--
juniIpRouteMapV2Table OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIpRouteMapV2Entry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for route maps instances."
    ::= { juniIpRouteMapTree 2 }

juniIpRouteMapV2Entry OBJECT-TYPE
    SYNTAX      JuniIpRouteMapV2Entry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry is a specific instance of the Route Map."
    INDEX     { juniIpRouteMapV2Name,
                juniIpRouteMapV2SequenceNum }
    ::= { juniIpRouteMapV2Table 1 }

JuniIpRouteMapV2Entry ::= SEQUENCE {
    juniIpRouteMapV2Name             JuniIpPolicyName,
    juniIpRouteMapV2SequenceNum      Integer32,
    juniIpRouteMapV2Policy           JuniIpPolicyPolicy,
    juniIpRouteMapV2RowStatus        RowStatus }

juniIpRouteMapV2Name OBJECT-TYPE
    SYNTAX      JuniIpPolicyName
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The name of the route map to which this instance entry belongs."
    ::= { juniIpRouteMapV2Entry 1 }

juniIpRouteMapV2SequenceNum OBJECT-TYPE
    SYNTAX      Integer32 (1..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Multiple instances of the same route map can be created by assigning a
        different sequence number to it.  Each instance is identified by the
        route map name and the sequence number.  The value of the sequence
        number associated with the particular route map instance determines the
        order in which the routing protocol evaluates routes; the instance of
        having lowest sequence number is evaluated first.  If the routes pass
        all the match conditions specified in the lowest-numbered instance, and
        if all set clause elements are successfully configured, then no other
        instance of the route map is considered.  However, any routes that do
        not pass all the match conditions are evaluated against the next
        instance of the route map."
    ::= { juniIpRouteMapV2Entry 2 }

juniIpRouteMapV2Policy OBJECT-TYPE
    SYNTAX      JuniIpPolicyPolicy
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Indicates the policy action performed by this route map instance."
    DEFVAL    { permit }
    ::= { juniIpRouteMapV2Entry 3 }

juniIpRouteMapV2RowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        To create an entry in this table, the following entry objects MUST be
        explicitly configured:
            juniIpRouteMapV2RowStatus

        To delete an entry in this table, the following entry objects MUST be
        explicitly configured:
            juniIpRouteMapV2RowStatus

        Once created, juniIpRouteMapV2Policy attribute can be modified.
        To modify juniIpRouteMapV2Policy, set juniIpRouteMapV2RowStatus also.

        Note: Match, match-set and set clause elements can be configured for a
              specific instance of the route map.  First create the route map
              instance to make use of the same to configure in the clause table.
              Deletion of the route map instance will also delete all the clause
              elements confgured for that instance as clause elements are
              configured for that instance."
    ::= { juniIpRouteMapV2Entry 4 }


--
-- The IP route-map clauses(set, match-set and match) table
--
juniIpRouteMapClauseTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF JuniIpRouteMapClauseEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "This table contains entries for instances of the route map clause
        elements."
    ::= { juniIpRouteMapTree 3 }

juniIpRouteMapClauseEntry OBJECT-TYPE
    SYNTAX      JuniIpRouteMapClauseEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "Each entry describes the characteristics of one route map clause
        element instance."
    INDEX     { juniIpRouteMapV2Name,
                juniIpRouteMapV2SequenceNum,
                juniIpRouteMapClauseElemId,
                juniIpRouteMapClauseSubElemId }
    ::= { juniIpRouteMapClauseTable 1 }

JuniIpRouteMapClauseEntry ::= SEQUENCE {
    juniIpRouteMapClauseElemId          INTEGER,
    juniIpRouteMapClauseSubElemId       Integer32,
    juniIpRouteMapClauseElemIdAddon     INTEGER,
    juniIpRouteMapClauseElementValue    DisplayString,
    juniIpRouteMapClauseRowStatus       RowStatus }

juniIpRouteMapClauseElemId OBJECT-TYPE
    SYNTAX      INTEGER {
                 -- match clause element selection options
                    matchNotKnown(0),
                    matchAsPath(1),
                    matchCommunity(2),
                    matchExtendedCommunity(3),
                    matchDistance(4),
                    matchAccessList(5),
                    matchNextHop(6),
                    matchPrefixList(7),
                    matchNextHopPreList(8),
                    matchPrefixTree(9),
                    matchNextHopPreTree(10),
                    matchLevel(11),
                    matchMetric(12),
                    matchMetricType(13),
                    matchTag(14),
                    matchRouteType(15),
                    matchSource(16),
                    matchPolicyList(17),
                 -- set clause element selection options
                    setAsPath(100),
                    setAsPathCreateList(101),
                    setAutoTag(102),
                    setCommList(103),
                    setCommunityNone(104),
                    setCommunityAdd(105),
                    setCommunity(106),
                    setCommunityCreateListAdd(107),
                    setCommunityCreateList(108),
                    setExtendedCommunityCreateAdd(109),
                    setExtendedCommunityCreate(110),
                    setNextHop(111),
                    setNextHopPeerAddr(112),
                    setLocalPref(113),
                    setWeight(114),
                    setLevel(115),
                    setMetric(116),
                    setMetricType(117),
                    setTag(118),
                    setOrigin(119),
                    setRouteType(220),
                    setDampingCreate(221),
                    setDistance(222),
                 -- match-set clause element selection option
                    matchSetSummary(300) }
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The clause element selection option.  Select the appropriate element
        option to configure each element instance of match, match-set and set
        clauses.  For the complete configuration map table refer to the
        juniIpRouteMapClauseRowStatus object's DESCRIPTION."
    ::= { juniIpRouteMapClauseEntry 1 }

juniIpRouteMapClauseSubElemId OBJECT-TYPE
    SYNTAX      Integer32 (1..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
        "The clause element sub ID used to distinguish specific instance of the
        element.  This value is determined by choosing the next available by
        walking the table."
    ::= { juniIpRouteMapClauseEntry 2 }

juniIpRouteMapClauseElemIdAddon OBJECT-TYPE
    SYNTAX      INTEGER {
                    notApplicable(0),
                    exact(1),
                    delete(2),
                    relativeNeg(3),
                    relativePos(4),
                    extCommRt(5),
                    extCommSoo(6),
                    interfaceValue(7),
                    ipAddress(8) }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This represents clause element instance add-on option selected along
        with the main option (juniIpRouteMapClauseElemId) whenever it applies.
        For more information on how to map this object value to each value,
        refer to the mapping table in the juniIpRouteMapClauseRowStatus object's
        DESCRIPTION."
    DEFVAL    { notApplicable }
    ::= { juniIpRouteMapClauseEntry 3 }

juniIpRouteMapClauseElementValue OBJECT-TYPE
    SYNTAX      DisplayString (SIZE(0..100))
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "This represents set, match-set and match clauses' different element
        instance values in character string form.  Whatever may be the data type
        of the attribute element instance value, it is always interpreted as a
        set of characters for both configuration and display purposes.  It is up
        to the user to know the element's data type mapping in order to input
        the correct value while configuring.  Refer to the mapping table in the
        juniIpRouteMapClauseRowStatus object descrption for detailed
        information."
    ::= { juniIpRouteMapClauseEntry 4 }

juniIpRouteMapClauseRowStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
        "Controls creation/deletion of entries in this table according to the
        RowStatus textual convention, constrained to support the following
        values only:
            createAndGo
            destroy

        To create/delete an entry in this table, the following entry objects
        MUST be explicitly configured:
            juniIpRouteMapClauseElementValue
            juniIpRouteMapClauseRowStatus

        Additional object juniIpRouteMapClauseElemIdAddon may become OPTIONAL
        for some elements creation/deletion along with the above.  Refer the
        mapping table below to determine which elements are required.

        The table entry elements may not be modified.  Only create and delete
        are allowed.

        Note#1: Make sure route map(s) are created before configuring their
                corresponding clause elements.
        Note#2: The mapping table below is the extensive guide for the options,
                values and ranges of the table objects
                juniIpRouteMapClauseElemId, juniIpRouteMapClauseElemIdAddon and
                juniIpRouteMapClauseElementValue.

                Clause element configuration selection mapping table
                ====================================================
        ClauseElemId               ClauseElemIdAddon ClauseElementValue
        ============               ================= ==================

        matchAsPath                notApplicable     DisplayString (SIZE(1..32))
        matchCommunity             exact/            DisplayString (SIZE(1..32))
                                   notApplicable
        matchExtendedCommunity     exact/            DisplayString (SIZE(1..32))
                                   notApplicable

        Note#3: At a given time only one can be configured for access list and
                prefix-list/trees'.
        matchAccessList            notApplicable     DisplayString (SIZE(1..32))
        matchPrefixList            notApplicable     DisplayString (SIZE(1..32))
        matchPrefixTree            notApplicable     DisplayString (SIZE(1..32))
        matchNextHop               notApplicable     DisplayString (SIZE(1..32))
        matchNextHopPreList        notApplicable     DisplayString (SIZE(1..32))
        matchNextHopPreTree        notApplicable     DisplayString (SIZE(1..32))

        Note#4: For matchLevel, matchMetricType and matchRouteType element
                selection choose the exact case-sensitive string to set the
                option.
                Example: For matchLevel, option levelOne, levelOneAndTwo, etc.
                         can be set.
        matchLevel                 notApplicable     { levelOne,
                                                       levelOneAndTwo,
                                                       levelTwo,
                                                       backbone,
                                                       stubArea }
        matchMetricType            notApplicable     { internal or typeOne,
                                                       external or typeTwo }
        matchRouteType             notApplicable     { external,
                                                       internal,
                                                       internalInter,
                                                       internalIntra }

        matchDistance              notApplicable     Integer32 (0..255)
        matchMetric                notApplicable     Unsigned32
        matchTag                   notApplicable     Unsigned32
        matchPolicyList            notApplicable     DisplayString (SIZE(1..32))

        setAsPath                  notApplicable     DisplayString (SIZE(1..32))
        setCommunityAdd            notApplicable     DisplayString (SIZE(1..32))
        setCommList                delete/           DisplayString (SIZE(1..32))
                                   notApplicable
        setCommunity               notApplicable     DisplayString (SIZE(1..32))

        Note#5: For below elements selection choose the exact case-sensitive
                string to set the option.
                Example: For setOrigin, egp or igp or incomplete will be the
                         valid options to select.
        setAutoTag                 notApplicable     { autoTag }
        setCommunityNone           notApplicable     { communityNone }

        Note#6: setCommunityCreateList and setCommunityCreateListAdd will have
                only one instance and all will be set in one instance of the
                element (either setCommunityCreateList or
                setCommunityCreateListAdd), i.e., all options and values will
                aggregate in one SubElementId.
        setCommunityCreateList     notApplicable     Unsigned32
        setCommunityCreateListAdd  notApplicable     Unsigned32
        setCommunityCreateList     notApplicable     { none,
                                                       localAs,
                                                       noAdvertise,
                                                       noExport }
        setCommunityCreateListAdd  notApplicable     { none,
                                                       localAs,
                                                       noAdvertise,
                                                       noExport }

        setLevel                  notApplicable      { backbone,
                                                       levelOne,
                                                       levelOneAndTwo,
                                                       levelTwo,
                                                       stubArea }
        setRouteType              notApplicable      { external,
                                                       internal,
                                                       internalInter,
                                                       internalIntra }
        setNextHopPeerAddr        notApplicable      { peerAddress }
        setMetricType             notApplicable      { external,
                                                       internal }
        setOrigin                 notApplicable      { egp,
                                                       igp,
                                                       incomplete }

        setAsPathCreateList       notApplicable      Interger32 (1..65535)
        setTag                    notApplicable      Unsigned32
        setWeight                 notApplicable      Unsigned32
        setDistance               notApplicable      Interger32 (1..255)
        setLocalPref              notApplicable      Unsigned32
        setMetric                 relativeNeg/       Unsigned32
                                  relativePos/
                                  notApplicable

        Note#7: setExtendedCommunityCreate and setExtendedCommunityCreateAdd
                will have only one instance and all will be set in one instance
                of the element (either setExtendedCommunityCreate or
                setExtendedCommunityCreateAdd) i.e. all options and values will
                aggregate in one SubElementId.
        setExtendedCommunityCreate extCommRt/        IPADDRESS:Unsigned32 or
                                   notApplicable     IPADDRESS-in-ASN:Unsigned32
        setExtendedCommunityCreate extCommSoo/       IPADDRESS:Unsigned32 or
                                   notApplicable     IPADDRESS-in-ASN:Unsigned32
        setExtendedCommunityCreateAdd extCommRt/     IPADDRESS:Unsigned32 or
                                      notApplicable  IPADDRESS-in-ASN:Unsigned32
        setExtendedCommunityCreateAdd extCommSoo/    IPADDRESS:Unsigned32
                                      notApplicable  IPADDRESS-in-ASN:Unsigned32

        Note#8: Damping element has only one instance at any given time.  It can
                be deleted by just refering to the instance (elementID and
                subElementId) without refering the exact value; i.e., while
                deleting, values doesn't matter.
        setDampingCreate          notApplicable
                                 1. HalfLifeiTime-Interger32 (1..45)
                                 2. RtSuppressTime-Interger32 (1..20000)
                                 3. SuppressedRtReuseTime-Interger32 (1..20000)
                                 4. MaxRtSuppressTime-Interger32 (1..255)
                                 5. UnreachableRtHalfLifeTime-Interger32 (1..45)
        Note#9: 1, 2, 3 and 4 values are MUST values to be specified (in
                minutes) for route flap damping and 5th one is optional.  Format
                for specifying the values are very rigid and strict.  Always
                specify four MUST values.  The first value shouldn't be preceded
                with space characters and last the value always should be
                followed with one space character.  From first value to till
                last value, all the values will be separated from each other by
                one space character.

        setNextHop                interfaceValue/    Unsigned32
                                  notApplicable
        setNextHop                ipAddress/         IPADDRESS
                                  notApplicable "
    ::= { juniIpRouteMapClauseEntry 5 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Notifications
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- No notifications are defined in this MIB.  Placeholders follow.
-- juniIpPolicyTrapEnables OBJECT IDENTIFIER ::= { juniIpPolicyMIB 2 }
-- juniIpPolicyTraps       OBJECT IDENTIFIER ::= { juniIpPolicyMIB 3 }
-- juniIpPolicyTrapPrefix  OBJECT IDENTIFIER ::= { juniIpPolicyTraps 0 }


-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
-- Conformance information
-- +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
juniIpPolicyConformance     OBJECT IDENTIFIER ::= { juniIpPolicyMIB 4 }
juniIpPolicyCompliances     OBJECT IDENTIFIER ::= { juniIpPolicyConformance 1 }
juniIpPolicyGroups          OBJECT IDENTIFIER ::= { juniIpPolicyConformance 2 }

--
-- compliance statements
--
juniIpPolicyCompliance  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "An obsolete compliance statement for entities that implement the
        Juniper IP Policy MIB.  This statement became obsolete when support was
        added for the IP Named Access List."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpAccessListGroup }
    ::= { juniIpPolicyCompliances 1 }                              -- JUNOSe 1.0

juniIpPolicyCompliance2  MODULE-COMPLIANCE
    STATUS      obsolete
    DESCRIPTION
        "An obsolete compliance statement for entities that implement the
        Juniper IP Policy MIB.  This statement became obsolete when support was
        added for the IP ASP Access List, the IP Prefix List, the IP Prefix
        Tree, the IP Community List, the IP Extended Community List, IP Dynamic
        Route Redistribution, and the IP Route Map."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpAccessListGroup,
            juniIpNamedAccessListGroup }
    ::= { juniIpPolicyCompliances 2 }                              -- JUNOSe 2.0

juniIpPolicyCompliance3  MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "An obsolete compliance statement for entities that implement the
        Juniper IP Policy MIB.  This statement became obsolete when support was
        added for the IP Route Map configurations."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpAccessListGroup,
            juniIpNamedAccessListGroup,
            juniIpAspAccessListGroup,
            juniIpPrefixListGroup,
            juniIpPrefixTreeGroup,
            juniIpCommunityListGroup,
            juniIpExtCommunityListGroup,
            juniIpRedistributeGroup,
            juniIpRouteMapGroup }
    ::= { juniIpPolicyCompliances 3 }                              -- JUNOSe 3.0

juniIpPolicyCompliance4  MODULE-COMPLIANCE
    STATUS      current
    DESCRIPTION
        "The compliance statement for entities that implement the Juniper IP
        Policy MIB."
    MODULE   -- this module
        MANDATORY-GROUPS {
            juniIpAccessListGroup,
            juniIpNamedAccessListGroup,
            juniIpAspAccessListGroup,
            juniIpPrefixListGroup,
            juniIpPrefixTreeGroup,
            juniIpCommunityListGroup,
            juniIpExtCommunityListGroup,
            juniIpRedistributeGroup,
            juniIpRouteMapGroup2 }
    ::= { juniIpPolicyCompliances 4 }                              -- JUNOSe 5.1

--
-- units of conformance
--
juniIpAccessListGroup  OBJECT-GROUP
    OBJECTS {
        juniIpAccessListRowStatus,
        juniIpAccessListAction,
        juniIpAccessListSrc,
        juniIpAccessListSrcMask,
        juniIpAccessListDst,
        juniIpAccessListDstMask,
        juniIpAccessListProtocol }
    STATUS      current
    DESCRIPTION
        "A collection of objects for managing IP access list capabilities in a
        Juniper product."
    ::= { juniIpPolicyGroups 1 }

juniIpNamedAccessListGroup  OBJECT-GROUP
    OBJECTS {
        juniIpNamedAccessListRowStatus,
        juniIpNamedAccessListAction,
        juniIpNamedAccessListSrc,
        juniIpNamedAccessListSrcMask,
        juniIpNamedAccessListDst,
        juniIpNamedAccessListDstMask,
        juniIpNamedAccessListProtocol }
    STATUS      current
    DESCRIPTION
        "A named collection of objects for managing IP access list capabilities
        in a Juniper product."
    ::= { juniIpPolicyGroups 2 }

juniIpAspAccessListGroup  OBJECT-GROUP
    OBJECTS {
        juniIpAspAccessCreatedInternally,
        juniIpAspAccessPolicy,
        juniIpAspAccessExpression,
        juniIpAspAccessRowStatus }
    STATUS      current
    DESCRIPTION
        "A named collection of objects for managing AS-Path access list
        capabilities in a Juniper product."
    ::= { juniIpPolicyGroups 3 }

juniIpPrefixListGroup  OBJECT-GROUP
    OBJECTS {
        juniIpPrefixListPolicy,
        juniIpPrefixListGeValue,
        juniIpPrefixListLeValue,
        juniIpPrefixListDescription,
        juniIpPrefixListHitCount,
        juniIpPrefixListRowStatus }
    STATUS      current
    DESCRIPTION
        "A named collection of objects for managing Prefix list capabilities in
        a Juniper product."
    ::= { juniIpPolicyGroups 4 }

juniIpPrefixTreeGroup  OBJECT-GROUP
    OBJECTS {
        juniIpPrefixTreePolicy,
        juniIpPrefixTreeDescription,
        juniIpPrefixTreeHitCount,
        juniIpPrefixTreeRowStatus }
    STATUS      current
    DESCRIPTION
        "A named collection of objects for managing Prefix Tree capabilities in
        a Juniper product."
    ::= { juniIpPolicyGroups 5 }

juniIpCommunityListGroup  OBJECT-GROUP
    OBJECTS {
        juniIpCommunityListCreatedInternally,
        juniIpCommunityListExtended,
        juniIpCommunityListPolicy,
        juniIpCommunityListExpression,
        juniIpCommunityListRowStatus }
    STATUS      current
    DESCRIPTION
        "A named collection of objects for managing Community List capabilities
        in a Juniper product."
    ::= { juniIpPolicyGroups 6 }

juniIpExtCommunityListGroup  OBJECT-GROUP
    OBJECTS {
        juniIpExtCommunityListCreatedInternally,
        juniIpExtCommunityListPolicy,
        juniIpExtCommunityListExpression,
        juniIpExtCommunityListRowStatus }
    STATUS      current
    DESCRIPTION
        "A named collection of objects for managing Extended Community List
        capabilities in a Juniper product."
    ::= { juniIpPolicyGroups 7 }

juniIpRedistributeGroup  OBJECT-GROUP
    OBJECTS {
        juniIpDynRedistributeState,
        juniIpDynRedistributeRowStatus,
        juniIpRedistributeState,
        juniIpRedistributeRouteMapName,
        juniIpRedistributeRowStatus }
    STATUS      current
    DESCRIPTION
        "A collection of objects for managing IP route redistribution list
        capabilities in a Juniper product."
    ::= { juniIpPolicyGroups 8 }

juniIpRouteMapGroup  OBJECT-GROUP
    OBJECTS {
        juniIpRouteMapCreatedInternally,
        juniIpRouteMapPolicy,
        juniIpRouteMapDisplay }
    STATUS      obsolete
    DESCRIPTION
        "A collection of objects for managing IP route map list capabilities in
        a Juniper product."
    ::= { juniIpPolicyGroups 9 }

juniIpRouteMapGroup2  OBJECT-GROUP
    OBJECTS {
        juniIpRouteMapCreatedInternally,
        juniIpRouteMapPolicy,
        juniIpRouteMapDisplay,
        juniIpRouteMapV2Policy,
        juniIpRouteMapV2RowStatus,
        juniIpRouteMapClauseElemIdAddon,
        juniIpRouteMapClauseElementValue,
        juniIpRouteMapClauseRowStatus }
    STATUS      current
    DESCRIPTION
        "A collection of objects for managing IP route map list capabilities in
        a Juniper product."
    ::= { juniIpPolicyGroups 10 }

END
