ALCATEL-IND1-SLB-MIB DEFINITIONS ::= BEGIN

  IMPORTS
    MODULE-IDENTITY,
    OBJECT-IDENTITY,
    OBJECT-TYPE,
    NOTIFICATION-TYPE,
    IpAddress,
    Counter32,
    Integer32,
    Unsigned32,
    Counter64 						FROM SNMPv2-SMI

    MODULE-COMPLIANCE,
    OBJECT-GROUP,
    NOTIFICATION-GROUP     FROM SNMPv2-CONF

		SnmpAdminString FROM SNMP-FRAMEWORK-MIB

    MacAddress,
    TEXTUAL-CONVENTION,
    RowStatus              FROM SNMPv2-TC

    softentIND1Slb,
    slbTraps              FROM ALCATEL-IND1-BASE;

--
-- Module Identity
--

alcatelIND1SLBMIB MODULE-IDENTITY
   LAST-UPDATED    "200704030000Z"
   ORGANIZATION    "Alcatel-Lucent"
   CONTACT-INFO
       "Please consult with Customer Service to ensure the most appropriate
        version of this document is used with the products in question:
    
                   Alcatel-Lucent, Enterprise Solutions Division
                  (Formerly Alcatel Internetworking, Incorporated)
                          26801 West Agoura Road
                       Agoura Hills, CA  91301-5122
                         United States Of America
   
       Telephone:               North America  +1 800 995 2696
                                Latin America  +1 877 919 9526
                                Europe         +31 23 556 0100
                                Asia           +65 394 7933
                                All Other      +1 818 878 4507
   
       Electronic Mail:         support@ind.alcatel.com
       World Wide Web:          http://alcatel-lucent.com/wps/portal/enterprise
       File Transfer Protocol:  ftp://ftp.ind.alcatel.com/pub/products/mibs"


   DESCRIPTION
       "This module describes an authoritative enterprise-specific Simple
        Network Management Protocol (SNMP) Management Information Base (MIB):

            For the Birds Of Prey Product Line
            Configuration and monitoring of the Server Load Balancing feature

        The right to make changes in specification and other information
        contained in this document without prior notice is reserved.

        No liability shall be assumed for any incidental, indirect, special, or
        consequential damages whatsoever arising from or related to this
        document or the information contained herein.

        Vendors, end-users, and other interested parties are granted
        non-exclusive license to use this specification in connection with
        management of the products for which it is intended to be used.

                    Copyright (C) 1995-2007 Alcatel-Lucent
                        ALL RIGHTS RESERVED WORLDWIDE"
   ::= { softentIND1Slb 1 }

--
-- Object roots used in this MIB
--

alcatelIND1SLBMIBObjects OBJECT-IDENTITY
   STATUS current
   DESCRIPTION 
      "Branch for server load balancing application objects"
   ::= { alcatelIND1SLBMIB 1 }

alcatelIND1SLBMIBConformance OBJECT-IDENTITY
   STATUS current
   DESCRIPTION
      "Branch for server load balancing application conformance information"
   ::= { alcatelIND1SLBMIB 2 }

alcatelIND1SLBMIBGroups OBJECT-IDENTITY
   STATUS current
   DESCRIPTION
      "Branch for server load balancing application units of conformance"
   ::= { alcatelIND1SLBMIBConformance 1 }

alcatelIND1SLBMIBCompliances OBJECT-IDENTITY
   STATUS current
   DESCRIPTION
      "Branch for server load balancing application compliance statements"
   ::= { alcatelIND1SLBMIBConformance 2 }

 
--
-- Textual Conventions
--

-- An Administrative State
SlbAdminState ::= TEXTUAL-CONVENTION
        STATUS          current
        DESCRIPTION
                "The administrative state of various SLB entities
                'disable' : The entity has been disabled.
                'enable'  : The entity is enabled so it can participate
                            in the load balancing activity."
        SYNTAX INTEGER {
                disable(1),
                enable(2)
        }

-- A Basic Operational State
SlbOperState ::= TEXTUAL-CONVENTION
        STATUS          current
        DESCRIPTION
                "The operational state of various SLB entities
                'outOfService' : The entity is out of service.
                'inService'    : The entity operates properly."
        SYNTAX INTEGER {
                outOfService(1),
                inService(2)
        }

-- The SLB Redirection Algorithm
SlbRedirectAlgorithm ::= TEXTUAL-CONVENTION
        STATUS          current
        DESCRIPTION
                "The load-balancing algorithm being used on a 
                cluster to distribute load evenly among real servers. 
		'roundRobin' load-balancing delivers connections evenly 
                amongst real servers while 'serverFailover' gives new 
                connections to the real server only when the previous 
                has failed."
        SYNTAX INTEGER {
                roundRobin(1),
                serverFailover(2)
        }

SlbServerOperState ::= TEXTUAL-CONVENTION
        STATUS          current
        DESCRIPTION
                "The server operational state represents the state of a
                real server being load-balanced by SLB.
                'inService'  : Server is in use as a destination
                               for SLB client connections.
                'linkDown'   : The link by which the server can be
                               reached has failed, so the server
                               is considered out of service.
                'noAnswer'   : The server has not answered to a sequence
                               of ping retries, so the server
                               is considered out of service.
                'disabled'   : Server has been disabled by the admin
                               status, so the server is considered
                               out of service.
                'retrying'   : The server is currently being tested
                               for a number of retries. It is still
                               considered in service.
                'discovery'  : The server is currently being tested to
                               get its MAC address. The server is considered
                               out of service."
        SYNTAX INTEGER {
                inService(1),
                linkDown(2),
                noAnswer(3),
                disabled(4),
                retrying(5),
                discovery(6)
        }

--
--  SLB Feature (global parameters)
--

slbFeature OBJECT IDENTIFIER ::= { alcatelIND1SLBMIBObjects 1 }

slbAdminStatus          OBJECT-TYPE
        SYNTAX          SlbAdminState
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "The administrative status of the SLB feature.
                It allows to turn on/off the feature"
        DEFVAL          { disable }
        ::= { slbFeature 1 }

slbOperStatus           OBJECT-TYPE
        SYNTAX          SlbOperState
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "The operational status of the SLB feature.
                'inService'    means that at least one cluster of
                               servers is inService.
                'outOfService' means that all of defined clusters
                               of servers are outOfService."
        ::= { slbFeature 2 }

slbClustersCount        OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "The number of configured clusters."
        ::= { slbFeature 3 }

slbResetStatistics      OBJECT-TYPE
				SYNTAX INTEGER {
		 				notSignificant(0),
				 		resetSlbStats(1)
       }
        MAX-ACCESS      read-write
        STATUS          current
        DESCRIPTION
                "Resets the SLB statistics."
        ::= { slbFeature 4 }


--
-- SLB Cluster of servers Table
--

slbClusters OBJECT IDENTIFIER ::= { alcatelIND1SLBMIBObjects 2 }

slbClusterTable         OBJECT-TYPE
        SYNTAX          SEQUENCE OF SlbClusterTableEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "This is a table of clusters, each of which is a
                group of real servers to be used by SLB for load
                balancing.  Columnar objects can be modified when the
                row is 'active'.  Rows can be created and destroyed.
                Entries are added to this table via
                slbClusterRowStatus in accordance with the
                RowStatus convention."
        ::= { slbClusters 1 }

slbClusterTableEntry    OBJECT-TYPE
        SYNTAX          SlbClusterTableEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "Information about a particular Cluster." 
        INDEX   {
                slbClusterName
        }
        ::= { slbClusterTable 1 }

SlbClusterTableEntry ::= SEQUENCE {
        slbClusterName                    SnmpAdminString,
        slbClusterAdminStatus             SlbAdminState,
        slbClusterOperStatus              SlbOperState,
        slbClusterVIP                     IpAddress,
        slbClusterRoutedFlowsSuccessRatio Unsigned32,
        slbClusterPingPeriod              Unsigned32,
        slbClusterPingTimeout             Unsigned32,
        slbClusterPingRetries             Unsigned32,
        slbClusterRedirectAlgorithm       SlbRedirectAlgorithm,
        slbClusterIdleTimer               Unsigned32,
        slbClusterNumberOfServers         Unsigned32,
        slbClusterNewFlows                Counter32,
        slbClusterRowStatus               RowStatus,
        slbClusterProbeName               SnmpAdminString,
        slbClusterPackets                 Counter32,
        slbClusterCondition               SnmpAdminString,
        slbClusterType                    INTEGER
}

slbClusterName          OBJECT-TYPE
        SYNTAX          SnmpAdminString (SIZE (1..23))
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "The name of the cluster."
        ::= { slbClusterTableEntry 1 }

slbClusterAdminStatus   OBJECT-TYPE
        SYNTAX          SlbAdminState
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "The administrative state of the cluster."
        DEFVAL          { disable }
        ::= { slbClusterTableEntry 2 }

slbClusterOperStatus    OBJECT-TYPE
        SYNTAX          SlbOperState
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "The operational state of the cluster."
        ::= { slbClusterTableEntry 3 }

slbClusterVIP           OBJECT-TYPE
        SYNTAX          IpAddress
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "The Virtual IP address for that cluster."
        ::= { slbClusterTableEntry 4 }

slbClusterRoutedFlowsSuccessRatio  OBJECT-TYPE
        SYNTAX             Unsigned32
        UNITS              "%"
        MAX-ACCESS         read-only
        STATUS             current
        DESCRIPTION
                "The ratio (in %) of sucessfully routed flows per total
                 number of flows in the cluster."
        ::= { slbClusterTableEntry 5 }

slbClusterPingPeriod    OBJECT-TYPE
        SYNTAX          Unsigned32 (0..3600) 
        UNITS           "seconds"
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "The ping period to check health of servers."
        DEFVAL          { 60 }
        ::= { slbClusterTableEntry 6 }

slbClusterPingTimeout   OBJECT-TYPE
        SYNTAX          Unsigned32 (1..3600000)
        UNITS           "milliseconds"
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "The timeout used to wait for ping answers."
        DEFVAL          { 3000 }
        ::= { slbClusterTableEntry 7 }

slbClusterPingRetries   OBJECT-TYPE
        SYNTAX          Unsigned32 (0..255)
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "The number of ping retries before deciding
                 that a server is OutOfService."
        DEFVAL          { 3 }
        ::= { slbClusterTableEntry 8 }

slbClusterRedirectAlgorithm   OBJECT-TYPE
        SYNTAX                SlbRedirectAlgorithm
        MAX-ACCESS            read-create
        STATUS                current
        DESCRIPTION           "The load balancing algorithm in use
                               by the cluster."
        DEFVAL                { roundRobin }
        ::= { slbClusterTableEntry 9 }

slbClusterIdleTimer     OBJECT-TYPE
        SYNTAX          Unsigned32 (0..86400)
        UNITS           "seconds"
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "The maximum delay with no activity a client is
                 kept attached to a real server."
        DEFVAL          { 1200 }
        ::= { slbClusterTableEntry 10 }

slbClusterNumberOfServers  OBJECT-TYPE
        SYNTAX             Unsigned32
        MAX-ACCESS         read-only
        STATUS             current
        DESCRIPTION
                "The number of real servers in this cluster."
        DEFVAL             { 0 }
        ::= { slbClusterTableEntry 11 }

slbClusterNewFlows         OBJECT-TYPE
        SYNTAX             Counter32
        MAX-ACCESS         read-only
        STATUS             current
        DESCRIPTION
                "The number of flows balanced for this cluster."
        ::= { slbClusterTableEntry 12 }

slbClusterRowStatus        OBJECT-TYPE
        SYNTAX             RowStatus
        MAX-ACCESS         read-create
        STATUS             current
        DESCRIPTION
                "The object is used by a management station to create
                or delete the row entry in slbClusterTable following
                the RowStatus textual convention."
        ::= { slbClusterTableEntry 13 }

slbClusterProbeName        OBJECT-TYPE
        SYNTAX             SnmpAdminString (SIZE (0..23))
        MAX-ACCESS         read-create
        STATUS             current
        DESCRIPTION
                "The name of the cluster's probe."
        ::= { slbClusterTableEntry 14 }

slbClusterPackets          OBJECT-TYPE
        SYNTAX             Counter32
        MAX-ACCESS         read-only
        STATUS             current
        DESCRIPTION
                "The number of packets passed for this cluster."
        ::= { slbClusterTableEntry 15 }

slbClusterCondition        OBJECT-TYPE
        SYNTAX             SnmpAdminString (SIZE (0..23))
        MAX-ACCESS         read-create
        STATUS             current
        DESCRIPTION
                "The Condition name rule.
								Mutually exclusive with VIP" 
        ::= { slbClusterTableEntry 16 }

slbClusterType             OBJECT-TYPE
        SYNTAX             INTEGER {
                                     l3(1),
                                     l2(2)
				}
        MAX-ACCESS         read-create
        STATUS             current
        DESCRIPTION
                "The type of load balancing.  l3 - routed, l2flows - 
								distribute bridged flows"
        DEFVAL          { l3 }
        ::= { slbClusterTableEntry 17 }
--
-- SLB Server Table
--

slbServers OBJECT IDENTIFIER ::= { alcatelIND1SLBMIBObjects 3 }

slbServerTable          OBJECT-TYPE
        SYNTAX          SEQUENCE OF SlbServerTableEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "A table of real servers.  Columnar objects can be
                modified when the row is 'active'.  Rows can be created
                and destroyed.  Entries are added to this table via
                slbServerRowStatus in accordance with the RowStatus
                convention."
        ::= { slbServers 1 }

slbServerTableEntry     OBJECT-TYPE
        SYNTAX          SlbServerTableEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "Information about a particular real server in a
                particular cluster."
        INDEX   {
                slbServerClusterName,
                slbServerIpAddress
        }
        ::= { slbServerTable 1 }

SlbServerTableEntry ::= SEQUENCE {
        slbServerClusterName           SnmpAdminString,
        slbServerIpAddress             IpAddress,
        slbServerAdminStatus           SlbAdminState,
        slbServerOperStatus            SlbServerOperState,
        slbServerAdminWeight           Unsigned32,
        slbServerMacAddress            MacAddress,
        slbServerSlotNumber            Integer32,
        slbServerPortNumber            Integer32,
        slbServerUpTime                Integer32,
        slbServerLastRTT               Integer32,
        slbServerPingFails             Counter32,
        slbServerPortDown              Counter32,
        slbServerFlows                 Counter32,
        slbServerRowStatus             RowStatus,
        slbServerProbeName             SnmpAdminString,
        slbServerProbeStatus           SnmpAdminString
}

slbServerClusterName    OBJECT-TYPE
        SYNTAX          SnmpAdminString (SIZE (1..23))
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "The server's cluster name."
        ::= { slbServerTableEntry 1 }

slbServerIpAddress      OBJECT-TYPE
        SYNTAX          IpAddress
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "The IP address of real server."
        ::= { slbServerTableEntry 2 }

slbServerAdminStatus    OBJECT-TYPE
        SYNTAX          SlbAdminState
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "The administrative status of the server."
        DEFVAL          { enable }
        ::= { slbServerTableEntry 3 }

slbServerOperStatus     OBJECT-TYPE
        SYNTAX          SlbServerOperState
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "The operational status of the server."
        ::= { slbServerTableEntry 4 }

slbServerAdminWeight    OBJECT-TYPE
        SYNTAX          Unsigned32 (0..32)
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "The Administrative weight of the real server used
                by the load-balancing algorithms.  A weight of zero
                indicates that the server is a backup server and is
                not assigned if all non-backup servers are inservice.
                Higher weight values indicate to the load-balancing
                algorithms a higher proportionality hash buckets
                to accept more work."
        DEFVAL          { 1 }
        ::= { slbServerTableEntry 5 }

slbServerMacAddress     OBJECT-TYPE
        SYNTAX          MacAddress
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "The MAC address of the server."
        ::= { slbServerTableEntry 6 }

slbServerSlotNumber     OBJECT-TYPE
        SYNTAX          Integer32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "The physical slot number to which is
                 connected the server."
        ::= { slbServerTableEntry 7 }

slbServerPortNumber     OBJECT-TYPE
        SYNTAX          Integer32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "The physical port number to which is
                 connected the server."
        ::= { slbServerTableEntry 8 }

slbServerUpTime         OBJECT-TYPE
        SYNTAX          Integer32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "The server availibility in %"
        ::= { slbServerTableEntry 9 }

slbServerLastRTT        OBJECT-TYPE
        SYNTAX          Integer32
        UNITS           "milliseconds"
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "The last valid round trip time measured
                 by ping."
        ::= { slbServerTableEntry 10}

slbServerPingFails      OBJECT-TYPE
        SYNTAX          Counter32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "The number of pings that have failed on
                 this server."
        ::= { slbServerTableEntry 11}

slbServerPortDown       OBJECT-TYPE
        SYNTAX          Counter32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "The number of down events received at server port."
        ::= { slbServerTableEntry 12 }

slbServerFlows          OBJECT-TYPE
        SYNTAX          Counter32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "The number of flows directed to this server."
        ::= { slbServerTableEntry 13 }

slbServerRowStatus      OBJECT-TYPE
        SYNTAX          RowStatus
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "The object used by a management station to create
                or delete the row entry in slbServerTable following the
                RowStatus textual convention."
        ::= { slbServerTableEntry 14 }

slbServerProbeName    OBJECT-TYPE
        SYNTAX          SnmpAdminString (SIZE (0..23))
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "The server's probe name."
        ::= { slbServerTableEntry 15 }

slbServerProbeStatus    OBJECT-TYPE
        SYNTAX          SnmpAdminString (SIZE (0..32))
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION
                "The status from doing a probe."
        ::= { slbServerTableEntry 16 }

--
-- SLB Probes Table
--

slbProbes OBJECT IDENTIFIER ::= { alcatelIND1SLBMIBObjects 4 }

slbProbeTable           OBJECT-TYPE
        SYNTAX          SEQUENCE OF SlbProbeTableEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "This is a table of probes, each of which can be 
                used in either the server or cluster tables to 
                define the method that the will be used to determine
                the status of servers.
                Columnar objects can be modified when the
                row is 'active'.  Rows can be created and destroyed.
                Entries are added to this table via
                slbProbeRowStatus in accordance with the
                RowStatus convention."
        ::= { slbProbes 1 }

slbProbeTableEntry      OBJECT-TYPE
        SYNTAX          SlbProbeTableEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "Information about a particular Probe." 
        INDEX   {
                slbProbeName
        }
        ::= { slbProbeTable 1 }

SlbProbeTableEntry ::= SEQUENCE {
        slbProbeName                      SnmpAdminString,
        slbProbeMethod                    INTEGER,
        slbProbePeriod                    Unsigned32,
        slbProbeTimeout                   Unsigned32,
        slbProbeRetries                   Unsigned32,
        slbProbePort                      Integer32,
        slbProbeExpect                    SnmpAdminString,
        slbProbeSend                      SnmpAdminString,
        slbProbeSSL                       INTEGER,
        slbProbeHttpStatus                Integer32,
        slbProbeHttpUrl                   SnmpAdminString,
        slbProbeHttpUsername              SnmpAdminString,
        slbProbeHttpPassword              SnmpAdminString,
        slbProbeRowStatus                 RowStatus
}

slbProbeName            OBJECT-TYPE
        SYNTAX          SnmpAdminString (SIZE (0..23))
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "The name of the probe."
        ::= { slbProbeTableEntry 1 }

slbProbeMethod          OBJECT-TYPE
        SYNTAX          INTEGER {
                          ping(1),
                          http(2),
                          https(3),
                          udp(4),
                          tcp(5),
                          ftp(6),
                          smtp(7),
                          pop(8),
                          pops(9),
                          imap(10),
                          imaps(11),
                          nntp(12)
                    }
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "The probe method used to check the health of servers."
        DEFVAL          { 1 }
        ::= { slbProbeTableEntry 2 }


slbProbePeriod          OBJECT-TYPE
        SYNTAX          Unsigned32 (0..3600) 
        UNITS           "seconds"
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "The probe period to check health of servers."
        DEFVAL          { 60 }
        ::= { slbProbeTableEntry 3 }

slbProbeTimeout         OBJECT-TYPE
        SYNTAX          Unsigned32 (1..3600000)
        UNITS           "milliseconds"
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "The timeout used to wait for probe answers."
        DEFVAL          { 3000 }
        ::= { slbProbeTableEntry 4 }

slbProbeRetries         OBJECT-TYPE
        SYNTAX          Unsigned32 (0..255)
        MAX-ACCESS      read-create
        STATUS          current
        DESCRIPTION
                "The number of probe retries before deciding
                 that a server is OutOfService."
        DEFVAL          { 3 }
        ::= { slbProbeTableEntry 5 }

slbProbePort             OBJECT-TYPE
        SYNTAX           Integer32
        MAX-ACCESS       read-create
        STATUS           current
        DESCRIPTION  
                "The TCP/UDP port the probe should
                be sent on."
        DEFVAL                { 0 }
        ::= { slbProbeTableEntry 6 }

slbProbeExpect           OBJECT-TYPE
        SYNTAX           SnmpAdminString (SIZE (0..32))
        MAX-ACCESS       read-create
        STATUS           current
        DESCRIPTION
                "An ASCII string used to compare a response from 
                a server to verify the health of the server."
        ::= { slbProbeTableEntry 7 }

slbProbeSSL               OBJECT-TYPE
        SYNTAX            INTEGER {
                            enable(1),
                            disable(2)
        }
        MAX-ACCESS        read-create
        STATUS            current
        DESCRIPTION
                "Indicates if a TCP/UDP probe uses SSL."
                DEFVAL { disable }
        ::= { slbProbeTableEntry 8 }

slbProbeSend              OBJECT-TYPE
        SYNTAX            SnmpAdminString (SIZE (0..32))
        MAX-ACCESS        read-create
        STATUS            current
        DESCRIPTION
                "An ASCII string sent to a server to invoke a 
                response from a server to verify the health of 
                the server."
        ::= { slbProbeTableEntry 9 }

slbProbeHttpStatus            OBJECT-TYPE
        SYNTAX            Integer32      
        MAX-ACCESS        read-create
        STATUS            current
        DESCRIPTION
                "The expected status returned from an HTTP GET to
                verify the health of the server."
        DEFVAL            { 200 }
        ::= { slbProbeTableEntry 10 }

slbProbeHttpUrl               OBJECT-TYPE
        SYNTAX            SnmpAdminString (SIZE (0..128))
        MAX-ACCESS        read-create
        STATUS            current
        DESCRIPTION
                "A URL sent to a server for an HTTP GET to verify 
                the health of the server."
        ::= { slbProbeTableEntry 11 }


slbProbeHttpUsername          OBJECT-TYPE
        SYNTAX            SnmpAdminString (SIZE (0..32))
        MAX-ACCESS        read-create
        STATUS            current
        DESCRIPTION
                "An ASCII string sent to a server as credentials for
                an HTTP GET to verify the health of the server."
        ::= { slbProbeTableEntry 12 }

slbProbeHttpPassword          OBJECT-TYPE
        SYNTAX            SnmpAdminString (SIZE (0..32))
        MAX-ACCESS        read-create
        STATUS            current
        DESCRIPTION
                "An ASCII string sent to a server as credentials for
                an HTTP GET to verify the health of the server.  This
                string will be encrypted so it will not display readable."
        ::= { slbProbeTableEntry 13 }


slbProbeRowStatus         OBJECT-TYPE
        SYNTAX            RowStatus
        MAX-ACCESS        read-create
        STATUS            current
        DESCRIPTION
                "The object is used by a management station to create
                or delete the row entry in slbProbeTable following
                the RowStatus textual convention."
        ::= { slbProbeTableEntry 14 }



--
-- SLB Statistic Tables
--

slbStats OBJECT IDENTIFIER ::= { alcatelIND1SLBMIBObjects 5 }

slbStatsTable           OBJECT-TYPE
        SYNTAX          SEQUENCE OF SlbStatsTableEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "Contains the counters statistics for SLB NI entries"
        ::= { slbStats 1 }

slbStatsTableEntry      OBJECT-TYPE
        SYNTAX          SlbStatsTableEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "Cluster statistics table." 
        INDEX   {
                slbStatsClusterName,
                slbStatsIndex
        }
        ::= { slbStatsTable 1 }

SlbStatsTableEntry ::= SEQUENCE {
        slbStatsClusterName               SnmpAdminString,
        slbStatsIndex                     INTEGER,
        slbStatsCounter                   Counter64
}

slbStatsClusterName     OBJECT-TYPE
        SYNTAX           SnmpAdminString (SIZE (1..23))
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "The name of the cluster."
        ::= { slbStatsTableEntry 1 }
				
slbStatsIndex           OBJECT-TYPE
        SYNTAX          INTEGER(1..2000)
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "The sequence number for cluster statistics counter."
        ::= { slbStatsTableEntry 2 }

slbStatsCounter        OBJECT-TYPE
        SYNTAX         Counter64 
        MAX-ACCESS     read-only
        STATUS          current
        DESCRIPTION
                "The statistics counter."
        ::= { slbStatsTableEntry 3 }


slbStatsQual OBJECT IDENTIFIER ::= { alcatelIND1SLBMIBObjects 6 }

slbStatsQualTable       OBJECT-TYPE
        SYNTAX          SEQUENCE OF SlbStatsQualTableEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "The description for the statistics counter.  Describes the 
								qualification parameters on the counter."
        ::= { slbStats 2 }

slbStatsQualTableEntry   OBJECT-TYPE
        SYNTAX          SlbStatsQualTableEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION
                "Information about a particular counter." 
        INDEX   {
                slbStatsClusterName,
                slbStatsIndex,
								slbStatsQualType
        }
        ::= { slbStatsQualTable 1 }

SlbStatsQualTableEntry ::= SEQUENCE {
				slbStatsQualType INTEGER,
				slbStatsQualDataIp IpAddress,
				slbStatsQualDataIpMask IpAddress,
				slbStatsQualDataSlot INTEGER,
				slbStatsQualDataStartPort INTEGER,
				slbStatsQualDataEndPort INTEGER,
				slbStatsQualDataVlan INTEGER,
				slbStatsQualDataL4Port INTEGER,
				slbStatsQualDataIpProtocol INTEGER,
				slbStatsQualDataMac MacAddress,
				slbStatsQualDataMacMask MacAddress,
				slbStatsQualDataEthertype INTEGER,
				slbStatsQualDataIcmpData INTEGER,
				slbStatsQualDataTcpFlags OCTET STRING,
				slbStatsQualDataTos  OCTET STRING,
				slbStatsQualData8021p  INTEGER
}

slbStatsQualType       OBJECT-TYPE
        SYNTAX         INTEGER {
                        dstIp(1),
                        srcIp(2),
                        srcPort(3),
                        srcPortGroup(4),
                        srcVlan(5),
                        ipProtocol(6),
                        dstIpPort(7),
                        srcIpPort(8),
                        dstIpTcpPort(9),
                        srcIpTcpPort(10),
                        dstIpUdpPort(11),
                        srcIpUdpPort(12),
												srcMac(13),
												dstMac(14),
												d8021p(15),
												ethertype(16),
												icmpType(17),
												icmpCode(18),
												tcpFlags(19),
												tos(20),
												dstPort(21),
												dstPortGroup(22)

				}
        MAX-ACCESS     not-accessible
        STATUS          current
        DESCRIPTION
                "The qualification parameter."
        ::= { slbStatsQualTableEntry 1 }

slbStatsQualDataIp     OBJECT-TYPE
        SYNTAX         IpAddress
        MAX-ACCESS     read-only
        STATUS          current
        DESCRIPTION
                "The IP Address of the qualifier."
        ::= { slbStatsQualTableEntry 2 }

slbStatsQualDataIpMask     OBJECT-TYPE
        SYNTAX         IpAddress
        MAX-ACCESS     read-only
        STATUS          current
        DESCRIPTION
                "The IP Address Mask of the qualifier."
        ::= { slbStatsQualTableEntry 3 }

slbStatsQualDataSlot OBJECT-TYPE
        SYNTAX         INTEGER(0..255)
        MAX-ACCESS     read-only
        STATUS          current
        DESCRIPTION
                "The Slot of the qualifier."
        ::= { slbStatsQualTableEntry 4 }

slbStatsQualDataStartPort OBJECT-TYPE
        SYNTAX         INTEGER(0..255)
        MAX-ACCESS     read-only
        STATUS          current
        DESCRIPTION
                "The Start Port of the qualifier."
        ::= { slbStatsQualTableEntry 5 }

slbStatsQualDataEndPort OBJECT-TYPE
        SYNTAX         INTEGER(0..255)
        MAX-ACCESS     read-only
        STATUS          current
        DESCRIPTION
                "The End Port of the qualifier."
        ::= { slbStatsQualTableEntry 6 }

slbStatsQualDataIpProtocol OBJECT-TYPE
        SYNTAX         INTEGER(0..255)
        MAX-ACCESS     read-only
        STATUS          current
        DESCRIPTION
                "The IP Protocol of the qualifier."
        ::= { slbStatsQualTableEntry 7 }

slbStatsQualDataVlan OBJECT-TYPE
        SYNTAX         INTEGER (0..4094)
        MAX-ACCESS     read-only
        STATUS          current
        DESCRIPTION
                "The VLAN of the qualifier. 0 indicates no vlan"
        ::= { slbStatsQualTableEntry 8 }

slbStatsQualDataL4Port OBJECT-TYPE
        SYNTAX         INTEGER (0..65535)
        MAX-ACCESS     read-only
        STATUS          current
        DESCRIPTION
                "The L4 Port of the qualifier."
        ::= { slbStatsQualTableEntry 9 }

slbStatsQualDataMac OBJECT-TYPE
        SYNTAX         MacAddress
        MAX-ACCESS     read-only
        STATUS          current
        DESCRIPTION
                "The MAC Address of the qualifier."
        ::= { slbStatsQualTableEntry 10 }

slbStatsQualDataMacMask OBJECT-TYPE
        SYNTAX         MacAddress
        MAX-ACCESS     read-only
        STATUS          current
        DESCRIPTION
                "The MAC Address Mask of the qualifier."
        ::= { slbStatsQualTableEntry 11 }

slbStatsQualDataEthertype OBJECT-TYPE
        SYNTAX         INTEGER (0..65535)
        MAX-ACCESS     read-only
        STATUS          current
        DESCRIPTION
                "The Ethertype of the qualifier."
        ::= { slbStatsQualTableEntry 12 }

slbStatsQualDataIcmpData OBJECT-TYPE
        SYNTAX         INTEGER (0..255)
        MAX-ACCESS     read-only
        STATUS          current
        DESCRIPTION
                "The ICMP code or type of the qualifier."
        ::= { slbStatsQualTableEntry 13 }

slbStatsQualDataTcpFlags OBJECT-TYPE
        SYNTAX         OCTET STRING (SIZE (3))
        MAX-ACCESS     read-only
        STATUS          current
        DESCRIPTION
                "The TCP flag/mask/<any|all> of the qualifier."
        ::= { slbStatsQualTableEntry 14 }

slbStatsQualDataTos OBJECT-TYPE
        SYNTAX         OCTET STRING (SIZE (2))
        MAX-ACCESS     read-only
        STATUS          current
        DESCRIPTION
                "The TOS/mask of the qualifier."
        ::= { slbStatsQualTableEntry 15 }

slbStatsQualData8021p OBJECT-TYPE
        SYNTAX         INTEGER(0..255)
        MAX-ACCESS     read-only
        STATUS          current
        DESCRIPTION
                "The 802.1p of the qualifier."
        ::= { slbStatsQualTableEntry 16 }


--
-- Server Load Balancing Traps
--

slbTrapsDesc OBJECT IDENTIFIER ::= { slbTraps 1 }
slbTrapsObj  OBJECT IDENTIFIER ::= { slbTraps 2 }

--
-- Traps description
--

-- Software exception
slbTrapException       NOTIFICATION-TYPE
    OBJECTS {
      slbTrapInfoException
    }
    STATUS  current
    DESCRIPTION
        "Software exception in SLB module."
    ::= { slbTrapsDesc 0 1 }

-- Configuration change
slbTrapConfigChanged   NOTIFICATION-TYPE
    OBJECTS {
      slbTrapInfoEntityGroup,
      slbTrapInfoClusterName,
      slbTrapInfoServerIpAddr
    }
    STATUS  current
    DESCRIPTION
        "A change occured in SLB configuration."
    ::= { slbTrapsDesc 0 2 }

-- Operational status changed
slbTrapOperStatus         NOTIFICATION-TYPE
    OBJECTS {
      slbTrapInfoEntityGroup,
      slbTrapInfoOperStatus,
      slbTrapInfoClusterName,
      slbTrapInfoServerIpAddr
    }
    STATUS  current
    DESCRIPTION
        "A change occured in the operational status of a slb entity."
    ::= { slbTrapsDesc 0 3 }

--
-- Trap objects
--

-- A Cluster Name
slbTrapInfoClusterName        OBJECT-TYPE
    SYNTAX                    SnmpAdminString (SIZE (1..23))
    MAX-ACCESS                read-only
    STATUS                    current
    DESCRIPTION               "The name of a cluster."
    ::= { slbTrapsObj 1 }

-- The Operational Status of a cluster
slbTrapInfoOperStatus  OBJECT-TYPE
    SYNTAX                    SlbOperState
    MAX-ACCESS                read-only
    STATUS                    current
    DESCRIPTION               "The operational status of slb, cluster or
                               server."
    ::= { slbTrapsObj 2 }

-- The IP addr of a server
slbTrapInfoServerIpAddr       OBJECT-TYPE
    SYNTAX                    IpAddress
    MAX-ACCESS                read-only
    STATUS                    current
    DESCRIPTION               "The IP address of a server."
    ::= { slbTrapsObj 3 }

-- The Managed entity sub-group
slbTrapInfoEntityGroup        OBJECT-TYPE
    SYNTAX                    INTEGER {
                                slb(1),
                                cluster(2),
                                server(3)
	  }
    MAX-ACCESS 	              read-only
    STATUS                    current
    DESCRIPTION               "The entity group inside slb management."
    ::= { slbTrapsObj 4 }

-- A sofware exception number
slbTrapInfoException          OBJECT-TYPE
    SYNTAX                    Integer32
    MAX-ACCESS                read-only
    STATUS                    current
    DESCRIPTION               "A number identifying the sofware exception."
    ::= { slbTrapsObj 5 }


--
-- COMPLIANCE
--

alcatelIND1SLBMIBCompliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
        "Compliance statement for Server Load Balancing."
    MODULE
        MANDATORY-GROUPS
        {
            slbFeatureGroup,
            slbClustersGroup,
            slbServersGroup,
            slbProbesGroup,
	    slbTrapsGroup
        }
    ::= { alcatelIND1SLBMIBCompliances 1 }


--
-- UNITS OF CONFORMANCE
--

slbFeatureGroup OBJECT-GROUP
   OBJECTS
   {
      slbAdminStatus,
      slbOperStatus,
      slbClustersCount
   }
   STATUS current
   DESCRIPTION
      "Collection of objects for management of Server Load Balancing"
   ::= { alcatelIND1SLBMIBGroups 1 }

slbClustersGroup OBJECT-GROUP
   OBJECTS
   {
      slbClusterAdminStatus,
      slbClusterOperStatus,
      slbClusterVIP,
      slbClusterRoutedFlowsSuccessRatio,
      slbClusterPingPeriod,
      slbClusterPingTimeout,
      slbClusterPingRetries,
      slbClusterRedirectAlgorithm,
      slbClusterIdleTimer,
      slbClusterNumberOfServers,
      slbClusterNewFlows,
      slbClusterRowStatus,
      slbClusterProbeName,
      slbClusterPackets,
      slbClusterCondition,
      slbClusterType
   }
   STATUS current
   DESCRIPTION
      "Collection of objects for management of Server Load Balancing clusters"
   ::= { alcatelIND1SLBMIBGroups 2 }

slbServersGroup OBJECT-GROUP
   OBJECTS
   {
      slbServerAdminStatus,
      slbServerOperStatus,
      slbServerAdminWeight,
      slbServerMacAddress,
      slbServerSlotNumber, 
      slbServerPortNumber,
      slbServerUpTime,
      slbServerLastRTT,
      slbServerPingFails,
      slbServerPortDown,
      slbServerFlows,
      slbServerRowStatus,
      slbServerProbeName,
      slbServerProbeStatus
   }
   STATUS current
   DESCRIPTION
      "Collection of objects for management of Server Load Balancing servers"
   ::= { alcatelIND1SLBMIBGroups 3 }

slbTrapsGroup NOTIFICATION-GROUP
   NOTIFICATIONS 
   {
      slbTrapException,
      slbTrapConfigChanged,
      slbTrapOperStatus
   }
   STATUS current
   DESCRIPTION
      "Collection of traps for management of Server Load Balancing"
   ::= { alcatelIND1SLBMIBGroups 4 }

slbProbesGroup OBJECT-GROUP
   OBJECTS
   { 
      slbProbeMethod,
      slbProbePeriod,
      slbProbeTimeout,
      slbProbeRetries,
      slbProbePort,
      slbProbeExpect,
      slbProbeSend,
      slbProbeSSL,
      slbProbeHttpStatus,
      slbProbeHttpUrl,
      slbProbeHttpUsername,
      slbProbeHttpPassword,
      slbProbeRowStatus
   }
   STATUS current
   DESCRIPTION
      "Collection of objects for management of Server Load Balancing probes"
   ::= { alcatelIND1SLBMIBGroups 5 }


slbStatsGroup OBJECT-GROUP
   OBJECTS
   { 
      slbStatsCounter,  
			slbStatsQualDataIp,
			slbStatsQualDataIpMask,
			slbStatsQualDataSlot,
			slbStatsQualDataStartPort,
			slbStatsQualDataEndPort,
			slbStatsQualDataVlan,
			slbStatsQualDataL4Port,
			slbStatsQualDataMac,
			slbStatsQualDataEthertype,
			slbStatsQualDataIcmpData,
			slbStatsQualDataTcpFlags,
			slbStatsQualDataTos
   }
   STATUS current
   DESCRIPTION
      "Collection of objects for management of Server Load Balancing probes"
   ::= { alcatelIND1SLBMIBGroups 6 }
END

